H04J   1/00  \	0	0	5K022	H04J   1/00	6359	周波数分割多重化方式（Ｈ０４Ｊ１４／０２が優先）［５］	Frequency-division multiplex systems () [5]
H04J   1/02  \	1	1	5K022	H04J   1/02	445	細部	Details
H04J   1/04  \	2	2	5K022	H04J   1/04	247	周波数変換配置	Frequency-transposition arrangements
H04J   1/04 100 \	3	3	5K022	H04J   1/04	26	周波数転換に利用されるフィルター	filter used for converting frequency
H04J   1/05  \	3	3	5K022	H04J   1/05	180	デジタル技術を用いるもの［３］	using digital techniques [3]
H04J   1/06  \	2	2	5K022	H04J   1/06	175	搬送波供給配置	Arrangements for supplying the carrier waves
H04J   1/08  \	2	2	5K022	H04J   1/08	198	チャンネル結合配置	Arrangements for combining channels
H04J   1/10  \	2	2	5K022	H04J   1/10	120	中間局配置，例．分岐用，傍受用	Intermediate station arrangements, e.g. for branching, for tapping-off
H04J   1/12  \	2	2	5K022	H04J   1/12	108	チャネル間漏話低減配置	Arrangements for reducing cross-talk between channels
H04J   1/14  \	2	2	5K022	H04J   1/14	146	呼出信号または監視信号に備えるための配置	Arrangements providing for calling or supervisory signals
H04J   1/16  \	2	2	5K022	H04J   1/16	179	監視配置	Monitoring arrangements
H04J   1/18  \	1	1	5K022	H04J   1/18	9	全搬送波が振幅変調されているもの（Ｈ０４Ｊ１／０２が優先）［３］	in which all the carriers are amplitude-modulated (H04J 1/02 takes precedence) [3]
H04J   1/20  \	1	1	5K022	H04J   1/20	28	少くとも一搬送波が角度変調されているもの（Ｈ０４Ｊ１／０２が優先）［３］	in which at least one carrier is angle-modulated (H04J 1/02 takes precedence) [3]
H04J   3/00  \	0	0	5K028	H04J   3/00	281	時分割多重化方式（Ｈ０４Ｊ１４／０８が優先）［４，５］	Time-division multiplex systems () [4,5]
H04J   3/00  A	0	0	5K028	H04J   3/00	1290	多重化・多重分離化方式	Multiplexing or multi-separation system
H04J   3/00  B	0	1	5K028	H04J   3/00	1157	フレ−ム構成に特徴のあるの	characterized by the frame configuration
H04J   3/00  C	0	1	5K028	H04J   3/00	244	信号の形式に特徴のあるもの	characterized by the signal format
H04J   3/00  D	0	2	5K028	H04J   3/00	78	ＰＡＭ信号	PAM signal
H04J   3/00  E	0	2	5K028	H04J   3/00	165	ＰＰＭ信号	PPM signal
H04J   3/00  F	0	2	5K028	H04J   3/00	54	ＰＷＭ信号	PWM signal
H04J   3/00  G	0	2	5K028	H04J   3/00	68	多値信号	Many-valued signal
H04J   3/00  H	0	0	5K028	H04J   3/00	3346	ＴＤＭＡ〔衛星通信を除く〕	TDMA (excluding satellite communication)
H04J   3/00  J	0	1	5K028	H04J   3/00	124	ＡＧＣ	AGC
H04J   3/00  K	0	1	5K028	H04J   3/00	545	多方向多重	Multi-direction multiplexing
H04J   3/00  L	0	0	5K028	H04J   3/00	77	ＦＤＭよりＴＤＭへの変換	Conversion from FDM into TDM
H04J   3/00  M	0	0	5K028	H04J   3/00	2040	映像信号の多重	Video signal multiplexing
H04J   3/00  N	0	0	5K028	H04J   3/00	82	ＴＶ信号帰線期間中の信号多重〔文献分類〕	Signal multiplexing during the TV signal retrace line period (literary categorisation)
H04J   3/00  P	0	0	5K028	H04J   3/00	142	商用電源波形を利用するもの	utilising the commercial power supply waveform
H04J   3/00  Q	0	0	5K028	H04J   3/00	582	光を利用するもの〔多重に特徴のないものは，Ｈ０４Ｂ９／００〕	utilising light (not characterized by multiplexing H 04 B 9/00)
H04J   3/00  R	0	0	5K028	H04J   3/00	587	現用・予備〔多重通信系の現用・予備切換，Ｈ０４Ｌ１／２２も分類〕	In-service/standby (change-over between in-service and standby of the multi-communication system. H 04 L 1/22 also applicable.)
H04J   3/00  S	0	0	5K028	H04J   3/00	159	時間圧縮多重	Time compression multiplexing
H04J   3/00  T	0	0	5K028	H04J   3/00	366	交換関連のもの〔文献分類〕	related to switching (literary categorisation)
H04J   3/00  U	0	0	5K028	H04J   3/00	1380	新同期デジタルハイアラーキ（ＳＤＨ，ＳＯＮＥＴ）	New synchronisation digital hierarchy (SDH, SONET)
H04J   3/00  V	0	1	5K028	H04J   3/00	365	オーバーヘッド	Overhead
H04J   3/00  W	0	2	5K028	H04J   3/00	242	ポインタ	Pointer
H04J   3/00  X	0	0	5K028	H04J   3/00	240	クロスコネクタ	Cross-connector
H04J   3/00  Y	0	0	5K028	H04J   3/00	287	ＩＳＤＮ（多重処理に関するもの）	ISDN (related to the multiplexing process)
H04J   3/00  Z	0	0	5K028	H04J   3/00	1354	その他のもの	Others
H04J   3/02  \	1	1	5K028	H04J   3/02	238	細部	Details
H04J   3/04  \	2	2	5K028	H04J   3/04	26	変調器または復調器と結合された分配器	Distributors combined with modulators or demodulators
H04J   3/04  A	2	0	5K028	H04J   3/04	306	復調器と結合された分配器	Distributor coupled with the demodulator
H04J   3/04  Z	2	0	5K028	H04J   3/04	807	その他のもの〔多重化回路〕	Others (multiplexing circuit)
H04J   3/06  \	2	2	5K028	H04J   3/06	115	同期配置	Synchronising arrangements
H04J   3/06  A	2	0	5K028	H04J   3/06	1913	フレ−ム同期〔Ｈ０４Ｌ７／０８にも分類〕	Frame synchronisation (also categorised into H 04 L 7/08)
H04J   3/06  B	2	1	5K028	H04J   3/06	408	フレ−ム同期保護	Frame synchronisation protection
H04J   3/06  C	2	0	5K028	H04J   3/06	541	多重変換	Multi-conversion
H04J   3/06  D	2	0	5K028	H04J   3/06	939	位相同期	Phase synchronisation
H04J   3/06  Z	2	0	5K028	H04J   3/06	1452	その他のもの	Others
H04J   3/07  \	3	3	5K028	H04J   3/07	568	異なるまたは変動する情報速度をもつ系のためにスタッフパルスを用いるもの［３］	using pulse stuffing for systems with different or fluctuating information rates [3]
H04J   3/08  \	2	2	5K028	H04J   3/08	14	中間局配置，例．分岐用，傍受用	Intermediate station arrangements, e.g. for branching, for tapping-off
H04J   3/08  A	2	0	5K028	H04J   3/08	379	中継	Relay
H04J   3/08  B	2	0	5K028	H04J   3/08	362	分岐・挿入	Branch or insertion
H04J   3/08  Z	2	0	5K028	H04J   3/08	30	その他のもの	Others
H04J   3/10  \	2	2	5K028	H04J   3/10	47	チャネル間漏話低減配置	Arrangements for reducing cross-talk between channels
H04J   3/12  \	2	2	5K028	H04J   3/12	442	呼出信号または監視信号に備えるための配置	Arrangements providing for calling or supervisory signals
H04J   3/14  \	2	2	5K028	H04J   3/14	61	監視配置	Monitoring arrangements
H04J   3/14  A	2	0	5K028	H04J   3/14	917	監視信号によるもの	using the observation signal
H04J   3/14  Z	2	0	5K028	H04J   3/14	1452	その他のもの	Others
H04J   3/16  \	1	1	5K028	H04J   3/16	116	一伝送サイクル内の個々のチャンネルに対する時間割り当てが可変であるもの，例．複数の信号の組合せが次々に変ってゆくのを調整するもの，伝送チャンネルの数を変化させるもの（Ｈ０４Ｊ３／１７，Ｈ０４Ｊ３／２４が優先）［４］	in which the time allocation to individual channels within a transmission cycle is variable, e.g. to accommodate varying complexity of signals, to vary number of channels transmitted (H04J 3/17, H04J 3/24 take precedence) [4]
H04J   3/16  A	1	0	5K028	H04J   3/16	240	優先伝送	Preferential transmission
H04J   3/16  Z	1	0	5K028	H04J   3/16	1190	その他のもの	Others
H04J   3/17  \	1	1	5K028	H04J   3/17	49	第１番目の使用者が休止したとき，その使用者に割り当てられていた伝送チャンネルを解放して第２番目の使用者に割り当てるもの，例．ＴＡＳＩ［２００６．０１］	in which the transmission channel allotted to a first user may be taken away and re-allotted to a second user if the first user becomes inactive, e.g. TASI [2006.01]
H04J   3/17  A	1	0	5K028	H04J   3/17	246	音声休止チヤンネルにデ−タを割り当てるもの	Data assigned to the voice paused channel
H04J   3/17  Z	1	0	5K028	H04J   3/17	480	その他のもの	Others
H04J   3/18  \	1	1	5K028	H04J   3/18	23	個々の信号の周波数圧縮およびその後に続く周波数伸張を用いるもの	using frequency compression and subsequent expansion of the individual signals
H04J   3/20  \	1	1	5K028	H04J   3/20	65	レゾナントトランスファーを用いるもの［２］	using resonant transfer [2]
H04J   3/22  \	1	1	5K028	H04J   3/22	506	複数の送信源が異なる速度または符号をもつもの［４］	in which the sources have different rates or codes [4]
H04J   3/24  \	1	1	5K028	H04J   3/24	391	割り当てがアドレスによって指示されるもの（Ｈ０４Ｊ３／１７が優先）［４］	in which the allocation is indicated by an address () [4]
H04J   3/26  \	2	2	5K028	H04J   3/26	37	情報およびアドレスが同時に伝送されるもの［４］	in which the information and the address are simultaneously transmitted [4]
H04J   4/00  \	0	0	5K022	H04J   4/00	438	時分割多重化方式と周波数分割多重化方式との組み合せ（Ｈ０４Ｊ１３／００が優先）［２］	Combined time-division and frequency-division multiplex systems (H04J 13/00 takes precedence) [2]
H04J   7/00  \	0	0	5K022	H04J   7/00	172	個々のチャネルの信号の振幅または持続時間がそれらのチャネルに特有であるような多重化方式	Multiplex systems in which the amplitudes or durations of the signals in individual channels are characteristic of those channels
H04J   7/02  \	1	1	5K022	H04J   7/02	9	振幅の極性が特有であるようなもの	in which the polarity of the amplitude is characteristic
H04J   9/00  \	0	0	5K022	H04J   9/00	284	各チャネルが相異なる搬送波変調形式によって表わされる多重化方式	Multiplex systems in which each channel is represented by a different type of modulation of the carrier
H04J  11/00  \	0	0	5K022	H04J  11/00	190	直交多重化方式（Ｈ０４Ｊ１３／００が優先）［２］	Orthogonal multiplex systems (H04J 13/00 takes precedence) [2]
H04J  11/00  A	0	0	5K022	H04J  11/00	289	位相直交多重化方式	Phase orthogonal multiplexing system
H04J  11/00  B	0	0	5K022	H04J  11/00	790	偏波直交多重化方式	Polarisation orthogonal multiplexing system
H04J  11/00  Z	0	0	5K022	H04J  11/00	17640	その他のもの	Others
H04J  13/00  \	0	0	5K022	H04J  13/00	4829	符号分割多重化方式（周波数ホッピングのためのものＨ０４Ｂ１／７１３）［２，２０１１．０１］	Code division multiplex systems (for frequency hopping H04B  1/713)
H04J  13/10  \	1	1	5K022	H04J  13/10	632	符号の生成［２０１１．０１］	Code generation
H04J  13/12  \	2	2	5K022	H04J  13/12	234	直交符号の生成［２０１１．０１］	Generation of orthogonal codes
H04J  13/14  \	2	2	5K022	H04J  13/14	87	ＺＣＺ符号の生成［２０１１．０１］	Generation of codes with a zero correlation zone
H04J  13/16  \	1	1	5K022	H04J  13/16	1145	符号割当て［２０１１．０１］	Code allocation
H04J  13/18  \	2	2	5K022	H04J  13/18	827	直交符号の割当て［２０１１．０１］	Allocation of orthogonal codes
H04J  13/20  \	3	3	5K022	H04J  13/20	99	直交可変拡散率［ＯＶＳＦ］符号の割当て［２０１１．０１］	having an orthogonal variable spreading factor [OVSF]
H04J  13/22  \	2	2	5K022	H04J  13/22	234	零相関範囲［ＺＣＺ］符号の割当て［２０１１．０１］	Allocation of codes with a zero correlation zone
H04J  14/00  \	0	0	5K102	H04J  14/00	1116	光学的多重化方式［５］	Optical multiplex systems [5]
H04J  14/00 150 \	1	1	5K102	H04J  14/00	173	光符号多重化方式	Optical Code Multiplex
H04J  14/02  \	1	1	5K102	H04J  14/02	6854	波長分割多重化方式［５］	Wavelength-division multiplex systems [5]
H04J  14/02 101 \	2	2	5K102	H04J  14/02	1273	アッド　アンド　ドロップ多重処理	Add and drop multiplexing
H04J  14/02 121 \	2	2	5K102	H04J  14/02	335	パワー制御，例．総光パワーの一定維持	Power, e.g. constant maintenance of the total optical power
H04J  14/02 198 \	2	2	5K102	H04J  14/02	381	サブキャリア多重化処理［ＳＣＭ］を有するもの	with sub-carrier multiplexing [SCM]
H04J  14/04  \	1	1	5K102	H04J  14/04	181	モード多重化方式［５］	Mode multiplex systems [5]
H04J  14/06  \	1	1	5K102	H04J  14/06	434	偏波多重化方式［５］	Polarization multiplex systems [5]
H04J  14/08  \	1	1	5K102	H04J  14/08	1054	時分割多重化方式［５］	Time-division multiplex systems [5]
H04J  14/08 130 \	2	2	5K102	H04J  14/08	50	アッド　アンド　ドロップ多重処理	Add and drop multiplexing
H04J  99/00  \	0	0	5K022	H04J  99/00	9308	このサブクラスの他のグループには分類されない主題事項［２００９．０１］	Subject matters not provided for in other groups of this subclass [2009.01]
H04J  99/00 100 \	1	1	5K022	H04J  99/00	495	非直交多重化方式	Non-orthogonal multiple access system
