E06B1/00	7	Border constructions of openings in walls, floors, or ceilings; Frames to be rigidly mounted in such openings (E06B5/00 takes precedence; features relating also to inner frames or wing frames, features relating solely to the mounting of inner frames E06B3/00; corner joints or edge joints E06B3/96)	E06B1/00	E06B1/00		214
E06B1/003	8	{Cavity wall closers; Fastening door or window frames in cavity walls (lintels E04C3/02)}	E06B1/00	E06B1/00		366
E06B1/006	8	{of curvilinear outline}	E06B1/00	E06B1/00		272
E06B1/02	8	Base frames, i.e. template frames for openings in walls or the like, provided with means for securing a further rigidly-mounted frame; Special adaptations of frames to be fixed therein {(E06B1/003, E06B1/24 take precedence; fastening door or window frames per seE06B1/56)}	E06B1/02	E06B1/02		1462
E06B1/04	8	Frames for doors, windows, or the like to be fixed in openings ({of curvilinear outline E06B1/006; } special adaptations for fixing in base frames E06B1/02; features relating solely to the mounting of glass panes or other sheets E06B3/00)	E06B1/04	E06B1/04		497
E06B1/045	9	{with separate wing abutment strips, e.g. adjustable; Door stops (sealing arrangements E06B7/16)}	E06B1/04	E06B1/04		276
E06B1/06	9	Wooden frames	E06B1/06	E06B1/06		249
E06B1/08	10	composed of several parts with respect to the cross-section of the frame itself	E06B1/08	E06B1/08		442
E06B1/10	11	adjustable with respect to the thickness of walls	E06B1/10	E06B1/10		271
E06B1/12	9	Metal frames	E06B1/12	E06B1/12		654
E06B1/14	10	of special cross-section (E06B1/18, E06B1/22 take precedence){not used}	E06B1/14	E06B1/14		36
E06B1/16	11	Hollow frames	E06B1/16	E06B1/16		236
E06B1/18	10	composed of several parts with respect to the cross-section of the frame itself	E06B1/18	E06B1/18		460
E06B1/20	11	adjustable with respect to the thickness of walls	E06B1/20	E06B1/20		322
E06B1/22	10	with integral thresholds of special form	E06B1/22	E06B1/22		15
E06B1/24	9	Frames of natural stone, concrete, or other stone-like material	E06B1/24	E06B1/24		411
E06B1/26	9	Frames of plastics	E06B1/26	E06B1/26		260
E06B1/28	10	Hollow frames (E06B1/30 takes precedence)	E06B1/28	E06B1/28		158
E06B1/30	10	composed of several parts with respect to the cross-section of the frame itself	E06B1/30	E06B1/30		434
E06B1/32	9	Frames composed of parts made of different materials	E06B1/32	E06B1/32		779
E06B1/325	10	{comprising insulation between two metal section members}	E06B1/32	E06B1/32		347
E06B1/34	9	Coverings, e.g. protecting against weather, for decorative purposes	E06B1/34	E06B1/34		1398
E06B1/342	10	{Reveal covering members disposed alongside of a window frame}	E06B1/34	E06B1/34		455
E06B1/345	10	{Renovation window frames covering the existing old frames}	E06B1/34	E06B1/34		171
E06B1/347	10	{Renovation door frames covering the existing old frames}	E06B1/34	E06B1/34		220
E06B1/36	9	Frames uniquely adapted for windows	E06B1/36	E06B1/36		1549
E06B1/363	10	{Bay windows}	E06B1/36	E06B1/36		357
E06B1/366	10	{Mullions or transoms therefor}	E06B1/36	E06B1/36		392
E06B1/38	10	for shop, show, or like large windows	E06B1/38	E06B1/38		821
E06B1/40	10	Frames with parts removable to admit the glass (E06B1/38 takes precedence)	E06B1/40	E06B1/40		35
E06B1/52	9	Frames specially adapted for doors	E06B1/52	E06B1/52		1838
E06B1/522	10	{for overhead garage doors}	E06B1/52	E06B1/52		162
E06B1/524	10	{Mullions; Transoms}	E06B1/52	E06B1/52		351
E06B1/526	10	{for door wings that can be set up to open either left or right, outwards or inwards, e.g. provided with grooves for easily detachable hinges or latch plates (locks therefor E05B63/04; hinges therefor E05D7/02)}	E06B1/52	E06B1/52		571
E06B1/528	10	{with ducts for cables or pipes}	E06B1/52	E06B1/52		129
E06B1/56	8	Fastening frames to the border of openings {or to similar contiguous frames (E06B1/003 takes precedence)}	E06B1/56	E06B1/56		425
E06B1/58	9	by filling up the joints, e.g. by cementing	E06B1/58	E06B1/58		648
E06B1/60	9	by mechanical means, e.g. anchoring means	E06B1/60	E06B1/60		842
E06B1/6007	10	{between similar contiguous frames (bay windows E06B1/363)}	E06B1/60	E06B1/60		263
E06B1/6015	10	{Anchoring means (E06B1/6007, E06B1/6046&#160;-&#160;E06B1/6092 take precedence)}	E06B1/60	E06B1/60		1178
E06B1/6023	11	{completely hidden between the frame and the border of the opening, at least part of the means being previously fixed to the wall (E06B1/6038 takes precedence)}	E06B1/60	E06B1/60		278
E06B1/603	12	{adjustable}	E06B1/60	E06B1/60		300
E06B1/6038	11	{specially adapted for being embedded in the wall}	E06B1/60	E06B1/60		385
E06B1/6046	10	{Clamping means acting perpendicular to the wall opening; Fastening frames by tightening or drawing them against a surface parallel to the opening (E06B1/6007 takes precedence)}	E06B1/60	E06B1/60		315
E06B1/6053	11	{the frame being moved perpendicularly towards the opening and held by means of snap action behind a protrusion on the border of the opening}	E06B1/60	E06B1/60		161
E06B1/6061	11	{with separate clamping means acting on opposite wall or associated surfaces}	E06B1/60	E06B1/60		144
E06B1/6069	10	{Separate spacer means acting exclusively in the plane of the opening; Shims; Wedges; Tightening of a complete frame inside a wall opening (E06B1/6084 takes precedence)}	E06B1/60	E06B1/60		441
E06B1/6076	11	{of screw-type}	E06B1/60	E06B1/60		595
E06B1/6084	10	{Mounting frames elastically, e.g. with springs or other elastic material, between the wall and the frame (E06B1/6046 takes precedence)}	E06B1/60	E06B1/60		147
E06B1/6092	10	{Fastening door frames to the floor or ceiling; Jamb feet; Cross members uniting the jamb feet (E06B1/70 and E06B3/9632 take precedence)}	E06B1/60	E06B1/60		223
E06B1/62	8	Tightening or covering joints between the border of openings and the frame {or between contiguous frames}(E06B1/34 takes precedence)	E06B1/62	E06B1/62		1943
E06B2001/622	9	{especially adapted for door frames; Joint covering devices where the wall surface is parallel to the adjacent door or window frame part}	E06B1/62	E06B1/62		416
E06B2001/624	9	{with parts to be embedded in the stucco layer or otherwise linked to this layer}	E06B1/62	E06B1/62		362
E06B2001/626	9	{comprising expanding foam strips}	E06B1/62	E06B1/62		321
E06B2001/628	9	{Separate flexible joint covering strips; Flashings}	E06B1/62	E06B1/62		616
E06B1/64	9	by loosely-inserted means, e.g. strip, resilient tongue	E06B1/64	E06B1/64		369
E06B1/66	9	by labyrinth packings	E06B1/66	E06B1/66		21
E06B1/68	9	by profiled external parts	E06B1/68	E06B1/68		470
E06B1/70	8	Sills; Thresholds	E06B1/70	E06B1/70		1635
E06B1/702	9	{Window sills}	E06B1/70	E06B1/70		1311
E06B1/705	10	{End-caps therefor}	E06B1/70	E06B1/70		319
E06B2001/707	9	{Thresholds with special provision for insulation}	E06B1/70	E06B1/70		430
E06B3/00	7	Window sashes, door leaves, or like elements for closing {wall or like} openings; Layout of fixed or moving closures, e.g. windows {in wall or like openings}; Features of rigidly-mounted outer frames relating to the mounting of wing frames (E06B5/00 takes precedence; shutters or the like E06B9/00; glass panes C03)	E06B3/00	E06B3/00		732
E06B3/01	8	Removable or disappearing walls for hangars or other halls, e.g. for aircraft (wall constructions E04B2/00)	E06B3/01	E06B3/01		380
E06B3/02	8	Wings made completely of glass {(E06B3/4681 takes precedence)}	E06B3/02	E06B3/02		1031
E06B3/025	9	{consisting of multiple glazing units (units per seE06B3/66)}	E06B3/02	E06B3/02		370
E06B3/04	8	Wing frames not characterised by the manner of movement (features relating to the manner of movement E06B3/32)	E06B3/04	E06B3/04		249
E06B3/06	9	Single frames	E06B3/06	E06B3/06		244
E06B3/08	10	Constructions depending on the use of specified materials (E06B3/24 takes precedence)	E06B3/08	E06B3/08		544
E06B3/10	11	of wood	E06B3/10	E06B3/10		510
E06B3/105	12	{reinforced}	E06B3/10	E06B3/10		121
E06B3/12	11	of metal	E06B3/12	E06B3/12		896
E06B3/14	12	of special cross-section {(not used, see subgroup and E06B3/12)}	E06B3/14	E06B3/14		22
E06B3/16	13	Hollow frames {of special construction, e.g. made of folded sheet metal or of two or more section parts connected together}	E06B3/16	E06B3/16		552
E06B3/163	14	{with a filled cavity}	E06B3/16	E06B3/16		131
E06B2003/166	14	{with a filled cavity}	E06B3/16	E06B3/16		8
E06B3/18	11	of concrete or other stone-like material	E06B3/18	E06B3/18		49
E06B3/20	11	of plastics	E06B3/20	E06B3/20		333
E06B3/205	12	{moulded or extruded around a core}	E06B3/20	E06B3/20		269
E06B3/22	12	Hollow frames {(E06B3/205 takes precedence)}	E06B3/22	E06B3/22		472
E06B3/221	13	{with the frame member having local reinforcements in some parts of its cross-section or with a filled cavity}	E06B3/22	E06B3/22		342
E06B3/222	14	{with internal prefabricated reinforcing section members inserted after manufacturing of the hollow frame}	E06B3/22	E06B3/22		767
E06B3/223	15	{the hollow frame members comprising several U-shaped parts assembled around a reinforcing core member}	E06B3/22	E06B3/22		91
E06B2003/224	15	{with reinforcing plastic section members}	E06B3/22	E06B3/22		81
E06B2003/225	15	{Means for stabilising the insert}	E06B3/22	E06B3/22		94
E06B2003/226	16	{by adhesives or filling up the remainder of the cavity, e.g. together with foam}	E06B3/22	E06B3/22		103
E06B2003/227	15	{with reinforcing wooden section members}	E06B3/22	E06B3/22		35
E06B2003/228	14	{with separate reinforcements situated outside the cavity or in the walls}	E06B3/22	E06B3/22		87
E06B3/24	10	specially adapted for double glazing (separable parts for securing panes E06B3/64)	E06B3/24	E06B3/24		519
E06B3/26	9	Compound frames, i.e. one frame within or behind another (E06B3/28 takes precedence; arrangements of movable frames E06B3/32)	E06B3/26	E06B3/26		921
E06B3/2605	10	{with frames permanently mounted behind or within each other, each provided with a pane or screen}	E06B3/26	E06B3/26		1305
E06B2003/261	11	{Frames made of wood}	E06B3/26	E06B3/26		305
E06B2003/2615	11	{Frames made of metal}	E06B3/26	E06B3/26		456
E06B2003/262	11	{Frames made of plastic material}	E06B3/26	E06B3/26		142
E06B2003/2625	11	{with different frames made from different materials}	E06B3/26	E06B3/26		279
E06B3/263	9	Frames with special provision for insulation	E06B3/263	E06B3/263		1323
E06B3/26301	10	{with prefabricated insulating strips between two metal section members (with two metal frame members having interpenetrating or overlapping parts when mounted E06B3/26336; combined with insulating elements formed in situE06B3/2675)}	E06B3/263	E06B3/263		593
E06B3/26303	11	{with thin strips, e.g. defining a hollow space between the metal section members}	E06B3/263	E06B3/263		1009
E06B3/26305	11	{Connection details (deformation of portions of the metal frame members E06B3/273; expansion of the extremities of the insulating elements E06B3/277)}	E06B3/263	E06B3/263		376
E06B3/26307	12	{Insulating strips and metal section members both having L-shaped ribs, the engagement being made by a movement transversal to the plane of the strips}	E06B3/263	E06B3/263		158
E06B2003/26309	12	{using glue}	E06B3/263	E06B3/263		107
E06B2003/2631	12	{Screw or pin connections}	E06B3/263	E06B3/263		96
E06B2003/26312	12	{Snap connections}	E06B3/263	E06B3/263		197
E06B2003/26314	12	{Provisions for reducing the shift between the strips and the metal section members}	E06B3/263	E06B3/263		104
E06B2003/26316	12	{Disconnectable connections or permitting shifting between the sections}	E06B3/263	E06B3/263		79
E06B2003/26318	12	{Connecting by rotating the metal section or the strip around its longitudinal axis}	E06B3/263	E06B3/263		15
E06B3/2632	10	{with arrangements reducing the heat transmission, other than an interruption in a metal section}	E06B3/263	E06B3/263		563
E06B2003/26321	11	{with additional prefab insulating materials in the hollow space}	E06B3/263	E06B3/263		318
E06B2003/26323	11	{with coatings reducing the radiation}	E06B3/263	E06B3/263		51
E06B2003/26325	11	{the convection or radiation in a hollow space being reduced, e.g. by subdividing the hollow space}	E06B3/263	E06B3/263		67
E06B2003/26327	12	{with separate thin walled inserts}	E06B3/263	E06B3/263		75
E06B2003/26329	12	{the insulating strips between the metal sections being interconnected}	E06B3/263	E06B3/263		99
E06B2003/2633	12	{the insulating strips between the metal sections having ribs extending into the hollow space}	E06B3/263	E06B3/263		138
E06B2003/26332	11	{Arrangements reducing the heat transfer in the glazing rabbet or the space between the wing and the casing frame}	E06B3/263	E06B3/263		261
E06B2003/26334	11	{Contact reducing arrangements between the insulating strips and the metal sections}	E06B3/263	E06B3/263		34
E06B3/26336	10	{with two metal frame members having interpenetrating or overlapping parts when mounted (involving sheet metal section members E06B3/2735)}	E06B3/263	E06B3/263		198
E06B3/26338	10	{comprising short insulating elements disposed at intervals}	E06B3/263	E06B3/263		200
E06B3/2634	10	{without separate insulating elements, e.g. the heat transmission being reduced by a smaller cross-section}	E06B3/263	E06B3/263		121
E06B3/26341	10	{comprising only one metal frame member combined with an insulating frame member}	E06B3/263	E06B3/263		274
E06B3/26343	10	{with two or more separate insulating zones alternating with metal section members}	E06B3/263	E06B3/263		97
E06B3/26345	10	{for wooden or plastic section members}	E06B3/263	E06B3/263		261
E06B3/26347	10	{specially adapted for sliding doors or windows}	E06B3/263	E06B3/263		612
E06B2003/26349	10	{Details of insulating strips}	E06B3/263	E06B3/263		70
E06B2003/2635	11	{Specific form characteristics}	E06B3/263	E06B3/263		168
E06B2003/26352	12	{hollow}	E06B3/263	E06B3/263		368
E06B2003/26354	13	{filled}	E06B3/263	E06B3/263		88
E06B2003/26356	13	{Honeycomb}	E06B3/263	E06B3/263		27
E06B2003/26358	12	{stepped or undulated}	E06B3/263	E06B3/263		100
E06B2003/26359	12	{making flush mounting with neighbouring metal section members possible}	E06B3/263	E06B3/263		145
E06B2003/26361	12	{Openings, incisions or indents}	E06B3/263	E06B3/263		86
E06B2003/26363	12	{Screw channels}	E06B3/263	E06B3/263		20
E06B2003/26365	12	{Composed of several similar parts positioned one after the other}	E06B3/263	E06B3/263		44
E06B2003/26367	11	{making flush mounting with neighbouring metal section members possible}	E06B3/263	E06B3/263		13
E06B2003/26369	11	{Specific material characteristics}	E06B3/263	E06B3/263		129
E06B2003/2637	12	{reinforced}	E06B3/263	E06B3/263		101
E06B2003/26372	12	{with coatings}	E06B3/263	E06B3/263		51
E06B2003/26374	12	{with parts of differing nature}	E06B3/263	E06B3/263		117
E06B2003/26376	12	{Non-plastic materials, e.g. wood, metal}	E06B3/263	E06B3/263		71
E06B2003/26378	12	{comprising foam}	E06B3/263	E06B3/263		103
E06B2003/26379	11	{Specific characteristics concerning the disposition between the metal section members}	E06B3/263	E06B3/263		26
E06B2003/26381	12	{disposed obliquely}	E06B3/263	E06B3/263		31
E06B2003/26383	12	{with two similar parallel strips, one shifted to one side}	E06B3/263	E06B3/263		42
E06B2003/26385	12	{with strips disposed perpendicular to each other}	E06B3/263	E06B3/263		38
E06B2003/26387	11	{Performing extra functions}	E06B3/263	E06B3/263		205
E06B2003/26389	12	{Holding sealing strips or forming sealing abutments}	E06B3/263	E06B3/263		441
E06B2003/2639	12	{Provisions for fittings, e.g. locks or hinges}	E06B3/263	E06B3/263		104
E06B2003/26392	10	{Glazing bars}	E06B3/263	E06B3/263		97
E06B2003/26394	10	{Strengthening arrangements in case of fire}	E06B3/263	E06B3/263		124
E06B2003/26396	10	{specially adapted for sheet metal frames}	E06B3/263	E06B3/263		90
E06B2003/26398	10	{with two metal sections clamping a pane}	E06B3/263	E06B3/263		83
E06B3/267	10	with insulating elements formed in situ	E06B3/267	E06B3/267		618
E06B3/2675	11	{combined with prefabricated insulating elements}	E06B3/267	E06B3/267		533
E06B3/273	10	with prefabricated insulating elements held in position by deformation of portions of the {metal} frame members	E06B3/273	E06B3/273		277
E06B3/2735	11	{comprising a sheet metal member, an edge or which is bent over the edge of the other metal member with interposition of an insulating element}	E06B3/273	E06B3/273		42
E06B3/277	10	with prefabricated insulating elements held in position by expansion of the {extremities of the} insulating elements	E06B3/277	E06B3/277		70
E06B3/28	9	with additional removable glass panes or the like, framed or unframed	E06B3/28	E06B3/28		1044
E06B3/285	10	{flexible transparent foils without a proper frame fixed and sealed at a distance from the existing glass pane}	E06B3/28	E06B3/28		219
E06B3/30	8	Coverings, e.g. protecting against weather, for decorative purposes {(for door leaves E06B3/7001)}	E06B3/30	E06B3/30		1083
E06B3/301	9	{consisting of prefabricated profiled members or glass}	E06B3/30	E06B3/30		284
E06B3/302	10	{Covering wooden frames with metal or plastic profiled members}	E06B3/30	E06B3/30		800
E06B3/303	10	{Covering metal or plastic frames with wooden profiled members}	E06B3/30	E06B3/30		282
E06B3/304	11	{the frames consist of two metal section members with insulating zone in between}	E06B3/30	E06B3/30		15
E06B3/305	10	{Covering metal frames with plastic or metal profiled members}	E06B3/30	E06B3/30		491
E06B3/306	10	{Covering plastic frames with metal or plastic profiled members}	E06B3/30	E06B3/30		319
E06B3/307	10	{Coverings with special provisions for insulation, e.g. foam filled}	E06B3/30	E06B3/30		43
E06B3/308	9	{Wing frames covered on the outside by a rigidly-mounted outer frame}	E06B3/30	E06B3/30		563
E06B3/32	8	Arrangements of wings characterised by the manner of movement; Arrangements of movable wings in openings; Features of wings or frames relating solely to the manner of movement of the wing {(fittings or supporting means, separable from the frame, for guiding or controlling the movement of wings, arrangements of wings characterised by particular forms of such means E05D)}	E06B3/32	E06B3/32		256
E06B3/325	9	{Wings opening towards the outside}	E06B3/32	E06B3/32		286
E06B3/34	9	with only one kind of movement (E06B3/48 takes precedence)	E06B3/34	E06B3/34		426
E06B3/341	10	{Tilt-and-turn wings}	E06B3/34	E06B3/34		119
E06B2003/343	10	{with at least two axes of rotation without additional frame within the wing}	E06B3/34	E06B3/34		99
E06B2003/345	10	{with additional rotating frame within the wing}	E06B3/34	E06B3/34		4
E06B2003/346	11	{where the additional frame rotates around a vertical axis}	E06B3/34	E06B3/34		60
E06B2003/348	11	{where the additional frame rotates around a horizontal axis}	E06B3/34	E06B3/34		27
E06B3/36	10	with a single vertical axis of rotation at one side of the opening, or swinging through the opening (wings requiring lifting before opening E06B3/52)	E06B3/36	E06B3/36		2920
E06B3/362	11	{Double winged doors or windows}	E06B3/36	E06B3/36		1220
E06B3/365	12	{Astragals for double doors}	E06B3/36	E06B3/36		191
E06B3/367	11	{specially adapted for furniture}	E06B3/36	E06B3/36		596
E06B3/38	10	with a horizontal axis of rotation at the top or bottom of the opening {(E06B3/5036 takes precedence)}	E06B3/38	E06B3/38		1221
E06B3/385	11	{specially adapted for furniture}	E06B3/38	E06B3/38		285
E06B3/40	10	with a vertical or horizontal axis of rotation not at one side of the opening, e.g. turnover wings	E06B3/40	E06B3/40		894
E06B2003/403	11	{where the axis of rotation is horizontal}	E06B3/40	E06B3/40		118
E06B2003/406	11	{where the axis of rotation is vertical}	E06B3/40	E06B3/40		169
E06B3/42	10	Sliding wings; Details of frames with respect to guiding {(E06B3/26347 and E06B3/92 take precedence)}	E06B3/42	E06B3/42		265
E06B3/44	11	Vertically-sliding wings	E06B3/44	E06B3/44		3262
E06B3/4407	12	{Single-hung, i.e. having a single vertical sliding panel}	E06B3/44	E06B3/44		563
E06B3/4415	12	{Double-hung, i.e. with two vertical sliding panels}	E06B3/44	E06B3/44		168
E06B3/4423	12	{disappearing in a wall pocket; Pockets therefor}	E06B3/44	E06B3/44		215
E06B3/443	12	{specially adapted for furniture}	E06B3/44	E06B3/44		71
E06B2003/4438	12	{characterised by the material used for the frames}	E06B3/44	E06B3/44		2
E06B2003/4446	13	{Wood}	E06B3/44	E06B3/44		454
E06B2003/4453	13	{Metal}	E06B3/44	E06B3/44		594
E06B2003/4461	13	{Plastics}	E06B3/44	E06B3/44		112
E06B2003/4469	13	{with at least two frames made from different materials}	E06B3/44	E06B3/44		10
E06B2003/4476	12	{Coverings, e.g. for protecting against weather or for decorative purposes}	E06B3/44	E06B3/44		73
E06B2003/4484	12	{Special provisions for mounting or dismounting sashes}	E06B3/44	E06B3/44		12
E06B2003/4492	12	{provided with screens}	E06B3/44	E06B3/44		352
E06B3/46	11	Horizontally-sliding wings {(E06B3/487 takes precedence)}	E06B3/46	E06B3/46		1549
E06B3/4609	12	{for windows (E06B3/4654&#160;-&#160;E06B3/4681 take precedence)}	E06B3/46	E06B3/46		3323
E06B3/4618	13	{the sliding wing being arranged beside a fixed wing (E06B3/4627 takes precedence)}	E06B3/46	E06B3/46		469
E06B3/4627	13	{with the sliding wing flush closing or moving a considerable distance towards the opening when closing}	E06B3/46	E06B3/46		225
E06B3/4636	12	{for doors (E06B3/4609 and E06B3/4654&#160;-&#160;E06B3/4681 take precedence; sliding shower doors A47K3/34)}	E06B3/46	E06B3/46		3038
E06B3/4645	13	{with the sliding wing flush closing or moving a considerable distance towards the opening when closing}	E06B3/46	E06B3/46		243
E06B3/4654	12	{disappearing in pockets in the wall; Pockets therefor}	E06B3/46	E06B3/46		684
E06B3/4663	12	{specially adapted for furniture}	E06B3/46	E06B3/46		794
E06B3/4672	13	{with the sliding wing flush closing or moving a considerable distance towards the opening when closing}	E06B3/46	E06B3/46		134
E06B3/4681	12	{made of glass panes without frames (E06B3/4663 takes precedence)}	E06B3/46	E06B3/46		362
E06B3/469	12	{Arrangements at the overlapping vertical edges of the wings that engage when closing}	E06B3/46	E06B3/46		201
E06B3/48	9	Wings connected at their edges, e.g. foldable wings	E06B3/48	E06B3/48		657
E06B3/481	10	{Wings foldable in a zig-zag manner or bi-fold wings}	E06B3/48	E06B3/48		1636
E06B3/482	11	{specially adapted for furniture}	E06B3/48	E06B3/48		252
E06B3/483	11	{folding upwardly (E06B3/482 takes precedence)}	E06B3/48	E06B3/48		226
E06B3/485	10	{Sectional doors}	E06B3/48	E06B3/48		1206
E06B3/486	11	{with hinges being at least partially integral part of the section panels}	E06B3/48	E06B3/48		236
E06B3/487	11	{sliding laterally}	E06B3/48	E06B3/48		34
E06B3/488	11	{with horizontal strengthening means; anti-sag devices}	E06B3/48	E06B3/48		22
E06B3/50	9	with more than one kind of movement (E06B3/48 takes precedence){(E06B3/92 takes precedence)}	E06B3/50	E06B3/50		2688
E06B3/5009	10	{where the sliding and rotating movements are necessarily performed simultaneously (E06B3/5027, E06B3/5036 take precedence)}	E06B3/50	E06B3/50		375
E06B3/5018	11	{where the pivot axis slides during pivoting of the wing}	E06B3/50	E06B3/50		217
E06B3/5027	10	{"Austral" windows}	E06B3/50	E06B3/50		101
E06B3/5036	10	{Louvre type windows, e.g. windows made of movable strips of glass}	E06B3/50	E06B3/50		68
E06B3/5045	10	{specially adapted for furniture (E06B3/52 takes precedence)}	E06B3/50	E06B3/50		487
E06B3/5054	10	{where the sliding and rotating movements are independent of each other}	E06B3/50	E06B3/50		269
E06B3/5063	11	{the vertical sliding wings having the possibility of an additional rotational movement}	E06B3/50	E06B3/50		1528
E06B3/5072	11	{the horizontal sliding wings having the possibility of an additional rotational movement}	E06B3/50	E06B3/50		314
E06B3/5081	11	{at least two wings have a different kind of movement}	E06B3/50	E06B3/50		107
E06B3/509	10	{where one of the sliding and rotating movements necessarily precedes the other}	E06B3/50	E06B3/50		226
E06B3/52	10	Wings requiring lifting before opening	E06B3/52	E06B3/52		428
E06B3/54	8	Fixing of glass panes or like plates	E06B3/54	E06B3/54		774
E06B3/5409	9	{Means for locally spacing the pane from the surrounding frame}	E06B3/54	E06B3/54		684
E06B3/5418	9	{Permanently fixing of an additional unframed pane (compound frames E06B3/2605)}	E06B3/54	E06B3/54		218
E06B3/5427	9	{the panes mounted flush with the surrounding frame or with the surrounding panes (E06B3/5436 takes precedence; supporting structures for curtain walls E04B2/885)}	E06B3/54	E06B3/54		1046
E06B3/5436	9	{involving holes or indentations in the pane}	E06B3/54	E06B3/54		632
E06B3/5445	10	{Support arms engaging the holes or indentations}	E06B3/54	E06B3/54		211
E06B3/5454	9	{inside U-shaped section members}	E06B3/54	E06B3/54		943
E06B2003/5463	10	{in a preassembled frame, the pane being consecutively introduced obliquely, rotated and shifted}	E06B3/54	E06B3/54		85
E06B2003/5472	10	{in an at least partly preassembled frame by introducing it through a slot in one of the frame members or inserting the pane before completing the frame}	E06B3/54	E06B3/54		138
E06B3/5481	9	{by means of discrete fixing elements, e.g. glazing clips, glaziers points}	E06B3/54	E06B3/54		438
E06B3/549	9	{by clamping the pane between two subframes}	E06B3/54	E06B3/54		307
E06B3/56	9	by means of putty, cement, or adhesives only (E06B3/64{E06B3/5427} take precedence)	E06B3/56	E06B3/56		687
E06B3/58	9	by means of borders, cleats, or the like ({E06B3/30} , E06B3/64 take precedence)	E06B3/58	E06B3/58		951
E06B3/5807	10	{not adjustable}	E06B3/58	E06B3/58		228
E06B3/5814	11	{together with putty or fixed by glue}	E06B3/58	E06B3/58		174
E06B3/5821	11	{hooked on or in the frame member, fixed by clips or otherwise elastically fixed (E06B3/585 takes precedence)}	E06B3/58	E06B3/58		699
E06B3/5828	12	{on or with auxiliary pieces}	E06B3/58	E06B3/58		365
E06B3/5835	13	{together with parts of the border in the same undercut groove in the frame (E06B3/5842 takes precedence)}	E06B3/58	E06B3/58		93
E06B3/5842	11	{fixed by a tongue-and-groove or mortise-and-tenon connection substantially parallel to the pane}	E06B3/58	E06B3/58		224
E06B3/585	10	{adjustable, e.g. for accommodating panes of various thickness, or with provisions for altering the clamping force on the pane (E06B3/5871 takes precedence)}	E06B3/58	E06B3/58		160
E06B3/5857	11	{the fixing being adjustable, e.g. in one of several possible positions}	E06B3/58	E06B3/58		140
E06B3/5864	12	{with adjusting screws, wedges or cams}	E06B3/58	E06B3/58		204
E06B3/5871	10	{pivotally fixed on the frame; Borders with pivoting parts}	E06B3/58	E06B3/58		113
E06B3/5878	10	{the borders being pre-assembled in a frame-like manner on the pane or on the frame before the pane is fitted to the frame (E06B3/645 takes precedence)}	E06B3/58	E06B3/58		201
E06B3/5885	10	{Corner arrangements for borders; Devices for making rounded corners}	E06B3/58	E06B3/58		171
E06B3/5892	10	{Fixing of window panes in openings in door leaves}	E06B3/58	E06B3/58		944
E06B3/60	10	of clamping cleats of metal	E06B3/60	E06B3/60		520
E06B3/605	11	{made of sheet metal}	E06B3/60	E06B3/60		222
E06B3/62	10	of rubber-like elastic cleats	E06B3/62	E06B3/62		1161
E06B3/6202	11	{positioned between adjoining panes without separate glazing bar}	E06B3/62	E06B3/62		123
E06B3/6205	11	{having on at least one lateral side no backing from a separate rigid glazing bead or other stiff part of the window frame}	E06B3/62	E06B3/62		392
E06B2003/6208	11	{with adjustable dimensions}	E06B3/62	E06B3/62		100
E06B2003/6211	12	{with tear away strips}	E06B3/62	E06B3/62		36
E06B2003/6214	11	{specially adapted for glazing bars}	E06B3/62	E06B3/62		86
E06B2003/6217	11	{with specific fixing means}	E06B3/62	E06B3/62		28
E06B2003/622	12	{using nails or the like}	E06B3/62	E06B3/62		52
E06B2003/6223	12	{with protruding parts anchored in grooves}	E06B3/62	E06B3/62		555
E06B2003/6226	12	{with locking strips}	E06B3/62	E06B3/62		180
E06B2003/6229	12	{with grooves anchoring the cleat on a rim}	E06B3/62	E06B3/62		273
E06B2003/6232	12	{using glue}	E06B3/62	E06B3/62		113
E06B2003/6235	12	{moulded on the pane}	E06B3/62	E06B3/62		22
E06B2003/6238	11	{having extra functions}	E06B3/62	E06B3/62		30
E06B2003/6241	12	{with drainage means}	E06B3/62	E06B3/62		84
E06B2003/6244	12	{with extra parts sealing against the bottom of the glazing rebate or against the edge of the pane}	E06B3/62	E06B3/62		375
E06B2003/6247	12	{with extra parts sealing against the fixed or another window frame}	E06B3/62	E06B3/62		92
E06B2003/625	11	{Specific form characteristics}	E06B3/62	E06B3/62		46
E06B2003/6252	12	{wedge-shaped}	E06B3/62	E06B3/62		106
E06B2003/6255	12	{H-shaped}	E06B3/62	E06B3/62		8
E06B2003/6258	12	{U-shaped}	E06B3/62	E06B3/62		294
E06B2003/6261	12	{S-shaped}	E06B3/62	E06B3/62		60
E06B2003/6264	12	{hollow}	E06B3/62	E06B3/62		336
E06B2003/6267	12	{consisting of several separate parts}	E06B3/62	E06B3/62		85
E06B2003/627	11	{with specific characteristics concerning the material}	E06B3/62	E06B3/62		39
E06B2003/6273	12	{reinforced, e.g. against elongation}	E06B3/62	E06B3/62		107
E06B2003/6276	12	{with parts of differing nature, e.g. hardness}	E06B3/62	E06B3/62		278
E06B2003/6279	12	{with coverings or embellisher strips}	E06B3/62	E06B3/62		125
E06B2003/6282	12	{of cellular nature}	E06B3/62	E06B3/62		92
E06B2003/6285	12	{with provisions for receiving putty or pasty adhesives}	E06B3/62	E06B3/62		104
E06B2003/6288	12	{with fire resisting properties}	E06B3/62	E06B3/62		17
E06B2003/6291	11	{Corner arrangements}	E06B3/62	E06B3/62		159
E06B2003/6294	12	{using separate corner members}	E06B3/62	E06B3/62		42
E06B2003/6297	11	{for glazing panels of special shape, e.g. with undulating or U-shaped cross-section}	E06B3/62	E06B3/62		13
E06B3/64	9	Fixing of more than one pane to a frame<br><br><u>NOTE</u><br><br> Fixing of multiple glazing units to frames is classified in the relevant groups E06B3/5409&#160;-&#160;E06B3/62, except for the fixing thereof to frames designed for one pane only, which is classified in group E06B3/645	E06B3/64	E06B3/64		838
E06B3/645	10	{of units comprising two or more parallel panes to frames designed for single panes only, e.g. having too shallow a rabbet}	E06B3/64	E06B3/64		315
E06B3/66	8	Units comprising two or more parallel glass or like panes permanently secured together {(reforming and uniting glass sheets by fusing C03B23/00; joining glass to glass or to other materials C03C27/00; laminated glass B32B17/10)}	E06B3/66	E06B3/66		2267
E06B3/6604	9	{comprising false glazing bars or similar decorations between the panes (connectors therefor E06B3/6675)}	E06B3/66	E06B3/66		561
E06B3/6608	9	{without separate spacing elements (E06B3/6707 and E06B3/6715 take precedence)}	E06B3/66	E06B3/66		147
E06B3/6612	9	{Evacuated glazing units}	E06B3/66	E06B3/66		1276
E06B3/6617	9	{one of the panes being larger than another}	E06B3/66	E06B3/66		435
E06B3/6621	9	{with special provisions for fitting in window frames or to adjacent units; Separate edge protecting strips (E06B3/66347 takes precedence)}	E06B3/66	E06B3/66		654
E06B3/6625	10	{molded on the edges}	E06B3/66	E06B3/66		92
E06B3/663	9	Elements for spacing panes	E06B3/663	E06B3/663		616
E06B3/66304	10	{Discrete spacing elements, e.g. for evacuated glazing units}	E06B3/663	E06B3/663		643
E06B3/66309	10	{Section members positioned at the edges of the glazing unit}	E06B3/663	E06B3/663		391
E06B3/66314	11	{of tubular shape (E06B3/66323 and E06B3/66333 take precedence)}	E06B3/663	E06B3/663		377
E06B3/66319	12	{of rubber, plastics or similar materials}	E06B3/663	E06B3/663		232
E06B3/66323	11	{comprising an interruption of the heat flow in a direction perpendicular to the unit}	E06B3/663	E06B3/663		121
E06B3/66328	11	{of rubber, plastics or similar materials (E06B3/66314, E06B3/66323 and E06B3/66342 take precedence; transparent materials E06B3/66333)}	E06B3/663	E06B3/663		405
E06B3/66333	11	{of unusual substances, e.g. wood or other fibrous materials, glass or other transparent materials}	E06B3/663	E06B3/663		289
E06B2003/66338	12	{of glass}	E06B3/663	E06B3/663		161
E06B3/66342	11	{characterised by their sealed connection to the panes}	E06B3/663	E06B3/663		536
E06B3/66347	12	{with integral grooves or rabbets for holding the panes (E06B3/66366 takes precedence)}	E06B3/663	E06B3/663		207
E06B3/66352	12	{with separate sealing strips between the panes and the spacer}	E06B3/663	E06B3/663		176
E06B3/66357	12	{Soldered connections or the like}	E06B3/663	E06B3/663		147
E06B3/66361	11	{with special structural provisions for holding drying agents, e.g. packed in special containers}	E06B3/663	E06B3/663		288
E06B3/66366	11	{specially adapted for units comprising more than two panes or for attaching intermediate sheets}	E06B3/663	E06B3/663		368
E06B3/66371	11	{positioned entirely outside the gap between the panes}	E06B3/663	E06B3/663		29
E06B3/66376	11	{comprising lighting means}	E06B3/663	E06B3/663		89
E06B2003/6638	11	{with coatings}	E06B3/663	E06B3/663		276
E06B2003/66385	11	{with special shapes}	E06B3/663	E06B3/663		128
E06B2003/6639	11	{sinuous}	E06B3/663	E06B3/663		112
E06B2003/66395	11	{U-shape}	E06B3/663	E06B3/663		119
E06B3/667	10	Connectors therefor	E06B3/667	E06B3/667		840
E06B3/6675	11	{for connection between the spacing elements and false glazing bars}	E06B3/667	E06B3/667		175
E06B3/67	9	characterised by additional arrangements or devices for heat or sound insulation {or for controlled passage of light}	E06B3/67	E06B3/67		560
E06B3/6707	10	{specially adapted for increased acoustical insulation (doors, windows for insulation against noise E06B5/20)}	E06B3/67	E06B3/67		525
E06B3/6715	10	{specially adapted for increased thermal insulation or for controlled passage of light (E06B3/66323 takes precedence; coating of glass pains C03C17/00; devices or arrangements for controlling the intensity, colour, phase, polarisation or direction of light G02F1/00)}	E06B3/67	E06B3/67		1718
E06B3/6722	11	{with adjustable passage of light}	E06B3/67	E06B3/67		979
E06B3/673	9	Assembling the units (E06B3/677 takes precedence {; making hollow glass sheets or bricks C03B23/24})	E06B3/673	E06B3/673		449
E06B3/67304	10	{Preparing rigid spacer members before assembly}	E06B3/673	E06B3/673		110
E06B3/67308	11	{Making spacer frames, e.g. by bending or assembling straight sections (connectors E06B3/667)}	E06B3/673	E06B3/673		100
E06B3/67313	12	{by bending}	E06B3/673	E06B3/673		161
E06B3/67317	11	{Filling of hollow spacer elements with absorbants; Closing off the spacers thereafter}	E06B3/673	E06B3/673		107
E06B3/67321	11	{Covering spacer elements, e.g. with sealants}	E06B3/673	E06B3/673		127
E06B3/67326	10	{Assembling spacer elements with the panes}	E06B3/673	E06B3/673		300
E06B3/6733	11	{by applying, e.g. extruding, a ribbon of hardenable material on or between the panes}	E06B3/673	E06B3/673		268
E06B3/67334	11	{by soldering; Preparing the panes therefor}	E06B3/673	E06B3/673		155
E06B3/67339	10	{Working the edges of already assembled units}	E06B3/673	E06B3/673		94
E06B3/67343	11	{Filling or covering the edges with synthetic hardenable substances}	E06B3/673	E06B3/673		172
E06B3/67347	12	{by extrusion techniques}	E06B3/673	E06B3/673		112
E06B3/67352	12	{by forming techniques}	E06B3/673	E06B3/673		26
E06B3/67356	11	{Covering the edges with bands or profiles}	E06B3/673	E06B3/673		55
E06B3/6736	11	{Heat treatment (for soldering E06B3/67334)}	E06B3/673	E06B3/673		133
E06B3/67365	10	{Transporting or handling panes, spacer frames or units during assembly (E06B3/67304&#160;-&#160;E06B3/67339 take precedence)}	E06B3/673	E06B3/673		321
E06B3/67369	11	{Layout of the assembly streets}	E06B3/673	E06B3/673		151
E06B3/67373	11	{Rotating panes, spacer frames or units}	E06B3/673	E06B3/673		102
E06B2003/67378	11	{Apparatus travelling around the periphery of the pane or the unit}	E06B3/673	E06B3/673		125
E06B3/67382	11	{Transport of panes or units without touching the bottom edge}	E06B3/673	E06B3/673		57
E06B3/67386	11	{Presses; Clamping means holding the panes during assembly}	E06B3/673	E06B3/673		146
E06B3/67391	10	{Apparatus travelling around the periphery of the pane or the unit}	E06B3/673	E06B3/673		46
E06B2003/67395	10	{Non-planar units or of curvilinear outline, e.g. for vehicles}	E06B3/673	E06B3/673		59
E06B3/677	9	Evacuating or filling the gap between the panes {; Equilibration of inside and outside pressure}; Preventing condensation in the gap between the panes (by means of spacing elements E06B3/663); Cleaning the gap between the panes	E06B3/677	E06B3/677		1508
E06B3/6775	10	{Evacuating or filling the gap during assembly}	E06B3/677	E06B3/677		602
E06B3/68	8	Window bars {(bay windows E06B1/363; joints for frame members crossing each other E06B3/9628)}	E06B3/68	E06B3/68		781
E06B3/685	9	{False glazing bars (E06B3/6604 takes precedence)}	E06B3/68	E06B3/68		431
E06B3/70	8	Door leaves (wing frames E06B3/04)	E06B3/70	E06B3/70		2927
E06B3/7001	9	{Coverings therefor; Door leaves imitating traditional raised panel doors, e.g. engraved or embossed surfaces, with trim strips applied to the surfaces}	E06B3/70	E06B3/70		1896
E06B3/7003	9	{consisting of several adjacent similar elements, e.g. planks, without outer covering panels}	E06B3/70	E06B3/70		375
E06B3/7005	10	{without a separate supporting frame}	E06B3/70	E06B3/70		183
E06B3/7007	9	{Door leaves with curved, e.g. cylindrical or oval cross-section (E06B3/7001 takes precedence)}	E06B3/70	E06B3/70		202
E06B3/7009	9	{Door leaves with two similar parts placed one above the other, pivoting separately}	E06B3/70	E06B3/70		75
E06B2003/7011	9	{with easily replaceable or interchangeable panels}	E06B3/70	E06B3/70		248
E06B2003/7013	10	{put in place through a slot in the frame}	E06B3/70	E06B3/70		78
E06B3/7015	9	{characterised by the filling between two external panels (fireproof doors E06B5/16; noise insulating doors E06B5/20)}	E06B3/70	E06B3/70		1356
E06B3/7017	10	{of grating type}	E06B3/70	E06B3/70		392
E06B2003/7019	10	{of corrugated type}	E06B3/70	E06B3/70		105
E06B2003/7021	10	{consisting of wooden strips filling the whole door}	E06B3/70	E06B3/70		62
E06B2003/7023	10	{of foam type}	E06B3/70	E06B3/70		606
E06B2003/7025	10	{of cork; of wood or similar fibres}	E06B3/70	E06B3/70		181
E06B2003/7026	10	{of granular type}	E06B3/70	E06B3/70		44
E06B2003/7028	10	{of cementituous type, e.g. concrete}	E06B3/70	E06B3/70		147
E06B2003/703	10	{containing a metallic layer}	E06B3/70	E06B3/70		204
E06B2003/7032	10	{of non-vegetal fibrous material, e.g. glass or rock wool}	E06B3/70	E06B3/70		253
E06B2003/7034	11	{of asbestos}	E06B3/70	E06B3/70		63
E06B2003/7036	10	{of plaster}	E06B3/70	E06B3/70		87
E06B2003/7038	10	{made from a slurry}	E06B3/70	E06B3/70		43
E06B2003/704	10	{of mineral material which is not further specified}	E06B3/70	E06B3/70		81
E06B2003/7042	10	{with a fire retardant layer}	E06B3/70	E06B3/70		447
E06B2003/7044	9	{Garage doors}	E06B3/70	E06B3/70		380
E06B2003/7046	9	{with provisions for locks, hinges or other fittings}	E06B3/70	E06B3/70		728
E06B2003/7048	9	{with arcuate periphery; with openings having an arcuate periphery}	E06B3/70	E06B3/70		74
E06B2003/7049	9	{Specific panel characteristics}	E06B3/70	E06B3/70		666
E06B2003/7051	10	{of layered construction involving different materials}	E06B3/70	E06B3/70		819
E06B2003/7053	10	{corrugated}	E06B3/70	E06B3/70		80
E06B2003/7055	9	{Left-right hinged interchangeable door leaves}	E06B3/70	E06B3/70		60
E06B2003/7057	9	{with little passing through doors}	E06B3/70	E06B3/70		208
E06B2003/7059	9	{Specific frame characteristics}	E06B3/70	E06B3/70		206
E06B2003/7061	10	{Wooden frames}	E06B3/70	E06B3/70		121
E06B2003/7063	11	{reinforced; in combination with other materials, e.g. foam, honeycomb}	E06B3/70	E06B3/70		178
E06B2003/7065	11	{Wood fibres}	E06B3/70	E06B3/70		21
E06B2003/7067	11	{of layered construction}	E06B3/70	E06B3/70		105
E06B2003/7069	11	{with cladding}	E06B3/70	E06B3/70		42
E06B2003/7071	11	{made of a plurality of separate blocks or strips}	E06B3/70	E06B3/70		129
E06B2003/7073	11	{with fire retardant measures in frame}	E06B3/70	E06B3/70		82
E06B2003/7074	10	{Metal frames}	E06B3/70	E06B3/70		285
E06B2003/7076	11	{insulated}	E06B3/70	E06B3/70		124
E06B2003/7078	11	{with fire retardant measures in frame}	E06B3/70	E06B3/70		110
E06B2003/708	10	{insulated}	E06B3/70	E06B3/70		59
E06B2003/7082	10	{Plastic frames}	E06B3/70	E06B3/70		129
E06B2003/7084	11	{reinforced with metal or wood sections}	E06B3/70	E06B3/70		85
E06B2003/7086	10	{One-piece frames, e.g. made out of a single panel by cutting out a middle portion, moulded frames}	E06B3/70	E06B3/70		86
E06B2003/7088	10	{Two-piece frames made of a stile and an U-shaped part surrounding the panel}	E06B3/70	E06B3/70		18
E06B2003/709	10	{Frame parts being attached to both sides of the panel which extends till the door edge}	E06B3/70	E06B3/70		43
E06B2003/7092	10	{with frame members not directly or resiliently connected to each other}	E06B3/70	E06B3/70		31
E06B2003/7094	9	{with ventilated innerspace}	E06B3/70	E06B3/70		165
E06B2003/7096	9	{with possibilities to alter the extension of the door}	E06B3/70	E06B3/70		197
E06B2003/7098	9	{with bracing means crossing each other, e.g. diagonally disposed}	E06B3/70	E06B3/70		111
E06B3/72	9	consisting of frame and panels {, e.g. of raised panel type (E06B3/7001&#160;-&#160;E06B3/7015 and E06B3/82 take precedence)}	E06B3/72	E06B3/72		1336
E06B3/721	10	{with panels on one lateral side of the frame only}	E06B3/72	E06B3/72		229
E06B3/723	10	{at least one side of the frame consisting solely of a bent panel edge}	E06B3/72	E06B3/72		74
E06B3/725	10	{with separate hollow frames, e.g. foam-filled}	E06B3/72	E06B3/72		104
E06B3/726	11	{of metal}	E06B3/72	E06B3/72		146
E06B3/728	12	{of sheet metal}	E06B3/72	E06B3/72		158
E06B3/74	10	with wooden panels {or frame (E06B3/721, E06B3/725 and E06B3/76 take precedence)}	E06B3/74	E06B3/74		647
E06B3/76	10	with metal panels {(E06B3/721&#160;-&#160;E06B3/725 take precedence)}	E06B3/76	E06B3/76		353
E06B3/78	10	with panels of plastics {(E06B3/721&#160;-&#160;E06B3/725 take precedence)}	E06B3/78	E06B3/78		214
E06B3/80	9	flexible {(upwardly folding flexible screens E06B9/262)}	E06B3/80	E06B3/80		545
E06B3/805	10	{folding sideways (doors of the bellows type E06B3/94)}	E06B3/80	E06B3/80		82
E06B3/82	9	Flush doors, i.e. with completely flat surface (E06B3/02, {E06B3/7003 and E06B3/7015} take precedence)	E06B3/82	E06B3/82		207
E06B3/822	10	{with an internal foursided frame}	E06B3/82	E06B3/82		583
E06B3/825	11	{with a wooden frame}	E06B3/82	E06B3/82		431
E06B3/827	10	{of metal without an internal frame, e.g. with exterior panels substantially of metal}	E06B3/82	E06B3/82		469
E06B3/84	10	of plywood {or other wooden panels without an internal frame, e.g. with exterior panels substantially of wood}	E06B3/84	E06B3/84		99
E06B3/86	10	of plastics {without an internal frame, e.g. with exterior panels substantially of plastics}	E06B3/86	E06B3/86		152
E06B3/88	9	Edge-protecting devices for door leaves ({astragals for double doors E06B3/365} ; finger guards for doors or windows E06B7/36)	E06B3/88	E06B3/88		729
E06B3/90	8	Revolving doors; Cages or housings therefor (turnstiles E06B11/08)	E06B3/90	E06B3/90		816
E06B3/903	9	{consisting of arcuate wings revolving around a parallel axis situated outside the wing, e.g. a cylindrical wing revolving around its axis (E06B3/906 takes precedence)}	E06B3/90	E06B3/90		139
E06B3/906	9	{combining radially extending wings and separately movable arcuate wings}	E06B3/90	E06B3/90		53
E06B3/92	8	Doors or windows extensible when set in position (foldable wings E06B3/48; sliding wings for windows E06B3/42; wall-closing devices which may be rolled up, e.g. shutters, E06B9/11){(E06B3/01 takes precedence)}	E06B3/92	E06B3/92		197
E06B3/921	9	{with several parts mounted telescopically inside each other}	E06B3/92	E06B3/92		116
E06B3/922	9	{with several wings opening horizontally towards the same side of the opening and each closing a separate part of the opening (E06B3/921 and E06B3/928 take precedence)}	E06B3/92	E06B3/92		212
E06B3/924	10	{positioned in one plane when closed}	E06B3/92	E06B3/92		220
E06B3/925	9	{with several wings opening vertically towards the same side of the opening and each closing a separate part of the opening (E06B3/921 and E06B3/928 take precedence)}	E06B3/92	E06B3/92		105
E06B3/927	10	{positioned in one plane when closed}	E06B3/92	E06B3/92		60
E06B3/928	9	{Doors or windows of the lazy tongs type}	E06B3/92	E06B3/92		86
E06B3/94	9	Doors of the bellows type	E06B3/94	E06B3/94		317
E06B3/96	8	Corner joints or edge joints for windows, doors, or the like frames or wings {(E06B3/663 takes precedence)}	E06B3/96	E06B3/96		820
E06B3/9604	9	{Welded or soldered joints (E06B3/988, E06B3/99 take precedence; welding of plastics B29C65/00, soldering or welding of metals B23K)}	E06B3/96	E06B3/96		133
E06B3/9608	10	{Mitre joints}	E06B3/96	E06B3/96		359
E06B3/9612	9	{by filling in situ the hollow ends of the abutted frame members with a hardenable substance}	E06B3/96	E06B3/96		111
E06B3/9616	9	{characterised by the sealing at the junction of the frame members (E06B3/9632 takes precedence)}	E06B3/96	E06B3/96		226
E06B3/962	10	{Mitre joints}	E06B3/96	E06B3/96		100
E06B3/9624	9	{with means specially adapted for aligning the frontal surfaces of adjacent frame member ends}	E06B3/96	E06B3/96		105
E06B3/9628	9	{Mitre joints concealed to look like butt joints}	E06B3/96	E06B3/96		61
E06B3/9632	9	{between a jamb and the threshold or sill of window or door frames}	E06B3/96	E06B3/96		332
E06B3/9636	9	{for frame members having longitudinal screw receiving channels}	E06B3/96	E06B3/96		349
E06B3/964	9	using separate connection pieces, e.g. T-connection pieces (E06B3/9604&#160;-&#160;E06B3/9636 and E06B3/984&#160;-&#160;E06B3/99 take precedence)	E06B3/964	E06B3/964		715
E06B3/9641	10	{part of which remains visible (E06B3/9647 takes precedence)}	E06B3/964	E06B3/964		512
E06B3/9642	10	{Butt type joints with at least one frame member cut off square; T-shape joints (E06B3/9641, E06B3/9644, E06B3/9647, E06B3/9649, E06B3/968 take precedence)}	E06B3/964	E06B3/964		577
E06B3/9643	11	{for frame members being in one line with each other}	E06B3/964	E06B3/964		84
E06B3/9644	10	{L-shaped corner pieces having two articulated or flexible joined legs; Corner joints with variable angle}	E06B3/964	E06B3/964		238
E06B3/9645	10	{Mitre joints (E06B3/9641, E06B3/9644, E06B3/9647, E06B3/9649, E06B3/968 take precedence)}	E06B3/964	E06B3/964		263
E06B3/9646	11	{using two similar connecting pieces each connected with one or the frame members and drawn together at the joint}	E06B3/964	E06B3/964		175
E06B3/9647	10	{the connecting piece being part of or otherwise linked to the window or door fittings}	E06B3/964	E06B3/964		325
E06B3/9648	11	{Mitre joints}	E06B3/964	E06B3/964		219
E06B3/9649	10	{Tie rods spanning the whole width or height of the frame; Straps encircling the frame}	E06B3/964	E06B3/964		119
E06B3/968	10	characterised by the way the connecting pieces are fixed in or on the frame members	E06B3/968	E06B3/968		404
E06B3/9681	11	{by press fit or adhesion}	E06B3/968	E06B3/968		247
E06B3/9682	12	{Mitre joints}	E06B3/968	E06B3/968		396
E06B3/9684	11	{by hooking protrusions on the connecting piece in openings of the frame member, e.g. by snap-locking (E06B3/972, E06B3/976, E06B3/98 take precedence)}	E06B3/968	E06B3/968		123
E06B3/9685	12	{Mitre joints}	E06B3/968	E06B3/968		122
E06B3/9687	11	{with screws blocking the connecting piece inside or on the frame member (E06B3/972, E06B3/976 take precedence)}	E06B3/968	E06B3/968		529
E06B3/9688	12	{Mitre joints}	E06B3/968	E06B3/968		248
E06B3/972	11	by increasing the cross-section of the connecting pieces, e.g. by expanding the connecting pieces with wedges (E06B3/976 takes precedence)	E06B3/972	E06B3/972		139
E06B3/9725	12	{Mitre joints}	E06B3/972	E06B3/972		236
E06B3/976	11	by deformation of the frame members {(making sheet metal frames for openings B21D53/74)}	E06B3/976	E06B3/976		37
E06B3/9765	12	{Mitre joints}	E06B3/976	E06B3/976		130
E06B3/98	11	the connecting pieces being specially adapted for drawing the frame members towards each other (E06B3/9684, E06B3/972, E06B3/976 take precedence)	E06B3/98	E06B3/98		149
E06B3/982	12	{Mitre joints}	E06B3/98	E06B3/98		290
E06B3/984	9	specially adapted for frame members of wood or other material worked in a similar way (E06B3/99 takes precedence)	E06B3/984	E06B3/984		509
E06B3/9845	10	{Mitre joints}	E06B3/984	E06B3/984		284
E06B3/988	9	specially adapted for sheet metal frame members with an open U-shaped cross-section	E06B3/988	E06B3/988		255
E06B3/9885	10	{Mitre joints}	E06B3/988	E06B3/988		239
E06B3/99	9	for continuous frame members crossing each other with out interruption (window bars E06B3/68)	E06B3/99	E06B3/99		248
E06B5/00	7	Doors, windows, or like closures for special purposes {(insulated compound frames specially adapted for sliding doors or windows E06B3/26347)}; Border constructions therefor	E06B5/00	E06B5/00		1826
E06B5/003	8	{Storm doors; Combination-screen-and-storm-doors}	E06B5/00	E06B5/00		284
E06B5/006	8	{for furniture (E06B3/00, E06B9/115 take precedence)}	E06B5/00	E06B5/00		913
E06B5/01	8	Trap-doors	E06B5/01	E06B5/01		384
E06B5/02	8	for out-buildings or cellars; Other simple closures not designed to be close-fitting	E06B5/02	E06B5/02		331
E06B5/025	9	{Provisional closures, e.g. temporary security doors}	E06B5/02	E06B5/02		173
E06B5/04	9	with fixed wooden frames	E06B5/04	E06B5/04		7
E06B5/06	9	with fixed metal frames	E06B5/06	E06B5/06		49
E06B5/08	9	with fixed frames made of concrete, stone-like material or plastics	E06B5/08	E06B5/08		55
E06B5/10	8	for protection against air-raid or other war-like action; for other protective purposes	E06B5/10	E06B5/10		1882
E06B5/103	9	{safety foils therefor}	E06B5/10	E06B5/10		22
E06B5/106	9	{Frames for bullet-proof windows (transparent bullet-proof laminates F41H5/0407)}	E06B5/10	E06B5/10		211
E06B5/11	9	against burglary	E06B5/11	E06B5/11		2342
E06B5/113	10	{Arrangements at the edges of the wings, e.g. with door guards to prevent the insertion of prying tools (protection of the locking region by preventing insertion of a tool E05B17/2003; means to prevent forced opening by attack, tampering or jimmying of lock E05B17/2084; anti-tamper devices arranged on or near the hinges E05D11/0018)}	E06B5/11	E06B5/11		547
E06B5/116	10	{Arrangements preventing the removal of glazing panels}	E06B5/11	E06B5/11		165
E06B5/12	9	against air pressure, explosion, or gas	E06B5/12	E06B5/12		1148
E06B5/125	10	{Closures for relieving excess pressure inside the building}	E06B5/12	E06B5/12		98
E06B5/14	10	Gasproof doors or similar closures; Adaptation of fixed constructions therefor	E06B5/14	E06B5/14		367
E06B5/16	9	Fireproof doors or similar closures; Adaptations of fixed constructions therefor	E06B5/16	E06B5/16		4585
E06B5/161	10	{Profile members therefor}	E06B5/16	E06B5/16		1287
E06B5/162	10	{Fireproof doors having windows or other openings, e.g. for permitting ventilation or escape}	E06B5/16	E06B5/16		544
E06B5/164	10	{Sealing arrangements between the door or window and its frame, e.g. intumescent seals specially adapted therefor}	E06B5/16	E06B5/16		1772
E06B5/165	10	{Fireproof windows (layered glass panes with expansion layers for fire protection B32B17/10311)}	E06B5/16	E06B5/16		810
E06B5/167	10	{Devices blocking doors or windows inside its frame in case of fire}	E06B5/16	E06B5/16		187
E06B5/168	10	{Shape of edges of wing and/or its frame specially adapted therefor}	E06B5/16	E06B5/16		303
E06B5/18	9	against harmful radiation (against heat E06B5/16)	E06B5/18	E06B5/18		665
E06B5/20	8	for insulation against noise	E06B5/20	E06B5/20		2006
E06B5/205	9	{windows therefor}	E06B5/20	E06B5/20		769
E06B7/00	7	Special arrangements or measures in connection with doors or windows ({arrangements against burglary at the edges of the wings E06B5/113} ; screening or similar protective devices E06B9/00)	E06B7/00	E06B7/00		511
E06B7/02	8	for providing ventilation, e.g. through double windows; Arrangement of ventilation roses (airflow control members per seF24F13/08)	E06B7/02	E06B7/02		3412
E06B2007/023	9	{Air flow induced by fan}	E06B7/02	E06B7/02		973
E06B2007/026	9	{with air flow between panes}	E06B7/02	E06B7/02		361
E06B7/03	9	Ventilating devices for inserting under upwardly-sliding windows (rain or draught deflectors E06B7/26)	E06B7/03	E06B7/03		316
E06B7/04	9	with ventilation wings (E06B7/08 takes precedence)	E06B7/04	E06B7/04		310
E06B7/06	10	with one ventilation wing only	E06B7/06	E06B7/06		367
E06B7/08	9	Louvre doors, windows or grilles {(shutters E06B9/04; louvre awnings E04F10/08&#160;-&#160;E04F10/10)}	E06B7/08	E06B7/08		678
E06B7/082	10	with rigid or slidable lamellae	E06B7/082	E06B7/082		886
E06B7/084	10	with rotatable lamellae	E06B7/084	E06B7/084		1771
E06B7/086	11	interconnected for concurrent movement	E06B7/086	E06B7/086		1244
E06B7/088	12	with facing protective grille or safety guard	E06B7/088	E06B7/088		33
E06B7/09	12	mounted in movable wing, e.g. door	E06B7/09	E06B7/09		147
E06B7/092	12	operable in two or more distinct sets	E06B7/092	E06B7/092		62
E06B7/094	12	operable in sequence; characterised by additional independent movement	E06B7/094	E06B7/094		19
E06B7/096	12	operated or interconnected by gearing (wing operators with gearing in general E05F11/00)	E06B7/096	E06B7/096		263
E06B7/098	12	with weather seal	E06B7/098	E06B7/098		104
E06B7/10	9	by special construction of the frame members	E06B7/10	E06B7/10		1509
E06B7/12	8	Measures preventing the formation of condensed water (double glazing E06B3/24&#160;-&#160;E06B3/28{and E06B3/677} ; heating arrangements specially adapted for transparent or reflecting areas H05B3/84)	E06B7/12	E06B7/12		682
E06B7/14	8	Measures for draining-off condensed water or water leaking-in {frame members for draining off condensation water, throats at the bottom of a sash}	E06B7/14	E06B7/14		3055
E06B2007/145	9	{for glass fa&#231;ade, e.g. curtain wall}	E06B7/14	E06B7/14		113
E06B7/16	8	Sealing arrangements on wings or parts co-operating with the wings ({specially adapted for fireproof or similar closures E06B5/164; }E06B7/098 takes precedence {; fixed sealing joints E04B1/68; devices for fitting sealing strips E04F21/00})	E06B7/16	E06B7/16		3623
E06B7/18	9	by means of movable edgings, e.g. draught sealings additionally used for bolting {, e.g. by spring force or with operating lever}	E06B7/18	E06B7/18		1489
E06B7/20	10	automatically withdrawn when the wing is opened {, e.g. by means of magnetic attraction, a pin or an inclined surface, especially for sills}	E06B7/20	E06B7/20		1617
E06B2007/202	11	{Actuator connected to wing frame}	E06B7/20	E06B7/20		155
E06B7/205	11	with sealing strip mounted on sill	E06B7/205	E06B7/205		275
E06B7/21	11	with sealing strip movable in plane of wing	E06B7/21	E06B7/21		418
E06B7/215	11	with sealing strip being moved to a retracted position by elastic means, e.g. springs	E06B7/215	E06B7/215		666
E06B7/22	9	by means of elastic edgings, e.g. elastic rubber tubes; by means of resilient edgings, e.g. felt or plush strips, resilient metal strips (E06B7/18 takes precedence)	E06B7/22	E06B7/22		2429
E06B7/23	10	Plastic, sponge rubber, or like strips or tubes	E06B7/23	E06B7/23		2107
E06B7/2301	11	{without an integrally formed part for fixing the edging}	E06B7/23	E06B7/23		336
E06B7/2303	12	{hollow}	E06B7/23	E06B7/23		175
E06B7/2305	11	{with an integrally formed part for fixing the edging (E06B7/2316 takes precedence)}	E06B7/23	E06B7/23		588
E06B7/2307	12	{with a single sealing-line or -plane between the wing and the part co-operating with the wing}	E06B7/23	E06B7/23		519
E06B7/2309	13	{with a hollow sealing part}	E06B7/23	E06B7/23		822
E06B7/231	13	{with a solid sealing part}	E06B7/23	E06B7/23		845
E06B7/2312	12	{with two or more sealing-lines or -planes between the wing and part co-operating with the wing}	E06B7/23	E06B7/23		885
E06B7/2314	11	{characterised by the material}	E06B7/23	E06B7/23		1096
E06B7/2316	11	{used as a seal between the floor and the wing}	E06B7/23	E06B7/23		926
E06B7/2318	11	{by applying over- or under-pressure, e.g. inflatable (gasproof doors or windows E06B5/12; for vehicles B60J10/244)}	E06B7/23	E06B7/23		843
E06B7/232	10	Resilient strips of hard material, e.g. metal	E06B7/232	E06B7/232		734
E06B7/24	9	without separate sealing members, e.g. with labyrinth	E06B7/24	E06B7/24		167
E06B7/26	8	Rain or draught deflectors, e.g. under sliding wings {also protection against light for doors}	E06B7/26	E06B7/26		1401
E06B7/28	8	Other arrangements on doors or windows, e.g. door-plates, windows adapted to carry plants, hooks for window cleaners {(edge protecting devices for door leaves E06B3/88; special glazing; emergency glazing; double glazing E06B3/66)}	E06B7/28	E06B7/28		9875
E06B7/285	9	{Finger plates (escutcheons E05B15/02)}	E06B7/28	E06B7/28		62
E06B7/30	9	Peep-holes; Devices for speaking through; Doors having windows	E06B7/30	E06B7/30		1873
E06B2007/305	10	{Microphone}	E06B7/30	E06B7/30		61
E06B7/32	9	Serving doors; Passing-through doors {; Pet-doors}	E06B7/32	E06B7/32		1328
E06B7/34	9	Doors containing cupboards (cabinet constructions per seA47B)	E06B7/34	E06B7/34		182
E06B7/36	9	Finger guards {or other measures preventing harmful access between the door and the door frame (safety devices for doors in railway cars B61D19/026; for lift doors B66B13/26; detection of obstructions E05F15/40)}	E06B7/36	E06B7/36		1018
E06B7/362	10	{the gap between the door and the door frame at the hinge side being constructed in a way to remain too small or too wide to cause injury}	E06B7/36	E06B7/36		260
E06B2007/365	11	{Rounded shape at gap, e.g. cylindrical}	E06B7/36	E06B7/36		183
E06B7/367	10	{by covering the gap between the door and the door frame at the hinge side}	E06B7/36	E06B7/36		614
E06B9/00	7	Screening or protective devices for {wall or similar} openings, with or without operating or securing mechanisms; Closures of similar construction (E06B5/10 takes precedence; wings for doors or windows, connected at their edges, E06B3/48; additional indoor equipment of doors or windows, not forming part of the proper finishing work of a building, e.g. curtains, A47H; gratings as building elements E04C2/24; fastening means E05; operating-mechanisms for wings in general E05F)	E06B9/00	E06B9/00		1445
E06B2009/002	8	{Safety guards or gates}	E06B9/00	E06B9/00		914
E06B2009/005	8	{Storm panels; hurricane shutters}	E06B9/00	E06B9/00		453
E06B2009/007	8	{Flood panels}	E06B9/00	E06B9/00		1472
E06B9/01	8	Grilles fixed to walls, doors, or windows; Grilles moving with doors or windows; Walls formed as grilles, e.g. claustra {(emergency release of window grilles E05B65/1033; security bars for wings E05C19/003)}	E06B9/01	E06B9/01		1843
E06B2009/015	9	{Mounting details}	E06B9/01	E06B9/01		457
E06B9/02	8	Shutters, movable grilles, or other safety closing devices, e.g. against burglary (louvre windows or grilles E06B7/08; lamellar blinds E06B9/26)	E06B9/02	E06B9/02		2029
E06B9/04	9	of wing type, e.g. revolving or sliding {(trap doors; louvre doors or windows E06B7/08)}	E06B9/04	E06B9/04		2054
E06B9/06	9	collapsible or foldable, e.g. of the bellows or lazy-tongs type (bellows-type doors E06B3/94; roll-type grilles E06B9/18)	E06B9/06	E06B9/06		443
E06B9/0607	10	{comprising a plurality of similar rigid closing elements movable to a storage position}	E06B9/06	E06B9/06		35
E06B9/0615	11	{characterised by the closing elements}	E06B9/06	E06B9/06		36
E06B9/0623	12	{Grilles}	E06B9/06	E06B9/06		256
E06B9/063	12	{Bars or rods perpendicular to the closing direction}	E06B9/06	E06B9/06		402
E06B9/0638	12	{Slats or panels}	E06B9/06	E06B9/06		1117
E06B9/0646	11	{characterised by the relative arrangement of the closing elements in the stored position}	E06B9/06	E06B9/06		72
E06B9/0653	12	{stored side by side in the closing plane}	E06B9/06	E06B9/06		197
E06B9/0661	13	{Lazy tongue, pantograph or scissor-like systems in the plane of the opening}	E06B9/06	E06B9/06		313
E06B9/0669	12	{stored in a zig-zag arrangement}	E06B9/06	E06B9/06		514
E06B9/0676	12	{stored in a stacked configuration}	E06B9/06	E06B9/06		385
E06B2009/0684	12	{stored in a spiral like arrangement}	E06B9/06	E06B9/06		107
E06B9/0692	10	{comprising flexible sheets as closing screen}	E06B9/06	E06B9/06		296
E06B9/08	9	Roll-type closures (roller blinds E06B9/40; operating, guiding or securing devices or arrangements for roll-type closures E06B9/56; usable only as awnings E04F10/06)	E06B9/08	E06B9/08		1260
E06B9/11	10	Roller shutters	E06B9/11	E06B9/11		645
E06B9/115	11	{specially adapted for furniture}	E06B9/11	E06B9/11		697
E06B9/13	11	with closing members of one piece, e.g. of corrugated sheet metal	E06B9/13	E06B9/13		964
E06B2009/135	12	{Horizontal shutter reinforcements}	E06B9/13	E06B9/13		159
E06B9/15	11	with closing members formed of slats or the like	E06B9/15	E06B9/15		2648
E06B2009/1505	12	{Slat details}	E06B9/15	E06B9/15		326
E06B2009/1511	13	{Coatings}	E06B9/15	E06B9/15		117
E06B2009/1516	13	{Means to increase resistance against bending}	E06B9/15	E06B9/15		138
E06B2009/1522	13	{Sealing joint between adjacent slats}	E06B9/15	E06B9/15		138
E06B2009/1527	13	{Transparent slats or transparent sections in slats}	E06B9/15	E06B9/15		378
E06B2009/1533	12	{Slat connections}	E06B9/15	E06B9/15		195
E06B2009/1538	13	{Slats directly connected}	E06B9/15	E06B9/15		229
E06B2009/1544	14	{Engaging section has curved articulation surfaces}	E06B9/15	E06B9/15		261
E06B2009/155	13	{Slats connected by separate elements}	E06B9/15	E06B9/15		235
E06B2009/1555	14	{Flexible elements, e.g. tapes, strips, cords or chains}	E06B9/15	E06B9/15		156
E06B2009/1561	15	{Strips}	E06B9/15	E06B9/15		79
E06B2009/1566	14	{Rigid elements, e.g. hinges, hooks or profiles}	E06B9/15	E06B9/15		231
E06B2009/1572	13	{Locking means to prevent slat disengagement}	E06B9/15	E06B9/15		182
E06B2009/1577	12	{Slat end pieces used for guiding shutter}	E06B9/15	E06B9/15		223
E06B2009/1583	13	{inserted in slat cavity}	E06B9/15	E06B9/15		339
E06B2009/1588	13	{inserted in engaging section of adjacent slats}	E06B9/15	E06B9/15		90
E06B2009/1594	13	{attached to outer surface of slat}	E06B9/15	E06B9/15		146
E06B9/165	12	with slats disappearing in each other; with slats the distance between which can be altered	E06B9/165	E06B9/165		725
E06B9/17	11	Parts or details of roller shutters, e.g. suspension devices, shutter boxes, wicket doors, ventilation openings	E06B9/17	E06B9/17		1605
E06B9/17007	12	{Shutter boxes; Details or component parts thereof}	E06B9/17	E06B9/17		1273
E06B9/17015	13	{made of at most two pieces; Front opening details}	E06B9/17	E06B9/17		385
E06B9/17023	13	{made of more than two pieces}	E06B9/17	E06B9/17		285
E06B9/1703	13	{Fixing of the box; External plastering of the box}	E06B9/17	E06B9/17		489
E06B2009/17038	12	{Shutter cleaning arrangements}	E06B9/17	E06B9/17		43
E06B9/17046	12	{Bottom bars}	E06B9/17	E06B9/17		428
E06B2009/17053	12	{Door in shutter screen; wicket door}	E06B9/17	E06B9/17		122
E06B9/17061	12	{Connection of the box to the guides}	E06B9/17	E06B9/17		342
E06B2009/17069	12	{Insulation}	E06B9/17	E06B9/17		557
E06B9/17076	12	{Sealing or antirattling arrangements}	E06B9/17	E06B9/17		535
E06B2009/17084	13	{closing outlet slot of shutter box}	E06B9/17	E06B9/17		64
E06B2009/17092	12	{Manufacturing}	E06B9/17	E06B9/17		124
E06B9/171	12	Rollers therefor; Fastening roller shutters to rollers	E06B9/171	E06B9/171		437
E06B2009/1713	13	{Telescopic rollers}	E06B9/171	E06B9/171		35
E06B2009/1716	13	{Arrangements to improve rolling of the shutter on the roller}	E06B9/171	E06B9/171		84
E06B9/172	13	by clamping bars	E06B9/172	E06B9/172		31
E06B9/173	13	by clasps or buttons	E06B9/173	E06B9/173		40
E06B9/174	12	Bearings specially adapted therefor	E06B9/174	E06B9/174		821
E06B2009/1743	13	{allowing radial roller movement}	E06B9/174	E06B9/174		92
E06B2009/1746	13	{Axial connection of rollers}	E06B9/174	E06B9/174		149
E06B9/18	10	Roll-type grilles	E06B9/18	E06B9/18		324
E06B9/24	8	Screens or other constructions affording protection against light, especially against sunshine; Similar screens for privacy or appearance; {Slat blinds}(operating, guiding or securing devices or arrangements for roll-type closures E06B9/56; free-hanging flexible screens A47H23/00)	E06B9/24	E06B9/24		4655
E06B2009/2405	9	{Areas of differing opacity for light transmission control}	E06B9/24	E06B9/24		582
E06B2009/2411	9	{Coloured fluid flow for light transmission control}	E06B9/24	E06B9/24		202
E06B2009/2417	9	{Light path control; means to control reflection}	E06B9/24	E06B9/24		1012
E06B2009/2423	9	{Combinations of at least two screens}	E06B9/24	E06B9/24		113
E06B2009/2429	10	{One vertical sheet and slats}	E06B9/24	E06B9/24		82
E06B2009/2435	10	{Two vertical sheets and slats in-between}	E06B9/24	E06B9/24		134
E06B2009/2441	10	{Screens joined one below the other}	E06B9/24	E06B9/24		165
E06B2009/2447	10	{Parallel screens}	E06B9/24	E06B9/24		124
E06B2009/2452	11	{moving independently}	E06B9/24	E06B9/24		405
E06B2009/2458	11	{moving simultaneously}	E06B9/24	E06B9/24		216
E06B2009/2464	9	{featuring transparency control by applying voltage, e.g. LCD, electrochromic panels}	E06B9/24	E06B9/24		1341
E06B2009/247	9	{Electrically powered illumination}	E06B9/24	E06B9/24		236
E06B2009/2476	9	{Solar cells}	E06B9/24	E06B9/24		737
E06B2009/2482	9	{Special shape}	E06B9/24	E06B9/24		113
E06B2009/2488	10	{Curved perimeter}	E06B9/24	E06B9/24		166
E06B2009/2494	10	{Trapezoidal or triangular}	E06B9/24	E06B9/24		182
E06B9/26	9	Lamellar or like blinds, e.g. venetian blinds {(for vehicles B60J1/2088)}	E06B9/26	E06B9/26		419
E06B9/262	10	with flexibly-interconnected horizontal or vertical strips; Concertina blinds {, i.e. upwardly folding flexible screens}	E06B9/262	E06B9/262		2619
E06B2009/2622	11	{Gathered vertically; Roman, Austrian or festoon blinds}	E06B9/262	E06B9/262		912
E06B2009/2625	11	{Pleated screens, e.g. concertina- or accordion-like}	E06B9/262	E06B9/262		970
E06B2009/2627	11	{Cellular screens, e.g. box or honeycomb-like}	E06B9/262	E06B9/262		631
E06B9/264	10	Combinations of lamellar blinds with roller shutters, screen windows, windows, or double panes; Lamellar blinds with special devices	E06B9/264	E06B9/264		2186
E06B2009/2643	11	{Screens between double windows}	E06B9/264	E06B9/264		673
E06B2009/2646	12	{Magnetic screen operator}	E06B9/264	E06B9/264		204
E06B9/266	10	Devices or accessories for making or mounting lamellar blinds or parts thereof {(cleaning of lamellar blinds A47L4/00; joining plastics plates for making venetian blinds B29C66/437)}	E06B9/266	E06B9/266		908
E06B9/28	10	with horizontal lamellae, e.g. non-liftable (louvre windows or gratings E06B7/08)	E06B9/28	E06B9/28		883
E06B2009/285	11	{Means for actuating a rod (being tilt rod or lift rod)}	E06B9/28	E06B9/28		409
E06B9/30	11	liftable	E06B9/30	E06B9/30		545
E06B9/302	12	without ladder-tape, e.g. with lazy-tongs, with screw spindle	E06B9/302	E06B9/302		303
E06B9/303	12	with ladder-tape	E06B9/303	E06B9/303		682
E06B9/304	13	with tilting bar and separate raising shaft	E06B9/304	E06B9/304		106
E06B9/305	13	with tilting bar and raising cords guided along fixed bar	E06B9/305	E06B9/305		243
E06B9/306	13	with tilting bar along which the raising cords are guided	E06B9/306	E06B9/306		78
E06B9/307	13	Details of tilting bars and their operation	E06B9/307	E06B9/307		578
E06B9/308	13	with coaxial tilting bar and raising shaft	E06B9/308	E06B9/308		242
E06B9/32	12	Operating, guiding, or securing devices therefor (operation of tilting bars E06B9/307)	E06B9/32	E06B9/32		1516
E06B9/322	13	Details of operating devices, e.g. pulleys, brakes, spring drums, drives ({operating devices E06B9/68} ; devices of general interest specially adapted or mounted for storing and repeatedly paying-out and re-storing lengths of material B65H75/34)	E06B9/322	E06B9/322		2719
E06B2009/3222	14	{Cordless, i.e. user interface without cords}	E06B9/322	E06B9/322		673
E06B2009/3225	14	{Arrangements to aid the winding of cords rollers}	E06B9/322	E06B9/322		271
E06B2009/3227	15	{Axially moving rollers}	E06B9/322	E06B9/322		97
E06B9/323	13	Structure or support of upper box	E06B9/323	E06B9/323		1198
E06B9/324	13	Cord-locks {(cord-locks for curtains A47H3/00)}	E06B9/324	E06B9/324		561
E06B9/325	13	Immobilising devices preventing raising	E06B9/325	E06B9/325		127
E06B9/326	13	Details of cords, e.g. buckles, drawing knobs	E06B9/326	E06B9/326		802
E06B2009/3265	14	{Emergency release to prevent strangulation or excessive load}	E06B9/326	E06B9/326		247
E06B9/327	13	Guides for raisable lamellar blinds with horizontal lamellae	E06B9/327	E06B9/327		649
E06B9/34	11	roller-type; {Roller shutters with adjustable lamellae}	E06B9/34	E06B9/34		711
E06B9/36	10	with vertical lamellae {; Supporting rails therefor}	E06B9/36	E06B9/36		1094
E06B9/361	11	{Transmissions located at the end of the supporting rail}	E06B9/36	E06B9/36		175
E06B9/362	11	{Travellers; Lamellae suspension stems}	E06B9/36	E06B9/36		290
E06B9/364	12	{Operating mechanisms therein}	E06B9/36	E06B9/36		271
E06B9/365	12	{Distance pieces therefor}	E06B9/36	E06B9/36		99
E06B9/367	11	{Lamellae suspensions (E06B9/362 takes precedence); Bottom weights; Bottom guides}	E06B9/36	E06B9/36		422
E06B9/368	11	{Driving means other than pulling cords}	E06B9/36	E06B9/36		350
E06B9/38	10	Other details	E06B9/38	E06B9/38		948
E06B9/382	11	Details of ladder-tapes or ladder chains, e.g. buckles for local shortening of tapes	E06B9/382	E06B9/382		324
E06B9/384	11	Details of interconnection or interaction of tapes and lamellae	E06B9/384	E06B9/384		530
E06B9/386	11	Details of lamellae	E06B9/386	E06B9/386		2140
E06B9/388	11	Details of bottom or upper slats or their attachment	E06B9/388	E06B9/388		517
E06B9/40	9	Roller blinds (usable only as awnings E04F10/06)	E06B9/40	E06B9/40		3109
E06B2009/402	10	{adjustable without the use of tools or cutting instruments}	E06B9/40	E06B9/40		60
E06B2009/405	10	{Two rollers}	E06B9/40	E06B9/40		406
E06B2009/407	10	{Telescopic roller}	E06B9/40	E06B9/40		97
E06B9/42	10	Parts or details of roller blinds, e.g. suspension devices, blind boxes (brackets or adjustable mountings for roller blinds and drawable curtains A47H1/13)	E06B9/42	E06B9/42		4685
E06B2009/425	11	{Pull chain or cord attached to bottom edge of screen}	E06B9/42	E06B9/42		131
E06B9/44	11	Rollers therefor; Fastening roller blinds to rollers	E06B9/44	E06B9/44		1040
E06B2009/445	12	{by adhesive}	E06B9/44	E06B9/44		53
E06B9/46	12	by clamping bars	E06B9/46	E06B9/46		183
E06B9/48	12	by clasps or buttons	E06B9/48	E06B9/48		86
E06B9/50	11	Bearings specially adapted therefor	E06B9/50	E06B9/50		2298
E06B9/52	8	Devices affording protection against insects, e.g. fly screens; Mesh windows for other purposes {(screens A47G5/00)}	E06B9/52	E06B9/52		6252
E06B9/521	9	{Frameless fly screens; Tensioning means therefor (E06B9/54 takes precedence)}	E06B9/52	E06B9/52		527
E06B9/522	9	{Dimensionally adjustable fly screens (E06B9/54 and E06B9/521 take precedence)}	E06B9/52	E06B9/52		490
E06B2009/524	9	{Mesh details}	E06B9/52	E06B9/52		492
E06B2009/525	9	{Patches for mesh repair or decoration}	E06B9/52	E06B9/52		55
E06B2009/527	9	{Mounting of screens to window or door}	E06B9/52	E06B9/52		1719
E06B2009/528	9	{Screens extending between movable wing and fixed frame of window or door}	E06B9/52	E06B9/52		316
E06B9/54	9	Roller fly screens (operating, guiding or securing devices therefor E06B9/56)	E06B9/54	E06B9/54		2473
E06B2009/543	10	{Horizontally moving screens}	E06B9/54	E06B9/54		534
E06B2009/546	10	{connected to end- or bottom-bar of roller shutter}	E06B9/54	E06B9/54		93
E06B9/56	8	Operating, guiding or securing devices or arrangements for roll-type closures; Spring drums; Tape drums; Counterweighting arrangements therefor (devices of general interest specially adapted or mounted for storing and repeatedly paying-out and re-storing lengths of material B65H75/34)	E06B9/56	E06B9/56		1166
E06B9/58	9	Guiding devices	E06B9/58	E06B9/58		2568
E06B9/581	10	{Means to prevent or induce disengagement of shutter from side rails}	E06B9/58	E06B9/58		1241
E06B9/582	10	{Means to increase gliss, light, sound or thermal insulation}	E06B9/58	E06B9/58		637
E06B2009/583	10	{Cords or cables}	E06B9/58	E06B9/58		278
E06B2009/585	10	{Emergency release to prevent damage of shutter or guiding device}	E06B9/58	E06B9/58		173
E06B2009/586	10	{with heating to prevent frost or condensate}	E06B9/58	E06B9/58		25
E06B2009/587	10	{Mounting of guiding devices to supporting structure}	E06B9/58	E06B9/58		383
E06B2009/588	10	{Sealings for guides}	E06B9/58	E06B9/58		214
E06B9/60	9	Spring drums operated only by closure members	E06B9/60	E06B9/60		1314
E06B9/62	9	Counterweighting arrangements (E06B9/60 takes precedence)	E06B9/62	E06B9/62		514
E06B9/64	9	with lowerable roller	E06B9/64	E06B9/64		457
E06B9/66	9	with a roller situated at the bottom	E06B9/66	E06B9/66		225
E06B9/68	9	Operating devices or mechanisms, e.g. with electric drive	E06B9/68	E06B9/68		3453
E06B2009/6809	10	{Control}	E06B9/68	E06B9/68		773
E06B2009/6818	11	{using sensors}	E06B9/68	E06B9/68		760
E06B2009/6827	12	{sensing light}	E06B9/68	E06B9/68		458
E06B2009/6836	12	{sensing obstacle}	E06B9/68	E06B9/68		301
E06B2009/6845	12	{sensing position}	E06B9/68	E06B9/68		289
E06B2009/6854	12	{sensing torque}	E06B9/68	E06B9/68		155
E06B2009/6863	12	{sensing wind speed}	E06B9/68	E06B9/68		109
E06B2009/6872	11	{using counters to determine shutter position}	E06B9/68	E06B9/68		191
E06B2009/6881	12	{Mechanical counters}	E06B9/68	E06B9/68		251
E06B2009/689	11	{using end switches}	E06B9/68	E06B9/68		117
E06B9/70	10	comprising an electric motor positioned outside the roller	E06B9/70	E06B9/70		1545
E06B9/72	10	comprising an electric motor positioned inside the roller	E06B9/72	E06B9/72		1173
E06B2009/725	11	{with epicyclic or planetary gear train}	E06B9/72	E06B9/72		136
E06B9/74	10	adapted for selective electrical or manual operation	E06B9/74	E06B9/74		501
E06B9/76	10	using crank handles	E06B9/76	E06B9/76		460
E06B9/78	9	for direct manual operation, e.g. by tassels, by handles	E06B9/78	E06B9/78		1850
E06B2009/785	10	{by belts, straps, bands, tapes, cords, tassels}	E06B9/78	E06B9/78		785
E06B9/80	9	Safety measures against dropping or unauthorised opening; Braking or immobilising devices; Devices for limiting unrolling (securing devices or arrangements for direct manual operation E06B9/78)	E06B9/80	E06B9/80		1392
E06B2009/801	10	{Locking arrangements}	E06B9/80	E06B9/80		421
E06B2009/802	11	{located in or close to shutter box}	E06B9/80	E06B9/80		200
E06B2009/804	11	{acting directly on the shutter}	E06B9/80	E06B9/80		158
E06B2009/805	11	{located on or in the guides}	E06B9/80	E06B9/80		360
E06B2009/807	10	{Brakes preventing fast screen movement}	E06B9/80	E06B9/80		224
E06B2009/808	11	{Fluid brakes}	E06B9/80	E06B9/80		77
E06B9/82	10	automatic	E06B9/82	E06B9/82		539
E06B9/84	11	against dropping	E06B9/84	E06B9/84		597
E06B9/86	11	against unauthorised opening	E06B9/86	E06B9/86		927
E06B9/88	11	for limiting unrolling	E06B9/88	E06B9/88		813
E06B2009/885	12	{Braking mechanism activated by the bottom bar}	E06B9/88	E06B9/88		117
E06B9/90	11	for immobilising the closure member in various chosen positions	E06B9/90	E06B9/90		893
E06B2009/905	12	{using wrap spring clutches}	E06B9/90	E06B9/90		150
E06B9/92	9	Means allowing the closures to be shifted out of the plane of the opening	E06B9/92	E06B9/92		470
E06B11/00	7	Means for allowing passage through fences, barriers or the like, e.g. stiles (general features of doors E06B1/00&#160;-&#160;E06B9/00; {cattle grids A01K3/002; features peculiar to electrified wire fencing A01K3/005})	E06B11/00	E06B11/00		195
E06B11/02	8	Gates; Doors	E06B11/02	E06B11/02		1858
E06B11/021	9	{Wire gates, e.g. traction gates; Fastenings therefor (insulators, poles, handles, or the like, in electric fences H01B17/145)}	E06B11/02	E06B11/02		201
E06B11/022	9	{characterised by the manner of movement}	E06B11/02	E06B11/02		282
E06B11/023	10	{where the gate opens within the plane of the gate}	E06B11/02	E06B11/02		86
E06B11/025	11	{vertically}	E06B11/02	E06B11/02		161
E06B11/026	11	{horizontally}	E06B11/02	E06B11/02		356
E06B11/027	10	{where the gate rotates around a horizontal axis parallel to the plane of the gate}	E06B11/02	E06B11/02		124
E06B11/028	9	{with posts connected underground}	E06B11/02	E06B11/02		70
E06B11/04	9	characterised by the kind of suspension (suspensions per seE05D)	E06B11/04	E06B11/04		1092
E06B11/045	10	{exclusively for horizontally sliding gates}	E06B11/04	E06B11/04		394
E06B11/08	8	Turnstiles; {Gates for control of entry or exit of persons, e.g. in supermarkets}(control gates on vehicles B60N5/00{; bank protection devices E05G5/00}; with registering means G07C9/10{; coin-freed facilities for turnstiles G07F17/14})	E06B11/08	E06B11/08		579
E06B11/085	9	{non-rotary or with a limited angle of rotation, e.g. 90&#176;}	E06B11/08	E06B11/08		435
