B62D1/00	7	Steering controls, i.e. means for initiating a change of direction of the vehicle	B62D1/00	B62D1/00		478
B62D1/02	8	vehicle-mounted	B62D1/02	B62D1/02		486
B62D1/04	9	Hand wheels	B62D1/04	B62D1/04		3466
B62D1/043	10	{with a device allowing single-hand operation of the steering wheel}	B62D1/04	B62D1/04		452
B62D1/046	10	{Adaptations on rotatable parts of the steering wheel for accommodation of switches}	B62D1/04	B62D1/04		1968
B62D1/06	10	Rims, e.g. with heating means; Rim covers (B62D1/11 takes precedence)	B62D1/06	B62D1/06		2701
B62D1/065	11	{Steering wheels with heating and ventilating means (heating and ventilation of steering wheel when connected to vehicle HVAC B60H1/00292)}	B62D1/06	B62D1/06		1017
B62D1/08	10	Spokes, e.g. resilient (B62D1/11 takes precedence)	B62D1/08	B62D1/08		608
B62D1/10	10	Hubs; Connecting hubs to steering columns, e.g. adjustable (B62D1/11 takes precedence)	B62D1/10	B62D1/10		1135
B62D1/105	11	{Non-rotatable hubs, e.g. the central part of the steering wheel not rotating}	B62D1/10	B62D1/10		385
B62D1/11	10	incorporating energy-absorbing arrangements, e.g. by being yieldable or collapsible (padded linings associated with the steering wheel B60R21/05; shock absorbers using plastic deformation of members in general F16F7/12)	B62D1/11	B62D1/11		648
B62D1/12	9	Hand levers	B62D1/12	B62D1/12		530
B62D1/14	10	Tillers, i.e. hand levers operating on steering columns	B62D1/14	B62D1/14		255
B62D1/16	9	Steering columns	B62D1/16	B62D1/16		3167
B62D1/163	10	{Part of the steering column replaced by flexible means, e.g. cable or belt}	B62D1/16	B62D1/16		170
B62D1/166	10	{Means changing the transfer ratio between steering wheel and steering gear}	B62D1/16	B62D1/16		140
B62D1/18	10	yieldable or adjustable, e.g. tiltable (padded linings associated with the steering column B60R21/05)<br><br><u>NOTE</u><br><br> Group B62D1/181 takes precedence over groups B62D1/183 - B62D1/187. 	B62D1/18	B62D1/18		770
B62D1/181	11	with power actuated adjustment, e.g. with position memory	B62D1/181	B62D1/181		1293
B62D1/183	11	adjustable between in-use and out-of-use positions, e.g. to improve access	B62D1/183	B62D1/183		651
B62D1/184	11	Mechanisms for locking columns at selected positions	B62D1/184	B62D1/184		2426
B62D1/185	11	adjustable by axial displacement, e.g. telescopically (B62D1/183, B62D1/187, B62D1/19 take precedence)	B62D1/185	B62D1/185		1502
B62D1/187	11	with tilt adjustment; with tilt and axial adjustment (B62D1/183, B62D1/19 takes precedence)	B62D1/187	B62D1/187		1423
B62D1/189	12	the entire column being tiltable as a unit	B62D1/189	B62D1/189		374
B62D1/19	11	incorporating energy-absorbing arrangements, e.g. by being yieldable or collapsible (shock absorbers using plastic deformation of members in general F16F7/12)	B62D1/19	B62D1/19		987
B62D1/192	12	{Yieldable or collapsible columns}	B62D1/19	B62D1/19		1780
B62D1/195	12	{Yieldable supports for the steering column}	B62D1/19	B62D1/19		1277
B62D1/197	12	{incorporating devices for preventing ingress of the steering column into the passengers space in case of accident}	B62D1/19	B62D1/19		466
B62D1/20	10	Connecting steering column to steering gear	B62D1/20	B62D1/20		1043
B62D1/22	9	Alternative steering-control elements, e.g. for teaching purposes	B62D1/22	B62D1/22		492
B62D1/24	8	not vehicle-mounted	B62D1/24	B62D1/24		187
B62D1/26	9	mechanical, e.g. by a non-load-bearing guide (railways B61)	B62D1/26	B62D1/26		363
B62D1/265	10	{especially adapted for guiding road vehicles carrying loads or passengers, e.g. in urban networks for public transportation}	B62D1/26	B62D1/26		421
B62D1/28	9	non-mechanical {, e.g. following a line or other known markers}	B62D1/28	B62D1/28		645
B62D1/283	10	{for unmanned vehicles}	B62D1/28	B62D1/28		156
B62D1/286	10	{Systems for interrupting non-mechanical steering due to driver intervention}	B62D1/28	B62D1/28		420
B62D3/00	7	Steering gears (power assisted or power driven B62D5/00; steering linkages B62D7/00; for non-deflectable wheels B62D11/00; gearing in general F16H)	B62D3/00	B62D3/00		263
B62D3/02	8	mechanical	B62D3/02	B62D3/02		1632
B62D3/04	9	of worm type	B62D3/04	B62D3/04		495
B62D3/06	10	with screw and nut	B62D3/06	B62D3/06		422
B62D3/08	11	using intermediate balls or the like	B62D3/08	B62D3/08		354
B62D3/10	10	with worm engaging in sector or roller gear	B62D3/10	B62D3/10		337
B62D3/12	9	of rack-and-pinion type	B62D3/12	B62D3/12		2827
B62D3/123	10	{characterised by pressure yokes}	B62D3/12	B62D3/12		874
B62D3/126	10	{characterised by the rack}	B62D3/12	B62D3/12		677
B62D3/14	8	hydraulic	B62D3/14	B62D3/14		246
B62D5/00	7	Power-assisted or power-driven steering (for non-deflectable wheels B62D11/00; fluid-pressure servomotors in general F15B)	B62D5/00	B62D5/00		375
B62D5/001	8	{Mechanical components or aspects of steer-by-wire systems, not otherwise provided for in this maingroup}	B62D5/00	B62D5/00		1051
B62D5/003	9	{Backup systems, e.g. for manual steering (B62D5/30 takes precedence)}	B62D5/00	B62D5/00		643
B62D5/005	9	{means for generating torque on steering wheel or input member, e.g. feedback}	B62D5/00	B62D5/00		483
B62D5/006	10	{power actuated}	B62D5/00	B62D5/00		1115
B62D5/008	8	{Changing the transfer ratio between the steering wheel and the steering gear by variable supply of energy, e.g. by using a superposition gear}	B62D5/00	B62D5/00		946
B62D5/02	8	mechanical, e.g. using a power-take-off mechanism for taking power from a rotating shaft of the vehicle and applying it to the steering gear	B62D5/02	B62D5/02		241
B62D5/04	8	electrical, e.g. using an electric servo-motor connected to, or forming part of, the steering gear	B62D5/04	B62D5/04		3215
B62D5/0403	9	{characterised by constructional features, e.g. common housing for motor and gear box}	B62D5/04	B62D5/04		1692
B62D5/0406	10	{including housing for electronic control unit}	B62D5/04	B62D5/04		790
B62D5/0409	9	{Electric motor acting on the steering column}	B62D5/04	B62D5/04		1662
B62D5/0412	10	{the axes of motor and steering column being parallel}	B62D5/04	B62D5/04		237
B62D5/0415	11	{the axes being coaxial}	B62D5/04	B62D5/04		201
B62D5/0418	9	{Electric motor acting on road wheel carriers}	B62D5/04	B62D5/04		1108
B62D5/0421	9	{Electric motor acting on or near steering gear}	B62D5/04	B62D5/04		1467
B62D5/0424	10	{the axes of motor and final driven element of steering gear, e.g. rack, being parallel}	B62D5/04	B62D5/04		779
B62D5/0427	11	{the axes being coaxial}	B62D5/04	B62D5/04		239
B62D5/043	9	{characterised by clutch means between driving element, e.g. motor, and driven element, e.g. steering column or steering gear}	B62D5/04	B62D5/04		259
B62D5/0433	10	{the clutch being of on-off type}	B62D5/04	B62D5/04		66
B62D5/0436	11	{the clutch being a controlled emergency clutch, e.g. for disconnecting at motor break-down}	B62D5/04	B62D5/04		41
B62D5/0439	10	{Controllable friction clutches (B62D5/0436 takes precedence)}	B62D5/04	B62D5/04		77
B62D5/0442	9	{Conversion of rotational into longitudinal movement}	B62D5/04	B62D5/04		280
B62D5/0445	10	{Screw drives}	B62D5/04	B62D5/04		359
B62D5/0448	11	{Ball nuts}	B62D5/04	B62D5/04		908
B62D5/0451	10	{Roller spindle drives}	B62D5/04	B62D5/04		60
B62D5/0454	10	{Worm gears}	B62D5/04	B62D5/04		564
B62D5/0457	9	{characterised by control features of the drive means as such}	B62D5/04	B62D5/04		753
B62D5/046	10	{Controlling the motor}	B62D5/04	B62D5/04		3181
B62D5/0463	11	{calculating assisting torque from the motor based on driver input}	B62D5/04	B62D5/04		3734
B62D5/0466	11	{for returning the steering wheel to neutral position}	B62D5/04	B62D5/04		719
B62D5/0469	11	{End-of-stroke control}	B62D5/04	B62D5/04		424
B62D5/0472	11	{for damping vibrations}	B62D5/04	B62D5/04		727
B62D5/0475	10	{Controlling other elements}	B62D5/04	B62D5/04		186
B62D5/0478	11	{Clutches}	B62D5/04	B62D5/04		189
B62D5/0481	10	{monitoring the steering system, e.g. failures}	B62D5/04	B62D5/04		2117
B62D5/0484	11	{for reaction to failures, e.g. limp home}	B62D5/04	B62D5/04		1335
B62D5/0487	11	{detecting motor faults (B62D5/0496 takes precedence)}	B62D5/04	B62D5/04		738
B62D5/049	11	{detecting sensor failures}	B62D5/04	B62D5/04		646
B62D5/0493	11	{detecting processor errors, e.g. plausibility of steering direction}	B62D5/04	B62D5/04		311
B62D5/0496	11	{by using a temperature sensor}	B62D5/04	B62D5/04		263
B62D5/06	8	fluid, i.e. using a pressurised fluid for most or all the force required for steering a vehicle	B62D5/06	B62D5/06		1979
B62D5/061	9	{provided with effort, steering lock, or end-of-stroke limiters}	B62D5/06	B62D5/06		449
B62D5/062	9	{Details, component parts}	B62D5/06	B62D5/06		1685
B62D5/063	10	{Pump driven by vehicle engine (B62D5/065 takes precedence)}	B62D5/06	B62D5/06		379
B62D5/064	10	{Pump driven independently from vehicle engine, e.g. electric driven pump (B62D5/065 takes precedence)}	B62D5/06	B62D5/06		636
B62D5/065	9	characterised by specially adapted means for varying pressurised fluid supply based on need, e.g. on-demand, variable assist	B62D5/065	B62D5/065		1086
B62D5/07	9	Supply of pressurised fluid for steering also supplying other consumers {; control thereof}	B62D5/07	B62D5/07		1133
B62D5/075	10	{using priority valves}	B62D5/07	B62D5/07		240
B62D5/08	9	characterised by type of {steering} valve used (valves in general F16K)	B62D5/08	B62D5/08		838
B62D5/081	10	{Seat valves}	B62D5/08	B62D5/08		27
B62D5/083	10	Rotary valves	B62D5/083	B62D5/083		929
B62D5/0832	11	{with elastic means other than a torsion bar, e.g. leaf springs}	B62D5/083	B62D5/083		63
B62D5/0835	11	{characterised by means for actively influencing the deflection angle of the valve, e.g. depending on driving parameters}	B62D5/083	B62D5/083		151
B62D5/0837	11	{characterised by the shape of the control edges, e.g. to reduce noise}	B62D5/083	B62D5/083		78
B62D5/087	10	Sliding spool valves	B62D5/087	B62D5/087		340
B62D5/09	9	characterised by means for actuating valves	B62D5/09	B62D5/09		779
B62D5/091	10	{Hydraulic steer-by-wire systems, e.g. the valve being actuated by an electric motor}	B62D5/09	B62D5/09		250
B62D5/092	11	{the electric motor being connected to the final driven element of the steering gear, e.g. rack}	B62D5/09	B62D5/09		80
B62D5/093	10	Telemotor driven by steering wheel movement (hydraulic steering gear B62D3/14)	B62D5/093	B62D5/093		392
B62D5/097	11	gerotor type	B62D5/097	B62D5/097		402
B62D5/10	9	characterised by type of power unit	B62D5/10	B62D5/10		214
B62D5/12	10	Piston and cylinder	B62D5/12	B62D5/12		869
B62D5/14	10	Rotary motor	B62D5/14	B62D5/14		141
B62D5/16	10	Expansible chamber with flexible wall	B62D5/16	B62D5/16		17
B62D5/18	9	characterised by power transmitting means	B62D5/18	B62D5/18		149
B62D5/20	9	specially adapted for particular type of steering gear or particular application (steering gears per seB62D3/00; steering linkages not characterised by being power-assisted or power-driven B62D7/00)	B62D5/20	B62D5/20		130
B62D5/22	10	for rack-and-pinion type	B62D5/22	B62D5/22		964
B62D5/24	10	for worm type	B62D5/24	B62D5/24		687
B62D5/26	10	for pivoted axles	B62D5/26	B62D5/26		30
B62D5/28	10	for pivoted bogies	B62D5/28	B62D5/28		36
B62D5/30	9	Safety devices, e.g. alternate emergency power supply or transmission means to ensure steering upon failure of the primary steering means	B62D5/30	B62D5/30		737
B62D5/32	10	for telemotor systems	B62D5/32	B62D5/32		235
B62D6/00	7	Arrangements for automatically controlling steering depending on driving conditions sensed and responded to, e.g. control circuits (means for initiating a change in direction B62D1/00; steering valves B62D5/06; combined with means for inclining the vehicle body or wheels on bends B62D9/00)<br><br><u>NOTE</u><br><br> When classifying in this group, classification is also made in the appropriate one of groups B62D1/00&#160;-&#160;B62D5/00 or B62D7/00&#160;-&#160;B62D19/00 if other aspects of the steering system are of interest 	B62D6/00	B62D6/00		3922
B62D6/001	8	{the torque NOT being among the input parameters}	B62D6/00	B62D6/00		837
B62D6/002	8	{computing target steering angles for front or rear wheels (B62D7/159 takes precedence)}	B62D6/00	B62D6/00		1840
B62D6/003	9	{in order to control vehicle yaw movement, i.e. around a vertical axis (B62D6/007 takes precedence)}	B62D6/00	B62D6/00		899
B62D6/005	10	{treating sensor outputs to obtain the actual yaw rate}	B62D6/00	B62D6/00		164
B62D6/006	9	{using a measured or estimated road friction coefficient}	B62D6/00	B62D6/00		226
B62D6/007	8	{adjustable by the driver, e.g. sport mode}	B62D6/00	B62D6/00		656
B62D6/008	8	{Control of feed-back to the steering input member, e.g. simulating road feel in steer-by-wire applications}	B62D6/00	B62D6/00		2096
B62D6/02	8	responsive only to vehicle speed	B62D6/02	B62D6/02		1328
B62D6/04	8	responsive only to forces disturbing the intended course of the vehicle, e.g. forces acting transversely to the direction of vehicle travel	B62D6/04	B62D6/04		638
B62D6/06	8	responsive only to vehicle vibration dampening arrangements (steering dampers for cycles B62K21/08)	B62D6/06	B62D6/06		84
B62D6/08	8	responsive only to {driver} input torque	B62D6/08	B62D6/08		296
B62D6/10	9	characterised by means for sensing {or determining} torque	B62D6/10	B62D6/10		2073
B62D7/00	7	Steering linkage; Stub axles or their mountings (B62D13/00 takes precedence; power-assisted or power-driven steering B62D5/00)	B62D7/00	B62D7/00		638
B62D7/02	8	for pivoted bogies	B62D7/02	B62D7/02		569
B62D7/023	9	{Steering turntables}	B62D7/02	B62D7/02		1125
B62D7/026	9	{characterised by comprising more than one bogie, e.g. situated in more than one plane transversal to the longitudinal centre line of the vehicle}	B62D7/02	B62D7/02		281
B62D7/04	9	with more than one wheel	B62D7/04	B62D7/04		462
B62D7/06	8	for individually-pivoted wheels, e.g. on king-pins	B62D7/06	B62D7/06		465
B62D7/08	9	the pivotal axes being situated in a single plane transverse to the longitudinal centre line of the vehicle	B62D7/08	B62D7/08		265
B62D7/09	10	characterised by means varying the ratio between the steering angles of the steered wheels (varying the ratio automatically depending on driving conditions B62D6/00)	B62D7/09	B62D7/09		175
B62D7/10	10	with single-output steering gear	B62D7/10	B62D7/10		82
B62D7/12	10	with twin-output steering gear	B62D7/12	B62D7/12		50
B62D7/14	9	the pivotal axes being situated in more than one plane transverse to the longitudinal centre line of the vehicle, e.g. all-wheel steering	B62D7/14	B62D7/14		598
B62D7/142	10	{specially adapted for particular vehicles, e.g. tractors, carts, earth-moving vehicles, trucks}	B62D7/14	B62D7/14		465
B62D7/144	11	{for vehicles with more than two axles}	B62D7/14	B62D7/14		752
B62D7/146	10	{characterised by comprising means for steering by acting on the suspension system, e.g. on the mountings of the suspension arms}	B62D7/14	B62D7/14		460
B62D7/148	10	{provided with safety devices}	B62D7/14	B62D7/14		554
B62D7/15	10	characterised by means varying the ratio between the steering angles of the steered wheels {(B62D7/148 takes precedence)}	B62D7/15	B62D7/15		211
B62D7/1509	11	{with different steering modes, e.g. crab-steering, or steering specially adapted for reversing of the vehicle}	B62D7/15	B62D7/15		802
B62D7/1518	11	{comprising a mechanical interconnecting system between the steering control means of the different axles}	B62D7/15	B62D7/15		54
B62D7/1527	12	{comprising only mechanical parts, i.e. without assistance means}	B62D7/15	B62D7/15		359
B62D7/1536	12	{provided with hydraulic assistance}	B62D7/15	B62D7/15		215
B62D7/1545	12	{provided with electrical assistance}	B62D7/15	B62D7/15		252
B62D7/1554	11	{comprising a fluid interconnecting system between the steering control means of the different axles}	B62D7/15	B62D7/15		31
B62D7/1563	12	{provided with fluid control means (B62D7/1572 takes precedence)}	B62D7/15	B62D7/15		116
B62D7/1572	12	{provided with electro-hydraulic control means}	B62D7/15	B62D7/15		268
B62D7/1581	11	{characterised by comprising an electrical interconnecting system between the steering control means of the different axles}	B62D7/15	B62D7/15		355
B62D7/159	11	{characterised by computing methods or stabilisation processes or systems, e.g. responding to yaw rate, lateral wind, load, road condition}	B62D7/15	B62D7/15		1361
B62D7/16	8	Arrangement of linkage connections (pivots per seF16C)	B62D7/16	B62D7/16		1590
B62D7/163	9	{substantially in axial direction, e.g. between rack bar and tie-rod}	B62D7/16	B62D7/16		264
B62D7/166	9	{substantially perpendicular, e.g. between tie-rod and steering knuckle}	B62D7/16	B62D7/16		220
B62D7/18	8	Steering knuckles; King pins	B62D7/18	B62D7/18		2573
B62D7/20	8	Links, e.g. track rods (means for adjusting camber, castor, or toe-in B62D17/00)	B62D7/20	B62D7/20		1540
B62D7/22	8	Arrangements for reducing or eliminating reaction, e.g. vibration, from parts, e.g. wheels, of the steering system	B62D7/22	B62D7/22		998
B62D7/222	9	{acting on the steering wheel}	B62D7/22	B62D7/22		232
B62D7/224	9	{acting between the steering wheel and the steering gear, e.g. on the steering column}	B62D7/22	B62D7/22		322
B62D7/226	9	{acting on the steering gear}	B62D7/22	B62D7/22		145
B62D7/228	9	{acting between the steering gear and the road wheels, e.g. on tie-rod}	B62D7/22	B62D7/22		205
B62D9/00	7	Steering deflectable wheels not otherwise provided for (steering positon indicators B62D15/02)	B62D9/00	B62D9/00		888
B62D9/002	8	{combined with means for differentially distributing power on the deflectable wheels during cornering}	B62D9/00	B62D9/00		219
B62D9/005	8	{Emergency systems using brakes for steering}	B62D9/00	B62D9/00		166
B62D9/007	8	{Emergency systems using the steering system for braking}	B62D9/00	B62D9/00		45
B62D9/02	8	combined with means for inwardly inclining vehicle body on bends	B62D9/02	B62D9/02		493
B62D9/04	8	combined with means for {inwardly} inclining wheels on bends (B62D9/02 takes precedence)	B62D9/04	B62D9/04		84
B62D11/00	7	Steering non-deflectable wheels; Steering endless tracks or the like<br><br><u>NOTE</u><br><br> Gearings of interest apart from this application are also classified in the relevant group of subclass F16H covering gearings per se	B62D11/00	B62D11/00		244
B62D11/001	8	{control systems (B62D11/183 takes precedence)}<br><br><u>NOTE</u><br><br><br>When classifying in this group, classification is also made in the appropriate one of groups B62D11/02&#160;-&#160;B62D11/24 if other aspects of the steering system are of interest	B62D11/00	B62D11/00		108
B62D11/003	9	{Electric or electronic control systems}	B62D11/00	B62D11/00		528
B62D11/005	9	{Hydraulic control systems}	B62D11/00	B62D11/00		161
B62D11/006	9	{Mechanical control systems}	B62D11/00	B62D11/00		142
B62D11/008	9	{Pneumatic control systems}	B62D11/00	B62D11/00		6
B62D11/02	8	by differentially driving ground-engaging elements on opposite vehicle sides	B62D11/02	B62D11/02		310
B62D11/04	9	by means of separate power sources	B62D11/04	B62D11/04		1005
B62D11/06	9	by means of a single main power source	B62D11/06	B62D11/06		134
B62D11/08	10	using brakes or clutches as main steering-effecting means	B62D11/08	B62D11/08		1567
B62D11/10	10	using gearings with differential power outputs on opposite sides, e.g. twin-differential or epicyclic gears	B62D11/10	B62D11/10		549
B62D11/105	11	{using variable ratio belt and pulley gearings}	B62D11/10	B62D11/10		29
B62D11/12	11	using separate change-speed gearings	B62D11/12	B62D11/12		90
B62D11/14	11	differential power outputs being effected by additional power supply to one side, e.g. power originating from secondary power source	B62D11/14	B62D11/14		112
B62D11/16	12	the additional power supply being supplied mechanically	B62D11/16	B62D11/16		97
B62D11/18	12	the additional power supply being supplied hydraulically	B62D11/18	B62D11/18		357
B62D11/183	13	{Control systems therefor}	B62D11/18	B62D11/18		619
B62D11/186	13	{Uncoupling devices for the hydraulic motors, e.g. to allow towing}	B62D11/18	B62D11/18		7
B62D11/20	8	Endless-track steering having pivoted bogie carrying track (B62D11/02 takes precedence)	B62D11/20	B62D11/20		314
B62D11/22	8	Endless track steering being effected by deflecting endless track rollers or the like	B62D11/22	B62D11/22		83
B62D11/24	8	Endless track steering specially adapted for vehicles having both steerable wheels and endless track	B62D11/24	B62D11/24		248
B62D12/00	7	Steering specially adapted for vehicles operating in tandem or having pivotally connected frames (steering endless tracks or the like B62D11/00; steering specially adapted for trailers B62D13/00)	B62D12/00	B62D12/00		742
B62D12/02	8	for vehicles operating in tandem	B62D12/02	B62D12/02		220
B62D13/00	7	Steering specially adapted for trailers (combined traction and steering hitches B60D)	B62D13/00	B62D13/00		1136
B62D13/005	8	{operated from tractor steering system}	B62D13/00	B62D13/00		265
B62D13/02	8	for centrally-pivoted axles	B62D13/02	B62D13/02		795
B62D13/025	9	{the pivoted movement being initiated by the coupling means between tractor and trailer}	B62D13/02	B62D13/02		374
B62D13/04	8	for individually-pivoted wheels	B62D13/04	B62D13/04		1444
B62D13/06	8	for backing a normally drawn trailer	B62D13/06	B62D13/06		988
B62D15/00	7	Steering not otherwise provided for	B62D15/00	B62D15/00		635
B62D15/02	8	Steering position indicators {; Steering position determination; Steering aids}	B62D15/02	B62D15/02		1359
B62D15/0205	9	{Mechanical indicators, e.g. in or near steering wheel}	B62D15/02	B62D15/02		240
B62D15/021	9	{Determination of steering angle}	B62D15/02	B62D15/02		1527
B62D15/0215	10	{by measuring on the steering column}	B62D15/02	B62D15/02		998
B62D15/022	11	{on or near the connection between the steering wheel and steering column}	B62D15/02	B62D15/02		176
B62D15/0225	10	{by measuring on a steering gear element, e.g. on a rack bar}	B62D15/02	B62D15/02		488
B62D15/023	10	{by measuring on the king pin}	B62D15/02	B62D15/02		152
B62D15/0235	10	{by measuring or deriving directly at the electric power steering motor}	B62D15/02	B62D15/02		460
B62D15/024	10	{Other means for determination of steering angle without directly measuring it, e.g. deriving from wheel speeds on different sides of the car}	B62D15/02	B62D15/02		407
B62D15/0245	10	{Means or methods for determination of the central position of the steering system, e.g. straight ahead position}	B62D15/02	B62D15/02		619
B62D15/025	9	{Active steering aids, e.g. helping the driver by actively influencing the steering system after environment evaluation (B62D1/28 takes precedence)}	B62D15/02	B62D15/02		3285
B62D15/0255	10	{Automatic changing of lane, e.g. for passing another vehicle}	B62D15/02	B62D15/02		487
B62D15/026	10	{combined with automatic distance control, i.e. electronic tow bar}	B62D15/02	B62D15/02		153
B62D15/0265	10	{Automatic obstacle avoidance by steering}	B62D15/02	B62D15/02		940
B62D15/027	9	{Parking aids, e.g. instruction means}	B62D15/02	B62D15/02		1356
B62D15/0275	10	{by overlaying a vehicle path based on present steering angle over an image without processing that image}	B62D15/02	B62D15/02		348
B62D15/028	10	{Guided parking by providing commands to the driver, e.g. acoustically or optically}	B62D15/02	B62D15/02		714
B62D15/0285	10	{Parking performed automatically}	B62D15/02	B62D15/02		3726
B62D15/029	9	{Steering assistants using warnings or proposing actions to the driver without influencing the steering system}	B62D15/02	B62D15/02		1028
B62D15/0295	10	{by overlaying a vehicle path based on present steering angle over an image without processing that image}	B62D15/02	B62D15/02		239
B62D17/00	7	Means on vehicles for adjusting camber, castor, or toe-in	B62D17/00	B62D17/00		2106
B62D19/00	7	Radius rods, i.e. distance members	B62D19/00	B62D19/00		140
B62D21/00	7	Understructures, i.e. chassis frame on which a vehicle body may be mounted (combined frame and vehicle body B62D23/00{; characterised by the material thereof B62D29/00})	B62D21/00	B62D21/00		1990
B62D21/02	8	comprising longitudinally or transversely arranged frame members	B62D21/02	B62D21/02		5069
B62D21/03	9	transverse members providing body support	B62D21/03	B62D21/03		710
B62D21/04	9	single longitudinal type	B62D21/04	B62D21/04		385
B62D21/05	9	pinched frame type, i.e. formed of at least two longitudinal frame sections connected by other longitudinal frame sections of lesser transverse dimension	B62D21/05	B62D21/05		87
B62D21/06	8	of X-shaped or fork-shaped construction, i.e. having members which form an X or fork as the frame is seen in plan view	B62D21/06	B62D21/06		270
B62D21/07	8	wide-hipped frame type, i.e. a wide box-shaped mid portion with narrower sections extending from said mid portion in both fore and aft directions	B62D21/07	B62D21/07		160
B62D21/08	8	built up with interlaced cross members	B62D21/08	B62D21/08		425
B62D21/09	8	Means for mounting load bearing surfaces	B62D21/09	B62D21/09		1584
B62D21/10	8	in which the main member is plate-like	B62D21/10	B62D21/10		451
B62D21/11	8	with resilient means for suspension {, e.g. of wheels or engine; sub-frames for mounting engine or suspensions}<br><br><u>NOTE</u><br><br> This group does not cover subject matter primarily relating to the suspension, with only a nominal recitation of frame structure, which are covered by subclass  B60G	B62D21/11	B62D21/11		3543
B62D21/12	8	assembled from readily detachable parts	B62D21/12	B62D21/12		697
B62D21/14	8	of adjustable length or width	B62D21/14	B62D21/14		1068
B62D21/15	8	having impact absorbing means, e.g. a frame designed to permanently or temporarily change shape or dimension upon impact with another body (bumpers B60R19/02; shock absorbers in general F16F)	B62D21/15	B62D21/15		2480
B62D21/152	9	{Front or rear frames}	B62D21/15	B62D21/15		3779
B62D21/155	10	{Sub-frames or underguards}	B62D21/15	B62D21/15		1428
B62D21/157	9	{for side impacts}	B62D21/15	B62D21/15		1908
B62D21/16	8	having fluid storage compartment	B62D21/16	B62D21/16		390
B62D21/17	8	forming fluid or electrical conduit means or having other means to accommodate the transmission of a force or signal	B62D21/17	B62D21/17		416
B62D21/18	8	characterised by the vehicle type and not provided for in groups B62D21/02&#160;-&#160;B62D21/17	B62D21/18	B62D21/18		908
B62D21/183	9	{specially adapted for sports vehicles, e.g. race, dune buggies, go-karts (tubular skeleton B62D23/005)}	B62D21/18	B62D21/18		544
B62D21/186	9	{for building site vehicles or multi-purpose tractors (tracked vehicles B62D55/10; tractors in general B62D49/00; building site vehicles in general E02F; lift-trucks B66F)}	B62D21/18	B62D21/18		666
B62D21/20	9	trailer type, i.e. a frame specifically constructed for use in a non-powered vehicle	B62D21/20	B62D21/20		1084
B62D23/00	7	Combined superstructure and frame, i.e. monocoque constructions ({having impact absorbing means B62D21/15; } superstructure {or monocoque structure} sub-units {or parts or details thereof}B62D25/00{; characterised by the material thereof B62D29/00})	B62D23/00	B62D23/00		781
B62D23/005	8	{with integrated chassis in the whole shell, e.g. meshwork, tubes, or the like (B62D33/044 takes precedence)}	B62D23/00	B62D23/00		1033
B62D24/00	7	Connections between vehicle body and vehicle frame (B62D23/00, B62D33/077 take precedence)	B62D24/00	B62D24/00		503
B62D24/02	8	Vehicle body, not intended to move relatively to the vehicle frame, and mounted on vibration absorbing mountings, e.g. rubber pads	B62D24/02	B62D24/02		394
B62D24/04	8	Vehicle body mounted on resilient suspension for movement relative to the vehicle frame	B62D24/04	B62D24/04		234
B62D25/00	7	Superstructure {or monocoque structure} sub-units; Parts or details thereof not otherwise provided for {(having impact absorbing means B62D21/15; running-boards, steps, or the like as superstructure sub-unit B60R3/00)}	B62D25/00	B62D25/00		2402
B62D25/02	8	Side panels {(B62D33/046 takes precedence; sideboards for open load compartments B62D33/023)}	B62D25/02	B62D25/02		2665
B62D25/025	9	{Side sills thereof}	B62D25/02	B62D25/02		3351
B62D25/04	8	Door pillars {; windshield pillars}	B62D25/04	B62D25/04		5857
B62D25/06	8	Fixed roofs (non-fixed roofs or like shelters B60J7/00; roof liners B60R13/02; insulating elements B60R13/08)	B62D25/06	B62D25/06		4700
B62D25/07	9	having water drainage or guide means integral with roof structure	B62D25/07	B62D25/07		389
B62D25/08	8	Front or rear portions {(sub-frames for mounting engine or suspensions B62D21/11)}	B62D25/08	B62D25/08		4381
B62D25/081	9	{Cowls (ventilating openings situated directly in front of the vehicle front window B60H1/28)}	B62D25/08	B62D25/08		2029
B62D25/082	9	{Engine compartments}	B62D25/08	B62D25/08		2382
B62D25/084	10	{Radiator supports}	B62D25/08	B62D25/08		1557
B62D25/085	10	{Front-end modules}	B62D25/08	B62D25/08		1111
B62D25/087	9	{Luggage compartments}	B62D25/08	B62D25/08		1824
B62D25/088	9	{Details of structures as upper supports for springs or dampers}	B62D25/08	B62D25/08		1293
B62D25/10	9	Bonnets or lids {, e.g. for trucks, tractors, busses, work vehicles (for truck beds B60J7/1607; for boats B63B19/12; doors arranged at the vehicle rear B60J5/10; inlet covers for vehicle fuel tanks B60K15/05; for protecting non-occupants of a vehicle B60R21/38)}	B62D25/10	B62D25/10		1766
B62D25/105	10	{for motor cars}	B62D25/10	B62D25/10		1926
B62D25/12	10	Parts or details thereof (locks E05B, {E05B83/16; devices for holding open E05C17/00, e.g. while carrying oversize objects E05C17/042}; hinges E05D; counterbalancing means E05F; {checks, stops, buffers E05F5/00; } springs, {e.g. pneumatic springs}F16F)	B62D25/12	B62D25/12		4933
B62D25/14	9	Dashboards as superstructure sub-units (other dashboard aspects B60K)	B62D25/14	B62D25/14		1970
B62D25/142	10	{having ventilation channels incorporated therein}	B62D25/14	B62D25/14		334
B62D25/145	10	{having a crossbeam incorporated therein}	B62D25/14	B62D25/14		1498
B62D25/147	11	{with adjustable connection to the A-pillars}	B62D25/14	B62D25/14		177
B62D25/16	9	Mud-guards or wings; Wheel cover panels (equipped with means for freeing wheels or tyres from foreign matter B60S)	B62D25/16	B62D25/16		2111
B62D25/161	10	{Mud-guards made of non-conventional material, e.g. rubber, plastics}	B62D25/16	B62D25/16		576
B62D25/163	10	{Mounting devices}	B62D25/16	B62D25/16		1136
B62D25/165	11	{including sealing devices}	B62D25/16	B62D25/16		81
B62D25/166	11	{by rods or other distance-keeping devices}	B62D25/16	B62D25/16		189
B62D25/168	10	{Mud guards for utility vehicles}	B62D25/16	B62D25/16		593
B62D25/18	10	Parts or details thereof, e.g. mudguard flaps	B62D25/18	B62D25/18		1664
B62D25/182	11	{Movable mudguards, or mudguards comprising movable or detachable parts (B62D25/188 takes precedence)}	B62D25/18	B62D25/18		423
B62D25/184	12	{to facilitate access to wheels}	B62D25/18	B62D25/18		227
B62D25/186	12	{being attached or suspended laterally from the wheel (B62D25/184 takes precedence)}	B62D25/18	B62D25/18		1050
B62D25/188	11	{Mud-guard flaps for utility vehicles}	B62D25/18	B62D25/18		532
B62D25/20	8	Floors or bottom sub-units {(sub-frames for mounting engine or suspensions B62D21/11; drip trays F16N31/006)}	B62D25/20	B62D25/20		5272
B62D25/2009	9	{in connection with other superstructure subunits}	B62D25/20	B62D25/20		665
B62D25/2018	10	{the subunits being front structures}	B62D25/20	B62D25/20		936
B62D25/2027	10	{the subunits being rear structures}	B62D25/20	B62D25/20		1334
B62D25/2036	10	{the subunits being side panels, sills or pillars (B62D21/157 takes precedence)}	B62D25/20	B62D25/20		2387
B62D25/2045	10	{the subunits being fire walls}	B62D25/20	B62D25/20		281
B62D25/2054	9	{Load carrying floors for commercial vehicles}	B62D25/20	B62D25/20		1064
B62D25/2063	9	{Floor elements for repairs}	B62D25/20	B62D25/20		62
B62D25/2072	9	{Floor protection, e.g. from corrosion or scratching (floor mats B60N3/04, armour F41H7/042, insulation B60R13/08, streamlining B62D35/02)}	B62D25/20	B62D25/20		610
B62D25/2081	9	{Jack receiving devices}	B62D25/20	B62D25/20		132
B62D25/209	9	{Arrangements for the mounting of vehicle hitches (vehicle connections in general B60D)}	B62D25/20	B62D25/20		135
B62D25/24	8	Superstructure sub-units with access {or drainage} openings having movable or removable closures; {Sealing means therefor}(inlet covers for vehicle fuel tanks B60K15/05)	B62D25/24	B62D25/24		1865
B62D27/00	7	Connections between superstructure {or understructure} sub-units {(B62D33/0207, B62D33/044 take precedence; between sub-units predominently made of synthetic material B62D29/048)}	B62D27/00	B62D27/00		388
B62D27/02	8	rigid	B62D27/02	B62D27/02		2256
B62D27/023	9	{Assembly of structural joints}	B62D27/02	B62D27/02		2309
B62D27/026	9	{Connections by glue bonding (in general F16B11/00; processes C09J5/00)}	B62D27/02	B62D27/02		1182
B62D27/04	8	resilient	B62D27/04	B62D27/04		534
B62D27/06	8	readily releasable	B62D27/06	B62D27/06		767
B62D27/065	9	{using screwthread (connection of crossbeam to A- pillars B62D25/147; mounting load bearing surfaces B62D21/09; securing mudguards B62D25/163; connections for synthetic parts B62D29/048)}	B62D27/06	B62D27/06		1417
B62D29/00	7	Superstructures, {understructures, or sub-units thereof,} characterised by the material thereof {(B62D33/044, B62D33/048 take precedence)}	B62D29/00	B62D29/00		855
B62D29/001	8	{characterised by combining metal and synthetic material}	B62D29/00	B62D29/00		1150
B62D29/002	9	{a foamable synthetic material or metal being added in situ(shaping of substances in a plastic state by foaming, in general B29C44/00)}	B62D29/00	B62D29/00		840
B62D29/004	9	{the metal being over-moulded by the synthetic material, e.g. in a mould}	B62D29/00	B62D29/00		598
B62D29/005	9	{preformed metal and synthetic material elements being joined together, e.g. by adhesives}	B62D29/00	B62D29/00		758
B62D29/007	8	{predominantly of special steel or specially treated steel, e.g. stainless steel or locally surface hardened steel}	B62D29/00	B62D29/00		588
B62D29/008	8	{predominantly of light alloys, e.g. extruded}	B62D29/00	B62D29/00		2070
B62D29/02	8	predominantly of wood	B62D29/02	B62D29/02		425
B62D29/04	8	predominantly of synthetic material (working of plastics or substances in a plastic state B29)	B62D29/04	B62D29/04		1122
B62D29/041	9	{Understructures}	B62D29/04	B62D29/04		449
B62D29/043	9	{Superstructures (B62D25/161 takes precedence)}	B62D29/04	B62D29/04		1528
B62D29/045	10	{Van bodies composed of substantially rectangular panels}	B62D29/04	B62D29/04		214
B62D29/046	9	{Combined superstructure and frame, i.e. monocoque constructions}	B62D29/04	B62D29/04		319
B62D29/048	9	{Connections therefor, e.g. joints (B62D29/045 takes precedence)}	B62D29/04	B62D29/04		557
B62D31/00	7	Superstructures for passenger vehicles (passenger vehicles specially adapted to co-operate with aircraft or terminal buildings B64F1/31)	B62D31/00	B62D31/00		662
B62D31/003	8	{compact cars, e.g. city cars}	B62D31/00	B62D31/00		643
B62D31/006	9	{foldable (droppable B60F5/006)}	B62D31/00	B62D31/00		155
B62D31/02	8	for carrying large numbers of passengers, e.g. omnibus	B62D31/02	B62D31/02		1542
B62D31/025	9	{having modular sections}	B62D31/02	B62D31/02		186
B62D31/04	8	with more than one deck	B62D31/04	B62D31/04		257
B62D33/00	7	Superstructures for load-carrying vehicles ({having impact absorbing means B62D21/15; } in which a load-carrying element is movable B60P; liners B60R13/00{; joining sheets or plates to one another or to strips or bars parallel to them F16B5/00})	B62D33/00	B62D33/00		481
B62D33/02	8	Platforms; Open load compartments {(flat wagons including posts or standards B61D3/08)}	B62D33/02	B62D33/02		2126
B62D33/0207	9	{Connections of movable or detachable racks or stanchions to platforms}	B62D33/02	B62D33/02		1139
B62D33/0215	10	{for log hauling vehicles (vehicles for log transport in general B60P3/41)}	B62D33/02	B62D33/02		287
B62D33/0222	9	{Connecting elements between stanchions, e.g. roof supporting elements, stiffeners (non-fixed roofs B60J7/00; securing and covering of load B60P7/00)}	B62D33/02	B62D33/02		346
B62D33/023	9	Sideboard or tailgate structures {(vehicle side panels in general B62D25/02)}	B62D33/023	B62D33/023		914
B62D33/027	10	movable	B62D33/027	B62D33/027		560
B62D33/0273	11	{Movable tailboards for vehicles comprising non-movable sideboards, e.g. pick-up trucks (B62D33/037 takes precedence)}	B62D33/027	B62D33/027		2444
B62D33/0276	11	{by vertical translation (B62D33/0273 takes precedence)}	B62D33/027	B62D33/027		154
B62D33/03	11	by swinging down {(B62D33/0273 takes precedence)}	B62D33/03	B62D33/03		888
B62D33/033	11	removable {(B62D33/0273 takes precedence)}	B62D33/033	B62D33/033		226
B62D33/037	11	Latching means therefor	B62D33/037	B62D33/037		957
B62D33/04	8	Enclosed load compartments {; Frameworks for movable panels, tarpaulins or side curtains (side curtains per seB60J5/065; tarpaulins per seB60J7/00, B60P7/04)}	B62D33/04	B62D33/04		2352
B62D33/042	9	{divided into compartments (movable bulk heads B60P7/14; cattle transport B60P3/04; bottled liquids B60P3/22)}	B62D33/04	B62D33/04		476
B62D33/044	9	{built up with profiles of constant elongated shape, e.g. extruded, mechanically interconnected by coupling members, e.g. by clamping, riveting or bolting}	B62D33/04	B62D33/04		408
B62D33/046	9	{built up with flat self-supporting panels; Fixed connections between panels (B62D29/045, B62D33/048 take precedence)}	B62D33/04	B62D33/04		740
B62D33/048	9	{for refrigerated goods vehicles}	B62D33/04	B62D33/04		690
B62D33/06	8	Drivers&apos; cabs {(overhead guards, e.g. against loads falling down B60R21/11; roll-over protection B60R21/13)}	B62D33/06	B62D33/06		1623
B62D33/0604	9	{Cabs insulated against vibrations or noise, e.g. with elastic suspension (resilient connections between superstructure sub-units B62D27/04; damping noise in general G10K11/00; for vehicles in general B60R13/08)}	B62D33/06	B62D33/06		951
B62D33/0608	10	{pneumatic or hydraulic suspension}	B62D33/06	B62D33/06		392
B62D33/0612	9	{Cabins with living accommodation, especially for long distance road vehicles, i.e. sleeping, cooking, or other facilities (beds in general adapted to be used in vahicles A47C17/80; sanitation devices in vehicles in general B60R15/00; living accommodation in vehicles in general B60P3/32; passenger fittings in general B60N3/00)}	B62D33/06	B62D33/06		578
B62D33/0617	9	{for tractors or off-the-road vehicles (protective devices for drivers in case of overturning of tractors B60R21/131)}	B62D33/06	B62D33/06		966
B62D33/0621	10	{able to be dismantled, folding}	B62D33/06	B62D33/06		198
B62D33/0625	10	{open}	B62D33/06	B62D33/06		297
B62D33/063	9	movable from one position into at least one other position, e.g. tiltable, pivotable about a vertical axis, displaceable from one side of the vehicle to the other	B62D33/063	B62D33/063		232
B62D33/0633	10	{pivotable about a vertical axis}	B62D33/063	B62D33/063		161
B62D33/0636	10	{displaceable along a linear path}	B62D33/063	B62D33/063		231
B62D33/067	10	tiltable	B62D33/067	B62D33/067		871
B62D33/07	11	characterised by the device for locking the cab in the tilted or in the driving position	B62D33/07	B62D33/07		399
B62D33/071	12	{Locking devices for cabins in driving position; Shock and vibration absorbing devices therefor}	B62D33/07	B62D33/07		207
B62D33/073	10	characterised by special adaptations of vehicle control devices	B62D33/073	B62D33/073		259
B62D33/077	8	characterised by the connection of the superstructure to the vehicle frame {(B62D33/06 takes precedence)}	B62D33/077	B62D33/077		473
B62D33/08	8	comprising adjustable means (B62D33/10 takes precedence)	B62D33/08	B62D33/08		1032
B62D33/10	9	comprising means for the suspension of the superstructure on the frame	B62D33/10	B62D33/10		331
B62D35/00	7	Vehicle bodies characterised by streamlining	B62D35/00	B62D35/00		1839
B62D35/001	8	{For commercial vehicles or tractor-trailer combinations, e.g. caravans}	B62D35/00	B62D35/00		1929
B62D35/002	9	{for caravans (B62D35/004 takes precedence)}	B62D35/00	B62D35/00		119
B62D35/004	9	{Inflatable nose or rear cones}	B62D35/00	B62D35/00		132
B62D35/005	8	{Front spoilers (B62D35/001 takes precedence)}	B62D35/00	B62D35/00		1247
B62D35/007	8	{Rear spoilers (B62D35/001 takes precedence)}	B62D35/00	B62D35/00		2600
B62D35/008	8	{Side spoilers (B62D35/001 takes precedence)}	B62D35/00	B62D35/00		552
B62D35/02	8	Streamlining the undersurfaces {(B62D35/005, B62D35/007, B62D35/008 take precedence)}	B62D35/02	B62D35/02		1530
B62D37/00	7	Stabilising vehicle bodies without controlling suspension arrangements	B62D37/00	B62D37/00		656
B62D37/02	8	by aerodynamic means	B62D37/02	B62D37/02		2877
B62D37/04	8	by means of movable masses	B62D37/04	B62D37/04		651
B62D37/06	9	using gyroscopes	B62D37/06	B62D37/06		238
B62D39/00	7	Vehicle bodies not otherwise provided for {, e.g. safety vehicles (safety equipment B60R21/00)}	B62D39/00	B62D39/00		468
B62D41/00	7	Fittings for identifying vehicles in case of collision; Fittings for marking or recording collision areas	B62D41/00	B62D41/00		1250
B62D43/00	7	Spare wheel stowing, holding, or mounting arrangements	B62D43/00	B62D43/00		524
B62D43/002	8	{Handling devices, mainly for heavy wheels (via cables and chains B62D43/045)}	B62D43/00	B62D43/00		558
B62D43/005	8	{Protective coverings for spare wheels}	B62D43/00	B62D43/00		550
B62D43/007	8	{Anti-theft devices for spare wheels}	B62D43/00	B62D43/00		335
B62D43/02	8	external to the vehicle body	B62D43/02	B62D43/02		1226
B62D43/04	9	attached beneath the vehicle body	B62D43/04	B62D43/04		573
B62D43/045	10	{the wheel or its cradle being attached to one or more chains or cables for handling}	B62D43/04	B62D43/04		457
B62D43/06	8	within the vehicle body	B62D43/06	B62D43/06		231
B62D43/08	9	and arranged substantially vertically	B62D43/08	B62D43/08		164
B62D43/10	9	and arranged substantially horizontally	B62D43/10	B62D43/10		1280
B62D47/00	7	Motor vehicles or trailers predominantly for carrying passengers (superstructures B62D31/00)	B62D47/00	B62D47/00		200
B62D47/003	8	{convertible in order to modify the number of seats (foldable compact cars B62D31/006; convertible from one use to a different one B60P3/42)}	B62D47/00	B62D47/00		463
B62D47/006	8	{Vehicles which can be divided in sub-vehicles; nestable vehicles}	B62D47/00	B62D47/00		148
B62D47/02	8	for large numbers of passengers, e.g. omnibus	B62D47/02	B62D47/02		522
B62D47/025	9	{articulated buses with interconnecting passageway, e.g. bellows (coupling aspects B60D5/00)}	B62D47/02	B62D47/02		406
B62D49/00	7	Tractors (of walk type B62D51/04; endless- track features B62D55/00{; transport specially adapted for underground galleries E21F13/02})	B62D49/00	B62D49/00		1216
B62D49/002	8	{characterised by being of the low ground pressure type}	B62D49/00	B62D49/00		50
B62D49/005	8	{Tractors for semi-trailers (combinations of tractor plus semi- trailer B62D53/06)}	B62D49/00	B62D49/00		164
B62D49/007	9	{Tractors for handling trailers, e.g. roll-trailers in terminals}	B62D49/00	B62D49/00		150
B62D49/02	8	modified to take lifting devices	B62D49/02	B62D49/02		650
B62D49/04	8	modified to take pushing devices	B62D49/04	B62D49/04		213
B62D49/06	8	adapted for multi-purpose use	B62D49/06	B62D49/06		820
B62D49/0607	9	{Straddle tractors, used for instance above vine stocks, rows of bushes, or the like}	B62D49/06	B62D49/06		521
B62D49/0614	9	{equipped with visual aids for positioning implements or to control working condition (optical signalling for vehicles in general B60Q1/26)}	B62D49/06	B62D49/06		63
B62D49/0621	9	{comprising traction increasing arrangements, e.g. all-wheel traction devices, multiple-axle traction arrangements, auxiliary traction increasing devices (anti-skid or anti-slip devices fitted onto the wheels B60B15/02, B60B39/12; arrangements of transmission for driving both front and rear wheels or tandem wheels of vehicles B60K17/34, B60K17/36)}	B62D49/06	B62D49/06		400
B62D49/0628	10	{using detachable weights (counterweights against overturning B62D49/085; movable stabilisation masses B62D37/04)}	B62D49/06	B62D49/06		128
B62D49/0635	10	{using additional ground engaging means, e.g. endless tracks (vehicles with endless tracks and either additional or alternative ground wheels B62D55/02, B62D55/04)}	B62D49/06	B62D49/06		456
B62D49/0642	10	{by coupling of tractors}	B62D49/06	B62D49/06		83
B62D49/065	9	{Coupling of multi-purpose tractors with equipment (towing bars B60D; with load transfer B62D53/08; power take-off B60K; with lifting devices B62D49/02; pushing gear B62D49/04)}	B62D49/06	B62D49/06		716
B62D49/0657	9	{Asymmetrical tractors}	B62D49/06	B62D49/06		139
B62D49/0664	9	{Light, simple, and economical tractors (B62D49/002 takes precedence)}	B62D49/06	B62D49/06		285
B62D49/0671	10	{the driver riding on the tractor}	B62D49/06	B62D49/06		107
B62D49/0678	9	{Tractors of variable track width or wheel base (for vehicles in general B60B23/12 and B60B35/10)}	B62D49/06	B62D49/06		368
B62D49/0685	9	{Reversible tractors adapted for shuttle work}	B62D49/06	B62D49/06		82
B62D49/0692	9	{characterised by the particular arrangement of control devices, e.g. having more than one control stand, operable from vehicle extension (control devices or systems characterised by mechanical features only)}	B62D49/06	B62D49/06		262
B62D49/08	8	having means for preventing overturning or tipping (safety devices for propulsion-unit control, specially adapted for, or arranged in, vehicles B60K28/00)	B62D49/08	B62D49/08		639
B62D49/085	9	{Counterweight}	B62D49/08	B62D49/08		395
B62D51/00	7	Motor vehicles characterised by the driver not being seated {(wheeled carriers for golf bags A63B55/60)}	B62D51/00	B62D51/00		62
B62D51/001	8	{characterised by the vehicle control device (mechanical features of control devices in general G05G; arrangements of vehicle control devices in general B60K20/00, B60K23/00, B60K26/00)}	B62D51/00	B62D51/00		522
B62D51/002	9	{comprising safety arrangements (safety devices for vehicle propulsion unit control B60K28/00)}	B62D51/00	B62D51/00		102
B62D51/004	8	{characterised by the transmission (arrangements or mounting of transmissions in vehicles B60K17/00; gearing in general F16H)}	B62D51/00	B62D51/00		231
B62D51/005	8	{Vehicular characteristics of load handling vehicles, e.g. pedestrian trucks (fork-lift trucks B66F9/06)}	B62D51/00	B62D51/00		213
B62D51/007	8	{the vehicle being of the endless track type (endless track vehicles in general B62D55/00)}	B62D51/00	B62D51/00		168
B62D51/008	8	{characterised by the vehicle being formed by articulated or separable units (road trains B62D53/00)}	B62D51/00	B62D51/00		103
B62D51/02	8	the driver standing in the vehicle	B62D51/02	B62D51/02		573
B62D51/04	8	the driver walking	B62D51/04	B62D51/04		774
B62D51/06	9	Uniaxle walk-type tractors	B62D51/06	B62D51/06		511
B62D51/065	10	{the vehicle baving only one wheel}	B62D51/06	B62D51/06		111
B62D53/00	7	Tractor-trailer combinations; Road trains (traction couplings other than fifth wheel coupling B60D{; tracked vehicles comprising at least two articulated parts B62D55/0655})	B62D53/00	B62D53/00		891
B62D53/005	8	{Combinations with at least three axles and comprising two or more articulated parts (articulated buses B62D47/025)}	B62D53/00	B62D53/00		490
B62D53/02	8	comprising a uniaxle tractor unit and a uniaxle trailer unit {(seeB60B11/00 - B60B11/08)}	B62D53/02	B62D53/02		848
B62D53/021	9	{comprising a universal coupling joint}	B62D53/02	B62D53/02		238
B62D53/023	9	{with two or more coupling joints allowing staggering of the units from a central plane}	B62D53/02	B62D53/02		50
B62D53/025	9	{Comprising a transmission shaft passing through the coupling joints (B62D53/021 takes precedence; trailers with powered axles B62D59/00)}	B62D53/02	B62D53/02		92
B62D53/026	10	{With all wheels powered}	B62D53/02	B62D53/02		142
B62D53/028	9	{Having only coupling joints other than directional (articulated frames B62D21/186 and B62D55/10)}	B62D53/02	B62D53/02		109
B62D53/04	8	comprising a vehicle carrying an essential part of the other vehicle&apos;s load by having supporting means for the front or rear part of the other vehicle	B62D53/04	B62D53/04		444
B62D53/045	9	{with rigid linkage in the horizontal plane (luggage trailers B62D63/064&#160;-&#160;B62D63/067)}	B62D53/04	B62D53/04		135
B62D53/06	9	Semi-trailers	B62D53/06	B62D53/06		992
B62D53/061	10	{of flat bed or low loader type or fitted with swan necks (detachable swan necks B62D53/065; swan neck-fifth wheel couplings B62D53/08)}	B62D53/06	B62D53/06		513
B62D53/062	11	{having inclinable, lowerable platforms; Lift bed trailers; Straddle trailers (lifting coupling saddles B62D53/0821; crane vehicles B60P3/28)}	B62D53/06	B62D53/06		513
B62D53/064	12	{inclining platforms by detachable bogies}	B62D53/06	B62D53/06		33
B62D53/065	12	{inclining platforms by detachable or folding swan necks}	B62D53/06	B62D53/06		326
B62D53/067	10	{Multi-purpose, convertible or extendable load surface semi-trailers (for container transport B60P1/6418; convertible road transport vehicles in general B60P3/42)}	B62D53/06	B62D53/06		452
B62D53/068	10	{having devices to equalise or modify the load between the fifth wheel and the rear wheels (adjustable couping saddles per seB62D53/0807; load transfer devices to permit coupling or uncoupling B62D53/0857; anti jack-knifing devices B62D53/0871)}	B62D53/06	B62D53/06		600
B62D53/08	9	Fifth wheel traction couplings {(tractors for handling trailers in terminals B62D49/007)}	B62D53/08	B62D53/08		960
B62D53/0807	10	{adjustable coupling saddles mounted on sub-frames; Mounting plates therefor}	B62D53/08	B62D53/08		297
B62D53/0814	11	{with adjustment of the clearance between the tractor or the trailer (devices modifying the load in tractor-trailer combinations B62D53/068)}	B62D53/08	B62D53/08		186
B62D53/0821	11	{Lifting saddles, i.e. to lift the trailer front (tilting body constructions B60P)}	B62D53/08	B62D53/08		204
B62D53/0828	11	{Removable or fold-away traction couplings for non-specialised tractor vehicles}	B62D53/08	B62D53/08		258
B62D53/0835	11	{Coupling saddles able to rock in all directions, e.g. for use in rough terrain}	B62D53/08	B62D53/08		107
B62D53/0842	10	{King pins}	B62D53/08	B62D53/08		433
B62D53/085	11	{fitted with anti-coupling devices, pivotal or retractable king pins, e.g. to prevent theft (vehicle fittings for preventing theft in general B60R25/00)}	B62D53/08	B62D53/08		170
B62D53/0857	10	{Auxiliary semi-trailer handling or loading equipment, e.g. ramps, rigs, coupling supports}	B62D53/08	B62D53/08		504
B62D53/0864	11	{Dollies for fifth wheel coupling}	B62D53/08	B62D53/08		527
B62D53/0871	10	{with stabilising means, e.g. to prevent jack-knifing, pitching, rolling, buck jumping (stabilising in general B62D37/00; tractors B62D49/08)}	B62D53/08	B62D53/08		394
B62D53/0878	11	{the fifth wheel coupling incorporating braking or restraining means}	B62D53/08	B62D53/08		228
B62D53/0885	10	{Comprising devices to limit or to compensate for wear or excessive play; Lubricating, shock absorbing, bearing devices, or the like}	B62D53/08	B62D53/08		342
B62D53/0892	10	{comprising power transmission shafts (trailers with driven ground wheels B62D59/00)}	B62D53/08	B62D53/08		17
B62D53/10	10	with means for preventing accidental uncoupling	B62D53/10	B62D53/10		290
B62D53/12	10	engaging automatically	B62D53/12	B62D53/12		330
B62D53/125	11	{with simultaneous coupling of the service lines}	B62D53/12	B62D53/12		186
B62D55/00	7	Endless track vehicles (steering aspects B62D11/00; {characterised by the driver not being seated B62D51/007})	B62D55/00	B62D55/00		477
B62D55/02	8	with tracks and additional ground wheels {(for multi-purpose tractors B62D49/0635)}	B62D55/02	B62D55/02		874
B62D55/04	8	with tracks and alternative ground wheels, e.g. changeable from endless track vehicle into wheeled vehicle and vice versa{(for multi-purpose tractors B62D49/0635)}	B62D55/04	B62D55/04		1210
B62D55/06	8	with tracks without ground wheels	B62D55/06	B62D55/06		1392
B62D55/062	9	{Tracked vehicles of great dimensions adapted for moving bulky loads or gear}	B62D55/06	B62D55/06		250
B62D55/065	9	Multi-track vehicles, i.e. more than two tracks {(soil-shifting machines E02F; mining machines E21C)}	B62D55/065	B62D55/065		2176
B62D55/0655	10	{Articulated endless track vehicles (steering specially adapted for trailers B62D13/00; articulated buses B62D47/025; tractor-trailer combinations or road trains comprising a uni-axle unit and a uni-axle trailer B62D53/02)}	B62D55/065	B62D55/065		296
B62D55/07	9	Mono-track vehicles	B62D55/07	B62D55/07		432
B62D55/075	9	Tracked vehicles for ascending or descending stairs, {steep slopes or vertical surfaces}(magnetic or pneumatic ground-engaging parts B62D55/265; chairs or multi-track cycles specially adapted for invalids A61G5/00)	B62D55/075	B62D55/075		1025
B62D55/08	8	Endless track units; Parts thereof	B62D55/08	B62D55/08		1867
B62D55/084	9	Endless-track units or carriages mounted separably, adjustably or extensibly on vehicles, e.g. portable track units (B62D55/07 takes precedence)	B62D55/084	B62D55/084		855
B62D55/0842	10	{Tracked vehicle with track carriages suspended on three points, e.g. by an equaliser bar}	B62D55/084	B62D55/084		329
B62D55/0845	10	{Protection devices}	B62D55/084	B62D55/084		114
B62D55/0847	10	{Track blocking devices mounted on the frame; Track guides}	B62D55/084	B62D55/084		154
B62D55/088	9	with means to exclude or remove foreign matter, e.g. sealing means, self-cleaning track links or sprockets, deflector plates or scrapers	B62D55/088	B62D55/088		359
B62D55/0882	10	{Track or sprocket cleaning devices mounted on the frame (wheel cleaning devices in general B60S)}	B62D55/088	B62D55/088		181
B62D55/0885	10	{Self-cleaning sprockets}	B62D55/088	B62D55/088		49
B62D55/0887	10	{Track-articulation sealings against dust, water, mud or the like (sealing of bearings in general F16C33/72; chain bushings in general F16G15/00)}	B62D55/088	B62D55/088		403
B62D55/092	9	with lubrication means (lubricating in general F16N)	B62D55/092	B62D55/092		275
B62D55/096	9	with noise reducing means	B62D55/096	B62D55/096		148
B62D55/0963	10	{Anti-noise driving sprockets}	B62D55/096	B62D55/096		144
B62D55/0966	10	{Low noise rollers, e.g. with antivibration means (elastic wheel rims in general B60B9/00)}	B62D55/096	B62D55/096		95
B62D55/10	9	Bogies; Frames (track-tensioning means B62D55/30)	B62D55/10	B62D55/10		1055
B62D55/104	9	Suspension devices for wheels, rollers, bogies or frames (vehicle suspension in general B60G)	B62D55/104	B62D55/104		495
B62D55/108	10	with mechanical springs, e.g. torsion bars	B62D55/108	B62D55/108		684
B62D55/1083	11	{Torsion-bar springs}	B62D55/108	B62D55/108		74
B62D55/1086	11	{Rubber springs}	B62D55/108	B62D55/108		84
B62D55/112	10	with fluid springs, e.g. hydraulic pneumatic	B62D55/112	B62D55/112		224
B62D55/1125	11	{Hydro-pneumatic or pneumatic, e.g. air-cushioned}	B62D55/112	B62D55/112		167
B62D55/116	10	Attitude or position control of chassis by action on suspension, e.g. to compensate for a slope	B62D55/116	B62D55/116		611
B62D55/12	9	Arrangement, location, or adaptation of driving sprockets	B62D55/12	B62D55/12		878
B62D55/125	10	Final drives	B62D55/125	B62D55/125		647
B62D55/13	11	readily interchangeable modular type	B62D55/13	B62D55/13		96
B62D55/135	10	with dismountable driving crown	B62D55/135	B62D55/135		86
B62D55/14	9	Arrangement, location, or adaptation of rollers	B62D55/14	B62D55/14		1148
B62D55/145	10	{Rollers with replaceable wear rings or rims (driving sprockets with replaceable rims B62D55/12)}	B62D55/14	B62D55/14		93
B62D55/15	10	Mounting devices, e.g. bushings, axles, bearings, sealings {(with lubrication means B62D55/092)}	B62D55/15	B62D55/15		761
B62D55/18	9	Tracks (self-cleaning track links B62D55/088)	B62D55/18	B62D55/18		311
B62D55/20	10	of articulated type, e.g. chains {(with lubrication means B62D55/092)}	B62D55/20	B62D55/20		616
B62D55/202	11	{Wheel engaging parts; Wheel guides on links}	B62D55/20	B62D55/20		274
B62D55/205	11	Connections between track links	B62D55/205	B62D55/205		436
B62D55/21	12	Links connected by transverse pivot pins	B62D55/21	B62D55/21		500
B62D55/211	13	{Bitubular chain links assembled by pins and double connectors}	B62D55/21	B62D55/21		267
B62D55/213	13	{Master track links}	B62D55/21	B62D55/21		166
B62D55/215	12	Resilient connections between links	B62D55/215	B62D55/215		106
B62D55/22	11	Arrangements for preventing or modifying back-flexing	B62D55/22	B62D55/22		148
B62D55/24	10	of continuously flexible type, e.g. rubber belts	B62D55/24	B62D55/24		1034
B62D55/242	11	{The flexible band being semi-rigid for resisting back-flexing and contributing to spring the vehicle}	B62D55/24	B62D55/24		33
B62D55/244	11	{Moulded in one piece, with either smooth surfaces or surfaces having projections, e.g. incorporating reinforcing elements}	B62D55/24	B62D55/24		697
B62D55/247	11	Gas filled or inflatable flexible tracks (connection of valves to inflatable elastic bodies B60C29/00)	B62D55/247	B62D55/247		117
B62D55/253	11	having elements interconnected by one or more cables or like elements	B62D55/253	B62D55/253		443
B62D55/26	10	Ground engaging parts or elements {(tracks specially adapted for amphibious vehicles B60F3/0015)}	B62D55/26	B62D55/26		775
B62D55/265	11	having magnetic or pneumatic adhesion	B62D55/265	B62D55/265		499
B62D55/27	11	having different types of crampons for progression over varying ground	B62D55/27	B62D55/27		152
B62D55/275	11	with street plate, i.e. means to prevent tread from cutting into road surface	B62D55/275	B62D55/275		270
B62D55/28	11	detachable	B62D55/28	B62D55/28		525
B62D55/283	12	{and movable, e.g. around an axis or perpendicularly to the track}	B62D55/28	B62D55/28		64
B62D55/286	12	{For soft grounds, e.g. consisting of snow or swamp}	B62D55/28	B62D55/28		175
B62D55/30	9	Track-tensioning means	B62D55/30	B62D55/30		1211
B62D55/305	10	{acting on pivotably mounted idlers}	B62D55/30	B62D55/30		448
B62D55/32	8	Assembly, disassembly, repair or servicing of endless-track systems	B62D55/32	B62D55/32		613
B62D57/00	7	Vehicles characterised by having other propulsion or other ground- engaging means than wheels or endless track, alone or in addition to wheels or endless track (sledges B62B; motor sledges B62M)	B62D57/00	B62D57/00		866
B62D57/02	8	with ground-engaging propulsion means, e.g. walking members	B62D57/02	B62D57/02		1969
B62D57/021	9	{the ground engaging means being sequentially inflatable bags for peristaltic movement (B62D57/024 takes precedence)}	B62D57/02	B62D57/02		68
B62D57/022	9	{consisting of members having both rotational and walking movements}	B62D57/02	B62D57/02		269
B62D57/024	9	specially adapted for moving on inclined or vertical surfaces (endless-track vehicles for ascending or descending stairs B62D55/075; hand-carts with provision for travelling up or down stairs B62B5/02)	B62D57/024	B62D57/024		3659
B62D57/028	9	having wheels and mechanical legs (B62D57/024 takes precedence; ground-engaging vehicle fittings for supporting, lifting or manoeuvring the vehicle, wholly or in part B60S9/00)	B62D57/028	B62D57/028		1365
B62D57/032	9	with alternately or sequentially lifted supporting base and legs; with alternately or sequentially lifted feet or skid (B62D57/024 takes precedence)	B62D57/032	B62D57/032		4616
B62D57/036	9	screw type, e.g. Archimedian screw {(amphibious vehicles comprising screw-type ground-engaging means B60F3/0023)}	B62D57/036	B62D57/036		234
B62D57/04	8	having other than ground-engaging propulsion means, e.g. having propellers (arrangement of jet-propulsion units B60K)	B62D57/04	B62D57/04		285
B62D59/00	7	Trailers with driven ground wheels or the like	B62D59/00	B62D59/00		150
B62D59/02	8	driven from external propulsion unit	B62D59/02	B62D59/02		510
B62D59/04	8	driven from propulsion unit on trailer	B62D59/04	B62D59/04		905
B62D61/00	7	Motor vehicles or trailers, characterised by the arrangement or number of wheels, not otherwise provided for, e.g. four wheels in diamond pattern	B62D61/00	B62D61/00		828
B62D61/02	8	with two road wheels in tandem on the longitudinal centre line of the vehicle	B62D61/02	B62D61/02		301
B62D61/04	9	with two other wheels which are coaxial	B62D61/04	B62D61/04		186
B62D61/06	8	with only three wheels	B62D61/06	B62D61/06		254
B62D61/065	9	{with single rear wheel}	B62D61/06	B62D61/06		423
B62D61/08	9	with single front wheel	B62D61/08	B62D61/08		673
B62D61/10	8	with more than four wheels {(tractors of the low ground pressure type B62D49/002)}	B62D61/10	B62D61/10		1361
B62D61/12	8	with variable number of ground engaging wheels, e.g. with some wheels arranged higher than others, or with retractable wheels (for manoeuvring purposes only B60S)	B62D61/12	B62D61/12		1419
B62D61/125	9	{the retractable wheel being a part of a set of tandem wheels (resilient suspension for a single set of tandem wheels B60G5/00)}	B62D61/12	B62D61/12		522
B62D63/00	7	Motor vehicles or trailers not otherwise provided for	B62D63/00	B62D63/00		186
B62D63/02	8	Motor vehicles	B62D63/02	B62D63/02		3554
B62D63/025	9	{Modular vehicles (superstructures for busses having modular sections B62D31/025)}	B62D63/02	B62D63/02		1038
B62D63/04	9	Component parts or accessories	B62D63/04	B62D63/04		3362
B62D63/06	8	Trailers (vehicles comprising living accommodation for people, e.g. caravans, camping or like vehicles B60P3/32)	B62D63/06	B62D63/06		1324
B62D63/061	9	{Foldable, extensible or yielding trailers (foldable caravans B60P3/34; adjustable chassis frames B62D21/14)}	B62D63/06	B62D63/06		1224
B62D63/062	9	{Trailers with one axle or two wheels (semi-trailers B62D53/06)}	B62D63/06	B62D63/06		770
B62D63/064	10	{light luggage or equipment trailers, e.g. for batteries, gas generators, gas bottles, stretchers (luggage carriers per seB60R)}	B62D63/06	B62D63/06		409
B62D63/065	10	{forming an extension of the towing vehicle, i.e. with two point fixation}	B62D63/06	B62D63/06		185
B62D63/067	11	{single wheeled (rigid or semi-rigid couping)}	B62D63/06	B62D63/06		221
B62D63/068	9	{with more than two axles or more than four wheels (vehicles with more than four wheels in general B62D61/10)}	B62D63/06	B62D63/06		261
B62D63/08	9	Component parts or accessories	B62D63/08	B62D63/08		1339
B62D65/00	7	Designing, manufacturing, e.g. assembling, facilitating disassembly, or structurally modifying motor vehicles or trailers, not otherwise provided for	B62D65/00	B62D65/00		1847
B62D65/005	8	{Inspection and final control devices}	B62D65/00	B62D65/00		650
B62D65/02	8	Joining sub-units or components to, or positioning sub-units or components with respect to, body shell or other sub-units or components	B62D65/02	B62D65/02		1876
B62D65/022	9	{Transferring or handling sub-units or components, e.g. in work stations or between workstations and transportation systems}	B62D65/02	B62D65/02		922
B62D65/024	9	{Positioning of sub-units or components with respect to body shell or other sub-units or components}	B62D65/02	B62D65/02		941
B62D65/026	10	{by using a jig or the like; Positioning of the jig}	B62D65/02	B62D65/02		1197
B62D65/028	10	{by determining relative positions by measurement}	B62D65/02	B62D65/02		237
B62D65/04	9	Joining preassembled modular units composed of sub-units performing diverse functions, e.g. engine and bonnet (B62D65/06&#160;-&#160;B62D65/16 take precedence)	B62D65/04	B62D65/04		698
B62D65/06	9	the sub-units or components being doors, windows, openable roofs, lids, bonnets, or weather strips or seals therefor {(assembling sealing arrangements with vehicle parts, e.g. doors, windows B60J10/45)}	B62D65/06	B62D65/06		2252
B62D65/10	9	the sub-units or components being engines, clutches or transmissions	B62D65/10	B62D65/10		473
B62D65/12	9	the sub-units or components being suspensions, brakes or wheel units	B62D65/12	B62D65/12		751
B62D65/14	9	the sub-units or components being passenger compartment fittings, e.g. seats, linings, trim, instrument panels	B62D65/14	B62D65/14		978
B62D65/16	9	the sub-units or components being exterior fittings, e.g. bumpers, lights, wipers {, exhausts}	B62D65/16	B62D65/16		785
B62D65/18	9	Transportation, conveyor or haulage systems specially adapted for motor vehicle or trailer assembly lines {(conveyors and haulage in general B65G)}	B62D65/18	B62D65/18		2911
B62D67/00	7	Systematic disassembly of vehicles for recovery of salvageable components, e.g. for recycling (for disposal of vehicles by destroying or transformation B09B3/00, B09B5/00{; general arrangement of separating plants B03B9/00; recovery of plastics B29B17/00})	B62D67/00	B62D67/00		419
