B22D1/00	7	Treatment of fused masses in the ladle or the supply runners before casting {(for continuous casting B22D11/10; metallurgical processing, e.g. refining of iron or other metal C21, C22, C25C)}	B22D1/00	B22D1/00		2248
B22D1/002	8	{Treatment with gases (C21C7/072, C22B9/05 take precedence)}	B22D1/00	B22D1/00		352
B22D1/005	9	{Injection assemblies therefor (features relating to gas injection, provided on closures of the sliding gate type B22D41/42; provided on pouring nozzles B22D41/58; provided on closures of the stopper-rod type B22D41/186)}	B22D1/00	B22D1/00		904
B22D1/007	8	{Treatment of the fused masses in the supply runners (B22D1/002, B22D1/005 take precedence)}	B22D1/00	B22D1/00		296
B22D2/00	7	Arrangement of indicating or measuring devices, e.g. for temperature or viscosity of the fused mass	B22D2/00	B22D2/00		1635
B22D2/001	8	{for the slag appearance in a molten metal stream}	B22D2/00	B22D2/00		112
B22D2/003	8	{for the level of the molten metal (B22D11/181 and B22D11/201 take precedence; level indicators in general G01F23/00)}	B22D2/00	B22D2/00		263
B22D2/005	8	{for the thickness of a frozen shell (B22D11/188 and B22D11/207 take precedence)}	B22D2/00	B22D2/00		22
B22D2/006	8	{for the temperature of the molten metal (measuring temperature in general G01K)}	B22D2/00	B22D2/00		476
B22D2/008	8	{for the viscosity of the molten metal (measuring viscosity in general G01N11/00)}	B22D2/00	B22D2/00		24
B22D3/00	7	Pig or like casting (equipment for conveying molten metal B22D35/00)	B22D3/00	B22D3/00		140
B22D3/02	8	Moulding of beds	B22D3/02	B22D3/02		33
B22D5/00	7	Machines or plants for pig or like casting	B22D5/00	B22D5/00		102
B22D5/005	8	{Devices for stacking pigs; Pigforms to be stacked}	B22D5/00	B22D5/00		134
B22D5/02	8	with rotary casting tables	B22D5/02	B22D5/02		229
B22D5/04	8	with endless casting conveyors	B22D5/04	B22D5/04		272
B22D7/00	7	Casting ingots, {e.g. from ferrous metals}(equipment for conveying molten metal B22D35/00)	B22D7/00	B22D7/00		996
B22D7/005	8	{from non-ferrous metals}	B22D7/00	B22D7/00		1583
B22D7/02	8	Casting compound ingots of two or more different metals in the molten state, i.e. integrally cast	B22D7/02	B22D7/02		399
B22D7/04	8	Casting hollow ingots	B22D7/04	B22D7/04		196
B22D7/06	8	Ingot moulds or their manufacture	B22D7/06	B22D7/06		832
B22D7/062	9	{Stools for ingot moulds}	B22D7/06	B22D7/06		180
B22D7/064	9	{Cooling the ingot moulds}	B22D7/06	B22D7/06		275
B22D7/066	9	{Manufacturing, repairing or reinforcing ingot moulds}	B22D7/06	B22D7/06		176
B22D7/068	10	{characterised by the materials used therefor}	B22D7/06	B22D7/06		85
B22D7/08	9	Divided ingot moulds	B22D7/08	B22D7/08		245
B22D7/10	9	Hot tops therefor {(heating the top discard of ingots B22D27/06)}	B22D7/10	B22D7/10		1147
B22D7/102	10	{from refractorial material only}	B22D7/10	B22D7/10		87
B22D7/104	10	{from exothermic material only}	B22D7/10	B22D7/10		172
B22D7/106	10	{Configuration of hot tops}	B22D7/10	B22D7/10		113
B22D7/108	10	{Devices for making or fixing hot tops}	B22D7/10	B22D7/10		310
B22D7/12	8	Appurtenances, e.g. for sintering, for preventing splashing	B22D7/12	B22D7/12		706
B22D9/00	7	Machines or plants for casting ingots	B22D9/00	B22D9/00		306
B22D9/003	8	{for top casting}	B22D9/00	B22D9/00		174
B22D9/006	8	{for bottom casting}	B22D9/00	B22D9/00		112
B22D11/00	7	Continuous casting of metals, i.e. casting in indefinite lengths (metal drawing, metal extruding B21C)	B22D11/00	B22D11/00		804
B22D11/001	8	{of specific alloys}	B22D11/00	B22D11/00		2144
B22D11/002	9	{Stainless steels}	B22D11/00	B22D11/00		258
B22D11/003	9	{Aluminium alloys}	B22D11/00	B22D11/00		995
B22D11/004	9	{Copper alloys}	B22D11/00	B22D11/00		755
B22D11/005	8	{of wire (casting on wire B22D19/14)}	B22D11/00	B22D11/00		683
B22D11/006	8	{of tubes}	B22D11/00	B22D11/00		576
B22D11/007	8	{of composite ingots, i.e. two or more molten metals of different compositions being used to integrally cast the ingots (casting of composite ingots in definite lengths B22D7/02)}	B22D11/00	B22D11/00		209
B22D11/008	8	{of clad ingots, i.e. the molten metal being cast against a continuous strip forming part of the cast product}	B22D11/00	B22D11/00		355
B22D11/009	8	{of work of special cross-section, e.g. I-beams, U-profiles}	B22D11/00	B22D11/00		162
B22D11/01	8	without moulds, e.g. on molten surfaces	B22D11/01	B22D11/01		109
B22D11/015	9	{using magnetic field for conformation, i.e. the metal is not in contact with a mould}	B22D11/01	B22D11/01		220
B22D11/04	8	into open-ended moulds (B22D11/06, B22D11/07 take precedence; plants for continuous casting, e.g. for upwardly drawing the strand B22D11/14)	B22D11/04	B22D11/04		974
B22D11/0401	9	{Moulds provided with a feed head}	B22D11/04	B22D11/04		218
B22D11/0403	9	{Multiple moulds}	B22D11/04	B22D11/04		122
B22D11/0405	9	{Rotating moulds}	B22D11/04	B22D11/04		60
B22D11/0406	9	{Moulds with special profile}	B22D11/04	B22D11/04		285
B22D11/0408	9	{Moulds for casting thin slabs}	B22D11/04	B22D11/04		177
B22D11/041	9	for vertical casting (B22D11/043, B22D11/049&#160;-&#160;B22D11/059 take precedence)	B22D11/041	B22D11/041		693
B22D11/043	9	Curved moulds (B22D11/049&#160;-&#160;B22D11/059 take precedence)	B22D11/043	B22D11/043		194
B22D11/045	9	for horizontal casting (B22D11/049&#160;-&#160;B22D11/059 take precedence)	B22D11/045	B22D11/045		487
B22D11/0455	10	{Bidirectional horizontal casting}	B22D11/045	B22D11/045		42
B22D11/047	10	Means for joining tundish to mould	B22D11/047	B22D11/047		225
B22D11/0475	11	{characterised by use of a break ring}	B22D11/047	B22D11/047		65
B22D11/049	9	for direct chill casting, e.g. electromagnetic casting	B22D11/049	B22D11/049		383
B22D11/05	9	into moulds having adjustable walls	B22D11/05	B22D11/05		367
B22D11/051	9	into moulds having oscillating walls	B22D11/051	B22D11/051		77
B22D11/053	9	Means for oscillating the moulds	B22D11/053	B22D11/053		799
B22D11/0535	10	{in a horizontal plane}	B22D11/053	B22D11/053		44
B22D11/055	9	Cooling the moulds {(B22D11/04 takes precedence)}	B22D11/055	B22D11/055		1191
B22D11/057	9	Manufacturing or calibrating the moulds	B22D11/057	B22D11/057		320
B22D11/059	9	Mould materials or platings	B22D11/059	B22D11/059		844
B22D11/06	8	into moulds with travelling walls, e.g. with rolls, plates, belts, caterpillars	B22D11/06	B22D11/06		1099
B22D11/0602	9	{formed by a casting wheel and belt, e.g. Properzi-process}	B22D11/06	B22D11/06		289
B22D11/0605	9	{formed by two belts, e.g. Hazelett-process}	B22D11/06	B22D11/06		402
B22D11/0608	9	{formed by caterpillars}	B22D11/06	B22D11/06		222
B22D11/0611	9	{formed by a single casting wheel, e.g. for casting amorphous metal strips or wires}	B22D11/06	B22D11/06		1174
B22D11/0614	10	{the casting wheel being immersed in a molten metal bath, and drawing out upwardly the casting strip}	B22D11/06	B22D11/06		68
B22D11/0617	10	{the casting wheel having its axis vertical and a casting strip formed in a peripheral groove of the wheel}	B22D11/06	B22D11/06		40
B22D11/062	10	{the metal being cast on the inside surface of the casting wheel}	B22D11/06	B22D11/06		91
B22D11/0622	9	{formed by two casting wheels}	B22D11/06	B22D11/06		1996
B22D11/0625	10	{the two casting wheels being immersed in a molten metal bath and drawing out upwardly the casting strip}	B22D11/06	B22D11/06		54
B22D11/0628	9	{formed by more than two casting wheels}	B22D11/06	B22D11/06		67
B22D11/0631	9	{formed by a travelling straight surface, e.g. through-like moulds, a belt}	B22D11/06	B22D11/06		257
B22D11/0634	9	{formed by a casting wheel and a co-operating shoe}	B22D11/06	B22D11/06		67
B22D11/0637	9	{Accessories therefor}	B22D11/06	B22D11/06		128
B22D11/064	10	{for supplying molten metal (supplying molten metal to open-ended moulds B22D11/10)}	B22D11/06	B22D11/06		683
B22D11/0642	11	{Nozzles (nozzles used in open-ended moulds B22D41/50)}	B22D11/06	B22D11/06		562
B22D11/0645	11	{Sealing means for the nozzle between the travelling surfaces}	B22D11/06	B22D11/06		69
B22D11/0648	10	{Casting surfaces}	B22D11/06	B22D11/06		25
B22D11/0651	11	{Casting wheels (B22D11/0682 takes precedence)}	B22D11/06	B22D11/06		444
B22D11/0654	11	{Casting belts (B22D11/0685 takes precedence)}	B22D11/06	B22D11/06		86
B22D11/0657	11	{Caterpillars (B22D11/0688 takes precedence)}	B22D11/06	B22D11/06		30
B22D11/066	11	{Side dams (B22D11/0691 takes precedence)}	B22D11/06	B22D11/06		519
B22D11/0662	12	{having electromagnetic confining means}	B22D11/06	B22D11/06		36
B22D11/0665	10	{for treating the casting surfaces, e.g. calibrating, cleaning, dressing, preheating}	B22D11/06	B22D11/06		149
B22D11/0668	11	{for dressing, coating or lubricating}	B22D11/06	B22D11/06		190
B22D11/0671	11	{for heating or drying}	B22D11/06	B22D11/06		105
B22D11/0674	11	{for machining}	B22D11/06	B22D11/06		68
B22D11/0677	10	{for guiding, supporting or tensioning the casting belts}	B22D11/06	B22D11/06		220
B22D11/068	10	{for cooling the cast product during its passage through the mould surfaces (cooling open-ended moulds B22D11/04; secondary cooling B22D11/124)}	B22D11/06	B22D11/06		94
B22D11/0682	11	{by cooling the casting wheel}	B22D11/06	B22D11/06		518
B22D11/0685	11	{by cooling the casting belts (B22D11/0677 takes precedence)}	B22D11/06	B22D11/06		136
B22D11/0688	11	{by cooling the caterpillars}	B22D11/06	B22D11/06		33
B22D11/0691	11	{by cooling the side dams}	B22D11/06	B22D11/06		22
B22D11/0694	10	{for peeling-off or removing the cast product}	B22D11/06	B22D11/06		183
B22D11/0697	10	{for casting in a protected atmosphere}	B22D11/06	B22D11/06		289
B22D11/07	8	Lubricating the moulds	B22D11/07	B22D11/07		608
B22D11/08	8	Accessories for starting the casting procedure	B22D11/08	B22D11/08		480
B22D11/081	9	{Starter bars}	B22D11/08	B22D11/08		201
B22D11/083	10	{Starter bar head; Means for connecting or detaching starter bars and ingots}	B22D11/08	B22D11/08		284
B22D11/085	9	{Means for storing or introducing the starter bars in the moulds}	B22D11/08	B22D11/08		154
B22D11/086	9	{Means for connecting cast ingots of different sizes or compositions}	B22D11/08	B22D11/08		62
B22D11/088	9	{Means for sealing the starter bar head in the moulds}	B22D11/08	B22D11/08		83
B22D11/10	8	Supplying or treating molten metal (B22D41/00 takes precedence)	B22D11/10	B22D11/10		2179
B22D11/103	9	Distributing the molten metal, e.g. using runners, floats, distributors	B22D11/103	B22D11/103		612
B22D11/106	9	Shielding the molten jet {(B22D41/50 takes precedence)}	B22D11/106	B22D11/106		247
B22D11/108	9	Feeding additives, powders, or the like	B22D11/108	B22D11/108		953
B22D11/11	9	Treating the molten metal	B22D11/11	B22D11/11		1012
B22D11/111	10	by using protecting powders	B22D11/111	B22D11/111		1657
B22D11/112	10	by accelerated cooling	B22D11/112	B22D11/112		245
B22D11/113	10	by vacuum treating	B22D11/113	B22D11/113		265
B22D11/114	10	by using agitating or vibrating means (B22D11/117 takes precedence)	B22D11/114	B22D11/114		382
B22D11/115	11	by using magnetic fields	B22D11/115	B22D11/115		2080
B22D11/116	10	Refining the metal	B22D11/116	B22D11/116		233
B22D11/117	11	by treating with gases (B22D11/118, B22D11/119 take precedence)	B22D11/117	B22D11/117		432
B22D11/118	11	by circulating the metal under, over or around weirs (B22D11/119 takes precedence)	B22D11/118	B22D11/118		283
B22D11/119	11	by filtering	B22D11/119	B22D11/119		274
B22D11/12	8	Accessories for subsequent treating or working cast stock in situ(rolling immediately subsequent to continuous casting B21B1/46, B21B13/22)	B22D11/12	B22D11/12		853
B22D11/1206	9	{for plastic shaping of strands (rolling mills B21B1/46)}	B22D11/12	B22D11/12		1200
B22D11/1213	9	{for heating or insulating strands}	B22D11/12	B22D11/12		304
B22D11/122	9	{using magnetic fields}	B22D11/12	B22D11/12		506
B22D11/1226	9	{for straightening strands}	B22D11/12	B22D11/12		243
B22D11/1233	9	{for marking strands}	B22D11/12	B22D11/12		56
B22D11/124	9	for cooling	B22D11/124	B22D11/124		1543
B22D11/1241	10	{by transporting the cast stock through a liquid medium bath or a fluidized bed}	B22D11/124	B22D11/124		85
B22D11/1243	10	{by using cooling grids or cooling plates}	B22D11/124	B22D11/124		101
B22D11/1245	10	{using specific cooling agents}	B22D11/124	B22D11/124		78
B22D11/1246	10	{Nozzles; Spray heads}	B22D11/124	B22D11/124		627
B22D11/1248	10	{Means for removing cooling agent from the surface of the cast stock}	B22D11/124	B22D11/124		55
B22D11/126	9	for cutting	B22D11/126	B22D11/126		1222
B22D11/1265	10	{having auxiliary devices for deburring}	B22D11/126	B22D11/126		146
B22D11/128	9	for removing	B22D11/128	B22D11/128		1002
B22D11/1281	10	{Vertical removing}	B22D11/128	B22D11/128		156
B22D11/1282	10	{Vertical casting and curving the cast stock to the horizontal}	B22D11/128	B22D11/128		454
B22D11/1284	10	{Horizontal removing}	B22D11/128	B22D11/128		253
B22D11/1285	10	{Segment changing devices for supporting or guiding frames}	B22D11/128	B22D11/128		124
B22D11/1287	10	{Rolls; Lubricating, cooling or heating rolls while in use}	B22D11/128	B22D11/128		1259
B22D11/1288	10	{Walking bar members}	B22D11/128	B22D11/128		40
B22D11/14	8	Plants for continuous casting	B22D11/14	B22D11/14		602
B22D11/141	9	{for vertical casting}	B22D11/14	B22D11/14		406
B22D11/142	9	{for curved casting}	B22D11/14	B22D11/14		239
B22D11/143	9	{for horizontal casting}	B22D11/14	B22D11/14		276
B22D11/144	9	{with a rotating mould}	B22D11/14	B22D11/14		118
B22D11/145	9	{for upward casting}	B22D11/14	B22D11/14		411
B22D11/146	9	{for inclined casting}	B22D11/14	B22D11/14		36
B22D11/147	9	{Multi-strand plants}	B22D11/14	B22D11/14		273
B22D11/148	9	{Safety arrangements}	B22D11/14	B22D11/14		122
B22D11/16	8	Controlling or regulating processes or operations	B22D11/16	B22D11/16		3599
B22D11/161	9	{for automatic starting the casting process}	B22D11/16	B22D11/16		103
B22D11/163	9	{for cutting cast stock}	B22D11/16	B22D11/16		261
B22D11/165	9	{for the supply of casting powder}	B22D11/16	B22D11/16		156
B22D11/166	9	{for mould oscillation}	B22D11/16	B22D11/16		241
B22D11/168	9	{for adjusting the mould size or mould taper}	B22D11/16	B22D11/16		261
B22D11/18	9	for pouring (B22D11/20 takes precedence)	B22D11/18	B22D11/18		1513
B22D11/181	10	{responsive to molten metal level or slag level}	B22D11/18	B22D11/18		462
B22D11/182	11	{by measuring temperature}	B22D11/18	B22D11/18		667
B22D11/183	11	{by measuring molten metal weight}	B22D11/18	B22D11/18		105
B22D11/185	11	{by using optical means}	B22D11/18	B22D11/18		165
B22D11/186	11	{by using electric, magnetic, sonic or ultrasonic means}	B22D11/18	B22D11/18		274
B22D11/187	11	{by using X-rays or nuclear radiation}	B22D11/18	B22D11/18		61
B22D11/188	10	{responsive to thickness of solidified shell}	B22D11/18	B22D11/18		54
B22D11/20	9	for removing cast stock	B22D11/20	B22D11/20		1385
B22D11/201	10	{responsive to molten metal level or slag level}	B22D11/20	B22D11/20		108
B22D11/202	11	{by measuring temperature}	B22D11/20	B22D11/20		140
B22D11/203	11	{by measuring molten metal weight}	B22D11/20	B22D11/20		18
B22D11/204	11	{by using optical means}	B22D11/20	B22D11/20		46
B22D11/205	11	{by using electric, magnetic, sonic or ultrasonic means}	B22D11/20	B22D11/20		48
B22D11/206	11	{by using X-rays or nuclear radiation}	B22D11/20	B22D11/20		37
B22D11/207	10	{responsive to thickness of solidified shell}	B22D11/20	B22D11/20		113
B22D11/208	10	{for aligning the guide rolls}	B22D11/20	B22D11/20		213
B22D11/22	9	for cooling cast stock or mould	B22D11/22	B22D11/22		1032
B22D11/225	10	{for secondary cooling}	B22D11/22	B22D11/22		1371
B22D13/00	7	Centrifugal casting; Casting by using centrifugal force	B22D13/00	B22D13/00		1078
B22D13/02	8	of elongated solid or hollow bodies, e.g. pipes, in moulds rotating around their longitudinal axis	B22D13/02	B22D13/02		894
B22D13/023	9	{the longitudinal axis being horizontal}	B22D13/02	B22D13/02		571
B22D13/026	9	{the longitudinal axis being vertical}	B22D13/02	B22D13/02		168
B22D13/04	8	of shallow solid or hollow bodies, e.g. wheels or rings, in moulds rotating around their axis of symmetry	B22D13/04	B22D13/04		720
B22D13/06	8	of solid or hollow bodies in moulds rotating around an axis arranged outside the mould	B22D13/06	B22D13/06		268
B22D13/063	9	{for dentistry or jewellery}	B22D13/06	B22D13/06		108
B22D13/066	9	{several moulds being disposed in a circle}	B22D13/06	B22D13/06		165
B22D13/08	8	in which a stationary mould is fed from a rotating mass of liquid metal	B22D13/08	B22D13/08		58
B22D13/10	8	Accessories for centrifugal casting apparatus, e.g. moulds, linings therefor, means for feeding molten metal, cleansing moulds, removing castings (making or lining moulds B22C)	B22D13/10	B22D13/10		799
B22D13/101	9	{Moulds}	B22D13/10	B22D13/10		711
B22D13/102	10	{Linings for moulds (making or lining moulds B22C)}	B22D13/10	B22D13/10		453
B22D13/104	10	{Cores}	B22D13/10	B22D13/10		243
B22D13/105	10	{Cooling for moulds or cores}	B22D13/10	B22D13/10		281
B22D13/107	9	{Means for feeding molten metal}	B22D13/10	B22D13/10		532
B22D13/108	9	{Removing of casting}	B22D13/10	B22D13/10		290
B22D13/12	8	Controlling, supervising, specially adapted to centrifugal casting, e.g. for safety reasons (controlling or regulating in general G05)	B22D13/12	B22D13/12		352
B22D15/00	7	Casting using a mould or core of which a part significant to the process is of high thermal conductivity, e.g. chill casting; Moulds or accessories specially adapted therefor	B22D15/00	B22D15/00		779
B22D15/005	8	{of rolls, wheels or the like (B22D19/16 takes precedence)}	B22D15/00	B22D15/00		392
B22D15/02	8	of cylinders, pistons, bearing shells or like thin-walled objects	B22D15/02	B22D15/02		892
B22D15/04	8	Machines or apparatus for chill casting ({B22D15/005}, B22D15/02 take precedence)	B22D15/04	B22D15/04		200
B22D17/00	7	Pressure die casting or injection die casting, i.e. casting in which the metal is forced into a mould under high pressure	B22D17/00	B22D17/00		2600
B22D17/002	8	{using movable moulds (for plastics B29C45/04)}	B22D17/00	B22D17/00		165
B22D17/005	8	{using two or more fixed moulds (for plastics B29C45/12)}	B22D17/00	B22D17/00		85
B22D17/007	8	{Semi-solid pressure die casting}	B22D17/00	B22D17/00		1126
B22D17/02	8	Hot chamber machines, i.e. with heated press chamber in which metal is melted	B22D17/02	B22D17/02		227
B22D17/04	9	Plunger machines	B22D17/04	B22D17/04		584
B22D17/06	9	Air injection machines	B22D17/06	B22D17/06		316
B22D17/08	8	Cold chamber machines, i.e. with unheated press chamber into which molten metal is ladled	B22D17/08	B22D17/08		281
B22D17/10	9	with horizontal press motion	B22D17/10	B22D17/10		497
B22D17/12	9	with vertical press motion	B22D17/12	B22D17/12		388
B22D17/14	8	Machines with evacuated die cavity	B22D17/14	B22D17/14		951
B22D17/145	9	{Venting means therefor (for permanent moulds B22C9/067)}	B22D17/14	B22D17/14		426
B22D17/16	8	specially adapted for casting slide fasteners or elements therefor	B22D17/16	B22D17/16		35
B22D17/18	8	Machines built up from units providing for different combinations	B22D17/18	B22D17/18		38
B22D17/20	8	Accessories: Details	B22D17/20	B22D17/20		1529
B22D17/2007	9	{Methods or apparatus for cleaning or lubricating moulds}	B22D17/20	B22D17/20		873
B22D17/2015	9	{Means for forcing the molten metal into the die (for plastics B29C45/46)}	B22D17/20	B22D17/20		696
B22D17/2023	10	{Nozzles or shot sleeves}	B22D17/20	B22D17/20		509
B22D17/203	10	{Injection pistons (B22D17/2053 takes precedence; for plastics B29C45/53)}	B22D17/20	B22D17/20		560
B22D17/2038	10	{Heating, cooling or lubricating the injection unit (for plastics B29C45/74, B29C45/83)}	B22D17/20	B22D17/20		484
B22D17/2046	10	{with provisions for damping the pressure peak}	B22D17/20	B22D17/20		28
B22D17/2053	10	{using two or more cooperating injection pistons}	B22D17/20	B22D17/20		81
B22D17/2061	10	{using screws}	B22D17/20	B22D17/20		87
B22D17/2069	10	{Exerting after-pressure on the moulding material}	B22D17/20	B22D17/20		215
B22D17/2076	9	{Cutting-off equipment for sprues or ingates (for plastics B29C45/38)}	B22D17/20	B22D17/20		388
B22D17/2084	9	{Manipulating or transferring devices for evacuating cast pieces}	B22D17/20	B22D17/20		506
B22D17/2092	9	{Safety devices (for plastics B29C45/84)}	B22D17/20	B22D17/20		101
B22D17/22	9	Dies (manufacture, see the appropriate class, e.g. B23P15/24); Die plates; Die supports; Cooling equipment for dies; Accessories for loosening and ejecting castings from dies	B22D17/22	B22D17/22		3364
B22D17/2209	10	{Selection of die materials (for permanent moulds B22C9/061)}	B22D17/22	B22D17/22		299
B22D17/2218	10	{Cooling or heating equipment for dies (for permanent moulds B22C9/065; for plastics B29C45/73)}	B22D17/22	B22D17/22		1557
B22D17/2227	10	{Die seals (for plastics B29C45/2608)}	B22D17/22	B22D17/22		187
B22D17/2236	10	{Equipment for loosening or ejecting castings from dies (for plastics B29C45/40)}	B22D17/22	B22D17/22		1189
B22D17/2245	10	{having walls provided with means for marking or patterning}	B22D17/22	B22D17/22		74
B22D17/2254	10	{having screw-threaded die walls}	B22D17/22	B22D17/22		28
B22D17/2263	10	{having tubular die cavities}	B22D17/22	B22D17/22		41
B22D17/2272	10	{Sprue channels}	B22D17/22	B22D17/22		567
B22D17/2281	11	{closure devices therefor}	B22D17/22	B22D17/22		80
B22D17/229	10	{with exchangeable die part (B22D17/2245 takes precedence)}	B22D17/22	B22D17/22		181
B22D17/24	10	Accessories for locating and holding cores or inserts	B22D17/24	B22D17/24		916
B22D17/26	9	Mechanisms or devices for locking or opening dies	B22D17/26	B22D17/26		738
B22D17/263	10	{mechanically}	B22D17/26	B22D17/26		249
B22D17/266	10	{hydraulically}	B22D17/26	B22D17/26		321
B22D17/28	9	Melting pots	B22D17/28	B22D17/28		419
B22D17/30	9	Accessories for supplying molten metal, e.g. in rations (supplying molten metal in ration in general B22D39/00)	B22D17/30	B22D17/30		1439
B22D17/32	9	Controlling equipment	B22D17/32	B22D17/32		2317
B22D18/00	7	Pressure casting; Vacuum casting (B22D17/00 takes precedence; treating the metal in the mould by using pressure or vacuum B22D27/00)	B22D18/00	B22D18/00		223
B22D18/02	8	Pressure casting making use of mechanical pressure devices, e.g. cast-forging (B22D18/04 takes precedence)	B22D18/02	B22D18/02		1723
B22D18/04	8	Low pressure casting, i.e. making use of pressures up to a few bars to fill the mould	B22D18/04	B22D18/04		3066
B22D18/06	8	Vacuum casting, i.e. making use of vacuum to fill the mould	B22D18/06	B22D18/06		1579
B22D18/08	8	Controlling, supervising, e.g. for safety reasons (controlling or regulating in general G05)	B22D18/08	B22D18/08		629
B22D19/00	7	Casting in, on, or around objects which form part of the product (B22D23/04 takes precedence; alumino-thermic welding B23K23/00; coating by casting molten material on the substrate C23C6/00)	B22D19/00	B22D19/00		2444
B22D19/0009	8	{Cylinders, pistons}	B22D19/00	B22D19/00		657
B22D19/0018	9	{cylinders with fins}	B22D19/00	B22D19/00		77
B22D19/0027	9	{pistons}	B22D19/00	B22D19/00		279
B22D19/0036	8	{gears}	B22D19/00	B22D19/00		49
B22D19/0045	8	{household utensils}	B22D19/00	B22D19/00		139
B22D19/0054	8	{rotors, stators for electrical motors}	B22D19/00	B22D19/00		279
B22D19/0063	8	{finned exchangers (cylinders B22D19/0018)}	B22D19/00	B22D19/00		96
B22D19/0072	8	{for making objects with integrated channels}	B22D19/00	B22D19/00		444
B22D19/0081	8	{pretreatment of the insert, e.g. for enhancing the bonding between insert and surrounding cast metal}	B22D19/00	B22D19/00		614
B22D19/009	8	{for casting objects the members of which can be separated afterwards}	B22D19/00	B22D19/00		36
B22D19/02	8	for making reinforced articles (B22D19/14 takes precedence)	B22D19/02	B22D19/02		677
B22D19/04	8	for joining parts	B22D19/04	B22D19/04		1142
B22D19/045	9	{for joining tubes}	B22D19/04	B22D19/04		70
B22D19/06	8	for manufacturing or repairing tools	B22D19/06	B22D19/06		406
B22D19/08	8	for building-up linings or coverings, e.g. of anti-frictional metal	B22D19/08	B22D19/08		715
B22D19/085	9	{of anti-frictional metal}	B22D19/08	B22D19/08		686
B22D19/10	8	Repairing defective or damaged objects by metal casting procedures (by other procedures B23P6/04; ingot mould B22D7/06; B22D19/06 takes precedence)	B22D19/10	B22D19/10		143
B22D19/12	8	for making objects, e.g. hinges, with parts which are movable relatively to one another	B22D19/12	B22D19/12		114
B22D19/14	8	the objects being filamentary or particulate in form (making alloys containing fibres or filaments by contacting the fibres or filaments with molten metal C22C47/08)	B22D19/14	B22D19/14		883
B22D19/16	8	for making compound objects cast of two or more different metals, e.g. for making rolls for rolling mills (casting compound ingots B22D7/02)	B22D19/16	B22D19/16		2013
B22D21/00	7	Casting non-ferrous metals or metallic compounds so far as their metallurgical properties are of importance for the casting procedure; Selection of compositions therefor {(non-ferrous ingots B22D7/005)}	B22D21/00	B22D21/00		210
B22D21/002	8	{Castings of light metals}	B22D21/00	B22D21/00		39
B22D21/005	9	{with high melting point, e.g. Be 1280 degrees C, Ti 1725 degrees C}	B22D21/00	B22D21/00		259
B22D21/007	9	{with low melting point, e.g. Al 659 degrees C, Mg 650 degrees C}	B22D21/00	B22D21/00		1518
B22D21/02	8	Casting exceedingly oxidisable non-ferrous metals, e.g. in inert atmosphere (use of inert atmosphere in casting metals in general B22D23/00; apparatus for vacuum casting B22D27/15)	B22D21/02	B22D21/02		79
B22D21/022	9	{Casting heavy metals, with exceedingly high melting points, i.e. more than 1600 degrees C, e.g. W 3380 degrees C, Ta 3000 degrees C, Mo 2620 degrees C, Zr 1860 degrees C, Cr 1765 degrees C, V 1715 degrees C}	B22D21/02	B22D21/02		74
B22D21/025	9	{Casting heavy metals with high melting point, i.e. 1000 - 1600 degrees C, e.g. Co 1490 degrees C, Ni 1450 degrees C, Mn 1240 degrees C, Cu 1083 degrees C}	B22D21/02	B22D21/02		262
B22D21/027	9	{Casting heavy metals with low melting point, i.e. less than 1000 degrees C, e.g. Zn 419 degrees C, Pb 327 degrees C, Sn 232 degrees C}	B22D21/02	B22D21/02		173
B22D21/04	9	Casting aluminium or magnesium {(no material; seeB22D21/007)}	B22D21/04	B22D21/04		1316
B22D21/06	8	Casting non-ferrous metals with a high melting point, e.g. metallic carbides (B22D21/02 takes precedence)	B22D21/06	B22D21/06		96
B22D23/00	7	Casting processes not provided for in groups B22D1/00&#160;-&#160;B22D21/00(making metallic powder by casting B22F9/08; alumino-thermic welding B23K23/00; remelting metals C22B9/16)	B22D23/00	B22D23/00		560
B22D23/003	8	{Moulding by spraying metal on a surface}	B22D23/00	B22D23/00		420
B22D23/006	8	{Casting by filling the mould through rotation of the mould together with a molten metal holding recipient, about a common axis}	B22D23/00	B22D23/00		189
B22D23/02	8	Top casting	B22D23/02	B22D23/02		98
B22D23/04	8	Casting by dipping (hot-dipping or immersion processes for applying coating material in the molten state without affecting the shape C23C2/00)	B22D23/04	B22D23/04		537
B22D23/06	8	Melting-down metal, e.g. metal particles, in the mould	B22D23/06	B22D23/06		365
B22D23/10	9	Electroslag casting {(electroslag remelting C22B9/18)}	B22D23/10	B22D23/10		653
B22D25/00	7	Special casting characterised by the nature of the product (B22D15/02, B22D17/16, B22D19/00 take precedence; casting stereotype plates B41D3/00)	B22D25/00	B22D25/00		249
B22D25/005	8	{Casting metal foams}	B22D25/00	B22D25/00		299
B22D25/02	8	by its peculiarity of shape; of works of art {(cylinders, pistons B22D15/02)}	B22D25/02	B22D25/02		1208
B22D25/023	9	{Casting chains or the like}	B22D25/02	B22D25/02		130
B22D25/026	9	{Casting jewelry articles (B22D13/063 takes precedence)}	B22D25/02	B22D25/02		172
B22D25/04	9	Casting metal electric battery plates or the like (manufacture thereof by multi-step processes H01M4/82)	B22D25/04	B22D25/04		974
B22D25/06	8	by its physical properties (B22D27/00 takes precedence)	B22D25/06	B22D25/06		236
B22D25/08	9	by uniform hardness (B22D15/00 takes precedence)	B22D25/08	B22D25/08		7
B22D27/00	7	Treating the metal in the mould while it is molten or ductile (B22D7/12, B22D11/10, B22D43/00 take precedence); {Pressure or vacuum casting (B22D17/00 takes precedence)}	B22D27/00	B22D27/00		234
B22D27/003	8	{by using inert gases}	B22D27/00	B22D27/00		412
B22D27/006	8	{by using reactive gases}	B22D27/00	B22D27/00		37
B22D27/02	8	Use of electric or magnetic effects {(for continuous casting B22D11/015, B22D11/11)}	B22D27/02	B22D27/02		812
B22D27/04	8	Influencing the temperature of the metal, e.g. by heating or cooling the mould	B22D27/04	B22D27/04		3720
B22D27/045	9	{Directionally solidified castings}	B22D27/04	B22D27/04		1136
B22D27/06	9	Heating the top discard of ingots (hot tops for ingot moulds B22D7/10)	B22D27/06	B22D27/06		461
B22D27/08	8	Shaking, vibrating, or turning of moulds	B22D27/08	B22D27/08		1105
B22D27/09	8	by using pressure	B22D27/09	B22D27/09		246
B22D27/11	9	making use of mechanical pressing devices	B22D27/11	B22D27/11		418
B22D27/13	9	making use of gas pressure	B22D27/13	B22D27/13		364
B22D27/15	8	by using vacuum	B22D27/15	B22D27/15		645
B22D27/18	8	Measures for using chemical processes for influencing the surface composition of castings, e.g. for increasing resistance to acid attack	B22D27/18	B22D27/18		161
B22D27/20	8	Measures not previously mentioned for influencing the grain structure or texture; Selection of compositions therefor	B22D27/20	B22D27/20		653
B22D29/00	7	Removing castings from moulds, not restricted to casting processes covered by a single main group; Removing cores; Handling ingots {(B22D13/10, B22D11/124, B22D17/00 take precedence)}	B22D29/00	B22D29/00		569
B22D29/001	8	{Removing cores}	B22D29/00	B22D29/00		277
B22D29/002	9	{by leaching, washing or dissolving}	B22D29/00	B22D29/00		278
B22D29/003	9	{using heat}	B22D29/00	B22D29/00		114
B22D29/005	9	{by vibrating or hammering}	B22D29/00	B22D29/00		230
B22D29/006	9	{by abrasive, water or air blasting}	B22D29/00	B22D29/00		160
B22D29/007	9	{by using explosive shock waves}	B22D29/00	B22D29/00		13
B22D29/008	10	{in a liquid medium}	B22D29/00	B22D29/00		58
B22D29/02	8	Vibratory apparatus specially designed for shaking out flasks	B22D29/02	B22D29/02		542
B22D29/04	8	Handling or stripping castings or ingots (grippers in general, see the relevant subclasses, e.g.  B66C)	B22D29/04	B22D29/04		1515
B22D29/06	9	Strippers actuated by fluid pressure	B22D29/06	B22D29/06		469
B22D29/08	9	Strippers actuated mechanically	B22D29/08	B22D29/08		373
B22D30/00	7	Cooling castings, not restricted to casting processes covered by a single main group (accessories for cooling cast stock in continuous casting of metals B22D11/124; controlling or regulating processes or operations for cooling cast stock or mould in continuous casting of metals B22D11/22; chill casting B22D15/00)	B22D30/00	B22D30/00		1153
B22D31/00	7	Cutting-off surplus material, e.g. gates; {Cleaning and working on castings (B22D17/2076 takes precedence)}	B22D31/00	B22D31/00		1266
B22D31/002	8	{Cleaning, working on castings}	B22D31/00	B22D31/00		1369
B22D31/005	9	{Sealing or impregnating porous castings}	B22D31/00	B22D31/00		141
B22D31/007	9	{Tumbling mills}	B22D31/00	B22D31/00		146
B22D33/00	7	Equipment for handling moulds	B22D33/00	B22D33/00		277
B22D33/005	8	{Transporting flaskless moulds}	B22D33/00	B22D33/00		182
B22D33/02	8	Turning or transposing moulds	B22D33/02	B22D33/02		1150
B22D33/04	8	Bringing together or separating moulds	B22D33/04	B22D33/04		798
B22D33/06	8	Burdening or relieving moulds	B22D33/06	B22D33/06		450
B22D35/00	7	Equipment for conveying molten metal into beds or moulds (B22D37/00 - B22D41/00 take precedence)	B22D35/00	B22D35/00		213
B22D35/02	8	into beds	B22D35/02	B22D35/02		19
B22D35/04	8	into moulds, e.g. base plates, runners	B22D35/04	B22D35/04		2139
B22D35/045	9	{Runner base plates for bottom casting ingots}	B22D35/04	B22D35/04		186
B22D35/06	8	Heating or cooling equipment	B22D35/06	B22D35/06		446
B22D37/00	7	Controlling or regulating the pouring of molten metal from a casting melt-holding vessel ({B22D11/18,}B22D39/00, B22D41/00 take precedence)	B22D37/00	B22D37/00		968
B22D37/005	8	{Shielding the molten metal stream (B22D11/106, B22D41/50 take precedence)}	B22D37/00	B22D37/00		67
B22D39/00	7	Equipment for supplying molten metal in rations	B22D39/00	B22D39/00		441
B22D39/003	8	{using electromagnetic field}	B22D39/00	B22D39/00		138
B22D39/006	9	{Electromagnetic conveyors}	B22D39/00	B22D39/00		54
B22D39/02	8	having means for controlling the amount of molten metal by volume	B22D39/02	B22D39/02		233
B22D39/023	9	{using a displacement member}	B22D39/02	B22D39/02		58
B22D39/026	9	{using a ladler}	B22D39/02	B22D39/02		252
B22D39/04	8	having means for controlling the amount of molten metal by weight	B22D39/04	B22D39/04		215
B22D39/06	8	having means for controlling the amount of molten metal by controlling the pressure above the molten metal	B22D39/06	B22D39/06		240
B22D41/00	7	Casting melt-holding vessels, e.g. ladles, tundishes, cups or the like (B22D39/00, B22D43/00 take precedence)	B22D41/00	B22D41/00		1740
B22D41/001	8	{devices for cleaning ladles (cleaning in general B08B)}	B22D41/00	B22D41/00		186
B22D41/003	8	{with impact pads}	B22D41/00	B22D41/00		179
B22D41/005	8	with heating or cooling means	B22D41/005	B22D41/005		160
B22D41/01	9	Heating means	B22D41/01	B22D41/01		533
B22D41/015	10	with external heating, i.e. the heat source not being a part of the ladle	B22D41/015	B22D41/015		631
B22D41/02	8	Linings	B22D41/02	B22D41/02		1487
B22D41/023	9	{Apparatus used for making or repairing linings (equipment used for making or repairing converter linings C21C5/441)}	B22D41/02	B22D41/02		436
B22D41/026	9	{Apparatus used for fracturing and removing of linings}	B22D41/02	B22D41/02		39
B22D41/04	8	tiltable	B22D41/04	B22D41/04		527
B22D41/05	9	Tea-pot spout ladles	B22D41/05	B22D41/05		137
B22D41/06	8	Equipment for tilting	B22D41/06	B22D41/06		778
B22D41/08	8	for bottom pouring (B22D41/14, B22D41/50 take precedence)	B22D41/08	B22D41/08		412
B22D41/12	8	Travelling ladles or similar containers; Cars for ladles (casting cranes B66C)	B22D41/12	B22D41/12		1460
B22D41/13	9	Ladle turrets	B22D41/13	B22D41/13		394
B22D41/14	8	Closures	B22D41/14	B22D41/14		472
B22D41/16	9	stopper-rod type, i.e. a stopper-rod being positioned downwardly through the vessel and the metal therein, for selective registry with the pouring opening	B22D41/16	B22D41/16		367
B22D41/18	10	Stopper-rods therefor	B22D41/18	B22D41/18		393
B22D41/183	11	{with cooling means}	B22D41/18	B22D41/18		17
B22D41/186	11	{with means for injecting a fluid into the melt}	B22D41/18	B22D41/18		138
B22D41/20	10	Stopper-rod operating equipment	B22D41/20	B22D41/20		297
B22D41/22	9	sliding-gate type, i.e. having a fixed plate and a movable plate in sliding contact with each other for selective registry of their openings	B22D41/22	B22D41/22		389
B22D41/24	10	characterised by a rectilinearly movable plate (B22D41/38&#160;-&#160;B22D41/42 take precedence)	B22D41/24	B22D41/24		319
B22D41/26	10	characterised by a rotatively movable plate (B22D41/38&#160;-&#160;B22D41/42 take precedence)	B22D41/26	B22D41/26		119
B22D41/28	10	Plates therefor (B22D41/38&#160;-&#160;B22D41/42 take precedence)	B22D41/28	B22D41/28		331
B22D41/30	11	Manufacturing or repairing thereof	B22D41/30	B22D41/30		86
B22D41/32	12	characterised by the materials used therefor	B22D41/32	B22D41/32		172
B22D41/34	11	Supporting, fixing or centering means therefor	B22D41/34	B22D41/34		177
B22D41/36	11	Treating the plates, e.g. lubricating, heating (ladles, cups or the like with heating means B22D41/01)	B22D41/36	B22D41/36		38
B22D41/38	10	Means for operating the sliding gate	B22D41/38	B22D41/38		205
B22D41/40	10	Means for pressing the plates together	B22D41/40	B22D41/40		148
B22D41/42	10	Features relating to gas injection	B22D41/42	B22D41/42		297
B22D41/44	9	Consumable closure means, i.e. closure means being used only once	B22D41/44	B22D41/44		192
B22D41/46	10	Refractory plugging masses	B22D41/46	B22D41/46		295
B22D41/465	11	{Unplugging a vessel discharge port}	B22D41/46	B22D41/46		67
B22D41/48	10	Meltable closures	B22D41/48	B22D41/48		82
B22D41/50	8	Pouring-nozzles	B22D41/50	B22D41/50		2257
B22D41/502	9	{Connection arrangements; Sealing means therefor}	B22D41/50	B22D41/50		288
B22D41/505	9	{Rings, inserts or other means preventing external nozzle erosion by the slag}	B22D41/50	B22D41/50		128
B22D41/507	9	{giving a rotating motion to the issuing molten metal}	B22D41/50	B22D41/50		119
B22D41/52	9	Manufacturing or repairing thereof	B22D41/52	B22D41/52		236
B22D41/54	10	characterised by the materials used therefor	B22D41/54	B22D41/54		517
B22D41/56	9	Means for supporting, manipulating or changing a pouring-nozzle	B22D41/56	B22D41/56		656
B22D41/58	9	with gas injecting means	B22D41/58	B22D41/58		663
B22D41/60	9	with heating or cooling means	B22D41/60	B22D41/60		433
B22D41/62	9	with stirring or vibrating means	B22D41/62	B22D41/62		133
B22D43/00	7	Mechanical cleaning, e.g. skimming of molten metals	B22D43/00	B22D43/00		558
B22D43/001	8	{Retaining slag during pouring molten metal}	B22D43/00	B22D43/00		188
B22D43/002	9	{by using floating means}	B22D43/00	B22D43/00		89
B22D43/004	9	{by using filtering means (B22C9/086 takes precedence)}	B22D43/00	B22D43/00		569
B22D43/005	8	{Removing slag from a molten metal surface}	B22D43/00	B22D43/00		247
B22D43/007	9	{by using scrapers}	B22D43/00	B22D43/00		238
B22D43/008	9	{by suction}	B22D43/00	B22D43/00		41
B22D45/00	7	Equipment for casting, not otherwise provided for	B22D45/00	B22D45/00		693
B22D45/005	8	{Evacuation of fumes, dust or waste gases during manipulations in the foundry (during steel manufacture C21C5/38; evacuation from furnaces F27D17/30)}	B22D45/00	B22D45/00		502
B22D46/00	7	Controlling, supervising, not restricted to casting covered by a single main group, e.g. for safety reasons (controlling or regulating in general G05)	B22D46/00	B22D46/00		1544
B22D47/00	7	Casting plants	B22D47/00	B22D47/00		630
B22D47/02	8	for both moulding and casting	B22D47/02	B22D47/02		394
