B62M1/00	7	Rider propulsion of wheeled vehicles (rider propulsion with additional source of power B62M6/00; propulsion by ground-engaging rods B62M29/02)<br><br><u>NOTE</u><br><br>Groups B62M1/12-B62M1/34 correspond to IPC2013.01	B62M1/00	B62M1/00		563
B62M1/10	8	involving devices which enable the mechanical storing and releasing of energy occasionally, e.g. arrangement of flywheels	B62M1/10	B62M1/10		667
B62M1/105	9	{using elastic elements}	B62M1/10	B62M1/10		230
B62M1/12	8	operated by both hand and foot power	B62M1/12	B62M1/12		1060
B62M1/14	8	operated exclusively by hand power	B62M1/14	B62M1/14		1017
B62M1/16	9	by means of a to-and-fro movable handlebar	B62M1/16	B62M1/16		388
B62M1/18	8	by movement of rider&apos;s saddle	B62M1/18	B62M1/18		419
B62M1/20	9	with additional rider propulsion means	B62M1/20	B62M1/20		135
B62M1/24	8	with reciprocating levers, e.g. foot levers (levers with can be immobilised as foot rests B62M5/00)	B62M1/24	B62M1/24		1055
B62M1/26	9	characterised by rotary cranks combined with reciprocating levers	B62M1/26	B62M1/26		778
B62M1/28	9	characterised by the use of flexible drive members, e.g. chains	B62M1/28	B62M1/28		1240
B62M1/30	9	characterised by the use of intermediate gears	B62M1/30	B62M1/30		570
B62M1/32	9	characterised by directly driving the wheel axle, e.g. by using a ratchet wheel	B62M1/32	B62M1/32		356
B62M1/34	8	by walking on an endless belt	B62M1/34	B62M1/34		92
B62M1/36	8	with rotary cranks, e.g. with pedal cranks (B62M1/34 takes precedence; combined with reciprocating levers B62M1/26; cranks which can be immobilised as foot rests B62M5/00)	B62M1/36	B62M1/36		1403
B62M1/38	9	for directly driving the wheel axle	B62M1/38	B62M1/38		210
B62M3/00	7	Construction of cranks operated by hand or foot	B62M3/00	B62M3/00		1322
B62M3/003	8	{Combination of crank axles and bearings housed in the bottom bracket (bottom bracket frame details B62K19/34)}	B62M3/00	B62M3/00		882
B62M2003/006	8	{Crank arrangements to overcome dead points}	B62M3/00	B62M3/00		256
B62M3/02	8	of adjustable length	B62M3/02	B62M3/02		354
B62M3/04	9	automatically adjusting	B62M3/04	B62M3/04		610
B62M3/06	8	with elliptical or other non-circular rotary movement	B62M3/06	B62M3/06		304
B62M3/08	8	Pedals	B62M3/08	B62M3/08		2143
B62M3/083	9	{Toe clip}	B62M3/08	B62M3/08		369
B62M3/086	9	{Attachments between shoe and pedal other than toe clips, e.g. cleats (shoes for cyclists A43B5/14)}	B62M3/08	B62M3/08		941
B62M3/10	9	All-metal pedals	B62M3/10	B62M3/10		48
B62M3/12	9	with reflectors	B62M3/12	B62M3/12		180
B62M3/14	8	Hand-grips for hand-operated cranks	B62M3/14	B62M3/14		53
B62M3/16	8	Accessories	B62M3/16	B62M3/16		297
B62M5/00	7	Foot-driven levers as pedal cranks which can be immobilised as foot-rests (immobilising against theft B62H5/10)	B62M5/00	B62M5/00		91
B62M6/00	7	Rider propulsion of wheeled vehicles with additional source of power, e.g. combustion engine or electric motor<br><br><u>NOTE</u><br><br>In this main group, the first place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the first appropriate place.	B62M6/00	B62M6/00		174
B62M6/10	8	Rider propelled cycles with auxiliary combustion engine	B62M6/10	B62M6/10		106
B62M6/15	9	Control or actuating devices therefor	B62M6/15	B62M6/15		33
B62M6/20	9	power-driven at crank shaft parts	B62M6/20	B62M6/20		79
B62M6/25	9	power-driven at axle parts	B62M6/25	B62M6/25		60
B62M6/30	9	power-driven at single endless flexible member, e.g. chain, between cycle crankshaft and wheel axle, the engine engaging the endless flexible member	B62M6/30	B62M6/30		13
B62M6/35	9	power-driven by friction rollers or gears engaging the ground wheel	B62M6/35	B62M6/35		73
B62M6/40	8	Rider propelled cycles with auxiliary electric motor	B62M6/40	B62M6/40		1545
B62M6/45	9	Control or actuating devices therefor	B62M6/45	B62M6/45		3079
B62M6/50	10	characterised by detectors or sensors, or arrangement thereof	B62M6/50	B62M6/50		2398
B62M6/55	9	power-driven at crank shafts parts	B62M6/55	B62M6/55		2520
B62M6/60	9	power-driven at axle parts	B62M6/60	B62M6/60		857
B62M6/65	10	with axle and driving shaft arranged coaxially	B62M6/65	B62M6/65		885
B62M6/70	9	power-driven at single endless flexible member, e.g. chain, between cycle crankshaft and wheel axle, the motor engaging the endless flexible member	B62M6/70	B62M6/70		260
B62M6/75	9	power-driven by friction rollers or gears engaging the ground wheel	B62M6/75	B62M6/75		381
B62M6/80	8	Accessories, e.g. power sources; Arrangements thereof	B62M6/80	B62M6/80		652
B62M6/85	9	Solar cells	B62M6/85	B62M6/85		292
B62M6/90	9	Batteries	B62M6/90	B62M6/90		2492
B62M7/00	7	Motorcycles characterised by position of motor or engine (rider propulsion with addition source of power, e.g. auxiliary combustion engine or electric motor B62M6/00; frames characterised by position of engine B62K11/00)	B62M7/00	B62M7/00		732
B62M2007/005	8	{the cycle being equipped with a pneumatic motor}	B62M7/00	B62M7/00		81
B62M7/02	8	with engine between front and rear wheels	B62M7/02	B62M7/02		877
B62M7/04	9	below the frame	B62M7/04	B62M7/04		383
B62M7/06	9	directly under the saddle or seat	B62M7/06	B62M7/06		163
B62M7/08	8	with the engine over the rear wheel	B62M7/08	B62M7/08		94
B62M7/10	8	with the engine over the front wheel	B62M7/10	B62M7/10		312
B62M7/12	8	with the engine beside or within the driven wheel	B62M7/12	B62M7/12		1595
B62M7/14	8	with the engine on an auxiliary wheeled unit, e.g. trailer, sidecar (trailers B60P, B62D; sidecars B62K27/00)	B62M7/14	B62M7/14		106
B62M7/16	9	{with wheel of unit driven by the engine}	B62M7/14	B62M7/16		68
B62M9/00	7	Transmissions characterised by use of an endless chain, belt, or the like (cycle chain guards B62J13/00)<br><br><u>NOTE</u><br><br>In this main group, the first place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the first appropriate place.	B62M9/00	B62M9/00		1200
B62M2009/002	8	{Non-circular chain rings or sprockets}	B62M9/00	B62M9/00		180
B62M2009/005	8	{Details of transmission chains specially adapted for bicycles}	B62M9/00	B62M9/00		221
B62M2009/007	8	{Guides to prevent chain from slipping off the sprocket}	B62M9/00	B62M9/00		220
B62M9/02	8	of unchangeable ratio	B62M9/02	B62M9/02		631
B62M9/04	8	of changeable ratio	B62M9/04	B62M9/04		644
B62M9/06	9	using a single chain, belt, or the like	B62M9/06	B62M9/06		559
B62M9/08	10	involving eccentrically- mounted or elliptically-shaped driving or driven wheel; with expansible driving or driven wheel	B62M9/08	B62M9/08		695
B62M9/085	11	{involving eccentrically mounted driving or driven wheel}	B62M9/08	B62M9/08		140
B62M9/10	10	involving different-sized wheels, {e.g. rear sprocket chain wheels} selectively engaged by the chain, belt, or the like {(bicycle hubs rotatably arranged on axle B60B27/023)}	B62M9/10	B62M9/10		1140
B62M9/105	11	{involving front sprocket chain-wheels engaged by the chain, belt or the like}	B62M9/10	B62M9/10		364
B62M9/12	11	the chain, belt, or the like being laterally shiftable {, e.g. using a rear derailleur}	B62M9/12	B62M9/12		421
B62M9/121	12	Rear derailleurs	B62M9/121	B62M9/121		234
B62M9/122	13	electrically or fluid actuated; Controls thereof	B62M9/122	B62M9/122		695
B62M9/123	13	changing gears automatically	B62M9/123	B62M9/123		223
B62M9/124	13	Mechanisms for shifting laterally	B62M9/124	B62M9/124		617
B62M2009/12406	14	{Rear derailleur comprising a rigid pivoting arm}	B62M9/124	B62M9/124		120
B62M2009/12413	14	{Rear derailleur comprising telescoping mechanisms}	B62M9/124	B62M9/124		283
B62M9/1242	14	characterised by the linkage mechanisms	B62M9/1242	B62M9/1242		288
B62M9/1244	14	limiting or positioning the movement	B62M9/1244	B62M9/1244		185
B62M9/1246	15	using cams or plates	B62M9/1246	B62M9/1246		63
B62M9/1248	14	characterised by the use of biasing means, e.g. springs; Arrangements thereof	B62M9/1248	B62M9/1248		204
B62M9/125	13	Mounting the derailleur on the frame	B62M9/125	B62M9/125		266
B62M9/126	13	Chain guides; Mounting thereof	B62M9/126	B62M9/126		466
B62M9/127	13	Mounting or guiding of cables	B62M9/127	B62M9/127		178
B62M9/128	13	Accessories, e.g. protectors	B62M9/128	B62M9/128		192
B62M9/131	12	Front derailleurs	B62M9/131	B62M9/131		132
B62M9/132	13	electrically or fluid actuated; Controls thereof	B62M9/132	B62M9/132		336
B62M9/133	13	changing gears automatically	B62M9/133	B62M9/133		93
B62M9/134	13	Mechanisms for shifting laterally	B62M9/134	B62M9/134		102
B62M9/1342	14	characterised by the linkage mechanisms	B62M9/1342	B62M9/1342		140
B62M9/1344	14	limiting or positioning the movement	B62M9/1344	B62M9/1344		49
B62M9/1346	15	using cams or plates	B62M9/1346	B62M9/1346		23
B62M9/1348	15	characterised by the use of biasing means, e.g. springs; Arrangements thereof	B62M9/1348	B62M9/1348		50
B62M9/135	13	Mounting the derailleur on the frame	B62M9/135	B62M9/135		102
B62M9/136	13	Chain guides; Mounting thereof	B62M9/136	B62M9/136		173
B62M9/137	13	Mounting or guiding of cables	B62M9/137	B62M9/137		64
B62M9/138	13	Accessories, e.g. protectors	B62M9/138	B62M9/138		48
B62M9/14	11	the wheels being laterally shiftable	B62M9/14	B62M9/14		102
B62M9/16	8	Tensioning or adjusting equipment for chains, belts or the like	B62M9/16	B62M9/16		1190
B62M11/00	7	Transmissions characterised by the use of interengaging toothed wheels or frictionally-engaging wheels (with roller engaging the periphery of ground wheel B62M13/00)	B62M11/00	B62M11/00		850
B62M11/02	8	of unchangeable ratio	B62M11/02	B62M11/02		665
B62M11/04	8	of changeable ratio	B62M11/04	B62M11/04		633
B62M11/06	9	with spur gear wheels (B62M11/14 takes precedence)	B62M11/06	B62M11/06		780
B62M11/08	10	{with a radially-shiftable intermediate gear wheel}	B62M11/06	B62M11/08		40
B62M11/10	9	with bevel gear wheels (B62M11/14 takes precedence)	B62M11/10	B62M11/10		252
B62M11/12	9	with frictionally-engaging wheels (B62M11/14 takes precedence)	B62M11/12	B62M11/12		126
B62M11/14	9	with planetary gears	B62M11/14	B62M11/14		1108
B62M11/145	10	{built in, or adjacent to, the bottom bracket}	B62M11/14	B62M11/14		727
B62M11/16	10	built in, or adjacent to, the ground-wheel hub	B62M11/16	B62M11/16		808
B62M11/18	10	with a plurality of planetary gear units	B62M11/18	B62M11/18		534
B62M13/00	7	Transmissions characterised by use of friction rollers engaging the periphery of the ground wheel (for rider propelled cycles with additional source of power B62M6/35, B62M6/75)	B62M13/00	B62M13/00		170
B62M13/02	8	with changeable ratio, e.g. with roller of varying diameter	B62M13/02	B62M13/02		29
B62M13/04	8	with means for moving roller into driving contact with ground wheel	B62M13/04	B62M13/04		126
B62M15/00	7	Transmissions characterised by use of crank shafts and coupling rods	B62M15/00	B62M15/00		206
B62M17/00	7	Transmissions characterised by use of rotary shaft, e.g. cardan shaft	B62M17/00	B62M17/00		751
B62M19/00	7	Transmissions characterised by use of non-mechanical gearing, e.g. fluid gearing	B62M19/00	B62M19/00		489
B62M21/00	7	Transmissions characterised by use of resilient elements therein	B62M21/00	B62M21/00		131
B62M23/00	7	Transmissions characterised by use of other elements; Other transmissions	B62M23/00	B62M23/00		649
B62M23/02	8	characterised by the use of two or more dissimilar sources of power, e.g. transmissions for hybrid motorcycles (transmissions for wheeled vehicles using rider propulsion with additional source of power B62M6/00)	B62M23/02	B62M23/02		537
B62M25/00	7	Actuators for gearing speed-change mechanisms specially adapted for cycles (rider operated controls for cycles in general B62K23/00; gearing speed change mechanisms F16H)	B62M25/00	B62M25/00		1398
B62M2025/003	8	{with gear indicating means, e.g. a display}	B62M25/00	B62M25/00		136
B62M2025/006	8	{with auxiliary shift assisting means}	B62M25/00	B62M25/00		178
B62M25/02	8	with mechanical transmitting systems, e.g. cables, levers	B62M25/02	B62M25/02		368
B62M25/04	9	hand actuated	B62M25/04	B62M25/04		1804
B62M25/045	10	{having single actuating means operating both front and rear derailleur}	B62M25/04	B62M25/04		121
B62M25/06	9	foot actuated	B62M25/06	B62M25/06		206
B62M25/08	8	with electrical or fluid transmitting systems	B62M25/08	B62M25/08		1701
B62M27/00	7	Propulsion devices for sledges or the like (pushed or pulled by persons or animals B62B, B62C; wind propulsion B62B15/00)	B62M27/00	B62M27/00		550
B62M27/02	8	power driven	B62M27/02	B62M27/02		1853
B62M2027/021	9	{Snow bikes resembling conventional motorcycles}	B62M27/02	B62M27/02		224
B62M2027/022	9	{Snow drive conversions for cycles with wheels}	B62M27/02	B62M27/02		107
B62M2027/023	9	{Snow mobiles characterised by engine mounting arrangements}	B62M27/02	B62M27/02		248
B62M2027/025	9	{Snow mobiles characterised by the skis}	B62M27/02	B62M27/02		204
B62M2027/026	9	{Snow mobiles characterised by the suspension means}	B62M27/02	B62M27/02		604
B62M2027/027	9	{Snow mobiles characterised by the tracks}	B62M27/02	B62M27/02		212
B62M2027/028	9	{Snow mobiles characterised by chassis or bodywork}	B62M27/02	B62M27/02		143
B62M29/00	7	Ground engaging propulsion devices for cycles, sledges, or rider-propelled wheeled vehicles, not otherwise provided for {(non-motorized scooters with skis or runners B62K3/002)}	B62M29/00	B62M29/00		144
B62M29/02	8	using ground-engaging rods	B62M29/02	B62M29/02		52
