B25G1/00	7	Handle constructions	B25G1/00	B25G1/00		1473
B25G1/002	8	{for rotary tools with additional levers, e.g. for increasing torque (B25G1/005 takes precedence)}	B25G1/00	B25G1/00		45
B25G1/005	8	{for screwdrivers, wrenches or spanners with additional levers, e.g. for increasing torque}	B25G1/00	B25G1/00		703
B25G1/007	9	{of crank type}	B25G1/00	B25G1/00		270
B25G1/01	8	Shock-absorbing means (B25G1/02 takes precedence)	B25G1/01	B25G1/01		482
B25G1/02	8	flexible (hammers heads having shock-absorbing means B25D1/12)	B25G1/02	B25G1/02		176
B25G1/025	9	{for screwdrivers, wrenches or spanners}	B25G1/02	B25G1/02		80
B25G1/04	8	telescopic; extensible; sectional	B25G1/04	B25G1/04		1908
B25G1/043	9	{for screwdrivers, wrenches or spanners}	B25G1/04	B25G1/04		630
B25G1/046	10	{with free-turning section at end of handle remote from tool}	B25G1/04	B25G1/04		146
B25G1/06	8	reversible or adjustable for position	B25G1/06	B25G1/06		820
B25G1/063	9	{for screwdrivers, wrenches or spanners}	B25G1/06	B25G1/06		888
B25G1/066	10	{the grip itself being angularly adjustable}	B25G1/06	B25G1/06		323
B25G1/08	8	with provision for storing tool elements	B25G1/08	B25G1/08		470
B25G1/085	9	{for screwdrivers, wrenches or spanners}	B25G1/08	B25G1/08		1162
B25G1/10	8	characterised by material or shape (B25G1/01, B25G1/02 take precedence {; for hand tools comprising coating rollers B05C17/0205})	B25G1/10	B25G1/10		1495
B25G1/102	9	{the shape being specially adapted to facilitate handling or improve grip}	B25G1/10	B25G1/10		1878
B25G1/105	9	{for screwdrivers, wrenches or spanners (B25G1/102, B25G1/125 take precedence)}	B25G1/10	B25G1/10		763
B25G1/107	10	{of thimble type}	B25G1/10	B25G1/10		43
B25G1/12	9	electrically insulating material	B25G1/12	B25G1/12		187
B25G1/125	10	{for screwdrivers, wrenches or spanners}	B25G1/12	B25G1/12		203
B25G3/00	7	Attaching handles to the implements	B25G3/00	B25G3/00		549
B25G3/02	8	Socket, tang, or like fixings (B25G3/34 takes precedence)	B25G3/02	B25G3/02		938
B25G3/04	9	with detachable or separate socket pieces (B25G3/12 takes precedence)	B25G3/04	B25G3/04		411
B25G3/06	9	with multiple socket, e.g. T-socket (B25G3/12 takes precedence)	B25G3/06	B25G3/06		91
B25G3/08	9	with dovetail or other groove (B25G3/12 takes precedence)	B25G3/08	B25G3/08		122
B25G3/10	9	with elastic, taper, or other self-grip socket or tang (B25G3/12 takes precedence)	B25G3/10	B25G3/10		310
B25G3/12	9	Locking and securing devices	B25G3/12	B25G3/12		647
B25G3/14	10	comprising barbs or teeth	B25G3/14	B25G3/14		221
B25G3/16	10	comprising bayonet joints	B25G3/16	B25G3/16		96
B25G3/18	10	comprising catches or pawls	B25G3/18	B25G3/18		571
B25G3/20	10	comprising clamping or contracting means acting concentrically on the handle or socket	B25G3/20	B25G3/20		296
B25G3/22	11	Chucks	B25G3/22	B25G3/22		152
B25G3/24	10	comprising clamping or contracting means acting transversely on the handle or socket	B25G3/24	B25G3/24		335
B25G3/26	10	comprising nails, screws, bolts, or pins traversing or entering the socket	B25G3/26	B25G3/26		676
B25G3/28	10	comprising wedges, keys, or like expanding means	B25G3/28	B25G3/28		579
B25G3/30	10	comprising screwed sockets or tangs	B25G3/30	B25G3/30		496
B25G3/32	10	in association with, or including, tang, bolt, or other member passing axially through whole length of handle	B25G3/32	B25G3/32		155
B25G3/34	8	by pressing the handle on the implements; using cement or molten metal, e.g. casting, moulding, by welding or the like	B25G3/34	B25G3/34		430
B25G3/36	8	Lap joints; Riveted, screwed, or like joints (socket, tang, or like fixings B25G3/02)	B25G3/36	B25G3/36		417
B25G3/38	8	Hinged, pivoted, swivelling, or folding joints	B25G3/38	B25G3/38		958
