H01R3/00	7	Electrically-conductive connections not otherwise provided for	H01R3/00	H01R3/00		75
H01R3/08	8	for making connection to a liquid {(slip rings with liquid contacts H01R39/30, H01R39/646)}	H01R3/08	H01R3/08		168
H01R4/00	7	Electrically-conductive connections between two or more conductive members in direct contact, i.e. touching one another; Means for effecting or maintaining such contact; Electrically-conductive connections having two or more spaced connecting locations for conductors and using contact members penetrating insulation	H01R4/00	H01R4/00		805
H01R4/01	8	Connections using shape memory materials, e.g. shape memory metal	H01R4/01	H01R4/01		222
H01R4/02	8	Soldered or welded connections {(H01R4/625, H01R4/723, H01R12/59 take precedence)}	H01R4/02	H01R4/02		1752
H01R4/021	9	{between two or more cables or wires}	H01R4/02	H01R4/02		449
H01R4/022	10	{comprising preapplied solder}	H01R4/02	H01R4/02		62
H01R4/023	9	{between cables or wires and terminals}	H01R4/02	H01R4/02		1212
H01R4/024	10	{comprising preapplied solder}	H01R4/02	H01R4/02		201
H01R4/025	9	{with built-in heat generating elements}	H01R4/02	H01R4/02		41
H01R4/026	9	{comprising means for eliminating an insulative layer prior to soldering or welding}	H01R4/02	H01R4/02		75
H01R4/027	9	{comprising means for positioning or holding the parts to be soldered or welded}	H01R4/02	H01R4/02		465
H01R4/028	9	{comprising means for preventing flowing or wicking of solder or flux in parts not desired}	H01R4/02	H01R4/02		386
H01R4/029	9	{Welded connections (H01R4/021&#160;-&#160;H01R4/028 take precedence)}	H01R4/02	H01R4/02		1142
H01R4/04	8	using electrically conductive adhesives	H01R4/04	H01R4/04		1097
H01R4/06	8	Riveted connections (by explosion H01R4/08)	H01R4/06	H01R4/06		464
H01R4/08	8	effected by an explosion	H01R4/08	H01R4/08		122
H01R4/10	8	effected solely by twisting, wrapping, bending, crimping, or other permanent deformation	H01R4/10	H01R4/10		501
H01R4/12	9	by twisting	H01R4/12	H01R4/12		274
H01R4/14	9	by wrapping	H01R4/14	H01R4/14		424
H01R4/16	9	by bending	H01R4/16	H01R4/16		189
H01R4/18	9	by crimping {(H01R4/01, H01R4/2495 take precedence; for coaxial cables H01R9/0518)}	H01R4/18	H01R4/18		1402
H01R4/182	10	{for flat conductive elements, e.g. flat cables (H01R4/01 takes precedence)}	H01R4/18	H01R4/18		201
H01R4/183	10	{for cylindrical elongated bodies, e.g. cables having circular cross-section (H01R4/01 takes precedence)}	H01R4/18	H01R4/18		855
H01R4/184	11	{comprising a U-shaped wire-receiving portion}	H01R4/18	H01R4/18		854
H01R4/185	12	{combined with a U-shaped insulation-receiving portion}	H01R4/18	H01R4/18		1638
H01R4/186	11	{using a body comprising a plurality of cable-accommodating recesses or bores}	H01R4/18	H01R4/18		278
H01R4/187	10	{combined with soldering or welding}	H01R4/18	H01R4/18		372
H01R4/188	10	{having an uneven wire-receiving surface to improve the contact}	H01R4/18	H01R4/18		468
H01R4/20	10	using a crimping sleeve {(H01R4/01 takes precedence)}	H01R4/20	H01R4/20		1814
H01R4/203	11	{having an uneven wire-receiving surface to improve the contact}	H01R4/20	H01R4/20		185
H01R4/206	12	{with transversal grooves or threads}	H01R4/20	H01R4/20		175
H01R4/22	8	End caps, i.e. of insulating or conductive material for covering or maintaining connections between wires entering the cap from the same end	H01R4/22	H01R4/22		1092
H01R4/24	8	Connections using contact members penetrating or cutting insulation or cable strands	H01R4/24	H01R4/24		859
H01R4/2404	9	the contact members having teeth, prongs, pins or needles penetrating the insulation	H01R4/2404	H01R4/2404		643
H01R4/2406	10	having needles or pins	H01R4/2406	H01R4/2406		639
H01R4/2407	10	having saw-tooth projections	H01R4/2407	H01R4/2407		171
H01R4/2408	10	actuated by clamping screws	H01R4/2408	H01R4/2408		716
H01R4/2412	10	actuated by insulated cams or wedges	H01R4/2412	H01R4/2412		267
H01R4/2416	9	the contact members having insulation-cutting edges, e.g. of tuning fork type	H01R4/2416	H01R4/2416		472
H01R4/242	10	the contact members being plates having a single slot	H01R4/242	H01R4/242		549
H01R4/2425	11	Flat plates, e.g. multi-layered flat plates	H01R4/2425	H01R4/2425		391
H01R4/2429	12	mounted in an insulating base	H01R4/2429	H01R4/2429		833
H01R4/2433	13	one part of the base being movable to push the cable into the slot	H01R4/2433	H01R4/2433		1492
H01R4/2437	11	Curved plates	H01R4/2437	H01R4/2437		74
H01R4/2441	12	tube-shaped	H01R4/2441	H01R4/2441		90
H01R4/2445	10	the contact members having additional means acting on the insulation or the wire, e.g. additional insulation penetrating means, strain relief means or wire cutting knives	H01R4/2445	H01R4/2445		420
H01R4/245	11	the additional means having two or more slotted flat portions	H01R4/245	H01R4/245		170
H01R4/2452	12	in serial configuration, e.g. opposing folded slots	H01R4/2452	H01R4/2452		16
H01R4/2454	12	forming a U-shape with slotted branches	H01R4/2454	H01R4/2454		311
H01R4/2455	13	forming a slotted bight	H01R4/2455	H01R4/2455		3
H01R4/2456	12	in parallel configuration	H01R4/2456	H01R4/2456		14
H01R4/2458	11	the contact members being in a slotted tubular configuration, e.g. slotted tube-end	H01R4/2458	H01R4/2458		98
H01R4/2462	11	the contact members being in a slotted bent configuration, e.g. slotted bight	H01R4/2462	H01R4/2462		193
H01R4/2466	11	the contact members having a channel-shaped part, the opposite sidewalls of which comprise insulation-cutting means	H01R4/2466	H01R4/2466		260
H01R4/247	9	the contact members penetrating the insulation being actuated by springs	H01R4/247	H01R4/247		73
H01R4/2475	9	the contact members penetrating the insulation being actuated by screws, nuts or bolts	H01R4/2475	H01R4/2475		132
H01R4/2479	10	penetrating the area under the screw head	H01R4/2479	H01R4/2479		39
H01R4/2483	10	penetrating the area under the screw tip	H01R4/2483	H01R4/2483		232
H01R4/2487	10	penetrating by means of the screw thread	H01R4/2487	H01R4/2487		38
H01R4/2491	9	the contact members penetrating the insulation being actuated by conductive cams or wedges	H01R4/2491	H01R4/2491		197
H01R4/2495	9	Insulation penetration combined with permanent deformation of the contact member, e.g. crimping	H01R4/2495	H01R4/2495		539
H01R4/26	8	Connections in which at least one of the connecting parts has projections which bite into or engage the other connecting part in order to improve the contact ({H01R4/188, H01R4/203, H01R4/5075 take precedence}; using shape memory materials H01R4/01)	H01R4/26	H01R4/26		1131
H01R4/28	8	Clamped connections, spring connections (made by means of terminals specially adapted for contact with, or insertion into, printed circuits H01R12/00)	H01R4/28	H01R4/28		963
H01R4/30	9	utilising a screw or nut clamping member (H01R4/50 takes precedence; utilising a clamping member acted on by screw or nut H01R4/38; {for coaxial cables H01R9/0521})	H01R4/30	H01R4/30		1816
H01R4/301	10	{having means for preventing complete unscrewing of screw or nut}	H01R4/30	H01R4/30		235
H01R4/302	10	{having means for preventing loosening of screw or nut, e.g. vibration-proof connection}	H01R4/30	H01R4/30		415
H01R4/304	10	{having means for improving contact}	H01R4/30	H01R4/30		400
H01R4/305	10	{having means for facilitating engagement of conductive member or for holding it in position}	H01R4/30	H01R4/30		410
H01R4/307	10	{characterised by the thread of the screw or nut}	H01R4/30	H01R4/30		161
H01R4/308	10	{Conductive members located parallel to axis of screw}	H01R4/30	H01R4/30		241
H01R4/32	10	Conductive members located in slot or hole in screw	H01R4/32	H01R4/32		784
H01R4/34	10	Conductive members located under head of screw	H01R4/34	H01R4/34		1858
H01R4/36	10	Conductive members located under tip of screw	H01R4/36	H01R4/36		1934
H01R4/363	11	{with intermediate part between tip and conductive member}	H01R4/36	H01R4/36		928
H01R4/366	12	{intermediate part attached to the tip of the screw}	H01R4/36	H01R4/36		341
H01R4/38	9	utilising a clamping member acted on by screw or nut (H01R4/50 takes precedence)	H01R4/38	H01R4/38		1682
H01R4/40	10	Pivotable clamping member	H01R4/40	H01R4/40		484
H01R4/42	10	Clamping area to one side of screw only	H01R4/42	H01R4/42		518
H01R4/44	10	Clamping areas on both sides of screw	H01R4/44	H01R4/44		618
H01R4/46	10	Clamping area between two screws placed side by side	H01R4/46	H01R4/46		377
H01R4/48	9	utilising a spring, clip, or other resilient member (H01R4/52 takes precedence)	H01R4/48	H01R4/48		2736
H01R4/4809	10	{using a leaf spring to bias the conductor toward the busbar}	H01R4/48	H01R4/48		371
H01R4/4811	11	{Spring details}	H01R4/48	H01R4/48		70
H01R4/4814	12	{Self-latching arrangements}	H01R4/48	H01R4/48		140
H01R4/4816	12	{the spring shape preventing insertion of the conductor end when the spring is unbiased}	H01R4/48	H01R4/48		556
H01R4/48185	11	{adapted for axial insertion of a wire end}	H01R4/48	H01R4/48		168
H01R4/4819	12	{the spring shape allowing insertion of the conductor end when the spring is unbiased}	H01R4/48	H01R4/48		12
H01R4/4821	13	{Single-blade spring}	H01R4/48	H01R4/48		2350
H01R4/4823	13	{Multiblade spring}	H01R4/48	H01R4/48		304
H01R4/4826	13	{and having a hole for the conductor, e.g. a wire, passing through}	H01R4/48	H01R4/48		76
H01R4/48275	12	{with an opening in the housing for insertion of a release tool}	H01R4/48	H01R4/48		23
H01R4/4828	11	{Spring-activating arrangements mounted on or integrally formed with the spring housing}	H01R4/48	H01R4/48		105
H01R4/483	12	{Pivoting arrangements, e.g. lever pushing on the spring}	H01R4/48	H01R4/48		761
H01R4/4833	12	{Sliding arrangements, e.g. sliding button}	H01R4/48	H01R4/48		826
H01R4/4835	12	{Mechanically bistable arrangements, e.g. locked by the housing when the spring is biased}	H01R4/48	H01R4/48		309
H01R4/48365	12	{with integral release means}	H01R4/48	H01R4/48		122
H01R4/4837	12	{Single arrangement activating multiple springs}	H01R4/48	H01R4/48		139
H01R4/484	11	{Spring housing details}	H01R4/48	H01R4/48		440
H01R4/4842	12	{the spring housing being provided with a single opening for insertion of a spring-activating tool}	H01R4/48	H01R4/48		636
H01R4/4844	12	{the spring housing being provided with multiple openings for insertion of a spring-activating tool}	H01R4/48	H01R4/48		18
H01R4/48455	11	{insertion of a wire only possible by pressing on the spring}	H01R4/48	H01R4/48		72
H01R4/4846	11	{Busbar details}	H01R4/48	H01R4/48		470
H01R4/4848	12	{Busbar integrally formed with the spring}	H01R4/48	H01R4/48		563
H01R4/485	12	{Single busbar common to multiple springs}	H01R4/48	H01R4/48		1104
H01R4/4852	12	{Means for improving the contact with the conductor, e.g. uneven wire-receiving surface}	H01R4/48	H01R4/48		303
H01R4/4854	10	{using a wire spring}	H01R4/48	H01R4/48		133
H01R4/4863	11	{Coil spring}	H01R4/48	H01R4/48		680
H01R4/4872	12	{axially compressed to retain wire end}	H01R4/48	H01R4/48		513
H01R4/4881	10	{using a louver type spring}	H01R4/48	H01R4/48		131
H01R4/489	10	{spring force increased by screw, cam, wedge, or other fastening means}	H01R4/48	H01R4/48		416
H01R4/50	9	utilising a cam, wedge, cone or ball {also combined with a screw}	H01R4/50	H01R4/50		601
H01R4/5008	10	{using rotatable cam}	H01R4/50	H01R4/50		356
H01R4/5016	10	{using a cone}	H01R4/50	H01R4/50		236
H01R4/5025	11	{combined with a threaded ferrule operating in a direction parallel to the conductor}	H01R4/50	H01R4/50		534
H01R4/5033	10	{using wedge or pin penetrating into the end of a wire in axial direction of the wire}	H01R4/50	H01R4/50		340
H01R4/5041	10	{using a tapered groove}	H01R4/50	H01R4/50		74
H01R4/505	10	{using an excentric element}	H01R4/50	H01R4/50		57
H01R4/5058	10	{using a ball}	H01R4/50	H01R4/50		67
H01R4/5066	10	{mounted in an insulating housing having a cover providing clamping force}	H01R4/50	H01R4/50		121
H01R4/5075	10	{having an uneven wire receiving surface to improve the contact}	H01R4/50	H01R4/50		80
H01R4/5083	10	{using a wedge}	H01R4/50	H01R4/50		411
H01R4/5091	11	{combined with a screw}	H01R4/50	H01R4/50		269
H01R4/52	10	which is spring loaded	H01R4/52	H01R4/52		481
H01R4/54	8	{Bayonet or keyhole}	H01R4/00	H01R4/54		121
H01R4/56	8	one conductor screwing into another	H01R4/56	H01R4/56		568
H01R4/58	8	characterised by the form or material of the contacting members (H01R4/01 takes precedence)	H01R4/58	H01R4/58		1082
H01R4/60	9	Connections between or with tubular conductors (H01R4/56 takes precedence)	H01R4/60	H01R4/60		818
H01R4/62	9	Connections between conductors of different materials; Connections between or with aluminium or steel-core aluminium conductors (H01R4/68 takes precedence)	H01R4/62	H01R4/62		1550
H01R4/625	10	{Soldered or welded connections}	H01R4/62	H01R4/62		568
H01R4/64	9	Connections between or with conductive parts having primarily a non-electric function, e.g. frame, casing, rail	H01R4/64	H01R4/64		2940
H01R4/643	10	{for rigid cylindrical bodies}	H01R4/64	H01R4/64		551
H01R4/646	10	{for cables or flexible cylindrical bodies}	H01R4/64	H01R4/64		781
H01R4/66	9	Connections with the terrestrial mass, e.g. earth plate, earth pin	H01R4/66	H01R4/66		4723
H01R4/68	9	Connections to or between superconductive connectors	H01R4/68	H01R4/68		563
H01R4/70	8	Insulation of connections (end caps H01R4/22)	H01R4/70	H01R4/70		2502
H01R4/72	9	using a heat shrinking insulating sleeve	H01R4/72	H01R4/72		851
H01R4/723	10	{Making a soldered electrical connection simultaneously with the heat shrinking}	H01R4/72	H01R4/72		201
H01R4/726	10	{Making a non-soldered electrical connection simultaneously with the heat shrinking}	H01R4/72	H01R4/72		93
H01R9/00	7	Structural associations of a plurality of mutually-insulated electrical connecting elements, e.g. terminal strips or terminal blocks; Terminals or binding posts mounted upon a base or in a case; Bases therefor	H01R9/00	H01R9/00		707
H01R9/03	8	Connectors arranged to contact a plurality of the conductors of a multiconductor cable {, e.g. tapping connections}	H01R9/03	H01R9/03		725
H01R9/031	9	{for multiphase cables, e.g. with contact members penetrating insulation of a plurality of conductors (insulation penetrating contact members in general H01R4/24)}	H01R9/03	H01R9/03		511
H01R9/05	9	for coaxial cables	H01R9/05	H01R9/05		1461
H01R9/0503	10	{Connection between two cable ends}	H01R9/05	H01R9/05		331
H01R9/0506	10	{Connection between three or more cable ends}	H01R9/05	H01R9/05		133
H01R9/0509	10	{Tapping connections}	H01R9/05	H01R9/05		128
H01R9/0512	10	{Connections to an additional grounding conductor}	H01R9/05	H01R9/05		333
H01R9/0515	10	{Connection to a rigid planar substrate, e.g. printed circuit board}	H01R9/05	H01R9/05		487
H01R9/0518	10	{Connection to outer conductor by crimping or by crimping ferrule}	H01R9/05	H01R9/05		1206
H01R9/0521	10	{Connection to outer conductor by action of a nut}	H01R9/05	H01R9/05		795
H01R9/0524	10	{Connection to outer conductor by action of a clamping member, e.g. screw fastening means (H01R9/0515 takes precedence)}	H01R9/05	H01R9/05		695
H01R9/0527	10	{Connection to outer conductor by action of a resilient member, e.g. spring}	H01R9/05	H01R9/05		409
H01R9/053	10	using contact members penetrating insulation	H01R9/053	H01R9/053		226
H01R9/11	8	End pieces for multiconductor cables supported by the cable and for facilitating connections to other conductive members {, e.g. for liquid cooled welding cables}	H01R9/11	H01R9/11		295
H01R9/15	8	Connectors for wire wrapping	H01R9/15	H01R9/15		47
H01R9/16	8	Fastening of connecting parts to base or case; Insulating connecting parts from base or case	H01R9/16	H01R9/16		1248
H01R9/18	9	Fastening by means of screw or nut	H01R9/18	H01R9/18		484
H01R9/20	9	Fastening by means of rivet or eyelet	H01R9/20	H01R9/20		144
H01R9/22	8	Bases, e.g. strip, block, panel {(for printed circuits H01R12/50)}	H01R9/22	H01R9/22		814
H01R9/223	9	{Insulating enclosures for terminals (for switches H01H9/0264)}	H01R9/22	H01R9/22		471
H01R9/226	9	{comprising a plurality of conductive flat strips providing connection between wires or components (H01R9/2425 takes precedence)}	H01R9/22	H01R9/22		422
H01R9/24	9	Terminal blocks	H01R9/24	H01R9/24		2193
H01R9/2408	10	{Modular blocks (H01R9/26 takes precedence)}	H01R9/24	H01R9/24		939
H01R9/2416	10	{Means for guiding or retaining wires or cables connected to terminal blocks}	H01R9/24	H01R9/24		943
H01R9/2425	10	{Structural association with built-in components (for coupling parts H01R13/66)}	H01R9/24	H01R9/24		361
H01R9/2433	11	{with built-in switch}	H01R9/24	H01R9/24		193
H01R9/2441	11	{with built-in overvoltage protection}	H01R9/24	H01R9/24		147
H01R9/245	11	{with built-in fuse}	H01R9/24	H01R9/24		128
H01R9/2458	10	{Electrical interconnections between terminal blocks}	H01R9/24	H01R9/24		497
H01R9/2466	11	{using a planar conductive structure, e.g. printed circuit board}	H01R9/24	H01R9/24		227
H01R9/2475	10	{Means facilitating correct wiring, e.g. marking plates, identification tags}	H01R9/24	H01R9/24		292
H01R9/2483	10	{specially adapted for ground connection}	H01R9/24	H01R9/24		243
H01R9/2491	10	{Terminal blocks structurally associated with plugs or sockets}	H01R9/24	H01R9/24		816
H01R9/26	10	Clip-on terminal blocks for side-by-side rail- or strip-mounting	H01R9/26	H01R9/26		1296
H01R9/2608	11	{Fastening means for mounting on support rail or strip (H01R9/2691 takes precedence; for switch or other electrical device H02B1/042)}	H01R9/26	H01R9/26		632
H01R9/2616	11	{End clamping members}	H01R9/26	H01R9/26		110
H01R9/2625	11	{with built-in electrical component}	H01R9/26	H01R9/26		248
H01R9/2633	12	{with built-in switch}	H01R9/26	H01R9/26		255
H01R9/2641	12	{with built-in overvoltage protection}	H01R9/26	H01R9/26		88
H01R9/265	12	{with built-in fuse}	H01R9/26	H01R9/26		52
H01R9/2658	12	{with built-in data-bus connection}	H01R9/26	H01R9/26		96
H01R9/2666	12	{with built-in test-points}	H01R9/26	H01R9/26		81
H01R9/2675	11	{Electrical interconnections between two blocks, e.g. by means of busbars}	H01R9/26	H01R9/26		620
H01R9/2683	11	{Marking plates or tabs}	H01R9/26	H01R9/26		192
H01R9/2691	11	{with ground wire connection to the rail}	H01R9/26	H01R9/26		232
H01R9/28	9	Terminal boards	H01R9/28	H01R9/28		475
H01R11/00	7	Individual connecting elements providing two or more spaced connecting locations for conductive members which are, or may be, thereby interconnected, e.g. end pieces for wires or cables supported by the wire or cable and having means for facilitating electrical connection to some other wire, terminal, or conductive member, blocks of binding posts	H01R11/00	H01R11/00		165
H01R11/01	8	characterised by the form or arrangement of the conductive interconnection between the connecting locations	H01R11/01	H01R11/01		2329
H01R11/03	8	characterised by the relationship between the connecting locations (H01R11/11 takes precedence)	H01R11/03	H01R11/03		314
H01R11/05	9	the connecting locations having different types of direct connections	H01R11/05	H01R11/05		791
H01R11/07	9	the connecting locations being of the same type but different sizes	H01R11/07	H01R11/07		203
H01R11/09	9	the connecting locations being identical	H01R11/09	H01R11/09		1743
H01R11/11	8	End pieces or tapping pieces for wires, supported by the wire and for facilitating electrical connection to some other wire, terminal or conductive member (H01R11/01 takes precedence)	H01R11/11	H01R11/11		2843
H01R11/12	9	End pieces terminating in an eye, hook, or fork	H01R11/12	H01R11/12		2342
H01R11/14	10	the hook being adapted for hanging on overhead or other suspended lines, e.g. hot line clamp	H01R11/14	H01R11/14		1646
H01R11/15	11	Hook in the form of a screw clamp	H01R11/15	H01R11/15		485
H01R11/16	9	End pieces terminating in a soldering tip or socket	H01R11/16	H01R11/16		88
H01R11/18	9	End pieces terminating in a probe	H01R11/18	H01R11/18		485
H01R11/20	9	End pieces terminating in a needle point or analogous contact for penetrating insulation or cable strands	H01R11/20	H01R11/20		222
H01R11/22	9	End pieces terminating in a spring clip	H01R11/22	H01R11/22		624
H01R11/24	10	with gripping jaws, e.g. crocodile clip	H01R11/24	H01R11/24		656
H01R11/26	9	End pieces terminating in a screw clamp, screw or nut	H01R11/26	H01R11/26		625
H01R11/28	9	End pieces consisting of a ferrule or sleeve	H01R11/28	H01R11/28		381
H01R11/281	10	{for connections to batteries}	H01R11/28	H01R11/28		1040
H01R11/282	11	{comprising means for facilitating engagement or disengagement, e.g. quick release terminal}	H01R11/28	H01R11/28		631
H01R11/283	11	{Bolt, screw or threaded ferrule parallel to the battery post}	H01R11/28	H01R11/28		443
H01R11/284	11	{comprising means for preventing corrosion, e.g. covers, enclosures filled with gel}	H01R11/28	H01R11/28		250
H01R11/285	11	{Battery post and cable secured by the same locking means}	H01R11/28	H01R11/28		136
H01R11/286	11	{having means for improving contact between battery post and clamping member, e.g. uneven interior surface}	H01R11/28	H01R11/28		169
H01R11/287	11	{Intermediate parts between battery post and cable end piece}	H01R11/28	H01R11/28		389
H01R11/288	11	{Interconnections between batteries}	H01R11/28	H01R11/28		344
H01R11/289	11	{characterised by the shape or the structure of the battery post}	H01R11/28	H01R11/28		236
H01R11/30	9	End pieces held in contact by a magnet	H01R11/30	H01R11/30		503
H01R11/32	9	End pieces with two or more terminations	H01R11/32	H01R11/32		298
H01R12/00	7	Structural associations of a plurality of mutually-insulated electrical connecting elements, specially adapted for printed circuits, e.g. printed circuit boards [PCB], flat or ribbon cables, or like generally planar structures, e.g. terminal strips, terminal blocks; Coupling devices specially adapted for printed circuits, flat or ribbon cables, or like generally planar structures; Terminals specially adapted for contact with, or insertion into, printed circuits, flat or ribbon cables, or like generally planar structures (printed connections to, or between, printed circuits H05K1/11)	H01R12/00	H01R12/00		1321
H01R12/50	8	Fixed connections	H01R12/50	H01R12/50		120
H01R12/51	9	for rigid printed circuits or like structures	H01R12/51	H01R12/51		750
H01R12/515	10	{Terminal blocks providing connections to wires or cables}	H01R12/51	H01R12/51		1003
H01R12/52	10	connecting to other rigid printed circuits or like structures	H01R12/52	H01R12/52		2133
H01R12/523	11	{by an interconnection through aligned holes in the boards or multilayer board}	H01R12/52	H01R12/52		640
H01R12/526	11	{the printed circuits being on the same board (with plated through holes H05K3/42)}	H01R12/52	H01R12/52		170
H01R12/53	10	connecting to cables except for flat or ribbon cables	H01R12/53	H01R12/53		823
H01R12/55	10	characterised by the terminals	H01R12/55	H01R12/55		827
H01R12/57	11	surface mounting terminals	H01R12/57	H01R12/57		4012
H01R12/58	11	terminals for insertion into holes	H01R12/58	H01R12/58		2871
H01R12/585	12	{Terminals having a press fit or a compliant portion and a shank passing through a hole in the printed circuit board}	H01R12/58	H01R12/58		1883
H01R12/59	9	for flexible printed circuits, flat or ribbon cables or like structures	H01R12/59	H01R12/59		524
H01R12/592	10	{connections to contact elements}	H01R12/59	H01R12/59		923
H01R12/594	10	{for shielded flat cable}	H01R12/59	H01R12/59		120
H01R12/596	11	{Connection of the shield to an additional grounding conductor, e.g. drain wire}	H01R12/59	H01R12/59		89
H01R12/598	11	{Each conductor being individually surrounded by shield, e.g. multiple coaxial cables in flat structure}	H01R12/59	H01R12/59		183
H01R12/61	10	connecting to flexible printed circuits, flat or ribbon cables or like structures	H01R12/61	H01R12/61		357
H01R12/613	11	{by means of interconnecting elements}	H01R12/61	H01R12/61		188
H01R12/616	12	{having contacts penetrating insulation for making contact with conductors, e.g. needle points}	H01R12/61	H01R12/61		237
H01R12/62	10	connecting to rigid printed circuits or like structures	H01R12/62	H01R12/62		1304
H01R12/63	10	connecting to another shape cable	H01R12/63	H01R12/63		151
H01R12/65	10	characterised by the terminal	H01R12/65	H01R12/65		324
H01R12/67	11	insulation penetrating terminals	H01R12/67	H01R12/67		419
H01R12/675	12	{with contacts having at least a slotted plate for penetration of cable insulation, e.g. insulation displacement contacts for round conductor flat cables}	H01R12/67	H01R12/67		770
H01R12/68	12	comprising deformable portions	H01R12/68	H01R12/68		242
H01R12/69	11	deformable terminals, e.g. crimping terminals	H01R12/69	H01R12/69		164
H01R12/70	8	Coupling devices	H01R12/70	H01R12/70		626
H01R12/7005	9	{Guiding, mounting, polarizing or locking means; Extractors (for printed circuit boards H05K)}	H01R12/70	H01R12/70		1703
H01R12/7011	10	{Locking or fixing a connector to a PCB}	H01R12/70	H01R12/70		587
H01R12/7017	11	{Snap means}	H01R12/70	H01R12/70		124
H01R12/7023	12	{integral with the coupling device}	H01R12/70	H01R12/70		513
H01R12/7029	12	{not integral with the coupling device}	H01R12/70	H01R12/70		612
H01R12/7035	11	{involving non-elastic deformation, e.g. plastic deformation, melting (H01R12/7064 takes precedence)}	H01R12/70	H01R12/70		40
H01R12/7041	11	{Gluing or taping}	H01R12/70	H01R12/70		50
H01R12/7047	11	{with a fastener through a screw hole in the coupling device}	H01R12/70	H01R12/70		638
H01R12/7052	11	{characterised by the locating members}	H01R12/70	H01R12/70		492
H01R12/7058	11	{characterised by the movement, e.g. pivoting, camming or translating parallel to the PCB}	H01R12/70	H01R12/70		204
H01R12/7064	11	{Press fitting}	H01R12/70	H01R12/70		573
H01R12/707	11	{Soldering or welding}	H01R12/70	H01R12/70		1802
H01R12/7076	9	{for connection between PCB and component, e.g. display}	H01R12/70	H01R12/70		1741
H01R12/7082	9	{Coupling device supported only by cooperation with PCB}	H01R12/70	H01R12/70		1070
H01R12/7088	9	{Arrangements for power supply}	H01R12/70	H01R12/70		811
H01R12/7094	9	{with switch operated by engagement of PCB}	H01R12/70	H01R12/70		195
H01R12/71	9	for rigid printing circuits or like structures	H01R12/71	H01R12/71		3102
H01R12/712	10	{co-operating with the surface of the printed circuit or with a coupling device exclusively provided on the surface of the printed circuit (H01R12/72 takes precedence)}	H01R12/71	H01R12/71		1138
H01R12/714	11	{with contacts abutting directly the printed circuit; Button contacts therefore provided on the printed circuit}	H01R12/71	H01R12/71		3542
H01R12/716	11	{Coupling device provided on the PCB}	H01R12/71	H01R12/71		6978
H01R12/718	12	{Contact members provided on the PCB without an insulating housing (contacts for abutting H01R12/714)}	H01R12/71	H01R12/71		876
H01R12/72	10	coupling with the edge of the rigid printed circuits or like structures	H01R12/72	H01R12/72		632
H01R12/721	11	{cooperating directly with the edge of the rigid printed circuits}	H01R12/72	H01R12/72		4200
H01R12/722	11	{coupling devices mounted on the edge of the printed circuits}	H01R12/72	H01R12/72		1186
H01R12/724	12	{containing contact members forming a right angle}	H01R12/72	H01R12/72		2919
H01R12/725	12	{containing contact members presenting a contact carrying strip, e.g. edge-like strip}	H01R12/72	H01R12/72		646
H01R12/727	12	{Coupling devices presenting arrays of contacts}	H01R12/72	H01R12/72		881
H01R12/728	12	{Coupling devices without an insulating housing provided on the edge of the PCB}	H01R12/72	H01R12/72		249
H01R12/73	11	connecting to other rigid printed circuits or like structures	H01R12/73	H01R12/73		2010
H01R12/732	12	{Printed circuits being in the same plane}	H01R12/73	H01R12/73		507
H01R12/735	12	{Printed circuits including an angle between each other}	H01R12/73	H01R12/73		71
H01R12/737	13	{Printed circuits being substantially perpendicular to each other (for printed connections H05K3/366)}	H01R12/73	H01R12/73		1073
H01R12/75	10	connecting to cables except for flat or ribbon cables	H01R12/75	H01R12/75		1117
H01R12/77	9	for flexible printed circuits, flat or ribbon cables or like structures	H01R12/77	H01R12/77		927
H01R12/771	10	{Details}	H01R12/77	H01R12/77		605
H01R12/772	11	{Strain relieving means}	H01R12/77	H01R12/77		399
H01R12/774	11	{Retainers}	H01R12/77	H01R12/77		883
H01R12/775	11	{Ground or shield arrangements}	H01R12/77	H01R12/77		533
H01R12/777	10	{Coupling parts carrying pins, blades or analogous contacts (H01R12/78, H01R12/79 take precedence)}	H01R12/77	H01R12/77		436
H01R12/778	10	{Coupling parts carrying sockets, clips or analogous counter-contacts (H01R12/78, H01R12/79 take precedence)}	H01R12/77	H01R12/77		458
H01R12/78	10	connecting to other flexible printed circuits, flat or ribbon cables or like structures	H01R12/78	H01R12/78		668
H01R12/79	10	connecting to rigid printed circuits or like structures	H01R12/79	H01R12/79		2774
H01R12/81	10	connecting to another cable except for flat or ribbon cable	H01R12/81	H01R12/81		176
H01R12/82	9	connected with low or zero insertion force	H01R12/82	H01R12/82		362
H01R12/83	10	connected with pivoting of printed circuits or like after insertion	H01R12/83	H01R12/83		379
H01R12/85	10	contact pressure producing means, contacts activated after insertion of printed circuits or like structures	H01R12/85	H01R12/85		191
H01R12/853	11	{Fluid activated}	H01R12/85	H01R12/85		38
H01R12/856	11	{activated by shape memory material}	H01R12/85	H01R12/85		21
H01R12/87	11	acting automatically by insertion of rigid printed or like structures	H01R12/87	H01R12/87		266
H01R12/88	11	acting manually by rotating or pivoting connector housing parts	H01R12/88	H01R12/88		1394
H01R12/89	11	acting manually by moving connector housing parts linearly, e.g. slider	H01R12/89	H01R12/89		499
H01R12/91	9	allowing relative movement between coupling parts, e.g. floating or self aligning (for coupling devices not specially adapted for printed circuits, flat or ribbon cables, or like generally planar structures, H01R13/6315 takes precedence)	H01R12/91	H01R12/91		1041
H01R13/00	7	Details of coupling devices of the kinds covered by groups H01R12/70 or H01R24/00 - H01R33/00	H01R13/00	H01R13/00		630
H01R13/005	8	{Electrical coupling combined with fluidic coupling}	H01R13/00	H01R13/00		779
H01R13/02	8	Contact members	H01R13/02	H01R13/02		9464
H01R13/025	9	{formed by the conductors of a cable end}	H01R13/02	H01R13/02		462
H01R13/03	9	characterised by the material, e.g. plating, or coating materials	H01R13/03	H01R13/03		3587
H01R13/035	10	{Plated dielectric material}	H01R13/03	H01R13/03		311
H01R13/04	9	Pins or blades for co-operation with sockets	H01R13/04	H01R13/04		4881
H01R13/05	10	Resilient pins or blades (carrying separate resilient parts H01R13/15)	H01R13/05	H01R13/05		847
H01R13/052	11	{co-operating with sockets having a circular transverse section}	H01R13/05	H01R13/05		614
H01R13/055	11	{co-operating with sockets having a rectangular transverse section}	H01R13/05	H01R13/05		325
H01R13/057	11	{co-operating with sockets having a square transverse section}	H01R13/05	H01R13/05		46
H01R13/08	10	Resiliently-mounted rigid pins or blades	H01R13/08	H01R13/08		435
H01R13/10	9	Sockets for co-operation with pins or blades	H01R13/10	H01R13/10		4118
H01R13/11	10	Resilient sockets (carrying separate resilient parts H01R13/15)	H01R13/11	H01R13/11		2569
H01R13/111	11	{co-operating with pins having a circular transverse section}	H01R13/11	H01R13/11		2185
H01R13/112	11	{forked sockets having two legs}	H01R13/11	H01R13/11		1397
H01R13/113	11	{co-operating with pins or blades having a rectangular transverse section}	H01R13/11	H01R13/11		2167
H01R13/114	11	{co-operating with pins or blades having a square transverse section}	H01R13/11	H01R13/11		321
H01R13/115	11	U-shaped sockets having inwardly bent legs, e.g. spade type	H01R13/115	H01R13/115		976
H01R13/14	10	Resiliently-mounted rigid sockets	H01R13/14	H01R13/14		205
H01R13/15	9	Pins, blades or sockets having separate spring member for producing or increasing contact pressure	H01R13/15	H01R13/15		1155
H01R13/17	10	with spring member on the pin	H01R13/17	H01R13/17		869
H01R13/18	10	with the spring member surrounding the socket	H01R13/18	H01R13/18		1028
H01R13/187	10	with spring member in the socket	H01R13/187	H01R13/187		2554
H01R13/193	9	Means for increasing contact pressure at the end of engagement of coupling part {, e.g. zero insertion force or no friction}	H01R13/193	H01R13/193		2015
H01R13/20	9	Pins, blades, or sockets shaped, or provided with separate member, to retain co-operating parts together	H01R13/20	H01R13/20		2013
H01R13/207	10	by screw-in connection	H01R13/207	H01R13/207		168
H01R13/213	10	by bayonet connection	H01R13/213	H01R13/213		280
H01R13/22	9	Contacts for co-operating by abutting	H01R13/22	H01R13/22		919
H01R13/24	10	resilient; resiliently-mounted	H01R13/24	H01R13/24		3097
H01R13/2407	11	{characterized by the resilient means}	H01R13/24	H01R13/24		1391
H01R13/2414	12	{conductive elastomers}	H01R13/24	H01R13/24		1774
H01R13/2421	12	{using coil springs}	H01R13/24	H01R13/24		2442
H01R13/2428	12	{using meander springs}	H01R13/24	H01R13/24		587
H01R13/2435	11	{with opposite contact points, e.g. C beam}	H01R13/24	H01R13/24		643
H01R13/2442	11	{with a single cantilevered beam}	H01R13/24	H01R13/24		1544
H01R13/245	11	{by stamped-out resilient contact arm}	H01R13/24	H01R13/24		230
H01R13/2457	11	{consisting of at least two resilient arms contacting the same counterpart}	H01R13/24	H01R13/24		280
H01R13/2464	11	{characterized by the contact point}	H01R13/24	H01R13/24		416
H01R13/2471	12	{pin shaped}	H01R13/24	H01R13/24		321
H01R13/2478	12	{spherical}	H01R13/24	H01R13/24		202
H01R13/2485	12	{for contacting a ball}	H01R13/24	H01R13/24		132
H01R13/2492	12	{multiple contact points}	H01R13/24	H01R13/24		435
H01R13/26	9	Pin or blade contacts for sliding co-operation on one side only {(for modular jack type connectors H01R24/62)}	H01R13/26	H01R13/26		1142
H01R13/28	9	Contacts for sliding cooperation with identically-shaped contact, e.g. for hermaphroditic coupling devices {(H01R24/84 takes precedence)}	H01R13/28	H01R13/28		901
H01R13/33	9	Contact members made of resilient wire	H01R13/33	H01R13/33		662
H01R13/35	9	for non-simultaneous co-operation with different types of contact member, e.g. socket co-operating with either round or flat pin	H01R13/35	H01R13/35		324
H01R13/40	8	Securing contact members in or to a base or case; Insulating of contact members	H01R13/40	H01R13/40		6609
H01R13/405	9	Securing in non-demountable manner, e.g. moulding, riveting	H01R13/405	H01R13/405		3635
H01R13/41	10	by frictional grip in grommet, panel or base	H01R13/41	H01R13/41		1484
H01R13/415	10	by permanent deformation of contact member	H01R13/415	H01R13/415		430
H01R13/42	9	Securing in a demountable manner	H01R13/42	H01R13/42		2231
H01R13/422	10	Securing in resilient one-piece base or case, {e.g. by friction}; One-piece base or case formed with resilient locking means	H01R13/422	H01R13/422		812
H01R13/4223	11	{comprising integral flexible contact retaining fingers}	H01R13/422	H01R13/422		1210
H01R13/4226	12	{comprising two or more integral flexible retaining fingers acting on a single contact}	H01R13/422	H01R13/422		229
H01R13/424	10	Securing in base or case composed of a plurality of insulating parts having at least one resilient insulating part	H01R13/424	H01R13/424		707
H01R13/426	10	Securing by a separate resilient retaining piece supported by base or case, e.g. collar {or metal contact-retention clip}	H01R13/426	H01R13/426		763
H01R13/428	10	by resilient locking means on the contact members; by locking means on resilient contact members	H01R13/428	H01R13/428		797
H01R13/432	11	by stamped-out resilient tongue snapping behind shoulder in base or case	H01R13/432	H01R13/432		1302
H01R13/434	11	by separate resilient locking means on contact member, e.g. retainer collar or ring around contact member	H01R13/434	H01R13/434		316
H01R13/436	10	Securing a plurality of contact members by one locking piece {or operation}	H01R13/436	H01R13/436		532
H01R13/4361	11	{Insertion of locking piece perpendicular to direction of contact insertion}	H01R13/436	H01R13/436		701
H01R13/4362	12	{comprising a temporary and a final locking position}	H01R13/436	H01R13/436		776
H01R13/4364	11	{Insertion of locking piece from the front}	H01R13/436	H01R13/436		379
H01R13/4365	12	{comprising a temporary and a final locking position}	H01R13/436	H01R13/436		346
H01R13/4367	11	{Insertion of locking piece from the rear}	H01R13/436	H01R13/436		405
H01R13/4368	12	{comprising a temporary and a final locking position}	H01R13/436	H01R13/436		239
H01R13/44	8	Means for preventing access to live contacts {(making use of a switch actuated by engagement of counterpart H01R13/7036)}	H01R13/44	H01R13/44		3252
H01R13/443	9	Dummy plugs	H01R13/443	H01R13/443		579
H01R13/447	9	Shutter or cover plate	H01R13/447	H01R13/447		4233
H01R13/453	10	Shutter or cover plate opened by engagement of counterpart	H01R13/453	H01R13/453		823
H01R13/4532	11	{Rotating shutter}	H01R13/453	H01R13/453		829
H01R13/4534	11	{Laterally sliding shutter}	H01R13/453	H01R13/453		923
H01R13/4536	11	{Inwardly pivoting shutter}	H01R13/453	H01R13/453		274
H01R13/4538	11	{Covers sliding or withdrawing in the direction of engagement}	H01R13/453	H01R13/453		777
H01R13/46	8	Bases; Cases	H01R13/46	H01R13/46		5023
H01R13/465	9	{Identification means, e.g. labels, tags, markings (H01R9/2475, H01R9/2683 take precedence)}	H01R13/46	H01R13/46		1336
H01R13/50	9	formed as an integral body (H01R13/514 takes precedence)	H01R13/50	H01R13/50		1192
H01R13/501	10	{comprising an integral hinge or a frangible part}	H01R13/50	H01R13/50		909
H01R13/502	9	composed of different pieces (H01R13/514 takes precedence)	H01R13/502	H01R13/502		15722
H01R13/5025	10	{one or more pieces being of resilient material}	H01R13/502	H01R13/502		474
H01R13/504	10	different pieces being moulded, cemented, welded, e.g. ultrasonic welding, or swaged together	H01R13/504	H01R13/504		1723
H01R13/5045	11	{different pieces being assembled by press-fit}	H01R13/504	H01R13/504		329
H01R13/506	10	assembled by snap action of the parts	H01R13/506	H01R13/506		5388
H01R13/508	10	assembled by {a separate} clip or spring	H01R13/508	H01R13/508		1329
H01R13/512	10	assembled by screw or screws	H01R13/512	H01R13/512		1833
H01R13/514	9	composed as a modular blocks or assembly, i.e. composed of co-operating parts provided with contact members or holding contact members between them	H01R13/514	H01R13/514		5181
H01R13/516	9	Means for holding or embracing insulating body, e.g. casing {, hoods}	H01R13/516	H01R13/516		3235
H01R13/518	10	for holding or embracing several coupling parts, e.g. frames	H01R13/518	H01R13/518		2224
H01R13/52	9	Dustproof, splashproof, drip-proof, waterproof, or flameproof cases	H01R13/52	H01R13/52		5666
H01R13/5202	10	{Sealing means between parts of housing or between housing part and a wall, e.g. sealing rings}	H01R13/52	H01R13/52		6122
H01R13/5205	10	{Sealing means between cable and housing, e.g. grommet (H01R13/5221 takes precedence)}	H01R13/52	H01R13/52		3197
H01R13/5208	11	{having at least two cable receiving openings}	H01R13/52	H01R13/52		1107
H01R13/521	10	{Sealing between contact members and housing, e.g. sealing insert}	H01R13/52	H01R13/52		2716
H01R13/5213	10	{Covers}	H01R13/52	H01R13/52		5056
H01R13/5216	10	{characterised by the sealing material, e.g. gels or resins}	H01R13/52	H01R13/52		2106
H01R13/5219	10	{Sealing means between coupling parts, e.g. interfacial seal}	H01R13/52	H01R13/52		4159
H01R13/5221	11	{having cable sealing means}	H01R13/52	H01R13/52		949
H01R13/5224	10	{for medical use}	H01R13/52	H01R13/52		371
H01R13/5227	10	{with evacuation of penetrating liquids}	H01R13/52	H01R13/52		646
H01R13/523	10	for use under water	H01R13/523	H01R13/523		1529
H01R13/527	10	Flameproof cases (H01R13/70 takes precedence)	H01R13/527	H01R13/527		503
H01R13/53	9	Bases or cases for heavy duty; Bases or cases {for high voltage} with means for preventing corona or arcing	H01R13/53	H01R13/53		2355
H01R13/533	9	Bases, cases made for use in extreme conditions, e.g. high temperature, radiation, vibration, corrosive environment, pressure (H01R13/52 takes precedence)	H01R13/533	H01R13/533		3146
H01R13/56	8	Means for preventing chafing or fracture of flexible leads at outlet from coupling part	H01R13/56	H01R13/56		1114
H01R13/562	9	{Bending-relieving}	H01R13/56	H01R13/56		924
H01R13/565	9	{Torsion-relieving}	H01R13/56	H01R13/56		168
H01R13/567	9	{Traverse cable outlet or wire connection}	H01R13/56	H01R13/56		451
H01R13/58	8	Means for relieving strain on wire connection, e.g. cord grip {, for avoiding loosening of connections between wires and terminals within a coupling device terminating a cable (for flat or ribbon cables H01R12/771)}	H01R13/58	H01R13/58		2134
H01R13/5804	9	{comprising a separate cable clamping part (H01R13/5841 takes precedence)}	H01R13/58	H01R13/58		1014
H01R13/5808	10	{formed by a metallic element crimped around the cable (H01R4/185 takes precedence)}	H01R13/58	H01R13/58		306
H01R13/5812	10	{the cable clamping being achieved by mounting the separate part on the housing of the coupling device}	H01R13/58	H01R13/58		988
H01R13/5816	10	{for cables passing through an aperture in a housing wall, the separate part being captured between cable and contour of aperture}	H01R13/58	H01R13/58		292
H01R13/582	9	{the cable being clamped between assembled parts of the housing}	H01R13/58	H01R13/58		594
H01R13/5825	10	{the means comprising additional parts captured between housing parts and cable}	H01R13/58	H01R13/58		433
H01R13/5829	10	{the clamping part being flexibly or hingedly connected to the housing}	H01R13/58	H01R13/58		343
H01R13/5833	9	{the cable being forced in a tortuous or curved path, e.g. knots in cable (H01R13/582 takes precedence)}	H01R13/58	H01R13/58		479
H01R13/5837	9	{specially adapted for accommodating various sized cables (H01R13/5825 takes precedence)}	H01R13/58	H01R13/58		289
H01R13/5841	9	{allowing different orientations of the cable with respect to the coupling direction}	H01R13/58	H01R13/58		372
H01R13/5845	9	{the strain relief being achieved by molding parts around cable and connections}	H01R13/58	H01R13/58		603
H01R13/585	9	Grip increasing with strain force	H01R13/585	H01R13/585		227
H01R13/59	9	Threaded ferrule or bolt operating in a direction parallel to the cable or wire	H01R13/59	H01R13/59		751
H01R13/595	9	Bolts operating in a direction transverse to the cable or wire	H01R13/595	H01R13/595		798
H01R13/60	8	Means for supporting coupling part when not engaged	H01R13/60	H01R13/60		2117
H01R13/62	8	Means for facilitating engagement or disengagement of coupling parts or for holding them in engagement	H01R13/62	H01R13/62		2792
H01R13/6205	9	{Two-part coupling devices held in engagement by a magnet}	H01R13/62	H01R13/62		3080
H01R13/621	9	Bolt, set screw or screw clamp	H01R13/621	H01R13/621		1044
H01R13/6215	10	{using one or more bolts}	H01R13/621	H01R13/621		1339
H01R13/622	9	Screw-ring or screw-casing (H01R13/623 takes precedence)	H01R13/622	H01R13/622		2051
H01R13/623	9	Casing or ring with helicoidal groove	H01R13/623	H01R13/623		678
H01R13/625	9	Casing or ring with bayonet engagement	H01R13/625	H01R13/625		1220
H01R13/627	9	Snap or like fastening	H01R13/627	H01R13/627		4714
H01R13/6271	10	{Latching means integral with the housing (H01R13/6276, H01R13/6277, H01R13/6278 take precedence)}	H01R13/627	H01R13/627		1271
H01R13/6272	11	{comprising a single latching arm}	H01R13/627	H01R13/627		2359
H01R13/6273	11	{comprising two latching arms}	H01R13/627	H01R13/627		1737
H01R13/6275	10	{Latching arms not integral with the housing (H01R13/6276, H01R13/6277, H01R13/6278 take precedence)}	H01R13/627	H01R13/627		3285
H01R13/6276	10	{comprising one or more balls engaging in a hole or a groove}	H01R13/627	H01R13/627		389
H01R13/6277	10	{comprising annular latching means, e.g. ring snapping in an annular groove}	H01R13/627	H01R13/627		812
H01R13/6278	10	{comprising a pin snapping into a recess}	H01R13/627	H01R13/627		854
H01R13/629	9	Additional means for facilitating engagement or disengagement of coupling parts, e.g. aligning or guiding means, levers, gas pressure {electrical locking indicators, manufacturing tolerances (separate tools or apparatus H01R43/26)}	H01R13/629	H01R13/629		11667
H01R13/62905	10	{comprising a camming member (H01R13/62933 and H01R13/641 take precedence)}	H01R13/629	H01R13/629		566
H01R13/62911	11	{U-shaped sliding element}	H01R13/629	H01R13/629		234
H01R13/62916	11	{Single camming plate}	H01R13/629	H01R13/629		66
H01R13/62922	11	{Pair of camming plates}	H01R13/629	H01R13/629		161
H01R13/62927	11	{Comprising supplementary or additional locking means}	H01R13/629	H01R13/629		217
H01R13/62933	10	{Comprising exclusively pivoting lever}	H01R13/629	H01R13/629		1298
H01R13/62938	11	{Pivoting lever comprising own camming means}	H01R13/629	H01R13/629		1053
H01R13/62944	11	{Pivoting lever comprising gear teeth}	H01R13/629	H01R13/629		354
H01R13/6295	11	{Pivoting lever comprising means indicating incorrect coupling of mating connectors}	H01R13/629	H01R13/629		177
H01R13/62955	11	{Pivoting lever comprising supplementary/additional locking means}	H01R13/629	H01R13/629		762
H01R13/62961	11	{Pivoting lever having extendable handle}	H01R13/629	H01R13/629		59
H01R13/62966	11	{Comprising two pivoting levers}	H01R13/629	H01R13/629		212
H01R13/62972	12	{Wherein the pivoting levers are two lever plates}	H01R13/629	H01R13/629		62
H01R13/62977	10	{Pivoting levers actuating linearly camming means}	H01R13/629	H01R13/629		272
H01R13/62983	10	{Linear camming means or pivoting lever for connectors for flexible or rigid printed circuit boards, flat or ribbon cables}	H01R13/629	H01R13/629		41
H01R13/62988	11	{Lever acting directly on flexible or rigid printed circuit boards, flat or ribbon cables, e.g. recess provided to this purposeon the surface or edge of the flexible or rigid printed circuit boards, flat or ribbon cables}	H01R13/629	H01R13/629		113
H01R13/62994	11	{Lever acting on a connector mounted onto the flexible or rigid printed circuit boards, flat or ribbon cables}	H01R13/629	H01R13/629		71
H01R13/631	10	for engagement only	H01R13/631	H01R13/631		5209
H01R13/6315	11	{allowing relative movement between coupling parts, e.g. floating connection (for coupling devices specially adapted for printed circuits, flat or ribbon cables, or like generally planar structures, H01R12/91 takes precedence)}	H01R13/631	H01R13/631		2686
H01R13/633	10	for disengagement only {(in combination with safety switch H01R13/7132)}	H01R13/633	H01R13/633		3098
H01R13/6335	11	{comprising a handle}	H01R13/633	H01R13/633		1330
H01R13/635	11	by mechanical pressure, e.g. spring force	H01R13/635	H01R13/635		2196
H01R13/637	11	by fluid pressure, e.g. explosion	H01R13/637	H01R13/637		173
H01R13/639	9	Additional means for holding or locking coupling parts together, after engagement, {e.g. separate keylock, retainer strap}	H01R13/639	H01R13/639		17830
H01R13/6392	10	{for extension cord}	H01R13/639	H01R13/639		735
H01R13/6395	10	{for wall or panel outlets}	H01R13/639	H01R13/639		1082
H01R13/6397	10	{with means for preventing unauthorised use}	H01R13/639	H01R13/639		1291
H01R13/64	8	Means for preventing incorrect coupling	H01R13/64	H01R13/64		4758
H01R13/641	9	by indicating incorrect coupling; by indicating correct or full engagement	H01R13/641	H01R13/641		2791
H01R13/642	9	by position or shape of contact members	H01R13/642	H01R13/642		1369
H01R13/645	9	by exchangeable elements on case or base	H01R13/645	H01R13/645		596
H01R13/6453	10	{comprising pin-shaped elements, capable of being orientated in different angular positions around their own longitudinal axes, e.g. pins with hexagonal base}	H01R13/645	H01R13/645		227
H01R13/6456	10	{comprising keying elements at different positions along the periphery of the connector}	H01R13/645	H01R13/645		650
H01R13/646	8	specially adapted for high-frequency, e.g. structures providing an impedance match or phase match (non-coaxed protective earth or shield arrangements H01R13/648; coaxed connectors specially adapted for high frequency H01R24/40)	H01R13/646	H01R13/646		768
H01R13/6461	9	Means for preventing cross-talk	H01R13/6461	H01R13/6461		1247
H01R13/6463	10	using twisted pairs of wires	H01R13/6463	H01R13/6463		370
H01R13/6464	10	by adding capacitive elements	H01R13/6464	H01R13/6464		281
H01R13/6466	11	on substrates, e.g. printed circuit boards [PCB]	H01R13/6466	H01R13/6466		335
H01R13/6467	10	by cross-over of signal conductors	H01R13/6467	H01R13/6467		240
H01R13/6469	11	on substrates	H01R13/6469	H01R13/6469		134
H01R13/6471	10	by special arrangement of ground and signal conductors, e.g. GSGS [Ground-Signal-Ground-Signal]	H01R13/6471	H01R13/6471		1648
H01R13/6473	9	Impedance matching	H01R13/6473	H01R13/6473		688
H01R13/6474	10	by variation of conductive properties, e.g. by dimension variations	H01R13/6474	H01R13/6474		685
H01R13/6476	11	by making an aperture, e.g. a hole	H01R13/6476	H01R13/6476		118
H01R13/6477	10	by variation of dielectric properties	H01R13/6477	H01R13/6477		524
H01R13/648	8	Protective earth or shield arrangements on coupling devices {, e.g. anti-static shielding} &#160; (coaxially arranged shields H01R24/38)	H01R13/648	H01R13/648		3872
H01R13/6485	9	{Electrostatic discharge protection (in general H05F1/00, for electric apparatus H05K9/0067)}	H01R13/648	H01R13/648		754
H01R13/652	9	with earth pin, blade or socket	H01R13/652	H01R13/652		2523
H01R13/655	9	with earth brace	H01R13/655	H01R13/655		673
H01R13/658	9	High frequency shielding arrangements, e.g. against EMI [Electro-Magnetic Interference] or EMP [Electro-Magnetic Pulse] {(coaxial coupling devices specially adapted for high frequency H01R24/40; for flat or ribbon cable connectors H01R12/774; for coaxial cable H01R9/05)}	H01R13/658	H01R13/658		1455
H01R13/6581	10	Shield structure	H01R13/6581	H01R13/6581		4404
H01R13/6582	11	with resilient means for engaging mating connector	H01R13/6582	H01R13/6582		2348
H01R13/6583	12	with separate conductive resilient members between mating shield members	H01R13/6583	H01R13/6583		748
H01R13/6584	13	formed by conductive elastomeric members, e.g. flat gaskets or O-rings	H01R13/6584	H01R13/6584		330
H01R13/6585	11	Shielding material individually surrounding or interposed between mutually spaced contacts	H01R13/6585	H01R13/6585		1957
H01R13/6586	12	for separating multiple connector modules	H01R13/6586	H01R13/6586		405
H01R13/6587	13	for mounting on PCBs	H01R13/6587	H01R13/6587		922
H01R13/6588	12	with through openings for individual contacts	H01R13/6588	H01R13/6588		319
H01R13/6589	12	with wires separated by conductive housing parts	H01R13/6589	H01R13/6589		209
H01R13/659	11	with plural ports for distinct connectors	H01R13/659	H01R13/659		363
H01R13/6591	10	Specific features or arrangements of connection of shield to conductive members	H01R13/6591	H01R13/6591		818
H01R13/65912	11	{for shielded multiconductor cable (coaxial cables with one conductor surrounded by shield H01R9/05; flat shielded cables H01R12/594)}	H01R13/6591	H01R13/6591		671
H01R13/65914	12	{Connection of shield to additional grounding conductors}	H01R13/6591	H01R13/6591		339
H01R13/65915	12	{Twisted pair of conductors surrounded by shield}	H01R13/6591	H01R13/6591		255
H01R13/65917	12	{Connection to shield by means of resilient members}	H01R13/6591	H01R13/6591		115
H01R13/65918	12	{wherein each conductor is individually surrounded by shield}	H01R13/6591	H01R13/6591		159
H01R13/6592	11	the conductive member being a shielded cable	H01R13/6592	H01R13/6592		1452
H01R13/6593	12	the shield being composed of different pieces	H01R13/6593	H01R13/6593		1066
H01R13/6594	11	the shield being mounted on a PCB and connected to conductive members	H01R13/6594	H01R13/6594		1979
H01R13/6595	12	with separate members fixing the shield to the PCB	H01R13/6595	H01R13/6595		331
H01R13/6596	11	the conductive member being a metal grounding panel	H01R13/6596	H01R13/6596		660
H01R13/6597	11	the conductive member being a contact of the connector	H01R13/6597	H01R13/6597		585
H01R13/6598	10	Shield material	H01R13/6598	H01R13/6598		317
H01R13/6599	11	Dielectric material made conductive, e.g. plastic material coated with metal	H01R13/6599	H01R13/6599		594
H01R13/66	8	Structural association with built-in electrical component (coupling devices having concentrically or coaxially-arranged contacts H01R24/38)	H01R13/66	H01R13/66		4090
H01R13/6608	9	{with built-in single component (H01R13/68, H01R13/70 take precedence)}	H01R13/66	H01R13/66		380
H01R13/6616	10	{with resistor}	H01R13/66	H01R13/66		786
H01R13/6625	10	{with capacitive component}	H01R13/66	H01R13/66		538
H01R13/6633	10	{with inductive component, e.g. transformer}	H01R13/66	H01R13/66		884
H01R13/6641	10	{with diode (with LED H01R13/7175)}	H01R13/66	H01R13/66		399
H01R13/665	9	{with built-in electronic circuit (H01R13/70, H01R13/719 take precedence)}	H01R13/66	H01R13/66		4830
H01R13/6658	10	{on printed circuit board (H01R13/6666&#160;-&#160;H01R13/6691 take precedence)}<br><br><u>WARNING</u><br>This group is no longer used for the classification of new documents as from 2011-01-01. The backlog of this group is being continuously reclassified to H01R13/6466 and H01R13/6469	H01R13/66	H01R13/66		2739
H01R13/6666	10	{with built-in overvoltage protection}	H01R13/66	H01R13/66		1013
H01R13/6675	10	{with built-in power supply}	H01R13/66	H01R13/66		1877
H01R13/6683	10	{with built-in sensor}	H01R13/66	H01R13/66		4091
H01R13/6691	10	{with built-in signalling means (H01R13/717 takes precedence)}	H01R13/66	H01R13/66		2341
H01R13/68	9	with built-in fuse<br><br><u>WARNING</u><br>The subgroups of H01R13/68 are not complete pending completion of a reclassification, see also this group	H01R13/68	H01R13/68		1612
H01R13/684	10	the fuse being removable	H01R13/684	H01R13/684		163
H01R13/688	11	with housing part adapted for accessing the fuse	H01R13/688	H01R13/688		177
H01R13/692	12	Turnable housing part	H01R13/692	H01R13/692		17
H01R13/696	10	the fuse being integral with the terminal, e.g. pin or socket	H01R13/696	H01R13/696		96
H01R13/70	9	with built-in switch	H01R13/70	H01R13/70		5552
H01R13/701	10	{the switch being actuated by an accessory, e.g. cover, locking member}	H01R13/70	H01R13/70		2007
H01R13/703	10	operated by engagement or disengagement of coupling parts, {e.g. dual-continuity coupling part}(H01R13/71 takes precedence)	H01R13/703	H01R13/703		2219
H01R13/7031	11	{Shorting, shunting or bussing of different terminals interrupted or effected on engagement of coupling part, e.g. for ESD protection, line continuity}	H01R13/703	H01R13/703		693
H01R13/7032	12	{making use of a separate bridging element directly cooperating with the terminals}	H01R13/703	H01R13/703		557
H01R13/7033	12	{making use of elastic extensions of the terminals}	H01R13/703	H01R13/703		345
H01R13/7034	12	{the terminals being in direct electric contact separated by double sided connecting element (for printed circuit boards H01R12/7094)}	H01R13/703	H01R13/703		116
H01R13/7035	11	{comprising a separated limit switch}	H01R13/703	H01R13/703		757
H01R13/7036	11	{the switch being in series with coupling part, e.g. dead coupling, explosion proof coupling}	H01R13/703	H01R13/703		868
H01R13/7037	12	{making use of a magnetically operated switch}	H01R13/703	H01R13/703		240
H01R13/7038	12	{making use of a remote controlled switch, e.g. relais, solid state switch activated by the engagement of the coupling parts}	H01R13/703	H01R13/703		706
H01R13/7039	11	{the coupling part with coding means activating the switch to establish different circuits}	H01R13/703	H01R13/703		112
H01R13/707	10	interlocked with contact members or counterpart	H01R13/707	H01R13/707		849
H01R13/71	10	Contact members of coupling parts operating as switch {, e.g. linear or rotational movement required after mechanical engagement of coupling part to establish electrical connection}	H01R13/71	H01R13/71		1119
H01R13/713	10	the switch being a safety switch	H01R13/713	H01R13/713		1885
H01R13/7132	11	{having ejecting mechanisms}	H01R13/713	H01R13/713		102
H01R13/7135	11	{with ground fault protector (H01R13/7132 takes precedence)}	H01R13/713	H01R13/713		317
H01R13/7137	11	{with thermal interrupter (H01R13/7132 takes precedence)}	H01R13/713	H01R13/713		638
H01R13/717	9	with built-in light source	H01R13/717	H01R13/717		2603
H01R13/7172	10	{Conduits for light transmission}	H01R13/717	H01R13/717		364
H01R13/7175	10	{Light emitting diodes (LEDs)}	H01R13/717	H01R13/717		2267
H01R13/7177	10	{filament or neon bulb}	H01R13/717	H01R13/717		222
H01R13/719	9	specially adapted for high frequency, e.g. with filters<br><br><u>WARNING</u><br>The subgroups of H01R13/719 are not complete pending completion of a reclassification, see also H01R13/646 and the respective subgroups 	H01R13/719	H01R13/719		1040
H01R13/7193	10	with ferrite filters	H01R13/7193	H01R13/7193		169
H01R13/7195	10	with planar filters with openings for contacts	H01R13/7195	H01R13/7195		290
H01R13/7197	10	with filters integral with or fitted onto contacts, e.g. tubular filters	H01R13/7197	H01R13/7197		311
H01R13/72	8	Means for accommodating flexible lead within the holder	H01R13/72	H01R13/72		3411
H01R13/73	8	Means for mounting coupling parts to apparatus or structures, e.g. to a wall	H01R13/73	H01R13/73		4169
H01R13/74	9	Means for mounting coupling parts in openings of a panel	H01R13/74	H01R13/74		1946
H01R13/741	10	{using snap fastening means}	H01R13/74	H01R13/74		285
H01R13/743	11	{integral with the housing}	H01R13/74	H01R13/74		831
H01R13/745	11	{separate from the housing}	H01R13/74	H01R13/74		478
H01R13/746	10	{using a screw ring}	H01R13/74	H01R13/74		305
H01R13/748	10	{using one or more screws (H01R13/746 takes precedence)}	H01R13/74	H01R13/74		1100
H01R24/00	7	Two-part coupling devices, or either of their cooperating parts, characterised by their overall structure (contact members H01R13/02; securing contact members in or to a base or case or insulating of contact members H01R13/40; bases or cases H01R13/46; means for supporting coupling part when not engaged H01R13/60; means for facilitating engagement or disengagement of coupling parts or for holding them in engagement H01R13/62; means for preventing, inhibiting or avoiding incorrect coupling H01R13/64)<br><br><u>NOTE</u><br><br> In this group, it is desirable to add the indexing codes of groups H01R2101/00&#160;-&#160;H01R2107/00	H01R24/00	H01R24/00		5042
H01R24/005	8	{requiring successive relative motions to complete the coupling, e.g. bayonet type}	H01R24/00	H01R24/00		1617
H01R24/20	8	Coupling parts carrying sockets, clips or analogous contacts and secured only to wire or cable	H01R24/20	H01R24/20		2129
H01R24/22	9	with additional earth or shield contacts	H01R24/22	H01R24/22		553
H01R24/28	8	Coupling parts carrying pins, blades or analogous contacts and secured only to wire or cable	H01R24/28	H01R24/28		3114
H01R24/30	9	with additional earth or shield contacts	H01R24/30	H01R24/30		1199
H01R24/38	8	having concentrically or coaxially arranged contacts	H01R24/38	H01R24/38		2247
H01R24/40	9	specially adapted for high frequency	H01R24/40	H01R24/40		2948
H01R24/42	10	comprising impedance matching means or electrical components, e.g. filters or switches	H01R24/42	H01R24/42		300
H01R24/44	11	comprising impedance matching means	H01R24/44	H01R24/44		660
H01R24/46	11	comprising switches	H01R24/46	H01R24/46		351
H01R24/48	11	comprising protection devices, e.g. overvoltage protection	H01R24/48	H01R24/48		146
H01R24/50	10	mounted on a PCB [Printed Circuit Board]	H01R24/50	H01R24/50		1515
H01R24/52	10	mounted in or to a panel or structure	H01R24/52	H01R24/52		659
H01R24/525	11	{Outlets}	H01R24/52	H01R24/52		225
H01R24/54	10	Intermediate parts, e.g. adapters, splitters or elbows	H01R24/54	H01R24/54		255
H01R24/542	11	{Adapters}	H01R24/54	H01R24/54		541
H01R24/545	11	{Elbows}	H01R24/54	H01R24/54		216
H01R24/547	11	{Splitters}	H01R24/54	H01R24/54		137
H01R24/56	10	specially adapted to a specific shape of cables, e.g. corrugated cables, twisted pair cables, cables with two screens or hollow cables	H01R24/56	H01R24/56		107
H01R24/562	11	{Cables with two screens}	H01R24/56	H01R24/56		77
H01R24/564	11	{Corrugated cables}	H01R24/56	H01R24/56		281
H01R24/566	11	{Hollow cables}	H01R24/56	H01R24/56		87
H01R24/568	11	{Twisted pair cables}	H01R24/56	H01R24/56		63
H01R24/58	8	Contacts spaced along longitudinal axis of engagement	H01R24/58	H01R24/58		2925
H01R24/60	8	Contacts spaced along planar side wall transverse to longitudinal axis of engagement	H01R24/60	H01R24/60		3172
H01R24/62	9	Sliding engagements with one side only, e.g. modular jack coupling devices	H01R24/62	H01R24/62		2152
H01R24/64	10	for high frequency, e.g. RJ 45	H01R24/64	H01R24/64		2974
H01R24/66	8	with pins, blades or analogous contacts and secured to apparatus or structure, e.g. to a wall	H01R24/66	H01R24/66		767
H01R24/68	9	mounted on directly pluggable apparatus	H01R24/68	H01R24/68		601
H01R24/70	9	with additional earth or shield contacts	H01R24/70	H01R24/70		286
H01R24/76	8	with sockets, clips or analogous contacts and secured to apparatus or structure, e.g. to a wall	H01R24/76	H01R24/76		2330
H01R24/78	9	with additional earth or shield contacts	H01R24/78	H01R24/78		1556
H01R24/84	8	Hermaphroditic coupling devices	H01R24/84	H01R24/84		426
H01R24/86	8	Parallel contacts arranged about a common axis	H01R24/86	H01R24/86		699
H01R25/00	7	Coupling parts adapted for simultaneous co-operation with two or more identical counterparts, e.g. for distributing energy to two or more circuits (supported only by co-operation with a counterpart H01R31/00; with a holder adapted for supporting apparatus to which its counterpart is attached H01R33/88)	H01R25/00	H01R25/00		1443
H01R25/003	8	{the coupling part being secured only to wires or cables}	H01R25/00	H01R25/00		2218
H01R25/006	8	{the coupling part being secured to apparatus or structure, e.g. duplex wall receptacle}	H01R25/00	H01R25/00		2804
H01R25/14	8	Rails or bus-bars constructed so that the counterparts can be connected thereto at any point along their length (supporting elements for lighting devices, displaceable along guiding elements and making electrical contact with conductors running along the guiding elements F21V21/35)	H01R25/14	H01R25/14		1675
H01R25/142	9	{Their counterparts}	H01R25/14	H01R25/14		1511
H01R25/145	9	{Details, e.g. end pieces or joints (H01R25/147 takes precedence)}	H01R25/14	H01R25/14		1111
H01R25/147	9	{Low voltage devices, i.e. safe to touch live conductors}	H01R25/14	H01R25/14		395
H01R25/16	8	Rails or bus-bars provided with a plurality of discrete connecting locations for counterparts	H01R25/16	H01R25/16		738
H01R25/161	9	{Details}	H01R25/16	H01R25/16		611
H01R25/162	10	{Electrical connections between or with rails or bus-bars (rails having primarily a non electrical function H01R4/64)}	H01R25/16	H01R25/16		1143
H01R25/164	9	{Connecting locations formed by flush mounted apparatus}	H01R25/16	H01R25/16		220
H01R25/165	9	{Connecting locations formed by surface mounted apparatus}	H01R25/16	H01R25/16		135
H01R25/167	9	{Connecting locations formed by staggering mounted apparatus}	H01R25/16	H01R25/16		53
H01R25/168	9	{the connecting locations being situated away from the rail or bus-bar}	H01R25/16	H01R25/16		64
H01R27/00	7	Coupling parts adapted for co-operation with two or more dissimilar counterparts ({for dissimilar contact members H01R13/35}; supported only by co-operation with a counterpart H01R31/00; with a holder adapted for supporting apparatus to which its counterpart is attached H01R33/90)	H01R27/00	H01R27/00		4774
H01R27/02	8	for simultaneous co-operation with two or more {dissimilar} counterparts	H01R27/02	H01R27/02		2743
H01R29/00	7	Coupling parts for selective co-operation with a counterpart in different ways to establish different circuits, e.g. for voltage selection, for series-parallel selection, {programmable connectors}	H01R29/00	H01R29/00		2292
H01R31/00	7	Coupling parts supported only by co-operation with counterpart	H01R31/00	H01R31/00		876
H01R31/005	8	{Intermediate parts for distributing signals}	H01R31/00	H01R31/00		669
H01R31/02	8	Intermediate parts for distributing energy to two or more circuits in parallel, e.g. splitter (with a holder adapted for supporting apparatus to which its counterpart is attached H01R33/92)	H01R31/02	H01R31/02		2471
H01R31/06	8	Intermediate parts for linking two coupling parts, e.g. adapter (with a holder adapted for supporting apparatus to which its counterpart is attached H01R33/94)	H01R31/06	H01R31/06		8626
H01R31/065	9	{with built-in electric apparatus}	H01R31/06	H01R31/06		3332
H01R31/08	8	Short-circuiting members for bridging contacts in a counterpart	H01R31/08	H01R31/08		1239
H01R31/085	9	{Short circuiting bus-strips}	H01R31/08	H01R31/08		409
H01R33/00	7	Coupling devices specially adapted for supporting apparatus and having one part acting as a holder providing support and electrical connection via a counterpart which is structurally associated with the apparatus, e.g. lamp holders; Separate parts thereof	H01R33/00	H01R33/00		529
H01R33/02	8	Single-pole devices, e.g. holder for supporting one end of a tubular incandescent or neon lamp	H01R33/02	H01R33/02		1061
H01R33/05	8	Two-pole devices	H01R33/05	H01R33/05		666
H01R33/06	9	with two current-carrying pins, blades or analogous contacts, having their axes parallel to each other	H01R33/06	H01R33/06		600
H01R33/065	10	{for supporting starter switches}	H01R33/06	H01R33/06		94
H01R33/08	10	for supporting tubular fluorescent lamp	H01R33/08	H01R33/08		1015
H01R33/0809	11	{having contacts on one side only}	H01R33/08	H01R33/08		231
H01R33/0818	11	{for a plurality of lamps}	H01R33/08	H01R33/08		112
H01R33/0827	11	{characterised by the contacts}	H01R33/08	H01R33/08		165
H01R33/0836	11	{characterised by the lamp holding means}	H01R33/08	H01R33/08		423
H01R33/0845	12	{with axially resilient member}	H01R33/08	H01R33/08		286
H01R33/0854	12	{with lamp rotating means}	H01R33/08	H01R33/08		183
H01R33/0863	11	{characterised by the mounting means}	H01R33/08	H01R33/08		110
H01R33/0872	12	{for mounting in an opening of a structure}	H01R33/08	H01R33/08		53
H01R33/0881	11	{composed of different pieces}	H01R33/08	H01R33/08		51
H01R33/089	11	{integral with starter holding structure (H01R33/065 for starters only)}	H01R33/08	H01R33/08		96
H01R33/09	10	for baseless lamp bulb	H01R33/09	H01R33/09		1091
H01R33/18	9	having only abutting contacts	H01R33/18	H01R33/18		156
H01R33/20	9	having concentrically or coaxially arranged contacts	H01R33/20	H01R33/20		94
H01R33/205	10	{secured to structure or printed circuit board}	H01R33/20	H01R33/20		39
H01R33/22	9	for screw type base, e.g. for lamp	H01R33/22	H01R33/22		1627
H01R33/225	10	{secured to structure or printed circuit board}	H01R33/22	H01R33/22		49
H01R33/46	9	for bayonet type base	H01R33/46	H01R33/46		1272
H01R33/465	10	{secured to structure or printed circuit board}	H01R33/46	H01R33/46		78
H01R33/72	8	Three-pole devices	H01R33/72	H01R33/72		104
H01R33/74	8	Devices having four or more poles {, e.g. holders for compact fluorescent lamps}	H01R33/74	H01R33/74		274
H01R33/76	9	Holders with sockets, clips, or analogous contacts adapted for axially-sliding engagement with parallely-arranged pins, blades, or analogous contacts on counterpart, e.g. electronic tube socket	H01R33/76	H01R33/76		755
H01R33/7607	10	{the parallel terminal pins having a circular disposition}	H01R33/76	H01R33/76		31
H01R33/7614	11	{the terminals being connected to individual wires}	H01R33/76	H01R33/76		13
H01R33/7621	12	{the wires being connected using screw, clamp, wrap or spring connection}	H01R33/76	H01R33/76		223
H01R33/7628	12	{the wires being connected using solder}	H01R33/76	H01R33/76		589
H01R33/7635	11	{the terminals being collectively connected, e.g. to a PCB}	H01R33/76	H01R33/76		93
H01R33/7642	12	{socket snap fastened in an opening of a PCB}	H01R33/76	H01R33/76		43
H01R33/765	10	{the terminal pins having a non-circular disposition}	H01R33/76	H01R33/76		180
H01R33/7657	10	{characterised by keying or marking means}	H01R33/76	H01R33/76		32
H01R33/7664	10	{having additional guiding, adapting, shielding, anti-vibration or mounting means}	H01R33/76	H01R33/76		389
H01R33/7671	10	{having multiple positions or sockets, e.g. stacked sockets while mounting}	H01R33/76	H01R33/76		66
H01R33/7678	10	{having a separated part for spark preventing means}	H01R33/76	H01R33/76		53
H01R33/7685	10	{having internal socket contact by abutting}	H01R33/76	H01R33/76		82
H01R33/7692	10	{for supporting a tubular fluorescent lamp (for two-pole devices H01R33/06)}	H01R33/76	H01R33/76		27
H01R33/88	8	adapted for simultaneous co-operation with two or more identical counterparts	H01R33/88	H01R33/88		270
H01R33/90	8	adapted for co-operation with two or more dissimilar counterparts	H01R33/90	H01R33/90		173
H01R33/92	8	Holders formed as intermediate parts for distributing energy in parallel through two or more counterparts at least one of which is attached to apparatus to be held	H01R33/92	H01R33/92		358
H01R33/94	8	Holders formed as intermediate parts for linking a counter-part to a coupling part	H01R33/94	H01R33/94		1522
H01R33/942	9	{for tubular fluorescent lamps}	H01R33/94	H01R33/94		199
H01R33/945	8	Holders with built-in electrical component	H01R33/945	H01R33/945		442
H01R33/9453	9	{for screw type coupling devices}	H01R33/945	H01R33/945		224
H01R33/9456	9	{for bayonet type coupling devices}	H01R33/945	H01R33/945		88
H01R33/95	9	with fuse; with thermal switch	H01R33/95	H01R33/95		199
H01R33/955	9	with switch operated manually and independent of engagement or disengagement of coupling	H01R33/955	H01R33/955		365
H01R33/9555	10	{for screw type coupling devices}	H01R33/955	H01R33/955		754
H01R33/96	9	with switch operated by engagement or disengagement of coupling	H01R33/96	H01R33/96		169
H01R33/962	10	{for screw type coupling devices}	H01R33/96	H01R33/96		134
H01R33/965	8	Dustproof, splashproof, drip-proof, waterproof, or flameproof holders	H01R33/965	H01R33/965		319
H01R33/9651	9	{for screw type coupling devices}	H01R33/965	H01R33/965		204
H01R33/9653	10	{neither pole becoming electrically connected until the coupling parts are substantially engaged}	H01R33/965	H01R33/965		15
H01R33/9655	9	{for bayonet type coupling devices}	H01R33/965	H01R33/965		85
H01R33/9656	10	{neither pole becoming electrically connected until the coupling parts are substantially engaged}	H01R33/965	H01R33/965		22
H01R33/9658	9	{for tubular fluorescent lamps}	H01R33/965	H01R33/965		171
H01R33/97	8	Holders with separate means to prevent loosening of the coupling or unauthorised removal of apparatus held	H01R33/97	H01R33/97		224
H01R33/971	9	{for screw type coupling devices}	H01R33/97	H01R33/97		353
H01R33/973	9	{for bayonet type coupling devices}	H01R33/97	H01R33/97		237
H01R33/975	8	Holders with resilient means for protecting apparatus against vibrations or shocks	H01R33/975	H01R33/975		236
H01R33/9753	9	{for screw type coupling devices}	H01R33/975	H01R33/975		127
H01R33/9756	9	{for bayonet type coupling devices}	H01R33/975	H01R33/975		66
H01R35/00	7	Flexible or turnable line connectors {, i.e. the rotation angle being limited}(rotary current collectors, distributors H01R39/00)	H01R35/00	H01R35/00		1219
H01R35/02	8	Flexible line connectors {without frictional contact members}	H01R35/02	H01R35/02		1092
H01R35/025	9	{having a flexible conductor wound around a rotation axis}	H01R35/02	H01R35/02		733
H01R35/04	8	Turnable line connectors with limited rotation angle {with frictional contact members}	H01R35/04	H01R35/04		2128
H01R39/00	7	Rotary current collectors, distributors or interrupters	H01R39/00	H01R39/00		678
H01R39/02	8	Details {for dynamo electric machines (for current collectors not particularly for dynamo electric machines H01R39/60, H01R39/64)}	H01R39/02	H01R39/02		126
H01R39/022	9	{characterised by the materials used, e.g. ceramics}	H01R39/02	H01R39/02		28
H01R39/025	10	{Conductive materials}	H01R39/02	H01R39/02		159
H01R39/027	10	{Insulating materials}	H01R39/02	H01R39/02		15
H01R39/04	9	Commutators (wherein the segments are formed by extensions of dynamo-electric machine winding H02K)	H01R39/04	H01R39/04		1266
H01R39/045	10	{the commutators being made of carbon}	H01R39/04	H01R39/04		261
H01R39/06	10	other than with external cylindrical contact surface, e.g. flat commutators	H01R39/06	H01R39/06		335
H01R39/08	9	Slip-rings	H01R39/08	H01R39/08		1268
H01R39/085	10	{the slip-rings being made of carbon}	H01R39/08	H01R39/08		118
H01R39/10	10	other than with external cylindrical contact surface, e.g. flat slip-rings	H01R39/10	H01R39/10		164
H01R39/12	10	using bearing or shaft surface as contact surface	H01R39/12	H01R39/12		157
H01R39/14	9	Fastenings of commutators or slip-rings to shafts	H01R39/14	H01R39/14		219
H01R39/16	10	by means of moulded or cast material applied during or after assembly	H01R39/16	H01R39/16		62
H01R39/18	9	Contacts for co-operation with commutator or slip-ring, e.g. contact brush	H01R39/18	H01R39/18		283
H01R39/20	10	characterised by the material thereof	H01R39/20	H01R39/20		524
H01R39/22	11	incorporating lubricating or polishing ingredient	H01R39/22	H01R39/22		239
H01R39/24	10	Laminated contacts; Wire contacts, e.g. metallic brush, carbon fibres	H01R39/24	H01R39/24		740
H01R39/26	10	Solid sliding contacts, e.g. carbon brush	H01R39/26	H01R39/26		708
H01R39/27	11	End caps on carbon brushes to transmit spring pressure	H01R39/27	H01R39/27		74
H01R39/28	10	Roller contacts; Ball contacts	H01R39/28	H01R39/28		125
H01R39/30	10	Liquid contacts	H01R39/30	H01R39/30		95
H01R39/32	9	Connections of conductor to commutator segment	H01R39/32	H01R39/32		506
H01R39/34	9	Connections of conductor to slip-ring	H01R39/34	H01R39/34		268
H01R39/36	9	Connections of cable or wire to brush	H01R39/36	H01R39/36		504
H01R39/38	9	Brush holders	H01R39/38	H01R39/38		850
H01R39/381	10	{characterised by the application of pressure to brush}	H01R39/38	H01R39/38		1094
H01R39/383	10	{characterised by the electrical connection to the brush holder}	H01R39/38	H01R39/38		284
H01R39/385	10	{Means for mechanical fixation of the brush holder}	H01R39/38	H01R39/38		360
H01R39/386	11	{Electrically insulated bolts}	H01R39/38	H01R39/38		42
H01R39/388	10	{characterised by the material of the brush holder}	H01R39/38	H01R39/38		77
H01R39/39	10	wherein the brush is fixedly mounted in the holder	H01R39/39	H01R39/39		603
H01R39/40	10	enabling brush movement within holder during current collection	H01R39/40	H01R39/40		576
H01R39/41	10	cartridge type	H01R39/41	H01R39/41		341
H01R39/415	11	with self-recoiling spring	H01R39/415	H01R39/415		166
H01R39/42	9	Devices for lifting brushes	H01R39/42	H01R39/42		113
H01R39/44	9	Devices for shifting brushes	H01R39/44	H01R39/44		64
H01R39/46	9	Auxiliary means for improving current transfer, or for reducing or preventing sparking or arcing	H01R39/46	H01R39/46		207
H01R39/48	10	by air blast; by surrounding collector with non-conducting liquid or gas	H01R39/48	H01R39/48		55
H01R39/50	10	Barriers placed between brushes	H01R39/50	H01R39/50		11
H01R39/52	10	by use of magnets	H01R39/52	H01R39/52		9
H01R39/54	10	by use of impedance between brushes or segments	H01R39/54	H01R39/54		61
H01R39/56	9	Devices for lubricating or polishing slip-rings or commutators during operation of the collector	H01R39/56	H01R39/56		84
H01R39/58	9	Means structurally associated with the current collector for indicating condition thereof, e.g. for indicating brush wear	H01R39/58	H01R39/58		509
H01R39/59	9	Means structurally associated with the brushes for interrupting current (H01R39/58 takes precedence)	H01R39/59	H01R39/59		48
H01R39/60	8	Devices for interrupted current collection, e.g. commutating device, distributor, interrupter (self-interrupters H01H, e.g. H01H51/34)	H01R39/60	H01R39/60		218
H01R39/62	9	with more than one brush co-operating with the same set of segments	H01R39/62	H01R39/62		11
H01R39/64	8	Devices for uninterrupted current collection	H01R39/64	H01R39/64		1232
H01R39/643	9	{through ball or roller bearing}	H01R39/64	H01R39/64		419
H01R39/646	9	{through an electrical conductive fluid}	H01R39/64	H01R39/64		221
H01R41/00	7	Non-rotary current collectors for maintaining contact between moving and stationary parts of an electric circuit (end pieces terminating in a hook or the like H01R11/12; current collectors for power supply lines of electrically-propelled vehicles B60L5/00)	H01R41/00	H01R41/00		785
H01R41/02	8	Devices for interrupted current collection, e.g. distributor (electrically-operated selector switches H01H67/00)	H01R41/02	H01R41/02		27
H01R43/00	7	Apparatus or processes specially adapted for manufacturing, assembling, maintaining, or repairing of line connectors or current collectors or for joining electric conductors (of trolley lines B60M1/28)	H01R43/00	H01R43/00		4695
H01R43/002	8	{Maintenance of line connectors, e.g. cleaning}	H01R43/00	H01R43/00		483
H01R43/005	8	{for making dustproof, splashproof, drip-proof, waterproof, or flameproof connection, coupling, or casing}	H01R43/00	H01R43/00		1405
H01R43/007	8	{for elastomeric connecting elements}	H01R43/00	H01R43/00		308
H01R43/01	8	for connecting unstripped conductors to contact members having insulation cutting edges	H01R43/01	H01R43/01		718
H01R43/015	9	{Handtools}	H01R43/01	H01R43/01		450
H01R43/02	8	for soldered or welded connections	H01R43/02	H01R43/02		2233
H01R43/0207	9	{Ultrasonic-, H.F.-, cold- or impact welding}	H01R43/02	H01R43/02		933
H01R43/0214	9	{Resistance welding (H01R43/0228 takes precedence)}	H01R43/02	H01R43/02		275
H01R43/0221	9	{Laser welding (H01R43/0228 takes precedence)}	H01R43/02	H01R43/02		475
H01R43/0228	9	{without preliminary removing of insulation before soldering or welding}	H01R43/02	H01R43/02		169
H01R43/0235	9	{for applying solder (H01R43/0228 takes precedence)}	H01R43/02	H01R43/02		412
H01R43/0242	9	{comprising means for controlling the temperature, e.g. making use of the curie point}	H01R43/02	H01R43/02		116
H01R43/0249	9	{for simultaneous welding or soldering of a plurality of wires to contact elements}	H01R43/02	H01R43/02		247
H01R43/0256	9	{for soldering or welding connectors to a printed circuit board}	H01R43/02	H01R43/02		904
H01R43/0263	9	{for positioning or holding parts during soldering or welding process}	H01R43/02	H01R43/02		818
H01R43/027	8	for connecting conductors by clips	H01R43/027	H01R43/027		690
H01R43/0275	9	{by using explosive force}	H01R43/027	H01R43/027		45
H01R43/033	8	for wrapping or unwrapping wire connections	H01R43/033	H01R43/033		796
H01R43/0335	9	{for unwraping}	H01R43/033	H01R43/033		37
H01R43/04	8	for forming connections by deformation, e.g. crimping tool	H01R43/04	H01R43/04		826
H01R43/042	9	Hand tools for crimping	H01R43/042	H01R43/042		1094
H01R43/0421	10	{combined with other functions, e.g. cutting}	H01R43/042	H01R43/042		324
H01R43/0422	10	{operated by an explosive force}	H01R43/042	H01R43/042		67
H01R43/0424	10	{with more than two radially actuated mandrels}	H01R43/042	H01R43/042		168
H01R43/0425	10	{with mandrels actuated in axial direction to the wire}	H01R43/042	H01R43/042		132
H01R43/0427	10	{fluid actuated hand crimping tools}	H01R43/042	H01R43/042		380
H01R43/0428	10	{Power-driven hand crimping tools}	H01R43/042	H01R43/042		142
H01R43/045	10	with contact member feeding mechanism	H01R43/045	H01R43/045		152
H01R43/048	9	Crimping apparatus or processes (H01R43/042 takes precedence)	H01R43/048	H01R43/048		3104
H01R43/0482	10	{combined with contact member manufacturing mechanism}	H01R43/048	H01R43/048		251
H01R43/0484	10	{for eyelet contact members}	H01R43/048	H01R43/048		86
H01R43/0486	10	{with force measuring means}	H01R43/048	H01R43/048		233
H01R43/0488	10	{with crimp height adjusting means}	H01R43/048	H01R43/048		258
H01R43/05	10	with wire-insulation stripping	H01R43/05	H01R43/05		1068
H01R43/052	10	with wire-feeding mechanism	H01R43/052	H01R43/052		1408
H01R43/055	10	with contact member feeding mechanism	H01R43/055	H01R43/055		954
H01R43/058	9	Crimping mandrels	H01R43/058	H01R43/058		735
H01R43/0585	10	{for crimping apparatus with more than two radially actuated mandrels}	H01R43/058	H01R43/058		110
H01R43/06	8	Manufacture of commutators	H01R43/06	H01R43/06		774
H01R43/08	9	in which segments are not separated until after assembly	H01R43/08	H01R43/08		381
H01R43/10	8	Manufacture of slip-rings	H01R43/10	H01R43/10		250
H01R43/12	8	Manufacture of brushes	H01R43/12	H01R43/12		797
H01R43/14	8	Maintenance of current collectors, e.g. reshaping of brushes, cleaning of commutators	H01R43/14	H01R43/14		318
H01R43/16	8	for manufacturing contact members, e.g. by punching and by bending	H01R43/16	H01R43/16		5773
H01R43/18	8	for manufacturing bases or cases for contact members	H01R43/18	H01R43/18		1562
H01R43/20	8	for assembling or disassembling contact members with insulating base, case or sleeve	H01R43/20	H01R43/20		5647
H01R43/205	9	{with a panel or printed circuit board}	H01R43/20	H01R43/20		1383
H01R43/22	9	Hand tools	H01R43/22	H01R43/22		559
H01R43/24	9	Assembling by moulding on contact members	H01R43/24	H01R43/24		2593
H01R43/26	8	for engaging or disengaging the two parts of a coupling device (structural association with two-part coupling device H01R13/629)	H01R43/26	H01R43/26		3636
H01R43/28	8	for wire processing before connecting to contact members, not provided for in groups H01R43/02 - H01R43/26	H01R43/28	H01R43/28		4028
H01R2101/00	7	One pole	H01R101/00	H01R101/00		1548
H01R2103/00	7	Two poles	H01R103/00	H01R103/00		13335
H01R2105/00	7	Three poles	H01R105/00	H01R105/00		1106
H01R2107/00	7	Four or more poles	H01R107/00	H01R107/00		5895
H01R2201/00	7	Connectors or connections adapted for particular applications	CPCONLY	H01R2201/00		108
H01R2201/02	8	for antennas	CPCONLY	H01R2201/02		1097
H01R2201/04	8	for network, e.g. LAN connectors	CPCONLY	H01R2201/04		1245
H01R2201/06	8	for computer periphery	CPCONLY	H01R2201/06		2382
H01R2201/08	8	for halogen lamps	CPCONLY	H01R2201/08		116
H01R2201/10	8	for dynamoelectric machines	CPCONLY	H01R2201/10		729
H01R2201/12	8	for medicine and surgery	CPCONLY	H01R2201/12		1370
H01R2201/14	8	seismic connectors	CPCONLY	H01R2201/14		29
H01R2201/16	8	for telephony	CPCONLY	H01R2201/16		2277
H01R2201/18	8	for television	CPCONLY	H01R2201/18		366
H01R2201/20	8	for testing or measuring purposes	CPCONLY	H01R2201/20		2554
H01R2201/22	8	for transformers or coils	CPCONLY	H01R2201/22		152
H01R2201/24	8	for radio transmission	CPCONLY	H01R2201/24		191
H01R2201/26	8	for vehicles	CPCONLY	H01R2201/26		11330
