B60R1/00	7	Optical viewing arrangements; Real-time viewing arrangements for drivers or passengers using optical image capturing systems, e.g. cameras or video systems specially adapted for use in or on vehicles<br><br><u>NOTE</u><br><br>This group covers optical viewing arrangements using mirrors as well as real-time viewing arrangements using optical image capturing systems, e.g. the special adaptation of cameras or video systems in or on vehicles, for assisting drivers or passengers. In this context, "viewing" refers to a visual assistance of drivers or passengers using mirrors, cameras or the like.	B60R1/00	B60R1/00		4567
B60R1/001	8	{integrated in the windows, e.g. Fresnel lenses}	B60R1/00	B60R1/00		295
B60R1/002	8	{specially adapted for covering the peripheral part of the vehicle, e.g. for viewing tyres, bumpers or the like (integrated in the windows B60R1/001; combined with rear-view mirrors B60R1/08)}	B60R1/00	B60R1/00		570
B60R1/003	9	{for viewing trailer hitches}	B60R1/00	B60R1/00		310
B60R1/005	8	{specially adapted for viewing traffic-lights}	B60R1/00	B60R1/00		94
B60R1/006	8	{Side-view mirrors, e.g. V-shaped mirrors located at the front or rear part of the vehicle (combined with rear-view mirrors B60R1/08; side-view periscopes B60R1/10)}	B60R1/00	B60R1/00		530
B60R1/007	9	{specially adapted for covering the lateral blind spot not covered by the usual rear-view mirror}	B60R1/00	B60R1/00		358
B60R1/008	8	{allowing the driver to see passengers, e.g. for busses (combined with rear-view mirrors B60R1/08)}	B60R1/00	B60R1/00		185
B60R1/02	8	Rear-view mirror arrangements (periscope arrangements B60R1/10)	B60R1/02	B60R1/02		737
B60R1/025	9	{comprising special mechanical means for correcting the field of view in relation to particular driving conditions, e.g. change of lane; scanning mirrors}	B60R1/02	B60R1/02		955
B60R1/04	9	mounted inside vehicle {(B60R1/025, B60R1/08 take precedence)}	B60R1/04	B60R1/04		3338
B60R1/06	9	mounted on vehicle exterior {(B60R1/025, B60R1/08 take precedence)}	B60R1/06	B60R1/06		4537
B60R1/0602	10	{comprising means for cleaning or deicing}	B60R1/06	B60R1/06		2098
B60R1/0605	10	{specially adapted for mounting on trucks, e.g. by C-shaped support means}	B60R1/06	B60R1/06		544
B60R1/0607	11	{with remote position control adjustment}	B60R1/06	B60R1/06		35
B60R1/061	12	{by manually actuated mechanical means, e.g. push-pull cables}	B60R1/06	B60R1/06		55
B60R1/0612	12	{by electrically actuated means}	B60R1/06	B60R1/06		193
B60R1/0615	12	{by hydraulically or pneumatically actuated means}	B60R1/06	B60R1/06		24
B60R1/0617	11	{foldable along the vehicle, e.g. in case of external force applied thereon}	B60R1/06	B60R1/06		248
B60R1/062	10	with remote control for adjusting position {(B60R1/0607 takes precedence)}	B60R1/062	B60R1/062		496
B60R1/0625	11	{by hydraulically or pneumatically powered actuators}	B60R1/062	B60R1/062		87
B60R1/064	11	by manually powered actuators	B60R1/064	B60R1/064		259
B60R1/066	12	for adjusting the mirror relative to its housing	B60R1/066	B60R1/066		238
B60R1/068	13	using cables	B60R1/068	B60R1/068		239
B60R1/07	11	by electrically powered actuators	B60R1/07	B60R1/07		1131
B60R1/072	12	for adjusting the mirror relative to its housing	B60R1/072	B60R1/072		1504
B60R1/074	12	for retracting the mirror arrangements to a non-use position alongside the vehicle	B60R1/074	B60R1/074		1298
B60R1/076	10	yieldable to excessive external force and provided with an indexed use position ({B60R1/0617, B60R1/074} take precedence)	B60R1/076	B60R1/076		658
B60R1/078	10	easily removable; mounted for bodily outward movement, e.g. when towing	B60R1/078	B60R1/078		682
B60R1/08	9	involving special optical features, e.g. avoiding blind spots {, e.g. convex mirrors; Side-by-side associations of rear-view and other mirrors (B60R1/025, B60R1/10 take precedence)}	B60R1/08	B60R1/08		1235
B60R1/081	10	{avoiding blind spots, e.g. by using a side-by-side association of mirrors}	B60R1/08	B60R1/08		1338
B60R1/082	11	{using a single wide field mirror or an association of rigidly connected mirrors}	B60R1/08	B60R1/08		1129
B60R1/083	10	{Anti-glare mirrors, e.g. "day-night" mirrors}	B60R1/08	B60R1/08		309
B60R1/084	11	{using a removable filtering or hiding screen (associated with windows or windscreens B60J3/00)}	B60R1/08	B60R1/08		115
B60R1/085	11	{using a combination of interchangeable reflecting surfaces, e.g. reversible mirrors}	B60R1/08	B60R1/08		112
B60R1/086	11	{using a mirror angularly movable between a position of use and a non-glare position reflecting a dark field to the user, e.g. situated behind a transparent glass used as low-reflecting surface; Wedge-shaped mirrors}	B60R1/08	B60R1/08		302
B60R1/087	12	{with remote or automatic control means}	B60R1/08	B60R1/08		251
B60R1/088	11	{using a cell of electrically changeable optical characteristic, e.g. liquid-crystal or electrochromic mirrors}	B60R1/08	B60R1/08		1006
B60R1/089	11	{using a liquid filtering layer of variable thickness}	B60R1/08	B60R1/08		27
B60R1/10	8	Front-view mirror arrangements; {(specially adapted for covering the peripheral part of the vehicle B60R1/002)}; Periscope arrangements {, i.e. optical devices using combinations of mirrors, lenses, prisms or the like (specially adapted for covering the peripheral part of the vehicle B60R1/002; for viewing traffic-lights B60R1/005); Other mirror arrangements giving a view from above or under the vehicle}	B60R1/10	B60R1/10		879
B60R1/105	9	{Optical arrangements giving a view under the vehicle, e.g. using periscopes}	B60R1/10	B60R1/10		40
B60R1/12	8	Mirror assemblies combined with other articles, e.g. clocks	B60R1/12	B60R1/12		4101
B60R1/1207	9	{with lamps; with turn indicators}	B60R1/12	B60R1/12		1761
B60R2001/1215	9	{with information displays}	B60R1/12	B60R1/12		1265
B60R2001/1223	9	{with sensors or transducers}	B60R1/12	B60R1/12		962
B60R2001/123	9	{with thermometers}	B60R1/12	B60R1/12		63
B60R2001/1238	9	{with vanity mirrors}	B60R1/12	B60R1/12		64
B60R2001/1246	9	{with clocks}	B60R1/12	B60R1/12		70
B60R2001/1253	9	{with cameras, video cameras or video screens}	B60R1/12	B60R1/12		2174
B60R2001/1261	9	{with antennae}	B60R1/12	B60R1/12		139
B60R2001/1269	9	{with sun visors}	B60R1/12	B60R1/12		85
B60R2001/1276	9	{with radio receivers, loud-speakers or buzzers}	B60R1/12	B60R1/12		136
B60R2001/1284	9	{with communication systems other than radio-receivers, e.g. keyless entry systems, navigation systems; with anti-collision systems}	B60R1/12	B60R1/12		355
B60R2001/1292	9	{with holding means for personal articles}	B60R1/12	B60R1/12		116
B60R1/20	8	Real-time viewing arrangements for drivers or passengers using optical image capturing systems, e.g. cameras or video systems specially adapted for use in or on vehicles	B60R1/20	B60R1/20		188
B60R1/22	9	for viewing an area outside the vehicle, e.g. the exterior of the vehicle	B60R1/22	B60R1/22		901
B60R1/23	10	with a predetermined field of view	B60R1/23	B60R1/23		677
B60R1/24	11	in front of the vehicle	B60R1/24	B60R1/24		1044
B60R1/25	11	to the sides of the vehicle	B60R1/25	B60R1/25		529
B60R1/26	11	to the rear of the vehicle	B60R1/26	B60R1/26		2636
B60R1/27	11	providing all-round vision, e.g. using omnidirectional cameras	B60R1/27	B60R1/27		1548
B60R1/28	10	with an adjustable field of view	B60R1/28	B60R1/28		1177
B60R1/29	9	for viewing an area inside the vehicle, e.g. for viewing passengers or cargo	B60R1/29	B60R1/29		568
B60R1/30	9	providing vision in the non-visible spectrum, e.g. night or infrared vision	B60R1/30	B60R1/30		467
B60R1/31	9	providing stereoscopic vision	B60R1/31	B60R1/31		315
B60R3/00	7	Arrangements of steps {or ladders facilitating access to or on the vehicle}, e.g. running-boards ({construction of steps for railway vehicles B61D23/00} ; ladders E06C)	B60R3/00	B60R3/00		864
B60R3/002	8	{Running boards (for vehicle tops B60R3/005; at the sides of the vehicle for carrying loads B60R9/02)}	B60R3/00	B60R3/00		1425
B60R3/005	8	{Catwalks, running boards for vehicle tops, access means for vehicle tops; Handrails therefor}	B60R3/00	B60R3/00		533
B60R3/007	8	{Removable steps or ladders, e.g. foldable (as access means for vehicle tops B60R3/005)}	B60R3/00	B60R3/00		1188
B60R3/02	8	Retractable steps {or ladders, e.g. movable under shock (B60R3/005 takes precedence)}	B60R3/02	B60R3/02		3165
B60R3/04	8	with provisions for shoe scraping	B60R3/04	B60R3/04		279
B60R5/00	7	Compartments within vehicle body primarily intended or sufficiently spacious for trunks, suit-cases, or the like (primarily intended for stowing loads in load-transporting vehicles B60P; arrangements for stowing spare wheels B62D43/00)	B60R5/00	B60R5/00		477
B60R5/003	8	{Luggage racks, e.g. for busses (primarily intended for passengers&apos; property smaller than suitcases B60R7/04; B60R7/08; luggage racks for rail vehicles B61D37/003)}	B60R5/00	B60R5/00		427
B60R5/006	8	{stowing or holding means for elongated articles, e.g. skis inside vehicles}	B60R5/00	B60R5/00		431
B60R5/02	8	arranged at front of vehicle {(B60R5/003 takes precedence)}	B60R5/02	B60R5/02		289
B60R5/04	8	arranged at rear of vehicle {(B60R5/003, B60R5/006 take precedence; external trunks arranged at rear of vehicle B60R9/065)}	B60R5/04	B60R5/04		3286
B60R5/041	9	{extensible externally of the vehicle body, e.g. to create an open luggage compartment of increased capacity (devices for anchoring the boot lid while carrying oversize objects E05C17/042)}	B60R5/04	B60R5/04		389
B60R5/042	10	{to create an enclosed luggage compartment of increased capacity, e.g. with ventilation apertures for transporting dogs}	B60R5/04	B60R5/04		182
B60R5/044	9	{luggage covering means, e.g. parcel shelves}	B60R5/04	B60R5/04		987
B60R5/045	10	{collapsible or transformable}	B60R5/04	B60R5/04		961
B60R5/047	11	{collapsible by rolling-up}	B60R5/04	B60R5/04		1100
B60R5/048	11	{of accordion-type, i.e. collapsible by sliding and folding}	B60R5/04	B60R5/04		142
B60R7/00	7	Stowing or holding appliances inside vehicle primarily intended for personal property smaller than suit-cases, e.g. travelling articles, or maps (for radio sets, television sets, telephones or the like, mounting of cameras operative during drive, tools, or spare parts B60R11/00; for receptacles for refuse, food, beverages, cigarettes B60N)	B60R7/00	B60R7/00		378
B60R7/005	8	{Nets or elastic pockets tensioned against walls or backrests}	B60R7/00	B60R7/00		643
B60R7/02	8	in separate luggage compartment {(B60R7/005 takes precedence)}	B60R7/02	B60R7/02		2262
B60R7/04	8	in driver or passenger space {, e.g. using racks (B60R7/005, B60R7/08 take precedence)}	B60R7/04	B60R7/04		5882
B60R7/043	9	{mounted on or under a seat}	B60R7/04	B60R7/04		2357
B60R7/046	9	{mounted on door}	B60R7/04	B60R7/04		892
B60R7/05	9	mounted on sun visor	B60R7/05	B60R7/05		402
B60R7/06	9	mounted on or below dashboards	B60R7/06	B60R7/06		3270
B60R7/08	8	Disposition of racks, clips {, holders, containers} or the like {for supporting specific articles (B60R7/005 takes precedence)}	B60R7/08	B60R7/08		2403
B60R7/081	9	{for supporting maps}	B60R7/08	B60R7/08		211
B60R7/082	9	{for supporting spectacles}	B60R7/08	B60R7/08		397
B60R7/084	9	{for supporting tissues or tissue boxes}	B60R7/08	B60R7/08		297
B60R7/085	9	{for supporting flowers or flower vases}	B60R7/08	B60R7/08		54
B60R7/087	9	{for stowing money or valuables, e.g. using safes}	B60R7/08	B60R7/08		395
B60R7/088	9	{for stowing tape cartridges, compact discs, or the like}	B60R7/08	B60R7/08		260
B60R7/10	9	for supporting hats, clothes or clothes hangers	B60R7/10	B60R7/10		1254
B60R7/12	9	for supporting umbrellas	B60R7/12	B60R7/12		710
B60R7/14	9	for supporting weapons	B60R7/14	B60R7/14		363
B60R9/00	7	Supplementary fittings on vehicle exterior for carrying loads, e.g. luggage, sports gear or the like	B60R9/00	B60R9/00		1142
B60R9/02	8	at the sides, e.g. on running-board	B60R9/02	B60R9/02		828
B60R9/04	8	Carriers associated with vehicle roof (B60R9/08 takes precedence)	B60R9/04	B60R9/04		1595
B60R9/042	9	Carriers characterised by means to facilitate loading or unloading of the load, e.g. rollers, tracks, or the like	B60R9/042	B60R9/042		631
B60R9/0423	10	{for ladders}	B60R9/042	B60R9/042		205
B60R9/0426	10	{for small vehicles, e.g. invalid chairs, perambulators}	B60R9/042	B60R9/042		69
B60R9/045	9	Carriers being adjustable or transformable, e.g. expansible, collapsible {(transformable into tents B60P3/36; into beds B60P3/38)}	B60R9/045	B60R9/045		1764
B60R9/048	9	Carriers characterised by article-gripping {, -covering,}-retaining, or -locking means	B60R9/048	B60R9/048		891
B60R9/0485	10	{for ladders (B60R9/0423 takes precedence)}	B60R9/048	B60R9/048		154
B60R9/05	9	Carriers characterised by wind deflecting means (wind deflectors for open roofs B60J7/22)	B60R9/05	B60R9/05		191
B60R9/052	9	Carriers comprising elongate members extending only transversely of vehicle (B60R9/08 takes precedence)	B60R9/052	B60R9/052		209
B60R9/055	9	Enclosure-type carriers, e.g. containers, boxes (B60R9/048 takes precedence)	B60R9/055	B60R9/055		1207
B60R9/058	9	characterised by releasable attaching means between carrier and roof	B60R9/058	B60R9/058		1541
B60R9/06	8	at vehicle front or rear {(rear luggage compartments within vehicle extensible externally of the vehicle body B60R5/041)}	B60R9/06	B60R9/06		3846
B60R9/065	9	{Enclosure-type carriers, e.g. trunks}	B60R9/06	B60R9/06		769
B60R9/08	8	specially adapted for sports gear (vehicles specially adapted for carrying aeroplanes, for carrying boats B60P)	B60R9/08	B60R9/08		819
B60R9/10	9	for cycles	B60R9/10	B60R9/10		2565
B60R9/12	9	for skis	B60R9/12	B60R9/12		628
B60R11/00	7	Arrangements for holding or mounting articles, not otherwise provided for	B60R11/00	B60R11/00		7614
B60R2011/0001	8	{characterised by position}	B60R11/00	B60R11/00		101
B60R2011/0003	9	{inside the vehicle}	B60R11/00	B60R11/00		1852
B60R2011/0005	10	{Dashboard}	B60R11/00	B60R11/00		3807
B60R2011/0007	10	{Mid-console}	B60R11/00	B60R11/00		2234
B60R2011/0008	10	{Ventilation grilles}	B60R11/00	B60R11/00		352
B60R2011/001	10	{Vehicle control means, e.g. steering-wheel or column}	B60R11/00	B60R11/00		684
B60R2011/0012	10	{Seats or parts thereof}	B60R11/00	B60R11/00		800
B60R2011/0014	11	{Arm-rests}	B60R11/00	B60R11/00		486
B60R2011/0015	11	{Back-rests}	B60R11/00	B60R11/00		961
B60R2011/0017	11	{Head-rests}	B60R11/00	B60R11/00		1121
B60R2011/0019	10	{Side or rear panels}	B60R11/00	B60R11/00		209
B60R2011/0021	11	{Doors}	B60R11/00	B60R11/00		1084
B60R2011/0022	11	{Pillars}	B60R11/00	B60R11/00		417
B60R2011/0024	11	{Rear shelves}	B60R11/00	B60R11/00		314
B60R2011/0026	10	{Windows, e.g. windscreen}	B60R11/00	B60R11/00		1839
B60R2011/0028	10	{Ceiling, e.g. roof rails}	B60R11/00	B60R11/00		1959
B60R2011/0029	10	{Floor, e.g. side sills, fire wall}	B60R11/00	B60R11/00		427
B60R2011/0031	10	{Seat belts}	B60R11/00	B60R11/00		101
B60R2011/0033	10	{Rear-view mirrors}	B60R11/00	B60R11/00		559
B60R2011/0035	10	{Sun visors}	B60R11/00	B60R11/00		560
B60R2011/0036	10	{Luggage compartment}	B60R11/00	B60R11/00		1440
B60R2011/0038	10	{Engine compartment}	B60R11/00	B60R11/00		131
B60R2011/004	9	{outside the vehicle}	B60R11/00	B60R11/00		5139
B60R2011/0042	8	{characterised by mounting means}	B60R11/00	B60R11/00		1028
B60R2011/0043	9	{for integrated articles, i.e. not substantially protruding from the surrounding parts}	B60R11/00	B60R11/00		592
B60R2011/0045	10	{with visible part, e.g. flush mounted}	B60R11/00	B60R11/00		335
B60R2011/0047	11	{using hidden fastening means}	B60R11/00	B60R11/00		489
B60R2011/0049	9	{for non integrated articles}	B60R11/00	B60R11/00		220
B60R2011/005	10	{Connection with the vehicle part}	B60R11/00	B60R11/00		866
B60R2011/0052	11	{using screws, bolts, rivets or the like}	B60R11/00	B60R11/00		1760
B60R2011/0054	11	{using cigarette lighter}	B60R11/00	B60R11/00		116
B60R2011/0056	11	{using suction cups}	B60R11/00	B60R11/00		1132
B60R2011/0057	11	{using magnetic means}	B60R11/00	B60R11/00		575
B60R2011/0059	11	{using clips, clamps, straps or the like}	B60R11/00	B60R11/00		2130
B60R2011/0061	11	{using key-type connections}	B60R11/00	B60R11/00		342
B60R2011/0063	11	{using adhesive means, e.g. hook and loop fasteners}	B60R11/00	B60R11/00		1109
B60R2011/0064	10	{Connection with the article}	B60R11/00	B60R11/00		312
B60R2011/0066	11	{using screws, bolts, rivets or the like}	B60R11/00	B60R11/00		512
B60R2011/0068	11	{using suction cups}	B60R11/00	B60R11/00		166
B60R2011/007	11	{using magnetic means}	B60R11/00	B60R11/00		474
B60R2011/0071	11	{using latches, clips, clamps, straps or the like}	B60R11/00	B60R11/00		2242
B60R2011/0073	11	{using key-type connections}	B60R11/00	B60R11/00		339
B60R2011/0075	11	{using a containment or docking space}	B60R11/00	B60R11/00		1909
B60R2011/0077	11	{using adhesive means, e.g. hook and loop fasteners}	B60R11/00	B60R11/00		306
B60R2011/0078	10	{Quick-disconnect two-parts mounting means}	B60R11/00	B60R11/00		722
B60R2011/008	9	{Adjustable or movable supports}	B60R11/00	B60R11/00		2240
B60R2011/0082	10	{collapsible, e.g. for storing after use}	B60R11/00	B60R11/00		2138
B60R2011/0084	10	{with adjustment by linear movement in their operational position}	B60R11/00	B60R11/00		2053
B60R2011/0085	10	{with adjustment by rotation in their operational position}	B60R11/00	B60R11/00		3525
B60R2011/0087	11	{around two axes}	B60R11/00	B60R11/00		385
B60R2011/0089	11	{around three axes, i.e. universally mounted}	B60R11/00	B60R11/00		489
B60R2011/0091	12	{the article being mounted on a flexible shaft}	B60R11/00	B60R11/00		131
B60R2011/0092	10	{with motorization}	B60R11/00	B60R11/00		2576
B60R2011/0094	8	{characterised by means for covering after user, e.g. boxes, shutters or the like}	B60R11/00	B60R11/00		1502
B60R2011/0096	8	{Theft prevention of articles}	B60R11/00	B60R11/00		559
B60R2011/0098	9	{using electric or electronic means, e.g. alarms, codes}	B60R11/00	B60R11/00		216
B60R11/02	8	for radio sets, television sets, telephones, or the like; Arrangement of controls thereof	B60R11/02	B60R11/02		7135
B60R11/0205	9	{for radio sets (B60R11/0211 takes precedence)}	B60R11/02	B60R11/02		923
B60R11/0211	9	{for record carriers apparatus, e.g. video recorders, tape players or CD players}	B60R11/02	B60R11/02		2335
B60R11/0217	9	{for loud-speakers}	B60R11/02	B60R11/02		2476
B60R11/0223	10	{of flat type}	B60R11/02	B60R11/02		184
B60R11/0229	9	{for displays, e.g. cathodic tubes}	B60R11/02	B60R11/02		3016
B60R11/0235	10	{of flat type, e.g. LCD}	B60R11/02	B60R11/02		3374
B60R11/0241	9	{for telephones}	B60R11/02	B60R11/02		4183
B60R11/0247	9	{for microphones or earphones}	B60R11/02	B60R11/02		820
B60R11/0252	9	{for personal computers, e.g. laptops, notebooks}	B60R11/02	B60R11/02		1056
B60R11/0258	9	{for navigation systems}	B60R11/02	B60R11/02		1331
B60R11/0264	9	{for control means}	B60R11/02	B60R11/02		1180
B60R2011/027	9	{for Din-sized apparatus}	B60R11/02	B60R11/02		106
B60R2011/0276	9	{for rear passenger use}	B60R11/02	B60R11/02		326
B60R2011/0282	9	{for the use of several passengers, e.g. simultaneously}	B60R11/02	B60R11/02		120
B60R2011/0288	9	{Apparatus made of several modules independently mounted}	B60R11/02	B60R11/02		168
B60R2011/0294	9	{Apparatus with multi-functionalities, e.g. radio and telephone}	B60R11/02	B60R11/02		426
B60R11/04	8	Mounting of cameras operative during drive; Arrangement of controls thereof relative to the vehicle	B60R11/04	B60R11/04		8807
B60R11/06	8	for tools or spare parts (for vehicle roof parts B60J7/20; for spare wheels B62D)	B60R11/06	B60R11/06		2120
B60R13/00	7	Elements for body-finishing, identifying, or decorating; Arrangements or adaptations for advertising purposes	B60R13/00	B60R13/00		1838
B60R13/005	8	{Manufacturers&apos; emblems, name plates, bonnet ornaments, mascots or the like; Mounting means therefor}	B60R13/00	B60R13/00		1984
B60R13/01	8	Liners for load platforms or load compartments	B60R13/01	B60R13/01		842
B60R13/011	9	{for internal load compartments, e.g. car trunks}	B60R13/01	B60R13/01		600
B60R13/013	10	{comprising removable or hinged parts, e.g. for accessing storage compartments}	B60R13/01	B60R13/01		350
B60R2013/015	9	{made of a plurality of visible parts}	B60R13/01	B60R13/01		54
B60R2013/016	9	{integrating other functions or accessories}	B60R13/01	B60R13/01		217
B60R2013/018	9	{Connection or positioning of adjacent panels}	B60R13/01	B60R13/01		120
B60R13/02	8	{Internal} Trim mouldings {; Internal} Ledges; Wall liners {for passenger compartments}; Roof liners (B60R13/01 takes precedence {; padded linings for the vehicle interior B60R21/04; arrangements or adaptations of floor mats or carpets in vehicles B60N3/04; internal lining for trains B61D17/18})	B60R13/02	B60R13/02		5667
B60R13/0206	9	{Arrangements of fasteners and clips specially adapted for attaching inner vehicle liners or mouldings (devices for fastening or securing F16B)}	B60R13/02	B60R13/02		3707
B60R13/0212	9	{Roof or head liners (movable head-liners B60J7/0007)}	B60R13/02	B60R13/02		1492
B60R13/0218	10	{supported by adhesion with the roof panel}	B60R13/02	B60R13/02		271
B60R13/0225	10	{self supporting head liners}	B60R13/02	B60R13/02		804
B60R13/0231	10	{specially adapted for roofs with openings}	B60R13/02	B60R13/02		303
B60R13/0237	9	{Side or rear panels}	B60R13/02	B60R13/02		336
B60R13/0243	10	{Doors}	B60R13/02	B60R13/02		2333
B60R13/025	10	{Pillars; Roof rails}	B60R13/02	B60R13/02		1086
B60R13/0256	9	{Dashboard liners}	B60R13/02	B60R13/02		876
B60R13/0262	9	{Mid-console liners}	B60R13/02	B60R13/02		281
B60R13/0268	9	{Rear parcel liners (used as luggage covering means B60R5/044)}	B60R13/02	B60R13/02		123
B60R13/0275	9	{comprising removable or hinged parts (for accessing storage compartments B60R7/04; for airbag deployment B60R21/215)}	B60R13/02	B60R13/02		353
B60R2013/0281	9	{made of a plurality of visible parts}	B60R13/02	B60R13/02		497
B60R2013/0287	9	{integrating other functions or accessories}	B60R13/02	B60R13/02		2461
B60R2013/0293	9	{Connection or positioning of adjacent panels}	B60R13/02	B60R13/02		741
B60R13/04	8	{External} Ornamental or guard strips; Ornamental inscriptive devices {thereon (fastening strips or bars to sheets or plates by means of clips F16B5/12)}	B60R13/04	B60R13/04		5441
B60R13/043	9	{Door edge guards}	B60R13/04	B60R13/04		567
B60R2013/046	9	{Foot boards}	B60R13/04	B60R13/04		240
B60R13/06	8	Sealing strips (sealing arrangements for vehicle windows, windscreens, non-fixed roofs, doors, or similar devices B60J10/00)	B60R13/06	B60R13/06		1985
B60R13/07	8	Water drainage or guide means not integral with roof structure (B60R13/06, {B60J10/25} take precedence; {integral with roof structure B62D25/07; drainage openings having movable or removable closures B62D25/24})	B60R13/07	B60R13/07		1174
B60R13/08	8	Insulating elements, e.g. for sound insulation {(sound insulating linings for trains B61D17/185; drivers&apos; cabs for load-carrying vehicles insulated against vibrations or noise B62D33/0604; thermal or acoustic insulation of engines F02B77/11; damping of sounds using compensation by electro-acoustic methods G10K11/178)}	B60R13/08	B60R13/08		2786
B60R2013/0807	9	{Arrangements of fasteners or clips specially adapted therefore}	B60R13/08	B60R13/08		242
B60R13/0815	9	{Acoustic or thermal insulation of passenger compartments (wall or roof liners integrating the insulating function B60R13/02; insulating floor mats or carpets B60N3/04)}	B60R13/08	B60R13/08		1507
B60R13/0823	10	{Insulating partitions, e.g. between front and rear seats}	B60R13/08	B60R13/08		112
B60R13/083	10	{for fire walls or floors}	B60R13/08	B60R13/08		718
B60R13/0838	9	{for engine compartments}	B60R13/08	B60R13/08		1226
B60R13/0846	9	{for duct, cable or rod passages, e.g. between engine and passenger compartments}	B60R13/08	B60R13/08		295
B60R13/0853	10	{specially adapted for movable parts, e.g. gears levers, pedals}	B60R13/08	B60R13/08		121
B60R13/0861	9	{for covering undersurfaces of vehicles, e.g. wheel houses}	B60R13/08	B60R13/08		881
B60R13/0869	9	{for protecting heat sensitive parts, e.g. electronic components}	B60R13/08	B60R13/08		182
B60R13/0876	9	{for mounting around heat sources, e.g. exhaust pipes}	B60R13/08	B60R13/08		502
B60R13/0884	9	{for mounting around noise sources, e.g. air blowers}	B60R13/08	B60R13/08		529
B60R13/0892	9	{for humidity insulation (sealing strips B60R13/06)}	B60R13/08	B60R13/08		299
B60R13/10	8	Registration, licensing, or like devices	B60R13/10	B60R13/10		2433
B60R13/105	9	{Licence- or registration plates, provided with mounting means, e.g. frames, holders, retainers, brackets}	B60R13/10	B60R13/10		2534
B60R15/00	7	Arrangements or adaptations of sanitation devices	B60R15/00	B60R15/00		684
B60R15/02	8	Washing facilities {(in railway vehicles B61D35/002)}	B60R15/02	B60R15/02		591
B60R15/04	8	Toilet facilities {(in railway vehicles B61D35/005)}	B60R15/04	B60R15/04		817
B60R16/00	7	Electric or fluid circuits specially adapted for vehicles and not otherwise provided for; Arrangement of elements of electric or fluid circuits specially adapted for vehicles and not otherwise provided for {(devices for protecting vehicle occupants in case of accidents B60R21/00; safety belts B60R22/00; central door locking E05B49/00, E05B77/50)}	B60R16/00	B60R16/00		584
B60R16/005	8	{Electro-mechanical devices, e.g. switched (electric switches in general H01H)}	B60R16/00	B60R16/00		3923
B60R16/02	8	electric {constitutive elements}	B60R16/02	B60R16/02		11467
B60R16/0207	9	{Wire harnesses}	B60R16/02	B60R16/02		2216
B60R16/0215	10	{Protecting, fastening and routing means therefor}	B60R16/02	B60R16/02		7749
B60R16/0222	11	{Grommets}	B60R16/02	B60R16/02		1148
B60R16/023	9	for transmission of signals between vehicle parts or subsystems	B60R16/023	B60R16/023		9748
B60R16/0231	10	{Circuits relating to the driving or the functioning of the vehicle (monitoring tyres B60C23/00; indicating overspeed B60K31/00; for dash boards B60K37/00, B60Q3/10; for indicating emergencies B60Q1/52; brake control systems B60T; registering or indicating the working of vehicles G07C5/00; measuring distance G01C, e.g. combinations of speed and distance G01C23/00; engine indicators G01L; measuring speed or acceleration G01P)}	B60R16/023	B60R16/023		6163
B60R16/0232	11	{for measuring vehicle parameters and indicating critical, abnormal or dangerous conditions}	B60R16/023	B60R16/023		4605
B60R16/0233	12	{Vehicle tilting, overturning or roll over}	B60R16/023	B60R16/023		198
B60R16/0234	12	{related to maintenance or repairing of vehicles}	B60R16/023	B60R16/023		998
B60R16/0235	11	{for lighting devices combined with starting or ignition devices for road vehicles}	B60R16/023	B60R16/023		322
B60R16/0236	11	{for economical driving}	B60R16/023	B60R16/023		541
B60R16/0237	10	{circuits concerning the atmospheric environment (meteorology G01W)}	B60R16/023	B60R16/023		304
B60R16/0238	10	{Electrical distribution centers}	B60R16/023	B60R16/023		1599
B60R16/0239	10	{Electronic boxes}	B60R16/023	B60R16/023		2452
B60R16/027	10	between relatively movable parts of the vehicle, e.g. between steering wheel and column {(devices for measuring, signalling or controlling tyre pressure or temperature specially adapted for mounting on vehicles B60C23/00)}	B60R16/027	B60R16/027		1829
B60R16/03	9	for supply of electrical power to vehicle subsystems {or for (circuit arrangements for charging batteries H02J7/00)}	B60R16/03	B60R16/03		9259
B60R16/0307	10	{using generators driven by a machine different from the vehicle motor}	B60R16/03	B60R16/03		547
B60R16/0315	10	{using multiplexing techniques (multiplexing for transmission of signals G08C15/00; multiplexing for electrical communication in general H04J)}	B60R16/03	B60R16/03		1907
B60R2016/0322	11	{Temporary code for documents to be reclassified to G08C, H04L or H04Q}	B60R16/03	B60R16/03		161
B60R16/033	10	characterised by the use of electrical cells or batteries (for propulsion puposes B60K1/04; supplying batteries to, or removing batteries from, vehicles B60S5/06; testing of charge state G01R31/36)	B60R16/033	B60R16/033		6442
B60R16/037	9	for occupant comfort {, e.g. for automatic adjustment of appliances according to personal settings, e.g. seats, mirrors, steering wheel}	B60R16/037	B60R16/037		4761
B60R16/0373	10	{Voice control (in general G10L)}	B60R16/037	B60R16/037		1634
B60R16/04	9	Arrangement of batteries	B60R16/04	B60R16/04		2447
B60R16/06	9	for removing electrostatic charges (carrying-off electrostatic charges in general H05F3/00)	B60R16/06	B60R16/06		602
B60R16/08	8	fluid	B60R16/08	B60R16/08		747
B60R17/00	7	Arrangements or adaptations of lubricating systems or devices (lubricating in general F16N)	B60R17/00	B60R17/00		643
B60R17/02	8	Systems, e.g. central lubrication systems	B60R17/02	B60R17/02		458
B60R19/00	7	Wheel guards; Radiator guards, {e.g. grilles}; Obstruction removers; Fittings damping bouncing force in collisions ({reinforcement elements for side doors B60J5/0412; } mudguards B62D)	B60R19/00	B60R19/00		785
B60R2019/002	8	{Wheel guards}	B60R19/00	B60R19/00		105
B60R2019/005	8	{Crash attenuators, i.e. means added to highway service vehicles for softening high speed impacts}	B60R19/00	B60R19/00		128
B60R2019/007	8	{Means for adjusting or regulating the crash absorption capacity of the vehicle, e.g. when detecting an impending collision}	B60R19/00	B60R19/00		326
B60R19/02	8	Bumpers, i.e. impact receiving or absorbing members for protecting vehicles or fending off blows from other vehicles or objects ({B60R19/56 takes precedence; initiating brake action by contact of bumper with an external object B60T7/22; for rail vehicles B61F19/04; safety equipment for cycles B62J27/00;} integral with waterborne vessels or specially adapted therefor B63B59/02)	B60R19/02	B60R19/02		1764
B60R19/023	9	{Details}	B60R19/02	B60R19/02		1924
B60R2019/026	9	{Buffers, i.e. bumpers of limited extent}	B60R19/02	B60R19/02		561
B60R19/03	9	characterised by material, e.g. composite (B60R19/18 takes precedence)	B60R19/03	B60R19/03		1056
B60R19/04	9	formed from more than one section {in a side-by-side arrangement}	B60R19/04	B60R19/04		939
B60R19/12	10	vertically spaced	B60R19/12	B60R19/12		611
B60R19/14	10	having folding parts	B60R19/14	B60R19/14		224
B60R19/16	10	having deflecting members, e.g. rollers, balls	B60R19/16	B60R19/16		252
B60R19/18	9	{characterised by the cross-section;} Means within the bumper to absorb impact	B60R19/18	B60R19/18		5244
B60R2019/1806	10	{Structural beams therefor, e.g. shock-absorbing}	B60R19/18	B60R19/18		1237
B60R2019/1813	11	{made of metal}	B60R19/18	B60R19/18		581
B60R2019/182	12	{of light metal, e.g. extruded}	B60R19/18	B60R19/18		380
B60R2019/1826	12	{of high-tension steel}	B60R19/18	B60R19/18		185
B60R2019/1833	11	{made of plastic material}	B60R19/18	B60R19/18		294
B60R2019/184	12	{Blow moulded}	B60R19/18	B60R19/18		61
B60R2019/1846	12	{comprising a cellular structure}	B60R19/18	B60R19/18		141
B60R2019/1853	12	{of reinforced plastic material}	B60R19/18	B60R19/18		261
B60R2019/186	10	{Additional energy absorbing means supported on bumber beams, e.g. cellular structures or material}	B60R19/18	B60R19/18		1074
B60R2019/1866	11	{Cellular structures}	B60R19/18	B60R19/18		409
B60R2019/1873	11	{Cellular materials}	B60R19/18	B60R19/18		344
B60R2019/188	11	{Blow molded structures}	B60R19/18	B60R19/18		46
B60R2019/1886	10	{Bumper fascias and fastening means therefor}	B60R19/18	B60R19/18		1313
B60R2019/1893	10	{comprising a multiplicity of identical adjacent shock-absorbing means}	B60R19/18	B60R19/18		410
B60R19/20	10	containing {mainly} gas or liquid, e.g. inflatable (connection of valves to inflatable elastic bodies B60C29/00)	B60R19/20	B60R19/20		838
B60R19/205	11	{inflatable in the direction of an obstacle upon impending impact, e.g. using air bags}	B60R19/20	B60R19/20		636
B60R19/22	10	containing {mainly} cellular material, e.g. solid foam	B60R19/22	B60R19/22		490
B60R19/24	9	Arrangements for mounting bumpers on vehicles	B60R19/24	B60R19/24		3028
B60R2019/242	10	{on two vertical sleeves, e.g. on energy absorber ends}	B60R19/24	B60R19/24		179
B60R2019/245	10	{with adjusting means to compensate manufacturing tolerances, e.g. between bumper and energy absorbers}	B60R19/24	B60R19/24		178
B60R2019/247	10	{Fastening of bumpers&apos; side ends}	B60R19/24	B60R19/24		905
B60R19/26	10	comprising yieldable mounting means ({B60R19/38 takes precedence;} springs, shock absorbers, or means for damping vibrations per seF16F)	B60R19/26	B60R19/26		1424
B60R2019/262	11	{with means to adjust or regulate the amount of energy to be absorbed}	B60R19/26	B60R19/26		304
B60R2019/264	11	{using cellular structures}	B60R19/26	B60R19/26		66
B60R2019/266	11	{using friction sufaces}	B60R19/26	B60R19/26		53
B60R2019/268	11	{with rebound preventing means, e.g. ratchets}	B60R19/26	B60R19/26		20
B60R19/28	11	Metallic springs	B60R19/28	B60R19/28		700
B60R19/285	12	{comprising only leaf springs, e.g. the mounting means forming part of the guard itself}	B60R19/28	B60R19/28		999
B60R19/30	11	Elastomeric material {(B60R19/34 takes precedence)}	B60R19/30	B60R19/30		323
B60R19/32	11	Fluid shock absorbers {, e.g. with coaxial coil springs}	B60R19/32	B60R19/32		613
B60R19/34	11	destroyed upon impact, e.g. one-shot type	B60R19/34	B60R19/34		2929
B60R19/36	11	Combinations of yieldable mounting means of different types {(fluid shock absorbers with coaxial coil springs B60R19/32)}	B60R19/36	B60R19/36		432
B60R19/38	10	adjustably or movably mounted, e.g. horizontally displaceable for securing a space between parked vehicles {(adjustably mounted for compensating manufacturing tolerances B60R19/24, B60R19/26)}	B60R19/38	B60R19/38		773
B60R19/40	11	in the direction of an obstacle before a collision {, or extending during driving of the vehicle, i.e. to increase the energy absorption capacity of the bumper (inflatable bumpers B60R19/20)}	B60R19/40	B60R19/40		637
B60R19/42	9	extending primarily along the sides of, or completely encircling, a vehicle (ornamental or guard strips B60R13/04)	B60R19/42	B60R19/42		823
B60R19/44	9	Bumper guards	B60R19/44	B60R19/44		561
B60R19/445	10	{Guard strips}	B60R19/44	B60R19/44		205
B60R19/46	10	spring- or pivotally-mounted	B60R19/46	B60R19/46		79
B60R19/48	9	combined with, or convertible into, other devices or objects, e.g. bumpers combined with road brushes, bumpers convertible into beds	B60R19/48	B60R19/48		1928
B60R19/483	10	{with obstacle sensors of electric or electronic type}	B60R19/48	B60R19/48		1690
B60R2019/486	10	{with air passages, e.g. for cooling}	B60R19/48	B60R19/48		288
B60R19/50	10	with lights or registration plates	B60R19/50	B60R19/50		712
B60R2019/505	11	{with lights}	B60R19/50	B60R19/50		486
B60R19/52	8	Radiator or grille guards {; Radiator grilles (cooling aspects B60K11/08)}	B60R19/52	B60R19/52		2103
B60R2019/522	9	{Bull bars}	B60R19/52	B60R19/52		89
B60R2019/525	9	{Radiator grilles}	B60R19/52	B60R19/52		1102
B60R2019/527	10	{integral with bumpers}	B60R19/52	B60R19/52		232
B60R19/54	8	Obstruction removers or deflectors (B60R19/16, B60R21/34 take precedence)	B60R19/54	B60R19/54		486
B60R19/545	9	{Devices for cutting wire-type obstructions}	B60R19/54	B60R19/54		63
B60R19/56	8	{Fittings damping bouncing force in truck collisions, e.g. bumpers;} Arrangements on high-riding vehicles, e.g. lorries, for preventing vehicles or objects from running thereunder	B60R19/56	B60R19/56		815
B60R19/565	9	{on vehicle sides}	B60R19/56	B60R19/56		329
B60R21/00	7	Arrangements or fittings on vehicles for protecting or preventing injuries to occupants or pedestrians in case of accidents or other traffic risks (safety belts or body harnesses in vehicles B60R22/00; seats constructed to protect the occupant from the effect of abnormal g-forces, e.g. crash or safety seats, B60N2/42; energy-absorbing arrangements for hand wheels for steering vehicles B62D1/11; energy-absorbing arrangements for vehicle steering columns B62D1/19)	B60R21/00	B60R21/00		2747
B60R2021/0002	8	{Type of accident}	B60R21/00	B60R21/00		131
B60R2021/0004	9	{Frontal collision}	B60R21/00	B60R21/00		1679
B60R2021/0006	9	{Lateral collision}	B60R21/00	B60R21/00		3342
B60R2021/0009	9	{Oblique collision}	B60R21/00	B60R21/00		370
B60R2021/0011	9	{Rear collision or recoiling bounce after frontal collision}	B60R21/00	B60R21/00		411
B60R2021/0013	9	{Free fall}	B60R21/00	B60R21/00		40
B60R2021/0016	9	{Fall in water}	B60R21/00	B60R21/00		653
B60R2021/0018	9	{Roll-over}	B60R21/00	B60R21/00		896
B60R2021/002	9	{Underrun collision}	B60R21/00	B60R21/00		44
B60R2021/0023	9	{Offset collision}	B60R21/00	B60R21/00		155
B60R2021/0025	9	{Pole collision}	B60R21/00	B60R21/00		32
B60R2021/0027	8	{Post collision measures, e.g. notifying emergency services}	B60R21/00	B60R21/00		725
B60R2021/003	8	{characterised by occupant or pedestian}	B60R21/00	B60R21/00		314
B60R2021/0032	9	{Position of passenger}	B60R21/00	B60R21/00		192
B60R2021/0034	10	{lying down}	B60R21/00	B60R21/00		103
B60R2021/0037	10	{standing}	B60R21/00	B60R21/00		48
B60R2021/0039	9	{Body parts of the occupant or pedestrian affected by the accident}	B60R21/00	B60R21/00		99
B60R2021/0041	10	{Arms}	B60R21/00	B60R21/00		41
B60R2021/0044	10	{Chest}	B60R21/00	B60R21/00		345
B60R2021/0046	10	{Feet}	B60R21/00	B60R21/00		152
B60R2021/0048	10	{Head}	B60R21/00	B60R21/00		1159
B60R2021/0051	10	{Knees}	B60R21/00	B60R21/00		784
B60R2021/0053	10	{Legs}	B60R21/00	B60R21/00		261
B60R2021/0055	10	{Pelvis}	B60R21/00	B60R21/00		158
B60R2021/0058	10	{Shoulders}	B60R21/00	B60R21/00		144
B60R2021/006	9	{Type of passenger}	B60R21/00	B60R21/00		122
B60R2021/0062	10	{woman, e.g. pregnant}	B60R21/00	B60R21/00		16
B60R2021/0065	8	{Type of vehicles}	B60R21/00	B60R21/00		35
B60R2021/0067	9	{Buses}	B60R21/00	B60R21/00		346
B60R2021/0069	9	{Trailers, e.g. caravans}	B60R21/00	B60R21/00		55
B60R2021/0072	9	{Convertible cars}	B60R21/00	B60R21/00		72
B60R2021/0074	9	{Utility vehicles}	B60R21/00	B60R21/00		213
B60R2021/0076	10	{Agricultural vehicles, e.g. tractors}	B60R21/00	B60R21/00		33
B60R2021/0079	10	{Fork-lift trucks}	B60R21/00	B60R21/00		37
B60R2021/0081	10	{Working vehicles}	B60R21/00	B60R21/00		69
B60R2021/0083	10	{Pick-up trucks; Light trucks; Sport utility vehicles}	B60R21/00	B60R21/00		64
B60R2021/0086	9	{Racing cars}	B60R21/00	B60R21/00		57
B60R2021/0088	9	{Cycles, e.g. motorcycles}	B60R21/00	B60R21/00		284
B60R2021/009	9	{Railway vehicles}	B60R21/00	B60R21/00		56
B60R2021/0093	9	{Aircraft}	B60R21/00	B60R21/00		139
B60R2021/0095	9	{Boats}	B60R21/00	B60R21/00		21
B60R2021/0097	9	{Amusement vehicles}	B60R21/00	B60R21/00		111
B60R21/01	8	Electrical circuits for triggering {passive} safety arrangements, {e.g. airbags, safety belt tighteners,} in case of vehicle accidents or impending vehicle accidents {(electrical circuits for transmission of signals between steering wheel and the vehicle itself B60R16/027; for electrically actuating belt retractor locking means B60R22/343)}	B60R21/01	B60R21/01		2897
B60R2021/01006	9	{Mounting of electrical components in vehicles}	B60R21/01	B60R21/01		452
B60R2021/01013	9	{Means for detecting collision, impending collision or roll-over}	B60R21/01	B60R21/01		848
B60R2021/0102	10	{the monitored value being used for calculating occupant displacement}	B60R21/01	B60R21/01		39
B60R2021/01027	10	{Safing sensors}	B60R21/01	B60R21/01		256
B60R2021/01034	9	{Controlling a plurality of restraint devices}	B60R21/01	B60R21/01		241
B60R2021/0104	9	{Communication circuits for data transmission}	B60R21/01	B60R21/01		133
B60R2021/01047	10	{Architecture}	B60R21/01	B60R21/01		20
B60R2021/01054	11	{Bus}	B60R21/01	B60R21/01		67
B60R2021/01061	12	{between the airbag system and other vehicle electronic systems}	B60R21/01	B60R21/01		77
B60R2021/01068	12	{between different sensors and airbag control unit}	B60R21/01	B60R21/01		165
B60R2021/01075	12	{between the airbag control unit and pyrotechnic fuses or equivalent actuators}	B60R21/01	B60R21/01		118
B60R2021/01081	10	{Transmission medium}	B60R21/01	B60R21/01		6
B60R2021/01088	11	{wireless}	B60R21/01	B60R21/01		239
B60R2021/01095	11	{optical}	B60R21/01	B60R21/01		80
B60R2021/01102	10	{Transmission method}	B60R21/01	B60R21/01		18
B60R2021/01109	11	{power and data signal using transmission medium}	B60R21/01	B60R21/01		41
B60R2021/01115	11	{specific data frames}	B60R21/01	B60R21/01		119
B60R2021/01122	9	{Prevention of malfunction}	B60R21/01	B60R21/01		127
B60R2021/01129	10	{Problems or faults}	B60R21/01	B60R21/01		35
B60R2021/01136	11	{Cut lines}	B60R21/01	B60R21/01		21
B60R2021/01143	11	{Short circuits}	B60R21/01	B60R21/01		22
B60R2021/0115	11	{Current leakage}	B60R21/01	B60R21/01		8
B60R2021/01156	11	{Current or voltage overload}	B60R21/01	B60R21/01		12
B60R2021/01163	11	{Insufficient current or voltage}	B60R21/01	B60R21/01		21
B60R2021/0117	11	{Noise}	B60R21/01	B60R21/01		35
B60R2021/01177	11	{Misdeployment, e.g. during assembly, disassembly, accident salvage or recycling}	B60R21/01	B60R21/01		47
B60R2021/01184	10	{Fault detection or diagnostic circuits}	B60R21/01	B60R21/01		263
B60R2021/0119	11	{Plausibility check}	B60R21/01	B60R21/01		159
B60R2021/01197	11	{Warning devices}	B60R21/01	B60R21/01		74
B60R2021/01204	9	{Actuation parameters of safety arrangents}	B60R21/01	B60R21/01		160
B60R2021/01211	10	{Expansion of air bags}	B60R21/01	B60R21/01		862
B60R2021/01218	11	{control of expansion speed}	B60R21/01	B60R21/01		76
B60R2021/01225	11	{control of expansion volume}	B60R21/01	B60R21/01		144
B60R2021/01231	11	{control of expansion timing or sequence}	B60R21/01	B60R21/01		236
B60R2021/01238	11	{control of expansion shape}	B60R21/01	B60R21/01		91
B60R2021/01245	11	{selection of seat for bag expansion}	B60R21/01	B60R21/01		98
B60R2021/01252	10	{Devices other than bags}	B60R21/01	B60R21/01		525
B60R2021/01259	11	{Brakes}	B60R21/01	B60R21/01		177
B60R2021/01265	11	{Seat belts}	B60R21/01	B60R21/01		282
B60R2021/01272	12	{Belt tensioners}	B60R21/01	B60R21/01		451
B60R2021/01279	12	{Load limiters}	B60R21/01	B60R21/01		44
B60R2021/01286	9	{Electronic control units}	B60R21/01	B60R21/01		740
B60R2021/01293	10	{programmable for use in different vehicles or with different airbags configurations}	B60R21/01	B60R21/01		16
B60R21/013	9	including means for detecting collisions, impending collisions or roll-over	B60R21/013	B60R21/013		3755
B60R2021/01302	10	{monitoring vehicle body vibrations or noise}	B60R21/013	B60R21/013		123
B60R2021/01304	10	{monitoring rough road condition}	B60R21/013	B60R21/013		53
B60R2021/01306	10	{monitoring vehicle inclination}	B60R21/013	B60R21/013		239
B60R2021/01308	10	{monitoring distance between vehicle body and road}	B60R21/013	B60R21/013		36
B60R2021/01311	10	{monitoring the braking system, e.g. ABS}	B60R21/013	B60R21/013		188
B60R2021/01313	10	{monitoring the vehicle steering system or the dynamic control system}	B60R21/013	B60R21/013		204
B60R2021/01315	10	{monitoring occupant displacement}	B60R21/013	B60R21/013		190
B60R2021/01317	10	{monitoring seat belt tensiont}	B60R21/013	B60R21/013		70
B60R21/0132	10	responsive to vehicle motion parameters {, e.g. to vehicle longitudinal or transversal deceleration or speed value}	B60R21/0132	B60R21/0132		2533
B60R2021/01322	11	{comprising variable thresholds, e.g. depending from other collision parameters}	B60R21/0132	B60R21/0132		440
B60R2021/01325	11	{Vertical acceleration}	B60R21/0132	B60R21/0132		193
B60R2021/01327	11	{Angular velocity or angular acceleration}	B60R21/0132	B60R21/0132		354
B60R21/0133	11	{by integrating the amplitude of the input signal}	B60R21/0132	B60R21/013		295
B60R21/01332	11	{by frequency or waveform analysis}	B60R21/0132	B60R21/013		191
B60R21/01334	12	{using Fourier analysis}	B60R21/0132	B60R21/013		21
B60R21/01336	12	{using filtering}	B60R21/0132	B60R21/013		187
B60R21/01338	12	{using vector analysis}	B60R21/0132	B60R21/013		59
B60R21/0134	10	responsive to imminent contact with an obstacle {, e.g. using radar systems}	B60R21/0134	B60R21/0134		3903
B60R2021/01345	11	{using mechanical sensing means}	B60R21/0134	B60R21/0134		91
B60R21/0136	10	responsive to actual contact with an obstacle {, e.g. to vehicle deformation, bumper displacement or bumper velocity relative to the vehicle (monitoring crash strength in combination with passenger seat detection B60R21/01558)}	B60R21/0136	B60R21/0136		3085
B60R21/015	9	including means for detecting the presence or position of passengers, passenger seats or child seats {, and the related safety parameters therefor, e.g. speed or timing of airbag inflation in relation to occupant position or seat belt use}	B60R21/015	B60R21/015		961
B60R21/01504	10	{detecting bag displacement}	B60R21/015	B60R21/015		85
B60R21/01508	10	{detecting forces or pressure in bags or modules}	B60R21/015	B60R21/015		92
B60R21/01512	10	{Passenger detection systems}	B60R21/015	B60R21/015		1135
B60R21/01516	11	{using force or pressure sensing means}	B60R21/015	B60R21/015		1625
B60R21/0152	12	{using strain gauges}	B60R21/015	B60R21/015		361
B60R21/01522	12	{using fluid means}	B60R21/015	B60R21/015		31
B60R21/01524	12	{using electric switches}	B60R21/015	B60R21/015		72
B60R21/01526	12	{using piezoelectric elements}	B60R21/015	B60R21/015		231
B60R21/01528	11	{mounted on the bag}	B60R21/015	B60R21/015		42
B60R21/0153	11	{using field detection presence sensors}	B60R21/015	B60R21/015		443
B60R21/01532	12	{using electric or capacitive field sensors}	B60R21/015	B60R21/015		583
B60R21/01534	12	{using electromagneticwaves, e.g. infrared}	B60R21/015	B60R21/015		665
B60R21/01536	12	{using ultrasonic waves}	B60R21/015	B60R21/015		311
B60R21/01538	12	{for image processing, e.g. cameras or sensor arrays}	B60R21/015	B60R21/015		924
B60R21/0154	12	{in combination with seat heating}	B60R21/015	B60R21/015		178
B60R21/01542	11	{detecting passenger motion}	B60R21/015	B60R21/015		499
B60R21/01544	11	{detecting seat belt parameters, e.g. length, tension or height-adjustment}	B60R21/015	B60R21/015		495
B60R21/01546	12	{using belt buckle sensors}	B60R21/015	B60R21/015		461
B60R21/01548	12	{sensing the amount of belt winded on retractor}	B60R21/015	B60R21/015		230
B60R21/0155	12	{sensing belt tension}	B60R21/015	B60R21/015		205
B60R21/01552	11	{detecting position of specific human body parts, e.g. face, eyes or hands}	B60R21/015	B60R21/015		496
B60R21/01554	10	{Seat position sensors}	B60R21/015	B60R21/015		804
B60R21/01556	10	{Child-seat detection systems}	B60R21/015	B60R21/015		577
B60R21/01558	10	{monitoring crash strength}	B60R21/015	B60R21/015		156
B60R21/0156	11	{by deceleration}	B60R21/015	B60R21/015		58
B60R21/01562	11	{by speed}	B60R21/015	B60R21/015		30
B60R21/01564	10	{Manually or key-actuated inhibition switches}	B60R21/015	B60R21/015		115
B60R21/01566	10	{Devices for warning or indicating mode of inhibition}	B60R21/015	B60R21/015		235
B60R21/017	9	including arrangements for providing electric power to safety arrangements {or their actuating means, e.g. to pyrotechnic fuses or electro-mechanic valves}	B60R21/017	B60R21/017		882
B60R21/0173	10	{Diagnostic or recording means therefor}	B60R21/017	B60R21/017		443
B60R21/0176	11	{for firing circuits using only mechanical switches as collision detecting means, in series with pyrotechnic fuses}	B60R21/017	B60R21/017		70
B60R21/02	8	Occupant safety arrangements or fittings {, e.g. crash pads (seat belts with crash pads B60R22/14; removable children&apos;s seats having a front guard or barrier B60N2/2839)}	B60R21/02	B60R21/02		2847
B60R2021/0206	9	{Self-supporting restraint systems, e.g. restraining arms, plates or the like}	B60R21/02	B60R21/02		113
B60R2021/0213	10	{mounted on floor}	B60R21/02	B60R21/02		106
B60R2021/022	10	{mounted on seats}	B60R21/02	B60R21/02		488
B60R2021/0226	10	{mounted on fire wall}	B60R21/02	B60R21/02		21
B60R2021/0233	10	{mounted on steering-wheel}	B60R21/02	B60R21/02		22
B60R2021/024	10	{mounted on dash-board}	B60R21/02	B60R21/02		179
B60R2021/0246	10	{mounted on side walls}	B60R21/02	B60R21/02		103
B60R2021/0253	10	{mounted on roof}	B60R21/02	B60R21/02		68
B60R21/026	9	{Rigid partitions inside vehicles, e.g. between passengers and load compartments (B60R21/12 takes precedence)}	B60R21/02	B60R21/02		937
B60R2021/0266	10	{comprising energy absorbing means}	B60R21/02	B60R21/02		91
B60R2021/0273	9	{automatically movable to an operative position, e.g. in case of collision or impending collision}	B60R21/02	B60R21/02		304
B60R2021/028	9	{Means preventing passenger from falling out of vehicles}	B60R21/02	B60R21/02		147
B60R21/0286	9	{Padded or energy absorbing driving control initiating means, e.g. gear lever, pedals (B60R21/09 takes precedence; padded linings for steering control means B60R21/05)}	B60R21/02	B60R21/02		50
B60R2021/0293	9	{Additional pads or cushions in vehicle compartments, e.g. movably mounted}	B60R21/02	B60R21/02		235
B60R21/04	9	Padded linings for the vehicle interior {; Energy absorbing structures associated with padded or non-padded linings}	B60R21/04	B60R21/04		972
B60R2021/0407	10	{using gas or liquid as energy absorbing means}	B60R21/04	B60R21/04		225
B60R2021/0414	10	{using energy absorbing ribs}	B60R21/04	B60R21/04		261
B60R2021/0421	10	{using honeycomb structures}	B60R21/04	B60R21/04		96
B60R21/0428	10	{associated with the side doors or panels, e.g. displaced towards the occupants in case of a side collision}	B60R21/04	B60R21/04		564
B60R2021/0435	10	{associated with the side or roof pillars}	B60R21/04	B60R21/04		387
B60R2021/0442	10	{associated with the roof panel}	B60R21/04	B60R21/04		172
B60R21/045	10	associated with the instrument panel or dashboard	B60R21/045	B60R21/045		1128
B60R21/05	10	associated with the steering wheel, {steering} hand lever or {steering} column (yieldable steering columns B62D1/18)	B60R21/05	B60R21/05		509
B60R21/055	9	Padded {or energy-absorbing} fittings {, e.g. seat belt anchors (sun visors B60J3/00; head rests B60N2/80)}	B60R21/055	B60R21/055		542
B60R21/06	9	Safety nets, transparent sheets, curtains, or the like, e.g. between occupants and glass ({B60R21/026} , B60R21/11, B60R21/12, B60R21/16 take precedence)	B60R21/06	B60R21/06		991
B60R2021/065	10	{comprising energy absorbing mounting means}	B60R21/06	B60R21/06		60
B60R21/08	10	{automatically} movable from an inoperative to an operative position, e.g. in a collision (electrical circuits for triggering safety arrangements B60R21/01)	B60R21/08	B60R21/08		507
B60R21/09	9	Control elements or operating handles movable from an operative to an out-of-the way position, e.g. {pedals,} switch knobs, window cranks {(specially adapted for brake pedals, e.g. by venting of master cylinder or destruction of force transmitting rod, B60T7/065)}	B60R21/09	B60R21/09		763
B60R21/11	9	Overhead guards, e.g. against loads falling down {(specially adapted for fork-lift trucks B66F9/07545)}	B60R21/11	B60R21/11		232
B60R21/12	9	which protect the occupants against personal attack from the inside or the outside of the vehicle	B60R21/12	B60R21/12		1140
B60R21/13	9	Roll-over protection (electrical circuits for triggering safety arrangements B60R21/01)	B60R21/13	B60R21/13		1433
B60R21/131	10	{Protective devices for drivers in case of overturning of tractors (means for preventing overturning or tipping of tractors B62D49/08)}	B60R21/13	B60R21/13		539
B60R2021/132	10	{Roll bars for convertible vehicles}	B60R21/13	B60R21/13		159
B60R2021/134	11	{movable from a retracted to a protection position}	B60R21/13	B60R21/13		99
B60R2021/135	12	{automatically during an accident}	B60R21/13	B60R21/13		435
B60R2021/137	10	{Reinforcement cages for closed vehicle bodies}	B60R21/13	B60R21/13		109
B60R2021/138	10	{using external airbags}	B60R21/13	B60R21/13		71
B60R21/16	9	Inflatable occupant restraints or confinements designed to inflate upon impact or impending impact, e.g. air bags ({protective garments with automatically inflatable shock-absorbing means A41D13/018; } connection of valves to inflatable elastic bodies B60C29/00)	B60R21/16	B60R21/16		2094
B60R2021/161	10	{characterised by additional means for controlling deployment trajectory}	B60R21/16	B60R21/16		1272
B60R2021/162	10	{Means for diverting, destroying or blocking the bag in case of dangerous deployment, e.g. during rescue operations or use of rear-facing children seats}	B60R21/16	B60R21/16		103
B60R21/164	10	{combined with vehicle venting means for reducing or avoiding the passenger compartment overpressure during inflation}	B60R21/16	B60R21/16		67
B60R2021/165	10	{reusable, e.g. in case of multiple collisions}	B60R21/16	B60R21/16		83
B60R2021/167	10	{comprising anti-theft devices}	B60R21/16	B60R21/16		35
B60R2021/168	10	{for restraining luggages}	B60R21/16	B60R21/16		17
B60R21/18	10	the inflatable member formed as a belt or harness or combined with a belt or harness arrangement	B60R21/18	B60R21/18		925
B60R21/20	10	Arrangements for storing inflatable members in their non-use or deflated condition; Arrangement or mounting of air bag modules or components	B60R21/20	B60R21/20		1260
B60R21/201	11	Packaging straps or envelopes for inflatable members	B60R21/201	B60R21/201		707
B60R21/203	11	in steering wheels or steering columns	B60R21/203	B60R21/203		1658
B60R21/2032	12	{the inflator or inflatable member not being rotatable with the steering wheel; Arrangements using the steering column or steering wheel rim for storing, supplying or evacuating the inflation gas or for storing the inflatable member}	B60R21/203	B60R21/203		272
B60R21/2035	12	{using modules containing inflator, bag and cover attachable to the steering wheel as a complete sub-unit (steering wheel covers with tear lines B60R21/21656; assembling of modules B60R21/217)}	B60R21/203	B60R21/203		537
B60R21/2037	13	{the module or a major component thereof being yieldably mounted, e.g. for actuating the horn switch or for protecting the driver in a non-deployment situation (horn switches integrated in steering wheel covers with tear lines B60R21/21658)}	B60R21/203	B60R21/203		702
B60R21/205	11	in dashboards	B60R21/205	B60R21/205		2473
B60R21/206	12	in the lower part of dashboards, e.g. for protecting the knees	B60R21/206	B60R21/206		778
B60R21/207	11	in vehicle seats	B60R21/207	B60R21/207		3384
B60R21/2072	12	{in children&apos;s seats}	B60R21/207	B60R21/207		141
B60R2021/2074	12	{in head rests}	B60R21/207	B60R21/207		323
B60R2021/2076	12	{Removable covers with tear seams}	B60R21/207	B60R21/207		183
B60R2021/2078	12	{in rear seats}	B60R21/207	B60R21/207		113
B60R21/21	11	in vehicle side panels, e.g. doors (pillar mounted arrangements B60R21/213)	B60R21/21	B60R21/21		616
B60R21/213	11	in vehicle roof frames or pillars	B60R21/213	B60R21/213		1994
B60R21/214	11	in roof panels	B60R21/214	B60R21/214		585
B60R21/215	11	characterised by the covers for the inflatable member {(B60R21/2176 takes precedence)}	B60R21/215	B60R21/215		1898
B60R2021/21506	12	{comprising tearing tabs, legs or the like for holding the lid before deployment}	B60R21/215	B60R21/215		197
B60R2021/21512	12	{the lid being displaced towards the occupant during deployment (B60R2021/2161, B60R2021/21525 take precedence)}	B60R21/215	B60R21/215		57
B60R2021/21518	12	{comprising a lock unlocked during deployment}	B60R21/215	B60R21/215		57
B60R2021/21525	12	{the lid being fixed on the bag, or forming part of the bag wall, or the bag itself being used as wall liner}	B60R21/215	B60R21/215		158
B60R2021/21531	12	{using a strechable wall liner}	B60R21/215	B60R21/215		58
B60R2021/21537	12	{characterised by hinges}	B60R21/215	B60R21/215		597
B60R2021/21543	12	{with emblems}	B60R21/215	B60R21/215		325
B60R21/2155	12	with complex motion of the cover; Retraction under the lining during opening	B60R21/2155	B60R21/2155		153
B60R21/216	12	comprising tether means for limitation of cover motion during deployment	B60R21/216	B60R21/216		523
B60R2021/2161	13	{the cover being displaced towards the occupant during deployment}	B60R21/216	B60R21/216		102
B60R2021/2163	13	{with energy absorbing or elastic means}	B60R21/216	B60R21/216		96
B60R21/2165	12	characterised by a tear line for defining a deployment opening	B60R21/2165	B60R21/2165		2016
B60R2021/21652	13	{the tearing being done or assisted by cutters}	B60R21/2165	B60R21/2165		114
B60R2021/21654	13	{the tearing being done or assisted by heating or pyrotechnic means}	B60R21/2165	B60R21/2165		62
B60R21/21656	13	{Steering wheel covers or similar cup-shaped covers}	B60R21/2165	B60R21/2165		481
B60R21/21658	14	{with integrated switches, e.g. horn switches}	B60R21/2165	B60R21/2165		212
B60R21/217	11	Inflation fluid source retainers, e.g. reaction canisters; Connection of bags, covers, diffusers or inflation fluid sources therewith or together	B60R21/217	B60R21/217		1563
B60R21/2171	12	{specially adapted for elongated cylindrical or bottle-like inflators with a symmetry axis perpendicular to the main direction of bag deployment, e.g. extruded reaction canisters (B60R21/2176 takes precedence)}	B60R21/217	B60R21/217		1148
B60R2021/2172	12	{the cover being connected to the surrounding part and to the module, e.g. floating mounts}	B60R21/217	B60R21/217		137
B60R2021/2173	12	{the module or part thereof being movably mounted on the vehicle}	B60R21/217	B60R21/217		207
B60R2021/2175	13	{using energy absorbing means}	B60R21/217	B60R21/217		41
B60R21/2176	12	{the air bag components being completely enclosed in a soft or semi-rigid housing or cover}	B60R21/217	B60R21/217		390
B60R2021/2177	12	{Reaction canisters characterised by material}	B60R21/217	B60R21/217		43
B60R2021/2178	13	{Plastic}	B60R21/217	B60R21/217		47
B60R21/23	10	Inflatable members (B60R21/18 takes precedence; connection to inflation fluid source retainers B60R21/217)	B60R21/23	B60R21/23		386
B60R21/231	11	characterised by their shape, construction or spatial configuration	B60R21/231	B60R21/231		2458
B60R2021/23107	12	{the bag being integrated in a multi-bag system}	B60R21/231	B60R21/231		914
B60R2021/23115	12	{with inflatable support compartments creating an internal suction volume}	B60R21/231	B60R21/231		150
B60R2021/23123	12	{Heat protection panels}	B60R21/231	B60R21/231		164
B60R2021/2313	12	{comprising sensitive compartments}	B60R21/231	B60R21/231		23
B60R21/23138	12	{specially adapted for side protection (B60R21/23184, B60R21/232 take precedence)}	B60R21/231	B60R21/231		2352
B60R2021/23146	13	{seat mounted}	B60R21/231	B60R21/231		1145
B60R2021/23153	12	{specially adapted for rear seat passengers}	B60R21/231	B60R21/231		564
B60R2021/23161	12	{specially adapted for protecting at least two passengers, e.g. preventing them from hitting each other}	B60R21/231	B60R21/231		579
B60R2021/23169	12	{specially adapted for knee protection}	B60R21/231	B60R21/231		723
B60R2021/23176	12	{specially adapted for foot protection}	B60R21/231	B60R21/231		96
B60R21/23184	12	{Tubular air bags connected to the vehicle at their two extremities}	B60R21/231	B60R21/231		141
B60R2021/23192	12	{Roof bags, i.e. protecting the occupant in a roll-over situation}	B60R21/231	B60R21/231		201
B60R21/232	12	Curtain-type airbags deploying mainly in a vertical direction from their top edge	B60R21/232	B60R21/232		2439
B60R21/233	12	comprising a plurality of individual compartments; comprising two or more bag-like members, one within the other (B60R21/232 takes precedence)	B60R21/233	B60R21/233		2500
B60R2021/23308	13	{the individual compartments defining the external shape of the bag}	B60R21/233	B60R21/233		605
B60R2021/23316	13	{Inner seams, e.g. creating separate compartments or used as tethering means}	B60R21/233	B60R21/233		574
B60R2021/23324	13	{Inner walls crating separate compartments, e.g. communicating with vents}	B60R21/233	B60R21/233		922
B60R2021/23332	14	{using independent bags, one within the other}	B60R21/233	B60R21/233		193
B60R21/2334	12	Expansion control features	B60R21/2334	B60R21/2334		616
B60R21/2338	13	Tethers	B60R21/2338	B60R21/2338		2907
B60R2021/23382	14	{Internal tether means}	B60R21/2338	B60R21/2338		1393
B60R2021/23384	15	{having ends which are movable or detachable during deployment}	B60R21/2338	B60R21/2338		365
B60R2021/23386	14	{External tether means}	B60R21/2338	B60R21/2338		1336
B60R2021/23388	15	{having ends which are movable or detachable during deployment}	B60R21/2338	B60R21/2338		278
B60R21/2342	13	Tear seams	B60R21/2342	B60R21/2342		546
B60R21/2346	13	Soft diffusers	B60R21/2346	B60R21/2346		673
B60R21/235	11	characterised by their material	B60R21/235	B60R21/235		1540
B60R2021/23504	12	{characterised by material}	B60R21/235	B60R21/235		119
B60R2021/23509	13	{Fabric}	B60R21/235	B60R21/235		530
B60R2021/23514	14	{coated fabric}	B60R21/235	B60R21/235		389
B60R2021/23519	13	{Resin}	B60R21/235	B60R21/235		151
B60R2021/23523	13	{Composite}	B60R21/235	B60R21/235		113
B60R2021/23528	13	{Metal}	B60R21/235	B60R21/235		66
B60R2021/23533	12	{characterised by the manufacturing process}	B60R21/235	B60R21/235		161
B60R2021/23538	13	{Sewing}	B60R21/235	B60R21/235		310
B60R2021/23542	13	{Weaving}	B60R21/235	B60R21/235		121
B60R2021/23547	14	{one piece weaving}	B60R21/235	B60R21/235		170
B60R2021/23552	13	{Knitting}	B60R21/235	B60R21/235		22
B60R2021/23557	13	{Molding}	B60R21/235	B60R21/235		43
B60R2021/23561	13	{Sealing}	B60R21/235	B60R21/235		22
B60R2021/23566	13	{Nesting of panels, i.e. for material utilisation}	B60R21/235	B60R21/235		32
B60R2021/23571	12	{characterised by connections between panels}	B60R21/235	B60R21/235		67
B60R2021/23576	13	{Sewing}	B60R21/235	B60R21/235		431
B60R2021/2358	13	{Bonding}	B60R21/235	B60R21/235		117
B60R2021/23585	13	{Vulcanisation}	B60R21/235	B60R21/235		6
B60R2021/2359	13	{Welding}	B60R21/235	B60R21/235		80
B60R2021/23595	13	{Sealing}	B60R21/235	B60R21/235		62
B60R21/237	11	characterised by the way they are folded	B60R21/237	B60R21/237		1777
B60R2021/2375	12	{Folding devices}	B60R21/237	B60R21/237		271
B60R21/239	11	characterised by their venting means	B60R21/239	B60R21/239		1689
B60R2021/2395	12	{comprising means to control the venting}	B60R21/239	B60R21/239		544
B60R21/26	10	characterised by the inflation fluid source or means to control inflation fluid flow {(arrangement or mounting thereof to the vehicle B60R21/20; blasting cartridges for producing gas under pressure in general F42B3/04; initiators or igniters therefor F42B3/10)}	B60R21/26	B60R21/26		2015
B60R21/26005	11	{the inflation fluid being transferred to the inflatable member by the mechanical deformation of the fluid container during an impact}	B60R21/26	B60R21/26		81
B60R2021/26011	11	{using a filter through which the inflation gas passes}	B60R21/26	B60R21/26		281
B60R2021/26017	11	{a cooling agent being added to the inflation fluid}	B60R21/26	B60R21/26		53
B60R2021/26023	11	{for filling the bag with foam}	B60R21/26	B60R21/26		24
B60R2021/26029	11	{Ignitors}	B60R21/26	B60R21/26		667
B60R2021/26035	12	{triggered by mechanical means}	B60R21/26	B60R21/26		48
B60R2021/26041	12	{of elongated shape}	B60R21/26	B60R21/26		44
B60R2021/26047	12	{of film shape}	B60R21/26	B60R21/26		15
B60R2021/26052	12	{using fluid materials}	B60R21/26	B60R21/26		10
B60R2021/26058	11	{using a combination of inflators}	B60R21/26	B60R21/26		209
B60R2021/26064	11	{characterised by auto-ignition means}	B60R21/26	B60R21/26		108
B60R2021/2607	11	{characterised by heating or heat insulating means, e.g. for use under extreme temperatures}	B60R21/26	B60R21/26		33
B60R2021/26076	11	{characterised by casing}	B60R21/26	B60R21/26		216
B60R2021/26082	12	{Material}	B60R21/26	B60R21/26		45
B60R2021/26088	13	{Plastic}	B60R21/26	B60R21/26		29
B60R2021/26094	11	{characterised by fluid flow controlling valves}	B60R21/26	B60R21/26		521
B60R21/261	11	with means other than bag structure to diffuse or guide inflation fluid	B60R21/261	B60R21/261		968
B60R2021/2612	12	{Gas guiding means, e.g. ducts}	B60R21/261	B60R21/261		537
B60R2021/2615	13	{for diverting the gas into a plurality of bags}	B60R21/261	B60R21/261		192
B60R2021/2617	13	{Curtain bag nozzles}	B60R21/261	B60R21/261		251
B60R21/262	12	Elongated tubular diffusers, e.g. curtain-type	B60R21/262	B60R21/262		141
B60R21/263	11	using a variable source, e.g. plural stage or controlled output (hybrid inflators B60R21/272)	B60R21/263	B60R21/263		198
B60R2021/2633	12	{with a plurality of inflation levels}	B60R21/263	B60R21/263		653
B60R2021/2636	13	{The volume of gas being continuously adjustable}	B60R21/263	B60R21/263		51
B60R21/264	11	using instantaneous generation of gas, e.g. pyrotechnic (B60R21/268 takes precedence)	B60R21/264	B60R21/264		1405
B60R2021/2642	12	{comprising a plurality of combustion chambers or sub-chambers}	B60R21/264	B60R21/264		160
B60R21/2644	12	{using only solid reacting substances, e.g. pellets, powder}	B60R21/264	B60R21/264		1639
B60R21/2646	13	{the reacting substances being supported by the inflatable member walls, or by a flexible support within it}	B60R21/264	B60R21/264		88
B60R2021/2648	13	{comprising a plurality of combustion chambers or sub-chambers}	B60R21/264	B60R21/264		506
B60R21/268	11	using instantaneous release of stored pressurised gas {(B60R21/26005 takes precedence)}	B60R21/268	B60R21/268		689
B60R2021/2685	12	{comprising a plurality of pressure chambers}	B60R21/268	B60R21/268		96
B60R21/272	12	with means for increasing the pressure of the gas just before or during liberation, e.g. hybrid inflators	B60R21/272	B60R21/272		764
B60R2021/2725	13	{using a fluid fuel gas generator}	B60R21/272	B60R21/272		69
B60R21/274	12	characterised by means to rupture or open the fluid source	B60R21/274	B60R21/274		271
B60R21/276	11	with means to vent the inflation fluid source, e.g. in case of overpressure {(B60R21/30 takes precedence; venting means on inflatable member walls B60R21/239)}	B60R21/276	B60R21/276		635
B60R2021/2765	12	{comprising means to control the venting}	B60R21/276	B60R21/276		339
B60R21/30	11	with means to draw ambient air into the flow line and mix such air with the inflation fluid	B60R21/30	B60R21/30		147
B60R21/33	10	Arrangements for non-electric triggering of inflation (electrical circuits for triggering safety arrangements B60R21/01)	B60R21/33	B60R21/33		365
B60R2021/335	11	{Connections between collision detecting means and inflators using pyrothechnic transmission lines}	B60R21/33	B60R21/33		24
B60R21/34	8	Protecting non-occupants of a vehicle, e.g. pedestrians {(B60R19/02 takes precedence)}	B60R21/34	B60R21/34		5262
B60R2021/343	9	{using deformable body panel, bodywork or components}	B60R21/34	B60R21/34		1754
B60R2021/346	9	{means outside vehicle body}	B60R21/34	B60R21/34		449
B60R21/36	9	using airbags	B60R21/36	B60R21/36		1109
B60R21/38	9	using means for lifting bonnets	B60R21/38	B60R21/38		1555
B60R22/00	7	Safety belts or body harnesses in vehicles (safety belts or body harnesses in general A62B35/00)	B60R22/00	B60R22/00		781
B60R22/001	8	{Knee, leg or head belts}	B60R22/00	B60R22/00		194
B60R2022/003	8	{for restraining detainees}	B60R22/00	B60R22/00		40
B60R2022/005	8	{for restraining luggages}	B60R22/00	B60R22/00		82
B60R2022/006	8	{Sleeve or tubular members enveloping the seat belt for enhancing comfort or protection}	B60R22/00	B60R22/00		89
B60R2022/008	8	{Belts; Fixing thereof specially adapted for pregnant users}	B60R22/00	B60R22/00		100
B60R22/02	8	Semi-passive restraint systems, e.g. systems applied or removed automatically but not both {; Manual restraint systems (knee, leg or head belts B60R22/001; devices for releasing in an emergency, remote or automatic unbuckling devices B60R22/32)}	B60R22/02	B60R22/02		699
B60R2022/021	9	{Means for holding the tongue or buckle in a non-use position, e.g. for easy access by the user}	B60R22/02	B60R22/02		358
B60R22/022	9	{with means for facilitating access to rear seats in two-door cars}	B60R22/02	B60R22/02		84
B60R22/023	9	{Three-point seat belt systems comprising two side lower and one side upper anchoring devices (B60R22/022, B60R22/03 take precedence)}	B60R22/02	B60R22/02		653
B60R22/024	10	{Adaptations for use by small passengers, e.g. children (B60R22/20 takes precedence; using belt anti-slip devices B60R22/30)}	B60R22/02	B60R22/02		293
B60R2022/025	10	{Adaptations for use with children seats or luggages}	B60R22/02	B60R22/02		45
B60R2022/026	10	{at least two ends of the belt being retractable after use}	B60R22/02	B60R22/02		117
B60R2022/027	9	{Four-point seat belt systems, e.g. with the two upper points connected together}	B60R22/02	B60R22/02		330
B60R2022/028	9	{specially adapted for use in sleeping position, e.g. for reclining seats}	B60R22/02	B60R22/02		51
B60R2022/029	9	{Belt storage; Devices or systems for controlling winding up of unused seat belt}	B60R22/02	B60R22/02		36
B60R22/03	9	Means for presenting the belt or part thereof to the wearer {, e.g. foot-operated}	B60R22/03	B60R22/03		522
B60R22/04	8	Passive restraint systems, i.e. systems both applied and removed automatically, e.g. by movement of the vehicle door	B60R22/04	B60R22/04		513
B60R22/06	9	having the belt or harness connected to a member slidable in a vehicle-mounted track	B60R22/06	B60R22/06		433
B60R22/08	9	having the belt retractor mounted on or in a vehicle closure, e.g. the door	B60R22/08	B60R22/08		53
B60R22/10	8	specially adapted for children or animals (children&apos;s seats B60N2/24)<br><br><u>NOTE</u><br><br> Groups B60R22/02B60R22/022 - B60R22/08, B60R22/18&#160;-&#160;B60R22/48 take precedence over group B60R22/10	B60R22/10	B60R22/10		328
B60R22/105	9	{for children (adaptation of children&apos;s seats for seat belts B60N2/265, B60N2/2803)}	B60R22/10	B60R22/10		1208
B60R22/12	8	Construction of belts or harnesses (B60R21/18 takes precedence {; woven fabrics for safety belts D03D1/0005})	B60R22/12	B60R22/12		1385
B60R22/14	9	incorporating enlarged restraint areas, e.g. vests, nets {, crash pads, optionally for children (crash pads for occupants&apos; safety on vehicles in general B60R21/02)}	B60R22/14	B60R22/14		701
B60R22/16	9	using belts which become permanently deformed, i.e. one time use	B60R22/16	B60R22/16		166
B60R22/18	8	Anchoring devices	B60R22/18	B60R22/18		2186
B60R2022/1806	9	{for buckles}	B60R22/18	B60R22/18		1375
B60R2022/1812	9	{Connections between seat belt and buckle tongue}	B60R22/18	B60R22/18		506
B60R2022/1818	9	{Belt guides}	B60R22/18	B60R22/18		1189
B60R2022/1825	10	{using rollers}	B60R22/18	B60R22/18		199
B60R2022/1831	10	{comprising a slotted plate sliding in its plane, e.g. inside circular guides}	B60R22/18	B60R22/18		123
B60R2022/1837	10	{comprising a universal mounting, e.g. spherical or cardan-type}	B60R22/18	B60R22/18		43
B60R2022/1843	10	{comprising an elongated sleeve}	B60R22/18	B60R22/18		88
B60R22/185	9	with stopping means for acting directly upon the belt in an emergency, e.g. by clamping or friction {(B60R22/195 takes precedence; combined with the retractor B60R22/42)}	B60R22/185	B60R22/185		231
B60R22/1855	10	{the means being sensitive to belt tension}	B60R22/185	B60R22/185		135
B60R22/19	9	with means for reducing belt tension during use under normal conditions {(included in the retractor B60R22/44)}	B60R22/19	B60R22/19		471
B60R22/195	9	with means to tension the belt in an emergency, {e.g. means of the through-anchor or splitted reel type}(electrical circuits for triggering safety arrangements {B60R21/01})<br><br><u>NOTE</u><br><br> If the type of belt tensioner is not specified and can be used indifferently for pulling belt anchors or rotating belt reels, the documents are classified in B60R22/46	B60R22/195	B60R22/195		343
B60R22/1951	10	{characterised by arrangements in vehicle or relative to seat belt}	B60R22/195	B60R22/195		349
B60R22/1952	10	{Transmission of tensioning power by cable; Return motion locking means therefor}	B60R22/195	B60R22/195		497
B60R22/1953	11	{the cable being pulled by mechanical means, e.g. pre-stressed springs, bumper displacement during crash}	B60R22/195	B60R22/195		105
B60R22/1954	10	{characterised by fluid actuators, e.g. pyrotechnic gas generators (actuating a cable B60R22/1952)}	B60R22/195	B60R22/195		155
B60R22/1955	11	{Linear actuators}	B60R22/195	B60R22/195		327
B60R22/1956	11	{Mechanical triggering means therefor (also adapted for air bag inflators B60R21/33)}	B60R22/195	B60R22/195		37
B60R2022/1957	10	{characterised by electric actuators}	B60R22/195	B60R22/195		93
B60R22/1958	10	{characterised by spring actuators (B60R22/1953 takes precedence)}	B60R22/195	B60R22/195		76
B60R22/20	9	adjustable in position, e.g. in height	B60R22/20	B60R22/20		1004
B60R22/201	10	{with the belt anchor connected to a slider movable in a vehicle-mounted track (for passive restraint systems B60R22/06)}	B60R22/20	B60R22/20		555
B60R22/202	11	{the slider comprising spring-actuated locking means (B60R22/205 takes precedence)}	B60R22/20	B60R22/20		134
B60R22/203	12	{the locking means being movably mounted on the slider}	B60R22/20	B60R22/20		246
B60R22/205	11	{the slider comprising emergency actuated locking means}	B60R22/20	B60R22/20		69
B60R22/206	10	{Adjustable stop members for restraint systems comprising belt anchor vehicle mounted tracks, e.g. for passive seat belts}	B60R22/20	B60R22/20		59
B60R2022/207	10	{Horizontally or transversally adjustable}	B60R22/20	B60R22/20		391
B60R2022/208	10	{by automatic or remote control means}	B60R22/20	B60R22/20		394
B60R22/22	9	secured to the vehicle floor	B60R22/22	B60R22/22		749
B60R22/24	9	secured to the side, door, or roof of the vehicle	B60R22/24	B60R22/24		1613
B60R22/26	9	secured to the seat	B60R22/26	B60R22/26		2809
B60R2022/263	10	{Front seats}	B60R22/26	B60R22/26		121
B60R2022/266	10	{Rear seats, e.g. benches}	B60R22/26	B60R22/26		246
B60R22/28	8	incorporating energy-absorbing devices {(belt anchors provided with energy-absorbing means for protecting the occupants in case of physical contact therewith B60R21/055; belt retractors comprising energy-absorbing means B60R22/341, B60R22/4676)}	B60R22/28	B60R22/28		1352
B60R2022/281	9	{for buckles}	B60R22/28	B60R22/28		137
B60R2022/282	9	{using fluids or vico-elastic materials}	B60R22/28	B60R22/28		177
B60R2022/283	9	{using tearing or scoring of material}	B60R22/28	B60R22/28		97
B60R2022/284	9	{using electric or magnetic braking means}	B60R22/28	B60R22/28		53
B60R2022/285	9	{using friction surfaces}	B60R22/28	B60R22/28		111
B60R2022/286	9	{using deformation of material}	B60R22/28	B60R22/28		370
B60R2022/287	10	{of torsion rods or tubes}	B60R22/28	B60R22/28		420
B60R2022/288	9	{with means to adjust or regulate the amount of energy to be absorbed}	B60R22/28	B60R22/28		412
B60R2022/289	9	{Energy-absorption curves}	B60R22/28	B60R22/28		75
B60R22/30	8	Coupling devices other than buckles, including length-adjusting fittings {or anti-slip devices (adaptations of manual three-point seat belt systems for use by small passengers using other means than belt anti-slip devices B60R22/024; buckles A44B11/00; releasable fastenings in general F16B)}	B60R22/30	B60R22/30		543
B60R22/32	8	Devices for releasing in an emergency, e.g. after an accident {; Remote or automatic unbuckling devices (unlocking devices for retractors B60R22/3416)}	B60R22/32	B60R22/32		441
B60R22/321	9	{using electric means}	B60R22/32	B60R22/32		231
B60R22/322	9	{using automatic actuating means (B60R22/321 takes precedence)}	B60R22/32	B60R22/32		178
B60R22/324	10	{triggered by strong traction on the seat belt, e.g. with temporisation}	B60R22/32	B60R22/32		191
B60R22/325	9	{using remote control means (B60R22/321, B60R22/322 take precedence)}	B60R22/32	B60R22/32		78
B60R2022/327	9	{using pyrotechnic means}	B60R22/32	B60R22/32		28
B60R2022/328	9	{comprising means for cutting the belt}	B60R22/32	B60R22/32		184
B60R22/34	8	Belt retractors, e.g. reels (anchoring devices {, e.g. guide loops} , with means to tension the belt in an emergency B60R22/195)	B60R22/34	B60R22/34		1607
B60R2022/3402	9	{Retractor casings; Mounting thereof}	B60R22/34	B60R22/34		461
B60R22/3405	9	{of the non-rotary type}	B60R22/34	B60R22/34		139
B60R22/3408	9	{without locking means (B60R22/3405 takes precedence)}	B60R22/34	B60R22/34		103
B60R22/341	9	{comprising energy-absorbing means}	B60R22/34	B60R22/34		227
B60R22/3413	10	{operating between belt reel and retractor frame (B60R22/4676 takes precedence)}	B60R22/34	B60R22/34		614
B60R22/3416	9	{Unlocking devices for retractors (B60R22/3405 takes precedence)}	B60R22/34	B60R22/34		95
B60R2022/3419	9	{with end lock preventing means}	B60R22/34	B60R22/34		81
B60R2022/3421	9	{with means for locking the belt reel in a non-use position, e.g. for seat mounted retractor when the seat is in a non-locked condition}	B60R22/34	B60R22/34		48
B60R2022/3424	9	{Multi-spool or multi-belt retractors}	B60R22/34	B60R22/34		152
B60R2022/3427	9	{Seat belt connection on reels}	B60R22/34	B60R22/34		194
B60R22/343	9	with electrically actuated locking means {(B60R22/3405 takes precedence)}	B60R22/343	B60R22/343		383
B60R22/347	9	with means for permanently locking the retractor during the wearing of the belt ({B60R22/3405} , B60R22/343, B60R22/415 take precedence)	B60R22/347	B60R22/347		128
B60R2022/3475	10	{having means for acting directly upon the belt, e.g. by clamping or friction}	B60R22/347	B60R22/347		48
B60R22/35	10	the locking means being automatically actuated	B60R22/35	B60R22/35		73
B60R22/353	11	in response to belt movement when a wearer applies the belt	B60R22/353	B60R22/353		94
B60R2022/3535	12	{comprising anti-cinch devices}	B60R22/353	B60R22/353		16
B60R22/357	11	in response to fastening of the belt buckle	B60R22/357	B60R22/357		79
B60R22/36	9	self-locking in an emergency ({B60R22/3405} , B60R22/343 take precedence)	B60R22/36	B60R22/36		409
B60R22/38	10	responsive only to belt movement	B60R22/38	B60R22/38		360
B60R2022/385	11	{with adjustable sensitivity}	B60R22/38	B60R22/38		36
B60R22/40	10	responsive only to vehicle movement	B60R22/40	B60R22/40		688
B60R2022/401	11	{with adjustable sensor}	B60R22/40	B60R22/40		104
B60R2022/402	12	{automatically adjustable to keep a vertical position, e.g. irrespective of seat or vehicle tilting}	B60R22/40	B60R22/40		80
B60R2022/403	13	{using externally controlled means, e.g. linked with seat back hinge}	B60R22/40	B60R22/40		39
B60R2022/404	11	{with remote sensor, e.g. for mounting on seat}	B60R22/40	B60R22/40		12
B60R22/405	10	responsive to belt movement and vehicle movement	B60R22/405	B60R22/405		564
B60R22/41	10	with additional means for preventing locking {during unwinding} under predetermined conditions	B60R22/41	B60R22/41		191
B60R22/415	10	with additional means allowing a permanent locking of the retractor during the wearing of the belt	B60R22/415	B60R22/415		198
B60R22/42	10	having means for acting directly upon the belt, e.g. by clamping or friction {(not combined with the retractor B60R22/185)}	B60R22/42	B60R22/42		279
B60R22/44	9	with means for reducing belt tension during use under normal conditions {(not included in the retractor B60R22/19; B60R22/3405 takes precedence)}	B60R22/44	B60R22/44		997
B60R2022/4406	10	{Spring shapes; Spring characteristic; Springs with adjustable anchoring means}	B60R22/44	B60R22/44		46
B60R2022/4413	10	{by connecting the retracting spring to the belt reel by means of a transmission which decreases the spring force when the belt is pulled out, e.g. using conical pulleys}	B60R22/44	B60R22/44		54
B60R2022/442	10	{using one spring and one additional retraction device in parallel}	B60R22/44	B60R22/44		3
B60R2022/4426	11	{the additional retraction device being a second spring}	B60R22/44	B60R22/44		30
B60R2022/4433	12	{externally controlled}	B60R22/44	B60R22/44		19
B60R2022/444	11	{the additional retraction device being an electric actuator}	B60R22/44	B60R22/44		84
B60R2022/4446	10	{using one spring and one additional retraction device in series}	B60R22/44	B60R22/44		3
B60R2022/4453	11	{the additional retraction device being a second spring}	B60R22/44	B60R22/44		52
B60R2022/446	12	{with external control means}	B60R22/44	B60R22/44		22
B60R2022/4466	11	{the additional retraction device being an electric actuator}	B60R22/44	B60R22/44		55
B60R2022/4473	10	{using an electric retraction device}	B60R22/44	B60R22/44		226
B60R2022/448	10	{using a fluid actuated retraction device}	B60R22/44	B60R22/44		12
B60R2022/4486	10	{for cancelling the belt tension}	B60R22/44	B60R22/44		62
B60R2022/4493	10	{for braking the belt reel using friction surfaces or the like}	B60R22/44	B60R22/44		39
B60R22/46	9	{Reels} with means to tension the belt in an emergency {by forced winding up}(electrical circuits for triggering safety arrangements B60R21/01{; tensioners using reels only guiding the belt during normal use, e.g. splitted reels B60R22/195})	B60R22/46	B60R22/46		1304
B60R22/4604	10	{characterised by arrangements in vehicle or relative to seat belt}	B60R22/46	B60R22/46		126
B60R2022/4609	11	{using a plurality of tensioners}	B60R22/46	B60R22/46		91
B60R2022/4614	11	{one pretensioner acting on a plurality of belts}	B60R22/46	B60R22/46		47
B60R22/4619	10	{Transmission of tensioning power by cable, e.g. using a clutch on reel side}	B60R22/46	B60R22/46		235
B60R22/4623	11	{the cable being pulled by mechanical means, e.g. pre-stressed springs, bumper displacement during crash}	B60R22/46	B60R22/46		47
B60R22/4628	10	{characterised by fluid actuators, e.g. pyrotechnic gas generators (actuating a cable B60R22/4619)}	B60R22/46	B60R22/46		701
B60R22/4633	11	{Linear actuators, e.g. comprising a piston moving along reel axis and rotating along its own axis}	B60R22/46	B60R22/46		337
B60R2022/4638	12	{comprising a piston moving along or in parallel to the reel axis}	B60R22/46	B60R22/46		56
B60R2022/4642	11	{the gas directly propelling a flexible driving means, e.g. a plurality of successive masses, in a tubular chamber}	B60R22/46	B60R22/46		281
B60R2022/4647	12	{the driving means being a belt, a chain or the like}	B60R22/46	B60R22/46		56
B60R22/4652	11	{Mechanical triggering means therefor (also adapted for air bag inflators B60R21/33)}	B60R22/46	B60R22/46		75
B60R2022/4657	11	{comprising a plurality of charges}	B60R22/46	B60R22/46		56
B60R2022/4661	11	{comprising venting means, e.g. for avoiding overpressure in case of fire or for allowing return motion with energy absorption}	B60R22/46	B60R22/46		108
B60R2022/4666	10	{characterised by electric actuators}	B60R22/46	B60R22/46		577
B60R22/4671	10	{characterised by spring actuators (B60R22/4623 takes precedence)}	B60R22/46	B60R22/46		82
B60R22/4676	10	{comprising energy-absorbing means operating between belt reel and retractor frame}	B60R22/46	B60R22/46		350
B60R2022/468	10	{characterised by clutching means between actuator and belt reel}	B60R22/46	B60R22/46		504
B60R2022/4685	10	{with means to adjust or regulate the tensioning force in relation to external parameters}	B60R22/46	B60R22/46		254
B60R2022/469	10	{reusable}	B60R22/46	B60R22/46		107
B60R2022/4695	10	{without winding function during normal use}	B60R22/46	B60R22/46		14
B60R22/48	8	Control systems, alarms, or interlock systems, for the correct application of the belt or harness	B60R22/48	B60R22/48		2944
B60R2022/4808	9	{Sensing means arrangements therefor}	B60R22/48	B60R22/48		549
B60R2022/4816	10	{for sensing locking of buckle}	B60R22/48	B60R22/48		1440
B60R2022/4825	10	{for sensing amount of belt winded on retractor}	B60R22/48	B60R22/48		301
B60R2022/4833	10	{for sensing locking of retractor}	B60R22/48	B60R22/48		30
B60R2022/4841	10	{for sensing belt tension}	B60R22/48	B60R22/48		236
B60R2022/485	10	{for sensing belt anchor position, belt orientation, or the like}	B60R22/48	B60R22/48		202
B60R2022/4858	10	{for sensing pressure on seat}	B60R22/48	B60R22/48		534
B60R2022/4866	9	{Displaying or indicating arrangements thereof}	B60R22/48	B60R22/48		810
B60R2022/4875	10	{on vehicle exterior}	B60R22/48	B60R22/48		56
B60R2022/4883	9	{Interlock systems}	B60R22/48	B60R22/48		81
B60R2022/4891	10	{preventing use of the vehicle when the seatbelt is not fastened}	B60R22/48	B60R22/48		317
B60R25/00	7	Fittings or systems for preventing or indicating unauthorised use or theft of vehicles (locks for vehicles E05B77/00-E05B85/00)	B60R25/00	B60R25/00		2361
B60R25/001	8	{Anti-theft devices acting on jacking means or props, e.g. for trailers}	B60R25/00	B60R25/00		168
B60R25/002	8	{Locking of control actuating or transmitting means (of steering mechanism B60R25/02)}	B60R25/00	B60R25/00		126
B60R25/003	9	{locking of control actuating means}	B60R25/00	B60R25/00		88
B60R25/005	10	{of foot actuated control means (rods connecting pedals and steering wheels B60R25/0221)}	B60R25/00	B60R25/00		520
B60R25/006	11	{using means preventing access, e.g. boxes, shutters}	B60R25/00	B60R25/00		63
B60R25/007	10	{of hand actuated control means}	B60R25/00	B60R25/00		693
B60R25/008	11	{comprising means for locking two or more control means together, e.g. hand-brake handle and gear shift lever}	B60R25/00	B60R25/00		83
B60R25/01	8	operating on vehicle systems or fittings, e.g. on doors, seats or windscreens	B60R25/01	B60R25/01		2024
B60R25/012	9	{Airbags triggered}	B60R25/01	B60R25/01		18
B60R25/014	9	{comprising means for locking the seat or parts thereof in a driving prevention position}	B60R25/01	B60R25/01		168
B60R25/016	9	{comprising means for shuttering the windscreen or part thereof}	B60R25/01	B60R25/01		98
B60R25/018	9	{Thief traps}	B60R25/01	B60R25/01		69
B60R25/02	9	operating on the steering mechanism	B60R25/02	B60R25/02		491
B60R25/021	10	restraining movement of the steering column or steering wheel hub, e.g. restraining means controlled by ignition switch	B60R25/021	B60R25/021		583
B60R25/02102	11	{with supplementary safety device preventing operation of the starter of an engine already running}	B60R25/021	B60R25/021		35
B60R25/02105	11	{Arrangement of the steering column thereof}	B60R25/021	B60R25/021		140
B60R25/02107	12	{comprising overload clutching means}	B60R25/021	B60R25/021		93
B60R25/0211	11	{comprising a locking member radially and linearly moved towards the steering column}	B60R25/021	B60R25/021		148
B60R25/02113	12	{manually actuated, e.g. using removable locking means}	B60R25/021	B60R25/021		241
B60R25/02115	12	{key actuated}	B60R25/021	B60R25/021		162
B60R25/02118	13	{with linear bolt motion parallel to the lock axis}	B60R25/021	B60R25/021		98
B60R25/02121	14	{comprising safety devices avoiding locking until removal of the key}	B60R25/021	B60R25/021		81
B60R25/02123	15	{using an axially slidable lock cylinder}	B60R25/021	B60R25/021		9
B60R25/02126	13	{with linear bolt motion perpendicular to the lock axis}	B60R25/021	B60R25/021		254
B60R25/02128	14	{comprising safety devices avoiding locking until removal of the key}	B60R25/021	B60R25/021		164
B60R25/02131	15	{by using an axially slidable lock cylinder}	B60R25/021	B60R25/021		95
B60R25/02134	11	{comprising a locking member axially moved along the steering column}	B60R25/021	B60R25/021		20
B60R25/02136	12	{manually actuated, e.g. using removable locking members}	B60R25/021	B60R25/021		84
B60R25/02139	12	{key actuated}	B60R25/021	B60R25/021		65
B60R25/02142	11	{comprising externally controlled safety devices for preventing locking during vehicle running condition}	B60R25/021	B60R25/021		227
B60R25/02144	12	{interlocked with gear box or gear lever}	B60R25/021	B60R25/021		138
B60R25/02147	11	{comprising a locking member having other than linear, axial or radial motion, e.g. rotatable; Steering column locking using balls, rollers or the like}	B60R25/021	B60R25/021		142
B60R25/0215	11	using electric means, e.g. electric motors or solenoids	B60R25/0215	B60R25/0215		197
B60R25/02153	12	{comprising a locking member radially and linearly moved towards the steering column}	B60R25/0215	B60R25/0215		389
B60R25/02156	12	{comprising a locking member axially moved along the steering column}	B60R25/0215	B60R25/0215		51
B60R25/022	10	operating on the steering wheel, e.g. bars locked to the steering wheel rim (B60R25/021 takes precedence)	B60R25/022	B60R25/022		120
B60R25/0221	11	{restraining means joining the steering wheel with another part of the car, e.g. pedals}	B60R25/022	B60R25/022		405
B60R25/0222	11	{by disjoining steering wheel and column}	B60R25/022	B60R25/022		403
B60R25/0224	11	{restraining of steering wheel by collapsing against column}	B60R25/022	B60R25/022		30
B60R25/0225	11	{using a rod locked on the steering wheel rim (B60R25/0221 takes precedence)}	B60R25/022	B60R25/022		452
B60R25/0227	11	{using means preventing access, e.g. boxes enclosing the steering wheel (B60R25/014 takes precedence)}	B60R25/022	B60R25/022		83
B60R25/0228	11	{comprising a locking bolt or fork slidable between or around the steering wheel spokes}	B60R25/022	B60R25/022		64
B60R25/023	10	Countermeasures against the physical destruction of the steering lock	B60R25/023	B60R25/023		126
B60R25/04	9	operating on the propulsion system, e.g. engine or drive motor	B60R25/04	B60R25/04		5449
B60R2025/0405	10	{from the external}	B60R25/04	B60R25/04		154
B60R2025/041	10	{Preventing use of engine operating on the fluid supply}	B60R25/04	B60R25/04		55
B60R2025/0415	10	{with safe immobilisation}	B60R25/04	B60R25/04		69
B60R25/042	10	operating on the fuel supply	B60R25/042	B60R25/042		920
B60R25/043	10	by blocking the exhaust	B60R25/043	B60R25/043		80
B60R25/044	10	by limiting or blocking the air supply	B60R25/044	B60R25/044		26
B60R25/045	10	by limiting or cutting the electrical supply to the propulsion unit	B60R25/045	B60R25/045		1003
B60R25/06	10	operating on the vehicle transmission	B60R25/06	B60R25/06		292
B60R25/063	11	{Locking of foot actuated control actuating means}	B60R25/06	B60R25/06		28
B60R25/066	11	{Locking of hand actuated control actuating means}	B60R25/06	B60R25/06		673
B60R25/08	9	operating on brakes or brake systems	B60R25/08	B60R25/08		590
B60R25/083	10	{Locking of foot-actuated control actuating means}	B60R25/08	B60R25/08		39
B60R25/086	10	{Locking of hand-actuated control actuating means}	B60R25/08	B60R25/08		218
B60R25/09	9	by restraining wheel rotation, e.g. wheel clamps	B60R25/09	B60R25/09		357
B60R25/093	10	{comprising ground-engaging means}	B60R25/09	B60R25/09		343
B60R25/096	10	{comprising means for deflating tyres}	B60R25/09	B60R25/09		45
B60R25/10	8	actuating a signalling device	B60R25/10	B60R25/10		2386
B60R25/1001	9	{Alarm systems associated with another car fitting or mechanism, e.g. door lock or knob, pedals (features related to the general power supply B60R25/1018)}	B60R25/10	B60R25/10		1064
B60R25/1003	9	{Alarm systems characterised by arm or disarm features}	B60R25/10	B60R25/10		909
B60R25/1004	9	{Alarm systems characterised by the type of sensor, e.g. current sensing means (using door lock sensors B60R25/1001)}	B60R25/10	B60R25/10		1647
B60R25/1006	10	{Mechanical sensors, e.g. pendulums (B60R25/101 takes precedence)}	B60R25/10	B60R25/10		219
B60R25/1007	11	{comprising associated circuitry}	B60R25/10	B60R25/10		98
B60R25/1009	10	{Sonic sensors; Signal treatment therefor}	B60R25/10	B60R25/10		234
B60R25/101	10	{Fuel level sensors}	B60R25/10	B60R25/10		58
B60R25/1012	10	{Zone surveillance means, e.g. parking lots, truck depots}	B60R25/10	B60R25/10		221
B60R2025/1013	9	{Alarm systems characterised by the type of warning signal, e.g. visual, audible}	B60R25/10	B60R25/10		743
B60R2025/1015	10	{Signal coming from the exhaust}	B60R25/10	B60R25/10		3
B60R2025/1016	10	{Remote signals alerting owner or authorities, e.g. radio signals}	B60R25/10	B60R25/10		378
B60R25/1018	9	{Alarm systems characterised by features related to the general power supply}	B60R25/10	B60R25/10		479
B60R25/102	9	a signal being sent to a remote location, e.g. a radio signal being transmitted to a police station, a security company or the owner	B60R25/102	B60R25/102		3786
B60R25/1025	10	{preventing jamming or interference of said signal}	B60R25/102	B60R25/102		73
B60R25/104	9	characterised by the type of theft warning signal, e.g. visual or audible signals with special characteristics	B60R25/104	B60R25/104		1282
B60R25/1045	10	{Signal comming from the exhaust}	B60R25/104	B60R25/104		22
B60R25/20	8	Means to switch the anti-theft system on or off	B60R25/20	B60R25/20		1973
B60R25/2009	9	{Antitheft state indicator}	B60R25/20	B60R25/20		291
B60R25/2018	9	{Central base unlocks or authorises unlocking}	B60R25/20	B60R25/20		612
B60R25/2027	9	{with data signals passing through the human body}	B60R25/20	B60R25/20		104
B60R25/2036	9	{by using the door logic and door and engine unlock means}	B60R25/20	B60R25/20		239
B60R25/2045	9	{by hand gestures}	B60R25/20	B60R25/20		264
B60R25/2054	9	{by foot gestures}	B60R25/20	B60R25/20		262
B60R25/2063	9	{Ignition switch geometry}	B60R25/20	B60R25/20		410
B60R25/2072	9	{with means for preventing jamming or interference of a remote switch control signal}	B60R25/20	B60R25/20		201
B60R25/2081	9	{combined with personal settings of other vehicle devices, e.g. mirrors, seats, steering wheels}	B60R25/20	B60R25/20		303
B60R25/209	9	{Remote starting of engine}	B60R25/20	B60R25/20		680
B60R25/21	9	using hidden switches	B60R25/21	B60R25/21		124
B60R25/22	9	using mechanical identifiers	B60R25/22	B60R25/22		86
B60R25/225	10	{key in lock presence switch}	B60R25/22	B60R25/22		86
B60R25/23	9	using manual input of alphanumerical codes	B60R25/23	B60R25/23		744
B60R25/24	9	using electronic identifiers containing a code not memorised by the user	B60R25/24	B60R25/24		5949
B60R25/241	10	{whereby access privileges are related to the identifiers}	B60R25/24	B60R25/24		795
B60R25/243	10	{with more than one way to gain access}	B60R25/24	B60R25/24		137
B60R25/245	10	{where the antenna reception area plays a role}	B60R25/24	B60R25/24		1639
B60R25/246	10	{characterised by the challenge triggering}	B60R25/24	B60R25/24		511
B60R25/248	10	{Electronic key extraction prevention}	B60R25/24	B60R25/24		336
B60R25/25	9	using biometry	B60R25/25	B60R25/25		1688
B60R25/252	10	{Fingerprint recognition}	B60R25/25	B60R25/25		1157
B60R25/255	10	{Eye recognition}	B60R25/25	B60R25/25		372
B60R25/257	10	{Voice recognition}	B60R25/25	B60R25/25		531
B60R25/30	8	Detection related to theft or to other events relevant to anti-theft systems	B60R25/30	B60R25/30		735
B60R25/302	9	{using recording means, e.g. black box}	B60R25/30	B60R25/30		355
B60R25/305	9	{using a camera}	B60R25/30	B60R25/30		1532
B60R25/307	9	{using data concerning maintenance or configuration}	B60R25/30	B60R25/30		90
B60R25/31	9	of human presence inside or outside the vehicle	B60R25/31	B60R25/31		942
B60R25/32	9	of vehicle dynamic parameters, e.g. speed or acceleration	B60R25/32	B60R25/32		263
B60R25/33	9	of global position, e.g. by providing GPS coordinates	B60R25/33	B60R25/33		1680
B60R25/34	9	of conditions of vehicle components, e.g. of windows, door locks or gear selectors	B60R25/34	B60R25/34		1097
B60R25/40	8	Features of the power supply for the anti-theft system, e.g. anti-theft batteries, back-up power supply or means to save battery power	B60R25/40	B60R25/40		244
B60R25/403	9	{Power supply in the vehicle}	B60R25/40	B60R25/40		381
B60R25/406	9	{Power supply in the remote key}	B60R25/40	B60R25/40		327
B60R99/00	7	Subject matter not provided for in other groups of this subclass	B60R99/00	B60R99/00		846
B60R2099/005	8	{Protections against martens or rodents}	B60R99/00	B60R99/00		88
B60R2225/00	7	Means indicating the functioning state of the alarm system, e.g. indicating arming, using leds	CPCONLY	B60R2225/00		123
B60R2300/00	7	Details of viewing arrangements using cameras and displays, specially adapted for use in a vehicle	CPCONLY	B60R2300/00		148
B60R2300/10	8	characterised by the type of camera system used	CPCONLY	B60R2300/10		550
B60R2300/101	9	using cameras with adjustable capturing direction	CPCONLY	B60R2300/101		684
B60R2300/102	9	using 360 degree surveillance camera system	CPCONLY	B60R2300/102		464
B60R2300/103	9	using camera systems provided with artificial illumination device, e.g. IR light source	CPCONLY	B60R2300/103		326
B60R2300/105	9	using multiple cameras	CPCONLY	B60R2300/105		3687
B60R2300/106	9	using night vision cameras	CPCONLY	B60R2300/106		421
B60R2300/107	9	using stereoscopic cameras	CPCONLY	B60R2300/107		303
B60R2300/108	9	using &apos;non-standard&apos; camera systems, e.g. camera sensor used for additional purposes i.a. rain sensor, camera sensor split in multiple image areas	CPCONLY	B60R2300/108		157
B60R2300/20	8	characterised by the type of display used	CPCONLY	B60R2300/20		865
B60R2300/202	9	displaying a blind spot scene on the vehicle part responsible for the blind spot	CPCONLY	B60R2300/202		591
B60R2300/205	9	using a head-up display	CPCONLY	B60R2300/205		1042
B60R2300/207	9	using multi-purpose displays, e.g. camera image and navigation or video on same display	CPCONLY	B60R2300/207		609
B60R2300/30	8	characterised by the type of image processing	CPCONLY	B60R2300/30		1300
B60R2300/301	9	combining image information with other obstacle sensor information, e.g. using RADAR/LIDAR/SONAR sensors for estimating risk of collision	CPCONLY	B60R2300/301		990
B60R2300/302	9	combining image information with GPS information or vehicle data, e.g. vehicle speed, gyro, steering angle data	CPCONLY	B60R2300/302		810
B60R2300/303	9	using joined images, e.g. multiple camera images	CPCONLY	B60R2300/303		1413
B60R2300/304	9	using merged images, e.g. merging camera image with stored images	CPCONLY	B60R2300/304		536
B60R2300/305	10	merging camera image with lines or icons	CPCONLY	B60R2300/305		608
B60R2300/306	9	using a re-scaling of images	CPCONLY	B60R2300/306		385
B60R2300/307	9	virtually distinguishing relevant parts of a scene from the background of the scene	CPCONLY	B60R2300/307		512
B60R2300/308	10	by overlaying the real scene, e.g. through a head-up display on the windscreen	CPCONLY	B60R2300/308		305
B60R2300/40	8	characterised by the details of the power supply or the coupling to vehicle components	CPCONLY	B60R2300/40		188
B60R2300/402	9	Image calibration	CPCONLY	B60R2300/402		305
B60R2300/404	9	triggering from stand-by mode to operation mode	CPCONLY	B60R2300/404		221
B60R2300/406	9	using wireless transmission	CPCONLY	B60R2300/406		277
B60R2300/408	9	using a data bus	CPCONLY	B60R2300/408		63
B60R2300/50	8	characterised by the display information being shared, e.g. external display, data transfer to other traffic participants or centralised traffic controller	CPCONLY	B60R2300/50		306
B60R2300/60	8	characterised by monitoring and displaying vehicle exterior scenes from a transformed perspective	CPCONLY	B60R2300/60		269
B60R2300/602	9	with an adjustable viewpoint	CPCONLY	B60R2300/602		211
B60R2300/605	10	the adjustment being automatic	CPCONLY	B60R2300/605		347
B60R2300/607	9	from a bird&apos;s eye viewpoint	CPCONLY	B60R2300/607		958
B60R2300/70	8	characterised by an event-triggered choice to display a specific image among a selection of captured images	CPCONLY	B60R2300/70		769
B60R2300/80	8	characterised by the intended use of the viewing arrangement	CPCONLY	B60R2300/80		577
B60R2300/8006	9	for monitoring and displaying scenes of vehicle interior, e.g. for monitoring passengers or cargo	CPCONLY	B60R2300/8006		553
B60R2300/8013	10	for child monitoring	CPCONLY	B60R2300/8013		91
B60R2300/802	9	for monitoring and displaying vehicle exterior blind spot views	CPCONLY	B60R2300/802		2093
B60R2300/8026	10	in addition to a rear-view mirror system	CPCONLY	B60R2300/8026		684
B60R2300/8033	9	for pedestrian protection	CPCONLY	B60R2300/8033		260
B60R2300/804	9	for lane monitoring	CPCONLY	B60R2300/804		771
B60R2300/8046	9	for replacing a rear-view mirror system	CPCONLY	B60R2300/8046		936
B60R2300/8053	9	for bad weather conditions or night vision	CPCONLY	B60R2300/8053		444
B60R2300/806	9	for aiding parking	CPCONLY	B60R2300/806		1274
B60R2300/8066	9	for monitoring rearward traffic	CPCONLY	B60R2300/8066		1286
B60R2300/8073	9	for vehicle security, e.g. parked vehicle surveillance, burglar detection	CPCONLY	B60R2300/8073		385
B60R2300/808	9	for facilitating docking to a trailer	CPCONLY	B60R2300/808		227
B60R2300/8086	9	for vehicle path indication	CPCONLY	B60R2300/8086		329
B60R2300/8093	9	for obstacle warning	CPCONLY	B60R2300/8093		1288
B60R2325/00	7	Indexing scheme relating to vehicle anti-theft devices	CPCONLY	B60R2325/00		3
B60R2325/10	8	Communication protocols, communication systems of vehicle anti-theft devices	CPCONLY	B60R2325/10		281
B60R2325/101	9	Bluetooth&#174;	CPCONLY	B60R2325/101		1029
B60R2325/103	9	Near field communication [NFC]	CPCONLY	B60R2325/103		379
B60R2325/105	9	Radio frequency identification data [RFID]	CPCONLY	B60R2325/105		373
B60R2325/106	9	Internet	CPCONLY	B60R2325/106		119
B60R2325/108	9	Encryption	CPCONLY	B60R2325/108		275
B60R2325/20	8	Communication devices for vehicle anti-theft devices	CPCONLY	B60R2325/20		194
B60R2325/202	9	Personal digital assistant [PDA]	CPCONLY	B60R2325/202		209
B60R2325/205	9	Mobile phones	CPCONLY	B60R2325/205		1946
B60R2325/207	9	Satellites	CPCONLY	B60R2325/207		80
B60R2325/30	8	Vehicles applying the vehicle anti-theft devices	CPCONLY	B60R2325/30		470
B60R2325/302	9	Airplanes	CPCONLY	B60R2325/302		27
B60R2325/304	9	Boats	CPCONLY	B60R2325/304		296
B60R2325/306	9	Motorcycles	CPCONLY	B60R2325/306		432
B60R2325/308	9	Industrial vehicles	CPCONLY	B60R2325/308		68
B60R2325/40	8	Programmable elements	CPCONLY	B60R2325/40		29
