B67B1/00	7	Closing bottles, jars or similar containers by applying stoppers (stoppers per seB65D39/00)	B67B1/00	B67B1/00		205
B67B1/005	8	{Feeding stoppers (in general B65G)}	B67B1/00	B67B1/00		319
B67B1/03	8	Pretreatment of stoppers, e.g. cleaning, steaming, heating, impregnating or coating; Applying resilient rings to stoppers (mechanical working of cork B27J5/00)	B67B1/03	B67B1/03		208
B67B1/04	8	by inserting threadless stoppers, e.g. corks	B67B1/04	B67B1/04		572
B67B1/045	9	{using hand operated devices}	B67B1/04	B67B1/04		179
B67B1/06	8	by inserting and rotating screw stoppers	B67B1/06	B67B1/06		48
B67B1/08	8	Securing stoppers, e.g. swing stoppers, which are held in position by associated pressure-applying means coacting with the bottle neck	B67B1/08	B67B1/08		163
B67B1/10	8	by inserting disc closures	B67B1/10	B67B1/10		184
B67B3/00	7	Closing bottles, jars or similar containers by applying caps (caps per seB65D41/00)	B67B3/00	B67B3/00		770
B67B3/003	8	{Pretreatment of caps, e.g. cleaning, steaming, heating or sterilizing}	B67B3/00	B67B3/00		240
B67B3/006	8	{Applying date marks, code marks, or the like, to caps during capping (applying marks to labels B65C9/46)}	B67B3/00	B67B3/00		26
B67B3/02	8	by applying flanged caps, e.g. crown caps, and securing by deformation of flanges	B67B3/02	B67B3/02		784
B67B3/023	9	{using additional means for securing the cap, e.g. adhesives}	B67B3/02	B67B3/02		65
B67B3/026	9	{the caps being made of thermoplastic material (B67B3/023 takes precedence)}	B67B3/02	B67B3/02		57
B67B3/04	9	Cutting caps from strip material in capping machines (devices for registering moving strip material B65H23/00)	B67B3/04	B67B3/04		63
B67B3/06	9	Feeding caps to capping heads	B67B3/06	B67B3/06		483
B67B3/061	10	{the caps having an asymmetric footprint, e.g. comprising a gripping lip}	B67B3/06	B67B3/06		53
B67B3/062	10	from a magazine {(B67B3/061 takes precedence)}	B67B3/062	B67B3/062		310
B67B3/064	10	from a hopper {(B67B3/061 takes precedence)}	B67B3/064	B67B3/064		380
B67B3/0645	11	{with means for orientating the caps to a position ready to be applied to the container}	B67B3/064	B67B3/064		262
B67B3/10	9	Capping heads for securing caps {(B67B3/023 takes precedence)}	B67B3/10	B67B3/10		714
B67B3/12	10	characterised by being movable axially relative to cap to deform flanges thereof, e.g. to press projecting flange rims inwardly	B67B3/12	B67B3/12		325
B67B3/14	10	characterised by having movable elements, e.g. hinged fingers, for applying radial pressure to the flange of the cap (B67B3/16, B67B3/18 take precedence)	B67B3/14	B67B3/14		538
B67B3/16	10	characterised by having resilient deforming elements, e.g. resilient sleeves or collars (B67B3/18 takes precedence)	B67B3/16	B67B3/16		92
B67B3/18	10	characterised by being rotatable, e.g. for forming screw threads in situ	B67B3/18	B67B3/18		347
B67B3/20	8	by applying and rotating preformed threaded caps (forming threads in situ by resilient deforming means B67B3/16, by rotary capping heads B67B3/18)	B67B3/20	B67B3/20		1030
B67B3/2006	9	{using manually-controlled or manually operated devices}	B67B3/20	B67B3/20		90
B67B3/2013	9	{by carousel-type capping machines}	B67B3/20	B67B3/20		155
B67B3/202	10	{using friction means for screwing the caps, e.g. belts or guides (B67B3/2026, B67B3/2033 take precedence)}	B67B3/20	B67B3/20		41
B67B3/2026	10	{comprising stationary capping heads}	B67B3/20	B67B3/20		70
B67B3/2033	10	{comprising carousel co-rotating capping heads}	B67B3/20	B67B3/20		296
B67B3/204	9	{Linear-type capping machines}	B67B3/20	B67B3/20		72
B67B3/2046	10	{using friction means for screwing the caps, e.g. belts or wheels (B67B3/2053 takes precedence)}	B67B3/20	B67B3/20		192
B67B3/2053	10	{comprising capping heads}	B67B3/20	B67B3/20		232
B67B3/206	9	{Means for preventing rotation of the container or cap}	B67B3/20	B67B3/20		241
B67B3/2066	9	{Details of capping heads (B67B3/2073 takes precedence)}	B67B3/20	B67B3/20		447
B67B3/2073	9	{comprising torque limiting means (torque limiters in wrenches or screwdrivers B25B23/14; couplings or clutches per seF16D)}	B67B3/20	B67B3/20		229
B67B3/208	10	{Electrical means responsive to the torque applied and acting on motor control means, e.g. strain gauges or power measurement means (B67B3/2093 takes precedence)}	B67B3/20	B67B3/20		49
B67B3/2086	10	{Magnetic or electromagnetic clutches}	B67B3/20	B67B3/20		58
B67B3/2093	10	{whereby the applied torque limit is varied}	B67B3/20	B67B3/20		20
B67B3/22	8	by applying snap-on caps	B67B3/22	B67B3/22		173
B67B3/24	8	Special measures for applying and securing caps under vacuum	B67B3/24	B67B3/24		398
B67B3/26	8	Applications of control, warning, or safety devices in capping machinery	B67B3/26	B67B3/26		393
B67B3/261	9	{Devices for controlling the tightening of threaded caps, e.g. testing the release torque (torque testers in general G01L5/00)}	B67B3/26	B67B3/26		113
B67B3/262	9	{Devices for controlling the caps}	B67B3/26	B67B3/26		78
B67B3/264	10	{positioning of the caps}	B67B3/26	B67B3/26		114
B67B3/265	10	{presence of a cap}	B67B3/26	B67B3/26		29
B67B3/267	10	{positioning of the cap-label}	B67B3/26	B67B3/26		1
B67B3/268	9	{devices for avoiding damage to the closing machine}	B67B3/26	B67B3/26		52
B67B3/28	8	Mechanisms for causing relative movement between bottle or jar and capping head	B67B3/28	B67B3/28		197
B67B5/00	7	Applying protective or decorative covers to closures; Devices for securing bottle closures with wire (infant feeding teats with means for fastening to bottles A61J11/04)	B67B5/00	B67B5/00		262
B67B5/03	8	Applying protective or decorative covers to closures, e.g. by forming in situ	B67B5/03	B67B5/03		249
B67B5/032	9	{Dies for securing overcaps}	B67B5/03	B67B5/03		92
B67B5/034	9	{the covers being elastic}	B67B5/03	B67B5/03		12
B67B5/036	9	{the covers being heat-shrinkable}	B67B5/03	B67B5/03		134
B67B5/038	9	{the covers being applied wet, whereby shrinkage occurs on drying}	B67B5/03	B67B5/03		17
B67B5/05	9	by applying liquids, e.g. by dipping	B67B5/05	B67B5/05		101
B67B5/06	8	Devices for securing bottle closures with wire (B67B1/08 takes precedence)	B67B5/06	B67B5/06		202
B67B6/00	7	Closing bottles, jars or similar containers by applying closure members, not provided for in groups B67B1/00 - B67B5/00	B67B6/00	B67B6/00		177
B67B7/00	7	Hand- or power-operated devices for opening closed containers (nail pullers or extractors B25C11/00; attached to, or incorporated in, containers or container closures {B65D75/58, B65D77/30})	B67B7/00	B67B7/00		611
B67B7/02	8	for removing stoppers	B67B7/02	B67B7/02		203
B67B7/04	9	Cork-screws	B67B7/04	B67B7/04		230
B67B7/0405	10	{Power-operated cork-screws, e.g. operated by an electric motor}	B67B7/04	B67B7/04		143
B67B7/0411	10	{without supporting means for assisting the pulling action}	B67B7/04	B67B7/04		182
B67B7/0417	10	{with supporting means for assisting the pulling action}	B67B7/04	B67B7/04		34
B67B7/0423	11	{of wine-waiter, i.e. sommelier type}	B67B7/04	B67B7/04		134
B67B7/0429	12	{having means for varying the effective lever arm length}	B67B7/04	B67B7/04		81
B67B7/0435	11	{with a pantograph extracting mechanism}	B67B7/04	B67B7/04		26
B67B7/0441	11	{whereby the supporting means abut around the whole periphery of the neck of the bottle}	B67B7/04	B67B7/04		316
B67B7/0447	11	{whereby the supporting means abut around parts of the periphery of the neck of the bottle}	B67B7/04	B67B7/04		70
B67B7/0452	10	{adapted to be mounted on walls}	B67B7/04	B67B7/04		23
B67B2007/0458	10	{Means for cutting sealing capsules}	B67B7/04	B67B7/04		190
B67B2007/0464	10	{Means for counting}	B67B7/04	B67B7/04		
B67B2007/047	10	{Means for reducing friction}	B67B7/04	B67B7/04		1
B67B2007/0476	11	{by coating the screw}	B67B7/04	B67B7/04		5
B67B2007/0482	11	{by using roller-bearings}	B67B7/04	B67B7/04		2
B67B2007/0488	10	{Means for measuring temperature}	B67B7/04	B67B7/04		14
B67B2007/0494	10	{Means for varying the lever arm}	B67B7/04	B67B7/04		9
B67B7/06	9	Other cork removers	B67B7/06	B67B7/06		171
B67B7/063	10	{using one or more blades to be inserted between the cork and the inner surface of the bottle neck}	B67B7/06	B67B7/06		86
B67B7/066	10	{specially adapted for opening pressurised bottles, e.g. champagne or sparkling wine bottles}	B67B7/06	B67B7/06		140
B67B7/08	10	using air or gas pressure	B67B7/08	B67B7/08		120
B67B7/10	9	with means for retrieving stoppers from the interior of the container	B67B7/10	B67B7/10		73
B67B7/12	8	for removing disc-closures	B67B7/12	B67B7/12		242
B67B7/14	8	for removing tightly-fitting lids or covers, e.g. of shoe-polish tins, by gripping and rotating	B67B7/14	B67B7/14		775
B67B7/15	9	finger grapple type	B67B7/15	B67B7/15		56
B67B7/16	8	for removing flanged caps, e.g. crown caps	B67B7/16	B67B7/16		1931
B67B7/162	9	{the removing device being formed by at least two articulated parts, e.g. pliers (B67B7/164 takes precedence)}	B67B7/16	B67B7/16		164
B67B7/164	9	{Power-operated devices}	B67B7/16	B67B7/16		141
B67B2007/166	9	{Means for attaching the opener to fingers}	B67B7/16	B67B7/16		49
B67B2007/168	9	{Means for counting}	B67B7/16	B67B7/16		14
B67B7/18	8	for removing threaded caps (B67B7/14 takes precedence; wrenches B25B13/00)	B67B7/18	B67B7/18		1376
B67B7/182	9	{power-operated}	B67B7/18	B67B7/18		368
B67B7/184	9	{by use of a flexible loop gripping the cap skirt or the container body by friction}	B67B7/18	B67B7/18		89
B67B7/186	10	{the loop having an adjustable length}	B67B7/18	B67B7/18		198
B67B2007/188	9	{Means for attaching the opener to fingers}	B67B7/18	B67B7/18		7
B67B7/20	8	for breaking vacuum seals between lids or covers and bodies of preserving jars, e.g. by wedge action	B67B7/20	B67B7/20		218
B67B7/22	9	incorporating loops, e.g. of wire, which are tightened around seal	B67B7/22	B67B7/22		19
B67B7/24	8	{Hole-piercing devices}	B67B7/00	B67B7/24		954
B67B7/26	9	{combined with spouts}	B67B7/00	B67B7/26		898
B67B7/28	10	{and associated with receptacle hodlers}	B67B7/86	B67B7/28		694
B67B7/30	8	{Hand-operated cutting devices}	B67B7/46	B67B7/30		1470
B67B2007/303	9	{can openers}	B67B7/46	B67B7/30		68
B67B2007/306	10	{Means for counting}	B67B7/46	B67B7/30		
B67B7/32	9	{propelled by rotary gears or wheels around periphery of container}	B67B7/70	B67B7/32		351
B67B7/34	9	{with rotatable cutters}	B67B7/46	B67B7/34		712
B67B7/36	9	{adapted to be mounted on walls}	B67B7/46	B67B7/36		233
B67B7/38	8	{Power-operated cutting devices (machines for domestic use with a plurality of interchangeable units A47J43/06, A47J44/00)}	B67B7/00	B67B7/38		595
B67B7/385	9	{specially adapted to be hand-held}	B67B7/00	B67B7/38		88
B67B7/40	8	Devices for engaging tags, strips, or tongues for opening by tearing, e.g. slotted keys for opening sardine tins	B67B7/40	B67B7/40		320
B67B7/403	9	{adapted for engaging the ring of a pull tab for opening an aperture}	B67B7/40	B67B7/40		310
B67B7/406	10	{and subsequently tearing off the top of the can}	B67B7/40	B67B7/40		97
B67B7/42	8	Devices for removing barrel bungs	B67B7/42	B67B7/42		94
B67B7/44	8	Combination tools, e.g. comprising cork-screws, can piercers, crowncap removers (combinations of opening devices with cutting tools B26; with devices serving other purposes, see appropriate subclasses, e.g. B25F; B43K29/00)	B67B7/44	B67B7/44		1302
B67B7/92	8	by breaking, e.g. for ampoules	B67B7/92	B67B7/92		910
B67B2201/00	7	Indexing codes relating to constructional features of closing machines	CPCONLY	B67B2201/00		6
B67B2201/01	8	Orienting closure means	CPCONLY	B67B2201/01		5
B67B2201/012	9	Stoppers	CPCONLY	B67B2201/012		7
B67B2201/015	10	Cylindrical stoppers	CPCONLY	B67B2201/015		18
B67B2201/017	9	Caps	CPCONLY	B67B2201/017		28
B67B2201/03	8	applying two closures on a container	CPCONLY	B67B2201/03		10
B67B2201/06	8	Details of cap feeding devices	CPCONLY	B67B2201/06		86
B67B2201/065	9	Use of magnets	CPCONLY	B67B2201/065		22
B67B2201/08	8	Aseptic features	CPCONLY	B67B2201/08		87
B67B2201/10	8	Quick or easy connection means for connecting a capping head to a spindle	CPCONLY	B67B2201/10		46
B67B2201/12	8	Details related to spray caps, i.e. caps comprising a pump and a tube for dispensing content from a container	CPCONLY	B67B2201/12		27
