B05B1/00	7	Nozzles, spray heads or other outlets, with or without auxiliary devices such as valves, heating means (B05B3/00, B05B5/00, B05B7/00 take precedence; devices for applying liquids or other fluent materials to surfaces by contact B05C; nozzles for ink-jet printing mechanisms B41J2/135; nozzles for liquid-dispensing, e.g. in vehicle service stations, B67D7/42)	B05B1/00	B05B1/00		1419
B05B1/002	8	{designed to reduce the generation or the transmission of noise or to produce a particular sound; associated with noise monitoring means}	B05B1/00	B05B1/00		220
B05B1/005	8	{Nozzles or other outlets specially adapted for discharging one or more gases}	B05B1/00	B05B1/00		1806
B05B1/02	8	designed to produce a jet, spray, or other discharge of particular shape or nature, e.g. in single drops, {or having an outlet of particular shape}(B05B1/26, B05B1/28, B05B1/34 take precedence)	B05B1/02	B05B1/02		2345
B05B1/04	9	in flat form, e.g. fan-like, sheet-like	B05B1/04	B05B1/04		725
B05B1/042	10	{Outlets having two planes of symmetry perpendicular to each other, one of them defining the plane of the jet (B05B1/044, B05B1/046 take precedence)}	B05B1/04	B05B1/04		512
B05B1/044	10	{Slits, e.g. narrow openings defined by two straight and parallel lips; Elongated outlets for producing very wide discharges, e.g. fluid curtains (B05B1/046 takes precedence)}	B05B1/04	B05B1/04		864
B05B1/046	10	{Outlets formed, e.g. cut, in the circumference of tubular or spherical elements}	B05B1/04	B05B1/04		251
B05B1/048	10	{having a flow conduit with, immediately behind the outlet orifice, an elongated cross section, e.g. of oval or elliptic form, of which the major axis is perpendicular to the plane of the jet}	B05B1/04	B05B1/04		114
B05B1/06	9	in annular, tubular or hollow conical form	B05B1/06	B05B1/06		861
B05B1/08	9	of pulsating nature, e.g. delivering liquid in successive separate quantities	B05B1/08	B05B1/08		629
B05B1/083	10	{the pulsating mechanism comprising movable parts}	B05B1/08	B05B1/08		511
B05B1/085	11	{rotated by the liquid or other fluent material discharged, e.g. liquid rotated turbines}<br><br><u>WARNING</u><br>Group B05B1/085 is incomplete pending reclassification of documents from group B05B3/04. <br>Groups B05B3/04 and B05B1/085 should be considered in order to perform a complete search.	B05B1/08	B05B1/08		5
B05B1/0852	12	{the liquid or other fluent material actuating several pulsating mechanisms}<br><br><u>WARNING</u><br>Group B05B1/0852 is incomplete pending reclassification of documents from group B05B3/0495. <br>Groups B05B3/0495 and B05B1/0852 should be considered in order to perform a complete search.	B05B1/08	B05B1/08		1
B05B1/0854	12	{the pulsating mechanism being provided with means for preventing rotation}<br><br><u>WARNING</u><br>Group B05B1/0854 is incomplete pending reclassification of documents from group B05B3/049. <br>Groups B05B3/049 and B05B1/0854 should be considered in order to perform a complete search.	B05B1/08	B05B1/08		1
B05B1/0856	12	{the pulsating mechanism comprising movable balls}	B05B1/08	B05B1/08		73
B05B1/086	11	{with a resiliently deformable element, e.g. sleeve}	B05B1/08	B05B1/08		106
B05B1/10	9	in the form of a fine jet, e.g. for use in wind-screen washers	B05B1/10	B05B1/10		740
B05B1/12	8	capable of producing different kinds of discharge, e.g. either jet or spray (having selectively-effective outlets B05B1/16)	B05B1/12	B05B1/12		1421
B05B1/14	8	with multiple outlet openings (B05B1/02, B05B1/26 take precedence); with strainers in or outside the outlet opening<br><br><u>WARNING</u><br>Group B05B1/14 is impacted by reclassification into groups B05B1/1421, B05B1/1422, B05B1/1423, B05B1/1424, B05B1/1425 and B05B13/002. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/14	B05B1/14		4800
B05B1/1421	9	{the multiple outlet openings arranged in plural groups or rows (for roses or shower heads B05B1/1821)}<br><br><u>WARNING</u><br>Groups B05B1/1421, B05B1/1422, B05B1/1423, B05B1/1424 and B05B1/1425 are incomplete pending reclassification of documents from group B05B1/14. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/14	B05B1/14		5
B05B1/1422	10	{with all groups or rows being identical}	B05B1/14	B05B1/14		5
B05B1/1423	10	{comprising concentric or coaxial groups}	B05B1/14	B05B1/14		6
B05B1/1424	11	{the outlet openings traversing a concavo-convex wall}	B05B1/14	B05B1/14		2
B05B1/1425	10	{having three or more dissimilar groups or rows}	B05B1/14	B05B1/14		1
B05B1/16	9	having selectively- effective outlets	B05B1/16	B05B1/16		957
B05B1/1609	10	{with a selecting mechanism comprising a lift valve (B05B1/1681 takes precedence)}	B05B1/16	B05B1/16		378
B05B1/1618	11	{where said valve is a double-seat lift valve}	B05B1/16	B05B1/16		213
B05B1/1627	10	{with a selecting mechanism comprising a gate valve, a sliding valve or a cock (B05B1/1681 takes precedence)}	B05B1/16	B05B1/16		171
B05B1/1636	11	{by relative rotative movement of the valve elements (B05B1/1672 takes precedence)}	B05B1/16	B05B1/16		723
B05B1/1645	12	{the outlets being rotated during selection}	B05B1/16	B05B1/16		340
B05B1/1654	13	{about an axis parallel to the liquid passage in the stationary valve element}	B05B1/16	B05B1/16		524
B05B1/1663	11	{by relative translatory movement of the valve elements (B05B1/1672 takes precedence)}	B05B1/16	B05B1/16		230
B05B1/1672	11	{the selectively-effective outlets being arranged on a tube or pipe}	B05B1/16	B05B1/16		168
B05B1/1681	10	{with a selecting mechanism comprising a gate valve, sliding valve or cock and a lift valve}	B05B1/16	B05B1/16		149
B05B1/169	10	{having three or more selectively effective outlets}	B05B1/16	B05B1/16		413
B05B1/18	9	Roses; Shower heads<br><br><u>WARNING</u><br>Group B05B1/18 is impacted by reclassification into groups B05B1/188, B05B1/1881, B05B1/1882, B05B1/1884, B05B1/1886, B05B1/1887, B05B1/189, B05B1/1892, B05B1/1894, B05B1/1896 and B05B1/192. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/18	B05B1/18		5488
B05B1/182	10	{characterised by their outlet openings or elements; Mounting arrangements therefor}<br><br><u>WARNING</u><br>Groups B05B1/182, B05B1/1821, B05B1/1822, B05B1/1823, B05B1/1824 and B05B1/1825 are incomplete pending reclassification of documents from group B05B1/185. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/18	B05B1/18		17
B05B1/1821	11	{the outlet openings arranged in plural groups or rows}	B05B1/18	B05B1/18		2
B05B1/1822	12	{with all groups or rows being identical}	B05B1/18	B05B1/18		7
B05B1/1823	12	{Concentric or coaxial groups}	B05B1/18	B05B1/18		11
B05B1/1824	13	{the outlet openings traversing a concavo-convex outlet wall}	B05B1/18	B05B1/18		4
B05B1/1825	12	{with three or more dissimilar groups or rows}	B05B1/18	B05B1/18		1
B05B1/185	10	{characterised by their outlet element; Mounting arrangements therefor}<br><br><u>WARNING</u><br>Group B05B1/185 is no longer used for the classification of documents as of 2025-08-01. The content of this group is being reclassified into groups B05B1/182, B05B1/1821, B05B1/1822, B05B1/1823, B05B1/1824 and B05B1/1825.<br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/18	B05B1/18		1681
B05B1/188	10	{with user-actuated controlling members}<br><br><u>WARNING</u><br>Groups B05B1/188, B05B1/1881, B05B1/1882, B05B1/1884, B05B1/1886, B05B1/1887, B05B1/189, B05B1/1892, B05B1/1894 and B05B1/1896 are incomplete pending reclassification of documents from group B05B1/18. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B1/18	B05B1/18		3
B05B1/1881	11	{associated with position or movement indicating means}	B05B1/18	B05B1/18		1
B05B1/1882	11	{actuated by a linear movement, e.g. push buttons}	B05B1/18	B05B1/18		5
B05B1/1884	12	{actuated by a sliding movement along an outer surface of the roses or of the shower heads}	B05B1/18	B05B1/18		5
B05B1/1886	12	{the linear movement of the controlling member being converted into a rotational movement of the controlled element}	B05B1/18	B05B1/18		4
B05B1/1887	11	{actuated by a pivoting movement}	B05B1/18	B05B1/18		3
B05B1/189	11	{actuated by a rotating movement}	B05B1/18	B05B1/18		9
B05B1/1892	11	{located in or on the handle}	B05B1/18	B05B1/18		7
B05B1/1894	11	{located in or on the outlet wall}	B05B1/18	B05B1/18		5
B05B1/1896	11	{located in or on the housing}	B05B1/18	B05B1/18		4
B05B1/192	10	{combined with features functioning other than as a support or as a portion of the fluid handling elements, e.g. audio systems, speakers or lights}<br><br><u>WARNING</u><br>Group B05B1/192 is incomplete pending reclassification of documents from group B05B1/18. <br>Groups B05B1/18 and B05B1/192 should be considered in order to perform a complete search.	B05B1/18	B05B1/192		3
B05B1/20	9	Perforated pipes or troughs, e.g. spray booms; Outlet elements therefor	B05B1/20	B05B1/20		2066
B05B1/202	10	{comprising inserted outlet elements}	B05B1/20	B05B1/20		415
B05B1/205	10	{characterised by the longitudinal shape of the elongated body}	B05B1/20	B05B1/20		334
B05B1/207	11	{the elongated body being a closed loop}	B05B1/20	B05B1/20		221
B05B1/22	8	Spouts (anti-splash devices for water-taps E03C1/08)	B05B1/22	B05B1/22		445
B05B1/24	8	incorporating means for heating the liquid or other fluent material, e.g. electrically	B05B1/24	B05B1/24		583
B05B1/26	8	with means for mechanically breaking-up or deflecting the jet after discharge, e.g. with fixed deflectors; Breaking-up the discharged liquid or other fluent material by impinging jets	B05B1/26	B05B1/26		1111
B05B1/262	9	{with fixed deflectors}	B05B1/26	B05B1/26		583
B05B1/265	10	{the liquid or other fluent material being symmetrically deflected about the axis of the nozzle}	B05B1/26	B05B1/26		1375
B05B1/267	10	{the liquid or other fluent material being deflected in determined directions}	B05B1/26	B05B1/26		953
B05B1/28	8	with integral means for shielding the discharged liquid or other fluent material, e.g. to limit area of spray; with integral means for catching drips or collecting surplus liquid or other fluent material	B05B1/28	B05B1/28		1048
B05B1/30	8	designed to control volume of flow, e.g. with adjustable passages {(B05B11/0094 takes precedence)}	B05B1/30	B05B1/30		1725
B05B1/3006	9	{the controlling element being actuated by the pressure of the fluid to be sprayed (B05B1/323 takes precedence; single-unit outlet valves actuated by the pressure of the fluid to be sprayed B05B11/0062)}	B05B1/30	B05B1/30		1222
B05B1/3013	9	{Lift valves (B05B1/3033 takes precedence)}	B05B1/30	B05B1/30		691
B05B1/302	10	{with a ball shaped valve member}	B05B1/30	B05B1/30		223
B05B1/3026	9	{Gate valves; Sliding valves; Cocks (B05B1/326 takes precedence)}	B05B1/30	B05B1/30		1194
B05B1/3033	9	{the control being effected by relative coaxial longitudinal movement of the controlling element and the spray head (B05B1/3026 takes precedence)}	B05B1/30	B05B1/30		236
B05B1/304	10	{the controlling element being a lift valve}	B05B1/30	B05B1/30		299
B05B1/3046	11	{the valve element, e.g. a needle, co-operating with a valve seat located downstream of the valve element and its actuating means, generally in the proximity of the outlet orifice (B05B1/308 takes precedence)}	B05B1/30	B05B1/30		942
B05B1/3053	12	{the actuating means being a solenoid}	B05B1/30	B05B1/30		340
B05B1/306	12	{the actuating means being a fluid}	B05B1/30	B05B1/30		438
B05B1/3066	12	{the valve element being at least partially hollow and liquid passing through it when the valve is opened}	B05B1/30	B05B1/30		115
B05B1/3073	10	{the controlling element being a deflector acting as a valve in co-operation with the outlet orifice}	B05B1/30	B05B1/30		308
B05B1/308	10	{the controlling element comprising both a lift valve and a deflector separated from the lift valve}	B05B1/30	B05B1/30		124
B05B1/3086	10	{the controlling element being a grooved body, which is movable in the outlet orifice}	B05B1/30	B05B1/30		118
B05B1/3093	9	{Recirculation valves, i.e. the valve element opens a passage to the nozzle and simultaneously closes at least partially a return passage the feeding means}	B05B1/30	B05B1/30		105
B05B1/32	9	in which a valve member forms part of the outlet opening {(B05B1/3033 takes precedence)}	B05B1/32	B05B1/32		440
B05B1/323	10	{the valve member being actuated by the pressure of the fluid to be sprayed (single unit outlet valves actuated by the pressure of the fluid to be sprayed B05B11/0062)}	B05B1/32	B05B1/32		486
B05B1/326	10	{Gate valves; Sliding valves; Cocks}	B05B1/32	B05B1/32		211
B05B1/34	8	designed to influence the nature of flow of the liquid or other fluent material, e.g. to produce swirl (designed to control volume of flow B05B1/30)	B05B1/34	B05B1/34		1124
B05B1/3402	9	{to avoid or reduce turbulence, e.g. with fluid flow straightening means}	B05B1/34	B05B1/34		413
B05B1/3405	9	{to produce swirl}	B05B1/34	B05B1/34		506
B05B1/341	10	{before discharging the liquid or other fluent material, e.g. in a swirl chamber upstream the spray outlet}	B05B1/34	B05B1/34		498
B05B1/3415	11	{with swirl imparting inserts upstream of the swirl chamber}	B05B1/34	B05B1/34		376
B05B1/3421	11	{with channels emerging substantially tangentially in the swirl chamber}	B05B1/34	B05B1/34		226
B05B1/3426	12	{the channels emerging in the swirl chamber perpendicularly to the outlet axis (B05B1/3436 takes precedence)}	B05B1/34	B05B1/34		506
B05B1/3431	12	{the channels being formed at the interface of cooperating elements, e.g. by means of grooves}	B05B1/34	B05B1/34		148
B05B1/3436	13	{the interface being a plane perpendicular to the outlet axis}	B05B1/34	B05B1/34		911
B05B1/3442	13	{the interface being a cone having the same axis as the outlet}	B05B1/34	B05B1/34		235
B05B1/3447	13	{the interface being a cylinder having the same axis as the outlet}	B05B1/34	B05B1/34		350
B05B1/3452	13	{the cooperating elements being movable, e.g. adjustable relative to one another}	B05B1/34	B05B1/34		84
B05B1/3457	14	{in response to liquid pressure}	B05B1/34	B05B1/34		37
B05B1/3463	12	{the channels extending outwardly, e.g. radially from the inside to the outside}	B05B1/34	B05B1/34		44
B05B1/3468	11	{with means for controlling the flow of liquid entering or leaving the swirl chamber (B05B1/3452 takes precedence)}	B05B1/34	B05B1/34		63
B05B1/3473	12	{in response to liquid pressure}	B05B1/34	B05B1/34		70
B05B1/3478	11	{the liquid flowing at least two different courses before reaching the swirl chamber}	B05B1/34	B05B1/34		171
B05B1/3484	11	{with a return channel extending from the swirl chamber by-passing the swirl imparting means}	B05B1/34	B05B1/34		22
B05B1/3489	11	{Nozzles having concentric outlets}	B05B1/34	B05B1/34		51
B05B1/3494	11	{the discharge outlet being not on the axis of the swirl chamber}	B05B1/34	B05B1/34		31
B05B1/36	8	Outlets for discharging by overflow	B05B1/36	B05B1/36		74
B05B3/00	7	Spraying or sprinkling apparatus with moving outlet elements or moving deflecting elements	B05B3/00	B05B3/00		312
B05B3/001	8	{incorporating means for heating or cooling, e.g. the material to be sprayed}	B05B3/00	B05B3/00		253
B05B3/002	8	{comprising a moving member supported by a fluid cushion}	B05B3/00	B05B3/00		36
B05B3/003	8	{with braking means, e.g. friction rings designed to provide a substantially constant revolution speed}	B05B3/00	B05B3/00		156
B05B3/005	9	{using viscous dissipation, e.g. a rotor movable in a chamber filled with oil}	B05B3/00	B05B3/00		122
B05B3/006	9	{using induced currents; using magnetic means}	B05B3/00	B05B3/00		54
B05B3/007	8	{with friction clutch means}	B05B3/00	B05B3/00		17
B05B3/008	8	{comprising a wobbling or nutating element, e.g. rotating about an axis describing a cone during spraying (B05B3/043 takes precedence)}	B05B3/00	B05B3/00		178
B05B3/02	8	with rotating elements (electric spraying discharge apparatus characterised by having rotary outlet or deflecting elements B05B5/04)<br><br><u>WARNING</u><br>Group B05B3/02 is impacted by reclassification into group B05B3/0202. <br>Groups B05B3/02 and B05B3/0202 should be considered in order to perform a complete search.	B05B3/02	B05B3/02		1770
B05B3/0202	9	{being deflecting elements (the liquid driven rotor being a deflecting rotating element B05B3/0426; discharging over substantially the whole periphery of the rotating member B05B3/10)}<br><br><u>WARNING</u><br>Group B05B3/0202 is incomplete pending reclassification of documents from group B05B3/02. <br>Groups B05B3/02 and B05B3/0202 should be considered in order to perform a complete search.	B05B3/02	B05B3/02		2
B05B3/0204	10	{being a ventilator or fan}	B05B3/02	B05B3/02		184
B05B3/021	9	{with means for regulating the jet relative to the horizontal angular position of the nozzle, e.g. for spraying non-circular areas by changing the elevation of the nozzle or by varying the nozzle flow-rate (when the rotating elements are rotated by the liquid or other fluent material discharged B05B3/0453)}	B05B3/02	B05B3/02		266
B05B3/025	9	{Rotational joints}	B05B3/02	B05B3/02		113
B05B3/026	10	{the fluid passing axially from one joint element to another}	B05B3/02	B05B3/02		172
B05B3/027	10	{with radial fluid passages}	B05B3/02	B05B3/02		54
B05B3/028	9	{the rotation being orbital (comprising liquid driven rotors wherein the movement of the outlet elements are a combination of two movements, one being rotational B05B3/0444; when the rotating elements are rotated by jet reaction of the liquid or other fluent material discharged B05B3/066)}	B05B3/02	B05B3/02		66
B05B3/04	9	driven by the liquid or other fluent material discharged, e.g. the liquid actuating a motor before passing to the outlet<br><br><u>WARNING</u><br>Group B05B3/04 is impacted by reclassification into groups B05B3/0417 and B05B1/085. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B3/04	B05B3/04		919
B05B3/0412	10	{comprising a liquid driven piston motor}	B05B3/04	B05B3/04		141
B05B3/0417	10	{comprising a liquid driven rotor, e.g. a turbine}<br><br><u>WARNING</u><br>Group B05B3/0417 is incomplete pending reclassification of documents from group B05B3/04. <br>Groups B05B3/04 and B05B3/0417 should be considered in order to perform a complete search.	B05B3/04	B05B3/04		459
B05B3/0419	11	{the liquid or other fluent material powering several rotors}<br><br><u>WARNING</u><br>Group B05B3/0419 is incomplete pending reclassification of documents from group B05B3/0495. <br>Groups B05B3/0495 and B05B3/0419 should be considered in order to perform a complete search.	B05B3/04	B05B3/04		1
B05B3/0421	11	{provided with means for preventing rotation}<br><br><u>WARNING</u><br>Group B05B3/0421 is incomplete pending reclassification of documents from group B05B3/049. <br>Groups B05B3/049 and B05B3/0421 should be considered in order to perform a complete search.	B05B3/04	B05B3/04		2
B05B3/0423	11	{the rotor axis not being parallel to the rotation axis of the moving outlet elements, e.g. being perpendicular thereto}	B05B3/04	B05B3/04		38
B05B3/0425	11	{actuated downstream of the outlet elements}	B05B3/04	B05B3/04		165
B05B3/0426	12	{the liquid driven rotor being a deflecting rotating element}	B05B3/04	B05B3/04		533
B05B3/0429	11	{the rotating outlet elements being directly attached to the rotor or being an integral part thereof}	B05B3/04	B05B3/04		245
B05B3/043	12	{Rotor nozzles}	B05B3/04	B05B3/04		254
B05B3/0432	11	{the rotation of the outlet elements being reversible (B05B3/0444 takes precedence)}	B05B3/04	B05B3/04		199
B05B3/0435	12	{by reversing the direction of rotation for the rotor}	B05B3/04	B05B3/04		97
B05B3/0438	12	{Tubular elements holding several outlets, e.g. apertured tubes, oscillating about an axis substantially parallel to the tubular element}	B05B3/04	B05B3/04		306
B05B3/0444	11	{the movement of the outlet elements being a combination of two movements, one being rotational}	B05B3/04	B05B3/04		175
B05B3/0446	11	{with automatic means for regulating the discharged jet (B05B3/0444 takes precedence)}	B05B3/04	B05B3/04		37
B05B3/0453	12	{relative to the angular position of the outlet elements or to the direction of rotation for the outlet elements, e.g. when spraying non-circular areas}	B05B3/04	B05B3/04		172
B05B3/0455	10	{the outlet elements being rotated by a deflecting element being successively moved into the discharged jet by the action of a biasing means and out of the discharged jet by the discharged jet}	B05B3/04	B05B3/04		474
B05B3/0461	11	{the rotation of the outlet elements being reversible}	B05B3/04	B05B3/04		165
B05B3/049	10	{comprising mechanical means for preventing a rotor from rotating despite being submerged in a streaming fluid}<br><br><u>WARNING</u><br>Group B05B3/049 is no longer used for the classification of documents as of 2025-08-01. The content of this group is being reclassified into groups B05B1/0854 and B05B3/0421.<br>Groups B05B3/049, B05B1/0854 and B05B3/0421 should be considered in order to perform a complete search.	B05B3/04	B05B3/04		43
B05B3/0495	10	{the liquid or other fluent material discharged powering several motors, e.g. several turbines}<br><br><u>WARNING</u><br>Group B05B3/0495 is no longer used for the classification of documents as of 2025-08-01. The content of this group is being reclassified into groups B05B1/0852 and B05B3/0419.<br>Groups B05B3/0495, B05B1/0852 and B05B3/0419 should be considered in order to perform a complete search.	B05B3/04	B05B3/04		35
B05B3/06	10	by jet reaction	B05B3/06	B05B3/06		1474
B05B3/063	11	{using a member, e.g. a deflector, for creating the tangential component of the jet}	B05B3/06	B05B3/06		158
B05B3/066	11	{the movement of the outlet elements being a combination of two movements, one being rotational}	B05B3/06	B05B3/06		120
B05B3/08	9	in association with stationary outlet or deflecting elements	B05B3/08	B05B3/08		185
B05B3/082	10	{the spraying being effected by centrifugal forces}	B05B3/08	B05B3/08		176
B05B3/085	11	{in association with sectorial deflectors}	B05B3/08	B05B3/08		118
B05B3/087	12	{Spray guns comprising this arrangement}	B05B3/08	B05B3/08		74
B05B3/10	9	discharging over substantially the whole periphery of the rotating member {(B05B3/082 takes precedence)}	B05B3/10	B05B3/10		464
B05B3/1007	10	{characterised by the rotating member (B05B3/105 takes precedence)}	B05B3/10	B05B3/10		546
B05B3/1014	11	{with a spraying edge, e.g. like a cup or a bell}	B05B3/10	B05B3/10		542
B05B3/1021	11	{with individual passages at its periphery}	B05B3/10	B05B3/10		314
B05B3/1028	12	{the passages comprising an insert}	B05B3/10	B05B3/10		50
B05B3/1035	10	{Driving means; Parts thereof, e.g. turbine, shaft, bearings}	B05B3/10	B05B3/10		388
B05B3/1042	11	{Means for connecting, e.g. reversibly, the rotating spray member to its driving shaft}	B05B3/10	B05B3/10		120
B05B3/105	10	{Fan or ventilator arrangements therefor}	B05B3/10	B05B3/10		217
B05B3/1057	10	{with at least two outlets, other than gas and cleaning fluid outlets, for discharging, selectively or not, different or identical liquids or other fluent materials on the rotating element}	B05B3/10	B05B3/10		219
B05B3/1064	10	{the liquid or other fluent material to be sprayed being axially supplied to the rotating member through a hollow rotating shaft}	B05B3/10	B05B3/10		493
B05B3/1071	10	{with two rotating members rotating at different speeds}	B05B3/10	B05B3/10		17
B05B3/1078	11	{the rotating members rotating in opposite directions}	B05B3/10	B05B3/10		30
B05B3/1085	10	{with means for detecting or controlling the rotational speed}	B05B3/10	B05B3/10		57
B05B3/1092	10	{Means for supplying shaping gas}	B05B3/10	B05B3/10		344
B05B3/12	9	with spray booms or the like rotating around an axis by means independent of the liquid or other fluent material discharged	B05B3/12	B05B3/12		115
B05B3/14	8	with oscillating elements; with intermittent operation	B05B3/14	B05B3/14		756
B05B3/16	9	driven or controlled by the liquid or other fluent material discharged, e.g. the liquid actuating a motor before passing to the outlet {(comprising liquid driven rotors wherein the rotation of the outlet element is reversible B05B3/0432; the outlet elements being rotated by a deflecting element successively moved into the discharged jet by the action of a biasing means and out of the discharged jet by the discharged jet with the rotation of the outlet elements being reversible B05B3/0461)}	B05B3/16	B05B3/16		346
B05B3/18	8	with elements moving in a straight line, e.g. along a track; Mobile sprinklers {(watering arrangements making use of movable installations A01G25/09)}	B05B3/18	B05B3/18		545
B05B5/00	7	Electrostatic spraying apparatus; Spraying apparatus with means for charging the spray electrically; Apparatus for spraying liquids or other fluent materials by other electric means	B05B5/00	B05B5/00		276
B05B5/001	8	{incorporating means for heating or cooling, e.g. the material to be sprayed}	B05B5/00	B05B5/00		339
B05B5/002	8	{comprising means for neutralising the spray of charged droplets or particules}	B05B5/00	B05B5/00		48
B05B5/003	9	{by mixing two sprays of opposite polarity}	B05B5/00	B05B5/00		23
B05B5/004	9	{by alternating the polarity of the spray}	B05B5/00	B05B5/00		15
B05B5/005	8	{the high voltage supplied to an electrostatic spraying apparatus being adjustable during spraying operation, e.g. for modifying spray width, droplet size}	B05B5/00	B05B5/00		77
B05B5/006	9	{the adjustement of high voltage is responsive to a condition, e.g. a condition of material discharged, of ambient medium or of target}	B05B5/00	B05B5/00		60
B05B5/007	8	{the high voltage supplied to an electrostatic spraying apparatus during spraying operation being periodical or in time, e.g. sinusoidal}	B05B5/00	B05B5/00		44
B05B5/008	9	{with periodical change of polarity}	B05B5/00	B05B5/00		12
B05B5/025	8	Discharge apparatus, e.g. electrostatic spray guns	B05B5/025	B05B5/025		740
B05B5/0255	9	{spraying and depositing by electrostatic forces only}	B05B5/025	B05B5/025		688
B05B5/03	9	characterised by the use of gas {, e.g. electrostatically assisted pneumatic spraying (B05B5/04, B05B5/043, B05B5/047 take precedence)}	B05B5/03	B05B5/03		719
B05B5/032	10	{for spraying particulate materials}	B05B5/03	B05B5/03		774
B05B5/035	9	characterised by gasless spraying {, e.g. electrostatically assisted airless spraying (B05B5/04, B05B5/043, B05B5/047 take precedence)}	B05B5/035	B05B5/035		170
B05B5/04	9	characterised by having rotary outlet or deflecting elements {, i.e. spraying being also effected by centrifugal forces}	B05B5/04	B05B5/04		399
B05B5/0403	10	{characterised by the rotating member}	B05B5/04	B05B5/04		168
B05B5/0407	11	{with a spraying edge, e.g. like a cup or a bell}	B05B5/04	B05B5/04		648
B05B5/0411	11	{with individual passages at its periphery}	B05B5/04	B05B5/04		67
B05B5/0415	10	{Driving means; Parts thereof, e.g. turbine, shaft, bearings}	B05B5/04	B05B5/04		231
B05B5/0418	10	{designed for spraying particulate material}	B05B5/04	B05B5/04		134
B05B5/0422	10	{comprising means for controlling speed of rotation}	B05B5/04	B05B5/04		67
B05B5/0426	10	{Means for supplying shaping gas}	B05B5/04	B05B5/04		476
B05B5/043	9	using induction-charging	B05B5/043	B05B5/043		281
B05B5/047	9	using tribo-charging	B05B5/047	B05B5/047		275
B05B5/053	9	Arrangements for supplying power, e.g. charging power	B05B5/053	B05B5/053		359
B05B5/0531	10	{Power generators}	B05B5/053	B05B5/053		225
B05B5/0532	11	{driven by a gas turbine}	B05B5/053	B05B5/053		39
B05B5/0533	10	{Electrodes specially adapted therefor; Arrangements of electrodes}	B05B5/053	B05B5/053		705
B05B5/0535	11	{at least two electrodes having different potentials being held on the discharge apparatus, one of them being a charging electrode of the corona type located in the spray or close to it, and another being of the non-corona type located outside of the path for the material}	B05B5/053	B05B5/053		106
B05B5/0536	11	{Dimensional characteristics of electrodes, e.g. diameter or radius of curvature of a needle-like corona electrode}	B05B5/053	B05B5/053		55
B05B5/0537	10	{comprising a charge return path between the target and the spraying apparatus which is not the "true" earth, i.e. using a direct charge return path like a wire or the like, e.g. "floating earth"}	B05B5/053	B05B5/053		15
B05B5/0538	10	{the operator being part of a charge return path between target and apparatus}	B05B5/053	B05B5/053		17
B05B5/057	9	Arrangements for discharging liquids or other fluent material without using a gun or nozzle	B05B5/057	B05B5/057		345
B05B5/06	8	using electric arc	B05B5/06	B05B5/06		45
B05B5/08	8	Plant for applying liquids or other fluent materials to objects	B05B5/08	B05B5/08		915
B05B5/081	9	{specially adapted for treating particulate materials}	B05B5/08	B05B5/08		566
B05B5/082	9	{characterised by means for supporting, holding or conveying the objects}	B05B5/08	B05B5/08		638
B05B5/084	10	{the objects lying on, or being supported above conveying means, e.g. conveyor belts}	B05B5/08	B05B5/08		273
B05B5/085	9	{the plant being provided on a vehicle}	B05B5/08	B05B5/08		56
B05B5/087	9	{Arrangements of electrodes, e.g. of charging, shielding, collecting electrodes (B05B5/12, B05B5/14 take precedence; arrangements of electrodes on the discharge apparatus B05B5/0533)}	B05B5/08	B05B5/08		423
B05B5/088	10	{for creating electric field curtains}	B05B5/08	B05B5/08		26
B05B5/10	9	Arrangements for supplying power, e.g. charging power (in discharge apparatus B05B5/053)	B05B5/10	B05B5/10		398
B05B5/12	9	specially adapted for coating the interior of hollow bodies	B05B5/12	B05B5/12		219
B05B5/14	9	specially adapted for coating continuously moving elongated bodies, e.g. wires, strips, pipes	B05B5/14	B05B5/14		368
B05B5/16	8	Arrangements for supplying liquids or other fluent material	B05B5/16	B05B5/16		398
B05B5/1608	9	{the liquid or other fluent material being electrically conductive}	B05B5/16	B05B5/16		253
B05B5/1616	10	{and the arrangement comprising means for insulating a grounded material source from high voltage applied to the material}	B05B5/16	B05B5/16		114
B05B5/1625	11	{the insulating means comprising an intermediate container alternately connected to the grounded material source for filling, and then disconnected and electrically insulated therefrom}	B05B5/16	B05B5/16		117
B05B5/1633	12	{the arrangement comprising several supply lines arranged in parallel, each comprising such an intermediate container}	B05B5/16	B05B5/16		69
B05B5/1641	12	{an additional container being provided downstream the intermediate container}	B05B5/16	B05B5/16		32
B05B5/165	11	{by dividing the material into discrete quantities, e.g. droplets}	B05B5/16	B05B5/16		38
B05B5/1658	11	{Details}	B05B5/16	B05B5/16		2
B05B5/1666	12	{Voltage blocking valves, e.g. with axially separable coupling elements}	B05B5/16	B05B5/16		30
B05B5/1675	10	{the supply means comprising a piston, e.g. a piston pump}	B05B5/16	B05B5/16		152
B05B5/1683	9	{specially adapted for particulate materials}	B05B5/16	B05B5/16		478
B05B5/1691	9	{Apparatus to be carried on or by a person or with a container fixed to the discharge device}	B05B5/16	B05B5/16		337
B05B7/00	7	Spraying apparatus for discharge of liquids or other fluent materials from two or more sources, e.g. of liquid and air, of powder and gas (B05B3/00, B05B5/00{, B05B11/06} take precedence)	B05B7/00	B05B7/00		410
B05B7/0006	8	{Spraying by means of explosions}	B05B7/00	B05B7/00		205
B05B7/0012	8	{Apparatus for achieving spraying before discharge from the apparatus}	B05B7/00	B05B7/00		1128
B05B7/0018	8	{with devices for making foam}	B05B7/00	B05B7/00		463
B05B7/0025	9	{with a compressed gas supply}	B05B7/00	B05B7/00		435
B05B7/0031	10	{with disturbing means promoting mixing, e.g. balls, crowns}	B05B7/00	B05B7/00		77
B05B7/0037	11	{including sieves, porous members or the like}	B05B7/00	B05B7/00		554
B05B7/0043	11	{including a plurality of individual elements, e.g. needles, baffles, rotatable blades}	B05B7/00	B05B7/00		43
B05B7/005	9	{wherein ambient air is aspirated by a liquid flow}	B05B7/00	B05B7/00		158
B05B7/0056	10	{with disturbing means promoting mixing, e.g. balls, crowns}	B05B7/00	B05B7/00		80
B05B7/0062	11	{including sieves, porous members or the like}	B05B7/00	B05B7/00		139
B05B7/0068	11	{including a plurality of individual elements, e.g. needles, baffles, rotatable blades}	B05B7/00	B05B7/00		36
B05B7/0075	8	{Nozzle arrangements in gas streams}	B05B7/00	B05B7/00		700
B05B7/0081	8	{Apparatus supplied with low pressure gas, e.g. "hvlp"-guns; air supplied by a fan}	B05B7/00	B05B7/00		454
B05B7/0087	9	{Atmospheric air being sucked by a gas stream, generally flowing through a venturi, at a location upstream or inside the spraying apparatus}	B05B7/00	B05B7/00		96
B05B7/0093	8	{At least a part of the apparatus, e.g. a container, being provided with means, e.g. wheels or casters for allowing its displacement relative to the ground}	B05B7/00	B05B7/00		231
B05B7/02	8	Spray pistols; Apparatus for discharge (for spraying particulate material B05B7/14; with means for heating the material to be sprayed B05B7/16; with means for supplying fluent material to a discharge device B05B7/24)	B05B7/02	B05B7/02		898
B05B7/025	9	{Nozzles having elongated outlets, e.g. slots, for the material to be sprayed}	B05B7/02	B05B7/02		235
B05B7/04	9	with arrangements for mixing liquids or other fluent materials before discharge (mixing in general B01F, e.g. B01F25/00; mixing valves F16K11/00)	B05B7/04	B05B7/04		991
B05B7/0408	10	{with arrangements for mixing two or more liquids}	B05B7/04	B05B7/04		1549
B05B7/0416	10	{with arrangements for mixing one gas and one liquid}	B05B7/04	B05B7/04		1931
B05B7/0425	11	{without any source of compressed gas, e.g. the air being sucked by the pressurised liquid}	B05B7/04	B05B7/04		656
B05B7/0433	11	{with one inner conduit of gas surrounded by an external conduit of liquid upstream the mixing chamber}	B05B7/04	B05B7/04		416
B05B7/0441	11	{with one inner conduit of liquid surrounded by an external conduit of gas upstream the mixing chamber}	B05B7/04	B05B7/04		181
B05B7/045	12	{the gas and liquid flows being parallel just upstream the mixing chamber (B05B7/0458, B05B7/0466 take precedence)}	B05B7/04	B05B7/04		233
B05B7/0458	12	{the gas and liquid flows being perpendicular just upstream the mixing chamber}	B05B7/04	B05B7/04		174
B05B7/0466	12	{with means for deflecting the central liquid flow towards the peripheral gas flow}	B05B7/04	B05B7/04		172
B05B7/0475	12	{with means for deflecting the peripheral gas flow towards the central liquid flow (B05B7/0458 takes precedence)}	B05B7/04	B05B7/04		461
B05B7/0483	11	{with gas and liquid jets intersecting in the mixing chamber}	B05B7/04	B05B7/04		660
B05B7/0491	11	{the liquid and the gas being mixed at least twice along the flow path of the liquid}	B05B7/04	B05B7/04		173
B05B7/06	9	with {at least} one outlet orifice surrounding another approximately in the same plane	B05B7/06	B05B7/06		189
B05B7/061	10	{with several liquid outlets discharging one or several liquids}	B05B7/06	B05B7/06		219
B05B7/062	10	{with only one liquid outlet and at least one gas outlet}	B05B7/06	B05B7/06		93
B05B7/063	11	{one fluid being sucked by the other}	B05B7/06	B05B7/06		32
B05B7/064	12	{the liquid being sucked by the gas}	B05B7/06	B05B7/06		118
B05B7/065	11	{an inner gas outlet being surrounded by an annular adjacent liquid outlet}	B05B7/06	B05B7/06		220
B05B7/066	11	{with an inner liquid outlet surrounded by at least one annular gas outlet}	B05B7/06	B05B7/06		1268
B05B7/067	12	{the liquid outlet being annular}	B05B7/06	B05B7/06		216
B05B7/068	12	{the annular gas outlet being supplied by a gas conduit having an axially concave curved internal surface just upstream said outlet}	B05B7/06	B05B7/06		129
B05B7/08	9	with separate outlet orifices, e.g. to form parallel jets {, i.e. the axis of the jets being parallel}, to form intersecting jets {, i.e. the axis of the jets converging but not necessarily intersecting at a point}	B05B7/08	B05B7/08		477
B05B7/0807	10	{to form intersecting jets}	B05B7/08	B05B7/08		338
B05B7/0815	11	{with at least one gas jet intersecting a jet constituted by a liquid or a mixture containing a liquid for controlling the shape of the latter}	B05B7/08	B05B7/08		1328
B05B7/0823	12	{comprising a rotatable spray pattern adjusting plate controlling the flow rate of the spray shaping gas jets}	B05B7/08	B05B7/08		50
B05B7/083	12	{comprising rotatable spray shaping gas jet outlets}	B05B7/08	B05B7/08		98
B05B7/0838	12	{comprising a single means controlling simultaneously the flow rates of shaping and spraying gas jets}	B05B7/08	B05B7/08		64
B05B7/0846	11	{with jets being only jets constituted by a liquid or a mixture containing a liquid}	B05B7/08	B05B7/08		226
B05B7/0853	11	{with one single gas jet and several jets constituted by a liquid or a mixture containing a liquid (B05B7/0815 takes precedence)}	B05B7/08	B05B7/08		66
B05B7/0861	11	{with one single jet constituted by a liquid or a mixture containing a liquid and several gas jets (B05B7/0815 takes precedence)}	B05B7/08	B05B7/08		376
B05B7/0869	10	{the liquid or other fluent material being sucked or aspirated from an outlet orifice by another fluid, e.g. a gas, coming from another outlet orifice}	B05B7/08	B05B7/08		114
B05B7/0876	10	{to form parallel jets constituted by a liquid or a mixture containing a liquid (B05B7/0884, B05B7/0892 take precedence)}	B05B7/08	B05B7/08		132
B05B7/0884	10	{the outlet orifices for jets constituted by a liquid or a mixture containing a liquid being aligned}	B05B7/08	B05B7/08		365
B05B7/0892	10	{the outlet orifices for jets constituted by a liquid or a mixture containing a liquid being disposed on a circle}	B05B7/08	B05B7/08		274
B05B7/10	9	producing a swirling discharge	B05B7/10	B05B7/10		1140
B05B7/12	9	designed to control volume of flow, e.g. with adjustable passages	B05B7/12	B05B7/12		1481
B05B7/1209	10	{the controlling means for each liquid or other fluent material being manual and interdependent}	B05B7/12	B05B7/12		919
B05B7/1218	11	{With means for adjusting or modifying the action of the controlling means}	B05B7/12	B05B7/12		91
B05B7/1227	11	{Non linear relationship between the controlling means displacement and the valve element displacement}	B05B7/12	B05B7/12		8
B05B7/1236	11	{with three or more interdependent valves}	B05B7/12	B05B7/12		33
B05B7/1245	11	{A gas valve being opened before a liquid valve}	B05B7/12	B05B7/12		106
B05B7/1254	10	{the controlling means being fluid actuated}	B05B7/12	B05B7/12		113
B05B7/1263	11	{pneumatically actuated}	B05B7/12	B05B7/12		225
B05B7/1272	12	{actuated by gas involved in spraying, i.e. exiting the nozzle, e.g. as a spraying or jet shaping gas}	B05B7/12	B05B7/12		249
B05B7/1281	13	{Serial arrangement, i.e. a single gas stream acting on the controlling means first and flowing downstream thereof to the nozzle}	B05B7/12	B05B7/12		62
B05B7/129	10	{Hand guns comprising a gas valve located at the bottom of the handle (B05B7/0087 takes precedence)}	B05B7/12	B05B7/12		45
B05B7/14	8	designed for spraying particulate materials (B05B7/16 takes precedence)	B05B7/14	B05B7/14		327
B05B7/1404	9	{Arrangements for supplying particulate material}	B05B7/14	B05B7/14		955
B05B7/1409	10	{specially adapted for short fibres or chips (B05B7/145 takes precedence)}	B05B7/14	B05B7/14		96
B05B7/1413	10	{Apparatus to be carried on or by a person, e.g. by hand; Apparatus comprising a container fixed to the discharge device}	B05B7/14	B05B7/14		314
B05B7/1418	11	{comprising means for supplying an additional liquid}	B05B7/14	B05B7/14		94
B05B7/1422	11	{the means for supplying particulate material comprising moving mechanical means, e.g. to impart vibration}	B05B7/14	B05B7/14		89
B05B7/1427	11	{Apparatus to be carried on the back of the user}	B05B7/14	B05B7/14		96
B05B7/1431	10	{comprising means for supplying an additional liquid (B05B7/1418 takes precedence)}	B05B7/14	B05B7/14		212
B05B7/1436	11	{to a container where the particulate material and the additional liquid are brought together (mixing in general B01F)}	B05B7/14	B05B7/14		141
B05B7/144	10	{the means for supplying particulate material comprising moving mechanical means (B05B7/1422, B05B7/1459 take precedence)}	B05B7/14	B05B7/14		423
B05B7/1445	11	{involving vibrations (B05B7/145 takes precedence)}	B05B7/14	B05B7/14		220
B05B7/145	11	{specially adapted for short fibres or chips}	B05B7/14	B05B7/14		55
B05B7/1454	10	{comprising means for supplying collected oversprayed particulate material (spray booth with arrangements for collecting oversprayed material B05B14/40)}	B05B7/14	B05B7/14		161
B05B7/1459	10	{comprising a chamber, inlet and outlet valves upstream and downstream the chamber and means for alternately sucking particulate material into and removing particulate material from the chamber through the valves (conveying material in bulk by using a combination of gas pressure and suction B65G53/28; pumps in general F04B; apparatus for repeatedly measuring and separating a predetermined volume of fluent solid material from a supply or container G01F11/00)}	B05B7/14	B05B7/14		146
B05B7/1463	10	{the means for supplying particulate material comprising a gas inlet for pressurising or avoiding depressurisation of a powder container}	B05B7/14	B05B7/14		131
B05B7/1468	10	{the means for supplying particulate material comprising a recirculation loop}	B05B7/14	B05B7/14		62
B05B7/1472	10	{Powder extracted from a powder container in a direction substantially opposite to gravity by a suction device dipped into the powder}	B05B7/14	B05B7/14		436
B05B7/1477	10	{means for supplying to several spray apparatus}	B05B7/14	B05B7/14		175
B05B7/1481	9	{Spray pistols or apparatus for discharging particulate material}	B05B7/14	B05B7/14		292
B05B7/1486	10	{for spraying particulate material in dry state}	B05B7/14	B05B7/14		899
B05B7/149	10	{with separate inlets for a particulate material and a liquid to be sprayed}	B05B7/14	B05B7/14		200
B05B7/1495	11	{and with separate outlets for the particulate material and the liquid}	B05B7/14	B05B7/14		243
B05B7/16	8	incorporating means for heating {or cooling} the material to be sprayed {(spraying by means of explosions B05B7/0006)}	B05B7/16	B05B7/16		315
B05B7/1606	9	{the spraying of the material involving the use of an atomising fluid, e.g. air (B05B7/168, B05B7/1686, B05B7/20, B05B7/22 take precedence)}	B05B7/16	B05B7/16		247
B05B7/1613	10	{comprising means for heating the atomising fluid before mixing with the material to be sprayed}	B05B7/16	B05B7/16		178
B05B7/162	11	{and heat being transferred from the atomising fluid to the material to be sprayed}	B05B7/16	B05B7/16		140
B05B7/1626	12	{at the moment of mixing}	B05B7/16	B05B7/16		182
B05B7/1633	11	{and heat being transferred from the material to be sprayed to the atomising fluid}	B05B7/16	B05B7/16		26
B05B7/164	11	{the material to be sprayed and the atomising fluid being heated by independent sources of heat, without transfer of heat between atomising fluid and material to be sprayed}	B05B7/16	B05B7/16		45
B05B7/1646	11	{the material to be sprayed and the atomising fluid being heated by the same source of heat, without transfer of heat between atomising fluid and material to be sprayed}	B05B7/16	B05B7/16		80
B05B7/1653	12	{the source of heat being a heat conductive fluid}	B05B7/16	B05B7/16		30
B05B7/166	9	{the material to be sprayed being heated in a container (B05B7/208 takes precedence)}	B05B7/16	B05B7/16		207
B05B7/1666	10	{fixed to the discharge device}	B05B7/16	B05B7/16		117
B05B7/1673	9	{heat being transferred to the material to be sprayed by a heat transfer conductive fluid (B05B7/162, B05B7/1653 take precedence)}	B05B7/16	B05B7/16		77
B05B7/168	9	{with means for heating or cooling after mixing (B05B7/201, B05B7/22 take precedence)}	B05B7/16	B05B7/16		167
B05B7/1686	9	{involving vaporisation of the material to be sprayed or of an atomising-fluid-generating product}	B05B7/16	B05B7/16		273
B05B7/1693	9	{with means for heating the material to be sprayed or an atomizing fluid in a supply hose or the like}	B05B7/16	B05B7/16		201
B05B7/18	9	the material having originally the shape of a wire, rod or the like {(B05B7/203, B05B7/224 take precedence)}	B05B7/18	B05B7/18		143
B05B7/20	9	by flame or combustion	B05B7/20	B05B7/20		200
B05B7/201	10	{downstream of the nozzle}	B05B7/20	B05B7/20		119
B05B7/203	11	{the material to be sprayed having originally the shape of a wire, rod or the like}	B05B7/20	B05B7/20		274
B05B7/205	11	{the material to be sprayed being originally a particulate material}	B05B7/20	B05B7/20		464
B05B7/206	12	{in a container fixed to the discharge device}	B05B7/20	B05B7/20		140
B05B7/208	10	{the material to be sprayed being heated in a container}	B05B7/20	B05B7/20		47
B05B7/22	9	electrically {, magnetically or electromagnetically}, e.g. by arc {(B05B7/20 takes precedence)}	B05B7/22	B05B7/22		278
B05B7/222	10	{using an arc}	B05B7/22	B05B7/22		111
B05B7/224	11	{the material having originally the shape of a wire, rod or the like}	B05B7/22	B05B7/22		376
B05B7/226	11	{the material being originally a particulate material}	B05B7/22	B05B7/22		411
B05B7/228	10	{using electromagnetic radiation, e.g. laser}	B05B7/22	B05B7/22		157
B05B7/24	8	with means, e.g. a container, for supplying liquid or other fluent material to a discharge device (B05B7/14, B05B7/16, B05B11/00 take precedence)	B05B7/24	B05B7/24		722
B05B7/2402	9	{Apparatus to be carried on or by a person, e.g. by hand; Apparatus comprising containers fixed to the discharge device (B05B7/0012 takes precedence)}	B05B7/24	B05B7/24		211
B05B7/2405	10	{using an atomising fluid as carrying fluid for feeding, e.g. by suction or pressure, a carried liquid from the container to the nozzle (B05B7/2459&#160;-&#160;B05B7/247 take precedence)}	B05B7/24	B05B7/24		179
B05B7/2408	11	{characterised by the container or its attachment means to the spray apparatus}	B05B7/24	B05B7/24		663
B05B7/241	12	{the container being pressurised}	B05B7/24	B05B7/24		197
B05B7/2413	12	{with means for changing the position or the orientation of the container relative to the spray apparatus}	B05B7/24	B05B7/24		45
B05B7/2416	11	{characterised by the means for producing or supplying the atomising fluid, e.g. air hoses, air pumps, gas containers, compressors, fans, ventilators, their drives}	B05B7/24	B05B7/24		580
B05B7/2418	12	{Air pumps actuated by the operator, e.g. manually actuated}	B05B7/24	B05B7/24		141
B05B7/2421	12	{Gas containers}	B05B7/24	B05B7/24		165
B05B7/2424	11	{the carried liquid and the main stream of atomising fluid being brought together downstream of the container before discharge (B05B7/2435 takes precedence)}	B05B7/24	B05B7/24		435
B05B7/2427	12	{and a secondary stream of atomising fluid being brought together in the container or putting the carried liquid under pressure in the container}	B05B7/24	B05B7/24		195
B05B7/2429	11	{the carried liquid and the main stream of atomising fluid being brought together after discharge (B05B7/2435 takes precedence)}	B05B7/24	B05B7/24		383
B05B7/2432	12	{and a secondary stream of atomising fluid being brought together in the container or putting the carried liquid under pressure in the container}	B05B7/24	B05B7/24		53
B05B7/2435	11	{the carried liquid and the main stream of atomising fluid being brought together by parallel conduits placed one inside the other}	B05B7/24	B05B7/24		553
B05B7/2437	12	{and a secondary stream of atomising fluid being brought together in the container or putting the carried fluid under pressure in the container}	B05B7/24	B05B7/24		358
B05B7/244	10	{using carrying liquid for feeding, e.g. by suction, pressure or dissolution, a carried liquid from the container to the nozzle (B05B7/2459&#160;-&#160;B05B7/247 take precedence)}	B05B7/24	B05B7/24		77
B05B7/2443	11	{the carried liquid and the main stream of carrying liquid being brought together downstream of the container before discharge (B05B7/2454 takes precedence)}	B05B7/24	B05B7/24		450
B05B7/2445	12	{and a secondary stream of carrying liquid being brought together in the container or putting the carried liquid under pressure in the container}	B05B7/24	B05B7/24		123
B05B7/2448	11	{the carried liquid and the main stream of carrying liquid being brought together after discharge (B05B7/2454 takes precedence)}	B05B7/24	B05B7/24		42
B05B7/2451	12	{and a secondary stream of carrying liquid being brought together in the container or putting the carried liquid in the container}	B05B7/24	B05B7/24		5
B05B7/2454	11	{the carried liquid and the main stream of carrying liquid being brought together by parallel conduits, one conduit being in the other}	B05B7/24	B05B7/24		43
B05B7/2456	12	{and a secondary stream of carrying liquid being brought together in the container or putting the carried liquid under pressure in the container}	B05B7/24	B05B7/24		18
B05B7/2459	10	{a liquid being fed by capillarity from the container to the nozzle}	B05B7/24	B05B7/24		55
B05B7/2462	10	{using a carrying liquid flowing through the container for dissolving a block of solid material}	B05B7/24	B05B7/24		155
B05B7/2464	10	{a liquid being fed by mechanical pumping from the container to the nozzle}	B05B7/24	B05B7/24		213
B05B7/2467	10	{a liquid being fed by a pressure generated in the container, which is not produced by a carrying fluid}	B05B7/24	B05B7/24		118
B05B7/247	10	{a liquid being fed by gravity only from the container to the nozzle (B05B7/2478 takes precedence)}	B05B7/24	B05B7/24		36
B05B7/2472	10	{comprising several containers}	B05B7/24	B05B7/24		403
B05B7/2475	10	{comprising a container carried on the back of the user}	B05B7/24	B05B7/24		170
B05B7/2478	10	{Gun with a container which, in normal use, is located above the gun}	B05B7/24	B05B7/24		809
B05B7/2481	10	{with a flexible container for liquid or other fluent material}	B05B7/24	B05B7/24		191
B05B7/2483	9	{the supplying means involving no pressure or aspiration, e.g. means involving gravity or capillarity (B05B7/2459, B05B7/247 take precedence)}	B05B7/24	B05B7/24		90
B05B7/2486	9	{with means for supplying liquid or other fluent material to several discharge devices}	B05B7/24	B05B7/24		302
B05B7/2489	9	{an atomising fluid, e.g. a gas, being supplied to the discharge device (B05B7/2402, B05B7/2483, B05B7/262 take precedence)}	B05B7/24	B05B7/24		506
B05B7/2491	10	{characterised by the means for producing or supplying the atomising fluid, e.g. air hoses, air pumps, gas containers, compressors, fans, ventilators, their drives}	B05B7/24	B05B7/24		737
B05B7/2494	10	{a liquid being supplied from a pressurized or compressible container to the discharge device}	B05B7/24	B05B7/24		325
B05B7/2497	10	{several liquids from different sources being supplied to the discharge device}	B05B7/24	B05B7/24		252
B05B7/26	9	Apparatus in which liquids or other fluent materials from different sources are brought together before entering the discharge device {(B05B7/2402 takes precedence)}	B05B7/26	B05B7/26		350
B05B7/262	10	{a liquid and a gas being brought together before entering the discharge device}	B05B7/26	B05B7/26		120
B05B7/265	11	{the liquid being fed by gravity, or sucked into the gas}	B05B7/26	B05B7/26		44
B05B7/267	11	{the liquid and the gas being both under pressure}	B05B7/26	B05B7/26		118
B05B7/28	10	in which one liquid or other fluent material is fed or drawn through an orifice into a stream of a carrying fluid {(B05B7/262 takes precedence)}	B05B7/28	B05B7/28		124
B05B7/30	11	the first liquid or other fluent material being fed by gravity, or sucked into the carrying fluid	B05B7/30	B05B7/30		314
B05B7/32	11	the fed liquid or other fluent material being under pressure	B05B7/32	B05B7/32		651
B05B9/00	7	Spraying apparatus for discharge of liquids or other fluent material, without essentially mixing with gas or vapour (B05B11/00 takes precedence)	B05B9/00	B05B9/00		265
B05B9/002	8	{incorporating means for heating or cooling, e.g. the material to be sprayed}	B05B9/00	B05B9/00		1113
B05B9/005	8	{the liquid or other fluent material being a fluid close to a change of phase}	B05B9/00	B05B9/00		71
B05B9/007	8	{At least a part of the apparatus, e.g. a container, being provided with means, e.g. wheels, for allowing its displacement relative to the ground}	B05B9/00	B05B9/00		1381
B05B9/01	8	Spray pistols, {discharge devices}(B05B9/03 takes precedence)	B05B9/01	B05B9/01		2050
B05B9/03	8	characterised by means for supplying liquid or other fluent material {(B05B9/002 takes precedence)}	B05B9/03	B05B9/03		1132
B05B9/035	9	{to several spraying apparatus (B05B9/0423 takes precedence)}	B05B9/03	B05B9/03		325
B05B9/04	9	with pressurised or compressible container (aerosol containers B65D83/14); with pump	B05B9/04	B05B9/04		1798
B05B9/0403	10	{with pumps for liquids or other fluent material (B05B9/043 takes precedence)}	B05B9/04	B05B9/04		4519
B05B9/0406	11	{with several pumps}	B05B9/04	B05B9/04		453
B05B9/0409	11	{the pumps being driven by a hydraulic or a pneumatic fluid}	B05B9/04	B05B9/04		635
B05B9/0413	11	{with reciprocating pumps, e.g. membrane pump, piston pump, bellow pump (B05B9/0409 takes precedence)}	B05B9/04	B05B9/04		686
B05B9/0416	11	{with pumps comprising rotating pumping parts, e.g. gear pump, centrifugal pump, screw-type pump (B05B9/042 takes precedence)}	B05B9/04	B05B9/04		197
B05B9/042	11	{with peristaltic pumps}	B05B9/04	B05B9/04		84
B05B9/0423	11	{for supplying liquid or other fluent material to several spraying apparatus}	B05B9/04	B05B9/04		1295
B05B9/0426	11	{with a pump attached to the spray gun or discharge device (single-units hand-held apparatus in which the flow is effected by a pump B05B11/10)}	B05B9/04	B05B9/04		333
B05B9/043	10	having pump readily separable from container	B05B9/043	B05B9/043		175
B05B9/047	10	supply being effected by follower in container, e.g. membrane or floating piston {, or by deformation of container (B05B9/0838 takes precedence)}	B05B9/047	B05B9/047		912
B05B9/06	10	the delivery being related to the movement of a vehicle, e.g. the pump being driven by a vehicle wheel	B05B9/06	B05B9/06		367
B05B9/08	10	Apparatus to be carried on or by a person, e.g. of knapsack type ({B05B9/0426, B05B11/00 take precedence } ; details or components, e.g. casings, bodies of portable power-driven tools not particularly related to the operation performed B25F5/00)	B05B9/08	B05B9/08		430
B05B9/0805	11	{comprising a pressurised or compressible container for liquid or other fluent material (B05B9/085 takes precedence)}	B05B9/08	B05B9/08		367
B05B9/0811	12	{comprising air supplying means actuated by the operator to pressurise or compress the container}	B05B9/08	B05B9/08		132
B05B9/0816	13	{the air supplying means being a manually actuated air pump}	B05B9/08	B05B9/08		437
B05B9/0822	14	{a discharge device being fixed to the container}	B05B9/08	B05B9/08		320
B05B9/0827	14	{the air pump being actuated by shaking}	B05B9/08	B05B9/08		21
B05B9/0833	12	{comprising a compressed gas container, e.g. a nitrogen cartridge}	B05B9/08	B05B9/08		216
B05B9/0838	12	{supply being effected by follower in container, e.g. membrane or floating piston, or by deformation of container}	B05B9/08	B05B9/08		378
B05B9/0844	12	{the container being pressurised or compressed by a gas generated by a chemical reaction}	B05B9/08	B05B9/08		40
B05B9/085	11	{with a liquid pump}	B05B9/08	B05B9/08		249
B05B9/0855	12	{the pump being motor-driven (B05B9/0866, B05B9/0872 take precedence)}	B05B9/08	B05B9/08		95
B05B9/0861	13	{the motor being electric}	B05B9/08	B05B9/08		763
B05B9/0866	12	{the pump being a gear, centrifugal or screw-type pump}	B05B9/08	B05B9/08		94
B05B9/0872	12	{the pump being a peristaltic pump}	B05B9/08	B05B9/08		59
B05B9/0877	12	{the pump being of pressure-accumulation type or being connected to a pressure accumulation chamber}	B05B9/08	B05B9/08		206
B05B9/0883	13	{having a discharge device fixed to the container}	B05B9/08	B05B9/08		165
B05B9/0888	11	{Carrying means for knapsack sprayers}	B05B9/08	B05B9/08		196
B05B9/0894	11	{Gun with a container which, in normal use, is located above the gun}	B05B9/08	B05B9/08		124
B05B11/00	7	Single-unit hand-held apparatus in which flow of contents is produced by the muscular force of the operator at the moment of use	B05B11/00	B05B11/00		425
B05B11/0002	8	{incorporating means for heating or cooling, e.g. the material to be sprayed}	B05B11/00	B05B11/00		148
B05B11/0005	8	{Components or details (of single units wherein the flow is effected by a pump B05B11/1042)}	B05B11/00	B05B11/00		943
B05B11/0008	9	{Sealing or attachment arrangements between sprayer and container (between pump and container B05B11/1043)}	B05B11/00	B05B11/00		462
B05B11/001	10	{Snap-on-twist-off type connections}	B05B11/00	B05B11/00		67
B05B11/0013	10	{Attachment arrangements comprising means cooperating with the inner surface of the container}	B05B11/00	B05B11/00		156
B05B11/0027	9	{Means for neutralising the actuation of the sprayer (pump locking means B05B11/1059); Means for preventing access to the sprayer actuation means}	B05B11/00	B05B11/00		401
B05B11/0029	10	{Valves not actuated by pressure (B05B11/0032, B05B11/0094 take precedence; automatically opened during actuation of a spray pump B05B11/1053)}	B05B11/00	B05B11/00		250
B05B11/0032	10	{Manually actuated means located downstream the discharge nozzle for closing or covering it, e.g. shutters (automatically removed during actuation of a spray pump B05B11/1053)}	B05B11/00	B05B11/00		1114
B05B11/0035	9	{Pen-like sprayers}	B05B11/00	B05B11/00		224
B05B11/0037	9	{Containers (for several components B05B11/0078)}	B05B11/00	B05B11/00		1320
B05B11/0038	10	{Inner container disposed in an outer shell or outer casing}	B05B11/00	B05B11/00		1181
B05B11/0039	10	{associated with means for compensating the pressure difference between the ambient pressure and the pressure inside the container, e.g. pressure relief means}	B05B11/00	B05B11/00		155
B05B11/0041	11	{compensating underpressure without contact of the fluid remaining in the container with the atmospheric air (B05B11/026 and B05B11/028 take precedence)}	B05B11/00	B05B11/00		76
B05B11/00411	12	{the means being an inert gas}	B05B11/00	B05B11/00		22
B05B11/0044	11	{compensating underpressure by ingress of atmospheric air into the container, i.e. with venting means (venting means for deformable containers B05B11/047)}	B05B11/00	B05B11/00		843
B05B11/00442	12	{the means being actuated by the difference between the atmospheric pressure and the pressure inside the container}	B05B11/00	B05B11/00		245
B05B11/00444	12	{with provision for filtering or cleaning the air flow drawn into the container}	B05B11/00	B05B11/00		137
B05B11/00446	12	{the means being located at the bottom of the container or of an enclosure surrounding the container}	B05B11/00	B05B11/00		79
B05B11/0054	10	{Cartridges, i.e. containers specially designed for easy attachment to or easy removal from the rest of the sprayer (attachment arrangements between pump and container B05B11/1043)}	B05B11/00	B05B11/00		710
B05B11/0056	10	{with an additional opening for filling or refilling}	B05B11/00	B05B11/00		443
B05B11/0059	9	{allowing operation in any orientation, e.g. for discharge in inverted position}	B05B11/00	B05B11/00		746
B05B11/0062	9	{Outlet valves actuated by the pressure of the fluid to be sprayed (fluid-actuated pump outlet valve arrangements B05B11/1016, B05B11/1022, B05B11/1033, B05B11/1036, B05B11/104, B05B11/1064, B05B11/1097)}	B05B11/00	B05B11/00		267
B05B11/0064	10	{Lift valves (B05B11/007 takes precedence)}	B05B11/00	B05B11/00		340
B05B11/0067	11	{having a valve seat located downstream the valve element}	B05B11/00	B05B11/00		206
B05B11/007	10	{being opened by deformation of a sealing element made of resiliently deformable material, e.g. flaps, skirts, duck-bill valves}	B05B11/00	B05B11/00		644
B05B11/0072	10	{A valve member forming part of an outlet opening}	B05B11/00	B05B11/00		425
B05B11/0075	10	{Two outlet valves being placed in a delivery conduit, one downstream the other}	B05B11/00	B05B11/00		176
B05B11/0078	9	{Arrangements for separately storing several components (arrangements for pumping several liquids or other fluent materials from several containers B05B11/1081)}	B05B11/00	B05B11/00		353
B05B11/0081	10	{and for mixing the components in a common container as a mixture ready for use before discharging the latter}	B05B11/00	B05B11/00		222
B05B11/0083	11	{one of the components being in powder form}	B05B11/00	B05B11/00		53
B05B11/0086	9	{Arrangements for allowing spraying and pouring}	B05B11/00	B05B11/00		159
B05B11/0089	9	{Dispensing tubes}	B05B11/00	B05B11/00		293
B05B11/0091	10	{movable, e.g. articulated on the sprayer}	B05B11/00	B05B11/00		88
B05B11/0094	11	{movement of the dispensing tube controlling a valve}	B05B11/00	B05B11/00		139
B05B11/0097	9	{Means for filling or refilling the sprayer (through additional openings in the container B05B11/0056)}	B05B11/00	B05B11/00		402
B05B11/01	8	characterised by the means producing the flow	B05B11/01	B05B11/01		22
B05B11/02	9	Membranes or pistons acting on the contents inside the container, e.g. follower pistons	B05B11/02	B05B11/02		615
B05B11/025	10	{with stepwise advancement of the piston, e.g. for spraying a predetermined quantity of content}	B05B11/02	B05B11/02		115
B05B11/026	10	{Membranes separating the content remaining in the container from the atmospheric air to compensate underpressure inside the container}	B05B11/02	B05B11/02		964
B05B11/027	11	{inverted during outflow of content}	B05B11/02	B05B11/02		55
B05B11/028	10	{Pistons separating the content remaining in the container from the atmospheric air to compensate underpressure inside the container}	B05B11/02	B05B11/02		1165
B05B11/029	11	{located on top of the remaining content}	B05B11/02	B05B11/02		108
B05B11/04	9	Deformable containers producing the flow, e.g. squeeze bottles	B05B11/04	B05B11/04		219
B05B11/041	10	{designed for spraying particulate material (B05B11/045 takes precedence)}	B05B11/04	B05B11/04		134
B05B11/042	10	{the spray being effected by a gas or vapour flow in the nozzle, spray head, outlet or dip tube}	B05B11/04	B05B11/04		80
B05B11/043	11	{designed for spraying a liquid (B05B11/046 takes precedence)}	B05B11/04	B05B11/04		563
B05B11/045	11	{designed for spraying particulate material (B05B11/046 takes precedence)}	B05B11/04	B05B11/04		62
B05B11/046	11	{the gas or vapour flow coming from a source where the gas or vapour is not in contact with the liquid or other fluent material to be sprayed, e.g. from a compressive bulb, an air pump or an enclosure surrounding the container}	B05B11/04	B05B11/04		52
B05B11/047	10	{characterised by the outlet or venting means (B05B11/041 and B05B11/042 take precedence)}	B05B11/04	B05B11/04		394
B05B11/048	10	{characterised by the container, e.g. this latter being surrounded by an enclosure, or the means for deforming it (B05B11/041, B05B11/046 take precedence)}	B05B11/04	B05B11/04		423
B05B11/06	9	Gas or vapour producing the flow, e.g. from a compressible bulb or air pump	B05B11/06	B05B11/06		1512
B05B11/061	10	{characterised by the means producing the gas or vapour pressure}	B05B11/06	B05B11/06		271
B05B11/062	10	{designed for spraying particulate material}	B05B11/06	B05B11/06		498
B05B11/064	11	{the particulate material being stored in several discrete quantities delivered one at a time}	B05B11/06	B05B11/06		12
B05B11/065	11	{the particulate material being separated from a main storage in discrete quantities delivered one at a time}	B05B11/06	B05B11/06		17
B05B11/067	12	{the particulate material being separated from the main storage by a dosing device}	B05B11/06	B05B11/06		9
B05B11/068	10	{comprising a liquid-absorbent material}	B05B11/06	B05B11/06		73
B05B11/10	9	Pump arrangements for transferring the contents from the container to a pump chamber by a sucking effect and forcing the contents out through the dispensing nozzle	B05B11/10	B05B11/10		863
B05B11/1001	10	{Piston pumps (B05B11/1087, B05B11/1088, B05B11/109 take precedence)}	B05B11/10	B05B11/10		2437
B05B11/1002	11	{the direction of the pressure stroke being substantially perpendicular to the major axis of the container (B05B11/1009, B05B11/1015 take precedence)}	B05B11/10	B05B11/10		298
B05B11/1004	11	{comprising a movable cylinder and a stationary piston}	B05B11/10	B05B11/10		337
B05B11/1005	11	{with means for adjusting or modifying pump stroke}	B05B11/10	B05B11/10		59
B05B11/1007	12	{by adjusting or modifying the pump end-of-sucking-stroke position}	B05B11/10	B05B11/10		92
B05B11/1008	12	{by adjusting or modifying the pump end-of-dispensing-stroke position}	B05B11/10	B05B11/10		181
B05B11/1009	11	{actuated by a lever}	B05B11/10	B05B11/10		257
B05B11/1011	12	{without substantial movement of the nozzle in the direction of the pressure stroke}	B05B11/10	B05B11/10		1432
B05B11/1012	12	{the pump chamber being arranged substantially coaxially to the neck of the container (B05B11/1011 takes precedence)}	B05B11/10	B05B11/10		38
B05B11/1014	13	{the pump chamber being arranged substantially coaxially to the container}	B05B11/10	B05B11/10		193
B05B11/1015	11	{actuated without substantial movement of the nozzle in the direction of the pressure stroke (B05B11/1011 takes precedence)}	B05B11/10	B05B11/10		655
B05B11/1016	11	{the outlet valve having a valve seat located downstream a movable valve element controlled by a pressure actuated controlling element (B05B11/1022, B05B11/1023 take precedence)}	B05B11/10	B05B11/10		347
B05B11/1018	12	{and the controlling element cooperating with means for opening or closing the inlet valve (B05B11/1019 takes precedence)}	B05B11/10	B05B11/10		226
B05B11/1019	12	{the inlet valve moving concurrently with the controlling element during whole pressure and aspiration strokes, e.g. a cage for an inlet valve ball being part of the controlling element}	B05B11/10	B05B11/10		105
B05B11/1021	11	{having an outlet valve which is a gate valve (B05B11/1023, B05B11/1038 take precedence)}	B05B11/10	B05B11/10		27
B05B11/1022	12	{actuated by pressure}	B05B11/10	B05B11/10		71
B05B11/1023	11	{having an outlet valve opened by deformation or displacement of the piston relative to its actuating stem}	B05B11/10	B05B11/10		1772
B05B11/1025	12	{a spring urging the outlet valve in its closed position (B05B11/1026 takes precedence)}	B05B11/10	B05B11/10		384
B05B11/1026	12	{the piston being deformable and its deformation allowing opening of the outlet}	B05B11/10	B05B11/10		144
B05B11/1028	10	{Pumps having a pumping chamber with a deformable wall (B05B11/1087 take precedence)}	B05B11/10	B05B11/10		314
B05B11/1029	11	{actuated by a lever}	B05B11/10	B05B11/10		53
B05B11/103	12	{without substantial movement of the nozzle in the direction of the pressure stroke}	B05B11/10	B05B11/10		209
B05B11/1032	11	{actuated without substantial movement of the nozzle in the direction of the pressure stroke (B05B11/103 takes precedence)}	B05B11/10	B05B11/10		503
B05B11/1033	11	{the deformable wall, the inlet and outlet valve elements being integrally formed, e.g. moulded}	B05B11/10	B05B11/10		213
B05B11/1035	11	{the pumping chamber being a bellow}	B05B11/10	B05B11/10		433
B05B11/1036	11	{the outlet valve being opened in the direction opposite to the fluid flow downstream the outlet valve by the pressure acting on a valve controlling element}	B05B11/10	B05B11/10		45
B05B11/1038	10	{Pressure accumulation pumps, i.e. pumps comprising a pressure accumulation chamber}	B05B11/10	B05B11/10		87
B05B11/1039	11	{the outlet valve being mechanically opened after a defined accumulation stroke}	B05B11/10	B05B11/10		158
B05B11/104	11	{the outlet valve being opened by pressure after a defined accumulation stroke}	B05B11/10	B05B11/10		232
B05B11/1042	10	{Components or details}	B05B11/10	B05B11/10		858
B05B11/1043	11	{Sealing or attachment arrangements between pump and container (sealing arrangements around pump actuating stem B05B11/105)}	B05B11/10	B05B11/10		280
B05B11/1045	12	{the pump being preassembled as an independent unit before being mounted on the container (B05B11/1047, B05B11/1049 take precedence)}	B05B11/10	B05B11/10		320
B05B11/1046	12	{the pump chamber being arranged substantially coaxially to the neck of the container (B05B11/1049 takes precedence)}	B05B11/10	B05B11/10		110
B05B11/1047	13	{the pump being preassembled as an independent unit before being mounted on the container}	B05B11/10	B05B11/10		3213
B05B11/1049	12	{Attachment arrangements comprising a deformable or resilient ferrule clamped or locked onto the neck of the container by displacing, e.g. sliding, a sleeve surrounding the ferrule}	B05B11/10	B05B11/10		214
B05B11/105	11	{Sealing arrangements around pump actuating stem}	B05B11/10	B05B11/10		267
B05B11/1052	11	{Actuation means (locking means therefor B05B11/1059; the dispensing stroke being affected by the stored energy of a spring B05B11/109)}	B05B11/10	B05B11/10		997
B05B11/1053	12	{combined with means, other than pressure, for automatically opening a valve during actuation; combined with means for automatically removing closures or covers from the discharge nozzle during actuation}	B05B11/10	B05B11/10		452
B05B11/1054	13	{the valve being located upstream of an outlet valve}	B05B11/10	B05B11/10		62
B05B11/1056	12	{comprising rotatable or articulated levers (B05B11/1053 takes precedence; lever actuated piston pumps B05B11/1009; lever actuated pumps with deformable chamber B05B11/1029)}	B05B11/10	B05B11/10		270
B05B11/1057	13	{Triggers, i.e. actuation means consisting of a single lever having one end rotating or pivoting around an axis or a hinge fixedly attached to the container, and another end directly actuated by the user}	B05B11/10	B05B11/10		960
B05B11/1059	11	{Means for locking a pump or its actuation means in a fixed position (B05B11/1091 takes precedence)}	B05B11/10	B05B11/10		1258
B05B11/106	12	{in a retracted position, e.g. in an end-of-dispensing-stroke position}	B05B11/10	B05B11/10		668
B05B11/1061	11	{Pump priming means}	B05B11/10	B05B11/10		186
B05B11/1063	12	{Air exhausted from the pump chamber being discharged into the container during priming}	B05B11/10	B05B11/10		70
B05B11/1064	11	{Pump inlet and outlet valve elements integrally formed of a deformable material (pump chambers having a deformable wall integrally formed with inlet and outlet valve elements B05B11/1033)}	B05B11/10	B05B11/10		240
B05B11/1066	11	{Pump inlet valves (B05B11/1018, B05B11/1019, B05B11/1064 take precedence)}	B05B11/10	B05B11/10		196
B05B11/1067	12	{actuated by pressure}	B05B11/10	B05B11/10		750
B05B11/1069	13	{the valve being made of a resiliently deformable material or being urged in a closed position by a spring}	B05B11/10	B05B11/10		856
B05B11/107	12	{Gate valves; Sliding valves}	B05B11/10	B05B11/10		162
B05B11/1071	12	{Two inlet valves being placed in a supply conduit one upstream of the other}	B05B11/10	B05B11/10		26
B05B11/1073	11	{Springs}	B05B11/10	B05B11/10		362
B05B11/1074	12	{located outside pump chambers}	B05B11/10	B05B11/10		2151
B05B11/1076	12	{Traction springs, e.g. stretchable sleeve}	B05B11/10	B05B11/10		97
B05B11/1077	12	{characterised by a particular shape or material (B05B11/1076 takes precedence)}	B05B11/10	B05B11/10		1184
B05B11/1078	12	{Vacuum chambers acting like springs}	B05B11/10	B05B11/10		68
B05B11/108	11	{Means for counting the number of dispensing strokes}	B05B11/10	B05B11/10		203
B05B11/1081	10	{Arrangements for pumping several liquids or other fluent materials from several containers, e.g. for mixing them at the moment of pumping}	B05B11/10	B05B11/10		285
B05B11/1083	11	{in adjustable proportion}	B05B11/10	B05B11/10		106
B05B11/1084	11	{each liquid or other fluent material being pumped by a separate pump}	B05B11/10	B05B11/10		652
B05B11/1085	12	{the pumps being coaxial}	B05B11/10	B05B11/10		61
B05B11/1087	10	{Combination of liquid and air pumps}	B05B11/10	B05B11/10		784
B05B11/1088	10	{the pump being a double-acting pump}	B05B11/10	B05B11/10		56
B05B11/109	10	{the dispensing stroke being affected by the stored energy of a spring (B05B11/1088 takes precedence)}	B05B11/10	B05B11/10		142
B05B11/1091	11	{being first hold in a loaded state by locking means or the like, then released (B05B11/1092 takes precedence)}	B05B11/10	B05B11/10		181
B05B11/1092	11	{automatically released from a loaded state at the end of the loading stroke}	B05B11/10	B05B11/10		76
B05B11/1094	10	{having inlet or outlet valves not being actuated by pressure or having no inlet or outlet valve}	B05B11/10	B05B11/10		200
B05B11/1095	10	{with movable suction side}	B05B11/10	B05B11/10		159
B05B11/1097	10	{with means for sucking back the liquid or other fluent material in the nozzle after a dispensing stroke}	B05B11/10	B05B11/10		240
B05B11/1098	10	{Air being permanently entrapped or sucked into the liquid pump chamber}	B05B11/10	B05B11/10		52
B05B12/00	7	Arrangements for controlling delivery; Arrangements for controlling the spray area	B05B12/00	B05B12/00		2632
B05B12/002	8	{Manually-actuated controlling means, e.g. push buttons, levers or triggers (for single units B05B11/00)}	B05B12/00	B05B12/00		2100
B05B12/0022	9	{associated with means for restricting their movement}	B05B12/00	B05B12/00		219
B05B12/0024	10	{to a single position}	B05B12/00	B05B12/00		253
B05B12/0026	11	{to inhibit delivery}	B05B12/00	B05B12/00		243
B05B12/004	8	{comprising sensors for monitoring the delivery, e.g. by displaying the sensed value or generating an alarm (B05B12/08 takes precedence; registering or indicating the condition or the working of machines or other apparatus in general G07C3/00)}	B05B12/00	B05B12/00		992
B05B12/006	9	{Pressure or flow rate sensors}	B05B12/00	B05B12/00		518
B05B12/008	10	{integrated in or attached to a discharge apparatus, e.g. a spray gun}	B05B12/00	B05B12/00		422
B05B12/02	8	for controlling time, or sequence, of delivery	B05B12/02	B05B12/02		1415
B05B12/04	9	for sequential operation or multiple outlets<br><br><u>WARNING</u><br>Group B05B12/04 is impacted by reclassification into group B05B13/002. <br>Groups B05B12/04 and B05B13/002 should be considered in order to perform a complete search.	B05B12/04	B05B12/04		948
B05B12/06	9	for effecting pulsating flow {(nozzles, spray heads or other outlets with means for generating a discharge of pulsating nature B05B1/08)}	B05B12/06	B05B12/06		465
B05B12/08	8	responsive to condition of liquid or other fluent material {to be} discharged, of ambient medium or of target {; responsive to condition of spray devices or of supply means, e.g. pipes, pumps or their drive means}	B05B12/08	B05B12/08		1252
B05B12/081	9	{responsive to the weight of a reservoir or container for liquid or other fluent material; responsive to level or volume of liquid or other fluent material in a reservoir or container}	B05B12/08	B05B12/08		791
B05B12/082	9	{responsive to a condition of the discharged jet or spray, e.g. to jet shape, spray pattern or droplet size}	B05B12/08	B05B12/08		683
B05B12/084	9	{responsive to condition of liquid or other fluent material already sprayed on the target, e.g. coating thickness, weight or pattern}	B05B12/08	B05B12/08		1136
B05B12/085	9	{responsive to flow or pressure of liquid or other fluent material to be discharged (B05B1/3006, B05B1/323 take precedence; spray pistols designed to control volume of flow with the controlling means being fluid actuated B05B7/1254)}	B05B12/08	B05B12/08		1328
B05B12/087	10	{Flow or presssure regulators, i.e. non-electric unitary devices comprising a sensing element, e.g. a piston or a membrane, and a controlling element, e.g. a valve}	B05B12/08	B05B12/08		830
B05B12/088	11	{the sensing element being a flexible member, e.g. membrane, diaphragm, bellows}	B05B12/08	B05B12/08		159
B05B12/10	9	responsive to temperature or viscosity of liquid or other fluent material discharged	B05B12/10	B05B12/10		510
B05B12/12	9	responsive to conditions of ambient medium or target, e.g. humidity, temperature {position or movement of the target relative to the spray apparatus (B05B12/082, B05B12/084 take precedence)}	B05B12/12	B05B12/12		2338
B05B12/122	10	{responsive to presence or shape of target (B05B12/124 takes precedence)}	B05B12/12	B05B12/12		2130
B05B12/124	10	{responsive to distance between spray apparatus and target}	B05B12/12	B05B12/12		1145
B05B12/126	10	{responsive to target velocity, e.g. to relative velocity between spray apparatus and target (B05B9/06 takes precedence)}	B05B12/12	B05B12/12		300
B05B12/14	8	for supplying a selected one of a plurality of liquids or other fluent materials {or several in selected proportions} to a {spray apparatus, e.g. to a} single spray outlet	B05B12/14	B05B12/14		861
B05B12/1409	9	{the selection means being part of the discharge apparatus, e.g. part of the spray gun}	B05B12/14	B05B12/14		291
B05B12/1418	9	{for supplying several liquids or other fluent materials in selected proportions to a single spray outlet (controlling ratio of two or more flows of fluid G05D11/02)}	B05B12/14	B05B12/14		836
B05B12/1427	10	{a condition of a first liquid or other fluent material in a first supply line controlling a condition of a second one in a second supply line}	B05B12/14	B05B12/14		12
B05B12/1436	11	{the controlling condition of the first liquid or other fluent material in the first supply line being its flow rate or its pressure}	B05B12/14	B05B12/14		72
B05B12/1445	10	{pumping means for the liquids or other fluent materials being mechanically linked, e.g. leader-follower pumps}	B05B12/14	B05B12/14		63
B05B12/1454	9	{separate units comprising both a material container and a spray device permanently connected thereto being removably attached to a part of the spray apparatus, e.g. to a robot arm}	B05B12/14	B05B12/14		49
B05B12/1463	9	{separate containers for different materials to be sprayed being moved from a first location, e.g. a filling station, where they are fluidically disconnected from the spraying apparatus, to a second location, generally close to the spraying apparatus, where they are fluidically connected to the latter (B05B12/1454 takes precedence)}	B05B12/14	B05B12/14		119
B05B12/1472	9	{separate supply lines supplying different materials to separate outlets of the spraying apparatus (B05B12/1454 takes precedence)}<br><br><u>WARNING</u><br>Group B05B12/1472 is impacted by reclassification into group B05B13/002. <br>Groups B05B12/1472 and B05B13/002 should be considered in order to perform a complete search.	B05B12/14	B05B12/14		325
B05B12/1481	9	{comprising pigs, i.e. movable elements sealingly received in supply pipes, for separating different fluids, e.g. liquid coating materials from solvent or air (cleaning pipes with pigs B08B9/0557, pigs per seF16L55/26)}	B05B12/14	B05B12/14		151
B05B12/149	9	{characterised by colour change manifolds or valves therefor (B05B12/1409 takes precedence)}	B05B12/14	B05B12/14		353
B05B12/16	8	for controlling the spray area (B05B3/00 takes precedence)	B05B12/16	B05B12/16		1426
B05B12/18	9	using fluids, e.g. gas streams	B05B12/18	B05B12/18		1111
B05B12/20	9	Masking elements, i.e. elements defining uncoated areas on an object to be coated	B05B12/20	B05B12/20		1415
B05B12/22	10	movable relative to the spray area	B05B12/22	B05B12/22		242
B05B12/24	10	made at least partly of flexible material, e.g. sheets of paper or fabric	B05B12/24	B05B12/24		935
B05B12/26	10	for masking cavities	B05B12/26	B05B12/26		409
B05B12/265	11	{between a door and a post, e.g. foam strips}	B05B12/26	B05B12/26		78
B05B12/28	10	for defining uncoated areas that are not enclosed within coated areas or vice versa, e.g. for defining U-shaped border lines	B05B12/28	B05B12/28		288
B05B12/29	10	{with adjustable size}	B05B12/20	B05B12/29		88
B05B12/30	10	specially adapted for vehicle wheels	B05B12/30	B05B12/30		161
B05B12/32	9	Shielding elements, i.e. elements preventing overspray from reaching areas other than the object to be sprayed (nozzles with integral shielding elements B05B1/28)	B05B12/32	B05B12/32		1218
B05B12/34	10	movable relative to the spray area	B05B12/34	B05B12/34		206
B05B12/36	10	Side shields, i.e. shields extending in a direction substantially parallel to the spray jet	B05B12/36	B05B12/36		444
B05B12/40	9	{Devices for making a normally hidden area accessible for the spray material}	B05B12/16	B05B12/40		52
B05B13/00	7	Machines or plants for applying liquids or other fluent materials to surfaces of objects or other work by spraying, not covered by groups B05B1/00 - B05B11/00(means for supplying or discharging liquid or other fluent material for this purpose, see the relevant one of groups B05B1/00 - B05B12/00; processes for applying liquids or other fluent materials to surfaces in general B05D)	B05B13/00	B05B13/00		698
B05B13/002	8	{Machines or plants for applying coating liquids or other fluent materials by inkjet}<br><br><u>WARNING</u><br>Group B05B13/002 is incomplete pending reclassification of documents from groups B05B1/14, B05B12/04, B05B12/1472, B05B13/0431 and B05B13/0452. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B13/00	B05B13/00		26
B05B13/005	8	{mounted on vehicles or designed to apply a liquid on a very large surface, e.g. on the road, on the surface of large containers}	B05B13/00	B05B13/00		1873
B05B13/02	8	Means for supporting work; Arrangement or mounting of spray heads; Adaptation or arrangement of means for feeding work (B05B13/06 takes precedence)	B05B13/02	B05B13/02		2762
B05B13/0207	9	{the work being an elongated body, e.g. wire or pipe (B05B13/0436, B05B13/0463 take precedence)}	B05B13/02	B05B13/02		1172
B05B13/0214	10	{the liquid or other fluent material being applied to the whole periphery of the cross section of the elongated body}	B05B13/02	B05B13/02		574
B05B13/0221	9	{characterised by the means for moving or conveying the objects or other work, e.g. conveyor belts (B05B13/0207 takes precedence; conveyors in general B65G)}	B05B13/02	B05B13/02		6670
B05B13/0228	10	{the movement of the objects being rotative (B05B13/0242 takes precedence)}	B05B13/02	B05B13/02		4848
B05B13/0235	10	{the movement of the objects being a combination of rotation and linear displacement (B05B13/0242 takes precedence)}	B05B13/02	B05B13/02		1047
B05B13/0242	10	{the objects being individually presented to the spray heads by a rotating element, e.g. turntable}	B05B13/02	B05B13/02		865
B05B13/025	10	{the objects or work being present in bulk}	B05B13/02	B05B13/02		592
B05B13/0257	11	{in a moving container, e.g. a rotatable foraminous drum}	B05B13/02	B05B13/02		279
B05B13/0264	10	{Overhead conveying means, i.e. the object or other work being suspended from the conveying means; Details thereof, e.g. hanging hooks}	B05B13/02	B05B13/02		1396
B05B13/0271	10	{the object or work standing still during the spraying operation}	B05B13/02	B05B13/02		741
B05B13/0278	9	{Arrangement or mounting of spray heads (B05B13/0207 takes precedence)}	B05B13/02	B05B13/02		7345
B05B13/0285	9	{Stands for supporting individual articles to be sprayed, e.g. doors, vehicle body parts}	B05B13/02	B05B13/02		2590
B05B13/0292	9	{devices for holding several workpieces to be sprayed in a spaced relationship, e.g. vehicle doors spacers}	B05B13/02	B05B13/02		794
B05B13/04	9	the spray heads being moved during {spraying} operation	B05B13/04	B05B13/04		1823
B05B13/0405	10	{with reciprocating or oscillating spray heads (B05B13/0436, B05B13/0442, B05B13/0447, B05B13/0468 take precedence)}	B05B13/04	B05B13/04		1109
B05B13/041	11	{with spray heads reciprocating along a straight line}	B05B13/04	B05B13/04		4304
B05B13/0415	12	{the angular position of the spray heads relative to the straight line being modified during the reciprocating movement}	B05B13/04	B05B13/04		309
B05B13/0421	10	{with rotating spray heads}	B05B13/04	B05B13/04		1574
B05B13/0426	10	{with spray heads moved along a closed path (B05B13/0421 takes precedence)}	B05B13/04	B05B13/04		490
B05B13/0431	10	{with spray heads moved by robots or articulated arms, e.g. for applying liquid or other fluent material to three-dimensional [3D] surfaces}<br><br><u>WARNING</u><br>Group B05B13/0431 is incomplete pending reclassification of documents from group B05B13/0457. Group B05B13/0431 is also impacted by reclassification into groups B05B13/002 and B05B13/0433. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B05B13/04	B05B13/04		3278
B05B13/0433	11	{the work being vehicle components, e.g. vehicle bodies}<br><br><u>WARNING</u><br>Group B05B13/0433 is incomplete pending reclassification of documents from groups B05B13/0431 and B05B13/0452. <br>Groups B05B13/0431, B05B13/0452 and B05B13/0433 should be considered in order to perform a complete search.	B05B13/04	B05B13/04		20
B05B13/0436	10	{Installations or apparatus for applying liquid or other fluent material to elongated bodies, e.g. light poles, pipes (B05B13/0442, B05B13/0463 take precedence)}	B05B13/04	B05B13/04		462
B05B13/0442	10	{Installation or apparatus for applying liquid or other fluent material to separate articles rotated during spraying operation}	B05B13/04	B05B13/04		698
B05B13/0447	10	{Installation or apparatus for applying liquid or other fluent material to conveyed separate articles (B05B13/0442 takes precedence)}	B05B13/04	B05B13/04		353
B05B13/0452	11	{the objects being vehicle components, e.g. vehicle bodies}<br><br><u>WARNING</u><br>Group B05B13/0452 is impacted by reclassification into groups B05B13/002 and B05B13/0433. <br>Groups B05B13/0452, B05B13/002 and B05B13/0433 should be considered in order to perform a complete search.	B05B13/04	B05B13/04		752
B05B13/0457	11	{specially designed for applying liquid or other fluent material to three-dimensional [3D] surfaces of the work, e.g. by using several moving spray heads (B05B13/0431, B05B13/0452 take precedence)}<br><br><u>WARNING</u><br>Group B05B13/0457 is impacted by reclassification into group B05B13/0431. <br>Groups B05B13/0457 and B05B13/0431 should be considered in order to perform a complete search.	B05B13/04	B05B13/04		193
B05B13/0463	10	{Installation or apparatus for applying liquid or other fluent material to moving work of indefinite length}	B05B13/04	B05B13/04		67
B05B13/0468	11	{with reciprocating or oscillating spray heads}	B05B13/04	B05B13/04		103
B05B13/0473	12	{with spray heads reciprocating along a straight line}	B05B13/04	B05B13/04		228
B05B13/0478	13	{the angular position of the spray heads relative to the straight line being modified during the reciprocating movement}	B05B13/04	B05B13/04		28
B05B13/0484	11	{with spray heads having a circular motion, e.g. being attached to a rotating supporting element (B05B13/0468 takes precedence)}	B05B13/04	B05B13/04		96
B05B13/0489	12	{around the moving work}	B05B13/04	B05B13/04		27
B05B13/0494	11	{with spray heads being moved along a closed path (B05B13/0484 takes precedence)}	B05B13/04	B05B13/04		35
B05B13/06	8	specially designed for treating the inside of hollow bodies (spray heads B05B1/00&#160;-&#160;B05B7/00; {devices for covering leaks in pipes or hoses, e.g. hose-menders, from inside the pipe F16L55/162; sprayed layers of rubber or plastics for internal protection of pipes or pipe fittings against corrosion or incrustation F16L58/1027})	B05B13/06	B05B13/06		818
B05B13/0609	9	{the hollow bodies being automatically fed to, or removed from, the machine}	B05B13/06	B05B13/06		329
B05B13/0618	9	{only a part of the inside of the hollow bodies being treated}	B05B13/06	B05B13/06		231
B05B13/0627	9	{Arrangements of nozzles or spray heads specially adapted for treating the inside of hollow bodies (B05B13/0645 takes precedence)}	B05B13/06	B05B13/06		1314
B05B13/0636	10	{by means of rotatable spray heads or nozzles}	B05B13/06	B05B13/06		1204
B05B13/0645	9	{the hollow bodies being rotated during treatment operation (B05B13/0618 takes precedence)}	B05B13/06	B05B13/06		280
B05B13/0654	10	{and a treating nozzles being translated through the hollow bodies in a direction essentially parallel to the rotational axis (B05B13/0681 takes precedence)}	B05B13/06	B05B13/06		207
B05B13/0663	10	{and the hollow bodies being translated in a direction parallel to the rotational axis (B05B13/0681 takes precedence)}	B05B13/06	B05B13/06		52
B05B13/0672	10	{and the inclination or the distance of a treating nozzle being modified relative to the rotation axis, e.g. for treating irregular internal surfaces}	B05B13/06	B05B13/06		29
B05B13/0681	10	{the hollow bodies comprising a closed end to be treated (B05B13/0672 takes precedence)}	B05B13/06	B05B13/06		86
B05B13/069	9	{the hollow bodies having a closed end}	B05B13/06	B05B13/06		214
B05B14/00	7	Arrangements for collecting, re-using or eliminating excess spraying material (arrangements integral with nozzles B05B1/28)	B05B14/00	B05B14/00		3589
B05B14/10	8	the excess material being particulate (for spray booths B05B14/48)	B05B14/10	B05B14/10		534
B05B14/20	8	from moving belts, e.g. filtering belts or conveying belts	B05B14/20	B05B14/20		179
B05B14/30	8	comprising enclosures close to, or in contact with, the object to be sprayed and surrounding or confining the discharged spray or jet but not the object to be sprayed	B05B14/30	B05B14/30		459
B05B14/40	8	for use in spray booths	B05B14/40	B05B14/40		1854
B05B14/41	9	by cleaning the walls of the booth	B05B14/41	B05B14/41		254
B05B14/412	10	{wherein the walls of the booth is perforated or porous walls and the walls are cleaned of or prevented from being contacted with excess material by a flow of fluid, e.g. air or water, directed into the booth}	B05B14/41	B05B14/41		36
B05B14/42	9	using electrostatic means	B05B14/42	B05B14/42		120
B05B14/43	9	by filtering the air charged with excess material	B05B14/43	B05B14/43		1489
B05B14/435	10	with means for cleaning the filters by gas flow, e.g. blasts of air	B05B14/435	B05B14/435		124
B05B14/437	10	{with means for introducing solid material into the air charged with excess material for preventing clogging of the filter}	B05B14/43	B05B14/43		41
B05B14/44	9	using walls specially adapted for promoting separation of the excess material from the air, e.g. baffle plates (using wetted walls B05B14/465)	B05B14/44	B05B14/44		156
B05B14/45	9	using cyclone separators	B05B14/45	B05B14/45		232
B05B14/46	9	by washing the air charged with excess material	B05B14/46	B05B14/46		801
B05B14/462	10	and separating the excess material from the washing liquid, e.g. for recovery	B05B14/462	B05B14/462		341
B05B14/463	11	{by means of ultrafiltration}	B05B14/462	B05B14/46		38
B05B14/465	10	using substantially vertical liquid curtains or wetted walls behind the object to be sprayed	B05B14/465	B05B14/465		484
B05B14/468	10	with scrubbing means arranged below the booth floor	B05B14/468	B05B14/468		285
B05B14/469	10	{wherein the washing material is the spraying material}	B05B14/46	B05B14/46		43
B05B14/48	9	specially adapted for particulate material	B05B14/48	B05B14/48		929
B05B14/49	9	specially adapted for solvents	B05B14/49	B05B14/49		159
B05B15/00	7	Details of spraying plant or spraying apparatus not otherwise provided for; Accessories	B05B15/00	B05B15/00		4852
B05B15/14	8	Arrangements for preventing or controlling structural damage to spraying apparatus or its outlets, e.g. for breaking at desired places; Arrangements for handling or replacing damaged parts	B05B15/14	B05B15/14		570
B05B15/16	9	for preventing non-intended contact between spray heads or nozzles and foreign bodies, e.g. nozzle guards	B05B15/16	B05B15/16		881
B05B15/18	9	for improving resistance to wear, e.g. inserts or coatings; for indicating wear; for handling or replacing worn parts	B05B15/18	B05B15/18		440
B05B15/20	8	Arrangements for agitating the material to be sprayed, e.g. for stirring, mixing or homogenising	B05B15/20	B05B15/20		730
B05B15/25	9	using moving elements, e.g. rotating blades	B05B15/25	B05B15/25		4645
B05B15/30	8	Dip tubes	B05B15/30	B05B15/30		1127
B05B15/33	9	Weighted	B05B15/33	B05B15/33		116
B05B15/37	9	with decorative elements	B05B15/37	B05B15/37		40
B05B15/40	8	Filters located upstream of the spraying outlets	B05B15/40	B05B15/40		2387
B05B15/50	8	Arrangements for cleaning; Arrangements for preventing deposits, drying-out or blockage; Arrangements for detecting improper discharge caused by the presence of foreign matter	B05B15/50	B05B15/50		3905
B05B15/52	9	for removal of clogging particles	B05B15/52	B05B15/52		996
B05B15/522	10	using cleaning elements penetrating the discharge openings	B05B15/522	B05B15/522		197
B05B15/5223	11	{the cleaning element, e.g. a needle, and the discharge opening being movable relative to each other in a direction substantially parallel to the flow of liquid or other fluent material through said opening}	B05B15/522	B05B15/522		164
B05B15/5225	12	{the cleaning element being located upstream of the discharge opening or being actuated upstream therefrom}	B05B15/522	B05B15/522		368
B05B15/525	10	by increasing the cross section of the discharge openings	B05B15/525	B05B15/525		97
B05B15/528	10	by resilient deformation of the nozzle	B05B15/528	B05B15/528		159
B05B15/531	10	using backflow	B05B15/531	B05B15/531		98
B05B15/534	11	by reversing the nozzle relative to the supply conduit	B05B15/534	B05B15/534		188
B05B15/55	9	using cleaning fluids	B05B15/55	B05B15/55		2293
B05B15/555	10	discharged by cleaning nozzles	B05B15/555	B05B15/555		1043
B05B15/557	10	{the cleaning fluid being a mixture of gas and liquid}	B05B15/55	B05B15/55		147
B05B15/58	9	preventing deposits, drying-out or blockage by recirculating the fluid to be sprayed from upstream of the discharge opening back to the supplying means {(B05B1/3093 takes precedence)}	B05B15/58	B05B15/58		431
B05B15/60	8	Arrangements for mounting, supporting or holding spraying apparatus	B05B15/60	B05B15/60		1556
B05B15/62	9	Arrangements for supporting spraying apparatus, e.g. suction cups	B05B15/62	B05B15/62		2371
B05B15/622	10	ground-penetrating	B05B15/622	B05B15/622		437
B05B15/625	10	designed to be placed on the ground	B05B15/625	B05B15/625		718
B05B15/628	10	of variable length	B05B15/628	B05B15/628		738
B05B15/63	9	Handgrips	B05B15/63	B05B15/63		581
B05B15/65	9	Mounting arrangements for fluid connection of the spraying apparatus or its outlets to flow conduits	B05B15/65	B05B15/65		2206
B05B15/652	10	whereby the jet can be oriented	B05B15/652	B05B15/652		1196
B05B15/654	11	using universal joints	B05B15/654	B05B15/654		669
B05B15/656	10	whereby the flow conduit length is changeable	B05B15/656	B05B15/656		515
B05B15/658	10	the spraying apparatus or its outlet axis being perpendicular to the flow conduit	B05B15/658	B05B15/658		726
B05B15/68	9	Arrangements for adjusting the position of spray heads (B05B15/628, B05B15/652, B05B15/656 take precedence)	B05B15/68	B05B15/68		7282
B05B15/70	8	Arrangements for moving spray heads automatically to or from the working position	B05B15/70	B05B15/70		700
B05B15/72	9	using hydraulic or pneumatic means	B05B15/72	B05B15/72		122
B05B15/74	10	driven by the discharged fluid	B05B15/74	B05B15/74		1052
B05B15/80	8	Arrangements in which the spray area is not enclosed, e.g. spray tables	B05B15/80	B05B15/80		234
B05B16/00	7	Spray booths (arrangements for collecting, re-using or eliminating excess spraying material in spray booths B05B14/40)	B05B16/00	B05B16/00		1175
B05B16/20	8	Arrangements for spraying in combination with other operations, e.g. drying; Arrangements enabling a combination of spraying operations	B05B16/20	B05B16/20		7839
B05B16/25	9	for both automatic and manual spraying	B05B16/25	B05B16/25		90
B05B16/40	8	Construction elements specially adapted therefor, e.g. floors, walls or ceilings (ceiling elements filtering inflow of air into the booth B05B16/60; walls specially adapted for promoting separation of excess material B05B14/44)	B05B16/40	B05B16/40		2077
B05B16/405	9	{Partly or totally cylindrical walls; Round floors}	B05B16/40	B05B16/40		100
B05B16/60	8	Ventilation arrangements specially adapted therefor	B05B16/60	B05B16/60		1557
B05B16/80	8	Movable spray booths	B05B16/80	B05B16/80		328
B05B16/90	8	{comprising conveying means for moving objects or other work to be sprayed in and out of the booth, e.g. through the booth}	B05B16/00	B05B16/90		725
B05B16/95	9	{the objects or other work to be sprayed lying on, or being held above the conveying means, i.e. not hanging from the conveying means}	B05B16/00	B05B16/95		1180
B05B17/00	7	Apparatus for spraying or atomising liquids or other fluent materials, not covered by the preceding groups (dropping or releasing powdered, liquid or gaseous matter in flight B64D1/16)	B05B17/00	B05B17/00		280
B05B17/04	8	operating with special methods	B05B17/04	B05B17/04		662
B05B17/06	9	using ultrasonic {or other kinds of} vibrations	B05B17/06	B05B17/06		1564
B05B17/0607	10	{generated by electrical means, e.g. piezoelectric transducers}	B05B17/06	B05B17/06		1426
B05B17/0615	11	{spray being produced at the free surface of the liquid or other fluent material in a container and subjected to the vibrations}	B05B17/06	B05B17/06		1184
B05B17/0623	11	{coupled with a vibrating horn}	B05B17/06	B05B17/06		610
B05B17/063	12	{having an internal channel for supplying the liquid or other fluent material}	B05B17/06	B05B17/06		419
B05B17/0638	11	{spray being produced by discharging the liquid or other fluent material through a plate comprising a plurality of orifices}	B05B17/00	B05B17/06		353
B05B17/0646	12	{Vibrating plates, i.e. plates being directly subjected to the vibrations, e.g. having a piezoelectric transducer attached thereto}	B05B17/00	B05B17/06		1478
B05B17/0653	11	{Details}	B05B17/06	B05B17/06		444
B05B17/0661	12	{Transducer materials}	B05B17/06	B05B17/06		126
B05B17/0669	12	{Excitation frequencies}	B05B17/06	B05B17/06		275
B05B17/0676	12	{Feeding means}	B05B17/06	B05B17/06		352
B05B17/0684	13	{Wicks or the like}	B05B17/06	B05B17/06		592
B05B17/0692	10	{generated by a fluid (B05B17/0607 takes precedence)}	B05B17/06	B05B17/06		198
B05B17/08	8	Fountains (drinking fountains E03B9/20; wash fountains E03C1/16)	B05B17/08	B05B17/08		2527
B05B17/085	9	{designed to produce sheets or curtains of liquid, e.g. water walls}	B05B17/08	B05B17/08		555
