B30B1/00	7	Presses, using a press ram, characterised by the features of the drive therefor, pressure being transmitted directly, or through simple thrust or tension members only, to the press ram or platen	B30B1/00	B30B1/00		397
B30B1/001	8	{by explosive charges}	B30B1/00	B30B1/00		78
B30B1/002	8	{by internal combustion mechanism}	B30B1/00	B30B1/00		19
B30B1/003	8	{by an elastic bag or diaphragm expanded by fluid pressure}	B30B1/00	B30B1/00		270
B30B1/005	8	{by thermal expansion or evaporation}	B30B1/00	B30B1/00		56
B30B1/006	8	{by a scissor or lazy-tongs mechanism}	B30B1/00	B30B1/00		147
B30B1/007	8	{using a fluid connection between the drive means and the press ram}	B30B1/00	B30B1/00		99
B30B1/008	8	{by a rod swinging between a fixed plane and the ram}	B30B1/00	B30B1/00		182
B30B1/02	8	by lever mechanism (by toggle mechanism B30B1/10)	B30B1/02	B30B1/02		179
B30B1/04	9	operated by hand or foot	B30B1/04	B30B1/04		296
B30B1/06	9	operated by cams, eccentrics, or cranks	B30B1/06	B30B1/06		298
B30B1/08	9	operated by fluid-pressure means	B30B1/08	B30B1/08		198
B30B1/10	8	by toggle mechanism	B30B1/10	B30B1/10		284
B30B1/103	9	{operated by screw means}	B30B1/10	B30B1/10		309
B30B1/106	9	{operated by another toggle mechanism}	B30B1/10	B30B1/10		128
B30B1/12	9	operated by hand or foot	B30B1/12	B30B1/12		113
B30B1/14	9	operated by cams, eccentrics, or cranks	B30B1/14	B30B1/14		795
B30B1/16	9	operated by fluid-pressure means	B30B1/16	B30B1/16		332
B30B1/18	8	by screw means {(B30B9/3064 takes precedence)}	B30B1/18	B30B1/18		948
B30B1/181	9	{the screw being directly driven by an electric motor}	B30B1/18	B30B1/18		207
B30B1/183	9	{Braking mechanisms for the return movement of the press ram}	B30B1/18	B30B1/18		34
B30B1/185	9	{driven through friction roller means}	B30B1/18	B30B1/18		54
B30B1/186	9	{Control arrangements}	B30B1/18	B30B1/18		205
B30B1/188	9	{driven by a continuously rotatable flywheel with a coupling arranged between the flywheel and the screw}	B30B1/18	B30B1/18		98
B30B1/20	9	driven by hand	B30B1/20	B30B1/20		215
B30B1/22	9	driven through friction disc means	B30B1/22	B30B1/22		256
B30B1/23	9	operated by fluid-pressure means	B30B1/23	B30B1/23		102
B30B1/24	8	by rack-and-pinion means {(B30B9/3067 takes precedence)}	B30B1/24	B30B1/24		367
B30B1/26	8	by cams, eccentrics, or cranks	B30B1/26	B30B1/26		886
B30B1/261	9	{by cams}	B30B1/26	B30B1/26		430
B30B1/263	9	{work stroke adjustment means}	B30B1/26	B30B1/26		282
B30B1/265	9	{using a fluid connecting unit between drive shaft and press ram}	B30B1/26	B30B1/26		137
B30B1/266	9	{Drive systems for the cam, eccentric or crank axis}	B30B1/26	B30B1/26		927
B30B1/268	9	{using a toggle connection between driveshaft and press ram}	B30B1/26	B30B1/26		186
B30B1/28	9	the cam, crank, or eccentric being disposed below the lower platen or table and operating to pull down the upper platen or slide	B30B1/28	B30B1/28		214
B30B1/30	8	by the pull of chains or ropes {(B30B9/3071 takes precedence)}	B30B1/30	B30B1/30		105
B30B1/32	8	by plungers under fluid pressure	B30B1/32	B30B1/32		1980
B30B1/323	9	{using low pressure long stroke opening and closing means, and high pressure short stroke cylinder means}	B30B1/32	B30B1/32		171
B30B1/326	9	{operated by hand or foot, e.g. using hydraulic jacks}	B30B1/32	B30B1/32		98
B30B1/34	9	involving a plurality of plungers acting on the platen (gas operated B30B1/38)	B30B1/34	B30B1/34		426
B30B1/36	9	having telescoping plungers (gas operated B30B1/38)	B30B1/36	B30B1/36		77
B30B1/38	9	wherein the plungers are operated by pressure of a gas, e.g. steam, air	B30B1/38	B30B1/38		483
B30B1/40	8	by wedge means	B30B1/40	B30B1/40		239
B30B1/42	8	by magnetic means, e.g. electromagnetic	B30B1/42	B30B1/42		304
B30B3/00	7	Presses characterised by the use of rotary pressing members, e.g. rollers, rings, discs	B30B3/00	B30B3/00		408
B30B3/005	8	{Roll constructions}	B30B3/00	B30B3/00		519
B30B3/02	8	co-operating with a fixed member	B30B3/02	B30B3/02		123
B30B3/04	8	co-operating with one another, e.g. with co-operating cones	B30B3/04	B30B3/04		779
B30B3/045	9	{with co-operating cones}	B30B3/04	B30B3/04		60
B30B3/06	9	arranged one within another, e.g. with a roller disposed within a rotating ring and co-operating with the inner surface thereof	B30B3/06	B30B3/06		28
B30B5/00	7	Presses characterised by the use of pressing means other than those mentioned in the preceding groups	B30B5/00	B30B5/00		68
B30B5/02	8	wherein the pressing means is in the form of a flexible element, e.g. diaphragm, urged by fluid pressure	B30B5/02	B30B5/02		773
B30B5/04	8	wherein the pressing means is in the form of an endless band	B30B5/04	B30B5/04		196
B30B5/06	9	co-operating with another endless band	B30B5/06	B30B5/06		958
B30B5/062	10	{urged by directly-acting fluid pressure}	B30B5/06	B30B5/06		118
B30B5/065	10	{using anti-friction means for the pressing band}	B30B5/06	B30B5/06		53
B30B5/067	11	{using anti-friction roller means}	B30B5/06	B30B5/06		274
B30B7/00	7	Presses characterised by a particular arrangement of the pressing members	B30B7/00	B30B7/00		123
B30B7/02	8	having several platens arranged one above the other	B30B7/02	B30B7/02		679
B30B7/023	9	{Feeding or discharging means}	B30B7/02	B30B7/02		227
B30B7/026	9	{Spacer elements; Changing means therefor}	B30B7/02	B30B7/02		39
B30B7/04	8	wherein pressing is effected in different directions simultaneously or in turn	B30B7/04	B30B7/04		628
B30B9/00	7	Presses specially adapted for particular purposes	B30B9/00	B30B9/00		1050
B30B9/02	8	for squeezing-out liquid from liquid-containing material, e.g. juice from fruits, oil from oil-containing material (kitchen equipment A47J; filtering, e.g. straining solids from liquids, using presses in combination with filtering elements B01D; expelling water from textile fabrics or laundry D06C, D06F; drying F26{; clothes presses D06F69/00, D06F71/00})	B30B9/02	B30B9/02		1297
B30B9/04	9	using press rams	B30B9/04	B30B9/04		1240
B30B9/042	10	{co-operating with casings mounted on a movable carrier, e.g. turntable}	B30B9/04	B30B9/04		290
B30B9/045	10	{co-operating with several adjacent casings}	B30B9/04	B30B9/04		219
B30B9/047	10	{Control arrangements}	B30B9/04	B30B9/04		214
B30B9/06	10	co-operating with permeable casings or strainers	B30B9/06	B30B9/06		2356
B30B9/062	11	{Extrusion presses}	B30B9/06	B30B9/06		883
B30B9/065	11	{for making briquettes, e.g. from paper}	B30B9/06	B30B9/06		104
B30B9/067	11	{with a retractable abutment member closing one end of the press chamber}	B30B9/06	B30B9/06		276
B30B9/08	10	co-operating with a rotary casing	B30B9/08	B30B9/08		166
B30B9/10	10	without use of a casing	B30B9/10	B30B9/10		169
B30B9/105	11	{using a press ram co-operating with an intermittently moved endless conveyor}	B30B9/10	B30B9/10		98
B30B9/12	9	using pressing worms or screws co-operating with a permeable casing	B30B9/12	B30B9/12		1398
B30B9/121	10	{Screw constructions}	B30B9/12	B30B9/12		1052
B30B9/122	10	{Means preventing the material from turning with the screw or returning towards the feed hopper}	B30B9/12	B30B9/12		175
B30B9/124	10	{using a rotatable and axially movable screw}	B30B9/12	B30B9/12		101
B30B9/125	10	{Control arrangements}	B30B9/12	B30B9/12		324
B30B9/127	10	{Feed means}	B30B9/12	B30B9/12		400
B30B9/128	10	{Vertical or inclined screw presses}	B30B9/12	B30B9/12		409
B30B9/14	10	operating with only one screw or worm	B30B9/14	B30B9/14		1379
B30B9/16	10	operating with two or more screws or worms	B30B9/16	B30B9/16		402
B30B9/163	11	{working in different chambers}	B30B9/16	B30B9/16		143
B30B9/166	11	{the screws being coaxially disposed in the same chamber}	B30B9/16	B30B9/16		109
B30B9/18	10	with means for adjusting the outlet for the solid	B30B9/18	B30B9/18		593
B30B9/20	9	using rotary pressing members, other than worms or screws, e.g. rollers, rings, discs	B30B9/20	B30B9/20		1351
B30B9/202	10	{with co-operating cones}	B30B9/20	B30B9/20		124
B30B9/205	10	{using a roller with radially arranged vanes dividing the pressing space in separate chambers}	B30B9/20	B30B9/20		52
B30B9/207	10	{Roller-and-ring presses}	B30B9/20	B30B9/20		140
B30B9/22	9	using a flexible member, e.g. diaphragm, urged by fluid pressure	B30B9/22	B30B9/22		528
B30B9/225	10	{the diaphragm being tubular}	B30B9/22	B30B9/22		113
B30B9/24	9	using an endless pressing band	B30B9/24	B30B9/24		582
B30B9/241	10	{co-operating with a drum or roller}	B30B9/24	B30B9/24		377
B30B9/242	10	{comprising compartments which are recurrently constricted and expanded}	B30B9/24	B30B9/24		6
B30B9/243	10	{The squeezing-out being performed in several stages}	B30B9/24	B30B9/24		71
B30B9/245	10	{the edges of the band being folded over the material}	B30B9/24	B30B9/24		53
B30B9/246	10	{The material being conveyed around a drum between pressing bands}	B30B9/24	B30B9/24		213
B30B9/247	10	{Pressing band constructions}	B30B9/24	B30B9/24		95
B30B9/248	10	{Means for sealing the press zone}	B30B9/24	B30B9/24		61
B30B9/26	9	Permeable casings or strainers	B30B9/26	B30B9/26		2025
B30B9/262	10	{means disposed in the casing facilitating the squeezing-out of liquid}	B30B9/26	B30B9/26		374
B30B9/265	10	{Press cloths}	B30B9/26	B30B9/26		58
B30B9/267	10	{Strainer bars; Spacers}	B30B9/26	B30B9/26		158
B30B9/28	8	for forming shaped articles (from material in powder, granular, or paste form, e.g. briquetting presses B30B11/00)	B30B9/28	B30B9/28		732
B30B9/30	8	for baling; Compression boxes therefor (baling hay, straw, or the like A01F)	B30B9/30	B30B9/30		1247
B30B9/3003	9	{Details}	B30B9/30	B30B9/30		1360
B30B9/3007	10	{Control arrangements}	B30B9/30	B30B9/30		1011
B30B9/301	10	{Feed means}	B30B9/30	B30B9/30		1204
B30B9/3014	10	{Ejection means}	B30B9/30	B30B9/30		990
B30B9/3017	10	{Odor eliminating means}	B30B9/30	B30B9/30		176
B30B9/3021	10	{Press rams}	B30B9/30	B30B9/30		748
B30B9/3025	10	{Extrusion chambers with adjustable outlet opening}	B30B9/30	B30B9/30		180
B30B9/3028	10	{Retaining dogs}	B30B9/30	B30B9/30		169
B30B9/3032	10	{Press boxes}	B30B9/30	B30B9/30		982
B30B9/3035	10	{Means for conditioning the material to be pressed, e.g. paper shredding means}	B30B9/30	B30B9/30		543
B30B9/3039	10	{Fluid removing means}	B30B9/30	B30B9/30		366
B30B9/3042	9	{Containers provided with, or connectable to, compactor means}	B30B9/30	B30B9/30		877
B30B9/3046	10	{Containers with built-in compactor means}	B30B9/30	B30B9/30		422
B30B9/305	9	{Drive arrangements for the press ram}	B30B9/30	B30B9/30		498
B30B9/3053	10	{Hand- or foot-operated presses}	B30B9/30	B30B9/30		662
B30B9/3057	9	{Fluid-driven presses}	B30B9/30	B30B9/30		1005
B30B9/306	9	{Mechanically-driven presses}	B30B9/30	B30B9/30		720
B30B9/3064	10	{by screw means}	B30B9/30	B30B9/30		640
B30B9/3067	10	{by rack-and-pinion means}	B30B9/30	B30B9/30		353
B30B9/3071	10	{by the pull of chains or ropes}	B30B9/30	B30B9/30		245
B30B9/3075	9	{with press boxes on a movable carrier, e.g. turntable}	B30B9/30	B30B9/30		214
B30B9/3078	9	{with precompression means}	B30B9/30	B30B9/30		562
B30B9/3082	9	{with compression means other than rams performing a rectilinear movement}	B30B9/30	B30B9/30		710
B30B9/3085	9	{using a stationary press ram co-operating with a movable press box}	B30B9/30	B30B9/30		92
B30B9/3089	9	{Extrusion presses}	B30B9/30	B30B9/30		339
B30B9/3092	9	{with two or more stationary press boxes co-operating alternately with a press ram or simultaneously with press rams}	B30B9/30	B30B9/30		329
B30B9/3096	9	{the means against which, or wherein, the material is compacted being retractable}	B30B9/30	B30B9/30		325
B30B9/32	8	for consolidating scrap metal or for compacting used cars	B30B9/32	B30B9/32		1060
B30B9/321	9	{for consolidating empty containers, e.g. cans}	B30B9/32	B30B9/32		2178
B30B9/322	10	{between jaws pivoting with respect to each other}	B30B9/32	B30B9/32		185
B30B9/323	11	{operated by hand or foot}	B30B9/32	B30B9/32		438
B30B9/325	10	{between rotary pressing members, e.g. rollers, discs}	B30B9/32	B30B9/32		687
B30B9/326	9	{provided with shearing means for the scrap metal, or adapted to co-operate with a shearing machine}	B30B9/32	B30B9/32		378
B30B9/327	9	{for briquetting scrap metal}	B30B9/32	B30B9/32		1148
B30B9/328	9	{for making furnace charges}	B30B9/32	B30B9/32		84
B30B11/00	7	Presses specially adapted for forming shaped articles from material in particulate or plastic state, e.g. briquetting presses, tabletting presses (for clay or mixtures containing cement B28B; for plastics materials B29)	B30B11/00	B30B11/00		600
B30B11/001	8	{using a flexible element, e.g. diaphragm, urged by fluid pressure; Isostatic presses}	B30B11/00	B30B11/00		565
B30B11/002	9	{Isostatic press chambers; Press stands therefor}	B30B11/00	B30B11/00		850
B30B11/003	8	{using a roller with radially arranged vanes dividing the pressing space in separate chambers}	B30B11/00	B30B11/00		37
B30B11/004	8	{involving the use of very high pressures, (for the formation of artificial diamonds or boronitrides B01J3/065)}	B30B11/00	B30B11/00		446
B30B11/005	8	{Control arrangements}	B30B11/00	B30B11/00		989
B30B11/006	9	{for roller presses}	B30B11/00	B30B11/00		160
B30B11/007	8	{using a plurality of pressing members working in different directions}	B30B11/00	B30B11/00		492
B30B11/008	8	{Applying a magnetic field to the material}	B30B11/00	B30B11/00		114
B30B11/02	8	using a ram exerting pressure on the material in a moulding space	B30B11/02	B30B11/02		1257
B30B11/022	9	{whereby the material is subjected to vibrations}	B30B11/02	B30B11/02		469
B30B11/025	9	{whereby the material is transferred into the press chamber by relative movement between a ram and the press chamber}	B30B11/02	B30B11/02		195
B30B11/027	9	{Particular press methods or systems}	B30B11/02	B30B11/02		530
B30B11/04	9	co-operating with a fixed mould	B30B11/04	B30B11/04		1714
B30B11/06	10	each charge of the material being compressed against the previously formed body	B30B11/06	B30B11/06		280
B30B11/08	9	co-operating with moulds carried by a turntable	B30B11/08	B30B11/08		2053
B30B11/085	10	{for multi-layer articles}	B30B11/08	B30B11/08		101
B30B11/10	10	intermittently rotated	B30B11/10	B30B11/10		467
B30B11/12	9	co-operating with moulds on the circumference of a rotating drum	B30B11/12	B30B11/12		295
B30B11/14	9	co-operating with moulds on a movable carrier other than a turntable or a rotating drum	B30B11/14	B30B11/14		433
B30B11/16	8	using pocketed rollers, e.g. two co-operating pocketed rollers	B30B11/16	B30B11/16		720
B30B11/165	9	{Roll constructions}	B30B11/16	B30B11/16		318
B30B11/18	8	using profiled rollers	B30B11/18	B30B11/18		390
B30B11/20	8	Roller-and-ring machines, i.e. with roller disposed within a ring and co-operating with the inner surface of the ring	B30B11/20	B30B11/20		227
B30B11/201	9	{for extruding material}	B30B11/20	B30B11/20		555
B30B11/202	10	{Ring constructions}	B30B11/20	B30B11/20		260
B30B11/204	11	{Rings with adjustable extrusion openings}	B30B11/20	B30B11/20		36
B30B11/205	10	{using an annular series of radial die cells, especially for crop material}	B30B11/20	B30B11/20		120
B30B11/207	10	{Feed means}	B30B11/20	B30B11/20		254
B30B11/208	10	{Roller constructions; Mounting of the rollers}	B30B11/20	B30B11/20		337
B30B11/22	8	Extrusion presses; Dies therefor (extruding by the use of roller-and-ring machines B30B11/20)	B30B11/22	B30B11/22		574
B30B11/221	9	{extrusion dies}	B30B11/22	B30B11/22		703
B30B11/222	9	{using several circumferentially spaced rollers, e.g. skewed rollers}	B30B11/22	B30B11/22		181
B30B11/224	9	{Extrusion chambers}	B30B11/22	B30B11/22		212
B30B11/225	10	{with adjustable outlet opening}	B30B11/22	B30B11/22		186
B30B11/227	9	{Means for dividing the extruded material into briquets}	B30B11/22	B30B11/22		331
B30B11/228	9	{using pressing means, e.g. rollers moving over a perforated die plate}	B30B11/22	B30B11/22		633
B30B11/24	9	using screws or worms	B30B11/24	B30B11/24		587
B30B11/241	10	{Drive means therefor; screw bearings}	B30B11/24	B30B11/24		296
B30B11/243	10	{using two or more screws working in the same chamber}	B30B11/24	B30B11/24		196
B30B11/245	10	{using two or more screws working in different chambers}	B30B11/24	B30B11/24		129
B30B11/246	10	{Screw constructions}	B30B11/24	B30B11/24		281
B30B11/248	10	{Means preventing the material from turning with the screw or returning towards the feed hopper}	B30B11/24	B30B11/24		117
B30B11/26	9	using press rams	B30B11/26	B30B11/26		770
B30B11/265	10	{with precompression means}	B30B11/26	B30B11/26		189
B30B11/28	9	using perforated rollers or discs	B30B11/28	B30B11/28		309
B30B11/30	9	using directly-acting fluid pressure	B30B11/30	B30B11/30		28
B30B11/34	8	for coating articles, e.g. tablets	B30B11/34	B30B11/34		313
B30B12/00	7	Presses not provided for in groups B30B1/00&#160;-&#160;B30B11/00	B30B12/00	B30B12/00		130
B30B13/00	7	Methods of pressing not special to the use of presses of any one of the preceding main groups	B30B13/00	B30B13/00		174
B30B15/00	7	Details of, or accessories for, presses; Auxiliary measures in connection with pressing (safety devices F16P)	B30B15/00	B30B15/00		4329
B30B15/0005	8	{for briquetting presses}	B30B15/00	B30B15/00		541
B30B15/0011	9	{lubricating means}	B30B15/00	B30B15/00		303
B30B15/0017	9	{Deairing means}	B30B15/00	B30B15/00		277
B30B15/0023	8	{Drive arrangements for movable carriers, e.g. turntables}	B30B15/00	B30B15/00		307
B30B15/0029	8	{means for adjusting the space between the press slide and the press table, i.e. the shut height}	B30B15/00	B30B15/00		542
B30B15/0035	9	{using an adjustable connection between the press drive means and the press slide}	B30B15/00	B30B15/00		477
B30B15/0041	9	{Control arrangements therefor}	B30B15/00	B30B15/00		247
B30B15/0047	8	{releasing means for jammed presses}	B30B15/00	B30B15/00		134
B30B15/0052	8	{for fluid driven presses}	B30B15/00	B30B15/00		891
B30B15/0058	8	{Inclinable presses}	B30B15/00	B30B15/00		110
B30B15/0064	8	{Counterbalancing means for movable press elements}	B30B15/00	B30B15/00		500
B30B15/007	8	{Means for maintaining the press table, the press platen or the press ram against tilting or deflection}	B30B15/00	B30B15/00		474
B30B15/0076	8	{Noise or vibration isolation means}	B30B15/00	B30B15/00		710
B30B15/0082	8	{Dust eliminating means; Mould or press ram cleaning means}	B30B15/00	B30B15/00		1535
B30B15/0088	8	{Lubricating means (B30B15/0011 takes precedence)}	B30B15/00	B30B15/00		410
B30B15/0094	8	{Press load monitoring means (B30B15/281 takes precedence)}	B30B15/00	B30B15/00		608
B30B15/02	8	Dies; Inserts therefor; Mounting thereof; Moulds (extrusion dies B30B11/22)	B30B15/02	B30B15/02		1834
B30B15/022	9	{Moulds for compacting material in powder, granular of pasta form}	B30B15/02	B30B15/02		858
B30B15/024	10	{using elastic mould parts}	B30B15/02	B30B15/02		317
B30B15/026	9	{Mounting of dies, platens or press rams}	B30B15/02	B30B15/02		1417
B30B15/028	9	{Loading or unloading of dies, platens or press rams}	B30B15/02	B30B15/02		993
B30B15/04	8	Frames; Guides	B30B15/04	B30B15/04		1658
B30B15/041	9	{Guides}	B30B15/04	B30B15/04		1235
B30B15/042	9	{Prestressed frames}	B30B15/04	B30B15/04		205
B30B15/044	9	{Means preventing deflection of the frame, especially for C-frames}	B30B15/04	B30B15/04		157
B30B15/045	9	{Mountings of press columns}	B30B15/04	B30B15/04		151
B30B15/047	9	{C-shaped frames (with means for preventing deflection B30B15/044)}	B30B15/04	B30B15/04		281
B30B15/048	9	{Laminated frame structures}	B30B15/04	B30B15/04		157
B30B15/06	8	Platens or press rams	B30B15/06	B30B15/06		421
B30B15/061	9	{Cushion plates}	B30B15/06	B30B15/06		515
B30B15/062	9	{Press plates}	B30B15/06	B30B15/06		681
B30B15/064	10	{with heating or cooling means}	B30B15/06	B30B15/06		971
B30B15/065	9	{Press rams}	B30B15/06	B30B15/06		951
B30B15/067	10	{with means for equalizing the pressure exerted by a plurality of press rams}	B30B15/06	B30B15/06		171
B30B15/068	9	{Drive connections, e.g. pivotal}	B30B15/06	B30B15/06		334
B30B15/08	8	Accessory tools, e.g. knives; Mountings therefor	B30B15/08	B30B15/08		1691
B30B15/10	8	Brakes specially adapted for presses (brakes in general F16D)	B30B15/10	B30B15/10		446
B30B15/12	8	Clutches specially adapted for presses (clutches in general F16D)	B30B15/12	B30B15/12		270
B30B15/14	8	Control arrangements for mechanically-driven presses	B30B15/14	B30B15/14		709
B30B15/142	9	{controlling the brake or the clutch}	B30B15/14	B30B15/14		289
B30B15/144	9	{for stopping the press shaft in a predetermined angular position}	B30B15/14	B30B15/14		94
B30B15/146	9	{for synchronising a line of presses}	B30B15/14	B30B15/14		145
B30B15/148	9	{Electrical control arrangements}	B30B15/14	B30B15/14		687
B30B15/16	8	Control arrangements for fluid-driven presses (pumps per seF04; hydraulic accumulators per seF15B; valves per seF16K; control devices in general G05)	B30B15/16	B30B15/16		1578
B30B15/161	9	{controlling the ram speed and ram pressure, e.g. fast approach speed at low pressure, low pressing speed at high pressure}	B30B15/16	B30B15/16		402
B30B15/163	9	{for accumulator-driven presses}	B30B15/16	B30B15/16		234
B30B15/165	9	{for pneumatically-hydraulically driven presses}	B30B15/16	B30B15/16		137
B30B15/166	9	{Electrical control arrangements}	B30B15/16	B30B15/16		374
B30B15/168	9	{for pneumatically driven presses (B30B15/165 takes precedence)}	B30B15/16	B30B15/16		77
B30B15/18	9	controlling the reciprocating motion of the ram	B30B15/18	B30B15/18		390
B30B15/183	10	{Controlling the filling of the press cylinder during the approach stroke of the ram, e.g. prefill-valves}	B30B15/18	B30B15/18		96
B30B15/186	10	{Controlling the return movement of the ram, e.g. decompression valves}	B30B15/18	B30B15/18		89
B30B15/20	10	controlling the speed of the ram, e.g. the speed of the approach, pressing or return strokes	B30B15/20	B30B15/20		169
B30B15/22	9	controlling the degree of pressure applied by the ram during the pressing stroke	B30B15/22	B30B15/22		396
B30B15/24	9	controlling the movement of a plurality of actuating members to maintain parallel movement of the platen or press beam	B30B15/24	B30B15/24		380
B30B15/245	10	{using auxiliary cylinder and piston means as actuating members}	B30B15/24	B30B15/24		120
B30B15/26	8	Program-control arrangements	B30B15/26	B30B15/26		1543
B30B15/28	8	Arrangements for preventing distortion of, or damage to, presses or parts thereof	B30B15/28	B30B15/28		1227
B30B15/281	9	{overload limiting devices (in general F16H35/10)}	B30B15/28	B30B15/28		444
B30B15/282	10	{using a breakage element}	B30B15/28	B30B15/28		69
B30B15/284	10	{releasing fluid from a fluid chamber subjected to overload pressure}	B30B15/28	B30B15/28		292
B30B15/285	9	{preventing a full press stroke if there is an obstruction in the working area}	B30B15/28	B30B15/28		222
B30B15/287	9	{preventing unintended ram movement, e.g. using blocking devices}	B30B15/28	B30B15/28		262
B30B15/288	9	{preventing over-run or reverse-run of the press shaft}	B30B15/28	B30B15/28		114
B30B15/30	8	Feeding material to presses	B30B15/30	B30B15/30		2808
B30B15/302	9	{Feeding material in particulate or plastic state to moulding presses}	B30B15/30	B30B15/30		1872
B30B15/304	10	{by using feed frames or shoes with relative movement with regard to the mould or moulds}	B30B15/30	B30B15/30		896
B30B15/306	11	{for multi-layer articles}	B30B15/30	B30B15/30		116
B30B15/308	10	{in a continuous manner, e.g. for roller presses, screw extrusion presses}	B30B15/30	B30B15/30		838
B30B15/32	8	Discharging presses	B30B15/32	B30B15/32		4181
B30B15/34	8	Heating or cooling presses or parts thereof	B30B15/34	B30B15/34		2299
