E04F10/00	7	Sunshades, {e.g. Florentine blinds or jalousies; Outside screens (E06B9/26 takes precedence)}; Awnings {or baldachins (for caravans B60P3/343)}; (trailer awnings E04H15/08; for tents E04H15/58)	E04F10/00	E04F10/00		731
E04F10/005	8	{Rigidly-arranged sunshade roofs with coherent surfaces}	E04F10/00	E04F10/00		666
E04F10/02	8	of flexible canopy materials, e.g. canvas {; Baldachins}	E04F10/02	E04F10/02		1342
E04F10/04	9	with material fixed on sections of a collapsible frame {especially Florentine blinds}	E04F10/04	E04F10/04		413
E04F10/06	9	comprising a roller-blind with means for holding the end away from a building	E04F10/06	E04F10/06		640
E04F10/0603	10	{with telescopic arms}	E04F10/06	E04F10/06		298
E04F10/0607	10	{with guiding-sections for supporting the movable end of the blind}	E04F10/06	E04F10/06		803
E04F10/0611	10	{with articulated arms supporting the movable end of the blind for deployment of the blind}	E04F10/06	E04F10/06		155
E04F10/0614	11	{whereby the pivot axis of the articulation is parallel to the roller}	E04F10/06	E04F10/06		826
E04F10/0618	11	{whereby the pivot axis of the articulation is perpendicular to the roller}	E04F10/06	E04F10/06		980
E04F10/0622	12	{whereby the plane defined by three consecutive articulation points of an articulated arm is not parallel to the rotation axis of the roller, e.g. to create a saddle type roof construction or to prevent contact between the cloth and the arm sections}	E04F10/06	E04F10/06		136
E04F10/0625	11	{whereby the roller is installed on the articulated arms}	E04F10/06	E04F10/06		178
E04F10/0629	11	{whereby the arm is of the lazy tong type}	E04F10/06	E04F10/06		30
E04F10/0633	10	{Arrangements for fastening the flexible canopy material to the supporting structure (fastening roller shutters to rollers E06B9/171)}	E04F10/06	E04F10/06		420
E04F10/0637	10	{with mechanisms for adjusting the inclination of the blind}	E04F10/06	E04F10/06		475
E04F10/064	11	{whereby the mechanism changes the inclination of the blind during unrolling}	E04F10/06	E04F10/06		46
E04F10/0644	10	{with mechanisms for unrolling or balancing the blind}	E04F10/06	E04F10/06		164
E04F10/0648	11	{acting on the roller tube}	E04F10/06	E04F10/06		588
E04F10/0651	11	{acting on the arms}	E04F10/06	E04F10/06		436
E04F10/0655	11	{acting on the movable end, e.g. front bar}	E04F10/06	E04F10/06		341
E04F10/0659	11	{Control systems therefor}	E04F10/06	E04F10/06		209
E04F10/0662	10	{with arrangements for fastening the blind to the building}	E04F10/06	E04F10/06		599
E04F10/0666	10	{Accessories}	E04F10/06	E04F10/06		410
E04F10/067	11	{acting as intermediate support of the flexible canopy}	E04F10/06	E04F10/06		167
E04F10/0674	11	{acting as separate supporting bar}	E04F10/06	E04F10/06		300
E04F10/0677	11	{acting as centre bearing}	E04F10/06	E04F10/06		121
E04F10/0681	11	{Support posts for the movable end of the blind}	E04F10/06	E04F10/06		325
E04F10/0685	10	{Covers or housings for the rolled-up blind}	E04F10/06	E04F10/06		454
E04F10/0688	11	{with the housing taking up the articulated arms}	E04F10/06	E04F10/06		227
E04F10/0692	10	{Front bars}	E04F10/06	E04F10/06		281
E04F10/0696	11	{with means to attach an auxiliary screen}	E04F10/06	E04F10/06		128
E04F10/08	8	of a plurality of similar rigid parts, e.g. slabs, lamellae {(E04F10/005 takes precedence)}	E04F10/08	E04F10/08		1129
E04F10/10	9	collapsible {or extensible; metallic Florentine blinds; awnings with movable parts such as louvres; (shutters E06B9/04; louvre windows E06B7/08)}	E04F10/10	E04F10/10		1588
E04F11/00	7	Stairways, ramps, or like structures (mounting or marking-off stairways E04F21/26; of temporary {use during building} construction E04G27/00; means for facilitating access to swimming pools E04H4/144; {means for facilitating access to swimming pools E04H4/144; appliances for aiding patients or disabled persons to walk A61H3/00}); Balustrades; Handrails (ladders permanently attached to fixed structures E06C9/00)	E04F11/00	E04F11/00		255
E04F11/002	8	{Ramps}	E04F11/00	E04F11/00		648
E04F2011/005	9	{collapsible, e.g. folding, telescopic}	E04F11/00	E04F11/00		288
E04F2011/007	9	{characterised by the supporting structure}	E04F11/00	E04F11/00		223
E04F11/02	8	Stairways; Layouts thereof	E04F11/02	E04F11/02		1853
E04F11/0201	9	{Space-saving stairways, e.g. having half steps}	E04F11/02	E04F11/02		119
E04F2011/0203	9	{Miscellaneous features of stairways not otherwise provided for}	E04F11/02	E04F11/02		82
E04F2011/0205	10	{Stairways characterised by the use of specific materials for the supporting structure of the treads}	E04F11/02	E04F11/02		95
E04F2011/0207	11	{mainly of wood}	E04F11/02	E04F11/02		44
E04F2011/0209	11	{mainly of metal}	E04F11/02	E04F11/02		258
E04F2011/021	11	{mainly of stone or stone like materials, e.g. concrete;  mainly of glass}	E04F11/02	E04F11/02		25
E04F2011/0212	12	{mainly of concrete}	E04F11/02	E04F11/02		240
E04F2011/0214	13	{cast in situ}	E04F11/02	E04F11/02		127
E04F2011/0216	12	{mainly of glass}	E04F11/02	E04F11/02		11
E04F2011/0218	11	{mainly of organic plastics with or without reinforcements or filling materials}	E04F11/02	E04F11/02		32
E04F11/022	9	characterised by the supporting structure	E04F11/022	E04F11/022		1016
E04F11/0223	10	{Cantilevered stairways (E04F11/032 takes precedence)}	E04F11/022	E04F11/022		90
E04F11/0226	10	{Stairways having treads supported by balusters}	E04F11/022	E04F11/022		28
E04F11/025	10	Stairways having stringers {(E04F11/035 takes precedence)}	E04F11/025	E04F11/025		951
E04F11/0255	11	{having adjustable gradient (E04F11/1041 takes precedence)}	E04F11/025	E04F11/025		242
E04F11/028	11	having a central stringer	E04F11/028	E04F11/028		116
E04F11/032	10	Spiral stairways supported by a central column	E04F11/032	E04F11/032		561
E04F11/035	10	Stairways consisting of a plurality of assembled modular parts without further support {(E04F11/032 takes precedence)}	E04F11/035	E04F11/035		870
E04F11/038	11	each modular part having a load-bearing balustrade part	E04F11/038	E04F11/038		76
E04F11/04	9	Movable stairways, e.g. of loft ladders which may or may not be concealable or extensible (ship ladders B63B; stairs for aircraft B64F; escalators or moving walkways B66B)	E04F11/04	E04F11/04		361
E04F11/06	10	collapsible, e.g. folding, telescopic	E04F11/06	E04F11/06		327
E04F11/062	11	{folding}	E04F11/06	E04F11/06		203
E04F11/064	12	{with stringers overlapping when folded}	E04F11/06	E04F11/06		212
E04F11/066	12	{folding like scissors or accordions}	E04F11/06	E04F11/06		84
E04F11/068	11	{telescopic}	E04F11/06	E04F11/06		174
E04F11/09	9	Tread-and-riser units	E04F11/09	E04F11/09		266
E04F11/104	9	Treads	E04F11/104	E04F11/104		584
E04F11/1041	10	{having means to adjust the height, the depth and/or the slope of the stair steps (E04F11/1042&#160;-&#160;E04F11/116 take precedence)}	E04F11/104	E04F11/104		327
E04F11/1042	10	{with an upper layer of fibres or chips, e.g. bonded with synthetic resins}	E04F11/104	E04F11/104		21
E04F11/1043	10	{with an upper layer of organic plastics with or without reinforcements or filling materials}	E04F11/104	E04F11/104		71
E04F11/1045	10	{composed of several layers, e.g. sandwich panels (layered products in general B32B; producing decorative panels or veneers B44C5/04)}	E04F11/104	E04F11/104		151
E04F2011/1046	10	{Miscellaneous features of treads not otherwise provided for}	E04F11/104	E04F11/104		102
E04F2011/1047	11	{with means for eliminating squeak}	E04F11/104	E04F11/104		40
E04F2011/1048	11	{with lighting means}	E04F11/104	E04F11/104		334
E04F11/108	10	of wood {or with an upper layer of wood}	E04F11/108	E04F11/108		331
E04F11/112	10	of metal {or with an upper layer of metal}	E04F11/112	E04F11/112		365
E04F11/116	10	of stone, concrete or like material {or with an upper layer of stone or stone like material, e.g. ceramics, concrete; of glass or with an upper layer of glass}	E04F11/116	E04F11/116		678
E04F11/16	10	Surfaces thereof; Protecting means for edges or corners thereof ({loosely laid coverings,} floor fabrics, fastenings therefor A47G27/00)	E04F11/16	E04F11/16		835
E04F11/163	11	{Protecting means for edges or corners}	E04F11/16	E04F11/16		482
E04F11/166	12	{with means for fixing a separate edging strip}	E04F11/16	E04F11/16		406
E04F11/17	11	Surfaces {(guard covers of stairs E04G21/30)}	E04F11/17	E04F11/17		746
E04F11/175	12	{Covering panels for tread restoration}	E04F11/17	E04F11/17		183
E04F11/18	8	Balustrades; Handrails (guard-rails on ships B63B; for bridges E01D19/10; for roads E01F13/00, E01F15/00; fences E04H17/00{; safety measures for persons during the construction of buildings E04G21/32})	E04F11/18	E04F11/18		1078
E04F11/1802	9	{Handrails mounted on walls, e.g. on the wall side of stairs}	E04F11/18	E04F11/18		172
E04F11/1804	10	{Details of anchoring to the wall}	E04F11/18	E04F11/18		374
E04F2011/1806	10	{Balcony guard with additional child safety means}	E04F11/18	E04F11/18		33
E04F11/1808	10	{Handrail members; Connections between handrail members}	E04F11/18	E04F11/18		215
E04F11/181	9	{Balustrades}	E04F11/18	E04F11/18		1688
E04F11/1812	10	{Details of anchoring to the wall or floor}	E04F11/18	E04F11/18		1539
E04F11/1814	11	{Covers for the base portions of the balustrade posts}	E04F11/18	E04F11/18		176
E04F11/1817	10	{Connections therefor (E04F11/1812 and E04F11/1836 take precedence)}	E04F11/18	E04F11/18		1538
E04F2011/1819	11	{between balustrade posts and horizontal or sloping balustrade members}	E04F11/18	E04F11/18		498
E04F2011/1821	12	{between balustrade posts and handrails}	E04F11/18	E04F11/18		673
E04F2011/1823	11	{between balustrade filling members, e.g. balusters or panels, and horizontal or sloping balustrade members}	E04F11/18	E04F11/18		276
E04F2011/1825	12	{between balustrade filling members, e.g. balusters or panels, and handrails}	E04F11/18	E04F11/18		32
E04F2011/1827	13	{between balusters and handrails}	E04F11/18	E04F11/18		206
E04F2011/1829	13	{between filling panels and handrails}	E04F11/18	E04F11/18		57
E04F2011/1831	11	{between balustrade filling members, e.g. panels, and balustrade posts}	E04F11/18	E04F11/18		230
E04F11/1834	11	{with adjustable angle, e.g. pivotal connections}	E04F11/18	E04F11/18		714
E04F11/1836	10	{Handrails of balustrades; Connections between handrail members}	E04F11/18	E04F11/18		824
E04F11/1838	11	{Laterally displaced handrail}	E04F11/18	E04F11/18		82
E04F11/184	11	{of variable curvature; flexible}	E04F11/18	E04F11/18		106
E04F11/1842	10	{Balusters; Grille-type elements}	E04F11/18	E04F11/18		656
E04F11/1844	11	{Grille-type elements}	E04F11/18	E04F11/18		81
E04F11/1846	11	{Balusters with means for fixing to the floor}	E04F11/18	E04F11/18		149
E04F11/1848	11	{Separate means for spacing balusters apart}	E04F11/18	E04F11/18		20
E04F11/1851	10	{Filling panels, e.g. concrete, sheet metal panels}	E04F11/18	E04F11/18		565
E04F11/1853	11	{Glass panels}	E04F11/18	E04F11/18		790
E04F11/1855	11	{Wire mesh panels}	E04F11/18	E04F11/18		24
E04F11/1857	11	{Flexible panels or nets}	E04F11/18	E04F11/18		29
E04F11/1859	10	{Wire cables or the like filling elements}	E04F11/18	E04F11/18		93
E04F11/1861	10	{with additional safety means for children, e.g. nets or fillings between balusters}	E04F11/18	E04F11/18		179
E04F11/1863	9	{Built-in aids for ascending or descending stairs (lifts associated with stairs B66B9/08)}	E04F11/18	E04F11/18		206
E04F11/1865	9	{Collapsible or portable balustrades}	E04F11/18	E04F11/18		480
E04F2011/1868	9	{Miscellaneous features of handrails not otherwise provided for}	E04F11/18	E04F11/18		239
E04F2011/187	10	{lengthwise adjustable, e.g. telescopic}	E04F11/18	E04F11/18		217
E04F2011/1872	10	{illuminated}	E04F11/18	E04F11/18		450
E04F2011/1874	10	{Noise reduction}	E04F11/18	E04F11/18		13
E04F2011/1876	10	{Movable elements, e.g. against sunlight}	E04F11/18	E04F11/18		229
E04F2011/1878	10	{Heat exchanger}	E04F11/18	E04F11/18		20
E04F2011/188	10	{with flower pots}	E04F11/18	E04F11/18		82
E04F2011/1882	10	{with traction cable inside post or rail}	E04F11/18	E04F11/18		100
E04F2011/1885	9	{Handrails or balusters characterized by the use of specific materials}	E04F11/18	E04F11/18		61
E04F2011/1887	10	{mainly of wood}	E04F11/18	E04F11/18		163
E04F2011/1889	10	{mainly of metal}	E04F11/18	E04F11/18		231
E04F2011/1891	10	{mainly of stone or stone like materials, e.g. concrete;  mainly of glass}	E04F11/18	E04F11/18		9
E04F2011/1893	11	{mainly of concrete}	E04F11/18	E04F11/18		29
E04F2011/1895	11	{mainly of glass}	E04F11/18	E04F11/18		60
E04F2011/1897	10	{mainly of organic plastics with or without reinforcements or filling materials}	E04F11/18	E04F11/18		224
E04F13/00	7	Coverings or linings, e.g. for walls or ceilings (flooring E04F15/00; decoration of surfaces, mosaic work B44, e.g. paper-hanging B44C7/00; made of webs, e.g. of fabrics or wallpaper {, as such, or their manufacturing}D03D, D04G, D04H, D06N, D21H; construction of {false} ceilings E04B9/00; roofings or similar water-tight coverings against precipitation E04D)	E04F13/00	E04F13/00		742
E04F13/002	8	{made of webs, e.g. of fabrics, or wallpaper, used as coverings or linings (of a number of similar elements carried by a common web E04F13/0862; paperhanging, tapestry work B44C7/00)}	E04F13/00	E04F13/00		1185
E04F13/005	9	{Stretched foil- or web-like elements attached with edge gripping devices}	E04F13/00	E04F13/00		212
E04F13/007	8	{Outer coverings for walls with ventilating means}	E04F13/00	E04F13/00		600
E04F13/02	8	of plastic materials hardening after applying, e.g. plaster (surface treatment in painting technique B44D; inorganic or bituminous masses C04B; organic plastics C08L{; implements for applying plasticised materials E04F21/02})	E04F13/02	E04F13/02		2144
E04F13/04	9	Bases for plaster (sub-ceilings with plaster-carrying means E04B9/06)	E04F13/04	E04F13/04		2444
E04F13/042	10	{Joint tapes}	E04F13/04	E04F13/04		226
E04F13/045	10	{Means for fastening plaster-bases to a supporting structure}	E04F13/04	E04F13/04		639
E04F13/047	10	{Plaster carrying meshes}	E04F13/04	E04F13/04		573
E04F13/06	10	Edge-protecting borders {(borders for joints between plaster layers and window or door frames or like E06B1/62)}	E04F13/06	E04F13/06		1325
E04F2013/061	11	{for arched or curved edges}	E04F13/06	E04F13/06		83
E04F2013/063	11	{for corners}	E04F13/06	E04F13/06		951
E04F2013/065	11	{for lower edges of outer insulation layers}	E04F13/06	E04F13/06		150
E04F2013/066	11	{for expansion joints between two plaster layers}	E04F13/06	E04F13/06		132
E04F13/068	11	{combined with mesh material or the like to allow plaster to bond therewith}	E04F13/06	E04F13/06		407
E04F13/07	8	composed of covering or lining elements; Sub-structures therefor; Fastening means therefor	E04F13/07	E04F13/07		416
E04F13/072	9	composed of specially adapted, structured or shaped covering or lining elements	E04F13/072	E04F13/072		1046
E04F13/073	10	for particular building parts, e.g. corners or columns	E04F13/073	E04F13/073		281
E04F13/0733	11	{for corners}	E04F13/073	E04F13/073		677
E04F13/0736	11	{for columns}	E04F13/073	E04F13/073		298
E04F13/074	10	for accommodating service installations or utility lines, e.g. heating conduits, electrical lines, lighting devices or service outlets {(not used; accommodating heating conduits F24D; accommodating electrical cables or lines H02G3/00; accommodating lighting devices F21V33/006)}	E04F13/074	E04F13/074		197
E04F13/075	10	for insulation or surface protection, e.g. against noise or impact {(not used; for insulation, e.g. against noise E04B1/00)}	E04F13/075	E04F13/075		297
E04F13/076	10	characterised by the joints between neighbouring elements, e.g. with joint fillings or with tongue and groove connections {(not used, seeE04F13/0889)}	E04F13/076	E04F13/076		159
E04F13/077	10	composed of several layers, e.g. sandwich panels (E04F13/075 takes precedence){(not used, seeE04F13/0866)}	E04F13/077	E04F13/077		178
E04F13/078	10	Stretched foil- or web-like elements attached with edge gripping devices {(not used, seeE04F13/005)}	E04F13/078	E04F13/078		8
E04F13/08	9	composed of a plurality of similar covering or lining elements, (E04F13/072 takes precedence; borders, skirtings E04F19/02; {of webs or fabrics E04F13/002; fixing strips E04F19/06; separate provisional spacers between adjacent tiles E04F21/0092; implements or means for setting tiles E04F21/18})	E04F13/08	E04F13/08		2924
E04F13/0801	10	{Separate fastening elements (E04F13/088, E04F13/0885 take precedence)}	E04F13/08	E04F13/08		1602
E04F13/0803	11	{with load-supporting elongated furring elements between wall and covering elements}	E04F13/08	E04F13/08		3400
E04F13/0805	12	{with additional fastening elements between furring elements and the wall}	E04F13/08	E04F13/08		1502
E04F13/0807	13	{adjustable perpendicular to the wall}	E04F13/08	E04F13/08		795
E04F13/0808	13	{adjustable in several directions one of which is perpendicular to the wall}	E04F13/08	E04F13/08		576
E04F13/081	12	{with additional fastening elements between furring elements and covering elements}	E04F13/08	E04F13/08		1576
E04F13/0812	13	{fixed by means of spring action}	E04F13/08	E04F13/08		589
E04F13/0814	13	{fixed by means of clamping action}	E04F13/08	E04F13/08		640
E04F13/0816	13	{the additional fastening elements extending into the back side of the covering elements (E04F13/083 takes precedence)}	E04F13/08	E04F13/08		737
E04F13/0817	14	{extending completely through the covering elements}	E04F13/08	E04F13/08		174
E04F13/0819	14	{inserted into grooves in the back side of the covering elements}	E04F13/08	E04F13/08		386
E04F13/0821	13	{the additional fastening elements located in-between two adjacent covering elements}	E04F13/08	E04F13/08		657
E04F13/0823	14	{piercing the side faces of the covering elements}	E04F13/08	E04F13/08		121
E04F13/0825	14	{engaging side holes preformed into the covering elements}	E04F13/08	E04F13/08		327
E04F13/0826	14	{engaging side grooves running along the whole length of the covering elements}	E04F13/08	E04F13/08		1031
E04F13/0828	14	{engaging the outer surface of the covering elements, e.g. at the corners}	E04F13/08	E04F13/08		197
E04F13/083	13	{Hooking means on the back side of the covering elements}	E04F13/08	E04F13/08		696
E04F13/0832	11	{without load-supporting elongated furring elements between wall and covering elements}	E04F13/08	E04F13/08		865
E04F13/0833	12	{not adjustable (E04F13/0857 takes precedence)}	E04F13/08	E04F13/08		123
E04F13/0835	13	{the fastening elements extending into the back side of the covering elements (E04F13/0851 takes precedence)}	E04F13/08	E04F13/08		1137
E04F13/0837	14	{extending completely through the covering elements}	E04F13/08	E04F13/08		636
E04F13/0839	13	{the fastening elements situated at the corners of the covering elements, not extending through the covering}	E04F13/08	E04F13/08		157
E04F13/0841	13	{the fastening elements engaging the outer surface of the covering elements, not extending through the covering (E04F13/0839 and E04F13/0846 take precedence)}	E04F13/08	E04F13/08		284
E04F13/0842	14	{specially adapted for thin sheet-like materials, e.g. sheet-metal or plastics}	E04F13/08	E04F13/08		170
E04F13/0844	14	{with means piercing the side faces of the covering elements}	E04F13/08	E04F13/08		98
E04F13/0846	13	{the fastening elements engaging holes or grooves in the side faces of the covering elements (E04F13/0835 and E04F13/0839 take precedence)}	E04F13/08	E04F13/08		827
E04F13/0848	14	{specially adapted for thin sheet-like materials, e.g. sheet-metal or plastics}	E04F13/08	E04F13/08		144
E04F13/085	14	{with means piercing the side faces of the covering elements}	E04F13/08	E04F13/08		92
E04F13/0851	13	{Hooking means on the back side of the covering elements}	E04F13/08	E04F13/08		274
E04F13/0853	12	{adjustable perpendicular to the wall}	E04F13/08	E04F13/08		724
E04F13/0855	13	{adjustable in several directions, one of which is perpendicular to the wall}	E04F13/08	E04F13/08		593
E04F13/0857	12	{Supporting consoles, e.g. adjustable only in a direction parallel to the wall (E04F13/0853 takes precedence)}	E04F13/08	E04F13/08		337
E04F13/0858	12	{fixed by means of spring action}	E04F13/08	E04F13/08		140
E04F13/086	12	{fixed by means of clamping action}	E04F13/08	E04F13/08		95
E04F13/0862	10	{composed of a number of elements which are identical or not, e.g. carried by a common web, support plate or grid}	E04F13/08	E04F13/08		2399
E04F13/0864	10	{composed of superposed elements which overlap each other and of which the flat outer surface includes an acute angle with the surface to cover}	E04F13/08	E04F13/08		1319
E04F13/0866	10	{composed of several layers, e.g. sandwich panels or layered panels (layered products as such in general B32B; producing decorative panels or veneers B44C5/04; E04F13/0864, E04F13/0875 take precedence)}	E04F13/08	E04F13/08		2526
E04F13/0867	10	{having acoustic absorption means on the visible surface}	E04F13/08	E04F13/08		320
E04F13/0869	10	{having conduits for fluids}	E04F13/08	E04F13/08		493
E04F13/0871	10	{having an ornamental or specially shaped visible surface (E04F13/0867 takes precedence)}	E04F13/08	E04F13/08		1863
E04F13/0873	11	{the visible surface imitating natural stone, brick work, tiled surface or the like (E04F13/105, E04F13/123, E04F13/147, E04F13/165, E04F13/185 take precedence)}	E04F13/08	E04F13/08		309
E04F13/0875	10	{having a basic insulating layer and at least one covering layer}	E04F13/08	E04F13/08		4313
E04F13/0876	11	{the covering layer comprising mutual alignment or interlocking means}	E04F13/08	E04F13/08		265
E04F13/0878	11	{the basic insulating layer comprising mutual alignment or interlocking means}	E04F13/08	E04F13/08		303
E04F13/088	10	{fixed directly to the wall by means of magnets, hook and loop-type or similar fasteners, not necessarily involving the side faces of the covering element}	E04F13/08	E04F13/08		249
E04F13/0882	11	{by hook and loop-type fasteners}	E04F13/08	E04F13/08		137
E04F13/0883	11	{by magnets}	E04F13/08	E04F13/08		329
E04F13/0885	10	{specially adapted for being adhesively fixed to the wall; Fastening means therefor; Fixing by means of plastics materials hardening after application}	E04F13/08	E04F13/08		1478
E04F13/0887	11	{Adhesive means specially adapted therefor, e.g. adhesive foils or strips}	E04F13/08	E04F13/08		340
E04F13/0889	10	{characterised by the joints between neighbouring elements, e.g. with joint fillings or with tongue and groove connections}	E04F13/08	E04F13/08		1876
E04F13/0891	11	{with joint fillings}	E04F13/08	E04F13/08		486
E04F13/0892	11	{with means for aligning the outer surfaces of the covering elements (E04F13/0894 takes precedence)}	E04F13/08	E04F13/08		416
E04F13/0894	11	{with tongue and groove connections}	E04F13/08	E04F13/08		1912
E04F13/0896	11	{with adhesive joining strips (E04F13/0894, E04F13/0898 take precedence)}	E04F13/08	E04F13/08		100
E04F13/0898	11	{with sealing elements between coverings (sealings of joints between building constructions in general E04B1/68)}	E04F13/08	E04F13/08		562
E04F13/09	10	of elements attached to a common web, support plate or grid {(not used, seeE04F13/0862)}	E04F13/09	E04F13/09		64
E04F13/10	10	of wood {or with an outer layer of wood (E04F13/0864 takes precedence)}	E04F13/10	E04F13/10		1244
E04F13/105	11	{with an outer layer imitating natural stone, brick work, tiled surface or the like}	E04F13/10	E04F13/10		31
E04F13/12	10	of metal {or with an outer layer of metal or enameled metal (E04F13/0864 takes precedence)}	E04F13/12	E04F13/12		2246
E04F13/123	11	{with an outer layer imitating natural stone, brick work, tiled surface or the like}	E04F13/12	E04F13/12		73
E04F13/126	11	{with an outer layer of wire mesh, wire grid or the like, e.g. gabions}	E04F13/12	E04F13/12		49
E04F13/14	10	stone or stone-like materials, e.g. ceramics {concrete,}; of glass {or with an outer layer of stone or stone-like materials or glass (E04F13/0864 takes precedence; producing shaped elements from concrete, ceramic compositions or other stone-like materials B28B; prefabricated panels in general E04C2/00)}	E04F13/14	E04F13/14		1919
E04F13/141	11	{with an outer layer of concrete (E04F13/147 takes precedence)}	E04F13/14	E04F13/14		583
E04F13/142	11	{with an outer layer of ceramics or clays}	E04F13/14	E04F13/14		1279
E04F13/144	11	{with an outer layer of marble or other natural stone}	E04F13/14	E04F13/14		765
E04F13/145	11	{with an outer layer of glass}	E04F13/14	E04F13/14		575
E04F13/147	11	{with an outer layer imitating natural stone, brick work or the like}	E04F13/14	E04F13/14		854
E04F13/148	11	{with an outer layer of asbestos cement or the like}	E04F13/14	E04F13/14		148
E04F13/15	11	characterised by the use of glass elements {, i.e. wherein an outer layer is not of glass (E04F13/145 takes precedence)}	E04F13/15	E04F13/15		189
E04F13/16	10	of fibres or chips, e.g. bonded with synthetic resins {, or with an outer layer of fibres or chips (E04F13/0864 takes precedence)}	E04F13/16	E04F13/16		686
E04F13/165	11	{with an outer layer imitating natural stone, brick work, tiled surface or the like}	E04F13/16	E04F13/16		84
E04F13/18	10	of organic plastics with or without reinforcements or filling materials (of plastic-bound fibres or chips E04F13/16){or with an outer layer of organic plastics with or without reinforcements or filling materials; plastic tiles (E04F13/0864 takes precedence)}	E04F13/18	E04F13/18		1832
E04F13/185	11	{with an outer layer imitating natural stone, brick work, tiled surface or the like}	E04F13/18	E04F13/18		305
E04F13/21	9	Fastening means specially adapted for covering or lining elements {(not used, seeE04F13/0801)}	E04F13/21	E04F13/21		192
E04F13/22	10	Anchors, support angles or consoles {(not used, seeE04F13/0801)}	E04F13/22	E04F13/22		121
E04F13/23	11	adjustable {(not used, seeE04F13/0801)}	E04F13/23	E04F13/23		35
E04F13/24	10	Hidden fastening means on the rear of the covering or lining elements (E04F13/30 takes precedence){(not used, seeE04F13/0801)}	E04F13/24	E04F13/24		154
E04F13/25	11	adjustable {(not used, seeE04F13/0801)}	E04F13/25	E04F13/25		35
E04F13/26	10	Edge engaging fastening means, e.g. clamps, clips or border profiles {(not used, seeE04F13/0801)}	E04F13/26	E04F13/26		90
E04F13/28	11	adjustable {(not used, seeE04F13/0801)}	E04F13/28	E04F13/28		14
E04F13/30	10	Magnetic fastening means {(not used, seeE04F13/0883)}	E04F13/30	E04F13/30		25
E04F15/00	7	Flooring (stair treads E04F11/104; coverings not specially adapted for floors E04F13/00; borders, skirtings E04F19/02; {implements for laying flooring E04F21/20;} gratings for cleaning soles of footwear A47L23/24; {built-in gratings E04F19/10; removing floor coverings E04G23/00; carpets A47G27/00;} of similar materials to roads E01C; basic or rough floors {, structural floors}E04B5/00)	E04F15/00	E04F15/00		670
E04F15/02	8	Flooring or floor layers composed of a number of similar elements (of webs E04F15/16)	E04F15/02	E04F15/02		6771
E04F15/02005	9	{Construction of joints, e.g. dividing strips (E04F15/024, E04F15/04, E04F15/06, E04F15/10 and E04F15/14 take precedence; separate provisional spacers E04F21/0092)}	E04F15/02	E04F15/02		843
E04F15/02011	10	{with joint fillings integrated in the flooring elements}	E04F15/02	E04F15/02		194
E04F15/02016	10	{with sealing elements between flooring elements (sealings of joints between building constructions in general E04B1/68)}	E04F15/02	E04F15/02		720
E04F15/02022	10	{with means for aligning the outer surfaces of the flooring elements (E04F15/02038 takes precedence)}	E04F15/02	E04F15/02		356
E04F15/02027	10	{Means for spacing the flooring from an adjoining wall}	E04F15/02	E04F15/02		125
E04F15/02033	10	{Joints with beveled or recessed upper edges}	E04F15/02	E04F15/02		444
E04F15/02038	9	{characterised by tongue and groove connections between neighbouring flooring elements}	E04F15/02	E04F15/02		3085
E04F15/02044	9	{Separate elements for fastening to an underlayer (E04F15/02133, E04F15/0215 take precedence)}	E04F15/02	E04F15/02		1670
E04F2015/0205	10	{with load-supporting elongated furring elements between the flooring elements and the underlayer}	E04F15/02	E04F15/02		477
E04F2015/02055	11	{with additional supporting elements between furring elements and underlayer}	E04F15/02	E04F15/02		172
E04F2015/02061	12	{adjustable perpendicular to the underlayer}	E04F15/02	E04F15/02		271
E04F2015/02066	11	{with additional fastening elements between furring elements and flooring elements}	E04F15/02	E04F15/02		146
E04F2015/02072	12	{the additional fastening elements extending into the back side of the flooring elements (E04F2015/021 takes precedence)}	E04F15/02	E04F15/02		185
E04F2015/02077	12	{the additional fastening elements located in-between two adjacent flooring elements}	E04F15/02	E04F15/02		124
E04F2015/02083	13	{Piercing the side faces of the flooring elements}	E04F15/02	E04F15/02		42
E04F2015/02088	13	{Engaging side holes preformed into the flooring elements}	E04F15/02	E04F15/02		47
E04F2015/02094	13	{Engaging side grooves running along the whole length of the flooring elements}	E04F15/02	E04F15/02		576
E04F2015/021	12	{fixed by means of hooking means on the back side of the flooring elements}	E04F15/02	E04F15/02		54
E04F2015/02105	10	{without load-supporting elongated furring elements between the flooring elements and the underlayer}	E04F15/02	E04F15/02		59
E04F2015/02111	11	{not adjustable}	E04F15/02	E04F15/02		120
E04F2015/02116	12	{with fastening elements extending into the back side of the flooring elements}	E04F15/02	E04F15/02		90
E04F2015/02122	12	{with fastening elements engaging holes or grooves in the side faces of the flooring elements (E04F2015/02116 takes precedence)}	E04F15/02	E04F15/02		191
E04F2015/02127	11	{adjustable perpendicular to the underlayer (E04F15/02464 takes precedence)}	E04F15/02	E04F15/02		198
E04F15/02133	9	{fixed directly to an underlayer by means of magnets, hook and loop-type or similar fasteners, not necessarily involving the side faces of the flooring elements}	E04F15/02	E04F15/02		67
E04F15/02138	10	{by hook and loop-type fasteners}	E04F15/02	E04F15/02		112
E04F15/02144	10	{by magnets}	E04F15/02	E04F15/02		133
E04F15/0215	9	{specially adapted for being adhesively fixed to an underlayer; Fastening means therefor; Fixing by means of plastics materials hardening after application}	E04F15/02	E04F15/02		498
E04F15/02155	10	{Adhesive means specially adapted therefor, e.g. adhesive foils or strips}	E04F15/02	E04F15/02		193
E04F15/02161	9	{Floor elements with grooved main surface}	E04F15/02	E04F15/02		429
E04F15/02166	10	{wherein the grooves are filled with inserts}	E04F15/02	E04F15/02		195
E04F15/02172	9	{Floor elements with an anti-skid main surface, other than with grooves}	E04F15/02	E04F15/02		888
E04F15/02177	9	{Floor elements for use at a specific location (not used, see subgroups)}	E04F15/02	E04F15/02		47
E04F15/02183	10	{for outdoor use, e.g. in decks, patios, terraces, verandas or the like}	E04F15/02	E04F15/02		1336
E04F15/02188	10	{for use in wet rooms}	E04F15/02	E04F15/02		582
E04F15/02194	9	{Flooring consisting of a number of elements carried by a non-rollable common support plate or grid (E04F15/022 takes precedence)}	E04F15/02	E04F15/02		756
E04F15/022	9	Flooring consisting of parquetry tiles on a non-rollable sub-layer of other material, e.g. board, concrete, cork	E04F15/022	E04F15/022		686
E04F15/024	9	Sectional false floors, e.g. computer floors {(height-adjustable supports for terrace roof coverings E04D11/00; underfloor heating using water F24D3/142, using air F24D5/10; installation of cables, lines or protective tubing in floors H02G3/28)}	E04F15/024	E04F15/024		1040
E04F15/02405	10	{Floor panels}	E04F15/024	E04F15/024		1056
E04F15/02411	11	{with integrated feet (E04F15/02417 takes precedence)}	E04F15/024	E04F15/024		187
E04F15/02417	11	{made of box-like elements}	E04F15/024	E04F15/024		116
E04F15/02423	12	{filled with core material}	E04F15/024	E04F15/024		122
E04F15/02429	13	{the core material hardening after application}	E04F15/024	E04F15/024		259
E04F15/02435	11	{Sealing joints}	E04F15/024	E04F15/024		132
E04F15/02441	12	{Sealing strips integrated with the floor panels}	E04F15/024	E04F15/024		89
E04F15/02447	10	{Supporting structures}	E04F15/024	E04F15/024		795
E04F15/02452	11	{Details of junctions between the supporting structures and the panels or a panel-supporting framework}	E04F15/024	E04F15/024		979
E04F15/02458	11	{Framework supporting the panels}	E04F15/024	E04F15/024		955
E04F15/02464	11	{Height adjustable elements for supporting the panels or a panel-supporting framework}	E04F15/024	E04F15/024		657
E04F15/0247	12	{Screw jacks}	E04F15/024	E04F15/024		612
E04F15/02476	13	{height-adjustable from the upper side of the floor}	E04F15/024	E04F15/024		337
E04F15/02482	13	{with a variable angle between panel and support}	E04F15/024	E04F15/024		130
E04F15/02488	12	{filled with material hardening after application}	E04F15/024	E04F15/024		94
E04F15/02494	11	{with a plurality of base plates or like, each base plate having a plurality of pedestals upstanding therefrom to receive the floor panels}	E04F15/024	E04F15/024		140
E04F15/04	9	only of wood {or with a top layer of wood}, e.g. with wooden {or metal} connecting members (rollable parquet E04F15/16)	E04F15/04	E04F15/04		3950
E04F15/041	10	{with a top layer of wood in combination with a lower layer of other material}	E04F15/04	E04F15/04		700
E04F15/042	11	{the lower layer being of fibrous or chipped material, e.g. bonded with synthetic resins}	E04F15/04	E04F15/04		197
E04F15/043	11	{the lower layer being of organic plastic with or without reinforcements or filling materials}	E04F15/04	E04F15/04		250
E04F15/045	10	{Layered panels only of wood}	E04F15/04	E04F15/04		434
E04F15/046	11	{Plywood panels}	E04F15/04	E04F15/04		197
E04F15/047	10	{with a butcher-block like top surface}	E04F15/04	E04F15/04		82
E04F15/048	10	{with a top surface of assembled elongated wooden strip type}	E04F15/04	E04F15/04		153
E04F15/06	9	of metal, whether or not in combination with other material (gratings as building elements E04C2/42{; of elements with a metal upper layer; E04F15/02405 takes precedence; metal treads E04F11/112})	E04F15/06	E04F15/06		958
E04F15/08	9	only of stone or stone-like material, e.g. {ceramics}, concrete; of glass {or with a top layer of stone or stone-like material, e.g. ceramics, concrete or glass (E04F15/02005 takes precedence)}	E04F15/08	E04F15/08		1964
E04F15/082	10	{with a top layer of stone or stone-like material, e.g. ceramics, concrete or glass in combination with a lower layer of other material}	E04F15/08	E04F15/08		673
E04F15/085	11	{The lower layer being of fibrous or chipped material, e.g. bonded with synthetic resins}	E04F15/08	E04F15/08		84
E04F15/087	11	{The lower layer being of organic plastic with or without reinforcements or filling materials}	E04F15/08	E04F15/08		226
E04F15/10	9	of other materials, e.g. fibrous or chipped materials, organic plastics, magnesite {tiles}, hardboard {, or with a top layer of other materials}	E04F15/10	E04F15/10		2401
E04F15/102	10	{of fibrous or chipped materials, e.g. bonded with synthetic resins}	E04F15/10	E04F15/10		964
E04F15/105	10	{of organic plastics with or without reinforcements or filling materials}	E04F15/10	E04F15/10		2064
E04F15/107	10	{composed of several layers, e.g. sandwich panels (layered products in general B32B; producing decorative panels or veneers B44C5/04)}	E04F15/10	E04F15/10		2932
E04F15/12	8	Flooring or floor layers made of masses in situ, e.g. seamless magnesite floors, terrazzo {gypsum floors}(inorganic or bituminous masses C04B; organic plastic masses C08L)	E04F15/12	E04F15/12		2476
E04F15/123	9	{Lost formworks for producing hollow floor screed layers, e.g. for receiving installations, ducts, cables (structural floors E04B5/00; filling elements for building-up floors E04B5/26; installation of cables, lines or protective tubing in floors H02G3/28)}	E04F15/12	E04F15/12		87
E04F15/126	9	{Terrazzo floors}	E04F15/12	E04F15/12		108
E04F15/14	9	Construction of joints, e.g. dividing strips ({E04F15/02005 takes precedence;} sealing joints not restricted to flooring E04B1/68{, construction of joints in roads or airfields E01C11/02})	E04F15/14	E04F15/14		887
E04F15/142	10	{Dividing strips or boundary strips}	E04F15/14	E04F15/14		268
E04F15/145	11	{adjustable in height}	E04F15/14	E04F15/14		32
E04F15/147	11	{interconnected to form a grid-like structure}	E04F15/14	E04F15/14		14
E04F15/16	8	Flooring, e.g. parquet on flexible web, laid as flexible webs; Webs specially adapted for use as flooring; {Parquet on flexible web}(resiliently-mounted floors, e.g. sprung floors, E04F15/22; linoleum D06N; {carpets A47G27/00})	E04F15/16	E04F15/16		342
E04F15/163	9	{Webs specially adapted for use as finishing layers}	E04F15/16	E04F15/16		97
E04F15/166	9	{Flooring consisting of a number of elements carried by a common flexible web, e.g. rollable parquet}	E04F15/16	E04F15/16		169
E04F15/18	8	Separately-laid insulating layers; Other additional insulating measures; Floating floors (insulating of buildings in general E04B1/62)	E04F15/18	E04F15/18		2916
E04F15/181	9	{Insulating layers integrally formed with the flooring or the flooring elements}	E04F15/18	E04F15/18		1715
E04F15/182	9	{Underlayers coated with adhesive or mortar to receive the flooring}	E04F15/18	E04F15/18		981
E04F15/183	10	{for areas prone to frost damage, e.g. for balconies or terraces}	E04F15/18	E04F15/18		63
E04F15/185	9	{Underlayers in the form of studded or ribbed plates}	E04F15/18	E04F15/18		817
E04F15/186	9	{Underlayers covered with a mesh or the like}	E04F15/18	E04F15/18		322
E04F15/187	9	{Underlayers specially adapted to be laid with overlapping edges}	E04F15/18	E04F15/18		138
E04F15/188	9	{Edge insulation strips, e.g. for floor screed layers (boundary strips in layers made of masses in situE04F15/142)}	E04F15/18	E04F15/18		287
E04F15/20	9	for sound insulation	E04F15/20	E04F15/20		2377
E04F15/203	10	{Separately-laid layers for sound insulation}	E04F15/20	E04F15/20		1493
E04F15/206	10	{Layered panels for sound insulation}	E04F15/20	E04F15/20		1324
E04F15/22	8	Resiliently-mounted floors, e.g. sprung floors (laid as webs E04F15/16)	E04F15/22	E04F15/22		1249
E04F15/225	9	{Shock absorber members therefor}	E04F15/22	E04F15/22		935
E04F17/00	7	Vertical ducts; Channels, e.g. for drainage (pipes in general F16L; pipe-line systems F17D{; drainage devices in floors E03F5/04; roof drainage E04D13/04})	E04F17/00	E04F17/00		461
E04F17/005	8	{Lift shafts}	E04F17/00	E04F17/00		616
E04F17/02	8	for carrying away waste gases, e.g. flue gases (free-standing chimneys E04H12/28; connections between fireplace and chimney, chimney fittings, covers for cleaning holes of chimneys F23J; chimney tops F23L); Building elements specially designed therefor, e.g. shaped bricks or sets thereof {(coke-ovens C10B; working measures on existing vertical ducts E04G23/02; apparatus for inserting new lining elements in existing ducts E04G21/16; metallic chimneys, linings, joints and spacers therefor F23J11/00, F23J13/00)}	E04F17/02	E04F17/02		1348
E04F17/023	9	{made of masonry, concrete or other stone-like material; Insulating measures and joints therefor}	E04F17/02	E04F17/02		444
E04F17/026	9	{Exterior cladding, e.g. of chimney parts extending above the roof; Rain covers for chimney tops without draught-inducing aspects (inducing draught in chimneys F23L17/00)}	E04F17/02	E04F17/02		280
E04F17/04	8	Air-ducts or air channels {(heating in general F24; ventilating rooms in general F24F)}	E04F17/04	E04F17/04		1129
E04F17/06	8	Light shafts, e.g. for cellars	E04F17/06	E04F17/06		544
E04F17/08	8	for receiving utility lines, e.g. cables, pipes (covers giving access to the ducts or channels, covers of inspection holes E04F19/08)	E04F17/08	E04F17/08		1063
E04F17/10	8	Arrangements in buildings for the disposal of refuse (refuse bins, gathering or removal of refuse B65F)	E04F17/10	E04F17/10		515
E04F17/12	9	Chutes	E04F17/12	E04F17/12		601
E04F17/123	10	{Cleaning or disinfecting thereof}	E04F17/12	E04F17/12		70
E04F17/126	11	{with water flushing}	E04F17/12	E04F17/12		101
E04F19/00	7	Other details of constructional parts for finishing work on buildings (ladders, e.g. climbing irons, E06C9/04)	E04F19/00	E04F19/00		589
E04F19/005	8	{Chimney mantel pieces}	E04F19/00	E04F19/00		104
E04F19/02	8	Borders; Finishing strips, e.g. beadings; Light coves (for protecting edges of plaster E04F13/06)	E04F19/02	E04F19/02		1924
E04F19/022	9	{for use at vertical intersections of walls (E04F19/028 takes precedence)}	E04F19/02	E04F19/02		407
E04F19/024	10	{for outside use, e.g. imitating brickwork}	E04F19/02	E04F19/02		110
E04F19/026	9	{specially adapted for cushioning impacts}	E04F19/02	E04F19/02		286
E04F19/028	10	{used at protruding corners}	E04F19/02	E04F19/02		269
E04F19/04	9	for use between floor or ceiling and wall, e.g. skirtings	E04F19/04	E04F19/04		1734
E04F2019/0404	10	{characterised by the material}	E04F19/04	E04F19/04		45
E04F2019/0409	11	{of wood}	E04F19/04	E04F19/04		209
E04F2019/0413	11	{of metal}	E04F19/04	E04F19/04		652
E04F2019/0418	11	{of stone or stone like material, e.g. ceramics, concrete;  of glass}	E04F19/04	E04F19/04		142
E04F2019/0422	11	{of organic plastics with or without reinforcements or filling materials}	E04F19/04	E04F19/04		605
E04F2019/0427	12	{with a integrally formed hinge}	E04F19/04	E04F19/04		126
E04F2019/0431	11	{of two or more materials}	E04F19/04	E04F19/04		277
E04F19/0436	10	{between ceiling and wall}	E04F19/04	E04F19/04		842
E04F2019/044	10	{with conduits}	E04F19/04	E04F19/04		555
E04F2019/0445	11	{Ventilating plinths}	E04F19/04	E04F19/04		81
E04F19/045	10	{Hygienic or watertight plinths}	E04F19/04	E04F19/04		496
E04F2019/0454	10	{with decorative effects}	E04F19/04	E04F19/04		674
E04F19/0459	10	{characterised by the fixing method}	E04F19/04	E04F19/04		97
E04F19/0463	11	{Plinths fixed by snap-action in a direction perpendicular to the wall}	E04F19/04	E04F19/04		564
E04F19/0468	11	{Plinths fixed by hooking in a direction parallel to the wall}	E04F19/04	E04F19/04		388
E04F19/0472	11	{Plinths fixed by means of magnets, hook and loop-type or similar fasteners}	E04F19/04	E04F19/04		122
E04F19/0477	11	{Plinths fixed by means of adhesive}	E04F19/04	E04F19/04		431
E04F19/0481	10	{Skirtings or crown mouldings with a separate cladding strip}	E04F19/04	E04F19/04		268
E04F19/0486	10	{Corner filling pieces}	E04F19/04	E04F19/04		214
E04F19/049	10	{Plinths specially adapted for joining wall coverings to floor surfaces}	E04F19/04	E04F19/04		302
E04F19/0495	10	{Plinths fixed around wall openings or around corners of walls}	E04F19/04	E04F19/04		515
E04F19/06	9	specially designed for securing panels {or masking the edges of wall- or floor-covering elements (E04F19/022, E04F19/026 and E04F19/04 take precedence)}	E04F19/06	E04F19/06		758
E04F19/061	10	{used to finish off an edge or corner of a wall or floor covering area (in connection with floor fabrics A47G27/045; sealings between walls and baths A47K3/008)}	E04F19/06	E04F19/06		917
E04F19/062	10	{used between similar elements (separate provisional spacers E04F21/0092)}	E04F19/06	E04F19/06		728
E04F19/063	11	{for simultaneously securing panels having different thicknesses}	E04F19/06	E04F19/06		203
E04F19/064	11	{in corners}	E04F19/06	E04F19/06		393
E04F19/065	10	{Finishing profiles with a T-shaped cross-section or the like}	E04F19/06	E04F19/06		327
E04F19/066	11	{fixed onto a base profile by means of a separate connector}	E04F19/06	E04F19/06		232
E04F19/067	11	{with means preventing a tipping movement}	E04F19/06	E04F19/06		38
E04F19/068	11	{with means allowing a tipping movement}	E04F19/06	E04F19/06		61
E04F19/08	8	Built-in cupboards; Masks of niches; Covers of holes enabling access to installations ({inspection openings in bathtub aprons A47K3/1615; covers for electrical distribution boxes H02G3/14; movable ceiling parts E04B9/003; removable wall partitions E04B2/74; } clean-out doors of chimneys F23J)	E04F19/08	E04F19/08		1265
E04F19/083	9	{Covers with fixing means providing for snap locking}	E04F19/08	E04F19/08		130
E04F19/086	9	{Covers with magnetic fixing means}	E04F19/08	E04F19/08		68
E04F19/10	8	Built-in gratings, e.g. foot-scrapers	E04F19/10	E04F19/10		356
E04F21/00	7	Implements for finishing work on buildings (for working or treating building elements of stone or stone-like material B28D)	E04F21/00	E04F21/00		1977
E04F21/0007	8	{for mounting doors, windows or frames; their fitting (door-lifters B66F15/00)}	E04F21/00	E04F21/00		384
E04F21/0015	9	{for mounting frames}	E04F21/00	E04F21/00		748
E04F21/0023	9	{for mounting door leaves, window sashes or the like}	E04F21/00	E04F21/00		374
E04F21/003	8	{for marking doors, windows or frames (templates for marking the position of hinges E05D11/0009; templates for marking the position of doorlocks E05B17/06)}	E04F21/00	E04F21/00		272
E04F21/0038	8	{for fitting sealing strips or like}	E04F21/00	E04F21/00		143
E04F21/0046	8	{for reshaping butt joints between adjacent panels, e.g. drywall panels (E04F21/165 takes precedence)}	E04F21/00	E04F21/00		32
E04F21/0053	8	{for installing edge-protecting borders}	E04F21/00	E04F21/00		47
E04F21/0061	9	{with crimping means}	E04F21/00	E04F21/00		21
E04F21/0069	8	{for cutting or mounting plinths}	E04F21/00	E04F21/00		126
E04F21/0076	8	{for marking and cutting tiles}	E04F21/00	E04F21/00		349
E04F21/0084	8	{Implements for removing filling material from joints}	E04F21/00	E04F21/00		167
E04F21/0092	8	{Separate provisional spacers used between adjacent floor or wall tiles (E04F13/0889, E04F15/02005 takes precedence)}	E04F21/00	E04F21/00		570
E04F21/02	8	for applying plasticised masses to surfaces, e.g. plastering walls ({wall covering made of hardening materials E04F13/02}; specially for flooring E04F21/20; implements for painting or decorating B44; applying liquids or other fluent materials to surfaces, in general B05)	E04F21/02	E04F21/02		443
E04F21/023	9	{for applying adhesive, e.g. glue or mortar, on the covering elements, in particular tiles}	E04F21/02	E04F21/02		453
E04F21/026	9	{for applying adhesive or joint compound to joint tapes, in particular drywall tapes (joint tapes E04F13/042; drywall taper tools E04F21/1657)}	E04F21/02	E04F21/02		251
E04F21/04	9	Patterns or templates; Jointing rulers {(profile trowels E04F21/16)}	E04F21/04	E04F21/04		817
E04F21/05	10	Supports for jointing rulers	E04F21/05	E04F21/05		239
E04F21/06	9	Implements for applying plaster, insulating material, or the like {(finishing E04F21/16)}	E04F21/06	E04F21/06		1299
E04F21/08	10	Mechanical implements (E04F21/14 takes precedence; spraying in general B05B; sand-blasting B24C)	E04F21/08	E04F21/08		4728
E04F21/085	11	{for filling building cavity walls with insulating materials}	E04F21/08	E04F21/08		307
E04F21/10	11	centrifugally acting	E04F21/10	E04F21/10		238
E04F21/12	11	acting by gas pressure, e.g. steam pressure	E04F21/12	E04F21/12		1626
E04F21/14	10	in shafts, e.g. chimneys	E04F21/14	E04F21/14		133
E04F21/16	9	Implements for after-treatment of plaster or the like {before it has hardened or dried}, e.g. smoothing-tools, profile trowels {(E04F21/04, E04F21/165 take precedence)}	E04F21/16	E04F21/16		1250
E04F21/161	10	{Trowels}	E04F21/16	E04F21/16		612
E04F21/162	11	{with a blade having a notched or toothed edge}	E04F21/16	E04F21/16		201
E04F21/163	11	{with exchangeable blades}	E04F21/16	E04F21/16		221
E04F21/165	8	for finishing joints, e.g. implements for raking or filling joints, jointers (bricklayers&apos; tools E04G21/16; repairing, e.g. filling cracks, E04G23/02{; wallpaper scrapers or the like B44C7/02; implements for cleaning joints A47L13/10})	E04F21/165	E04F21/165		1844
E04F21/1652	9	{for smoothing and shaping joint compound to a desired contour}	E04F21/165	E04F21/165		881
E04F21/1655	9	{for finishing corner joints}	E04F21/165	E04F21/165		550
E04F21/1657	9	{for applying tape to joints, e.g. drywall taper tools}	E04F21/165	E04F21/165		289
E04F21/18	8	for setting wall or ceiling slabs or plates (tools for mosaic work B44C)	E04F21/18	E04F21/18		842
E04F21/1805	9	{Ceiling panel lifting devices}	E04F21/18	E04F21/18		258
E04F21/1811	10	{with hand-driven crank systems, e.g. rope, cable or chain winding or rack-and-pinion mechanisms (E04F21/1816, E04F21/1822 and E04F21/1827 take precedence)}	E04F21/18	E04F21/18		136
E04F21/1816	10	{fluid pressure-operated (E04F21/1822 and E04F21/1827 take precedence)}	E04F21/18	E04F21/18		65
E04F21/1822	10	{with pivotally mounted arms}	E04F21/18	E04F21/18		201
E04F21/1827	10	{Lazy-tongs mechanisms}	E04F21/18	E04F21/18		28
E04F21/1833	10	{spring-force actuated}	E04F21/18	E04F21/18		38
E04F21/1838	9	{for setting a plurality of similar elements (E04F21/1805 and E04F21/1894 take precedence; separate provisional spacers E04F21/0092)}	E04F21/18	E04F21/18		571
E04F21/1844	10	{by applying them one by one}	E04F21/18	E04F21/18		598
E04F21/185	11	{Temporary edge support brackets}	E04F21/18	E04F21/18		352
E04F21/1855	11	{of elongated elements, e.g. sidings}	E04F21/18	E04F21/18		352
E04F21/1861	11	{for setting insulating panels}	E04F21/18	E04F21/18		131
E04F21/1866	11	{using magnets, hook and loop-type fastener or similar means}	E04F21/18	E04F21/18		32
E04F21/1872	11	{using suction-cups}	E04F21/18	E04F21/18		329
E04F21/1877	10	{Leveling devices}	E04F21/18	E04F21/18		401
E04F21/1883	10	{by simultaneously applying several elements, e.g. templates}	E04F21/18	E04F21/18		192
E04F21/1888	11	{using suction-cups}	E04F21/18	E04F21/18		96
E04F21/1894	9	{Lever-type lifters gripping the bottom edge of wall panels (door lifters B66F15/00)}	E04F21/18	E04F21/18		195
E04F21/20	8	for laying flooring (made of similar material to roads or pavements E01C{; arrangements for removing of previously fixed floor covering E04G23/00})	E04F21/20	E04F21/20		851
E04F21/22	9	of single elements, e.g. flooring cramps {; flexible webs (cutting tiles B28D1/225)}	E04F21/22	E04F21/22		2524
E04F21/24	9	of masses made in situ, e.g. smoothing tools {(E04F21/04 takes precedence; finishing of concrete roads or pavings E01C19/40; devices for levelling concrete floors E04G21/10; devices for solidifying concrete floors by vibrating E04G21/066)}	E04F21/24	E04F21/24		1070
E04F21/241	10	{Elongated smoothing blades or plates, e.g. screed apparatus}	E04F21/24	E04F21/24		533
E04F21/242	11	{with vibrating means, e.g. vibrating screeds}	E04F21/24	E04F21/24		255
E04F21/244	11	{with means to adjust the working angle of the leveling blade or plate}	E04F21/24	E04F21/24		257
E04F21/245	10	{Rotary power trowels, i.e. helicopter trowels}	E04F21/24	E04F21/24		272
E04F21/247	11	{used by an operator sitting on the trowel, i.e. ride-on power trowels}	E04F21/24	E04F21/24		118
E04F21/248	11	{used by an operator walking behind the trowel, i.e. walk-behind power trowels}	E04F21/24	E04F21/24		301
E04F21/26	8	for mounting staircases, e.g. tools for marking steps	E04F21/26	E04F21/26		376
E04F21/28	8	for glazing (glass cutters C03B33/10)	E04F21/28	E04F21/28		193
E04F21/30	9	Putty squeezers or guns {(not used, seeB05C17/002)}	E04F21/30	E04F21/30		28
E04F21/32	9	Putty knives; Putty removers	E04F21/32	E04F21/32		200
E04F2201/00	7	Joining sheets or plates or panels	CPCONLY	E04F2201/00		29
E04F2201/01	8	Joining sheets, plates or panels with edges in abutting relationship	CPCONLY	E04F2201/01		239
E04F2201/0107	9	by moving the sheets, plates or panels substantially in their own plane, perpendicular to the abutting edges	CPCONLY	E04F2201/0107		742
E04F2201/0115	10	with snap action of the edge connectors	CPCONLY	E04F2201/0115		745
E04F2201/0123	9	by moving the sheets, plates or panels parallel to the abutting edges	CPCONLY	E04F2201/0123		179
E04F2201/013	10	with snap action of the edge connectors	CPCONLY	E04F2201/013		17
E04F2201/0138	9	by moving the sheets, plates or panels perpendicular to the main plane	CPCONLY	E04F2201/0138		680
E04F2201/0146	10	with snap action of the edge connectors	CPCONLY	E04F2201/0146		451
E04F2201/0153	9	by rotating the sheets, plates or panels around an axis which is parallel to the abutting edges, possibly combined with a sliding movement	CPCONLY	E04F2201/0153		1080
E04F2201/0161	10	with snap action of the edge connectors	CPCONLY	E04F2201/0161		190
E04F2201/0169	9	by rotating the sheets, plates or panels around an axis which is perpendicular to the abutting edges and parallel to the main plane, possibly combined with a sliding movement	CPCONLY	E04F2201/0169		30
E04F2201/0176	10	with snap action of the edge connectors	CPCONLY	E04F2201/0176		54
E04F2201/0184	9	by rotating the sheets, plates or panels around an axis which is perpendicular to the abutting edges and perpendicular to the main plane, possibly combined with a sliding movement	CPCONLY	E04F2201/0184		12
E04F2201/0192	10	with snap action of the edge connectors	CPCONLY	E04F2201/0192		1
E04F2201/02	8	Non-undercut connections, e.g. tongue and groove connections	CPCONLY	E04F2201/02		238
E04F2201/021	9	with separate protrusions	CPCONLY	E04F2201/021		258
E04F2201/022	10	with tongue or grooves alternating longitudinally along the edge	CPCONLY	E04F2201/022		138
E04F2201/023	9	with a continuous tongue or groove	CPCONLY	E04F2201/023		1372
E04F2201/025	9	with tongue and grooves alternating transversally in the direction of the thickness of the panel, e.g. multiple tongue and grooves oriented parallel to each other	CPCONLY	E04F2201/025		261
E04F2201/026	9	with rabbets, e.g. being stepped	CPCONLY	E04F2201/026		377
E04F2201/027	9	connected by tongues and grooves, the centerline of the connection being inclined to the top surface	CPCONLY	E04F2201/027		86
E04F2201/028	9	connected by tongues and grooves with triangular shape	CPCONLY	E04F2201/028		128
E04F2201/03	8	Undercut connections, e.g. using undercut tongues or grooves	CPCONLY	E04F2201/03		344
E04F2201/035	9	Dovetail connections	CPCONLY	E04F2201/035		150
E04F2201/04	8	Other details of tongues or grooves	CPCONLY	E04F2201/04		147
E04F2201/041	9	Tongues or grooves with slits or cuts for expansion or flexibility	CPCONLY	E04F2201/041		206
E04F2201/042	9	with grooves positioned on the rear-side of the panel	CPCONLY	E04F2201/042		400
E04F2201/043	9	with tongues and grooves being formed by projecting or recessed parts of the panel layers	CPCONLY	E04F2201/043		762
E04F2201/044	9	with tongues or grooves comprising elements which are not manufactured in one piece with the sheets, plates or panels but which are permanently fixedly connected to the sheets, plates or panels, e.g. at the factory	CPCONLY	E04F2201/044		93
E04F2201/045	10	wherein the elements are made of wood	CPCONLY	E04F2201/045		16
E04F2201/046	10	wherein the elements are made of metal	CPCONLY	E04F2201/046		33
E04F2201/047	10	wherein the elements are made of stone or stone like material, e.g. ceramics, concrete; of glass	CPCONLY	E04F2201/047		2
E04F2201/048	10	wherein the elements are made of fibres or chips, e.g. bonded with synthetic resins	CPCONLY	E04F2201/048		6
E04F2201/049	10	wherein the elements are made of organic plastics with or without reinforcements or filling materials	CPCONLY	E04F2201/049		101
E04F2201/05	8	Separate connectors or inserts, e.g. pegs, pins, keys or strips	CPCONLY	E04F2201/05		908
E04F2201/0505	9	Pegs or pins	CPCONLY	E04F2201/0505		371
E04F2201/0511	9	Strips or bars, e.g. nailing strips	CPCONLY	E04F2201/0511		522
E04F2201/0517	9	U- or C-shaped brackets and clamps	CPCONLY	E04F2201/0517		651
E04F2201/0523	9	Separate tongues; Interlocking keys, e.g. joining mouldings of circular, square or rectangular shape	CPCONLY	E04F2201/0523		352
E04F2201/0529	10	the interlocking key acting as a dovetail-type key	CPCONLY	E04F2201/0529		110
E04F2201/0535	10	adapted for snap locking	CPCONLY	E04F2201/0535		138
E04F2201/0541	10	adapted to be moved along the joint edge	CPCONLY	E04F2201/0541		63
E04F2201/0547	10	adapted to be moved perpendicular to the joint edge	CPCONLY	E04F2201/0547		172
E04F2201/0552	10	adapted to be rotated around an axis parallel to the joint edge	CPCONLY	E04F2201/0552		86
E04F2201/0558	10	adapted to be rotated around an axis perpendicular to the joint edge	CPCONLY	E04F2201/0558		18
E04F2201/0564	10	depending on the use of specific materials	CPCONLY	E04F2201/0564		1
E04F2201/057	11	of wood	CPCONLY	E04F2201/057		10
E04F2201/0576	11	of metal	CPCONLY	E04F2201/0576		22
E04F2201/0582	11	of fibres or chips, e.g. bonded with synthetic resins	CPCONLY	E04F2201/0582		6
E04F2201/0588	11	of organic plastics with or without reinforcements or filling materials	CPCONLY	E04F2201/0588		60
E04F2201/0594	9	Hinge-like connectors	CPCONLY	E04F2201/0594		107
E04F2201/06	8	Magnets	CPCONLY	E04F2201/06		127
E04F2201/07	8	with connections using a special adhesive material	CPCONLY	E04F2201/07		589
E04F2201/08	8	hook and loop-type fastener or similar fixing means	CPCONLY	E04F2201/08		97
E04F2201/09	8	Puzzle-type connections for interlocking male and female panel edge-parts	CPCONLY	E04F2201/09		42
E04F2201/091	9	with the edge-parts forming part of the panel body	CPCONLY	E04F2201/091		206
E04F2201/093	9	with the edge-parts being separate elements not being part of the panel body	CPCONLY	E04F2201/093		25
E04F2201/095	9	with both connection parts, i.e. male and female connection parts alternating on one edge	CPCONLY	E04F2201/095		231
E04F2201/096	9	with only one type of connection parts, i.e. with male or female on one edge	CPCONLY	E04F2201/096		104
E04F2201/098	9	wherein the interlocking male and female edge-parts have a dovetail, mushroom or similar shape	CPCONLY	E04F2201/098		98
E04F2203/00	7	Specially structured or shaped covering, lining or flooring elements not otherwise provided for	CPCONLY	E04F2203/00		86
E04F2203/02	8	having particular shapes, other than square or rectangular, e.g. triangular, hexagonal, circular, irregular	CPCONLY	E04F2203/02		162
E04F2203/023	9	having triangular shapes	CPCONLY	E04F2203/023		65
E04F2203/026	9	having hexagonal shapes	CPCONLY	E04F2203/026		64
E04F2203/04	8	comprising a plurality of internal elongated cavities arranged in substantially parallel rows	CPCONLY	E04F2203/04		442
E04F2203/06	8	comprising two layers fixedly secured to one another, in offset relationship in order to form a rebate	CPCONLY	E04F2203/06		122
E04F2203/065	9	in offset relationship longitudinally as well as transversely	CPCONLY	E04F2203/065		82
E04F2203/08	8	with a plurality of grooves or slits in the back side, to increase the flexibility or bendability of the elements	CPCONLY	E04F2203/08		154
E04F2290/00	7	Specially adapted covering, lining or flooring elements not otherwise provided for	CPCONLY	E04F2290/00		211
E04F2290/02	8	for accommodating service installations or utility lines, e.g. heating conduits, electrical lines, lighting devices or service outlets	CPCONLY	E04F2290/02		821
E04F2290/023	9	for heating	CPCONLY	E04F2290/023		2591
E04F2290/026	9	for lighting	CPCONLY	E04F2290/026		656
E04F2290/04	8	for insulation or surface protection, e.g. against noise, impact or fire	CPCONLY	E04F2290/04		2677
E04F2290/041	9	against noise	CPCONLY	E04F2290/041		2748
E04F2290/042	10	with a facing or top layer for sound insulation	CPCONLY	E04F2290/042		175
E04F2290/043	10	with a bottom layer for sound insulation	CPCONLY	E04F2290/043		715
E04F2290/044	9	against impact	CPCONLY	E04F2290/044		1324
E04F2290/045	9	against fire	CPCONLY	E04F2290/045		973
E04F2290/046	10	with a facing or top layer for fire insulation	CPCONLY	E04F2290/046		194
E04F2290/047	10	with a bottom layer for fire insulation	CPCONLY	E04F2290/047		185
E04F2290/048	9	against static electricity	CPCONLY	E04F2290/048		235
