F16D1/00	7	Couplings for rigidly connecting two coaxial shafts or other movable machine elements (attachment of wheels to axles for railway carriages B60B; for attachment of cranks to their shafts F16C3/10)	F16D1/00	F16D1/00		232
F16D1/02	8	for connecting two abutting shafts or the like	F16D1/02	F16D1/02		826
F16D1/027	9	non-disconnectable, e.g. involving gluing, welding or the like	F16D1/027	F16D1/027		201
F16D1/033	9	by clamping together two faces perpendicular to the axis of rotation, e.g. with bolted flanges	F16D1/033	F16D1/033		849
F16D1/04	9	with clamping hub; with hub and longitudinal key	F16D1/04	F16D1/04		637
F16D1/05	10	with radial clamping due to axial loading of at least one pair of conical surfaces	F16D1/05	F16D1/05		264
F16D1/06	8	for attachment of a member on a shaft or on a shaft-end (attachment of marine propellers on shafts B63H23/34)	F16D1/06	F16D1/06		1652
F16D2001/062	9	{characterised by adaptors where hub bores being larger than the shaft}	F16D1/06	F16D1/06		201
F16D1/064	9	non-disconnectable	F16D1/064	F16D1/064		70
F16D1/068	10	involving gluing, welding or the like	F16D1/068	F16D1/068		462
F16D1/072	10	involving plastic deformation (plastic welding F16D1/068)	F16D1/072	F16D1/072		790
F16D1/076	9	by clamping together two faces perpendicular to the axis of rotation, e.g. with bolted flanges	F16D1/076	F16D1/076		1051
F16D1/08	9	with clamping hub; with hub and longitudinal key	F16D1/08	F16D1/08		611
F16D1/0805	10	{with radial clamping due to deformation of a resilient body or a body of fluid (F16D1/091 takes precedence; elastic couplings F16D3/80; fluid pressure clutches F16D25/04)}	F16D1/08	F16D1/08		276
F16D1/0811	10	{with radial clamping due to tilting of a hub part or ring about a diametral axis}	F16D1/08	F16D1/08		64
F16D1/0817	10	{with radial clamping due to rotation along an eccentric surface, e.g. arcuate wedging elements (similar clutches F16D17/00; similar free-wheel clutches F16D41/06)}	F16D1/08	F16D1/08		198
F16D1/0823	10	{with radial clamping of a helical wrap spring on the shaft or in the hub bore (similar clutches F16D13/025, F16D13/08, F16D27/025, F16D27/105; similar slip couplings F16D7/022; similar free-wheel clutches F16D41/206)}	F16D1/08	F16D1/08		38
F16D1/0829	10	{with radial loading of both hub and shaft by an intermediate ring or sleeve (F16D1/0817, F16D1/0823, F16D1/093 take precedence)}	F16D1/08	F16D1/08		105
F16D1/0835	11	{due to the elasticity of the ring or sleeve}	F16D1/08	F16D1/08		368
F16D1/0841	11	{due to axial loading of the ring or sleeve, e.g. Belleville washers}	F16D1/08	F16D1/08		96
F16D1/0847	10	{with radial clamping due to a radial screw}	F16D1/08	F16D1/08		403
F16D1/0852	10	{with radial clamping between the mating surfaces of the hub and shaft (F16D1/0805&#160;-&#160;F16D1/0817, F16D1/09 take precedence)}	F16D1/08	F16D1/08		75
F16D1/0858	11	{due to the elasticity of the hub (including shrink fits)}	F16D1/08	F16D1/08		553
F16D1/0864	11	{due to tangential loading of the hub, e.g. a split hub}	F16D1/08	F16D1/08		855
F16D1/087	11	{due to other loading elements in the hub or shaft}	F16D1/08	F16D1/08		135
F16D1/0876	10	{with axial keys and no other radial clamping}	F16D1/08	F16D1/08		801
F16D1/0882	11	{the key being axially tapered and tightening when loaded axially}	F16D1/08	F16D1/08		116
F16D1/0888	12	{the key having two axially tapered interengaging parts}	F16D1/08	F16D1/08		97
F16D1/0894	10	{with other than axial keys, e.g. diametral pins, cotter pins and no other radial clamping}	F16D1/08	F16D1/08		359
F16D1/09	10	with radial clamping due to axial loading of at least one pair of conical surfaces {(tapered keys F16D1/0882)}	F16D1/09	F16D1/09		337
F16D2001/0903	11	{the clamped shaft being hollow}	F16D1/09	F16D1/09		111
F16D2001/0906	11	{using a hydraulic fluid to clamp or disconnect, not provided for in F16D1/091}	F16D1/09	F16D1/09		93
F16D1/091	11	and comprising a chamber including a tapered piston moved axially by fluid pressure to effect clamping	F16D1/091	F16D1/091		74
F16D1/092	11	the pair of conical mating surfaces being provided on the coupled hub and shaft	F16D1/092	F16D1/092		391
F16D1/093	11	using one or more elastic segmented conical rings forming at least one of the conical surfaces, the rings being expanded or contracted to effect clamping (F16D1/091 takes precedence)	F16D1/093	F16D1/093		201
F16D1/094	12	using one or more pairs of elastic or segmented rings with mutually mating conical surfaces, one of the mating rings being contracted and the other being expanded	F16D1/094	F16D1/094		399
F16D2001/0945	13	{using multiple pairs of elastic or segmented rings to effect clamping}	F16D1/094	F16D1/094		55
F16D1/095	12	with clamping effected by ring contraction only {(for connecting two abutting shafts F16D1/02)}	F16D1/095	F16D1/095		290
F16D2001/0955	13	{the clamping is effected by hub contraction, i.e. a compression of the hub instead of the ring}	F16D1/095	F16D1/095		42
F16D1/096	13	the ring or rings being located between the shaft and the hub	F16D1/096	F16D1/096		523
F16D1/097	12	with clamping effected by ring expansion only, e.g. with an expanded ring located between hub and shaft	F16D1/097	F16D1/097		206
F16D1/10	8	Quick-acting couplings in which the parts are connected by simply bringing them together axially	F16D1/10	F16D1/10		889
F16D1/101	9	{without axial retaining means rotating with the coupling}	F16D1/10	F16D1/10		872
F16D2001/102	9	{the torque is transmitted via polygon shaped connections}	F16D1/10	F16D1/10		527
F16D2001/103	9	{the torque is transmitted via splined connections}	F16D1/10	F16D1/10		2117
F16D1/104	9	having retaining means rotating with the coupling and acting only by friction	F16D1/104	F16D1/104		217
F16D1/108	9	having retaining means rotating with the coupling and acting by interengaging parts, i.e. positive coupling	F16D1/108	F16D1/108		711
F16D1/112	10	the interengaging parts comprising torque-transmitting surfaces, e.g. bayonet joints	F16D1/112	F16D1/112		375
F16D1/116	10	the interengaging parts including a continuous or interrupted circumferential groove in the surface of one of the coupling parts (circlips for retaining hubs on shafts F16B21/18)	F16D1/116	F16D1/116		954
F16D1/12	8	allowing adjustment of the parts about the axis (during motion F16D3/10)	F16D1/12	F16D1/12		407
F16D3/00	7	Yielding couplings, i.e. with means permitting movement between the connected parts during the drive (couplings disconnectable simply by axial movement F16D1/10; slip couplings F16D7/00)	F16D3/00	F16D3/00		416
F16D3/005	8	{incorporating leaf springs, flexible parts of reduced thickness or the like acting as pivots}	F16D3/00	F16D3/00		214
F16D3/02	8	adapted to specific functions	F16D3/02	F16D3/02		497
F16D3/04	9	specially adapted to allow radial displacement, e.g. Oldham couplings	F16D3/04	F16D3/04		971
F16D3/06	9	specially adapted to allow axial displacement	F16D3/06	F16D3/06		1787
F16D3/065	10	{by means of rolling elements}	F16D3/06	F16D3/06		503
F16D3/08	9	Couplings for intersecting shafts, provided with intermediate bars bent in an angle corresponding with the angle of intersection	F16D3/08	F16D3/08		142
F16D3/10	9	Couplings with means for varying the angular relationship of two coaxial shafts during motion	F16D3/10	F16D3/10		695
F16D3/12	9	specially adapted for accumulation of energy to absorb shocks or vibration (by making use of fluid elements F16D3/80)	F16D3/12	F16D3/12		1430
F16D3/14	9	combined with a friction coupling for damping vibration or absorbing shock	F16D3/14	F16D3/14		429
F16D3/16	8	Universal joints in which flexibility is produced by means of pivots or sliding or rolling connecting parts	F16D3/16	F16D3/16		815
F16D3/18	9	the coupling parts (1) having slidably-interengaging teeth	F16D3/18	F16D3/18		428
F16D3/185	10	{radial teeth connecting concentric inner and outer coupling parts}	F16D3/18	F16D3/18		1180
F16D3/20	9	one coupling part entering a sleeve of the other coupling part and connected thereto by sliding or rolling members (F16D3/18, F16D3/24 take precedence)<br><br><u>NOTE</u><br><br>"coupling parts" means the driving member and the driven member of the coupling to be mounted on and rotate as a unit with the shafts or their equivalents between which the coupling is placed. An intermediate member interconnecting these parts is regarded as such an equivalent.	F16D3/20	F16D3/20		554
F16D3/202	10	one coupling part having radially projecting pins, e.g. tripod joints	F16D3/202	F16D3/202		205
F16D2003/2023	11	{with linear rolling bearings between raceway and trunnion mounted shoes}	F16D3/202	F16D3/202		178
F16D2003/2026	11	{with trunnion rings, i.e. with tripod joints having rollers supported by a ring on the trunnion}	F16D3/202	F16D3/202		523
F16D3/205	11	the pins extending radially outwardly from the coupling part	F16D3/205	F16D3/205		187
F16D3/2052	12	{having two pins}	F16D3/205	F16D3/205		494
F16D3/2055	12	{having three pins, i.e. true tripod joints}	F16D3/205	F16D3/205		1472
F16D3/2057	12	{having four or more pins, e.g. with compensation for relative pin movement}	F16D3/205	F16D3/205		119
F16D3/207	11	the pins extending radially inwardly from the coupling part	F16D3/207	F16D3/207		207
F16D3/22	10	the rolling members being balls, rollers, or the like, guided in grooves or sockets in both coupling parts	F16D3/22	F16D3/22		388
F16D3/221	11	the rolling members being located in sockets in one of the coupling parts	F16D3/221	F16D3/221		369
F16D3/223	11	the rolling members being guided in grooves in both coupling parts	F16D3/223	F16D3/223		1414
F16D2003/22303	12	{Details of ball cages}	F16D3/223	F16D3/223		724
F16D2003/22306	12	{having counter tracks, i.e. ball track surfaces which diverge in opposite directions}	F16D3/223	F16D3/223		193
F16D2003/22309	12	{Details of grooves}	F16D3/223	F16D3/223		434
F16D2003/22313	12	{Details of the inner part of the core or means for attachment of the core on the shaft}	F16D3/223	F16D3/223		336
F16D2003/22316	12	{Means for fastening or attaching the bellows or gaiters}	F16D3/223	F16D3/223		275
F16D2003/2232	12	{Elements arranged in the hollow space between the end of the inner shaft and the outer joint member}	F16D3/223	F16D3/223		218
F16D2003/22323	12	{Attachments to the shaft of the inner joint member whereby the attachments are distanced from the core}	F16D3/223	F16D3/223		131
F16D2003/22326	12	{Attachments to the outer joint member, i.e. attachments to the exterior of the outer joint member or to the shaft of the outer joint member}	F16D3/223	F16D3/223		654
F16D3/2233	12	where the track is made up of two curves with a point of inflexion in between, i.e. S-track joints	F16D3/2233	F16D3/2233		85
F16D3/2237	12	where the grooves are composed of radii and adjoining straight lines, i.e. undercut free [UF] type joints	F16D3/2237	F16D3/2237		321
F16D3/224	12	the groove centre-lines in each coupling part lying on a sphere	F16D3/224	F16D3/224		428
F16D3/2245	13	where the groove centres are offset from the joint centre	F16D3/2245	F16D3/2245		302
F16D3/226	12	the groove centre-lines in each coupling part lying on a cylinder co-axial with the respective coupling part	F16D3/226	F16D3/226		109
F16D3/2265	13	{the joints being non-telescopic}	F16D3/226	F16D3/226		73
F16D3/227	13	the joints being telescopic	F16D3/227	F16D3/227		645
F16D3/229	12	Prismatic coupling parts having each groove centre-line lying on planes parallel to the axis of the respective coupling part (F16D3/224, F16D3/226 take precedence)	F16D3/229	F16D3/229		52
F16D3/24	9	comprising balls, rollers, or the like between overlapping driving faces, e.g. cogs, on both coupling parts	F16D3/24	F16D3/24		358
F16D3/26	9	Hooke&apos;s joints or other joints with an equivalent intermediate member to which each coupling part is pivotally or slidably connected (F16D3/18, F16D3/20 take precedence)	F16D3/26	F16D3/26		648
F16D3/265	10	{in which one coupling part has a tongue received with the intermediate member(s) in a recess with a transverse axis in the other coupling part}	F16D3/26	F16D3/26		272
F16D3/28	10	in which the interconnecting pivots include elastic members	F16D3/28	F16D3/28		264
F16D3/30	10	in which the coupling is specially adapted to constant velocity-ratio	F16D3/30	F16D3/30		269
F16D3/32	11	by the provision of two intermediate members each having two relatively perpendicular trunnions or bearings	F16D3/32	F16D3/32		467
F16D3/33	12	with ball or roller bearings	F16D3/33	F16D3/33		136
F16D3/34	11	parts being connected by ridges, pins, balls, or the like guided in grooves or between cogs	F16D3/34	F16D3/34		290
F16D3/36	10	in which each pivot between the coupling parts and the intermediate member comprises a single ball	F16D3/36	F16D3/36		105
F16D3/38	10	with a single intermediate member with trunnions or bearings arranged on two axes perpendicular to one another (F16D3/36 takes precedence)	F16D3/38	F16D3/38		538
F16D3/382	11	{constructional details of other than the intermediate member}	F16D3/38	F16D3/38		344
F16D3/385	12	{Bearing cup; Bearing construction; Bearing seal; Mounting of bearing on the intermediate member (mounting of bearing in fork F16D3/382)}	F16D3/38	F16D3/38		838
F16D3/387	12	{Fork construction; Mounting of fork on shaft; Adapting shaft for mounting of fork}	F16D3/38	F16D3/38		1130
F16D3/40	11	with intermediate member provided with two pairs of outwardly-directed trunnions on intersecting axes	F16D3/40	F16D3/40		920
F16D3/405	12	{Apparatus for assembling or dismantling}	F16D3/40	F16D3/40		135
F16D3/41	12	with ball or roller bearings	F16D3/41	F16D3/41		1222
F16D3/42	11	with ring-shaped intermediate member provided with bearings or inwardly-directed trunnions	F16D3/42	F16D3/42		213
F16D3/43	12	with ball or roller bearings	F16D3/43	F16D3/43		45
F16D3/44	10	the intermediate member being connected to the coupling parts by ridges, pins, balls, or the like guided in grooves or between cogs	F16D3/44	F16D3/44		152
F16D3/46	11	each coupling part embracing grooves or ridges on the intermediate member	F16D3/46	F16D3/46		214
F16D3/48	9	one coupling part having pins arranged parallel to the axis and entering holes in the other coupling part	F16D3/48	F16D3/48		130
F16D3/50	8	with the coupling parts connected by one or more intermediate members (F16D3/16 takes precedence)	F16D3/50	F16D3/50		887
F16D3/52	9	comprising a continuous strip, spring, or the like engaging the coupling parts at a number of places	F16D3/52	F16D3/52		309
F16D3/54	9	Couplings comprising a chain or strip surrounding two wheels arranged side by side and provided with teeth or the equivalent	F16D3/54	F16D3/54		257
F16D3/56	9	comprising elastic metal lamellae, elastic rods, or the like, e.g. arranged radially or parallel to the axis, the members being shear-loaded collectively by the total load	F16D3/56	F16D3/56		1039
F16D3/58	10	the intermediate members being made of rubber or like material	F16D3/58	F16D3/58		438
F16D3/60	9	comprising pushing or pulling links attached to both parts (F16D3/64 takes precedence)	F16D3/60	F16D3/60		478
F16D3/62	10	the links or their attachments being elastic	F16D3/62	F16D3/62		830
F16D3/64	9	comprising elastic elements arranged between substantially-radial walls of both coupling parts	F16D3/64	F16D3/64		217
F16D3/66	10	the elements being metallic, e.g. in the form of coils	F16D3/66	F16D3/66		523
F16D3/68	10	the elements being made of rubber or similar material	F16D3/68	F16D3/68		1726
F16D3/70	9	comprising elastic elements arranged in holes in one coupling part and surrounding pins on the other coupling part	F16D3/70	F16D3/70		381
F16D3/72	9	with axially-spaced attachments to the coupling parts (F16D3/56 takes precedence)	F16D3/72	F16D3/72		1446
F16D3/725	10	{with an intermediate member made of fibre-reinforced resin (made of rubber-like material F16D3/74; shafts made of fibre-reinforced resin F16C3/026)}	F16D3/72	F16D3/72		118
F16D3/74	10	the intermediate member or members being made of rubber or other {rubber-like} flexible material	F16D3/74	F16D3/74		1039
F16D2003/745	11	{Tyre type coupling, i.e. bellows with only one fold}	F16D3/74	F16D3/74		311
F16D3/76	9	shaped as an elastic ring centered on the axis, surrounding a portion of one coupling part and surrounded by a sleeve of the other coupling part	F16D3/76	F16D3/76		1050
F16D3/77	10	the ring being metallic	F16D3/77	F16D3/77		167
F16D3/78	9	shaped as an elastic disc or flat ring, arranged perpendicular to the axis of the coupling parts, different sets of spots of the disc or ring being attached to each coupling part, e.g. Hardy couplings	F16D3/78	F16D3/78		1223
F16D3/79	10	the disc or ring being metallic	F16D3/79	F16D3/79		389
F16D3/80	8	in which a fluid is used (fluid couplings allowing continuous slip F16D31/00&#160;-&#160;F16D35/00)	F16D3/80	F16D3/80		396
F16D3/82	9	with a coupling element in the form of a pneumatic tube (similar clutches F16D25/04)	F16D3/82	F16D3/82		36
F16D3/84	8	Shrouds, e.g. casings, covers; Sealing means specially adapted therefor	F16D3/84	F16D3/84		559
F16D3/841	9	{Open covers, e.g. guards for agricultural p.t.o. shafts}	F16D3/84	F16D3/84		406
F16D3/843	9	{enclosed covers}	F16D3/84	F16D3/84		318
F16D3/845	10	{allowing relative movement of joint parts due to the flexing of the cover}	F16D3/84	F16D3/84		1428
F16D2003/846	11	{Venting arrangements for flexible seals, e.g. ventilation holes}	F16D3/84	F16D3/84		123
F16D3/848	10	{allowing relative movement of joint parts due to sliding between parts of the cover}	F16D3/84	F16D3/84		290
F16D5/00	7	Impulse couplings, i.e. couplings that alternately accelerate and decelerate the driven member	F16D5/00	F16D5/00		234
F16D7/00	7	Slip couplings, e.g. slipping on overload, for absorbing shock (combined with yielding shaft couplings F16D3/14; fluid slip couplings F16D31/00&#160;-&#160;F16D35/00)	F16D7/00	F16D7/00		254
F16D7/002	8	{the torque being transmitted and limited by yielding of an elastomeric race}	F16D7/00	F16D7/00		89
F16D7/005	8	{the torque being transmitted and limited by rolling friction, e.g. ball bearings axially loaded}	F16D7/00	F16D7/00		88
F16D7/007	8	{the torque being transmitted and limited by rolling surfaces skidding, e.g. skew needle rollers}	F16D7/00	F16D7/00		54
F16D7/02	8	of the friction type	F16D7/02	F16D7/02		443
F16D7/021	9	{with radially applied torque-limiting friction surfaces (F16D7/022 takes precedence)}	F16D7/02	F16D7/02		437
F16D7/022	9	{with a helical band or equivalent member co-operating with a cylindrical torque limiting coupling surface}	F16D7/02	F16D7/02		251
F16D7/024	9	{with axially applied torque limiting friction surfaces}	F16D7/02	F16D7/02		124
F16D7/025	10	{with flat clutching surfaces, e.g. discs}	F16D7/02	F16D7/02		871
F16D7/027	11	{with multiple lamellae}	F16D7/02	F16D7/02		326
F16D7/028	10	{with conical friction surfaces}	F16D7/02	F16D7/02		175
F16D7/04	8	of the ratchet type (similar gearings based on repeated accumulation and delivery of inertia-energy F16H33/08; {overload clutches of the ratchet type F16D43/202})	F16D7/04	F16D7/04		156
F16D7/042	9	{with at least one part moving axially between engagement and disengagement (F16D7/08 takes precedence)}	F16D7/04	F16D7/04		61
F16D7/044	10	{the axially moving part being coaxial with the rotation, e.g. a gear with face teeth}	F16D7/04	F16D7/04		488
F16D7/046	10	{with a plurality of axially moving parts}	F16D7/04	F16D7/04		57
F16D7/048	9	{with parts moving radially between engagement and disengagement (F16D7/10 takes precedence)}	F16D7/04	F16D7/04		345
F16D7/06	9	with intermediate balls or rollers	F16D7/06	F16D7/06		78
F16D7/08	10	moving axially between engagement and disengagement	F16D7/08	F16D7/08		480
F16D7/10	10	moving radially between engagement and disengagement	F16D7/10	F16D7/10		392
F16D9/00	7	Couplings with safety member for disconnecting, e.g. breaking or melting member	F16D9/00	F16D9/00		150
F16D9/02	8	by thermal means, e.g. melting member	F16D9/02	F16D9/02		108
F16D9/04	8	by tensile breaking	F16D9/04	F16D9/04		56
F16D9/06	8	by breaking due to shear stress	F16D9/06	F16D9/06		459
F16D9/08	9	over a single area encircling the axis of rotation, e.g. shear necks on shafts (F16D9/10 takes precedence)	F16D9/08	F16D9/08		185
F16D9/10	9	having a part movable after disconnection so as to provide reconnection, e.g. advanceable shear pins	F16D9/10	F16D9/10		48
F16D11/00	7	Clutches in which the members have interengaging parts (arrangements for synchronisation F16D23/02)	F16D11/00	F16D11/00		429
F16D2011/002	8	{using an external and axially slidable sleeve for coupling the teeth of both coupling components together}	F16D11/00	F16D11/00		456
F16D2011/004	8	{using an internal or intermediate axially slidable sleeve, coupling both components together, whereby the intermediate sleeve is arranged internally at least with respect to one of the components}	F16D11/00	F16D11/00		216
F16D2011/006	8	{Locking or detent means, i.e. means to keep the clutch in engaged condition}	F16D11/00	F16D11/00		250
F16D2011/008	8	{characterised by the form of the teeth forming the inter-engaging parts; Details of shape or structure of these teeth}	F16D11/00	F16D11/00		634
F16D11/02	8	disengaged by a contact of a part mounted on the clutch with a stationarily-mounted member	F16D11/02	F16D11/02		72
F16D11/04	9	with clutching members movable only axially	F16D11/04	F16D11/04		519
F16D11/06	9	with clutching members movable otherwise than only axially, e.g. rotatable keys	F16D11/06	F16D11/06		489
F16D11/08	8	actuated by moving a non-rotating part axially	F16D11/08	F16D11/08		62
F16D11/10	9	with clutching members movable only axially	F16D11/10	F16D11/10		1350
F16D11/12	9	with clutching members movable otherwise than only axially	F16D11/12	F16D11/12		180
F16D11/14	8	with clutching members movable only axially (F16D11/02, F16D11/08 take precedence)	F16D11/14	F16D11/14		1853
F16D11/16	8	with clutching members movable otherwise than only axially (F16D11/02, F16D11/08 take precedence)	F16D11/16	F16D11/16		460
F16D13/00	7	Friction clutches (arrangements for synchronisation F16D23/02)	F16D13/00	F16D13/00		161
F16D13/02	8	disengaged by the contact of a part mounted on the clutch with a stationarily-mounted member	F16D13/02	F16D13/02		167
F16D13/025	9	{with a helical band or equivalent member with two or more turns embracing a drum or the like (electromagnetically actuated F16D27/105)}	F16D13/02	F16D13/02		188
F16D13/04	8	with means for actuating or keeping engaged by a force derived at least partially from one of the shafts to be connected (automatic clutches F16D43/00)	F16D13/04	F16D13/04		470
F16D13/06	9	with clutching members movable otherwise than only axially (F16D13/08, F16D13/12 take precedence)	F16D13/06	F16D13/06		134
F16D13/08	8	with a helical band or equivalent member, which may be built up from linked parts, with more than one turn embracing a drum or the like, with or without an additional clutch actuating the end of the band (F16D13/02 takes precedence; {similar slip couplings F16D7/022; similar clutches electromagnetically actuated F16D27/025, F16D27/105} ; similar free-wheel clutches F16D41/20; similar brakes F16D49/02)	F16D13/08	F16D13/08		411
F16D13/10	8	with clutching members co-operating with the periphery of a drum, a wheel-rim, or the like (F16D13/02&#160;-&#160;F16D13/08 take precedence; similar brakes F16D49/00)	F16D13/10	F16D13/10		327
F16D13/12	8	with an expansible band or coil co-operating with the inner surface of a drum or the like (F16D13/02 takes precedence; similar brakes F16D51/02)	F16D13/12	F16D13/12		415
F16D13/14	8	with outwardly-movable clutching members co-operating with the inner surface of a drum or the like (F16D13/02, F16D13/06, F16D13/12 take precedence; similar brakes F16D51/00)	F16D13/14	F16D13/14		125
F16D13/16	9	shaped as radially-movable segments	F16D13/16	F16D13/16		380
F16D13/18	9	shaped as linked or separately-pivoted segments	F16D13/18	F16D13/18		282
F16D13/20	8	with clutching members co-operating with both the periphery and the inner surface of a drum or wheel-rim (similar brakes F16D53/00)	F16D13/20	F16D13/20		153
F16D13/22	8	with axially-movable clutching members (similar brakes F16D55/00)	F16D13/22	F16D13/22		89
F16D13/24	9	with conical friction surfaces {cone clutches}	F16D13/24	F16D13/24		102
F16D13/26	10	in which the or each axially-movable member is pressed exclusively against an axially-located member	F16D13/26	F16D13/26		320
F16D13/28	11	with means for increasing the effective force between the actuating sleeve or equivalent member and the pressure member	F16D13/28	F16D13/28		188
F16D13/30	12	in which the clutching pressure is produced by springs only	F16D13/30	F16D13/30		69
F16D13/32	10	in which two or more axially-movable members are pressed from one side towards an axially-located member	F16D13/32	F16D13/32		68
F16D13/34	11	with means for increasing the effective force between the actuating sleeve or equivalent member and the pressure member	F16D13/34	F16D13/34		15
F16D13/36	12	in which the clutching pressure is produced by springs only	F16D13/36	F16D13/36		8
F16D13/38	9	with flat clutching surfaces, e.g. discs	F16D13/38	F16D13/38		347
F16D13/385	10	{double clutches, i.e. comprising two friction disc mounted on one driven shaft (with two concentric driven shafts F16D21/06)}	F16D13/38	F16D13/38		629
F16D13/40	10	in which the or each axially-movable member is pressed exclusively against an axially-located member	F16D13/40	F16D13/40		328
F16D13/42	11	with means for increasing the effective force between the actuating sleeve or equivalent member and the pressure member	F16D13/42	F16D13/42		59
F16D13/44	12	in which the clutching pressure is produced by springs only	F16D13/44	F16D13/44		69
F16D13/46	10	in which two axially-movable members, of which one is attached to the driving side and the other to the driven side, are pressed from one side towards an axially-located member	F16D13/46	F16D13/46		194
F16D13/48	11	with means for increasing the effective force between the actuating sleeve or equivalent member and the pressure member	F16D13/48	F16D13/48		107
F16D13/50	12	in which the clutching pressure is produced by springs only	F16D13/50	F16D13/50		345
F16D13/505	13	{Devices located between the flywheel and the driven disc, and biassing the driven disc away from the flywheel towards the disengaged position}	F16D13/50	F16D13/50		38
F16D13/52	10	Clutches with multiple lamellae {; Clutches in which three or more axially moveable members are fixed alternately to the shafts to be coupled and are pressed from one side towards an axially-located member (F16D13/385 takes precedence)}	F16D13/52	F16D13/52		2073
F16D13/54	11	with means for increasing the effective force between the actuating sleeve or equivalent member and the pressure member	F16D13/54	F16D13/54		330
F16D13/56	12	in which the clutching pressure is produced by springs only	F16D13/56	F16D13/56		352
F16D2013/565	13	{with means for releasing the clutch pressure in case of back torque}	F16D13/56	F16D13/56		135
F16D13/58	8	Details {(tools for assembling or disassembling clutches B25B27/0064)}	F16D13/58	F16D13/58		1142
F16D2013/581	9	{Securing means for transportation or shipping}	F16D13/58	F16D13/58		347
F16D13/583	9	{Diaphragm-springs, e.g. Belleville (co-operation with a disengaging thrust ring or bearing F16D23/14)}	F16D13/58	F16D13/58		504
F16D13/585	10	{Arrangements or details relating to the mounting or support of the diaphragm on the clutch on the clutch cover or the pressure plate}	F16D13/58	F16D13/58		1047
F16D2013/586	9	{the cover housing is formed by diaphragm springs}	F16D13/58	F16D13/58		23
F16D2013/588	10	{the diaphragm springs are arranged outside the cover housing}	F16D13/58	F16D13/58		15
F16D13/60	9	Clutching elements (friction lining or attachment thereof F16D69/00)	F16D13/60	F16D13/60		318
F16D13/62	10	Clutch-bands; Clutch shoes; Clutch-drums (brake-bands, brake-shoes, brake-drums F16D65/00)	F16D13/62	F16D13/62		158
F16D13/64	10	Clutch-plates; Clutch-lamellae (brake-plates, brake-lamellae F16D65/12)	F16D13/64	F16D13/64		2325
F16D2013/642	11	{with resilient attachment of frictions rings or linings to their supporting discs or plates for allowing limited axial displacement of these rings or linings}	F16D13/64	F16D13/64		656
F16D13/644	11	{Hub construction}	F16D13/64	F16D13/64		454
F16D13/646	12	{Mounting of the discs on the hub}	F16D13/64	F16D13/64		386
F16D13/648	11	{for clutches with multiple lamellae}	F16D13/64	F16D13/64		1288
F16D13/66	11	of conical shape	F16D13/66	F16D13/66		127
F16D13/68	11	Attachments of plates or lamellae to their supports {(one or more discs connected to the linings transmitting torque to one or more discs connected to the hub by helical springs in windows in the discs, i.e. rotary vibration dampers F16F15/12)}	F16D13/68	F16D13/68		580
F16D13/683	12	{for clutches with multiple lamellae}	F16D13/68	F16D13/68		905
F16D13/686	12	{with one or more intermediate members made of rubber or like material transmitting torque from the linings to the hub}	F16D13/68	F16D13/68		265
F16D13/69	11	Arrangements for spreading lamellae in the released state	F16D13/69	F16D13/69		385
F16D13/70	9	Pressure members, e.g. pressure plates, for clutch-plates or lamellae; Guiding arrangements for pressure members {(clutch flywheels comprising two or more masses with a rotational damper F16F15/12)}	F16D13/70	F16D13/70		1734
F16D2013/703	10	{the pressure plate on the flywheel side is combined with a damper}	F16D13/70	F16D13/70		299
F16D2013/706	10	{the axially movable pressure plate is supported by leaf springs}	F16D13/70	F16D13/70		849
F16D13/71	10	in which the clutching pressure is produced by springs only	F16D13/71	F16D13/71		1702
F16D13/72	9	Features relating to cooling	F16D13/72	F16D13/72		1412
F16D13/74	9	Features relating to lubrication	F16D13/74	F16D13/74		725
F16D13/75	9	Features relating to adjustment, e.g. slack adjusters	F16D13/75	F16D13/75		354
F16D13/752	10	{the adjusting device being located in the actuating mechanism arranged outside the clutch (adjusting "Bowden" mechanisms F16C1/22)}	F16D13/75	F16D13/75		273
F16D13/755	10	{the adjusting device being located in or near the release bearing}	F16D13/75	F16D13/75		128
F16D13/757	10	{the adjusting device being located on or inside the clutch cover, e.g. acting on the diaphragm or on the pressure plate}	F16D13/75	F16D13/75		1197
F16D13/76	8	specially adapted to incorporate with other transmission parts, i.e. at least one of the clutch parts also having another function, e.g. being the disc of a pulley	F16D13/76	F16D13/76		288
F16D15/00	7	Clutches with wedging balls or rollers or with other wedgeable separate clutching members (freewheels, freewheel clutches F16D41/00)	F16D15/00	F16D15/00		653
F16D17/00	7	Clutches in which the drive is transmitted solely by virtue of the eccentricity of the contacting surfaces of clutch members which fit one around the other	F16D17/00	F16D17/00		69
F16D19/00	7	Clutches with mechanically-actuated clutching members not otherwise provided for	F16D19/00	F16D19/00		132
F16D21/00	7	Systems comprising a plurality of actuated clutches (for synchronisation F16D23/04)	F16D21/00	F16D21/00		310
F16D21/02	8	for interconnecting three or more shafts or other transmission members in different ways (in endless-track vehicles B62D)	F16D21/02	F16D21/02		311
F16D21/04	9	with a shaft carrying a number of rotatable transmission members, e.g. gears, each of which can be connected to the shaft by a clutching member or members between the shaft and the hub of the transmission member	F16D21/04	F16D21/04		730
F16D21/06	9	at least two driving shafts or two driven shafts being concentric	F16D21/06	F16D21/06		1818
F16D2021/0607	10	{Double clutch with torque input plate in-between the two clutches, i.e. having a central input plate}	F16D21/06	F16D21/06		336
F16D2021/0615	11	{the central input plate is supported by bearings in-between the two clutches}	F16D21/06	F16D21/06		313
F16D2021/0623	11	{the central input plate having a damper in-between the two clutches}	F16D21/06	F16D21/06		28
F16D2021/063	10	{Electric arrangements for clutch control}	F16D21/06	F16D21/06		19
F16D2021/0638	10	{Electrically actuated multiple lamellae clutches}	F16D21/06	F16D21/06		31
F16D2021/0646	10	{Electrically actuated clutch with two clutch plates}	F16D21/06	F16D21/06		53
F16D2021/0653	10	{Hydraulic arrangements for clutch control}	F16D21/06	F16D21/06		47
F16D2021/0661	10	{Hydraulically actuated multiple lamellae clutches}	F16D21/06	F16D21/06		927
F16D2021/0669	10	{Hydraulically actuated clutches with two clutch plates}	F16D21/06	F16D21/06		189
F16D2021/0676	10	{Mechanically actuated multiple lamellae clutches}	F16D21/06	F16D21/06		133
F16D2021/0684	10	{Mechanically actuated clutches with two clutch plates}	F16D21/06	F16D21/06		527
F16D2021/0692	10	{with two clutches arranged axially without radial overlap}	F16D21/06	F16D21/06		311
F16D21/08	8	Serially-arranged clutches interconnecting two shafts only when all the clutches are engaged (F16D13/08, F16D13/12 take precedence)	F16D21/08	F16D21/08		228
F16D23/00	7	Details of mechanically-actuated clutches not specific for one distinct type	F16D23/00	F16D23/00		136
F16D23/02	8	Arrangements for synchronisation, also for power-operated clutches (shape or mounting of interengaging parts of clutch members to facilitate engagement F16D11/08)	F16D23/02	F16D23/02		724
F16D23/025	9	{Synchro rings}	F16D23/02	F16D23/02		1207
F16D23/04	9	with an additional friction clutch (synchro rings per seF16D23/025)	F16D23/04	F16D23/04		1122
F16D23/06	10	and a blocking mechanism preventing the engagement of the main clutch prior to synchronisation	F16D23/06	F16D23/06		2552
F16D23/0606	11	{the blocking mechanism comprising an axially-extending shouldered pin passing through a hole in a radial wall}	F16D23/06	F16D23/06		232
F16D23/0612	11	{the blocking mechanism comprising a radial pin in an axial slot with at least one branch}	F16D23/06	F16D23/06		342
F16D2023/0618	11	{Details of blocking mechanism comprising a helical spring loaded element, e.g. ball}	F16D23/06	F16D23/06		773
F16D2023/0625	11	{Details of members being coupled, e.g. gears}	F16D23/06	F16D23/06		472
F16D2023/0631	11	{Sliding sleeves; Details thereof}	F16D23/06	F16D23/06		432
F16D2023/0637	11	{Details relating to the hub member on which the sliding is arranged}	F16D23/06	F16D23/06		335
F16D2023/0643	11	{Synchro friction clutches with flat plates, discs or lamellae}	F16D23/06	F16D23/06		222
F16D2023/065	11	{Means to provide additional axial force for self-energising, e.g. by using torque from the friction clutch}	F16D23/06	F16D23/06		122
F16D2023/0656	11	{Details of the tooth structure; Arrangements of teeth}	F16D23/06	F16D23/06		757
F16D2023/0662	12	{Details relating to special geometry of arrangements of teeth}	F16D23/06	F16D23/06		312
F16D2023/0668	12	{Details relating to tooth end or tip geometry}	F16D23/06	F16D23/06		183
F16D2023/0675	12	{Details relating to special undercut geometry}	F16D23/06	F16D23/06		68
F16D2023/0681	11	{Double cone synchromesh clutches}	F16D23/06	F16D23/06		374
F16D2023/0687	11	{Clutches with electrical actuation}	F16D23/06	F16D23/06		69
F16D2023/0693	11	{Clutches with hydraulic actuation}	F16D23/06	F16D23/06		74
F16D23/08	9	with a blocking mechanism that only releases the clutching member on synchronisation (in combination with an additional friction clutch F16D23/06)	F16D23/08	F16D23/08		90
F16D23/10	9	automatically producing the engagement of the clutch when the clutch members are moving at the same speed; Indicating synchronisation	F16D23/10	F16D23/10		309
F16D23/12	8	Mechanical clutch-actuating mechanisms arranged outside the clutch as such (specific for combined clutches F16D21/00; mechanisms specific for synchronisation F16D23/02)	F16D23/12	F16D23/12		2695
F16D2023/123	9	{Clutch actuation by cams, ramps or ball-screw mechanisms}	F16D23/12	F16D23/12		1543
F16D2023/126	9	{Actuation by rocker lever; Rocker levers therefor}	F16D23/12	F16D23/12		373
F16D23/14	9	Clutch-actuating sleeves {or bearings}; Actuating members directly connected to clutch-actuating sleeves {or bearings}	F16D23/14	F16D23/14		2075
F16D2023/141	10	{characterised by using a fork; Details of forks}	F16D23/14	F16D23/14		555
F16D23/142	10	{with a resilient member acting radially between the bearing and its guide means}	F16D23/14	F16D23/14		188
F16D23/143	10	{Arrangements or details for the connection between the release bearing and the diaphragm}	F16D23/14	F16D23/14		204
F16D23/144	11	{With a disengaging thrust-ring distinct from the release bearing, and secured to the diaphragm}	F16D23/14	F16D23/14		65
F16D23/145	12	{Arrangements for the connection between the thrust-ring and the diaphragm}	F16D23/14	F16D23/14		156
F16D23/146	12	{Arrangements for the connection between the thrust-ring and the release bearing}	F16D23/14	F16D23/14		218
F16D23/147	10	{bearing with rolling elements having at least one race or part fixed to the race blind axially, e.g. cup-shaped}	F16D23/14	F16D23/14		36
F16D23/148	10	{Guide-sleeve receiving the clutch release bearing}	F16D23/14	F16D23/14		205
F16D25/00	7	Fluid-actuated clutches	F16D25/00	F16D25/00		217
F16D25/02	8	with means for actuating or keeping engaged by a force derived at least partially from one of the shafts to be connected	F16D25/02	F16D25/02		141
F16D25/04	8	in which the fluid actuates an elastic clutching, {i.e. elastic actuating} member, e.g. a diaphragm or a pneumatic tube (F16D25/02 takes precedence; coupling using a pneumatic tube F16D3/82)	F16D25/04	F16D25/04		85
F16D25/042	9	{the elastic actuating member rotating with the clutch}	F16D25/04	F16D25/04		63
F16D25/044	10	{and causing purely axial movement}	F16D25/04	F16D25/04		213
F16D25/046	10	{and causing purely radial movement}	F16D25/04	F16D25/04		237
F16D25/048	9	{the elastic actuating member not rotating with a coupling part}	F16D25/04	F16D25/04		65
F16D25/06	8	in which the fluid actuates a piston incorporated in, {i.e. rotating with} the clutch (F16D25/02 takes precedence)	F16D25/06	F16D25/06		284
F16D25/061	9	the clutch having interengaging clutch members	F16D25/061	F16D25/061		366
F16D25/062	9	the clutch having friction surfaces	F16D25/062	F16D25/062		114
F16D25/063	10	with clutch members exclusively moving axially	F16D25/063	F16D25/063		120
F16D25/0632	11	with conical friction surfaces, e.g. cone clutches	F16D25/0632	F16D25/0632		158
F16D25/0635	11	with flat friction surfaces, e.g. discs	F16D25/0635	F16D25/0635		658
F16D25/0638	12	with more than two discs, e.g. multiple lamellae	F16D25/0638	F16D25/0638		3814
F16D25/064	11	the friction surface being grooved	F16D25/064	F16D25/064		88
F16D25/065	10	with clutching members having a movement which has at least a radial component	F16D25/065	F16D25/065		132
F16D25/08	8	with fluid-actuated member not rotating with a clutching member (F16D25/02 takes precedence {F16D25/048 takes precedence})	F16D25/08	F16D25/08		1186
F16D2025/081	9	{Hydraulic devices that initiate movement of pistons in secondary cylinders for actuating clutches, i.e. primary cylinders}	F16D25/08	F16D25/08		1006
F16D25/082	9	{the line of action of the fluid-actuated members co-inciding with the axis of rotation}	F16D25/08	F16D25/08		996
F16D25/083	10	{Actuators therefor (F16D25/085&#160;-&#160;F16D25/087 take precedence)}	F16D25/08	F16D25/08		1598
F16D25/085	10	{the clutch actuation being of the pull type}	F16D25/08	F16D25/08		106
F16D25/086	10	{the clutch being actuated by a push rod extending coaxially through the input or output shaft}	F16D25/08	F16D25/08		143
F16D25/087	10	{the clutch being actuated by the fluid-actuated member via a diaphragm spring or an equivalent array of levers (F16D25/085, F16D25/086 take precedence)}	F16D25/08	F16D25/08		557
F16D25/088	9	{the line of action of the fluid-actuated members being distinctly separate from the axis of rotation}	F16D25/08	F16D25/08		852
F16D25/10	8	Clutch systems with a plurality of fluid-actuated clutches (arrangements or mounting of clutches in vehicles B60K17/00)	F16D25/10	F16D25/10		2540
F16D25/12	8	Details not specific to one of the before-mentioned types	F16D25/12	F16D25/12		2419
F16D25/123	9	{in view of cooling and lubrication}	F16D25/12	F16D25/12		1375
F16D25/126	9	{adjustment for wear or play}	F16D25/12	F16D25/12		417
F16D25/14	9	{Fluid pressure control}	F16D48/02	F16D25/14		1952
F16D27/00	7	Magnetically- {or electrically-} actuated clutches; Control or electric circuits therefor (clutches with magnetisable particles F16D37/02; {with electro-rheological fluids F16D37/008})	F16D27/00	F16D27/00		464
F16D2027/001	8	{Means for electric connection of the coils of the electromagnetic clutches}	F16D27/00	F16D27/00		196
F16D2027/002	8	{Electric or electronic circuits relating to actuation of electromagnetic clutches}	F16D27/00	F16D27/00		277
F16D27/004	8	{with permanent magnets combined with electromagnets}	F16D27/00	F16D27/00		726
F16D2027/005	8	{Details relating to the internal construction of coils or to clutches having more than one coil in the same housing}	F16D27/00	F16D27/00		267
F16D2027/007	8	{Bias of an armature of an electromagnetic clutch by flexing of substantially flat springs, e.g. leaf springs}	F16D27/00	F16D27/00		224
F16D2027/008	8	{Details relating to the magnetic circuit, or to the shape of the clutch parts to achieve a certain magnetic path}	F16D27/00	F16D27/00		782
F16D27/01	8	with permanent magnets	F16D27/01	F16D27/01		355
F16D27/02	8	with electromagnets incorporated in the clutch, i.e. with collecting rings {(F16D27/004 takes precedence)}	F16D27/02	F16D27/02		348
F16D27/025	9	{and with a helical band or equivalent member co-operating with a cylindrical coupling surface}	F16D27/02	F16D27/02		50
F16D27/04	9	with axially-movable friction surfaces	F16D27/04	F16D27/04		163
F16D27/06	10	with friction surfaces arranged within the flux	F16D27/06	F16D27/06		517
F16D27/08	10	with friction surfaces arranged externally to the flux	F16D27/08	F16D27/08		304
F16D27/09	9	and with interengaging jaws or gear-teeth	F16D27/09	F16D27/09		250
F16D27/10	8	with an electromagnet not rotating with a clutching member, i.e. without collecting rings {(F16D27/004 takes precedence)}	F16D27/10	F16D27/10		393
F16D27/102	9	with radially movable clutching members (F16D27/105 takes precedence)	F16D27/102	F16D27/102		106
F16D27/105	9	with a helical band or equivalent member co-operating with a cylindrical coupling surface	F16D27/105	F16D27/105		339
F16D27/108	9	with axially movable clutching members	F16D27/108	F16D27/108		222
F16D27/11	10	with conical friction surfaces, e.g. cone clutches	F16D27/11	F16D27/11		80
F16D27/112	10	with flat friction surfaces, e.g. discs	F16D27/112	F16D27/112		1638
F16D27/115	11	with more than two discs, e.g. multiple lamellae	F16D27/115	F16D27/115		475
F16D27/118	9	with interengaging jaws or gear teeth	F16D27/118	F16D27/118		556
F16D27/12	8	Clutch systems with a plurality of electro-magnetically-actuated clutches {(F16D27/004 takes precedence)}	F16D27/12	F16D27/12		371
F16D27/14	8	Details	F16D27/14	F16D27/14		1290
F16D28/00	7	Electrically-actuated clutches (arrangements for synchronisation F16D23/02; clutches actuated directly by means of an electromagnet F16D27/00; automatic clutches F16D43/00&#160;-&#160;F16D45/00; external control F16D48/00)	F16D28/00	F16D28/00		1612
F16D29/00	7	Clutches and systems of clutches involving both fluid and magnetic actuation	F16D29/00	F16D29/00		70
F16D29/005	8	{with a fluid pressure piston driven by an electric motor}	F16D29/00	F16D29/00		316
F16D31/00	7	Fluid couplings or clutches with pumping sets of the volumetric type, i.e. in the case of liquid passing a predetermined volume per revolution	F16D31/00	F16D31/00		115
F16D31/02	8	using pumps with pistons or plungers working in cylinders	F16D31/02	F16D31/02		826
F16D31/04	8	using gear-pumps	F16D31/04	F16D31/04		404
F16D31/06	8	using pumps of types differing from those before-mentioned	F16D31/06	F16D31/06		430
F16D31/08	8	Control of slip	F16D31/08	F16D31/08		213
F16D33/00	7	Rotary fluid couplings or clutches of the hydrokinetic type	F16D33/00	F16D33/00		457
F16D33/02	8	controlled by changing the flow of the liquid in the working circuit, while maintaining a completely filled working circuit	F16D33/02	F16D33/02		118
F16D33/04	9	by altering the position of blades	F16D33/04	F16D33/04		205
F16D33/06	8	controlled by changing the amount of liquid in the working circuit	F16D33/06	F16D33/06		228
F16D33/08	9	by devices incorporated in the fluid coupling, with or without remote control	F16D33/08	F16D33/08		131
F16D33/10	10	consisting of controllable supply and discharge openings	F16D33/10	F16D33/10		214
F16D33/12	11	controlled automatically by self-actuated valves	F16D33/12	F16D33/12		84
F16D33/14	10	consisting of shiftable or adjustable scoops	F16D33/14	F16D33/14		172
F16D33/16	9	by means arranged externally of the coupling or clutch (mounting of such means in vehicles B60K23/00, e.g. B60K23/02)	F16D33/16	F16D33/16		273
F16D33/18	8	Details (applicable also to fluid gearing F16H41/24)	F16D33/18	F16D33/18		420
F16D33/20	9	Shape of wheels, blades, or channels with respect to function	F16D33/20	F16D33/20		316
F16D35/00	7	Fluid clutches in which the clutching is predominantly obtained by fluid adhesion (F16D37/00 takes precedence {; arrangements of viscous clutches in four-wheel drives - B60K17/3465 and B60K17/351})	F16D35/00	F16D35/00		465
F16D35/005	8	{with multiple lamellae}	F16D35/00	F16D35/00		454
F16D35/02	8	with rotary working chambers and rotary reservoirs, e.g. in one coupling part	F16D35/02	F16D35/02		113
F16D35/021	9	{actuated by valves}	F16D35/02	F16D35/02		88
F16D35/022	10	{the valve being actuated by a bimetallic strip (F16D35/026 takes precedence)}	F16D35/02	F16D35/02		169
F16D35/023	10	{the valve being actuated by a bimetallic coil (F16D35/026 takes precedence)}	F16D35/02	F16D35/02		203
F16D35/024	10	{the valve being actuated electrically, e.g. by an electromagnet (F16D35/026 takes precedence)}	F16D35/02	F16D35/02		192
F16D35/025	10	{the valve being actuated by inertia, e.g. using a flyweight or a centrifugal mass (F16D35/026 takes precedence)}	F16D35/02	F16D35/02		21
F16D35/026	10	{actuated by a plurality of valves; the valves being actuated by a combination of mechanisms covered by more than one of groups F16D35/022&#160;-&#160;F16D35/025}	F16D35/02	F16D35/02		79
F16D35/027	9	{actuated by emptying and filling with viscous fluid from outside the coupling during operation}	F16D35/02	F16D35/02		41
F16D35/028	9	{actuated electrically, e.g. by an electromagnet (valves actuated electrically F16D35/024)}	F16D35/02	F16D35/02		47
F16D35/029	9	{actuated by varying the volume of the reservoir chamber}	F16D35/02	F16D35/02		42
F16D37/00	7	Clutches in which the drive is transmitted through a medium consisting of small particles, e.g. centrifugally speed-responsive	F16D37/00	F16D37/00		268
F16D2037/001	8	{Electric arrangements for clutch control}	F16D37/00	F16D37/00		135
F16D2037/002	8	{characterised by a single substantially axial gap in which the fluid or medium consisting of small particles is arranged}	F16D37/00	F16D37/00		515
F16D2037/004	8	{characterised by multiple substantially axial gaps in which the fluid or medium consisting of small particles is arranged}	F16D37/00	F16D37/00		101
F16D2037/005	8	{characterised by a single substantially radial gap in which the fluid or medium consisting of small particles is arranged}	F16D37/00	F16D37/00		155
F16D2037/007	8	{characterised by multiple substantially radial gaps in which the fluid or medium consisting of small particles is arranged}	F16D37/00	F16D37/00		113
F16D37/008	8	{the particles being carried by a fluid, to vary viscosity when subjected to electric change, i.e. electro-rheological or smart fluids (composition of such fluids C10M171/001)}	F16D37/00	F16D37/00		202
F16D37/02	8	the particles being magnetisable	F16D37/02	F16D37/02		992
F16D39/00	7	Combinations of couplings according to two or more of the groups F16D31/00&#160;-&#160;F16D37/00	F16D39/00	F16D39/00		38
F16D41/00	7	Freewheels or freewheel clutches (cycle brakes controlled by back-pedalling B62L5/00{; one-way linear clutches F16B7/16})	F16D41/00	F16D41/00		845
F16D41/02	8	disengaged by contact of a part of or on the freewheel or freewheel clutch with a stationarily-mounted member	F16D41/02	F16D41/02		240
F16D41/04	8	combined with a clutch for locking the driving and driven members (F16D41/02, F16D41/24 take precedence)	F16D41/04	F16D41/04		251
F16D41/06	8	with intermediate wedging coupling members between an inner and an outer surface (F16D41/02, F16D41/24 take precedence)	F16D41/06	F16D41/06		613
F16D2041/0601	9	{with a sliding bearing or spacer}	F16D41/06	F16D41/06		138
F16D2041/0603	9	{Sprag details}	F16D41/06	F16D41/06		229
F16D2041/0605	9	{Spring details}	F16D41/06	F16D41/06		326
F16D2041/0606	9	{the intermediate coupling members having parts wedging by movement other than pivoting or rolling but combined with pivoting or rolling parts, e.g. shoes on pivot bars or on rollers}	F16D41/06	F16D41/06		17
F16D2041/0608	9	{Races with a regular polygon shape}	F16D41/06	F16D41/06		69
F16D41/061	9	the intermediate members wedging by movement having an axial component	F16D41/061	F16D41/061		216
F16D41/063	9	the intermediate members wedging by moving along the inner and the outer surface without pivoting or rolling, e.g. sliding wedges (F16D41/061 takes precedence)	F16D41/063	F16D41/063		327
F16D41/064	9	the intermediate members wedging by rolling and having a circular cross-section, e.g. balls (F16D41/061 takes precedence)	F16D41/064	F16D41/064		656
F16D2041/0643	10	{the intermediate coupling members being of more than one size}	F16D41/064	F16D41/064		18
F16D2041/0646	10	{the intermediate coupling members moving between recesses in an inner race and recesses in an outer race}	F16D41/064	F16D41/064		95
F16D41/066	10	all members having the same size and only one of the two surfaces being cylindrical	F16D41/066	F16D41/066		966
F16D2041/0665	11	{characterised by there being no cage other than the inner and outer race for distributing the intermediate members}	F16D41/066	F16D41/066		169
F16D41/067	11	and the members being distributed by a separate cage encircling the axis of rotation	F16D41/067	F16D41/067		1092
F16D41/069	9	the intermediate members wedging by pivoting or rocking, e.g. sprags (F16D41/061 takes precedence)	F16D41/069	F16D41/069		303
F16D41/07	10	between two cylindrical surfaces	F16D41/07	F16D41/07		1221
F16D41/073	11	{each member comprising at least two elements at different radii}	F16D41/07	F16D41/07		150
F16D41/076	11	{the wedging coupling members being non-releasably joined to form a single annular piece, e.g. either the members being integral projections from the piece, or the piece being an elastic ring cast round the radial centres of the members}	F16D41/07	F16D41/07		56
F16D41/08	9	with provision for altering the freewheeling action	F16D41/08	F16D41/08		365
F16D41/082	10	{the intermediate coupling members wedging by movement other than pivoting or rolling}	F16D41/08	F16D41/08		64
F16D41/084	10	{the intermediate coupling members wedging by pivoting or rocking}	F16D41/08	F16D41/08		195
F16D41/086	10	{the intermediate members being of circular cross-section and wedging by rolling (F16D41/10 takes precedence)}	F16D41/08	F16D41/08		132
F16D41/088	11	{the intermediate members being of only one size and wedging by a movement not having an axial component, between inner and outer races, one of which is cylindrical}	F16D41/08	F16D41/08		714
F16D41/10	10	with self-actuated reversing	F16D41/10	F16D41/10		229
F16D41/105	11	{the intermediate members being of circular cross-section, of only one size and wedging by rolling movement not having an axial component between inner and outer races, one of which is cylindrical}	F16D41/10	F16D41/10		360
F16D41/12	8	with hinged pawl co-operating with teeth, cogs, or the like (F16D41/02, F16D41/24 take precedence)	F16D41/12	F16D41/12		1436
F16D41/125	9	{the pawl movement having an axial component}	F16D41/12	F16D41/12		358
F16D41/14	9	the effective stroke of the pawl being adjustable	F16D41/14	F16D41/14		370
F16D41/16	9	the action being reversible	F16D41/16	F16D41/16		539
F16D41/18	8	with non-hinged detent (F16D41/02, F16D41/24 take precedence)	F16D41/18	F16D41/18		308
F16D41/185	9	{the engaging movement having an axial component}	F16D41/18	F16D41/18		119
F16D41/20	8	with expandable or contractable clamping ring or band (F16D41/02, F16D41/24 take precedence)	F16D41/20	F16D41/20		171
F16D41/203	9	{having coils overlapping in a single radial plane, e.g. Archimedian spiral}	F16D41/20	F16D41/20		73
F16D41/206	9	{having axially adjacent coils, e.g. helical wrap-springs}	F16D41/20	F16D41/20		671
F16D41/22	8	with clutching ring or disc axially shifted as a result of lost motion between actuating members (F16D41/02, F16D41/24 take precedence)	F16D41/22	F16D41/22		662
F16D41/24	8	specially adapted for cycles	F16D41/24	F16D41/24		277
F16D41/26	9	with provision for altering the action	F16D41/26	F16D41/26		123
F16D41/28	9	with intermediate wedging coupling members	F16D41/28	F16D41/28		214
F16D41/30	9	with hinged pawl co-operating with teeth, cogs, or the like	F16D41/30	F16D41/30		517
F16D41/32	9	with non-hinged detent	F16D41/32	F16D41/32		58
F16D41/34	9	with expandable or contractable clamping ring or band	F16D41/34	F16D41/34		13
F16D41/36	9	with clutching ring or disc axially shifted as a result of lost motion between actuating members	F16D41/36	F16D41/36		161
F16D43/00	7	Automatic clutches (varying the relationship between two coaxial shafts F16D3/10; freewheels, freewheel clutches F16D41/00)	F16D43/00	F16D43/00		98
F16D43/02	8	actuated entirely mechanically	F16D43/02	F16D43/02		389
F16D43/04	9	controlled by angular speed (F16D43/24 takes precedence; clutches in which the drive is transmitted through a medium consisting of small particles F16D37/00)	F16D43/04	F16D43/04		338
F16D43/06	10	with centrifugal masses actuating axially a movable pressure ring or the like	F16D43/06	F16D43/06		118
F16D43/08	11	the pressure ring actuating friction plates, cones or similar axially-movable friction surfaces	F16D43/08	F16D43/08		191
F16D43/09	12	in which the carrier of the centrifugal masses can be stopped	F16D43/09	F16D43/09		70
F16D43/10	12	the centrifugal masses acting directly on the pressure ring, no other actuating mechanism for the pressure ring being provided	F16D43/10	F16D43/10		516
F16D43/12	12	the centrifugal masses acting on, or forming a part of, an actuating mechanism by which the pressure ring can also be actuated independently of the masses	F16D43/12	F16D43/12		374
F16D43/14	10	with centrifugal masses actuating the clutching members directly in a direction which has at least a radial component; with centrifugal masses themselves being the clutching members	F16D43/14	F16D43/14		236
F16D2043/145	11	{the centrifugal masses being pivoting}	F16D43/14	F16D43/14		640
F16D43/16	11	with clutching members having interengaging parts	F16D43/16	F16D43/16		265
F16D43/18	11	with friction clutching members	F16D43/18	F16D43/18		1897
F16D43/20	9	controlled by torque, e.g. overload-release clutches, slip-clutches with means by which torque varies the clutching pressure	F16D43/20	F16D43/20		420
F16D43/202	10	of the ratchet type (slip couplings of the ratchet type F16D7/04)	F16D43/202	F16D43/202		172
F16D43/2022	11	{with at least one part moving axially between engagement and disengagement (F16D43/206 takes precedence)}	F16D43/202	F16D43/202		52
F16D43/2024	12	{the axially moving part being coaxial with the rotation, e.g. a gear with face teeth}	F16D43/202	F16D43/202		266
F16D43/2026	12	{with a plurality of axially moving parts}	F16D43/202	F16D43/202		42
F16D43/2028	11	{with at least one part moving radially between engagement and disengagement (F16D43/208 takes precedence)}	F16D43/202	F16D43/202		248
F16D43/204	11	with intermediate balls or rollers	F16D43/204	F16D43/204		50
F16D43/206	12	moving axially between engagement and disengagement	F16D43/206	F16D43/206		342
F16D43/208	12	moving radially between engagement and disengagement	F16D43/208	F16D43/208		171
F16D43/21	10	with friction members {(slip couplings of the friction type F16D7/02)}	F16D43/21	F16D43/21		145
F16D43/211	11	{with radially applied torque-limiting friction surfaces}	F16D43/21	F16D43/21		190
F16D43/213	11	{with axially applied torque-limiting friction surfaces}	F16D43/21	F16D43/21		41
F16D43/215	12	{with flat friction surfaces, e.g. discs}	F16D43/21	F16D43/21		213
F16D43/216	13	{with multiple lamellae}	F16D43/21	F16D43/21		276
F16D43/218	12	{with conical friction surfaces}	F16D43/21	F16D43/21		82
F16D43/22	9	controlled by both speed and torque	F16D43/22	F16D43/22		174
F16D43/24	9	controlled by acceleration or deceleration of angular speed	F16D43/24	F16D43/24		132
F16D43/25	9	controlled by thermo-responsive elements	F16D43/25	F16D43/25		243
F16D43/26	9	acting at definite angular position or disengaging after {consecutive} definite number of rotations (actuating by means of stationary abutment F16D11/02, F16D13/02, F16D15/00; control of change-speed or reversing-gearings conveying rotary motion F16H59/00&#160;-&#160;F16H63/00)	F16D43/26	F16D43/26		363
F16D43/28	8	actuated by fluid pressure	F16D43/28	F16D43/28		131
F16D43/284	9	controlled by angular speed	F16D43/284	F16D43/284		410
F16D43/286	9	controlled by torque	F16D43/286	F16D43/286		161
F16D43/30	8	Systems of a plurality of automatic clutches	F16D43/30	F16D43/30		83
F16D45/00	7	Freewheels or freewheel clutches combined with automatic clutches	F16D45/00	F16D45/00		320
F16D47/00	7	Systems of clutches, or clutches and couplings, comprising devices of types grouped under at least two of the following sets of groups: F16D1/00 - F16D9/00, F16D11/00 - F16D23/00, F16D25/00 - F16D29/00, F16D31/00 - F16D39/00, F16D41/00 - F16D45/00(freewheels combined with a clutch to lock the driving and driven members of the freewheel F16D41/04, F16D41/26)	F16D47/00	F16D47/00		248
F16D47/02	8	of which at least one is a coupling	F16D47/02	F16D47/02		450
F16D47/04	8	of which at least one is a freewheel (F16D47/02, F16D47/06 take precedence; freewheels combined with a clutch to lock the driving and driven members of the freewheel F16D41/04, F16D41/26)	F16D47/04	F16D47/04		433
F16D47/06	8	of which at least one is a clutch with a fluid or a semifluid as power-transmitting means	F16D47/06	F16D47/06		515
F16D48/00	7	External control of clutches	F16D48/00	F16D48/00		245
F16D48/02	8	Control by fluid pressure	F16D48/02	F16D48/02		2679
F16D2048/0203	9	{with an accumulator; Details thereof}	F16D48/02	F16D48/02		236
F16D48/0206	9	{in a system with a plurality of fluid-actuated clutches}	F16D48/02	F16D48/02		654
F16D2048/0209	9	{characterised by fluid valves having control pistons, e.g. spools}	F16D48/02	F16D48/02		693
F16D2048/0212	9	{Details of pistons for primary or secondary cylinders especially adapted for fluid control}	F16D48/02	F16D48/02		894
F16D2048/0215	9	{for damping of pulsations within the fluid system}	F16D48/02	F16D48/02		376
F16D2048/0218	9	{Reservoirs for clutch control systems; Details thereof}	F16D48/02	F16D48/02		91
F16D2048/0221	9	{Valves for clutch control systems; Details thereof}	F16D48/02	F16D48/02		1212
F16D2048/0224	9	{Details of conduits, connectors or the adaptors therefor specially adapted for clutch control}	F16D48/02	F16D48/02		428
F16D2048/0227	9	{Source of pressure producing the clutch engagement or disengagement action within a circuit; Means for initiating command action in power assisted devices}	F16D48/02	F16D48/02		39
F16D2048/023	10	{by pedal actuation}	F16D48/02	F16D48/02		196
F16D2048/0233	10	{by rotary pump actuation}	F16D48/02	F16D48/02		238
F16D2048/0236	11	{with multiple independent pumps, e.g. one per clutch, or for supplying fluid to different systems}	F16D48/02	F16D48/02		57
F16D2048/0239	12	{One fluid source supplying fluid at high pressure and one fluid source supplying fluid at low pressure}	F16D48/02	F16D48/02		22
F16D2048/0242	12	{Two or more rotating pumps driven together by the same power source, e.g. connected by a shaft, or a single pump having two or more fluid outputs}	F16D48/02	F16D48/02		41
F16D2048/0245	11	{Electrically driven rotary pumps}	F16D48/02	F16D48/02		112
F16D2048/0248	12	{Reversible rotary pumps, i.e. pumps that can be rotated in the two directions}	F16D48/02	F16D48/02		89
F16D2048/0251	11	{Electric motor driving a piston, e.g. for actuating the primary cylinder}	F16D48/02	F16D48/02		49
F16D2048/0254	10	{Double actuation, i.e. two actuation means can produce independently an engagement or disengagement of the clutch}	F16D48/02	F16D48/02		211
F16D2048/0257	9	{Hydraulic circuit layouts, i.e. details of hydraulic circuit elements or the arrangement thereof}	F16D48/02	F16D48/02		142
F16D2048/026	10	{The controlling actuation is directly performed by the pressure source, i.e. there is no intermediate valve for controlling flow or pressure}	F16D48/02	F16D48/02		45
F16D2048/0263	10	{Passive valves between pressure source and actuating cylinder, e.g. check valves or throttle valves}	F16D48/02	F16D48/02		158
F16D2048/0266	10	{Actively controlled valves between pressure source and actuation cylinder}	F16D48/02	F16D48/02		286
F16D2048/0269	10	{Single valve for switching between fluid supply to actuation cylinder or draining to the sump}	F16D48/02	F16D48/02		136
F16D2048/0272	10	{Two valves, where one valve is supplying fluid to the cylinder and the other valve is for draining fluid to the sump}	F16D48/02	F16D48/02		49
F16D2048/0275	10	{Two valves arranged in parallel, e.g. one for coarse and the other for fine control during supplying or draining fluid from the actuation cylinder}	F16D48/02	F16D48/02		80
F16D2048/0278	10	{Two valves in series arrangement for controlling supply to actuation cylinder}	F16D48/02	F16D48/02		88
F16D2048/0281	10	{Complex circuits with more than two valves in series or special arrangements thereof not provided for in previous groups}	F16D48/02	F16D48/02		233
F16D2048/0284	10	{characterised by valve arrangements supplying fluid to a two chamber- cylinder}	F16D48/02	F16D48/02		78
F16D2048/0287	10	{Hydraulic circuits combining clutch actuation and other hydraulic systems}	F16D48/02	F16D48/02		84
F16D2048/029	11	{Hydraulic circuits combining clutch actuation with clutch lubrication or cooling}	F16D48/02	F16D48/02		166
F16D2048/0293	11	{Hydraulic circuits combining clutch and transmission actuation}	F16D48/02	F16D48/02		64
F16D2048/0296	10	{Hydraulic circuits controlled exclusively by hydraulic pressure, i.e. with no electrically controlled valves}	F16D48/02	F16D48/02		24
F16D48/04	9	providing power assistance	F16D48/04	F16D48/04		769
F16D2048/045	10	{Vacuum boosters therefor}	F16D48/04	F16D48/04		159
F16D48/06	8	Control by electric or electronic means, e.g. of fluid pressure	F16D48/06	F16D48/06		3249
F16D48/062	9	{of a clutch system with a plurality of fluid actuated clutches}	F16D48/06	F16D48/06		330
F16D48/064	9	{Control of electrically or electromagnetically actuated clutches (F16D48/062, F16D48/068 take precedence)}	F16D48/06	F16D48/06		1348
F16D48/066	9	{Control of fluid pressure, e.g. using an accumulator (F16D48/062, F16D48/068 take precedence)}	F16D48/06	F16D48/06		1909
F16D48/068	9	{using signals from a manually actuated gearshift linkage}	F16D48/06	F16D48/06		362
F16D48/08	9	Regulating clutch take-up on starting	F16D48/08	F16D48/08		527
F16D48/10	9	Preventing unintentional or unsafe engagement	F16D48/10	F16D48/10		171
F16D49/00	7	Brakes with a braking member co-operating with the periphery of a drum, wheel-rim, or the like (similar clutches F16D13/10)	F16D49/00	F16D49/00		824
F16D49/02	8	shaped as a helical band or coil with more than one turn, with or without intensification of the braking force by the tension of the band or contracting member (similar clutches F16D13/08)	F16D49/02	F16D49/02		179
F16D49/04	9	mechanically actuated	F16D49/04	F16D49/04		94
F16D49/06	9	fluid actuated	F16D49/06	F16D49/06		23
F16D49/08	8	shaped as an encircling band extending over approximately 360 degrees	F16D49/08	F16D49/08		538
F16D49/10	9	mechanically actuated (self-tightening F16D49/20)	F16D49/10	F16D49/10		674
F16D49/12	9	fluid actuated	F16D49/12	F16D49/12		185
F16D49/14	8	shaped as a fluid-filled flexible member actuated by variation of the fluid pressure	F16D49/14	F16D49/14		67
F16D49/16	8	Brakes with two brake-blocks (self-tightening F16D49/20)	F16D49/16	F16D49/16		1218
F16D49/18	8	Brakes with three or more brake-blocks (self-tightening F16D49/20)	F16D49/18	F16D49/18		119
F16D49/20	8	Self-tightening brakes (with helical or coil with more than one turn F16D49/02)	F16D49/20	F16D49/20		86
F16D49/22	9	with an auxiliary friction member initiating or increasing the action of the brake	F16D49/22	F16D49/22		13
F16D51/00	7	Brakes with outwardly-movable braking members co-operating with the inner surface of a drum or the like (similar clutches F16D13/14)	F16D51/00	F16D51/00		631
F16D2051/001	8	{Parts or details of drum brakes}	F16D51/00	F16D51/00		112
F16D2051/003	9	{Brake supports}	F16D51/00	F16D51/00		445
F16D2051/005	9	{Protective covers}	F16D51/00	F16D51/00		232
F16D2051/006	9	{Braking members arranged axially spaced, e.g. side by side}	F16D51/00	F16D51/00		31
F16D2051/008	9	{Brakes with only one substantially rigid braking member}	F16D51/00	F16D51/00		34
F16D51/02	8	shaped as one or more circumferential band (similar clutches F16D13/12)	F16D51/02	F16D51/02		95
F16D51/04	9	mechanically actuated	F16D51/04	F16D51/04		464
F16D51/06	9	fluid actuated	F16D51/06	F16D51/06		110
F16D51/08	8	shaped as an expansible fluid-filled flexible member	F16D51/08	F16D51/08		183
F16D51/10	8	shaped as exclusively radially-movable brake-shoes	F16D51/10	F16D51/10		192
F16D51/12	9	mechanically actuated	F16D51/12	F16D51/12		280
F16D51/14	9	fluid actuated	F16D51/14	F16D51/14		199
F16D51/16	8	shaped as brake-shoes pivoted on a fixed or nearly-fixed axis	F16D51/16	F16D51/16		92
F16D51/18	9	with two brake-shoes	F16D51/18	F16D51/18		313
F16D51/20	10	extending in opposite directions from their pivots	F16D51/20	F16D51/20		758
F16D51/22	11	mechanically actuated	F16D51/22	F16D51/22		920
F16D51/24	11	fluid actuated	F16D51/24	F16D51/24		726
F16D51/26	10	both extending in the same direction from their pivots	F16D51/26	F16D51/26		100
F16D51/28	11	mechanically actuated	F16D51/28	F16D51/28		151
F16D51/30	11	fluid actuated	F16D51/30	F16D51/30		180
F16D51/32	9	with three or more brake shoes	F16D51/32	F16D51/32		48
F16D51/34	10	extending in opposite directions from their pivots	F16D51/34	F16D51/34		16
F16D51/36	11	mechanically actuated	F16D51/36	F16D51/36		34
F16D51/38	11	fluid actuated	F16D51/38	F16D51/38		21
F16D51/40	10	all extending in the same direction from their pivots	F16D51/40	F16D51/40		26
F16D51/42	11	mechanically actuated	F16D51/42	F16D51/42		46
F16D51/44	11	fluid actuated	F16D51/44	F16D51/44		14
F16D51/46	8	Self-tightening brakes with pivoted brake shoes, {i.e. the braked member increases the braking action}	F16D51/46	F16D51/46		53
F16D51/48	9	with two linked or directly-interacting brake shoes	F16D51/48	F16D51/48		395
F16D51/50	10	mechanically actuated	F16D51/50	F16D51/50		454
F16D51/52	10	fluid actuated	F16D51/52	F16D51/52		233
F16D51/54	9	with three or more brake-shoes, at least two of them being linked or directly interacting	F16D51/54	F16D51/54		24
F16D51/56	10	mechanically actuated	F16D51/56	F16D51/56		215
F16D51/58	10	fluid actuated	F16D51/58	F16D51/58		18
F16D51/60	9	with wedging action of a brake-shoe, e.g. the shoe entering as a wedge between the brake-drum and a stationary part	F16D51/60	F16D51/60		70
F16D51/62	10	mechanically actuated	F16D51/62	F16D51/62		8
F16D51/64	10	fluid actuated	F16D51/64	F16D51/64		
F16D51/66	9	an actuated brake-shoe being carried along and thereby engaging a member for actuating another brake-shoe	F16D51/66	F16D51/66		174
F16D51/68	10	mechanically actuated	F16D51/68	F16D51/68		2
F16D51/70	10	fluid actuated	F16D51/70	F16D51/70		1
F16D53/00	7	Brakes with braking members co-operating with both the periphery and the inner surface of a drum, wheel-rim, or the like (similar clutches F16D13/20)	F16D53/00	F16D53/00		344
F16D55/00	7	Brakes with substantially-radial braking surfaces pressed together in axial direction, e.g. disc brakes (similar clutches F16D13/38)	F16D55/00	F16D55/00		670
F16D2055/0004	8	{Parts or details of disc brakes}	F16D55/00	F16D55/00		95
F16D2055/0008	9	{Brake supports}	F16D55/00	F16D55/00		969
F16D2055/0012	10	{integral with vehicle suspension}	F16D55/00	F16D55/00		165
F16D2055/0016	9	{Brake calipers}	F16D55/00	F16D55/00		1184
F16D2055/002	10	{assembled from a plurality of parts}	F16D55/00	F16D55/00		747
F16D2055/0025	10	{comprising a flat frame member}	F16D55/00	F16D55/00		206
F16D2055/0029	10	{Retraction devices}	F16D55/00	F16D55/00		199
F16D2055/0033	9	{Fully-enclosing housings}	F16D55/00	F16D55/00		76
F16D2055/0037	9	{Protective covers}	F16D55/00	F16D55/00		522
F16D2055/0041	9	{Resilient elements interposed directly between the actuating member and the brake support, e.g. anti-rattle springs}	F16D55/00	F16D55/00		593
F16D2055/0045	9	{Braking members arranged non-symmetrically with respect to the brake disc}	F16D55/00	F16D55/00		115
F16D2055/005	9	{Brakes straddling an annular brake disc radially internally}	F16D55/00	F16D55/00		225
F16D2055/0054	9	{Brakes located in the radial gap between two coplanarly arranged annular brake discs}	F16D55/00	F16D55/00		39
F16D2055/0058	9	{Fully lined, i.e. braking surface extending over the entire disc circumference}	F16D55/00	F16D55/00		1627
F16D2055/0062	9	{Partly lined, i.e. braking surface extending over only a part of the disc circumference}	F16D55/00	F16D55/00		404
F16D2055/0066	9	{Brakes having more than one actuator on the same side of the disc}	F16D55/00	F16D55/00		90
F16D2055/007	9	{Pins holding the braking members}	F16D55/00	F16D55/00		746
F16D2055/0075	8	{Constructional features of axially engaged brakes}	F16D55/00	F16D55/00		43
F16D2055/0079	9	{with braking members arranged non-symmetrically with respect to the rotor}	F16D55/00	F16D55/00		18
F16D2055/0083	9	{with brake actuator located radially inside of an annular rotor}	F16D55/00	F16D55/00		33
F16D2055/0087	9	{with brake actuator located between two coplanar annular rotors}	F16D55/00	F16D55/00		12
F16D2055/0091	9	{Plural actuators arranged side by side on the same side of the rotor}	F16D55/00	F16D55/00		833
F16D2055/0095	9	{Plural rotors with different properties, e.g. to influence working conditions like wear or temperature}	F16D55/00	F16D55/00		42
F16D55/02	8	with axially-movable discs or pads pressed against axially-located rotating members	F16D55/02	F16D55/02		728
F16D55/025	9	{with two or more rotating discs at least one of them being located axially}	F16D55/02	F16D55/02		94
F16D55/04	9	by moving discs or pads away from one another against radial walls of drums or cylinders	F16D55/04	F16D55/04		66
F16D55/06	10	without self-tightening action	F16D55/06	F16D55/06		247
F16D55/08	11	Mechanically-actuated brakes	F16D55/08	F16D55/08		47
F16D55/10	11	Brakes actuated by a fluid-pressure device arranged in or on the brake	F16D55/10	F16D55/10		219
F16D55/12	12	comprising an expansible fluid-filled flexible member coaxial with the brake	F16D55/12	F16D55/12		17
F16D55/14	10	with self-tightening action, e.g. by means of coacting helical surfaces or balls and inclined surfaces	F16D55/14	F16D55/14		535
F16D55/15	11	initiated by means of brake-bands or brake-shoes	F16D55/15	F16D55/15		31
F16D55/16	11	Mechanically-actuated brakes	F16D55/16	F16D55/16		31
F16D55/18	11	Brakes actuated by a fluid-pressure device arranged in or on the brake	F16D55/18	F16D55/18		39
F16D55/20	12	comprising an expansible fluid-filled flexible member coaxial with the brake	F16D55/20	F16D55/20		6
F16D55/22	9	by clamping an axially-located rotating disc between movable braking members, e.g. movable brake discs or brake pads	F16D55/22	F16D55/22		1116
F16D55/224	10	with a common actuating member for the braking members	F16D55/224	F16D55/224		867
F16D55/2245	11	{in which the common actuating member acts on two levers carrying the braking members, e.g. tong-type brakes (similar brakes for rail vehicles B61H5/00)}	F16D55/224	F16D55/224		1419
F16D55/225	11	the braking members being brake pads	F16D55/225	F16D55/225		526
F16D55/2255	12	in which the common actuating member is pivoted	F16D55/2255	F16D55/2255		606
F16D55/226	12	in which the common actuating member is moved axially {, e.g. floating caliper disc brakes}	F16D55/226	F16D55/226		2884
F16D55/2262	13	{the axial movement being guided by open sliding surfaces, e.g. grooves}	F16D55/226	F16D55/226		491
F16D55/2265	13	the axial movement being guided by one or more pins {engaging bores in the brake support or the brake housing}	F16D55/2265	F16D55/2265		366
F16D55/22655	14	{Constructional details of guide pins}	F16D55/2265	F16D55/2265		763
F16D55/227	14	by two {or more} pins	F16D55/227	F16D55/227		1390
F16D55/228	10	with a separate actuating member for each side	F16D55/228	F16D55/228		1442
F16D55/24	8	with a plurality of axially-movable discs, lamellae, or pads, pressed from one side towards an axially-located member	F16D55/24	F16D55/24		323
F16D55/26	9	without self-tightening action	F16D55/26	F16D55/26		235
F16D55/28	10	Brakes with only one rotating disc	F16D55/28	F16D55/28		531
F16D55/30	11	mechanically actuated	F16D55/30	F16D55/30		126
F16D55/31	12	by means of an intermediate leverage	F16D55/31	F16D55/31		75
F16D55/32	11	actuated by a fluid-pressure device arranged in or on the brake	F16D55/32	F16D55/32		403
F16D55/33	12	by means of an intermediate leverage	F16D55/33	F16D55/33		49
F16D55/34	12	comprising an expansible fluid-filled flexible member coaxial with the brake	F16D55/34	F16D55/34		15
F16D55/36	10	Brakes with a plurality of rotating discs all lying side by side	F16D55/36	F16D55/36		868
F16D55/38	11	mechanically actuated	F16D55/38	F16D55/38		231
F16D55/39	12	by means of an intermediate leverage	F16D55/39	F16D55/39		79
F16D55/40	11	actuated by a fluid-pressure device arranged in or one the brake	F16D55/40	F16D55/40		1328
F16D55/41	12	by means of an intermediate leverage	F16D55/41	F16D55/41		38
F16D55/42	12	comprising an expansible fluid-filled flexible member coaxial with the brake	F16D55/42	F16D55/42		14
F16D55/44	10	with the rotating part consisting of both central plates and ring-shaped plates arranged concentrically around the central plates	F16D55/44	F16D55/44		4
F16D55/46	9	with self-tightening action	F16D55/46	F16D55/46		240
F16D55/48	10	with discs or pads having a small free angular travel relative to their support, which produces the self-tightening action	F16D55/48	F16D55/48		24
F16D55/50	10	with auxiliary friction members, which may be of different type, producing the self-tightening action	F16D55/50	F16D55/50		22
F16D57/00	7	Liquid-resistance brakes; {Brakes using the internal friction of fluids or fluid-like media, e.g. powders (for braking drums, barrels or ropes of cranes, lift hoists or winches B66D5/026)}	F16D57/00	F16D57/00		446
F16D57/002	8	{comprising a medium with electrically or magnetically controlled internal friction, e.g. electrorheological fluid, magnetic powder}	F16D57/00	F16D57/00		463
F16D57/005	8	{Details of blades, e.g. shape}	F16D57/00	F16D57/00		166
F16D57/007	8	{with variable brake geometry, e.g. axially movable rotor or stator}	F16D57/00	F16D57/00		38
F16D57/02	8	with blades or like members braked by the fluid	F16D57/02	F16D57/02		428
F16D57/04	8	with blades causing a directed flow, e.g. F&#246;ttinger type	F16D57/04	F16D57/04		883
F16D57/06	8	comprising a pump circulating fluid, braking being effected by throttling of the circulation	F16D57/06	F16D57/06		737
F16D59/00	7	Self-acting brakes, e.g. coming into operation at a predetermined speed	F16D59/00	F16D59/00		1254
F16D59/02	8	spring-loaded and adapted to be released by mechanical, fluid, or electromagnetic means	F16D59/02	F16D59/02		1726
F16D61/00	7	Brakes with means for making the energy absorbed available for use (F16D57/00 takes precedence)	F16D61/00	F16D61/00		723
F16D63/00	7	Brakes not otherwise provided for; Brakes combining more than one of the types of groups F16D49/00 - F16D61/00	F16D63/00	F16D63/00		762
F16D63/002	8	{Brakes with direct electrical or electro-magnetic actuation}	F16D63/00	F16D63/00		939
F16D63/004	8	{comprising a rotor engaged both axially and radially by braking members, e.g. combined drum and disc brakes}	F16D63/00	F16D63/00		231
F16D63/006	8	{Positive locking brakes}	F16D63/00	F16D63/00		898
F16D63/008	8	{Brakes acting on a linearly moving member}	F16D63/00	F16D63/00		660
F16D65/00	7	Parts or details (similar members for clutches F16D13/58)	F16D65/00	F16D65/00		624
F16D65/0006	8	{Noise or vibration control}	F16D65/00	F16D65/00		2409
F16D65/0012	9	{Active vibration dampers}	F16D65/00	F16D65/00		144
F16D65/0018	9	{Dynamic vibration dampers, e.g. mass-spring systems}	F16D65/00	F16D65/00		171
F16D65/0025	8	{Rust- or corrosion-preventing means}	F16D65/00	F16D65/00		235
F16D65/0031	8	{Devices for retaining friction material debris, e.g. dust collectors or filters}	F16D65/00	F16D65/00		664
F16D65/0037	8	{Devices for conditioning friction surfaces, e.g. cleaning or abrasive elements}	F16D65/00	F16D65/00		362
F16D65/0043	8	{Brake maintenance and assembly, tools therefor}	F16D65/00	F16D65/00		473
F16D65/005	8	{Components of axially engaging brakes not otherwise provided for}	F16D65/00	F16D65/00		103
F16D65/0056	9	{Brake supports}	F16D65/00	F16D65/00		318
F16D65/0062	10	{integral with vehicle suspension, e.g. with the steering knuckle}	F16D65/00	F16D65/00		67
F16D65/0068	9	{Brake calipers}	F16D65/00	F16D65/00		886
F16D65/0075	10	{assembled from a plurality of parts}	F16D65/00	F16D65/00		321
F16D65/0081	9	{Brake covers}	F16D65/00	F16D65/00		238
F16D65/0087	9	{Brake housing guide members, e.g. caliper pins; Accessories therefor, e.g. dust boots}	F16D65/00	F16D65/00		337
F16D65/02	8	Braking members; Mounting thereof (friction linings or attachment thereof F16D69/00)	F16D65/02	F16D65/02		880
F16D2065/022	9	{Rollers}	F16D65/02	F16D65/02		30
F16D2065/024	9	{the braking surface being inclined with respect to the rotor&apos;s axis of rotation at an angle other than 90 degrees, e.g. comprising a conical rotor}	F16D65/02	F16D65/02		548
F16D2065/026	9	{characterised by a particular outline shape of the braking member, e.g. footprint of friction lining}	F16D65/02	F16D65/02		274
F16D65/028	9	{Rollers}	F16D65/02	F16D65/02		68
F16D65/04	9	Bands, shoes or pads; Pivots or supporting members therefor	F16D65/04	F16D65/04		871
F16D65/06	10	for externally-engaging brakes	F16D65/06	F16D65/06		457
F16D65/062	11	{engaging the tread of a railway wheel}	F16D65/06	F16D65/06		1597
F16D65/065	11	{Brake bands}	F16D65/06	F16D65/06		67
F16D65/067	12	{with means for mounting, e.g. end connection members}	F16D65/06	F16D65/06		186
F16D65/08	10	for internally-engaging brakes	F16D65/08	F16D65/08		1116
F16D65/09	11	Pivots or supporting members therefor	F16D65/09	F16D65/09		909
F16D65/091	12	{for axially holding the segments}	F16D65/09	F16D65/09		474
F16D65/092	10	for axially-engaging brakes, e.g. disc brakes	F16D65/092	F16D65/092		3071
F16D65/095	11	Pivots or supporting members therefor	F16D65/095	F16D65/095		1566
F16D65/097	12	Resilient means interposed between pads and supporting members {or other brake parts}	F16D65/097	F16D65/097		460
F16D65/0971	13	{transmitting brake actuation force, e.g. elements interposed between brake piston and pad}	F16D65/097	F16D65/097		525
F16D65/0972	13	{transmitting brake reaction force, e.g. elements interposed between torque support plate and pad}	F16D65/097	F16D65/097		640
F16D65/0973	13	{not subjected to brake forces}	F16D65/097	F16D65/097		79
F16D65/0974	14	{acting on or in the vicinity of the pad rim in a direction substantially transverse to the brake disc axis}	F16D65/097	F16D65/097		108
F16D65/0975	15	{Springs made from wire}	F16D65/097	F16D65/097		250
F16D65/0976	16	{acting on one pad only}	F16D65/097	F16D65/097		207
F16D65/0977	15	{Springs made from sheet metal}	F16D65/097	F16D65/097		718
F16D65/0978	16	{acting on one pad only}	F16D65/097	F16D65/097		399
F16D65/0979	14	{acting on the rear side of the pad or an element affixed thereto, e.g. spring clips securing the pad to the brake piston or caliper}	F16D65/097	F16D65/097		467
F16D65/10	9	Drums for externally- or internally-engaging brakes	F16D65/10	F16D65/10		1545
F16D65/12	9	Discs; Drums for disc brakes	F16D65/12	F16D65/12		2719
F16D65/121	10	{consisting of at least three circumferentially arranged segments}	F16D65/12	F16D65/12		258
F16D65/122	10	{adapted for mounting of friction pads}	F16D65/12	F16D65/12		402
F16D65/123	10	{comprising an annular disc secured to a hub member; Discs characterised by means for mounting}	F16D65/12	F16D65/12		1556
F16D65/124	11	{adapted for mounting on the wheel of a railway vehicle}	F16D65/12	F16D65/12		332
F16D65/125	10	{characterised by the material used for the disc body}	F16D65/12	F16D65/12		951
F16D65/126	11	{the material being of low mechanical strength, e.g. carbon, beryllium; Torque transmitting members therefor}	F16D65/12	F16D65/12		568
F16D65/127	10	{characterised by properties of the disc surface; Discs lined with friction material}	F16D65/12	F16D65/12		1074
F16D65/128	10	{characterised by means for cooling}	F16D65/12	F16D65/12		2032
F16D2065/13	9	{Parts or details of discs or drums}	F16D65/02	F16D65/13		67
F16D2065/1304	10	{Structure}	F16D65/02	F16D65/13		198
F16D2065/1308	11	{one-part}	F16D65/02	F16D65/13		424
F16D2065/1312	11	{circumferentially segmented}	F16D65/02	F16D65/13		295
F16D2065/1316	11	{radially segmented}	F16D65/02	F16D65/13		1219
F16D2065/132	11	{layered}	F16D65/02	F16D65/13		860
F16D2065/1324	11	{carrying friction elements}	F16D65/02	F16D65/13		248
F16D2065/1328	11	{internal cavities, e.g. cooling channels}	F16D65/02	F16D65/13		1619
F16D2065/1332	11	{external ribs, e.g. for cooling or reinforcement}	F16D65/02	F16D65/13		667
F16D2065/1336	11	{integral part of vehicle wheel}	F16D65/02	F16D65/13		128
F16D2065/134	10	{Connection}	F16D65/02	F16D65/13		103
F16D2065/1344	11	{permanent, e.g. by casting}	F16D65/02	F16D65/13		485
F16D2065/1348	11	{resilient}	F16D65/02	F16D65/13		417
F16D2065/1352	11	{articulated}	F16D65/02	F16D65/13		23
F16D2065/1356	11	{interlocking}	F16D65/02	F16D65/13		351
F16D2065/136	12	{with relative movement radially}	F16D65/02	F16D65/13		412
F16D2065/1364	12	{with relative movement axially}	F16D65/02	F16D65/13		237
F16D2065/1368	12	{with relative movement both radially and axially}	F16D65/02	F16D65/13		439
F16D2065/1372	11	{outer circumference}	F16D65/02	F16D65/13		211
F16D2065/1376	11	{inner circumference}	F16D65/02	F16D65/13		180
F16D2065/138	11	{to wheel}	F16D65/02	F16D65/13		272
F16D2065/1384	11	{to wheel hub}	F16D65/02	F16D65/13		520
F16D2065/1388	11	{to shaft or axle}	F16D65/02	F16D65/13		138
F16D2065/1392	11	{Connection elements}	F16D65/02	F16D65/13		1403
F16D2065/1396	12	{Ancillary resilient elements, e.g. anti-rattle or retraction springs}	F16D65/02	F16D65/13		405
F16D65/14	8	Actuating mechanisms for brakes; Means for initiating operation at a predetermined position (brake control systems, parts thereof B60T)<br><br><u>NOTE</u><br><br>In this group, it is desirable to add the indexing codes of groups F16D2121/00 - F16D2131/00 relating to actuators.	F16D65/14	F16D65/14		3536
F16D65/16	9	arranged in or on the brake	F16D65/16	F16D65/16		1159
F16D65/18	10	adapted for drawing members together {, e.g. for disc brakes}	F16D65/18	F16D65/18		5918
F16D65/183	11	{with force-transmitting members arranged side by side acting on a spot type force-applying member}	F16D65/18	F16D65/18		1437
F16D65/186	11	{with full-face force-applying member, e.g. annular}	F16D65/18	F16D65/18		1038
F16D65/22	10	adapted for pressing members apart {, e.g. for drum brakes}	F16D65/22	F16D65/22		3224
F16D65/28	9	arranged apart from the brake	F16D65/28	F16D65/28		907
F16D65/38	8	Slack adjusters	F16D65/38	F16D65/38		269
F16D2065/383	9	{for adjusting the spring force in spring-applied brakes}	F16D65/38	F16D65/38		118
F16D2065/386	9	{driven electrically}	F16D65/38	F16D65/38		323
F16D65/40	9	mechanical	F16D65/40	F16D65/40		148
F16D65/42	10	non-automatic	F16D65/42	F16D65/42		314
F16D65/44	11	by means of direct linear adjustment	F16D65/44	F16D65/44		75
F16D65/46	11	with screw-thread and nut	F16D65/46	F16D65/46		814
F16D65/48	11	with eccentric or helical body	F16D65/48	F16D65/48		145
F16D65/50	11	for angular adjustment of two concentric parts of the brake control system	F16D65/50	F16D65/50		87
F16D65/52	10	self-acting in one direction for adjusting excessive play	F16D65/52	F16D65/52		589
F16D65/54	11	by means of direct linear adjustment	F16D65/54	F16D65/54		1077
F16D65/543	12	{comprising a plastically-deformable member}	F16D65/54	F16D65/54		127
F16D65/546	12	{for mounting within the confines of a drum brake}	F16D65/54	F16D65/54		384
F16D65/56	11	with screw-thread and nut	F16D65/56	F16D65/56		496
F16D65/561	12	{for mounting within the confines of a drum brake}	F16D65/56	F16D65/56		200
F16D65/562	13	{arranged between service brake actuator and braking member, and subjected to service brake force}	F16D65/56	F16D65/56		258
F16D65/563	13	{arranged adjacent to service brake actuator, e.g. on parking brake lever, and not subjected to service brake force}	F16D65/56	F16D65/56		335
F16D65/565	13	{arranged diametrically opposite to service brake actuator, and subjected to service brake force}	F16D65/56	F16D65/56		278
F16D65/566	13	{having a temperature-sensitive element preventing adjustment when brake is hot}	F16D65/56	F16D65/56		78
F16D65/567	12	{for mounting on a disc brake}	F16D65/56	F16D65/56		1371
F16D65/568	13	{for synchronous adjustment of actuators arranged in parallel}	F16D65/56	F16D65/56		387
F16D65/58	11	with eccentric or helical body	F16D65/58	F16D65/58		209
F16D65/60	11	for angular adjustment of two concentric parts of the brake control systems	F16D65/60	F16D65/60		361
F16D65/62	10	self-acting in both directions for adjusting excessive and insufficient play	F16D65/62	F16D65/62		54
F16D65/64	11	by means of direct linear adjustment	F16D65/64	F16D65/64		35
F16D65/66	11	with screw-thread and nut	F16D65/66	F16D65/66		93
F16D65/68	11	with eccentric or helical body	F16D65/68	F16D65/68		13
F16D65/70	11	for angular adjustment of two concentric parts of the brake control system	F16D65/70	F16D65/70		5
F16D65/72	9	hydraulic	F16D65/72	F16D65/72		76
F16D65/74	10	self-acting in one direction	F16D65/74	F16D65/74		357
F16D65/76	10	self-acting in both directions	F16D65/76	F16D65/76		21
F16D65/78	8	Features relating to cooling	F16D65/78	F16D65/78		1054
F16D2065/781	9	{involving phase change of material}	F16D65/78	F16D65/78		203
F16D2065/782	9	{the brake-actuating fluid being used as a coolant}	F16D65/78	F16D65/78		145
F16D2065/783	9	{cooling control or adjustment}	F16D65/78	F16D65/78		440
F16D2065/784	9	{the coolant not being in direct contact with the braking surface}	F16D65/78	F16D65/78		302
F16D2065/785	9	{Heat insulation or reflection}	F16D65/78	F16D65/78		448
F16D2065/786	9	{Fluid spray devices}	F16D65/78	F16D65/78		98
F16D2065/787	9	{Pumps}	F16D65/78	F16D65/78		169
F16D2065/788	9	{Internal cooling channels}	F16D65/78	F16D65/78		382
F16D2065/789	9	{External cooling ribs}	F16D65/78	F16D65/78		227
F16D65/80	9	for externally-engaging brakes	F16D65/80	F16D65/80		46
F16D65/807	10	with open cooling system, e.g. cooled by air	F16D65/807	F16D65/807		144
F16D65/813	10	with closed cooling system	F16D65/813	F16D65/813		75
F16D65/82	9	for internally-engaging brakes	F16D65/82	F16D65/82		71
F16D65/827	10	with open cooling system, e.g. cooled by air	F16D65/827	F16D65/827		547
F16D65/833	10	with closed cooling system	F16D65/833	F16D65/833		146
F16D65/84	9	for disc brakes {(discs characterised by means for cooling F16D65/128)}	F16D65/84	F16D65/84		438
F16D65/847	10	with open cooling system, e.g. cooled by air	F16D65/847	F16D65/847		1814
F16D65/853	10	with closed cooling system	F16D65/853	F16D65/853		970
F16D66/00	7	Arrangements for monitoring working conditions, e.g. wear, temperature	F16D66/00	F16D66/00		1682
F16D2066/001	8	{Temperature}	F16D66/00	F16D66/00		1038
F16D2066/003	8	{Position, angle or speed}	F16D66/00	F16D66/00		1028
F16D2066/005	8	{Force, torque, stress or strain}	F16D66/00	F16D66/00		1043
F16D2066/006	8	{without direct measurement of the quantity monitored, e.g. wear or temperature calculated form force and duration of braking}	F16D66/00	F16D66/00		508
F16D2066/008	8	{of clutches}	F16D66/00	F16D66/00		156
F16D66/02	8	Apparatus for indicating wear	F16D66/02	F16D66/02		1203
F16D66/021	9	{using electrical detection or indication means}	F16D66/02	F16D66/02		646
F16D66/022	10	{indicating that a lining is worn to minimum allowable thickness}	F16D66/02	F16D66/02		269
F16D66/023	11	{directly sensing the position of braking members}	F16D66/02	F16D66/02		236
F16D66/024	12	{Sensors mounted on braking members adapted to contact the brake disc or drum, e.g. wire loops severed on contact}	F16D66/02	F16D66/02		571
F16D66/025	11	{sensing the position of parts of the brake system other than the braking members, e.g. limit switches mounted on primary cylinders}	F16D66/02	F16D66/02		334
F16D66/026	10	{indicating different degrees of lining wear}	F16D66/02	F16D66/02		404
F16D66/027	11	{Sensors therefor}	F16D66/02	F16D66/02		367
F16D66/028	10	{with non-electrical sensors or signal transmission, e.g. magnetic, optical}	F16D66/02	F16D66/02		272
F16D67/00	7	Combinations of couplings and brakes; Combinations of clutches and brakes (combinations of couplings and clutches F16D47/02; conjoint control of brake systems and driveline clutches in vehicles B60W10/02, B60W10/18)	F16D67/00	F16D67/00		1053
F16D67/02	8	Clutch-brake combinations	F16D67/02	F16D67/02		1584
F16D67/04	9	fluid actuated	F16D67/04	F16D67/04		728
F16D67/06	9	electromagnetically actuated	F16D67/06	F16D67/06		488
F16D69/00	7	Friction linings; Attachment thereof; Selection of coacting friction substances or surfaces (clutching elements F16D13/60; braking members F16D65/02)	F16D69/00	F16D69/00		1285
F16D2069/001	8	{Material of friction lining and support element of same or similar composition}	F16D69/00	F16D69/00		58
F16D2069/002	8	{Combination of different friction materials}	F16D69/00	F16D69/00		746
F16D2069/003	8	{Selection of coacting friction materials}	F16D69/00	F16D69/00		95
F16D2069/004	8	{Profiled friction surfaces, e.g. grooves, dimples}	F16D69/00	F16D69/00		1948
F16D2069/005	8	{having a layered structure}	F16D69/00	F16D69/00		420
F16D2069/006	9	{comprising a heat-insulating layer}	F16D69/00	F16D69/00		99
F16D2069/007	9	{comprising a resilient layer}	F16D69/00	F16D69/00		182
F16D2069/008	9	{Layers of fibrous materials}	F16D69/00	F16D69/00		85
F16D2069/009	8	{Linings attached to both sides of a central support element, e.g. a carrier plate}	F16D69/00	F16D69/00		111
F16D69/02	8	Composition of linings {; Methods of manufacturing}<br><br><u>NOTE</u><br><br> Indexing codes F16D69/021&#160;-&#160;F16D2250/0053 are used for indexing aspects relating to compositions or manufacturing of friction linings 	F16D69/02	F16D69/02		2105
F16D69/021	9	{containing asbestos}	F16D69/02	F16D69/02		165
F16D69/022	10	{in the form of fibres}	F16D69/02	F16D69/02		593
F16D69/023	9	{Composite materials containing carbon and carbon fibres or fibres made of carbonizable material}	F16D69/02	F16D69/02		1228
F16D69/025	9	{Compositions based on an organic binder}	F16D69/02	F16D69/02		491
F16D69/026	10	{containing fibres}	F16D69/02	F16D69/02		1526
F16D69/027	9	{Compositions based on metals or inorganic oxides}	F16D69/02	F16D69/02		1173
F16D69/028	10	{containing fibres}	F16D69/02	F16D69/02		424
F16D69/04	8	Attachment of linings	F16D69/04	F16D69/04		848
F16D69/0408	9	{specially adapted for plane linings}	F16D69/04	F16D69/04		1018
F16D69/0416	9	{specially adapted for curved linings}	F16D69/04	F16D69/04		584
F16D2069/0425	9	{Attachment methods or devices}	F16D69/04	F16D69/04		75
F16D2069/0433	10	{Connecting elements not integral with the braking member, e.g. bolts, rivets}	F16D69/04	F16D69/04		660
F16D2069/0441	10	{Mechanical interlocking, e.g. roughened lining carrier, mating profiles on friction material and lining carrier}	F16D69/04	F16D69/04		794
F16D2069/045	10	{Bonding}	F16D69/04	F16D69/04		175
F16D2069/0458	11	{metallurgic, e.g. welding, brazing, sintering}	F16D69/04	F16D69/04		234
F16D2069/0466	11	{chemical, e.g. using adhesives, vulcanising}	F16D69/04	F16D69/04		345
F16D2069/0475	12	{comprising thermal treatment}	F16D69/04	F16D69/04		260
F16D2069/0483	10	{Lining or lining carrier material shaped in situ}	F16D69/04	F16D69/04		393
F16D2069/0491	10	{Tools, machines, processes}	F16D69/04	F16D69/04		522
F16D71/00	7	Mechanisms for bringing members to rest in a predetermined position (combined with or controlling clutches F16D43/26; means for initiating operation of brakes at a predetermined position F16D65/14; means for securing members after operation F16B1/02)	F16D71/00	F16D71/00		323
F16D71/02	8	comprising auxiliary means for producing the final movement	F16D71/02	F16D71/02		29
F16D71/04	8	providing for selection between a plurality of positions (F16D71/02 takes precedence)	F16D71/04	F16D71/04		129
F16D2121/00	7	Type of actuator operation force	F16D121/00	F16D121/00		5
F16D2121/005	8	{unspecified force for releasing a normally applied brake}	F16D121/00	F16D121/00		38
F16D2121/02	8	Fluid pressure	F16D121/02	F16D121/02		3469
F16D2121/04	9	acting on a piston-type actuator, e.g. for liquid pressure	F16D121/04	F16D121/04		2762
F16D2121/06	10	for releasing a normally applied brake	F16D121/06	F16D121/06		246
F16D2121/08	9	acting on a membrane-type actuator, e.g. for gas pressure	F16D121/08	F16D121/08		220
F16D2121/10	10	for releasing a normally applied brake	F16D121/10	F16D121/10		61
F16D2121/12	9	for releasing a normally applied brake, the type of actuator being irrelevant or not provided for in groups F16D2121/04 - F16D2121/10	F16D121/12	F16D121/12		807
F16D2121/14	8	Mechanical	F16D121/14	F16D121/14		3516
F16D2121/16	9	for releasing a normally applied brake	F16D121/16	F16D121/16		255
F16D2121/18	8	Electric or magnetic	F16D121/18	F16D121/18		277
F16D2121/20	9	using electromagnets	F16D121/20	F16D121/20		1878
F16D2121/22	10	for releasing a normally applied brake	F16D121/22	F16D121/22		1731
F16D2121/24	9	using motors	F16D121/24	F16D121/24		3827
F16D2121/26	10	for releasing a normally applied brake	F16D121/26	F16D121/26		238
F16D2121/28	9	using electrostrictive or magnetostrictive elements, e.g. piezoelectric elements	F16D121/28	F16D121/28		237
F16D2121/30	10	for releasing a normally applied brake	F16D121/30	F16D121/30		23
F16D2121/32	9	using shape memory {or other thermo-mechanical} elements	F16D121/32	F16D121/32		72
F16D2121/34	10	for releasing a normally applied brake	F16D121/34	F16D121/34		10
F16D2123/00	7	Multiple operation forces	F16D123/00	F16D123/00		1868
F16D2125/00	7	Components of actuators	F16D125/00	F16D125/00		11
F16D2125/02	8	Fluid-pressure mechanisms	F16D125/02	F16D125/02		436
F16D2125/023	9	{Pumps}	F16D125/02	F16D125/02		125
F16D2125/026	9	{Pressure-to-pressure converters, e.g. hydropneumatic}	F16D125/02	F16D125/02		35
F16D2125/04	9	Cylinders	F16D125/04	F16D125/04		565
F16D2125/06	9	Pistons	F16D125/06	F16D125/06		1343
F16D2125/08	9	Seals, e.g. piston seals	F16D125/08	F16D125/08		489
F16D2125/10	9	Plural pistons interacting by fluid pressure, e.g. hydraulic force amplifiers using different sized pistons	F16D125/10	F16D125/10		249
F16D2125/12	9	Membrane or diaphragm types	F16D125/12	F16D125/12		103
F16D2125/14	9	Fluid-filled flexible members, e.g. enclosed air bladders	F16D125/14	F16D125/14		170
F16D2125/16	9	Devices for bleeding or filling	F16D125/16	F16D125/16		248
F16D2125/18	8	Mechanical mechanisms	F16D125/18	F16D125/18		60
F16D2125/20	9	converting rotation to linear movement or vice versa	F16D125/20	F16D125/20		93
F16D2125/22	10	acting transversely to the axis of rotation	F16D125/22	F16D125/22		88
F16D2125/24	11	Rack-and-pinion	F16D125/24	F16D125/24		175
F16D2125/26	11	Cranks	F16D125/26	F16D125/26		573
F16D2125/28	11	Cams; Levers with cams	F16D125/28	F16D125/28		399
F16D2125/30	12	acting on two or more cam followers, e.g. S-cams	F16D125/30	F16D125/30		1190
F16D2125/32	12	acting on one cam follower	F16D125/32	F16D125/32		757
F16D2125/34	10	acting in the direction of the axis of rotation	F16D125/34	F16D125/34		144
F16D2125/36	11	Helical cams, Ball-rotating ramps	F16D125/36	F16D125/36		1612
F16D2125/38	12	with plural cam or ball-ramp mechanisms arranged concentrically with the brake rotor axis	F16D125/38	F16D125/38		139
F16D2125/40	11	Screw-and-nut	F16D125/40	F16D125/40		2604
F16D2125/405	12	{with differential thread}	F16D125/40	F16D125/40		46
F16D2125/42	11	Rack-and-worm gears	F16D125/42	F16D125/42		72
F16D2125/44	9	transmitting rotation	F16D125/44	F16D125/44		50
F16D2125/46	10	Rotating members in mutual engagement	F16D125/46	F16D125/46		59
F16D2125/48	11	with parallel stationary axes, e.g. spur gears	F16D125/48	F16D125/48		852
F16D2125/50	11	with parallel non-stationary axes, e.g. planetary gearing	F16D125/50	F16D125/50		628
F16D2125/52	11	with non-parallel stationary axes, e.g. worm or bevel gears	F16D125/52	F16D125/52		425
F16D2125/54	11	with non-parallel non-stationary axes	F16D125/54	F16D125/54		12
F16D2125/56	10	Shafts for transmitting torque directly	F16D125/56	F16D125/56		249
F16D2125/565	11	{flexible}	F16D125/56	F16D125/56		14
F16D2125/58	9	transmitting linear movement	F16D125/58	F16D125/58		137
F16D2125/582	10	{Flexible element, e.g. spring, other than the main force generating element}	F16D125/58	F16D125/58		270
F16D2125/585	11	{arranged in parallel with a force-applying member}	F16D125/58	F16D125/58		44
F16D2125/587	10	{Articulation, e.g. ball-socket}	F16D125/58	F16D125/58		144
F16D2125/60	10	Cables or chains, e.g. Bowden cables	F16D125/60	F16D125/60		1090
F16D2125/62	11	Fixing arrangements therefor, e.g. cable end attachments	F16D125/62	F16D125/62		264
F16D2125/64	10	Levers	F16D125/64	F16D125/64		1165
F16D2125/645	11	{with variable leverage, e.g. movable fulcrum}	F16D125/64	F16D125/64		62
F16D2125/66	10	Wedges	F16D125/66	F16D125/66		1046
F16D2125/68	10	Lever-link mechanisms, e.g. toggles with change of force ratio	F16D125/68	F16D125/68		542
F16D2125/70	10	Rods	F16D125/70	F16D125/70		197
F16D2127/00	7	Auxiliary mechanisms	F16D127/00	F16D127/00		52
F16D2127/001	8	{for automatic or self-acting brake operation}	F16D127/00	F16D127/00		41
F16D2127/002	9	{speed-responsive}	F16D127/00	F16D127/00		132
F16D2127/004	9	{direction-responsive}	F16D127/00	F16D127/00		94
F16D2127/005	9	{force- or torque-responsive}	F16D127/00	F16D127/00		105
F16D2127/007	8	{for non-linear operation}	F16D127/00	F16D127/00		153
F16D2127/008	8	{Trigger mechanisms}	F16D127/00	F16D127/00		87
F16D2127/02	8	Release mechanisms	F16D127/02	F16D127/02		697
F16D2127/04	9	for manual operation	F16D127/04	F16D127/04		431
F16D2127/06	8	Locking mechanisms, e.g. acting on actuators, on release mechanisms or on force transmission mechanisms	F16D127/06	F16D127/06		983
F16D2127/08	8	Self-amplifying or de-amplifying mechanisms	F16D127/08	F16D127/08		317
F16D2127/085	9	{having additional fluid pressure elements}	F16D127/08	F16D127/08		46
F16D2127/10	9	having wedging elements	F16D127/10	F16D127/10		506
F16D2127/12	9	having additional frictional elements	F16D127/12	F16D127/12		115
F16D2129/00	7	Type of operation source for auxiliary mechanisms	F16D129/00	F16D129/00		3
F16D2129/02	8	Fluid-pressure	F16D129/02	F16D129/02		166
F16D2129/04	8	Mechanical	F16D129/04	F16D129/04		68
F16D2129/043	9	{Weights}	F16D129/04	F16D129/04		107
F16D2129/046	9	{Flywheels}	F16D129/04	F16D129/04		12
F16D2129/06	8	Electric or magnetic	F16D129/06	F16D129/06		27
F16D2129/065	9	{Permanent magnets}	F16D129/06	F16D129/06		215
F16D2129/08	9	Electromagnets	F16D129/08	F16D129/08		255
F16D2129/10	9	Motors	F16D129/10	F16D129/10		98
F16D2129/12	9	Electrostrictive or magnetostrictive elements, e.g. piezoelectric	F16D129/12	F16D129/12		48
F16D2129/14	8	Shape memory {or other thermo-mechanical} elements	F16D129/14	F16D129/14		26
F16D2131/00	7	Overall arrangement of the actuators or their elements, e.g. modular construction	F16D131/00	F16D131/00		131
F16D2131/02	8	of the actuator controllers	F16D131/02	F16D131/02		50
F16D2200/00	7	Materials; Production methods therefor	CPCONLY	F16D2200/00		61
F16D2200/0004	8	metallic	CPCONLY	F16D2200/0004		299
F16D2200/0008	9	Ferro	CPCONLY	F16D2200/0008		195
F16D2200/0013	10	Cast iron	CPCONLY	F16D2200/0013		410
F16D2200/0017	10	corrosion-resistant	CPCONLY	F16D2200/0017		104
F16D2200/0021	10	Steel	CPCONLY	F16D2200/0021		503
F16D2200/0026	9	Non-ferro	CPCONLY	F16D2200/0026		362
F16D2200/003	10	Light metals, e.g. aluminium	CPCONLY	F16D2200/003		569
F16D2200/0034	8	non-metallic	CPCONLY	F16D2200/0034		450
F16D2200/0039	9	Ceramics	CPCONLY	F16D2200/0039		374
F16D2200/0043	10	Ceramic base, e.g. metal oxides or ceramic binder	CPCONLY	F16D2200/0043		121
F16D2200/0047	10	Ceramic composite, e.g. C/C composite infiltrated with Si or B, or ceramic matrix infiltrated with metal	CPCONLY	F16D2200/0047		345
F16D2200/0052	9	Carbon	CPCONLY	F16D2200/0052		701
F16D2200/0056	9	Elastomers	CPCONLY	F16D2200/0056		383
F16D2200/006	8	containing fibres or particles	CPCONLY	F16D2200/006		860
F16D2200/0065	9	Inorganic, e.g. non-asbestos mineral fibres	CPCONLY	F16D2200/0065		434
F16D2200/0069	9	being characterised by their size	CPCONLY	F16D2200/0069		224
F16D2200/0073	9	having lubricating properties	CPCONLY	F16D2200/0073		130
F16D2200/0078	8	laminated	CPCONLY	F16D2200/0078		139
F16D2200/0082	8	Production methods therefor	CPCONLY	F16D2200/0082		461
F16D2200/0086	9	Moulding materials together by application of heat and pressure	CPCONLY	F16D2200/0086		760
F16D2200/0091	9	Impregnating a mat of fibres with a binder	CPCONLY	F16D2200/0091		109
F16D2200/0095	9	Mixing an aqueous slurry of fibres with a binder, e.g. papermaking process	CPCONLY	F16D2200/0095		86
F16D2250/00	7	Manufacturing; Assembly	CPCONLY	F16D2250/00		1135
F16D2250/0007	8	Casting	CPCONLY	F16D2250/0007		423
F16D2250/0015	9	around inserts	CPCONLY	F16D2250/0015		261
F16D2250/0023	8	Shaping by pressure	CPCONLY	F16D2250/0023		783
F16D2250/003	8	Chip removing	CPCONLY	F16D2250/003		154
F16D2250/0038	8	Surface treatment	CPCONLY	F16D2250/0038		349
F16D2250/0046	9	Coating	CPCONLY	F16D2250/0046		530
F16D2250/0053	9	Hardening	CPCONLY	F16D2250/0053		186
F16D2250/0061	8	Joining	CPCONLY	F16D2250/0061		196
F16D2250/0069	9	Adhesive bonding	CPCONLY	F16D2250/0069		218
F16D2250/0076	9	Welding, brazing	CPCONLY	F16D2250/0076		284
F16D2250/0084	8	Assembly or disassembly	CPCONLY	F16D2250/0084		755
F16D2250/0092	8	Tools or machines for producing linings	CPCONLY	F16D2250/0092		277
F16D2300/00	7	Special features for couplings or clutches	CPCONLY	F16D2300/00		42
F16D2300/02	8	Overheat protection, i.e. means for protection against overheating	CPCONLY	F16D2300/02		92
F16D2300/021	9	Cooling features not provided for in group F16D13/72 or F16D25/123, e.g. heat transfer details	CPCONLY	F16D2300/021		101
F16D2300/0212	10	Air cooling	CPCONLY	F16D2300/0212		302
F16D2300/0214	10	Oil or fluid cooling	CPCONLY	F16D2300/0214		248
F16D2300/04	8	Heating means	CPCONLY	F16D2300/04		7
F16D2300/06	8	Lubrication details not provided for in group F16D13/74	CPCONLY	F16D2300/06		1128
F16D2300/08	8	Details or arrangements of sealings not provided for in group F16D3/84	CPCONLY	F16D2300/08		1191
F16D2300/10	8	Surface characteristics; Details related to material surfaces	CPCONLY	F16D2300/10		528
F16D2300/12	8	Mounting or assembling	CPCONLY	F16D2300/12		1686
F16D2300/14	8	Clutches which are normally open, i.e. not engaged in released state	CPCONLY	F16D2300/14		220
F16D2300/18	8	Sensors; Details or arrangements thereof	CPCONLY	F16D2300/18		1035
F16D2300/20	8	Auxiliary indicators or alarms	CPCONLY	F16D2300/20		155
F16D2300/22	8	Vibration damping	CPCONLY	F16D2300/22		1404
F16D2300/24	8	Concentric actuation rods, e.g. actuation rods extending concentrically through a shaft	CPCONLY	F16D2300/24		125
F16D2300/26	8	Cover or bell housings; Details or arrangements thereof	CPCONLY	F16D2300/26		674
F16D2500/00	7	External control of clutches by electric or electronic means	CPCONLY	F16D2500/00		3
F16D2500/10	8	System to be controlled	CPCONLY	F16D2500/10		4
F16D2500/102	9	Actuator	CPCONLY	F16D2500/102		55
F16D2500/1021	10	Electrical type	CPCONLY	F16D2500/1021		95
F16D2500/1022	11	Electromagnet	CPCONLY	F16D2500/1022		702
F16D2500/1023	11	Electric motor	CPCONLY	F16D2500/1023		182
F16D2500/1024	12	combined with hydraulic actuation	CPCONLY	F16D2500/1024		344
F16D2500/1025	12	with threaded transmission	CPCONLY	F16D2500/1025		195
F16D2500/1026	10	Hydraulic	CPCONLY	F16D2500/1026		945
F16D2500/1027	11	Details about the hydraulic valves	CPCONLY	F16D2500/1027		115
F16D2500/1028	10	Pneumatic	CPCONLY	F16D2500/1028		261
F16D2500/104	9	Clutch	CPCONLY	F16D2500/104		92
F16D2500/10406	10	Clutch position	CPCONLY	F16D2500/10406		43
F16D2500/10412	11	Transmission line of a vehicle	CPCONLY	F16D2500/10412		2067
F16D2500/10418	11	Accessory clutch, e.g. cooling fan, air conditioning	CPCONLY	F16D2500/10418		121
F16D2500/10425	11	Differential clutch	CPCONLY	F16D2500/10425		73
F16D2500/10431	11	4WD Clutch dividing power between the front and the rear axle	CPCONLY	F16D2500/10431		205
F16D2500/10437	11	Power Take Off clutch	CPCONLY	F16D2500/10437		112
F16D2500/10443	10	Clutch type	CPCONLY	F16D2500/10443		6
F16D2500/1045	11	Friction clutch	CPCONLY	F16D2500/1045		1267
F16D2500/10456	11	Synchro clutch	CPCONLY	F16D2500/10456		30
F16D2500/10462	11	Dog-type clutch	CPCONLY	F16D2500/10462		201
F16D2500/10468	11	Fluid adhesion clutch	CPCONLY	F16D2500/10468		27
F16D2500/10475	11	Magnetic field, e.g. electro-rheological, magnetisable particles	CPCONLY	F16D2500/10475		133
F16D2500/10481	11	Automatic clutch, e.g. centrifugal masses	CPCONLY	F16D2500/10481		119
F16D2500/10487	11	Fluid coupling	CPCONLY	F16D2500/10487		83
F16D2500/10493	11	One way clutch	CPCONLY	F16D2500/10493		88
F16D2500/106	9	Engine	CPCONLY	F16D2500/106		59
F16D2500/1062	10	Diesel	CPCONLY	F16D2500/1062		13
F16D2500/1064	10	Electric	CPCONLY	F16D2500/1064		53
F16D2500/1066	10	Hybrid	CPCONLY	F16D2500/1066		452
F16D2500/1068	10	Engine supercharger or turbocharger	CPCONLY	F16D2500/1068		30
F16D2500/108	9	Gear	CPCONLY	F16D2500/108		25
F16D2500/1081	10	Actuation type	CPCONLY	F16D2500/1081		4
F16D2500/1082	11	Manual transmission	CPCONLY	F16D2500/1082		143
F16D2500/1083	11	Automated manual transmission	CPCONLY	F16D2500/1083		186
F16D2500/1085	11	Automatic transmission	CPCONLY	F16D2500/1085		270
F16D2500/1086	10	Concentric shafts	CPCONLY	F16D2500/1086		167
F16D2500/1087	10	Planetary gearing	CPCONLY	F16D2500/1087		63
F16D2500/1088	10	CVT	CPCONLY	F16D2500/1088		136
F16D2500/11	9	Application	CPCONLY	F16D2500/11		12
F16D2500/1102	10	Lawnmower	CPCONLY	F16D2500/1102		10
F16D2500/1105	10	Marine applications	CPCONLY	F16D2500/1105		56
F16D2500/1107	10	Vehicles	CPCONLY	F16D2500/1107		384
F16D2500/111	11	Agricultural	CPCONLY	F16D2500/111		117
F16D2500/1112	11	Heavy vehicle	CPCONLY	F16D2500/1112		180
F16D2500/1115	11	Racing	CPCONLY	F16D2500/1115		10
F16D2500/1117	11	Motorcycle	CPCONLY	F16D2500/1117		124
F16D2500/112	9	Details of the arrangement of the system	CPCONLY	F16D2500/112		4
F16D2500/30	8	Signal inputs	CPCONLY	F16D2500/30		2
F16D2500/302	9	from the actuator	CPCONLY	F16D2500/302		61
F16D2500/3021	10	Angle	CPCONLY	F16D2500/3021		144
F16D2500/3022	10	Current	CPCONLY	F16D2500/3022		275
F16D2500/3023	10	Force	CPCONLY	F16D2500/3023		118
F16D2500/3024	10	Pressure	CPCONLY	F16D2500/3024		800
F16D2500/3025	10	Fluid flow	CPCONLY	F16D2500/3025		40
F16D2500/3026	10	Stroke	CPCONLY	F16D2500/3026		972
F16D2500/3027	10	Torque	CPCONLY	F16D2500/3027		135
F16D2500/3028	10	Voltage	CPCONLY	F16D2500/3028		160
F16D2500/304	9	from the clutch	CPCONLY	F16D2500/304		75
F16D2500/30401	10	On-off signal indicating the engage or disengaged position of the clutch	CPCONLY	F16D2500/30401		284
F16D2500/30402	10	Clutch friction coefficient	CPCONLY	F16D2500/30402		116
F16D2500/30403	10	Number of clutch actuations	CPCONLY	F16D2500/30403		17
F16D2500/30404	10	Clutch temperature	CPCONLY	F16D2500/30404		333
F16D2500/30405	11	Estimated clutch temperature	CPCONLY	F16D2500/30405		201
F16D2500/30406	10	Clutch slip	CPCONLY	F16D2500/30406		679
F16D2500/30407	11	Clutch slip change rate	CPCONLY	F16D2500/30407		49
F16D2500/30408	10	Relative rotational position of the input and output parts, e.g. for facilitating positive clutch engagement	CPCONLY	F16D2500/30408		60
F16D2500/30409	11	Signals detecting the transmission of zero torque	CPCONLY	F16D2500/30409		3
F16D2500/3041	10	from the input shaft	CPCONLY	F16D2500/3041		7
F16D2500/30412	11	Torque of the input shaft	CPCONLY	F16D2500/30412		184
F16D2500/30415	11	Speed of the input shaft	CPCONLY	F16D2500/30415		607
F16D2500/30417	12	Speed change rate of the input shaft	CPCONLY	F16D2500/30417		45
F16D2500/3042	10	from the output shaft	CPCONLY	F16D2500/3042		7
F16D2500/30421	11	Torque of the output shaft	CPCONLY	F16D2500/30421		443
F16D2500/30423	12	Signal detecting the transmission of zero torque	CPCONLY	F16D2500/30423		7
F16D2500/30425	12	Estimation of the transmitted clutch torque, e.g. applying dynamic torque balance equation	CPCONLY	F16D2500/30425		38
F16D2500/30426	11	Speed of the output shaft	CPCONLY	F16D2500/30426		619
F16D2500/30428	12	Speed change rate of the output shaft	CPCONLY	F16D2500/30428		53
F16D2500/305	9	from the clutch cooling	CPCONLY	F16D2500/305		9
F16D2500/3051	10	Flow amount of cooling fluid	CPCONLY	F16D2500/3051		28
F16D2500/3053	11	On/off signal indicating the presence of cooling oil flow	CPCONLY	F16D2500/3053		1
F16D2500/3055	10	Cooling oil properties	CPCONLY	F16D2500/3055		5
F16D2500/3056	11	Cooling oil temperature	CPCONLY	F16D2500/3056		146
F16D2500/3058	11	Cooling oil pressure	CPCONLY	F16D2500/3058		55
F16D2500/306	9	from the engine	CPCONLY	F16D2500/306		62
F16D2500/3061	10	Engine inlet air flow rate	CPCONLY	F16D2500/3061		49
F16D2500/3062	10	Engine braking signal indicating the use of the engine as a brake	CPCONLY	F16D2500/3062		22
F16D2500/3063	10	Engine fuel flow rate	CPCONLY	F16D2500/3063		50
F16D2500/3064	10	Temperature of the engine	CPCONLY	F16D2500/3064		85
F16D2500/3065	10	Torque of the engine	CPCONLY	F16D2500/3065		487
F16D2500/3066	11	Torque change rate of the engine	CPCONLY	F16D2500/3066		25
F16D2500/3067	10	Speed of the engine	CPCONLY	F16D2500/3067		1350
F16D2500/3068	11	Speed change of rate of the engine	CPCONLY	F16D2500/3068		132
F16D2500/3069	10	Engine ignition switch	CPCONLY	F16D2500/3069		190
F16D2500/308	9	from the transmission	CPCONLY	F16D2500/308		64
F16D2500/30801	10	Number of shift actuations	CPCONLY	F16D2500/30801		18
F16D2500/30802	10	Transmission oil properties	CPCONLY	F16D2500/30802		12
F16D2500/30803	11	Oil temperature	CPCONLY	F16D2500/30803		191
F16D2500/30805	11	Oil pressure	CPCONLY	F16D2500/30805		24
F16D2500/30806	10	Engaged transmission ratio	CPCONLY	F16D2500/30806		461
F16D2500/30807	11	Estimation of the engaged transmission ratio	CPCONLY	F16D2500/30807		41
F16D2500/30808	11	Detection of transmission in neutral	CPCONLY	F16D2500/30808		164
F16D2500/3081	10	from the input shaft	CPCONLY	F16D2500/3081		6
F16D2500/30812	11	Direction of rotation of the input shaft	CPCONLY	F16D2500/30812		6
F16D2500/30814	11	Torque of the input shaft	CPCONLY	F16D2500/30814		69
F16D2500/30816	11	Speed of the input shaft	CPCONLY	F16D2500/30816		378
F16D2500/30818	12	Speed change rate of the input shaft	CPCONLY	F16D2500/30818		50
F16D2500/3082	10	from the output shaft	CPCONLY	F16D2500/3082		6
F16D2500/30822	11	Torque of the output shaft	CPCONLY	F16D2500/30822		38
F16D2500/30825	11	Speed of the output shaft	CPCONLY	F16D2500/30825		171
F16D2500/30827	12	Speed change rate of the output shaft	CPCONLY	F16D2500/30827		13
F16D2500/31	9	from the vehicle	CPCONLY	F16D2500/31		60
F16D2500/3101	10	Detection of a brake actuation by a sensor on the brake	CPCONLY	F16D2500/3101		149
F16D2500/3102	10	Vehicle direction of travel, i.e. forward/reverse	CPCONLY	F16D2500/3102		60
F16D2500/3104	10	Travelled distance	CPCONLY	F16D2500/3104		22
F16D2500/3105	10	Operational Time of clutches during vehicle life	CPCONLY	F16D2500/3105		6
F16D2500/3107	10	Vehicle weight	CPCONLY	F16D2500/3107		57
F16D2500/3108	10	Vehicle speed	CPCONLY	F16D2500/3108		593
F16D2500/3109	11	Vehicle acceleration	CPCONLY	F16D2500/3109		171
F16D2500/3111	11	Standing still, i.e. signal detecting when the vehicle is standing still or bellow a certain limit speed	CPCONLY	F16D2500/3111		179
F16D2500/3112	11	Vehicle acceleration change rate	CPCONLY	F16D2500/3112		15
F16D2500/3114	10	Vehicle wheels	CPCONLY	F16D2500/3114		13
F16D2500/3115	11	Vehicle wheel speed	CPCONLY	F16D2500/3115		192
F16D2500/3117	11	Vehicle wheel torque	CPCONLY	F16D2500/3117		25
F16D2500/3118	11	Slip of vehicle wheels	CPCONLY	F16D2500/3118		54
F16D2500/312	9	External to the vehicle	CPCONLY	F16D2500/312		13
F16D2500/3121	10	Ambient conditions, e.g. air humidity, air temperature, ambient pressure	CPCONLY	F16D2500/3121		38
F16D2500/3122	11	Ambient temperature	CPCONLY	F16D2500/3122		81
F16D2500/3124	10	Driving conditions, e.g. climbing hills, cornering, traffic	CPCONLY	F16D2500/3124		58
F16D2500/3125	10	Driving resistance, i.e. external factors having an influence in the traction force, e.g. road friction, air resistance, road slope	CPCONLY	F16D2500/3125		63
F16D2500/3127	11	Road slope	CPCONLY	F16D2500/3127		113
F16D2500/3128	10	Distance from the vehicle to an external element, e.g. to an obstacle, to an other vehicle or a target	CPCONLY	F16D2500/3128		25
F16D2500/314	9	from the user	CPCONLY	F16D2500/314		28
F16D2500/31406	10	input from pedals	CPCONLY	F16D2500/31406		37
F16D2500/31413	11	Clutch pedal position	CPCONLY	F16D2500/31413		417
F16D2500/3142	12	Clutch pedal position rate	CPCONLY	F16D2500/3142		36
F16D2500/31426	11	Brake pedal position	CPCONLY	F16D2500/31426		258
F16D2500/31433	12	Brake pedal position threshold, e.g. switch	CPCONLY	F16D2500/31433		78
F16D2500/3144	11	Accelerator pedal position	CPCONLY	F16D2500/3144		716
F16D2500/31446	12	Accelerator pedal position change rate	CPCONLY	F16D2500/31446		53
F16D2500/31453	12	Accelerator pedal position threshold, e.g. switch	CPCONLY	F16D2500/31453		116
F16D2500/3146	10	input from levers	CPCONLY	F16D2500/3146		88
F16D2500/31466	11	Gear lever	CPCONLY	F16D2500/31466		515
F16D2500/31473	11	Parking brake lever	CPCONLY	F16D2500/31473		55
F16D2500/3148	10	Detection of user presence	CPCONLY	F16D2500/3148		26
F16D2500/31486	10	Recognition of user style of driving, e.g. sportive, calm, nervous	CPCONLY	F16D2500/31486		25
F16D2500/31493	10	Switches on the dashboard	CPCONLY	F16D2500/31493		143
F16D2500/316	9	Other signal inputs not covered by the groups above	CPCONLY	F16D2500/316		25
F16D2500/3161	10	Signal providing information about the state of engine accessories	CPCONLY	F16D2500/3161		26
F16D2500/3163	10	Using the natural frequency of a component as input for the control	CPCONLY	F16D2500/3163		34
F16D2500/3165	10	Using the moment of inertia of a component as input for the control	CPCONLY	F16D2500/3165		74
F16D2500/3166	10	Detection of an elapsed period of time	CPCONLY	F16D2500/3166		667
F16D2500/3168	10	Temperature detection of any component of the control system	CPCONLY	F16D2500/3168		101
F16D2500/50	8	Problem to be solved by the control system	CPCONLY	F16D2500/50		3
F16D2500/501	9	Relating the actuator	CPCONLY	F16D2500/501		109
F16D2500/5012	10	Accurate determination of the clutch positions, e.g. treating the signal from the position sensor, or by using two position sensors for determination	CPCONLY	F16D2500/5012		160
F16D2500/5014	10	Filling the actuator cylinder with fluid	CPCONLY	F16D2500/5014		131
F16D2500/5016	10	Shifting operation, i.e. volume compensation of the primary cylinder due to wear, temperature changes or leaks in the cylinder	CPCONLY	F16D2500/5016		84
F16D2500/5018	10	Calibration or recalibration of the actuator	CPCONLY	F16D2500/5018		164
F16D2500/502	9	Relating the clutch	CPCONLY	F16D2500/502		54
F16D2500/50203	10	Transition between manual and automatic control of the clutch	CPCONLY	F16D2500/50203		55
F16D2500/50206	10	Creep control	CPCONLY	F16D2500/50206		119
F16D2500/50209	11	Activation of the creep control operation	CPCONLY	F16D2500/50209		15
F16D2500/50212	12	Accelerator pedal	CPCONLY	F16D2500/50212		26
F16D2500/50215	12	Brake pedal	CPCONLY	F16D2500/50215		34
F16D2500/50218	12	Clutch pedal	CPCONLY	F16D2500/50218		1
F16D2500/50221	12	Manual switch actuated by the user	CPCONLY	F16D2500/50221		16
F16D2500/50224	10	Drive-off	CPCONLY	F16D2500/50224		358
F16D2500/50227	10	Control of clutch to control engine	CPCONLY	F16D2500/50227		78
F16D2500/5023	10	Determination of the clutch wear	CPCONLY	F16D2500/5023		155
F16D2500/50233	10	Clutch wear adjustment operation	CPCONLY	F16D2500/50233		108
F16D2500/50236	10	Adaptations of the clutch characteristics, e.g. curve clutch capacity torque - clutch actuator displacement	CPCONLY	F16D2500/50236		323
F16D2500/50239	10	Soft clutch engagement	CPCONLY	F16D2500/50239		237
F16D2500/50242	10	Cleaning of clutches, e.g. controlling the engine or the clutch to provoke vibrations eliminating particles from the clutch friction surfaces	CPCONLY	F16D2500/50242		9
F16D2500/50245	10	Calibration or recalibration of the clutch touch-point	CPCONLY	F16D2500/50245		215
F16D2500/50248	11	During assembly	CPCONLY	F16D2500/50248		37
F16D2500/50251	11	During operation	CPCONLY	F16D2500/50251		221
F16D2500/50254	12	Brake actuated	CPCONLY	F16D2500/50254		37
F16D2500/50257	12	During a creep operation	CPCONLY	F16D2500/50257		32
F16D2500/5026	12	Gear engaged	CPCONLY	F16D2500/5026		35
F16D2500/50263	12	During standing still	CPCONLY	F16D2500/50263		55
F16D2500/50266	11	Way of detection	CPCONLY	F16D2500/50266		29
F16D2500/50269	12	Engine speed	CPCONLY	F16D2500/50269		65
F16D2500/50272	12	Gearing speed	CPCONLY	F16D2500/50272		45
F16D2500/50275	12	Estimation of the displacement of the clutch touch-point due to the modification of relevant parameters, e.g. temperature, wear	CPCONLY	F16D2500/50275		97
F16D2500/50278	12	Stalling	CPCONLY	F16D2500/50278		2
F16D2500/50281	12	Transmitted torque	CPCONLY	F16D2500/50281		71
F16D2500/50284	10	Control of secondary clutch in the driveline, i.e. not including clutches in automatic transmission, e.g. in the vicinity of rear axle or on parallel drive shaft	CPCONLY	F16D2500/50284		17
F16D2500/50287	10	Torque control	CPCONLY	F16D2500/50287		326
F16D2500/5029	11	Reducing drag torque	CPCONLY	F16D2500/5029		57
F16D2500/50293	10	Reduction of vibrations	CPCONLY	F16D2500/50293		355
F16D2500/50296	10	Limit clutch wear	CPCONLY	F16D2500/50296		250
F16D2500/503	9	relating to the accumulator	CPCONLY	F16D2500/503		1
F16D2500/5035	10	Filling level of an accumulator providing fluid for the engagement of the clutch	CPCONLY	F16D2500/5035		11
F16D2500/504	9	Relating the engine	CPCONLY	F16D2500/504		33
F16D2500/5041	10	Control of engine accessories, e.g. air conditioning, pumps, auxiliary drive	CPCONLY	F16D2500/5041		20
F16D2500/5043	10	Engine fuel consumption	CPCONLY	F16D2500/5043		69
F16D2500/5045	10	Control of engine at idle, i.e. controlling engine idle conditions, e.g. idling speed	CPCONLY	F16D2500/5045		71
F16D2500/5046	10	Preventing engine over-speed, e.g. by actuation of the main clutch	CPCONLY	F16D2500/5046		47
F16D2500/5048	10	Stall prevention	CPCONLY	F16D2500/5048		130
F16D2500/506	9	Relating the transmission	CPCONLY	F16D2500/506		45
F16D2500/50607	10	Facilitating engagement of a dog clutches, e.g. preventing of gear butting	CPCONLY	F16D2500/50607		67
F16D2500/50615	10	Facilitating disengagement of a dog clutch, e.g. by applying a pretension on the disengaging elements	CPCONLY	F16D2500/50615		19
F16D2500/50623	10	Preventing transmission load change	CPCONLY	F16D2500/50623		20
F16D2500/5063	10	Shaft dither, i.e. applying a pulsating torque to a (transmission) shaft to create a buzz or dither, e.g. to prevent tooth butting or gear locking	CPCONLY	F16D2500/5063		23
F16D2500/50638	10	Shaft speed synchronising, e.g. using engine, clutch outside transmission	CPCONLY	F16D2500/50638		58
F16D2500/50646	10	Control of the main clutch to prevent or release a tooth-to-tooth condition in the transmission	CPCONLY	F16D2500/50646		4
F16D2500/50653	10	Gearing shifting without the interruption of drive	CPCONLY	F16D2500/50653		76
F16D2500/50661	10	Limit transmission input torque	CPCONLY	F16D2500/50661		23
F16D2500/50669	10	Neutral control, i.e. preventing creep or drag torque being transmitted in a transmission with a torque converter when the vehicle is stationary	CPCONLY	F16D2500/50669		16
F16D2500/50676	10	Optimising drive-train operating point, e.g. selecting gear ratio giving maximum fuel economy, best performance	CPCONLY	F16D2500/50676		33
F16D2500/50684	10	Torque resume after shifting	CPCONLY	F16D2500/50684		141
F16D2500/50692	10	Simulate the characteristics of a torque converter	CPCONLY	F16D2500/50692		6
F16D2500/507	9	Relating the vehicle	CPCONLY	F16D2500/507		19
F16D2500/5075	10	Prevention or regulation of vehicle&apos;s wheel slip	CPCONLY	F16D2500/5075		53
F16D2500/508	9	Relating driving conditions	CPCONLY	F16D2500/508		41
F16D2500/50808	10	Cold starting	CPCONLY	F16D2500/50808		33
F16D2500/50816	10	Control during a braking operation, e.g. during ABS control	CPCONLY	F16D2500/50816		44
F16D2500/50825	10	Hill climbing or descending	CPCONLY	F16D2500/50825		67
F16D2500/50833	10	Control during a stability control operation [ESP]	CPCONLY	F16D2500/50833		5
F16D2500/50841	10	Hill hold	CPCONLY	F16D2500/50841		60
F16D2500/5085	10	Coasting	CPCONLY	F16D2500/5085		130
F16D2500/50858	10	Selecting a Mode of operation	CPCONLY	F16D2500/50858		180
F16D2500/50866	10	Parking, i.e. control of drive units during parking	CPCONLY	F16D2500/50866		13
F16D2500/50875	10	Driving in reverse	CPCONLY	F16D2500/50875		9
F16D2500/50883	10	Stop-and-go, i.e. repeated stopping and starting, e.g. in traffic jams	CPCONLY	F16D2500/50883		79
F16D2500/50891	10	Towing or towed	CPCONLY	F16D2500/50891		12
F16D2500/51	9	Relating safety	CPCONLY	F16D2500/51		120
F16D2500/5102	10	Detecting abnormal operation, e.g. unwanted slip or excessive temperature	CPCONLY	F16D2500/5102		169
F16D2500/5104	10	Preventing failures	CPCONLY	F16D2500/5104		143
F16D2500/5106	11	Overheat protection	CPCONLY	F16D2500/5106		223
F16D2500/5108	10	Failure diagnosis	CPCONLY	F16D2500/5108		251
F16D2500/511	11	Leak detection	CPCONLY	F16D2500/511		47
F16D2500/5112	11	Using signals from redundant sensors	CPCONLY	F16D2500/5112		25
F16D2500/5114	10	Failsafe	CPCONLY	F16D2500/5114		253
F16D2500/5116	10	Manufacture, testing, calibrating, i.e. test or calibration of components during or soon after assembly, e.g. at the end of the production line (F16D2500/50248 takes precedence)	CPCONLY	F16D2500/5116		67
F16D2500/5118	10	Maintenance	CPCONLY	F16D2500/5118		53
F16D2500/512	9	Relating to the driver	CPCONLY	F16D2500/512		7
F16D2500/5122	10	Improve passengers comfort	CPCONLY	F16D2500/5122		103
F16D2500/5124	10	Driver error, i.e. preventing effects of unintended or incorrect driver inputs	CPCONLY	F16D2500/5124		47
F16D2500/5126	10	Improving response to driver inputs	CPCONLY	F16D2500/5126		85
F16D2500/5128	10	Driver workload reduction	CPCONLY	F16D2500/5128		70
F16D2500/52	9	General	CPCONLY	F16D2500/52		4
F16D2500/525	10	Improve response of control system	CPCONLY	F16D2500/525		221
F16D2500/70	8	Details about the implementation of the control system	CPCONLY	F16D2500/70		1
F16D2500/702	9	Look-up tables	CPCONLY	F16D2500/702		72
F16D2500/70205	10	Clutch actuator	CPCONLY	F16D2500/70205		19
F16D2500/70211	11	Force	CPCONLY	F16D2500/70211		61
F16D2500/70217	11	Pressure	CPCONLY	F16D2500/70217		188
F16D2500/70223	11	Current	CPCONLY	F16D2500/70223		93
F16D2500/70229	11	Voltage	CPCONLY	F16D2500/70229		30
F16D2500/70235	11	Displacement	CPCONLY	F16D2500/70235		189
F16D2500/70241	11	Angle	CPCONLY	F16D2500/70241		21
F16D2500/70247	10	Engine	CPCONLY	F16D2500/70247		48
F16D2500/70252	10	Clutch torque	CPCONLY	F16D2500/70252		207
F16D2500/70258	11	Throttle	CPCONLY	F16D2500/70258		30
F16D2500/70264	11	Stroke	CPCONLY	F16D2500/70264		145
F16D2500/7027	11	Engine speed	CPCONLY	F16D2500/7027		119
F16D2500/70276	11	Slip	CPCONLY	F16D2500/70276		32
F16D2500/70282	11	Time	CPCONLY	F16D2500/70282		77
F16D2500/70288	11	Clutch pedal position	CPCONLY	F16D2500/70288		34
F16D2500/70294	10	Valve look-up tables	CPCONLY	F16D2500/70294		25
F16D2500/704	9	Output parameters from the control unit; Target parameters to be controlled	CPCONLY	F16D2500/704		4
F16D2500/70402	10	Actuator parameters	CPCONLY	F16D2500/70402		22
F16D2500/70404	11	Force	CPCONLY	F16D2500/70404		161
F16D2500/70406	11	Pressure	CPCONLY	F16D2500/70406		645
F16D2500/70408	11	Torque	CPCONLY	F16D2500/70408		164
F16D2500/7041	11	Position	CPCONLY	F16D2500/7041		1230
F16D2500/70412	12	Clutch position change rate	CPCONLY	F16D2500/70412		86
F16D2500/70414	12	Quick displacement to clutch touch point	CPCONLY	F16D2500/70414		133
F16D2500/70416	11	Angle	CPCONLY	F16D2500/70416		18
F16D2500/70418	11	Current	CPCONLY	F16D2500/70418		585
F16D2500/7042	11	Voltage	CPCONLY	F16D2500/7042		228
F16D2500/70422	10	Clutch parameters	CPCONLY	F16D2500/70422		21
F16D2500/70424	11	Outputting a clutch engaged-disengaged signal	CPCONLY	F16D2500/70424		230
F16D2500/70426	11	Clutch slip	CPCONLY	F16D2500/70426		454
F16D2500/70428	12	Clutch slip change rate	CPCONLY	F16D2500/70428		23
F16D2500/7043	11	Clutch temperature	CPCONLY	F16D2500/7043		60
F16D2500/70432	11	From the input shaft	CPCONLY	F16D2500/70432		1
F16D2500/70434	12	Input shaft torque	CPCONLY	F16D2500/70434		25
F16D2500/70436	12	Input shaft speed	CPCONLY	F16D2500/70436		41
F16D2500/70438	11	From the output shaft	CPCONLY	F16D2500/70438		1
F16D2500/7044	12	Output shaft torque	CPCONLY	F16D2500/7044		521
F16D2500/70442	12	Output shaft speed	CPCONLY	F16D2500/70442		76
F16D2500/70444	13	Output shaft speed rate	CPCONLY	F16D2500/70444		8
F16D2500/70446	10	Clutch cooling parameters	CPCONLY	F16D2500/70446		16
F16D2500/70448	11	for regulating the amount of fluid flow	CPCONLY	F16D2500/70448		77
F16D2500/7045	12	On/off switching of the cooling fluid flow	CPCONLY	F16D2500/7045		20
F16D2500/70452	10	Engine parameters	CPCONLY	F16D2500/70452		31
F16D2500/70454	11	Engine speed	CPCONLY	F16D2500/70454		195
F16D2500/70456	12	Engine speed change rate	CPCONLY	F16D2500/70456		10
F16D2500/70458	11	Engine torque	CPCONLY	F16D2500/70458		158
F16D2500/7046	12	Engine torque change rate	CPCONLY	F16D2500/7046		5
F16D2500/70462	11	Opening of the throttle valve	CPCONLY	F16D2500/70462		29
F16D2500/70464	10	Transmission parameters	CPCONLY	F16D2500/70464		16
F16D2500/70466	11	Input shaft	CPCONLY	F16D2500/70466		
F16D2500/70468	12	Input shaft torque	CPCONLY	F16D2500/70468		11
F16D2500/7047	13	Input shaft torque change rate	CPCONLY	F16D2500/7047		
F16D2500/70472	12	Input shaft speed	CPCONLY	F16D2500/70472		22
F16D2500/70474	13	Input shaft speed change rate	CPCONLY	F16D2500/70474		4
F16D2500/70476	11	Output shaft	CPCONLY	F16D2500/70476		
F16D2500/70478	12	Output shaft power	CPCONLY	F16D2500/70478		
F16D2500/7048	12	Output shaft torque	CPCONLY	F16D2500/7048		20
F16D2500/70482	13	Output shaft torque change rate	CPCONLY	F16D2500/70482		
F16D2500/70484	12	Output shaft speed	CPCONLY	F16D2500/70484		8
F16D2500/70486	13	Output shaft speed change rate	CPCONLY	F16D2500/70486		1
F16D2500/70488	11	Selection of the gear ratio	CPCONLY	F16D2500/70488		103
F16D2500/7049	10	Brake parameters	CPCONLY	F16D2500/7049		22
F16D2500/70492	10	Vehicle parameters	CPCONLY	F16D2500/70492		5
F16D2500/70494	11	Vehicle speed	CPCONLY	F16D2500/70494		23
F16D2500/70496	12	Vehicle acceleration	CPCONLY	F16D2500/70496		15
F16D2500/70498	13	Vehicle acceleration change rate	CPCONLY	F16D2500/70498		2
F16D2500/706	9	Strategy of control	CPCONLY	F16D2500/706		17
F16D2500/70605	10	Adaptive correction; Modifying control system parameters, e.g. gains, constants, look-up tables	CPCONLY	F16D2500/70605		578
F16D2500/7061	10	Feed-back	CPCONLY	F16D2500/7061		176
F16D2500/70615	11	PI control	CPCONLY	F16D2500/70615		67
F16D2500/70621	11	PD control	CPCONLY	F16D2500/70621		8
F16D2500/70626	11	PID control	CPCONLY	F16D2500/70626		99
F16D2500/70631	10	Feed-forward	CPCONLY	F16D2500/70631		39
F16D2500/70636	10	Fuzzy logic	CPCONLY	F16D2500/70636		7
F16D2500/70642	10	Inverse model	CPCONLY	F16D2500/70642		13
F16D2500/70647	10	Neuronal network	CPCONLY	F16D2500/70647		17
F16D2500/70652	10	Open loop	CPCONLY	F16D2500/70652		20
F16D2500/70657	10	Predictor methods	CPCONLY	F16D2500/70657		37
F16D2500/70663	10	State analysis; Analysing potential states of the machine and developing control strategies at each state	CPCONLY	F16D2500/70663		79
F16D2500/70668	10	Signal filtering	CPCONLY	F16D2500/70668		234
F16D2500/70673	10	Statistical calculations	CPCONLY	F16D2500/70673		50
F16D2500/70678	11	using histograms	CPCONLY	F16D2500/70678		5
F16D2500/70684	11	using regressions	CPCONLY	F16D2500/70684		13
F16D2500/70689	11	using maximum or minimum values	CPCONLY	F16D2500/70689		69
F16D2500/70694	11	with plausibility checks	CPCONLY	F16D2500/70694		15
F16D2500/708	9	Mathematical model	CPCONLY	F16D2500/708		38
F16D2500/7082	10	of the clutch	CPCONLY	F16D2500/7082		126
F16D2500/7085	10	of the driver	CPCONLY	F16D2500/7085		3
F16D2500/7087	10	of the vehicle	CPCONLY	F16D2500/7087		7
F16D2500/71	9	Actions	CPCONLY	F16D2500/71		1
F16D2500/7101	10	Driver alarm	CPCONLY	F16D2500/7101		169
F16D2500/7102	11	by provoking vibrations of a vehicle part	CPCONLY	F16D2500/7102		16
F16D2500/7103	11	Acoustic alarms	CPCONLY	F16D2500/7103		49
F16D2500/7104	11	Visual alarms	CPCONLY	F16D2500/7104		78
F16D2500/7105	10	Inhibit control automatically	CPCONLY	F16D2500/7105		95
F16D2500/7106	10	Gearshift to neutral	CPCONLY	F16D2500/7106		14
F16D2500/7107	10	Others	CPCONLY	F16D2500/7107		1
F16D2500/7108	11	Engine torque calculation	CPCONLY	F16D2500/7108		6
F16D2500/7109	11	Pulsed signal; Generating or processing pulsed signals; PWM, width modulation, frequency or amplitude modulation	CPCONLY	F16D2500/7109		300
