E05C1/00	7	Fastening devices with bolts moving rectilinearly	E05C1/00	E05C1/00		109
E05C1/002	8	{perpendicular to the surface on which the fastener is mounted}	E05C1/00	E05C1/00		131
E05C1/004	8	{parallel to the surface on which the fastener is mounted}	E05C1/00	E05C1/00		314
E05C1/006	9	{parallel to the wing edge}	E05C1/00	E05C1/00		142
E05C2001/008	8	{the axis of the bolt movement forming an oblique angle with the surface from which the bolt protrudes, e.g. the wing edge}	E05C1/00	E05C1/00		38
E05C1/02	8	without latching action	E05C1/02	E05C1/02		262
E05C1/04	9	with operating handle or equivalent member rigid with the bolt	E05C1/04	E05C1/04		1620
E05C1/06	9	with operating handle or equivalent member moving otherwise than rigidly with the bolt	E05C1/06	E05C1/06		825
E05C1/065	10	{flush}	E05C1/06	E05C1/06		185
E05C1/08	8	with latching action	E05C1/08	E05C1/08		571
E05C1/085	9	{With means for assisting depression of the latch bolt during latching}	E05C1/08	E05C1/08		68
E05C1/10	9	with operating handle or equivalent member rigid with the latch	E05C1/10	E05C1/10		1100
E05C1/12	9	with operating handle or equivalent member moving otherwise than rigidly with the latch	E05C1/12	E05C1/12		488
E05C1/14	10	the handle or member moving essentially towards or away from the plane of the wing or frame	E05C1/14	E05C1/14		774
E05C1/145	11	{flush}	E05C1/14	E05C1/14		196
E05C1/16	10	the handle or member moving essentially in a plane substantially parallel to the wing or frame	E05C1/16	E05C1/16		748
E05C1/163	11	{Cylindrical or tubular latches}	E05C1/16	E05C1/16		564
E05C1/166	11	{with sliding handle}	E05C1/16	E05C1/16		56
E05C3/00	7	Fastening devices with bolts moving pivotally or rotatively	E05C3/00	E05C3/00		165
E05C3/002	8	{sliding in an arcuate guide or the like (locks with circular bolts E05B63/123)}	E05C3/00	E05C3/00		20
E05C3/004	8	{about an axis perpendicular to the surface on which the fastener is mounted}	E05C3/00	E05C3/00		187
E05C3/006	8	{about an axis parallel to the surface on which the fastener is mounted}	E05C3/00	E05C3/00		92
E05C3/008	9	{parallel to the wing edge}	E05C3/00	E05C3/00		66
E05C3/02	8	without latching action	E05C3/02	E05C3/02		160
E05C3/04	9	with operating handle or equivalent member rigid with the bolt	E05C3/04	E05C3/04		292
E05C3/041	10	{rotating about an axis perpendicular to the surface on which the fastener is mounted}	E05C3/04	E05C3/04		377
E05C3/042	11	{the handle being at one side, the bolt at the other side or inside the wing}	E05C3/04	E05C3/04		1126
E05C3/043	11	{the pivot being between bolt and handle (E05C3/042 takes precedence)}	E05C3/04	E05C3/04		263
E05C3/044	11	{the bolt and handle being at the same side of the pivot (E05C3/045, E05C3/046 take precedence)}	E05C3/04	E05C3/04		185
E05C3/045	11	{in the form of a hook (hook-like fastenings E05C19/10)}	E05C3/04	E05C3/04		220
E05C3/046	11	{in the form of a crescent-shaped cam (hooks E05C3/045)}	E05C3/04	E05C3/04		416
E05C3/047	10	{rotating about an axis parallel to the surface on which the fastener is mounted}	E05C3/04	E05C3/04		102
E05C3/048	11	{parallel to the wing edge}	E05C3/04	E05C3/04		222
E05C3/06	9	with operating handle or equivalent member moving otherwise than rigidly with the bolt	E05C3/06	E05C3/06		168
E05C3/08	10	the handle or member moving essentially towards or away from the plane of the wing or frame	E05C3/08	E05C3/08		116
E05C3/10	10	the handle or member moving essentially in a plane substantially parallel to the wing {or frame}	E05C3/10	E05C3/10		118
E05C3/12	8	with latching action (devices in which the securing part is formed or merely carried by a spring and moves only by distortion of the spring, e.g. snaps, E05C19/06; tilt-plate latches E05C19/007)	E05C3/12	E05C3/12		566
E05C3/122	9	{flush}	E05C3/12	E05C3/12		91
E05C3/124	9	{with latch under compression force between its pivot and the striker (E05C3/122, E05C3/14, E05C3/16 and E05B65/0852 take precedence)}	E05C3/12	E05C3/12		377
E05C2003/126	9	{Only part of the latch movable for latching}	E05C3/12	E05C3/12		7
E05C2003/128	9	{Pendulum-type bolt}	E05C3/12	E05C3/12		11
E05C3/14	9	with operating handle or equivalent member rigid with the latch {(E05C3/122 takes precedence)}	E05C3/14	E05C3/14		959
E05C3/145	10	{pivoting about an axis perpendicular to the wing}	E05C3/14	E05C3/14		231
E05C3/16	9	with operating handle or equivalent member moving otherwise than rigidly with the latch {(E05C3/122 takes precedence)}	E05C3/16	E05C3/16		208
E05C3/162	10	{the handle or member moving essentially towards or away of the plane of the wing or frame (E05C3/167 takes precedence)}	E05C3/16	E05C3/16		312
E05C3/165	10	{the handle or member moving substantially parallel to the wing or frame (E05C3/167 takes precedence)}	E05C3/16	E05C3/16		96
E05C3/167	10	{the latch pivoting about an axis perpendicular to the wing}	E05C3/16	E05C3/16		187
E05C3/22	10	the bolt being spring controlled	E05C3/22	E05C3/22		98
E05C3/24	11	in the form of a bifurcated member {(automatic catches with a bifurcated latch E05C19/024; locks with a bifurcated bolt E05B65/0046, E05B85/243)}	E05C3/24	E05C3/24		742
E05C3/26	12	engaging a stud-like keeper (stud-like keepers per seE05B2015/0235)	E05C3/26	E05C3/26		23
E05C3/28	13	with simultaneously operating double bolts {(vehicle locks with a pair of bifurcated bolts E05B85/245)}	E05C3/28	E05C3/28		44
E05C3/30	11	in the form of a hook {(hook-like fastenings E05C19/10; locks for sliding wings with pivoting bolts E05B65/0811, E05B65/0835)}	E05C3/30	E05C3/30		436
E05C3/34	12	with simultaneously operating double bolts {(locks for sliding wings with bolts pivoting about an axis parallel to the wings E05B65/0835, comprising simultaneously pivoting double hook-like locking members E05B65/0858)}	E05C3/34	E05C3/34		213
E05C3/36	11	in the form of a rotary gear {(vehicle door locks E05B85/28)}	E05C3/36	E05C3/36		32
E05C3/38	11	with bolts engaging a hooked keeper (E05C3/24, E05C3/30, E05C3/36 take precedence)	E05C3/38	E05C3/38		4
E05C3/40	11	with bolts engaging a stud-like keeper (E05C3/24, E05C3/30, E05C3/36 take precedence)	E05C3/40	E05C3/40		105
E05C5/00	7	Fastening devices with bolts moving otherwise than only rectilinearly and only pivotally or rotatively {(E05C9/1883, E05C19/009, E05B63/125, E05B63/126, E05B63/127 take precedence; pivotally-mounted hooks-like fastenings with toggle action E05C19/14; bayonet-type locks E05B63/125; locks for sliding wings, with additional movement E05B65/0817)}	E05C5/00	E05C5/00		659
E05C2005/005	8	{Pivoting bolts or catches being able to move in an additional direction, e.g. by sliding or by pivoting about an additional axis, in order to allow closing of the wing even if the bolt or catch is in its locked position}	E05C5/00	E05C5/00		72
E05C5/02	8	both moving axially and turning about their axis to secure the wing	E05C5/02	E05C5/02		244
E05C5/04	9	performing both movements simultaneously, e.g. screwing into a keeper	E05C5/04	E05C5/04		314
E05C7/00	7	Fastening devices specially adapted for two wings<br><br><u>NOTE</u><br><br>If a fastening device merely secures one wing to another wing which is already closed it is not regarded as specially adapted for two wings	E05C7/00	E05C7/00		318
E05C7/002	8	{for sluice doors (for nuclear reactors G21C13/0285)}	E05C7/00	E05C7/00		99
E05C7/005	8	{for "Dutch doors", i.e. upper and lower wings}	E05C7/00	E05C7/00		55
E05C2007/007	8	{for a double-wing sliding door or window, i.e. where both wings are slidable}	E05C7/00	E05C7/00		332
E05C7/02	8	for wings which lie one behind the other when closed {(E05C7/002 takes precedence)}	E05C7/02	E05C7/02		406
E05C7/04	8	for wings which abut when closed {(pillarless vehicle doors E05B83/38)}	E05C7/04	E05C7/04		787
E05C7/045	9	{Sliding bolts mounted on or in the edge of a normally closed wing of a double-door or -window}	E05C7/04	E05C7/04		207
E05C7/06	9	a fastening device for one wing being actuated or controlled by closing another wing {(locking one vehicle door by shutting another E05B77/52)}	E05C7/06	E05C7/06		369
E05C9/00	7	Arrangements of simultaneously actuated bolts or other securing devices at well-separated positions on the same wing ({Locking, cross or security bars E05C19/003; locks for safes or the like E05B65/0075; of the vertical-rod type for panic or emergency doors E05B65/1006}; similar constructions for engineering closures F16J13/08)	E05C9/00	E05C9/00		663
E05C9/002	8	{with arrangements allowing the wing to be slam-shut, e.g. by securing elements with latching action (E05B63/20, E05B63/24 take precedence)}	E05C9/00	E05C9/00		116
E05C9/004	8	{Faceplates (for other locks or fasteners E05B9/002); Fixing the faceplates to the wing}	E05C9/00	E05C9/00		363
E05C9/006	8	{Details of bars}	E05C9/00	E05C9/00		228
E05C9/008	8	{mounted in an elongate casing on the surface of the wing}	E05C9/00	E05C9/00		111
E05C9/02	8	with one sliding bar for fastening when moved in one direction and unfastening when moved in opposite direction; with two sliding bars moved in the same direction when fastening or unfastening	E05C9/02	E05C9/02		810
E05C9/021	9	{with rack and pinion mechanism}	E05C9/02	E05C9/02		571
E05C9/023	10	{between a lock cylinder and the bar}	E05C9/02	E05C9/02		147
E05C9/025	9	{with pins engaging slots}	E05C9/02	E05C9/02		211
E05C9/026	9	{comprising key-operated locks, e.g. a lock cylinder to drive auxiliary deadbolts or latch bolts (E05C9/023 takes precedence)}	E05C9/02	E05C9/02		434
E05C9/028	9	{externally mounted on the wing, i.e. surface mounted (E05C9/008 takes precedence)}	E05C9/02	E05C9/02		109
E05C9/04	8	with two sliding bars moved in opposite directions when fastening or unfastening	E05C9/04	E05C9/04		855
E05C9/041	9	{with rack and pinion mechanism}	E05C9/04	E05C9/04		1042
E05C9/042	9	{with pins engaging slots}	E05C9/04	E05C9/04		447
E05C9/043	9	{with crank pins and connecting rods}	E05C9/04	E05C9/04		867
E05C9/045	9	{with inclined surfaces, e.g. spiral or helicoidal}	E05C9/04	E05C9/04		279
E05C9/046	9	{with two interconnected mechanisms each driving one rod}	E05C9/04	E05C9/04		266
E05C9/047	9	{comprising key-operated locks, e.g. a lock cylinder to drive auxiliary deadbolts or latch bolts (E05C9/041 takes precedence)}	E05C9/04	E05C9/04		547
E05C9/048	9	{externally mounted on the wing, i.e. surface mounted (E05C9/008 takes precedence)}	E05C9/04	E05C9/04		274
E05C9/06	8	with three or more sliding bars {(for watertight doors in bulkheads of vessels B63B43/24, B63B43/32; for safe doors E05B65/0075; covers or similar closures for pressure vessels F16J13/00)}	E05C9/06	E05C9/06		559
E05C9/063	9	{extending along three or more sides of the wing or frame (means for transmitting movements between vertical and horizontal bars E05F7/08)}	E05C9/06	E05C9/06		489
E05C9/066	10	{Locks for windows or doors specially adapted for tilt and turn}	E05C9/06	E05C9/06		317
E05C9/08	8	with a rotary bar for actuating the fastening means {(E05B83/10 and E05B65/468 take precedence; for a plurality of drawers E05B65/465)}	E05C9/08	E05C9/08		708
E05C9/085	9	{pivoting about an axis perpendicular to the door (locking bars or the like pivoted about an axis perpendicular to the plane of the wing E05C19/005)}	E05C9/08	E05C9/08		51
E05C9/10	8	Actuating mechanisms for bars {(E05C9/02&#160;-&#160;E05C9/06 take precedence)}	E05C9/10	E05C9/10		541
E05C9/12	9	with rack and pinion mechanism {(E05C9/021, E05C9/041 take precedence)}	E05C9/12	E05C9/12		260
E05C9/14	9	with pins engaging slots {(E05C9/025, E05C9/042 take precedence)}	E05C9/14	E05C9/14		123
E05C9/16	9	with crank pins and connecting rods {(E05C9/043 takes precedence)}	E05C9/16	E05C9/16		255
E05C9/18	8	Details of fastening means or of fixed retaining means for the ends of bars	E05C9/18	E05C9/18		169
E05C9/1808	9	{Keepers}	E05C9/18	E05C9/18		716
E05C2009/1816	10	{snap-mounted without screw fasteners}	E05C9/18	E05C9/18		25
E05C9/1825	9	{Fastening means}	E05C9/18	E05C9/18		76
E05C9/1833	10	{performing sliding movements}	E05C9/18	E05C9/18		97
E05C9/1841	11	{perpendicular to actuating bar}	E05C9/18	E05C9/18		391
E05C9/185	11	{parallel with actuating bar}	E05C9/18	E05C9/18		659
E05C9/1858	12	{of the roller bolt type}	E05C9/18	E05C9/18		239
E05C2009/1866	12	{of the keyhole slot type}	E05C9/18	E05C9/18		40
E05C9/1875	10	{performing pivoting movements (E05C9/08 takes precedence)}	E05C9/18	E05C9/18		489
E05C9/1883	11	{pivotally mounted on the actuation bar}	E05C9/18	E05C9/18		101
E05C9/1891	11	{pivoting around an axis parallel to the bar}	E05C9/18	E05C9/18		43
E05C9/20	8	Coupling means for sliding bars, rods, or cables {(connecting means between actuating rods for vehicle door locks E05B79/14)}	E05C9/20	E05C9/20		577
E05C9/22	8	Guides for sliding bars, rods or cables	E05C9/22	E05C9/22		407
E05C9/24	8	Means for transmitting movements between vertical and horizontal sliding bars, rods or cables {for the fastening of wings}, e.g. corner guides (means for transmitting movements between vertical and horizontal sliding bars, rods or cables, for moving wings into open or closed position E05F7/08)	E05C9/24	E05C9/24		315
E05C17/00	7	Devices for holding wings open; Devices for limiting opening of wings or for holding wings open by a movable member extending between frame and wing; Braking devices, stops or buffers, combined therewith (combined with hinges E05D11/00; combined with operating apparatus for wings E05F; other braking devices, stops, buffers E05F5/00)	E05C17/00	E05C17/00		351
E05C17/003	8	{Power-actuated devices for limiting the opening of vehicle doors}	E05C17/00	E05C17/00		269
E05C17/006	9	{with means for detecting obstacles outside the doors}	E05C17/00	E05C17/00		200
E05C17/02	8	by mechanical means (E05C17/60 takes precedence)	E05C17/02	E05C17/02		644
E05C17/025	9	{Means acting between hinged edge and frame (E05C17/203 takes precedence)}	E05C17/00	E05C17/02		376
E05C17/04	9	with a movable bar or equivalent member extending between frame and wing	E05C17/04	E05C17/04		588
E05C17/042	10	{for anchoring the trunk lid of a car while carrying oversize objects (E05C17/36 takes precedence)}	E05C17/04	E05C17/04		184
E05C17/045	10	{Hinges for the movable bar (E05C17/163, E05C17/26, E05C17/345 take precedence; hinges in general F16C11/04, E05D)}	E05C17/04	E05C17/04		213
E05C17/047	10	{Portable bars or the like, i.e. completely removable (E05C17/042 takes precedence)}	E05C17/04	E05C17/04		157
E05C17/08	10	with special means for release, e.g. automatic release by further opening	E05C17/08	E05C17/08		100
E05C17/085	11	{automatic release by further opening}	E05C17/08	E05C17/08		297
E05C17/12	10	consisting of a single rod	E05C17/12	E05C17/12		463
E05C17/14	11	Hook and eye, or equivalent	E05C17/14	E05C17/14		294
E05C17/16	11	pivoted only at one end and having an elongated slot	E05C17/16	E05C17/16		241
E05C17/163	12	{with clamping or securing means at the pivot, e.g. friction hinge}	E05C17/16	E05C17/16		43
E05C17/166	12	{Security devices}	E05C17/16	E05C17/16		427
E05C17/18	11	pivoted only at one end having a row of holes, notches, or pins	E05C17/18	E05C17/18		596
E05C17/20	11	sliding through a guide (E05C17/18 takes precedence)	E05C17/20	E05C17/20		341
E05C17/203	12	{concealed, e.g. for vehicles}	E05C17/20	E05C17/20		928
E05C17/206	13	{with elastomeric springs to hold wing open}	E05C17/20	E05C17/20		182
E05C17/22	12	with braking, clamping or securing means in the guide {(E05C17/203 takes precedence)}	E05C17/22	E05C17/22		589
E05C17/24	11	pivoted at one end, and with the other end running along a guide member	E05C17/24	E05C17/24		350
E05C17/26	12	with braking, clamping or securing means at the pivot of the rod	E05C17/26	E05C17/26		78
E05C17/28	12	with braking, clamping or securing means at the connection to the guide member	E05C17/28	E05C17/28		759
E05C17/30	10	of extensible, e.g. telescopic, construction (flexible members E05C17/36{; locking of telescopic systems in general F16B7/10; lockable telescopic gas springs F16F9/0254})	E05C17/30	E05C17/30		953
E05C17/305	11	{with hydraulic locks}	E05C17/30	E05C17/30		137
E05C17/32	10	consisting of two or more pivoted rods	E05C17/32	E05C17/32		933
E05C17/34	11	with means for holding in more than one position	E05C17/34	E05C17/34		185
E05C17/345	12	{using friction, e.g. friction hinge}	E05C17/34	E05C17/34		105
E05C17/36	10	comprising a flexible member, e.g. chains	E05C17/36	E05C17/36		374
E05C17/365	11	{Security chains}	E05C17/36	E05C17/36		376
E05C17/38	9	with a curved rail rigid with the frame for engagement with means on the wing, or vice versa	E05C17/38	E05C17/38		329
E05C17/40	9	Bars or like parts connecting a right wing with a left wing which move against each other when being closed	E05C17/40	E05C17/40		96
E05C17/42	9	connecting exterior and interior wings	E05C17/42	E05C17/42		28
E05C17/44	9	with a device carried on the wing for frictional or like engagement with a fixed flat surface, e.g. {for holding wings open or closed by} retractable feet {(with wedging action between the wing and a flat surface E05C17/54)}	E05C17/44	E05C17/44		405
E05C17/443	10	{of the pivoted lever or eccentric type, e.g. for sliding windows}	E05C17/44	E05C17/44		463
E05C17/446	10	{of the retractable sliding feet type (similar devices for sliding wings E05C17/64)}	E05C17/44	E05C17/44		382
E05C17/46	9	in which the wing or a member fixed thereon is engaged by a movable fastening member in a fixed position; in which a movable fastening member mounted on the wing engages a stationary member	E05C17/46	E05C17/46		429
E05C17/48	10	comprising a sliding securing member	E05C17/48	E05C17/48		377
E05C17/50	10	comprising a single pivoted securing member	E05C17/50	E05C17/50		720
E05C17/505	11	{acting directly on the knob or handle}	E05C17/50	E05C17/50		41
E05C17/52	10	comprising a snap, catch, or the like	E05C17/52	E05C17/52		376
E05C17/525	11	{comprising a suction cup}	E05C17/52	E05C17/52		47
E05C17/54	9	Portable devices, e.g. wedges; wedges for holding wings open or closed (E05C17/047 takes precedence)	E05C17/54	E05C17/54		897
E05C17/56	8	by magnetic or electromagnetic attraction {or operated by electric or electromagnetic means (for closed wings E05C19/16)}; (operation of locks or fasteners by electric or magnetic means E05B47/00)	E05C17/56	E05C17/56		858
E05C17/58	8	operated or controlled from a distance {, e.g. pneumatically (E05C17/56 takes precedence)}	E05C17/58	E05C17/58		54
E05C17/60	8	holding sliding wings open {(E05C17/443, E05C17/54 take precedence)}	E05C17/60	E05C17/60		650
E05C17/62	9	using notches	E05C17/62	E05C17/62		159
E05C17/64	9	by friction	E05C17/64	E05C17/64		161
E05C19/00	7	Other devices specially designed for securing wings, {e.g. with suction cups}(movable draft sealings additionally used for bolting E06B7/18)	E05C19/00	E05C19/00		963
E05C19/001	8	{with bolts extending over a considerable extent, e.g. nearly along the whole length of at least one side of the wing (movable sealing strips E06B7/18)}	E05C19/00	E05C19/00		328
E05C19/002	9	{Rotating about a longitudinal axis}	E05C19/00	E05C19/00		185
E05C19/003	8	{Locking bars, cross bars, security bars (for sliding wings E05B65/0888; for a plurality of drawers E05B65/467)}	E05C19/00	E05C19/00		813
E05C19/004	9	{at an angle between door and floor or wall}	E05C19/00	E05C19/00		296
E05C19/005	9	{pivoted about an axis on the wing, perpendicular to the plane of the wing}	E05C19/00	E05C19/00		86
E05C19/006	8	{by displacement of the wing substantially in its own plane (E05F7/02 takes precedence)}	E05C19/00	E05C19/00		192
E05C19/007	8	{Latches with wedging action (wedges between wing itself and fixed surface E05C17/54)}	E05C19/00	E05C19/00		139
E05C19/008	9	{Tilt-plate latches}	E05C19/00	E05C19/00		43
E05C19/009	8	{Latches with floating bolts, e.g. rings, balls}	E05C19/00	E05C19/00		106
E05C19/02	8	Automatic catches, i.e. released by pull or pressure on the wing (E05C19/06 takes precedence {; with locking means E05B63/22})	E05C19/02	E05C19/02		644
E05C19/022	9	{Released by pushing in the closing direction}	E05C19/02	E05C19/02		705
E05C19/024	9	{with a bifurcated latch}	E05C19/02	E05C19/02		261
E05C19/026	9	{with a keeper caught between two pivoting bolts}	E05C19/02	E05C19/02		68
E05C19/028	9	{with sliding bolt(s)}	E05C19/02	E05C19/02		243
E05C19/04	9	Ball or roller catches	E05C19/04	E05C19/04		305
E05C19/06	8	in which the securing part if formed or carried by a spring and moves only by distortion of the spring, e.g. snaps	E05C19/06	E05C19/06		1498
E05C19/063	9	{Released by pull or pressure on the wing (E05C19/022 takes precedence)}	E05C19/06	E05C19/06		440
E05C19/066	10	{made of plastics, e.g. hook-and-loop type fastener}	E05C19/06	E05C19/06		190
E05C19/08	8	Hasps; Hasp fastenings; Spring catches therefor	E05C19/08	E05C19/08		796
E05C19/10	8	Hook fastenings; Fastenings in which a link engages a fixed hook-like member	E05C19/10	E05C19/10		728
E05C19/105	9	{Butterfly latches}	E05C19/10	E05C19/10		91
E05C19/12	9	pivotally mounted {around an axis (E05C3/045, E05C3/40 take precedence)}	E05C19/12	E05C19/12		281
E05C19/14	10	with toggle action	E05C19/14	E05C19/14		847
E05C19/145	11	{flush}	E05C19/14	E05C19/14		279
E05C19/16	8	Devices holding the wing by magnetic or electromagnetic attraction {(E05C17/56 takes precedence)}	E05C19/16	E05C19/16		1395
E05C19/161	9	{magnetic gaskets}	E05C19/16	E05C19/16		445
E05C19/163	9	{a movable bolt being held in the striker by a permanent magnet}	E05C19/16	E05C19/16		259
E05C19/165	9	{released by pushing in the closing direction}	E05C19/16	E05C19/16		61
E05C19/166	9	{electromagnetic}	E05C19/16	E05C19/16		745
E05C19/168	10	{a movable bolt being electromagnetically held in the striker by electromagnetic attraction}	E05C19/16	E05C19/16		86
E05C19/18	8	Portable devices specially adapted for securing wings ({E05C17/54, E05C19/003, E05B65/0894, E05B67/00 take precedence}; preventing operation of handles E05B13/00)	E05C19/18	E05C19/18		520
E05C19/182	9	{insertable in the gap between the wing and the frame or in the gap between a lock and its striker, e.g. for cooperation with the striker}	E05C19/18	E05C19/18		658
E05C19/184	9	{a portable member cooperating with a fixed member or an opening on the wing or the frame, for locking the wing}	E05C19/18	E05C19/18		339
E05C19/186	9	{with a pair of hooks, which are movable towards each other for grasping of an element on the wing, respectively on the frame, or for grasping of an element on each of the wings forming a double door}	E05C19/18	E05C19/18		140
E05C19/188	9	{Removably mounted securing devices, e.g. devices clamped to the wing or the frame (E05C19/182&#160;-&#160;E05C19/186 take precedence)}	E05C19/18	E05C19/18		178
E05C21/00	7	Arrangements or combinations of wing fastening, securing, or holding devices, not covered by a single preceding main group; {Locking kits}	E05C21/00	E05C21/00		225
E05C21/005	8	{Provisional arrangements between door and frame for holding vehicle doors closed or partially open during manufacturing or maintenance}	E05C21/00	E05C21/00		171
