D03C1/00	7	Dobbies	D03C1/00	D03C1/00		309
D03C1/005	8	{Electronic dobbies}	D03C1/00	D03C1/00		18
D03C1/02	8	Single-lift dobbies, i.e. dobbies in which the same draw-knife or equivalent operates for every pick (D03C1/10 takes precedence)	D03C1/02	D03C1/02		47
D03C1/04	9	Open-shed single-lift dobbies	D03C1/04	D03C1/04		110
D03C1/06	8	Double-lift dobbies, i.e. dobbies in which separate draw-knives or equivalent operate on alternate picks	D03C1/06	D03C1/06		323
D03C1/08	9	reversible, i.e. correct sheds open automatically when the loom is driven backwards	D03C1/08	D03C1/08		15
D03C1/10	8	Centre-shed dobbies, i.e. shed formed by lifting some threads and lowering the others from central shed-closed position	D03C1/10	D03C1/10		26
D03C1/12	8	Dobbies employing toothed gearing instead of draw-knives	D03C1/12	D03C1/12		145
D03C1/14	8	Features common to dobbies of different types (stop motions acting on defective operation of shedding mechanisms D03D51/46)	D03C1/14	D03C1/14		279
D03C1/142	9	{Leveling mechanisms}	D03C1/14	D03C1/14		41
D03C1/144	9	{linking to the heald frame}	D03C1/14	D03C1/14		347
D03C1/146	9	{Independent drive motor}	D03C1/14	D03C1/14		64
D03C1/148	9	{Eccentrics}	D03C1/14	D03C1/14		35
D03C1/16	9	Arrangements of dobby in relation to loom	D03C1/16	D03C1/16		151
D03C1/18	9	Knives; Knife frames	D03C1/18	D03C1/18		35
D03C1/20	9	Hooks; Lifters	D03C1/20	D03C1/20		19
D03C1/22	9	Needles; Needle boxes; Needle boards	D03C1/22	D03C1/22		267
D03C1/24	9	Cylinders; Cylinder battens	D03C1/24	D03C1/24		3
D03C1/26	9	Facilitating engagement of lifting-hooks with draw-knives	D03C1/26	D03C1/26		72
D03C1/28	10	by creating and then eliminating back-lash between hooks and knives	D03C1/28	D03C1/28		1
D03C1/30	10	wherein all the hooks are disengaged from the knives, and selected hooks then re-engaged	D03C1/30	D03C1/30		1
D03C1/32	10	wherein all the hooks are engaged with the knives, and unselected hooks then disengaged	D03C1/32	D03C1/32		
D03C1/34	9	Arrangements wherein warp threads pass one another at different heights to avoid congestion	D03C1/34	D03C1/34		30
D03C1/36	9	Card- or chain-saving arrangements, e.g. cross-border dobbies	D03C1/36	D03C1/36		198
D03C3/00	7	Jacquards (controlling jacquard by scanning design D03C17/06; for gripper Axminster looms D03D39/08)	D03C3/00	D03C3/00		142
D03C3/02	8	Single-lift jacquards	D03C3/02	D03C3/02		52
D03C3/04	9	of open-shed type	D03C3/04	D03C3/04		1
D03C3/06	8	Double-lift jacquards	D03C3/06	D03C3/06		108
D03C3/08	9	of open-shed type	D03C3/08	D03C3/08		29
D03C3/10	8	Centre-shed jacquards	D03C3/10	D03C3/10		5
D03C3/12	8	Multiple-shed jacquards, i.e. jacquards which move warp threads to several different heights, e.g. for weaving pile fabrics	D03C3/12	D03C3/12		97
D03C3/14	8	Jacquards not employing lifting-hooks, e.g. employing knotted cords in conjunction with keyhole slots	D03C3/14	D03C3/14		
D03C3/16	8	Verdol or other jacquards having intermediate power-operated needles between reading needles and lifting-hooks	D03C3/16	D03C3/16		59
D03C3/18	8	Selvedge jacquards	D03C3/18	D03C3/18		12
D03C3/20	8	Electrically-operated jacquards	D03C3/20	D03C3/20		564
D03C3/205	9	{Independently actuated lifting cords}	D03C3/20	D03C3/20		50
D03C3/22	8	Fluid-operated jacquards	D03C3/22	D03C3/22		32
D03C3/24	8	Features common to jacquards of different types	D03C3/24	D03C3/24		942
D03C3/26	9	General arrangements of jacquards, or disposition in relation to loom	D03C3/26	D03C3/26		120
D03C3/28	9	Pick-finding arrangements; Arrangements for preventing next shed from being opened during stopping of loom	D03C3/28	D03C3/28		23
D03C3/30	9	Arrangements wherein hooks are positively operated to close shed	D03C3/30	D03C3/30		2
D03C3/32	9	Jacquard driving mechanisms	D03C3/32	D03C3/32		131
D03C3/34	10	Cylinder operating mechanisms	D03C3/34	D03C3/34		25
D03C3/36	10	Griffe operating mechanisms	D03C3/36	D03C3/36		121
D03C3/38	9	Comber boards	D03C3/38	D03C3/38		72
D03C3/40	9	Constructions of lifting-cords	D03C3/40	D03C3/40		240
D03C3/42	9	Arrangements of lifting-cords	D03C3/42	D03C3/42		71
D03C3/44	9	Lingoes	D03C3/44	D03C3/44		34
D03C5/00	7	Cam or other direct-acting shedding mechanisms, i.e. operating heald frames without intervening power-supplying devices	D03C5/00	D03C5/00		356
D03C5/005	8	{Leveling mechanisms}	D03C5/00	D03C5/00		54
D03C5/02	8	operated by rotating cams	D03C5/02	D03C5/02		444
D03C5/04	9	Construction or shape of cams (cams in general F16H53/00)	D03C5/04	D03C5/04		24
D03C5/06	8	operated by cam devices other than rotating cams	D03C5/06	D03C5/06		44
D03C7/00	7	Leno or similar shedding mechanisms	D03C7/00	D03C7/00		389
D03C7/005	8	{Combined leno and patterned shedding motion}	D03C7/00	D03C7/00		21
D03C7/02	8	Gauze healds	D03C7/02	D03C7/02		116
D03C7/04	8	Mechanisms having discs oscillating about a weftwise axis and having apertures for warp threads	D03C7/04	D03C7/04		66
D03C7/06	8	Mechanisms having eyed needles for moving warp threads from side to side of other warp threads	D03C7/06	D03C7/06		176
D03C7/08	8	Devices for twisting warp threads repeatedly in the same direction	D03C7/08	D03C7/08		96
D03C9/00	7	Healds; Heald frames (for leno shedding D03C7/00)	D03C9/00	D03C9/00		81
D03C9/02	8	Healds	D03C9/02	D03C9/02		578
D03C9/022	9	{anti-buckling}	D03C9/02	D03C9/02		7
D03C9/024	9	{Eyelets}	D03C9/02	D03C9/02		287
D03C9/026	9	{Material used}	D03C9/02	D03C9/02		39
D03C9/04	9	Metal healds	D03C9/04	D03C9/04		40
D03C9/06	8	Heald frames	D03C9/06	D03C9/06		180
D03C9/0608	9	{Construction of frame parts}	D03C9/06	D03C9/06		106
D03C9/0616	10	{Horizontal upper or lower rods}	D03C9/06	D03C9/06		17
D03C9/0625	11	{Composition or used material}	D03C9/06	D03C9/06		162
D03C9/0633	11	{Heald bars or their connection to other frame parts}	D03C9/06	D03C9/06		552
D03C9/0641	11	{Distance guides for keeping distance to the next frame}	D03C9/06	D03C9/06		39
D03C9/065	10	{Side stays}	D03C9/06	D03C9/06		95
D03C9/0658	10	{Intermediate supports or their connection to other frame parts}	D03C9/06	D03C9/06		116
D03C9/0666	9	{Connection of frame parts (D03C9/0633 and D03C9/0658 take precedence)}	D03C9/06	D03C9/06		61
D03C9/0675	10	{Corner connections between horizontal rods and side stays}	D03C9/06	D03C9/06		298
D03C9/0683	9	{Arrangements or means for the linking to the drive system}	D03C9/06	D03C9/06		421
D03C9/0691	9	{Arrangements of means for damping or noise reduction}	D03C9/06	D03C9/06		94
D03C11/00	7	Selvedge shedding mechanisms not forming part of main shedding mechanism (selvedge jacquards D03C3/18; leno selvedge mechanism D03C7/00)	D03C11/00	D03C11/00		51
D03C13/00	7	Shedding mechanisms not otherwise provided for	D03C13/00	D03C13/00		440
D03C13/02	8	{with independent drive motors (D03C1/146 and D03C3/205 take precedence)}	D03C13/00	D03C13/02		31
D03C13/025	9	{with independent frame drives}	D03C13/00	D03C13/02		138
D03C15/00	7	Pattern cards or chains	D03C15/00	D03C15/00		72
D03C15/02	8	Chains of metal, wood, or similar material with projecting pattern-indicating elements	D03C15/02	D03C15/02		38
D03C15/04	8	Cards or paper perforated to indicate pattern	D03C15/04	D03C15/04		38
D03C15/06	8	Apparatus for setting pegs in, or removing pegs from, pattern cards	D03C15/06	D03C15/06		3
D03C15/08	8	Apparatus for interconnecting, e.g. by lacing, or disconnecting pattern cards	D03C15/08	D03C15/08		27
D03C17/00	7	Card-punching apparatus (marking record carriers in digital fashion G06K)	D03C17/00	D03C17/00		297
D03C17/02	8	manually-controlled, i.e. holes to be punched determined by the operator	D03C17/02	D03C17/02		1
D03C17/04	9	power-operated	D03C17/04	D03C17/04		5
D03C17/06	8	automatic, i.e. design scanned optically or otherwise to control punching apparatus or to control loom jacquard directly	D03C17/06	D03C17/06		25
D03C19/00	7	Methods or devices concerned with designing or making patterns, not provided for in other groups of this subclass	D03C19/00	D03C19/00		255
D03C19/005	8	{Electronic}	D03C19/00	D03C19/00		215
D03C2700/00	7	Shedding mechanisms	CPCONLY	D03C2700/00		1
D03C2700/01	8	Shedding mechanisms using heald frames	CPCONLY	D03C2700/01		14
D03C2700/0105	9	Cam-driven heald frame movement	CPCONLY	D03C2700/0105		126
D03C2700/0111	10	Devices for levelling the heald frames; Coupling and uncoupling the drive for the heald frames; Devices for holding the shed open	CPCONLY	D03C2700/0111		36
D03C2700/0116	10	Arrangements in which warp threads pass one another at different heights	CPCONLY	D03C2700/0116		40
D03C2700/0122	10	Devices for adjusting the geometric and time parameters of shed opening	CPCONLY	D03C2700/0122		38
D03C2700/0127	9	Program-controlled heald frame movement	CPCONLY	D03C2700/0127		11
D03C2700/0133	10	with mechanical transmission	CPCONLY	D03C2700/0133		36
D03C2700/0138	11	using hooks or lifters	CPCONLY	D03C2700/0138		4
D03C2700/0144	12	Single-lift mechanisms	CPCONLY	D03C2700/0144		
D03C2700/015	13	of closed-shed type	CPCONLY	D03C2700/015		42
D03C2700/0155	12	Double-lift mechanisms	CPCONLY	D03C2700/0155		12
D03C2700/0161	13	of negatively-driven type	CPCONLY	D03C2700/0161		54
D03C2700/0166	13	of positively-driven type	CPCONLY	D03C2700/0166		58
D03C2700/0172	13	Constructional details	CPCONLY	D03C2700/0172		63
D03C2700/0177	10	Devices for levelling the heald frames; Coupling and uncoupling the drive for the heald frames; Devices for holding the shed open	CPCONLY	D03C2700/0177		114
D03C2700/0183	10	Devices for adjusting the geometric and time parameters of shed opening	CPCONLY	D03C2700/0183		36
D03C2700/0188	9	Heald frame return devices	CPCONLY	D03C2700/0188		57
D03C2700/0194	9	Frame-operating devices for ribbon looms	CPCONLY	D03C2700/0194		52
D03C2700/14	9	Heald frame lifting devices	CPCONLY	D03C2700/14		238
