F16C1/00	7	Flexible shafts (flexible shafts in dental machines for boring or cutting A61C1/18); Mechanical means for transmitting movement in a flexible sheathing	F16C1/00	F16C1/00		166
F16C1/02	8	for conveying rotary movements	F16C1/02	F16C1/02		439
F16C1/04	9	Articulated shafts	F16C1/04	F16C1/04		315
F16C1/06	9	with guiding sheathing, tube or box (F16C1/04 takes precedence; guiding sheathings F16C1/26)	F16C1/06	F16C1/06		498
F16C1/08	9	End connections	F16C1/08	F16C1/08		410
F16C1/10	8	Means for transmitting linear movement in a flexible sheathing, e.g. "Bowden-mechanisms" (guiding-sheathings F16C1/26)	F16C1/10	F16C1/10		853
F16C1/101	9	{Intermediate connectors for joining portions of split flexible shafts and/or sheathings}	F16C1/10	F16C1/10		463
F16C1/102	9	{Arrangements to mount end fittings of the sheathings to support walls or brackets}	F16C1/10	F16C1/10		112
F16C1/103	10	{to a hole in the wall or bracket}	F16C1/10	F16C1/10		138
F16C1/105	10	{to a slot in the bracket}	F16C1/10	F16C1/10		284
F16C1/106	9	{Plurality of transmitting means, e.g. two or more parallel "Bowden cables"}	F16C1/10	F16C1/10		198
F16C1/107	9	{Sealing details}	F16C1/10	F16C1/10		201
F16C1/108	9	{Reducing or controlling of vibrations, e.g. by resilient damping of noise}	F16C1/10	F16C1/10		275
F16C1/12	9	Arrangements for transmitting movement to or from the flexible member	F16C1/12	F16C1/12		608
F16C1/14	10	Construction of the end-piece of the flexible member; Attachment thereof to the flexible member	F16C1/14	F16C1/14		829
F16C1/145	11	{Attachment of the end-piece to the flexible member}	F16C1/14	F16C1/14		177
F16C1/16	10	in which the end-piece is guided rectilinearly	F16C1/16	F16C1/16		469
F16C1/18	10	in which the end portion of the flexible member is laid along a curved surface of a pivoted member	F16C1/18	F16C1/18		350
F16C1/20	9	Construction of flexible members moved to and fro in the sheathing	F16C1/20	F16C1/20		580
F16C1/205	10	{Details of the outer surface of the flexible member, e.g. coatings}	F16C1/20	F16C1/20		104
F16C1/22	9	Adjusting; Compensating length	F16C1/22	F16C1/22		452
F16C1/223	10	{by adjusting the effective length of the flexible member}	F16C1/22	F16C1/22		307
F16C1/226	10	{by adjusting the effective length of the sheathing}	F16C1/22	F16C1/22		395
F16C1/24	8	Lubrication; Lubricating equipment	F16C1/24	F16C1/24		196
F16C1/26	8	Construction of guiding-sheathings or guiding-tubes	F16C1/26	F16C1/26		780
F16C1/262	9	{End fittings; Attachment thereof to the sheathing or tube}	F16C1/26	F16C1/26		927
F16C1/265	10	{with a swivel tube connected to the end-fitting of a sheathing, e.g. with a spherical joint}	F16C1/26	F16C1/26		212
F16C1/267	9	{Details of the inner surface of the sheathing or tube, e.g. coatings}	F16C1/26	F16C1/26		109
F16C1/28	9	with built in bearings {, e.g. sheathing with rolling elements between the sheathing and the core element}	F16C1/28	F16C1/28		237
F16C3/00	7	Shafts (flexible shafts F16C1/00; marine propeller shafts, paddle wheel shafts B63H23/34); Axles; Cranks; Eccentrics	F16C3/00	F16C3/00		113
F16C3/02	8	Shafts; Axles	F16C3/02	F16C3/02		2941
F16C3/023	9	{made of several parts, e.g. by welding}	F16C3/02	F16C3/02		944
F16C3/026	9	{Shafts made of fibre reinforced resin}	F16C3/02	F16C3/02		703
F16C3/03	9	telescopic (axially displaceable couplings F16D3/06)	F16C3/03	F16C3/03		662
F16C3/035	10	with built-in bearings	F16C3/035	F16C3/035		456
F16C3/04	8	Crankshafts, eccentric-shafts; Cranks, eccentrics	F16C3/04	F16C3/04		86
F16C3/06	9	Crankshafts	F16C3/06	F16C3/06		875
F16C3/08	10	made in one piece (features relating to lubrication F16C3/14, to cooling F16C3/16)	F16C3/08	F16C3/08		492
F16C3/10	10	assembled of several parts, e.g. by welding {by crimping}	F16C3/10	F16C3/10		577
F16C3/12	11	releasably connected	F16C3/12	F16C3/12		504
F16C3/14	10	Features relating to lubrication	F16C3/14	F16C3/14		945
F16C3/16	10	Features relating to cooling	F16C3/16	F16C3/16		58
F16C3/18	9	Eccentric-shafts	F16C3/18	F16C3/18		226
F16C3/20	9	Shape of crankshafts or eccentric-shafts having regard to balancing	F16C3/20	F16C3/20		585
F16C3/22	9	Cranks; Eccentrics (constructional features of crank-pins F16C11/02)	F16C3/22	F16C3/22		291
F16C3/24	10	with return cranks, i.e. a second crank carried by the crank-pin	F16C3/24	F16C3/24		7
F16C3/26	10	Elastic crank-webs; Resiliently-mounted crank-pins	F16C3/26	F16C3/26		27
F16C3/28	10	Adjustable cranks or eccentrics	F16C3/28	F16C3/28		799
F16C3/30	10	with arrangements for overcoming dead-centres	F16C3/30	F16C3/30		24
F16C5/00	7	Crossheads; Constructions of connecting-rod heads or piston-rod connections rigid with crossheads (piston-rods, i.e. rods rigidly connected to the piston, F16J7/00)	F16C5/00	F16C5/00		578
F16C7/00	7	Connecting-rods or like links pivoted at both ends (coupling-rods for locomotive driving-wheels B61C17/10); Construction of connecting-rod heads (heads rigid with crossheads F16C5/00)	F16C7/00	F16C7/00		261
F16C7/02	8	Constructions of connecting-rods with constant length	F16C7/02	F16C7/02		670
F16C7/023	9	{for piston engines, pumps or the like}	F16C7/02	F16C7/02		1379
F16C7/026	9	{made of fibre reinforced resin}	F16C7/02	F16C7/02		564
F16C7/04	8	with elastic intermediate part of fluid cushion	F16C7/04	F16C7/04		451
F16C7/06	8	Adjustable connecting-rods	F16C7/06	F16C7/06		1061
F16C7/08	8	made from sheet metal	F16C7/08	F16C7/08		195
F16C9/00	7	Bearings for crankshafts or connecting-rods; Attachment of connecting-rods (lubrication of connecting-rods in connection with crankshafts F16C3/14; connections to crossheads F16C5/00; to pistons F16J1/14)	F16C9/00	F16C9/00		317
F16C9/02	8	Crankshaft bearings	F16C9/02	F16C9/02		1818
F16C9/03	9	Arrangements for adjusting play	F16C9/03	F16C9/03		79
F16C9/04	8	Connecting-rod bearings; Attachments thereof	F16C9/04	F16C9/04		2146
F16C9/045	9	{the bearing cap of the connecting rod being split by fracturing}	F16C9/04	F16C9/04		331
F16C9/06	9	Arrangements for adjusting play in bearings, operating either automatically or not	F16C9/06	F16C9/06		226
F16C11/00	7	Pivots; Pivotal connections (arrangements of steering linkage connections B62D7/16)	F16C11/00	F16C11/00		236
F16C11/02	8	Trunnions; Crank-pins (fastening crank-pins to webs, crank-pins integral with cranks F16C3/06, F16C3/22)	F16C11/02	F16C11/02		606
F16C11/04	8	Pivotal connections (hinges for doors, windows or wings E05D)	F16C11/04	F16C11/04		5995
F16C11/045	9	{with at least a pair of arms pivoting relatively to at least one other arm, all arms being mounted on one pin (crank-pins F16C11/02)}	F16C11/04	F16C11/04		2623
F16C11/06	9	Ball-joints; Other joints having more than one degree of angular freedom, i.e. universal joints (universal joints in which flexibility is produced by means of pivots or sliding or rolling connecting parts F16D3/16)	F16C11/06	F16C11/06		2260
F16C11/0604	10	{Construction of the male part}	F16C11/06	F16C11/06		1186
F16C11/0609	11	{made from two or more parts}	F16C11/06	F16C11/06		617
F16C11/0614	10	{the female part of the joint being open on two sides}	F16C11/06	F16C11/06		1596
F16C11/0619	10	{the female part comprising a blind socket receiving the male part}	F16C11/06	F16C11/06		824
F16C11/0623	11	{Construction or details of the socket member}	F16C11/06	F16C11/06		745
F16C11/0628	12	{with linings}	F16C11/06	F16C11/06		504
F16C11/0633	13	{the linings being made of plastics}	F16C11/06	F16C11/06		629
F16C11/0638	14	{characterised by geometrical details}	F16C11/06	F16C11/06		521
F16C11/0642	12	{Special features of the plug or cover on the blind end of the socket}	F16C11/06	F16C11/06		363
F16C11/0647	12	{Special features relating to adjustment for wear or play; Wear indicators}	F16C11/06	F16C11/06		471
F16C11/0652	12	{combined with a damper other than elastic linings}	F16C11/06	F16C11/06		198
F16C11/0657	12	{the socket member being mainly made of plastics}	F16C11/06	F16C11/06		420
F16C11/0661	10	{the two co-operative parts each having both convex and concave interfaces}	F16C11/06	F16C11/06		307
F16C11/0666	10	{Sealing means between the socket and the inner member shaft}	F16C11/06	F16C11/06		337
F16C11/0671	11	{allowing operative relative movement of joint parts due to flexing of the sealing means}	F16C11/06	F16C11/06		1008
F16C11/0676	11	{allowing operational relative movement of joint parts due to sliding between parts of the sealing means}	F16C11/06	F16C11/06		239
F16C11/068	10	{Special features relating to lubrication}	F16C11/06	F16C11/06		472
F16C11/0685	10	{Manufacture of ball-joints and parts thereof, e.g. assembly of ball-joints}	F16C11/06	F16C11/06		982
F16C11/069	11	{with at least one separate part to retain the ball member in the socket; Quick-release systems}	F16C11/06	F16C11/06		694
F16C11/0695	10	{Mounting of ball-joints, e.g. fixing them to a connecting rod}	F16C11/06	F16C11/06		829
F16C11/08	10	with resilient bearings	F16C11/08	F16C11/08		165
F16C11/083	11	{by means of parts of rubber or like materials}	F16C11/08	F16C11/08		206
F16C11/086	12	{with an elastomeric member in the blind end of a socket}	F16C11/08	F16C11/08		93
F16C11/10	9	Arrangements for locking	F16C11/10	F16C11/10		2385
F16C11/103	10	{frictionally clamped}	F16C11/10	F16C11/10		725
F16C11/106	11	{for ball joints}	F16C11/10	F16C11/10		620
F16C11/12	9	incorporating flexible connections, e.g. leaf springs	F16C11/12	F16C11/12		1464
F16C13/00	7	Rolls, drums, discs, or the like (guide rollers in feeding webs B65H27/00; calender rolls, bearings therefor D21G1/02; rotary drums or rollers for heat-exchange or heat-transfer apparatus F28F5/02); Bearings or mountings therefor	F16C13/00	F16C13/00		2454
F16C13/003	8	{Bowed or curved rolls (rollers with a bowed axis as tentering devices for tensioning, smoothing or guiding webs B65H23/0258)}	F16C13/00	F16C13/00		127
F16C13/006	8	{Guiding rollers, wheels or the like, formed by or on the outer element of a single bearing or bearing unit, e.g. two adjacent bearings, whose ratio of length to diameter is generally less than one}	F16C13/00	F16C13/00		2164
F16C13/02	8	Bearings	F16C13/02	F16C13/02		1991
F16C13/022	9	{supporting a hollow roll mantle rotating with respect to a yoke or axle}	F16C13/02	F16C13/02		455
F16C13/024	10	{adjustable for positioning, e.g. radial movable bearings for controlling the deflection along the length of the roll mantle}	F16C13/02	F16C13/02		262
F16C13/026	11	{by fluid pressure}	F16C13/02	F16C13/02		266
F16C13/028	12	{with a plurality of supports along the length of the roll mantle, e.g. hydraulic jacks}	F16C13/02	F16C13/02		542
F16C13/04	9	Bearings with only partial enclosure of the member to be borne; Bearings with local support at two or more points	F16C13/04	F16C13/04		749
F16C13/06	9	self-adjusting	F16C13/06	F16C13/06		70
F16C15/00	7	Construction of rotary bodies to resist centrifugal force (flywheels, correction weights F16F15/30, F16F15/32)	F16C15/00	F16C15/00		169
F16C17/00	7	Sliding-contact bearings for exclusively rotary movement (F16C32/06 takes precedence; adjustable bearings F16C23/00, F16C25/00)	F16C17/00	F16C17/00		401
F16C17/02	8	for radial load only	F16C17/02	F16C17/02		3488
F16C17/022	9	{with a pair of essentially semicircular bearing sleeves}	F16C17/02	F16C17/02		608
F16C17/024	9	{with flexible leaves to create hydrodynamic wedge, e.g. radial foil bearings}	F16C17/02	F16C17/02		968
F16C17/026	9	{with helical grooves in the bearing surface to generate hydrodynamic pressure, e.g. herringbone grooves}	F16C17/02	F16C17/02		959
F16C17/028	9	{with fixed wedges to generate hydrodynamic pressure, e.g. multi-lobe bearings}	F16C17/02	F16C17/02		356
F16C17/03	9	with tiltably-supported segments, e.g. Michell bearings {(hydrostatic bearings with tiltably supported bearing pads F16C32/0666; made from a plurality of rods F16C33/26; with flexible leaves F16C17/024; hydrodynamic bearings with chambers F16C33/1075)}	F16C17/03	F16C17/03		1032
F16C17/035	10	{the segments being integrally formed with, or rigidly fixed to, a support-element}	F16C17/03	F16C17/03		162
F16C17/04	8	for axial load only	F16C17/04	F16C17/04		2214
F16C17/042	9	{with flexible leaves to create hydrodynamic wedge, e.g. axial foil bearings}	F16C17/04	F16C17/04		489
F16C17/045	9	{with grooves in the bearing surface to generate hydrodynamic pressure, e.g. spiral groove thrust bearings}	F16C17/04	F16C17/04		687
F16C17/047	9	{with fixed wedges to generate hydrodynamic pressure}	F16C17/04	F16C17/04		417
F16C17/06	9	with tiltably-supported segments, e.g. Michell bearings {(with flexible leaves F16C17/042; hydrostatic F16C32/0666)}	F16C17/06	F16C17/06		967
F16C17/065	10	{the segments being integrally formed with, or rigidly fixed to, a support-element}	F16C17/06	F16C17/06		145
F16C17/08	9	for supporting the end face of a shaft or other member, e.g. footstep bearings	F16C17/08	F16C17/08		1443
F16C17/10	8	for both radial and axial load	F16C17/10	F16C17/10		2411
F16C17/102	9	{with grooves in the bearing surface to generate hydrodynamic pressure}	F16C17/10	F16C17/10		218
F16C17/105	10	{with at least one bearing surface providing angular contact, e.g. conical or spherical bearing surfaces}	F16C17/10	F16C17/10		413
F16C17/107	10	{with at least one surface for radial load and at least one surface for axial load}	F16C17/10	F16C17/10		1476
F16C17/12	8	characterised by features not related to the direction of the load	F16C17/12	F16C17/12		228
F16C17/14	9	specially adapted for operating in water	F16C17/14	F16C17/14		277
F16C17/18	9	with floating brasses or brushing, rotatable at a reduced speed {(F16C17/03, F16C17/06 take precedence)}	F16C17/18	F16C17/18		908
F16C17/20	9	with emergency supports or bearings	F16C17/20	F16C17/20		172
F16C17/22	9	with arrangements compensating for thermal expansion	F16C17/22	F16C17/22		267
F16C17/24	9	with devices affected by abnormal or undesired positions, e.g. for preventing overheating, for safety	F16C17/24	F16C17/24		722
F16C17/243	10	{related to temperature and heat, e.g. for preventing overheating}	F16C17/24	F16C17/24		351
F16C17/246	10	{related to wear, e.g. sensors for measuring wear}	F16C17/24	F16C17/24		370
F16C17/26	8	Systems consisting of a plurality of sliding-contact bearings	F16C17/26	F16C17/26		736
F16C19/00	7	Bearings with rolling contact, for exclusively rotary movement (adjustable bearings F16C23/00, F16C25/00{; electrically insulating bearings H02K5/173})	F16C19/00	F16C19/00		452
F16C19/02	8	with bearing balls essentially of the same size in one or more circular rows	F16C19/02	F16C19/02		479
F16C19/04	9	for radial load mainly	F16C19/04	F16C19/04		348
F16C19/06	10	with a single row or balls	F16C19/06	F16C19/06		10577
F16C19/08	10	with two or more rows of balls	F16C19/08	F16C19/08		928
F16C19/10	9	for axial load mainly	F16C19/10	F16C19/10		1905
F16C19/12	10	for supporting the end face of a shaft or other member, e.g. footstep bearings	F16C19/12	F16C19/12		262
F16C19/14	9	for both radial and axial load	F16C19/14	F16C19/14		199
F16C19/16	10	with a single row of balls	F16C19/16	F16C19/16		1105
F16C19/163	11	{with angular contact}	F16C19/16	F16C19/16		3070
F16C19/166	12	{Four-point-contact ball bearings}	F16C19/16	F16C19/16		848
F16C19/18	10	with two or more rows of balls	F16C19/18	F16C19/18		861
F16C19/181	11	{with angular contact}	F16C19/18	F16C19/18		366
F16C19/182	12	{in tandem arrangement}	F16C19/18	F16C19/18		268
F16C19/183	12	{with two rows at opposite angles}	F16C19/18	F16C19/18		633
F16C19/184	13	{in O-arrangement}	F16C19/18	F16C19/18		1755
F16C19/185	14	{with two raceways provided integrally on a part other than a race ring, e.g. a shaft or housing}	F16C19/18	F16C19/18		590
F16C19/186	14	{with three raceways provided integrally on parts other than race rings, e.g. third generation hubs}	F16C19/18	F16C19/18		2889
F16C19/187	14	{with all four raceways integrated on parts other than race rings, e.g. fourth generation hubs}	F16C19/18	F16C19/18		370
F16C19/188	11	{with at least one row for radial load in combination with at least one row for axial load}	F16C19/18	F16C19/18		167
F16C19/20	9	with loose spacing bodies, e.g. balls, between the bearing balls	F16C19/20	F16C19/20		390
F16C19/22	8	with bearing rollers essentially of the same size in one or more circular rows, e.g. needle bearings	F16C19/22	F16C19/22		355
F16C19/225	9	{Details of the ribs supporting the end of the rollers}	F16C19/22	F16C19/22		325
F16C19/24	9	for radial load mainly	F16C19/24	F16C19/24		361
F16C19/26	10	with a single row of rollers	F16C19/26	F16C19/26		4115
F16C19/28	10	with two or more rows of rollers	F16C19/28	F16C19/28		1022
F16C19/30	9	for axial load mainly	F16C19/30	F16C19/30		1920
F16C19/305	10	{consisting of rollers held in a cage}	F16C19/30	F16C19/30		370
F16C19/32	10	for supporting the end face of a shaft or other member, e.g. footstep bearings	F16C19/32	F16C19/32		85
F16C19/34	9	for both radial and axial load	F16C19/34	F16C19/34		166
F16C19/36	10	with a single row of rollers	F16C19/36	F16C19/36		733
F16C19/361	11	{with cylindrical rollers}	F16C19/36	F16C19/36		268
F16C19/362	12	{the rollers being crossed within the single row}	F16C19/36	F16C19/36		470
F16C19/364	11	{with tapered rollers, i.e. rollers having essentially the shape of a truncated cone}	F16C19/36	F16C19/36		3752
F16C19/38	10	with two or more rows of rollers	F16C19/38	F16C19/38		2274
F16C19/381	11	{with at least one row for radial load in combination with at least one row for axial load}	F16C19/38	F16C19/38		601
F16C19/383	11	{with tapered rollers, i.e. rollers having essentially the shape of a truncated cone}	F16C19/38	F16C19/38		104
F16C19/385	12	{with two rows, i.e. double-row tapered roller bearings}	F16C19/38	F16C19/38		505
F16C19/386	13	{in O-arrangement}	F16C19/38	F16C19/38		2352
F16C19/388	12	{with four rows, i.e. four row tapered roller bearings}	F16C19/38	F16C19/38		281
F16C19/40	9	with loose spacing bodies between the rollers	F16C19/40	F16C19/40		585
F16C19/44	9	Needle bearings	F16C19/44	F16C19/44		209
F16C19/46	10	with one row or needles	F16C19/46	F16C19/46		1219
F16C19/463	11	{consisting of needle rollers held in a cage, i.e. subunit without race rings}	F16C19/46	F16C19/46		620
F16C19/466	11	{comprising needle rollers and an outer ring, i.e. subunit without inner ring}	F16C19/46	F16C19/46		799
F16C19/48	10	with two or more rows of needles	F16C19/48	F16C19/48		329
F16C19/49	8	Bearings with both balls and rollers	F16C19/49	F16C19/49		822
F16C19/492	9	{with two or more rows with angular contact}	F16C19/49	F16C19/49		43
F16C19/495	10	{with two rows}	F16C19/49	F16C19/49		29
F16C19/497	11	{in O-arrangement}	F16C19/49	F16C19/49		83
F16C19/50	8	Other types of ball or roller bearings	F16C19/50	F16C19/50		682
F16C19/502	9	{with rolling elements in rows not forming a full circle}	F16C19/50	F16C19/50		336
F16C19/505	9	{with the diameter of the rolling elements of one row differing from the diameter of those of another row}	F16C19/50	F16C19/50		668
F16C19/507	9	{with rolling elements journaled in one of the moving parts, e.g. stationary rollers to support a rotating part}	F16C19/50	F16C19/50		272
F16C19/52	8	with devices affected by abnormal or undesired conditions	F16C19/52	F16C19/52		1774
F16C19/522	9	{related to load on the bearing, e.g. bearings with load sensors or means to protect the bearing against overload}	F16C19/52	F16C19/52		899
F16C19/525	9	{related to temperature and heat, e.g. insulation}	F16C19/52	F16C19/52		952
F16C19/527	9	{related to vibration and noise}	F16C19/52	F16C19/52		785
F16C19/54	8	Systems consisting of a plurality of bearings with rolling friction (spindle bearings F16C35/08)	F16C19/54	F16C19/54		2797
F16C19/541	9	{Systems consisting of juxtaposed rolling bearings including at least one angular contact bearing}	F16C19/54	F16C19/54		157
F16C19/542	10	{with two rolling bearings with angular contact}	F16C19/54	F16C19/54		339
F16C19/543	11	{in O-arrangement}	F16C19/54	F16C19/54		547
F16C19/545	9	{Systems comprising at least one rolling bearing for radial load in combination with at least one rolling bearing for axial load}	F16C19/54	F16C19/54		486
F16C19/546	9	{Systems with spaced apart rolling bearings including at least one angular contact bearing}	F16C19/54	F16C19/54		259
F16C19/547	10	{with two angular contact rolling bearings}	F16C19/54	F16C19/54		539
F16C19/548	11	{in O-arrangement}	F16C19/54	F16C19/54		1616
F16C19/55	9	with intermediate floating {or independently-driven} rings rotating at reduced speed {or with other differential ball or roller bearings}	F16C19/55	F16C19/55		630
F16C19/56	9	in which the rolling bodies of one bearing differ in diameter from those of another	F16C19/56	F16C19/56		462
F16C21/00	7	Combinations of sliding-contact bearings with ball or roller bearings, for exclusively rotary movement (F16C17/24, F16C19/52 take precedence)	F16C21/00	F16C21/00		1231
F16C21/005	8	{the external zone of a bearing with rolling members, e.g. needles, being cup-shaped, with or without a separate thrust-bearing disc or ring, e.g. for universal joints (seals F16C33/72, F16D3/38)}	F16C21/00	F16C21/00		770
F16C23/00	7	Bearings for exclusively rotary movement adjustable for aligning or positioning (F16C27/00 takes precedence {; hydrostatic bearings F16C32/067})	F16C23/00	F16C23/00		308
F16C23/02	8	Sliding-contact bearings	F16C23/02	F16C23/02		494
F16C23/04	9	self-adjusting	F16C23/04	F16C23/04		854
F16C23/041	10	{with edge relief}	F16C23/04	F16C23/04		149
F16C23/043	10	{with spherical surfaces, e.g. spherical plain bearings}	F16C23/04	F16C23/04		465
F16C23/045	11	{for radial load mainly, e.g. radial spherical plain bearings}	F16C23/04	F16C23/04		1411
F16C23/046	12	{with split outer rings}	F16C23/04	F16C23/04		151
F16C23/048	11	{for axial load mainly}	F16C23/04	F16C23/04		109
F16C23/06	8	Ball or roller bearings	F16C23/06	F16C23/06		505
F16C23/08	9	self-adjusting	F16C23/08	F16C23/08		930
F16C23/082	10	{by means of at least one substantially spherical surface}	F16C23/08	F16C23/08		146
F16C23/084	11	{sliding on a complementary spherical surface}	F16C23/08	F16C23/08		996
F16C23/086	11	{forming a track for rolling elements}	F16C23/08	F16C23/08		2292
F16C23/088	10	{by means of crowning}	F16C23/08	F16C23/08		201
F16C23/10	8	Bearings, parts of which are eccentrically adjustable with respect to each other	F16C23/10	F16C23/10		668
F16C25/00	7	Bearings for exclusively rotary movement adjustable for wear or play (F16C27/00 takes precedence)	F16C25/00	F16C25/00		86
F16C25/02	8	Sliding-contact bearings	F16C25/02	F16C25/02		847
F16C25/04	9	self-adjusting	F16C25/04	F16C25/04		472
F16C25/045	10	{with magnetic means to preload the bearing}	F16C25/04	F16C25/04		121
F16C25/06	8	Ball or roller bearings	F16C25/06	F16C25/06		1743
F16C25/08	9	self-adjusting	F16C25/08	F16C25/08		1142
F16C25/083	10	{with resilient means acting axially on a race ring to preload the bearing}	F16C25/08	F16C25/08		1465
F16C25/086	10	{with magnetic means to preload the bearing}	F16C25/08	F16C25/08		68
F16C27/00	7	Elastic or yielding bearings or bearing supports, for exclusively rotary movement (shock-damping bearings for watches or clocks G04B31/02)	F16C27/00	F16C27/00		465
F16C27/02	8	Sliding-contact bearings	F16C27/02	F16C27/02		2008
F16C27/04	8	Ball or roller bearings, e.g. with resilient rolling bodies	F16C27/04	F16C27/04		1746
F16C27/045	9	{with a fluid film, e.g. squeeze film damping}	F16C27/04	F16C27/04		884
F16C27/06	8	by means of parts of rubber or like materials (F16C27/08 takes precedence; with sliding surfaces of rubber or synthetic rubber F16C33/22)	F16C27/06	F16C27/06		249
F16C27/063	9	{Sliding contact bearings}	F16C27/06	F16C27/06		945
F16C27/066	9	{Ball or roller bearings}	F16C27/06	F16C27/06		1681
F16C27/08	8	primarily for axial load, e.g. for vertically-arranged shafts	F16C27/08	F16C27/08		800
F16C29/00	7	Bearings for parts moving only linearly (F16C32/06 takes precedence; incorporated in flexible shafts F16C1/28{; parts of bearings in general and special methods for making bearings or parts thereof in general F16C33/00})	F16C29/00	F16C29/00		644
F16C29/001	8	{adjustable for alignment or positioning}	F16C29/00	F16C29/00		379
F16C29/002	8	{Elastic or yielding linear bearings or bearing supports}	F16C29/00	F16C29/00		350
F16C29/004	8	{Fixing of a carriage or rail, e.g. rigid mounting to a support structure or a movable part}	F16C29/00	F16C29/00		519
F16C29/005	8	{Guide rails or tracks for a linear bearing, i.e. adapted for movement of a carriage or bearing body there along}	F16C29/00	F16C29/00		1406
F16C29/007	8	{Hybrid linear bearings, i.e. including more than one bearing type, e.g. sliding contact bearings as well as rolling contact bearings}	F16C29/00	F16C29/00		159
F16C29/008	8	{Systems with a plurality of bearings, e.g. four carriages supporting a slide on two parallel rails}	F16C29/00	F16C29/00		587
F16C29/02	8	Sliding-contact bearings	F16C29/02	F16C29/02		2352
F16C29/025	9	{Hydrostatic or aerostatic (this type of bearing for rotary parts F16C32/06)}	F16C29/02	F16C29/02		1028
F16C29/04	8	Ball or roller bearings	F16C29/04	F16C29/04		2247
F16C29/041	9	{having rollers crossed within a row}	F16C29/04	F16C29/04		199
F16C29/043	9	{with two massive rectangular rails having facing grooves}	F16C29/04	F16C29/04		173
F16C29/045	9	{having rolling elements journaled in one of the moving parts}	F16C29/04	F16C29/04		937
F16C29/046	10	{with balls journaled in pockets}	F16C29/04	F16C29/04		318
F16C29/048	9	{with thin walled races, e.g. tracks of sheet metal}	F16C29/04	F16C29/04		270
F16C29/06	9	in which the rolling bodies circulate partly without carrying load	F16C29/06	F16C29/06		589
F16C29/0602	10	{Details of the bearing body or carriage or parts thereof, e.g. methods for manufacturing or assembly}	F16C29/06	F16C29/06		351
F16C29/0604	11	{of the load bearing section}	F16C29/06	F16C29/06		171
F16C29/0607	12	{of parts or members for retaining the rolling elements, i.e. members to prevent the rolling elements from falling out of the bearing body or carriage}	F16C29/06	F16C29/06		260
F16C29/0609	11	{of the ends of the bearing body or carriage where the rolling elements change direction, e.g. end caps}	F16C29/06	F16C29/06		538
F16C29/0611	11	{of the return passages, i.e. the passages where the rolling elements do not carry load}	F16C29/06	F16C29/06		215
F16C29/0614	10	{with a shoe type bearing body, e.g. a body facing one side of the guide rail or track only}	F16C29/06	F16C29/06		29
F16C29/0616	11	{for supporting load essentially in a single direction}	F16C29/06	F16C29/06		85
F16C29/0619	12	{with rollers or needles}	F16C29/06	F16C29/06		264
F16C29/0621	11	{for supporting load in essentially two directions, e.g. by multiple points of contact or two rows of rolling elements}	F16C29/06	F16C29/06		7
F16C29/0623	12	{with balls}	F16C29/06	F16C29/06		168
F16C29/0626	12	{with rollers}	F16C29/06	F16C29/06		52
F16C29/0628	13	{crossed within a row}	F16C29/06	F16C29/06		22
F16C29/063	10	{with a bearing body, e.g. a carriage or part thereof, provided between the legs of a U-shaped guide rail or track}	F16C29/06	F16C29/06		274
F16C29/0633	10	{with a bearing body defining a U-shaped carriage, i.e. surrounding a guide rail or track on three sides}	F16C29/06	F16C29/06		238
F16C29/0635	11	{whereby the return paths are provided as bores in a main body of the U-shaped carriage, e.g. the main body of the U-shaped carriage is a single part with end caps provided at each end}	F16C29/06	F16C29/06		104
F16C29/0638	12	{with balls}	F16C29/06	F16C29/06		155
F16C29/064	13	{with two rows of balls, one on each side of the rail}	F16C29/06	F16C29/06		294
F16C29/0642	13	{with four rows of balls}	F16C29/06	F16C29/06		289
F16C29/0645	14	{with load directions in O-arrangement}	F16C29/06	F16C29/06		190
F16C29/0647	14	{with load directions in X-arrangement}	F16C29/06	F16C29/06		356
F16C29/065	12	{with rollers}	F16C29/06	F16C29/06		395
F16C29/0652	11	{whereby the return paths are at least partly defined by separate parts, e.g. covers attached to the legs of the main body of the U-shaped carriage}	F16C29/06	F16C29/06		16
F16C29/0654	12	{with balls}	F16C29/06	F16C29/06		21
F16C29/0657	13	{with two rows of balls, one on each side of the rail}	F16C29/06	F16C29/06		115
F16C29/0659	13	{with four rows of balls}	F16C29/06	F16C29/06		57
F16C29/0661	14	{with load directions in O-arrangement}	F16C29/06	F16C29/06		38
F16C29/0664	14	{with load directions in X-arrangement}	F16C29/06	F16C29/06		59
F16C29/0666	12	{with rollers}	F16C29/06	F16C29/06		68
F16C29/0669	11	{whereby the main body of the U-shaped carriage is an assembly of at least three major parts, e.g. an assembly of a top plate with two separate legs attached thereto in the form of bearing shoes (bearing shoes per seF16C29/0614)}	F16C29/06	F16C29/06		20
F16C29/0671	12	{with balls}	F16C29/06	F16C29/06		99
F16C29/0673	12	{with rollers}	F16C29/06	F16C29/06		68
F16C29/0676	10	{with a bearing body or carriage almost fully embracing the guide rail or track, e.g. a circular sleeve with a longitudinal slot for the support posts of the rail}	F16C29/06	F16C29/06		131
F16C29/0678	10	{with a bearing body, i.e. the body carrying the circulating rolling elements, provided in the interior of a sleeve-like guide member defining the opposing raceways, e.g. in a telescopic shaft (telescopic shafts with built-in bearings F16C3/035; yielding coupling allowing axial displacement by rolling elements F16D3/065)}	F16C29/06	F16C29/06		68
F16C29/068	10	{with the bearing body fully encircling the guide rail or track}	F16C29/06	F16C29/06		32
F16C29/0683	11	{the bearing body encircles a rail or rod of circular cross-section, i.e. the linear bearing is not suited to transmit torque}	F16C29/06	F16C29/06		38
F16C29/0685	12	{with balls}	F16C29/06	F16C29/06		93
F16C29/0688	13	{whereby a sleeve surrounds the circulating balls and thicker part of the sleeve form the load bearing tracks}	F16C29/06	F16C29/06		234
F16C29/069	13	{whereby discrete load bearing elements, e.g. discrete load bearing plates or discrete rods, are provided in a retainer and form the load bearing tracks}	F16C29/06	F16C29/06		144
F16C29/0692	11	{the bearing body encircles a guide rail or track of non-circular cross-section, e.g. with grooves or protrusions, i.e. the linear bearing is suited to transmit torque (telescopic shafts with built-in bearings F16C3/035; yielding coupling allowing axial displacement by rolling elements F16D3/065)}	F16C29/06	F16C29/06		35
F16C29/0695	12	{with balls}	F16C29/06	F16C29/06		169
F16C29/0697	13	{with polygonal guide rail or track}	F16C29/06	F16C29/06		66
F16C29/08	8	Arrangements for covering or protecting the ways {(protective coverings for parts of machine tools B23Q11/08)}	F16C29/08	F16C29/08		312
F16C29/082	9	{fixed to the way}	F16C29/08	F16C29/08		250
F16C29/084	9	{fixed to the carriage or bearing body movable along the guide rail or track}	F16C29/08	F16C29/08		238
F16C29/086	10	{Seals being essentially U-shaped, e.g. for a U-shaped carriage}	F16C29/08	F16C29/08		244
F16C29/088	10	{Seals extending in the longitudinal direction of the carriage or bearing body}	F16C29/08	F16C29/08		215
F16C29/10	8	Arrangements for locking the bearings	F16C29/10	F16C29/10		478
F16C29/12	8	Arrangements for adjusting play	F16C29/12	F16C29/12		593
F16C29/123	9	{using elastic means}	F16C29/12	F16C29/12		338
F16C29/126	9	{using tapered surfaces or wedges}	F16C29/12	F16C29/12		142
F16C31/00	7	Bearings for parts which both rotate and move linearly	F16C31/00	F16C31/00		50
F16C31/02	8	Sliding-contact bearings	F16C31/02	F16C31/02		135
F16C31/04	8	Ball or roller bearings	F16C31/04	F16C31/04		220
F16C31/06	9	in which the rolling bodies circulate partly without carrying load	F16C31/06	F16C31/06		86
F16C32/00	7	Bearings not otherwise provided for	F16C32/00	F16C32/00		200
F16C32/02	8	Knife-edge bearings	F16C32/02	F16C32/02		118
F16C32/04	8	using magnetic or electric supporting means	F16C32/04	F16C32/04		328
F16C32/0402	9	{combined with other supporting means, e.g. hybrid bearings with both magnetic and fluid supporting means}	F16C32/04	F16C32/04		514
F16C32/0404	9	{Electrostatic bearings}	F16C32/04	F16C32/04		42
F16C32/0406	9	{Magnetic bearings}	F16C32/04	F16C32/04		349
F16C32/0408	10	{Passive magnetic bearings}	F16C32/04	F16C32/04		288
F16C32/041	11	{with permanent magnets on one part attracting the other part}	F16C32/04	F16C32/04		75
F16C32/0412	12	{for radial load mainly}	F16C32/04	F16C32/04		85
F16C32/0414	13	{with facing axial projections}	F16C32/04	F16C32/04		61
F16C32/0417	12	{for axial load mainly}	F16C32/04	F16C32/04		140
F16C32/0419	13	{with facing radial projections}	F16C32/04	F16C32/04		32
F16C32/0421	12	{for both radial and axial load}	F16C32/04	F16C32/04		47
F16C32/0423	11	{with permanent magnets on both parts repelling each other}	F16C32/04	F16C32/04		141
F16C32/0425	12	{for radial load mainly}	F16C32/04	F16C32/04		339
F16C32/0427	12	{for axial load mainly}	F16C32/04	F16C32/04		340
F16C32/0429	12	{for both radial and axial load, e.g. conical magnets}	F16C32/04	F16C32/04		184
F16C32/0431	13	{with bearings for axial load combined with bearings for radial load}	F16C32/04	F16C32/04		90
F16C32/0434	12	{for parts moving linearly}	F16C32/04	F16C32/04		72
F16C32/0436	11	{with a conductor on one part movable with respect to a magnetic field, e.g. a body of copper on one part and a permanent magnet on the other part}	F16C32/04	F16C32/04		77
F16C32/0438	12	{with a superconducting body, e.g. a body made of high temperature superconducting material such as YBaCuO}	F16C32/04	F16C32/04		514
F16C32/044	10	{Active magnetic bearings}	F16C32/04	F16C32/04		714
F16C32/0442	11	{with devices affected by abnormal, undesired or non-standard conditions such as shock-load, power outage, start-up or touchdown}	F16C32/04	F16C32/04		677
F16C32/0444	11	{Details of devices to control the actuation of the electromagnets}	F16C32/04	F16C32/04		714
F16C32/0446	12	{Determination of the actual position of the moving member, e.g. details of sensors}	F16C32/04	F16C32/04		491
F16C32/0448	13	{by using the electromagnet itself as sensor, e.g. sensorless magnetic bearings}	F16C32/04	F16C32/04		122
F16C32/0451	12	{Details of controllers, i.e. the units determining the power to be supplied, e.g. comparing elements, feedback arrangements with P.I.D. control}	F16C32/04	F16C32/04		665
F16C32/0453	13	{for controlling two axes, i.e. combined control of x-axis and y-axis}	F16C32/04	F16C32/04		87
F16C32/0455	13	{including digital signal processing [DSP] and analog/digital conversion [A/D, D/A]}	F16C32/04	F16C32/04		81
F16C32/0457	12	{Details of the power supply to the electromagnets}	F16C32/04	F16C32/04		239
F16C32/0459	11	{Details of the magnetic circuit}	F16C32/04	F16C32/04		445
F16C32/0461	12	{of stationary parts of the magnetic circuit}	F16C32/04	F16C32/04		288
F16C32/0463	13	{with electromagnetic bias, e.g. by extra bias windings}	F16C32/04	F16C32/04		71
F16C32/0465	13	{with permanent magnets provided in the magnetic circuit of the electromagnets}	F16C32/04	F16C32/04		434
F16C32/0468	12	{of moving parts of the magnetic circuit, e.g. of the rotor}	F16C32/04	F16C32/04		302
F16C32/047	11	{Details of housings; Mounting of active magnetic bearings}	F16C32/04	F16C32/04		352
F16C32/0472	11	{for linear movement}	F16C32/04	F16C32/04		147
F16C32/0474	11	{for rotary movement}	F16C32/04	F16C32/04		290
F16C32/0476	12	{with active support of one degree of freedom, e.g. axial magnetic bearings}	F16C32/04	F16C32/04		491
F16C32/0478	13	{with permanent magnets to support radial load}	F16C32/04	F16C32/04		67
F16C32/048	12	{with active support of two degrees of freedom, e.g. radial magnetic bearings}	F16C32/04	F16C32/04		450
F16C32/0482	13	{with three electromagnets to control the two degrees of freedom}	F16C32/04	F16C32/04		42
F16C32/0485	12	{with active support of three degrees of freedom}	F16C32/04	F16C32/04		172
F16C32/0487	12	{with active support of four degrees of freedom}	F16C32/04	F16C32/04		100
F16C32/0489	12	{with active support of five degrees of freedom, e.g. two radial magnetic bearings combined with an axial bearing}	F16C32/04	F16C32/04		335
F16C32/0491	13	{with electromagnets acting in axial and radial direction, e.g. with conical magnets}	F16C32/04	F16C32/04		76
F16C32/0493	12	{integrated in an electrodynamic machine, e.g. self-bearing motor}	F16C32/04	F16C32/04		225
F16C32/0495	13	{generating torque and axial force}	F16C32/04	F16C32/04		35
F16C32/0497	13	{generating torque and radial force}	F16C32/04	F16C32/04		135
F16C32/06	8	with moving member supported by a fluid cushion formed, at least to a large extent, otherwise than by movement of the shaft, e.g. hydrostatic air-cushion bearings	F16C32/06	F16C32/06		1080
F16C32/0603	9	{supported by a gas cushion, e.g. an air cushion}	F16C32/06	F16C32/06		769
F16C32/0607	10	{the gas being retained in a gap, e.g. squeeze film bearings}	F16C32/06	F16C32/06		92
F16C32/0611	11	{by means of vibrations}	F16C32/06	F16C32/06		59
F16C32/0614	10	{the gas being supplied under pressure, e.g. aerostatic bearings}	F16C32/06	F16C32/06		772
F16C32/0618	11	{via porous material}	F16C32/06	F16C32/06		359
F16C32/0622	11	{via nozzles, restrictors}	F16C32/06	F16C32/06		468
F16C32/0625	11	{via supply slits}	F16C32/06	F16C32/06		149
F16C32/0629	9	{supported by a liquid cushion, e.g. oil cushion}	F16C32/06	F16C32/06		319
F16C32/0633	10	{the liquid being retained in a gap}	F16C32/06	F16C32/06		110
F16C32/0637	11	{by a magnetic field, e.g. ferrofluid bearings}	F16C32/06	F16C32/06		77
F16C32/064	10	{the liquid being supplied under pressure}	F16C32/06	F16C32/06		352
F16C32/0644	11	{Details of devices to control the supply of liquids to the bearings}	F16C32/06	F16C32/06		312
F16C32/0648	12	{by sensors or pressure-responsive control devices in or near the bearings}	F16C32/06	F16C32/06		186
F16C32/0651	11	{Details of the bearing area per se}	F16C32/06	F16C32/06		286
F16C32/0655	12	{of supply openings}	F16C32/06	F16C32/06		115
F16C32/0659	12	{of pockets or grooves}	F16C32/06	F16C32/06		356
F16C32/0662	9	{Details of hydrostatic bearings independent of fluid supply or direction of load}	F16C32/06	F16C32/06		270
F16C32/0666	10	{of bearing pads}	F16C32/06	F16C32/06		462
F16C32/067	10	{of bearings adjustable for aligning, positioning, wear or play}	F16C32/06	F16C32/06		326
F16C32/0674	11	{by means of pre-load on the fluid bearings}	F16C32/06	F16C32/06		59
F16C32/0677	10	{of elastic or yielding bearings or bearing supports}	F16C32/06	F16C32/06		73
F16C32/0681	9	{Construction or mounting aspects of hydrostatic bearings, for exclusively rotary movement, related to the direction of load}	F16C32/06	F16C32/06		56
F16C32/0685	10	{for radial load only}	F16C32/06	F16C32/06		335
F16C32/0688	11	{with floating bearing elements}	F16C32/06	F16C32/06		59
F16C32/0692	10	{for axial load only}	F16C32/06	F16C32/06		385
F16C32/0696	10	{for both radial and axial load}	F16C32/06	F16C32/06		501
F16C33/00	7	Parts of bearings; Special methods for making bearings or parts thereof	F16C33/00	F16C33/00		417
F16C33/02	8	Parts of sliding-contact bearings	F16C33/02	F16C33/02		444
F16C33/04	9	Brasses; Bushes; Linings	F16C33/04	F16C33/04		1750
F16C33/043	10	{Sliding surface consisting mainly of ceramics, cermets or hard carbon, e.g. diamond like carbon [DLC]}	F16C33/04	F16C33/04		1127
F16C33/046	10	{divided or split, e.g. half-bearings or rolled sleeves}	F16C33/04	F16C33/04		634
F16C33/06	10	Sliding surface mainly made of metal (F16C33/24&#160;-&#160;F16C33/28 take precedence; {casting metal bearing surfaces  B22D15/02, B22D19/08})	F16C33/06	F16C33/06		668
F16C33/08	11	Attachment of brasses, bushes or linings to the bearing housing	F16C33/08	F16C33/08		1015
F16C33/10	11	Construction relative to lubrication {(lubrication in general F16N)}	F16C33/10	F16C33/10		1558
F16C33/1005	12	{with gas, e.g. air, as lubricant}	F16C33/10	F16C33/10		150
F16C33/101	13	{Details of the bearing surface, e.g. means to generate pressure such as lobes or wedges}	F16C33/10	F16C33/10		88
F16C33/1015	14	{Pressure generating grooves}	F16C33/10	F16C33/10		161
F16C33/102	12	{with grease as lubricant}	F16C33/10	F16C33/10		839
F16C33/1025	12	{with liquid, e.g. oil, as lubricant}	F16C33/10	F16C33/10		431
F16C33/103	13	{retained in or near the bearing}	F16C33/10	F16C33/10		1547
F16C33/1035	14	{by a magnetic field acting on a magnetic liquid}	F16C33/10	F16C33/10		204
F16C33/104	14	{in a porous body, e.g. oil impregnated sintered sleeve}	F16C33/10	F16C33/10		424
F16C33/1045	13	{Details of supply of the liquid to the bearing}	F16C33/10	F16C33/10		760
F16C33/105	14	{Conditioning, e.g. metering, cooling, filtering}	F16C33/10	F16C33/10		177
F16C33/1055	14	{from radial inside, e.g. via a passage through the shaft and/or inner sleeve}	F16C33/10	F16C33/10		220
F16C33/106	13	{Details of distribution or circulation inside the bearings, e.g. details of the bearing surfaces to affect flow or pressure of the liquid}	F16C33/10	F16C33/10		619
F16C33/1065	14	{Grooves on a bearing surface for distributing or collecting the liquid}	F16C33/10	F16C33/10		1325
F16C33/107	14	{Grooves for generating pressure}	F16C33/10	F16C33/10		1834
F16C33/1075	14	{Wedges, e.g. ramps or lobes, for generating pressure}	F16C33/10	F16C33/10		860
F16C33/108	14	{with a plurality of elements forming the bearing surfaces, e.g. bearing pads}	F16C33/10	F16C33/10		264
F16C33/1085	14	{Channels or passages to recirculate the liquid in the bearing}	F16C33/10	F16C33/10		556
F16C33/109	13	{Lubricant compositions or properties, e.g. viscosity}	F16C33/10	F16C33/10		239
F16C33/1095	12	{with solids as lubricant, e.g. dry coatings, powder}	F16C33/10	F16C33/10		574
F16C33/12	11	Structural composition; Use of special materials or surface treatments, e.g. for rust-proofing	F16C33/12	F16C33/12		1542
F16C33/121	12	{Use of special materials}	F16C33/12	F16C33/12		1642
F16C33/122	12	{Multilayer structures of sleeves, washers or liners}	F16C33/12	F16C33/12		486
F16C33/124	13	{Details of overlays}	F16C33/12	F16C33/12		325
F16C33/125	13	{Details of bearing layers, i.e. the lining}	F16C33/12	F16C33/12		353
F16C33/127	13	{Details of intermediate layers, e.g. nickel dams}	F16C33/12	F16C33/12		144
F16C33/128	12	{Porous bearings, e.g. bushes of sintered alloy}	F16C33/12	F16C33/12		347
F16C33/14	11	Special methods of manufacture; Running-in	F16C33/14	F16C33/14		2697
F16C33/145	12	{of sintered porous bearings}	F16C33/14	F16C33/14		327
F16C33/16	10	Sliding surface consisting mainly of graphite	F16C33/16	F16C33/16		376
F16C33/18	10	Sliding surface consisting mainly of wood or fibrous material	F16C33/18	F16C33/18		244
F16C33/20	10	Sliding surface consisting mainly of plastics (F16C33/22&#160;-&#160;F16C33/28 take precedence)	F16C33/20	F16C33/20		1609
F16C33/201	11	{Composition of the plastic}	F16C33/20	F16C33/20		2491
F16C33/203	11	{Multilayer structures, e.g. sleeves comprising a plastic lining}	F16C33/20	F16C33/20		197
F16C33/205	12	{with two layers}	F16C33/20	F16C33/20		251
F16C33/206	12	{with three layers}	F16C33/20	F16C33/20		291
F16C33/208	11	{Methods of manufacture, e.g. shaping, applying coatings}	F16C33/20	F16C33/20		804
F16C33/22	10	Sliding surface consisting mainly of rubber or synthetic rubber (F16C33/24&#160;-&#160;F16C33/28 take precedence)	F16C33/22	F16C33/22		318
F16C33/24	10	with different areas of the sliding surface consisting of different materials	F16C33/24	F16C33/24		669
F16C33/26	10	made from wire coils; made from a number of discs, rings, rods, or other members	F16C33/26	F16C33/26		577
F16C33/28	10	with embedded reinforcements shaped as frames or meshed materials	F16C33/28	F16C33/28		306
F16C33/30	8	Parts of ball or roller bearings	F16C33/30	F16C33/30		849
F16C33/303	9	{of hybrid bearings, e.g. rolling bearings with steel races and ceramic rolling elements}	F16C33/30	F16C33/30		232
F16C33/306	9	{Means to synchronise movements}	F16C33/30	F16C33/30		521
F16C33/32	9	Balls	F16C33/32	F16C33/32		1257
F16C33/34	9	Rollers; Needles	F16C33/34	F16C33/34		1353
F16C33/36	10	with bearing-surfaces other than cylindrical, e.g. tapered; with grooves in the bearing surfaces	F16C33/36	F16C33/36		978
F16C33/363	11	{with grooves in the bearing-surfaces}	F16C33/36	F16C33/36		246
F16C33/366	11	{Tapered rollers, i.e. rollers generally shaped as truncated cones}	F16C33/36	F16C33/36		540
F16C33/37	9	Loose spacing bodies	F16C33/37	F16C33/37		311
F16C33/3706	10	{with concave surfaces conforming to the shape of the rolling elements, e.g. the spacing bodies are in sliding contact with the rolling elements}	F16C33/37	F16C33/37		659
F16C33/3713	10	{with other rolling elements serving as spacing bodies, e.g. the spacing bodies are in rolling contact with the load carrying rolling elements}	F16C33/37	F16C33/37		489
F16C33/372	10	rigid	F16C33/372	F16C33/372		43
F16C33/374	10	resilient	F16C33/374	F16C33/374		134
F16C33/38	9	Ball cages	F16C33/38	F16C33/38		816
F16C33/3806	10	{Details of interaction of cage and race, e.g. retention, centring}	F16C33/38	F16C33/38		590
F16C33/3812	10	{formed of interconnected segments, e.g. chains}	F16C33/38	F16C33/38		212
F16C33/3818	10	{formed of unconnected segments}	F16C33/38	F16C33/38		120
F16C33/3825	10	{formed as a flexible belt, e.g. spacers connected by a thin film}	F16C33/38	F16C33/38		230
F16C33/3831	10	{with hybrid structure, i.e. with parts made of distinct materials}	F16C33/38	F16C33/38		270
F16C33/3837	10	{Massive or moulded cages having cage pockets surrounding the balls, e.g. machined window cages}	F16C33/38	F16C33/38		101
F16C33/3843	11	{formed as one-piece cages, i.e. monoblock cages}	F16C33/38	F16C33/38		403
F16C33/385	12	{made from metal, e.g. cast or machined window cages}	F16C33/38	F16C33/38		127
F16C33/3856	12	{made from plastic, e.g. injection moulded window cages}	F16C33/38	F16C33/38		562
F16C33/3862	11	{comprising two annular parts joined together}	F16C33/38	F16C33/38		230
F16C33/3868	12	{made from metal, e.g. two cast parts joined by rivets}	F16C33/38	F16C33/38		67
F16C33/3875	12	{made from plastic, e.g. two injection moulded parts joined by a snap fit}	F16C33/38	F16C33/38		273
F16C33/3881	11	{with more than three parts, e.g. two end rings connected by individual stays}	F16C33/38	F16C33/38		62
F16C33/3887	10	{Details of individual pockets, e.g. shape or ball retaining means}	F16C33/38	F16C33/38		662
F16C33/3893	10	{with rolling elements with smaller diameter than the load carrying balls, e.g. cages with counter-rotating spacers}	F16C33/38	F16C33/38		110
F16C33/40	10	for multiple rows of balls	F16C33/40	F16C33/40		590
F16C33/405	11	{with two or more juxtaposed cages joined together or interacting with each other}	F16C33/40	F16C33/40		83
F16C33/41	10	comb-shaped	F16C33/41	F16C33/41		509
F16C33/412	11	{Massive or moulded comb cages, e.g. snap ball cages}	F16C33/41	F16C33/41		72
F16C33/414	12	{formed as one-piece cages, i.e. monoblock comb cages}	F16C33/41	F16C33/41		297
F16C33/416	13	{made from plastic, e.g. injection moulded comb cages}	F16C33/41	F16C33/41		934
F16C33/418	11	{Details of individual pockets, e.g. shape or ball retaining means}	F16C33/41	F16C33/41		369
F16C33/42	10	made from wire or sheet metal strips (F16C33/40, F16C33/41 take precedence)	F16C33/42	F16C33/42		280
F16C33/422	11	{made from sheet metal}	F16C33/42	F16C33/42		185
F16C33/425	12	{from a single part, e.g. ribbon cages with one corrugated annular part}	F16C33/42	F16C33/42		399
F16C33/427	12	{from two parts, e.g. ribbon cages with two corrugated annular parts}	F16C33/42	F16C33/42		590
F16C33/44	10	Selection of substances (F16C33/40, F16C33/41 take precedence)	F16C33/44	F16C33/44		816
F16C33/445	11	{Coatings}	F16C33/44	F16C33/44		213
F16C33/46	9	Cages for rollers or needles	F16C33/46	F16C33/46		984
F16C33/4605	10	{Details of interaction of cage and race, e.g. retention or centring}	F16C33/46	F16C33/46		1064
F16C33/4611	10	{with hybrid structure, i.e. with parts made of distinct materials}	F16C33/46	F16C33/46		395
F16C33/4617	10	{Massive or moulded cages having cage pockets surrounding the rollers, e.g. machined window cages}	F16C33/46	F16C33/46		168
F16C33/4623	11	{formed as one-piece cages, i.e. monoblock cages}	F16C33/46	F16C33/46		566
F16C33/4629	12	{made from metal, e.g. cast or machined window cages}	F16C33/46	F16C33/46		297
F16C33/4635	12	{made from plastic, e.g. injection moulded window cages}	F16C33/46	F16C33/46		973
F16C33/4641	11	{comprising two annular parts joined together}	F16C33/46	F16C33/46		267
F16C33/4647	12	{made from metal, e.g. two cast parts joined by rivets}	F16C33/46	F16C33/46		72
F16C33/4652	12	{made from plastic, e.g. two injection moulded parts joined by a snap fit}	F16C33/46	F16C33/46		104
F16C33/4658	11	{comprising three annular parts, i.e. three piece roller cages}	F16C33/46	F16C33/46		46
F16C33/4664	11	{with more than three parts, e.g. two end rings connected by individual stays}	F16C33/46	F16C33/46		283
F16C33/467	10	{Details of individual pockets, e.g. shape or roller retaining means}	F16C33/46	F16C33/46		367
F16C33/4676	11	{of the stays separating adjacent cage pockets, e.g. guide means for the bearing-surface of the rollers}	F16C33/46	F16C33/46		650
F16C33/4682	11	{of the end walls, e.g. interaction with the end faces of the rollers}	F16C33/46	F16C33/46		291
F16C33/4688	10	{with rolling elements with smaller diameter than the load carrying rollers, e.g. cages with counter-rotating spacers}	F16C33/46	F16C33/46		185
F16C33/4694	10	{Single-split roller or needle cages}	F16C33/46	F16C33/46		223
F16C33/48	10	for multiple rows of rollers or needles	F16C33/48	F16C33/48		800
F16C33/485	11	{with two or more juxtaposed cages joined together or interacting with each other}	F16C33/48	F16C33/48		261
F16C33/49	10	comb-shaped	F16C33/49	F16C33/49		231
F16C33/491	11	{applied as pairs for retaining both ends of the rollers or needles}	F16C33/49	F16C33/49		63
F16C33/492	12	{joined by rods}	F16C33/49	F16C33/49		40
F16C33/494	11	{Massive or moulded comb cages}	F16C33/49	F16C33/49		106
F16C33/495	12	{formed as one piece cages, i.e. monoblock comb cages}	F16C33/49	F16C33/49		184
F16C33/497	13	{made from metal, e.g. cast or machined comb cages}	F16C33/49	F16C33/49		60
F16C33/498	13	{made from plastic, e.g. injection moulded comb cages}	F16C33/49	F16C33/49		119
F16C33/50	10	formed of interconnected members, e.g. chains	F16C33/50	F16C33/50		244
F16C33/502	11	{formed of arcuate segments retaining one or more rollers or needles}	F16C33/50	F16C33/50		190
F16C33/504	12	{with two segments, e.g. two semicircular cage parts}	F16C33/50	F16C33/50		130
F16C33/506	11	{formed as a flexible belt}	F16C33/50	F16C33/50		153
F16C33/508	11	{formed of links having an H-shape, i.e. links with a single stay placed between two rollers and with two end portions extending along the end faces of the two rollers}	F16C33/50	F16C33/50		59
F16C33/51	10	formed of unconnected members	F16C33/51	F16C33/51		126
F16C33/513	11	{formed of arcuate segments for carrying one or more rollers}	F16C33/51	F16C33/51		203
F16C33/516	12	{with two segments, e.g. double-split cages with two semicircular parts}	F16C33/51	F16C33/51		157
F16C33/52	10	with no part entering between, or touching, the bearing surfaces of the rollers (F16C33/50 takes precedence)	F16C33/52	F16C33/52		260
F16C33/523	11	{with pins extending into holes or bores on the axis of the rollers}	F16C33/52	F16C33/52		117
F16C33/526	12	{extending through the rollers and joining two lateral cage parts}	F16C33/52	F16C33/52		381
F16C33/54	10	made from wire, strips, or sheet metal (F16C33/48, F16C33/49 take precedence)	F16C33/54	F16C33/54		275
F16C33/541	11	{Details of individual pockets, e.g. shape or roller retaining means}	F16C33/54	F16C33/54		266
F16C33/542	11	{made from sheet metal}	F16C33/54	F16C33/54		160
F16C33/543	12	{from a single part}	F16C33/54	F16C33/54		1331
F16C33/545	13	{rolled from a band}	F16C33/54	F16C33/54		147
F16C33/546	13	{with a M- or W-shaped cross section}	F16C33/54	F16C33/54		275
F16C33/547	12	{from two parts, e.g. two discs or rings joined together}	F16C33/54	F16C33/54		332
F16C33/548	12	{with more than three parts, e.g. two end rings connected by a plurality of stays or pins}	F16C33/54	F16C33/54		197
F16C33/56	10	Selection of substances (F16C33/48, F16C33/49 take precedence)	F16C33/56	F16C33/56		538
F16C33/565	11	{Coatings}	F16C33/56	F16C33/56		218
F16C33/58	9	Raceways; Race rings	F16C33/58	F16C33/58		2141
F16C33/581	10	{integral with other parts, e.g. with housings or machine elements such as shafts or gear wheels}	F16C33/58	F16C33/58		1574
F16C33/583	10	{Details of specific parts of races}	F16C33/58	F16C33/58		1974
F16C33/585	11	{of raceways, e.g. ribs to guide the rollers}	F16C33/58	F16C33/58		2240
F16C33/586	11	{outside the space between the races, e.g. end faces or bore of inner ring}	F16C33/58	F16C33/58		2332
F16C33/588	10	{Races of sheet metal}	F16C33/58	F16C33/58		1381
F16C33/60	10	divided {or split, e.g. comprising two juxtaposed rings}	F16C33/60	F16C33/60		3115
F16C33/605	11	{with a separate retaining member, e.g. flange, shoulder, guide ring, secured to a race ring, adjacent to the race surface, so as to abut the end of the rolling elements, e.g. rollers, or the cage}	F16C33/60	F16C33/60		1194
F16C33/61	11	formed by wires	F16C33/61	F16C33/61		417
F16C33/62	10	Selection of substances	F16C33/62	F16C33/62		2201
F16C33/64	10	Special methods of manufacture	F16C33/64	F16C33/64		2872
F16C33/66	9	Special parts or details in view of lubrication	F16C33/66	F16C33/66		994
F16C33/6603	10	{with grease as lubricant}	F16C33/66	F16C33/66		447
F16C33/6607	11	{Retaining the grease in or near the bearing}	F16C33/66	F16C33/66		607
F16C33/6611	12	{in a porous or resinous body, e.g. a cage impregnated with the grease}	F16C33/66	F16C33/66		169
F16C33/6614	12	{in recesses or cavities provided in retainers, races or rolling elements}	F16C33/66	F16C33/66		719
F16C33/6618	12	{in a reservoir in the sealing means}	F16C33/66	F16C33/66		193
F16C33/6622	11	{Details of supply and/or removal of the grease, e.g. purging grease}	F16C33/66	F16C33/66		1020
F16C33/6625	12	{Controlling or conditioning the grease supply}	F16C33/66	F16C33/66		247
F16C33/6629	11	{Details of distribution or circulation inside the bearing, e.g. grooves on the cage or passages in the rolling elements}	F16C33/66	F16C33/66		470
F16C33/6633	11	{Grease properties or compositions, e.g. rheological properties}	F16C33/66	F16C33/66		535
F16C33/6637	10	{with liquid lubricant}	F16C33/66	F16C33/66		512
F16C33/664	11	{Retaining the liquid in or near the bearing}	F16C33/66	F16C33/66		621
F16C33/6644	12	{by a magnetic field acting on a magnetic liquid}	F16C33/66	F16C33/66		52
F16C33/6648	12	{in a porous or resinous body, e.g. a cage impregnated with the liquid}	F16C33/66	F16C33/66		498
F16C33/6651	12	{in recesses or cavities provided in retainers, races or rolling elements}	F16C33/66	F16C33/66		757
F16C33/6655	12	{in a reservoir in the sealing means}	F16C33/66	F16C33/66		96
F16C33/6659	11	{Details of supply of the liquid to the bearing, e.g. passages or nozzles}	F16C33/66	F16C33/66		2104
F16C33/6662	12	{the liquid being carried by air or other gases, e.g. mist lubrication}	F16C33/66	F16C33/66		266
F16C33/6666	12	{from an oil bath in the bearing housing, e.g. by an oil ring or centrifugal disc}	F16C33/66	F16C33/66		279
F16C33/667	12	{related to conditioning, e.g. cooling, filtering}	F16C33/66	F16C33/66		352
F16C33/6674	12	{related to the amount supplied, e.g. gaps to restrict flow of the liquid}	F16C33/66	F16C33/66		562
F16C33/6677	12	{from radial inside, e.g. via a passage through the shaft and/or inner ring}	F16C33/66	F16C33/66		627
F16C33/6681	11	{Details of distribution or circulation inside the bearing, e.g. grooves on the cage or passages in the rolling elements}	F16C33/66	F16C33/66		1437
F16C33/6685	11	{Details of collecting or draining, e.g. returning the liquid to a sump}	F16C33/66	F16C33/66		524
F16C33/6688	11	{Lubricant compositions or properties, e.g. viscosity}	F16C33/66	F16C33/66		165
F16C33/6692	12	{Liquids other than oil, e.g. water, refrigerants, liquid metal}	F16C33/66	F16C33/66		113
F16C33/6696	10	{with solids as lubricant, e.g. dry coatings, powder}	F16C33/66	F16C33/66		626
F16C33/72	8	Sealings	F16C33/72	F16C33/72		582
F16C33/723	9	{Shaft end sealing means, e.g. cup-shaped caps or covers}	F16C33/72	F16C33/72		1369
F16C33/726	9	{with means to vent the interior of the bearing}	F16C33/72	F16C33/72		322
F16C33/74	9	of sliding-contact bearings	F16C33/74	F16C33/74		2283
F16C33/741	10	{by means of a fluid}	F16C33/74	F16C33/74		93
F16C33/743	11	{retained in the sealing gap}	F16C33/74	F16C33/74		85
F16C33/745	12	{by capillary action}	F16C33/74	F16C33/74		346
F16C33/746	12	{by a magnetic field}	F16C33/74	F16C33/74		82
F16C33/748	11	{flowing to or from the sealing gap, e.g. vacuum seals with differential exhaust}	F16C33/74	F16C33/74		138
F16C33/76	9	of ball or roller bearings	F16C33/76	F16C33/76		1568
F16C33/761	10	{specifically for bearings with purely axial load}	F16C33/76	F16C33/76		375
F16C33/762	10	{by means of a fluid}	F16C33/76	F16C33/76		109
F16C33/763	11	{retained in the sealing gap}	F16C33/76	F16C33/76		50
F16C33/765	12	{by a magnetic field}	F16C33/76	F16C33/76		235
F16C33/766	12	{by pumping action}	F16C33/76	F16C33/76		37
F16C33/767	10	{integral with the race}	F16C33/76	F16C33/76		268
F16C33/768	10	{between relatively stationary parts, i.e. static seals}	F16C33/76	F16C33/76		602
F16C33/78	10	with a diaphragm, disc, or ring, with or without resilient members {(F16C33/761 takes precedence)}	F16C33/78	F16C33/78		1605
F16C33/7803	11	{suited for particular types of rolling bearings}	F16C33/78	F16C33/78		205
F16C33/7806	12	{for spherical roller bearings}	F16C33/78	F16C33/78		1158
F16C33/7809	12	{for needle roller bearings}	F16C33/78	F16C33/78		572
F16C33/7813	12	{for tapered roller bearings}	F16C33/78	F16C33/78		772
F16C33/7816	11	{Details of the sealing or parts thereof, e.g. geometry, material}	F16C33/78	F16C33/78		834
F16C33/782	12	{of the sealing region}	F16C33/78	F16C33/78		513
F16C33/7823	13	{of sealing lips}	F16C33/78	F16C33/78		1070
F16C33/7826	13	{of the opposing surface cooperating with the seal, e.g. a shoulder surface of a bearing ring}	F16C33/78	F16C33/78		447
F16C33/783	12	{of the mounting region}	F16C33/78	F16C33/78		1337
F16C33/7833	12	{Special methods of manufacture}	F16C33/78	F16C33/78		122
F16C33/7836	11	{floating with respect to both races}	F16C33/78	F16C33/78		103
F16C33/784	11	{mounted to a groove in the inner surface of the outer race and extending toward the inner race}	F16C33/78	F16C33/78		113
F16C33/7843	12	{with a single annular sealing disc}	F16C33/78	F16C33/78		318
F16C33/7846	13	{with a gap between the annular disc and the inner race}	F16C33/78	F16C33/78		459
F16C33/785	14	{Bearing shields made of sheet metal}	F16C33/78	F16C33/78		271
F16C33/7853	13	{with one or more sealing lips to contact the inner race}	F16C33/78	F16C33/78		788
F16C33/7856	14	{with a single sealing lip}	F16C33/78	F16C33/78		497
F16C33/7859	12	{with a further sealing element}	F16C33/78	F16C33/78		170
F16C33/7863	13	{mounted to the inner race, e.g. a flinger to use centrifugal effect}	F16C33/78	F16C33/78		213
F16C33/7866	13	{with sealing lips}	F16C33/78	F16C33/78		132
F16C33/7869	11	{mounted with a cylindrical portion to the inner surface of the outer race and having a radial portion extending inward}	F16C33/78	F16C33/78		142
F16C33/7873	12	{with a single sealing ring of generally L-shaped cross-section}	F16C33/78	F16C33/78		93
F16C33/7876	13	{with sealing lips}	F16C33/78	F16C33/78		656
F16C33/7879	12	{with a further sealing ring}	F16C33/78	F16C33/78		598
F16C33/7883	13	{mounted to the inner race and of generally L-shape, the two sealing rings defining a sealing with box-shaped cross-section}	F16C33/78	F16C33/78		761
F16C33/7886	11	{mounted outside the gap between the inner and outer races, e.g. sealing rings mounted to an end face or outer surface of a race}	F16C33/78	F16C33/78		1952
F16C33/7889	11	{mounted to an inner race and extending toward the outer race}	F16C33/78	F16C33/78		568
F16C33/7893	11	{mounted to a cage or integral therewith}	F16C33/78	F16C33/78		375
F16C33/7896	11	{with two or more discrete sealings arranged in series}	F16C33/78	F16C33/78		429
F16C33/80	10	Labyrinth sealings {(F16C33/761 takes precedence)}	F16C33/80	F16C33/80		1926
F16C33/805	11	{in addition to other sealings, e.g. dirt guards to protect sealings with sealing lips}	F16C33/80	F16C33/80		1041
F16C33/82	10	Arrangements for electrostatic or magnetic action against dust or other particles	F16C33/82	F16C33/82		117
F16C35/00	7	Rigid support of bearing units; Housings, e.g. caps, covers (F16C23/00 takes precedence)	F16C35/00	F16C35/00		1656
F16C35/02	8	in the case of sliding-contact bearings	F16C35/02	F16C35/02		2758
F16C35/04	8	in the case of ball or roller bearings	F16C35/04	F16C35/04		1033
F16C35/042	9	{Housings for rolling element bearings for rotary movement}	F16C35/04	F16C35/04		916
F16C35/045	10	{with a radial flange to mount the housing}	F16C35/04	F16C35/04		518
F16C35/047	10	{with a base plate substantially parallel to the axis of rotation, e.g. horizontally mounted pillow blocks}	F16C35/04	F16C35/04		618
F16C35/06	9	Mounting {or dismounting} of ball or roller bearings; Fixing them onto shaft or in housing	F16C35/06	F16C35/06		1991
F16C35/061	10	{mounting a plurality of bearings side by side}	F16C35/06	F16C35/06		460
F16C35/062	10	{Dismounting of ball or roller bearings}	F16C35/06	F16C35/06		278
F16C35/063	10	Fixing them on the shaft (with interposition of an element F16C35/07)	F16C35/063	F16C35/063		2766
F16C35/0635	11	{the bore of the inner ring being of special non-cylindrical shape which co-operates with a complementary shape on the shaft, e.g. teeth, polygonal sections}	F16C35/063	F16C35/063		321
F16C35/067	10	Fixing them in a housing (with interposition of an element F16C35/07)	F16C35/067	F16C35/067		3380
F16C35/07	10	Fixing them on the shaft or housing with interposition of an element	F16C35/07	F16C35/07		368
F16C35/073	11	between shaft and inner race ring	F16C35/073	F16C35/073		1322
F16C35/077	11	between housing and outer race ring	F16C35/077	F16C35/077		2488
F16C35/078	10	using pressure fluid as mounting aid	F16C35/078	F16C35/078		114
F16C35/08	8	for spindles	F16C35/08	F16C35/08		199
F16C35/10	9	with sliding-contact bearings	F16C35/10	F16C35/10		263
F16C35/12	9	with ball or roller bearings {(adjustable bearings F16C23/00, F16C25/00; elastic bearings F16C27/00)}	F16C35/12	F16C35/12		584
F16C37/00	7	Cooling of bearings	F16C37/00	F16C37/00		1194
F16C37/002	8	{of fluid bearings}	F16C37/00	F16C37/00		610
F16C37/005	8	{of magnetic bearings}	F16C37/00	F16C37/00		295
F16C37/007	8	{of rolling bearings}	F16C37/00	F16C37/00		1273
F16C39/00	7	Relieving load on bearings	F16C39/00	F16C39/00		46
F16C39/02	8	using mechanical means	F16C39/02	F16C39/02		801
F16C39/04	8	using hydraulic or pneumatic means	F16C39/04	F16C39/04		286
F16C39/06	8	using magnetic means	F16C39/06	F16C39/06		323
F16C39/063	9	{Permanent magnets}	F16C39/06	F16C39/06		734
F16C39/066	10	{with opposing permanent magnets repelling each other}	F16C39/06	F16C39/06		126
F16C41/00	7	Other accessories, {e.g. devices integrated in the bearing not relating to the bearing function as such}	F16C41/00	F16C41/00		1345
F16C41/001	8	{Integrated brakes or clutches for stopping or coupling the relatively movable parts}	F16C41/00	F16C41/00		408
F16C41/002	8	{Conductive elements, e.g. to prevent static electricity}	F16C41/00	F16C41/00		521
F16C41/004	8	{Electro-dynamic machines, e.g. motors, generators, actuators}	F16C41/00	F16C41/00		397
F16C41/005	8	{Fluid passages not relating to lubrication or cooling}	F16C41/00	F16C41/00		200
F16C41/007	8	{Encoders, e.g. parts with a plurality of alternating magnetic poles}	F16C41/00	F16C41/00		2769
F16C41/008	8	{Identification means, e.g. markings, RFID-tags; Data transfer means}	F16C41/00	F16C41/00		674
F16C41/02	8	Arrangements for equalising the load on a plurality of bearings or their elements	F16C41/02	F16C41/02		448
F16C41/04	8	Preventing damage to bearings during storage or transport thereof or when otherwise out of use	F16C41/04	F16C41/04		654
F16C41/045	9	{Devices for provisionally retaining needles or rollers in a bearing race before mounting of the bearing on a shaft}	F16C41/04	F16C41/04		143
F16C43/00	7	Assembling bearings	F16C43/00	F16C43/00		227
F16C43/02	8	Assembling sliding-contact bearings	F16C43/02	F16C43/02		1209
F16C43/04	8	Assembling rolling-contact bearings	F16C43/04	F16C43/04		2410
F16C43/045	9	{Mounting or replacing seals}	F16C43/04	F16C43/04		404
F16C43/06	9	Placing rolling bodies in cages or bearings	F16C43/06	F16C43/06		1678
F16C43/065	10	{in cages}	F16C43/06	F16C43/06		409
F16C43/08	10	by deforming the cages or the races	F16C43/08	F16C43/08		322
F16C43/083	11	{by plastic deformation of the cage}	F16C43/08	F16C43/08		148
F16C43/086	11	{by plastic deformation of the race}	F16C43/08	F16C43/08		76
F16C2202/00	7	Solid materials defined by their properties	CPCONLY	F16C2202/00		20
F16C2202/02	8	Mechanical properties	CPCONLY	F16C2202/02		82
F16C2202/04	9	Hardness	CPCONLY	F16C2202/04		489
F16C2202/06	9	Strength or rigidity	CPCONLY	F16C2202/06		154
F16C2202/08	9	Resilience, elasticity, super-elasticity	CPCONLY	F16C2202/08		108
F16C2202/10	9	Porosity	CPCONLY	F16C2202/10		140
F16C2202/20	8	Thermal properties	CPCONLY	F16C2202/20		91
F16C2202/22	9	Coefficient of expansion	CPCONLY	F16C2202/22		239
F16C2202/24	9	Insulating	CPCONLY	F16C2202/24		93
F16C2202/28	9	Shape memory material	CPCONLY	F16C2202/28		106
F16C2202/30	8	Electric properties; Magnetic properties	CPCONLY	F16C2202/30		173
F16C2202/32	9	Conductivity	CPCONLY	F16C2202/32		265
F16C2202/34	10	Superconductivity	CPCONLY	F16C2202/34		27
F16C2202/36	9	Piezoelectric	CPCONLY	F16C2202/36		116
F16C2202/40	9	Magnetic	CPCONLY	F16C2202/40		88
F16C2202/42	10	soft-magnetic, ferromagnetic	CPCONLY	F16C2202/42		33
F16C2202/44	10	hard-magnetic, permanent magnetic, e.g. samarium-cobalt	CPCONLY	F16C2202/44		32
F16C2202/50	8	Lubricating properties	CPCONLY	F16C2202/50		258
F16C2202/52	9	Graphite	CPCONLY	F16C2202/52		202
F16C2202/54	9	Molybdenum disulfide	CPCONLY	F16C2202/54		179
F16C2202/60	8	Oil repelling	CPCONLY	F16C2202/60		79
F16C2202/64	8	Water absorbing	CPCONLY	F16C2202/64		18
F16C2202/66	8	Water repelling	CPCONLY	F16C2202/66		52
F16C2202/70	8	Anti-bacterial, anti-microbial	CPCONLY	F16C2202/70		5
F16C2204/00	7	Metallic materials; Alloys (alloys in general C22C; F16C2206/00 takes precedence)	CPCONLY	F16C2204/00		117
F16C2204/02	8	Noble metals	CPCONLY	F16C2204/02		11
F16C2204/04	9	based on silver	CPCONLY	F16C2204/04		76
F16C2204/10	8	Alloys based on copper	CPCONLY	F16C2204/10		513
F16C2204/12	9	with tin as the next major constituent	CPCONLY	F16C2204/12		344
F16C2204/14	9	with zinc as the next major constituent	CPCONLY	F16C2204/14		133
F16C2204/16	9	with lead as the next major constituent	CPCONLY	F16C2204/16		89
F16C2204/18	9	with bismuth as the next major constituent	CPCONLY	F16C2204/18		37
F16C2204/20	8	Alloys based on aluminium	CPCONLY	F16C2204/20		543
F16C2204/22	9	with tin as the next major constituent	CPCONLY	F16C2204/22		134
F16C2204/24	9	with lead as the next major constituent	CPCONLY	F16C2204/24		30
F16C2204/26	8	Alloys based on magnesium	CPCONLY	F16C2204/26		32
F16C2204/30	8	Alloys based on one of tin, lead, antimony, bismuth, indium, e.g. materials for providing sliding surfaces	CPCONLY	F16C2204/30		79
F16C2204/32	9	Alloys based on lead	CPCONLY	F16C2204/32		88
F16C2204/34	9	Alloys based on tin	CPCONLY	F16C2204/34		136
F16C2204/36	9	Alloys based on bismuth	CPCONLY	F16C2204/36		30
F16C2204/40	8	Alloys based on refractory metals	CPCONLY	F16C2204/40		20
F16C2204/42	9	Alloys based on titanium	CPCONLY	F16C2204/42		106
F16C2204/44	9	Alloys based on chromium	CPCONLY	F16C2204/44		68
F16C2204/46	9	Alloys based on molybdenum	CPCONLY	F16C2204/46		41
F16C2204/50	8	Alloys based on zinc	CPCONLY	F16C2204/50		101
F16C2204/52	8	Alloys based on nickel, e.g. Inconel	CPCONLY	F16C2204/52		168
F16C2204/60	8	Ferrous alloys, e.g. steel alloys	CPCONLY	F16C2204/60		678
F16C2204/62	9	Low carbon steel, i.e. carbon content below 0.4 wt%	CPCONLY	F16C2204/62		171
F16C2204/64	9	Medium carbon steel, i.e. carbon content from 0.4 to 0,8 wt%	CPCONLY	F16C2204/64		186
F16C2204/66	9	High carbon steel, i.e. carbon content above 0.8 wt%, e.g. through-hardenable steel	CPCONLY	F16C2204/66		255
F16C2204/70	9	with chromium as the next major constituent	CPCONLY	F16C2204/70		238
F16C2204/72	10	with nickel as further constituent, e.g. stainless steel	CPCONLY	F16C2204/72		109
F16C2204/74	9	with manganese as the next major constituent	CPCONLY	F16C2204/74		68
F16C2204/80	8	Amorphous alloys	CPCONLY	F16C2204/80		16
F16C2206/00	7	Materials with ceramics, cermets, hard carbon or similar non-metallic hard materials as main constituents	CPCONLY	F16C2206/00		67
F16C2206/02	8	Carbon based material	CPCONLY	F16C2206/02		109
F16C2206/04	9	Diamond like carbon [DLC]	CPCONLY	F16C2206/04		342
F16C2206/06	9	Composite carbon material, e.g. carbon fibre reinforced carbon (C/C)	CPCONLY	F16C2206/06		91
F16C2206/40	8	Ceramics, e.g. carbides, nitrides, oxides, borides of a metal	CPCONLY	F16C2206/40		252
F16C2206/42	9	based on ceramic oxides	CPCONLY	F16C2206/42		67
F16C2206/44	10	based on aluminium oxide (Al2O3)	CPCONLY	F16C2206/44		78
F16C2206/48	10	based on zirconia (ZrO2)	CPCONLY	F16C2206/48		65
F16C2206/56	9	based on ceramic carbides, e.g. silicon carbide (SiC)	CPCONLY	F16C2206/56		113
F16C2206/58	9	based on ceramic nitrides	CPCONLY	F16C2206/58		63
F16C2206/60	10	Silicon nitride (Si3N4)l	CPCONLY	F16C2206/60		115
F16C2206/80	8	Cermets, i.e. composites of ceramics and metal	CPCONLY	F16C2206/80		65
F16C2206/82	9	based on tungsten carbide [WC]	CPCONLY	F16C2206/82		91
F16C2208/00	7	Plastics; Synthetic resins, e.g. rubbers	CPCONLY	F16C2208/00		193
F16C2208/02	8	comprising fillers, fibres	CPCONLY	F16C2208/02		613
F16C2208/04	9	Glass fibres	CPCONLY	F16C2208/04		237
F16C2208/10	8	Elastomers; Rubbers	CPCONLY	F16C2208/10		242
F16C2208/12	9	Polyurethan [PU]	CPCONLY	F16C2208/12		105
F16C2208/14	9	Silicone rubber	CPCONLY	F16C2208/14		31
F16C2208/20	8	Thermoplastic resins	CPCONLY	F16C2208/20		238
F16C2208/22	9	comprising two or more thermoplastics	CPCONLY	F16C2208/22		45
F16C2208/30	9	Fluoropolymers (F16C2208/58 takes precedence)	CPCONLY	F16C2208/30		102
F16C2208/32	10	Polytetrafluorethylene [PTFE] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/32		685
F16C2208/34	10	Polyvinylidenefluoride [PVDF] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/34		22
F16C2208/36	9	Polyarylene ether ketones [PAEK], e.g. PEK, PEEK (F16C2208/58 takes precedence)	CPCONLY	F16C2208/36		328
F16C2208/40	9	Imides, e.g. polyimide [PI], polyetherimide [PEI] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/40		170
F16C2208/42	10	Polyamideimide [PAI] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/42		103
F16C2208/44	10	Polybenzimidazole [PBI] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/44		20
F16C2208/48	9	Liquid crystal polymers [LCP] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/48		10
F16C2208/52	9	Polyphenylene sulphide [PPS] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/52		172
F16C2208/54	9	Polysulphones, e.g. polysulphone [PSU], polyethersulphone [PES], polyethersulphone-block copolymer [PPSU] (F16C2208/58 takes precedence)	CPCONLY	F16C2208/54		17
F16C2208/58	9	Several materials as provided for in F16C2208/30&#160;-&#160;F16C2208/54 mentioned as option	CPCONLY	F16C2208/58		152
F16C2208/60	9	Polyamides [PA]	CPCONLY	F16C2208/60		652
F16C2208/62	10	high performance polyamides, e.g. PA12, PA46	CPCONLY	F16C2208/62		62
F16C2208/66	9	Acetals, e.g. polyoxymethylene [POM]	CPCONLY	F16C2208/66		298
F16C2208/70	9	Polyesters, e.g. polyethylene-terephthlate [PET], polybutylene-terephthlate [PBT]	CPCONLY	F16C2208/70		167
F16C2208/72	9	Acrylics, e.g. polymethylmethacrylate [PMMA]	CPCONLY	F16C2208/72		24
F16C2208/76	9	Polyolefins, e.g. polyproylene [PP]	CPCONLY	F16C2208/76		123
F16C2208/78	10	Polyethylene [PE], e.g. ultra-high molecular weight polyethylene [UHMWPE]	CPCONLY	F16C2208/78		182
F16C2208/80	8	Thermosetting resins	CPCONLY	F16C2208/80		76
F16C2208/82	9	Composites, i.e. fibre reinforced thermosetting resins	CPCONLY	F16C2208/82		158
F16C2208/86	9	Epoxy resins	CPCONLY	F16C2208/86		181
F16C2208/90	9	Phenolic resin	CPCONLY	F16C2208/90		154
F16C2210/00	7	Fluids	CPCONLY	F16C2210/00		16
F16C2210/02	8	defined by their properties	CPCONLY	F16C2210/02		14
F16C2210/04	9	by viscosity	CPCONLY	F16C2210/04		60
F16C2210/06	9	magnetic fluids	CPCONLY	F16C2210/06		41
F16C2210/08	8	molten metals	CPCONLY	F16C2210/08		49
F16C2210/10	8	water based	CPCONLY	F16C2210/10		53
F16C2212/00	7	Natural materials, i.e. based on animal or plant products such as leather, wood or cotton or extracted therefrom, e.g. lignin	CPCONLY	F16C2212/00		37
F16C2212/04	8	Wood	CPCONLY	F16C2212/04		17
F16C2212/08	8	Woven, unwoven fabrics, e.g. felt	CPCONLY	F16C2212/08		44
F16C2220/00	7	Shaping	CPCONLY	F16C2220/00		49
F16C2220/02	8	by casting	CPCONLY	F16C2220/02		315
F16C2220/04	9	by injection-moulding	CPCONLY	F16C2220/04		927
F16C2220/06	9	in situ casting or moulding	CPCONLY	F16C2220/06		159
F16C2220/08	9	by compression-moulding	CPCONLY	F16C2220/08		67
F16C2220/20	8	by sintering pulverised material, e.g. powder metallurgy	CPCONLY	F16C2220/20		811
F16C2220/24	8	by built-up welding	CPCONLY	F16C2220/24		156
F16C2220/28	8	by winding impregnated fibres	CPCONLY	F16C2220/28		171
F16C2220/40	8	by deformation without removing material	CPCONLY	F16C2220/40		188
F16C2220/42	9	by working of thin-walled material such as sheet or tube	CPCONLY	F16C2220/42		234
F16C2220/44	9	by rolling	CPCONLY	F16C2220/44		303
F16C2220/46	9	by forging	CPCONLY	F16C2220/46		263
F16C2220/48	9	by extrusion, e.g. of metallic profiles	CPCONLY	F16C2220/48		134
F16C2220/60	8	by removing material, e.g. machining	CPCONLY	F16C2220/60		490
F16C2220/62	9	by turning, boring, drilling	CPCONLY	F16C2220/62		302
F16C2220/66	9	by milling	CPCONLY	F16C2220/66		118
F16C2220/68	9	by electrical discharge or electrochemical machining	CPCONLY	F16C2220/68		71
F16C2220/70	9	by grinding	CPCONLY	F16C2220/70		350
F16C2220/80	8	by separating parts, e.g. by severing, cracking	CPCONLY	F16C2220/80		36
F16C2220/82	9	by cutting	CPCONLY	F16C2220/82		336
F16C2220/84	9	by perforating; by punching; by stamping-out	CPCONLY	F16C2220/84		183
F16C2223/00	7	Surface treatments; Hardening; Coating	CPCONLY	F16C2223/00		76
F16C2223/02	8	Mechanical treatment, e.g. finishing	CPCONLY	F16C2223/02		168
F16C2223/04	9	by sizing, by shaping to final size by small plastic deformation, e.g. by calibrating or coining	CPCONLY	F16C2223/04		186
F16C2223/06	9	polishing	CPCONLY	F16C2223/06		137
F16C2223/08	9	shot-peening, blasting	CPCONLY	F16C2223/08		160
F16C2223/10	8	Hardening, e.g. carburizing, carbo-nitriding	CPCONLY	F16C2223/10		279
F16C2223/12	9	with carburizing	CPCONLY	F16C2223/12		95
F16C2223/14	9	with nitriding	CPCONLY	F16C2223/14		97
F16C2223/16	9	with carbo-nitriding	CPCONLY	F16C2223/16		91
F16C2223/18	9	with induction hardening	CPCONLY	F16C2223/18		115
F16C2223/30	8	Coating surfaces	CPCONLY	F16C2223/30		500
F16C2223/32	9	by attaching pre-existing layers, e.g. resin sheets or foils by adhesion to a substrate; Laminating	CPCONLY	F16C2223/32		219
F16C2223/40	9	by dipping in molten material	CPCONLY	F16C2223/40		119
F16C2223/42	9	by spraying the coating material, e.g. plasma spraying	CPCONLY	F16C2223/42		374
F16C2223/44	9	by casting molten material on the substrate	CPCONLY	F16C2223/44		207
F16C2223/46	9	by welding, e.g. by using a laser to build a layer	CPCONLY	F16C2223/46		155
F16C2223/60	9	by vapour deposition, e.g. PVD, CVD	CPCONLY	F16C2223/60		181
F16C2223/70	9	by electroplating or electrolytic coating, e.g. anodising, galvanising	CPCONLY	F16C2223/70		368
F16C2223/80	9	by powder coating	CPCONLY	F16C2223/80		82
F16C2226/00	7	Joining parts; Fastening; Assembling or mounting parts	CPCONLY	F16C2226/00		81
F16C2226/10	8	Force connections, e.g. clamping	CPCONLY	F16C2226/10		326
F16C2226/12	9	by press-fit, e.g. plug-in	CPCONLY	F16C2226/12		504
F16C2226/14	9	by shrink fit, i.e. heating and shrinking part to allow assembly	CPCONLY	F16C2226/14		129
F16C2226/16	9	by wedge action, e.g. by tapered or conical parts	CPCONLY	F16C2226/16		578
F16C2226/18	9	by magnets, i.e. magnetic attraction to hold parts together	CPCONLY	F16C2226/18		60
F16C2226/30	8	Material joints	CPCONLY	F16C2226/30		242
F16C2226/32	9	by soldering	CPCONLY	F16C2226/32		82
F16C2226/34	10	by brazing	CPCONLY	F16C2226/34		86
F16C2226/36	9	by welding	CPCONLY	F16C2226/36		815
F16C2226/38	10	with ultrasonic welding	CPCONLY	F16C2226/38		36
F16C2226/40	9	with adhesive	CPCONLY	F16C2226/40		524
F16C2226/50	8	Positive connections	CPCONLY	F16C2226/50		484
F16C2226/52	9	with plastic deformation, e.g. caulking or staking	CPCONLY	F16C2226/52		283
F16C2226/54	10	with rivets	CPCONLY	F16C2226/54		77
F16C2226/60	9	with threaded parts, e.g. bolt and nut connections	CPCONLY	F16C2226/60		1464
F16C2226/62	9	with pins, bolts or dowels	CPCONLY	F16C2226/62		336
F16C2226/70	9	with complementary interlocking parts	CPCONLY	F16C2226/70		252
F16C2226/72	10	with bayonet joints, i.e. parts are rotated to create positive interlock	CPCONLY	F16C2226/72		65
F16C2226/74	10	with snap-fit, e.g. by clips	CPCONLY	F16C2226/74		942
F16C2226/76	10	with tongue and groove or key and slot	CPCONLY	F16C2226/76		412
F16C2226/78	11	of jigsaw-puzzle type	CPCONLY	F16C2226/78		94
F16C2226/80	9	with splines, serrations or similar profiles to prevent movement between joined parts	CPCONLY	F16C2226/80		175
F16C2229/00	7	Setting preload	CPCONLY	F16C2229/00		789
F16C2231/00	7	Running-in; Initial operation	CPCONLY	F16C2231/00		116
F16C2233/00	7	Monitoring condition, e.g. temperature, load, vibration	CPCONLY	F16C2233/00		1536
F16C2235/00	7	Cleaning	CPCONLY	F16C2235/00		161
F16C2237/00	7	Repair or replacement	CPCONLY	F16C2237/00		229
F16C2240/00	7	Specified values or numerical ranges of parameters; Relations between them	CPCONLY	F16C2240/00		17
F16C2240/02	8	Flow, e.g. volume flow or mass flow	CPCONLY	F16C2240/02		37
F16C2240/06	8	Temperature	CPCONLY	F16C2240/06		188
F16C2240/08	8	Time	CPCONLY	F16C2240/08		43
F16C2240/12	8	Force, load, stress, pressure	CPCONLY	F16C2240/12		82
F16C2240/14	9	Preload	CPCONLY	F16C2240/14		39
F16C2240/18	9	Stress	CPCONLY	F16C2240/18		91
F16C2240/22	9	Fluid pressure	CPCONLY	F16C2240/22		16
F16C2240/26	8	Speed, e.g. rotational speed	CPCONLY	F16C2240/26		65
F16C2240/30	8	Angles, e.g. inclinations	CPCONLY	F16C2240/30		741
F16C2240/34	9	Contact angles	CPCONLY	F16C2240/34		348
F16C2240/40	8	Linear dimensions, e.g. length, radius, thickness, gap	CPCONLY	F16C2240/40		1221
F16C2240/42	9	Groove sizes	CPCONLY	F16C2240/42		356
F16C2240/44	9	Hole or pocket sizes	CPCONLY	F16C2240/44		250
F16C2240/46	9	Gap sizes or clearances	CPCONLY	F16C2240/46		458
F16C2240/48	9	Particle sizes	CPCONLY	F16C2240/48		185
F16C2240/50	9	Crowning, e.g. crowning height or crowning radius	CPCONLY	F16C2240/50		352
F16C2240/54	9	Surface roughness	CPCONLY	F16C2240/54		487
F16C2240/56	9	Tolerances; Accuracy of linear dimensions	CPCONLY	F16C2240/56		61
F16C2240/60	9	Thickness, e.g. thickness of coatings	CPCONLY	F16C2240/60		905
F16C2240/64	10	in the nanometer range	CPCONLY	F16C2240/64		113
F16C2240/70	9	Diameters; Radii	CPCONLY	F16C2240/70		816
F16C2240/76	10	Osculation, i.e. relation between radii of balls and raceway groove	CPCONLY	F16C2240/76		257
F16C2240/80	10	Pitch circle diameters [PCD]	CPCONLY	F16C2240/80		355
F16C2240/82	11	Degree of filling, i.e. sum of diameters of rolling elements in relation to PCD	CPCONLY	F16C2240/82		37
F16C2240/84	12	with full complement of balls or rollers, i.e. sum of clearances less than diameter of one rolling element	CPCONLY	F16C2240/84		523
F16C2240/90	8	Surface areas	CPCONLY	F16C2240/90		87
F16C2240/94	8	Volume	CPCONLY	F16C2240/94		37
F16C2300/00	7	Application independent of particular apparatuses	CPCONLY	F16C2300/00		17
F16C2300/02	8	General use or purpose, i.e. no use, purpose, special adaptation or modification indicated or a wide variety of uses mentioned	CPCONLY	F16C2300/02		2770
F16C2300/10	8	related to size	CPCONLY	F16C2300/10		5
F16C2300/12	9	Small applications, e.g. miniature bearings	CPCONLY	F16C2300/12		99
F16C2300/14	9	Large applications, e.g. bearings having an inner diameter exceeding 500 mm	CPCONLY	F16C2300/14		2599
F16C2300/20	8	related to type of movement	CPCONLY	F16C2300/20		91
F16C2300/22	9	High-speed rotation	CPCONLY	F16C2300/22		534
F16C2300/28	9	Reciprocating movement	CPCONLY	F16C2300/28		142
F16C2300/30	8	related to direction with respect to gravity	CPCONLY	F16C2300/30		6
F16C2300/32	9	Horizontal, e.g. bearings for supporting a horizontal shaft	CPCONLY	F16C2300/32		52
F16C2300/34	9	Vertical, e.g. bearings for supporting a vertical shaft	CPCONLY	F16C2300/34		431
F16C2300/40	8	related to environment, i.e. operating conditions	CPCONLY	F16C2300/40		57
F16C2300/42	9	corrosive, i.e. with aggressive media or harsh conditions	CPCONLY	F16C2300/42		159
F16C2300/52	9	low temperature, e.g. cryogenic temperature	CPCONLY	F16C2300/52		48
F16C2300/54	9	high-temperature	CPCONLY	F16C2300/54		102
F16C2300/62	9	low pressure, e.g. elements operating under vacuum conditions	CPCONLY	F16C2300/62		265
F16C2300/64	9	high pressure, e.g. elements exposed to high pressure gases or fluids	CPCONLY	F16C2300/64		6
F16C2310/00	7	Agricultural machines	CPCONLY	F16C2310/00		398
F16C2314/00	7	Personal or domestic articles, e.g. household appliances such as washing machines, dryers	CPCONLY	F16C2314/00		173
F16C2314/70	8	Furniture	CPCONLY	F16C2314/70		105
F16C2314/72	9	Drawers	CPCONLY	F16C2314/72		140
F16C2314/73	9	Chairs	CPCONLY	F16C2314/73		29
F16C2316/00	7	Apparatus in health or amusement	CPCONLY	F16C2316/00		17
F16C2316/10	8	in medical appliances, e.g. in diagnosis, dentistry, instruments, prostheses, medical imaging appliances	CPCONLY	F16C2316/10		452
F16C2316/13	9	Dental machines	CPCONLY	F16C2316/13		277
F16C2316/18	9	Pumps for pumping blood	CPCONLY	F16C2316/18		131
F16C2316/30	8	Articles for sports, games and amusement, e.g. roller skates, toys	CPCONLY	F16C2316/30		228
F16C2320/00	7	Apparatus used in separating or mixing	CPCONLY	F16C2320/00		36
F16C2320/16	8	Mixing apparatus	CPCONLY	F16C2320/16		38
F16C2320/23	8	Milling apparatus	CPCONLY	F16C2320/23		77
F16C2320/42	8	Centrifuges	CPCONLY	F16C2320/42		47
F16C2322/00	7	Apparatus used in shaping articles	CPCONLY	F16C2322/00		234
F16C2322/12	8	Rolling apparatus, e.g. rolling stands, rolls	CPCONLY	F16C2322/12		698
F16C2322/14	8	Stamping, deep-drawing or punching, e.g. die sets	CPCONLY	F16C2322/14		95
F16C2322/34	8	Sawing machines	CPCONLY	F16C2322/34		21
F16C2322/39	8	General buildup of machine tools, e.g. spindles, slides, actuators	CPCONLY	F16C2322/39		2969
F16C2322/50	8	Hand tools, workshop equipment or manipulators	CPCONLY	F16C2322/50		95
F16C2322/59	9	Manipulators, e.g. robot arms	CPCONLY	F16C2322/59		176
F16C2324/00	7	Apparatus used in printing	CPCONLY	F16C2324/00		11
F16C2324/16	8	Printing machines	CPCONLY	F16C2324/16		95
F16C2326/00	7	Articles relating to transporting	CPCONLY	F16C2326/00		255
F16C2326/01	8	Parts of vehicles in general	CPCONLY	F16C2326/01		1030
F16C2326/02	9	Wheel hubs or castors	CPCONLY	F16C2326/02		6685
F16C2326/05	9	Vehicle suspensions, e.g. bearings, pivots or connecting rods used therein	CPCONLY	F16C2326/05		2064
F16C2326/06	9	Drive shafts	CPCONLY	F16C2326/06		1092
F16C2326/08	9	Vehicle seats, e.g. in linear movable seats	CPCONLY	F16C2326/08		121
F16C2326/09	9	Windscreen wipers, e.g. pivots therefore	CPCONLY	F16C2326/09		393
F16C2326/10	8	Railway vehicles	CPCONLY	F16C2326/10		1314
F16C2326/20	8	Land vehicles	CPCONLY	F16C2326/20		747
F16C2326/24	9	Steering systems, e.g. steering rods or columns	CPCONLY	F16C2326/24		2173
F16C2326/26	9	Bicycle steering or suspension	CPCONLY	F16C2326/26		116
F16C2326/28	9	Bicycle propulsion, e.g. crankshaft and its support	CPCONLY	F16C2326/28		391
F16C2326/30	8	Ships, e.g. propelling shafts and bearings therefor	CPCONLY	F16C2326/30		831
F16C2326/43	8	Aeroplanes; Helicopters	CPCONLY	F16C2326/43		1044
F16C2326/47	8	Cosmonautic vehicles, i.e. bearings adapted for use in outer-space	CPCONLY	F16C2326/47		213
F16C2326/58	8	Conveyor systems, e.g. rollers or bearings therefor	CPCONLY	F16C2326/58		788
F16C2340/00	7	Apparatus for treating textiles	CPCONLY	F16C2340/00		626
F16C2340/18	8	Apparatus for spinning or twisting	CPCONLY	F16C2340/18		501
F16C2340/24	8	Godet rolls	CPCONLY	F16C2340/24		35
F16C2350/00	7	Machines or articles related to building	CPCONLY	F16C2350/00		349
F16C2350/26	8	Excavators	CPCONLY	F16C2350/26		880
F16C2350/52	8	Locks, e.g. cables to actuate door locks	CPCONLY	F16C2350/52		201
F16C2350/54	8	Hinges, e.g. sliding bearings for hinges	CPCONLY	F16C2350/54		95
F16C2352/00	7	Apparatus for drilling	CPCONLY	F16C2352/00		827
F16C2360/00	7	Engines or pumps	CPCONLY	F16C2360/00		1038
F16C2360/18	8	Camshafts	CPCONLY	F16C2360/18		355
F16C2360/22	8	Internal combustion engines	CPCONLY	F16C2360/22		1630
F16C2360/23	8	Gas turbine engines	CPCONLY	F16C2360/23		1768
F16C2360/24	9	Turbochargers	CPCONLY	F16C2360/24		1813
F16C2360/31	8	Wind motors	CPCONLY	F16C2360/31		1942
F16C2360/42	8	Pumps with cylinders or pistons	CPCONLY	F16C2360/42		913
F16C2360/43	8	Screw compressors	CPCONLY	F16C2360/43		152
F16C2360/44	8	Centrifugal pumps	CPCONLY	F16C2360/44		1148
F16C2360/45	9	Turbo-molecular pumps	CPCONLY	F16C2360/45		944
F16C2360/46	8	Fans, e.g. ventilators	CPCONLY	F16C2360/46		298
F16C2361/00	7	Apparatus or articles in engineering in general	CPCONLY	F16C2361/00		185
F16C2361/31	8	Axle	CPCONLY	F16C2361/31		198
F16C2361/41	8	Couplings	CPCONLY	F16C2361/41		722
F16C2361/43	8	Clutches, e.g. disengaging bearing	CPCONLY	F16C2361/43		959
F16C2361/45	8	Brakes	CPCONLY	F16C2361/45		266
F16C2361/53	8	Spring-damper, e.g. gas springs	CPCONLY	F16C2361/53		179
F16C2361/55	8	Flywheel systems	CPCONLY	F16C2361/55		599
F16C2361/61	8	Toothed gear systems, e.g. support of pinion shafts	CPCONLY	F16C2361/61		3549
F16C2361/63	8	Gears with belts and pulleys	CPCONLY	F16C2361/63		827
F16C2361/65	8	Gear shifting, change speed gear, gear box	CPCONLY	F16C2361/65		677
F16C2361/71	8	Chains	CPCONLY	F16C2361/71		21
F16C2361/91	8	Valves	CPCONLY	F16C2361/91		99
F16C2362/00	7	Apparatus for lighting or heating	CPCONLY	F16C2362/00		60
F16C2362/40	8	Ovens or other heatings	CPCONLY	F16C2362/40		23
F16C2362/52	8	Compressors of refrigerators, e.g. air-conditioners	CPCONLY	F16C2362/52		226
F16C2370/00	7	Apparatus relating to physics, e.g. instruments	CPCONLY	F16C2370/00		1078
F16C2370/12	8	Hard disk drives or the like	CPCONLY	F16C2370/12		2022
F16C2370/20	8	Optical, e.g. movable lenses or mirrors; Spectacles	CPCONLY	F16C2370/20		108
F16C2370/22	9	Polygon mirror	CPCONLY	F16C2370/22		38
F16C2370/38	8	Electrographic apparatus	CPCONLY	F16C2370/38		29
F16C2380/00	7	Electrical apparatus	CPCONLY	F16C2380/00		351
F16C2380/16	8	X-ray tubes	CPCONLY	F16C2380/16		95
F16C2380/18	8	Handling tools for semiconductor devices	CPCONLY	F16C2380/18		33
F16C2380/26	8	Dynamo-electric machines or combinations therewith, e.g. electro-motors and generators	CPCONLY	F16C2380/26		3618
F16C2380/27	9	Motor coupled with a gear, e.g. worm gears	CPCONLY	F16C2380/27		381
F16C2380/28	9	Motor, generator coupled with a flywheel	CPCONLY	F16C2380/28		64
