B67C3/00	7	Bottling liquids or semiliquids; Filling jars or cans with liquids or semiliquids using bottling or like apparatus; Filling casks or barrels with liquids or semiliquids	B67C3/00	B67C3/00		225
B67C3/001	8	{Cleaning of filling devices}	B67C3/00	B67C3/00		586
B67C3/002	9	{using cups or dummies to be placed under the filling heads}	B67C3/00	B67C3/00		115
B67C3/004	10	{permanently attached to the filling machine and movable between a rest and a working position}	B67C3/00	B67C3/00		130
B67C3/005	9	{Cleaning outside parts of filling devices}	B67C3/00	B67C3/00		106
B67C3/007	8	{Applications of control, warning or safety devices in filling machinery (flow-control B67C3/28)}	B67C3/00	B67C3/00		1035
B67C3/008	8	{Bottling or like apparatus specially adapted to be transported, e.g. positioned on a truck or in a container}	B67C3/00	B67C3/00		38
B67C3/02	8	Bottling liquids or semiliquids; Filling jars or cans with liquids or semiliquids using bottling or like apparatus	B67C3/02	B67C3/02		709
B67C3/023	9	{Filling multiple liquids in a container (B67C3/208 takes precedence)}	B67C3/02	B67C3/02		134
B67C3/026	10	{Filling the liquids simultaneously}	B67C3/02	B67C3/02		60
B67C3/04	9	without applying pressure	B67C3/04	B67C3/04		506
B67C3/045	10	{Apparatus specially adapted for filling bottles with hot liquids}	B67C3/04	B67C3/04		127
B67C3/06	9	using counterpressure, i.e. filling while the container is under pressure	B67C3/06	B67C3/06		681
B67C3/065	10	{Filling siphons, e.g. carbonating beverages during filling (siphons B67D1/0456)}	B67C3/06	B67C3/06		106
B67C3/08	10	and subsequently lowering the counterpressure	B67C3/08	B67C3/08		106
B67C3/10	10	preliminary filling with inert gases, e.g. carbon dioxide	B67C3/10	B67C3/10		373
B67C3/12	10	Pressure-control devices	B67C3/12	B67C3/12		199
B67C3/14	10	specially adapted for filling with hot liquids	B67C3/14	B67C3/14		51
B67C3/16	9	using suction	B67C3/16	B67C3/16		622
B67C3/18	9	using siphoning arrangements	B67C3/18	B67C3/18		153
B67C3/20	9	with provision for metering the liquids to be introduced, e.g. when adding syrups (measuring volume, or volume flow, in general G01F)	B67C3/20	B67C3/20		314
B67C3/202	10	{by weighing}	B67C3/20	B67C3/20		273
B67C3/204	10	{using dosing chambers}	B67C3/20	B67C3/20		218
B67C3/206	10	{using arrangements of cylinders and pistons (B67C3/208 takes precedence)}	B67C3/20	B67C3/20		218
B67C3/208	10	{specially adapted for adding small amounts of additional liquids, e.g. syrup}	B67C3/20	B67C3/20		138
B67C3/22	9	Details	B67C3/22	B67C3/22		3300
B67C2003/221	10	{Automatic exchange of components}	B67C3/22	B67C3/22		26
B67C3/222	10	{Head-space air removing devices, e.g. by inducing foam}	B67C3/22	B67C3/22		330
B67C3/223	11	{by squeezing the container elastically}	B67C3/22	B67C3/22		29
B67C3/225	10	{Means for filling simultaneously, e.g. in a rotary filling apparatus or multiple rows of containers}	B67C3/22	B67C3/22		248
B67C2003/226	10	{Additional process steps or apparatuses related to filling with hot liquids, e.g. after-treatment}	B67C3/22	B67C3/22		141
B67C2003/227	10	{Additional apparatus related to blow-moulding of the containers, e.g. a complete production line forming filled containers from preforms}	B67C3/22	B67C3/22		265
B67C2003/228	10	{Aseptic features}	B67C3/22	B67C3/22		399
B67C3/24	10	Devices for supporting or handling bottles (transport or storing devices in general B65G)	B67C3/24	B67C3/24		3573
B67C3/242	11	{engaging with bottle necks (B67C3/26 takes precedence)}	B67C3/24	B67C3/24		345
B67C3/244	11	{Bottle lifting devices actuated by jacks, e.g. hydraulic, pneumatic (B67C3/242 takes precedence)}	B67C3/24	B67C3/24		136
B67C3/246	11	{Bottle lifting devices actuated by cams (B67C3/242 takes precedence)}	B67C3/24	B67C3/24		164
B67C3/248	11	{Bottle lifting devices actuated by threads (B67C3/242 takes precedence)}	B67C3/24	B67C3/24		3
B67C3/26	10	Filling-heads; Means for engaging filling-heads with bottle necks	B67C3/26	B67C3/26		3725
B67C2003/2602	11	{Details of vent-tubes}	B67C3/26	B67C3/26		117
B67C2003/2605	12	{Piston-like check valves}	B67C3/26	B67C3/26		15
B67C3/2608	11	{comprising anti-dripping means}	B67C3/26	B67C3/26		488
B67C3/2611	12	{to prevent dripping from sources other than the filling product, e.g. deflectors for vapours condensed on the outer surface of the filling device}	B67C3/26	B67C3/26		15
B67C3/2614	11	{specially adapted for counter-pressure filling}	B67C3/26	B67C3/26		414
B67C3/2617	12	{the liquid valve being opened by mechanical or electrical actuation}	B67C3/26	B67C3/26		143
B67C3/262	13	{and the filling operation stopping when the liquid rises to a level at which it closes a vent opening}	B67C3/26	B67C3/26		126
B67C3/2622	13	{and the filling operation stopping when probes, e.g. electrical or optical probes, sense the wanted liquid level (level control in general G01F)}	B67C3/26	B67C3/26		55
B67C3/2625	12	{the liquid valve being opened automatically when a given counter-pressure is obtained in the container to be filled}	B67C3/26	B67C3/26		10
B67C3/2628	13	{and the filling operation stopping when the liquid rises to a level at which it closes a vent opening}	B67C3/26	B67C3/26		198
B67C3/2631	13	{and the filling operation stopping when probes, e.g. electrical or optical probes, sense the wanted liquid level (level control in general G01F)}	B67C3/26	B67C3/26		25
B67C3/2634	11	{specially adapted for vacuum or suction filling}	B67C3/26	B67C3/26		288
B67C3/2637	11	{comprising a liquid valve opened by relative movement between the container and the filling head}	B67C3/26	B67C3/26		461
B67C3/264	12	{and the filling operation being carried out manually}	B67C3/26	B67C3/26		90
B67C3/2642	11	{specially adapted for sterilising prior to filling}	B67C3/26	B67C3/26		118
B67C2003/2645	11	{Means to avoid overfilling by preventing gas returning from the container into the filling tank via the liquid valve, e.g. mesh screens}	B67C3/26	B67C3/26		66
B67C2003/2648	11	{Inflatable gaskets for sealingly engaging bottle necks or bodies}	B67C3/26	B67C3/26		41
B67C2003/2651	11	{The liquid valve being carried by the vent tube}	B67C3/26	B67C3/26		124
B67C2003/2654	12	{specially adapted for bottom filling, e.g. the liquid valve being located at the lowest part of the vent tube}	B67C3/26	B67C3/26		33
B67C2003/2657	11	{specially adapted for filling cans}	B67C3/26	B67C3/26		224
B67C2003/266	11	{Means for centering the container with the filling head}	B67C3/26	B67C3/26		146
B67C2003/2662	12	{with means for detecting the presence of a container}	B67C3/26	B67C3/26		24
B67C2003/2665	11	{Means for locking the filling head in a given position once engaged by a container}	B67C3/26	B67C3/26		12
B67C2003/2668	11	{Means for adapting the filling head to various sizes of containers}	B67C3/26	B67C3/26		275
B67C2003/2671	11	{Means for preventing foaming of the liquid}	B67C3/26	B67C3/26		308
B67C2003/2674	12	{by creating a conical shaped flow directed to the container wall at the container neck height}	B67C3/26	B67C3/26		6
B67C2003/2677	13	{by means of a deflector}	B67C3/26	B67C3/26		45
B67C2003/268	13	{by means of a flow channel integral with the filling nozzle}	B67C3/26	B67C3/26		68
B67C2003/2682	12	{by creating a conical shaped flow directed to the container wall just above the container bottom}	B67C3/26	B67C3/26		6
B67C2003/2685	11	{Details of probes}	B67C3/26	B67C3/26		159
B67C2003/2688	11	{Means for filling containers in defined atmospheric conditions}	B67C3/26	B67C3/26		43
B67C2003/2691	12	{by enclosing one container in a chamber}	B67C3/26	B67C3/26		38
B67C2003/2694	12	{by enclosing a set of containers in a chamber}	B67C3/26	B67C3/26		53
B67C2003/2697	12	{by enclosing the container partly in a chamber}	B67C3/26	B67C3/26		69
B67C3/28	10	Flow-control devices, e.g. using valves ({B67C3/2617, B67C3/2625, B67C3/2637 take precedence}; valves in general F16K)	B67C3/28	B67C3/28		1500
B67C3/281	11	{Profiled valve bodies for smoothing the flow at the outlet of the filling nozzle}	B67C3/28	B67C3/28		125
B67C3/282	11	{related to filling level control (B67C3/2617, B67C3/2625 take precedence)}	B67C3/28	B67C3/28		115
B67C3/283	12	{using pressure sensing means}	B67C3/28	B67C3/28		44
B67C3/284	12	{using non-liquid contact sensing means (B67C3/283 takes precedence)}	B67C3/28	B67C3/28		71
B67C3/285	12	{using liquid contact sensing means (B67C3/283 takes precedence)}	B67C3/28	B67C3/28		88
B67C3/286	11	{related to flow rate control, i.e. controlling slow and fast filling phases}	B67C3/28	B67C3/28		259
B67C3/287	11	{related to flow control using predetermined or real-time calculated parameters}	B67C3/28	B67C3/28		134
B67C3/288	12	{using leader-follower controls}	B67C3/28	B67C3/28		21
B67C3/30	8	Filling of barrels or casks	B67C3/30	B67C3/30		926
B67C3/32	9	using counterpressure, i.e. filling while the container is under pressure	B67C3/32	B67C3/32		130
B67C3/34	9	Devices for engaging filling-heads with filling-apertures	B67C3/34	B67C3/34		160
B67C7/00	7	Concurrent cleaning, filling, and closing of bottles; Processes or devices for at least two of these operations	B67C7/00	B67C7/00		1461
B67C7/0006	8	{Conveying; Synchronising}	B67C7/00	B67C7/00		513
B67C7/0013	9	{Synchronising}	B67C7/00	B67C7/00		114
B67C7/002	9	{General lay-out of bottle-handling machines}	B67C7/00	B67C7/00		228
B67C7/0026	9	{the containers travelling along a linear path}	B67C7/00	B67C7/00		423
B67C7/0033	10	{the operation being performed batch-wise}	B67C7/00	B67C7/00		113
B67C7/004	9	{the containers travelling along a circular path}	B67C7/00	B67C7/00		348
B67C7/0046	10	{Infeed and outfeed devices}	B67C7/00	B67C7/00		383
B67C7/0053	11	{using grippers (for supporting bottle necks during filling B67C3/242)}	B67C7/00	B67C7/00		144
B67C2007/006	9	{Devices particularly adapted for container filling}	B67C7/00	B67C7/00		866
B67C2007/0066	9	{Devices particularly adapted for container closing}	B67C7/00	B67C7/00		790
B67C7/0073	8	{Sterilising, aseptic filling and closing (B67C3/2642 takes precedence)}	B67C7/00	B67C7/00		984
B67C7/008	9	{comprising a cleaning step between two closing steps}	B67C7/00	B67C7/00		32
B67C7/0086	9	{Sterilisation being restricted to the area of application of the closure}	B67C7/00	B67C7/00		59
B67C7/0093	8	{Lever action devices operated by hand or foot}	B67C7/00	B67C7/00		62
B67C9/00	7	Devices for emptying bottles, not otherwise provided for {(during preparation of alcoholic beverages except beer C12G1/00)}	B67C9/00	B67C9/00		625
B67C11/00	7	Funnels, e.g. for liquids (filter funnels B01D29/085; volume flow-meters G01F)	B67C11/00	B67C11/00		267
B67C11/02	8	without discharge valves	B67C11/02	B67C11/02		1242
B67C2011/022	9	{for draining oil from engines}	B67C11/02	B67C11/02		32
B67C2011/025	10	{with integral tool for opening the draining plug}	B67C11/02	B67C11/02		21
B67C2011/027	9	{for filling oil into engines}	B67C11/02	B67C11/02		71
B67C11/04	8	with non-automatic discharge valves	B67C11/04	B67C11/04		362
B67C11/06	8	with automatic discharge valves	B67C11/06	B67C11/06		14
B67C11/063	9	{for preventing spilling or dripping}	B67C11/06	B67C11/06		158
B67C11/066	9	{for preventing overflow of the filled container}	B67C11/06	B67C11/06		185
B67C2011/20	8	{comprising closures, e.g. stoppers, caps or lids}	B67C11/00	B67C2011/20		111
B67C2011/30	8	{comprising venting means}	B67C11/00	B67C2011/30		264
B67C2011/40	8	{comprising level indicating means}	B67C11/00	B67C2011/40		77
