A62C2/00	7	Fire prevention or containment (A62C3/00 takes precedence; flame traps A62C4/00)	A62C2/00	A62C2/00		332
A62C2/04	8	Removing or cutting-off the supply of inflammable material	A62C2/04	A62C2/04		614
A62C2/06	8	Physical fire-barriers	A62C2/06	A62C2/06		1723
A62C2/065	9	{having as the main closure device materials, whose characteristics undergo an irreversible change under high temperatures, e.g. intumescent}	A62C2/06	A62C2/06		1029
A62C2/08	9	Water curtains (nozzles A62C31/02)	A62C2/08	A62C2/08		414
A62C2/10	9	Fire-proof curtains	A62C2/10	A62C2/10		1002
A62C2/12	9	Hinged dampers	A62C2/12	A62C2/12		747
A62C2/14	10	with two or more blades	A62C2/14	A62C2/14		272
A62C2/16	11	multi-vane roll or fold-up type	A62C2/16	A62C2/16		269
A62C2/18	9	Sliding dampers	A62C2/18	A62C2/18		427
A62C2/20	10	at 90 degrees to the plane of the opening	A62C2/20	A62C2/20		79
A62C2/22	9	Fire-dampers with provision for the removal of an obstacle, e.g. rails, conveyors, before closing the opening	A62C2/22	A62C2/22		104
A62C2/24	9	Operating or controlling mechanisms {(emergency operation of doors and windows E05F1/002, E05F15/72)}	A62C2/24	A62C2/24		762
A62C2/241	10	{having mechanical actuators and heat sensitive parts}	A62C2/24	A62C2/24		254
A62C2/242	11	{with fusible links}	A62C2/24	A62C2/24		257
A62C2/243	11	{with frangible elements}	A62C2/24	A62C2/24		33
A62C2/245	11	{with thermostatic elements, e.g. bimetallic, resettable actuators}	A62C2/24	A62C2/24		62
A62C2/246	10	{having non-mechanical actuators}	A62C2/24	A62C2/24		47
A62C2/247	11	{electric}	A62C2/24	A62C2/24		376
A62C2/248	11	{pneumatic}	A62C2/24	A62C2/24		127
A62C3/00	7	Fire prevention, containment or extinguishing specially adapted for particular objects or places ({in oil wells E21B29/08, A62C35/00; in mines or tunnels E21F5/00} ; for nuclear reactors G21C9/04)	A62C3/00	A62C3/00		1707
A62C3/002	8	{for warehouses, storage areas or other installations for storing goods}	A62C3/00	A62C3/00		619
A62C3/004	9	{for freezing warehouses and storages}	A62C3/00	A62C3/00		142
A62C3/006	8	{for kitchens or stoves}	A62C3/00	A62C3/00		644
A62C3/008	8	{for decorations, e.g. Christmas trees (Christmas tree decorations incorporating fire extinguishing or fire prevention means A47G33/0872; blowing or snuffing out candle-flames F23Q25/00)}	A62C3/00	A62C3/00		30
A62C3/02	8	for area conflagrations, e.g. forest fires, subterranean fires	A62C3/02	A62C3/02		1221
A62C3/0207	9	{by blowing air or gas currents with or without dispersion of fire extinguishing agents; Apparatus therefor, e.g. fans}	A62C3/02	A62C3/02		351
A62C3/0214	9	{for buildings or installations in fire storms}	A62C3/02	A62C3/02		673
A62C3/0221	9	{for tunnels}	A62C3/02	A62C3/02		484
A62C3/0228	9	{with delivery of fire extinguishing material by air or aircraft (fire-fighting aircraft B64D1/16)}	A62C3/02	A62C3/02		319
A62C3/0235	10	{by means of containers, e.g. buckets}	A62C3/02	A62C3/02		242
A62C3/0242	10	{by spraying extinguishants from the aircraft (spraying from aircraft in general B64D1/16)}	A62C3/02	A62C3/02		673
A62C3/025	10	{Fire extinguishing bombs; Projectiles and launchers therefor (launching apparatus for projectiles, missiles or torpedoes in general F41F1/00, F41F3/00, F41F7/00)}	A62C3/02	A62C3/02		713
A62C3/0257	9	{Fire curtains, blankets, walls, fences}	A62C3/02	A62C3/02		258
A62C3/0264	10	{by creating water curtains}	A62C3/02	A62C3/02		91
A62C3/0271	9	{Detection of area conflagration fires (fire alarms for forest fires G08B17/005)}	A62C3/02	A62C3/02		324
A62C3/0278	9	{by creating zones devoid of flammable material}	A62C3/02	A62C3/02		116
A62C3/0285	10	{with creation of a fire zone by an explosion or a counter-fire}	A62C3/02	A62C3/02		40
A62C3/0292	9	{by spraying extinguishants directly into the fire (A62C3/0242 takes precedence)}	A62C3/02	A62C3/02		566
A62C3/04	8	for dust or loosely-baled or loosely-piled materials, e.g. in silos, in chimneys (flame traps A62C4/00)	A62C3/04	A62C3/04		467
A62C3/06	8	of highly inflammable material, e.g. light metals, petroleum products	A62C3/06	A62C3/06		1681
A62C3/065	9	{for containers filled with inflammable liquids}	A62C3/06	A62C3/06		536
A62C3/07	8	in vehicles, e.g. in road vehicles	A62C3/07	A62C3/07		3633
A62C3/08	9	in aircraft {(A62C3/0207 takes precedence)}	A62C3/08	A62C3/08		886
A62C3/10	9	in ships {(A62C3/0207 takes precedence)}	A62C3/10	A62C3/10		999
A62C3/14	8	{in connection with doors, windows, ventilators, partitions, or shutters, e.g. automatic closing}	A62C2/06	A62C3/14		507
A62C3/16	8	in electrical installations, e.g. cableways	A62C3/16	A62C3/16		11915
A62C4/00	7	Flame traps allowing passage of gas but not of flame or explosion wave	A62C4/00	A62C4/00		691
A62C4/02	8	in gas-pipes (safety valves F16K17/00)	A62C4/02	A62C4/02		967
A62C4/04	8	in flues or chimneys	A62C4/04	A62C4/04		94
A62C5/00	7	Making of fire-extinguishing materials immediately before use (nozzles A62C31/02)	A62C5/00	A62C5/00		276
A62C5/002	8	{Apparatus for mixing extinguishants with water}	A62C5/00	A62C5/00		1045
A62C5/004	8	{for producing carbon-dioxide snow, carbon-dioxide ice, carbon-dioxide gas, carbon-dioxide liquid, or mixtures thereof (carbon-dioxide jet-pipes or snow jet-pipes A62C31/03)}	A62C5/00	A62C5/00		166
A62C5/006	8	{Extinguishants produced by combustion}	A62C5/00	A62C5/00		244
A62C5/008	8	{for producing other mixtures of different gases or vapours, water and chemicals, e.g. water and wetting agents, water and gases}	A62C5/00	A62C5/00		205
A62C5/02	8	of foam	A62C5/02	A62C5/02		1159
A62C5/022	9	{with air or gas present as such}	A62C5/02	A62C5/02		141
A62C5/024	10	{Apparatus in the form of pipes (jet-pipes for foam A62C31/12)}	A62C5/02	A62C5/02		89
A62C5/027	9	Heavy foam	A62C5/027	A62C5/027		10
A62C5/033	8	of gel	A62C5/033	A62C5/033		94
A62C8/00	7	Hand tools or accessories specially adapted for fire-fighting, e.g. tool boxes	A62C8/00	A62C8/00		439
A62C8/005	8	{Receptacles or other utensils for water carrying; Bombs filled with extinguishing agents}	A62C8/00	A62C8/00		265
A62C8/02	8	Buckets or pails	A62C8/02	A62C8/02		49
A62C8/04	8	Rakes or beaters	A62C8/04	A62C8/04		81
A62C8/06	8	Fire-blankets	A62C8/06	A62C8/06		501
A62C8/08	8	Shields	A62C8/08	A62C8/08		87
A62C11/00	7	Portable extinguishers with manually-operated pumps	A62C11/00	A62C11/00		84
A62C11/005	8	{Receptacles of extinguishing agent with manually operable pump}	A62C11/00	A62C11/00		315
A62C13/00	7	Portable extinguishers which are permanently pressurised or pressurised immediately before use (A62C11/00 takes precedence)	A62C13/00	A62C13/00		336
A62C13/003	8	{Extinguishers with spraying and projection of extinguishing agents by pressurised gas}	A62C13/00	A62C13/00		2324
A62C13/006	8	{for the propulsion of extinguishing powder}	A62C13/00	A62C13/00		512
A62C13/02	8	with pressure gas produced by chemicals	A62C13/02	A62C13/02		34
A62C13/04	9	with separate acid container	A62C13/04	A62C13/04		23
A62C13/06	10	with acid container without closure device	A62C13/06	A62C13/06		3
A62C13/08	10	with acid container with closure device	A62C13/08	A62C13/08		8
A62C13/10	11	with loose-lid closure device (loosely-engaging lids or covers for containers for liquids without means for effecting sealing of container in general B65D51/02)	A62C13/10	A62C13/10		2
A62C13/12	11	with valve closure device	A62C13/12	A62C13/12		9
A62C13/14	10	with acid container the shell of which is ruptured by pin, screw-pin, or similar device	A62C13/14	A62C13/14		30
A62C13/16	10	with movable acid container ruptured by falling when operated	A62C13/16	A62C13/16		3
A62C13/18	10	with acid container ruptured by a striking weight, e.g. by a falling weight	A62C13/18	A62C13/18		2
A62C13/20	9	with the chemicals in a single case, e.g. in a cartridge	A62C13/20	A62C13/20		24
A62C13/22	9	with incendiary substances producing pressure gas	A62C13/22	A62C13/22		197
A62C13/62	8	with a single permanently pressurised container	A62C13/62	A62C13/62		303
A62C13/64	9	the extinguishing material being released by means of a valve	A62C13/64	A62C13/64		551
A62C13/66	8	with extinguishing material and pressure gas being stored in separate containers	A62C13/66	A62C13/66		265
A62C13/68	9	characterised by means for releasing the extinguishing material	A62C13/68	A62C13/68		104
A62C13/70	9	characterised by means for releasing the pressure gas	A62C13/70	A62C13/70		186
A62C13/72	9	characterised by releasing means operating essentially simultaneously on both containers	A62C13/72	A62C13/72		45
A62C13/74	10	the pressure gas container being pierced or broken	A62C13/74	A62C13/74		126
A62C13/76	8	Details or accessories	A62C13/76	A62C13/76		1979
A62C13/78	9	Suspending or supporting devices	A62C13/78	A62C13/78		1247
A62C15/00	7	Extinguishers essentially of the knapsack type (knapsacks, carrying-frames, pack-frames carried on the body A45F3/00)	A62C15/00	A62C15/00		222
A62C17/00	7	Hand fire-extinguishers essentially in the form of pistols or rifles	A62C17/00	A62C17/00		191
A62C19/00	7	Hand fire-extinguishers in which the extinguishing substance is expelled by an explosion; Exploding containers thrown into the fire	A62C19/00	A62C19/00		1039
A62C25/00	7	Portable extinguishers with power-driven pumps	A62C25/00	A62C25/00		169
A62C25/005	8	{Accessories}	A62C25/00	A62C25/00		231
A62C27/00	7	Fire-fighting land vehicles	A62C27/00	A62C27/00		4807
A62C29/00	7	Fire-fighting vessels or like floating structures	A62C29/00	A62C29/00		121
A62C31/00	7	Delivery of fire-extinguishing material (pumps F04; {suction or pressure} hoses, {joints or couplings therefor}F16L)	A62C31/00	A62C31/00		4596
A62C31/005	8	{using nozzles}<br><br><u>WARNING</u><br><br>see warning after subclass title	A62C31/00	A62C31/00		3038
A62C31/02	8	Nozzles specially adapted for fire-extinguishing	A62C31/02	A62C31/02		4769
A62C31/03	9	adjustable, e.g. from spray to jet or vice versa	A62C31/03	A62C31/03		2276
A62C31/05	9	with two or more outlets	A62C31/05	A62C31/05		1669
A62C31/07	10	for different media	A62C31/07	A62C31/07		171
A62C31/12	9	for delivering foam or atomised foam	A62C31/12	A62C31/12		1041
A62C31/22	9	specially adapted for piercing walls, heaped materials, or the like	A62C31/22	A62C31/22		352
A62C31/24	9	attached to ladders, poles, towers, or other structures with or without rotary heads	A62C31/24	A62C31/24		903
A62C31/28	8	Accessories for delivery devices, e.g. supports	A62C31/28	A62C31/28		7493
A62C33/00	7	Hose accessories	A62C33/00	A62C33/00		839
A62C33/02	8	Apparatus for cleaning or drying hoses (drying shelves F26B)	A62C33/02	A62C33/02		473
A62C33/04	8	Supports or clamps for fire hoses	A62C33/04	A62C33/04		1206
A62C33/06	8	Hose or pipe bridges	A62C33/06	A62C33/06		466
A62C35/00	7	Permanently-installed equipment (A62C31/00, A62C33/00, A62C37/00 take precedence; for forming water curtains A62C2/08)	A62C35/00	A62C35/00		412
A62C35/02	8	with containers for delivering the extinguishing substance	A62C35/02	A62C35/02		1011
A62C35/023	9	{the extinguishing material being expelled by compressed gas, taken from storage tanks, or by generating a pressure gas (for foam generation A62C5/02)}	A62C35/02	A62C35/02		909
A62C35/026	9	{the extinguishing material being put under pressure by means other than pressure gas, e.g. pumps}	A62C35/02	A62C35/02		266
A62C35/04	9	Swingable or tiltable containers	A62C35/04	A62C35/04		25
A62C35/06	9	Containers destroyed or opened by falling	A62C35/06	A62C35/06		57
A62C35/08	9	Containers destroyed or opened by bursting charge	A62C35/08	A62C35/08		343
A62C35/10	9	Containers destroyed or opened by flames or heat	A62C35/10	A62C35/10		1146
A62C35/11	9	controlled by a signal from the danger zone	A62C35/11	A62C35/11		270
A62C35/13	10	with a finite supply of extinguishing material	A62C35/13	A62C35/13		344
A62C35/15	10	with a system for topping-up the supply of extinguishing material automatically	A62C35/15	A62C35/15		85
A62C35/20	8	Hydrants, e.g. wall-hoses, wall units, plug-in cabinets (hydrants in streets E03B9/02)	A62C35/20	A62C35/20		1551
A62C35/58	8	Pipe-line systems	A62C35/58	A62C35/58		854
A62C35/60	9	wet, i.e. containing extinguishing material even when not in use	A62C35/60	A62C35/60		401
A62C35/605	10	{operating and sounding alarm automatically}<br><br><u>WARNING</u><br><br>see warning after subclass title	A62C35/60	A62C35/60		1367
A62C35/62	9	dry, i.e. empty of extinguishing material when not in use	A62C35/62	A62C35/62		428
A62C35/64	9	pressurised	A62C35/64	A62C35/64		284
A62C35/645	10	{with compressed gas in pipework}<br><br><u>WARNING</u><br><br>see warning after subclass title	A62C35/64	A62C35/64		709
A62C35/66	10	Accelerators	A62C35/66	A62C35/66		55
A62C35/68	9	Details, e.g. of pipes or valve systems (valves in general F16K)	A62C35/68	A62C35/68		4016
A62C37/00	7	Control of fire-fighting equipment (heat-sensitive devices G01K)	A62C37/00	A62C37/00		4389
A62C37/04	8	{with electrically-controlled release}	A62C37/36	A62C37/04		1385
A62C37/08	8	comprising an outlet device containing a sensor, or itself being the sensor, i.e. self-contained sprinklers	A62C37/08	A62C37/08		888
A62C37/09	9	telescopic or adjustable	A62C37/09	A62C37/09		388
A62C37/10	9	Releasing means, e.g. electrically released	A62C37/10	A62C37/10		888
A62C37/11	10	heat-sensitive	A62C37/11	A62C37/11		1367
A62C37/12	11	with fusible links	A62C37/12	A62C37/12		1056
A62C37/14	11	with frangible vessels	A62C37/14	A62C37/14		959
A62C37/16	11	with thermally-expansible links	A62C37/16	A62C37/16		169
A62C37/20	9	Resetting after use; Tools therefor	A62C37/20	A62C37/20		103
A62C37/21	10	automatic	A62C37/21	A62C37/21		51
A62C37/36	8	an actuating signal being generated by a sensor separate from an outlet device	A62C37/36	A62C37/36		1736
A62C37/38	9	by both sensor and actuator, e.g. valve, being in the danger zone	A62C37/38	A62C37/38		1912
A62C37/40	10	with electric connection between sensor and actuator	A62C37/40	A62C37/40		3559
A62C37/42	10	with mechanical connection between sensor and actuator, e.g. rods, levers	A62C37/42	A62C37/42		435
A62C37/44	9	only the sensor being in the danger zone	A62C37/44	A62C37/44		280
A62C37/46	9	Construction of the actuator	A62C37/46	A62C37/46		345
A62C37/48	10	Thermally sensitive initiators	A62C37/48	A62C37/48		214
A62C37/50	8	Testing or indicating devices for determining the state of readiness of the equipment	A62C37/50	A62C37/50		2583
A62C99/00	7	Subject matter not provided for in other groups of this subclass	A62C99/00	A62C99/00		368
A62C99/0009	8	{Methods of extinguishing or preventing the spread of fire by cooling down or suffocating the flames}	A62C99/00	A62C99/00		405
A62C99/0018	9	{using gases or vapours that do not support combustion, e.g. steam, carbon dioxide}	A62C99/00	A62C99/00		1255
A62C99/0027	10	{Carbon dioxide extinguishers}	A62C99/00	A62C99/00		1019
A62C99/0036	9	{using foam}	A62C99/00	A62C99/00		275
A62C99/0045	9	{using solid substances, e.g. sand, ashes; using substances forming a crust}	A62C99/00	A62C99/00		545
A62C99/0054	9	{using counter-fire}	A62C99/00	A62C99/00		34
A62C99/0063	9	{with simultaneous removal of inflammable materials}	A62C99/00	A62C99/00		38
A62C99/0072	9	{using sprayed or atomised water}	A62C99/00	A62C99/00		1212
A62C99/0081	8	{Training methods or equipment for fire-fighting}	A62C99/00	A62C99/00		773
A62C99/009	8	{Methods or equipment not provided for in groups A62C99/0009&#160;-&#160;A62C99/0081}	A62C99/00	A62C99/00		933
