H04J1/00	7	Frequency-division multiplex systems (H04J14/00 takes precedence)	H04J1/00	H04J1/00		546
H04J1/02	8	Details	H04J1/02	H04J1/02		123
H04J1/04	9	Frequency-transposition arrangements {(modulation with carrier or side-band suppression H03C1/52, H03C1/60; single-band suppression H04B1/00, H04B15/00; telegraphic communication H04L27/02, H04L25/49; transference of modulation from one carrier to another, e.g. frequency- changing H03D7/00; demodulation or transference of modulation of modulated electromagnetic waves H03D9/00)}	H04J1/04	H04J1/04		360
H04J1/045	10	{Filters applied to frequency transposition}	H04J1/04	H04J1/04		143
H04J1/05	10	using digital techniques	H04J1/05	H04J1/05		153
H04J1/06	9	Arrangements for supplying the carrier waves {; Arrangements for supplying synchronisation signals (synchronisation in general H03B; frequency multiplication H03B19/00, H03B21/00; mixing H03D7/00, H03D9/00; carrier supply H04L5/10)}	H04J1/06	H04J1/06		405
H04J1/065	10	{Synchronisation of carrier sources at the receiving station with the carrier source at the transmitting station}	H04J1/06	H04J1/06		109
H04J1/08	9	Arrangements for combining channels {(branching filters H01P1/213, H03H7/46)}	H04J1/08	H04J1/08		252
H04J1/085	10	{Terminal station; Combined modulator and demodulator circuits}	H04J1/08	H04J1/08		65
H04J1/10	9	Intermediate station arrangements, e.g. for branching, for tapping-off {(repeater circuits H04B3/36, H04B3/58; two-way amplifiers H03F3/62)}	H04J1/10	H04J1/10		219
H04J1/12	9	Arrangements for reducing cross-talk between channels {(in line transmission systems H04B3/32; in cables or lines H04B3/26&#160;-&#160;H04B3/30)}	H04J1/12	H04J1/12		297
H04J1/14	9	Arrangements providing for calling or supervisory signals	H04J1/14	H04J1/14		399
H04J1/16	9	Monitoring arrangements {(for transmission in general H04B17/00; for amplifiers H03F1/52, H03F1/523)}	H04J1/16	H04J1/16		399
H04J1/18	8	in which all the carriers are amplitude-modulated (H04J1/02 takes precedence {in telephony H04Q11/02, H04Q11/023; in stereophony H04H; in telegraphy H04L5/06; in telemetry G08C15/02, G08C15/04})	H04J1/18	H04J1/18		118
H04J1/20	8	in which at least one carrier is angle-modulated (H04J1/02 takes precedence; FM without multiplex H04B1/00, H04B14/006, H04B15/00; PSK H04L5/12; impulse-modulation without multiplex H04B14/02; time-division multiplexing for data transmission H04L5/22; telemetry G08C15/06&#160;-&#160;G08C15/12; telephony H04Q11/00, H04Q11/04, H04Q11/0407)	H04J1/20	H04J1/20		107
H04J3/00	7	Time-division multiplex systems (H04J14/00 takes precedence; relay systems H04B7/14; selecting techniques H04Q)	H04J3/00	H04J3/00		906
H04J3/02	8	Details (electronic switching or gating H03K17/00)	H04J3/02	H04J3/02		273
H04J3/025	9	{Filter arrangements (H04J3/08 takes precedence; filters per seH03H7/00, H03H9/00)}	H04J3/02	H04J3/02		54
H04J3/04	9	Distributors combined with modulators or demodulators {(pulse distributors in general H03K5/15; pulse counters H03K21/00&#160;-&#160;H03K29/06; for telegraphy H04L5/22, H04L13/00&#160;-&#160;H04L23/00, H04L25/45; for telephony H04Q11/04)}	H04J3/04	H04J3/04		327
H04J3/042	10	{Distributors with electron or gas discharge tubes}	H04J3/04	H04J3/04		267
H04J3/045	10	{Distributors with CRT}	H04J3/04	H04J3/04		168
H04J3/047	10	{Distributors with transistors or integrated circuits}	H04J3/04	H04J3/04		826
H04J3/06	9	Synchronising arrangements {(for television systems H04N5/04; bit-synchronisation H04L7/00)}	H04J3/06	H04J3/06		1020
H04J3/0602	10	{Systems characterised by the synchronising information used}	H04J3/06	H04J3/06		784
H04J3/0605	11	{Special codes used as synchronising signal}	H04J3/06	H04J3/06		668
H04J3/0608	12	{Detectors therefor, e.g. correlators, state machines}	H04J3/06	H04J3/06		599
H04J3/0611	12	{PN codes (H04J3/0608 takes precedence)}	H04J3/06	H04J3/06		82
H04J3/0614	11	{the synchronising signal being characterised by the amplitude, duration or polarity}	H04J3/06	H04J3/06		158
H04J3/0617	11	{the synchronising signal being characterised by the frequency or phase}	H04J3/06	H04J3/06		380
H04J3/062	10	{Synchronisation of signals having the same nominal but fluctuating bit rates, e.g. using buffers (pulse-stuffing H04J3/07; asynchronous-synchronous conversion H04L5/24; speed conversion H04L25/05; speed conversion in computers G06F5/06)}	H04J3/06	H04J3/06		282
H04J3/0623	11	{Synchronous multiplexing systems, e.g. synchronous digital hierarchy/synchronous optical network (SDH/SONET), synchronisation with a pointer process}	H04J3/06	H04J3/06		374
H04J3/0626	11	{plesiochronous multiplexing systems, e.g. plesiochronous digital hierarchy [PDH], jitter attenuators}	H04J3/06	H04J3/06		305
H04J3/0629	12	{in a network, e.g. in combination with switching or multiplexing, slip buffers}	H04J3/06	H04J3/06		199
H04J3/0632	11	{Synchronisation of packets and cells, e.g. transmission of voice via a packet network, circuit emulation service [CES] (queuing arrangements in packet switching elements H04L49/90; synchronising systems for the synchronous transmission of a pulse code modulated video signal with one or more other pulse code modulated signals H04N7/56)}	H04J3/06	H04J3/06		897
H04J3/0635	10	{Clock or time synchronisation in a network (timer in protocols H04L69/28)}	H04J3/06	H04J3/06		695
H04J3/0638	11	{Clock or time synchronisation among nodes; Internode synchronisation (synchronization for ring networks H04L12/422; data switching networks with synchronous transmission H04L12/43)}	H04J3/06	H04J3/06		2870
H04J3/0641	12	{Change of the master or reference, e.g. take-over or failure of the master}	H04J3/06	H04J3/06		886
H04J3/0644	12	{External master-clock}	H04J3/06	H04J3/06		968
H04J3/0647	12	{Synchronisation among TDM nodes}	H04J3/06	H04J3/06		283
H04J3/065	13	{using timestamps}	H04J3/06	H04J3/06		264
H04J3/0652	12	{Synchronisation among time division multiple access [TDMA] nodes, e.g. time triggered protocol [TTP] (bus network with centralized control in which slots are of a TDMA packet structure H04L12/4035)}	H04J3/06	H04J3/06		344
H04J3/0655	13	{using timestamps}	H04J3/06	H04J3/06		287
H04J3/0658	12	{Clock or time synchronisation among packet nodes}	H04J3/06	H04J3/06		1166
H04J3/0661	13	{using timestamps}	H04J3/06	H04J3/06		1172
H04J3/0664	14	{unidirectional timestamps}	H04J3/06	H04J3/06		570
H04J3/0667	14	{Bidirectional timestamps, e.g. NTP or PTP for compensation of clock drift and for compensation of propagation delays (arrangements for monitoring round trip delays in packet switching networks H04L43/0864)}	H04J3/06	H04J3/06		3038
H04J3/067	14	{Details of the timestamp structure}	H04J3/06	H04J3/06		118
H04J3/0673	13	{using intermediate nodes, e.g. modification of a received timestamp before further transmission to the next packet node, e.g. including internal delay time or residence time into the packet}	H04J3/06	H04J3/06		372
H04J3/0676	11	{Mutual}	H04J3/06	H04J3/06		275
H04J3/0679	11	{by determining clock distribution path in a network}	H04J3/06	H04J3/06		206
H04J3/0682	11	{by delay compensation, e.g. by compensation of propagation delay or variations thereof, by ranging}	H04J3/06	H04J3/06		2044
H04J3/0685	11	{Clock or time synchronisation in a node; Intranode synchronisation}	H04J3/06	H04J3/06		1259
H04J3/0688	12	{Change of the master or reference, e.g. take-over or failure of the master}	H04J3/06	H04J3/06		566
H04J3/0691	12	{Synchronisation in a TDM node}	H04J3/06	H04J3/06		171
H04J3/0694	12	{Synchronisation in a TDMA node, e.g. TTP}	H04J3/06	H04J3/06		81
H04J3/0697	12	{Synchronisation in a packet node}	H04J3/06	H04J3/06		697
H04J3/07	10	using pulse stuffing for systems with different or fluctuating information rates {or bit rates}	H04J3/07	H04J3/07		395
H04J3/073	11	{Bit stuffing, e.g. PDH}	H04J3/07	H04J3/07		202
H04J3/076	11	{Bit and byte stuffing, e.g. SDH/PDH desynchronisers, bit-leaking}	H04J3/07	H04J3/07		233
H04J3/08	9	Intermediate station arrangements, e.g. for branching, for tapping-off	H04J3/08	H04J3/08		397
H04J3/085	10	{for ring networks, e.g. SDH/SONET rings, self-healing rings, meashed SDH/SONET networks}	H04J3/08	H04J3/08		552
H04J3/10	9	Arrangements for reducing cross-talk between channels	H04J3/10	H04J3/10		331
H04J3/12	9	Arrangements providing for calling or supervisory signals	H04J3/12	H04J3/12		681
H04J3/125	10	{One of the channel pulses or the synchronisation pulse is also used for transmitting monitoring or supervisory signals}	H04J3/12	H04J3/12		204
H04J3/14	9	Monitoring arrangements {(for SDH/SONET rings H04J3/085)}	H04J3/14	H04J3/14		2031
H04J3/16	8	in which the time allocation to individual channels within a transmission cycle is variable, e.g. to accommodate varying complexity of signals, to vary number of channels transmitted (H04J3/17, H04J3/24 take precedence)	H04J3/16	H04J3/16		569
H04J3/1605	9	{Fixed allocated frame structures}	H04J3/16	H04J3/16		191
H04J3/1611	10	{Synchronous digital hierarchy [SDH] or SONET (H04J3/1664 takes precedence for interactions with OTN)}	H04J3/16	H04J3/16		908
H04J3/1617	11	{carrying packets or ATM cells}	H04J3/16	H04J3/16		410
H04J3/1623	10	{Plesiochronous digital hierarchy [PDH]}	H04J3/16	H04J3/16		127
H04J3/1629	11	{Format building algorithm}	H04J3/16	H04J3/16		72
H04J3/1635	11	{Format conversion, e.g. CEPT/US}	H04J3/16	H04J3/16		85
H04J3/1641	11	{Hierarchical systems}	H04J3/16	H04J3/16		91
H04J3/1647	11	{Subrate or multislot multiplexing}	H04J3/16	H04J3/16		259
H04J3/1652	10	{Optical Transport Network [OTN]}	H04J3/16	H04J3/16		820
H04J3/1658	11	{carrying packets or ATM cells; (H04J3/1664 takes precedence for payloads with different packet types)}	H04J3/16	H04J3/16		280
H04J3/1664	11	{carrying hybrid payloads, e.g. different types of packets or carrying frames and packets in the paylaod}	H04J3/16	H04J3/16		158
H04J3/167	11	{interaction with SDH/SONET, e.g. carrying SDH/SONET frames, interfacing with SDH/SONET (H04J3/1664 takes precedence)}	H04J3/16	H04J3/16		60
H04J3/1676	9	{Time-division multiplex with pulse-position, pulse-interval, or pulse-width modulation}	H04J3/16	H04J3/16		177
H04J3/1682	9	{Allocation of channels according to the instantaneous demands of the users, e.g. concentrated multiplexers, statistical multiplexers}	H04J3/16	H04J3/16		593
H04J3/1688	10	{the demands of the users being taken into account after redundancy removal, e.g. by predictive coding, by variable sampling (reducing bandwidth of signals in general H04B1/66; in PCM-systems H04B14/046; removal of redundancy in telegraph communication H03M7/30)}	H04J3/16	H04J3/16		236
H04J3/1694	9	{Allocation of channels in TDM/TDMA networks, e.g. distributed multiplexers (Passive Optical Networks H04Q11/0062)}	H04J3/16	H04J3/16		1049
H04J3/17	8	in which the transmission channel allotted to a first user may be taken away and re-allotted to a second user if the first user becomes inactive, e.g. TASI {(speech analysis or identification G10L)}	H04J3/17	H04J3/17		210
H04J3/172	9	{Digital speech interpolation, i.e. DSI}	H04J3/17	H04J3/17		62
H04J3/175	9	{Speech activity or inactivity detectors (echo suppressors H04B3/20)}	H04J3/17	H04J3/17		83
H04J3/177	9	{Freeze-out systems, e.g. taking away active sources from transmission}	H04J3/17	H04J3/17		31
H04J3/18	8	using frequency compression and subsequent expansion of the individual signals	H04J3/18	H04J3/18		189
H04J3/20	8	using resonant transfer	H04J3/20	H04J3/20		203
H04J3/22	8	in which the sources have different rates or codes {(simultaneous speech and digital data or video transmission H04M11/06; see provisional also H04J3/16)}	H04J3/22	H04J3/22		183
H04J3/24	8	in which the allocation is indicated by an address {the different channels being transmitted sequentially}(H04J3/17 takes precedence; in computers G06F12/00, G06F13/00{code multiplex systems H04J13/00; selecting techniques H04Q; relay systems H04B7/14})	H04J3/24	H04J3/24		178
H04J3/242	9	{the frames being of variable length}	H04J3/24	H04J3/24		34
H04J3/245	9	{in which the allocation protocols between more than two stations share the same transmission medium (stations for satellite systems H04B7/185)}	H04J3/24	H04J3/24		88
H04J3/247	9	{ATM or packet multiplexing}	H04J3/24	H04J3/24		268
H04J3/26	9	in which the information and the address are simultaneously transmitted	H04J3/26	H04J3/26		84
H04J4/00	7	Combined time-division and frequency-division multiplex systems (H04J13/00 takes precedence {; data transmission H04L5/26; telemetry G08C15/00})	H04J4/00	H04J4/00		262
H04J4/005	8	{Transmultiplexing}	H04J4/00	H04J4/00		136
H04J7/00	7	Multiplex systems in which the amplitudes or durations of the signals in individual channels are characteristic of those channels	H04J7/00	H04J7/00		193
H04J7/02	8	in which the polarity of the amplitude is characteristic	H04J7/02	H04J7/02		55
H04J9/00	7	Multiplex systems in which each channel is represented by a different type of modulation of the carrier	H04J9/00	H04J9/00		243
H04J11/00	7	Orthogonal multiplex systems, {e.g. using WALSH codes}(H04J13/00 takes precedence)	H04J11/00	H04J11/00		1732
H04J2011/0003	8	{Combination with other multiplexing techniques}	H04J11/00	H04J11/00		29
H04J2011/0006	9	{with CDM/CDMA}	H04J11/00	H04J11/00		63
H04J2011/0009	9	{with FDM/FDMA}	H04J11/00	H04J11/00		89
H04J2011/0013	9	{with TDM/TDMA}	H04J11/00	H04J11/00		54
H04J2011/0016	9	{with FDM/FDMA and TDM/TDMA}	H04J11/00	H04J11/00		53
H04J2011/002	9	{Delay multiplexing}	H04J11/00	H04J11/00		9
H04J11/0023	8	{Interference mitigation or co-ordination (direct sequence spread spectrum [DSSS] systems H04B1/7097; frequency hopping H04B1/713; allocation criteria for ingress interference avoidance H04L5/0062; frequency allocation criteria for requirements on out-of-channel emissions H04L5/0066; arrangements for removing intersymbol interference or baseband equalisers H04L25/03006; peak power aspects in multicarrier modulation H04L27/2614; power management H04W52/00; traffic scheduling H04W72/54, H04W72/541)}	H04J11/00	H04J11/00		990
H04J11/0026	9	{of multi-user interference}	H04J11/00	H04J11/00		271
H04J11/003	10	{at the transmitter (transmission to multiple receive units in multiple input multiple output [MIMO] H04B7/0452; transmit antenna weighting H04B7/0615)}	H04J11/00	H04J11/00		268
H04J11/0033	11	{by pre-cancellation of known interference, e.g. using a matched filter, dirty paper coder or Thomlinson-Harashima precoder (correlative coding in synchronous or start-stop systems H04L25/497)}	H04J11/00	H04J11/00		106
H04J11/0036	10	{at the receiver}	H04J11/00	H04J11/00		278
H04J11/004	11	{using regenerative subtractive interference cancellation}	H04J11/00	H04J11/00		389
H04J11/0043	12	{by grouping or ordering the users}	H04J11/00	H04J11/00		53
H04J11/0046	11	{using joint detection algorithms}	H04J11/00	H04J11/00		72
H04J11/005	9	{of intercell interference}	H04J11/00	H04J11/00		1108
H04J11/0053	10	{using co-ordinated multipoint transmission/reception (co-ordinated antenna or beam-forming aspects H04B7/022)}	H04J11/00	H04J11/00		454
H04J11/0056	10	{Inter-base station aspects}	H04J11/00	H04J11/00		514
H04J11/0059	10	{Out-of-cell user aspects}	H04J11/00	H04J11/00		98
H04J11/0063	9	{of multipath interference, e.g. Rake receivers}	H04J11/00	H04J11/00		126
H04J11/0066	9	{of narrowband interference (narrowband interference reduction H04B1/1036)}	H04J11/00	H04J11/00		120
H04J11/0069	8	{Cell search, i.e. determining cell identity [cell-ID] (design of multiplexing codes H04J13/00; processing access restriction or access information H04W48/16; discovery of network devices for network data management H04W8/005; sounding signals for channel estimation H04L25/0226; structure of reference signals in multicarrier modulation systems H04L27/2613; frame, time or carrier synchronisation in multicarrier modulation systems H04L27/2655)}	H04J11/00	H04J11/00		1288
H04J11/0073	9	{Acquisition of primary synchronisation channel, e.g. detection of cell-ID within cell-ID group}	H04J11/00	H04J11/00		683
H04J11/0076	9	{Acquisition of secondary synchronisation channel, e.g. detection of cell-ID group}	H04J11/00	H04J11/00		622
H04J11/0079	9	{Acquisition of downlink reference signals, e.g. detection of cell-ID}	H04J11/00	H04J11/00		301
H04J11/0083	9	{Multi-mode cell search, i.e. where several modes or systems can be used, e.g. backwards compatible, dual mode or flexible systems}	H04J11/00	H04J11/00		51
H04J11/0086	9	{Search parameters, e.g. search strategy, accumulation length, range of search, thresholds (code acquisition in DSSS H04B1/7075)}	H04J11/00	H04J11/00		209
H04J11/0089	9	{Search hardware arrangements, e.g. sharing of correlators to reduce complexity}	H04J11/00	H04J11/00		18
H04J11/0093	9	{Neighbour cell search}	H04J11/00	H04J11/00		234
H04J2011/0096	8	{Network synchronisation}	H04J11/00	H04J11/00		214
H04J13/00	7	Code division multiplex systems (for frequency hopping H04B1/713)<br><br><u>NOTE</u><br><br> When classifying in this group, any aspect of spread spectrum techniques not specific to frequency hopping, and which is considered to represent information of interest for search, may also be classified in group H04B1/69. 	H04J13/00	H04J13/00		1075
H04J13/0003	8	{Code application, i.e. aspects relating to how codes are applied to form multiplexed channels}	H04J13/00	H04J13/00		417
H04J13/0007	8	{Code type}<br><br><u>NOTE</u><br><br>Code type information should be classified in addition to other relevant aspects. This should also be done in cases where the other relevant symbol refers to code type, e.g. H04J13/14, H04J13/20) 	H04J13/00	H04J13/00		56
H04J13/0011	9	{Complementary}	H04J13/00	H04J13/00		31
H04J13/0014	10	{Golay}	H04J13/00	H04J13/00		135
H04J13/0018	9	{Chaotic}	H04J13/00	H04J13/00		62
H04J13/0022	9	{PN, e.g. Kronecker}	H04J13/00	H04J13/00		712
H04J13/0025	10	{M-sequences}	H04J13/00	H04J13/00		160
H04J13/0029	10	{Gold}	H04J13/00	H04J13/00		190
H04J13/0033	10	{Kasami}	H04J13/00	H04J13/00		17
H04J2013/0037	9	{Multilevel codes}	H04J13/00	H04J13/00		61
H04J13/004	9	{Orthogonal}	H04J13/00	H04J13/00		700
H04J13/0044	10	{OVSF [orthogonal variable spreading factor]}	H04J13/00	H04J13/00		298
H04J13/0048	10	{Walsh}	H04J13/00	H04J13/00		714
H04J13/0051	10	{Orthogonal gold}	H04J13/00	H04J13/00		23
H04J13/0055	9	{ZCZ [zero correlation zone]}	H04J13/00	H04J13/00		94
H04J13/0059	10	{CAZAC [constant-amplitude and zero auto-correlation]}	H04J13/00	H04J13/00		232
H04J13/0062	11	{Zadoff-Chu}	H04J13/00	H04J13/00		671
H04J13/0066	11	{GCL [generalized chirp-like] sequences}	H04J13/00	H04J13/00		22
H04J13/007	10	{LAS, i.e. LA, LS and LAS codes}	H04J13/00	H04J13/00		26
H04J13/0074	8	{Code shifting or hopping}	H04J13/00	H04J13/00		392
H04J13/0077	8	{Multicode, e.g. multiple codes assigned to one user}	H04J13/00	H04J13/00		429
H04J2013/0081	9	{with FDM/FDMA}	H04J13/00	H04J13/00		13
H04J2013/0085	9	{with TDM/TDMA}	H04J13/00	H04J13/00		4
H04J2013/0088	9	{with FDM/FDMA and TDM/TDMA}	H04J13/00	H04J13/00		6
H04J2013/0092	9	{Delay multiplexing}	H04J13/00	H04J13/00		
H04J2013/0096	8	{Network synchronisation}	H04J13/00	H04J13/00		50
H04J13/10	8	Code generation	H04J13/10	H04J13/10		989
H04J13/102	9	{Combining codes}	H04J13/10	H04J13/10		162
H04J13/105	10	{by extending}	H04J13/10	H04J13/10		36
H04J13/107	10	{by concatenation}	H04J13/10	H04J13/10		128
H04J13/12	9	Generation of orthogonal codes	H04J13/12	H04J13/12		490
H04J13/14	9	Generation of codes with a zero correlation zone	H04J13/14	H04J13/14		130
H04J13/16	8	Code allocation	H04J13/16	H04J13/16		927
H04J2013/165	9	{Joint allocation of code together with frequency or time}	H04J13/16	H04J13/16		40
H04J13/18	9	Allocation of orthogonal codes	H04J13/18	H04J13/18		603
H04J13/20	10	having an orthogonal variable spreading factor [OVSF]	H04J13/20	H04J13/20		178
H04J13/22	9	Allocation of codes with a zero correlation zone	H04J13/22	H04J13/22		126
H04J14/00	7	Optical multiplex systems	H04J14/00	H04J14/00		221
H04J14/002	8	{Coherencemultiplexing}	H04J14/00	H04J14/00		106
H04J14/005	8	{Optical Code Multiplex}	H04J14/00	H04J14/00		324
H04J14/007	9	{Orthogonal Optical Code Multiplex}	H04J14/00	H04J14/00		73
H04J14/02	8	Wavelength-division multiplex systems	H04J14/02	H04J14/02		1976
H04J14/0201	9	{Add-and-drop multiplexing}	H04J14/02	H04J14/02		611
H04J14/0202	10	{Arrangements therefor}	H04J14/02	H04J14/02		673
H04J14/0204	11	{Broadcast and select arrangements, e.g. with an optical splitter at the input before adding or dropping}	H04J14/02	H04J14/02		738
H04J14/0205	11	{Select and combine arrangements, e.g. with an optical combiner at the output after adding or dropping}	H04J14/02	H04J14/02		587
H04J14/0206	11	{Express channels arrangements}	H04J14/02	H04J14/02		568
H04J14/0208	11	{Interleaved arrangements}	H04J14/02	H04J14/02		202
H04J14/0209	11	{Multi-stage arrangements, e.g. by cascading multiplexers or demultiplexers}	H04J14/02	H04J14/02		533
H04J14/021	11	{Reconfigurable arrangements, e.g. reconfigurable optical add/drop multiplexers [ROADM] or tunable optical add/drop multiplexers [TOADM]}	H04J14/02	H04J14/02		404
H04J14/0212	12	{using optical switches or wavelength selective switches [WSS]}	H04J14/02	H04J14/02		1031
H04J14/02122	12	{Colourless, directionless or contentionless [CDC] arrangements}	H04J14/02	H04J14/02		197
H04J14/02126	12	{Multicast switch arrangements}	H04J14/02	H04J14/02		73
H04J14/0213	11	{Groups of channels or wave bands arrangements}	H04J14/02	H04J14/02		931
H04J14/0215	10	{Architecture aspects}	H04J14/02	H04J14/02		112
H04J14/0216	11	{Bidirectional architectures}	H04J14/02	H04J14/02		256
H04J14/0217	11	{Multi-degree architectures, e.g. having a connection degree greater than two}	H04J14/02	H04J14/02		419
H04J14/0219	11	{Modular or upgradable architectures}	H04J14/02	H04J14/02		271
H04J14/022	11	{For interconnection of WDM optical networks}	H04J14/02	H04J14/02		164
H04J14/0221	9	{Power control, e.g. to keep the total optical power constant}	H04J14/02	H04J14/02		670
H04J14/02212	10	{by addition of a dummy signal}	H04J14/02	H04J14/02		86
H04J14/02214	10	{by re-allocation of data channels}	H04J14/02	H04J14/02		22
H04J14/02216	10	{by gain equalization}	H04J14/02	H04J14/02		751
H04J14/02218	10	{Centralized control}	H04J14/02	H04J14/02		45
H04J14/02219	10	{Distributed control}	H04J14/02	H04J14/02		36
H04J14/0223	9	{Conversion to or from optical TDM}	H04J14/02	H04J14/02		108
H04J14/0224	9	{Irregular wavelength spacing, e.g. to accommodate interference to all wavelengths}	H04J14/02	H04J14/02		174
H04J14/0226	9	{Fixed carrier allocation, e.g. according to service}	H04J14/02	H04J14/02		752
H04J14/0227	9	{Operation, administration, maintenance or provisioning [OAMP] of WDM networks, e.g. media access, routing or wavelength allocation}	H04J14/02	H04J14/02		2759
H04J14/0228	10	{Wavelength allocation for communications one-to-all, e.g. broadcasting wavelengths}	H04J14/02	H04J14/02		128
H04J14/023	11	{in WDM passive optical networks [WDM-PON]}	H04J14/02	H04J14/02		89
H04J14/0232	12	{for downstream transmission}	H04J14/02	H04J14/02		303
H04J14/0234	13	{using multiple wavelengths}	H04J14/02	H04J14/02		55
H04J14/0235	12	{for upstream transmission}	H04J14/02	H04J14/02		26
H04J14/0236	13	{using multiple wavelengths}	H04J14/02	H04J14/02		23
H04J14/0238	10	{Wavelength allocation for communications one-to-many, e.g. multicasting wavelengths}	H04J14/02	H04J14/02		270
H04J14/0239	11	{in WDM-PON sharing multiple downstream wavelengths for groups of optical network units [ONU], e.g. multicasting wavelengths}	H04J14/02	H04J14/02		89
H04J14/0241	10	{Wavelength allocation for communications one-to-one, e.g. unicasting wavelengths}	H04J14/02	H04J14/02		768
H04J14/0242	11	{in WDM-PON}	H04J14/02	H04J14/02		110
H04J14/0245	12	{for downstream transmission, e.g. optical line terminal [OLT] to ONU}	H04J14/02	H04J14/02		163
H04J14/0246	13	{using one wavelength per ONU}	H04J14/02	H04J14/02		999
H04J14/0247	13	{Sharing one wavelength for at least a group of ONUs}	H04J14/02	H04J14/02		500
H04J14/0249	12	{for upstream transmission, e.g. ONU-to-OLT or ONU-to-ONU}	H04J14/02	H04J14/02		154
H04J14/025	13	{using one wavelength per ONU, e.g. for transmissions from-ONU-to-OLT or from-ONU-to-ONU}	H04J14/02	H04J14/02		775
H04J14/0252	13	{Sharing one wavelength for at least a group of ONUs, e.g. for transmissions from-ONU-to-OLT or from-ONU-to-ONU}	H04J14/02	H04J14/02		491
H04J2014/0253	12	{Allocation of downstream wavelengths for upstream transmission}	H04J14/02	H04J14/02		156
H04J14/0254	10	{Optical medium access}	H04J14/02	H04J14/02		60
H04J14/0256	11	{at the optical channel layer}	H04J14/02	H04J14/02		357
H04J14/0257	12	{Wavelength assignment algorithms}	H04J14/02	H04J14/02		499
H04J14/0258	12	{Wavelength identification or labelling}	H04J14/02	H04J14/02		232
H04J14/026	12	{using WDM channels of different transmission rates}	H04J14/02	H04J14/02		142
H04J14/0261	11	{at the optical multiplex section layer}	H04J14/02	H04J14/02		53
H04J14/0263	12	{Multiplex section layer wavelength assignment algorithms}	H04J14/02	H04J14/02		34
H04J14/0264	12	{Multiplex identification or labelling}	H04J14/02	H04J14/02		18
H04J14/0265	12	{Multiplex arrangements in bidirectional systems, e.g. interleaved allocation of wavelengths or allocation of wavelength groups}	H04J14/02	H04J14/02		98
H04J14/0267	11	{Optical signaling or routing}	H04J14/02	H04J14/02		646
H04J14/0268	12	{Restoration of optical paths, e.g. p-cycles}	H04J14/02	H04J14/02		152
H04J14/0269	12	{using tables for routing}	H04J14/02	H04J14/02		188
H04J14/0271	12	{Impairment aware routing}	H04J14/02	H04J14/02		196
H04J14/0272	11	{Transmission of OAMP information}	H04J14/02	H04J14/02		246
H04J14/0273	12	{using optical overhead, e.g. overhead processing}	H04J14/02	H04J14/02		104
H04J14/0275	12	{using an optical service channel}	H04J14/02	H04J14/02		207
H04J14/0276	12	{using pilot tones}	H04J14/02	H04J14/02		90
H04J14/02762	11	{Spectrum slot allocation}	H04J14/02	H04J14/02		28
H04J14/02764	11	{Multiplex arrangements for radio-frequency networks access; policies therefor (radio over fibre arrangement H04B10/2575)}	H04J14/02	H04J14/02		28
H04J14/0278	9	{WDM optical network architectures}	H04J14/02	H04J14/02		167
H04J14/0279	10	{WDM point-to-point architectures}	H04J14/02	H04J14/02		453
H04J14/028	10	{WDM bus architectures}	H04J14/02	H04J14/02		266
H04J14/0282	10	{WDM tree architectures}	H04J14/02	H04J14/02		1627
H04J14/0283	10	{WDM ring architectures}	H04J14/02	H04J14/02		1313
H04J14/0284	10	{WDM mesh architectures}	H04J14/02	H04J14/02		701
H04J14/0286	10	{WDM hierarchical architectures}	H04J14/02	H04J14/02		331
H04J14/02862	10	{WDM data centre network [DCN] architectures}	H04J14/02	H04J14/02		23
H04J14/0287	9	{Protection in WDM systems}	H04J14/02	H04J14/02		273
H04J14/0289	10	{Optical multiplex section protection}	H04J14/02	H04J14/02		114
H04J14/029	11	{Dedicated protection at the optical multiplex section (1+1)}	H04J14/02	H04J14/02		143
H04J14/0291	11	{Shared protection at the optical multiplex section (1:1, n:m)}	H04J14/02	H04J14/02		392
H04J14/0293	10	{Optical channel protection}	H04J14/02	H04J14/02		161
H04J14/0294	11	{Dedicated protection at the optical channel (1+1)}	H04J14/02	H04J14/02		285
H04J14/0295	11	{Shared protection at the optical channel (1:1, n:m)}	H04J14/02	H04J14/02		483
H04J14/0297	10	{Optical equipment protection}	H04J14/02	H04J14/02		369
H04J14/0298	9	{with sub-carrier multiplexing [SCM]}	H04J14/02	H04J14/02		775
H04J14/03	9	{WDM arrangements (ADM arrangements H04J14/0202; WDM network architectures H04J14/0278)}	H04J14/02	H04J14/03		72
H04J14/0305	10	{in end terminals}	H04J14/02	H04J14/0305		611
H04J14/0307	10	{Multiplexers; Demultiplexers}	H04J14/02	H04J14/0307		899
H04J14/04	8	Mode multiplex systems	H04J14/04	H04J14/04		358
H04J14/05	8	{Spatial multiplexing systems}	H04J14/00	H04J14/05		82
H04J14/052	9	{using multicore fibre (mode multiplex systems H04J14/04)}	H04J14/00	H04J14/052		163
H04J14/06	8	Polarisation multiplex systems	H04J14/06	H04J14/06		1156
H04J14/07	8	{Orbital angular momentum [OAM] multiplex systems}	H04J14/00	H04J14/07		90
H04J14/08	8	Time-division multiplex systems	H04J14/08	H04J14/08		1060
H04J14/083	9	{Add and drop multiplexing}	H04J14/08	H04J14/08		73
H04J14/086	9	{Medium access (H04J3/16 takes precedence)}	H04J14/08	H04J14/08		64
H04J99/00	7	Subject matter not provided for in other groups of this subclass	H04J99/00	H04J99/00		342
H04J2203/00	7	Aspects of optical multiplex systems other than those covered by H04J14/05 and H04J14/07	CPCONLY	H04J2203/00		5
H04J2203/0001	8	Provisions for broadband connections in integrated services digital network using frames of the Optical Transport Network [OTN] or using synchronous transfer mode [STM], e.g. SONET, SDH	CPCONLY	H04J2203/0001		23
H04J2203/0003	9	Switching fabrics, e.g. transport network, control network	CPCONLY	H04J2203/0003		82
H04J2203/0005	10	Switching elements	CPCONLY	H04J2203/0005		92
H04J2203/0007	11	Space switch details	CPCONLY	H04J2203/0007		19
H04J2203/0008	11	Time switch details	CPCONLY	H04J2203/0008		18
H04J2203/001	11	using a shared central buffer	CPCONLY	H04J2203/001		13
H04J2203/0012	10	Switching modules and their interconnections	CPCONLY	H04J2203/0012		151
H04J2203/0014	11	Clos	CPCONLY	H04J2203/0014		11
H04J2203/0016	11	Crossbar	CPCONLY	H04J2203/0016		5
H04J2203/0017	11	Parallel switch planes	CPCONLY	H04J2203/0017		4
H04J2203/0019	10	Multicast/broadcast capabilities	CPCONLY	H04J2203/0019		25
H04J2203/0021	10	Control mechanisms	CPCONLY	H04J2203/0021		29
H04J2203/0023	10	Routing/path finding	CPCONLY	H04J2203/0023		22
H04J2203/0025	10	Peripheral units	CPCONLY	H04J2203/0025		91
H04J2203/0026	10	Physical details	CPCONLY	H04J2203/0026		65
H04J2203/0028	9	Local loop	CPCONLY	H04J2203/0028		43
H04J2203/003	10	Medium of transmission, e.g. fibre, cable, radio	CPCONLY	H04J2203/003		13
H04J2203/0032	11	Fibre	CPCONLY	H04J2203/0032		53
H04J2203/0033	11	Metallic	CPCONLY	H04J2203/0033		16
H04J2203/0035	11	Radio	CPCONLY	H04J2203/0035		54
H04J2203/0037	11	Satellite	CPCONLY	H04J2203/0037		5
H04J2203/0039	10	Topology	CPCONLY	H04J2203/0039		15
H04J2203/0041	11	Star, e.g. cross-connect, concentrator, subscriber group equipment, remote electronics	CPCONLY	H04J2203/0041		93
H04J2203/0042	11	Ring	CPCONLY	H04J2203/0042		333
H04J2203/0044	11	Bus, e.g. DQDB	CPCONLY	H04J2203/0044		19
H04J2203/0046	9	User Network Interface	CPCONLY	H04J2203/0046		92
H04J2203/0048	10	Network termination, e.g. NT1, NT2, PBX	CPCONLY	H04J2203/0048		67
H04J2203/005	10	Terminal equipment, e.g. codecs, synch	CPCONLY	H04J2203/005		57
H04J2203/0051	9	Network Node Interface, e.g. tandem connections, transit switching	CPCONLY	H04J2203/0051		111
H04J2203/0053	10	Routing	CPCONLY	H04J2203/0053		112
H04J2203/0055	10	Network design, dimensioning, topology or optimisation	CPCONLY	H04J2203/0055		32
H04J2203/0057	9	Operations, administration and maintenance [OAM]	CPCONLY	H04J2203/0057		174
H04J2203/0058	10	Network management, e.g. Intelligent nets	CPCONLY	H04J2203/0058		122
H04J2203/006	10	Fault tolerance and recovery	CPCONLY	H04J2203/006		931
H04J2203/0062	9	Testing	CPCONLY	H04J2203/0062		97
H04J2203/0064	9	Admission Control	CPCONLY	H04J2203/0064		14
H04J2203/0066	10	Signalling, e.g. protocols, reference model	CPCONLY	H04J2203/0066		99
H04J2203/0067	10	Resource management and allocation	CPCONLY	H04J2203/0067		149
H04J2203/0069	11	Channel allocation	CPCONLY	H04J2203/0069		132
H04J2203/0071	11	Monitoring	CPCONLY	H04J2203/0071		70
H04J2203/0073	9	Services, e.g. multimedia, GOS, QOS	CPCONLY	H04J2203/0073		71
H04J2203/0075	10	Connection-oriented	CPCONLY	H04J2203/0075		16
H04J2203/0076	10	Channel characteristics, e.g. BER, error detection, error correction, delay, jitter	CPCONLY	H04J2203/0076		48
H04J2203/0078	10	Support of N-ISDN	CPCONLY	H04J2203/0078		11
H04J2203/008	10	Support of video	CPCONLY	H04J2203/008		40
H04J2203/0082	10	Interaction of SDH with non-ATM protocols	CPCONLY	H04J2203/0082		165
H04J2203/0083	11	Support of the IP protocol	CPCONLY	H04J2203/0083		50
H04J2203/0085	11	Support of Ethernet	CPCONLY	H04J2203/0085		386
H04J2203/0087	10	Support of voice	CPCONLY	H04J2203/0087		16
H04J2203/0089	9	Multiplexing, e.g. coding, scrambling, SONET	CPCONLY	H04J2203/0089		583
H04J2203/0091	10	Time slot assignment	CPCONLY	H04J2203/0091		62
H04J2203/0092	10	Code Division Multiple Access [CDMA]	CPCONLY	H04J2203/0092		8
H04J2203/0094	10	Virtual Concatenation	CPCONLY	H04J2203/0094		199
H04J2203/0096	10	Serial Concatenation	CPCONLY	H04J2203/0096		50
H04J2203/0098	9	Traffic aspects, e.g. arbitration, load balancing, smoothing, buffer management	CPCONLY	H04J2203/0098		63
H04J2211/00	7	Orthogonal indexing scheme relating to orthogonal multiplex systems	CPCONLY	H04J2211/00		3
H04J2211/001	8	using small cells within macro cells, e.g. femto, pico or microcells	CPCONLY	H04J2211/001		95
H04J2211/003	8	within particular systems or standards	CPCONLY	H04J2211/003		17
H04J2211/005	9	Long term evolution [LTE]	CPCONLY	H04J2211/005		451
H04J2211/006	9	Single carrier frequency division multiple access [SC FDMA]	CPCONLY	H04J2211/006		50
H04J2211/008	9	Interleaved frequency division multiple access [IFDMA]	CPCONLY	H04J2211/008		17
