B60C1/00	7	Tyres characterised by the chemical composition or the physical arrangement or mixture of the composition<br><br><u>NOTE</u><br><br> Tyres characterised by compositions only, i.e. having no significant tyre structure, are classified only with the compositions, e.g. C08K, C08L	B60C1/00	B60C1/00		5502
B60C1/0008	8	{Compositions of the inner liner}	B60C1/00	B60C1/00		1099
B60C1/0016	8	{Compositions of the tread}	B60C1/00	B60C1/00		6948
B60C1/0025	8	{Compositions of the sidewalls}	B60C1/00	B60C1/00		1586
B60C2001/0033	8	{Compositions of the sidewall inserts, e.g. for runflat}	B60C1/00	B60C1/00		212
B60C1/0041	8	{Compositions of the carcass layers}	B60C1/00	B60C1/00		573
B60C2001/005	8	{Compositions of the bead portions, e.g. clinch or chafer rubber or cushion rubber}	B60C1/00	B60C1/00		349
B60C2001/0058	9	{Compositions of the bead apexes}	B60C1/00	B60C1/00		164
B60C2001/0066	8	{Compositions of the belt layers}	B60C1/00	B60C1/00		458
B60C2001/0075	8	{Compositions of belt cushioning layers}	B60C1/00	B60C1/00		102
B60C2001/0083	8	{Compositions of the cap ply layers}	B60C1/00	B60C1/00		117
B60C2001/0091	8	{Compositions of non-inflatable or solid tyres}	B60C1/00	B60C1/00		148
B60C3/00	7	Tyres characterised by the transverse section	B60C3/00	B60C3/00		367
B60C2003/005	8	{Twin tyres}	B60C3/00	B60C3/00		32
B60C3/02	8	Closed, e.g. toroidal, tyres	B60C3/02	B60C3/02		227
B60C3/04	8	characterised by the relative dimensions of the section, e.g. low profile (B60C3/06 takes precedence)	B60C3/04	B60C3/04		858
B60C3/06	8	asymmetric	B60C3/06	B60C3/06		215
B60C3/08	8	collapsible into storage or non-use condition, e.g. space-saving spare tyres	B60C3/08	B60C3/08		53
B60C5/00	7	Inflatable pneumatic tyres or inner tubes (B60C1/00, B60C9/00&#160;-&#160;B60C17/00 take precedence)	B60C5/00	B60C5/00		615
B60C5/001	8	{filled with gas other than air}	B60C5/00	B60C5/00		64
B60C5/002	8	{filled at least partially with foam material}	B60C5/00	B60C5/00		170
B60C5/004	8	{filled at least partially with liquid (B60C19/12 takes precedence)}	B60C5/00	B60C5/00		113
B60C5/005	9	{Ballast tyres}	B60C5/00	B60C5/00		44
B60C5/007	8	{made from other material than rubber}	B60C5/00	B60C5/00		344
B60C5/008	8	{Low pressure tyres, e.g. for all terrain vehicles}	B60C5/00	B60C5/00		28
B60C5/01	8	without substantial cord reinforcement, e.g. cordless tyres, cast tyres	B60C5/01	B60C5/01		248
B60C5/02	8	having separate inflatable inserts, e.g. with inner tubes; Means for lubricating, venting, preventing relative movement between tyre and inner tube (B60C5/20 takes precedence)	B60C5/02	B60C5/02		252
B60C5/025	9	{separated by a part of the tyre (inflatable inserts with several inflatable chambers B60C5/20)}	B60C5/02	B60C5/02		87
B60C5/04	9	Shape or construction of inflatable inserts (B60C5/10 takes precedence)	B60C5/04	B60C5/04		601
B60C5/08	10	having reinforcing means	B60C5/08	B60C5/08		332
B60C5/10	8	formed as a single discontinuous ring with contiguous ends which may be connected together	B60C5/10	B60C5/10		388
B60C5/12	8	without separate inflatable inserts, e.g. tubeless tyres with transverse section open to the rim (B60C5/20 takes precedence)	B60C5/12	B60C5/12		201
B60C5/14	9	with impervious liner or coating on the inner wall of the tyre	B60C5/14	B60C5/14		748
B60C5/142	10	{provided partially, i.e. not covering the whole inner wall}	B60C5/14	B60C5/14		153
B60C2005/145	10	{made of laminated layers}	B60C5/14	B60C5/14		258
B60C2005/147	10	{characterised by the joint or splice}	B60C5/14	B60C5/14		112
B60C5/16	9	Sealing means between beads and rims, e.g. bands	B60C5/16	B60C5/16		264
B60C5/18	8	Sectional casings, e.g. comprising replaceable arcuate parts	B60C5/18	B60C5/18		238
B60C5/20	8	having multiple separate inflatable chambers	B60C5/20	B60C5/20		646
B60C5/22	9	the chambers being annular	B60C5/22	B60C5/22		373
B60C5/24	9	the walls of the chambers extending transversely of the tyre	B60C5/24	B60C5/24		260
B60C7/00	7	Non-inflatable or solid tyres (B60C1/00 takes precedence)	B60C7/00	B60C7/00		1038
B60C2007/005	8	{made by casting, e.g. of polyurethane}	B60C7/00	B60C7/00		159
B60C7/02	8	made from ropes or bristles	B60C7/02	B60C7/02		38
B60C7/04	8	made of wood or leather	B60C7/04	B60C7/04		180
B60C7/06	8	made of metal	B60C7/06	B60C7/06		163
B60C7/08	8	built-up from a plurality of arcuate parts	B60C7/08	B60C7/08		146
B60C7/10	8	characterised by means for increasing resiliency	B60C7/10	B60C7/10		507
B60C7/101	9	{Tyre casings enclosing a distinct core, e.g. foam (enclosed chambers defined by a distinct core B60C7/121)}	B60C7/10	B60C7/10		291
B60C7/1015	10	{using foam material}	B60C7/10	B60C7/10		168
B60C7/102	9	{Tyres built-up with separate rubber parts}	B60C7/10	B60C7/10		628
B60C7/105	9	{using foam material (B60C7/1015 takes precedence)}	B60C7/10	B60C7/10		152
B60C7/107	9	{comprising lateral openings}	B60C7/10	B60C7/10		433
B60C7/12	9	using enclosed chambers, e.g. gas-filled	B60C7/12	B60C7/12		478
B60C7/121	10	{enclosed chambers defined by a distinct core}	B60C7/12	B60C7/12		357
B60C7/125	10	{enclosed chambers defined between rim and tread}	B60C7/12	B60C7/12		294
B60C7/14	9	using springs	B60C7/14	B60C7/14		1809
B60C7/143	10	{having a lateral extension disposed in a plane parallel to the wheel axis}	B60C7/14	B60C7/14		189
B60C7/146	10	{extending substantially radially, e.g. like spokes}	B60C7/14	B60C7/14		548
B60C7/16	10	of helical or flat coil form	B60C7/16	B60C7/16		588
B60C7/18	11	disposed radially relative to wheel axis	B60C7/18	B60C7/18		1095
B60C7/20	11	disposed circumferentially relative to wheel axis	B60C7/20	B60C7/20		387
B60C7/22	8	having inlays other than for increasing resiliency, e.g. for armouring	B60C7/22	B60C7/22		417
B60C7/24	8	characterised by means for securing tyres on rim or wheel body	B60C7/24	B60C7/24		888
B60C7/26	9	using bolts	B60C7/26	B60C7/26		315
B60C7/28	9	using straps or the like, e.g. vulcanised into the tyre	B60C7/28	B60C7/28		204
B60C9/00	7	Reinforcements or ply arrangement of pneumatic tyres (inserts having reinforcing means B60C5/08; bead structure, e.g. turnup or overlap construction, B60C15/00)<br><br><u>NOTE</u><br><br> When classifying in this group, classification is also made in subclass B32B insofar as any layered product is concerned 	B60C9/00	B60C9/00		517
B60C9/0007	8	{Reinforcements made of metallic elements, e.g. cords, yarns, filaments or fibres made from metal}	B60C9/00	B60C9/00		1405
B60C2009/0014	9	{Surface treatments of steel cords}	B60C9/00	B60C9/00		132
B60C2009/0021	9	{Coating rubbers for steel cords}	B60C9/00	B60C9/00		231
B60C9/0028	8	{Reinforcements comprising mineral fibres, e.g. glass or carbon fibres}	B60C9/00	B60C9/00		253
B60C2009/0035	8	{Reinforcements made of organic materials, e.g. rayon, cotton or silk}	B60C9/00	B60C9/00		178
B60C9/0042	8	{Reinforcements made of synthetic materials}	B60C9/00	B60C9/00		1706
B60C9/005	8	{Reinforcements made of different materials, e.g. hybrid or composite cords}	B60C9/00	B60C9/00		667
B60C9/0057	8	{Reinforcements comprising preshaped elements, e.g. undulated or zig-zag filaments}	B60C9/00	B60C9/00		271
B60C9/0064	8	{Reinforcements comprising monofilaments}	B60C9/00	B60C9/00		305
B60C2009/0071	8	{characterised by special physical properties of the reinforcements}	B60C9/00	B60C9/00		208
B60C2009/0078	9	{Modulus}	B60C9/00	B60C9/00		142
B60C2009/0085	9	{Tensile strength}	B60C9/00	B60C9/00		135
B60C2009/0092	9	{Twist structure}	B60C9/00	B60C9/00		247
B60C9/02	8	Carcasses	B60C9/02	B60C9/02		929
B60C9/0207	9	{Carcasses comprising an interrupted ply, i.e. where the carcass ply does not continuously extend from bead to bead but is interrupted, e.g. at the belt area, into two or more portions of the same ply}	B60C9/02	B60C9/02		267
B60C2009/0215	9	{Partial carcass reinforcing plies, i.e. the plies neither crossing the equatorial plane nor folded around the bead core}	B60C9/02	B60C9/02		73
B60C2009/0223	9	{comprising a cushion layer between adjacent carcass plies}	B60C9/02	B60C9/02		26
B60C9/023	9	{built up from narrow strips, individual cords or filaments, e.g. using filament winding}	B60C9/02	B60C9/02		267
B60C9/0238	9	{characterised by special physical properties of the carcass ply}	B60C9/02	B60C9/02		70
B60C2009/0246	10	{Modulus of the ply}	B60C9/02	B60C9/02		22
B60C2009/0253	11	{being different between adjacent plies}	B60C9/02	B60C9/02		14
B60C2009/0261	11	{being different within the same ply}	B60C9/02	B60C9/02		1
B60C2009/0269	9	{Physical properties or dimensions of the carcass coating rubber}	B60C9/02	B60C9/02		57
B60C2009/0276	10	{Modulus; Hardness; Loss modulus or "tangens delta"}	B60C9/02	B60C9/02		88
B60C2009/0284	10	{Thickness}	B60C9/02	B60C9/02		77
B60C9/0292	9	{Carcass ply curvature (sidewall curvature B60C13/003)}	B60C9/02	B60C9/02		180
B60C9/04	9	the reinforcing cords of each carcass ply arranged in a substantially parallel relationship	B60C9/04	B60C9/04		384
B60C2009/0408	10	{Carcass joints or splices}	B60C9/04	B60C9/04		23
B60C2009/0416	10	{Physical properties or dimensions of the carcass cords}	B60C9/04	B60C9/04		115
B60C2009/0425	11	{Diameters of the cords; Linear density thereof}	B60C9/04	B60C9/04		202
B60C2009/0433	11	{Modulus}	B60C9/04	B60C9/04		47
B60C2009/0441	11	{Density in width direction}	B60C9/04	B60C9/04		71
B60C2009/045	11	{Tensile strength}	B60C9/04	B60C9/04		71
B60C2009/0458	11	{Elongation of the reinforcements at break point}	B60C9/04	B60C9/04		53
B60C2009/0466	11	{Twist structures}	B60C9/04	B60C9/04		128
B60C2009/0475	10	{Particular materials of the carcass cords}	B60C9/04	B60C9/04		163
B60C2009/0483	10	{Different cords in the same layer}	B60C9/04	B60C9/04		19
B60C2009/0491	10	{with special path of the carcass cords, e.g. sinusoidal}	B60C9/04	B60C9/04		33
B60C9/06	10	the cords extend diagonally from bead to bead and run in opposite directions in each successive carcass ply, i.e. bias angle ply (B60C9/07, B60C9/09 take precedence)	B60C9/06	B60C9/06		426
B60C9/07	10	the cords curve from bead to bead in plural planes, e.g. S-shaped cords	B60C9/07	B60C9/07		139
B60C9/08	10	the cords extend transversely from bead to bead, i.e. radial ply (B60C9/07 takes precedence)	B60C9/08	B60C9/08		723
B60C9/09	11	combined with other carcass plies having cords extending diagonally from bead to bead, i.e. combined radial ply and bias angle ply	B60C9/09	B60C9/09		300
B60C9/10	9	the reinforcing cords within each carcass ply arranged in a crossing relationship	B60C9/10	B60C9/10		104
B60C9/11	10	Woven, braided, or knitted plies	B60C9/11	B60C9/11		101
B60C9/12	9	built-up with rubberised layers of discrete fibres or filaments	B60C9/12	B60C9/12		162
B60C9/13	10	with two or more differing cord materials	B60C9/13	B60C9/13		23
B60C9/14	9	built-up with sheets, webs, or films of homogeneous material, e.g. synthetics, sheet metal, rubber	B60C9/14	B60C9/14		277
B60C2009/145	10	{at the inner side of the carcass structure}	B60C9/14	B60C9/14		46
B60C9/16	9	built-up with metallic reinforcing inlays	B60C9/16	B60C9/16		306
B60C9/17	9	asymmetric to the midcircumferential plane of the tyre	B60C9/17	B60C9/17		68
B60C9/18	8	Structure or arrangement of belts or breakers, crown-reinforcing or cushioning layers	B60C9/18	B60C9/18		1732
B60C9/1807	9	{comprising fabric reinforcements}	B60C9/18	B60C9/18		190
B60C2009/1814	10	{square woven}	B60C9/18	B60C9/18		29
B60C9/1821	9	{comprising discrete fibres or filaments}	B60C9/18	B60C9/18		298
B60C2009/1828	9	{characterised by special physical properties of the belt ply}	B60C9/18	B60C9/18		124
B60C9/1835	9	{Rubber strips or cushions at the belt edges}	B60C9/18	B60C9/18		211
B60C2009/1842	10	{Width or thickness of the strips or cushions}	B60C9/18	B60C9/18		191
B60C9/185	10	{between adjacent or radially below the belt plies}	B60C9/18	B60C9/18		195
B60C2009/1857	10	{radially above the belt plies}	B60C9/18	B60C9/18		29
B60C2009/1864	10	{wrapped around the edges of the belt}	B60C9/18	B60C9/18		84
B60C2009/1871	9	{with flat cushions or shear layers between belt layers}	B60C9/18	B60C9/18		129
B60C2009/1878	9	{with flat cushions or shear layers between the carcass and the belt}	B60C9/18	B60C9/18		102
B60C2009/1885	9	{with belt ply between adjacent carcass plies}	B60C9/18	B60C9/18		9
B60C2009/1892	9	{with belt ply radial inside the carcass structure}	B60C9/18	B60C9/18		29
B60C9/20	9	built-up from rubberised plies each having all cords arranged substantially parallel	B60C9/20	B60C9/20		1374
B60C9/2003	10	{characterised by the materials of the belt cords}	B60C9/20	B60C9/20		160
B60C9/2006	11	{consisting of steel cord plies only}	B60C9/20	B60C9/20		1140
B60C9/2009	11	{comprising plies of different materials}	B60C9/20	B60C9/20		906
B60C2009/2012	10	{with particular configuration of the belt cords in the respective belt layers}	B60C9/20	B60C9/20		159
B60C2009/2016	11	{comprising cords at an angle of 10 to 30 degrees to the circumferential direction}	B60C9/20	B60C9/20		360
B60C2009/2019	11	{comprising cords at an angle of 30 to 60 degrees to the circumferential direction}	B60C9/20	B60C9/20		244
B60C2009/2022	11	{comprising cords at an angle of 60 to 90 degrees to the circumferential direction}	B60C9/20	B60C9/20		122
B60C2009/2025	11	{with angle different or variable in the same layer}	B60C9/20	B60C9/20		69
B60C2009/2029	11	{with different cords in the same layer, i.e. cords with different materials or dimensions}	B60C9/20	B60C9/20		66
B60C2009/2032	11	{characterised by the course of the belt cords, e.g. undulated or sinusoidal}	B60C9/20	B60C9/20		44
B60C2009/2035	10	{built-up by narrow strips}	B60C9/20	B60C9/20		84
B60C2009/2038	10	{using lateral belt strips at belt edges, e.g. edge bands}	B60C9/20	B60C9/20		127
B60C2009/2041	10	{with an interrupted belt ply, e.g. using two or more portions of the same ply}	B60C9/20	B60C9/20		127
B60C2009/2045	10	{with belt joints or splices}	B60C9/20	B60C9/20		20
B60C2009/2048	10	{characterised by special physical properties of the belt plies}	B60C9/20	B60C9/20		68
B60C2009/2051	11	{Modulus of the ply}	B60C9/20	B60C9/20		45
B60C2009/2054	12	{being different within the same ply}	B60C9/20	B60C9/20		6
B60C2009/2058	12	{being different between adjacent plies}	B60C9/20	B60C9/20		15
B60C2009/2061	10	{Physical properties or dimensions of the belt coating rubber}	B60C9/20	B60C9/20		61
B60C2009/2064	11	{Modulus; Hardness; Loss modulus or "tangens delta"}	B60C9/20	B60C9/20		154
B60C2009/2067	11	{Thickness}	B60C9/20	B60C9/20		111
B60C2009/207	11	{Double layers, e.g. using different rubbers in the same belt ply}	B60C9/20	B60C9/20		13
B60C2009/2074	10	{Physical properties or dimension of the belt cord}	B60C9/20	B60C9/20		147
B60C2009/2077	11	{Diameters of the cords; Linear density thereof}	B60C9/20	B60C9/20		378
B60C2009/208	11	{Modulus of the cords}	B60C9/20	B60C9/20		93
B60C2009/2083	11	{Density in width direction}	B60C9/20	B60C9/20		209
B60C2009/2087	12	{with variable density in the same layer}	B60C9/20	B60C9/20		26
B60C2009/209	11	{Tensile strength}	B60C9/20	B60C9/20		145
B60C2009/2093	11	{Elongation of the reinforcements at break point}	B60C9/20	B60C9/20		84
B60C2009/2096	11	{Twist structures}	B60C9/20	B60C9/20		178
B60C9/22	10	the plies being arranged with all cords disposed along the circumference of the tyre	B60C9/22	B60C9/22		996
B60C9/2204	11	{obtained by circumferentially narrow strip winding}	B60C9/22	B60C9/22		623
B60C2009/2209	12	{characterised by tension of the cord during winding}	B60C9/22	B60C9/22		50
B60C2009/2214	11	{characterised by the materials of the zero degree ply cords}	B60C9/22	B60C9/22		214
B60C2009/2219	11	{with a partial zero degree ply at the belt edges - edge band}	B60C9/22	B60C9/22		145
B60C2009/2223	11	{with an interrupted zero degree ply, e.g. using two or more portions for the same ply}	B60C9/22	B60C9/22		76
B60C2009/2228	11	{characterised by special physical properties of the zero degree plies}	B60C9/22	B60C9/22		20
B60C2009/2233	12	{Modulus of the zero degree ply}	B60C9/22	B60C9/22		32
B60C2009/2238	11	{Physical properties or dimensions of the ply coating rubber}	B60C9/22	B60C9/22		60
B60C2009/2242	12	{Modulus; Hardness; Loss modulus or "tangens delta"}	B60C9/22	B60C9/22		57
B60C2009/2247	12	{Thickness}	B60C9/22	B60C9/22		48
B60C2009/2252	11	{Physical properties or dimension of the zero degree ply cords}	B60C9/22	B60C9/22		69
B60C2009/2257	12	{Diameters of the cords; Linear density thereof}	B60C9/22	B60C9/22		153
B60C2009/2261	12	{Modulus of the cords}	B60C9/22	B60C9/22		115
B60C2009/2266	12	{Density of the cords in width direction}	B60C9/22	B60C9/22		101
B60C2009/2271	13	{with variable density}	B60C9/22	B60C9/22		84
B60C2009/2276	12	{Tensile strength}	B60C9/22	B60C9/22		50
B60C2009/228	12	{Elongation of the reinforcements at break point}	B60C9/22	B60C9/22		48
B60C2009/2285	12	{Twist structures}	B60C9/22	B60C9/22		97
B60C2009/229	12	{characterised by the course of the cords, e.g. undulated or sinusoidal}	B60C9/22	B60C9/22		13
B60C2009/2295	12	{with different cords in the same layer}	B60C9/22	B60C9/22		56
B60C9/24	9	built-up of arcuate parts	B60C9/24	B60C9/24		18
B60C9/26	9	Folded plies	B60C9/26	B60C9/26		398
B60C9/263	10	{further characterised by an endless zigzag configuration in at least one belt ply, i.e. no cut edge being present}	B60C9/26	B60C9/26		256
B60C2009/266	11	{combined with non folded cut-belt plies}	B60C9/26	B60C9/26		58
B60C9/28	9	characterised by the belt or breaker dimensions or curvature relative to carcass (B60C9/30 takes precedence)	B60C9/28	B60C9/28		734
B60C2009/283	10	{characterised by belt curvature}	B60C9/28	B60C9/28		44
B60C2009/286	11	{being substantially flat}	B60C9/28	B60C9/28		5
B60C9/30	9	asymmetric to the midcircumferential plane of the tyre	B60C9/30	B60C9/30		131
B60C11/00	7	Tyre tread bands; Tread patterns; Anti-skid inserts	B60C11/00	B60C11/00		1772
B60C11/0008	8	{characterised by the tread rubber}	B60C11/00	B60C11/00		599
B60C2011/0016	9	{Physical properties or dimensions}	B60C11/00	B60C11/00		476
B60C2011/0025	10	{Modulus or tan delta}	B60C11/00	B60C11/00		965
B60C2011/0033	10	{Thickness of the tread}	B60C11/00	B60C11/00		468
B60C11/0041	8	{comprising different tread rubber layers}	B60C11/00	B60C11/00		244
B60C11/005	9	{with cap and base layers}	B60C11/00	B60C11/00		1081
B60C11/0058	10	{with different cap rubber layers in the axial direction}	B60C11/00	B60C11/00		486
B60C11/0066	11	{having an asymmetric arrangement}	B60C11/00	B60C11/00		83
B60C11/0075	10	{with different base rubber layers in the axial direction}	B60C11/00	B60C11/00		147
B60C11/0083	8	{characterised by the curvature of the tyre tread}	B60C11/00	B60C11/00		634
B60C2011/0091	8	{built-up by narrow strip winding}	B60C11/00	B60C11/00		33
B60C11/01	8	Shape of the shoulders between tread and sidewall, e.g. rounded, stepped or cantilevered	B60C11/01	B60C11/01		1401
B60C2011/013	9	{provided with a recessed portion}	B60C11/01	B60C11/01		431
B60C2011/016	9	{different rubber for tread wings}	B60C11/01	B60C11/01		51
B60C11/02	8	Replaceable treads	B60C11/02	B60C11/02		836
B60C11/03	8	Tread patterns	B60C11/03	B60C11/03		1643
B60C11/0302	9	{directional pattern, i.e. with main rolling direction}	B60C11/03	B60C11/03		1549
B60C11/0304	9	{Asymmetric patterns}	B60C11/03	B60C11/03		1283
B60C11/0306	9	{Patterns comprising block rows or discontinuous ribs}	B60C11/03	B60C11/03		2323
B60C11/0309	10	{further characterised by the groove cross-section}	B60C11/03	B60C11/03		1047
B60C11/0311	9	{Patterns comprising tread lugs arranged parallel or oblique to the axis of rotation}	B60C11/03	B60C11/03		717
B60C2011/0313	10	{directional type}	B60C11/03	B60C11/03		199
B60C11/0316	10	{further characterised by the groove cross-section}	B60C11/03	B60C11/03		277
B60C11/0318	9	{irregular patterns with particular pitch sequence}	B60C11/03	B60C11/03		575
B60C11/032	9	{Patterns comprising isolated recesses}	B60C11/03	B60C11/03		903
B60C11/0323	10	{tread comprising channels under the tread surface, e.g. for draining water}	B60C11/03	B60C11/03		538
B60C11/0327	9	{characterised by special properties of the tread pattern}	B60C11/03	B60C11/03		303
B60C11/033	10	{by the void or net-to-gross ratios of the patterns}	B60C11/03	B60C11/03		722
B60C11/0332	10	{by the footprint-ground contacting area of the tyre tread}	B60C11/03	B60C11/03		439
B60C2011/0334	10	{Stiffness}	B60C11/03	B60C11/03		173
B60C2011/0337	9	{characterised by particular design features of the pattern}	B60C11/03	B60C11/03		238
B60C2011/0339	10	{Grooves}	B60C11/03	B60C11/03		284
B60C2011/0341	11	{Circumferential grooves}	B60C11/03	B60C11/03		971
B60C2011/0344	12	{provided at the equatorial plane}	B60C11/03	B60C11/03		289
B60C2011/0346	12	{with zigzag shape}	B60C11/03	B60C11/03		672
B60C2011/0348	12	{Narrow grooves, i.e. having a width of less than 4 mm}	B60C11/03	B60C11/03		470
B60C2011/0351	12	{Shallow grooves, i.e. having a depth of less than 50% of other grooves}	B60C11/03	B60C11/03		120
B60C2011/0353	12	{characterised by width}	B60C11/03	B60C11/03		640
B60C2011/0355	12	{characterised by depth}	B60C11/03	B60C11/03		582
B60C2011/0358	11	{Lateral grooves, i.e. having an angle of 45 to 90 degees to the equatorial plane}	B60C11/03	B60C11/03		621
B60C2011/036	12	{Narrow grooves, i.e. having a width of less than 3 mm}	B60C11/03	B60C11/03		224
B60C2011/0362	12	{Shallow grooves, i.e. having a depth of less than 50% of other grooves}	B60C11/03	B60C11/03		136
B60C2011/0365	12	{characterised by width}	B60C11/03	B60C11/03		569
B60C2011/0367	12	{characterised by depth}	B60C11/03	B60C11/03		307
B60C2011/0369	13	{with varying depth of the groove}	B60C11/03	B60C11/03		338
B60C2011/0372	12	{with particular inclination angles}	B60C11/03	B60C11/03		515
B60C2011/0374	11	{Slant grooves, i.e. having an angle of about 5 to 35 degrees to the equatorial plane}	B60C11/03	B60C11/03		746
B60C2011/0376	12	{characterised by width}	B60C11/03	B60C11/03		119
B60C2011/0379	12	{characterised by depth}	B60C11/03	B60C11/03		77
B60C2011/0381	11	{Blind or isolated grooves}	B60C11/03	B60C11/03		739
B60C2011/0383	12	{at the centre of the tread}	B60C11/03	B60C11/03		552
B60C2011/0386	10	{Continuous ribs}	B60C11/03	B60C11/03		176
B60C2011/0388	11	{provided at the equatorial plane}	B60C11/03	B60C11/03		807
B60C2011/039	11	{provided at the shoulder portion}	B60C11/03	B60C11/03		239
B60C2011/0393	11	{Narrow ribs, i.e. having a rib width of less than 8 mm}	B60C11/03	B60C11/03		43
B60C2011/0395	12	{for linking shoulder blocks}	B60C11/03	B60C11/03		64
B60C2011/0397	11	{Sacrificial ribs, i.e. ribs recessed from outer tread contour}	B60C11/03	B60C11/03		34
B60C11/04	9	in which the raised area of the pattern consists only of continuous circumferential ribs, e.g. zig-zag (B60C11/12, B60C11/13 take precedence)	B60C11/04	B60C11/04		1055
B60C11/042	10	{further characterised by the groove cross-section}	B60C11/04	B60C11/04		622
B60C11/045	11	{the groove walls having a three-dimensional shape}	B60C11/04	B60C11/04		148
B60C11/047	11	{the groove bottom comprising stone trapping protection elements, e.g. ribs}	B60C11/04	B60C11/04		251
B60C11/11	9	in which the raised area of the pattern consists only of isolated elements, e.g. blocks (B60C11/12, B60C11/13 take precedence)	B60C11/11	B60C11/11		1861
B60C11/12	9	characterised by the use of narrow slits or incisions, e.g. sipes	B60C11/12	B60C11/12		1868
B60C11/1204	10	{with special shape of the sipe}	B60C11/12	B60C11/12		773
B60C2011/1209	11	{straight at the tread surface}	B60C11/12	B60C11/12		830
B60C2011/1213	11	{sinusoidal or zigzag at the tread surface}	B60C11/12	B60C11/12		1455
B60C11/1218	11	{Three-dimensional shape with regard to depth and extending direction}	B60C11/12	B60C11/12		782
B60C11/1222	11	{Twisted or warped shape in the sipe plane}	B60C11/12	B60C11/12		58
B60C2011/1227	11	{having different shape within the pattern}	B60C11/12	B60C11/12		235
B60C2011/1231	11	{being shallow, i.e. sipe depth of less than 3 mm}	B60C11/12	B60C11/12		195
B60C11/1236	10	{with special arrangements in the tread pattern}	B60C11/12	B60C11/12		1132
B60C11/124	11	{inclined with regard to a plane normal to the tread surface}	B60C11/12	B60C11/12		239
B60C2011/1245	11	{being arranged in crossing relation, e.g. sipe mesh}	B60C11/12	B60C11/12		266
B60C11/125	11	{arranged at the groove bottom}	B60C11/12	B60C11/12		327
B60C2011/1254	11	{with closed sipe, i.e. not extending to a groove}	B60C11/12	B60C11/12		633
B60C11/1259	10	{Depth of the sipe}	B60C11/12	B60C11/12		507
B60C11/1263	11	{different within the same sipe}	B60C11/12	B60C11/12		455
B60C2011/1268	11	{being different from sipe to sipe}	B60C11/12	B60C11/12		288
B60C11/1272	10	{Width of the sipe}	B60C11/12	B60C11/12		419
B60C2011/1277	11	{being narrow, i.e. less than 0.3 mm}	B60C11/12	B60C11/12		46
B60C11/1281	11	{different within the same sipe, i.e. enlarged width portion at sipe bottom or along its length}	B60C11/12	B60C11/12		801
B60C2011/1286	11	{being different from sipe to sipe}	B60C11/12	B60C11/12		169
B60C2011/129	10	{Sipe density, i.e. the distance between the sipes within the pattern}	B60C11/12	B60C11/12		187
B60C2011/1295	11	{variable}	B60C11/12	B60C11/12		120
B60C11/13	9	characterised by the groove cross-section, e.g. for buttressing or preventing stone-trapping	B60C11/13	B60C11/13		1434
B60C11/1307	10	{with special features of the groove walls}	B60C11/13	B60C11/13		428
B60C11/1315	11	{having variable inclination angles, e.g. warped groove walls}	B60C11/13	B60C11/13		356
B60C11/1323	11	{asymmetric}	B60C11/13	B60C11/13		365
B60C2011/133	11	{comprising recesses}	B60C11/13	B60C11/13		345
B60C2011/1338	11	{comprising protrusions}	B60C11/13	B60C11/13		468
B60C11/1346	11	{covered by a rubber different from the tread rubber}	B60C11/13	B60C11/13		219
B60C11/1353	10	{with special features of the groove bottom}	B60C11/13	B60C11/13		370
B60C2011/1361	11	{with protrusions extending from the groove bottom}	B60C11/13	B60C11/13		466
B60C11/1369	10	{Tie bars for linking block elements and bridging the groove}	B60C11/13	B60C11/13		618
B60C11/1376	10	{Three dimensional block surfaces departing from the enveloping tread contour}	B60C11/13	B60C11/13		301
B60C11/1384	11	{with chamfered block corners}	B60C11/13	B60C11/13		261
B60C11/1392	11	{with chamfered block edges}	B60C11/13	B60C11/13		514
B60C11/14	8	Anti-skid inserts, e.g. vulcanised into the tread band	B60C11/14	B60C11/14		589
B60C2011/142	9	{Granular particles, e.g. hard granules}	B60C11/14	B60C11/14		25
B60C2011/145	9	{Discontinuous fibres}	B60C11/14	B60C11/14		71
B60C2011/147	9	{Foamed rubber or sponge rubber on the tread band}	B60C11/14	B60C11/14		67
B60C11/16	9	of plug form, e.g. made from metal, textile	B60C11/16	B60C11/16		957
B60C11/1606	10	{retractable plug}	B60C11/16	B60C11/16		169
B60C11/1612	11	{actuated by fluid, e.g. using fluid pressure difference}	B60C11/16	B60C11/16		338
B60C11/1618	11	{actuated by temperature, e.g. by means of temperature sensitive elements}	B60C11/16	B60C11/16		58
B60C11/1625	10	{Arrangements thereof in the tread patterns, e.g. irregular}	B60C11/16	B60C11/16		234
B60C11/1631	10	{inclined with regard to the radial direction}	B60C11/16	B60C11/16		17
B60C11/1637	10	{Attachment of the plugs into the tread, e.g. screwed}	B60C11/16	B60C11/16		138
B60C11/1643	10	{with special shape of the plug-body portion, i.e. not cylindrical}	B60C11/16	B60C11/16		162
B60C11/165	11	{conical}	B60C11/16	B60C11/16		26
B60C11/1656	11	{concave or convex, e.g. barrel-shaped}	B60C11/16	B60C11/16		83
B60C11/1662	11	{helical-shaped}	B60C11/16	B60C11/16		2
B60C11/1668	11	{with an additional collar}	B60C11/16	B60C11/16		52
B60C11/1675	10	{with special shape of the plug- tip}	B60C11/16	B60C11/16		166
B60C11/1681	11	{Spherical top portions}	B60C11/16	B60C11/16		8
B60C11/1687	11	{Multiple tips}	B60C11/16	B60C11/16		19
B60C11/1693	10	{Attachment of the plug-tip within the plug-body}	B60C11/16	B60C11/16		44
B60C11/18	9	of strip form, e.g. metallic combs, rubber strips of different wear resistance (B60C11/20 takes precedence)	B60C11/18	B60C11/18		306
B60C11/185	10	{of metal comb form, lamellar shaped or blade-like}	B60C11/18	B60C11/18		114
B60C11/20	9	in coiled form	B60C11/20	B60C11/20		83
B60C11/22	8	Tread rings between dual tyres	B60C11/22	B60C11/22		108
B60C11/24	8	Wear-indicating arrangements	B60C11/24	B60C11/24		935
B60C11/243	9	{Tread wear sensors, e.g. electronic sensors}	B60C11/24	B60C11/24		431
B60C11/246	9	{Tread wear monitoring systems}	B60C11/24	B60C11/24		865
B60C13/00	7	Tyre sidewalls; Protecting, decorating, marking, or the like, thereof (B60C17/08 takes precedence; tyre shoulders B60C11/01; removable tyre sidewall trim rings B60B7/01)	B60C13/00	B60C13/00		1053
B60C13/001	8	{Decorating, marking or the like}	B60C13/00	B60C13/00		1024
B60C13/002	8	{Protection against exterior elements}	B60C13/00	B60C13/00		332
B60C13/003	8	{characterised by sidewall curvature}	B60C13/00	B60C13/00		180
B60C13/004	9	{of the internal side of the tyre}	B60C13/00	B60C13/00		35
B60C2013/005	8	{Physical properties of the sidewall rubber}	B60C13/00	B60C13/00		72
B60C2013/006	9	{Modulus; Hardness; Loss modulus or "tangens delta"}	B60C13/00	B60C13/00		179
B60C2013/007	9	{Thickness}	B60C13/00	B60C13/00		199
B60C2013/008	8	{built-up by narrow strip winding}	B60C13/00	B60C13/00		6
B60C13/009	8	{comprising additional bead cores in the sidewall}	B60C13/00	B60C13/00		52
B60C13/02	8	Arrangement of grooves or ribs	B60C13/02	B60C13/02		857
B60C13/023	9	{preventing watersplash}	B60C13/02	B60C13/02		40
B60C2013/026	9	{provided at the interior side only}	B60C13/00	B60C13/02		51
B60C13/04	8	having annular inlays or covers, e.g. white sidewalls	B60C13/04	B60C13/04		342
B60C2013/045	9	{comprising different sidewall rubber layers}	B60C13/04	B60C13/04		159
B60C15/00	7	Tyre beads, e.g. ply turn-up or overlap	B60C15/00	B60C15/00		341
B60C15/0009	8	{features of the carcass terminal portion}	B60C15/00	B60C15/00		348
B60C15/0018	9	{not folded around the bead core, e.g. floating or down ply}	B60C15/00	B60C15/00		505
B60C15/0027	9	{with low ply turn-up, i.e. folded around the bead core and terminating at the bead core}	B60C15/00	B60C15/00		275
B60C15/0036	9	{with high ply turn-up, i.e. folded around the bead core and terminating radially above the point of maximum section width}	B60C15/00	B60C15/00		244
B60C15/0045	10	{with ply turn-up up to the belt edges, i.e. folded around the bead core and extending to the belt edges}	B60C15/00	B60C15/00		318
B60C15/0054	9	{with ply turn-up portion parallel and adjacent to carcass main portion}	B60C15/00	B60C15/00		103
B60C15/0063	9	{with ply turn-up portion diverging from carcass main portion}	B60C15/00	B60C15/00		23
B60C15/0072	9	{with ply reverse folding, i.e. carcass layer folded around the bead core from the outside to the inside}	B60C15/00	B60C15/00		258
B60C15/0081	9	{the carcass plies folded around or between more than one bead core}	B60C15/00	B60C15/00		163
B60C2015/009	9	{Height of the carcass terminal portion defined in terms of a numerical value or ratio in proportion to section height}	B60C15/00	B60C15/00		239
B60C15/02	8	Seating or securing beads on rims (sealing means between beads and rims of tubeless tyres B60C5/16; means for securing solid tyres on rims B60C7/24)	B60C15/02	B60C15/02		491
B60C15/0203	9	{using axially extending bead seating, i.e. the bead and the lower sidewall portion extend in the axial direction (B60C15/0206 takes precedence)}	B60C15/02	B60C15/02		112
B60C15/0206	9	{using inside rim bead seating, i.e. the bead being seated at a radially inner side of the rim}	B60C15/02	B60C15/02		208
B60C15/0209	9	{Supplementary means for securing the bead}	B60C15/02	B60C15/02		123
B60C15/0213	10	{the bead being clamped by rings, cables, rim flanges or other parts of the rim}	B60C15/02	B60C15/02		222
B60C15/0216	10	{the bead being pierced by bolts, rivets, clips or other elements}	B60C15/02	B60C15/02		50
B60C15/022	10	{the bead being secured by turned-in rim flanges, e.g. rim of the clincher type}	B60C15/02	B60C15/02		72
B60C15/0223	10	{the bead being secured by clip-hook elements not forming part of the rim flange}	B60C15/02	B60C15/02		54
B60C15/0226	10	{the bead being secured by protrusions of the rim extending from the bead seat, e.g. hump or serrations}	B60C15/02	B60C15/02		179
B60C15/023	10	{the bead being secured by bead extensions which extend over and wrap around the rim flange}	B60C15/02	B60C15/02		48
B60C15/0233	9	{Securing tyres without beads; Securing closed torus or tubular tyres}	B60C15/02	B60C15/02		163
B60C15/0236	9	{Asymmetric bead seats, e.g. different bead diameter or inclination angle (asymmetric transverse section B60C3/06)}	B60C15/02	B60C15/02		108
B60C15/024	9	Bead contour, e.g. lips, grooves, or ribs	B60C15/024	B60C15/024		671
B60C15/0242	10	{with bead extensions located radially outside the rim flange position, e.g. rim flange protectors}	B60C15/024	B60C15/024		89
B60C2015/0245	10	{Bead lips at the bead toe portion, i.e. the axially and radially inner end of the bead}	B60C15/024	B60C15/024		45
B60C15/0247	10	{with reverse bead seat inclination, i.e. the axially inner diameter of the bead seat is bigger than the axially outer diameter thereof}	B60C15/024	B60C15/024		78
B60C15/028	9	Spacers between beads (emergency load-supporting means B60C17/00)	B60C15/028	B60C15/028		446
B60C15/032	10	inflatable	B60C15/032	B60C15/032		54
B60C15/036	9	Tyres permanently fixed to the rim, e.g. by adhesive, by vulcanisation	B60C15/036	B60C15/036		56
B60C15/04	8	Bead cores	B60C15/04	B60C15/04		1163
B60C2015/042	9	{characterised by the material of the core, e.g. alloy}	B60C15/04	B60C15/04		161
B60C2015/044	9	{characterised by a wrapping layer}	B60C15/04	B60C15/04		222
B60C2015/046	9	{Cable cores, i.e. cores made-up of twisted wires}	B60C15/04	B60C15/04		156
B60C2015/048	9	{Polygonal cores characterised by the winding sequence}	B60C15/04	B60C15/04		127
B60C15/05	9	multiple, i.e. with two or more cores in each bead	B60C15/05	B60C15/05		239
B60C15/06	8	Flipper strips, fillers, or chafing strips {and reinforcing layers for the construction of the bead}	B60C15/06	B60C15/06		1623
B60C15/0603	9	{characterised by features of the bead filler or apex}	B60C15/06	B60C15/06		464
B60C15/0607	10	{comprising several parts, e.g. made of different rubbers}	B60C15/06	B60C15/06		639
B60C2015/061	10	{Dimensions of the bead filler in terms of numerical values or ratio in proportion to section height}	B60C15/06	B60C15/06		254
B60C2015/0614	9	{characterised by features of the chafer or clinch portion, i.e. the part of the bead contacting the rim}	B60C15/06	B60C15/06		561
B60C2015/0617	9	{comprising a cushion rubber other than the chafer or clinch rubber}	B60C15/06	B60C15/06		120
B60C2015/0621	10	{adjacent to the carcass turnup portion}	B60C15/06	B60C15/06		253
B60C2015/0625	10	{provided at the terminal edge portion of a carcass or reinforcing layer}	B60C15/06	B60C15/06		97
B60C15/0628	9	{comprising a bead reinforcing layer}	B60C15/06	B60C15/06		300
B60C15/0632	10	{using flippers in contact with and wrapped around the bead core and, at least partially, in contact with the bead filler}	B60C15/06	B60C15/06		81
B60C15/0635	10	{using chippers between the carcass layer and chafer rubber wrapped around the bead}	B60C15/06	B60C15/06		131
B60C2015/0639	10	{between carcass main portion and bead filler not wrapped around the bead core}	B60C15/06	B60C15/06		82
B60C2015/0642	10	{between carcass turn-up and bead filler not wrapped around the bead core}	B60C15/06	B60C15/06		55
B60C2015/0646	10	{at the axially inner side of the carcass main portion not wrapped around the bead core}	B60C15/06	B60C15/06		24
B60C2015/065	10	{at the axially outer side of the carcass turn-up portion not wrapped around the bead core}	B60C15/06	B60C15/06		122
B60C15/0653	10	{with particular configuration of the cords in the respective bead reinforcing layer}	B60C15/06	B60C15/06		49
B60C2015/0657	11	{comprising cords at an angle of maximal 10 degrees to the circumferential direction}	B60C15/06	B60C15/06		21
B60C2015/066	11	{comprising cords at an angle of 10 to 30 degrees to the circumferential direction}	B60C15/06	B60C15/06		20
B60C2015/0664	11	{comprising cords at an angle of 30 to 60 degrees to the circumferential direction}	B60C15/06	B60C15/06		28
B60C2015/0667	11	{comprising cords at an angle of 60 to 90 degrees to the circumferential direction}	B60C15/06	B60C15/06		17
B60C2015/0671	11	{the cord angle being different or variable within the same layer}	B60C15/06	B60C15/06		3
B60C2015/0675	11	{characterised by the course of the cords, e.g. undulated or sinusoidal}	B60C15/06	B60C15/06		11
B60C2015/0678	10	{Physical properties of the bead reinforcing layer, e.g. modulus of the ply}	B60C15/06	B60C15/06		67
B60C2015/0682	10	{Physical properties or dimensions of the coating rubber}	B60C15/06	B60C15/06		26
B60C2015/0685	10	{Physical properties or dimensions of the cords, e.g. modulus of the cords}	B60C15/06	B60C15/06		34
B60C2015/0689	11	{Cord density in width direction}	B60C15/06	B60C15/06		17
B60C2015/0692	10	{characterised by particular materials of the cords}	B60C15/06	B60C15/06		67
B60C2015/0696	9	{Asymmetric bead reinforcement, e.g. arrangement of bead reinforcing layer or apex}	B60C15/06	B60C15/06		42
B60C17/00	7	Tyres characterised by means enabling restricted operation in damaged or deflated condition; Accessories therefor	B60C17/00	B60C17/00		688
B60C17/0009	8	{comprising sidewall rubber inserts, e.g. crescent shaped inserts}	B60C17/00	B60C17/00		677
B60C17/0018	9	{two or more inserts in each sidewall portion}	B60C17/00	B60C17/00		128
B60C17/0027	9	{comprising portions of different rubbers in a single insert}	B60C17/00	B60C17/00		70
B60C17/0036	9	{comprising additional reinforcements}	B60C17/00	B60C17/00		52
B60C17/0045	9	{comprising grooves or ribs, e.g. at the inner side of the insert}	B60C17/00	B60C17/00		23
B60C2017/0054	9	{Physical properties or dimensions of the inserts}	B60C17/00	B60C17/00		48
B60C2017/0063	10	{Modulus; Hardness; Loss modulus or "tangens delta"}	B60C17/00	B60C17/00		90
B60C2017/0072	10	{Thickness}	B60C17/00	B60C17/00		76
B60C2017/0081	8	{comprising special reinforcing means in the crown area}	B60C17/00	B60C17/00		69
B60C17/009	8	{comprising annular protrusions projecting into the tyre cavity}	B60C17/00	B60C17/00		96
B60C17/01	8	utilising additional inflatable supports which become load-supporting in emergency	B60C17/01	B60C17/01		445
B60C17/02	9	inflated or expanded in emergency only	B60C17/02	B60C17/02		273
B60C17/04	8	utilising additional non-inflatable supports which become load-supporting in emergency	B60C17/04	B60C17/04		806
B60C17/041	9	{characterised by coupling or locking means between rim and support}	B60C17/04	B60C17/04		337
B60C17/042	10	{preventing sliding or rotation between support and rim}	B60C17/04	B60C17/04		101
B60C17/043	9	{made-up of an annular metallic shell}	B60C17/04	B60C17/04		105
B60C17/044	9	{Expandable supports}	B60C17/04	B60C17/04		47
B60C17/045	9	{Rotatable supports relative to the rim}	B60C17/04	B60C17/04		56
B60C17/046	10	{by means of ball bearings}	B60C17/04	B60C17/04		9
B60C17/047	9	{comprising circumferential ribs}	B60C17/04	B60C17/04		87
B60C17/048	9	{comprising transverse ribs}	B60C17/04	B60C17/04		43
B60C17/06	9	resilient	B60C17/06	B60C17/06		953
B60C17/061	10	{comprising lateral openings}	B60C17/06	B60C17/06		107
B60C2017/063	10	{comprising circumferentially extending reinforcements}	B60C17/06	B60C17/06		52
B60C17/065	10	{made-up of foam inserts (tyres filled with foam B60C5/002)}	B60C17/06	B60C17/06		199
B60C17/066	10	{made-up of plural spherical elements provided in the tyre chamber}	B60C17/06	B60C17/06		78
B60C2017/068	10	{comprising springs, e.g. helical springs}	B60C17/06	B60C17/06		218
B60C17/08	8	Means facilitating folding of sidewalls, e.g. run-flat sidewalls	B60C17/08	B60C17/08		65
B60C17/10	8	Internal lubrication	B60C17/10	B60C17/10		266
B60C17/103	9	{by means of surface coating, e.g. PTFE}	B60C17/10	B60C17/10		22
B60C17/106	9	{Composition of the lubricant}	B60C17/10	B60C17/10		7
B60C19/00	7	Tyre parts or constructions not otherwise provided for	B60C19/00	B60C19/00		2286
B60C19/001	8	{Tyres requiring an asymmetric or a special mounting}	B60C19/00	B60C19/00		373
B60C19/002	8	{Noise damping elements provided in the tyre structure or attached thereto, e.g. in the tyre interior}	B60C19/00	B60C19/00		1286
B60C19/003	8	{Balancing means attached to the tyre}	B60C19/00	B60C19/00		166
B60C2019/004	8	{Tyre sensors other than for detecting tyre pressure}	B60C19/00	B60C19/00		819
B60C2019/005	8	{Magnets integrated within the tyre structure}	B60C19/00	B60C19/00		108
B60C2019/006	8	{Warning devices, e.g. devices generating noise due to flat or worn tyres}	B60C19/00	B60C19/00		220
B60C2019/007	9	{triggered by sensors}	B60C19/00	B60C19/00		245
B60C2019/008	8	{Venting means, e.g. for expelling entrapped air}	B60C19/00	B60C19/00		63
B60C19/04	8	Tyre with openings closeable by means other than the rim; Closing means therefor	B60C19/04	B60C19/04		82
B60C19/08	8	Electric-charge-dissipating arrangements	B60C19/08	B60C19/08		413
B60C19/082	9	{comprising a conductive tread insert}	B60C19/08	B60C19/08		221
B60C19/084	9	{using conductive carcasses}	B60C19/08	B60C19/08		85
B60C19/086	9	{using conductive sidewalls}	B60C19/08	B60C19/08		59
B60C19/088	9	{using conductive beads}	B60C19/08	B60C19/08		52
B60C19/12	8	Puncture preventing arrangements	B60C19/12	B60C19/12		831
B60C19/122	9	{disposed inside of the inner liner}	B60C19/12	B60C19/12		1387
B60C19/125	9	{disposed removably on the tyre}	B60C19/12	B60C19/12		212
B60C19/127	9	{for inner tubes}	B60C19/12	B60C19/12		256
B60C23/00	7	Devices for measuring, signalling, controlling, or distributing tyre pressure or temperature, specially adapted for mounting on vehicles; Arrangement of tyre inflating devices on vehicles, e.g. of pumps or of tanks; Tyre cooling arrangements	B60C23/00	B60C23/00		1000
B60C23/001	8	{Devices for manually or automatically controlling or distributing tyre pressure whilst the vehicle is moving}	B60C23/00	B60C23/00		496
B60C23/002	9	{by monitoring conditions other than tyre pressure or deformation}	B60C23/00	B60C23/00		439
B60C23/003	9	{comprising rotational joints between vehicle-mounted pressure sources and the tyres}	B60C23/00	B60C23/00		102
B60C23/00305	10	{Wheel circumventing supply lines, e.g. not through or about the axles}	B60C23/00	B60C23/00		64
B60C23/00309	10	{characterised by the location of the components, e.g. valves, sealings, conduits or sensors}	B60C23/00	B60C23/00		33
B60C23/00318	11	{on the wheels or the hubs}	B60C23/00	B60C23/00		627
B60C23/00327	12	{integrally with the hub caps}	B60C23/00	B60C23/00		45
B60C23/00336	11	{on the axles}	B60C23/00	B60C23/00		260
B60C23/00345	10	{Details of the rotational joints}	B60C23/00	B60C23/00		363
B60C23/00347	11	{comprising two or more feedthrough}	B60C23/00	B60C23/00		50
B60C23/00354	10	{Details of valves}	B60C23/00	B60C23/00		740
B60C23/00363	10	{Details of sealings}	B60C23/00	B60C23/00		592
B60C23/00372	10	{characterised by fluid diagrams}	B60C23/00	B60C23/00		515
B60C23/00381	10	{specially adapted for steerable wheels}	B60C23/00	B60C23/00		35
B60C23/0039	10	{specially adapted for driven wheels}	B60C23/00	B60C23/00		63
B60C23/004	9	{the control being done on the wheel, e.g. using a wheel-mounted reservoir}	B60C23/00	B60C23/00		524
B60C23/005	8	{Devices specially adapted for special wheel arrangements}	B60C23/00	B60C23/00		28
B60C23/006	9	{having two wheels only}	B60C23/00	B60C23/00		121
B60C23/007	9	{having multiple wheels arranged side by side}	B60C23/00	B60C23/00		329
B60C23/008	9	{having wheels on more than two axles}	B60C23/00	B60C23/00		89
B60C23/009	9	{having wheels on a trailer}	B60C23/00	B60C23/00		210
B60C23/02	8	Signalling devices actuated by tyre pressure {(hand-held tyre pressure gauges G01L17/00)}	B60C23/02	B60C23/02		864
B60C23/04	9	mounted on the wheel or tyre	B60C23/04	B60C23/04		1652
B60C23/0401	10	{characterised by the type of alarm}	B60C23/04	B60C23/04		391
B60C23/0403	11	{Mechanically generated audible signals, e.g. by buzzer or whistle signals}	B60C23/04	B60C23/04		439
B60C23/0405	11	{Mechanically generated visible signals, e.g. by using a gauge needle}	B60C23/04	B60C23/04		269
B60C23/0406	11	{Alarms noticeable from outside the vehicle, e.g. indication in side mirror, front light or audible alarms (B60C23/0403, B60C23/0405 take precedence)}	B60C23/04	B60C23/04		162
B60C23/0408	10	{transmitting the signals by non-mechanical means from the wheel or tyre to a vehicle body mounted receiver}	B60C23/04	B60C23/04		2345
B60C23/041	11	{Means for supplying power to the signal- transmitting means on the wheel}	B60C23/04	B60C23/04		536
B60C23/0411	12	{Piezoelectric generators}	B60C23/04	B60C23/04		266
B60C23/0413	12	{Wireless charging of active radio frequency circuits}	B60C23/04	B60C23/04		228
B60C23/0415	11	{Automatically identifying wheel mounted units, e.g. after replacement or exchange of wheels}	B60C23/04	B60C23/04		244
B60C23/0416	12	{allocating a corresponding wheel position on vehicle, e.g. front/left or rear/right}	B60C23/04	B60C23/04		1020
B60C23/0418	11	{Sharing hardware components like housing, antenna, receiver or signal transmission line with other vehicle systems like keyless entry or brake control units}	B60C23/04	B60C23/04		129
B60C23/042	12	{cooperating with wheel hub mounted speed sensors}	B60C23/04	B60C23/04		56
B60C23/0422	11	{characterised by the type of signal transmission means}	B60C23/04	B60C23/04		172
B60C23/0423	12	{Photo-electric, infrared or visible light means}	B60C23/04	B60C23/04		50
B60C23/0425	12	{Means comprising permanent magnets, e.g. Hall-effect or Reed-switches}	B60C23/04	B60C23/04		161
B60C23/0427	12	{Near field transmission with inductive or capacitive coupling means}	B60C23/04	B60C23/04		68
B60C23/0428	13	{using passive wheel mounted resonance circuits}	B60C23/04	B60C23/04		151
B60C23/043	13	{using transformer type signal transducers, e.g. rotary transformers}	B60C23/04	B60C23/04		145
B60C23/0432	13	{using vehicle structural parts as signal path, e.g. chassis, axle or fender}	B60C23/04	B60C23/04		13
B60C23/0433	12	{Radio signals}	B60C23/04	B60C23/04		1058
B60C23/0435	13	{Vehicle body mounted circuits, e.g. transceiver or antenna fixed to central console, door, roof, mirror or fender}	B60C23/04	B60C23/04		85
B60C23/0437	14	{Means for detecting electromagnetic field changes not being part of the signal transmission per se, e.g. strength, direction, propagation or masking}	B60C23/04	B60C23/04		176
B60C23/0438	14	{comprising signal transmission means, e.g. for a bidirectional communication with a corresponding wheel mounted receiver}	B60C23/04	B60C23/04		80
B60C23/044	15	{Near field triggers, e.g. magnets or triggers with 125 KHz}	B60C23/04	B60C23/04		110
B60C23/0442	15	{the transmitted signal comprises further information, e.g. instruction codes, sensor characteristics or identification data}	B60C23/04	B60C23/04		326
B60C23/0444	14	{Antenna structures, control or arrangements thereof, e.g. for directional antennas, diversity antenna, antenna multiplexing or antennas integrated in fenders}	B60C23/04	B60C23/04		348
B60C23/0445	14	{Means for changing operating mode, e.g. sleep mode, factory mode or energy saving mode}	B60C23/04	B60C23/04		45
B60C23/0447	13	{Wheel or tyre mounted circuits}	B60C23/04	B60C23/04		207
B60C23/0449	14	{Passive transducers, e.g. using surface acoustic waves, backscatter technology or pressure sensitive resonators (near field passive transducers B60C23/0428)}	B60C23/04	B60C23/04		66
B60C23/045	14	{Means for detecting electromagnetic field changes being not part of the signal transmission per se, e.g. strength, direction, propagation or masking}	B60C23/04	B60C23/04		119
B60C23/0452	14	{Antenna structure, control or arrangement (vehicle tyre mounted antennas H01Q1/2241)}	B60C23/04	B60C23/04		321
B60C23/0454	14	{Means for changing operation mode, e.g. sleep mode, factory mode or energy save mode}	B60C23/04	B60C23/04		127
B60C23/0455	14	{Transmission control of wireless signals}	B60C23/04	B60C23/04		214
B60C23/0457	15	{self triggered by timer}	B60C23/04	B60C23/04		52
B60C23/0459	15	{self triggered by motion sensor}	B60C23/04	B60C23/04		104
B60C23/0461	15	{externally triggered, e.g. by wireless request signal, magnet or manual switch}	B60C23/04	B60C23/04		174
B60C23/0462	15	{Structure of transmission protocol}	B60C23/04	B60C23/04		371
B60C23/0464	15	{to avoid signal interference}	B60C23/04	B60C23/04		85
B60C23/0466	16	{with signals sent by transmitters mounted on adjacent vehicles}	B60C23/04	B60C23/04		37
B60C23/0467	12	{Electric contact means, e.g. slip-rings, rollers, brushes}	B60C23/04	B60C23/04		357
B60C23/0469	12	{Transmission by sound, e.g. ultra-sound}	B60C23/04	B60C23/04		42
B60C23/0471	11	{System initialisation, e.g. upload or calibration of operating parameters}	B60C23/04	B60C23/04		368
B60C23/0472	12	{to manually allocate ID codes or mounting positions, e.g. by service technicians}	B60C23/04	B60C23/04		167
B60C23/0474	11	{Measurement control, e.g. setting measurement rate or calibrating of sensors; Further processing of measured values, e.g. filtering, compensating or slope monitoring}	B60C23/04	B60C23/04		347
B60C23/0476	12	{Temperature compensation of measured pressure values}	B60C23/04	B60C23/04		134
B60C23/0477	12	{Evaluating waveform of pressure readings}	B60C23/04	B60C23/04		104
B60C23/0479	11	{Communicating with external units being not part of the vehicle, e.g. tools for diagnostic, mobile phones, electronic keys or service stations}	B60C23/04	B60C23/04		911
B60C23/0481	11	{System diagnostic, e.g. monitoring battery voltage, detecting hardware detachments or identifying wireless transmission failures}	B60C23/04	B60C23/04		202
B60C23/0483	11	{Wireless routers between wheel mounted transmitters and chassis mounted receivers}	B60C23/04	B60C23/04		161
B60C23/0484	11	{Detecting an ongoing tyre inflation}	B60C23/04	B60C23/04		100
B60C23/0486	10	{comprising additional sensors in the wheel or tyre mounted monitoring device, e.g. movement sensors, microphones or earth magnetic field sensors}	B60C23/04	B60C23/04		509
B60C23/0488	11	{Movement sensor, e.g. for sensing angular speed, acceleration or centripetal force}	B60C23/04	B60C23/04		798
B60C23/0489	11	{for detecting the actual angular position of the monitoring device while the wheel is turning}	B60C23/04	B60C23/04		281
B60C23/0491	10	{Constructional details of means for attaching the control device}	B60C23/04	B60C23/04		122
B60C23/0493	11	{for attachment on the tyre}	B60C23/04	B60C23/04		1012
B60C23/0494	11	{Valve stem attachments positioned inside the tyre chamber}	B60C23/04	B60C23/04		815
B60C23/0496	11	{Valve stem attachments positioned outside of the tyre chamber}	B60C23/04	B60C23/04		1009
B60C23/0498	11	{for rim attachments (B60C23/0494, B60C23/0496 take precedence)}	B60C23/04	B60C23/04		231
B60C23/04985	12	{using straps surrounding the rims}	B60C23/04	B60C23/04		107
B60C23/06	8	Signalling devices actuated by deformation of the tyre {, e.g. tyre mounted deformation sensors or indirect determination of tyre deformation based on wheel speed, wheel-centre to ground distance or inclination of wheel axle}	B60C23/06	B60C23/06		533
B60C23/061	9	{by monitoring wheel speed (measuring distance traversed on the ground by vehicles G01C22/00)}	B60C23/06	B60C23/06		787
B60C23/062	10	{Frequency spectrum analysis of wheel speed signals, e.g. using Fourier transformation}	B60C23/06	B60C23/06		213
B60C23/063	9	{Generating directly an audible signal by deformation of the tyre (by touching the ground B60C23/085)}	B60C23/06	B60C23/06		156
B60C23/064	9	{comprising tyre mounted deformation sensors, e.g. to determine road contact area}	B60C23/06	B60C23/06		385
B60C23/065	9	{by monitoring vibrations in tyres or suspensions (B60C23/062 takes precedence)}	B60C23/06	B60C23/06		71
B60C23/066	9	{by monitoring wheel-centre to ground distance}	B60C23/06	B60C23/06		142
B60C23/067	9	{by monitoring chassis to ground distance}	B60C23/06	B60C23/06		56
B60C23/068	9	{by monitoring chassis to tyre distance}	B60C23/06	B60C23/06		50
B60C23/08	9	by touching the ground	B60C23/08	B60C23/08		259
B60C23/085	10	{putting directly into action an audible signal}	B60C23/08	B60C23/08		24
B60C23/10	8	Arrangement of tyre-inflating pumps mounted on vehicles	B60C23/10	B60C23/10		695
B60C23/105	9	{the pump being mounted in the saddle-pillar of a bicycle}	B60C23/10	B60C23/10		126
B60C23/12	9	operated by a running wheel	B60C23/12	B60C23/12		125
B60C23/121	10	{the pumps being mounted on the tyres}	B60C23/12	B60C23/12		36
B60C23/123	11	{Elongate peristaltic pumps}	B60C23/12	B60C23/12		154
B60C23/124	11	{Bladders}	B60C23/12	B60C23/12		38
B60C23/126	10	{the pumps being mounted on the wheel rims}	B60C23/12	B60C23/12		252
B60C23/127	10	{the pumps being mounted on the hubs}	B60C23/12	B60C23/12		238
B60C23/129	10	{the pumps being mounted on wheel spokes}	B60C23/12	B60C23/12		102
B60C23/131	10	{activated by force of gravity}	B60C23/12	B60C23/131		49
B60C23/133	10	{activated by centrifugal force}	B60C23/12	B60C23/133		88
B60C23/135	10	{activated due to tyre deformation}	B60C23/12	B60C23/135		302
B60C23/137	10	{comprising cam driven pistons}	B60C23/12	B60C23/137		276
B60C23/14	9	operated by the prime mover of the vehicle	B60C23/14	B60C23/14		339
B60C23/16	8	Arrangement of air tanks mounted on vehicles	B60C23/16	B60C23/16		205
B60C23/18	8	Tyre cooling arrangements {, e.g. heat shields (wheels with cooling fins B60B19/10)}	B60C23/18	B60C23/18		405
B60C23/19	9	for dissipating heat	B60C23/19	B60C23/19		265
B60C23/20	8	Devices for measuring or signalling tyre temperature {only}	B60C23/20	B60C23/20		727
B60C25/00	7	Apparatus or tools adapted for mounting, removing or inspecting tyres (testing of tyres G01M17/02)	B60C25/00	B60C25/00		573
B60C25/002	8	{Inspecting tyres}	B60C25/00	B60C25/00		469
B60C25/005	9	{inside surface}	B60C25/00	B60C25/00		35
B60C25/007	9	{outside surface (measuring profile depth G01B11/22)}	B60C25/00	B60C25/00		150
B60C25/01	8	for removing tyres from or mounting tyres on wheels	B60C25/01	B60C25/01		131
B60C25/015	9	{for only breaking the beads}	B60C25/01	B60C25/01		28
B60C25/02	9	Tyre levers or the like, e.g. hand-held	B60C25/02	B60C25/02		773
B60C25/025	10	{with a jack}	B60C25/02	B60C25/02		247
B60C25/04	10	pivotal about the wheel axis, or movable along the rim edge, e.g. rollable	B60C25/04	B60C25/04		248
B60C25/05	9	Machines	B60C25/05	B60C25/05		120
B60C25/0503	10	{for mounting only}	B60C25/05	B60C25/05		131
B60C25/0506	10	{for demounting only}	B60C25/05	B60C25/05		173
B60C25/0509	10	{for inserting additional parts, e.g. support rings, sensors}	B60C25/05	B60C25/05		47
B60C25/0512	10	{Integrated systems performing multiple operations, e.g. assembly lines}	B60C25/05	B60C25/05		51
B60C25/0515	10	{Automated devices, e.g. mounting robots}	B60C25/05	B60C25/05		137
B60C25/0518	10	{Horizontal wheel axis in working position}	B60C25/05	B60C25/05		46
B60C25/0521	10	{Handling of rim or tyre, e.g. lifting and positioning devices}	B60C25/05	B60C25/05		158
B60C25/0524	10	{Separating tyres from rims, e.g. by destroying}	B60C25/05	B60C25/05		93
B60C25/0527	10	{Adapting to different wheel diameters, i.e. distance between support and tool}	B60C25/05	B60C25/05		65
B60C25/053	10	{Support of wheel parts during machine operation}	B60C25/05	B60C25/05		58
B60C25/0533	11	{Fixing the tyre only, e.g. gripping the tread portion for inserting the rim}	B60C25/05	B60C25/05		29
B60C25/0536	11	{axially fixing the rim, e.g. pulling devices}	B60C25/05	B60C25/05		30
B60C25/0539	11	{radially fixing the rim, e.g. with gripping claws}	B60C25/05	B60C25/05		81
B60C25/0542	11	{with self-centering means, e.g. cones}	B60C25/05	B60C25/05		43
B60C25/0545	11	{with rotary motion of tool or tyre support, e.g. turntables}	B60C25/05	B60C25/05		134
B60C25/0548	10	{equipped with sensing means, e.g. for positioning, measuring or controlling}	B60C25/05	B60C25/05		62
B60C25/0551	11	{mechanical}	B60C25/05	B60C25/05		36
B60C25/0554	11	{optical, e.g. cameras}	B60C25/05	B60C25/05		75
B60C25/0557	11	{thermal}	B60C25/05	B60C25/05		3
B60C25/056	11	{measuring speed, acceleration or forces}	B60C25/05	B60C25/05		41
B60C25/0563	10	{Tools interacting with the tyre and moved in relation to the tyre during operation}	B60C25/05	B60C25/05		39
B60C25/0566	11	{rolling only}	B60C25/05	B60C25/05		33
B60C25/0569	11	{gliding only}	B60C25/05	B60C25/05		11
B60C25/0572	11	{pressing only}	B60C25/05	B60C25/05		33
B60C25/0575	11	{levering only}	B60C25/05	B60C25/05		4
B60C25/0578	11	{hooking only}	B60C25/05	B60C25/05		86
B60C25/0581	11	{Translational tool trajectory only}	B60C25/05	B60C25/05		5
B60C25/0584	11	{Predetermined tool path, e.g. coulisse, multi-link}	B60C25/05	B60C25/05		11
B60C25/0587	11	{Programmed tool path, e.g. robot arm with multiple degrees of freedom}	B60C25/05	B60C25/05		7
B60C25/059	11	{Conjoint tool operations, i.e. at least two tools cooperating simultaneously}	B60C25/05	B60C25/05		31
B60C25/0593	11	{Multi-functional tools for performing at least two operations, e.g. bead breaking and bead seeking}	B60C25/05	B60C25/05		45
B60C25/0596	10	{Soaping devices}	B60C25/05	B60C25/05		46
B60C25/12	10	for only seating the beads	B60C25/12	B60C25/12		55
B60C25/122	11	acting on the tyre tread	B60C25/122	B60C25/122		12
B60C25/125	10	for only breaking the beads	B60C25/125	B60C25/125		25
B60C25/128	11	acting axially on the whole circumference of the bead or side wall	B60C25/128	B60C25/128		12
B60C25/13	11	acting axially on a part of the bead or side wall only at localised regions of the bead or side wall	B60C25/13	B60C25/13		127
B60C25/132	10	for removing and mounting tyres (for only seating the beads B60C25/12; for only breaking the beads B60C25/125{; for locating provisionally the beads of tubeless tyres against the sealing surfaces of the rims B60C25/145})	B60C25/132	B60C25/132		992
B60C25/135	11	having a tyre support or a tool, movable along wheel axis	B60C25/135	B60C25/135		151
B60C25/138	12	with rotary motion of tool or tyre support	B60C25/138	B60C25/138		454
B60C25/14	8	Apparatus or tools for spreading {or locating} tyre beads	B60C25/14	B60C25/14		115
B60C25/142	9	{Devices for tightening or expanding the felly, devices for spreading the tyres}	B60C25/14	B60C25/14		789
B60C25/145	9	{for locating provisionally the beads of tubeless tyres against the sealing surfaces of the rims, e.g. air filling bell}	B60C25/14	B60C25/14		267
B60C25/147	9	{Safety cages for inflation}	B60C25/14	B60C25/14		104
B60C25/15	9	with means for inverting the tyre	B60C25/15	B60C25/15		6
B60C25/16	8	{Tools for repairing damaged tyres}	B60C25/00	B60C25/16		225
B60C25/18	8	Tools for mounting or demounting air valves	B60C25/18	B60C25/18		173
B60C25/185	9	{Automated devices, e.g. robots}	B60C25/18	B60C25/18		21
B60C25/20	8	Tools for attaching metallic tyres, e.g. iron tyres upon wooden rims	B60C25/20	B60C25/20		40
B60C27/00	7	Non-skid devices temporarily attachable to resilient tyres or resiliently-tyred wheels	B60C27/00	B60C27/00		1246
B60C27/003	8	{Mounting aids, e.g. auxiliary tensioning tools, slotted ramps}	B60C27/00	B60C27/00		169
B60C27/006	8	{provided with protective parts, e.g. rubber elements to protect the rim portion}	B60C27/00	B60C27/00		38
B60C27/02	8	extending over restricted arcuate part of tread (B60C27/20 takes precedence)	B60C27/02	B60C27/02		498
B60C27/0207	9	{involving lugs or rings taking up wear, e.g. chain links, chain connectors (chain couplings for, e.g. hoisting F16G15/00)}	B60C27/02	B60C27/02		36
B60C27/0215	10	{Profiled links, e.g. cross-section other than round}	B60C27/02	B60C27/02		5
B60C27/0223	10	{Studded links, i.e. traction enhancing parts located on the link or inserted into the link}	B60C27/02	B60C27/02		58
B60C27/023	9	{provided with radial arms for supporting the ground engaging parts on the wheel}	B60C27/02	B60C27/02		136
B60C27/0238	9	{provided with tensioning means}	B60C27/02	B60C27/02		132
B60C27/0246	10	{Resilient pretension}	B60C27/02	B60C27/02		45
B60C27/0253	10	{Centrifugal forces for tensioning while driving}	B60C27/02	B60C27/02		2
B60C27/0261	9	{provided with fastening means}	B60C27/02	B60C27/02		52
B60C27/0269	10	{acting on the wheel, e.g. on the rim or wheel bolts}	B60C27/02	B60C27/02		198
B60C27/0276	11	{through apertures in the rim, e.g. fastening from one lateral side to the other lateral side of the rim; extending axially through the rim}	B60C27/02	B60C27/02		368
B60C27/0284	10	{acting on the tread portion, e.g. special fixing agents, fastened in the groove of the tyre}	B60C27/02	B60C27/02		35
B60C27/0292	10	{acting on the sidewall of the tyre}	B60C27/02	B60C27/02		68
B60C27/04	9	the ground-engaging part being rigid	B60C27/04	B60C27/04		681
B60C27/045	10	{involving retractable devices (fixing of spade lugs B60B15/00)}	B60C27/04	B60C27/04		415
B60C27/06	8	extending over the complete circumference of the tread, e.g. made of chains {or cables}(B60C27/20 takes precedence)	B60C27/06	B60C27/06		1600
B60C27/061	9	{provided with radial arms for supporting the ground engaging parts on the tread}	B60C27/06	B60C27/06		104
B60C27/062	9	{provided with fastening means}	B60C27/06	B60C27/06		186
B60C27/063	10	{acting on the wheel, e.g. on the rim or wheel bolts}	B60C27/06	B60C27/06		135
B60C27/064	10	{through apertures in the rim, e.g. fastening from one lateral side to the other lateral side of the rim; extending axially through the rim}	B60C27/06	B60C27/06		35
B60C27/065	10	{acting on the tread portion, e.g. special fixing agents, fastened in the groove of the tyre}	B60C27/06	B60C27/06		131
B60C27/066	10	{acting on the sidewall of the tyre}	B60C27/06	B60C27/06		56
B60C27/067	9	{Special chain layout;, i.e. distribution of chain portions over the tread, e.g. arranged in polygon pattern}	B60C27/06	B60C27/06		103
B60C27/068	9	{the ground-engaging part being rigid}	B60C27/06	B60C27/06		56
B60C27/08	9	involving lugs or rings taking up wear {, e.g. chain links, chain connectors }	B60C27/08	B60C27/08		2305
B60C27/083	10	{Profiled links, i.e. cross-section other than round, e.g. hexagonal}	B60C27/08	B60C27/08		20
B60C27/086	10	{Studded links, i.e. traction enhancing parts located on the link or inserted into the link}	B60C27/08	B60C27/08		156
B60C27/10	9	having tensioning means	B60C27/10	B60C27/10		972
B60C27/12	10	resilient {pretension}	B60C27/12	B60C27/12		513
B60C27/125	11	{Centrifugal forces for tensioning while driving}	B60C27/12	B60C27/12		4
B60C27/14	9	automatically attachable	B60C27/14	B60C27/14		403
B60C27/145	10	{the anti-skid device being wound around the wheel by its rotation from a point connected to the body frame of the vehicle}	B60C27/14	B60C27/14		155
B60C27/16	9	formed of close material, e.g. leather {or synthetic mats}	B60C27/16	B60C27/16		1183
B60C27/18	10	the material being fabric, e.g. woven wire {or textile}	B60C27/18	B60C27/18		209
B60C27/20	8	having ground-engaging plate-like elements	B60C27/20	B60C27/20		707
B60C27/22	8	for tandem tyres	B60C27/22	B60C27/22		175
B60C29/00	7	Arrangements of tyre-inflating valves to tyres or rims; Accessories for tyre-inflating valves, not otherwise provided for (tools for mounting or demounting valves B60C25/18)	B60C29/00	B60C29/00		504
B60C29/002	8	{characterised by particular features of the valve core}	B60C29/00	B60C29/00		122
B60C29/005	8	{characterised by particular features of the valve stem}	B60C29/00	B60C29/00		189
B60C29/007	8	{for tyres with segmental sections or for multi-chamber tyres}	B60C29/00	B60C29/00		231
B60C29/02	8	Connection to rims	B60C29/02	B60C29/02		734
B60C29/04	8	Connection to tyres {or inner tubes}	B60C29/04	B60C29/04		395
B60C29/06	8	Accessories for tyre-inflating valves, e.g. housings, guards, covers for valve caps, locks, not otherwise provided for {(B60C23/0496 takes precedence; tools for screwing and unscrewing valve caps B25B27/0057; pump connectors F04B33/005)}	B60C29/06	B60C29/06		1121
B60C29/062	9	{for filling a tyre with particular materials, e.g. liquids (B60C5/004, B60C5/005 take precedence)}	B60C29/06	B60C29/06		216
B60C29/064	9	{Hose connections for pneumatic tyres, e.g. to spare wheels}	B60C29/06	B60C29/06		486
B60C29/066	9	{Valve caps}	B60C29/06	B60C29/06		400
B60C29/068	9	{Pressure relief devices, i.e. safety devices for overpressure}	B60C29/06	B60C29/06		135
B60C99/00	7	Subject matter not provided for in other groups of this subclass	B60C99/00	B60C99/00		107
B60C99/003	8	{Tyre heating arrangements}	B60C99/00	B60C99/00		164
B60C99/006	8	{Computer aided tyre design or simulation}	B60C99/00	B60C99/00		354
B60C2200/00	7	Tyres specially adapted for particular applications	CPCONLY	B60C2200/00		72
B60C2200/02	8	for aircrafts	CPCONLY	B60C2200/02		524
B60C2200/04	8	for road vehicles, e.g. passenger cars	CPCONLY	B60C2200/04		855
B60C2200/06	8	for heavy duty vehicles	CPCONLY	B60C2200/06		1558
B60C2200/065	9	for construction vehicles	CPCONLY	B60C2200/065		353
B60C2200/08	8	for agricultural vehicles	CPCONLY	B60C2200/08		296
B60C2200/10	8	for motorcycles, scooters or the like	CPCONLY	B60C2200/10		1037
B60C2200/12	8	for bicycles	CPCONLY	B60C2200/12		516
B60C2200/14	8	for off-road use	CPCONLY	B60C2200/14		551
