F16P1/00	7	Safety devices independent of the control and operation of any machine (protective devices for the eyes or ears, worn on the body or carried in the hand, A61F9/00, A61F11/00)	F16P1/00	F16P1/00		488
F16P1/005	8	{Guards for rolls in calendering or other roll machines, e.g. nip guards, finger guards}	F16P1/00	F16P1/00		74
F16P1/02	8	Fixed screens or hoods	F16P1/02	F16P1/02		1609
F16P1/04	8	Screens or hoods rotating with rotary shafts	F16P1/04	F16P1/04		102
F16P1/06	8	specially designed for welding	F16P1/06	F16P1/06		632
F16P3/00	7	Safety devices acting in conjunction with the control or operation of a machine; Control arrangements requiring the simultaneous use of two or more parts of the body (F16P5/00 takes precedence)	F16P3/00	F16P3/00		650
F16P3/001	8	{Safety devices for guarding the human operator of punch presses or like machine tools performing an opening and closing travel}	F16P3/00	F16P3/00		137
F16P3/003	9	{by application of a specific control arrangement, e.g. specific switching systems or two-hand control}	F16P3/00	F16P3/00		56
F16P3/005	9	{having a movable screen or a sensor influencing the switching system}	F16P3/00	F16P3/00		217
F16P3/006	9	{having a screen moving with the machine and moving the operator out of danger, or restraining the operator, without influencing the switching system}	F16P3/00	F16P3/00		74
F16P3/008	8	{Devices for directly stopping or interrupting the drive or gear in case of danger to the machine, e.g. devices with clutches}	F16P3/00	F16P3/00		103
F16P3/02	8	Screens or other safety members moving in synchronism with members which move to and fro	F16P3/02	F16P3/02		385
F16P3/04	9	for machines with parts which approach one another during operation, e.g. for stamping presses	F16P3/04	F16P3/04		594
F16P3/06	10	in which body parts of the operator are removed from the danger zone on approach of the machine parts	F16P3/06	F16P3/06		198
F16P3/08	8	in connection with the locking of doors, covers, guards, or like members giving access to moving machine parts	F16P3/08	F16P3/08		1094
F16P3/10	9	in which the operation of locking the door or other member causes the machine to start	F16P3/10	F16P3/10		172
F16P3/12	8	with means, e.g. feelers, which in case of the presence of a body part of a person in or near the danger zone influence the control or operation of the machine (F16P3/08 takes precedence)	F16P3/12	F16P3/12		780
F16P3/125	9	{Guards for rolls in calendering or other roll machines, e.g. nip guards, finger guards}	F16P3/12	F16P3/12		48
F16P3/14	9	the means being photocells or other devices sensitive without mechanical contact	F16P3/14	F16P3/14		383
F16P3/141	10	{using sound propagation, e.g. sonar}	F16P3/14	F16P3/14		186
F16P3/142	10	{using image capturing devices}	F16P3/14	F16P3/14		525
F16P3/144	10	{using light grids}	F16P3/14	F16P3/14		1277
F16P3/145	10	{using magnetic technology}	F16P3/14	F16P3/14		125
F16P3/147	10	{using electro-magnetic technology, e.g. tags or radar}	F16P3/14	F16P3/14		563
F16P3/148	10	{using capacitive technology}	F16P3/14	F16P3/14		219
F16P3/16	9	with feeling members moved by the machine	F16P3/16	F16P3/16		191
F16P3/18	8	Control arrangements requiring the use of both hands	F16P3/18	F16P3/18		137
F16P3/20	9	for electric control systems	F16P3/20	F16P3/20		282
F16P3/22	9	for hydraulic or pneumatic control systems	F16P3/22	F16P3/22		139
F16P3/24	9	for mechanical controls	F16P3/24	F16P3/24		163
F16P5/00	7	Emergency means for rendering ineffective a coupling conveying reciprocating movement if the motion of the driven part is prematurely resisted	F16P5/00	F16P5/00		81
F16P5/005	8	{Overload protection by energy absorbing components, e.g. breaker blocks, shear sections}	F16P5/00	F16P5/00		109
F16P7/00	7	Emergency devices preventing damage to a machine or apparatus (F16P1/00, F16P3/00, F16P5/00 take precedence)	F16P7/00	F16P7/00		313
F16P7/02	8	by causing the machine to stop on the occurrence of dangerous conditions therein (devices in bearings affected by abnormal conditions F16C)	F16P7/02	F16P7/02		217
