F		機械工学；照明；加熱；武器；爆破<br>	MECHANICAL ENGINEERING; LIGHTING; HEATING; WEAPONS; BLASTING				
F01		機械または機関一般；機関設備一般；蒸気機関<br><br><b><ul>注</ul></b><br>このサブセクション，すなわちクラスＦ０１からＦ０４，の利用のための手引き<br>以下の注は，この部分の分類体系の利用を助けるためのものである；これらはいかなる場合にも分類体系を変更するものとして解釈すべきではない。<br>１．このサブセクションにおいては，“機関”または“ポンプ”を明示するサブクラスまたはグループは，他に特に分類されない限りそれらの操作方法を包含する。<br>２．このサブセクションにおいては，下記の用語または表現は以下に示す意味で用いる：<br>　・“機関”は流体エネルギを連続的に機械的動力に変換する装置を意味する。それ故，この語はそれ自体で，たとえば蒸気ピストン機関，蒸気タービン，または，内燃機関を含むが，一行程装置を除外する。“機関”はまた，それが特に計器に用いるのに適しているものを除き計器の流体作動部分をも包含する；<br>　・“ポンプ”は機械的または他の手段によって流体を連続的に押し揚げ，押圧し，圧縮または排出する装置を意味する；そしてこの用語はファンまたは送風機を含む；<br>　・“機械”は同様に機関およびポンプであり得る装置を意味し，かつ機関に限定された装置またはポンプに限定されたものを意味しない；<br>　・“容積形”は，作動流体エネルギの機械的エネルギへの変換およびその逆の変換において，作動流体の内容積変化が機械部材の変位に相当し，流体の動的影響が重要でないエネルギ変換方法を意味する；<br>　・“非容積形”は，作動流体エネルギの運動エネルギへの変換によって，作動流体のエネルギを機械的エネルギに変換する方法を意味する；その逆の変換の場合も同様である；<br>　・“揺動ピストン機械”とは流体と係合する仕事伝達部材が揺動する容積形機械を意味する。この定義は機関またはポンプに同様に適用する；<br>　・“回転ピストン機械”とは流体と係合する仕事伝達部材が固定軸のまわりに，もしくは円または同様の軌道に沿って移動する軸のまわりに，回転する容積形機械を意味する。この定義は機関またはポンプに同様に適用する；<br>　・“回転ピストン”とは回転ピストン機械の仕事伝達部材を意味し，適当な形式のもの，例．歯車のようなもの，でよい；<br>　・“共動部材”とは揺動ピストンまたは回転ピストンと，駆動作用またはポンプ作用を補助する他の部材，例．作動室壁，とを意味する；<br>　・“共動部材の運動”は，相対的，すなわち，たとえ文面上は“回転軸”とされていても，共動部材の一方は静止していることもあり，両方とも動くこともあると解釈すべきである；<br>　・“歯または歯に相当する部分”とは突出部，突起部，または係合部を含む；<br>　・“内部軸”形式とは内外の共動部材の回転軸がつねに外側部材内にあることを意味する，例．環状歯車の内歯とかみ合うピニオンと類似の態様であるもの<br>　・“自由ピストン”は行程の長さがそれによって駆動される部材によって限定されないピストンを意味する；<br>　・“シリンダ”は容積形作動室一般を意味し，そしてこの用語は円形断面のシリンダに限定されない；<br>　・“主軸”はピストンの往復運動を回転運動にまたはその反対に変換する軸を意味する；<br>　・“設備”は機関と機関を運転するのに必要な付加的装置を一緒にした意味である。たとえば，蒸気機関設備は蒸気機関および蒸気発生装置を含む；<br>　・“作動流体”はポンプにおける被駆動流体または機関における駆動流体を意味する。作動流体は圧縮性流体と呼ばれる圧縮性のガス体，例．蒸気，または液体でありうる。あるいは圧縮性流体と液相の共存も可能である。<br>　・“蒸気”は凝縮性蒸気一般を含み，また“特殊蒸気”は水蒸気以外の場合に用いる；<br>　・非容積形機械または機関に適用される“反動形”は圧力―速度変換が完全にまたは部分的に回転子において行なわれる機械または機関を意味し；回転子内における圧力―速度変換が全くないかわずかである機械または機関は“衝動形”と称する。<br>３．このサブセクションにおいては：<br>　・周期的に作動する弁，潤滑，ガス流消音器もしくは排気装置，または冷却はそれらの記述された応用に関係なくＦ０１Ｌ，Ｆ０１Ｍ，Ｆ０１Ｎ，Ｆ０１Ｐに分類する。ただしその分類の特徴がその応用に独特のものであるならば，その場合Ｆ０１ないしＦ０４の関連したサブクラスのみに分類する；<br>　・機械または機関の潤滑，ガス流消音器もしくは排気装置，または冷却はＦ０１Ｂに分類される蒸気機関に特有なものを除いてＦ０１Ｍ，Ｆ０１Ｎ，Ｆ０１Ｐに分類する。<br>４．このサブセクションを十分に理解して利用するため，この骨格をなす，Ｆ０１Ｂ，Ｆ０１Ｃ，Ｆ０１Ｄ，Ｆ０３ＢおよびＦ０４Ｂ，Ｆ０４Ｃ，Ｆ０４Ｄ，に関するかぎり<br>　・この分類表に存在する原則；<br>　・その要求する分類の特徴；および<br>　・その補足<br>を記憶しておくことが肝要である。<br>　　ｉ．原則<br>　　　これは上に挙げたサブグラスに本質的に関連している。より限定された事項を包含する他のサブグラス，特にＦ０２のものはここで考慮しない。<br>　　　各サブグラスは基本的に装置（機関またはポンプ）の類を包含し，また拡張によって同種の“機械”を同様に包含する。それ故に一方が他方より，より一般的性質を有する，２つの異なった主題は同じサブグラスに包含される。<br>　　　サブクラスが包含する２つの異なった主題の範囲をこえて，サブクラスＦ０１Ｂ，Ｆ０３Ｂ，Ｆ０４Ｂはさらに関連した類での異なった種類の装置に関係する他のサブクラスに関して一般性を有する。<br>　　　この一般性は，つねに同じサブクラスに関するものを除いて，異なった２つの主題の取り扱いに対しても同様に適用する。<br>　　　それ故，Ｆ０３Ｂはその機械を扱う部分においてＦ０４Ｂ，Ｆ０４Ｃに関する一般的クラスとして，および，その機関を扱う部分においてＦ０３Ｃに関する一般的クラスとして考えられるべきである。<br>　　ｉｉ．特徴<br>　　　ａ．サブグラスの主要な分類の特徴には機械；機関；ポンプの３つの可能性がある装置を級付けしていることである。<br>　　　ｂ．上記のごとく，“機械”はつねに他の２つの一方と関連している。これらの主分類は装置の一般的作動理論に従って：容積形；非容積形に再分類される。<br>　　　ｃ．容積形装置は作用理論を奏功する方法，すなわち，装置の種類に従って：単純往復ピストン；回転または揺動ピストン；その他にさらに再分類される。<br>　　　ｄ．他の分類の特徴は，すなわち：液体および圧縮性流体；圧縮性流体；流体の３種の装置が可能である，作動流体に関するものである。<br>　　ｉｉｉ．補足<br>　　　これは，装置または作動流体の種類に関し考慮のうえ特徴に従って，上に挙げたサブクラスの対との関連において存在する。<br>　　　種々の原則，特徴，補足と関連するサブクラスが下記のサブセクション内の索引に示されている。<br>次のようなことが索引から理解される。<br>・与えられた類の中の同種の装置に対して，“作動流体”の特徴が関連している：<br>　　Ｆ０１ＢおよびＦ０４Ｂ　機械<br>　　Ｆ０１ＣおよびＦ０４Ｃ　機械<br>　　Ｆ０１ＤおよびＦ０３Ｂ　機械<br>　　Ｆ０１ＢおよびＦ０３Ｃ　機関<br>　　Ｆ０１ＣおよびＦ０３Ｃ　機関<br>　　Ｆ０１ＤおよびＦ０３Ｂ　機関<br>・同じ種類の作動流体に対して，“装置”の特徴が相対的一般性から考えて同様にサブクラスに関連する。<br><br><b><ul>サブクラス内の索引</ul></b><br>機械<br>　容積形<br>　回転または揺動ピストン<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｃ<br>　　流体のみ　Ｆ０４Ｃ<br>　往復ピストンまたはその他<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｂ<br>　　流体のみ　Ｆ０４Ｂ<br>　非容積形<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｄ<br>　　流体のみ　Ｆ０３Ｂ<br>機関<br>　容積形<br>　回転または揺動ピストン<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｃ<br>　　流体のみ　Ｆ０３Ｃ<br>　往復ピストンまたはその他<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｂ<br>　　流体のみ　Ｆ０３Ｃ<br>　非容積形<br>　　液体および弾性流体または弾性流体　Ｆ０１Ｄ<br>　　流体のみ　Ｆ０３Ｂ<br>ポンプ<br>　容積形<br>　　回転または揺動ピストン　Ｆ０４Ｃ<br>　　往復ピストンまたはその他　Ｆ０４Ｂ<br>　非容積形　Ｆ０４Ｄ<br>	<br><br><b><u>Note(s)</u></b><br><br><ul style=""list-style:none""><li><u>Guide to the use of this subsection, i.e. classes</u> <b>F01-F04</b></li><li>The following notes are meant to assist in the use of this part of the classification scheme.<ul type=""1""><li>In this subsection, subclasses or groups designating &quot;engines&quot; or &quot;pumps&quot; cover methods of operating the same, unless otherwise specifically provided for.</li><li>In this subsection, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;engine&quot; means a device for continuously converting fluid energy into mechanical power. Thus, this term includes, for example, steam piston engines or steam turbines, <u>per se</u>, or internal-combustion piston engines, but it excludes single-stroke devices. &quot;Engine&quot; also includes the fluid-motive portion of a meter unless such portion is particularly adapted for use in a meter;</li><li>&quot;pump&quot; means a device for continuously raising, forcing, compressing, or exhausting fluid by mechanical or other means. Thus, this term includes fans or blowers;</li><li>&quot;machine&quot; means a device which could equally be an engine and a pump, and not a device which is restricted to an engine or one which is restricted to a pump;</li><li>&quot;positive displacement&quot; means the way the energy of a working fluid is transformed into mechanical energy, in which variations of volume created by the working fluid in a working chamber produce equivalent displacements of the mechanical member transmitting the energy, the dynamic effect of the fluid being of minor importance, and <u>vice versa</u> ;</li><li>&quot;non-positive displacement&quot; means the way the energy of a working fluid is transformed into mechanical energy, by transformation of the energy of the working fluid into kinetic energy, and <u>vice versa</u>;</li><li>&quot;oscillating-piston machine&quot; means a positive-displacement machine in which a fluid-engaging work-transmitting member oscillates. This definition applies also to engines and pumps;</li><li>&quot;rotary-piston machine&quot; means a positive-displacement machine in which a fluid-engaging work-transmitting member rotates about a fixed axis or about an axis moving along a circular or similar orbit. This definition applies also to engines and pumps;</li><li>&quot;rotary piston&quot; means the work-transmitting member of a rotary-piston machine and may be of any suitable form, e.g., like a toothed gear;</li><li>&quot;cooperating members&quot; means the &quot;oscillating piston&quot; or &quot;rotary piston&quot; and another member, e.g., the working-chamber wall, which assists in the driving or pumping action;</li><li>&quot;movement of the co-operating members&quot; is to be interpreted as relative, so that one of the &quot;co-operating members&quot; may be stationary, even though reference may be made to its rotational axis, or both may move;</li><li>&quot;teeth or tooth equivalents&quot; include lobes, projections or abutments;</li><li>&quot;internal-axis type&quot; means that the rotational axes of the inner and outer co-operating members remain at all times within the outer member, e.g., in a similar manner to that of a pinion meshing with the internal teeth of a ring gear;</li><li>&quot;free piston&quot; means a piston of which the length of stroke is not defined by any member driven thereby;</li><li>&quot;cylinders&quot; means positive-displacement working chambers in general. Thus, this term is not restricted to cylinders of circular cross-section;</li><li>&quot;main shaft&quot; means the shaft which converts reciprocating piston motion into rotary motion or <u>vice versa</u>;</li><li>&quot;plant&quot; means an engine together with such additional apparatus as is necessary to run the engine. For example, a steam engine plant includes a steam engine and means for generating the steam;</li><li>&quot;working fluid&quot; means the driven fluid in a pump or the driving fluid in an engine. The working fluid can be in a compressible, gaseous state, called elastic fluid, e.g. steam; in a liquid state; or in a state where there is coexistence of an elastic fluid and liquid phase.</li><li>&quot;steam&quot; includes condensable vapours in general, and &quot;special vapour&quot; is used when steam is excluded;</li><li>&quot;reaction type&quot; as applied to non-positive-displacement machines or engines means machines or engines in which pressure/velocity transformation takes place wholly or partly in the rotor. Machines or engines with no, or only slight, pressure/velocity transformation in the rotor are called &quot;impulse type&quot;.</li></ul></li><li>In this subsection:<ul type=""disc""><li>cyclically operating valves, lubricating, gas-flow silencers or exhaust apparatus, or cooling are classified in subclasses <b>F01L</b>, <b>F01M</b>, <b>F01N</b>, <b>F01P</b> irrespective of their stated application, unless their classifying features are peculiar to their application, in which case they are classified only in the relevant subclass of classes <b>F01-F04</b>;</li><li>lubricating, gas-flow silencers or exhaust apparatus, or cooling of machines or engines are classified in subclasses <b>F01M</b>, <b>F01N</b>, <b>F01P</b> except for those peculiar to steam engines which are classified in subclass <b>F01B</b>.</li></ul></li><li>For use of this subsection with a good understanding, it is essential to remember, so far as subclasses <b>F01B</b>, <b>F01C</b>, <b>F01D</b>, <b>F03B</b>, and <b>F04B</b>, <b>F04C</b>, <b>F04D</b>, which form its skeleton, are concerned:<ul type=""disc""><li>the principle which resides in their elaboration,</li><li>the classifying characteristics which they call for, and</li><li>their complementarity.<ul type=""i""><li><u>Principle</u><ul style=""list-style:none""><li>This concerns essentially the subclasses listed above. Other subclasses, notably those of class <b>F02</b>, which cover better-defined matter, are not considered here.</li><li>Each subclass <u>covers</u> fundamentally a genus of apparatus (engine or pump) and by extension covers equally &quot;machines&quot; of the same kind. Two different subjects, one having a more general character than the other, are thus covered by the same subclass.</li><li>Subclasses <b>F01B</b>, <b>F03B</b>, <b>F04B</b>, beyond the two subjects which they cover, have further a character of generality in relation to other subclasses concerning the different species of apparatus in the genus concerned.</li><li>This generality applies as well for the two subjects dealt with, without these always being in relation to the same subclasses.</li><li>Thus, subclass <b>F03B</b>, in its part dealing with &quot;machines&quot;, should be considered as being the general class relating to subclasses <b>F04B</b>, <b>F04C</b>, and in its part dealing with &quot;engines&quot; as being general in relation to subclass <b>F03C</b>.</li></ul></li><li><u>Characteristics</u><ul type=""a""><li>The principal classifying characteristic of the subclass is that of genera of apparatus, of which there are three possible:<ul style=""list-style:none""><li>Machines; engines; pumps.</li></ul></li><li>As stated above, &quot;machines&quot; are always associated with one of the other two genera. These main genera are subdivided according to the general principles of operation of the apparatus:<ul style=""list-style:none""><li>Positive displacement; non-positive displacement.</li></ul></li><li>The positive displacement apparatus are further subdivided according to the ways of putting into effect the principle of operation, that is, to the kind of apparatus:<ul style=""list-style:none""><li>Simple reciprocating piston; rotary or oscillating piston; other kind.</li></ul></li><li>Another classifying characteristic is that of the working fluid, in respect of which three kinds of apparatus are possible, namely:<ul style=""list-style:none""><li>Liquid and elastic fluid; elastic fluid; liquid.</li></ul></li></ul></li><li><u>Complementarity</u><ul style=""list-style:none""><li>This resides in association of pairs of the subclasses listed above, according to the characteristics under consideration in respect of kind of apparatus or working fluid.</li><li>The subclasses concerned with the various principles, characteristics and complementarity are shown in the subsection index below.</li></ul></li></ul></li></ul></li></ul></li><li>It is seen from this index that:<ul type=""disc""><li>For the same kind of apparatus in a given genus, the characteristics of &quot;working fluid&quot; associates:<ul style=""list-style:none""><li><b>F01B</b> and <b>F04B</b> to Machines</li><li><b>F01C</b> and <b>F04C</b> to Machines</li><li><b>F01D</b> and <b>F03B</b> to Machines</li><li><b>F01B</b> and <b>F03C</b> to Engines</li><li><b>F01C</b> and <b>F03C</b> to Engines</li><li><b>F01D</b> and <b>F03B</b> to Engines</li></ul></li><li>For the same kind of working fluid, the &quot;apparatus&quot; characteristic relates subclasses in the same way as considerations of relative generality.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">positive displacement</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">rotary or oscillating piston</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01C</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid only</td><td><b>F04C</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">reciprocating piston or other</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01B</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid only</td><td><b>F04B</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">non-positive displacement</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01D</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">liquid only</td><td><b>F03B</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">positive displacement</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">rotary or oscillating piston</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01C</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid only</td><td><b>F03C</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">reciprocating piston or other</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01B</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">liquid only</td><td><b>F03C</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">non-positive displacement</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">liquid <u>and</u> elastic fluid or elastic fluid</td><td><b>F01D</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">liquid only</td><td><b>F03B</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PUMPS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">positive displacement</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">rotary or oscillating piston</td><td><b>F04C</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">reciprocating piston or other</td><td><b>F04B</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">non-positive displacement</td><td><b>F04D</b></td></p></tr></p></tr></table>MACHINES OR ENGINES IN GENERAL; ENGINE PLANTS IN GENERAL; STEAM ENGINES				
F01B		機械または機関，例．蒸気機関，一般または容積形のもの（回転ピストン式または揺動ピストン式のものＦ０１Ｃ；非容積形のものＦ０１Ｄ；内燃式機関Ｆ０２Ｂ；燃焼生成物を利用する機関設備Ｆ０２Ｇ；容積形以外の液体用機械または機関Ｆ０３Ｂ；液体により駆動される容積形機関Ｆ０３Ｃ；風力原動機Ｆ０３Ｄ；液体用容積形機械Ｆ０４Ｂ；液体用回転ピストンまたは揺動ピストン容積形機械Ｆ０４Ｃ）<br><br><b><ul>注</ul></b><br>注<br>１．このサブクラスは，サブクラスＦ０１ＣからＦ０１Ｐに分類される事項を除いた以下のものを包含する：<br>・圧縮性流体用機関，例．蒸気機関；<br>・液体および圧縮性流体用機関；<br>・圧縮性流体用機械；<br>・液体および圧縮性流体用機械。<br>２．特に“蒸気”および“特殊蒸気”の定義に関しては，クラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>機械または機関<br>往復動ピストンをそなえたもの<br>ピストンの数と配置を特徴とするもの　１／００<br>主軸に対するシリンダ軸の配置を特徴とするもの　３／００，５／００<br>同一または共軸シリンダ内を往復動するピストンを特徴とするもの；上記以外のピストン―主軸連結を特徴とするもの　７／００，１／０８；９／００<br>回軸主軸の無いことを特徴とするもの　１１／００<br>シリンダの回転または他の運動を特徴とするもの　１３／００，１５／００<br>ユニフロー理論を特徴とするもの　１７／００<br>容積形で可とう壁をそなえたことを特徴とするもの　１９／００<br>機械または機関の組み合わせまたは応用　２１／００，２３／００<br>調節，制御，安全装置；始動　２５／００；２７／００<br>他の特徴，細部または付属品　２９／００；３１／００<br>	MACHINES OR ENGINES, IN GENERAL OR OF POSITIVE-DISPLACEMENT TYPE, e.g. STEAM ENGINES (of rotary-piston or oscillating-piston type <b>F01C</b>; of non-positive-displacement type <b>F01D</b>;  internal-combustion engines <b>F02B</b>;  combustion-product engine plants <b>F02G</b>;  machines or engines, other than of positive-displacement type, for liquids <b>F03B</b>;   positive-displacement engines driven by liquids <b>F03C</b>;   wind motors <b>F03D</b>;   positive displacement machines for liquids <b>F04B</b>;   rotary-piston, or oscillating-piston, positive-displacement machines for liquids <b>F04C</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>, with the exception of the matter provided for in subclasses <b>F01C-F01P</b>:<ul type=""disc""><li>engines for elastic fluids, e.g. steam engines;</li><li>engines for liquids and elastic fluids;</li><li>machines for elastic fluids;</li><li>machines for liquids and elastic fluids.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;steam&quot; and &quot;special vapour&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES OR ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With reciprocating pistons characterised by</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">number or relative disposition of cylinders</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">disposition of cylinder axes relative to main shaft</td><td><b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">pistons reciprocating in same or coaxial cylinders; piston-main-shaft connections other than covered above</td><td><b>7/00</b>, <b>1/08</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">no rotary main shaft</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">rotary or other movement of cylinders</td><td><b>13/00</b>, <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">uniflow principle</td><td><b>17/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With positive displacement of flexible-wall type</td><td><b>19/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OR ADAPTATIONS OF MACHINES OR ENGINES</td><td><b>21/00</b>, <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">REGULATING, CONTROLLING, SAFETY MEANS; STARTING</td><td><b>25/00</b>; <b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER CHARACTERISTICS; DETAILS, ACCESSORIES</td><td><b>29/00</b>; <b>31/00</b></td></p></tr></table>				
F01C		回転ピストン式または揺動ピストン式機械または機関（燃焼機関Ｆ０２；内部燃焼に関するものＦ０２Ｂ５３／００，Ｆ０２Ｂ５５／００；液体用機械Ｆ０３，Ｆ０４）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―圧縮性流体．例．水蒸気，を用いる回転ピストン式または揺動ピストン式機関；<br>―液体および圧縮性流体を用いる回転ピストン式または揺動ピストン式機関；<br>―圧縮性流体を用いる回転ピストン式または揺動ピストン式機械；<br>―液体および圧縮性流体を用いる回転ピストン式または揺動ピストン式機械。<br>（２）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“回転ピストン式機械”という用語はドイツ語の“Ｄｒｅｈｋｏｌｂｅｎｍａｓｃｈｉｎｅｎ”“Ｋｒｅｉｓｋｏｌｂｅｎｍａｓｃｈｉｎｅｎ”および“Ｕｍｌａｕｆｋｏｌｂｅｎｍａｓｃｈｉｎｅｎ”なる表現をも含んでいる。<br>（３）特に“回転ピストン式機械”，“揺動ピストン機械”，“回転ピストン”，“共動部材”，“共動部材の運動”，“歯または歯に相当する部分”および“内部軸”に関する定義についてはクラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>機械または機関<br>回転ピストン式のもの　１／００〜７／００<br>揺動ピストン式のもの　９／００<br>制御；監視；安全装置　２０／００<br>機械または機関の組み合わせ，および適用　１１／００，１３／００<br>共動する部材の駆動；密封装置　１７／００；１９／００<br>その他の細部および付属品　２１／００<br>	ROTARY-PISTON OR OSCILLATING-PISTON MACHINES OR ENGINES (combustion engines <b>F02</b>; internal-combustion aspects <b>F02B 53/00</b>, <b>F02B 55/00</b>; machines for liquids <b>F03</b>, <b>F04</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<ul type=""disc""><li>rotary-piston or oscillating-piston engines for elastic fluids, e.g. steam;</li><li>rotary-piston or oscillating-piston engines for liquids and elastic fluids;</li><li>rotary-piston or oscillating-piston machines for elastic fluids;</li><li>rotary-piston or oscillating-piston machines for liquids and elastic fluids.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated:<ul type=""disc""><li>&quot;rotary-piston machine&quot; includes the German expressions &quot;Drehkolbenmaschinen&quot;, &quot;Kreiskolbenmaschinen&quot;, and &quot;Umlaufkolbenmaschinen&quot;.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;rotary-piston machine&quot;, &quot;oscillating-piston machine&quot;, &quot;rotary piston&quot;, &quot;co-operating members&quot;, &quot;movement of co-operating members&quot;, &quot;teeth or tooth-equivalents&quot; and &quot;internal-axis&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES OR ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With rotary pistons</td><td><b>1/00-7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With oscillating pistons</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Control; monitoring; safety arrangements</td><td><b>20/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OR ADAPTATIONS OF MACHINES OR ENGINES</td><td><b>11/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DRIVE OF CO-OPERATING MEMBERS; SEALING ARRANGEMENTS</td><td><b>17/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER DETAILS OR ACCESSORIES</td><td><b>21/00</b></td></p></tr></table>				
F01D		非容積形機械または機関，例．蒸気タービン（燃焼機関Ｆ０２；液体用機械または機関Ｆ０３，Ｆ０４；非容積形ポンプＦ０４Ｄ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する；<br>―圧縮性流体用非容積形機関，例．蒸気タービン；<br>―液体および圧縮性流体用非容積形機関；<br>―圧縮性流体用非容積形機械；<br>―液体および圧縮性流体用非容積形機械<br>（２）特に“反動形”例．エアーフォイル形ブレード，及び“衝動形”，例．バケットタービン，の定義に関して，クラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>非容積形機械または機関<br>一般的特徴；軸推力平衝装置付；純粋な回転とは異なった方式をもつもの　１／００；３／００；２３／００<br>構成部分品<br>ブレードとその支持部材，ブレード保護部材；可調整ブレードをもつロータ；固定子　５／００；７／００；９／００<br>内部漏えいに対する手段　１１／００<br>機械や機関の組み合わせまたは結合　１３／００，１５／００<br>調速，制御，安全装置　１７／００，１９／００；２１／００<br>始動；停止　１９／００；２１／００<br>他の部品と付属品　２５／００<br>	NON-POSITIVE-DISPLACEMENT MACHINES OR ENGINES, e.g. STEAM TURBINES (combustion engines <b>F02</b>; machines or engines for liquids <b>F03</b>, <b>F04</b>; non-positive-displacement pumps <b>F04D</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<ul type=""disc""><li>non-positive-displacement engines for elastic fluids, e.g. steam turbines;</li><li>non-positive-displacement engines for liquids and elastic fluids;</li><li>non-positive-displacement machines for elastic fluids;</li><li>non-positive-displacement machines for liquids and elastic fluids.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;reaction type&quot;, e.g. with airfoil-like blades, and &quot;impulse type&quot;, e.g. bucket turbines.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">NON-POSITIVE-DISPLACEMENT MACHINES OR ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General characteristics; with axial-thrust balancing; with other than pure rotation</td><td><b>1/00</b>; <b>3/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Component parts</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">blades and carrying members, protection thereof; rotors with adjustable blades; stators</td><td><b>5/00</b>; <b>7/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">means against internal leakage</td><td><b>11/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OR ADAPTATIONS OF MACHINES OR ENGINES</td><td><b>13/00</b>, <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">REGULATION, CONTROLLING, SAFETY MEANS</td><td><b>17/00</b>, <b>19/00</b>, <b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STARTING; SHUTTING-DOWN</td><td><b>19/00</b>; <b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER DETAILS AND ACCESSORIES</td><td><b>25/00</b></td></p></tr></table>				
F01K		蒸気機関設備；蒸気アキュムレータ；他に分類されない機関設備；特殊な作動流体またはサイクルを用いた機関（ガスタービンあるいはジェット推進設備Ｆ０２；蒸気発生Ｆ２２；原子力動力設備，その機関の配設Ｇ２１Ｄ）<br><br><b><ul>注</ul></b><br>クラスＦ０１の前の注，特に“蒸気”および“特殊蒸気”に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>蒸気機関設備<br>次のものを使用する事を特徴とするもの<br>アキュムレータあるいは加熱器；アルカリ中に貯蔵する装置；特殊機関　３／００；５／００；７／００<br>特殊な蒸気系，サイクルまたはプロセスをもつもの　７／００<br>次のものの構成を特徴とするもの<br>復水器；機関とボイラまたは復水器の構造的結合　９／００；１１／００<br>他に分類されないもの　２１／００<br>一般的配置または運転法；特殊な用途への応用　１３／００；１５／００<br>蒸気への利用<br>給水加熱のためのもの；再生またはその他の処理におけるもの；他の目的のためのもの　７／３４；１９／００；１７／００<br>蒸気の利用に制限されない機関設備<br>異なった流体によって駆動される数個の機関をもったもの　２３／００<br>他に分類されないもの，特殊な動作流体をもったもの，または閉鎖サイクルで動作するもの　２５／００，２７／００<br>蒸気アキュムレータ　１／００<br>特殊な形の機関<br>蒸気機関　７／００<br>蒸気以外のもの　２５／００<br>	STEAM ENGINE PLANTS; STEAM ACCUMULATORS; ENGINE PLANTS NOT OTHERWISE PROVIDED FOR; ENGINES USING SPECIAL WORKING FLUIDS OR CYCLES (gas-turbine or jet-propulsion plants <b>F02</b>; steam generation <b>F22</b>; nuclear power plants, engine arrangements therein <b>G21D</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;steam&quot; and &quot;special vapour&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STEAM ENGINE PLANTS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characterised by the use of</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">accumulators or heaters; storing means in alkali; specific types of engines</td><td><b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">special steam systems, cycles, or processes</td><td><b>7/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characterised by the disposition of</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">condenser; structural combination of engine and boiler or condenser</td><td><b>9/00</b>; <b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Not otherwise provided for</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General layout or operation; adaptations for special use</td><td><b>13/00</b>; <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Utilisation of steam</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for feed-water heating; in the regeneration or other treating; for other purposes</td><td><b>7/34</b>; <b>19/00</b>; <b>17/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ENGINE PLANTS NOT RESTRICTED TO STEAM UTILISATION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With several engines driven by different fluids</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Not otherwise provided for, other types with special working fluids or working with enclosed cycles</td><td><b>25/00</b>, <b>27/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STEAM ACCUMULATORS</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPECIAL TYPES OF ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Steam engines</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other than steam</td><td><b>25/00</b></td></p></tr></p></tr></table>				
F01L		周期的に作動する機械または機関用弁<br><br><b><ul>注</ul></b><br>（１）　グループ１／００から１３／００は可変流体配分の装備をもたない弁装置または弁配列のみを包含する。［２００９．０１］<br>（２）　蒸気機関に特に適合する弁装置または弁配置はグループ１５／００から３５／００に包含される。［２００９．０１］<br>（３）　可変作動流体配分のある機械または機関に特に適合した弁装置または弁配置はグループ１５／００から３５／００に包含される。［２００９．０１］<br>（４）クラスＦ０１の前の注，特に注（３）に注意すること。<br>（５）上記注（３）に関して，Ｆ０１Ｂ３／１０，Ｆ０１Ｂ１５／０６，Ｆ０１Ｃ２０／２０，Ｆ０１Ｃ２１／１８，Ｆ０２Ｂ５３／０６，Ｆ０３Ｃ１／０８，Ｆ０４Ｂ１／１８，Ｆ０４Ｂ７／００，Ｆ０４Ｂ３９／０８，Ｆ０４Ｂ３９／１０，Ｆ０４Ｃ１４／００，Ｆ０４Ｃ１５／０６，Ｆ０４Ｃ２８／００およびＦ０４Ｃ２９／１２に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>弁装置または弁配列一般<br>一般的事項　１／００<br>作動<br>機械的なもの　１／００<br>機械的でないもの　９／００<br>リフト弁　３／００<br>スライド弁に関するもの　５／００，７／００<br>ピストンまたはピストンロッドにおける配列　１１／００<br>機関の動作を促進させるための変形　１３／００<br>作動流体を可変分配するための弁装置または弁配列<br>一般的事項　１／００<br>スライド弁をもつもの<br>シリンダまたはピストンをとり巻くもの　１７／００<br>回転または振動をするもの；組み合わせたもの　３３／００；１９／００<br>その他の事項　１５／００<br>リフト弁をもつもの　３５／００<br>特殊性をもつ配列；逆運動装置　２１／００〜２７／００；２９／００<br>その他の弁装置または配列　１５／００<br>駆動，制御，または調整　２５／００，３１／００<br>	CYCLICALLY OPERATING VALVES FOR MACHINES OR ENGINES<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Groups <b>F01L 1/00-F01L 13/00</b> <u>cover</u> only valve-gear or valve arrangements without provision for variable fluid distribution.<b>[2009.01]</b></li><li>Valve gear or valve arrangements specially adapted for steam engines are covered by groups <b>F01L 15/00-F01L 35/00</b>.</li><li>Valve-gear or valve arrangements specially adapted for machines or engines with variable working-fluid distribution are covered by groups <b>F01L 15/00-F01L 35/00</b>.</li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially Note (3).</li><li>As regards the above-mentioned Note (3), attention is drawn to <b>F01B 3/10</b>, <b>F01B 15/06</b>, <b>F01C 20/20</b>, <b>F01C 21/18</b>, <b>F02B 53/06</b>, <b>F03C 1/08</b>, <b>F04B 1/18</b>, <b>F04B 7/00</b>, <b>F04B 39/08</b>, <b>F04B 39/10</b>, <b>F04C 14/00</b>, <b>F04C 15/06</b>, <b>F04C 28/00</b> and <b>F04C 29/12</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VALVE-GEAR OR VALVE ARRANGEMENTS IN GENERAL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General features</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Operation</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">mechanical</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">non-mechanical</td><td><b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Lift valves</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Slide valves</td><td><b>5/00</b>, <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements in piston or piston-rod</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Modified to facilitate engine operations</td><td><b>13/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VALVE-GEAR OR VALVE ARRANGEMENTS FOR VARIABLE WORKING-FLUID DISTRIBUTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General features</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With slide valves</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">surrounding cylinder or piston</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with rotary or oscillatory motion; combined</td><td><b>33/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other features</td><td><b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With lift valves</td><td><b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements with particular characteristics; reversing gear</td><td><b>21/00-27/00</b>; <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other valve-gear or valve arrangements</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Drive, control, or adjustment</td><td><b>25/00</b>, <b>31/00</b></td></p></tr></p></tr></table>				
F01M		機械または機関の潤滑一般；内燃機関の潤滑；クランク室の換気［２］<br><br><b><ul>注</ul></b><br>（１）クラスＦ０１の前の注，特に注（３）に注意すること。<br>（２）以下の，特定の機械または機関の潤滑を包含する箇所に注意すること。［８］<br>Ｆ０１Ｂ　３１／１０　蒸気機関［８］<br>Ｆ０１Ｃ　２１／０４　回転ピストンまたは振動ピストン機械または機関［８］<br>Ｆ０１Ｄ　２５／１８　非容積形機械［８］<br>Ｆ０２Ｃ　　７／０６　ガスタービン設備［８］<br>Ｆ０２Ｆ　　１／２０　燃焼機関のシリンダ［８］<br>Ｆ０４Ｂ　３９／０２　圧縮性流体用ポンプ［８］<br>Ｆ０４Ｃ　２９／０２　流体用回転ピストンまたは振動ピストンポンプ［８］<br>Ｆ０４Ｄ　２９／０４　非容積形ポンプ［８］<br><br><b><ul>サブクラス内の索引</ul></b><br>強制潤滑　１／００<br>特殊な潤滑　３／００，７／００，９／００<br>潤滑剤の調整　５／００<br>部品，付属品　１１／００<br>クランク室の換気　１３／００<br>	LUBRICATING OF MACHINES OR ENGINES IN GENERAL; LUBRICATING INTERNAL-COMBUSTION ENGINES; CRANKCASE VENTILATING<b>[2]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards Note (3).<b>[8]</b></li><li>Attention is drawn to the following places, which cover lubrication of specific machines or engines:<table width="100%"><tr><td></td><td><b>F01B 31/10</b></td><td>Steam engines</td></tr><tr><td></td><td><b>F01C 21/04</b></td><td>Rotary-piston or oscillating-piston machines or engines</td></tr><tr><td></td><td><b>F01D 25/18</b></td><td>Non-positive-displacement machines</td></tr><tr><td></td><td><b>F02C 7/06</b></td><td>Gas-turbine plants</td></tr><tr><td></td><td><b>F02F 1/20</b></td><td>Cylinders of combustion engines</td></tr><tr><td></td><td><b>F04B 39/02</b></td><td>Pumps for elastic fluids</td></tr><tr><td></td><td><b>F04C 29/02</b></td><td>Rotary-piston or oscillating-piston pumps for liquids</td></tr><tr><td></td><td><b>F04D 29/04</b></td><td>Non-positive-displacement pumps</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PRESSURE LUBRICATION</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPECIAL LUBRICATION</td><td><b>3/00</b>, <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LUBRICANT CONDITIONING</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS, ACCESSORIES</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CRANKCASE VENTILATION</td><td><b>13/00</b></td></p></tr></table>				
F01N		機械または機関のためのガス流消音器または排気装置一般；内燃機関用ガス流消音器または排気装置（車両の推進装置の排気に関する配置Ｂ６０Ｋ１３／００；特に内燃機関に応用され，結合される燃焼空気入口消音器Ｆ０２Ｍ３５／００；雑音の防止あるいは軽減一般Ｇ１０Ｋ１１／１６）<br><br><b><ul>注</ul></b><br>クラスＦ０１の前の注，特に注（３）に注意すること。<br>	GAS-FLOW SILENCERS OR EXHAUST APPARATUS FOR MACHINES OR ENGINES IN GENERAL; GAS-FLOW SILENCERS OR EXHAUST APPARATUS FOR INTERNAL-COMBUSTION ENGINES (arrangements in connection with gas exhaust of propulsion units in vehicles <b>B60K 13/00</b>; combustion-air intake silencers specially adapted for, or arranged on, internal-combustion engines <b>F02M 35/00</b>; protecting against, or damping, noise in general <b>G10K 11/16</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards Note (3).</li></ul>				
F01P		機械またはエンジンの冷却；内燃機関の冷却（車両の推進装置の冷却に関する配置Ｂ６０Ｋ１１／００；伝熱，熱交換，または蓄熱用の物質Ｃ０９Ｋ５／００；熱交換一般，ラジエーターＦ２８）<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“空気”は他のガス状冷却流体も含む；<br>―“液体冷却”は液体が被冷却物体と空気との間の熱移送流体として使用される冷却，例．ラジエータを用いるものも含む；<br>―“空気冷却”は直接的な空気冷却を意味し，上記液体冷却で説明したように液体冷却系統内でおこる間接的な空気冷却は含まない；<br>―“冷却空気”は直接あるいは間接的に冷却空気として作用するものを含む。<br>（２）クラスＦ０１の前の注，特に注（３）に注意すること。<br>（３）潤滑剤による冷却は，潤滑に要旨があるときはＦ０１Ｍに，冷却に要旨があるときはＦ０１Ｐに分類される。<br>	COOLING OF MACHINES OR ENGINES IN GENERAL; COOLING OF INTERNAL-COMBUSTION ENGINES (arrangements in connection with cooling of propulsion units in vehicles <b>B60K 11/00</b>; heat-transfer, heat-exchange or heat-storage materials <b>C09K 5/00</b>; heat-exchange in general, radiators <b>F28</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;air&quot; also includes other gaseous cooling fluids;</li><li>&quot;liquid cooling&quot; also includes cooling where liquid is used as the heat-transferring fluid between parts to be cooled and the air, e.g. using radiators;</li><li>&quot;air cooling&quot; means direct air cooling and thus excludes indirect air cooling occurring in liquid cooling systems as explained under liquid cooling above;</li><li>&quot;cooling-air&quot; includes directly- or indirectly-acting cooling-air.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards Note (3).</li><li>Cooling by lubricant is classified in subclass <b>F01M</b> when the lubrication aspect predominates, and in subclass <b>F01P</b> when the cooling aspect predominates.</li></ul>				
F02		燃焼機関；熱ガスまたは燃焼生成物を利用する機関設備<br>	COMBUSTION ENGINES; HOT-GAS OR COMBUSTION-PRODUCT ENGINE PLANTS				
F02B		内燃式ピストン機関；燃焼機関一般（ガスタービン設備Ｆ０２Ｃ；燃焼生成物を利用する設備Ｆ０２Ｇ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“外部式点火”は動作流体に対して外的原因による点火，例．電気火花または白熱源によるもの，を意味する；<br>―“給気（Ｃｈａｒｇｉｎｇ）”は機関シリンダ内へ強制的に空気または燃料―空気混合気を入れることを意味し，過給のようなものも含む；<br>―“掃気”はシリンダから動作ピストンの運動による以外の強制的に燃焼残留物を排気することを意味し，排気方式を適合させるようなものも含む。<br>（２）クラスＦ０１の前の注，特に注（１）に注意すること。<br>（３）特殊なサイクルや多シリンダをもつ機関は他の特徴の分類が優先しないかぎり，グループ７５／０２または７５／１６に分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>流体燃料を利用する機関<br>加圧流体を特徴とするものまたは点火に特徴のあるもの　１／００〜１１／００<br>燃焼，吸入口または給気，または排気に特徴のあるもの<br>燃焼<br>予燃焼室；空気室；燃焼室　１９／００；２１／００；２３／００<br>給気；層状給気；給気の回転　１７／００；３１／００<br>燃料供給　１３／００，１５／００，４９／００<br>吸入口または給気，または掃気<br>一般的な特徴；細部　２５／００〜２９／００；２９／００<br>ポンプ；細部　３３／００〜３７／００；３９／００<br>効率改善のための特殊な手段　４１／００<br>液体でない燃料を利用する機関；燃料生成装置との組み合わせ　４３／００，４５／００<br>燃料，空気，混合気の処理または前処理に特徴のある操作　７／００，４７／００，４９／００，５１／００<br>特殊な形またはその応用<br>機関の種別<br>ピストンの種別：回転式，揺動式；回転式機関または可動シリンダ内で往復動するもの；自由ピストンまたは回転する主軸のないもの　５３／００，５５／００；５７／００，５９／００；７１／００<br>転用または相互に交換できる部品　６９／００<br>特殊な補助装置をもつもの　６７／００<br>その他の種別；構成部分，細部または付属部分　７５／００；７７／００<br>２つまたはそれ以上の機関の組み合わせでその他に分類されないもの　７３／００<br>特別な用途のための機関，その他の装置との組み合わせ　６１／００〜６７／００<br>運転　７９／００<br>	INTERNAL-COMBUSTION PISTON ENGINES; COMBUSTION ENGINES IN GENERAL (gas-turbine plants <b>F02C</b>; hot-gas or combustion-product positive-displacement engine plants <b>F02G</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following terms or expression are used with the meanings indicated:<ul type=""disc""><li>&quot;positive ignition&quot; means ignition by a source external to the working fluid, e.g. by spark or incandescent source;</li><li>&quot;charging&quot; means forcing air or fuel-air mixture into engine cylinders, and thus includes supercharging;</li><li>&quot;scavenging&quot; means forcing the combustion residues from the cylinders other than by movement of the working pistons, and thus includes tuned exhaust systems.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards Note (1).</li><li>Engines with specified cycles or number of cylinders are classified in group <b>F02B 75/02</b> or <b>F02B 75/16</b>, unless other classifying features predominate.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ENGINES USING FLUID FUEL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characterised by fluid to be compressed or by ignition</td><td><b>1/00-11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characterised by the combustion, inlet or charging, or evacuation</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">combustion</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">chambers for: precombustion; air storage; combustion</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">charge: stratification; rotation</td><td><b>17/00</b>; <b>31/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">introduction of fuel</td><td><b>13/00</b>, <b>15/00</b>, <b>49/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">inlet or charging, or scavenging</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">general characteristics; details</td><td><b>25/00-29/00</b>; <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">pumps; details</td><td><b>33/00-37/00</b>; <b>39/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Special means for improving efficiency</td><td><b>41/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ENGINES USING NON-LIQUID FUEL, THEIR COMBINATIONS WITH FUEL-GENERATING APPARATUS</td><td><b>43/00</b>, <b>45/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OPERATION CHARACTERISED BY TREATMENT OR PRETREATMENT OF FUEL, AIR, OR MIXTURE</td><td><b>7/00</b>, <b>47/00</b>, <b>49/00</b>, <b>51/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPECIAL FORMS OR APPLICATIONS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Kinds of engine</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">kinds of piston: rotary, oscillating; reciprocating in rotary engines or movable cylinders; free-piston or without rotating main shaft</td><td><b>53/00</b>, <b>55/00</b>; <b>57/00</b>, <b>59/00</b>; <b>71/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">convertible or with interchangeable parts</td><td><b>69/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with special auxiliary apparatus</td><td><b>67/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other kinds; component parts, details, or accessories</td><td><b>75/00</b>; <b>77/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations, not otherwise provided for, of two or more engines</td><td><b>73/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Engines for particular use, combinations with other devices</td><td><b>61/00-67/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">RUNNING-IN</td><td><b>79/00</b></td></p></tr></table>				
F02C		ガスタービン設備；ジェット推進設備のための空気の取り入れ；空気吸込ジェット推進設備における燃料供給制御（タービンの構造Ｆ０１Ｄ；ジェット推進設備Ｆ０２Ｋ；圧縮機又はファンの構造Ｆ０４；燃焼が燃料または他の粒子の流体層で発生する燃焼装置Ｆ２３Ｃ１０／００；高圧または高速の燃焼生成物の生成Ｆ２３Ｒ；圧縮冷凍設備におけるガスタービンの使用Ｆ２５Ｂ１１／００）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―燃焼ガスまたは高温ガスを使うタービン設備；<br>―内燃タービンまたはタービン設備；<br>―作動流体が加熱されない圧縮気体であるタービン設備。<br>（２）このサブクラスは以下のものを包含しない：<br>―Ｆ０１Ｋに包含される蒸気タービン設備；<br>―Ｆ０１Ｋに包含される特殊な蒸気による設備。<br>（３）このサブクラスにおいては，下記の表現は以下に示す意味で用いる。<br>―“ガスタービン設備”は注（１）のすべての主題事項を包含し，そしてさらにガスタービン設備と共通のジェット推進設備の特徴も包含する。<br>（４）クラスＦ０１の前の注に注意すること。<br>	GAS-TURBINE PLANTS; AIR INTAKES FOR JET-PROPULSION PLANTS; CONTROLLING FUEL SUPPLY IN AIR-BREATHING JET-PROPULSION PLANTS (construction of turbines <b>F01D</b>; jet-propulsion plants <b>F02K</b>; construction of compressors or fans <b>F04</b>; combustion apparatus in which combustion takes place in a fluidised bed of fuel or other particles <b>F23C 10/00</b>; generating combustion products of high pressure or high velocity <b>F23R</b>; using gas turbines in compression refrigeration plants <b>F25B 11/00</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<ul type=""disc""><li>combustion product or hot gas turbine plants;</li><li>internal combustion turbines or turbine plants;</li><li>turbine plants in which the working fluid is an unheated, pressurised gas.</li></ul></li><li>This subclass <u>does not cover</u>:<ul type=""disc""><li>steam turbine plants, which are covered by subclass <b>F01K</b>;</li><li>special vapour plants, which are covered by subclass <b>F01K</b>.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated:<ul type=""disc""><li>&quot;gas-turbine plants&quot; covers all the subject matter of Note (1) above and covers also features of jet-propulsion plants common to gas-turbine plants.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li></ul>				
F02D		燃焼機関の制御（車両速度を自動的に制御する車両付属品であって，単一のサブユニットのみに作用するものＢ６０Ｋ３１／００；異なる種類又は異なる機能の車両用サブユニットの関連制御，特定の単一のサブユニットの制御に関するものではない，特定の目的のための道路上の車両の運転制御システムＢ６０Ｗ）［２００６．０１］<br><br><b><ul>注</ul></b><br>注［４］<br>１．このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>・“燃料噴射”とは可燃性物質を，その背後で連続的かまたは周期的に作動する圧力源，例．ポンプ，によってある空間，例．シリンダ，に導入することを意味する；<br>・“過給”とは圧力源，例．ポンプ，によって圧縮された燃焼空気を動作空間，例．シリンダ，に供給することを意味する。<br>２．クラスＦ０１の前の注に注意すること。<br>３．このサブクラスにおいては，制御装置の電気的な観点に特徴があるものはグループ４１／００から４５／００に分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>燃焼機関の制御または調整一般<br>機関の運転中に作動することを特徴とするもの<br>噴射に関するもの：一般；低圧；その他の手段　１／００；３／００；７／００<br>空気または混合気の吸入または排出を絞ることによるもの　９／００<br>弁の作動周期に関するもの；圧縮比を変化させるもの　１３／００；１５／００<br>シリンダの作動の停止，機関を不作動または無負荷状態とするもの　１７／００<br>燃料または燃焼空気の配分に関するもので他に分類されないもの　３３／００<br>複数の相伴った機能に関するもので他に分類されないもの　３７／００<br>操作開始手段または駆動手段を特徴とするもの<br>操作開始が自動でないもの，例．オペレータによるもの　１１／００<br>速度検出の調速機によるか，または内部もしくは外部状態による起動で他に分類されないもの　３１／００，３５／００<br>プログラム制御　２８／００<br>特殊な機関の制御<br>燃料を特徴とする機関；使用された燃焼媒質の使用を特徴とする機関；過給を特徴とする機関のためのもの　１９／００；２１／００；２３／００<br>協働して作動する機関；逆転可能な機関；車両または特殊な装置を駆動する機関　２５／００；２７／００；２９／００<br>その他の制御<br>非電気的なもの　３９／００<br>電気的なもの　４１／００〜４５／００<br>	CONTROLLING COMBUSTION ENGINES (vehicle fittings, acting on a single sub-unit only, for automatically controlling vehicle speed <b>B60K 31/00</b>;  conjoint control of vehicle sub-units of different type or different function, road vehicle drive control systems for purposes other than the control of a single sub-unit <b>B60W</b>)<b>[4,8]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following term or expression is used with the meanings indicated:<b>[4]</b><ul type=""disc""><li>&quot;fuel injection&quot; means the introduction of a combustible substance into a space, e.g. cylinder, by means of a pressure source, e.g. a pump, continuously or cyclically acting behind the substance;</li><li>&quot;supercharging&quot; means supplying to the working space, e.g. cylinder, combustion-air pressurised by means of a pressure source, e.g. a pump.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li><li>In this subclass, electrical aspects of control arrangements are classified in groups <b>F02D 41/00-F02D 45/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROLLING COMBUSTION ENGINES IN GENERAL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">characterised by action on engine operation</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">on injection: general; low pressure; other means</td><td><b>1/00</b>; <b>3/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">by throttling air or fuel-and-air induction or exhaust</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">on valve-operating cycle; varying compression ratio</td><td><b>13/00</b>; <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">cutting-out cylinders, rendering engines inoperative or idling</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">on delivery of fuel or combustion-air, not otherwise provided for</td><td><b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">on two or more associated functions not otherwise provided for</td><td><b>37/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">characterised by initiating or actuating means</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">non-automatic initiation, e.g. by operator</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">initiation by speed-sensing governors or by interior or exterior conditions, not otherwise provided for</td><td><b>31/00</b>, <b>35/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Program control</td><td><b>28/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL OF PARTICULAR ENGINES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">engines: characterised by fuel; by combustion medium used; by supercharge</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">co-operating engines; reversible engines; engines driving vehicle or particular devices</td><td><b>25/00</b>; <b>27/00</b>; <b>29/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER CONTROL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">non-electrical</td><td><b>39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">electrical</td><td><b>41/00-45/00</b></td></p></tr></p></tr></table>				
F02F		燃焼機関のシリンダ，ピストンまたはケーシング；燃焼機関の密封装置の構成［２］<br><br><b><ul>注</ul></b><br>（１）クラスＦ０１の前の注に注意すること。<br>（２）主題事項が燃焼機関特有のものを除いてクラスＦ１６がこのサブクラスに優先。<br>	CYLINDERS, PISTONS, OR CASINGS FOR COMBUSTION ENGINES; ARRANGEMENTS OF SEALINGS IN COMBUSTION ENGINES<b>[2]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li><li>Class <b>F16</b> takes precedence over this subclass, except for subject matter specific to combustion engines.</li></ul>				
F02G		熱ガスまたは燃焼生成容積型機関設備（蒸気機関設備，特殊な蒸気設備，他の流体と共に熱ガスまたは燃焼生成ガスのいずれかで作動する設備Ｆ０１Ｋ；ガスタービン設備Ｆ０２Ｃ；ジェット推進設備Ｆ０２Ｋ）；燃焼機関の廃熱を利用するもので，他に分類されないもの<br><br><b><ul>注</ul></b><br>クラスＦ０１の前の注に注意すること。<br>	HOT-GAS OR COMBUSTION-PRODUCT POSITIVE-DISPLACEMENT ENGINE PLANTS (steam engine plants, special vapour plants, plants operating on either hot gas or combustion-product gases together with other fluid <b>F01K</b>; gas-turbine plants <b>F02C</b>; jet-propulsion plants <b>F02K</b>); USE OF WASTE HEAT OF COMBUSTION ENGINES, NOT OTHERWISE PROVIDED FOR<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li></ul>				
F02K		ジェット推進設備（陸上車または乗り物一般の中の，ジェット推進設備の配置または取り付けＢ６０Ｋ；船舶の中の，ジェット推進設備の配置または取り付けＢ６３Ｈ；噴出流の反動による航空機の姿勢，飛行角度または高度を制御するものＢ６４Ｃ１５／００，Ｂ６４Ｕ５０／１０；航空機内の，ジェット推進設備の配置または取り付けＢ６４Ｄ２７／００，Ｂ６４Ｕ５０／１０；ジェット推進と別の形態の推進との間に分けられている，作動流体の推進力に特徴がある設備，例．プロペラ，Ｆ０２Ｂ，Ｆ０２Ｃ；ガスタービン設備と共通するジェット推進設備の特徴，空気吸込ジェット推進設備の空気取入口または燃料供給制御Ｆ０２Ｃ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“ジェット推進装置”とは燃焼によって流体の流れを作り出し，それの反動によって推力を生じるような装置を意味する。<br>（２）クラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>パイプまたはノズルに特徴のある装置１／００，９／８０<br>圧縮機またはファンに特徴のある装置３／００，５／００<br>圧縮機またはファンのない装置７／００<br>ロケットエンジン設備９／００<br>制御１／１５，１／７６，７／００，９／００<br>その他の装置９９／００<br>	JET-PROPULSION PLANTS (arrangement or mounting of jet-propulsion plants in land vehicles or vehicles in general <b>B60K</b>; arrangement or mounting of jet-propulsion plants in waterborne vessels <b>B63H</b>; controlling aircraft attitude, flight direction or altitude by jet reaction <b>B64C 15/00</b>, <b>B64U 50/10</b>; arrangement or mounting of jet-propulsion plants in aircraft <b>B64D 27/00</b>, <b>B64U 50/10</b>; plants characterised by the power of the working fluid being divided between jet propulsion and another form of propulsion, e.g. propeller, <b>F02B</b>, <b>F02C</b>; features of jet-propulsion plants common to gas-turbine plants, air intakes or fuel supply control of air-breathing jet-propulsion plants <b>F02C</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following expression is used with the meaning indicated:<ul type=""disc""><li>&quot;jet-propulsion plants&quot; means plants using combustion to produce a fluid stream from which a propulsive thrust on the plants is obtained on the reaction principle.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PLANTS CHARACTERISED BY JET PIPE OR NOZZLE</td><td><b>1/00</b>, <b>9/80</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PLANTS WITH COMPRESSOR OR FAN</td><td><b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PLANTS WITHOUT COMPRESSOR OR FAN</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROCKET-ENGINE PLANTS</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL</td><td><b>1/15</b>, <b>1/76</b>, <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER PLANTS</td><td><b>99/00</b></td></p></tr></table>				
F02M		一般の燃焼機関への可燃混合物またはその成分の供給<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語または表現は以下の意味で用いる：<br>―“気化器”とは本来燃料と空気を混合する装置を意味し，その燃料は低空気圧で，例．ベンチュリー内で，空気と接触混合される；<br>―“燃料噴射装置”とは空間，例．機関シリンダ，に燃料を加圧して，例．燃料に作用するポンプによって，導入する装置を意味する。したがって，液体燃料が気体と混合せずに導入される，通称“無気燃料噴射”をも包含する；<br>―“低圧燃料噴射”とは噴射された燃料を含む燃料−空気混合物が機関の圧縮される燃料噴射を意味する；<br>―“ポンプ要素”とは往復動ピストン式燃料噴射ポンプ内の１組のピストン―シリンダユニットまたは他の形式の燃料噴射ポンプ内の同等のユニットを意味する。<br>（２）クラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>液体燃料の供給<br>気化器<br>始動，アイドリング；フロートにより制御される油面；混合気制御；絞り，混合室　１／００，３／００；５／００；７／００；９／００<br>加熱，冷却，絶縁　１５／００<br>多段，レジスタ形；気化器または燃料の組み合わせ；低圧噴射との組み合わせ　１１／００；１３／００；７１／００<br>他の特性；他の細部，または付属品　１７／００；１９／００<br>噴射装置<br>一般的特性，ガスを伴わぬ噴射<br>２種以上の連続的に供給するインゼクタをもつもの；２種以上の液体をもつもの　４１／００；４３／００<br>周期的送出特性を有するもの；流体操作弁をもつもの　４５／００；４７／００<br>シリンダ圧力またはそのピストンにより操作されるポンプまたはインゼクタをもつもの　４９／００<br>電気的に操作されるもの　５１／００<br>加熱，冷却または絶縁手段をもつもの；燃料管または通気手段に特徴のあるもの　５３／００；５５／００<br>他の装置と組み合わされたインゼクタ　５７／００<br>機関に関する装置の配列，ポンプ駆動部に関する装置の配列　３９／００<br>ポンプのその他の適用；その他のインゼクタ　５９／００；６１／００<br>他の装置，細部または付属品　６３／００，６９／００<br>試験　６５／００<br>高圧ガスの使用　６７／００<br>低圧装置　５１／０２，６９／００，７１／００<br>非液体燃料の供給　２１／００<br>燃料，空気または混合物の供給または前処理<br>燃料，空気または混合物の前処理<br>２次空気を加えるもの；非燃料物質または２次燃料を加えるもの　２３／００；２５／００<br>触媒，電気または磁気手段によるもの，あるいは音または輻射によるもの；熱的に行なうもの　２７／００；３１／００<br>再霧化または均質化することによるもの；空気清浄；他の処理　２９／００；３５／００；３３／００<br>空気取り入れ口または消音器，吸込系統　３５／００<br>気化器または噴射装置への燃料の供給　３７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	SUPPLYING COMBUSTION ENGINES IN GENERAL WITH COMBUSTIBLE MIXTURES OR CONSTITUENTS THEREOF<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;carburettors&quot; means essentially apparatus for mixing fuel with air, the fuel being brought into mixing contact with the air by lowering the air pressure, e.g. in a venturi;</li><li>&quot;fuel-injection apparatus&quot; means apparatus for introducing fuel into a space, e.g. engine cylinder, by pressurising the fuel, e.g. by a pump acting behind the fuel, and thus includes the so-called &quot;solid-fuel injection&quot; in which liquid fuel is introduced without any admixture of gas;</li><li>&quot;low-pressure fuel injection&quot; means fuel injection in which the fuel-air mixture containing fuel thus injected will be substantially compressed in the compression stroke of the engine;</li><li>&quot;pumping element&quot; means a single piston-cylinder unit in a reciprocating-piston fuel-injection pump or the equivalent unit in any other type of fuel-injection pump.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPLYING WITH LIQUID FUEL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Carburettors</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">starting, idling; float-controlled fuel level; mixture control; throttling, mixing chambers</td><td><b>1/00</b>, <b>3/00</b>; <b>5/00</b>; <b>7/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">heating, cooling, insulating</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">multi-stage, register type; combinations of carburettors or fuels; combination with low-pressure injection</td><td><b>11/00</b>; <b>13/00</b>; <b>71/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other characteristics; other details, or accessories</td><td><b>17/00</b>; <b>19/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Injection apparatus</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">general characteristics, injection without gas</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">with two or more sequentially-fed injectors; with two or more liquids</td><td><b>41/00</b>; <b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">with cyclic delivery characteristics; with fluid-actuated valves</td><td><b>45/00</b>; <b>47/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">with pump or injector actuated by cylinder pressure or by the piston</td><td><b>49/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">electrically-operated</td><td><b>51/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">with heating, cooling, or insulating means; characterised by fuel pipes or venting means</td><td><b>53/00</b>; <b>55/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">injectors combined with other devices</td><td><b>57/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">arrangements of apparatus relative to engine, related pump drives</td><td><b>39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">other adaptations of pumps; other injectors</td><td><b>59/00</b>; <b>61/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">other apparatus, details, or accessories</td><td><b>63/00</b>, <b>69/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">testing</td><td><b>65/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">using high-pressure gas</td><td><b>67/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">low-pressure apparatus</td><td><b>51/02</b>, <b>69/00</b>, <b>71/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPLYING WITH NON-LIQUID FUEL</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FEEDING OR PRETREATING AIR, FUEL, OR FUEL-AIR MIXTURE</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pre-treating fuel, air, or mixture</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">adding secondary air; adding non-fuel substances or secondary fuel; adding exhaust gases</td><td><b>23/00</b>; <b>25/00</b>;<b>26/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">by catalytic, electrical, or magnetic means, or by sound or radiation; thermally</td><td><b>27/00</b>; <b>31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">by re-atomising or homogenising; air cleaning; other treatment</td><td><b>29/00</b>; <b>35/00</b>; <b>33/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Air intakes or silencers, induction systems</td><td><b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fuel transfer to carburettors or injection apparatus</td><td><b>37/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F02N		燃焼機関の始動（自由ピストン燃焼機関の始動Ｆ０２Ｂ７１／０２；ガスタービン装置の始動Ｆ０２Ｃ７／２６）；他類に属しない機関の始動補助<br><br><b><ul>注</ul></b><br>（１）クラスＦ０１の前の注に注意すること。<br>（２）明らかに燃焼機関であるとは必ずしも言えない機関の始動でもそれら機関の始動が燃焼機関の始動に相当する限りこのサブクラスに分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>人力による始動　１／００，３／００，５／００<br>その他の始動<br>機械的エネルギの蓄積部をもつもの　５／００<br>流体原動機によるもの；電動機によるもの　７／００；１１／００<br>作動室内において直接運動するもの：流体圧力によるもの；爆薬によるもの　９／００；１３／００<br>他の装置によるもの，細部，付属品　１５／００<br>始動のための他の手段または補助　１９／００，９９／００<br>	STARTING OF COMBUSTION ENGINES; STARTING AIDS FOR SUCH ENGINES, NOT OTHERWISE PROVIDED FOR<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li><li>The starting of engines which are not explicitly stated to be combustion engines is classified in this subclass in so far as their starting is equivalent to that of combustion engines.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STARTING BY MUSCLE POWER</td><td><b>1/00</b>, <b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STARTING OTHERWISE</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With mechanical energy storage</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By fluid motor; by electric motor</td><td><b>7/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By direct action in the working chamber: by fluid pressure; by explosives</td><td><b>9/00</b>; <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By other apparatus, details, accessories</td><td><b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER MEANS OR AIDS FOR STARTING</td><td><b>19/00</b>, <b>99/00</b></td></p></tr></table>				
F02P		内燃機関の点火で圧縮点火以外のもの；圧縮点火機関の点火時期の試験（特に回転ピストンまたは揺動ピストン機関に適したものＦ０２Ｂ５３／１２；燃焼装置の点火一般，予熱プラグＦ２３Ｑ；物理的変数の測定一般Ｇ０１；制御一般Ｇ０５；データ処理一般Ｇ０６；電気的な構成部品一般セクションＨ；点火プラグＨ０１Ｔ）<br><br><b><ul>サブクラス内の索引</ul></b><br>電気火花点火<br>発電機に直結するもの；その他の装置　１／００；３／００<br>機関部品と結合した構造の点火プラグ　１３／００<br>制御：点火時期，配電；その他　５／００，７／００；９／００<br>安全装置　１１／００<br>その他の特徴　１５／００<br>試験　１７／００<br>電気火花以外の点火：白熱によるもの；直接の炎によるもの；他の手段によるもの　１９／００；２１／００；２３／００<br>	IGNITION, OTHER THAN COMPRESSION IGNITION, FOR INTERNAL-COMBUSTION ENGINES; TESTING OF IGNITION TIMING IN COMPRESSION-IGNITION ENGINES (specially adapted for rotary-piston or oscillating-piston engines <b>F02B 53/12</b>;  ignition of combustion apparatus in general, glowing plugs <b>F23Q</b>;  measuring of physical variables in general <b>G01</b>;  controlling in general <b>G05</b>;  data processing in general <b>G06</b>;  electrical components in general, <u>see</u> section <b>H</b>;  sparking plugs <b>H01T</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ELECTRIC SPARK IGNITION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Directly from generator; other installations</td><td><b>1/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Sparking plugs structurally combined with engine parts</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Control: timing, distributing; other</td><td><b>5/00</b>, <b>7/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Safety means</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other features</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Testing</td><td><b>17/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">IGNITION OTHERWISE THAN BY ELECTRIC SPARK: BY INCANDESCENCE; BY DIRECT FLAME; BY OTHER MEANS</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr></table>				
F03		液体用機械または機関；風力原動機，ばね原動機，重力原動機；他類に属さない機械動力または反動推進力を発生するもの<br>	MACHINES OR ENGINES FOR LIQUIDS; WIND, SPRING, OR WEIGHT MOTORS; PRODUCING MECHANICAL POWER OR A REACTIVE PROPULSIVE THRUST, NOT OTHERWISE PROVIDED FOR				
F03B		液体用機械または機関（液体および圧縮性流体用機械または機関Ｆ０１；液体用容積形機関Ｆ０３Ｃ；液体用容積形機械Ｆ０４）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包合する：<br>―液体により駆動される容積形以外の機関；<br>―容積形以外の流体機械。<br>（２）特に反動形の定義に関してクラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>反動または衝動タービン　１／００，３／００<br>機械または機関：無翼回転体形；水車；無限鎖帯形　５／００；７／００；９／００<br>上記の形の部品または細部　１／００，３／００，１１／００<br>応用または組み合わせ　１３／００<br>制御　１５／００<br>その他の機械または機関　１７／００<br>	MACHINES OR ENGINES FOR LIQUIDS (machines or engines for liquids and elastic fluids <b>F01</b>; positive-displacement engines for liquids <b>F03C</b>; positive-displacement machines for liquids <b>F04</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<ul type=""disc""><li>engines, other than of positive-displacement type, driven by liquids;</li><li>machines, other than of positive-displacement type, for liquids.</li></ul></li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definition of &quot;reaction type&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TURBINES: IMPULSE; REACTION</td><td><b>1/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES OR ENGINES: NON-BLADED ROTOR TYPE; WATER WHEELS; ENDLESS-CHAIN TYPE</td><td><b>5/00</b>; <b>7/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PARTS OR DETAILS OF ABOVE KINDS</td><td><b>1/00</b>, <b>3/00</b>, <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ADAPTATIONS OR COMBINATIONS</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROLLING</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER MACHINES OR ENGINES</td><td><b>17/00</b></td></p></tr></table>				
F03C		液体により駆動される容積形機関（液体および圧縮性流体用容積形機関Ｆ０１；液体用容積形機械Ｆ０４；流体圧アクチュエータＦ１５Ｂ；流体伝動装置Ｆ１６Ｈ）<br><br><b><ul>注</ul></b><br>“容積形”，“回転ピストン機械”，“揺動ピストン機械”，“回転ピストン”，“共動部材”，“共動部材の運動”，“歯または歯に相当するもの”および“内部軸”の定義に関して特にクラスＦ０１の前の注に注意すること。<br>	POSITIVE-DISPLACEMENT ENGINES DRIVEN BY LIQUIDS (positive-displacement engines for liquids and elastic fluids <b>F01</b>; positive-displacement machines for liquids <b>F04</b>; fluid-pressure actuators <b>F15B</b>; fluid gearing <b>F16H</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;positive displacement&quot;, &quot;rotary-piston machines&quot;, &quot;oscillating-piston machines&quot;, &quot;rotary-piston&quot;, &quot;co-operating members&quot;, &quot;movement of co-operating members&quot;, &quot;teeth or tooth-equivalents&quot;, and &quot;internal axis&quot;.</li></ul>				
F03D		風力原動機<br><br><b><ul>注</ul></b><br>（１）このサブクラスは風力原動機，すなわち風力のエネルギーを有用な機械的動力に変換するための機構と，その使用目的のための変換された動力の伝達，を包含する。［２０１２．０１］<br>（２）このサブクラスは電力の発電または風力発電所の配電の観点は包含しない。それらはセクションＨ，例．Ｈ０２ＪまたはＨ０２Ｐ，に包含される。［２０１２．０１］<br>（３）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“回転子”は風力原動機において風力の作用する部品とそれらを保持する回転部材を意味する；<br>―“回転軸”は回転子の回転軸を意味する。<br>	WIND MOTORS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> wind motors, i.e. mechanisms for converting the energy of wind into useful mechanical power, and the transmission of such power to its point of use.</li><li>This subclass <u>does not cover</u> electrical power generation or distribution aspects of wind-power plants, which are covered by section <b>H</b>, e.g. <b>H02J</b> or <b>H02P</b>.</li><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;rotor&quot; means the wind-engaging parts of the wind motor and the rotary member carrying them;</li><li>&quot;rotation axis&quot; means the axis of rotation of the rotor.</li></ul></li></ul>				
F03G		ばね，重力，慣性または同様な原動機；機械的動力を生み出す装置または機構であって，他類に属しないものまたは他類に属しないエネルギ源を用いるもの（車両における自然力からの動力供給に関する配置Ｂ６０Ｋ１６／００；車両における自然力からの動力供給による電気的推進Ｂ６０Ｌ８／００）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“原動機”は固体の位置エネルギから機械的動力を生み出すための機構を意味する。<br>	SPRING, WEIGHT, INERTIA, OR LIKE MOTORS; MECHANICAL-POWER-PRODUCING DEVICES OR MECHANISMS, NOT OTHERWISE PROVIDED FOR OR USING ENERGY SOURCES NOT OTHERWISE PROVIDED FOR (arrangements in connection with power supply in vehicles from force of nature <b>B60K 16/00</b>; electric propulsion with power supply in vehicles from force of nature <b>B60L 8/00</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following term is used with the meaning indicated:<ul type=""disc""><li>&quot;motors&quot; means mechanisms for producing mechanical power from potential energy of solid bodies.</li></ul></li></ul>				
F03H		反動推進力を産み出すもので，他類に属しないもの（燃焼生成物からのものＦ０２Ｋ）<br>	PRODUCING A REACTIVE PROPULSIVE THRUST, NOT OTHERWISE PROVIDED FOR (from combustion products <b>F02K</b>)				
F04		液体用容積形機械；液体または圧縮性流体用ポンプ<br><br><b><ul>注</ul></b><br>容積形ポンプと非容積形ポンプの組合わせは，ポンプのための一般的なサブクラスとしてはＦ０４Ｂ，サブクラスＦ０４Ｃ，Ｆ０４Ｄに特有な事項に関しては，Ｆ０４Ｃ，Ｆ０４Ｄに分類される。<br>	POSITIVE-DISPLACEMENT MACHINES FOR LIQUIDS; PUMPS FOR LIQUIDS OR ELASTIC FLUIDS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Combinations of positive-displacement and non-positive-displacement pumps are classified in subclass <b>F04B</b> as a general subclass for pumps, and in subclasses <b>F04C</b>, <b>F04D</b> in respect of matter specific to those subclasses.</li></ul>				
F04B		液体用容積形機械；ポンプ（回転ピストン形または揺動ピストン形の液体機械またはポンプＦ０４Ｃ；非容積形ポンプＦ０４Ｄ；他の液体との直接の接触により，またはポンプされる液体の慣性力を利用することによって流体をポンプするものＦ０４Ｆ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―このサブクラスにおいて，“ピストン”はプランジャーをも含む。<br>（２）“マイクロ構造装置”と“マイクロ構造システム”に関するクラスＢ８１とサブクラスＢ８１Ｂのタイトルの後の注に注意すること。［７］<br>（３）特に“機械”，“ポンプ”および“容積形”の定義に関してクラスＦ０１の前の注に注意すること。<br>（４）柔軟な作動部材を有する機械、ポンプまたはポンプ装置はグループ４３／００または４５／００に分類する。［２００９．０１］<br><br><b><ul>サブクラス内の索引</ul></b><br>液体用容積形機械，ポンプ一般<br>機械およびポンプの一般的特徴<br>多シリンダ，単シリンダ；シリンダ内で共動するピストン；面積差のあるピストン；柔軟な作動部材　１／００；３／００；５／００；４３／００<br>確実に駆動される分配用部材；作動部材の駆動手段または作動部材によって駆動される手段　７／００；９／００<br>波動の平滑化，キャビテーション防止　１１／００<br>他の特徴　１９／００<br>ポンプ，その適用または組み合わせに特有な特徴<br>計量された量の移送；特別な液体の取扱い；深い所からのくみ揚げ　１３／００；１５／００；４７／００<br>特別な駆動機関への取り付け　１７／００<br>その他の特徴　１９／００<br>ポンプ装置または系　２３／００，４３／００，４７／００<br>構成部分品，細部または付属品　５３／００<br>圧縮性流体用ポンプ<br>一般的特徴<br>多段；多シリンダ　２５／００；２７／００<br>自由ピストン；柔軟な作動部材；人力により作動するもの　３１／００；４５／００；３３／００<br>駆動装置　３５／００<br>深い所からくみ揚げるためのもの　４７／００<br>他の特徴；他の細部または付属品　３７／００；３９／００<br>ポンプ装置または系　４１／００，４５／００，４７／００<br>制御，安全手段；試験　４９／００；５１／００<br>構成要素；細部または付属品　５３／００<br>	POSITIVE-DISPLACEMENT MACHINES FOR LIQUIDS; PUMPS (machines for liquids, or pumps, of rotary-piston or oscillating-piston type <b>F04C</b>;  non-positive-displacement pumps <b>F04D</b>;  pumping of fluid by direct contact of another fluid or by using inertia of fluid to be pumped <b>F04F</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following term is used with the meaning indicated:<b>[7,2009.01]</b><ul type=""disc""><li>&quot;piston&quot; also covers a plunger.</li></ul></li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b>relating to &quot;microstructural devices&quot; and &quot;microstructural systems&quot;.</li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;machines&quot;, &quot;pumps&quot;, and &quot;positive-displacement&quot;.</li><li>Machines, pumps or pumping installations having flexible working members are classified in groups <b>F04B 43/00</b> or <b>F04B 45/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">POSITIVE-DISPLACEMENT MACHINES FOR LIQUIDS, PUMPS IN GENERAL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General characteristics of machines and pumps</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">multiple cylinders; single cylinders, pistons coacting in cylinder; differential-surface pistons; flexible working members</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">positively-driven distribution members; driving or driven means to or from working members</td><td><b>7/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">equalization of pulses, counteracting cavitation</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other characteristics</td><td><b>19/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characteristics peculiar to pumps, their adaptations or combinations</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">delivering measured quantities; handling specific fluids; pumping from great depths</td><td><b>13/00</b>; <b>15/00</b>; <b>47/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">associated with specific driving engines</td><td><b>17/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other characteristics</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pumping installations or systems</td><td><b>23/00</b>, <b>43/00</b>, <b>47/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Component parts, details or accessories</td><td><b>53/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PUMPS FOR ELASTIC FLUIDS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General characteristics</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">multiple stages; multiple cylinders</td><td><b>25/00</b>; <b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">free piston; flexible working member; actuation by muscle power</td><td><b>31/00</b>; <b>45/00</b>; <b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">driving means</td><td><b>35/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For pumping from great depths</td><td><b>47/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other characteristics; other details or accessories</td><td><b>37/00</b>; <b>39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pumping installations or systems</td><td><b>41/00</b>, <b>45/00</b>, <b>47/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL, SAFETY MEASURES; TESTING</td><td><b>49/00</b>; <b>51/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMPONENT PARTS, DETAILS OR ACCESSORIES</td><td><b>53/00</b></td></p></tr></table>				
F04C		液体用回転ピストンまたは揺動ピストン容積形機械（液体により駆動される機関Ｆ０３Ｃ）；回転ピストンまたは揺動ピストン容積形ポンプ（機関燃料噴射ポンプＦ０２Ｍ）<br><br><b><ul>注</ul></b><br>“機械”，“ポンプ”，“容積形”，“回転ピストン機械”，“揺動ピストン機械”，“回転ピストン”，“共動部材”，“共動部材の運動”，“歯または歯に相当するもの”および“内部軸”の定義に関して特にクラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>液体用機械；液体用ポンプまたは液体および圧縮性流体用ポンプ　　<br>回転ピストン<br>一般特性；平行でない共動部材の動作軸　２／００；３／００<br>弾性変形しうる室の壁；流体リング　５／００；７／００<br>揺動ピストン　９／００<br>組み合わせまたは適用　１１／００，１３／００<br>ポンプ装置　１１／００<br>制御；監視；安全装置　１４／００<br>他の細部または付属品　１５／００<br>圧縮性流体に特に適合したポンプ<br>回転ピストンポンプ　１８／００<br>流体リングまたは類似したものを有する回転ピストンポンプ　１９／００<br>揺動ピストンポンプ　２１／００<br>２以上のポンプの組み合わせで，それぞれが回転ピストンまたは揺動ピストン形であるもの；ポンプ装置；多段ポンプ　２３／００<br>特殊用途へのポンプの適用　２５／００<br>回転ピストンポンプでのシール装置　２７／００<br>制御，監視，安全装置　２８／００<br>他の部品，細部または付属品　２９／００<br>	ROTARY-PISTON, OR OSCILLATING-PISTON, POSITIVE-DISPLACEMENT MACHINES FOR LIQUIDS (engines driven by liquids <b>F03C</b>); ROTARY-PISTON, OR OSCILLATING-PISTON, POSITIVE-DISPLACEMENT PUMPS (engine fuel-injection pumps <b>F02M</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definitions of &quot;machines&quot;, &quot;pumps&quot;, &quot;positive displacement&quot;, &quot;rotary-piston machines&quot;, &quot;oscillating-piston machines&quot;, &quot;rotary piston&quot;, &quot;co-operating members&quot;, &quot;movement of co-operating members&quot;, &quot;teeth or tooth-equivalents&quot;, and &quot;internal axis&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES FOR LIQUIDS; PUMPS FOR LIQUIDS OR FOR LIQUIDS AND ELASTIC FLUIDS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Rotary-piston</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">general characteristics; non-parallel axes of movement of co-operating members</td><td><b>2/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">resiliently-deformable chamber walls; fluid ring</td><td><b>5/00</b>; <b>7/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Oscillating-piston</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations or adaptations</td><td><b>11/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pump installations</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Control; monitoring; safety arrangements</td><td><b>14/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other details or accessories</td><td><b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PUMPS SPECIALLY ADAPTED FOR ELASTIC FLUIDS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Rotary-piston pumps</td><td><b>18/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Rotary-piston pumps with fluid ring or the like</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Oscillating-piston pumps</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations of two or more pumps, each being of rotary-piston or oscillating-piston type; Pumping installations; Multi-stage pumps</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Adaptations of pumps for special use</td><td><b>25/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Sealing arrangements in rotary-piston pumps</td><td><b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Control; monitoring; safety arrangements</td><td><b>28/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other components parts, details or accessories</td><td><b>29/00</b></td></p></tr></p></tr></table>				
F04D		非容積形ポンプ（機関燃料噴射ポンプＦ０２Ｍ；イオンポンプＨ０１Ｊ４１／１２；電磁ポンプＨ０２Ｋ４４／０２）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは，回転形であろうと純粋な回転をもたないものであろうと，液体用，圧縮性流体用，または液体および圧縮性流体用の非容積形ポンプを包含する。<br>（２）このサブクラスは，非容積形ポンプと他の形式のポンプを組合せたものは包含せず，これらはサブクラスＦ０４Ｂに包含されるが，ただし非容積形ポンプの呼び水用または予圧用のように他の形式のポンプを用いるものは，このサブクラスに包含される。<br>（３）特に“ポンプ”という用語の定義に関して，クラスＦ０１の前の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>液体および圧縮流体または液体のみのための回転形ポンプ<br>流れの形：半径またはら旋遠心形；軸方向形；円周または横断形；その他　１／００；３／００；５／００；１１／００<br>特殊な流体を扱うためのもの　７／００<br>呼び水作用するもの，蒸気閉塞を防止するもの　９／００<br>ポンプ装置または系；制御　１３／００；１５／００<br>圧縮性流体のための回転形ポンプ<br>流れの形：半径またはら旋遠心形；軸方向形；その他　１７／００；１９／００；２３／００<br>超音速流体を含むもの　２１／００<br>ポンプ装置；制御　２５／００；２７／００<br>細部または付属品　２９／００<br>その他の種類のポンプ<br>同時に液体および圧縮性流体をポンプするもの　３１／００<br>他の純粋な回転形以外のものをもつもの　３３／００<br>波を発生するもの　３５／００<br>	NON-POSITIVE-DISPLACEMENT PUMPS (engine fuel-injection pumps <b>F02M</b>; ion pumps <b>H01J 41/12</b>; electrodynamic pumps <b>H02K 44/02</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> non-positive-displacement pumps for liquids, for elastic fluids, or for liquids and elastic fluids whether rotary or not having pure rotation.</li><li>This subclass <u>does not cover</u> combinations of non-positive-displacement pumps with other pumps, which are covered by subclass <b>F04B</b>, except that the use of such other pumps for priming or boosting non-positive-displacement is covered by this subclass.</li><li>Attention is drawn to the Notes preceding class <b>F01</b>, especially as regards the definition of &quot;pump&quot;.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROTARY PUMPS FOR LIQUID AND ELASTIC FLUID OR LIQUID ALONE</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Kind of flow: radial or helico-centrifugal; axial; circumferential or transverse; other</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For handling specific fluids</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Priming, preventing vapour lock</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pumping installations or systems; control</td><td><b>13/00</b>; <b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROTARY PUMPS FOR ELASTIC FLUID</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Kind of flow: radial or helico-centrifugal; axial; other</td><td><b>17/00</b>; <b>19/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Involving supersonic speed of fluid</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pumping installations; control</td><td><b>25/00</b>; <b>27/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS OR ACCESSORIES</td><td><b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER KINDS OF PUMPS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pumping liquid and elastic fluid at the same time</td><td><b>31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With other than pure rotation</td><td><b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Wave producers</td><td><b>35/00</b></td></p></tr></p></tr></table>				
F04F		他の流体との直接の接触により，またはポンプされる流体の慣性力を利用することによって流体をポンプするもの（内部のガス圧により液体または半液体の内容物を分配するための特殊な手段を有する容器または包装Ｂ６５Ｄ８３／１４）；サイホン［２］<br><br><b><ul>注</ul></b><br>（１）クラスＦ０１の前の注に注意すること。<br>（２）このクラスに包含されるポンプとその他のポンプとを組み合わせたものは，もしそのような他のポンプが拡散ポンプの粗（あら）引きポンプであるならば，このサブクラスにのみ分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>他の流体の流れ又は圧力を使うポンプ　１／００，５／００<br>負圧力を使うポンプ；流体の慣性力を使うポンプ　１／００，３／００；７／００<br>拡散ポンプ，例．粗引きポンプを有するもの　９／００<br>サイホン；その他のポンプ　１０／００；９９／００<br>圧力交換器　１３／００<br>ジェットポンプ装置　５／５４<br>	PUMPING OF FLUID BY DIRECT CONTACT OF ANOTHER FLUID OR BY USING INERTIA OF FLUID TO BE PUMPED (containers or packages with special means for dispensing liquid or semi-liquid contents by internal gaseous pressure <b>B65D 83/14</b>); SIPHONS<b>[2]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes preceding class <b>F01</b>.</li><li>Combinations of pumps covered by this subclass with other pumps are only classified in this subclass if such other pumps are intended for preliminary pumping for diffusion pumps.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PUMPS USING PRESSURE OR FLOW OF ANOTHER FLUID</td><td><b>1/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PUMPS USING NEGATIVE PRESSURE; PUMPS USING INERTIA OF THE FLUID</td><td><b>1/00</b>, <b>3/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DIFFUSION PUMPS, E.G. WITH FORE PUMPS</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SIPHONS; OTHER PUMPS</td><td><b>10/00</b>; <b>99/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PRESSURE EXCHANGERS</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">JET-PUMP INSTALLATIONS</td><td><b>5/54</b></td></p></tr></table>				
F15		流体圧アクチュエータ；水力学または空気力学一般<br>	FLUID-PRESSURE ACTUATORS; HYDRAULICS OR PNEUMATICS IN GENERAL				
F15B		流体手段によって作動する系一般；流体圧アクチュエータ，例．サーボモータ；他に分類されない流体圧系の細部<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“テレモータ”は，入力部材と出力部材の間に実質的に一定量の流体が封じこまれており，流体的なリンクとして作用する系または装置を意味する；<br>―“サーボモータ”は流体圧アクチュエータを意味する，例．イニシャル制御部材の操作に応答する弁または他の機器によって直接制御されるピストン・シリンダ；“サーボモータ”はテレモータを含まない。イニシャル制御部材はサーボモータに近接していてもよいし，離れていてもよく，たとえばハンドレバーであってもよい。<br><br><b><ul>サブクラス内の索引</ul></b><br>圧力流体の供給　１／００<br>増圧器または流体圧転換器；変換器　３／００；５／００<br>流体圧アクチュエータ系<br>テレモータまたはポンプの出力に関連する系　７／００<br>サーボモーター　９／００，１１／００，１３／００<br>部材を移すための機器　１５／００<br>テレモータとサーボモータの組み合わせ；その他の系；細部　１７／００；１８／００；２１／００<br>試験；安全　１９／００；２０／００<br>	SYSTEMS ACTING BY MEANS OF FLUIDS IN GENERAL; FLUID-PRESSURE ACTUATORS, e.g. SERVOMOTORS; DETAILS OF FLUID-PRESSURE SYSTEMS, NOT OTHERWISE PROVIDED FOR<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following terms are used with the meanings indicated:<ul type=""disc""><li>&quot;telemotor&quot; means a system or device in which a substantially constant amount of fluid is trapped between an input member and an output member to act as a fluid link;</li><li>&quot;servomotor&quot; means a fluid-pressure actuator, e.g. a piston and cylinder, directly controlled by a valve or other device which is responsive to operation of an initial controlling member; &quot;Servomotor&quot; does not cover a telemotor. The initial controlling member may be adjacent to the servomotor or at a distance, and may be, for example, a hand lever.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPLYING FLUID UNDER PRESSURE</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">INTENSIFIERS OR FLUID-PRESSURE CONVERTERS; TRANSDUCERS</td><td><b>3/00</b>; <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLUID-PRESSURE ACTUATOR SYSTEMS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Telemotors or systems related to the output of a pump</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Servomotors</td><td><b>9/00</b>, <b>11/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Devices for displacing a member</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations of telemotors and servomotors; other systems; details</td><td><b>17/00</b>; <b>18/00</b>; <b>21/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TESTING; SAFETY</td><td><b>19/00</b>; <b>20/00</b></td></p></tr></table>				
F15C		主として計算または制御目的に用いられる流体回路素子（トランスデューサＦ１５Ｂ５／００；流体力学一般Ｆ１５Ｄ；流体素子から成る計算機Ｇ０６Ｄ，Ｇ０６Ｇ）<br><br><b><ul>注</ul></b><br>“マイクロ構造装置”と“マイクロ構造システム”に関するクラスＢ８１とサブクラスＢ８１Ｂのタイトルの後の注に注意すること。［７］<br>	FLUID-CIRCUIT ELEMENTS PREDOMINANTLY USED FOR COMPUTING OR CONTROL PURPOSES (transducers <b>F15B 5/00</b>; fluid dynamics in general <b>F15D</b>; computers comprising fluid elements <b>G06D</b>, <b>G06G</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to &quot;microstructural devices&quot; and &quot;microstructural systems&quot;.<b>[7]</b></li></ul>				
F15D		流体力学，すなわち気体または液体の流れに影響を与える方法または手段<br><br><b><ul>注</ul></b><br>このサブクラスは束縛面に関連しておよびこれらの面を通過した後において流体の流れに影響を与えるための，他類に属しない境界層制御および他の装置，方法，例．乱流の発生または除去，噴流の偏向，管内のベンドにおける流れの案内，管内の流体の分布への作用，流体摩擦の減少を包含する。<br>	FLUID DYNAMICS, i.e. METHODS OR MEANS FOR INFLUENCING THE FLOW OF GASES OR LIQUIDS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> boundary-layer control and other arrangements and methods, not provided for in other classes, for influencing the flow of fluids relative to constraining surfaces and after leaving these surfaces, e.g. producing or removing turbulence, deflecting jets, guiding flow through bends in conduits, affecting distribution of fluid in a conduit, reducing fluid friction.</li></ul>				
F16		機械要素または単位；機械または装置の効果的機能を生じ維持するための一般的手段<br>	ENGINEERING ELEMENTS OR UNITS; GENERAL MEASURES FOR PRODUCING AND MAINTAINING EFFECTIVE FUNCTIONING OF MACHINES OR INSTALLATIONS; THERMAL INSULATION IN GENERAL				
F16B		構造部材または機械部品同志の締め付けまたは固定のための装置，例．くぎ，ボルト，サークリップ，クランプ，クリップまたはくさび；継ぎ手または接続（回転の伝達用継手Ｆ１６Ｄ）<br><br><b><ul>注</ul></b><br>（ａ）グループＥ０４Ｂ１／３８の次の注に注意すること。［５］<br>（ｂ）次の箇所に注意すること。<br>Ａ４４Ｂ　　バックル，スライドファスナー<br>Ａ４７Ｇ　　３／００　釘，ねじまたは類似のものの装飾した頭部<br>Ｂ４２Ｆ　　３／００　共に一時的に取付けられたシートのためのステープル以外の手段<br>Ｅ０１Ｂ　　９／１０　レールのまくら木用ねじくぎまたはボルト<br>Ｅ０１Ｂ　１１／００　レール継ぎ目<br>Ｅ０４　　建築構造物の接合<br>Ｅ０４Ｄ　１３／０８　屋根ふきに堅樋をとりつける締め付け手段<br>Ｅ０４Ｆ　１３／２１　建造物のための被覆またはライニング部材に特に適した締め付け手段［８］<br>Ｅ０４Ｇ　　５／０４　建造物に対する足場の固定<br>Ｅ０４Ｇ　　７／００　足場用継ぎ手<br>Ｅ０５Ｃ　　ウィング特にドアまたは窓用のボルトまたは固定装置<br>Ｆ１６Ｃ　２９／１０　直線運動だけする部品用の軸受のゆるみ止め<br>Ｆ１６Ｇ　１７／００　チェーンに必須の部品としてのフック<br>Ｆ１６Ｌ　　管継ぎ手<br>Ｆ１６Ｌ　　３／００　パイプ，ケーブルまたは保護管用支持具，例．ハンガ，支持体，クランプ，くさび形留め具，クリップ，ブラケット<br>Ｆ１６Ｌ　３３／０２　ホースを固定部材に接続するためのクリップ<br>Ｈ０１Ｆ　　７／００　磁力による保持装置<br>Ｈ０２Ｎ　１３／００　静電気による保持装置［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>締め付けの型<br>クランプ；くさびによるもの　２／００；３／００<br>収縮によるものまたは圧力ばめ；相互にはり付けまたは圧縮することによるもの；一部材を他の部材の穴にそう入するもの　４／００；１１／００；１７／００<br>板，条片，棒，または管を一緒にまたは平らな面に締めつけるもの　５／００，７／００，９／００<br>特殊な応用のためのもの<br>家具のためのもの　１２／００<br>壁に固定させるためのもの　１３／００<br>引張荷重を考慮して修正したねじ山によるもの　３１／００<br>締め付け手段<br>一般<br>クランプ，クリップ；くさび，キー　２／００；３／００<br>ジベル　１３／００<br>他の締め付け手段　１／００，４５／００，４７／００<br>ねじ山を使用しないもの<br>くぎ，かすがい；ボルト，ピンまたはリベット　１５／００；１９／００<br>軸方向の動きに対する植込みボルトとソケット締め付けによるゆるみ止め　２１／００<br>ねじ山を使用するもの<br>ねじ山；ボルト，安全ボルト，ナット　２５／００，１５／０６，２７／００；２７／００，３１／００，３５／００，３７／００<br>ボルトおよびねじの形状一般　２３／００，２７／００，３３／００<br>締め付ける間にナットまたはそれに類するものの変形をもつねじ結合；ねじ，ボルトまたはナットのゆるみ止め　２９／００；３９／００<br>締め付け手段の付属品　４１／００，４３／００<br>	DEVICES FOR FASTENING OR SECURING CONSTRUCTIONAL ELEMENTS OR MACHINE PARTS TOGETHER, e.g. NAILS, BOLTS, CIRCLIPS, CLAMPS, CLIPS OR WEDGES; JOINTS OR JOINTING (couplings for transmitting rotation <b>F16D</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to:<b>[5,8]</b><ul type=""a""><li>the Note following group <b>E04B 1/38</b>;</li><li>the following places:<table width="100%"><tr><td></td><td><b>A44B</b></td><td>Buckles, slide fasteners</td></tr><tr><td></td><td><b>A47G 3/00</b></td><td>Ornamental heads for nails, screws, or the like</td></tr><tr><td></td><td><b>B42F 3/00</b></td><td>Means, not using staples, for attaching sheets temporarily together</td></tr><tr><td></td><td><b>E01B 9/10</b></td><td>Screws or bolts for railway sleepers</td></tr><tr><td></td><td><b>E01B 11/00</b></td><td>Rail joints</td></tr><tr><td></td><td><b>E04</b></td><td>Connections for building</td></tr><tr><td></td><td><b>E04D 13/08</b></td><td>Clamping means for down pipes for roof drainage</td></tr><tr><td></td><td><b>E04F 13/21</b></td><td>Fastening means specially adapted for covering or lining elements for buildings</td></tr><tr><td></td><td><b>E04G 5/04</b></td><td>Fastening scaffolds against buildings</td></tr><tr><td></td><td><b>E04G 7/00</b></td><td>Scaffolding couplings</td></tr><tr><td></td><td><b>E05C</b></td><td>Bolts or fasteners for wings, specially for doors or windows</td></tr><tr><td></td><td><b>F16C 29/10</b></td><td>Locking bearings for parts moving only linearly</td></tr><tr><td></td><td><b>F16G 17/00</b></td><td>Hooks as integral parts of chains</td></tr><tr><td></td><td><b>F16L</b></td><td>Pipe joints</td></tr><tr><td></td><td><b>F16L 3/00</b></td><td>Supports for pipes, cables or protective tubing, e.g. hangers, holders, clamps, cleats, clips, brackets</td></tr><tr><td></td><td><b>F16L 33/02</b></td><td>Clips for connecting hoses to rigid members</td></tr><tr><td></td><td><b>H01F 7/00</b></td><td>Magnetic holding devices</td></tr><tr><td></td><td><b>H02N 13/00</b></td><td>Electrostatic holding devices.</td></tr></table></li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TYPES OF FASTENING</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By: clamping, wedging</td><td><b>2/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By: shrinking or force fit; sticking or pressing together; penetration of one member into a hole in another</td><td><b>4/00</b>; <b>11/00</b>; <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fastening of plates, strips, bars, or tubes together or to flat surfaces</td><td><b>5/00</b>, <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For specific applications</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for furniture</td><td><b>12/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for fixing in walls</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">by screw-thread modified in view of tensile load</td><td><b>31/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FASTENING MEANS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">clamps; clips; wedges, keys</td><td><b>2/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">dowels</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other fastening means</td><td><b>1/00</b>, <b>45/00</b>, <b>47/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Without screw-thread</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">nails, staples; bolts, pins, or rivets</td><td><b>15/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">locking stud-and-socket fastenings against axial movement</td><td><b>21/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With screw-thread</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">screws; bolts, break-bolts, nuts</td><td><b>25/00</b>, <b>15/06</b>, <b>27/00</b>; <b>27/00</b>, <b>31/00</b>, <b>35/00</b>, <b>37/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">features common to bolts and screws</td><td><b>23/00</b>, <b>27/00</b>, <b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">deformation of nut or equivalent while fastening; locking of screws, bolts, or nuts</td><td><b>29/00</b>; <b>39/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Accessories for fastening means</td><td><b>41/00</b>, <b>43/00</b></td></p></tr></p></tr></table>				
F16C		軸；たわみ軸；たわみ被覆の中で運動を伝達するための機械的な手段；クランク軸機構の要素；ピボット；枢着；伝動装置，継ぎ手，クラッチまたはブレーキ要素以外の回転工学の要素；軸受［５］<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―”伝動装置，継ぎ手，クラッチまたはブレーキの要素以外の回転機械要素”は，それが回転するという事実によってのみ機能・機構が影響される場合に限った回転するあらゆる機械要素であって，伝動装置，継ぎ手，クラッチまたはブレーキの要素以外のものを包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>たわみ伝動，軸，車軸，クランク，偏心軸　１／００，３／００<br>クロスヘッド，連接棒　５／００，７／００，９／００<br>ピボット　１１／００<br>ロール，ドラム，円板　１３／００<br>軸受<br>回転部品用　１３／００，１７／００〜２７／００<br>直線運動をする部品用　２９／００<br>回転運動および直線運動をする部品用　３１／００<br>クランク軸または連接棒用　９／００<br>他に分類されないもの　３２／００<br>支持；部品または付属品　２７／００，３３／００，３５／００；４１／００<br>冷却；荷重軽減　３７／００；３９／００<br>製造，組立　３３／００，４３／００<br>遠心力に対抗する回転体の構造　１５／００<br>	SHAFTS; FLEXIBLE SHAFTS; MECHANICAL MEANS FOR TRANSMITTING MOVEMENT IN A FLEXIBLE SHEATHING; ELEMENTS OF CRANKSHAFT MECHANISMS; PIVOTS; PIVOTAL CONNECTIONS; ROTARY ENGINEERING ELEMENTS OTHER THAN GEARING, COUPLING, CLUTCH OR BRAKE ELEMENTS; BEARINGS<b>[5]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following expression is used with the meaning indicated:<ul type=""disc""><li>&quot;rotary engineering elements other than gearing, coupling, clutch or brake elements&quot; covers any engineering element other than gearing, coupling, clutch or brake elements which rotates in so far as its features are affected only by the fact that it rotates.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLEXIBLE TRANSMISSIONS, SHAFTS, AXLES, CRANKS, ECCENTRICS</td><td><b>1/00</b>, <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CROSSHEADS, CONNECTING-RODS</td><td><b>5/00</b>, <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PIVOTS</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROLLS, DRUMS, DISCS</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BEARINGS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For rotatable parts</td><td><b>13/00</b>, <b>17/00-27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For linearly-movable parts</td><td><b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For parts which both rotate and move linearly</td><td><b>31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For crankshafts or connecting- rods</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Not otherwise provided for</td><td><b>32/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Supports; parts or accessories</td><td><b>27/00</b>, <b>35/00</b>; <b>33/00</b>, <b>41/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Cooling; relieving load</td><td><b>37/00</b>; <b>39/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MAKING, ASSEMBLING</td><td><b>33/00</b>, <b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONSTRUCTION OF ROTATABLE BODIES TO RESIST CENTRIFUGAL FORCE</td><td><b>15/00</b></td></p></tr></table>				
F16D		回転伝達用継ぎ手（回転運動を伝達する伝動装置Ｆ１６Ｈ，例．流体伝動装置Ｆ１６Ｈ３９／００〜Ｆ１６Ｈ４７／００）；クラッチ（電動クラッチＨ０２Ｋ４９／００；静電気の吸引力を利用したクラッチＨ０２Ｎ１３／００）；ブレーキ（車両用電気的制動方式一般Ｂ６０Ｌ７／００；電動のブレーキＨ０２Ｋ４９／００）［２］<br><br><b><ul>サブクラス内の索引</ul></b><br>継ぎ手<br>一般　１／００<br>たわみ；衝撃；すべり継ぎ手　３／００；５／００；７／００<br>安全部材をもつもの　９／００<br>動力伝達手段として流体を用いるもの　３１／００，３３／００，３９／００<br>クラッチ<br>機械的に作動されるもの<br>部材が直接接触しているもの　１１／００，１３／００，１７／００<br>分離した部材をもつもの　１５／００<br>その他のもの；組み合わせたもの　１９／００；２１／００<br>細部　２３／００<br>非機械的に作動されるもの<br>流体によるもの　２５／００，２９／００<br>磁気的に作動されるもの　２７／００，２９／００<br>電気的に作動されるもの　２８／００，２９／００<br>動力伝達手段として流体をもちいるもの　３１／００〜３７／００<br>フリーホイール，自動式のもの　４１／００，４３／００，４５／００<br>組み合わせたもの　４５／００，４７／００<br>クラッチの外部制御　４８／００<br>フリーホイールまたはフリーホイールクラッチ　４１／００，４５／００<br>ブレーキ<br>機能を特徴とするもの　４９／００〜５５／００<br>液体または気体の抵抗を用いるもの　５７／００<br>自動式のもの　５９／００<br>吸収エネルギーを利用する手段をもつもの　６１／００<br>その他のもの　６３／００<br>細部　６５／００，６９／００，７１／００<br>作動状態を監視するもの　６６／００<br>異なる機構を組み合わせたもの　４７／００，６７／００<br>	COUPLINGS FOR TRANSMITTING ROTATION (gearing for conveying rotation <b>F16H</b>, e.g. fluid gearing <b>F16H 39/00-F16H 47/00</b>); CLUTCHES (dynamo-electric clutches <b>H02K 49/00</b>; clutches using electrostatic attraction <b>H02N 13/00</b>); BRAKES (electrodynamic brake systems for vehicles in general <b>B60L 7/00</b>; dynamo-electric brakes <b>H02K 49/00</b>)<b>[2]</b><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COUPLINGS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">In general</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Yielding; impulse; slip</td><td><b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With safety members</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using a fluid as power-transmitting means</td><td><b>31/00</b>, <b>33/00</b>, <b>39/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CLUTCHES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Mechanically actuated</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">the members being in direct contact</td><td><b>11/00</b>, <b>13/00</b>, <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with separate members</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">others; combinations</td><td><b>19/00</b>; <b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">details</td><td><b>23/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Non-mechanically actuated</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">by fluid</td><td><b>25/00</b>, <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">magnetically actuated</td><td><b>27/00</b>, <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">electrically actuated</td><td><b>28/00</b>, <b>29/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using a fluid as power-transmitting means</td><td><b>31/00-37/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Freewheels, automatic</td><td><b>41/00</b>, <b>43/00</b>, <b>45/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations</td><td><b>45/00</b>, <b>47/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">External control of clutches</td><td><b>48/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FREEWHEELS OR FREEWHEEL CLUTCHES</td><td><b>41/00</b>, <b>45/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BRAKES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Characterised by their function</td><td><b>49/00-55/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using resistance of liquid or air</td><td><b>57/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Automatic</td><td><b>59/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With means for making available for use the energy absorbed</td><td><b>61/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Others</td><td><b>63/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details</td><td><b>65/00</b>, <b>69/00</b>, <b>71/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Monitoring working conditions</td><td><b>66/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OF DIFFERENT DEVICES</td><td><b>47/00</b>, <b>67/00</b></td></p></tr></table>				
F16F		ばね；緩衝装置；振動減衰手段<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―ばね，緩衝装置または振動減衰装置；<br>―もし特定の装置を包含するサブクラスに分類されなければその特定の装置への配置又はその為の適用［５］<br>（２）もし特定の装置，例えば以下の装置に関するサブクラスに分類されれば，このサブクラスには，特定装置におけるあるいはその為のばね，緩衝装置または振動減衰装置の配置または適用は包含しない。<br>Ａ４７Ｃ　２３／００〜２７／００　スプリングマットレス<br>Ａ６３Ｃ　　５／０７５　スキーの防振器<br>Ｂ６０Ｇ　　車両懸架装置<br>Ｂ６０Ｒ　１９／２４　車両へのバンパーの取付け<br>Ｂ６１Ｆ　　鉄道車両懸架装置<br>Ｂ６１Ｇ　１１／００　鉄道車両または市街車両の緩衝装置<br>Ｂ６２Ｄ　２１／１５　衝撃吸収手段を有する車台フレーム<br>Ｂ６２Ｊ　　１／０２　自転車用サドルの弾性的取付け<br>Ｂ６２Ｋ　２１／０８　ステアリングダンパ<br>Ｂ６３Ｈ　　１／１５　振動減衰装置を有する船舶用プロペラ<br>Ｂ６３Ｈ　２１／３０　船舶の推進設備の防振取付<br>Ｂ６４Ｃ　２５／５８　飛行機の降着装置のばねまたは緩衝装置<br>Ｂ６５Ｄ　８１／０２　緩衝手段をもつ容器，包装要素または包装体<br>Ｄ０６Ｆ　３７／２０　洗たく機の弾性的すえ付け<br>Ｄ０６Ｆ　４９／０６　家庭用遠心脱水機の弾性的すえ付け<br>Ｆ０３Ｇ　　１／００　ばね原動機<br>Ｆ２１Ｖ　１５／０４　照明装置の弾性的取り付け<br>Ｆ４１Ａ　２５／００　後座へ復座する砲架<br>Ｆ４１Ｂ　　５／２０　アーチェリーの弦のための振動減衰装置<br>Ｇ０１Ｄ　１１／００　測定に関する指示または記録<br>Ｇ０１Ｇ　２１／１０　重量測定装置の緩衝装置<br>Ｇ０４Ｂ　　時計，携帯時計<br>Ｇ１２Ｂ　　３／０８　器械の可動部の減衰<br>Ｇ２１Ｃ　　７／２０　原子炉の制御棒の衝撃吸収装置の配置［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>ばね<br>摩擦型；流体型；磁力型　１／００，３／００；５／００，９／００；６／００<br>振動減衰装置または緩衝装置<br>摩擦型；流体型　７／００，１１／００；９／００，１１／００<br>ばねと振動減衰装置または緩衝装置とを組み合わせた装置　１３／００<br>振動防止，釣合い　１５／００<br>	SPRINGS; SHOCK-ABSORBERS; MEANS FOR DAMPING VIBRATION<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<b>[5]</b><ul type=""disc""><li>springs, shock-absorbers or vibration-dampers;</li><li>their arrangement in, or adaptation for, particular apparatus, if not provided for in the subclasses covering said apparatus.</li></ul></li><li>This subclass <u>does not cover</u> the arrangement or adaptation of springs, shock-absorbers or vibration-dampers in, or for, particular apparatus, if provided for in the subclasses concerning the said apparatus, e.g.<table width="100%"><tr><td></td><td><b>A47C 23/00-A47C 27/00</b></td><td>Spring mattresses</td></tr><tr><td></td><td><b>A63C 5/075</b></td><td>Vibration dampers in skis</td></tr><tr><td></td><td><b>B60G</b></td><td>Vehicle suspensions</td></tr><tr><td></td><td><b>B60R 19/24</b></td><td>Mounting of bumpers on vehicles</td></tr><tr><td></td><td><b>B61F</b></td><td>Rail vehicle suspensions</td></tr><tr><td></td><td><b>B61G 11/00</b></td><td>Buffers for railway or tramway vehicles</td></tr><tr><td></td><td><b>B62D 21/15</b></td><td>Vehicle chassis frames having impact absorbing means</td></tr><tr><td></td><td><b>B62J 1/02</b></td><td>Resiliently mounted saddles on cycles</td></tr><tr><td></td><td><b>B62K 21/08</b></td><td>Steering dampers</td></tr><tr><td></td><td><b>B63H 1/15</b></td><td>Marine propellers having vibration-damping means</td></tr><tr><td></td><td><b>B63H 21/30</b></td><td>Anti-vibration mounting of marine propulsion plant in ships</td></tr><tr><td></td><td><b>B64C 25/58</b></td><td>Arrangement of shock-absorbers or springs in aeroplane alighting gear</td></tr><tr><td></td><td><b>B65D 81/02</b></td><td>Containers, packing elements or packages with shock-absorbing means</td></tr><tr><td></td><td><b>D06F 37/20</b></td><td>Resilient mountings in washing machines</td></tr><tr><td></td><td><b>D06F 49/06</b></td><td>Resilient mountings in domestic spin-dryers</td></tr><tr><td></td><td><b>F03G 1/00</b></td><td>Spring motors</td></tr><tr><td></td><td><b>F21V 15/04</b></td><td>Resilient mounting of lighting devices</td></tr><tr><td></td><td><b>F41A 25/00</b></td><td>Gun cradles to permit recoil</td></tr><tr><td></td><td><b>F41B 5/20</b></td><td>Vibration dampers for archery bows</td></tr><tr><td></td><td><b>G01D 11/00</b></td><td>Indicating or recording in connection with measuring</td></tr><tr><td></td><td><b>G01G 21/10</b></td><td>Weighing apparatus, e.g. arrangement of shock-absorbers in weighing apparatus</td></tr><tr><td></td><td><b>G04B</b></td><td>Clocks, watches</td></tr><tr><td></td><td><b>G12B 3/08</b></td><td>Damping of movements in instruments</td></tr><tr><td></td><td><b>G21C 7/20</b></td><td>Disposition of shock-absorbing devices for displacable control elements in nuclear reactors.</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPRINGS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Friction type; fluid type; magnetic type</td><td><b>1/00</b>, <b>3/00</b>; <b>5/00</b>, <b>9/00</b>; <b>6/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VIBRATION-DAMPERS OR SHOCK-ABSORBERS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Friction type; fluid type</td><td><b>7/00</b>, <b>11/00</b>; <b>9/00</b>, <b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">UNITS COMBINING SPRINGS AND VIBRATION-DAMPERS OR SHOCK-ABSORBERS</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPRESSION OF VIBRATION, BALANCING</td><td><b>15/00</b></td></p></tr></table>				
F16G		主として伝動用に使用されるベルト，ケーブルまたはロープ；チェーン；主としてそのために使用される付属品<br><br><b><ul>サブクラス内の索引</ul></b><br>ベルト；ベルト継ぎ手　１／００，５／００；３／００，７／００<br>ケーブルまたはロープ；その継ぎ手　９／００；１１／００<br>チェーン，チェーンフック　１３／００，１５／００，１７／００<br>	BELTS, CABLES, OR ROPES, PREDOMINANTLY USED FOR DRIVING PURPOSES; CHAINS; FITTINGS PREDOMINANTLY USED THEREFOR<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BELTS; BELT FASTENINGS</td><td><b>1/00</b>, <b>5/00</b>; <b>3/00</b>, <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CABLES OR ROPES; FASTENINGS THEREFOR</td><td><b>9/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CHAINS, CHAIN HOOKS</td><td><b>13/00</b>, <b>15/00</b>, <b>17/00</b></td></p></tr></table>				
F16H		伝動装置<br><br><b><ul>注</ul></b><br>（１）機械的伝動装置を含む組み合わせはグループ１／００から３５／００に分類されていない限りグループ３７／００から４７／００に分類する。［２００９．０１］<br>（２）このサブクラスにおいては，剛結合された部材は単一部材とみなす。<br>（３）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる；<br>―“歯車伝動装置”はウォーム伝動装置および歯または歯に相当するものを備えた少なくとも１つの車または扇形車を含む他の伝動装置を含み，チェーンや歯付きベルトによる伝動装置は摩擦伝動装置で取り扱うので除く；<br>―“運動の伝達”はエネルギを伝達することを含むとともに，入，出力運動が，たとえば速度，方向または大きさにおいて相違していようとも，同種であることを意味する；<br>―“回転”は回転が無限に続き得ることを意味する；<br>―“振動”は伝動装置の構造によって規制される範囲で，一回転以上をも含めて，軸のまわりを運動し，その運動は伝動装置の連続運転中，交互に前後することを意味する；<br>―“往復運動”は本質的に直線の運動を意味し，その運動は伝動装置の連続運転中，交互に前後することを意味する；<br>―“逆転する”または“逆転”は一方向の入力運動から生じる出力運動が２つの反対方向のどちらかに随意に切換え得ることを意味する；<br>―“中心歯車”はその軸が伝動装置の主軸あるすべての歯車を含む。<br>（４）次の箇所に注意すること。<br>Ａ０１Ｄ　６９／０６　収穫期または刈取機の伝動機構<br>Ａ６３Ｈ　３１／００　玩具の伝動装置<br>Ｂ２１Ｂ　３５／１２　金属圧延機の歯車伝動装置<br>Ｂ６０Ｋ　　車両用伝動装置の配置<br>Ｂ６１Ｃ　　９／００　機関車の伝動装置<br>Ｂ６２Ｄ　　３／００　自動車の操向伝動装置<br>Ｂ６２Ｍ　　車輪付車両の伝動装置<br>Ｂ６３Ｈ　２３／００　船舶推進の伝動装置<br>Ｂ６３Ｈ　２５／００　船舶の操向伝動装置<br>Ｆ０１〜Ｆ０４　　機械，機関，ポンプ<br>Ｆ１５Ｂ　１５／００　流体作動装置と組み合わせた伝動装置<br>Ｇ０１Ｄ　　５／０４　測定装置に関する指示または記録装置に用いられる伝動装置<br>Ｈ０３Ｊ　　１／００　同調共振回路の駆動装置の配置<br>Ｈ０４Ｌ　１３／０４　デジタル情報の伝動装置駆動機構［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>回転運動に限定されない伝動装置<br>機械的伝動装置<br>レバー，リンク，カムを用いるもの　２１／００〜２５／００<br>間欠駆動部材を用いるもの　２７／００〜３１／００<br>他の伝動装置；伝動装置の組み合わせ　１９／００，３３／００，３５／００，３７／００<br>細部　５１／００〜５７／００<br>流体伝動装置　４３／００<br>回転運動を伝動するための伝動装置<br>歯車伝動装置　１／００，３／００<br>無端可撓部材を用いるもの　７／００，９／００<br>他の摩擦伝動装置　１３／００，１５／００<br>流体伝動装置　３９／００，４１／００，４５／００<br>間欠伝動装置を用いるもの　２９／００<br>制御<br>変速用または逆転用回転運動伝動装置の制御　５９／００〜６３／００<br>伝動装置の組み合わせ；差動伝動装置；その他の伝動装置　４７／００，４８／００，４９／００<br>伝動装置の一般的な細部　５７／００<br>	GEARING<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Combinations including mechanical gearings are classified in groups <b>F16H 37/00</b>or <b>F16H 47/00</b>, unless they are provided for in groups <b>F16H 1/00-F16H 35/00</b>.<b>[5,2009.01]</b></li><li>In this subclass, sets of rigidly-connected members are regarded as single members.</li><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;toothed gearing&quot; includes worm gearing and other gearing involving at least one wheel or sector provided with teeth or the equivalent, <u>except</u> gearing with chains or toothed belts, which is treated as friction gearing;</li><li>&quot;conveying motion&quot; includes transmitting energy, and means that the applied and resultant motions are of the same kind, though they may differ in, e.g. speed, direction or extent;</li><li>&quot;rotary&quot; implies that the motion may continue indefinitely.</li><li>&quot;oscillating&quot; means moving about an axis to an extent which is limited by the construction of the gearing and which may exceed one revolution, the movement being alternately forwards and backwards during continued operation of the gearing;</li><li>&quot;reciprocating&quot; means moving substantially in a straight line, the movement being alternately forwards and backwards during continued operation of the gearing;</li><li>&quot;reversing&quot; or &quot;reversal&quot; means that an applied movement in one direction may produce a resultant movement in either of two opposed directions at will;</li><li>&quot;central gears&quot; includes any gears whose axis is the main axis of the gearing.</li></ul></li><li>Attention is drawn to the following places:<table width="100%"><tr><td></td><td><b>A01D 69/06</b></td><td>Gearings in harvesters or mowers</td></tr><tr><td></td><td><b>A63H 31/00</b></td><td>Gearing for toys</td></tr><tr><td></td><td><b>B21B 35/12</b></td><td>Toothed-wheel gearing for metal-rolling mills</td></tr><tr><td></td><td><b>B60K</b></td><td>Arrangement of transmissions in vehicles</td></tr><tr><td></td><td><b>B61C 9/00</b></td><td>Transmissions for railway locomotives</td></tr><tr><td></td><td><b>B62D 3/00</b></td><td>Vehicle steering gears</td></tr><tr><td></td><td><b>B62M</b></td><td>Transmissions for cycles</td></tr><tr><td></td><td><b>B63H 23/00</b></td><td>Transmissions for marine propulsion</td></tr><tr><td></td><td><b>B63H 25/00</b></td><td>Marine steering gears</td></tr><tr><td></td><td><b>F01-F04</b></td><td>Machines, engines, pumps</td></tr><tr><td></td><td><b>F15B 15/00</b></td><td>Gearings associated with fluid-actuated devices</td></tr><tr><td></td><td><b>G01D 5/04</b></td><td>Gearing used in indicating or recording apparatus in connection with measuring devices</td></tr><tr><td></td><td><b>H03J 1/00</b></td><td>Driving arrangements for tuning resonant circuits</td></tr><tr><td></td><td><b>H04L 13/04</b></td><td>Driving mechanisms for apparatus for transmission of coded digital information.</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GEARINGS NOT LIMITED TO ROTARY MOTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Mechanical gearings</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">using levers, links, or cams</td><td><b>21/00-25/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">using intermittently-driving members</td><td><b>27/00-31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other gearings; combinations of gearings</td><td><b>19/00</b>, <b>33/00</b>, <b>35/00</b>; <b>37/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">details</td><td><b>51/00-57/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fluid gearing</td><td><b>43/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GEARINGS FOR CONVEYING ROTARY MOTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Toothed gearings</td><td><b>1/00</b>, <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using endless flexible members</td><td><b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other friction gearing</td><td><b>13/00</b>, <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fluid gearing</td><td><b>39/00</b>, <b>41/00</b>, <b>45/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using intermittently-driving gearing</td><td><b>29/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">of change-speed- or reversing-gearings conveying rotary motion</td><td><b>59/00-63/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OF GEARINGS; DIFFERENTIAL GEARINGS; OTHER GEARINGS</td><td><b>47/00</b>; <b>48/00</b>; <b>49/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GENERAL DETAILS OF GEARINGS</td><td><b>57/00</b></td></p></tr></table>				
F16J		ピストン；シリンダ；圧力容器一般；密封装置<br><br><b><ul>注</ul></b><br>次の箇所に注意すること。<br>Ａ４７Ｊ　２７／０８　加圧調理器<br>Ｅ０４Ｂ　　１／６８　建築構造の接合シール<br>Ｅ０５Ｃ　　９／００　ウイングの複数箇所固着一般<br>Ｆ０１Ｂ　　容積形機械または機関，例．蒸気機関に特有のシリンダＦ０１Ｂ３１／２８<br>Ｆ０２Ｆ　　１／００　燃焼機関のシリンダ<br>Ｆ０２Ｆ　　３／００　燃焼機関のピストン<br>Ｆ０４Ｄ　２９／０８　非容積形ポンプのシール<br>Ｆ１７Ｂ　　１／０４　可変容量ガスタンクの可動部分密封装置<br>Ｆ２８Ｆ　　９／０４　熱交換器の管寄せ箱または鏡板内への密封要素のための装置［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>ピストン，トランクピストンまたはプランジャ；ピストン棒　１／００；７／００<br>ダイヤフラム，ベローズ，ベローズピストン；ピストンリング　３／００；９／００<br>シリンダ，中空体　１０／００<br>圧力容器；ふた　１２／００；１３／００<br>密封装置　１５／００<br>	PISTONS; CYLINDERS; PRESSURE VESSELS IN GENERAL; SEALINGS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the following places:<table width="100%"><tr><td></td><td><b>A47J 27/08</b></td><td>Pressure cookers</td></tr><tr><td></td><td><b>E04B 1/68</b></td><td>Sealing building joints</td></tr><tr><td></td><td><b>E05C 9/00</b></td><td>Multi-point fastening of wings in general</td></tr><tr><td></td><td><b>F01B</b></td><td>Machines or engines in general or of reciprocating type, e.g. cylinders peculiar to steam engines <b>F01B 31/28</b></td></tr><tr><td></td><td><b>F02F 1/00</b></td><td>Cylinders for combustion engines</td></tr><tr><td></td><td><b>F02F 3/00</b></td><td>Pistons for combustion engines</td></tr><tr><td></td><td><b>F04D 29/08</b></td><td>Sealings of non-positive displacement pumps</td></tr><tr><td></td><td><b>F17B 1/04</b></td><td>Sealing devices for sliding parts of gas holders of variable capacity</td></tr><tr><td></td><td><b>F28F 9/04</b></td><td>Arrangements for sealing elements into header boxes or end plates of heat-exchangers.</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PISTONS, TRUNK PISTONS, OR PLUNGERS; PISTON-RODS</td><td><b>1/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DIAPHRAGMS, BELLOWS, BELLOWS PISTONS; PISTON-RINGS</td><td><b>3/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CYLINDERS, HOLLOW BODIES</td><td><b>10/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PRESSURE VESSELS; COVERS</td><td><b>12/00</b>; <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SEALINGS</td><td><b>15/00</b></td></p></tr></table>				
F16K		弁；栓；コック；作動のフロート；排気または吸気装置<br><br><b><ul>注</ul></b><br>（１）”マイクロ構造の装置”および”マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。［７］<br>（２）サブクラスＧ０５Ｄのタイトルの後の注（２）およびそのサブクラスの細展開に注意すること。そのサブクラスにおいては，圧力調節器および流量調節器，例．圧力補償器をもった流量調節弁は，その調節システムの全部が弁内に設けられているものでさえ，その動作に補助動力を持つものまたは持たないものは，それぞれグループＧ０５Ｄ１６／００またはＧ０５Ｄ７／００に包含される。しかし，弁部品の細部それ自体はＦ１６Ｋの適当なグループに分類される。）［２］<br>（３）次の箇所に注意すること：［５］<br>Ａ４７Ｊ　２７／０９　加圧調理器の安全装置<br>Ａ４７Ｊ　３１／４６　飲料製造装置の注出口，排出弁または類似のもの<br>Ａ６１Ｂ　　５／０２３５　特に心臓または血管の圧力測定に適用された弁<br>Ａ６１Ｆ　　２／２４　心臓弁<br>Ａ６１Ｍ　１６／２０　医療用呼吸装置に特に適した弁<br>Ａ６１Ｍ　３９／００　医療用に特に適する管接続具，管継ぎ手，弁または分岐ユニット<br>Ａ６２Ｂ　　９／０２　呼吸装置用弁<br>Ａ６２Ｂ　１８／１０　呼吸マスクまたはヘルメットの弁<br>Ａ６２Ｃ　　消防<br>Ｂ０５Ｂ　　噴霧用ノズル，スプレーヘッドまたは他の排出口<br>Ｂ６０Ｃ　２９／００　タイヤまたはホイールリムと関連するタイヤ膨張弁の配置；弁とホイールリム，タイヤ，他の膨張可能な弾性体との接続<br>Ｂ６０Ｇ　１７／０４８　車両用流体ばねの特性を調整するのに特に適用された弁<br>Ｂ６０Ｔ　　ブレーキ制御システムに用いられる弁<br>Ｂ６２Ｄ　　５／０８　用いられるバルブの型式により特徴づけられる車両の動力補助される操向<br>Ｂ６３Ｂ　　７／００，<br>Ｂ６３Ｃ　　９／００　水上浮揚の人命救助装置用膨脹弁<br>Ｂ６５Ｄ　４７／０４　排出弁をもった容器の閉蓋部材<br>Ｂ６５Ｄ　８３／２８，<br>　８３／４４　エアゾール容器に特に適用されるノズルまたは弁<br>Ｂ６５Ｄ　９０／３２　大形容器の安全弁<br>Ｂ６５Ｄ　９０／５４　大形容器のゲートまたは締切部材<br>Ｂ６７Ｃ　　３／２８　容器への液体充てん用流量制御弁<br>Ｂ６７Ｄ　　液体の分配，放出または移送<br>Ｅ０２Ｂ　　８／００　えん堤またはせきの細部，例．弁<br>Ｅ０２Ｂ　１３／０２　かんがい用導水管路の締切り<br>Ｅ０３Ｂ　　９／０２　給水栓の弁装置［８］<br>Ｅ０３Ｄ　　水洗便所または小便所の洗浄弁<br>Ｅ０５Ｆ　　３／１２　扉開閉器の弁装置<br>Ｅ２１Ｂ　２１／１０　掘さく流体の循環システムにおける弁装置<br>Ｅ２１Ｂ　３４／００　抗井または井戸のための弁装置<br>Ｆ０１Ｂ　２５／１０　容積形機械または機関を制御する作動流体用弁<br>Ｆ０１Ｄ　１７／１０　非容積形機械または機関を制御する最終アクチュエーター<br>Ｆ０１Ｌ　　周期的に作動する機械または機関用弁<br>Ｆ０２Ｄ　　９／０８　燃焼機関を制御する絞り弁<br>Ｆ０２Ｋ　　９／５８　ロケットエンジンの推進剤供給弁<br>Ｆ０２Ｍ　　気化器の燃料噴射<br>Ｆ０２Ｍ　５９／４６　燃料噴射ポンプの弁<br>Ｆ０４　　ポンプ<br>Ｆ１６Ｆ　　９／３４　緩衝装置の弁<br>Ｆ１６Ｌ　２９／００，<br>　３７／２８　流体遮断手段をもつ管継ぎ手または迅速作動形連結器<br>Ｆ１６Ｌ　５５／００　管の弁装置<br>Ｆ１６Ｌ　５５／０５５　水撃作用を防ぎまたは減少させるために特に適用した弁<br>Ｆ１６Ｌ　５５／４６　ピグまたはモール用推進装置<br>Ｆ１６Ｎ　２３／００　潤滑装置の逆止弁<br>Ｆ１７Ｃ　１３／０４　圧力容器の弁装置<br>Ｆ２２Ｂ　３７／４４　蒸気ボイラの安全弁装置<br>Ｆ２２Ｄ　　５／３４　ボイラの自動的給水に適用される弁<br>Ｆ２３Ｌ　１３／００　バーナーへの給気制御弁<br>Ｆ２３Ｑ　　２／１７３　炎が調節可能なガス状燃料ライターの弁<br>Ｆ２４Ｃ　　３／１２，<br>　　５／１６　ストーブまたはレンジの弁装置<br>Ｆ２４Ｆ　　空気調和；換気<br>Ｆ２５Ｂ　４１／０４　冷凍機械の流体循環用弁の配置<br>Ｇ０５Ｄ　　非電気的量の制御<br>Ｇ１０Ｂ　　３／０６　オルガンの弁<br>Ｇ１０Ｄ　　９／０４　他に分類されない気鳴楽器の弁［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>構造上の形<br>機械的に作動するもの　１／００〜７／００<br>多方弁　１１／００<br>締め切り装置のその他の構造上の形，締め切りのための装置　１３／００<br>機能上の形<br>逆止弁；安全弁または平衡弁；流体を混合するための装置　１１／００；１５／００；１７／００<br>流体送り出し弁；ノズルからの滴下を防止するための弁　２１／００；２３／００<br>密閉体の排気または吸気　２４／００<br>細部または一般的な手段<br>手動または制御　２９／００，３１／００，３９／００，４３／００<br>補助手段　４７／００，４９／００<br>安全　３５／００，３７／００<br>細部：弁部材と弁座間の接触，ハウジング，フロート，シール　２５／００，２７／００，３３／００，４１／００<br>その他の細部　５１／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	VALVES; TAPS; COCKS; ACTUATING-FLOATS; DEVICES FOR VENTING OR AERATING<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to &quot;microstructural devices&quot; and &quot;microstructural systems&quot;.<b>[2,5,7]</b></li><li>Attention is drawn to Note (2) following the title of subclass <b>G05D</b> and also the subdivisions of that subclass, according to which pressure regulators and flow regulators, e.g. flow regulating valves with pressure compensator, even with the whole regulating system contained in a valve, operating with or without auxiliary power, are covered by groups <b>G05D 16/00</b> or <b>G05D 7/00</b>, respectively. However, details of the valve parts, <u>per se</u>, are classified in the appropriate groups of this subclass.</li><li>Attention is drawn to the following places:<table width="100%"><tr><td></td><td><b>A47J 27/09</b></td><td>Safety devices for pressure cookers</td></tr><tr><td></td><td><b>A47J 31/46</b></td><td>Dispensing spouts, drain valves or like beverage-making apparatus</td></tr><tr><td></td><td><b>A61B 5/0235</b></td><td>Valves specially adapted for measuring pressure in heart or blood vessels</td></tr><tr><td></td><td><b>A61F 2/24</b></td><td>Heart valves</td></tr><tr><td></td><td><b>A61M 16/20</b></td><td>Valves specially adapted for medical respiratory devices</td></tr><tr><td></td><td><b>A61M 39/00</b></td><td>Tube connectors, tube couplings, valves or branch units specially adapted for medical use in general</td></tr><tr><td></td><td><b>A62B 9/02</b></td><td>Valves for respiratory apparatus</td></tr><tr><td></td><td><b>A62B 18/10</b></td><td>Valves for breathing masks or helmets</td></tr><tr><td></td><td><b>A62C</b></td><td>Fire extinguishers</td></tr><tr><td></td><td><b>B05B</b></td><td>Nozzles, spray heads or other discharge apparatus for spraying or atomising</td></tr><tr><td></td><td><b>B60C 29/00</b></td><td>Arrangements of tyre-inflating valves relative to tyres or wheel rims; Connection of valves to wheel rims, tyres or other inflatable elastic bodies</td></tr><tr><td></td><td><b>B60G 17/048</b></td><td>Valves specially adapted for adjusting vehicle fluid-spring characteristics</td></tr><tr><td></td><td><b>B60T</b></td><td>Valves specially adapted for vehicle brake control systems</td></tr><tr><td></td><td><b>B62D 5/08</b></td><td>Vehicle power-assisted steering characterised by the type of valve used</td></tr><tr><td></td><td><b>B63B 7/00</b>, <b>B63C 9/00</b></td><td>Arrangement of inflating valves for floatable live-saving equipment</td></tr><tr><td></td><td><b>B65D 47/04</b></td><td>Container closures with discharging valves</td></tr><tr><td></td><td><b>B65D 83/28</b>, <b>B65D 83/44</b></td><td>Nozzles or valves specially adapted for aerosol containers</td></tr><tr><td></td><td><b>B65D 90/32</b></td><td>Safety valves for large containers</td></tr><tr><td></td><td><b>B65D 90/54</b></td><td>Gates or closures on large containers</td></tr><tr><td></td><td><b>B67C 3/28</b></td><td>Flow control devices for bottling liquids</td></tr><tr><td></td><td><b>B67D</b></td><td>Dispensing, delivering or transferring liquids</td></tr><tr><td></td><td><b>E02B 8/00</b></td><td>Details, e.g. valves, of barrages or weirs</td></tr><tr><td></td><td><b>E02B 13/02</b></td><td>Closures for irrigation conduits</td></tr><tr><td></td><td><b>E03B 9/02</b></td><td>Arrangement of valves in hydrants</td></tr><tr><td></td><td><b>E03D</b></td><td>Flushing valves for water-closets or urinals</td></tr><tr><td></td><td><b>E05F 3/12</b></td><td>Valve arrangement in door closers</td></tr><tr><td></td><td><b>E21B 21/10</b></td><td>Valve arrangements in drilling-fluid circulation systems</td></tr><tr><td></td><td><b>E21B 34/00</b></td><td>Valve arrangements for boreholes or wells</td></tr><tr><td></td><td><b>F01B 25/10</b></td><td>Working-fluid valves for controlling machines or engines in general or of positive-displacement type</td></tr><tr><td></td><td><b>F01D 17/10</b></td><td>Final actuators for controlling non-positive displacement machines or engines</td></tr><tr><td></td><td><b>F01L</b></td><td>Cyclically operated valves for machines or engines</td></tr><tr><td></td><td><b>F02D 9/08</b></td><td>Throttle valves for controlling combustion engines</td></tr><tr><td></td><td><b>F02K 9/58</b></td><td>Propellant feed valves for rocket-engines</td></tr><tr><td></td><td><b>F02M</b></td><td>Carburettors, fuel injection</td></tr><tr><td></td><td><b>F02M 59/46</b></td><td>Valves for fuel injection pumps</td></tr><tr><td></td><td><b>F04</b></td><td>Pumps</td></tr><tr><td></td><td><b>F16F 9/34</b></td><td>Valves for shock absorbers</td></tr><tr><td></td><td><b>F16L 29/00</b>, <b>F16L 37/28</b></td><td>Pipe joints or quick-acting couplings with fluid cut-off means</td></tr><tr><td></td><td><b>F16L 55/00</b></td><td>Arrangement of valves in pipes</td></tr><tr><td></td><td><b>F16L 55/055</b></td><td>Valves specially adapted to prevent or minimise the effect of water hammer</td></tr><tr><td></td><td><b>F16L 55/46</b></td><td>Launching devices for pigs or moles</td></tr><tr><td></td><td><b>F16N 23/00</b></td><td>Check valves for lubrication systems</td></tr><tr><td></td><td><b>F17C 13/04</b></td><td>Arrangement of valves in pressure vessels</td></tr><tr><td></td><td><b>F22B 37/44</b></td><td>Arrangement of safety valves on steam boilers</td></tr><tr><td></td><td><b>F22D 5/34</b></td><td>Application of valves to automatic water-feed in boiler</td></tr><tr><td></td><td><b>F23L 13/00</b></td><td>Valves for air supply control to burners</td></tr><tr><td></td><td><b>F23Q 2/173</b></td><td>Valves for lighters with gaseous fuel and adjustable flame</td></tr><tr><td></td><td><b>F24C 3/12</b>, <b>F24C 5/16</b></td><td>Arrangement of valves on stoves or ranges</td></tr><tr><td></td><td><b>F24F</b></td><td>Air conditioning; Ventilation</td></tr><tr><td></td><td><b>F25B 41/20</b></td><td>Disposition of fluid circulation valves in refrigeration machines</td></tr><tr><td></td><td><b>G05D</b></td><td>Controlling non-electric variables</td></tr><tr><td></td><td><b>G10B 3/06</b></td><td>Valves for organs</td></tr><tr><td></td><td><b>G10D 9/04</b></td><td>Valves for other wind-actuated musical instruments.</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONSTRUCTIONAL TYPES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Lift-valves, gate valves or sliding valves, taps, diaphragm cut-off apparatus</td><td><b>1/00-7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Multiple-way valves</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other constructional types of cut-off apparatus, arrangements for cutting off</td><td><b>13/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FUNCTIONAL TYPES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Check valves; safety or equalising valves; arrangements for mixing fluids</td><td><b>15/00</b>; <b>17/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fluid-delivery valves; valves for preventing drip from nozzles</td><td><b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For venting or aerating enclosures</td><td><b>24/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS OR GENERAL MEANS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Handling or control</td><td><b>29/00</b>, <b>31/00</b>, <b>39/00</b>, <b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Auxiliary means</td><td><b>47/00</b>, <b>49/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Safety</td><td><b>35/00</b>, <b>37/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details: contact between valve members and seats, housings, floats, sealings</td><td><b>25/00</b>, <b>27/00</b>, <b>33/00</b>, <b>41/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other details</td><td><b>51/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F16L		管；管の継ぎ手または取り付け具；管，ケーブルまたは保護管類の支持；熱絶縁手段一般<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“管”は流体，材料，または物体を輸送するために特に適用された，閉じた横断面を持つ導管を意味する。<br>―“ホース”は，上に定義された管において，本質的な特徴として可とう性をもつ管を意味する。［５］<br>（２）次の箇所に注意すること。<br>Ａ６１Ｍ　３９／００　特に医療用に適用された管継ぎ手または分岐単位<br>Ｂ０５Ｍ　　１／２０　穴をあけた管<br>Ｂ６３Ｂ　３５／０３　パイプ敷設船<br>Ｂ６４Ｄ　３９／０４　飛行中の燃料補給のためのホースの構造<br>Ｂ６７Ｄ　　７／３８　貯蔵槽から車両または携帯用容器への液体，例．燃料，の移送のための装置におけるホースの配置<br>Ｅ０１Ｄ　１９／１０　パイプまたはケーブルの橋への固定<br>Ｅ０３Ｂ　　配水設備<br>Ｅ０３Ｄ　１１／１７　水洗便所の便器を洗浄水管に連結する装置<br>Ｅ０３Ｄ　１１／１８　水洗便所のサイフォン<br>Ｅ０３Ｆ　　３／０４　特に下水に用いられる管または取り付け具<br>Ｅ０４Ｄ　１３／０８　屋根ふきの堅樋；そのための取り付け手段<br>Ｅ０４Ｆ　１７／００　建築物の垂直なダクト，水路，例．煙突<br>Ｅ２１Ｆ　　１／０４　坑道またはトンネルの風道；そのための接続具<br>Ｅ２１Ｆ　１７／０２　鉱山またはトンネルにおける管またはその類似物の懸垂装置<br>Ｆ０１Ｎ　　機械または機関のためのガス流消音器または排気装置<br>Ｆ１６Ｎ　２１／００　潤滑系の導管，継ぎ手<br>Ｆ１７Ｃ　　３／０２　液化または固化ガスを貯蔵する圧力のかかっていない容器，例．デュワーフラスコ，の断熱設備<br>Ｆ２２Ｂ　３７／１０　蒸気ボイラの水管<br>Ｆ２３Ｊ　１３／０４　煙突または煙道のための継手，連結部<br>Ｆ２４Ｈ　　９／１２　加熱器への循環パイプの結合<br>Ｆ２８Ｆ　　９／０４　熱交換器の管寄せ箱または鏡板内への密封要素の配置<br>Ｇ２１Ｃ　１５／２２　原子炉におけるヘッダまたは他の管と冷却管の結合構造<br>Ｈ０２Ｇ　　３／０４　電気ケーブルの保護チューブまたはコンジット<br>Ｈ０２Ｇ　　３／３０　壁，床，天井への電気ケーブルまたは電線の据え付け［７］<br>Ｈ０２Ｇ　　３／３６　壁，床，天井の内側への電気ケーブルまたは電線の据え付け［７］<br><br><b><ul>サブクラス内の索引</ul></b><br>管の敷設または埋設　１／００<br>支持　３／００，５／００，７／００<br>管　９／００，１１／００<br>管継ぎ手<br>構造上の種類<br>切り離しできないもの　１３／００<br>ねじ止め　１５／００<br>別々の継ぎ手をもつもの：押圧する部材；スリーブまたはソケット；フランジ継ぎ手　１９／００；２１／００；２３／００<br>ベンドまたはサイホン　４３／００<br>その他の継ぎ手　２５／００<br>機能上の種類<br>自己締め付け密閉をもつもの　１７／００<br>調節できるもの，または動きを許容するもの　２７／００<br>流体締め切り手段をもつもの　２９／００<br>迅速作動形のもの　３７／００<br>二重壁または多水路管用　３９／００<br>分岐管，壁に管を連結するもの　４１／００<br>ホース用の特殊なもの　３１／００，３３／００，３５／００<br>管用の特殊なもの：プラスチックのもの；脆性材料のもの　４７／００；４９／００<br>配管用装置<br>クリーニング　４５／００<br>補正装置　５１／００<br>加熱または冷却　５３／００<br>付属品　５５／００<br>保護：損傷；腐食または湯あかに対する保護；熱絶縁　５７／００；５８／００；５９／００<br>	PIPES; JOINTS OR FITTINGS FOR PIPES; SUPPORTS FOR PIPES, CABLES OR PROTECTIVE TUBING; MEANS FOR THERMAL INSULATION IN GENERAL<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following terms are used with the meanings indicated:<b>[5,7]</b><ul type=""disc""><li>&quot;pipe&quot; means a conduit of closed cross-section, which is specially adapted to convey fluids, materials or objects;</li><li>&quot;hose&quot; means a pipe, as defined above, which has flexibility as an essential characteristic.</li></ul></li><li>Attention is drawn to the following places:<table width="100%"><tr><td></td><td><b>A61M 39/00</b></td><td>Tube connectors, tube couplings or branch units, specially adapted for medical use</td></tr><tr><td></td><td><b>B05B 1/20</b></td><td>Perforated pipes</td></tr><tr><td></td><td><b>B63B 35/03</b></td><td>Pipe-laying vessels</td></tr><tr><td></td><td><b>B64D 39/04</b></td><td>Adaptation of hose constructions for refuelling aircraft during flight</td></tr><tr><td></td><td><b>B67D 7/38</b></td><td>Arrangements of hoses in apparatus for transferring liquids, e.g. fuel, from bulk to vehicles or portable containers</td></tr><tr><td></td><td><b>E01D 19/10</b></td><td>Fastening of pipes or cables to bridges</td></tr><tr><td></td><td><b>E03B</b></td><td>Water supply installations</td></tr><tr><td></td><td><b>E03D 11/17</b></td><td>Means for connecting water-closet bowls to the flushing pipe</td></tr><tr><td></td><td><b>E03D 11/18</b></td><td>Siphons for water-closets</td></tr><tr><td></td><td><b>E03F 3/04</b></td><td>Pipes or fittings specially adapted to sewers</td></tr><tr><td></td><td><b>E04D 13/08</b></td><td>Down pipes for roof drainage; Clamping means therefor</td></tr><tr><td></td><td><b>E04F 17/00</b></td><td>Vertical ducts, channels in buildings, e.g. chimneys</td></tr><tr><td></td><td><b>E21F 1/04</b></td><td>Air ducts for ventilation of mines or tunnels; Connections therefor</td></tr><tr><td></td><td><b>E21F 17/02</b></td><td>Suspension devices for tubes or the like in mines or tunnels</td></tr><tr><td></td><td><b>F01N</b></td><td>Gas flow silencers or exhaust apparatus for machines or engines</td></tr><tr><td></td><td><b>F16N 21/00</b></td><td>Conduits, junctions for lubrication systems</td></tr><tr><td></td><td><b>F17C 3/02</b></td><td>Thermal insulation of vessels not under pressure for storing liquified or solidified gases, e.g. Dewar flask</td></tr><tr><td></td><td><b>F22B 37/10</b></td><td>Water tubes of steam boilers</td></tr><tr><td></td><td><b>F23J 13/04</b></td><td>Joints, connections for chimneys or flues</td></tr><tr><td></td><td><b>F24H 9/12</b></td><td>Connecting circulation pipes to heaters</td></tr><tr><td></td><td><b>F28F 9/04</b></td><td>Arrangements for sealing elements into header boxes or end plates of heat-exchangers</td></tr><tr><td></td><td><b>G21C 15/22</b></td><td>Structural association of coolant tubes with headers or other pipes in nuclear reactors</td></tr><tr><td></td><td><b>H02G 3/04</b></td><td>Protective tubing or conduits for electric cables</td></tr><tr><td></td><td><b>H02G 3/30</b></td><td>Installations of electric cables or lines on walls, floors or ceilings</td></tr><tr><td></td><td><b>H02G 3/36</b></td><td>Installations of electric cables or lines in walls, floors or ceilings</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LAYING OR RECLAIMING PIPES</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPORTING</td><td><b>3/00</b>, <b>5/00</b>, <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PIPES</td><td><b>9/00</b>, <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PIPE JOINTS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Constructional kinds</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">non-disconnectable</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">screw-threaded</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with separate joints: pressing member; sleeve or socket; flanged joints</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">bends or siphons</td><td><b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">other joints</td><td><b>25/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Functional kinds</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with self-tightening sealings</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">adjustable or allowing movement</td><td><b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">with fluid cut-off means</td><td><b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">of quick-acting type</td><td><b>37/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for double-walled or multi-channel pipes</td><td><b>39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">branching pipes, joining pipes to walls</td><td><b>41/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">special for hoses</td><td><b>31/00</b>, <b>33/00</b>, <b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">special for pipes: of plastics; of brittle material</td><td><b>47/00</b>; <b>49/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PIPING UNITS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Cleaning features</td><td><b>45/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Compensation devices</td><td><b>51/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Heating or cooling</td><td><b>53/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Accessories</td><td><b>55/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PROTECTION: AGAINST DAMAGE; CORROSION OR INCRUSTATION; THERMAL INSULATION</td><td><b>57/00</b>; <b>58/00</b>; <b>59/00</b></td></p></tr></table>				
F16M		他の所に属するエンジン，機械または装置に特有でない，エンジン，機械または装置のフレーム，ケーシングまたはベッド；スタンド；支持体<br><br><b><ul>注</ul></b><br>次の箇所に注意すること。<br>Ｂ２１Ｂ　３１／０２　金属圧延スタンドのフレーム<br>Ｇ０１Ｄ　１１／３０　特に指示または記録装置に適用される支持［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>フレーム，ケーシングまたはベッド<br>移動できるもの　３／００<br>エンジン，機械または装置用　１／００，５／００<br>基礎；細部　９／００；７／００<br>スタンドまたは支持体　１１／００，１３／００<br>	FRAMES, CASINGS OR BEDS OF ENGINES, MACHINES OR APPARATUS, NOT SPECIFIC TO ENGINES, MACHINES OR APPARATUS PROVIDED FOR ELSEWHERE; STANDS; SUPPORTS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the following places:<table width="100%"><tr><td></td><td><b>B21B 31/02</b></td><td>Metal-rolling stand frames</td></tr><tr><td></td><td><b>G01D 11/30</b></td><td>Supports specially adapted for indicating or recording instruments.</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FRAMES, CASINGS, OR BEDS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Displaceable</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">For engines, machines, or apparatus</td><td><b>1/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Foundations; details</td><td><b>9/00</b>; <b>7/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STANDS OR SUPPORTS</td><td><b>11/00</b>, <b>13/00</b></td></p></tr></table>				
F16N		潤滑<br><br><b><ul>注</ul></b><br>次の，特定の装置の潤滑または特殊の方法での潤滑を包含する箇所に注意すること［８］<br>Ａ０１Ｄ　６９／１２　収穫機<br>Ｂ２１Ｂ　２５／０４　金属管圧延機のためのマンドレル［８］<br>Ｂ２１Ｂ　２７／０６　金属圧延機のためのロール［８］<br>Ｂ２１Ｄ　３７／１８　材料の除去なく金属を加工する機械のための工具［８］<br>Ｂ２１Ｊ　　３／００　鍛造またはプレス<br>Ｂ２２Ｄ　１１／０７　金属の連続鋳造のための鋳型［８］<br>Ｂ２３Ｃ　　５／２８　フライス［８］<br>Ｂ２３Ｄ　５９／０２，<br>　５９／０４　メタル・ソー［８］<br>Ｂ２３Ｑ　１１／１０，<br>　１１／１２　工作機械［８］<br>Ｂ２５Ｄ　１７／２６　携帯用動力衝撃工具<br>Ｂ２６Ｂ　１９／４０　散髪用バリカンまたは乾式ひげ剃り器［８］<br>Ｂ２７Ｂ　１３／１２　木材またはその類似物のための帯鋸歯［８］<br>Ｂ６０Ｒ　１７／００　車両<br>Ｂ６１Ｂ　１２／０８　鉄道のケーブル方式［８］<br>Ｂ６１Ｃ　１７／０８　機関車<br>Ｂ６１Ｆ　１７／００　鉄道車両の軸箱［８］<br>Ｂ６１Ｋ　　３／００　鉄道の軌条または車輪縁［８］<br>Ｂ６２Ｄ　５５／０９２　無限軌道帯<br>Ｂ６２Ｊ　３１／００　自転車［８］<br>Ｂ６５Ｇ　４５／０２　コンベヤ［８］<br>Ｂ６６Ｂ　　７／１２　エレベーターのロープ，ケーブルまたはガイド［８］<br>Ｄ０１Ｈ　　７／２０　糸または繊維を紡績またはねん糸するための機械のスピンドル［８］<br>Ｄ０４Ｂ　３５／２８　編み機<br>Ｄ０５Ｂ　７１／００　ミシン［８］<br>Ｄ０５Ｃ　１３／０４　刺しゅう機［８］<br>Ｅ０１Ｂ　　７／２６　鉄道の転てつ器［８］<br>Ｅ０５Ｂ　１７／０８　錠<br>Ｅ０５Ｄ　１１／０２　蝶番<br>Ｅ２１Ｂ　１０／２２　掘さく用ローラビット<br>Ｆ０１Ｃ　２１／０４　回転ピストン式または揺動ピストン式機械または機関［８］<br>Ｆ０１Ｄ　２５／１８　非容積形機械［８］<br>Ｆ０１Ｍ　　機械または機関一般［８］<br>Ｆ０２Ｃ　　７／０６　ガスタービン設備［８］<br>Ｆ０２Ｆ　　１／２０　燃焼機関のシリンダ［８］<br>Ｆ０４Ｂ　３９／０２　流体用ポンプ［８］<br>Ｆ０４Ｃ　２９／０２　回転ピストン式または揺動ピストン式流体用ポンプ［８］<br>Ｆ０４Ｄ　２９／０４　非容積形ポンプ［８］<br>Ｆ１６Ｃ　　１／２４　たわみ軸［８］<br>Ｆ１６Ｃ　３３／１０　すべり軸受［８］<br>Ｆ１６Ｃ　３３／６６　玉軸受またはころ軸受［８］<br>Ｆ１６Ｆ　　１／２４　スプリング［８］<br>Ｆ１６Ｈ　５７／０４　伝動装置［８］<br>Ｆ４１Ａ　２９／０４　小火器または砲［８］<br>Ｇ０４Ｂ　３１／０８　時計［８］<br>Ｈ０１Ｒ　３９／５６　回転形集電装置，配電器または断続器［８］<br><br><b><ul>サブクラス内の索引</ul></b><br>潤滑を確実にするための装置または機械の改良　１／００<br>潤滑装置<br>固定のもの；持ち運べるもの；手動のもの　７／００，１１／００；９／００；３／００，５／００<br>潤滑ポンプ　１３／００<br>細部：貯蔵器；導管類；逆止弁　１９／００；２１／００；２３／００<br>分配，比例，安全，制御，浄化のための設備　２３／００〜３３／００<br>潤滑剤の取り扱い，貯蔵　３３／００〜３９／００<br>特殊潤滑　１５／００，１７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	LUBRICATING<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the following places, which cover lubrication of specific apparatus or in particular processes:<b>[8]</b><table width="100%"><tr><td></td><td><b>A01D 69/12</b></td><td>Harvesters</td></tr><tr><td></td><td><b>B21B 25/04</b></td><td>Mandrels for metal tube rolling mills</td></tr><tr><td></td><td><b>B21B 27/06</b></td><td>Rolls for metal rolling mills</td></tr><tr><td></td><td><b>B21D 37/18</b></td><td>Tools for machines for working metal without removing material</td></tr><tr><td></td><td><b>B21J 3/00</b></td><td>Forging or pressing</td></tr><tr><td></td><td><b>B22D 11/07</b></td><td>Moulds for continuous casting of metals</td></tr><tr><td></td><td><b>B23C 5/28</b></td><td>Milling cutters</td></tr><tr><td></td><td><b>B23D 59/02</b>, <b>B23D 59/04</b></td><td>Metal saws</td></tr><tr><td></td><td><b>B23Q 11/10</b>, <b>B23Q 11/12</b></td><td>Machine tools</td></tr><tr><td></td><td><b>B25D 17/26</b></td><td>Portable power-driven percussive tools</td></tr><tr><td></td><td><b>B26B 19/40</b></td><td>Hair-clippers or dry-shavers</td></tr><tr><td></td><td><b>B27B 13/12</b></td><td>Band saw blades for wood or the like</td></tr><tr><td></td><td><b>B60R 17/00</b></td><td>Vehicles</td></tr><tr><td></td><td><b>B61B 12/08</b></td><td>Cable systems for railways</td></tr><tr><td></td><td><b>B61C 17/08</b></td><td>Railway locomotives</td></tr><tr><td></td><td><b>B61F 17/00</b></td><td>Axle-boxes of rail vehicles</td></tr><tr><td></td><td><b>B61K 3/00</b></td><td>Rail or wheel flanges of railways</td></tr><tr><td></td><td><b>B62D 55/092</b></td><td>Endless-track units for vehicles</td></tr><tr><td></td><td><b>B62J 31/00</b></td><td>Cycles</td></tr><tr><td></td><td><b>B65G 45/02</b></td><td>Conveyors</td></tr><tr><td></td><td><b>B66B 7/12</b></td><td>Ropes, cables or guides of elevators</td></tr><tr><td></td><td><b>D01H 7/20</b></td><td>Spindles of machines for spinning or twisting threads or fibres</td></tr><tr><td></td><td><b>D04B 35/28</b></td><td>Knitting machines</td></tr><tr><td></td><td><b>D05B 71/00</b></td><td>Sewing machines</td></tr><tr><td></td><td><b>D05C 13/04</b></td><td>Embroidering machines</td></tr><tr><td></td><td><b>E01B 7/26</b></td><td>Switches for railways</td></tr><tr><td></td><td><b>E05B 17/08</b></td><td>Locks</td></tr><tr><td></td><td><b>E05D 11/02</b></td><td>Hinges</td></tr><tr><td></td><td><b>E21B 10/22</b></td><td>Roller bits for earth drilling</td></tr><tr><td></td><td><b>F01C 21/04</b></td><td>Rotary-piston or oscillating-piston machines or engines</td></tr><tr><td></td><td><b>F01D 25/18</b></td><td>Non-positive-displacement machines</td></tr><tr><td></td><td><b>F01M</b></td><td>Machines or engines in general</td></tr><tr><td></td><td><b>F02C 7/06</b></td><td>Gas-turbine plants</td></tr><tr><td></td><td><b>F02F 1/20</b></td><td>Cylinders of combustion engines</td></tr><tr><td></td><td><b>F04B 39/02</b></td><td>Pumps for liquids</td></tr><tr><td></td><td><b>F04C 29/02</b></td><td>Rotary-piston or oscillating-piston pumps for liquids</td></tr><tr><td></td><td><b>F04D 29/04</b></td><td>Non-positive-displacement pumps</td></tr><tr><td></td><td><b>F16C 1/24</b></td><td>Flexible shafts</td></tr><tr><td></td><td><b>F16C 33/10</b></td><td>Sliding-contact bearings</td></tr><tr><td></td><td><b>F16C 33/66</b></td><td>Ball or roller bearings</td></tr><tr><td></td><td><b>F16F 1/24</b></td><td>Springs</td></tr><tr><td></td><td><b>F16H 57/04</b></td><td>Transmissions</td></tr><tr><td></td><td><b>F41A 29/04</b></td><td>Smallarms or ordnance</td></tr><tr><td></td><td><b>G04B 31/08</b></td><td>Clocks</td></tr><tr><td></td><td><b>H01R 39/56</b></td><td>Rotary current collectors, distributors or interrupters</td></tr></table></li></ul><br><br><b><u>Subclass indexes</u></b><br><table ><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MODIFICATIONS OF APPARATUS OR MACHINES TO ENSURE LUBRICATION</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LUBRICATION DEVICES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Stationary; mobile; manual</td><td><b>7/00</b>, <b>11/00</b>; <b>9/00</b>; <b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Lubricating-pumps</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details: reservoirs; conduits; check valves</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">EQUIPMENT FOR DISTRIBUTION, PROPORTIONING, SAFETY, CONTROL, CLEANING</td><td><b>23/00-33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">HANDLING OF LUBRICANTS, STORAGE</td><td><b>33/00-39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPECIAL LUBRICATION</td><td><b>15/00</b>, <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F16P		安全装置一般<br><br><b><ul>注</ul></b><br>下記の箇所に注意すること：<br>Ａ０１Ｄ　７５／１８，<br>　７５／２０　収穫機または刈取機［７］<br>Ａ０１Ｆ　２１／００　脱穀機または梱包用圧縮機<br>Ｂ０２Ｃ　２３／０４　破砕または粉砕機<br>Ｂ２１Ｂ　３３／００　金属の圧延<br>Ｂ２１Ｄ　５５／００　本質的には材料の除去が行われない金属板，金属管，金属棒または金属プロフィルの加工<br>Ｂ２３Ｂ　２５／０４　切削機械<br>Ｂ２３Ｑ　１１／００　工作機械<br>Ｂ２４Ｂ　５５／００　研削または研摩機械<br>Ｂ２５Ｄ　１７／１０　携帯用動力衝撃工具<br>Ｂ２５Ｊ　１９／０６　マニプレータ<br>Ｂ２６Ｄ　　７／２２　切断機械<br>Ｂ２７Ｇ　１９／００　木材鋸<br>Ｂ６５Ｂ　５７／００　包装機械または装置<br>Ｂ６５Ｇ　４３／００　コンベヤ<br>Ｂ６５Ｈ　２６／００　ウエブ送給機構<br>Ｂ６５Ｈ　６３／００　薄板状または線条材料の取扱いまたは巻取り<br>Ｄ０１Ｇ　３１／００　繊維の処理<br>Ｄ０１Ｈ　１３／１４　紡績またはねん糸<br>Ｄ０５Ｂ　８３／００　ミシン<br>Ｆ２１Ｖ　２５／００　照明装置<br>	SAFETY DEVICES IN GENERAL<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the following places:<b>[7]</b><table width="100%"><tr><td></td><td><b>A01D 75/18</b>, <b>A01D 75/20</b></td><td>Harvesters or mowers</td></tr><tr><td></td><td><b>A01F 21/00</b></td><td>Threshing machines or baling presses</td></tr><tr><td></td><td><b>B02C 23/04</b></td><td>Crushing or disintegrating machines</td></tr><tr><td></td><td><b>B21B 33/00</b></td><td>Rolling of metal</td></tr><tr><td></td><td><b>B21D 55/00</b></td><td>Working sheet metal or tubes, rods or profiles without essentially removing material</td></tr><tr><td></td><td><b>B23B 25/04</b></td><td>Turning-machines</td></tr><tr><td></td><td><b>B23Q 11/00</b></td><td>Machine tools</td></tr><tr><td></td><td><b>B24B 55/00</b></td><td>Grinding or polishing machines</td></tr><tr><td></td><td><b>B25D 17/10</b></td><td>Portable power-driven percussive tools</td></tr><tr><td></td><td><b>B25J 19/06</b></td><td>Manipulators</td></tr><tr><td></td><td><b>B26D 7/22</b></td><td>Cutting machines</td></tr><tr><td></td><td><b>B27G 19/00</b></td><td>Wood saws</td></tr><tr><td></td><td><b>B65B 57/00</b></td><td>Packaging machines or apparatus</td></tr><tr><td></td><td><b>B65G 43/00</b></td><td>Conveyors</td></tr><tr><td></td><td><b>B65H 26/00</b></td><td>Web-advancing mechanisms</td></tr><tr><td></td><td><b>B65H 63/00</b></td><td>Handling or winding of thin or filamentary material</td></tr><tr><td></td><td><b>D01G 31/00</b></td><td>Treatment of fibres</td></tr><tr><td></td><td><b>D01H 13/14</b></td><td>Spinning or twisting</td></tr><tr><td></td><td><b>D05B 83/00</b></td><td>Sewing machines</td></tr><tr><td></td><td><b>F21V 25/00</b></td><td>Lighting devices.</td></tr></table></li></ul>				
F16S		構造用要素一般；この要素より組み立てた構造物一般<br><br><b><ul>注</ul></b><br>このサブクラスは建築用に限定された同様の要素および構造物を包含しない。ただし，それらは，サブクラスＥ０４Ｃに包含される。<br>	CONSTRUCTIONAL ELEMENTS IN GENERAL; STRUCTURES BUILT-UP FROM SUCH ELEMENTS, IN GENERAL<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>does not cover</u> similar elements and structures, restricted to use in the building art, which are covered by subclass <b>E04C</b>.</li></ul>				
F16T		蒸気トラップまたは気体または蒸気を強制収容する密閉体から液体を排出する類似の装置<br>	STEAM TRAPS OR LIKE APPARATUS FOR DRAINING-OFF LIQUIDS FROM ENCLOSURES PREDOMINANTLY CONTAINING GASES OR VAPOURS				
F17		ガスまたは液体の貯蔵または分配<br>	STORING OR DISTRIBUTING GASES OR LIQUIDS				
F17B		容量可変のガスホルダ（自動ガス遮断装置Ａ４７Ｊ２７／６２，Ｇ０５Ｄ；火炎トラップＡ６２Ｃ４／００；ガス混合機Ｂ０１Ｆ，Ｆ１６Ｋ１１／００，Ｇ０５Ｄ１１／００；土木工学を用いた大量貯蔵容器の建造または組立てＥ０４Ｈ７／００；ガス圧縮機Ｆ０４；弁Ｆ１６Ｋ；弁または管の振動防止Ｆ１６Ｋ，Ｆ１６Ｌ；管Ｆ１６Ｌ；ガス主管の遮断装置Ｆ１６Ｌ５５／１０；圧縮，液化又は固化ガス所蔵用に適用された容器Ｆ１７Ｃ；ガス分配系Ｆ１７Ｄ１／０４；漏洩検知Ｆ１７Ｄ５／０２，Ｇ０１Ｍ；監視または警報装置Ｆ１７Ｄ５／０２，Ｇ０８Ｂ；パーナにおける燃焼の制御Ｆ２３Ｎ；ガスの量容または圧力調節装置Ｇ０５Ｄ）<br>	GAS-HOLDERS OF VARIABLE CAPACITY (self-acting gas cut-off devices <b>A47J 27/62</b>, <b>G05D</b>; flame traps <b>A62C 4/00</b>; gas mixers <b>B01F</b>, <b>F16K 11/00</b>, <b>G05D 11/00</b>; construction or assembling of bulk storage containers employing civil-engineering techniques <b>E04H 7/00</b>; gas compressors <b>F04</b>; valves <b>F16K</b>; damping pulsations in valves or pipes <b>F16K</b>, <b>F16L</b>; pipes <b>F16L</b>; stopping devices for gas mains <b>F16L 55/10</b>; vessels adapted for storing compressed, liquefied, or solidified gases <b>F17C</b>; gas distribution systems <b>F17D 1/04</b>; detecting leakage <b>F17D 5/02</b>, <b>G01M</b>; supervising or alarm devices <b>F17D 5/02</b>, <b>G08B</b>; control of combustion in burners <b>F23N</b>; gas flow or pressure regulators <b>G05D</b>)				
F17C		圧縮，液化または固化ガスの収容または貯蔵用容器；一定容量のガスホルダ；圧縮，液化または固化ガスの容器への充填，または容器からの放出（自然または人工的な地中の穴または室での流体貯蔵Ｂ６５Ｇ５／００；土木工学技術を用いた大型貯蔵容器の建設または組立てＥ０４Ｈ７／００；可変容量のガスホルダＦ１７Ｂ；液化または冷凍機械，プラントまたはシステムＦ２５）<br><br><b><ul>サブクラス内の索引</ul></b><br>圧力容器；圧力のかかっていない容器；細部　１／００；３／００；１３／００<br>充填；放出　５／００，６／００；７／００，９／００<br>ガス溶剤またはガス吸着剤を用いるもの　１１／００<br>	VESSELS FOR CONTAINING OR STORING COMPRESSED, LIQUEFIED, OR SOLIDIFIED GASES; FIXED-CAPACITY GAS-HOLDERS; FILLING VESSELS WITH, OR DISCHARGING FROM VESSELS, COMPRESSED, LIQUEFIED, OR SOLIDIFIED GASES (storing fluids in natural or artificial cavities or chambers in the earth <b>B65G 5/00</b>; construction or assembling of bulk storage containers employing civil-engineering techniques <b>E04H 7/00</b>; variable-capacity gas-holders <b>F17B</b>; liquefaction or refrigeration machines, plants, or systems <b>F25</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VESSELS UNDER PRESSURE; VESSELS NOT UNDER PRESSURE; DETAILS</td><td><b>1/00</b>; <b>3/00</b>; <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FILLING; DISCHARGING</td><td><b>5/00</b>, <b>6/00</b>; <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">USE OF GAS-SOLVENTS OR GAS-ABSORBENTS</td><td><b>11/00</b></td></p></tr></table>				
F17D		管路系；管路（水の分配Ｅ０３Ｂ；ポンプまたは圧縮機Ｆ０４；流体力学Ｆ１５Ｄ；弁または類似のものＦ１６Ｋ；管，管の敷設，支持具，継手，分岐管，修繕，管路全体に対する作業，付属品Ｆ１６Ｌ；蒸気トラップまたは類似のものＦ１６Ｔ；流体圧電気ケーブルＨ０１Ｂ９／０６）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“管路系”は協動する要素の配列のみならず，系統図に記載された系をも意味し，要素それ自体は関連したサブクラスに包含される。<br>	PIPE-LINE SYSTEMS; PIPE-LINES (distributing water <b>E03B</b>; pumps or compressors <b>F04</b>; fluid dynamics <b>F15D</b>; valves or the like <b>F16K</b>; pipes, laying pipes, supports, joints, branches, repairing, work on the entire line, accessories <b>F16L</b>; steam traps or the like <b>F16T</b>; fluid-pressure electric cables <b>H01B 9/06</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following expression is used with the meaning indicated:<ul type=""disc""><li>&quot;pipe-line systems&quot; means systems described in flow sheets as well as arrangements of co-operating elements, the elements <u>per se</u> being covered by the relevant subclasses.</li></ul></li></ul>				
F21		照明<br><br><b><ul>注</ul></b><br>セクションＨの注ＩＩＩ、特にクラスＦ２１に包含されるものと同じ技術主題の電気的な観点はサブクラスＨ０５Ｂに包含されることに、注意すること。<br>	LIGHTING				
F21H		白熱マントル；燃焼によって熱せられるその他の白熱体<br>	INCANDESCENT MANTLES; OTHER INCANDESCENT BODIES HEATED BY COMBUSTION				
F21K		ルミネセンスを用いる非電気的光源；電気化学発光を用いる光源；燃焼物質の点火を用いる光源；半導体装置を発光素子として用いる光源；他に分類されない光源<br><br><b><ul>注</ul></b><br>このサブクラスでは，サブクラスＦ２１ＷおよびＦ２１Ｙのインデキシングコードを付与することが望ましい。［２０１６．０１］<br>	NON-ELECTRIC LIGHT SOURCES USING LUMINESCENCE; LIGHT SOURCES USING ELECTROCHEMILUMINESCENCE; LIGHT SOURCES USING CHARGES OF COMBUSTIBLE MATERIAL; LIGHT SOURCES USING SEMICONDUCTOR DEVICES AS LIGHT-GENERATING ELEMENTS; LIGHT SOURCES NOT OTHERWISE PROVIDED FOR<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, it is desirable to add the indexing codes of subclasses <b>F21W</b> and <b>F21Y</b>.<b>[2016.01]</b></li></ul>				
F21L		携帯用または特に輸送に適した，照明装置またはそのためのシステム［１，７］<br><br><b><ul>注</ul></b><br>（１）このサブクラスには，必要な時に必要な場所を照らせるようにするため，たとえば手で運べるように，または車の付いた支持体に乗せてある場所から別の場所に運べるように，デザインされた，または適用された装置やシステムが分類される。［７］<br>（２）このサブクラスには，車両の照明のように固定して設置する装置やシステム，または基本的に常設の場所で使う装置やシステムは分類しない。これらはＦ２１Ｓに分類する。［７］<br>（３）非電気的照明装置は、非電気的な光源の使用に関連した特別な適応が重要な場合にのみグループＦ２１Ｌ１７／００〜Ｆ２１Ｌ２６／００に分類する。［２００９．０１］<br>（４）このサブクラスにおいては，サブクラスＦ２１ＷとＦ２１Ｙのインデキシングコードを付与することが望ましい。［７］<br><br><b><ul>サブクラス内の索引</ul></b><br>電気的装置<br>システム　２／００<br>バッテリーまたはセルを内蔵するもの　４／００<br>ジェネレータが組み込まれているもの　１３／００<br>電源を内蔵しないもの　１４／００<br>非電気的装置<br>トーチ，フレア；ランタン　１７／００；１９／００<br>ポケットランプ；鉱夫用手さげ灯　２１／００；２３／００<br>その他の携帯用照明装置またはそのシステム　２６／００<br>電気的および非電気的装置の組み合わせ　２７／００<br>	LIGHTING DEVICES OR SYSTEMS THEREOF, BEING PORTABLE OR SPECIALLY ADAPTED FOR TRANSPORTATION<b>[1,7]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> devices or systems designed or specially adapted to be carried, e.g. by hand, or otherwise transported from place to place, e.g. on wheeled supports, in order to provide illumination as and where required.<b>[7,2009.01]</b></li><li>This subclass <u>does not cover</u> devices or systems intended for fixed installation, e.g. vehicle lighting, or for use essentially at a permanent location, which are covered by subclass <b>F21S</b>.</li><li>Non-electric lighting devices are classified in groups <b>F21L 17/00-F21L 26/00</b> only if a special adaptation related to the use of a non-electric light source is of interest.</li><li>In this subclass, it is desirable to add the indexing codes of subclasses <b>F21W</b> and <b>F21Y</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ELECTRIC DEVICES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Systems</td><td><b>2/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">with self-contained batteries or cells</td><td><b>4/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">with built-in generators</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">without self-contained power source</td><td><b>14/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">NON-ELECTRIC DEVICES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Torches, flares; lanterns</td><td><b>17/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pocket-lamps; miners' hand-lamps</td><td><b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other portable lighting devices or systems thereof</td><td><b>26/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OF ELECTRIC AND NON-ELECTRIC DEVICES</td><td><b>27/00</b></td></p></tr></table>				
F21S		非携帯用の照明装置；そのシステム；車両外部に特に適合する車両照明［１，７］<br><br><b><ul>注</ul></b><br>１．このサブクラスは以下のものを包含する：<br>・固定して据え付けるため，または常設の場所で使うための装置またはシステム，例．自在に立てることを意図したフロア・スタンドまたは卓上スタンド<br>・車両外部に特に適合する車両照明装置の各要素の光学的，機械的，熱的または電気的配置に関連する観点，例．ヘッドランプ<br>・車両外部に特に適合する車両光信号装置の各要素の光学的，機械的，熱的または電気的配置に関連する観点，例．ブレーキランプまたは方向指示灯。<br><br>２．このサブクラスは以下のものを包含しない：<br>・輸送に特に適合する装置またはシステムであって，サブクラス２１Ｌに分類される；<br>・照明装置が配置される車両，例．車両の照明装置の配置または操作，に関連する観点であって，サブクラスＢ６０Ｑに分類される；<br>・全体としての車両に関連する車両照明装置の制御，例．水平化，回転または照準合わせ。そのような装置は，たとえ照明装置がランプ収容体内で動く場合でも，グループＢ６０Ｑ１／０６に分類される。<br><br>３．非電気照明装置またはシステムは，非電気光源の使用に関連する特殊な適合が重要である場合のみ，グループＦ２１Ｓ１１／００〜Ｆ２１Ｓ１５／００に分類される。<br><br>４．このサブクラスでは，サブクラスＦ２１ＷおよびＦ２１Ｙのインデキシングコードを追加することが望ましい。［７］<br><br><b><ul>サブクラス内の索引</ul></b><br>電気的照明<br>システム　２／００<br>ひも状または細片状の光源　４／００<br>自在に立てられるもの　６／００<br>固定するもの　８／００<br>電源を内蔵するもの　９／００<br>変化する照明効果を生み出すもの　１０／００<br>非電気的照明<br>昼光を用いるもの　１１／００<br>光源：点状または形状が特定されていないもの　１３／００<br>その他の装置　１５／００<br>電気的光源に非電気的光源を組み合わせたものを光源とする照明装置　１９／００<br>電気的および非電気的装置の組み合わせ　４１／００，４３／００，４５／００<br>	NON-PORTABLE LIGHTING DEVICES; SYSTEMS THEREOF; VEHICLE LIGHTING DEVICES SPECIALLY ADAPTED FOR VEHICLE EXTERIORS<b>[1,7]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u>:<b>[7,2009.01]</b><ul type=""disc""><li>devices or systems intended for fixed installation or for use at a permanent location, e.g. free-standing floor- or table-lamps;</li><li>aspects related to the optical, mechanical, thermal or electrical arrangement of elements in vehicle illuminating devices specially adapted for vehicle exterior, e.g. headlamps;</li><li>aspects related to the optical, mechanical, thermal or electrical arrangement of elements in vehicle light signalling devices specially adapted for vehicle exterior, e.g. brake lamps or direction indicator lights.</li></ul></li><li>This subclass <u>does not cover</u>:<ul type=""disc""><li>devices or systems specially adapted for transportation, which are covered by subclass <b>F21L</b>;</li><li>aspects related to the vehicles in which lighting devices are arranged, e.g. the arrangement or operation of lighting devices on vehicles, which are covered by subclass <b>B60Q</b>;</li><li>control of vehicle lighting devices in relation to the vehicle as a whole, e.g. for levelling, swivelling or aiming. Such arrangements are covered by group <b>B60Q 1/06</b>, even if the movement of the lighting device occurs inside the lamp housing.</li></ul></li><li>Non-electric lighting devices or systems are classified in groups <b>F21S 11/00-F21S 15/00</b> only if a special adaptation related to the use of a non-electric light source is of interest.</li><li>In this subclass, it is desirable to add the indexing codes of subclasses <b>F21W</b> and <b>F21Y</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ELECTRIC DEVICES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Systems</td><td><b>2/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">String or strip of light sources</td><td><b>4/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Free-standing</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fixed installation</td><td><b>8/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Built-in power supply</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Producing varying lighting effects</td><td><b>10/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">NON-ELECTRIC DEVICES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using daylight</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Light source: Point-like or of unspecified shape</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other devices</td><td><b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OF ELECTRIC AND NON-ELECTRIC DEVICES</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VEHICLE LIGHTING DEVICES FOR VEHICLE EXTERIORS</td><td><b>41/00</b>, <b>43/00</b>, <b>45/00</b></td></p></tr></table>				
F21V		照明装置またはそのシステムの機能的特徴あるいは細部；他に分類されない，その他の物品と照明装置との構造的な組み合わせ［１，７］<br><br><b><ul>注</ul></b><br>（１）グループＦ２１Ｖ１／００からＦ２１Ｖ１４／００は、光の発散または分配に関する観点を包含する。グループＦ２１Ｖ１５／００からＦ２１Ｖ３１／００は、光の発散または分配に関しない観点を包含する。［２００９．０１］<br>（２）非電気的照明装置またはシステムは、非電気的な光源の使用に関連した特別な適応が重要である場合にのみグループＦ２１Ｖ３５／００からＦ２１Ｖ３７／００に分類する。［２００９．０１］<br>（３）このサブクラスにおいては，サブクラスＦ２１ＷおよびＦ２１Ｙのインデキシングコードを付与することが望ましい。［７］<br><br><b><ul>サブクラス内の索引</ul></b><br>光の発散または分配に関する要素の細部<br>笠；グローブ；屈折器；反射器　１／００；３／００；５／００；７／００<br>ライトガイド　８／００<br>放射光の分光特性，偏光または強度を修正する要素　９／００<br>その他のスクリーン　１１／００<br>素子の組み合わせ　１３／００<br>光の分配を変えるもの　１４／００<br>光の発散または分配に関しない要素の細部<br>締め付け　１７／００；１９／００<br>支持またはつり下げ装置　２１／００<br>電気回路素子の配置　２３／００<br>ケーブル収納　２７／００<br>防護；保安；冷却；締め付け　１５／００；２５／００；２９／００；３１／００<br>その他の物品との組み合わせ　３３／００<br>ろうそく立て　３５／００<br>マントルまたはバーナの配置　３６／００<br>燃焼照明の細部　３７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	FUNCTIONAL FEATURES OR DETAILS OF LIGHTING DEVICES OR SYSTEMS THEREOF; STRUCTURAL COMBINATIONS OF LIGHTING DEVICES WITH OTHER ARTICLES, NOT OTHERWISE PROVIDED FOR<b>[1,7]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Groups <b>F21V 1/00-F21V 14/00</b> cover aspects related to light emission or distribution. Groups <b>F21V 15/00-F21V 31/00</b> cover aspects not related to light emission or distribution.<b>[7,2009.01]</b></li><li>Details of non-electric lighting devices or systems are classified in groups <b>F21V 35/00-F21V 37/00</b> only if a special adaptation related to the use of a non-electric light source is of interest.</li><li>In this subclass, it is desirable to add the indexing codes of subclasses <b>F21W</b> and <b>F21Y</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS OF ELEMENTS INVOLVED IN LIGHT EMISSION OR DISTRIBUTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Shades; globes; refractors; reflectors</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Light guides</td><td><b>8/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Elements for modifying spectral properties, polarisation or intensity of the light emitted</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other screens</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations of elements</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Controlling the distribution of the light</td><td><b>14/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS OF ELEMENTS NOT INVOLVED IN LIGHT EMISSION OR DISTRIBUTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fastening</td><td><b>17/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements for supporting or suspending</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements of electric circuit elements</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Cable stowing</td><td><b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Protection; safety; cooling; tightness</td><td><b>15/00</b>; <b>25/00</b>; <b>29/00</b>; <b>31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations with other articles</td><td><b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Candle holders</td><td><b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements of mantles or burners</td><td><b>36/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details of combustion lighting</td><td><b>37/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F21W		照明装置またはシステムの使用または適用に関するサブクラス　Ｆ２１Ｋ，Ｆ２１Ｌ，Ｆ２１Ｓ，およびＦ２１Ｖに結びつくインデキシング系列［７］<br><br><b><ul>注</ul></b><br>このサブクラスは，照明装置またはシステムの使用または適用に関する，サブクラスＦ２１Ｋ，Ｆ２１Ｌ，Ｆ２１Ｓ，およびＦ２１Ｖに結びつくインデキシング系列を構成する。［７］<br>	INDEXING SCHEME ASSOCIATED WITH SUBCLASSES <b>F21K</b>, <b>F21L</b>, <b>F21S</b> and <b>F21V</b>, RELATING TO USES OR APPLICATIONS OF LIGHTING DEVICES OR SYSTEMS<b>[7]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass constitutes an indexing scheme associated with subclasses <b>F21K</b>, <b>F21L</b>, <b>F21S</b> and <b>F21V</b>, relating to uses or applications of lighting devices or systems.<b>[7]</b></li></ul>				
F21Y		光源の形状もしくは種類または放射された光の色に関するサブクラスＦ２１Ｋ，Ｆ２１Ｌ，Ｆ２１Ｓ，およびＦ２１Ｖに関連するインデキシング系列［７］<br><br><b><ul>注</ul></b><br>このサブクラスは，光源の形状もしくは種類または放射された光の色に関するサブクラスＦ２１Ｋ，Ｆ２１Ｌ，Ｆ２１Ｓ，およびＦ２１Ｖと関連するインデキシング系列を構成している。［７］<br>	INDEXING SCHEME ASSOCIATED WITH SUBCLASSES <b>F21K</b>, <b>F21L</b>, <b>F21S</b> and <b>F21V</b>, RELATING TO THE FORM OR THE KIND OF THE LIGHT SOURCES OR OF THE COLOUR OF THE LIGHT EMITTED<b>[7]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass constitutes an indexing scheme associated with subclasses <b>F21K</b>, <b>F21L</b>, <b>F21S</b> and <b>F21V</b>, relating to the form or the kind of the light sources, or of the colour of the light emitted.<b>[7]</b></li></ul>				
F22		蒸気発生<br><br><b><ul>注</ul></b><br>このクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“蒸気”は，また他の凝縮性蒸気，例．水銀，ジフェニル，ジフェニル配化物を包含する。<br>	STEAM GENERATION<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this class, the following term is used with the meaning indicated:<ul type=""disc""><li>&quot;steam&quot; covers also other condensable vapours, e.g. mercury, diphenyl, diphenyl oxide.</li></ul></li></ul>				
F22B		蒸気発生法；蒸気ボイラ<br><br><b><ul>注</ul></b><br>このサブクラスは圧力下において加熱または動力の目的で蒸気を発生する方法または装置だけを包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>一般的蒸気発生法　１／００，３／００<br>蒸気ボイラ<br>一般的特徴<br>ドラム；炉筒；煙管；煙管と水管の組み合わせ；火室　５／００；７／００；９／００；１１／００；１３／００<br>水管形<br>補助管　１１／００<br>水平位置；水平に近い傾斜；水平に近い傾斜と垂直の結合；垂直または鋭い傾斜　１５／００；１７／００；１９／００；２１／００<br>間隙を置いて２重に囲まれた水管群または戻り形の配置；内部に配列された煙管をもつ水管群　２３／００；２５／００<br>特別な特徴　２７／００，２９／００<br>修正または配置；一般的な適用の細部　３１／００；３７／００<br>設備；制御方式　３３／００；３５／００<br>	METHODS OF STEAM GENERATION; STEAM BOILERS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> only methods of, or apparatus for, the generation of steam under pressure for heating or power purposes.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">METHODS FOR STEAM GENERATION</td><td><b>1/00</b>, <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STEAM BOILERS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General characteristics</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">having drum; having furnace tube; having fire tube; having combined fire tube and water tube; having fire-box</td><td><b>5/00</b>; <b>7/00</b>; <b>9/00</b>; <b>11/00</b>; <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">having water tubes</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">auxiliary tubes</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">horizontal; horizontally-inclined; combined horizontally-inclined and vertical; vertical or steeply-inclined</td><td><b>15/00</b>; <b>17/00</b>; <b>19/00</b>; <b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:4em;margin:0"">formed of sets of spaced double-walled water tubes or of return tubes; water tubes with internally-arranged flue tubes</td><td><b>23/00</b>; <b>25/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Special characteristics</td><td><b>27/00</b>, <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Modifications or arrangements; details of general application</td><td><b>31/00</b>; <b>37/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PLANTS; CONTROL SYSTEMS</td><td><b>33/00</b>; <b>35/00</b></td></p></tr></table>				
F22D		蒸気発生のための給水の予熱または予熱された給水の蓄積；蒸気発生のための給水の供給；蒸気発生のための水位の制御；蒸気ボイラ内の水循環を促進するための補助装置<br>	PREHEATING, OR ACCUMULATING PREHEATED, FEED-WATER FOR STEAM GENERATION; FEED-WATER SUPPLY FOR STEAM GENERATION; CONTROLLING WATER LEVEL FOR STEAM GENERATION; AUXILIARY DEVICES FOR PROMOTING WATER CIRCULATION WITHIN STEAM BOILERS				
F22G		蒸気の過熱［２００６．０１］<br>	SUPERHEATING OF STEAM				
F23		燃焼装置；燃焼方法<br><br><b><ul>注</ul></b><br>このクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“燃焼”は，可燃物質と分子酸素，例．空気中の，との間の発熱を伴う連鎖的な化学反応を意味し，大半の場合に炎または白熱の形式で光を発生させる；<br>―“燃焼室”は，それ自体で維持される火または炎を確立するために燃料がその中で燃焼するものであって，その火または炎を取り囲んでいる室を意味する；<br>―“バーナ”は，それ自体で維持される炎を発生するために流動性燃料が，または空気中に浮遊する固体燃料が，燃焼する燃焼空間へ導かれる装置を意味する；<br>―“空気”は，遊離した酸素を含み，および燃焼を促進または維持させ得る気体の混合物を意味する。<br>	COMBUSTION APPARATUS; COMBUSTION PROCESSES<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this class, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;combustion&quot; means a heat-producing sequence of chemical reactions between a burnable substance and molecular oxygen, e.g. in air, in most cases generating light in the form of flames or a glow;</li><li>&quot;combustion chamber&quot; means a chamber in which fuel is burned to establish a self-supporting fire or flame and which surrounds that fire or flame;</li><li>&quot;burner&quot; means a device by which fluid fuel, or solid fuel suspended in air, is passed to a combustion space where it burns to produce a self-supporting flame;</li><li>&quot;air&quot; means a mixture of gases containing free oxygen and able to promote or support combustion.</li></ul></li></ul>				
F23B		固体燃料のみを用いる燃焼方法または装置（室温では固体であるが溶解した状態で燃焼する燃料の燃焼のためのもの，例．ロウソクの蝋，Ｃ１１Ｃ５／００，Ｆ２３Ｃ，Ｆ２３Ｄ；空気中に浮遊した固体燃料を用いるものＦ２３Ｃ，Ｆ２３Ｄ１／００；液体中に浮遊した固体燃料を用いるものＦ２３Ｃ，Ｆ２３Ｄ１１／００；固体燃料を液体燃料と一緒に，あるいは空気中に浮遊する固体燃料と一緒に，同時にまたは択一的に用いるものＦ２３Ｃ，Ｆ２３Ｄ１７／００）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは，燃料自体が，流体搬送や浮遊状態ではなく機械的に輸送されて燃焼するか、本質的に静止したまま燃焼するか，のいずれかの燃焼のみを包含する。［８］<br>（２）このサブクラスでは，ファーストプレイス優先ルールが適用される。即ち，各階層レベルにおいて，相反する指示がない限り最初の適切な箇所に分類する。［８］<br>（３）このサブクラスでは，方法は，用いられている装置を包含しているグループに分類する。ある特殊なタイプの装置に関連していない方法は，グループＦ２３Ｂ９０／００に分類する。［８］<br>（４）このサブクラスでは，グループＦ２３Ｂ１０１／００〜Ｆ２３Ｂ１０３／００のインデキシングコードを付加することが望ましい。［８］<br><br><b><ul>サブクラス内の索引</ul></b><br>燃焼装置<br>２以上の燃焼室の組み合わせ　１０／００<br>特に携帯または移動可能なもの　２０／００<br>機能別　３０／００〜６０／００<br>固体の燃焼残滓を再循環するもの　７０／００<br>燃焼ガスのまたはその燃焼により放出される不燃焼ガスの明確な流路を作成するもの　８０／００<br>装置の種類によらない燃焼方法　９０／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	METHODS OR APPARATUS FOR COMBUSTION USING ONLY SOLID FUEL (for combustion of fuels that are solid at room temperatures, but burned in melted form, e.g. candle wax, <b>C11C 5/00</b>, <b>F23C</b>, <b>F23D</b>; using solid fuel suspended in air <b>F23C</b>, <b>F23D 1/00</b>; using solid fuel suspended in liquids <b>F23C</b>, <b>F23D 11/00</b>; using solid fuel together with fluid fuel or with solid fuel suspended in air, simultaneously or alternately, <b>F23C</b>, <b>F23D 17/00</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass only <u>covers</u> combustion wherein the main body of fuel is either essentially stationary during combustion or mechanically transported, as opposed to pneumatically transported or suspended in air, during combustion.<b>[8]</b></li><li>In this subclass, the first place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the first appropriate place.</li><li>In this subclass, methods are classified in the groups that cover the apparatus used. Methods that are not related to a particular type of apparatus are classified in group <b>F23B 90/00</b>.</li><li>In this subclass, it is desirable to add the indexing codes of groups <b>F23B 101/00-F23B 103/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBUSTION APPARATUS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations of two or more combustion chambers</td><td><b>10/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Specially adapted for portability or transportability</td><td><b>20/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Functional types</td><td><b>30/00-60/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Returning solid combustion residues to the combustion chamber</td><td><b>70/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Creating a distinct flow path for flue gases or for non-combusted gases given off by the fuel</td><td><b>80/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBUSTION METHODS NOT RELATED TO A PARTICULAR TYPE OF APPARATUS</td><td><b>90/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F23C		流体燃料あるいは空気中に浮遊する固体燃料を用いる燃焼方法または装置（バーナＦ２３Ｄ）<br><br><b><ul>注</ul></b><br>このサブクラスでは，方法は，用いられている装置を包含しているグループに分類する。［８］<br><br><b><ul>サブクラス内の索引</ul></b><br>２種類以上の燃料の燃焼に特に適した燃焼装置　１／００<br>２以上の燃焼室の組合せ　６／００<br>燃焼装置の種類別<br>流動層燃焼　１０／００<br>触媒燃焼　１３／００<br>振動燃焼　１５／００<br>細部に特徴のある燃焼装置<br>燃焼室　３／００<br>バーナの配置または据え付け　５／００<br>空気供給　７／００<br>燃焼ガスまたは燃焼生成物の再循環　９／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	METHODS OR APPARATUS FOR COMBUSTION USING FLUID FUEL OR SOLID FUEL SUSPENDED IN AIR (burners <b>F23D</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, methods are classified in the groups that cover the apparatus used.<b>[8]</b></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBUSTION APPARATUS SPECIALLY ADAPTED FOR COMBUSTION OF TWO OR MORE TYPES OF FUEL</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATIONS OF TWO OR MORE COMBUSTION CHAMBERS</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FUNCTIONAL TYPES OF COMBUSTION APPARATUS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fluidised bed combustion</td><td><b>10/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Catalytic combustion</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Resonant combustion</td><td><b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBUSTION APPARATUS CHARACTERISED BY SUBSYSTEMS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combustion chambers</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangement or mounting of burners</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Air supply</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements for returning flue gases or combustion products</td><td><b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F23D		バーナ<br><br><b><ul>サブクラス内の索引</ul></b><br>バーナ（高圧または高速の燃焼生成物の生成Ｆ２３Ｒ）<br>粉状燃料用バーナ　１／００<br>液体燃焼用バーナ<br>毛細管現象を用いるもの　３／００<br>燃料の気化を用いるもの；直接的噴霧作用を用いるもの　５／００；１１／００<br>面に対する燃料の衝撃を用いるもの　７／００，９／００<br>ガス燃焼用バーナ　１４／００<br>ガス状，液体または粉状の燃料の燃焼用バーナ　１７／００<br>２またはそれ以上のバーナの組み合わせ　２３／００<br>その他のバーナ　９９／００<br>	BURNERS<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BURNERS FOR PULVERULENT FUEL</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BURNERS FOR COMBUSTION OF A LIQUID</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using capillary action</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using fuel evaporation; direct spraying action</td><td><b>5/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using fuel impingement on a surface</td><td><b>7/00</b>, <b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BURNERS FOR COMBUSTION OF A GAS</td><td><b>14/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BURNERS FOR COMBUSTION OF GASEOUS OR LIQUID OR PULVERULENT FUEL</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ASSEMBLIES OF TWO OR MORE BURNERS</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER BURNERS</td><td><b>99/00</b></td></p></tr></table>				
F23G		火葬炉；燃焼により廃棄物または低級燃料を焼却するもの<br><br><b><ul>サブクラス内の索引</ul></b><br>火葬　１／００<br>燃焼により廃棄物または低級燃料を焼却するもの<br>処理；装置の機能別の種類　５／００<br>特定の廃棄物または燃料に適合したもの　７／００<br>細部；付属装置　５／４４<br>制御または安全装置　５／５０<br>	CREMATION FURNACES; CONSUMING WASTE OR LOW GRADE FUELS BY COMBUSTION<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CREMATION</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONSUMING WASTE OR LOW-GRADE FUELS BY COMBUSTION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Processes; Functional types of apparatus</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Adaptation for specific waste or fuels</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details; Accessories</td><td><b>5/44</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Control or safety arrangements</td><td><b>5/50</b></td></p></tr></p></tr></table>				
F23H		火格子（流動層燃焼装置のための流動化を行う空気の入口Ｆ２３Ｃ１０／２０）；火格子の灰落としまたはかきならし<br><br><b><ul>サブクラス内の索引</ul></b><br>火格子<br>中実棒を有するもの；中空棒を有するもの　１／００；３／００<br>２重火格子；傾斜火格子；回転または揺動する火格子；移床火格子　５／００；７／００；９／００；１１／００<br>他の型　１３／００<br>細部　１７／００<br>火格子のための清掃装置，火格子に沿って燃料を動かすもの　１５／００<br>	GRATES (inlets for fluidisation air for fluidised bed combustion apparatus <b>F23C 10/20</b>); CLEANING OR RAKING GRATES<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GRATES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With solid bars; with hollow bars</td><td><b>1/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Double; inclined; revolving or rocking; travelling</td><td><b>5/00</b>; <b>7/00</b>; <b>9/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other types</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Details</td><td><b>17/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CLEANING ARRANGEMENTS FOR GRATES, MOVING FUEL ALONG GRATE</td><td><b>15/00</b></td></p></tr></table>				
F23J		燃焼生成物または燃焼残滓（し）の除去または処理；煙道（煙またはガス，例．排気ガス，を焼却するための燃焼装置Ｆ２３Ｇ７／０６）［２００６．０１］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは燃焼生成物または燃焼残滓によって表面を汚染された炉管，炎管，水管，ボイラーの煙道等，熱交換または熱伝達管の表面の清掃を包含する。<br>（２）このサブクラスは燃焼生成物または燃焼残滓以外のものによって汚染されたボイラー，熱交換または熱伝達管の表面の清掃は包含しない。ただしそれらはサブクラスＦ２８Ｇに包含される。<br><br><b><ul>サブクラス内の索引</ul></b><br>固体の燃焼生成物または残滓の除去<br>燃焼室から　１／００<br>火の届かない場所から　３／００<br>燃焼生成物または残滓の処理<br>化学薬品の供給；凝固防止；煙またはガスの他の処理　７／００；９／００；１５／００<br>煙道，煙突または煙道のための取り付け具　１１／００，１３／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	REMOVAL OR TREATMENT OF COMBUSTION PRODUCTS OR COMBUSTION RESIDUES; FLUES (combustion apparatus for consuming smoke or fumes, e.g. exhaust gases, <b>F23G 7/06</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> also the cleaning of surfaces of furnace tubes, flame tubes, water tubes, flues or the like of boilers, heat-exchange or heat-transfer conduits, which surfaces are contaminated by combustion products or combustion residues.</li><li>This subclass <u>does not cover</u> the cleaning of surfaces of boilers, heat exchange or heat-transfer conduits contaminated by other than combustion products or combustion residues, which is covered by subclass <b>F28G</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">REMOVAL OF SOLID COMBUSTION PRODUCTS OR RESIDUES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">From combustion chamber</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">From places beyond the fire</td><td><b>3/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TREATMENT OF COMBUSTION PRODUCTS OR RESIDUES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Supply of chemicals; preventing solidification; Treating smoke or fumes</td><td><b>7/00</b>; <b>9/00</b>; <b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLUES, FITTINGS FOR CHIMNEYS OR FLUES</td><td><b>11/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F23K		燃焼装置への燃料の供給（流動層燃焼装置に特に適合させた燃料供給装置　Ｆ２３Ｃ１０／２２）［２００６．０１］<br>	FEEDING FUEL TO COMBUSTION APPARATUS (fuel feeders specially adapted for fluidised bed combustion apparatus <b>F23C 10/22</b>)				
F23L		空気または不燃性液体またはガスの燃焼装置への供給一般（空気または蒸気を供給する手段をもつ火橋Ｆ２３Ｍ３／０４；空気供給通路をもつ邪魔板または遮板Ｆ２３Ｍ９／０４）；燃焼装置への空気供給または通風の制御に特に適合したバルブまたはダンパ；燃焼装置への誘引通風；煙突または通風軸の先端；煙道の末端<br><br><b><ul>サブクラス内の索引</ul></b><br>空気供給<br>通路：１次空気のためのもの；２次空気のためのもの　１／００；９／００<br>バルブまたはダンパ<br>構造　１３／００<br>配置：火の前方のもの；火の後方のもの　３／００；１１／００<br>火の前方の送風発生装置；燃焼用空気の加熱　５／００；１５／００<br>火への空気以外の不燃性の液体またはガスの供給　７／００<br>通風誘引　１７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００［８］<br>	SUPPLYING AIR OR NON-COMBUSTIBLE LIQUIDS OR GASES TO COMBUSTION APPARATUS IN GENERAL (firebridges with means for feeding air or steam <b>F23M 3/04</b>; baffles or shields with air supply passages <b>F23M 9/04</b>); VALVES OR DAMPERS SPECIALLY ADAPTED FOR CONTROLLING AIR SUPPLY OR DRAUGHT IN COMBUSTION APPARATUS; INDUCING DRAUGHT IN COMBUSTION APPARATUS; TOPS FOR CHIMNEYS OR VENTILATING SHAFTS; TERMINALS FOR FLUES<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">AIR SUPPLY</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Passages for: primary air; secondary air</td><td><b>1/00</b>; <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Valves or dampers</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">construction</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">arrangements: before the fire; after the fire</td><td><b>3/00</b>; <b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Blast-producing apparatus before the fire; heating of air for combustion</td><td><b>5/00</b>; <b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUPPLYING NON-COMBUSTIBLE LIQUIDS OR GASES, OTHER THAN AIR, TO THE FIRE</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DRAUGHT-INDUCING</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F23M		燃焼室のためにとくに適合するケーシング，内張り，壁または扉，例．火橋；燃焼室内で空気，炎または燃焼生成物を転向させる装置；燃焼装置のために特に適合する安全装置；他に分類されない燃焼室の細部<br>	CASINGS, LININGS, WALLS OR DOORS SPECIALLY ADAPTED FOR COMBUSTION CHAMBERS, e.g. FIREBRIDGES; DEVICES FOR DEFLECTING AIR, FLAMES OR COMBUSTION PRODUCTS IN COMBUSTION CHAMBERS; SAFETY ARRANGEMENTS SPECIALLY ADAPTED FOR COMBUSTION APPARATUS; DETAILS OF COMBUSTION CHAMBERS, NOT OTHERWISE PROVIDED FOR				
F23N		燃焼の調整または制御（燃焼が燃料または他の粒子の流体層で発生する燃焼装置に特に適合した制御装置Ｆ２３Ｃ１０／２８；固形燃料用の開放式炉を備えた家庭用ストーブの，燃焼を調節するための状態反応制御Ｆ２４Ｂ１／１８７）［８］<br>	REGULATING OR CONTROLLING COMBUSTION (control devices specially adapted for combustion apparatus in which combustion takes place in a fluidised bed of fuel or other particles <b>F23C 10/28</b>; condition responsive controls for regulating combustion in domestic stoves with open fires for solid fuel <b>F24B 1/187</b>)				
F23Q		点火（マッチ点火用装置Ａ２４Ｆ；化学的点火器Ｃ０６Ｃ９／００）；消火装置<br><br><b><ul>サブクラス内の索引</ul></b><br>点火器<br>機械的なもの　１／００<br>電気火花を用いるもの　３／００，５／００<br>白熱するものを用いるもの　７／００<br>種火をもつもの　９／００<br>触媒によるもの　１１／００<br>その他のもの　１３／００<br>遠隔点火　２１／００<br>試験　２３／００<br>燃料入りライタ　２／００，３／０１，７／００<br>消火装置　２５／００<br>	IGNITION (devices for igniting matches <b>A24F</b>;  chemical igniters <b>C06C 9/00</b>); EXTINGUISHING DEVICES<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">IGNITERS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Mechanical</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using electric sparks</td><td><b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Incandescent</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With pilot flame</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By catalysis</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other</td><td><b>13/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">REMOTE IGNITION</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TESTING</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LIGHTERS CONTAINING FUEL</td><td><b>2/00</b>, <b>3/01</b>, <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">EXTINGUISHING DEVICES</td><td><b>25/00</b></td></p></tr></table>				
F23R		高圧または高速の燃焼生成物の生成，例．ガスタービン燃焼室（加圧下での操作に特に適合する流動床燃焼装置Ｆ２３Ｃ１０／１６）<br>	GENERATING COMBUSTION PRODUCTS OF HIGH PRESSURE OR HIGH VELOCITY, e.g. GAS-TURBINE COMBUSTION CHAMBERS (fluidised bed combustion apparatus specially adapted for operation at superatmospheric pressures <b>F23C 10/16</b>)				
F24		加熱；レンジ；換気<br><br><b><ul>注</ul></b><br>このクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“ストーブ”は開放式炉，例．暖炉，を持つような装置を包含する；<br>―“レンジ”は種々の調理操作または調理と加熱操作をする要素をもった調理装置を意味する。<br>	HEATING; RANGES; VENTILATING<br><br><b><u>Note(s)</u></b><br><br><ul style=""list-style:none""><li>In this class, the following terms are used with the meanings indicated:<ul type=""disc""><li>&quot;stove&quot; includes apparatus which may have an open fire, e.g. fireplace;</li><li>&quot;range&quot; means an apparatus for cooking having elements that perform different cooking operations or cooking and heating operations.</li></ul></li></ul>				
F24B		固体燃料使用の家庭用ストーブまたはレンジ（気体燃料，液体燃料または他の腫類のエネルギの供給と組み合わせて固形燃料を使用するためのものＦ２４Ｃ１／０２）；ストーブまたはレンジと共に使用するための装置［６］<br>	DOMESTIC STOVES OR RANGES FOR SOLID FUELS (for solid fuels in combination with gaseous fuels, liquid fuels or other kinds of energy supply <b>F24C 1/02</b>); IMPLEMENTS FOR USE IN CONNECTION WITH STOVES OR RANGES<b>[6]</b>				
F24C		家庭用ストーブまたはレンジ（固体燃料のみを使用するものＦ２４Ｂ）；一般的に適用される家庭用ストーブまたはレンジの細部<br><br><b><ul>サブクラス内の索引</ul></b><br>固体燃料に制限されないストーブまたはレンジ<br>一般的特徴　１／００<br>燃料またはエネルギーが単一の形のもの　３／００〜９／００<br>燃料またはエネルギの供給が２つ以上または特定されていないような形のもの　１／００<br>水加熱用に付加的手段をもつもの　１３／００<br>セルフクリーニング設備を有するもの　１４／００<br>ストーブまたはレンジの組み合わせ　１１／００<br>ストーブまたはレンジの細部一般　１５／００<br>	DOMESTIC STOVES OR RANGES (exclusively for solid fuels <b>F24B</b>); DETAILS OF DOMESTIC STOVES OR RANGES, OF GENERAL APPLICATION<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STOVES OR RANGES, NOT RESTRICTED TO SOLID FUEL</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">General characteristics</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With single kind of fuel or energy supply</td><td><b>3/00-9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With more than one, or unspecified kind of fuel or energy supply</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With additional means for heating water</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With self-cleaning provisions</td><td><b>14/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations of stoves or ranges</td><td><b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS OF STOVES OR RANGES IN GENERAL</td><td><b>15/00</b></td></p></tr></table>				
F24D		家庭用または区域暖房方式，例．中央暖房方式；家庭用温水供給方式；そのための要素または構成部材（加熱目的のために蒸気機関設備から抽出または排出された蒸気または復水の利用Ｆ０１Ｋ１７／０２）［２００６．０１］<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“中央暖房方式”は，そのシステムの中で熱が発生されまたは中央源に蓄積され，加熱される空間または地域へ伝達流体によって分配される方式を意味する。［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>中央暖房方式<br>下記の熱交換流体をもつもの：蒸気；温水；温風または排気ガス；他の流体　１／００；３／００；５／００；７／００<br>組み合わせ　９／００<br>地域暖房方式　１０／００<br>蓄熱によるもの　１１／００<br>他の方式　１２／００<br>他の家庭用または区域暖房方式<br>電気式；その他　１３／００；１５／００<br>家庭用温水供給　１７／００<br>小規模な熱電併給システム　１８／００<br>細部　１９／００<br>	DOMESTIC- OR SPACE-HEATING SYSTEMS, e.g. CENTRAL HEATING SYSTEMS; DOMESTIC HOT-WATER SUPPLY SYSTEMS; ELEMENTS OR COMPONENTS THEREFOR (using steam or condensate extracted or exhausted from steam engine plants for heating purposes <b>F01K 17/02</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following expression is used with the meaning indicated:<b>[5]</b><ul type=""disc""><li>&quot;central heating system&quot; means a system in which heat is generated or stored at central sources and is distributed by means of a transfer fluid to the spaces or areas to be heated.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CENTRAL HEATING SYSTEMS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With heat-transfer fluid: steam; hot water; hot air or exhaust gas; other fluid</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">District heating systems</td><td><b>10/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">By heat storage</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other systems</td><td><b>12/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER DOMESTIC- OR SPACE-HEATING SYSTEMS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Electric; Other</td><td><b>13/00</b>; <b>15/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DOMESTIC HOT-WATER SUPPLY</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SMALL-SCALE COMBINED HEAT AND POWER GENERATION SYSTEMS</td><td><b>18/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS</td><td><b>19/00</b></td></p></tr></table>				
F24F		空気調節；空気加湿；換気；しゃへいのためのエアカーテンの利用（発生場所からのじんあいまたは臭気の除去Ｂ０８Ｂ１５／００；建物から廃ガスを除去するための垂直ダクトＥ０４Ｆ１７／０２；煙突または通風軸（換気塔）の先端，煙道の末端Ｆ２３Ｌ１７／０２）<br><br><b><ul>注</ul></b><br>１．このサブクラスは、空気調和システムまたはルームユニットにおける、人の住居空間または作業空間に供給される空気の処理，例．浄化，を包含する。<br>２．このサブクラスにおいては：<br>・空気調和における，すなわち，空気が冷却されるか，ないしは加熱されるところのユニットにおける，補助処理としての空気加湿は，グループＦ２４Ｆ１／００またはＦ２４Ｆ３／１４に包含される；<br>・空気加湿それ自体，例．“部屋加湿器”，はグループＦ２４Ｆ６／００に包含される。<br>３．このサブクラスにおいては下記の用語は以下に示す意味で用いる：<br>・“空気調和”とは，冷却または冷却とさらなる種類の空気処理，例．加湿，加熱または空気浄化，との組み合わせにより，部屋または空間に空気を供給すること，または，部屋または空間の空気の処理をすることを意味する；<br>・”換気”とは，部屋または空間に空気を供給すること，またはそれから空気を抽出することおよび部屋または空間内において空気を循環させることを意味する。しかし，部屋または空間に供給される空気，それから抽出される空気，またはそのなかで循環させる空気を処理するだけのものは包含しない。<br>４．このサブクラスにおいては，制御または安全装置はＦ２４Ｆ１１／００に分類される。これらの装置が用いられる空気処理システムの種類を示すために，メイングループＦ２４Ｆ１／００〜Ｆ２４Ｆ９／００にて更なる分類が付与されることがある。<br><br><b><ul>サブクラス内の索引</ul></b><br>空気調和<br>ルームユニット；セントラル方式；他の方式または装置　１／００；３／００；５／００<br>空気加湿　６／００<br>換気　７／００<br>気流によるしゃへい　９／００<br>安全装置の制御　１１／００<br>エネルギ回収システムを用いるもの　１２／００<br>細部　１３／００<br>	AIR-CONDITIONING; AIR-HUMIDIFICATION; VENTILATION; USE OF AIR CURRENTS FOR SCREENING (removing dirt or fumes from areas where they are produced <b>B08B 15/00</b>; vertical ducts for carrying away waste gases from buildings <b>E04F 17/02</b>; tops for chimneys or ventilating shafts, terminals for flues <b>F23L 17/02</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> treatment, e.g. purification, of air supplied to human living or working spaces in air conditioning systems or in room units.<b>[3]</b></li><li>In this subclass:<ul type=""disc""><li>air-humidification as auxiliary treatment in air-conditioning, i.e. in units wherein the air is also either cooled or heated, is covered by groups <b>F24F 1/00</b> or <b>F24F 3/14</b>;</li><li>air-humidification per se, e.g. &quot;room humidifiers&quot;, is covered by group <b>F24F 6/00</b>.</li></ul></li><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;air-conditioning&quot; means the supply of air to or the treatment of air in rooms or spaces by means of cooling or a combination of cooling and a further kind of air treatment, e.g. humidification, heating or air purification;</li><li>&quot;ventilation&quot; means the supply of air to, or its extraction from, rooms or spaces, and systems for circulating air within rooms or spaces, but does not cover the mere treatment of air being supplied to, extracted from, or circulated within, rooms or spaces.</li></ul></li><li>In this subclass, control or safety arrangements are classified in group <b>F24F 11/00</b>. In order to indicate the type of air-treatment system in which these arrangements are used, further classification may be made in groups <b>F24F 1/00-F24F 9/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">AIR-CONDITIONING</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Room units; central systems; other systems or apparatus</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">AIR-HUMIDIFICATION</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">VENTILATION</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TREATMENT OTHER THAN BY HEATING, COOLING, HUMIDIFYING OR DRYING</td><td><b>8/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SCREENING BY AIR CURRENTS</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL OR SAFETY ARRANGEMENTS</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">USE OF ENERGY RECOVERY SYSTEMS</td><td><b>12/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS</td><td><b>13/00</b></td></p></tr></table>				
F24H		熱発生手段，例．ヒートポンプ，を有する流体加熱器一般，例．水加熱器または空気加熱器（蒸気発生Ｆ２２）<br><br><b><ul>注</ul></b><br>（１）このサブクラスに包含される空気加熱器の明瞭な特徴は，熱が対流によって，主として空気の強制循環によって，空気に主として放出されることがある。Ｆ２４Ｂ，Ｆ２４Ｃに包含される家庭用のストーブまたはレンジも，火炎による空気加熱器または電気的空気加熱器であろうが，それらはかなりの程度まで輻射により熱を放出し自然対流によりある程度まで熱を放出するだけである。［３］<br>（２）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“水”は他の液体を含み，かつ常に加熱される液体を意味する；［３］<br>―“空気”は他の気体または混合気体を含み，かつ常に加熱される気体を意味する；［３］<br>―“炉管”は加熱器の内側にある管であって該管内で燃焼が行われるものを意味する；［３］<br>―“煙管”は加熱器の内側にある管であって煙道ガスが該管の外側に位置する燃焼室から該管を通って流れるものを意味する；［３］<br>―“加熱器”は，熱発生手段および発生した熱を水または空気に伝達する手段とを共に含んだ装置を意味する。［３］<br>（３）すべての蓄熱式加熱器はグループ７／００に分類される。［３］<br><br><b><ul>サブクラス内の索引</ul></b><br>水加熱器　Ｆ２４Ｈ１／００<br>空気加熱器　Ｆ２４Ｈ３／００<br>ヒートポンプを使用する流体加熱器　Ｆ２４Ｈ４／００<br>水加熱器と空気加熱器の結合　Ｆ２４Ｈ６／００<br>蓄熱加熱器　Ｆ２４Ｈ７／００<br>煙道ガスから潜熱を抽出する流体加熱器　Ｆ２４Ｈ８／００<br>細部　Ｆ２４Ｈ９／００<br>制御　Ｆ２４Ｈ１５／００<br>	FLUID HEATERS, e.g. WATER OR AIR HEATERS, HAVING HEAT-GENERATING MEANS, e.g. HEAT PUMPS, IN GENERAL (steam generation <b>F22</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>The distinguishing feature of the air heaters covered by this subclass is that the heat is predominantly released to the air by convection, mostly by forced circulation of the air. The domestic stoves or ranges covered by subclass <b>F24B</b>, <b>F24C</b> may also be fired or electric air heaters but they release their heat to a considerable extent by radiation and only to some extent by natural convention.<b>[3]</b></li><li>In this subclass, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;water&quot; includes other liquids and means always the liquid to be heated;</li><li>&quot;air&quot; includes other gases or gas mixtures and means always the gas to be heated;</li><li>&quot;furnace tubes&quot; means tubes inside the heater wherein combustion is performed;</li><li>&quot;fire tubes&quot; means tubes inside the heater through which flue-gases flow from a combustion chamber located outside the tubes;</li><li>&quot;heater&quot; means apparatus including both heat generating means and means for transferring the generated heat to water or air.</li></ul></li><li>All storage heaters are classified in group <b>F24H 7/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">WATER HEATERS</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">AIR HEATERS</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLUID HEATERS USING HEAT PUMPS</td><td><b>4/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINED WATER AND AIR HEATERS</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STORAGE HEATERS</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLUID HEATERS FOR EXTRACTING LATENT HEAT FROM FLUE GASES</td><td><b>8/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONTROL</td><td><b>15/00</b></td></p></tr></table>				
F24S		太陽熱集熱器；太陽熱システム（太陽熱から機械動力を生成するものＦ０３Ｇ６／００）［２０１８．０１］<br><br><b><ul>注</ul></b><br>このサブクラスでは，下記の用語または表現は以下に示す意味で用いる：<br>−「太陽熱集熱器モジュール」は，単に「モジュール」としばしば呼ばれるが，下記のものをカバーする；<br>　ａ．太陽熱集熱器全体；<br>　ｂ．太陽熱集熱器の要素，例．反射器，レンズまたは蓄熱要素<br>−「吸収要素」は，太陽光線を吸収し熱に変換する要素をカバーする。<br>−「太陽熱システム」は，構成部品として太陽熱集熱器を有し集めた熱を用いるシステムをカバーする。<br>	SOLAR HEAT COLLECTORS; SOLAR HEAT SYSTEMS (for producing mechanical power from solar energy <b>F03G 6/00</b>)<b>[2018.01]</b><br><br><b><u>Note(s)</u></b><br><br><ul style=""list-style:none""><li>In this subclass, the following terms or expressions are used with the meanings indicated:<b>[2018.01]</b><ul type=""disc""><li>&ldquo;solar heat collector modules&rdquo;, often referred to simply as &ldquo;modules&rdquo;, <u>covers</u>:<ul type=""a""><li>whole solar heat collectors;</li><li>elements of solar heat collectors, e.g. reflectors, lenses or heat storage elements;</li></ul></li><li>&ldquo;absorbing elements&rdquo; <u>covers</u> elements for absorbing solar rays and converting it into heat;</li><li>&ldquo;solar heat systems&rdquo; <u>covers</u> systems having solar heat collectors as their components and using the collected heat.</li></ul></li></ul>				
F24T		地熱集熱器；地熱システム［２０１８．０１］<br>	GEOTHERMAL COLLECTORS; GEOTHERMAL SYSTEMS<b>[2018.01]</b>				
F24V		他に分類されない熱の収集，生成または使用［２０１８．０１］<br>	COLLECTION, PRODUCTION OR USE OF HEAT NOT OTHERWISE PROVIDED FOR<b>[2018.01]</b>				
F25		冷凍または冷却；加熱と冷凍との組み合わせシステム；ヒートポンプシステム；氷の製造または貯蔵；気体の液化または固体化<br>	REFRIGERATION OR COOLING; COMBINED HEATING AND REFRIGERATION SYSTEMS; HEAT PUMP SYSTEMS; MANUFACTURE OR STORAGE OF ICE; LIQUEFACTION OR SOLIDIFICATION OF GASES				
F25B		冷凍機械，プラントまたはシステム；加熱と冷凍の組み合わせシステム；ヒート・ポンプ・システム［２００６．０１］<br><br><b><ul>注</ul></b><br>サブクラスＦ２４Ｆのタイトルに続く注（２）に注意すること。［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>作動の様式<br>圧縮式<br>サイクルに特徴のあるもの　１／００，１３／００<br>配列に特徴のあるもの<br>自納式回転形のもの；数個の蒸発器回路をもつもの；数個の凝縮器回路をもつもの；カスケード式によるもの　３／００；５／００；６／００；７／００<br>冷媒に特徴のあるもの　９／００<br>タービンを用いるもの　１１／００<br>収着式　１５／００，１７／００<br>単一の作動様式をもつ他の形式のもの；回収を行なわない蒸発を用いたもの；電気または磁気効果を用いたもの；その他の効果を用いたもの　１９／００；２１／００；２３／００<br>組み合わせ；上記の作動様式の組み合わせ；加熱と冷凍との組み合わせ　２５／００；２９／００<br>ヒートポンプ　３０／００<br>特殊なエネルギ源を用いるもの　２７／００<br>細部，配置または部品<br>部分品；ボイラ，アナライザ，精溜器；吸収式機械用ボイラ；吸収器，吸着器；蒸発器，凝縮器；過冷却器，デスーパーヒータ，スーパーヒータ　３３／００；３５／００；３７／００；３９／００；４０／００<br>配置<br>圧縮機の配置；流体の循環；気体の分離または不純物除去　３１／００；４１／００；４３／００<br>冷媒の充填または排出のためのもの；腐食または付着物の対策のためのもの　４５／００；４７／００<br>制御および安全装置の取り付け　４９／００<br>	REFRIGERATION MACHINES, PLANTS OR SYSTEMS; COMBINED HEATING AND REFRIGERATION SYSTEMS; HEAT PUMP SYSTEMS<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MODE OF OPERATION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Compression type</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">characterised by the cycle</td><td><b>1/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">characterised by the arrangement</td><tr><td width="70%"><p style=""text-indent:4em;margin:0"">self-contained rotary; with several evaporation circuits; with several condenser circuits; with cascade operation</td><td><b>3/00</b>; <b>5/00</b>; <b>6/00</b>; <b>7/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">characterised by the refrigerant</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">using turbines</td><td><b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Sorption type</td><td><b>15/00</b>, <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other types having a single mode of operation, using: evaporation without recovery; electric or magnetic effects; other effect</td><td><b>19/00</b>; <b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations: of above modes of operation; of heating and refrigerating</td><td><b>25/00</b>; <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Heat pumps</td><td><b>30/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using special energy source</td><td><b>27/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS, ARRANGEMENTS, OR COMPONENTS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Components: boilers, analysers, rectifiers; boiler-absorbers; absorbers, adsorbers; evaporators, condensers; subcoolers, desuper- heaters, superheaters</td><td><b>33/00</b>; <b>35/00</b>; <b>37/00</b>; <b>39/00</b>; <b>40/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">compressor arrangement; fluid circulation; separating or purifying gases</td><td><b>31/00</b>; <b>41/00</b>; <b>43/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for charging or discharging refrigerant; for combating corrosion or deposits</td><td><b>45/00</b>; <b>47/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Mounting of control and safety devices</td><td><b>49/00</b></td></p></tr></p></tr></table>				
F25C		氷の製造，作業または取扱い［２］<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“氷”はあらゆる凍結した液体を意味し，また凍結した半液体状またはペースト状の物質をも含む。［２］<br>	PRODUCING, WORKING OR HANDLING ICE<b>[2]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this subclass, the following term is used with the meaning indicated:<b>[2]</b><ul type=""disc""><li>&quot;ice&quot; means any frozen liquid and also covers frozen semiliquids or pasty substances.</li></ul></li></ul>				
F25D		冷蔵庫，冷凍室，アイス・ボックス，他に包含されない冷蔵または冷凍器具（冷凍ショーケースＡ４７Ｆ３／０４；家庭用断熱容器Ａ４７Ｊ４１／００；冷凍車は，クラスＢ６０からＢ６４の適当なサブクラスを参照；断熱容器一般Ｂ６５Ｄ８１／３８；伝熱，熱交換，または蓄熱用物質，例．冷却剤；あるいは燃焼以外の化学反応によって熱または冷気を発生させる物質Ｃ０９Ｋ５／００；液化または固体化ガス用断熱容器Ｆ１７Ｃ；空気調節または空気加湿Ｆ２４Ｆ；冷凍機械，プラントまたはシステムＦ２５Ｂ；機器または同様の器具を，冷凍しないで，冷却するものＧ１２Ｂ）<br><br><b><ul>注</ul></b><br>（１）冷凍機械と関連する装置はグループ１１／００から１６／００に分類する。［２００９．０１］<br>（２）このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“装置”は冷却されるべき閉鎖空間を意味する；このような装置は冷凍機械または他の冷却源と関連する。前者の例としては冷蔵庫があげられ，後者の例としてはアイスボックスがあげられる。<br>（３）サブクラスＦ２４Ｆのタイトルの後の注（２）に注意すること。［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>冷凍機械と関連しない装置<br>冷空気または冷水を用いるもの；他の低温物質または蓄冷材　１／００；３／００<br>吸熱化学反応または回収しない蒸気を用いるもの　５／００，７／００<br>他の装置，組み合わせ　９／００<br>冷凍機械と関連した装置：冷凍機械内蔵可動式；固定式；その他　１１／００；１３／００；１５／００<br>　冷凍機械と関連しない冷却方式との組み合わせ　１６／００<br>構造的な部品および配置，一般的な適用：除霜；一般的な構造；冷却される物品の取り扱い　２１／００；２３／００；２５／００<br>冷却流体または気体の循環；照明　１７／００；２７／００<br>冷凍ユニットの配置と取り付け；制御および安全装置の配置と取り付け　１９／００；２９／００<br>他の器具　３１／００<br>	REFRIGERATORS; COLD ROOMS; ICE-BOXES; COOLING OR FREEZING APPARATUS NOT OTHERWISE PROVIDED FOR (refrigerated showcases <b>A47F 3/04</b>; thermally-insulated vessels for domestic use <b>A47J 41/00</b>; refrigerated vehicles, see the appropriate subclasses of classes <b>B60-B64</b>; containers with thermal insulation in general <b>B65D 81/38</b>; heat-transfer, heat-exchange or heat-storage materials, e.g. refrigerants, or materials for the production of heat or cold by chemical reactions other than by combustion <b>C09K 5/00</b>; thermally-insulated vessels for liquefied or solidified gases <b>F17C</b>; air-conditioning or air-humidification <b>F24F</b>; refrigeration machines, plants, or systems <b>F25B</b>; cooling of instruments or comparable apparatus without refrigeration <b>G12B</b>)<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Devices associated with refrigerating machinery are classified in groups <b>F25D 11/00-F25D 16/00</b>.<b>[5,2009.01]</b></li><li>In this subclass, the following term is used with the meaning indicated:<ul type=""disc""><li>&quot;device&quot; means an enclosed space to be cooled; such devices being associated either with refrigerating machinery, e.g. in a refrigerator, or with other cold sources, e.g. in an ice-box.</li></ul></li><li>Attention is drawn to Note (2) following the title of subclass <b>F24F</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DEVICES NOT ASSOCIATED WITH REFRIGERATING MACHINERY</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using cold air or water; other cold materials or bodies</td><td><b>1/00</b>; <b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Using endothermic chemical reactions, or evaporation without recovery</td><td><b>5/00</b>, <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other devices, combinations</td><td><b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DEVICES ASSOCIATED WITH REFRIGERATING MACHINERY: SELF-CONTAINED MOVABLE; STATIONARY; OTHER</td><td><b>11/00</b>; <b>13/00</b>; <b>15/00</b></td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">In combination with a cooling mode not associated with refrigerating machinery</td><td><b>16/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STRUCTURAL PARTS OR ARRANGEMENTS, OF GENERAL APPLICATION: DEFROSTING; GENERAL FEATURES; HANDLING OF ARTICLES TO BE COOLED</td><td><b>21/00</b>; <b>23/00</b>; <b>25/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CIRCULATING COOLING FLUID OR GAS; LIGHTING</td><td><b>17/00</b>; <b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARRANGEMENT OR MOUNTING: OF REFRIGERATION UNITS; OF CONTROL OR SAFETY DEVICES</td><td><b>19/00</b>; <b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER APPARATUS</td><td><b>31/00</b></td></p></tr></table>				
F25J		気体または気体混合物の加圧および冷却処理による液化，凝固または分離（極低温ポンプＦ０４Ｂ３７／０８；気体貯蔵容器，ガスタンクＦ１７；液化または固化ガスの注入または気化Ｆ１７Ｃ；冷凍機械，プラントまたはシステムＦ２５Ｂ）<br>	LIQUEFACTION, SOLIDIFICATION, OR SEPARATION OF GASES OR GASEOUS MIXTURES BY PRESSURE AND COLD TREATMENT (cryogenic pumps <b>F04B 37/08</b>; gas storage vessels, gas-holders <b>F17</b>; filling vessels with, or discharging from vessels, compressed, liquefied, or solidified gases <b>F17C</b>; refrigeration machines, plants, or systems <b>F25B</b>)				
F26		乾燥<br>	DRYING				
F26B		固体材料または固形物から液体を除去することによる乾燥（コンバインの乾燥装置Ａ０１Ｄ４１／１３３；果物または野菜の乾燥棚Ａ０１Ｆ２５／１２；食品の乾燥Ａ２３；頭髪の乾燥Ａ４５Ｄ２０／００；身体の乾燥用具Ａ４７Ｋ１０／００；家庭用具の乾燥Ａ４７Ｌ；ガスまたは蒸気の乾燥Ｂ０１Ｄ；脱水または固体からの液体の類似の分離のための化学的あるいは物理的プロセスＢ０１Ｄ４３／００；遠心分離装置Ｂ０４；セラミックの乾燥Ｃ０４Ｂ３３／３０；他の処理と関連した織り糸または織物の乾燥Ｄ０６Ｃ；加熱または強制空気循環のない洗たく物の乾燥枠，家庭用洗たく物乾燥機または遠心脱水機，洗たく物の搾水または熱プレスＤ０６Ｆ；炉，キルン，オーブンＦ２７）<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>乾燥プロセス<br>予備処理　１／００<br>プロセス；加熱を伴なうもの；加熱を伴なわないもの；両者の結合によるもの　３／００；５／００；７／００<br>乾燥のための機械または装置<br>静止してまたは部分的に振り動かして乾燥する物品を有するもの，家庭用の空気乾燥装置　９／００<br>非前送り運動をするもの　１１／００<br>前送り運動をするもの：織物または織糸に適したもの；物品およびひとかたまりの材料に適したもの；ひとかたまりになっていない材料に適したもの　１３／００；１５／００；１７／００<br>その他のもの　１９／００<br>上記のものの２以上を結合したもの　２０／００<br>一般に応用される装置または細部<br>乾燥用空気または他のガスのための装置；加熱　２１／００；２３／００<br>その他の細部　２５／００<br>	DRYING SOLID MATERIALS OR OBJECTS BY REMOVING LIQUID THEREFROM (drying devices for combines <b>A01D 41/133</b>; racks for drying fruit or vegetables <b>A01F 25/12</b>; drying foodstuffs <b>A23</b>; drying hair <b>A45D 20/00</b>; body-drying implements <b>A47K 10/00</b>; drying household articles <b>A47L</b>; drying gases or vapours <b>B01D</b>; chemical or physical processes for dewatering or like separating liquids from solids <b>B01D 43/00</b>; centrifugal apparatus <b>B04</b>; drying ceramics <b>C04B 33/30</b>; drying yarns or fabrics in association with some other form of treatment <b>D06C</b>; drying frames for laundry without heating or positive air circulation, domestic laundry-or spin-driers, wringing or hot pressing laundry <b>D06F</b>; furnaces, kilns, ovens <b>F27</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PROCESSES FOR DRYING</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Preliminary treatment</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Processes: with heat; without heat; by combination of both types</td><td><b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MACHINES OR APPARATUS FOR DRYING</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With articles to be dried at rest or locally agitated, domestic airing</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With non-progressive movement</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With progressive movement: for fabrics or yarns; for articles and compact batches; for material not in compact batches</td><td><b>13/00</b>; <b>15/00</b>; <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other kinds</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combinations using at least two of the above kinds</td><td><b>20/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARRANGEMENTS OR DETAILS OF GENERAL APPLICATIONS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Arrangements for air or other gases for drying; heating</td><td><b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other details</td><td><b>25/00</b></td></p></tr></p></tr></table>				
F27		炉；キルン，窯（かま）またはレトルト［４］<br><br><b><ul>注</ul></b><br>（１）このクラスは以下のものを包含する：<br>―炉，キルン，窯，レトルト，解放式焼結用装置，および材料または物品の熱処理をするための同様の装置，ならびに細部または付属物一般の配置；<br>―炉中または炉上の電熱要素の配列<br>（２）このクラスは以下のものは包含しない：<br>―燃焼装置それ自体，すなわち酸素ガスと可燃物質を直接燃焼する装置；［７］<br>―電熱要素それ自体；<br>―炉の内部で行なわれるプロセス。<br>（３）このクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“炉”はキルン，窯およびレトルトを包含する。<br>	FURNACES; KILNS, OVENS OR RETORTS<b>[4]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This class <u>covers</u>:<b>[7]</b><ul type=""disc""><li>furnaces, kilns, ovens, retorts, open sintering apparatus and other similar apparatus for heat treatment of materials or articles, and details or accessories therefor, in general;</li><li>the arrangement of electrical heating elements in or on furnaces.</li></ul></li><li>This class <u>does not cover</u>:<ul type=""disc""><li>combustion apparatus <u>per se</u>, i.e. apparatus for direct combination of oxygen gas and a burnable substance;</li><li>electrical heating elements <u>per se</u>;</li><li>processes carried on within the furnaces.</li></ul></li><li>In this class, the following term is used with the meaning indicated:<ul type=""disc""><li>&quot;furnaces&quot; covers kilns, ovens, or retorts.</li></ul></li></ul>				
F27B		炉，キルン，窯またはレトルト一般；開放式焼結用または類似の装置［２００６．０１］<br><br><b><ul>注</ul></b><br>クラスＦ２７のタイトルに続く注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>定置された装入物をもつ炉<br>竪形炉　１／００<br>横形炉　３／００，５／００<br>鐘形炉　１１／００<br>加熱が前進するもの　１３／００<br>るつぼ形炉，タンク炉　１４／００<br>装入物が機械的に移動する定置炉　９／００<br>回転炉　７／００，１３／００<br>その他の炉；組み合わせたもの　１５／００，１７／００；１９／００<br>開放式焼結用または類似の装置　２１／００<br>	FURNACES, KILNS, OVENS OR RETORTS IN GENERAL; OPEN SINTERING OR LIKE APPARATUS<br><br><b><u>Note(s)</u></b><br><br><ul style=""list-style:none""><li>Attention is drawn to the Notes following the title of class <b>F27</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FURNACES WITH STATIONARY CHARGE</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Shaft furnaces</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Horizontal furnaces</td><td><b>3/00</b>, <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Bell-type furnaces</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With progression of heating</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Crucible furnaces, tank furnaces</td><td><b>14/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STATIONARY FURNACES WITH MECHANICALLY-MOVED CHARGE</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROTARY FURNACES</td><td><b>7/00</b>, <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER FURNACES; COMBINATIONS</td><td><b>15/00</b>, <b>17/00</b>; <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OPEN SINTERING OR LIKE APPARATUS</td><td><b>21/00</b></td></p></tr></table>				
F27D		２種以上の炉に見出される種類のものである限りにおける，炉，キルン，窯またはレトルトの細部または付属品<br><br><b><ul>注</ul></b><br>クラスＦ２７のタイトルに続く注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>構造上の特徴　　Ｆ２７Ｄ　　１／００　　　　　　　　　　　　　　<br>装入物の取り扱いまたは支持　　Ｆ２７Ｄ　　３／００，　　Ｆ２７Ｄ　　５／００，　　Ｆ２７Ｄ　　１５／００　　　　　　　　　　　　　　<br>装入物の予熱；冷却；廃熱または廃ガス利用　　Ｆ２７Ｄ　　１３／００；　　Ｆ２７Ｄ　　９／００，　　Ｆ２７Ｄ　　１５／０２；　　Ｆ２７Ｄ　　１７／００　　　　　　　　　　　　　　<br>電気加熱の要素の配置　　Ｆ２７Ｄ　　１１／００　　　　　　　　　　　　　　<br>制御，　　監視または安全装置の配置　　Ｆ２７Ｄ　　１９／００，　　Ｆ２７Ｄ　　２１／００　　　　　　　　<br>その他の特徴；他の細部　　Ｆ２７Ｄ　　７／００；　　Ｆ２７Ｄ　　２５／００，　　Ｆ２７Ｄ　　２７／００，　　Ｆ２７Ｄ　　９９／００<br>	DETAILS OR ACCESSORIES OF FURNACES, KILNS, OVENS OR RETORTS, IN SO FAR AS THEY ARE OF KINDS OCCURRING IN MORE THAN ONE KIND OF FURNACE<br><br><b><u>Note(s)</u></b><br><br><ul style=""list-style:none""><li>Attention is drawn to the Notes following the title of class <b>F27</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CONSTRUCTIONAL FEATURES</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">HANDLING OR SUPPORTING THE CHARGE</td><td><b>3/00</b>, <b>5/00</b>, <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PREHEATING CHARGES; COOLING; USING WASTE HEAT OR WASTE GASES</td><td><b>13/00</b>; <b>9/00</b>, <b>15/02</b>; <b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARRANGEMENT OF ELECTRIC HEATING ELEMENTS</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARRANGEMENT OF CONTROL, MONITORING OR SAFETY DEVICES</td><td><b>19/00</b>, <b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER FEATURES; OTHER DETAILS</td><td><b>7/00</b>; <b>25/00</b>, <b>27/00</b>, <b>99/00</b></td></p></tr></table>				
F28		熱交換一般<br><br><b><ul>注</ul></b><br>（１）このクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“熱交換”とは，加熱または冷却流体または流動固体との直接または間接の接触によって，流体または流動固体を加熱または冷却することを意味する；<br>―“熱伝達”とは，加熱または冷却された表面または物体との直接接触によって，流体または流動固体を加熱または冷却することを意味する。<br>（２）熱交換または熱伝達（注（１）に規定されているような）を特別な目的に対して用いる装置は，サブクラスＦ２８Ｂ，または，たとえばクラスＦ２２，Ｆ２４，Ｆ２５，Ｆ２６またはＦ２７内の適当なサブクラスに分類される；これらのサブクラスが適当でない場合には，そのような装置は，Ｆ２８ＣまたはＤに分類される。<br>	HEAT EXCHANGE IN GENERAL<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>In this class, the following expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;heat exchange&quot; means the heating or cooling of a fluid or fluent solid by direct or indirect contact with a heated or cooled fluid or fluent solid;</li><li>&quot;heat transfer&quot; means the heating or cooling of a fluid or fluent solid by direct contact with a heated or cooled surface or body.</li></ul></li><li>Apparatus using heat exchange or heat transfer (as defined in Note (1) above) for specific purposes is classified either in subclass <b>F28B</b> or in the appropriate subclasses of, for example, classes <b>F22</b>, <b>F24</b>, <b>F25</b>, <b>F26</b>, or <b>F27</b>; if no such other subclass is appropriate, such apparatus is classified in subclass <b>F28C</b> or <b>F28D</b>.</li></ul>				
F28B		水蒸気または蒸気凝縮器（蒸気の凝縮Ｂ０１Ｄ５／００；分散粒子の静電沈降に先立つ気体の前処理中の凝縮Ｂ０３Ｃ３／０１４；凝縮器をもつ蒸気機関プラントＦ０１Ｋ；気体の液化Ｆ２５Ｊ；熱交換または熱伝達装置の細部一般Ｆ２８Ｆ）<br>	STEAM OR VAPOUR CONDENSERS (condensation of vapours <b>B01D 5/00</b>; condensation during pretreatment of gases prior to electrostatic precipitation of dispersed particles <b>B03C 3/014</b>; steam engine plants having condensers <b>F01K</b>; liquefaction of gases <b>F25J</b>; details of heat-exchange or heat-transfer arrangements of general application <b>F28F</b>)				
F28C		熱交換媒体が相互に化学作用を行なわずに直接接触する熱交換装置で，他のサブクラスに分類されないもの（伝熱，熱交換，または蓄熱用物質Ｃ０９Ｋ５／００；熱発生手段をもつ流体加熱器Ｆ２４Ｈ；熱交換媒体と直接接触を行なう中間熱伝達媒体をもつものＦ２８Ｄ１５／００〜Ｆ２８Ｄ１９／００；一般に使用される熱交換装置の細部Ｆ２８Ｆ）<br>	HEAT-EXCHANGE APPARATUS, NOT PROVIDED FOR IN ANOTHER SUBCLASS, IN WHICH THE HEAT-EXCHANGE MEDIA COME INTO DIRECT CONTACT WITHOUT CHEMICAL INTERACTION (heat-transfer, heat-exchange or heat-storage materials <b>C09K 5/00</b>;  fluid heaters having heat generating means <b>F24H</b>; with an intermediate heat-transfer medium coming into direct contact with heat-exchange media <b>F28D 15/00-F28D 19/00</b>; details of heat-exchange apparatus of general application <b>F28F</b>)				
F28D		熱交換媒体が直接接触しない熱交換装置で，他のサブクラスに分類されないもの（伝熱，熱交換，または蓄熱用物質Ｃ０９Ｋ５／００；熱発生手段または熱伝達手段をもつ流体加熱器Ｆ２４Ｈ；炉Ｆ２７；一般用の熱交換装置の細部Ｆ２８Ｆ）；蓄熱プラントまたは装置一般［４］<br><br><b><ul>サブクラス内の索引</ul></b><br>中間熱伝達媒体または物質をもたない熱交換装置<br>不動の流路群をもつもの<br>ただ一つの媒体を用いるためのもの：流体の量；散水または薄膜；蒸発の冷却効果　１／００；３／００；５／００<br>両媒体のためのもの：管状の流路によるもの；板状の流路によるもの　７／００；９／００<br>可動流路群をもつもの　１１／００<br>流動床をもつもの　１３／００<br>中間熱伝達媒体または物質をもつ熱交換装置<br>中間媒体をもつ閉鎖した管中の流路壁を通り抜けるもの　１５／００<br>中間媒体が他の媒体と相い次いで接触をするもの　１７／００，１９／００<br>蓄熱プラントまたは装置　２０／００<br>その他の熱交換装置　２１／００<br>	HEAT-EXCHANGE APPARATUS, NOT PROVIDED FOR IN ANOTHER SUBCLASS, IN WHICH THE HEAT-EXCHANGE MEDIA DO NOT COME INTO DIRECT CONTACT (heat-transfer, heat-exchange or heat-storage materials <b>C09K 5/00</b>;  fluid heaters having heat generating means and heat transferring means <b>F24H</b>; furnaces <b>F27</b>; details of heat-exchange apparatus of general application <b>F28F</b>); HEAT STORAGE PLANTS OR APPARATUS IN GENERAL<b>[4]</b><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">HEAT-EXCHANGE APPARATUS WITHOUT INTERMEDIATE HEAT-TRANSFER MEDIA OR BODIES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With stationary conduit assemblies</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for only one medium using: mass of fluid; trickle or film; the cooling effect of evaporation</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">for both media: by tubular conduits; by plate-like conduits</td><td><b>7/00</b>; <b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With moving conduit assemblies</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With fluidised bed</td><td><b>13/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">HEAT-EXCHANGE APPARATUS WITH INTERMEDIATE HEAT-TRANSFER MEDIA OR BODIES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">With the intermediate medium in closed tubes passing into or through the conduit walls</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">In which the intermediate medium or body is contacted successively by the other media</td><td><b>17/00</b>, <b>19/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">HEAT STORAGE PLANTS OR APPARATUS</td><td><b>20/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER HEAT-EXCHANGE APPARATUS</td><td><b>21/00</b></td></p></tr></table>				
F28F		一般的な用途の，熱交換または熱伝達装置の細部（伝熱，熱交換，または蓄熱用物質Ｃ０９Ｋ５／００；水または空気トラップ，空気抜きＦ１６）<br><br><b><ul>サブクラス内の索引</ul></b><br>細部およびその配置<br>熱交換または伝達の要素およびその組み立て<br>管状；板状；運動用；その他　１／００；３／００；５／００；７／００<br>要素の補助支持；密封　９／００；１１／００<br>外箱および管寄せ箱　９／００<br>沈積または腐食の予防　１７／００，１９／００<br>熱交換装置の特性<br>選択に特徴のあるもの：構成材料；中間熱交換物質　２１／００；２３／００<br>散水式冷却器の構成要素　２５／００<br>熱伝達の修正；装置の制御　１３／００；２７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００［８］<br>	DETAILS OF HEAT-EXCHANGE OR HEAT-TRANSFER APPARATUS, OF GENERAL APPLICATION (heat-transfer, heat-exchange or heat-storage materials <b>C09K 5/00</b>; water or air traps, air venting <b>F16</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">DETAILS AND THEIR ARRANGEMENTS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Elements for heat exchange or transfer and assemblies thereof</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">tubular; plate-like; for movement; others</td><td><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">auxiliary supports for elements; sealing</td><td><b>9/00</b>; <b>11/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Casings and header boxes</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Preventing deposits or corrosion</td><td><b>17/00</b>, <b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Special features of heat-exchange apparatus</td><tr><td width="70%"><p style=""text-indent:3em;margin:0"">characterised by the selection of: constructional material; intermediate heat-exchange material</td><td><b>21/00</b>; <b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:3em;margin:0"">component parts of trickle coolers</td><td><b>25/00</b></td></p></tr></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MODIFYING HEAT-TRANSFER; CONTROL OF APPARATUS</td><td><b>13/00</b>; <b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F28G		熱交換管または熱伝達管，例．ボイラの水管，の内面または外面の清掃（パイプまたはチューブの清掃一般Ｂ０８Ｂ９／０２；ボイラが作動中にボイラから水，無機物，またはスラッジを除去する機器または装置，またはボイラが運転されている間所定位置にとどまる同上の機器または装置，または他のどのような効用も伴わないボイラーに特に適用された同上の機器または装置Ｆ２２Ｂ３７／４８；燃焼生成物または燃焼残滓の除去または処理Ｆ２３Ｊ；熱交換装置からの氷の除去Ｆ２８Ｆ１７／００）<br><br><b><ul>サブクラス内の索引</ul></b><br>清掃の機器：非回転；回転；その他；細部　１／００；３／００；１３／００；１５／００<br>清掃の方法：ねじり；振動；フラッシングまたは洗浄；燃焼によるもの；その他　５／００；７／００；９／００；１１／００；１３／００<br>方法の組み合わせ　１３／００<br>	CLEANING OF INTERNAL OR EXTERNAL SURFACES OF HEAT-EXCHANGE OR HEAT-TRANSFER CONDUITS, e.g. WATER TUBES OF BOILERS (cleaning pipes or tubes in general <b>B08B 9/02</b>; devices or arrangements for removing water, minerals, or sludge from boilers while the boiler is in operation, or which remain in position while the boiler is in operation, or are specifically adapted to boilers without any other utility <b>F22B 37/48</b>; removal or treatment of combustion products or combustion residues <b>F23J</b>; removing ice from heat-exchange apparatus <b>F28F 17/00</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">APPLIANCES FOR CLEANING: NON-ROTARY; ROTARY; OTHERS; DETAILS</td><td><b>1/00</b>; <b>3/00</b>; <b>13/00</b>; <b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CLEANING PROCESSES BY: DISTORTION; VIBRATION; FLUSHING OR WASHING; COMBUSTION; OTHERS</td><td><b>5/00</b>; <b>7/00</b>; <b>9/00</b>; <b>11/00</b>; <b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMBINATION OF PROCESSES</td><td><b>13/00</b></td></p></tr></table>				
F41		武器<br><br><b><ul>注</ul></b><br>（１）シミュレータは一般にクラスＧ０９に包含されるが，このクラスはシミュレーションの特徴を有する，例．いわゆる“机上軍事演習”用の装置におけるような，演習および訓練のための装置も包含する。［４］<br>（２）このクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“小火器”は一般に発射のため片手または両手で保持される火器を意味するが，この用語は発射中三脚台または類似物上に支持される軽機関銃も含む；［５］<br>―“銃”は飛しょう体を発射するための砲身および引金または発射機構をもつすべての武器を意味する；それは砲または小火器の一部でありうる。それは燃焼性または爆発性推進装薬，空気圧，電磁気または他の推進力を使用しうる；［５］<br>―“リボルバ型銃”は，薬室として継続的に使用される回転するドラム型の弾倉を有する銃を意味する；［５］<br>―“リボルバ”はリボルバ型銃を意味する。［５］<br>―“半自動火器”は，引金が作動して弾丸が発射されると，次の弾丸が発射できるように，引金が再び作動状態になる火器を意味する；<br>―“自動火器”は最初の発射圧力が引金にかかっている間は発射を続ける火器を意味する；<br>―“照準”は，いわゆる“照準”器によって定められた方向と目標の方向とを視覚的に一致させることを意味する；<br>―“照準合わせ”は発射体が目標に命中するように，武器の照準方向を修正することを意味する；<br>―“照準する”とは目標に命中するように武器を正しい位置に定めることを意味する。<br>（３）クラスＦ４２のタイトルの後の注（２）に記載されている“発射体”，“飛しょう体”，および“ロケット”の定義に注意すること。［４］<br>	WEAPONS<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This class <u>covers</u> also means for practice and training which may have aspects of simulation, e.g. in apparatus for so-called &quot;military games&quot;, although simulators are generally covered by class <b>G09</b>.<b>[4,5]</b></li><li>In this class, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;smallarm&quot; means a firearm which is generally held with one or both hands for firing, but this term also includes a light machine-gun which may be supported on a tripod or the like during firing;</li><li>&quot;gun&quot; means any weapon having a barrel and a trigger or firing mechanism for projecting a missile; it may be a piece of ordnance or a smallarm. It may use combustible or explosive propellant charges, air pressure, electromagnetism or other propulsive forces;</li><li>&quot;revolver-type gun&quot; means a gun having a revolving drum magazine, the chambers of which are used successively as firing chamber;</li><li>&quot;revolver&quot; means a revolver-type pistol;</li><li>&quot;semi-automatic firearm&quot; means a firearm from which one shot is fired after actuation of the trigger and which then returns to a condition for firing a subsequent shot upon renewed actuation of the trigger;</li><li>&quot;automatic firearm&quot; means a firearm which will continue firing so long as the initial firing pressure is maintained on the trigger;</li><li>&quot;sighting&quot; means bringing into visual coincidence a direction defined by a so-called &quot;sighting&quot; device with the direction of a target;</li><li>&quot;aiming&quot; means bringing a weapon to a direction differing from the sighting direction by corrections in order that the projectile may hit the target;</li><li>&quot;laying&quot; means setting a weapon in the correct position for hitting a target.</li></ul></li><li>Attention is drawn to the definitions of &quot;projectile&quot;, &quot;missile&quot; and &quot;rocket&quot; given in Note (2) following the title of class <b>F42</b>.</li></ul>				
F41A		小火器と砲，例．大砲；に共通の機能的特徴または細部；小火器架または砲架［５］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは小火器および砲の両方に一般に適用しうる形式であると考えられる，または共通する固有の機能に関係すると考えられる特徴または細部を包含する。［５］<br>（２）このような特徴または細部は，たとえそれらが小火器にのみまたは砲にのみ適用されると述べていても，このサブクラスに分類される。［５］<br>（３）クラスＦ４１のタイトルの後の注（２）に記載されている定義に注意すること。［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>推進の形式　１／００<br>銃尾栓機構　３／００<br>閉鎖解放機構　５／００<br>銃の再装てん，外部に動力を備えた銃　７／００<br>給弾または装てん，弾倉　９／００<br>組み立ての特徴，モジュールの概念，連結式または折りたたみ式銃　１１／００<br>冷却，加熱，換気，吹出し　１３／００<br>抽筒子，蹴子　１５／００<br>安全装置　１７／００<br>発射または引金機構，撃鉄起こし　１９／００<br>砲身，銃身，銃砲口取付具　２１／００<br>砲架，例．車両上　２３／００<br>後座できるもの　２５／００<br>俯仰または旋回できるもの　２７／００<br>清掃または潤滑　２９／００<br>試験　３１／００<br>訓練への適用　３３／００<br>その他の付属具または細部　３５／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	FUNCTIONAL FEATURES OR DETAILS COMMON TO BOTH SMALLARMS AND ORDNANCE, e.g. CANNONS; MOUNTINGS FOR SMALLARMS OR ORDNANCE<b>[5]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> those features or details which are considered to be of a kind generally applicable to, or to be concerned with intrinsic functions common to, both smallarms and ordnance.<b>[5]</b></li><li>Such features or details are classified in this subclass, even if they are stated to be applied only to smallarms or only to ordnance.</li><li>Attention is drawn to the definitions given in Note (2) following the title of class <b>F41</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">KINDS OF PROPULSION</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BREECH MECHANISMS</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">UNLOCKING MECHANISMS</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GUN RECHARGERS, EXTERNALLY POWERED GUNS</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FEEDING OR LOADING, MAGAZINES</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ASSEMBLY FEATURES, MODULAR CONCEPTS, ARTICULATED OR COLLAPSIBLE GUNS</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COOLING, HEATING, VENTILATING, BLOWING TROUGH</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">EXTRACTORS, EJECTORS</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SAFETY ARRANGEMENTS</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FIRING OR TRIGGER MECHANISMS, COCKING</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BARRELS, GUN TUBES, MUZZLE ATTACHMENTS</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GUN MOUNTINGS, e.g. on vehicles</td><td><b>23/00</b></td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Permitting recoil</td><td><b>25/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Permitting elevation or traversing</td><td><b>27/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CLEANING OR LUBRICATING</td><td><b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TESTING</td><td><b>31/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ADAPTATIONS FOR TRAINING</td><td><b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER ACCESSORIES OR DETAILS</td><td><b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F41B		爆発性または燃焼性推進装薬を用いない飛しょう体発射用武器；他に分類されない武器（漁撈用の発射体，例．やす，Ａ０１Ｋ８１／００；投てきスポーツ用具Ａ６３Ｂ６５／００，例．ブーメランＡ６３Ｂ６５／０８；据えつけられたスポーツ投球，例．テニスボール装置，Ａ６３Ｂ６９／４０；投射または投射玩具Ａ６３Ｈ３３／１８；ナイフ，斧Ｂ２６Ｂ；発射手段としてばねを組込まない発射体または飛しょう体Ｆ４２Ｂ６／００）<br><br><b><ul>サブクラス内の索引</ul></b><br>吹矢筒　１／００<br>なげとばす武器　３／００<br>摩擦車によるランチャ　４／００<br>弓，十字弓　５／００<br>電磁気式ランチャ　６／００<br>ばね銃　７／００<br>液圧銃，例．水鉄砲　Ｆ４１Ｂ９／００<br>圧縮ガス銃，蒸気銃　Ｆ４１Ｂ１１／００<br>突く武器，着装武器として装着される武器Ｆ４１Ｂ１３／００<br>その他の武器　１５／００<br>	WEAPONS FOR PROJECTING MISSILES WITHOUT USE OF EXPLOSIVE OR COMBUSTIBLE PROPELLANT CHARGE; WEAPONS NOT OTHERWISE PROVIDED FOR (projectiles for fishing, e.g. fish-spears, <b>A01K 81/00</b>;  sports implements for throwing <b>A63B 65/00</b>, e.g. boomerangs <b>A63B 65/08</b>;  stationary apparatus for projecting sports balls, e.g. tennis balls, <b>A63B 69/40</b>;  throwing or slinging toys <b>A63H 33/18</b>; knives, axes <b>B26B</b>;  projectiles or missiles other than those incorporating springs as projecting means <b>F42B 6/00</b>)<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BLOW GUNS</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SLING WEAPONS</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FRICTION-WHEEL OPERATED LAUNCHERS</td><td><b>4/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BOWS, CROSSBOWS</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ELECTROMAGNETIC LAUNCHERS</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SPRING GUNS</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LIQUID PRESSURE GUNS, e.g. WATER PISTOLS</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">COMPRESSED-GAS GUNS, STEAM GUNS</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">THRUSTING WEAPONS, CUTTING WEAPONS CARRIED AS SIDE-ARMS</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER WEAPONS</td><td><b>15/00</b></td></p></tr></table>				
F41C		小火器，例．ピストルまたはライフル銃（爆発性または燃焼性推進装薬を用いないで飛しょう体を投射するものＦ４１Ｂ）；そのための付属具［５］<br><br><b><ul>注</ul></b><br>クラスＦ４１のタイトルの後の注（２）における定義に注意すること。［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>小火器の種類<br>ピストル，リボルバ　３／００<br>肩持ち小火器　７／００<br>他の小火器，例．隠ぺい，先込め，水中　９／００<br>床尾，床尾板，銃床　２３／００<br>付属具；他の細部　２７／００<br>装着または運搬手段　３３／００<br>	SMALLARMS, e.g. PISTOLS OR RIFLES (projecting missiles without use of explosive or combustible propellant charge <b>F41B</b>); ACCESSORIES THEREFOR<b>[5]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>Attention is drawn to the definitions in Note (2) following the title of class <b>F41</b>.<b>[5]</b></li></ul><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">KINDS OF SMALLARMS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Pistols, revolvers</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Shoulder-fired smallarms</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Other smallarms, e.g. hidden, muzzle-loaded, underwater</td><td><b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BUTTS, BUTT PLATES, STOCKS</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ACCESSORIES; OTHER DETAILS</td><td><b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">WEARING OR CARRYING-MEANS</td><td><b>33/00</b></td></p></tr></table>				
F41F		砲身からの発射体または飛しょう体発射装置，例．大砲（小火器Ｆ４１Ｃ）；ロケットまたは魚雷ランチャ；もり打ち砲（小火器および砲の両方に共通する機能的特徴または細部，そのための取付けＦ４１Ａ；爆発性または燃焼性推進装薬を用いない飛しょう体の発射Ｆ４１Ｂ）［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>砲身からの発射　１／００<br>ロケットまたは魚雷ランチャ　３／００<br>重力推進の発射体または飛しょう体の発射　５／００<br>他の発射装置　７／００<br>	APPARATUS FOR LAUNCHING PROJECTILES OR MISSILES FROM BARRELS, e.g. CANNONS (smallarms <b>F41C</b>); LAUNCHERS FOR ROCKETS OR TORPEDOES; HARPOON GUNS (functional features or details common to both smallarms and ordnance, mountings therefor <b>F41A</b>; projecting missiles without use of explosive or combustible propellant charge <b>F41B</b>)<b>[5]</b><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LAUNCHING FROM BARRELS</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ROCKET OR TORPEDO LAUNCHERS</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">LAUNCHING GRAVITY-PROPELLED PROJECTILES OR MISSILES</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER LAUNCHING APPARATUS</td><td><b>7/00</b></td></p></tr></table>				
F41G		武器用照準器；照準合わせ（それらの光学的特徴Ｇ０２Ｂ）<br>	WEAPON SIGHTS; AIMING (optical aspects thereof <b>G02B</b>)				
F41H		装甲；装甲砲塔；装甲車両または武装車両；攻撃または防御の手段一般，例．偽装一般<br><br><b><ul>サブクラス内の索引</ul></b><br>装甲<br>人員防御具　１／００<br>装甲板，たて　５／００<br>偽装　３／００<br>装甲車両または武装車両　７／００<br>火災，ガスまたは化学戦争　９／００<br>他の攻撃または防御手段　１１／００，１３／００<br>	ARMOUR; ARMOURED TURRETS; ARMOURED OR ARMED VEHICLES; MEANS OF ATTACK OR DEFENCE, e.g. CAMOUFLAGE, IN GENERAL<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARMOUR</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Personal protection gear</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Armour plates, shields</td><td><b>5/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CAMOUFLAGE</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARMOURED OR ARMED VEHICLES</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FLAME, GAS OR CHEMICAL WARFARE</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER ATTACK OR DEFENCE MEANS</td><td><b>11/00</b>, <b>13/00</b></td></p></tr></table>				
F41J		標的；射撃場；弾丸受け<br><br><b><ul>サブクラス内の索引</ul></b><br>標的<br>固定のものまたは移動可能のもの　１／００、７／００，９／００<br>反射するまたはアクティブなもの　２／００<br>矢またはダーツ用に特に適したもの　３／００<br>標的命中表示器または記録器　５／００<br>標的台；射撃場　１／００；１１／００<br>弾丸受け　１３／００<br>	TARGETS; TARGET RANGES; BULLET CATCHERS<br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TARGETS</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Stationary or movable</td><td><b>1/00</b>, <b>7/00</b>, <b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Reflecting or active</td><td><b>2/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Specially adapted for arrows or darts</td><td><b>3/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TARGET-HIT INDICATORS OR RECORDERS</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TARGET STANDS; TARGET RANGES</td><td><b>1/00</b>; <b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BULLET CATCHERS</td><td><b>13/00</b></td></p></tr></table>				
F42		弾薬；爆破<br><br><b><ul>注</ul></b><br>（１）シミュレータは一般にクラスＧ０９に包含されるが，このクラスは，模擬的な演習または訓練用の手段をも包含する。<br>（２）このクラスおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“火管”は連続した爆発における最初の爆発段階を生じさせる；［２］<br>―“撃発雷管”は爆発させるために撃たれる火管を意味する；［２］<br>―“点火薬”は爆発的である否かを問わず，最初の火花または熱の発生段階を生じさせる；［２］<br>―“発火手段”または“点火装置”（それぞれ武器および爆破に用いられる）は信管の一部であるか否かを問わず，火管に直接作用する器具を意味する；［２］<br>―“起爆筒”または“起爆薬”は火管の爆発を拡大するために用いられる装薬を意味する；［２］<br>―“信管”は爆発がある条件下でのみ起こりうるよう安全および安全解除機構を組み込んだ構成体または機構を意味する；この構成体または機構は発火の時期（瞬発または遅発）または仕方，例．衝撃，近接，静水圧など，も決める；［２］<br>―“弾薬”は他に明記してなければ単体か否かを問わず，装薬および発射体を含むものを意味する；［２］<br>―“発射体”，“飛しょう体”，または“発射体または飛しょう体”は発射されまたは推進されるすべての物体を意味する；［４］<br>―“誘導飛しょう体”はその弾道の少なくとも一部で誘導される発射体または飛しょう体を意味する；［４］<br>―“ロケット”はその弾道の少なくとも一部で，ロケットエンジン，すなわち．そのために燃料と酸化剤の両方をもった噴射推進エンジンによって自ら推進する発射体または飛しょう体を意味する。［４］<br>―“導火線”は爆破において爆薬を起爆するための通常の柔軟な線又はケーブル内に封入された装薬の連続した系列を意味する。［５］<br>	AMMUNITION; BLASTING<br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This class <u>covers</u> also means for practice or training which may have aspects of simulation, although simulators are generally covered by class <b>G09</b>.<b>[2,4,5]</b></li><li>In this class, the following terms or expressions are used with the meanings indicated:<ul type=""disc""><li>&quot;primer&quot; effects the first explosive step in the sequence of explosion;</li><li>&quot;percussion cap&quot; means a primer which is struck to explode;</li><li>&quot;igniter&quot; effects the first spark-producing or heat-producing step but may not be explosive;</li><li>&quot;firing-means&quot; or &quot;initiator&quot; (used respectively in the arts of weaponry and blasting) means a device acting directly on the primer, which device may or may not form part of the fuze;</li><li>&quot;detonator&quot; or &quot;detonator charge&quot; means a charge used to amplify the explosion of the primer;</li><li>&quot;fuze&quot; means an assembly or mechanism which incorporates safety and arming means in order that the explosion can only take place under certain conditions; this assembly or mechanism determines also the moment (instantaneous or delayed) or the manner, e.g. impact, proximity, hydrostatic pressure, of the firing;</li><li>&quot;ammunition&quot; covers propulsive charge and projectile whether or not forming a single body, unless otherwise made clear;</li><li>&quot;projectile&quot;, &quot;missile&quot; or &quot;projectile or missile&quot; means any body which is projected or propelled;</li><li>&quot;guided missile&quot; means projectile or missile which is guided during at least part of its trajectory;</li><li>&quot;rocket&quot; means projectile or missile which is self-propelled, during at least part of its trajectory, by a rocket engine, i.e. by a jet-propulsion engine carrying both fuel and oxidant therefor;</li><li>&quot;fuse&quot; or &quot;fuse cord&quot; means a continuous train of explosive enclosed in a usually flexible cord or cable for setting-off an explosive charge in the art of blasting.</li></ul></li></ul>				
F42B		装薬，例．爆破用；煙火；弾薬（爆発性組成物Ｃ０６Ｂ；信管Ｆ４２Ｃ；爆破Ｆ４２Ｄ）［２，５］<br><br><b><ul>サブクラス内の索引</ul></b><br>形状に特徴のある装薬　１／００<br>爆破薬包　３／００<br>点火装置　３／１０<br>煙火　４／００<br>弾薬包　５／００<br>吹矢筒，弓，ばね銃または空気銃用発射体　６／００<br>散弾銃弾薬　７／００<br>訓練用弾薬　８／００<br>弾薬の操舵，安定または減速　１０／００<br>弾頭，所期効果または材料に特徴のある弾薬　１２／００<br>砲身への弾薬の導入または封入，弾薬による砲身の潤滑または清掃　１４／００<br>弾薬の形式<br>弾頭形式　１２／００<br>噴進弾または飛しょう体，ロケット魚雷，魚雷　１５／００〜１９／００<br>爆雷　２１／００<br>機雷　２２／００<br>地雷　２３／００<br>投下爆弾　２５／００<br>手榴弾　２７／００<br>無音，無煙または無閃光発射体　２９／００<br>小銃弾，小銃てき弾，砲弾，銛（もり）　３０／００<br>弾薬の製造または解体　３３／００<br>弾薬の試験または検査　３５／００<br>弾薬または装薬の包装または貯蔵；その保安　３９／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	EXPLOSIVE CHARGES, e.g. FOR BLASTING; FIREWORKS; AMMUNITION (explosive compositions <b>C06B</b>; fuzes <b>F42C</b>; blasting <b>F42D</b>)<b>[2,5]</b><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CHARGES CHARACTERISED BY THE FORM</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">BLASTING CARTRIDGES</td><td><b>3/00</b></td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Initiators</td><td><b>3/10</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FIREWORKS</td><td><b>4/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CARTRIDGE AMMUNITION</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PROJECTILES FOR BLOWGUNS, BOWS, SPRING OR AIR GUNS</td><td><b>6/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SHOTGUN AMMUNITION</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TRAINING AMMUNITION</td><td><b>8/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">STEERING, STABILISING OR RETARDING OF AMMUNITION</td><td><b>10/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">AMMUNITION CHARACTERISED BY WARHEAD, INTENDED EFFECT OR MATERIAL</td><td><b>12/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">GUIDING OR SEALING AMMUNITION IN BARRELS, LUBRICATING OR CLEANING BARRELS BY AMMUNITION</td><td><b>14/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TYPES OF AMMUNITION</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Warhead types</td><td><b>12/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Self-propelled projectiles or missiles, rocket torpedoes, marine torpedoes</td><td><b>15/00-19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Depth charges</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Marine mines</td><td><b>22/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Land mines</td><td><b>23/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fall bombs</td><td><b>25/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Hand grenades</td><td><b>27/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Noiseless, smokeless or flashless projectiles</td><td><b>29/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Bullets, rifle grenades, ordnance projectiles, harpoons</td><td><b>30/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">MANUFACTURING OR DISMANTLING OF AMMUNITION</td><td><b>33/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">TESTING OR CHECKING OF AMMUNITION</td><td><b>35/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">PACKAGING OR STORAGE OF AMMUNITION OR EXPLOSIVE CHARGES, SAFETY FEATURES THEREOF</td><td><b>39/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F42C		信管（爆破薬包の点火装置Ｆ４２Ｂ３／１０；化学的事項Ｃ０６Ｃ）；安全解除機構または安全機構（信管の組み立てＦ４２Ｂ３３／０２；信管の中へ，または中から，の火管の装着または取り外しＦ４２Ｂ３３／０４；信管用容器Ｆ４２Ｂ３９／３０）［５］<br><br><b><ul>サブクラス内の索引</ul></b><br>信管作動の原理<br>衝撃　１／００<br>液体の接触　３／００<br>液体の圧力　５／００<br>機械力　７／００<br>非電気時限信管　９／００<br>電気信管　１１／００<br>近接信管　１３／００<br>複動信管　９／００<br>弾薬の形に特徴のある信管　１４／００<br>安全解除または安全機構　１５／００<br>信管設定　１７／００<br>その他の細部　１９／００<br>検査，試験　２１／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	AMMUNITION FUZES (blasting cartridge initiators <b>F42B 3/10</b>; chemical aspects <b>C06C</b>); ARMING OR SAFETY MEANS THEREFOR (filling fuzes <b>F42B 33/02</b>; fitting or extracting primers in or from fuzes <b>F42B 33/04</b>; containers for fuzes <b>F42B 39/30</b>)<b>[5]</b><br><br><b><u>Subclass indexes</u></b><br><table width="100%"><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FUZE-OPERATING PRINCIPLES</td><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Impact</td><td><b>1/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Liquid contact</td><td><b>3/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Fluid pressure</td><td><b>5/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Mechanical force</td><td><b>7/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Non-electric time fuzes</td><td><b>9/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Electric fuzes</td><td><b>11/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Proximity fuzes</td><td><b>13/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:2em;margin:0"">Combination fuzes</td><td><b>9/00</b></td></p></tr></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FUZES CHARACTERISED BY THE TYPE OF AMMUNITION</td><td><b>14/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">ARMING OR SAFETY MEANS</td><td><b>15/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">FUZE-SETTING</td><td><b>17/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">OTHER DETAILS</td><td><b>19/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">CHECKING, TESTING</td><td><b>21/00</b></td></p></tr><tr><td width="70%"><p style=""text-indent:1em;margin:0"">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b>99/00</b></td></p></tr></table>				
F42D		爆破（導火線Ｃ０６Ｃ５／００；爆破薬包Ｆ４２Ｂ３／００）<br>	BLASTING (fuses, e.g. fuse cords, <b>C06C 5/00</b>; blasting cartridges <b>F42B 3/00</b>)				
F99		このセクションの中で他に分類されない主題事項［８］<br>	SUBJECT MATTER NOT OTHERWISE PROVIDED FOR IN THIS SECTION<b>[8]</b>				
F99Z		このセクションの中で他に分類されない主題事項［８］<br><br><b><ul>注</ul></b><br>このサブクラスは，以下の主題事項を包含する：［８］<br>（ａ）このセクションのサブクラスに包含される主題事項に分類されないが，これに最も関連しているもの，［８］<br>（ｂ）別のセクションの何れのサブクラスにも明示的に包含されないもの。［８］<br>	SUBJECT MATTER NOT OTHERWISE PROVIDED FOR IN THIS SECTION<b>[8]</b><br><br><b><u>Note(s)</u></b><br><br><ul type=""1""><li>This subclass <u>covers</u> subject matter that:<b>[8]</b><ul type=""a""><li>is not provided for, but is most closely related to, the subject matter covered by the subclasses of this section, and</li><li>is not explicitly covered by any subclass of another section.</li></ul></li></ul>				
