F16G1/00	7	Driving-belts (V-belts F16G5/00; conveyor belt B65G)	F16G1/00	F16G1/00		310
F16G1/02	8	made of leather (F16G1/28 takes precedence; making thereof C14B9/00{; consisting of several parts F16G1/22})	F16G1/02	F16G1/02		97
F16G1/04	8	made of fibrous material, e.g. textiles, whether rubber-covered or not (F16G1/28 takes precedence; making thereof D03D{; consisting of several parts F16G1/22})	F16G1/04	F16G1/04		397
F16G1/06	8	made of rubber (F16G1/28 takes precedence {; consisting of several parts F16G1/22}; making thereof B29D29/00)	F16G1/06	F16G1/06		123
F16G1/08	9	with reinforcement bonded by the rubber	F16G1/08	F16G1/08		439
F16G1/10	10	with textile reinforcement	F16G1/10	F16G1/10		499
F16G1/12	10	with metal reinforcement	F16G1/12	F16G1/12		176
F16G1/14	8	made of plastics (F16G1/28 takes precedence {; consisting of several parts F16G1/22}; making thereof B29D29/00)	F16G1/14	F16G1/14		139
F16G1/16	9	with reinforcement bonded by the plastic material {(making thereof B32B)}	F16G1/16	F16G1/16		201
F16G1/18	8	made of wire (making thereof B21F43/00{; consisting of several parts F16G1/22})	F16G1/18	F16G1/18		58
F16G1/20	8	made of a single metal strip (making thereof B21D53/14)	F16G1/20	F16G1/20		97
F16G1/21	8	built-up from superimposed layers, e.g. zig-zag folded	F16G1/21	F16G1/21		78
F16G1/22	8	consisting of several parts	F16G1/22	F16G1/22		195
F16G1/24	9	in the form of links (in the shape of chain links F16G13/08)	F16G1/24	F16G1/24		155
F16G1/26	9	in the form of strips or lamellae	F16G1/26	F16G1/26		109
F16G1/28	8	with a contact surface of special shape, e.g. toothed	F16G1/28	F16G1/28		1886
F16G3/00	7	Belt fastenings, e.g. for conveyor belts (for V-belts F16G7/00)	F16G3/00	F16G3/00		848
F16G3/003	8	{Apparatus or tools for joining belts (stapler B25C5/00)}	F16G3/00	F16G3/00		558
F16G3/006	8	{Traction devices to bring together belts, cables or chains}	F16G3/00	F16G3/00		327
F16G3/02	8	with series of eyes or the like, interposed and linked by a pin to form a hinge (F16G3/09 takes precedence)	F16G3/02	F16G3/02		616
F16G3/04	9	in which the ends of separate U-shaped or like eyes are attached to the belt by parts penetrating into it	F16G3/04	F16G3/04		449
F16G3/06	8	with outwardly-bent, mutually-connected belt ends	F16G3/06	F16G3/06		307
F16G3/07	8	Friction clamps, e.g. of grommet-thimble type	F16G3/07	F16G3/07		31
F16G3/08	8	consisting of plates and screw-bolts or rivets (F16G3/06 takes precedence)	F16G3/08	F16G3/08		336
F16G3/09	9	the plates forming a hinge	F16G3/09	F16G3/09		17
F16G3/10	8	Joining belts by sewing, sticking, vulcanising, or the like; Constructional adaptations of the belt ends for this purpose	F16G3/10	F16G3/10		643
F16G3/12	8	Joining belts by lacing	F16G3/12	F16G3/12		34
F16G3/14	8	with extensible parts; with resilient parts	F16G3/14	F16G3/14		19
F16G3/16	8	Devices or machines for connecting driving-belts or the like	F16G3/16	F16G3/16		222
F16G5/00	7	V-belts, i.e. belts of tapered cross-section	F16G5/00	F16G5/00		187
F16G5/02	8	made of leather (F16G5/20 takes precedence {; consisting of several parts F16G5/16})	F16G5/02	F16G5/02		18
F16G5/04	8	made of rubber (F16G5/02 takes precedence {consisting of several parts F16G5/16})	F16G5/04	F16G5/04		113
F16G5/06	9	with reinforcement bonded by the rubber	F16G5/06	F16G5/06		665
F16G5/08	10	with textile reinforcement	F16G5/08	F16G5/08		477
F16G5/10	10	with metal reinforcement	F16G5/10	F16G5/10		114
F16G5/12	8	made of plastics (F16G5/20 takes precedence {consisting of several parts F16G5/16})	F16G5/12	F16G5/12		32
F16G5/14	9	with reinforcement bonded by the plastic material	F16G5/14	F16G5/14		73
F16G5/16	8	consisting of several parts	F16G5/16	F16G5/16		1027
F16G5/163	9	{with means allowing lubrication (F16G5/18 takes precedence)}	F16G5/16	F16G5/16		160
F16G5/166	9	{with non-metallic rings (F16G5/18 takes precedence)}	F16G5/16	F16G5/16		772
F16G5/18	9	in the form of links	F16G5/18	F16G5/18		953
F16G5/20	8	with a contact surface of special shape, e.g. toothed	F16G5/20	F16G5/20		1015
F16G5/22	8	built-up from superimposed layers	F16G5/22	F16G5/22		54
F16G5/24	9	zig-zag folded	F16G5/24	F16G5/24		
F16G7/00	7	V-belt fastenings	F16G7/00	F16G7/00		289
F16G7/02	8	locked, e.g. riveted	F16G7/02	F16G7/02		7
F16G7/04	8	quickly detachable	F16G7/04	F16G7/04		15
F16G7/06	8	adjustable, e.g. for tension	F16G7/06	F16G7/06		19
F16G9/00	7	Ropes or cables specially adapted for driving, or for being driven by, pulleys or other gearing elements (ropes or cables in general D07B)	F16G9/00	F16G9/00		306
F16G9/02	8	made of leather; having enveloping sheathings made of leather	F16G9/02	F16G9/02		1
F16G9/04	8	made of rubber or plastics (F16G9/02 takes precedence)	F16G9/04	F16G9/04		27
F16G11/00	7	Means for fastening cables or ropes to one another or to other objects; Caps or sleeves for fixing on cables or ropes (attaching ropes or cables to lift cars or cages B66B7/08, to winch drums or barrels B66D1/34; ground anchors E02D5/00; anchoring devices for prestressed members E04C5/00; rope clamps in earth drilling E21B19/12)	F16G11/00	F16G11/00		1608
F16G11/02	8	with parts deformable to grip the cable or cables; Fastening means which engage a sleeve or the like fixed on the cable	F16G11/02	F16G11/02		1410
F16G11/025	9	{Fastening means which engage a sleeve or the like fixed on the cable, e.g. caps (F16G11/143 and F16G11/146 take precedence)}	F16G11/02	F16G11/02		365
F16G11/03	8	incorporating resiliently-mounted members for attachment of the cable end	F16G11/03	F16G11/03		152
F16G11/04	8	with wedging action, e.g. friction clamps (F16G11/02, {F16G11/10} take precedence; {eyes for grommet-thimble type fastenings F16G11/146})	F16G11/04	F16G11/04		652
F16G11/042	9	{using solidifying liquid material forming a wedge}	F16G11/04	F16G11/04		286
F16G11/044	9	{friction clamps deforming the cable, wire, rope or cord}	F16G11/04	F16G11/04		85
F16G11/046	10	{by bending the cable around a surface}	F16G11/04	F16G11/04		710
F16G11/048	10	{by moving a surface into the cable}	F16G11/04	F16G11/04		1297
F16G11/05	9	by using conical plugs insertable between the strands	F16G11/05	F16G11/05		302
F16G11/06	8	with laterally-arranged screws (F16G11/02, F16G11/04 take precedence)	F16G11/06	F16G11/06		896
F16G11/08	8	Fastenings for securing ends of driving-cables to one another, the fastenings having approximately the same diameter as the cables	F16G11/08	F16G11/08		457
F16G11/09	9	incorporating hinge joints or pivots for the attachment of the cable ends	F16G11/09	F16G11/09		30
F16G11/10	8	Quick-acting fastenings; Clamps holding in one direction only	F16G11/10	F16G11/10		1286
F16G11/101	9	{deforming the cable by moving a part of the fastener}	F16G11/10	F16G11/10		785
F16G11/103	9	{deforming the cable by bending it around or inserting it into the fastener}	F16G11/10	F16G11/10		408
F16G11/105	9	{Clamps holding in one direction only}	F16G11/10	F16G11/10		319
F16G11/106	10	{using a toothed surface}	F16G11/10	F16G11/10		648
F16G11/108	10	{using a ball or a cylinder}	F16G11/10	F16G11/10		240
F16G11/12	8	Connections or attachments, e.g. turnbuckles, adapted for straining of cables, ropes, or wire (straining wire in general B21F9/00)	F16G11/12	F16G11/12		4307
F16G11/14	8	Devices or coupling-pieces designed for easy formation of adjustable loops, e.g. choker hooks; Hooks or eyes with integral parts designed to facilitate quick attachment to cables or ropes at any point, e.g. by forming loops	F16G11/14	F16G11/14		1282
F16G11/143	9	{Hooks}	F16G11/14	F16G11/14		361
F16G11/146	9	{Eyes}	F16G11/14	F16G11/14		322
F16G13/00	7	Chains (making thereof B21L)	F16G13/00	F16G13/00		382
F16G13/02	8	Driving-chains (specially adapted to gearings with variable gear-ratio F16H9/00)	F16G13/02	F16G13/02		832
F16G13/04	9	Toothed chains	F16G13/04	F16G13/04		909
F16G13/06	9	with links connected by parallel driving-pins with or without rollers {so called open links (if the parallel coupling pins have only a joining function - so called closed links - F16G13/02)}	F16G13/06	F16G13/06		2208
F16G13/07	10	the links being of identical shape, e.g. cranked	F16G13/07	F16G13/07		482
F16G13/08	9	with links closely interposed on the joint pins (F16G13/04 takes precedence)	F16G13/08	F16G13/08		207
F16G13/10	9	with universal joints	F16G13/10	F16G13/10		234
F16G13/12	8	Hauling- or hoisting-chains {so called ornamental chains}	F16G13/12	F16G13/12		593
F16G13/14	9	built up from readily-separable links	F16G13/14	F16G13/14		495
F16G13/16	9	with arrangements for holding electric cables, hoses, or the like	F16G13/16	F16G13/16		1759
F16G13/18	8	Chains having special overall characteristics	F16G13/18	F16G13/18		457
F16G13/20	9	stiff; Push-pull chains	F16G13/20	F16G13/20		500
F16G13/22	9	extensible {(not used, seeF16G13/18)}	F16G13/22	F16G13/22		8
F16G13/24	10	resilient {(not used, seeF16G13/18)}	F16G13/24	F16G13/24		9
F16G15/00	7	Chain couplings, Shackles; Chain joints; Chain links; Chain bushes (making chain elements B21L)	F16G15/00	F16G15/00		941
F16G15/02	8	for fastening more or less permanently	F16G15/02	F16G15/02		622
F16G15/04	8	Quickly-detachable chain couplings; Shackles {chain links with rapid junction means are classified according to the corresponding kind of chain}	F16G15/04	F16G15/04		818
F16G15/06	9	Shackles designed for attachment by joint pins to chain elements, e.g. D-shackles {so called harp links; the D-chain links are classified according to the corresponding kind of chain}	F16G15/06	F16G15/06		715
F16G15/08	8	Swivels	F16G15/08	F16G15/08		477
F16G15/10	8	Emergency joints or links	F16G15/10	F16G15/10		28
F16G15/12	8	Chain links	F16G15/12	F16G15/12		595
F16G15/14	9	made of sheet metal, e.g. profiled	F16G15/14	F16G15/14		64
F16G17/00	7	Hooks as integral parts of chains (hooks for cranes B66C1/34; hooks in general F16B45/00)	F16G17/00	F16G17/00		276
