G05G1/00	7	Controlling members, e.g. knobs or handles; Assemblies or arrangements thereof; Indicating position of controlling members (joysticks G05G9/04; steering wheels for motor vehicles B62D)<br><br><u>NOTE</u><br><br> In this group, the first place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the first appropriate place. 	G05G1/00	G05G1/00		220
G05G1/01	8	Arrangements of two or more controlling members with respect to one another (double foot control, e.g. for instruction vehicles G05G1/34; mounting units comprising an assembly with two or more pedals G05G1/36)	G05G1/01	G05G1/01		333
G05G1/015	8	Arrangements for indicating the position of a controlling member (means for continuously detecting pedal position G05G1/38; means for detecting position through tactile feedback G05G5/03)	G05G1/015	G05G1/015		315
G05G1/02	8	Controlling members for hand actuation by linear movement, e.g. push buttons	G05G1/02	G05G1/02		1772
G05G1/025	9	{actuated by sliding movement}	G05G1/02	G05G1/02		175
G05G1/04	8	Controlling members for hand actuation by pivoting movement, e.g. levers	G05G1/04	G05G1/04		2546
G05G1/06	9	Details of their grip parts {(G05G1/10 takes precedence)}	G05G1/06	G05G1/06		631
G05G1/08	8	Controlling members for hand actuation by rotary movement, e.g. hand wheels	G05G1/08	G05G1/08		1416
G05G1/082	9	{having safety devices, e.g. means for disengaging the control member from the actuated member}	G05G1/08	G05G1/08		156
G05G1/085	9	{Crank handles (G05G1/082 takes precedence)}	G05G1/08	G05G1/08		571
G05G1/087	9	{retractable; Flush control knobs}	G05G1/08	G05G1/08		200
G05G1/10	9	Details, e.g. of discs, knobs, wheels or handles {(G05G1/085 takes precedence)}	G05G1/10	G05G1/10		2264
G05G1/105	10	{comprising arrangements for illumination}	G05G1/10	G05G1/10		533
G05G1/12	10	Means for securing the members on rotatable spindles or the like	G05G1/12	G05G1/12		1260
G05G1/30	8	Controlling members actuated by foot	G05G1/30	G05G1/30		2511
G05G1/305	9	{Compound pedal co-operating with two or more controlled members}	G05G1/30	G05G1/30		157
G05G1/32	9	with means to prevent injury	G05G1/32	G05G1/32		473
G05G1/323	10	means disconnecting the connection between pedal and controlled member, e.g. by breaking or bending the connecting rod	G05G1/323	G05G1/323		74
G05G1/327	10	means disconnecting the pedal from its hinge or support, e.g. by breaking or bending the support	G05G1/327	G05G1/327		224
G05G1/34	9	Double foot controls, e.g. for instruction vehicles	G05G1/34	G05G1/34		204
G05G1/36	9	Mounting units comprising an assembly of two or more pedals, e.g. for facilitating mounting	G05G1/36	G05G1/36		327
G05G1/38	9	comprising means to continuously detect pedal position	G05G1/38	G05G1/38		718
G05G1/40	9	adjustable	G05G1/40	G05G1/40		364
G05G1/405	10	infinitely adjustable	G05G1/405	G05G1/405		575
G05G1/42	9	non-pivoting, e.g. sliding	G05G1/42	G05G1/42		165
G05G1/44	9	pivoting	G05G1/44	G05G1/44		1084
G05G1/445	10	about a central fulcrum	G05G1/445	G05G1/445		185
G05G1/46	9	Means, e.g. links, for connecting the pedal to the controlled unit	G05G1/46	G05G1/46		748
G05G1/48	9	Non-slip pedal treads; Pedal extensions or attachments characterised by mechanical features only	G05G1/48	G05G1/48		85
G05G1/483	10	Non-slip treads; Pedal extensions or attachments characterised by mechanical features only	G05G1/483	G05G1/483		221
G05G1/487	10	Pedal extensions	G05G1/487	G05G1/487		411
G05G1/50	9	Manufacturing of pedals; Pedals characterised by the material used	G05G1/50	G05G1/50		54
G05G1/503	10	{Controlling members for hand-actuation}	G05G1/50	G05G1/50		48
G05G1/506	10	{Controlling members for foot-actuation}	G05G1/50	G05G1/50		290
G05G1/52	8	Controlling members specially adapted for actuation by other parts of the human body than hand or foot	G05G1/52	G05G1/52		85
G05G1/54	8	Controlling members specially adapted for actuation by auxiliary operating members or extensions; Operating members or extensions therefor (pedal extensions)	G05G1/54	G05G1/54		143
G05G1/56	9	Controlling members specially adapted for actuation by keys, screwdrivers or like tools	G05G1/56	G05G1/56		31
G05G1/58	8	Rests or guides for relevant parts of the operator&apos;s body	G05G1/58	G05G1/58		80
G05G1/60	9	Foot rests or foot guides	G05G1/60	G05G1/60		314
G05G1/62	9	Arm rests	G05G1/62	G05G1/62		144
G05G3/00	7	Controlled members; Assemblies or arrangements thereof (interlocking of controlled members G05G5/08)	G05G3/00	G05G3/00		10
G05G5/00	7	Means for preventing, limiting or returning the movements of parts of a control mechanism, e.g. locking controlling member (G05G17/00 takes precedence)	G05G5/00	G05G5/00		158
G05G5/005	8	{for preventing unintentional use of a control mechanism (G05G5/28 takes precedence)}	G05G5/00	G05G5/00		370
G05G5/02	8	Means preventing undesired movements of a controlling member which can be moved in two or more separate steps or ways, e.g. restricting to a stepwise movement or to a particular sequence of movements (G05G5/28 takes precedence)	G05G5/02	G05G5/02		330
G05G5/03	8	Means for enhancing the operator&apos;s awareness of arrival of the controlling member at a command or datum position; Providing feel, e.g. means for creating a counterforce (arrangements for indicating the position of the controlling member G05G1/015)	G05G5/03	G05G5/03		2012
G05G5/04	8	Stops for limiting movement of members, e.g. adjustable stop (G05G5/03, G05G5/05, G05G5/28 take precedence)	G05G5/04	G05G5/04		810
G05G5/05	8	Means for returning or tending to return controlling members to an inoperative or neutral position, e.g. by providing return springs or resilient end-stops (G05G5/28 takes precedence)	G05G5/05	G05G5/05		940
G05G5/06	8	for holding members in one or a limited number of definite positions only ({G05G5/005}, G05G5/03, G05G5/05, G05G5/28 take precedence)	G05G5/06	G05G5/06		1263
G05G5/065	9	{using a spring-loaded ball}	G05G5/06	G05G5/06		276
G05G5/08	9	Interlocking of members, e.g. locking member in a particular position before or during the movement of another member	G05G5/08	G05G5/08		264
G05G5/12	8	for holding members in an indefinite number of positions, e.g. by a toothed quadrant (G05G5/28 takes precedence)	G05G5/12	G05G5/12		218
G05G5/14	9	by locking a member with respect to a fixed quadrant, rod, or the like	G05G5/14	G05G5/14		19
G05G5/16	10	by friction	G05G5/16	G05G5/16		207
G05G5/18	10	by positive interengagement, e.g. by a pawl	G05G5/18	G05G5/18		572
G05G5/20	9	by locking a quadrant, rod, or the like carried by the member	G05G5/20	G05G5/20		6
G05G5/22	10	by friction	G05G5/22	G05G5/22		107
G05G5/24	10	by positive interengagement, e.g. by a pawl	G05G5/24	G05G5/24		276
G05G5/26	9	by other means than a quadrant, rod, or the like	G05G5/26	G05G5/26		110
G05G5/28	8	for preventing unauthorised access to the controlling member or its movement to a command position	G05G5/28	G05G5/28		174
G05G7/00	7	Manually-actuated control mechanisms provided with one single controlling member co-operating with one single controlled member; Details thereof (controlling members G05G1/00)	G05G7/00	G05G7/00		168
G05G7/02	8	characterised by special provisions for conveying or converting motion, or for acting at a distance	G05G7/02	G05G7/02		689
G05G7/04	9	altering the ratio of motion or force between controlling member and controlled member as a function of the position of the controlling member	G05G7/04	G05G7/04		684
G05G7/06	9	in which repeated movement of the controlling member produces increments of movement of the controlled member (G05G7/08 takes precedence)	G05G7/06	G05G7/06		67
G05G7/08	9	in which repeated movement of the controlling member moves the controlling member through a cycle of distinct positions	G05G7/08	G05G7/08		115
G05G7/10	9	specially adapted for remote control (G05G7/04&#160;-&#160;G05G7/08 take precedence)	G05G7/10	G05G7/10		236
G05G7/12	8	specially adapted for actuating a member on a system in motion with respect to the controlling member, e.g. on a rotating shaft	G05G7/12	G05G7/12		119
G05G7/14	8	characterised by means for delaying initiation of, or making more gradual throughout, the movement of the controlled member in response to a given input from the controlling member, e.g. by providing lost motion in the command train	G05G7/14	G05G7/14		160
G05G7/16	8	Special provisions for reducing the effect of slight relative movement between supports of the mechanism, e.g. resulting from resilient mounting of a controlled mechanism	G05G7/16	G05G7/16		55
G05G9/00	7	Manually-actuated control mechanisms provided with one single controlling member co-operating with two or more controlled members, e.g. selectively, simultaneously	G05G9/00	G05G9/00		176
G05G9/02	8	the controlling member being movable in different independent ways, movement in each individual way actuating one controlled member only	G05G9/02	G05G9/02		163
G05G9/04	9	in which movement in two or more ways can occur simultaneously	G05G9/04	G05G9/04		199
G05G9/047	10	the controlling member being movable by hand about orthogonal axes, e.g. joysticks {(for switches H01H25/04)}	G05G9/047	G05G9/047		2693
G05G2009/04703	11	{Mounting of controlling member}	G05G9/047	G05G9/047		104
G05G2009/04707	12	{with ball joint}	G05G9/047	G05G9/047		421
G05G2009/04711	12	{with substantially hemispherical bearing part forced into engagement, e.g. by a spring}	G05G9/047	G05G9/047		92
G05G2009/04714	12	{with orthogonal axes}	G05G9/047	G05G9/047		179
G05G2009/04718	13	{with cardan or gimbal type joint}	G05G9/047	G05G9/047		317
G05G2009/04722	12	{elastic, e.g. flexible shaft}	G05G9/047	G05G9/047		72
G05G2009/04725	13	{with coil spring}	G05G9/047	G05G9/047		56
G05G2009/04729	13	{melastomeric}	G05G9/047	G05G9/047		51
G05G2009/04733	12	{with a joint having a nutating disc, e.g. forced by a spring}	G05G9/047	G05G9/047		91
G05G9/04737	11	{with six degrees of freedom}	G05G9/047	G05G9/047		145
G05G2009/0474	11	{characterised by means converting mechanical movement into electric signals}	G05G9/047	G05G9/047		175
G05G2009/04744	12	{Switches}	G05G9/047	G05G9/047		444
G05G2009/04748	12	{Position sensor for rotary movement, e.g. potentiometer}	G05G9/047	G05G9/047		205
G05G2009/04751	12	{Position sensor for linear movement}	G05G9/047	G05G9/047		71
G05G2009/04755	12	{Magnetic sensor, e.g. hall generator, pick-up coil}	G05G9/047	G05G9/047		345
G05G2009/04759	12	{Light-sensitive detector, e.g. photoelectric}	G05G9/047	G05G9/047		187
G05G2009/04762	12	{Force transducer, e.g. strain gauge}	G05G9/047	G05G9/047		127
G05G2009/04766	11	{providing feel, e.g. indexing means, means to create counterforce}	G05G9/047	G05G9/047		573
G05G2009/0477	12	{holding the member in a number of definite positions}	G05G9/047	G05G9/047		76
G05G2009/04774	11	{with additional switches or sensors on the handle}	G05G9/047	G05G9/047		448
G05G2009/04777	11	{with additional push or pull action on the handle}	G05G9/047	G05G9/047		256
G05G2009/04781	11	{with additional rotation of the controlling member}<br><br><u>NOTE</u><br><br>Provisional indexing codes related to scheme of trilateral project T021.	G05G9/047	G05G9/047		235
G05G9/04785	11	{the controlling member being the operating part of a switch arrangement}	G05G9/047	G05G9/047		259
G05G9/04788	12	{comprising additional control elements}	G05G9/047	G05G9/047		121
G05G9/04792	13	{for rotary control around the axis of the controlling member}	G05G9/047	G05G9/047		117
G05G9/04796	13	{for rectilinear control along the axis of the controlling member}	G05G9/047	G05G9/047		111
G05G9/053	11	the controlling member comprising a ball {(graph-reading using a tracing ball or mouse G06F3/033)}	G05G9/053	G05G9/053		38
G05G9/06	8	the controlled members being actuated successively by repeated movement of the controlling member	G05G9/06	G05G9/06		19
G05G9/08	8	the controlled members being actuated successively by progressive movement of the controlling member {(single lever throttle and clutch control for marine engines B63H21/213)}	G05G9/08	G05G9/08		206
G05G9/085	9	{the controlling member acting on a set of cams or slot cams}	G05G9/08	G05G9/08		31
G05G9/10	8	with preselection and subsequent movement of each controlled member by movement of the controlling member in two different ways, e.g. guided by a shift gate	G05G9/10	G05G9/10		96
G05G11/00	7	Manually-actuated control mechanisms provided with two or more controlling members co-operating with one single controlled member	G05G11/00	G05G11/00		402
G05G13/00	7	Manually-actuated control mechanisms provided with two or more controlling members and also two or more controlled members (interlocking G05G5/08)	G05G13/00	G05G13/00		329
G05G13/02	8	with separate controlling members for preselection and shifting of controlled members	G05G13/02	G05G13/02		17
G05G15/00	7	Mechanical devices for initiating a movement automatically due to a specific cause	G05G15/00	G05G15/00		146
G05G15/002	8	{due to an abnormal functioning of the controlled apparatus (if speed is abnormal G05G15/06)}	G05G15/00	G05G15/00		90
G05G15/005	8	{due to a dangerous situation for the operator}	G05G15/00	G05G15/00		5
G05G15/007	8	{due to an excerted pressure}	G05G15/00	G05G15/00		9
G05G15/02	8	due to alteration of the sense of movement of a member	G05G15/02	G05G15/02		31
G05G15/04	8	due to distance or angle travelled by a member	G05G15/04	G05G15/04		179
G05G15/06	8	due to the speed of rotation or of bodily movement of a member, e.g. passing an upper or lower limit thereof (speedometers G01P)	G05G15/06	G05G15/06		51
G05G15/08	8	due to the load or torque on a member, e.g. if exceeding a predetermined value thereof	G05G15/08	G05G15/08		257
G05G17/00	7	Mechanical devices for moving a member after being released; Trip or release mechanisms characterised thereby	G05G17/00	G05G17/00		332
G05G19/00	7	Servo-mechanisms with follow-up action, e.g. occurring in steps	G05G19/00	G05G19/00		249
G05G21/00	7	Mechanical apparatus for control of a series of operations, i.e. program control, e.g. involving a set of cams (G05G5/02 takes precedence)	G05G21/00	G05G21/00		268
G05G23/00	7	Means for ensuring the correct positioning of parts of control mechanisms, e.g. for taking-up play	G05G23/00	G05G23/00		469
G05G23/02	8	self-adjusting	G05G23/02	G05G23/02		52
G05G25/00	7	Other details or appurtenances of control mechanisms, e.g. supporting intermediate members elastically	G05G25/00	G05G25/00		407
G05G25/02	8	Inhibiting the generation or transmission of noise {(suppression of noise or vibrations in selector apparatus for gearings F16H59/0208)}	G05G25/02	G05G25/02		120
G05G25/04	8	Sealing against entry of dust, weather or the like {(in selector apparatus for gearings, F16H59/0213)}	G05G25/04	G05G25/04		424
G05G2505/00	7	Means for preventing, limiting or returning the movements of parts of a control mechanism, e.g. locking controlling member	CPCONLY	G05G2505/00		396
G05G2700/00	7	Control mechanisms or elements therefor applying a mechanical movement	CPCONLY	G05G2700/00		3
G05G2700/02	8	Means for regulating or adjusting control mechanisms, e.g. devices for automatic adjustment	CPCONLY	G05G2700/02		400
G05G2700/04	8	Control mechanisms limiting amplitude or adjusting datum position	CPCONLY	G05G2700/04		46
G05G2700/06	9	Control mechanisms for holding members in a number of positions comprising a device to limit the control range	CPCONLY	G05G2700/06		30
G05G2700/08	9	Control mechanisms for locking members in one or more positions	CPCONLY	G05G2700/08		390
G05G2700/10	9	Control mechanisms for locking or at least for blocking a member in one position out of a number of several positions	CPCONLY	G05G2700/10		62
G05G2700/12	8	Control mechanisms with one controlling member and one controlled member	CPCONLY	G05G2700/12		62
G05G2700/14	9	with one elastic element as essential part, e.g. elastic components as a part of an actuating mechanism	CPCONLY	G05G2700/14		261
G05G2700/16	9	Mechanisms for conveying motion or signals for or in relation with control mechanisms	CPCONLY	G05G2700/16		165
G05G2700/18	9	Systems wherein the control element may be placed in two or more positions	CPCONLY	G05G2700/18		72
G05G2700/20	8	Control mechanisms not otherwise provided for	CPCONLY	G05G2700/20		46
G05G2700/22	8	Mechanisms linking plurality of controlling or controlled members	CPCONLY	G05G2700/22		148
G05G2700/24	9	Locking controlled members of selectively controlled mechanisms	CPCONLY	G05G2700/24		75
G05G2700/26	9	with a control member moving selectively or simultaneously the controlled members	CPCONLY	G05G2700/26		51
G05G2700/28	10	with a control member that is moved for preselection in another direction than for final actuating	CPCONLY	G05G2700/28		60
G05G2700/30	10	without preselection or differentiation between selection and actuating, e.g. control members with a fix control sequence, after a determined advance cycle, in which the control device comprises cams actuating separately the controlled members	CPCONLY	G05G2700/30		121
G05G2700/32	9	with plurality of control members, e.g. preselection and actuating members actuating several controlled members	CPCONLY	G05G2700/32		49
