B05C1/00	7	Apparatus in which liquid or other fluent material is applied to the surface of the work by contact with a member carrying the liquid or other fluent material, e.g. a porous member loaded with a liquid to be applied as a coating (B05C5/02, B05C7/00 take precedence)	B05C1/00	B05C1/00		338
B05C1/003	8	{incorporating means for heating or cooling the liquid or other fluent material (B05C11/1042 takes precedence)}	B05C1/00	B05C1/00		342
B05C1/006	8	{for applying liquid or other fluent material to the edges of essentially flat articles}	B05C1/00	B05C1/00		210
B05C1/02	8	for applying liquid or other fluent material to separate articles {(B05C1/006 takes precedence)}	B05C1/02	B05C1/02		2045
B05C1/022	9	{to the outer surface of hollow articles (B05C1/027 takes precedence)}	B05C1/02	B05C1/02		510
B05C1/025	9	{to flat rectangular articles, e.g. flat sheets (B05C1/027 takes precedence)}	B05C1/02	B05C1/02		754
B05C1/027	9	{only at particular parts of the articles (at particular parts of work of indefinite length B05C1/16)}	B05C1/02	B05C1/02		815
B05C1/04	8	for applying liquid or other fluent material to work of indefinite length {(B05C1/003 takes precedence)}	B05C1/04	B05C1/04		206
B05C1/06	9	by rubbing contact, e.g. by brushes, by pads {(brushes in general A46B)}	B05C1/06	B05C1/06		2014
B05C1/08	9	using a roller {or other rotating member which contacts the work along a generating line}	B05C1/08	B05C1/08		1398
B05C1/0804	10	{the material being applied without contact with the roller}	B05C1/08	B05C1/08		61
B05C1/0808	10	{Details thereof, e.g. surface characteristics}	B05C1/08	B05C1/08		1287
B05C1/0813	10	{characterised by means for supplying liquid or other fluent material to the roller}	B05C1/08	B05C1/08		2324
B05C1/0817	10	{characterised by means for removing partially liquid or other fluent material from the roller, e.g. scrapers (coating roller co-operating with dosing rollers B05C1/0834)}	B05C1/08	B05C1/08		1066
B05C1/0821	10	{characterised by driving means for rollers or work}	B05C1/08	B05C1/08		738
B05C1/0826	10	{the work being a web or sheets (B05C1/0804, B05C1/0808, B05C1/0813, B05C1/0817, B05C1/0821, B05C1/10, B05C1/12 take precedence)}	B05C1/08	B05C1/08		1688
B05C1/083	11	{being passed between the coating roller and one or more backing rollers}	B05C1/08	B05C1/08		958
B05C1/0834	11	{the coating roller co-operating with other rollers, e.g. dosing, transfer rollers}	B05C1/08	B05C1/08		1234
B05C1/0839	10	{the work being unsupported at the line of contact between the coating roller and the work}	B05C1/08	B05C1/08		80
B05C1/0843	10	{the work being backed up by gas jet means for pushing the material in contact with the coating roller}	B05C1/08	B05C1/08		16
B05C1/0847	10	{the circumferential speed of the coating roller and the work speed having same direction but different value}	B05C1/08	B05C1/08		17
B05C1/0852	11	{the circumferential speed of the coating roller being higher than the work speed}	B05C1/08	B05C1/08		5
B05C1/0856	10	{Reverse coating rollers}	B05C1/08	B05C1/08		118
B05C1/086	10	{a pool of coating material being formed between a roller, e.g. a dosing roller and an element cooperating therewith}	B05C1/08	B05C1/08		146
B05C1/0865	11	{the cooperating element being a roller, e.g. a coating roller}	B05C1/08	B05C1/08		539
B05C1/0869	11	{the work contacting the pool}	B05C1/08	B05C1/08		77
B05C1/0873	10	{Controlling means responsive to conditions of the liquid or other fluent material, of the ambient medium, of the roller or of the work}	B05C1/08	B05C1/08		178
B05C1/0878	11	{responsive to the pressure applied between two rollers, e.g. between the coating roller and a backing roller or between the coating roller and a dosing roller}	B05C1/08	B05C1/08		71
B05C1/0882	11	{responsive to the distance between two rollers, e.g. between the coating roller and a backing roller}	B05C1/08	B05C1/08		146
B05C1/0886	11	{responsive to the condition of the work}	B05C1/08	B05C1/08		62
B05C1/0891	12	{responsive to the speed of moving of the work}	B05C1/08	B05C1/08		23
B05C1/0895	11	{responsive to the thickness of the weight of material applied to the work}	B05C1/08	B05C1/08		151
B05C1/10	10	the liquid or other fluent material being supplied from inside the roller	B05C1/10	B05C1/10		601
B05C1/12	10	the work being fed round the roller (B05C1/10 takes precedence)	B05C1/12	B05C1/12		681
B05C1/14	9	using a travelling band	B05C1/14	B05C1/14		269
B05C1/16	9	only at particular parts of the work {(at particular parts of separate articles B05C1/027)}	B05C1/16	B05C1/16		180
B05C1/165	10	{using a roller or other rotating member which contacts the work along a generating line}	B05C1/16	B05C1/16		444
B05C3/00	7	Apparatus in which the work is brought into contact with a bulk quantity of liquid or other fluent material	B05C3/00	B05C3/00		119
B05C3/005	8	{incorporating means for heating or cooling the liquid or other fluent material (B05C11/1042 takes precedence)}	B05C3/00	B05C3/00		175
B05C3/02	8	the work being immersed in the liquid or other fluent material	B05C3/02	B05C3/02		633
B05C3/04	9	with special provision for agitating the work or the liquid or other fluent material	B05C3/04	B05C3/04		344
B05C3/05	10	by applying vibrations thereto	B05C3/05	B05C3/05		152
B05C3/08	10	the work and the liquid or other fluent material being agitated together in a container, e.g. tumbled (B05C3/05 takes precedence)	B05C3/08	B05C3/08		240
B05C3/09	9	for treating separate articles	B05C3/09	B05C3/09		1256
B05C3/10	10	the articles being moved through the liquid or other fluent material (conveying articles through baths B65G, e.g. B65G49/02)	B05C3/10	B05C3/10		1532
B05C3/109	10	Passing liquids or other fluent materials into or through chambers containing stationary articles	B05C3/109	B05C3/109		222
B05C3/12	9	for treating work of indefinite length	B05C3/12	B05C3/12		457
B05C3/125	10	{the work being a web, band, strip or the like}	B05C3/12	B05C3/12		835
B05C3/132	10	supported on conveying means {(B05C3/125 takes precedence)}	B05C3/132	B05C3/132		124
B05C3/15	10	not supported on conveying means ({B05C3/125 takes precedence}; web or filament feeding arrangements B65H)	B05C3/15	B05C3/15		375
B05C3/152	11	the work passing in zig-zag fashion over rollers	B05C3/152	B05C3/152		61
B05C3/172	11	in endless form	B05C3/172	B05C3/172		23
B05C3/18	8	only one side of the work coming into contact with the liquid or other fluent material (B05C3/02 takes precedence)	B05C3/18	B05C3/18		640
B05C3/20	8	for applying liquid or other fluent material only at particular parts of the work (B05C3/02 takes precedence)	B05C3/20	B05C3/20		171
B05C5/00	7	Apparatus in which liquid or other fluent material is projected, poured or allowed to flow on to the surface of the work (B05C7/00 takes precedence; essentially involving spraying or electrostatic projection B05B)	B05C5/00	B05C5/00		1456
B05C5/001	8	{incorporating means for heating or cooling the liquid or other fluent material (B05C11/1042 takes precedence)}	B05C5/00	B05C5/00		1187
B05C5/002	8	{the work consisting of separate articles (B05C5/0208 takes precedence)}	B05C5/00	B05C5/00		572
B05C5/004	9	{the work consisting of separate rectangular flat articles, e.g. flat sheets}	B05C5/00	B05C5/00		250
B05C5/005	8	{Curtain coaters (B05C5/008 takes precedence)}	B05C5/00	B05C5/00		701
B05C5/007	8	{Slide-hopper coaters, i.e. apparatus in which the liquid or other fluent material flows freely on an inclined surface before contacting the work}	B05C5/00	B05C5/00		446
B05C5/008	9	{Slide-hopper curtain coaters}	B05C5/00	B05C5/00		391
B05C5/02	8	{the liquid or other fluent material being discharged through an outlet orifice by pressure, e.g.} from an outlet device in contact or almost in contact, with the work	B05C5/02	B05C5/02		5380
B05C5/0204	9	{for applying liquid or other fluent material to the edges of essentially flat articles}	B05C5/02	B05C5/02		525
B05C5/0208	9	{for applying liquid or other fluent material to separate articles (B05C5/0204 takes precedence)}	B05C5/02	B05C5/02		4077
B05C5/0212	10	{only at particular parts of the articles (at particular part of web, band, strip, belt or ribbon B05C5/025)}	B05C5/02	B05C5/02		1689
B05C5/0216	11	{by relative movement of article and outlet according to a predetermined path}	B05C5/02	B05C5/02		1090
B05C5/022	12	{the outlet being fixed during operation}	B05C5/02	B05C5/02		144
B05C5/0225	9	{characterised by flow controlling means, e.g. valves, located proximate the outlet (B05C5/0258, B05C5/0275 take precedence; supply valves upstream the coating head B05C11/1036)}	B05C5/02	B05C5/02		2254
B05C5/0229	10	{the valve being a gate valve or a sliding valve}<br><br><u>WARNING</u><br> Not complete, see B05C5/0225	B05C5/02	B05C5/02		137
B05C5/0233	11	{rotating valve, e.g. rotating perforated cylinder}<br><br><u>WARNING</u><br> Not complete, see B05C5/0225	B05C5/02	B05C5/02		130
B05C5/0237	10	{Fluid actuated valves}<br><br><u>WARNING</u><br> Not complete, see B05C5/0225	B05C5/02	B05C5/02		296
B05C5/0241	9	{for applying liquid or other fluent material to elongated work, e.g. wires, cables, tubes}	B05C5/02	B05C5/02		542
B05C5/0245	9	{for applying liquid or other fluent material to a moving work of indefinite length, e.g. to a moving web (B05C5/0241, B05C5/0254, B05C5/027, B05C5/0283 take precedence)}	B05C5/02	B05C5/02		856
B05C5/025	10	{only at particular part of the work (at particular part of separate articles B05C5/0212)}	B05C5/02	B05C5/02		222
B05C5/0254	9	{Coating heads with slot-shaped outlet (B05C5/0283 takes precedence)}	B05C5/02	B05C5/02		2238
B05C5/0258	10	{flow controlled, e.g. by a valve (B05C5/0262, B05C5/0266 take precedence)}	B05C5/02	B05C5/02		491
B05C5/0262	10	{adjustable in width, i.e. having lips movable relative to each other in order to modify the slot width, e.g. to close it}	B05C5/02	B05C5/02		403
B05C5/0266	10	{adjustable in length, e.g. for coating webs of different width}	B05C5/02	B05C5/02		248
B05C5/027	9	{Coating heads with several outlets, e.g. aligned transversally to the moving direction of a web to be coated (B05C5/0254 takes precedence)}	B05C5/02	B05C5/02		2144
B05C5/0275	10	{flow controlled, e.g. by a valve}	B05C5/02	B05C5/02		326
B05C5/0279	11	{independently, e.g. individually, flow controlled}	B05C5/02	B05C5/02		475
B05C5/0283	9	{Flat jet coaters, i.e. apparatus in which the liquid or other fluent material is projected from the outlet as a cohesive flat jet in direction of the work}	B05C5/02	B05C5/02		147
B05C5/0287	9	{with no relative movement between the outlet and a moving work during the application}	B05C5/02	B05C5/02		31
B05C5/0291	9	{the material being discharged on the work through discrete orifices as discrete droplets, beads or strips that coalesce on the work or are spread on the work so as to form a continuous coating}	B05C5/02	B05C5/02		223
B05C5/0295	9	{Floating coating heads or nozzles}	B05C5/02	B05C5/02		160
B05C7/00	7	Apparatus specially designed for applying liquid or other fluent material to the inside of hollow work	B05C7/00	B05C7/00		312
B05C7/005	8	{by devices in contact with moving work}	B05C7/00	B05C7/00		64
B05C7/02	8	the liquid or other fluent material being projected	B05C7/02	B05C7/02		377
B05C7/04	8	the liquid or other fluent material flowing or being moved through the work; the work being filled with liquid or other fluent material and emptied	B05C7/04	B05C7/04		380
B05C7/06	8	by devices moving in contact with the work	B05C7/06	B05C7/06		287
B05C7/08	9	for applying liquids or other fluent materials to the inside of tubes	B05C7/08	B05C7/08		491
B05C9/00	7	Apparatus or plant for applying liquid or other fluent material to surfaces by means not covered by any preceding group, or in which the means of applying the liquid or other fluent material is not important	B05C9/00	B05C9/00		167
B05C9/02	8	for applying liquid or other fluent material to surfaces by single means not covered by groups B05C1/00&#160;-&#160;B05C7/00, whether or not also using other means	B05C9/02	B05C9/02		341
B05C9/022	9	{to obtain ornamental coatings}	B05C9/02	B05C9/02		87
B05C9/025	10	{using silk screens or stencils}	B05C9/02	B05C9/02		51
B05C9/027	9	{using applicator shoes}	B05C9/02	B05C9/02		50
B05C9/04	8	for applying liquid or other fluent material to opposite sides of the work	B05C9/04	B05C9/04		1660
B05C9/045	9	{in which the opposite sides of the work are the internal and external surfaces of hollow articles}	B05C9/04	B05C9/04		93
B05C9/06	8	for applying two different liquids or other fluent materials, or the same liquid or other fluent material twice, to the same side of the work	B05C9/06	B05C9/06		1169
B05C9/08	8	for applying liquid or other fluent material and performing an auxiliary operation	B05C9/08	B05C9/08		357
B05C9/10	9	the auxiliary operation being performed before the application (B05C9/14 takes precedence)	B05C9/10	B05C9/10		1549
B05C9/12	9	the auxiliary operation being performed after the application (B05C9/14 takes precedence)	B05C9/12	B05C9/12		2032
B05C9/14	9	the auxiliary operation involving heating {or cooling}	B05C9/14	B05C9/14		5328
B05C11/00	7	Component parts, details or accessories not specifically provided for in groups B05C1/00&#160;-&#160;B05C9/00(means for manipulating or holding work B05C13/00; enclosures for apparatus, booths B05C15/00; spray booths B05B16/00)	B05C11/00	B05C11/00		2973
B05C11/02	8	Apparatus for spreading or distributing liquids or other fluent materials already applied to a surface {; Controlling means therefor}(B05C7/00 takes precedence; Hand tools for such purposes B05C17/10); Control of the thickness of a coating {by spreading or distributing liquids or other fluent materials already applied to the coated surface}(controlling supply of liquid or other fluent material B05C11/10)	B05C11/02	B05C11/02		686
B05C11/021	9	{Apparatus for spreading or distributing liquids or other fluent materials already applied to the surface of an elongated body, e.g. a wire, a tube}	B05C11/02	B05C11/02		289
B05C11/023	9	{Apparatus for spreading or distributing liquids or other fluent materials already applied to a surface (B05C11/021, B05C11/04 take precedence)}	B05C11/02	B05C11/02		1398
B05C11/025	10	{with an essentially cylindrical body, e.g. roll or rod}	B05C11/02	B05C11/02		1373
B05C11/026	10	{with an elongated body renewable by feeding it across the surface}	B05C11/02	B05C11/02		32
B05C11/028	10	{with a body having a large flat spreading or distributing surface}	B05C11/02	B05C11/02		451
B05C11/04	9	with blades	B05C11/04	B05C11/04		775
B05C11/041	10	{characterised by means for positioning, loading, or deforming the blades}	B05C11/04	B05C11/04		492
B05C11/042	11	{allowing local positioning, loading or deforming along the blades}	B05C11/04	B05C11/04		124
B05C11/044	10	{characterised by means for holding the blades}	B05C11/04	B05C11/04		139
B05C11/045	10	{characterised by the blades themselves}	B05C11/04	B05C11/04		210
B05C11/047	10	{provided with end dams}	B05C11/04	B05C11/04		39
B05C11/048	10	{Scrapers, i.e. metering blades having their edge oriented in the upstream direction in order to provide a reverse angle of attack}	B05C11/04	B05C11/04		310
B05C11/06	9	with a blast of gas or vapour	B05C11/06	B05C11/06		619
B05C11/08	9	Spreading liquid or other fluent material by manipulating the work, e.g. tilting	B05C11/08	B05C11/08		1225
B05C11/10	8	Storage, supply or control of liquid or other fluent material; Recovery of excess liquid or other fluent material {(B05C1/0813, B05C5/0225, B05C17/002 and B05C19/06 take precedence)}	B05C11/10	B05C11/10		8115
B05C11/1002	9	{Means for controlling supply, i.e. flow or pressure, of liquid or other fluent material to the applying apparatus, e.g. valves}	B05C11/10	B05C11/10		3237
B05C11/1005	10	{responsive to condition of liquid or other fluent material already applied to the surface, e.g. coating thickness, weight or pattern}	B05C11/10	B05C11/10		1210
B05C11/1007	10	{responsive to condition of liquid or other fluent material (B05C11/1005 takes precedence)}	B05C11/10	B05C11/10		379
B05C11/101	11	{responsive to weight of a container for liquid or other fluent material; responsive to level of liquid or other fluent material in a container}	B05C11/10	B05C11/10		584
B05C11/1013	11	{responsive to flow or pressure of liquid or other fluent material (B05C11/101 takes precedence; control of flow in general G05D7/00; control of fluid pressure in general G05D16/00)}	B05C11/10	B05C11/10		1105
B05C11/1015	10	{responsive to a conditions of ambient medium or target, e.g. humidity, temperature (B05C11/1005 takes precedence); responsive to position or movement of the coating head relative to the target}	B05C11/10	B05C11/10		1021
B05C11/1018	11	{responsive to distance of target}	B05C11/10	B05C11/10		394
B05C11/1021	11	{responsive to presence or shape of target (B05C11/1018 takes precedence)}	B05C11/10	B05C11/10		448
B05C11/1023	11	{responsive to velocity of target, e.g. to web advancement rate}	B05C11/10	B05C11/10		146
B05C11/1026	10	{Valves (in general F16K; B05C5/0225 takes precedence)}	B05C11/10	B05C11/10		681
B05C11/1028	11	{Lift valves}	B05C11/10	B05C11/10		93
B05C11/1031	11	{Gate valves; Sliding valves}	B05C11/10	B05C11/10		64
B05C11/1034	10	{specially designed for conducting intermittent application of small quantities, e.g. drops, of coating material (B05C5/0225, B05C11/1026 take precedence)}	B05C11/10	B05C11/10		520
B05C11/1036	9	{Means for supplying a selected one of a plurality of liquids or other fluent materials, or several in selected proportions, to the applying apparatus}	B05C11/10	B05C11/10		675
B05C11/1039	9	{Recovery of excess liquid or other fluent material; Controlling means therefor}	B05C11/10	B05C11/10		3742
B05C11/1042	9	{provided with means for heating or cooling the liquid or other fluent material in the supplying means upstream of the applying apparatus}	B05C11/10	B05C11/10		2001
B05C11/1044	9	{Apparatus or installations for supplying liquid or other fluent material to several applying apparatus or several dispensing outlets, e.g. to several extrusion nozzles}	B05C11/10	B05C11/10		312
B05C11/1047	9	{Apparatus or installations for supplying liquid or other fluent material comprising a buffer container or an accumulator between the supply source and the applicator}	B05C11/10	B05C11/10		359
B05C11/105	9	by capillary action, e.g. using wicks	B05C11/105	B05C11/105		57
B05C11/11	8	Vats or other containers for liquids or other fluent materials	B05C11/11	B05C11/11		1339
B05C11/115	9	Sealing means for work inlet or outlet	B05C11/115	B05C11/115		84
B05C13/00	7	Means for manipulating or holding work, e.g. for separate articles {(B05C1/0821 takes precedence)}	B05C13/00	B05C13/00		1652
B05C13/02	8	for particular articles	B05C13/02	B05C13/02		14515
B05C13/025	9	{relatively small cylindrical objects, e.g. cans, bottles}	B05C13/02	B05C13/02		475
B05C15/00	7	Enclosures for apparatus; Booths (spray booths B05B16/00)	B05C15/00	B05C15/00		716
B05C17/00	7	Hand tools or apparatus using hand held tools, for applying liquids or other fluent materials to, for spreading applied liquids or other fluent materials on, or for partially removing applied liquids or other fluent materials from, surfaces ({casings or accessories for storing or handling solid or pasty toilet or cosmetic substances A45D40/00;} brushes A46B; {shoe polish applicators A47L23/05; surgical glue applicators A61B17/00491;} absorbent pads, e.g. swabs, for applying media to the human body A61F13/15; {hand-held applicators for applying or spreading media, e.g. remedies, on the human body A61M35/003; implements for writing or drawing B43K; hand-held desk devices for applying liquid, e.g. adhesive, by contact to surfaces B43M11/06;} implements or apparatus for removing dry paint from surfaces B44D3/16{; container closures with pads or like contents-applying means B65D47/42})	B05C17/00	B05C17/00		827
B05C17/001	8	{incorporating means for heating or cooling the liquid or other fluent material (B05C17/00523 takes precedence)}	B05C17/00	B05C17/00		76
B05C17/002	8	{with feed system for supplying material from an external source; Supply controls therefor (B05C17/02 takes precedence)}	B05C17/00	B05C17/00		895
B05C17/003	9	{with means for filling or refilling the hand tool container}	B05C17/00	B05C17/00		101
B05C17/005	8	for discharging material {from a reservoir or container located in or on the hand tool} through an outlet orifice by pressure {without using surface contacting members like pads or brushes}	B05C17/005	B05C17/005		504
B05C17/00503	9	{Details of the outlet element (B05C17/00523 takes precedence; nozzles for deformable tubular containers B65D35/38)}	B05C17/005	B05C17/005		424
B05C17/00506	10	{Means for connecting the outlet element to, or for disconnecting it from, the hand tool or its container}	B05C17/005	B05C17/005		319
B05C17/00509	11	{of the bayonet type}	B05C17/005	B05C17/005		131
B05C17/00513	11	{of the thread type}	B05C17/005	B05C17/005		303
B05C17/00516	10	{Shape or geometry of the outlet orifice or the outlet element}	B05C17/005	B05C17/005		1697
B05C17/0052	9	{Accessories therefor}	B05C17/005	B05C17/005		584
B05C17/00523	9	{provided with means to heat the material}	B05C17/005	B05C17/005		189
B05C17/00526	10	{the material being supplied to the apparatus in a solid state, e.g. rod, and melted before application (B05C17/0054 takes precedence)}	B05C17/005	B05C17/005		131
B05C17/0053	11	{the driving means for the material being manual, mechanical or electrical}	B05C17/005	B05C17/005		202
B05C17/00533	12	{comprising a piston}	B05C17/005	B05C17/005		96
B05C17/00536	12	{the driving means comprising one or more rollers}	B05C17/005	B05C17/005		31
B05C17/0054	10	{the driving means for the material being pneumatic or hydraulic}	B05C17/005	B05C17/005		31
B05C17/00543	11	{comprising a piston}	B05C17/005	B05C17/005		47
B05C17/00546	10	{Details of the heating means}	B05C17/005	B05C17/005		217
B05C17/0055	11	{Burners, e.g. for catalytic combustion specially adapted for hand tools or apparatus using hand tools}	B05C17/005	B05C17/005		24
B05C17/00553	9	{with means allowing the stock of material to consist of at least two different components}	B05C17/005	B05C17/005		1210
B05C17/00556	10	{with means for adjusting the proportions of the components}	B05C17/005	B05C17/005		59
B05C17/00559	10	{the different components being stored in coaxial chambers}	B05C17/005	B05C17/005		193
B05C17/00563	11	{the chambers being at least initially placed in series}	B05C17/005	B05C17/005		22
B05C17/00566	10	{with a dynamic mixer in the nozzle}	B05C17/005	B05C17/005		154
B05C17/00569	9	{with a pump in the hand tool}	B05C17/005	B05C17/005		169
B05C17/00573	9	{the reservoir or container being pneumatically or hydraulically pressurized (B05C17/0054, B05C17/015 take precedence)}	B05C17/005	B05C17/005		74
B05C17/00576	9	{characterised by the construction of a piston as pressure exerting means, or of the co-operating container}	B05C17/005	B05C17/005		544
B05C17/00579	10	{comprising means for allowing entrapped air to escape to the atmosphere}	B05C17/005	B05C17/005		160
B05C17/00583	9	{the container for the material to be dispensed being deformable}	B05C17/005	B05C17/005		625
B05C17/00586	9	{Means, generally located near the nozzle, for piercing or perforating the front part of a cartridge}	B05C17/005	B05C17/005		223
B05C17/00589	9	{comprising a guiding rotating element, e.g. a wheel}	B05C17/005	B05C17/005		82
B05C17/00593	9	{Hand tools of the syringe type}	B05C17/005	B05C17/005		607
B05C17/00596	9	{The liquid or other fluent material being supplied from a rigid removable cartridge having no active dispensing means, i.e. the cartridge requiring cooperation with means of the handtool to expel the material}	B05C17/005	B05C17/005		715
B05C17/01	9	with {manually} mechanically or electrically actuated piston or the like {(B05C17/00533 takes precedence)}	B05C17/01	B05C17/01		1235
B05C17/0103	10	{with electrically actuated piston or the like}	B05C17/01	B05C17/01		582
B05C17/0106	10	{with means for longitudinally cutting container walls during relative displacement of the piston and its cooperating container}	B05C17/01	B05C17/01		53
B05C17/0109	10	{the piston being pulled during application}	B05C17/01	B05C17/01		34
B05C17/0113	10	{the piston rod being flexible or articulated (B05C17/0109 takes precedence)}	B05C17/01	B05C17/01		62
B05C17/0116	10	{characterised by the piston driving means (B05C17/0103, B05C17/0109, B05C17/0113, B05C17/015 take precedence)}	B05C17/01	B05C17/01		166
B05C17/012	11	{Stepwise advancing mechanism, e.g. pawl and ratchets}	B05C17/01	B05C17/01		74
B05C17/0123	12	{Lever actuated}	B05C17/01	B05C17/01		413
B05C17/0126	13	{comprising an element, e.g. an arc compensating element, articulated at one end on the lever and at the other end on the piston rod driving means, e.g. a pawl}	B05C17/01	B05C17/01		139
B05C17/013	13	{comprising a freely rotating element, e.g. a roller, between the lever and a piston rod driving means, e.g. a pawl}	B05C17/01	B05C17/01		25
B05C17/0133	11	{Nut and bolt advancing mechanism, e.g. threaded piston rods}	B05C17/01	B05C17/01		270
B05C17/0136	10	{comprising an energy storing element, e.g. a spring, for exerting, e.g. when released, pressure on the material (B05C17/015 takes precedence)}	B05C17/01	B05C17/01		155
B05C17/014	10	{comprising means for preventing oozing (B05C17/0146 takes precedence)}	B05C17/01	B05C17/01		186
B05C17/0143	10	{comprising means for cutting or cleaning the cartridge nozzle tip}	B05C17/01	B05C17/01		39
B05C17/0146	10	{comprising a valve in the proximity of the nozzle that is not actuated by pressure, e.g. manually actuated}	B05C17/01	B05C17/01		169
B05C17/015	9	with pneumatically {or hydraulically} actuated piston or the like {(B05C17/00543 takes precedence)}	B05C17/015	B05C17/015		666
B05C17/02	8	Rollers {(for applying toilet or cosmetic substances A45D34/04); Hand tools comprising coating rollers or coating endless belts}	B05C17/02	B05C17/02		855
B05C17/0202	9	{Hand tools comprising a coating endless belt}	B05C17/02	B05C17/02		22
B05C17/0205	9	{characterised by the handle, e.g. handle shape or material (B05C17/0217, B05C17/022 take precedence)}	B05C17/02	B05C17/02		363
B05C17/0207	9	{characterised by the cover, e.g. cover material or structure, special surface for producing patterns (B05C17/0212, B05C17/0352 take precedence)}	B05C17/02	B05C17/02		456
B05C17/021	9	{comprising means to avoid excessive crushing of the roller cover, e.g. a spacer}	B05C17/02	B05C17/02		17
B05C17/0212	9	{the coating surface of the roller being a body of revolution generated by a generatrix that is not a straight line parallel to the roller axis, e.g. for allowing coating of non planar surfaces (B05C17/0227, B05C17/0352 take precedence)}	B05C17/02	B05C17/02		116
B05C17/0215	9	{the coating roller itself, i.e. not only its cover being deformable, e.g. to allow proper coating of non-plane surfaces (B05C17/0227 takes precedence)}	B05C17/02	B05C17/02		64
B05C17/0217	9	{comprising a frame supporting the coating roller at both ends or being intented to be hold at both ends by the user (B05C17/0222, B05C17/0227, B05C17/0352, B05C17/0357 take precedence)}	B05C17/02	B05C17/02		325
B05C17/022	9	{comprising means for angularly adjusting or allowing angular movement of the roller relative to its handle (B05C17/0227 takes precedence)}	B05C17/02	B05C17/02		181
B05C17/0222	9	{comprising protecting shields, drip pans, spatter guards or the like (B05C17/03 take precedence)}	B05C17/02	B05C17/02		183
B05C17/0225	9	{comprising a lateral plate, edge guard or shield}	B05C17/02	B05C17/02		101
B05C17/0227	9	{comprising several coating rollers (B05C17/0352 takes precedence)}	B05C17/02	B05C17/02		81
B05C17/023	10	{all of them having parallel axises}	B05C17/02	B05C17/02		152
B05C17/0232	11	{all of them having the same axis}	B05C17/02	B05C17/02		95
B05C17/0235	9	{Rollers comprising an additional non-rotating applicator or comprising a coating roller replaceable by a non-rotating applicator}	B05C17/02	B05C17/02		78
B05C17/0237	9	{comprising means for preventing the rotation of the roller (B05C17/024 takes precedence)}	B05C17/02	B05C17/02		19
B05C17/024	9	{the coating roller being motor driven}	B05C17/02	B05C17/02		42
B05C17/0242	9	{comprising rotating guiding elements}	B05C17/02	B05C17/02		41
B05C17/0245	9	{Accessories}	B05C17/02	B05C17/02		341
B05C17/0247	9	{Rollers for coating under water}	B05C17/02	B05C17/02		7
B05C17/025	9	with self-contained reservoir {or container for liquid or other fluent material, located inside the coating roller}	B05C17/025	B05C17/025		194
B05C17/03	9	with feed system for supplying material from an external source {or with a reservoir or container for liquid or other fluent material located in or on the hand tool outside the coating roller}	B05C17/03	B05C17/03		62
B05C17/0308	10	{the liquid being supplied to the inside of the coating roller}	B05C17/03	B05C17/03		405
B05C17/0316	10	{with pressurised or compressible container}	B05C17/03	B05C17/03		113
B05C17/0325	11	{attached to the hand tool, e.g. into the handle}	B05C17/03	B05C17/03		126
B05C17/0333	10	{with pump}	B05C17/03	B05C17/03		163
B05C17/0341	11	{attached to the hand tool}	B05C17/03	B05C17/03		96
B05C17/035	10	direct {or indirectly} to the outer surface of the {coating} roller	B05C17/035	B05C17/035		176
B05C17/0352	11	{indirectly, i.e. by using transfer means, e.g. pads, brushes, rollers or bands}	B05C17/035	B05C17/035		44
B05C17/0355	12	{using transfer rollers}	B05C17/035	B05C17/035		285
B05C17/0357	11	{directly from a container attached to the hand tool, e.g. by gravity or dipping}	B05C17/035	B05C17/035		157
B05C17/04	9	Stencil rollers {(B05C17/0207 takes precedence)}	B05C17/04	B05C17/04		21
B05C17/06	8	Stencils (B05C17/04 takes precedence; stencils used in connection with printing plates or foils B41N1/24; drawing accessories B43L13/00)	B05C17/06	B05C17/06		562
B05C17/08	9	Stencil holders	B05C17/08	B05C17/08		82
B05C17/10	8	Hand tools for removing partially or for spreading or redistributing applied liquids or other fluent materials, e.g. colour touchers	B05C17/10	B05C17/10		569
B05C17/12	8	Other hand tools for producing patterns	B05C17/12	B05C17/12		146
B05C19/00	7	Apparatus specially adapted for applying particulate materials to surfaces	B05C19/00	B05C19/00		354
B05C19/001	8	{Flocking}	B05C19/00	B05C19/00		207
B05C19/002	9	{Electrostatic flocking (see for electrostatic projection or pulverisation B05B)}	B05C19/00	B05C19/00		378
B05C19/004	9	{from an outlet device in contact, or almost in contact with the work}	B05C19/00	B05C19/00		19
B05C19/005	8	{Apparatus specially designed for applying particulate materials to the inside of hollow work}	B05C19/00	B05C19/00		53
B05C19/007	9	{for applying the particulate materials to the inside of hollow tubes}	B05C19/00	B05C19/00		64
B05C19/008	8	{Accessories or implements for use in connection with applying particulate materials to surfaces; not provided elsewhere in B05C19/00}	B05C19/00	B05C19/00		163
B05C19/02	8	using fluidised-bed techniques (fluidised-bed technique in general B01J8/24)	B05C19/02	B05C19/02		324
B05C19/025	9	{Combined with electrostatic means}	B05C19/02	B05C19/02		172
B05C19/04	8	the particulate material being projected, poured or allowed to flow onto the surface of the work (B05C19/02 takes precedence; involving spraying or electrostatic projection B05B){(B05C19/005 takes precedence)}	B05C19/04	B05C19/04		912
B05C19/06	8	Storage, supply or control of the application of particulate material; Recovery of excess particulate material	B05C19/06	B05C19/06		745
B05C21/00	7	Accessories or implements for use in connection with applying liquids or other fluent materials to surfaces, not provided for in groups B05C1/00&#160;-&#160;B05C19/00(accessories or implements for use in connection with painting or artistic drawing and fully provided for in B44D3/02&#160;-&#160;B44D3/38, see subgroups of B44D3/00)	B05C21/00	B05C21/00		853
B05C21/005	8	{Masking devices (stencils B05C17/06; masking devices for which the means for applying liquids or other fluent material is spraying or is not important B05B12/20)}	B05C21/00	B05C21/00		591
