B60G1/00	7	Suspensions with rigid connection between axle and frame	B60G1/00	B60G1/00		116
B60G1/02	8	with continuous axle	B60G1/02	B60G1/02		56
B60G1/04	8	with divided axle	B60G1/04	B60G1/04		40
B60G3/00	7	Resilient suspensions for a single wheel (pivoted suspensions arms per se, attachment thereof to sprung part of the vehicle, buffer means for limiting movement of arms B60G7/00; {rigid axle suspensions B60G9/00;} characterised by arrangement, location or type of springs B60G11/00)	B60G3/00	B60G3/00		626
B60G3/01	8	the wheel being mounted for sliding movement, e.g. in or on a vertical guide (camber maintaining means B60G3/26)	B60G3/01	B60G3/01		820
B60G3/02	8	with a single pivoted arm	B60G3/02	B60G3/02		211
B60G3/04	9	the arm being essentially transverse to the longitudinal axis of the vehicle	B60G3/04	B60G3/04		103
B60G3/06	10	the arm being rigid	B60G3/06	B60G3/06		512
B60G3/08	11	the arm forming the axle housing	B60G3/08	B60G3/08		54
B60G3/10	10	the arm itself being resilient, e.g. leaf spring {(B60G7/003 takes precedence)}	B60G3/10	B60G3/10		99
B60G3/12	9	the arm being essentially parallel to the longitudinal axis of the vehicle	B60G3/12	B60G3/12		132
B60G3/14	10	the arm being rigid	B60G3/14	B60G3/14		613
B60G3/145	11	{the arm forming the axle housing}	B60G3/14	B60G3/14		310
B60G3/16	10	the arm itself being resilient, e.g. leaf spring {(B60G7/003 takes precedence)}	B60G3/16	B60G3/16		77
B60G3/18	8	with two or more pivoted arms, e.g. parallelogram	B60G3/18	B60G3/18		621
B60G3/185	9	{the arms being essentially parallel to the longitudinal axis of the vehicle}	B60G3/18	B60G3/18		106
B60G3/20	9	all arms being rigid	B60G3/20	B60G3/20		2796
B60G3/202	10	{having one longitudinal arm and two parallel transversal arms, e.g. dual-link type strut suspension}	B60G3/20	B60G3/20		277
B60G3/205	11	{with the pivotal point of the longitudinal arm being on the vertical plane defined by the wheel rotation axis and the wheel ground contact point}	B60G3/20	B60G3/20		113
B60G3/207	10	{the arms being essentially parallel to the longitudinal axis of the vehicle}	B60G3/20	B60G3/20		171
B60G3/22	10	a rigid arm forming the axle housing	B60G3/22	B60G3/22		133
B60G3/225	11	{the arm being of the trailing wishbone type}	B60G3/22	B60G3/22		118
B60G3/24	10	a rigid arm being formed by the live axle {(B60G3/22, B60G3/26 take precedence; driving arrangements B60K17/22, B60K17/30, B60K17/32)}	B60G3/24	B60G3/24		477
B60G3/26	10	Means for maintaining substantially-constant wheel camber during suspension movement {; Means for controlling the variation of the wheel position during suspension movement (B60G3/202, B60G3/22, B60G7/003, B60G7/006 take precedence; means for adjusting camber, castor, or toe-in B62D17/00)}	B60G3/26	B60G3/26		964
B60G3/265	11	{with a strut cylinder contributing to the suspension geometry by being linked to the wheel support via an articulation}	B60G3/26	B60G3/26		190
B60G3/28	9	at least one of the arms itself being resilient, e.g. leaf spring {(B60G7/003 takes precedence)}	B60G3/28	B60G3/28		239
B60G3/285	10	{the arm being essentially parallel to the longitudinal axis of the vehicle}	B60G3/28	B60G3/28		126
B60G5/00	7	Resilient suspensions for a set of tandem wheels or axles having interrelated movements	B60G5/00	B60G5/00		352
B60G5/005	8	{the wheels being fixed on a non-pivotal structure, e.g. a sliding mount}	B60G5/00	B60G5/00		108
B60G5/01	8	the set being characterised by having more than two successive axles	B60G5/01	B60G5/01		237
B60G5/02	8	mounted on a single pivoted arm {, e.g. the arm being rigid}	B60G5/02	B60G5/02		636
B60G5/025	9	{the arm being transverse to the longitudinal axis of the vehicle}	B60G5/02	B60G5/02		21
B60G5/03	9	the arm itself being resilient, e.g. a leafspring (B60G5/053 takes precedence)	B60G5/03	B60G5/03		227
B60G5/04	8	with two or more pivoted arms, the movements of which are resiliently interrelated {, e.g. the arms being rigid}	B60G5/04	B60G5/04		624
B60G5/043	9	{the arms being transverse to the longitudinal axis of the vehicle}	B60G5/04	B60G5/04		60
B60G5/047	9	at least one arm being resilient, e.g. a leafspring (B60G5/053 takes precedence)	B60G5/047	B60G5/047		499
B60G5/053	9	a leafspring being used as equilibration unit between two axle-supporting units	B60G5/053	B60G5/053		517
B60G5/06	9	the arms turning on a common pivot {, e.g. being rigid}	B60G5/06	B60G5/06		127
B60G5/065	10	{at least one arm being resilient}	B60G5/06	B60G5/06		8
B60G7/00	7	Pivoted suspension arms; Accessories thereof (means for maintaining substantially constant wheel camber during suspension movement B60G3/26; {articulations for wheels B60G5/00; leaf spring attaching means B60G11/10, B60G11/12; trailing arm twist beam axle attaching means B60G21/052; articulations in general F16C})	B60G7/00	B60G7/00		1625
B60G7/001	8	{Suspension arms, e.g. constructional features (B60G7/006 takes precedence)}	B60G7/00	B60G7/00		4245
B60G7/003	9	{of adjustable length}	B60G7/00	B60G7/00		409
B60G7/005	8	{Ball joints (B60G7/006 takes precedence; for steering linkage B62D7/16; ball joints per seF16C11/06)}	B60G7/00	B60G7/00		1970
B60G7/006	8	{Attaching arms to sprung or unsprung part of vehicle, characterised by comprising attachment means controlled by an external actuator, e.g. a fluid or electrical motor (B62D7/146 takes precedence)}	B60G7/00	B60G7/00		968
B60G7/008	8	{Attaching arms to unsprung part of vehicle (B60G7/005, B60G7/006 take precedence)}	B60G7/00	B60G7/00		1665
B60G7/02	8	Attaching arms to sprung part of vehicle {(B60G7/006 takes precedence)}	B60G7/02	B60G7/02		3481
B60G7/04	8	Buffer means for limiting movement of arms {(stops limiting fluid passage in fluid dampers F16F9/49; stroke-limiting stops for fluid dampers F16F9/58)}	B60G7/04	B60G7/04		1439
B60G9/00	7	Resilient suspensions of a rigid axle or axle housing for two or more wheels {(the axle being a part of a set of tandem axles B60G5/00-B60G5/065; with leaf springs B60G11/02-B60G11/08)}	B60G9/00	B60G9/00		1512
B60G9/003	8	{the axle being rigidly connected to a trailing guiding device}	B60G9/00	B60G9/00		1019
B60G9/006	8	{the axle being connected to two trailing arms with only one of them being rigidly connected to the axle}	B60G9/00	B60G9/00		31
B60G9/02	8	the axle or housing being pivotally mounted on the vehicle {, e.g. the pivotal axis being parallel to the longitudinal axis of the vehicle (B60G9/003 takes precedence)}	B60G9/02	B60G9/02		1449
B60G9/022	9	{the axle having an imaginary pivotal point}	B60G9/02	B60G9/02		132
B60G9/025	10	{using linkages for the suspension of the axle allowing its lateral swinging displacement}	B60G9/02	B60G9/02		58
B60G9/027	9	{the axle having either a triangular, a "T" or "U" shape and being directly articulated with the chassis only by its middle apex, e.g. De Dion suspension}	B60G9/02	B60G9/02		307
B60G9/04	8	the axle or housing not being pivotally mounted on the vehicle {(B60G9/003 takes precedence)}	B60G9/04	B60G9/04		229
B60G11/00	7	Resilient suspensions characterised by arrangement, location or kind of springs (single wheel suspension by pivoted arm resilient in itself B60G3/00; adjusting spring characteristic B60G17/00; springs per seF16F)<br><br><u>NOTE</u><br><br>The term "torsion bar" includes torsion tube or the like. The term "rubber" includes synthetic substitutes of a similar nature.	B60G11/00	B60G11/00		583
B60G11/003	8	{Lubrication devices for springs and dampers (vehicle lubrication devices in general B60R17/00; for leaf springs in general F16F1/24)}	B60G11/00	B60G11/00		52
B60G11/006	8	{Centrally located spring units, e.g. all wheels being connected to a common spring unit (B60G5/00, B60G17/033 take precedence)}	B60G11/00	B60G11/00		50
B60G11/02	8	having leaf springs only {(B60G11/006 takes precedence)}	B60G11/02	B60G11/02		1274
B60G11/025	9	{reparing devices for leaf springs}	B60G11/02	B60G11/02		47
B60G11/04	9	arranged substantially parallel to the longitudinal axis of the vehicle	B60G11/04	B60G11/04		1806
B60G11/06	9	arranged obliquely to the longitudinal axis of the vehicle	B60G11/06	B60G11/06		82
B60G11/08	9	arranged substantially transverse to the longitudinal axis of the vehicle	B60G11/08	B60G11/08		1273
B60G11/10	9	characterised by means specially adapted for attaching the spring to axle or sprung part of the vehicle	B60G11/10	B60G11/10		1002
B60G11/107	10	Sliding or rolling mountings	B60G11/107	B60G11/107		423
B60G11/113	10	Mountings on the axle (B60G11/107 takes precedence)	B60G11/113	B60G11/113		958
B60G11/12	10	Links, pins, or bushes	B60G11/12	B60G11/12		1262
B60G11/125	11	{Multiple-eye arrangements}	B60G11/12	B60G11/12		52
B60G11/14	8	having helical, spiral or coil springs only {(B60G11/006 takes precedence)}	B60G11/14	B60G11/14		1737
B60G11/15	9	Coil springs resisting deflection by winding up	B60G11/15	B60G11/15		270
B60G11/16	9	characterised by means specially adapted for attaching the spring to axle or sprung part of the vehicle	B60G11/16	B60G11/16		1070
B60G11/18	8	having torsion-bar springs only {(B60G11/006 takes precedence; having rubber springs of the torsional-energy-absorption type B60G11/23)}<br><br><u>NOTE</u><br><br>B60G11/184 takes precedence over B60G11/181&#160;-&#160;B60G11/183	B60G11/18	B60G11/18		596
B60G11/181	9	{arranged in a plane parallel to the longitudinal axis of the vehicle}	B60G11/18	B60G11/18		289
B60G11/182	9	{arranged in a plane oblique to the longitudinal axis of the vehicle}	B60G11/18	B60G11/18		89
B60G11/183	9	{arranged in a plane transverse to the longitudinal axis of the vehicle}	B60G11/18	B60G11/18		368
B60G11/184	9	{the torsion-bar consisting of a bundle of torsion elements}	B60G11/18	B60G11/18		22
B60G11/185	10	{the elements being rods}	B60G11/18	B60G11/18		44
B60G11/186	11	{of hexagonal cross-section}	B60G11/18	B60G11/18		6
B60G11/187	10	{the elements being leaf-springs loaded by twisting}	B60G11/18	B60G11/18		19
B60G11/188	10	{the elements being cables}	B60G11/18	B60G11/18		5
B60G11/189	9	{the torsion spring consisting of a tube with a slit}	B60G11/18	B60G11/18		10
B60G11/20	9	characterised by means specially adapted for attaching the spring to axle or sprung part of the vehicle	B60G11/20	B60G11/20		311
B60G11/22	8	having rubber springs only {(B60G11/006 takes precedence)}	B60G11/22	B60G11/22		951
B60G11/225	9	{Neidhart type rubber springs}	B60G11/22	B60G11/22		242
B60G11/23	9	of the torsional-energy-absorption type	B60G11/23	B60G11/23		296
B60G11/24	9	characterised by means specially adapted for attaching the spring to axle or sprung part of the vehicle	B60G11/24	B60G11/24		127
B60G11/26	8	having fluid springs only, e.g. hydropneumatic springs ({B60G11/006,}B60G15/12 take precedence)	B60G11/26	B60G11/26		336
B60G11/265	9	{hydraulic springs}	B60G11/26	B60G11/26		282
B60G11/27	9	wherein the fluid is a gas	B60G11/27	B60G11/27		2511
B60G11/28	9	characterised by means specially adapted for attaching the spring to axle or sprung part of the vehicle	B60G11/28	B60G11/28		864
B60G11/30	9	having pressure fluid accumulator therefor, e.g. accumulator arranged in vehicle frame {(dampers accumulating utilisable energy B60G13/14)}	B60G11/30	B60G11/30		435
B60G11/32	8	having springs of different kinds {(B60G11/006 takes precedence)}	B60G11/32	B60G11/32		153
B60G11/34	9	including leaf springs	B60G11/34	B60G11/34		361
B60G11/36	10	and also helical, spiral or coil springs	B60G11/36	B60G11/36		1353
B60G11/38	10	and also rubber springs	B60G11/38	B60G11/38		222
B60G11/40	11	the rubber springs being attached to the axle	B60G11/40	B60G11/40		109
B60G11/42	11	the rubber springs being attached to sprung part of the vehicle	B60G11/42	B60G11/42		641
B60G11/44	10	and also torsion-bar springs	B60G11/44	B60G11/44		246
B60G11/46	10	and also fluid springs	B60G11/46	B60G11/46		285
B60G11/465	11	{with a flexible wall}	B60G11/46	B60G11/46		682
B60G11/48	9	not including leaf springs	B60G11/48	B60G11/48		117
B60G11/50	10	having helical, spiral or coil springs, and also torsion-bar springs	B60G11/50	B60G11/50		155
B60G11/52	10	having helical, spiral or coil springs, and also rubber springs	B60G11/52	B60G11/52		303
B60G11/54	11	with rubber springs arranged within helical, spiral or coil springs	B60G11/54	B60G11/54		102
B60G11/56	10	having helical, spiral or coil springs, and also fluid springs	B60G11/56	B60G11/56		138
B60G11/58	11	arranged coaxially	B60G11/58	B60G11/58		180
B60G11/60	10	having both rubber springs and torsion-bar springs	B60G11/60	B60G11/60		137
B60G11/62	10	having both rubber springs and fluid springs	B60G11/62	B60G11/62		165
B60G11/64	10	having both torsion-bar springs and fluid springs	B60G11/64	B60G11/64		189
B60G13/00	7	Resilient suspensions characterised by arrangement, location or type of vibration dampers (adjusting damping effect B60G17/06; vibration dampers per seF16F)	B60G13/00	B60G13/00		603
B60G13/001	8	{Arrangements for attachment of dampers (mounting arrangements of combined spring and damper units B60G15/00; mountings of fluid dampers in general F16F9/54)}	B60G13/00	B60G13/00		567
B60G13/003	9	{characterised by the mounting on the vehicle body or chassis of the damper unit}	B60G13/00	B60G13/00		1152
B60G13/005	9	{characterised by the mounting on the axle or suspension arm of the damper unit}	B60G13/00	B60G13/00		737
B60G13/006	10	{on the stub axle}	B60G13/00	B60G13/00		325
B60G13/008	10	{involving use of an auxiliary cylinder (B60G13/006 takes precedence)}	B60G13/00	B60G13/00		171
B60G13/02	8	having dampers dissipating energy, e.g. frictionally	B60G13/02	B60G13/02		234
B60G13/04	9	mechanically, e.g. having frictionally-engaging springs as damping elements	B60G13/04	B60G13/04		581
B60G13/06	9	of fluid type	B60G13/06	B60G13/06		327
B60G13/08	10	hydraulic	B60G13/08	B60G13/08		1219
B60G13/10	10	pneumatic	B60G13/10	B60G13/10		286
B60G13/12	10	quasi-fluid, i.e. having powdered medium	B60G13/12	B60G13/12		10
B60G13/14	8	having dampers accumulating utilisable energy, e.g. compressing air {(fluid springs with an accumulator B60G11/30)}	B60G13/14	B60G13/14		765
B60G13/16	8	having dynamic absorbers as main damping means, i.e. spring-mass system vibrating out of phase	B60G13/16	B60G13/16		258
B60G13/18	9	combined with energy-absorbing means	B60G13/18	B60G13/18		171
B60G15/00	7	Resilient suspensions characterised by arrangement, location or type of combined spring and vibration damper, e.g. telescopic type (combined spring and vibration-dampers per seF16F)	B60G15/00	B60G15/00		377
B60G15/02	8	having mechanical spring	B60G15/02	B60G15/02		627
B60G15/04	9	and mechanical damper {or dynamic damper}	B60G15/04	B60G15/04		375
B60G15/06	9	and fluid damper	B60G15/06	B60G15/06		1115
B60G15/061	10	{with a coil spring being mounted inside the damper}	B60G15/06	B60G15/06		209
B60G15/062	10	{the spring being arranged around the damper (B60G15/061, B60G15/067, B60G15/07 take precedence)}	B60G15/06	B60G15/06		821
B60G15/063	11	{characterised by the mounting of the spring on the damper (B60G15/065, B60G15/066 take precedence)}	B60G15/06	B60G15/06		812
B60G15/065	11	{characterised by the use of a combination of springs}	B60G15/06	B60G15/06		236
B60G15/066	11	{the spring being different from a coil spring (B60G15/065 takes precedence)}	B60G15/06	B60G15/06		86
B60G15/067	10	{characterised by the mounting on the vehicle body or chassis of the spring and damper unit}	B60G15/06	B60G15/06		1085
B60G15/068	11	{specially adapted for MacPherson strut-type suspension}	B60G15/06	B60G15/06		1210
B60G15/07	10	the damper being connected to the stub axle and the spring being arranged around the damper {(B60G15/068 takes precedence)}	B60G15/07	B60G15/07		655
B60G15/08	8	having fluid spring	B60G15/08	B60G15/08		212
B60G15/10	9	and mechanical damper {or dynamic damper}	B60G15/10	B60G15/10		58
B60G15/12	9	and fluid damper	B60G15/12	B60G15/12		900
B60G15/14	10	the damper being connected to the stub axle and the spring being arranged around the damper	B60G15/14	B60G15/14		254
B60G17/00	7	Resilient suspensions having means for adjusting the spring or vibration-damper characteristics, for regulating the distance between a supporting surface and a sprung part of vehicle or for locking suspension during use to meet varying vehicular or surface conditions, e.g. due to speed or load {(levelling or stabilising systems for tippers B60P1/045)}	B60G17/00	B60G17/00		1057
B60G17/002	8	{by temperature regulation of the suspension unit, e.g. heat operated systems}	B60G17/00	B60G17/00		147
B60G17/005	8	Suspension locking arrangements {(for retractable wheels B62D61/12)}	B60G17/005	B60G17/005		1215
B60G17/015	8	the regulating means comprising electric or electronic elements ({B60G17/002}, B60G17/005 take precedence)	B60G17/015	B60G17/015		3457
B60G17/0152	9	{characterised by the action on a particular type of suspension unit (B60G17/01941 takes precedence)}	B60G17/015	B60G17/015		1260
B60G17/0155	10	{pneumatic unit}	B60G17/015	B60G17/015		1287
B60G17/0157	10	{non-fluid unit, e.g. electric motor}	B60G17/015	B60G17/015		1298
B60G17/016	9	characterised by their responsiveness, when the vehicle is travelling, to specific motion, a specific condition, or driver input {(B60G17/017 takes precedence)}	B60G17/016	B60G17/016		1462
B60G17/0161	10	{mainly during straight-line motion (B60G17/0164 takes precedence)}	B60G17/016	B60G17/016		145
B60G17/0162	10	{mainly during a motion involving steering operation, e.g. cornering, overtaking (B60G17/0164 takes precedence)}	B60G17/016	B60G17/016		1561
B60G17/0163	11	{the control involving steering geometry, e.g. four-wheel steering}	B60G17/016	B60G17/016		101
B60G17/0164	10	{mainly during accelerating or braking}	B60G17/016	B60G17/016		543
B60G17/0165	10	to an external condition, e.g. rough road surface, side wind	B60G17/0165	B60G17/0165		2302
B60G17/017	9	characterised by their use when the vehicle is stationary, e.g. during loading, engine start-up or switch-off	B60G17/017	B60G17/017		761
B60G17/018	9	characterised by the use of a specific signal treatment or control method	B60G17/018	B60G17/018		2759
B60G17/0182	10	{involving parameter estimation, e.g. observer, Kalman filter}	B60G17/018	B60G17/018		715
B60G17/0185	10	for failure detection	B60G17/0185	B60G17/0185		614
B60G17/019	9	characterised by the type of sensor or the arrangement thereof {(B60G17/01941 takes precedence)}	B60G17/019	B60G17/019		2482
B60G17/01908	10	{Acceleration or inclination sensors (characterised by the use of gyroscopes B60G21/08)}	B60G17/019	B60G17/019		805
B60G17/01916	11	{Mercury-switch type devices}	B60G17/019	B60G17/019		25
B60G17/01925	11	{Pendulum-type devices}	B60G17/019	B60G17/019		179
B60G17/01933	10	{Velocity, e.g. relative velocity-displacement sensors}	B60G17/019	B60G17/019		676
B60G17/01941	10	{characterised by the use of piezoelectric elements, e.g. sensors or actuators}	B60G17/019	B60G17/019		196
B60G17/0195	9	characterised by the regulation being combined with other vehicle control systems {(conjoint control of vehicle sub-units including control of suspension systems B60W10/22)}	B60G17/0195	B60G17/0195		1335
B60G17/02	8	Spring characteristics {, e.g. mechanical springs and mechanical adjusting means}(B60G17/005, B60G17/015 take precedence)	B60G17/02	B60G17/02		574
B60G17/021	9	{the mechanical spring being a coil spring (B60G17/0272 takes precedence)}	B60G17/02	B60G17/02		976
B60G17/023	9	{the mechanical spring being a leaf spring (B60G17/0275 takes precedence)}	B60G17/02	B60G17/02		336
B60G17/025	9	{the mechanical spring being a torsion spring (B60G17/0277, B60G21/0553 take precedence)}	B60G17/02	B60G17/02		359
B60G17/027	9	Mechanical springs regulated by fluid means (B60G17/033 takes precedence)	B60G17/027	B60G17/027		214
B60G17/0272	10	{the mechanical spring being a coil spring}	B60G17/027	B60G17/027		688
B60G17/0275	10	{the mechanical spring being a leaf spring}	B60G17/027	B60G17/027		182
B60G17/0277	10	{the mechanical spring being a torsion spring (B60G21/0553 takes precedence)}	B60G17/027	B60G17/027		173
B60G17/033	9	characterised by regulating means acting on more than one spring	B60G17/033	B60G17/033		917
B60G17/04	9	fluid spring characteristics	B60G17/04	B60G17/04		1284
B60G17/0408	10	{details, e.g. antifreeze for suspension fluid, pumps, retarding means  per se}	B60G17/04	B60G17/04		499
B60G17/0416	10	{regulated by varying the resiliency of hydropneumatic suspensions (B60G17/048 takes precedence)}	B60G17/04	B60G17/04		323
B60G17/0424	11	{by varying the air pressure of the accumulator}	B60G17/04	B60G17/04		172
B60G17/0432	11	{by varying the number of accumulators connected to the hydraulic cylinder (B60G17/0424 takes precedence)}	B60G17/04	B60G17/04		176
B60G17/044	10	Self-pumping fluid springs (pumps for liquids F04)	B60G17/044	B60G17/044		501
B60G17/048	10	with the regulating means inside the fluid springs (B60G17/044 takes precedence)	B60G17/048	B60G17/048		319
B60G17/0485	11	{the springs being pneumatic springs with a flexible wall, e.g. with levelling valves}	B60G17/048	B60G17/048		170
B60G17/052	10	Pneumatic spring characteristics (B60G17/048 takes precedence {; valves per seF16K})	B60G17/052	B60G17/052		1661
B60G17/0521	11	{the spring having a flexible wall}	B60G17/052	B60G17/052		311
B60G17/0523	11	{Regulating distributors or valves for pneumatic springs}	B60G17/052	B60G17/052		960
B60G17/0525	12	{Height adjusting or levelling valves}	B60G17/052	B60G17/052		1070
B60G17/0526	12	{Distributor units, e.g. for retractable wheels (vehicles with retractable wheels per seB62D61/12)}	B60G17/052	B60G17/052		149
B60G17/0528	12	{Pressure regulating or air filling valves}	B60G17/052	B60G17/052		381
B60G17/056	10	Regulating distributors or valves {for hydropneumatic systems}(B60G17/044&#160;-&#160;B60G17/048, {B60G17/0416} take precedence; {Fluid interconnection systems to control vehicle inclination B60G21/06, B60G21/10}; valves per seF16K)	B60G17/056	B60G17/056		875
B60G17/0565	11	{Height adjusting valves}	B60G17/056	B60G17/056		221
B60G17/06	8	Characteristics of dampers {, e.g. mechanical dampers}(B60G17/015 takes precedence)	B60G17/06	B60G17/06		1107
B60G17/08	9	Characteristics of fluid dampers (adjusting fluid dampers in general F16F9/44&#160;-&#160;F16F9/53)	B60G17/08	B60G17/08		2616
B60G21/00	7	Interconnection systems for two or more resiliently-suspended wheels, e.g. for stabilising a vehicle body with respect to acceleration, deceleration or centrifugal forces (B60G17/033 takes precedence {; levelling or stabilising systems for tippers B60P1/045}; steering deflectable wheels combined with means for inwardly inclining the vehicle body on bends B62D9/02)	B60G21/00	B60G21/00		263
B60G21/002	8	{longitudinally}	B60G21/00	B60G21/00		35
B60G21/005	8	{transversally}	B60G21/00	B60G21/00		197
B60G21/007	8	{means for adjusting the wheel inclination}	B60G21/00	B60G21/00		485
B60G21/02	8	permanently interconnected	B60G21/02	B60G21/02		88
B60G21/023	9	{longitudinally}	B60G21/02	B60G21/02		78
B60G21/026	9	{transversally}	B60G21/02	B60G21/02		212
B60G21/04	9	mechanically	B60G21/04	B60G21/04		578
B60G21/045	10	between wheels on different axles on the same side of the vehicle, i.e. the left or the right side	B60G21/045	B60G21/045		387
B60G21/05	10	between wheels on the same axle but on different sides of the vehicle, i.e. the left and right wheel suspensions being interconnected	B60G21/05	B60G21/05		1171
B60G21/051	11	{Trailing arm twist beam axles}	B60G21/05	B60G21/05		1595
B60G21/052	12	{Mounting means therefor}	B60G21/05	B60G21/05		369
B60G21/053	13	{adjustable}	B60G21/05	B60G21/05		86
B60G21/055	11	Stabiliser bars	B60G21/055	B60G21/055		2232
B60G21/0551	12	{Mounting means therefor}	B60G21/055	B60G21/055		2051
B60G21/0553	13	{adjustable}	B60G21/055	B60G21/055		526
B60G21/0555	14	{including an actuator inducing vehicle roll}	B60G21/055	B60G21/055		1104
B60G21/0556	14	{including a releasable coupling (B60G21/0555 takes precedence)}	B60G21/055	B60G21/055		362
B60G21/0558	14	{including means varying the stiffness of the stabiliser (B60G21/0556 takes precedence)}	B60G21/055	B60G21/055		333
B60G21/06	9	fluid	B60G21/06	B60G21/06		696
B60G21/067	10	between wheels on different axles on the same side of the vehicle, i.e. the left or the right side	B60G21/067	B60G21/067		321
B60G21/073	10	between wheels on the same axle but on different sides of the vehicle, i.e. the left and right wheel suspensions being interconnected	B60G21/073	B60G21/073		773
B60G21/08	8	characterised by use of gyroscopes (gyroscopes for stabilising vehicle bodies without controlling suspension arrangements B62D37/06)	B60G21/08	B60G21/08		106
B60G21/10	8	not permanently interconnected, e.g. operative only on acceleration, only on deceleration or only at off-straight position of steering	B60G21/10	B60G21/10		225
B60G21/103	9	{longitudinally}	B60G21/10	B60G21/10		47
B60G21/106	9	{transversally}	B60G21/10	B60G21/10		261
B60G99/00	7	Subject matter not provided for in other groups of this subclass	B60G99/00	B60G99/00		394
B60G99/002	8	{Suspension details of the suspension of the vehicle body on the vehicle chassis}	B60G99/00	B60G99/00		507
B60G99/004	8	{Other suspension arrangements with rubber springs}	B60G99/00	B60G99/00		276
B60G99/006	8	{Other suspension arrangements with metallic springs}	B60G99/00	B60G99/00		99
B60G99/008	8	{Other suspension arrangements with fluid springs}	B60G99/00	B60G99/00		104
B60G2200/00	7	Indexing codes relating to suspension types	CPCONLY	B60G2200/00		9
B60G2200/10	8	Independent suspensions	CPCONLY	B60G2200/10		767
B60G2200/13	9	with longitudinal arms only	CPCONLY	B60G2200/13		343
B60G2200/132	10	with a single trailing arm	CPCONLY	B60G2200/132		806
B60G2200/1322	11	with a wishbone or triangular arm	CPCONLY	B60G2200/1322		231
B60G2200/1324	11	with a resilient trailing arm	CPCONLY	B60G2200/1324		48
B60G2200/14	9	with lateral arms	CPCONLY	B60G2200/14		316
B60G2200/141	10	with one trailing arm and one lateral arm only	CPCONLY	B60G2200/141		157
B60G2200/142	10	with a single lateral arm, e.g. MacPherson type	CPCONLY	B60G2200/142		939
B60G2200/1422	11	the lateral arm being resilient	CPCONLY	B60G2200/1422		62
B60G2200/1424	11	the lateral arm having an L-shape	CPCONLY	B60G2200/1424		86
B60G2200/143	10	with lateral arms crossing each other, i.e. X formation as seen along the longitudinal axis	CPCONLY	B60G2200/143		100
B60G2200/144	10	with two lateral arms forming a parallelogram	CPCONLY	B60G2200/144		2007
B60G2200/1442	11	including longitudinal rods	CPCONLY	B60G2200/1442		230
B60G2200/154	10	the lateral arm having an L-shape	CPCONLY	B60G2200/154		104
B60G2200/156	10	wishbone-type arm formed by two links defining a virtual apex	CPCONLY	B60G2200/156		219
B60G2200/17	9	with a strut contributing to the suspension geometry by being articulated onto the wheel support	CPCONLY	B60G2200/17		207
B60G2200/18	9	Multilink suspensions, e.g. elastokinematic arrangements	CPCONLY	B60G2200/18		588
B60G2200/182	10	with one longitudinal arm or rod and lateral rods	CPCONLY	B60G2200/182		364
B60G2200/184	10	Assymetric arrangements	CPCONLY	B60G2200/184		201
B60G2200/20	8	Semi-rigid axle suspensions	CPCONLY	B60G2200/20		190
B60G2200/21	9	Trailing arms connected by a torsional beam, i.e. twist-beam axles	CPCONLY	B60G2200/21		733
B60G2200/22	9	Trailing arms connected by a straight torsion bar	CPCONLY	B60G2200/22		110
B60G2200/23	9	Trailing arms connected by a U-shaped torsion bar	CPCONLY	B60G2200/23		128
B60G2200/24	9	Interconnected split axles	CPCONLY	B60G2200/24		37
B60G2200/30	8	Rigid axle suspensions	CPCONLY	B60G2200/30		514
B60G2200/31	9	with two trailing arms rigidly connected to the axle	CPCONLY	B60G2200/31		1112
B60G2200/312	9	with one of the two trailing arms being rigidly connected to the axle	CPCONLY	B60G2200/312		24
B60G2200/314	9	with longitudinally arranged arms articulated on the axle	CPCONLY	B60G2200/314		590
B60G2200/315	10	at least one of the arms having an A or V shape	CPCONLY	B60G2200/315		254
B60G2200/318	9	two or more axles being mounted on a longitudinal rocking or walking beam	CPCONLY	B60G2200/318		257
B60G2200/32	9	pivoted	CPCONLY	B60G2200/32		328
B60G2200/322	10	with a single pivot point and a straight axle	CPCONLY	B60G2200/322		507
B60G2200/324	10	with a single pivot point and a triangular "T" or "U"-shaped axle, e.g. DeDion arrangement	CPCONLY	B60G2200/324		167
B60G2200/326	10	with two laterally spaced pivots, e.g. trailing frame	CPCONLY	B60G2200/326		42
B60G2200/34	9	Stabilising mechanisms, e.g. for lateral stability	CPCONLY	B60G2200/34		360
B60G2200/341	10	Panhard rod	CPCONLY	B60G2200/341		363
B60G2200/3415	11	Scott-Russel linkage	CPCONLY	B60G2200/3415		47
B60G2200/342	10	Watt linkage	CPCONLY	B60G2200/342		140
B60G2200/343	10	with an axle suspended by two pivoted rods in "V"-arrangement, the rods being coupled at its apex	CPCONLY	B60G2200/343		39
B60G2200/344	10	with an axle suspended by two pivoted rods in an inverted "V"-arrangement, the rods being coupled at its apex	CPCONLY	B60G2200/344		15
B60G2200/345	10	with an axle suspended by two pivoted rods in "X"-arrangement	CPCONLY	B60G2200/345		129
B60G2200/346	10	with an axle suspended by two laterally displaced rods having an imaginary point of intersection above the wheel axis	CPCONLY	B60G2200/346		31
B60G2200/347	10	with an axle suspended by two laterally displaced rods having an imaginary point of intersection below the wheel axis	CPCONLY	B60G2200/347		34
B60G2200/40	8	Indexing codes relating to the wheels in the suspensions	CPCONLY	B60G2200/40		32
B60G2200/42	9	Driven wheels or dead axles	CPCONLY	B60G2200/42		106
B60G2200/422	9	Driving wheels or live axles	CPCONLY	B60G2200/422		960
B60G2200/44	9	steerable	CPCONLY	B60G2200/44		1757
B60G2200/445	9	Self-steered wheels	CPCONLY	B60G2200/445		333
B60G2200/446	9	Non-steerable wheels	CPCONLY	B60G2200/446		61
B60G2200/46	9	camber angle	CPCONLY	B60G2200/46		1610
B60G2200/462	9	Toe-in/out	CPCONLY	B60G2200/462		1485
B60G2200/4622	10	Alignment adjustment	CPCONLY	B60G2200/4622		458
B60G2200/464	9	Caster angle	CPCONLY	B60G2200/464		524
B60G2200/466	9	Damping acceleration or deceleration torque on wheel axle	CPCONLY	B60G2200/466		131
B60G2202/00	7	Indexing codes relating to the type of spring, damper or actuator	CPCONLY	B60G2202/00		6
B60G2202/10	8	Type of spring	CPCONLY	B60G2202/10		76
B60G2202/11	9	Leaf spring	CPCONLY	B60G2202/11		592
B60G2202/112	10	longitudinally arranged	CPCONLY	B60G2202/112		1269
B60G2202/114	10	transversally arranged	CPCONLY	B60G2202/114		535
B60G2202/116	10	having a "C" form loaded only at its ends transversally to its central axis	CPCONLY	B60G2202/116		112
B60G2202/117	10	having a "C" form loaded parallel to its central axis	CPCONLY	B60G2202/117		22
B60G2202/12	9	Wound spring	CPCONLY	B60G2202/12		1618
B60G2202/122	10	subjected to tension	CPCONLY	B60G2202/122		49
B60G2202/13	9	Torsion spring	CPCONLY	B60G2202/13		221
B60G2202/132	10	comprising a longitudinal torsion bar and/or tube	CPCONLY	B60G2202/132		216
B60G2202/134	10	comprising a transversal torsion bar and/or tube	CPCONLY	B60G2202/134		219
B60G2202/135	10	Stabiliser bar and/or tube	CPCONLY	B60G2202/135		1336
B60G2202/1351	11	comprising at least two stabiliser bars parallel to each other	CPCONLY	B60G2202/1351		142
B60G2202/136	10	Twist-beam type arrangement	CPCONLY	B60G2202/136		281
B60G2202/1362	11	including a second torsional element, e.g. second beam, stabiliser bar or tube	CPCONLY	B60G2202/1362		211
B60G2202/14	9	Plastic spring, e.g. rubber	CPCONLY	B60G2202/14		178
B60G2202/141	10	subjected to tension	CPCONLY	B60G2202/141		14
B60G2202/142	10	subjected to shear, e.g. Neidhart type	CPCONLY	B60G2202/142		130
B60G2202/1422	11	Axial	CPCONLY	B60G2202/1422		84
B60G2202/1424	11	Torsional	CPCONLY	B60G2202/1424		272
B60G2202/143	10	subjected to compression	CPCONLY	B60G2202/143		540
B60G2202/144	10	of rotary type	CPCONLY	B60G2202/144		45
B60G2202/15	9	Fluid spring	CPCONLY	B60G2202/15		255
B60G2202/152	10	Pneumatic spring	CPCONLY	B60G2202/152		3613
B60G2202/1522	11	of rotary type	CPCONLY	B60G2202/1522		20
B60G2202/1524	11	with two air springs per wheel, arranged before and after the wheel axis	CPCONLY	B60G2202/1524		344
B60G2202/154	10	with an accumulator	CPCONLY	B60G2202/154		1008
B60G2202/16	9	Magnetic spring	CPCONLY	B60G2202/16		71
B60G2202/20	8	Type of damper	CPCONLY	B60G2202/20		211
B60G2202/21	9	with two dampers per wheel, arranged before and after the wheel axis	CPCONLY	B60G2202/21		108
B60G2202/22	9	Rotary Damper	CPCONLY	B60G2202/22		321
B60G2202/23	9	Friction Damper	CPCONLY	B60G2202/23		112
B60G2202/24	9	Fluid damper	CPCONLY	B60G2202/24		1729
B60G2202/242	10	Pneumatic damper	CPCONLY	B60G2202/242		240
B60G2202/25	9	Dynamic damper	CPCONLY	B60G2202/25		463
B60G2202/30	8	Spring/Damper and/or actuator Units	CPCONLY	B60G2202/30		167
B60G2202/31	9	with the spring arranged around the damper, e.g. MacPherson strut	CPCONLY	B60G2202/31		332
B60G2202/312	10	The spring being a wound spring	CPCONLY	B60G2202/312		1804
B60G2202/314	10	The spring being a pneumatic spring	CPCONLY	B60G2202/314		464
B60G2202/32	9	The spring being in series with the damper and/or actuator	CPCONLY	B60G2202/32		327
B60G2202/322	10	the damper being controllable	CPCONLY	B60G2202/322		79
B60G2202/40	8	Type of actuator	CPCONLY	B60G2202/40		326
B60G2202/41	9	Fluid actuator	CPCONLY	B60G2202/41		146
B60G2202/412	10	Pneumatic actuator	CPCONLY	B60G2202/412		493
B60G2202/413	10	Hydraulic actuator	CPCONLY	B60G2202/413		1643
B60G2202/414	10	using electrohydraulic valves	CPCONLY	B60G2202/414		301
B60G2202/415	10	using other types of valves, e.g. mechanically operated valves	CPCONLY	B60G2202/415		66
B60G2202/416	10	using a pump, e.g. in the line connecting the lower chamber to the upper chamber of the actuator	CPCONLY	B60G2202/416		562
B60G2202/42	9	Electric actuator	CPCONLY	B60G2202/42		1640
B60G2202/422	10	Linear motor	CPCONLY	B60G2202/422		213
B60G2202/424	10	electrostrictive materials, e.g. piezoelectric actuator	CPCONLY	B60G2202/424		76
B60G2202/43	9	Mechanical actuator	CPCONLY	B60G2202/43		115
B60G2202/432	10	Spring motor	CPCONLY	B60G2202/432		13
B60G2202/44	9	Axial actuator, e.g. telescopic	CPCONLY	B60G2202/44		191
B60G2202/441	10	where axial movement is translated to rotation of the connected end part	CPCONLY	B60G2202/441		56
B60G2202/442	9	Rotary actuator	CPCONLY	B60G2202/442		377
B60G2202/45	9	Other types, e.g. external jets for stability with particular characteristics	CPCONLY	B60G2202/45		32
B60G2202/49	9	Other type, e.g. external jets for stability	CPCONLY	B60G2202/49		3
B60G2204/00	7	Indexing codes related to suspensions per se or to auxiliary parts	CPCONLY	B60G2204/00		4
B60G2204/10	8	Mounting of suspension elements	CPCONLY	B60G2204/10		220
B60G2204/11	9	Mounting of sensors thereon	CPCONLY	B60G2204/11		531
B60G2204/111	10	on pneumatic springs	CPCONLY	B60G2204/111		209
B60G2204/112	10	on dampers, e.g. fluid dampers	CPCONLY	B60G2204/112		262
B60G2204/113	10	Tyre related sensors	CPCONLY	B60G2204/113		91
B60G2204/114	10	Steering column mounted sensors	CPCONLY	B60G2204/114		13
B60G2204/115	10	Wheel hub bearing sensors	CPCONLY	B60G2204/115		166
B60G2204/116	10	Sensors coupled to the suspension arm	CPCONLY	B60G2204/116		131
B60G2204/1162	11	directly mounted on the suspension arm	CPCONLY	B60G2204/1162		92
B60G2204/12	9	Mounting of springs or dampers	CPCONLY	B60G2204/12		255
B60G2204/121	10	Mounting of leaf springs	CPCONLY	B60G2204/121		1363
B60G2204/122	10	Mounting of torsion springs	CPCONLY	B60G2204/122		413
B60G2204/1222	11	Middle mounts of stabiliser on vehicle body or chassis	CPCONLY	B60G2204/1222		922
B60G2204/1224	11	End mounts of stabiliser on wheel suspension	CPCONLY	B60G2204/1224		853
B60G2204/1226	11	on the trailing arms of a twist beam type arrangement	CPCONLY	B60G2204/1226		209
B60G2204/124	10	Mounting of coil springs	CPCONLY	B60G2204/124		1386
B60G2204/1242	11	on a damper, e.g. MacPerson strut	CPCONLY	B60G2204/1242		969
B60G2204/12422	12	anchoring the end coils on the spring support plate	CPCONLY	B60G2204/12422		199
B60G2204/1244	11	on a suspension arm	CPCONLY	B60G2204/1244		486
B60G2204/1246	11	on twist beam axles	CPCONLY	B60G2204/1246		113
B60G2204/125	10	Mounting of rubber type springs	CPCONLY	B60G2204/125		351
B60G2204/126	10	Mounting of pneumatic springs	CPCONLY	B60G2204/126		751
B60G2204/1262	11	on a damper	CPCONLY	B60G2204/1262		164
B60G2204/127	10	with the mounting of springs or dampers moving so that the direction of the related force vector can be changed, thus contributing to a variation of the loading of the wheel	CPCONLY	B60G2204/127		171
B60G2204/128	10	Damper mount on vehicle body or chassis	CPCONLY	B60G2204/128		2253
B60G2204/129	10	Damper mount on wheel suspension or knuckle	CPCONLY	B60G2204/129		1614
B60G2204/13	10	with the spring, i.e. coil spring, or damper horizontally mounted	CPCONLY	B60G2204/13		250
B60G2204/1302	11	inside the vehicle frame	CPCONLY	B60G2204/1302		58
B60G2204/14	9	Mounting of suspension arms	CPCONLY	B60G2204/14		464
B60G2204/143	10	on the vehicle body or chassis	CPCONLY	B60G2204/143		2483
B60G2204/1431	11	of an L-shaped arm	CPCONLY	B60G2204/1431		210
B60G2204/1432	11	by vertical bolts or studs	CPCONLY	B60G2204/1432		223
B60G2204/1434	11	in twist-beam axles arrangement	CPCONLY	B60G2204/1434		311
B60G2204/147	10	on the vehicle engine body	CPCONLY	B60G2204/147		48
B60G2204/148	10	on the unsprung part of the vehicle, e.g. wheel knuckle or rigid axle	CPCONLY	B60G2204/148		1948
B60G2204/1482	11	on rigid axle by elastic mount	CPCONLY	B60G2204/1482		189
B60G2204/1484	11	on an intermediate upright strut upon which the stub axle is pivoted	CPCONLY	B60G2204/1484		98
B60G2204/149	10	Mounting of rigid axle on wheel knuckle	CPCONLY	B60G2204/149		101
B60G2204/15	9	Mounting of subframes	CPCONLY	B60G2204/15		1093
B60G2204/16	9	Mounting of vehicle body on chassis	CPCONLY	B60G2204/16		135
B60G2204/162	10	Cabins, e.g. for trucks, tractors	CPCONLY	B60G2204/162		124
B60G2204/17	9	Mounting of bogies, e.g. for trailers	CPCONLY	B60G2204/17		35
B60G2204/18	9	Mounting of vehicle engines	CPCONLY	B60G2204/18		140
B60G2204/182	10	Electric motor on wheel support	CPCONLY	B60G2204/182		157
B60G2204/19	9	Mounting of transmission differential	CPCONLY	B60G2204/19		176
B60G2204/20	9	Mounting of accessories, e.g. pump, compressor	CPCONLY	B60G2204/20		241
B60G2204/201	10	of fluid lines	CPCONLY	B60G2204/201		126
B60G2204/202	10	of cables	CPCONLY	B60G2204/202		185
B60G2204/2022	11	using a suspension element (e.g. link, damper or spring) as part of the electrical circuitry	CPCONLY	B60G2204/2022		20
B60G2204/22	9	Linking of trailers to trucks, e.g. truck-trailer connections	CPCONLY	B60G2204/22		13
B60G2204/30	9	In-wheel mountings	CPCONLY	B60G2204/30		485
B60G2204/40	8	Auxiliary suspension parts; Adjustment of suspensions	CPCONLY	B60G2204/40		122
B60G2204/41	9	Elastic mounts, e.g. bushings	CPCONLY	B60G2204/41		3762
B60G2204/4102	10	having a pin or stud extending perpendicularly to the axis of the elastic mount	CPCONLY	B60G2204/4102		97
B60G2204/4103	10	having an eccentrically located inner sleeve	CPCONLY	B60G2204/4103		45
B60G2204/4104	10	Bushings having modified rigidity in particular directions	CPCONLY	B60G2204/4104		498
B60G2204/41042	11	by using internal cam surfaces	CPCONLY	B60G2204/41042		229
B60G2204/41043	11	formed by a U-shaped external bracket	CPCONLY	B60G2204/41043		114
B60G2204/41044	11	in a shell for being loaded mainly in axial direction, e.g. piston rod mounts, longitudinal push-pull rod mounts	CPCONLY	B60G2204/41044		83
B60G2204/41046	11	having the axis of an inner sleeve or pin inclined to the axis of the bush	CPCONLY	B60G2204/41046		12
B60G2204/4106	10	Elastokinematic mounts	CPCONLY	B60G2204/4106		149
B60G2204/41062	11	hydromounts; interconnected mounts	CPCONLY	B60G2204/41062		134
B60G2204/4108	10	Resilient element being enclosed and or pres-tressed in a solid container	CPCONLY	B60G2204/4108		136
B60G2204/414	9	Cardan joints	CPCONLY	B60G2204/414		141
B60G2204/416	9	Ball or spherical joints	CPCONLY	B60G2204/416		2167
B60G2204/418	9	Bearings, e.g. ball or roller bearings	CPCONLY	B60G2204/418		1854
B60G2204/419	9	Gears	CPCONLY	B60G2204/419		598
B60G2204/4191	10	Planetary or epicyclic gears	CPCONLY	B60G2204/4191		343
B60G2204/4192	10	rack and pinion	CPCONLY	B60G2204/4192		215
B60G2204/4193	10	worm gears	CPCONLY	B60G2204/4193		172
B60G2204/42	9	Joints with cam surfaces	CPCONLY	B60G2204/42		466
B60G2204/421	9	Pivoted lever mechanisms for mounting suspension elements, e.g. Watt linkage	CPCONLY	B60G2204/421		996
B60G2204/422	9	Links for mounting suspension elements	CPCONLY	B60G2204/422		1761
B60G2204/4222	10	for movement on predefined locus of, e.g. the wheel center	CPCONLY	B60G2204/4222		116
B60G2204/423	9	Rails, tubes, or the like, for guiding the movement of suspension elements	CPCONLY	B60G2204/423		216
B60G2204/4232	10	Sliding mounts	CPCONLY	B60G2204/4232		772
B60G2204/424	9	Mechanisms for force adjustment, e.g. constant force mechanisms	CPCONLY	B60G2204/424		97
B60G2204/43	9	Fittings, brackets or knuckles	CPCONLY	B60G2204/43		2285
B60G2204/4302	10	for fixing suspension arm on the vehicle body or chassis	CPCONLY	B60G2204/4302		812
B60G2204/4304	10	Bracket for lower cylinder mount of McPherson strut	CPCONLY	B60G2204/4304		340
B60G2204/4305	10	Bracket for mounting of hydraulic lines on a damper cylinder	CPCONLY	B60G2204/4305		108
B60G2204/4306	10	Bracket or knuckle for rigid axles, e.g. for clamping	CPCONLY	B60G2204/4306		684
B60G2204/43065	11	U-shaped bolts crossing each other	CPCONLY	B60G2204/43065		91
B60G2204/4307	10	Bracket or knuckle for torsional springs	CPCONLY	B60G2204/4307		239
B60G2204/4308	10	Protecting guards, e.g. for rigid axle damage protection	CPCONLY	B60G2204/4308		219
B60G2204/44	9	Centering or positioning means	CPCONLY	B60G2204/44		925
B60G2204/4402	10	Spacers or shims	CPCONLY	B60G2204/4402		510
B60G2204/4404	10	Retainers for holding a fixing element, e.g. bushing, nut, bolt etc., until it is tightly fixed in position	CPCONLY	B60G2204/4404		282
B60G2204/45	9	Stops limiting travel	CPCONLY	B60G2204/45		908
B60G2204/4502	10	using resilient buffer	CPCONLY	B60G2204/4502		938
B60G2204/45021	11	for limiting upper mount movement of a McPherson strut	CPCONLY	B60G2204/45021		290
B60G2204/4504	10	using cable or band to prevent extension	CPCONLY	B60G2204/4504		244
B60G2204/46	9	Means for locking the suspension	CPCONLY	B60G2204/46		478
B60G2204/4602	10	Locking of a McPerson type strut upper mount on the vehicle body	CPCONLY	B60G2204/4602		50
B60G2204/4604	10	mechanically, e.g. using a hook as anticreep mechanism	CPCONLY	B60G2204/4604		207
B60G2204/4605	10	hydraulically, e.g. interrupting communication between the chambers of a hydraulic cylinder	CPCONLY	B60G2204/4605		147
B60G2204/47	9	Means for retracting the suspension	CPCONLY	B60G2204/47		320
B60G2204/4702	10	pneumatically	CPCONLY	B60G2204/4702		228
B60G2204/61	8	Adjustable during maintenance	CPCONLY	B60G2204/61		797
B60G2204/62	8	Adjustable continuously, e.g. during driving	CPCONLY	B60G2204/62		846
B60G2204/80	8	Interactive suspensions; arrangement affecting more than one suspension unit	CPCONLY	B60G2204/80		440
B60G2204/81	9	front and rear unit	CPCONLY	B60G2204/81		249
B60G2204/8102	10	diagonally arranged	CPCONLY	B60G2204/8102		89
B60G2204/82	9	left and right unit on same axle	CPCONLY	B60G2204/82		881
B60G2204/83	9	Type of interconnection	CPCONLY	B60G2204/83		28
B60G2204/8302	10	Mechanical	CPCONLY	B60G2204/8302		620
B60G2204/83022	11	using cables, wires, belts or chains	CPCONLY	B60G2204/83022		152
B60G2204/8304	10	using a fluid	CPCONLY	B60G2204/8304		550
B60G2204/8306	10	Permanent; Continuous	CPCONLY	B60G2204/8306		150
B60G2206/00	7	Indexing codes related to the manufacturing of suspensions: constructional features, the materials used, procedures or tools	CPCONLY	B60G2206/00		10
B60G2206/01	8	Constructional features of suspension elements, e.g. arms, dampers, springs	CPCONLY	B60G2206/01		66
B60G2206/011	9	Modular constructions	CPCONLY	B60G2206/011		414
B60G2206/0112	10	Bogies for heavy vehicles	CPCONLY	B60G2206/0112		88
B60G2206/0114	10	Independent suspensions on subframes	CPCONLY	B60G2206/0114		292
B60G2206/0116	10	Integrated distribution control units with valves, accumulators, PCB&apos;s or the like	CPCONLY	B60G2206/0116		128
B60G2206/012	9	Hollow or tubular elements	CPCONLY	B60G2206/012		1368
B60G2206/0122	10	having a U profile with plate closing the profile in the total or partial length of the element	CPCONLY	B60G2206/0122		45
B60G2206/013	9	with embedded inserts for material reinforcement	CPCONLY	B60G2206/013		239
B60G2206/014	9	with reinforcing nerves or branches	CPCONLY	B60G2206/014		457
B60G2206/016	9	allowing controlled deformation during collision	CPCONLY	B60G2206/016		372
B60G2206/017	9	forming an eye for the bushing	CPCONLY	B60G2206/017		189
B60G2206/10	9	Constructional features of arms	CPCONLY	B60G2206/10		769
B60G2206/11	10	the arm being a radius or track or torque or steering rod or stabiliser end link	CPCONLY	B60G2206/11		1317
B60G2206/111	11	of adjustable length	CPCONLY	B60G2206/111		157
B60G2206/1112	12	Manually, for alignment purposes	CPCONLY	B60G2206/1112		139
B60G2206/1114	12	Self-adjustable during driving	CPCONLY	B60G2206/1114		78
B60G2206/1116	12	Actively adjustable during driving	CPCONLY	B60G2206/1116		120
B60G2206/12	10	with two attachment points on the sprung part of the vehicle	CPCONLY	B60G2206/12		159
B60G2206/121	10	the arm having an H or X-shape	CPCONLY	B60G2206/121		365
B60G2206/122	10	the arm having L-shape	CPCONLY	B60G2206/122		458
B60G2206/123	10	the arm having T-shape	CPCONLY	B60G2206/123		31
B60G2206/124	10	the arm having triangular or Y-shape, e.g. wishbone	CPCONLY	B60G2206/124		672
B60G2206/13	10	with more than two attachment points on the sprung part of the vehicle	CPCONLY	B60G2206/13		21
B60G2206/14	10	the arm forming a U-shaped recess for fitting a bush	CPCONLY	B60G2206/14		52
B60G2206/141	11	The recess being integrally or seamlessly formed	CPCONLY	B60G2206/141		15
B60G2206/15	10	the arm being resilient	CPCONLY	B60G2206/15		144
B60G2206/16	10	the arm having a U profile and/or made of a plate	CPCONLY	B60G2206/16		376
B60G2206/161	11	with middle section narrower than end section	CPCONLY	B60G2206/161		4
B60G2206/162	11	with a plate closing the profile in the total or partial length of the arm	CPCONLY	B60G2206/162		224
B60G2206/20	9	Constructional features of semi-rigid axles, e.g. twist beam type axles	CPCONLY	B60G2206/20		857
B60G2206/201	10	with detachable cross beam and/or torsion stabiliser bar/tube	CPCONLY	B60G2206/201		139
B60G2206/202	10	with a radially deformed tube as a cross member	CPCONLY	B60G2206/202		113
B60G2206/203	10	with outwardly bent trailing arms to increase the width of the support or wheelbase	CPCONLY	B60G2206/203		64
B60G2206/30	9	Constructional features of rigid axles	CPCONLY	B60G2206/30		249
B60G2206/31	10	Straight axle	CPCONLY	B60G2206/31		144
B60G2206/312	10	Cranked axle	CPCONLY	B60G2206/312		50
B60G2206/32	10	Hollow cross section	CPCONLY	B60G2206/32		120
B60G2206/40	9	Constructional features of dampers and/or springs	CPCONLY	B60G2206/40		158
B60G2206/41	10	Dampers	CPCONLY	B60G2206/41		693
B60G2206/42	10	Springs	CPCONLY	B60G2206/42		494
B60G2206/422	11	Accumulators for hydropneumatic springs	CPCONLY	B60G2206/422		94
B60G2206/4222	12	with a flexible separating wall; Membrane construction	CPCONLY	B60G2206/4222		84
B60G2206/424	11	Plunger or top retainer construction for bellows or rolling lobe type air springs	CPCONLY	B60G2206/424		459
B60G2206/426	11	Coil springs having a particular shape, e.g. curved axis, pig-tail end coils	CPCONLY	B60G2206/426		125
B60G2206/427	11	Stabiliser bars or tubes	CPCONLY	B60G2206/427		1639
B60G2206/428	11	Leaf springs	CPCONLY	B60G2206/428		331
B60G2206/50	9	Constructional features of wheel supports or knuckles, e.g. steering knuckles, spindle attachments	CPCONLY	B60G2206/50		1557
B60G2206/60	9	Subframe construction	CPCONLY	B60G2206/60		887
B60G2206/601	10	Hanger bracket	CPCONLY	B60G2206/601		435
B60G2206/602	10	Single transverse beam	CPCONLY	B60G2206/602		167
B60G2206/604	10	with two parallel beams connected by cross members	CPCONLY	B60G2206/604		173
B60G2206/605	10	Flexible constructions	CPCONLY	B60G2206/605		120
B60G2206/606	10	Complex constructions	CPCONLY	B60G2206/606		42
B60G2206/70	9	Materials used in suspensions	CPCONLY	B60G2206/70		116
B60G2206/71	10	Light weight materials	CPCONLY	B60G2206/71		211
B60G2206/7101	11	Fiber-reinforced plastics [FRP]	CPCONLY	B60G2206/7101		932
B60G2206/7102	11	Aluminium alloys	CPCONLY	B60G2206/7102		410
B60G2206/7103	11	Magnesium alloys	CPCONLY	B60G2206/7103		37
B60G2206/7104	11	Thermoplastics	CPCONLY	B60G2206/7104		299
B60G2206/71042	12	Polyester elastomer	CPCONLY	B60G2206/71042		13
B60G2206/71043	12	Polyamid elastomer	CPCONLY	B60G2206/71043		31
B60G2206/71044	12	Soft nylon	CPCONLY	B60G2206/71044		7
B60G2206/7105	11	Porous materials, ceramics, e.g. as filling material	CPCONLY	B60G2206/7105		32
B60G2206/72	10	Steel	CPCONLY	B60G2206/72		375
B60G2206/722	11	Plates	CPCONLY	B60G2206/722		539
B60G2206/724	11	Wires, bars or the like	CPCONLY	B60G2206/724		81
B60G2206/73	10	Rubber; Elastomers	CPCONLY	B60G2206/73		889
B60G2206/80	9	Manufacturing procedures	CPCONLY	B60G2206/80		244
B60G2206/81	10	Shaping	CPCONLY	B60G2206/81		314
B60G2206/8101	11	by casting	CPCONLY	B60G2206/8101		321
B60G2206/81012	12	by injection moulding	CPCONLY	B60G2206/81012		309
B60G2206/8102	11	by stamping	CPCONLY	B60G2206/8102		318
B60G2206/81022	12	by forging	CPCONLY	B60G2206/81022		120
B60G2206/8103	11	by folding or bending	CPCONLY	B60G2206/8103		468
B60G2206/81035	12	involving heating to relieve internal stresses	CPCONLY	B60G2206/81035		27
B60G2206/8104	11	by drawing	CPCONLY	B60G2206/8104		46
B60G2206/8105	11	by extrusion	CPCONLY	B60G2206/8105		166
B60G2206/8106	11	by thermal treatment, e.g. curing hardening, vulcanisation	CPCONLY	B60G2206/8106		110
B60G2206/81062	12	to relieve internal stresses, e.g. during folding or bending	CPCONLY	B60G2206/81062		13
B60G2206/8107	11	by hydroforming	CPCONLY	B60G2206/8107		86
B60G2206/8108	11	by twisting	CPCONLY	B60G2206/8108		7
B60G2206/8109	11	by rolling	CPCONLY	B60G2206/8109		72
B60G2206/811	11	by cutting	CPCONLY	B60G2206/811		108
B60G2206/8111	11	by machining	CPCONLY	B60G2206/8111		38
B60G2206/8112	11	by thermal spraying of molten material	CPCONLY	B60G2206/8112		13
B60G2206/82	10	Joining	CPCONLY	B60G2206/82		301
B60G2206/8201	11	by welding	CPCONLY	B60G2206/8201		1196
B60G2206/82012	12	Pressure welding	CPCONLY	B60G2206/82012		8
B60G2206/82013	12	Friction or heat welding	CPCONLY	B60G2206/82013		71
B60G2206/82014	12	Magnetic pulse welding	CPCONLY	B60G2206/82014		12
B60G2206/8205	11	by conical or compressed rubber clamping inserts as joining means	CPCONLY	B60G2206/8205		30
B60G2206/8206	11	by riveting	CPCONLY	B60G2206/8206		71
B60G2206/8207	11	by screwing	CPCONLY	B60G2206/8207		1357
B60G2206/8208	11	by hemming or seaming, e.g. by folding of the rim	CPCONLY	B60G2206/8208		43
B60G2206/8209	11	by deformation	CPCONLY	B60G2206/8209		113
B60G2206/82092	12	by press-fitting	CPCONLY	B60G2206/82092		265
B60G2206/821	11	by gluing	CPCONLY	B60G2206/821		277
B60G2206/83	10	Punching	CPCONLY	B60G2206/83		67
B60G2206/84	10	Hardening	CPCONLY	B60G2206/84		29
B60G2206/8401	11	Annealing	CPCONLY	B60G2206/8401		11
B60G2206/8402	11	Quenching	CPCONLY	B60G2206/8402		38
B60G2206/8403	11	Shot-peening	CPCONLY	B60G2206/8403		40
B60G2206/85	10	Filament winding	CPCONLY	B60G2206/85		55
B60G2206/90	9	Maintenance	CPCONLY	B60G2206/90		60
B60G2206/91	10	Assembly procedures	CPCONLY	B60G2206/91		674
B60G2206/911	11	using a modification kit	CPCONLY	B60G2206/911		183
B60G2206/92	10	Tools or equipment used for assembling	CPCONLY	B60G2206/92		165
B60G2206/921	11	Coil spring compressor	CPCONLY	B60G2206/921		191
B60G2206/93	10	Tools used for adjustments	CPCONLY	B60G2206/93		122
B60G2206/931	11	McPherson strut positioning tool	CPCONLY	B60G2206/931		59
B60G2206/94	10	Tools used for supporting parts	CPCONLY	B60G2206/94		28
B60G2206/99	10	Suspension element selection procedure depending on loading or performance requirements, e.g. selection of damper, spring or bush	CPCONLY	B60G2206/99		126
B60G2300/00	7	Indexing codes relating to the type of vehicle	CPCONLY	B60G2300/00		65
B60G2300/02	8	Trucks; Load vehicles	CPCONLY	B60G2300/02		680
B60G2300/022	9	Fork lift trucks, Clark	CPCONLY	B60G2300/022		310
B60G2300/024	9	Light trucks	CPCONLY	B60G2300/024		110
B60G2300/026	9	Heavy duty trucks	CPCONLY	B60G2300/026		647
B60G2300/0262	10	Multi-axle trucks	CPCONLY	B60G2300/0262		315
B60G2300/03	8	Silo or fluid transporting vehicles	CPCONLY	B60G2300/03		102
B60G2300/04	8	Trailers	CPCONLY	B60G2300/04		822
B60G2300/042	9	Semi-trailers	CPCONLY	B60G2300/042		376
B60G2300/044	9	Truck-trailer connections	CPCONLY	B60G2300/044		53
B60G2300/06	8	Cranes	CPCONLY	B60G2300/06		131
B60G2300/07	8	Off-road vehicles	CPCONLY	B60G2300/07		664
B60G2300/08	8	Agricultural vehicles	CPCONLY	B60G2300/08		458
B60G2300/082	9	Tractors	CPCONLY	B60G2300/082		415
B60G2300/083	9	Boom carrying vehicles, e.g. for crop spraying	CPCONLY	B60G2300/083		124
B60G2300/084	9	Ridable lawn mowers	CPCONLY	B60G2300/084		56
B60G2300/09	8	Construction vehicles, e.g. graders, excavators	CPCONLY	B60G2300/09		375
B60G2300/10	8	Railway vehicles	CPCONLY	B60G2300/10		183
B60G2300/102	9	having track following mechanismn for lateral stability	CPCONLY	B60G2300/102		15
B60G2300/12	8	Cycles; Motorcycles	CPCONLY	B60G2300/12		593
B60G2300/122	9	Trikes	CPCONLY	B60G2300/122		422
B60G2300/124	9	Quads	CPCONLY	B60G2300/124		162
B60G2300/13	8	Small sized city motor vehicles	CPCONLY	B60G2300/13		268
B60G2300/14	8	Buses	CPCONLY	B60G2300/14		492
B60G2300/16	8	Aeroplanes	CPCONLY	B60G2300/16		20
B60G2300/18	8	Helicopters	CPCONLY	B60G2300/18		3
B60G2300/20	8	Toys	CPCONLY	B60G2300/20		82
B60G2300/22	8	Perambulators	CPCONLY	B60G2300/22		25
B60G2300/24	8	Wheelchairs	CPCONLY	B60G2300/24		148
B60G2300/26	8	Carts	CPCONLY	B60G2300/26		87
B60G2300/27	8	Racing vehicles, e.g. F1	CPCONLY	B60G2300/27		162
B60G2300/28	8	Amphibious vehicles	CPCONLY	B60G2300/28		78
B60G2300/30	8	Load ramps	CPCONLY	B60G2300/30		18
B60G2300/32	8	Track vehicles	CPCONLY	B60G2300/32		211
B60G2300/322	9	Snowmobiles	CPCONLY	B60G2300/322		67
B60G2300/34	8	Ambulances	CPCONLY	B60G2300/34		43
B60G2300/36	8	Independent Multi-axle long vehicles	CPCONLY	B60G2300/36		175
B60G2300/37	8	Vehicles having steerable wheels mounted on a vertically moving column	CPCONLY	B60G2300/37		223
B60G2300/38	8	Low or lowerable bed vehicles	CPCONLY	B60G2300/38		488
B60G2300/40	8	Variable track or wheelbase vehicles	CPCONLY	B60G2300/40		540
B60G2300/402	9	Extra load carrying wheels, e.g. tag axles	CPCONLY	B60G2300/402		195
B60G2300/45	8	Rolling frame vehicles	CPCONLY	B60G2300/45		480
B60G2300/50	8	Electric vehicles; Hybrid vehicles	CPCONLY	B60G2300/50		904
B60G2300/60	8	Vehicles using regenerative power	CPCONLY	B60G2300/60		374
B60G2400/00	7	Indexing codes relating to detected, measured or calculated conditions or factors	CPCONLY	B60G2400/00		24
B60G2400/05	8	Attitude	CPCONLY	B60G2400/05		171
B60G2400/051	9	Angle	CPCONLY	B60G2400/051		141
B60G2400/0511	10	Roll angle	CPCONLY	B60G2400/0511		515
B60G2400/0512	10	Pitch angle	CPCONLY	B60G2400/0512		305
B60G2400/0513	10	Yaw angle	CPCONLY	B60G2400/0513		83
B60G2400/0514	10	Wheel angle detection	CPCONLY	B60G2400/0514		24
B60G2400/05142	11	Wheel camber	CPCONLY	B60G2400/05142		81
B60G2400/05144	11	Wheel toe	CPCONLY	B60G2400/05144		84
B60G2400/05146	11	Wheel caster	CPCONLY	B60G2400/05146		22
B60G2400/0516	10	Angular position of a suspension element	CPCONLY	B60G2400/0516		61
B60G2400/05162	11	the element being a suspension arm	CPCONLY	B60G2400/05162		60
B60G2400/052	9	Angular rate	CPCONLY	B60G2400/052		61
B60G2400/0521	10	Roll rate	CPCONLY	B60G2400/0521		220
B60G2400/0522	10	Pitch rate	CPCONLY	B60G2400/0522		137
B60G2400/0523	10	Yaw rate	CPCONLY	B60G2400/0523		354
B60G2400/053	9	Angular acceleration	CPCONLY	B60G2400/053		16
B60G2400/0531	10	Roll acceleration	CPCONLY	B60G2400/0531		59
B60G2400/0532	10	Pitch acceleration	CPCONLY	B60G2400/0532		49
B60G2400/0533	10	Yaw acceleration	CPCONLY	B60G2400/0533		38
B60G2400/10	8	Acceleration; Deceleration	CPCONLY	B60G2400/10		603
B60G2400/102	9	vertical	CPCONLY	B60G2400/102		1122
B60G2400/104	9	lateral or transversal with regard to vehicle	CPCONLY	B60G2400/104		1146
B60G2400/1042	10	using at least two sensors	CPCONLY	B60G2400/1042		77
B60G2400/106	9	longitudinal with regard to vehicle, e.g. braking	CPCONLY	B60G2400/106		759
B60G2400/1062	10	using at least two sensors	CPCONLY	B60G2400/1062		17
B60G2400/20	8	Speed	CPCONLY	B60G2400/20		216
B60G2400/202	9	Piston speed; Relative velocity between vehicle body and wheel	CPCONLY	B60G2400/202		408
B60G2400/204	9	Vehicle speed	CPCONLY	B60G2400/204		2280
B60G2400/2042	10	Lateral speed	CPCONLY	B60G2400/2042		21
B60G2400/206	9	Body oscillation speed; Body vibration frequency	CPCONLY	B60G2400/206		358
B60G2400/208	9	of wheel rotation	CPCONLY	B60G2400/208		537
B60G2400/25	8	Stroke; Height; Displacement	CPCONLY	B60G2400/25		499
B60G2400/252	9	vertical	CPCONLY	B60G2400/252		2859
B60G2400/256	9	horizontal	CPCONLY	B60G2400/256		40
B60G2400/257	10	transversal with regard to vehicle	CPCONLY	B60G2400/257		12
B60G2400/258	10	longitudinal with regard to vehicle	CPCONLY	B60G2400/258		12
B60G2400/30	8	Propulsion unit conditions	CPCONLY	B60G2400/30		193
B60G2400/302	9	Selected gear ratio; Transmission function	CPCONLY	B60G2400/302		117
B60G2400/304	10	neutral position	CPCONLY	B60G2400/304		12
B60G2400/306	10	overdrive	CPCONLY	B60G2400/306		1
B60G2400/31	9	Clutch condition	CPCONLY	B60G2400/31		29
B60G2400/32	9	Torque on propulsion shaft	CPCONLY	B60G2400/32		71
B60G2400/33	9	Throttle position	CPCONLY	B60G2400/33		163
B60G2400/34	9	Accelerator pedal position	CPCONLY	B60G2400/34		144
B60G2400/35	9	Position of fuel or air injector	CPCONLY	B60G2400/35		8
B60G2400/36	9	Functioning of turbocharger	CPCONLY	B60G2400/36		1
B60G2400/37	9	Brake pad or disc friction	CPCONLY	B60G2400/37		34
B60G2400/38	9	Speed of engine rotation	CPCONLY	B60G2400/38		140
B60G2400/382	10	Ignition switch	CPCONLY	B60G2400/382		21
B60G2400/39	9	Brake pedal position	CPCONLY	B60G2400/39		235
B60G2400/40	8	Steering conditions	CPCONLY	B60G2400/40		223
B60G2400/41	9	Steering angle	CPCONLY	B60G2400/41		1126
B60G2400/412	10	of steering wheel or column	CPCONLY	B60G2400/412		221
B60G2400/4122	11	Neutral position detection	CPCONLY	B60G2400/4122		14
B60G2400/42	9	Steering torque	CPCONLY	B60G2400/42		64
B60G2400/44	9	Steering speed	CPCONLY	B60G2400/44		116
B60G2400/46	9	Steering frequency	CPCONLY	B60G2400/46		6
B60G2400/47	9	Rear wheel steering	CPCONLY	B60G2400/47		16
B60G2400/50	8	Pressure	CPCONLY	B60G2400/50		348
B60G2400/51	9	in suspension unit	CPCONLY	B60G2400/51		304
B60G2400/512	10	in spring	CPCONLY	B60G2400/512		25
B60G2400/5122	11	Fluid spring	CPCONLY	B60G2400/5122		95
B60G2400/51222	12	Pneumatic	CPCONLY	B60G2400/51222		481
B60G2400/518	10	in damper	CPCONLY	B60G2400/518		42
B60G2400/5182	11	Fluid damper	CPCONLY	B60G2400/5182		186
B60G2400/52	9	in tyre	CPCONLY	B60G2400/52		218
B60G2400/60	8	Load	CPCONLY	B60G2400/60		1020
B60G2400/61	9	Load distribution	CPCONLY	B60G2400/61		786
B60G2400/62	9	Seat occupation; Passenger presence	CPCONLY	B60G2400/62		63
B60G2400/63	9	Location of the center of gravity	CPCONLY	B60G2400/63		262
B60G2400/64	9	Wheel forces, e.g. on hub, spindle or bearing	CPCONLY	B60G2400/64		173
B60G2400/70	8	Temperature of vehicle part or in the vehicle	CPCONLY	B60G2400/70		52
B60G2400/71	9	of suspension unit	CPCONLY	B60G2400/71		59
B60G2400/712	10	of spring	CPCONLY	B60G2400/712		12
B60G2400/7122	11	Fluid spring	CPCONLY	B60G2400/7122		56
B60G2400/716	10	of damper	CPCONLY	B60G2400/716		14
B60G2400/7162	11	Fluid damper	CPCONLY	B60G2400/7162		59
B60G2400/72	9	in vehicle interior	CPCONLY	B60G2400/72		4
B60G2400/73	9	of other part than suspension unit	CPCONLY	B60G2400/73		37
B60G2400/732	10	of propulsion unit	CPCONLY	B60G2400/732		10
B60G2400/80	8	Exterior conditions	CPCONLY	B60G2400/80		141
B60G2400/82	9	Ground surface	CPCONLY	B60G2400/82		712
B60G2400/821	10	Uneven, rough road sensing affecting vehicle body vibration	CPCONLY	B60G2400/821		791
B60G2400/822	10	Road friction coefficient determination affecting wheel traction	CPCONLY	B60G2400/822		178
B60G2400/8222	11	Hydroplaning	CPCONLY	B60G2400/8222		19
B60G2400/823	10	Obstacle sensing	CPCONLY	B60G2400/823		369
B60G2400/824	10	Travel path sensing; Track monitoring	CPCONLY	B60G2400/824		233
B60G2400/84	9	Atmospheric conditions	CPCONLY	B60G2400/84		39
B60G2400/841	10	Wind	CPCONLY	B60G2400/841		84
B60G2400/842	10	Temperature	CPCONLY	B60G2400/842		52
B60G2400/8422	11	of air	CPCONLY	B60G2400/8422		46
B60G2400/8424	11	of ground or road	CPCONLY	B60G2400/8424		10
B60G2400/843	10	Humidity; Rainfall	CPCONLY	B60G2400/843		59
B60G2400/845	10	Darkness	CPCONLY	B60G2400/845		3
B60G2400/847	10	Sunshine; Light	CPCONLY	B60G2400/847		6
B60G2400/90	8	Other conditions or factors	CPCONLY	B60G2400/90		338
B60G2400/91	9	Frequency	CPCONLY	B60G2400/91		481
B60G2400/92	9	Travelling or driving time	CPCONLY	B60G2400/92		19
B60G2400/922	9	Travelling distance	CPCONLY	B60G2400/922		26
B60G2400/94	9	Deformation of a vehicle part	CPCONLY	B60G2400/94		47
B60G2400/942	10	of vehicle body	CPCONLY	B60G2400/942		6
B60G2400/95	9	Position of vehicle body elements	CPCONLY	B60G2400/95		65
B60G2400/952	10	of door or bonnet	CPCONLY	B60G2400/952		97
B60G2400/954	10	Wheelbase	CPCONLY	B60G2400/954		18
B60G2400/96	9	Presence, absence or inactivity of driver	CPCONLY	B60G2400/96		41
B60G2400/97	9	Relation between towing and towed vehicle, e.g. tractor-trailer combination	CPCONLY	B60G2400/97		60
B60G2400/972	10	Angle of articulation	CPCONLY	B60G2400/972		18
B60G2400/98	9	Stabiliser movement	CPCONLY	B60G2400/98		113
B60G2401/00	7	Indexing codes relating to the type of sensors based on the principle of their operation	CPCONLY	B60G2401/00		153
B60G2401/10	8	Piezoelectric elements	CPCONLY	B60G2401/10		217
B60G2401/11	8	Electrostrictive transducers	CPCONLY	B60G2401/11		24
B60G2401/12	8	Strain gauge	CPCONLY	B60G2401/12		209
B60G2401/122	9	Wheatstone bridge circuit	CPCONLY	B60G2401/122		14
B60G2401/14	8	Photo or light sensitive means, e.g. Infrared	CPCONLY	B60G2401/14		288
B60G2401/142	9	Visual Display Camera, e.g. LCD	CPCONLY	B60G2401/142		333
B60G2401/144	9	Fiber optic sensor	CPCONLY	B60G2401/144		18
B60G2401/15	8	Doppler effect	CPCONLY	B60G2401/15		29
B60G2401/16	8	GPS track data	CPCONLY	B60G2401/16		273
B60G2401/17	8	Magnetic/Electromagnetic	CPCONLY	B60G2401/17		201
B60G2401/172	9	Hall effect	CPCONLY	B60G2401/172		165
B60G2401/174	9	Radar	CPCONLY	B60G2401/174		185
B60G2401/176	9	Radio or audio sensitive means, e.g. Ultrasonic	CPCONLY	B60G2401/176		199
B60G2401/19	8	Speech recognising means	CPCONLY	B60G2401/19		4
B60G2401/20	8	Switches, e.g. mercury or ball type switches	CPCONLY	B60G2401/20		118
B60G2401/21	8	Laser	CPCONLY	B60G2401/21		117
B60G2401/22	8	Radioactivity sensitive materials	CPCONLY	B60G2401/22		5
B60G2401/23	8	Memory materials	CPCONLY	B60G2401/23		14
B60G2401/24	8	Heat sensitive materials; temperature gauge	CPCONLY	B60G2401/24		4
B60G2401/25	8	Capacitance type, e.g. as level indicator	CPCONLY	B60G2401/25		35
B60G2401/26	8	Resistance type, e.g. as level indicator	CPCONLY	B60G2401/26		57
B60G2401/27	8	Gravitational, e.g. pendulum or axial movement type	CPCONLY	B60G2401/27		20
B60G2401/28	8	Gyroscopes	CPCONLY	B60G2401/28		130
B60G2401/90	8	Single sensor for two or more measurements	CPCONLY	B60G2401/90		26
B60G2401/902	9	the sensor being an xy axis sensor	CPCONLY	B60G2401/902		17
B60G2401/904	9	the sensor being an xyz axis sensor	CPCONLY	B60G2401/904		35
B60G2500/00	7	Indexing codes relating to the regulated action or device	CPCONLY	B60G2500/00		49
B60G2500/02	8	Supply or exhaust flow rates; Pump operation	CPCONLY	B60G2500/02		267
B60G2500/022	9	Minimisation of pressure cavitation effects upon demand	CPCONLY	B60G2500/022		19
B60G2500/04	8	using inertia type valves	CPCONLY	B60G2500/04		11
B60G2500/10	8	Damping action or damper	CPCONLY	B60G2500/10		2273
B60G2500/102	9	stepwise	CPCONLY	B60G2500/102		200
B60G2500/104	9	continuous	CPCONLY	B60G2500/104		267
B60G2500/106	9	duty rate	CPCONLY	B60G2500/106		51
B60G2500/11	9	Damping valves	CPCONLY	B60G2500/11		450
B60G2500/112	10	Fluid actuation	CPCONLY	B60G2500/112		79
B60G2500/114	10	pressure regulating valves	CPCONLY	B60G2500/114		158
B60G2500/116	10	for damping pressure oscillations of the fluid in hydraulic lines	CPCONLY	B60G2500/116		10
B60G2500/20	8	Spring action or springs	CPCONLY	B60G2500/20		1478
B60G2500/201	9	Air spring system type	CPCONLY	B60G2500/201		165
B60G2500/2012	10	Open systems	CPCONLY	B60G2500/2012		128
B60G2500/2014	10	Closed systems	CPCONLY	B60G2500/2014		162
B60G2500/202	9	Height or leveling valve for air-springs	CPCONLY	B60G2500/202		351
B60G2500/2021	10	Arrangement of valves	CPCONLY	B60G2500/2021		194
B60G2500/2022	10	with valve seat actuation for selectively adjusting neutral height	CPCONLY	B60G2500/2022		50
B60G2500/203	9	Distributor valve units comprising several elements, e.g. valves, pump or accumulators	CPCONLY	B60G2500/203		261
B60G2500/204	9	Pressure regulating valves for air-springs	CPCONLY	B60G2500/204		249
B60G2500/2041	10	for variable volume air springs, e.g. using accumulators as expansion chambers	CPCONLY	B60G2500/2041		76
B60G2500/2042	10	Air filling valves	CPCONLY	B60G2500/2042		94
B60G2500/2043	10	Wheatstone bridge type valve arrangements	CPCONLY	B60G2500/2043		9
B60G2500/2044	10	Air exhausting valves	CPCONLY	B60G2500/2044		142
B60G2500/2046	10	Pressure equalising valves between two units	CPCONLY	B60G2500/2046		29
B60G2500/205	9	Air-compressor operation	CPCONLY	B60G2500/205		314
B60G2500/206	9	Variable pressure accumulators for hydropneumatic suspensions	CPCONLY	B60G2500/206		63
B60G2500/2062	10	by varying the air-pressure of the accumulator	CPCONLY	B60G2500/2062		67
B60G2500/2064	10	by varying the number of accumulators connected in parallel to the hydraulic cylinder	CPCONLY	B60G2500/2064		43
B60G2500/22	9	Spring constant	CPCONLY	B60G2500/22		616
B60G2500/30	8	Height or ground clearance	CPCONLY	B60G2500/30		3773
B60G2500/302	9	using distributor valves	CPCONLY	B60G2500/302		206
B60G2500/32	9	of only one vehicle part or side	CPCONLY	B60G2500/32		119
B60G2500/322	10	only front part	CPCONLY	B60G2500/322		66
B60G2500/324	10	only rear part	CPCONLY	B60G2500/324		111
B60G2500/326	10	only left or right side	CPCONLY	B60G2500/326		72
B60G2500/40	8	Steering	CPCONLY	B60G2500/40		257
B60G2500/42	9	Sensibility	CPCONLY	B60G2500/42		16
B60G2600/00	7	Indexing codes relating to particular elements, systems or processes used on suspension systems or suspension control systems	CPCONLY	B60G2600/00		13
B60G2600/02	8	Retarders, delaying means, dead zones, threshold values, cut-off frequency, timer interruption	CPCONLY	B60G2600/02		1060
B60G2600/04	8	Means for informing, instructing or displaying	CPCONLY	B60G2600/04		295
B60G2600/042	9	Monitoring means	CPCONLY	B60G2600/042		166
B60G2600/0422	10	involving data transmission, e.g. via satellite or GPS; for data monitoring, telemetry or platooning purposes	CPCONLY	B60G2600/0422		92
B60G2600/044	9	Alarm means	CPCONLY	B60G2600/044		283
B60G2600/07	8	Inhibiting means	CPCONLY	B60G2600/07		176
B60G2600/08	8	Failure or malfunction detecting means	CPCONLY	B60G2600/08		494
B60G2600/082	9	Sensor drift	CPCONLY	B60G2600/082		36
B60G2600/084	9	Supervisory systems	CPCONLY	B60G2600/084		55
B60G2600/086	9	Redundant systems	CPCONLY	B60G2600/086		19
B60G2600/09	8	Feedback signal	CPCONLY	B60G2600/09		103
B60G2600/11	8	Feedforward signal	CPCONLY	B60G2600/11		39
B60G2600/12	8	Sampling or average detecting; Addition or substraction	CPCONLY	B60G2600/12		111
B60G2600/122	9	Summation signal	CPCONLY	B60G2600/122		17
B60G2600/124	9	Error signal	CPCONLY	B60G2600/124		55
B60G2600/14	8	Differentiating means, i.e. differential control	CPCONLY	B60G2600/14		206
B60G2600/16	8	Integrating means, i.e. integral control	CPCONLY	B60G2600/16		172
B60G2600/17	8	Proportional control, i.e. gain control	CPCONLY	B60G2600/17		77
B60G2600/172	9	Weighting coefficients or factors	CPCONLY	B60G2600/172		42
B60G2600/18	8	Automatic control means	CPCONLY	B60G2600/18		233
B60G2600/181	9	Signal modulation; pulse-width, frequency-phase	CPCONLY	B60G2600/181		41
B60G2600/182	9	Active control means	CPCONLY	B60G2600/182		769
B60G2600/184	9	Semi-Active control means	CPCONLY	B60G2600/184		499
B60G2600/186	9	Analogue Controller Details and Signal Treatment	CPCONLY	B60G2600/186		6
B60G2600/187	9	Digital Controller Details and Signal Treatment	CPCONLY	B60G2600/187		81
B60G2600/1871	10	Optimal control; Kalman Filters	CPCONLY	B60G2600/1871		62
B60G2600/1872	10	Observer; Luaponov function	CPCONLY	B60G2600/1872		23
B60G2600/1873	10	Model Following	CPCONLY	B60G2600/1873		63
B60G2600/1874	10	Modal analysis	CPCONLY	B60G2600/1874		17
B60G2600/1875	10	Other parameter or state estimation methods not involving the mathematical modelling of the vehicle	CPCONLY	B60G2600/1875		56
B60G2600/1876	10	Artificial intelligence	CPCONLY	B60G2600/1876		18
B60G2600/1877	10	Adaptive Control	CPCONLY	B60G2600/1877		109
B60G2600/1878	10	Neural Networks	CPCONLY	B60G2600/1878		53
B60G2600/1879	10	Fuzzy Logic Control	CPCONLY	B60G2600/1879		60
B60G2600/188	9	Spectral analysis; Transformations	CPCONLY	B60G2600/188		44
B60G2600/1881	10	Integral	CPCONLY	B60G2600/1881		31
B60G2600/1882	10	Fourier	CPCONLY	B60G2600/1882		16
B60G2600/1883	10	z-transform	CPCONLY	B60G2600/1883		
B60G2600/1884	10	Laplace	CPCONLY	B60G2600/1884		6
B60G2600/1885	10	Euler equations	CPCONLY	B60G2600/1885		1
B60G2600/189	9	Statistical analysis	CPCONLY	B60G2600/189		12
B60G2600/20	8	Manual control or setting means	CPCONLY	B60G2600/20		519
B60G2600/202	9	using a remote, e.g. cordless, transmitter or receiver unit	CPCONLY	B60G2600/202		117
B60G2600/204	9	Joystick actuated suspension	CPCONLY	B60G2600/204		14
B60G2600/206	9	Control-by-wire	CPCONLY	B60G2600/206		20
B60G2600/21	8	Self-controlled or adjusted	CPCONLY	B60G2600/21		136
B60G2600/22	8	Magnetic elements	CPCONLY	B60G2600/22		132
B60G2600/24	9	permanent magnets	CPCONLY	B60G2600/24		114
B60G2600/26	9	Electromagnets; Solenoids	CPCONLY	B60G2600/26		793
B60G2600/28	8	Temporary fluctuations	CPCONLY	B60G2600/28		21
B60G2600/41	8	SISO system, i.e. single input - single output system	CPCONLY	B60G2600/41		4
B60G2600/43	8	MIMO system, i.e. multi input - multi output system	CPCONLY	B60G2600/43		4
B60G2600/44	8	Vibration noise suppression	CPCONLY	B60G2600/44		452
B60G2600/60	8	Signal noise suppression; Electronic filtering means	CPCONLY	B60G2600/60		233
B60G2600/602	9	high pass	CPCONLY	B60G2600/602		117
B60G2600/604	9	low pass	CPCONLY	B60G2600/604		250
B60G2600/66	8	Humidifying or drying means	CPCONLY	B60G2600/66		143
B60G2600/68	8	Filtering means, e.g. fluid filters	CPCONLY	B60G2600/68		61
B60G2600/70	8	Computer memory; Data storage, e.g. maps for adaptive control	CPCONLY	B60G2600/70		326
B60G2600/702	9	Parallel processing	CPCONLY	B60G2600/702		9
B60G2600/704	9	Electronic tags containing data, e.g. identification number of a component; Gain values for the control of the unit, etc.	CPCONLY	B60G2600/704		13
B60G2600/71	8	Distributed control; Hierarchical control structure, e.g. with one unit steering and other units following; Remote control units	CPCONLY	B60G2600/71		58
B60G2600/72	8	Cooling or warming means	CPCONLY	B60G2600/72		115
B60G2600/73	8	Electrical control	CPCONLY	B60G2600/73		71
B60G2600/74	8	Analog systems	CPCONLY	B60G2600/74		56
B60G2600/76	8	Digital systems	CPCONLY	B60G2600/76		117
B60G2600/77	8	A/D, D/A signal converters	CPCONLY	B60G2600/77		23
B60G2600/82	8	duty rate function	CPCONLY	B60G2600/82		53
B60G2600/85	8	Speed of regulation	CPCONLY	B60G2600/85		78
B60G2600/90	8	other signal treatment means	CPCONLY	B60G2600/90		98
B60G2800/00	7	Indexing codes relating to the type of movement or to the condition of the vehicle and to the end result to be achieved by the control action	CPCONLY	B60G2800/00		2
B60G2800/01	8	Attitude or posture control	CPCONLY	B60G2800/01		377
B60G2800/012	9	Rolling condition	CPCONLY	B60G2800/012		1670
B60G2800/0122	10	Roll rigidity ratio; Warping	CPCONLY	B60G2800/0122		117
B60G2800/0124	10	Roll-over conditions	CPCONLY	B60G2800/0124		162
B60G2800/014	9	Pitch; Nose dive	CPCONLY	B60G2800/014		793
B60G2800/016	9	Yawing condition	CPCONLY	B60G2800/016		146
B60G2800/019	9	Inclination due to load distribution or road gradient	CPCONLY	B60G2800/019		250
B60G2800/0192	10	longitudinal with regard to vehicle	CPCONLY	B60G2800/0192		155
B60G2800/0194	10	transversal with regard to vehicle	CPCONLY	B60G2800/0194		197
B60G2800/16	8	Running	CPCONLY	B60G2800/16		116
B60G2800/162	9	Reducing road induced vibrations	CPCONLY	B60G2800/162		1030
B60G2800/164	9	Heaving; Squatting	CPCONLY	B60G2800/164		105
B60G2800/166	9	Platooning	CPCONLY	B60G2800/166		19
B60G2800/18	8	Starting, accelerating	CPCONLY	B60G2800/18		143
B60G2800/182	9	Traction	CPCONLY	B60G2800/182		60
B60G2800/20	8	Stationary vehicle	CPCONLY	B60G2800/20		739
B60G2800/202	9	kneeling, e.g. for letting passengers on/off	CPCONLY	B60G2800/202		127
B60G2800/203	9	lowering the floor for loading/unloading	CPCONLY	B60G2800/203		142
B60G2800/204	9	adjusting floor height to the loading ramp level	CPCONLY	B60G2800/204		98
B60G2800/2042	10	using an anticreep mechanism to lock the height	CPCONLY	B60G2800/2042		26
B60G2800/205	9	jacking-up for changing tyre or vehicle inspection	CPCONLY	B60G2800/205		38
B60G2800/21	8	Traction, slip, skid or slide control	CPCONLY	B60G2800/21		183
B60G2800/212	9	Transversal; Side-slip during cornering	CPCONLY	B60G2800/212		57
B60G2800/213	9	by applying forward/backward torque on each wheel individually	CPCONLY	B60G2800/213		28
B60G2800/214	9	by varying the load distribution	CPCONLY	B60G2800/214		143
B60G2800/215	9	by applying a braking action on each wheel individually	CPCONLY	B60G2800/215		72
B60G2800/22	8	Braking, stopping	CPCONLY	B60G2800/22		440
B60G2800/222	9	during collision	CPCONLY	B60G2800/222		210
B60G2800/224	9	automatically, based on dangerous living style	CPCONLY	B60G2800/224		24
B60G2800/226	9	automatically, based on stopping at a preset or target point position	CPCONLY	B60G2800/226		14
B60G2800/24	8	Steering, cornering	CPCONLY	B60G2800/24		883
B60G2800/242	9	Obstacle avoidance manoeuvre	CPCONLY	B60G2800/242		35
B60G2800/244	9	Oversteer	CPCONLY	B60G2800/244		145
B60G2800/246	9	Understeer	CPCONLY	B60G2800/246		130
B60G2800/248	9	Neutral steering behaviour	CPCONLY	B60G2800/248		17
B60G2800/70	8	Estimating or calculating vehicle parameters or state variables	CPCONLY	B60G2800/70		386
B60G2800/702	9	Improving accuracy of a sensor signal	CPCONLY	B60G2800/702		312
B60G2800/7022	10	Calibration of a sensor, e.g. automatically	CPCONLY	B60G2800/7022		46
B60G2800/704	9	predicting unorthodox driving conditions for safe or optimal driving	CPCONLY	B60G2800/704		69
B60G2800/80	8	Detection or control after a system or component failure	CPCONLY	B60G2800/80		190
B60G2800/802	9	Diagnostics	CPCONLY	B60G2800/802		175
B60G2800/85	8	System Prioritisation	CPCONLY	B60G2800/85		92
B60G2800/87	8	System configuration based on vehicle type or model	CPCONLY	B60G2800/87		35
B60G2800/90	8	System Controller type	CPCONLY	B60G2800/90		96
B60G2800/91	9	Suspension Control	CPCONLY	B60G2800/91		428
B60G2800/912	10	Attitude Control; levelling control	CPCONLY	B60G2800/912		459
B60G2800/9122	11	ARS - Anti-Roll System Control	CPCONLY	B60G2800/9122		238
B60G2800/9123	11	Active Body Control [ABC]	CPCONLY	B60G2800/9123		73
B60G2800/9124	11	Roll-over protection systems, e.g. for warning or control	CPCONLY	B60G2800/9124		240
B60G2800/914	10	Height Control System	CPCONLY	B60G2800/914		922
B60G2800/915	10	Suspension load distribution	CPCONLY	B60G2800/915		195
B60G2800/916	10	Body Vibration Control	CPCONLY	B60G2800/916		367
B60G2800/92	9	ABS - Brake Control	CPCONLY	B60G2800/92		280
B60G2800/922	10	EBV - Electronic brake force distribution	CPCONLY	B60G2800/922		127
B60G2800/925	9	Airbag deployment systems	CPCONLY	B60G2800/925		44
B60G2800/93	9	Skid or slide control [ASR]	CPCONLY	B60G2800/93		56
B60G2800/94	9	Electronic Stability Program (ESP, i.e. ABS+ASC+EMS)	CPCONLY	B60G2800/94		109
B60G2800/95	9	Automatic Traction or Slip Control [ATC]	CPCONLY	B60G2800/95		82
B60G2800/952	10	Electronic driving torque distribution	CPCONLY	B60G2800/952		56
B60G2800/954	10	Four-wheel drive	CPCONLY	B60G2800/954		25
B60G2800/96	9	ASC - Assisted or power Steering control	CPCONLY	B60G2800/96		101
B60G2800/962	10	Four-wheel steering	CPCONLY	B60G2800/962		55
B60G2800/963	10	Steer-by-wire	CPCONLY	B60G2800/963		58
B60G2800/964	10	Auto-navigation	CPCONLY	B60G2800/964		10
B60G2800/965	10	Automatic or driver-independent manoeuvre, e.g. for obstacle avoidance or roll-over prevention	CPCONLY	B60G2800/965		18
B60G2800/97	9	Engine Management System [EMS]	CPCONLY	B60G2800/97		83
B60G2800/972	9	Electronic Differential Lock [EDS]	CPCONLY	B60G2800/972		3
B60G2800/98	9	Intelligent Transportation System or Bus [IDB]	CPCONLY	B60G2800/98		12
B60G2800/982	9	Active Cruise Control, e.g. DISTRONIC type	CPCONLY	B60G2800/982		14
B60G2800/984	9	Tyre Pressure Monitoring Systems	CPCONLY	B60G2800/984		47
