G04B1/00	7	Driving mechanisms {(driving mechanisms for Turkish time G04B19/22; driving mechanisms in the hands G04B45/043; driving mechanisms for phonographic apparatus G11B19/00; springs, driving weight engines F03G; driving mechanisms for cinematography G03B1/00; driving mechnisms; driving mechanisms for time fuses for missiles F42C; driving mechnisms for toys A63H29/00)}	G04B1/00	G04B1/00		123
G04B1/02	8	with driving weight	G04B1/02	G04B1/02		54
G04B1/04	9	Mechanisms in which the clockwork acts as the driving weight	G04B1/04	G04B1/04		34
G04B1/06	9	with several weights {(winding up several weights simultaneously G04B3/00)}	G04B1/06	G04B1/06		13
G04B1/08	9	Driving weights; Chains; Chain wheels; Arbors for chain wheels {(wheels and spindles in general F16F)}	G04B1/08	G04B1/08		50
G04B1/10	8	with mainspring {(synchronous motors with power reserve G04C15/0054; springs in general F16F)}	G04B1/10	G04B1/10		124
G04B1/105	9	{having a form other than a helix (G04B1/12 and G04B1/14 take precedence)}	G04B1/10	G04B1/10		47
G04B1/12	9	with several mainsprings {(installations with a mainspring and an auxiliary spring G04B1/225; winding-up several mainsprings simultaneously G04B3/008)}	G04B1/12	G04B1/12		162
G04B1/14	9	Mainsprings; Bridles therefor (mainsprings with bridles G04B1/18; alloys C22C; springs in general F16F{; constructions for compensation of changes in the motive power of the mainspring G04B1/22; construction of the hairspring G04B17/066; arrangements facilitating the removal of the mainspring G04B33/14})	G04B1/14	G04B1/14		97
G04B1/145	10	{Composition and manufacture of the springs (compositions and manufacture of components, wheels, spindles, pivots, or the like G04B13/02; compositions of component escapements G04B15/14; composition and manufacture or hairsprings G04B17/066; compensation for the effects of variations of temperature of springs using alloys, especially for hairsprings G04B17/227; materials for bearings of clockworks G04B31/00; heat treatment and chemical or mechanical treatment for control of the structure C21D8/00; iron and steel alloys C22C; non-ferrous alloys C22C and B22F)}	G04B1/14	G04B1/14		234
G04B1/16	9	Barrels; Arbors; Barrel axles (arrangements facilitating the removal of the mainspring G04B33/14)	G04B1/16	G04B1/16		336
G04B1/165	10	{Spring cylinder with friction transmission to the gearing (especially for Roskopf clockworks); (friction clutch between spring and spring cylinder G04B1/185)}	G04B1/16	G04B1/16		65
G04B1/18	9	Constructions for connecting the ends of the mainsprings with the barrel or the arbor {(mainsprings and bridles therefor G04B1/14; clamping the hairspring on the regulator G04B18/026; clamping the hairspring on the arbor G04B17/32)}	G04B1/18	G04B1/18		138
G04B1/185	10	{Friction clutch between spring and spring cylinder (friction transmission between spring cylinder and gearing G04B1/165; other arrangements for protection against rupture or overwinding G04B1/20)}	G04B1/18	G04B1/18		82
G04B1/20	10	Protecting arrangements against rupture or overwinding of the mainspring located in the barrel or attached to the barrel (in connection with keys or the like G04B3/06, G04B3/10; in connection with automatic winding devices G04B5/24{; protecting arrangements in which the spring and the spring cylinder are connected by friction G04B1/185; protecting arrangements G04B9/02; calibers with arrangements affording protection of the clockwork against damage as a consequence of a rupture of the mainspring G04B33/16; electric winding arrangements with protection against overwinding of mechanical clockworks G04C1/10; driving mechanisms for gramophones G11B19/22, G11B19/28})	G04B1/20	G04B1/20		134
G04B1/205	11	{Stop-mechanisms}	G04B1/20	G04B1/20		39
G04B1/22	9	Compensation of changes in the motive power of the mainspring (by mechanical shaping of the mainspring G04B1/14{; automatic regulation of the pendulum G04B18/003; of the regulator G04B19/28})	G04B1/22	G04B1/22		120
G04B1/225	10	{with the aid of an interposed power-accumulator (secondary spring) which is always tensioned (winding up several mainsprings or driving weights simultaneously G04B3/008)}	G04B1/22	G04B1/22		142
G04B1/24	8	with both mainsprings and driving weights {(winding up several mainsprings or driving weights simultaneously G04B3/008)}	G04B1/24	G04B1/24		19
G04B1/26	8	driven by liquids or gases; Liquid or gaseous drives for mechanically-controlled secondary clocks {(winding up by pneumatic means G04B3/12; winding up automatically by wind power G04B5/203; winding up by electro-thermal or electro-pneumatic arrangements G04C1/003; thermo-electric or thermo-pneumatic driving mechanisms G04C3/18)}	G04B1/26	G04B1/26		110
G04B1/265	9	{Clockwork systems working therewith (winding up electrical or mechanical clocks G04C1/006; electrical clockwork installations G04C13/00)}	G04B1/26	G04B1/26		45
G04B3/00	7	Normal winding of clockworks by hand or mechanically; Winding up several mainsprings or driving weights simultaneously {(automatic winding up G04B5/00; combined normal and automatic winding up G04B7/00; click devices G04B11/00; winding up the striking mechanism by the clockwork and vice versaG04B21/14; mechanical devices for setting the time-indication by using the winding means G04B27/02, G04B27/083; calibers of which the mainsprings are easily removable G04B33/14; winding mechanical clocks electrically G04C1/00; tools for setting springs G04D1/04; driving mechanisms for gramophones G11B19/00; driving mechanisms for cinematographs G03B1/00)}	G04B3/00	G04B3/00		139
G04B3/001	8	{by push button (crown combined with push button G04B3/046; construction of push button G04B3/048; waterproof push buttons G04B37/106)}	G04B3/00	G04B3/00		47
G04B3/003	8	{by lever mechanism}	G04B3/00	G04B3/00		54
G04B3/005	8	{by draw mechanism}	G04B3/00	G04B3/00		37
G04B3/006	8	{Mechanical winding up; winding up with special equipment (removably-mounted keys G04B3/02; winding up equipment for clocks with automatic winding up equipment G04B5/00)}	G04B3/00	G04B3/00		173
G04B3/008	8	{Winding up several mainsprings or driving weights simultaneously (driving mechanisms with several weights G04B1/06; driving mechanisms with several mainsprings G04B1/12; driving mechanisms with a mainspring and a secondary spring G04B1/225; driving mechanisms with mainsprings and driving weights G04B1/24; winding up the striking mechanisms with the clockwork and vice versaG04B21/14)}	G04B3/00	G04B3/00		49
G04B3/02	8	Removably-mounted keys or the like {(special tools for clockworks with difficult access, universal keys for watches with a small crown G04B3/006; keys with means preventing overwinding G04B3/06; protecting means preventing overwinding G04B3/10)}	G04B3/02	G04B3/02		95
G04B3/04	8	Rigidly-mounted keys, knobs or crowns {(jointed winding-stem G04B37/06)}	G04B3/04	G04B3/04		255
G04B3/041	9	{Construction of crowns for rotating movement; connection with the winding stem; winding stems}	G04B3/04	G04B3/04		272
G04B3/043	9	{Locking of the operating element, also by mounting in a concealed place}	G04B3/04	G04B3/04		152
G04B3/045	9	{Storing the operating element, also bringing it out of storage}	G04B3/04	G04B3/04		183
G04B3/046	9	{Operation by rotation and axial movement with extra function of axial shift of operating element, e.g. crown combined with push button (winding up by push button G04B3/001)}	G04B3/04	G04B3/04		181
G04B3/048	9	{Operation exclusively by axial movement of a push-button, e.g. for chronographs (winding up by push button G04B3/001; hermetically sealed push button G04B37/106)}	G04B3/04	G04B3/04		206
G04B3/06	8	Keys or the like with means preventing overwinding (protecting devices arranged in, or attached to, the barrel G04B1/20; in connection with automatic winding devices G04B1/24{; construction of removably-mounted keys G04B3/02; means preventing overwinding, including those attached to the case, G04B3/10; protecting means G04B9/02; protection against overwinding for electrical winding up arrangements for mechanical clocks G04C1/10})	G04B3/06	G04B3/06		87
G04B3/08	8	by parts of the cases {(setting the time-indicating means by parts of the case G04B27/00)}	G04B3/08	G04B3/08		90
G04B3/10	9	Protecting means preventing overwinding (arranged in, or attached to, the barrel G04B1/20; in connection with keys G04B3/06; in connection with automatic winding devices G04B5/24{; protection G04B9/02; of electrical winding up arrangements for mechanical clocks G04C1/10})	G04B3/10	G04B3/10		11
G04B3/12	8	by mechanical means, e.g. pneumatic motor (winding up with electric or electromechanical means G04C{; liquid or gas driving mechanisms G04B1/26; automatic winding up by wind power G04B5/203})	G04B3/12	G04B3/12		40
G04B5/00	7	Automatic winding up {(normal winding up by hand or mechanically G04B3/00; automatic winding in combination with hand winding G04B7/00; electrical winding of mechanical clockworks G04C1/00; advertising by making use of vibrations or shocks of land vehicles G09F21/045)}	G04B5/00	G04B5/00		102
G04B5/002	8	{by moving of parts of the clockwork which are not primarily for winding up}	G04B5/00	G04B5/00		90
G04B5/005	8	{by relative movement between watch bands, case or parts of the case}	G04B5/00	G04B5/00		27
G04B5/007	8	{Clockworks, which wind up by driving the function, e.g. perpetua mobilia(see also F03G7/10)}	G04B5/00	G04B5/00		23
G04B5/02	8	by self-winding caused by the movement of the watch {(bearings, suspensions for oscillating weights G04B5/18; mechanisms for transformation of an oscillating movement into a rotating movement in only one direction G04B11/00)}	G04B5/02	G04B5/02		311
G04B5/04	9	by oscillating weights the movement of which is limited {(setting the time indicating means with the aid of a rocking bar G04B27/00)}	G04B5/04	G04B5/04		34
G04B5/06	10	acting in one direction only	G04B5/06	G04B5/06		39
G04B5/08	10	acting in both directions	G04B5/08	G04B5/08		63
G04B5/10	9	by oscillating weights the movement of which is not limited	G04B5/10	G04B5/10		19
G04B5/12	10	acting in one direction only	G04B5/12	G04B5/12		36
G04B5/14	10	acting in both directions	G04B5/14	G04B5/14		164
G04B5/16	9	Construction of the weights	G04B5/16	G04B5/16		152
G04B5/165	10	{Weights consisting of several parts (diverse weights which are movable in more than one plane G04B5/187)}	G04B5/16	G04B5/16		80
G04B5/18	9	Supports, suspensions or guide arrangements, for oscillating weights {(transmission of the movement of the winding up weight to the mainspring G04B5/04, G04B5/10; support of the driving weight by protecting means which prevent overwinding, e.g. by interposing of a glide clutch G04B5/24; bearings in general G04B33/00)}	G04B5/18	G04B5/18		77
G04B5/181	10	{The bearing of the rocking bar is in the centre of rotation combined with a support or guide arrangement}	G04B5/18	G04B5/18		45
G04B5/182	10	{Guide arrangement of the moving weight in a straight course}	G04B5/18	G04B5/18		17
G04B5/184	10	{Guide arrangement of the moving weight in a circular course}	G04B5/18	G04B5/18		57
G04B5/185	10	{Suspension of the moving weight by elastic means (G04B5/187 takes precedence)}	G04B5/18	G04B5/18		27
G04B5/187	10	{Bearing, guide arrangements or suspension allowing movement in more than one plane, e.g. there is more than one moving weight, or more than one plane in which the weight moves, and it can change place relative to the clockwork}	G04B5/18	G04B5/18		31
G04B5/188	10	{Bearing, guide arrangements or suspension of the movement forming oscillating weight}	G04B5/18	G04B5/18		27
G04B5/19	10	Suspension of the oscillating weight at its centre of rotation	G04B5/19	G04B5/19		176
G04B5/195	11	{the centre of rotation not being the centre of the clockwork}	G04B5/19	G04B5/19		75
G04B5/20	8	by movements of other objects, e.g. by opening a hand-bag, by opening a case, by opening a door; Winding up by wind power	G04B5/20	G04B5/20		76
G04B5/203	9	{by liquids or gases (driven by liquids or gases G04B1/26; winding up by pneumatic motor G04B3/12; winding up by electrothermal or electropneumatic driving means G04C1/003; driving of the clockwork by such means G04C3/18)}	G04B5/20	G04B5/20		18
G04B5/206	9	{by rotating axles, e.g. tachometers (direct drive of the clockwork, e.g. without winding up of a spring or the like by a rotating axle G04B7/00; combination with measuring instruments in general G04B47/06)}	G04B5/20	G04B5/20		40
G04B5/22	8	by thermometric, barometric or like effects or alterations {(by electrothermal or electropneumatic driving means G04C1/003; driving the clockwork by such means G04C3/18)}	G04B5/22	G04B5/22		48
G04B5/24	8	Protecting means preventing overwinding (arranged in, or attached to, the barrel G04B1/20; in connection with keys or the like G04B3/06; in connection with parts of the cases G04B3/10{; support of the moving weight G04B5/18; protection means G04B9/02; electrical driving means for mechanical clockworks G04C1/10})	G04B5/24	G04B5/24		98
G04B5/245	9	{by locking the moving weight}	G04B5/24	G04B5/24		28
G04B7/00	7	Combined normal and automatic winding up {(normal winding up by hand or mechanically G04B3/00; automatic winding up G04B5/00; electric winding up of mechanical clockworks G04C1/003)}	G04B7/00	G04B7/00		94
G04B9/00	7	Supervision of the state of winding, e.g. indicating the amount of winding	G04B9/00	G04B9/00		228
G04B9/005	8	{by optical indication of the amount of winding}	G04B9/00	G04B9/00		258
G04B9/02	8	Devices controlled by such state, e.g. device affording protection means against overwinding (protecting means preventing overwinding arranged in or on the barrel G04B1/20; protecting means in connection with keys or the like G04B3/06; in connection with parts of the cases G04B3/10; in connection with automatic winding devices G04B5/24{; electric winding up of mechanical clockworks G04C1/10})	G04B9/02	G04B9/02		75
G04B9/025	9	{Acoustical or electrical indicating means}	G04B9/02	G04B9/02		21
G04B11/00	7	Click devices; Stop clicks; Clutches {(mechanisms for winding up by hand G04B3/00; automatic winding up G04B5/00; clutches in general, class 111)}	G04B11/00	G04B11/00		158
G04B11/001	8	{Clutch mechanism between two rotating members with transfer of movement in both directions, possibly with limitation on the transfer of power}	G04B11/00	G04B11/00		55
G04B11/003	9	{with friction member, e.g. with spring action}	G04B11/00	G04B11/00		132
G04B11/005	9	{with magnetic elements}	G04B11/00	G04B11/00		42
G04B11/006	8	{Clutch mechanism between two rotating members with transfer of movement in only one direction (free running devices)}	G04B11/00	G04B11/00		145
G04B11/008	9	{with friction members, e.g. click springs or jumper}	G04B11/00	G04B11/00		83
G04B11/02	8	Devices allowing the motion of a rotatable part in only one direction	G04B11/02	G04B11/02		42
G04B11/022	9	{with a ratchet which makes contact with the rotating member by means of teeth}	G04B11/02	G04B11/02		106
G04B11/024	10	{rotatable about a fixed axis by means of spring action}	G04B11/02	G04B11/02		90
G04B11/026	9	{with clamping member}	G04B11/02	G04B11/02		6
G04B11/028	9	{with friction member, e.g. click spring}	G04B11/02	G04B11/02		31
G04B11/04	9	Pawl constructions therefor, e.g. pawl secured to an oscillating member actuating a ratchet	G04B11/04	G04B11/04		279
G04B13/00	7	Gearwork {(gearwork for driving the hands G04B19/02; calibers G04B33/00; dispositions and components for transmission in general F16H)}	G04B13/00	G04B13/00		350
G04B13/001	8	{with the choice of adjustable or varying transmission ratio}	G04B13/00	G04B13/00		80
G04B13/002	8	{where rotation in one direction is changed into a stepping movement}	G04B13/00	G04B13/00		136
G04B13/003	9	{with a step for each complete revolution (counters in general H03K)}	G04B13/00	G04B13/00		48
G04B13/005	8	{where a revolution in both directions is changed into a revolution in one direction}	G04B13/00	G04B13/00		24
G04B13/006	9	{with two free wheel positions}	G04B13/00	G04B13/00		6
G04B13/007	8	{with differential work}	G04B13/00	G04B13/00		59
G04B13/008	9	{Differentials}	G04B13/00	G04B13/00		80
G04B13/02	8	Wheels; Pinions; Spindles; Pivots (bearings G04B31/00{; chain wheels, spindles for chain wheels, also chains and driving weights G04B1/08})	G04B13/02	G04B13/02		777
G04B13/021	9	{elastic fitting with a spindle, axis or shaft}	G04B13/02	G04B13/02		131
G04B13/022	10	{with parts made of hard material, e.g. silicon, diamond, sapphire, quartz and the like}	G04B13/02	G04B13/02		144
G04B13/023	10	{allowing rotational slipping when a threshold torque is exceeded}	G04B13/02	G04B13/02		61
G04B13/025	9	{with elastic means between the toothing and the hub of a toothed wheel}	G04B13/02	G04B13/02		74
G04B13/027	9	{planar toothing: shape and design (adjusting the backlash of the arbors G04B35/00)}	G04B13/02	G04B13/02		145
G04B13/028	9	{wheels in which the teeth are conic, contrate, etc; also column wheels construction (start-stop mechanisms with column wheels G04F7/0847)}	G04B13/02	G04B13/02		72
G04B15/00	7	Escapements ({in striking mechanisms G04B21/06;} electric or magnetic means for converting oscillatory to rotary motion in electromechanical time-pieces {G04C5/005})	G04B15/00	G04B15/00		240
G04B15/02	8	permanently in contact with the regulating mechanism	G04B15/02	G04B15/02		164
G04B15/04	9	Cylinder escapements	G04B15/04	G04B15/04		50
G04B15/06	8	Free escapements	G04B15/06	G04B15/06		331
G04B15/08	9	Lever escapements	G04B15/08	G04B15/08		600
G04B15/10	8	with constant impulses for the regulating mechanism {(electrically driven pendulums with mechanical pulse transmission and constant pulse G04C3/022; electrically driven pendulums with mechanical pulse transmission and constant pulse G04C3/045)}	G04B15/10	G04B15/10		215
G04B15/12	8	Adjusting (tools therefor G04D1/02); Restricting the amplitude of the lever or the like {(adjusting the gear train G04B35/00)}	G04B15/12	G04B15/12		262
G04B15/14	8	Component parts or constructional details, e.g. construction of the lever or the escape wheel {(assembly and manufacture of the spring G04B1/145; assembly and manufacture of components, e.g. pinions, spindles G04B13/02; lubrication of clockwork bearings G04B31/008; oils for clockwork bearings in general G04B31/08)}	G04B15/14	G04B15/14		1175
G04B17/00	7	Mechanisms for stabilising frequency {(for setting frequency G04B18/00; magnetic G04C5/005; in striking mechanisms G04B21/06; stopping and regulating of the running G04B23/023; electrically driven mechanical regulation G04C3/165; electrical and thermo-electric regulating mechanisms G04C5/00)}	G04B17/00	G04B17/00		111
G04B17/005	8	{Regulating mechanisms where the movement is maintained by pneumatic means (oscillation generation by pneumatic means G04F5/12)}	G04B17/00	G04B17/00		34
G04B17/02	8	Oscillators acting by gravity, e.g. pendulum swinging in a plane {(setting the pendulum to the required length G04B18/003; temperature compensation for pendulums G04B17/225; bearings in general, e.g. knife-edge G04B31/00; clocks fitted in pendulums G04B45/043; imitation pendulums driven by the clock mechanism G04B45/0046, G04B45/0053; pendulum ornamentation G04B45/0061; contacts actuated by a pendulum G04C13/065; measurement of force with a pendulum G01V7/12)}	G04B17/02	G04B17/02		206
G04B17/025	9	{Composite and multiple pendulums; Synchronisation of mechanical pendulums, e.g. electrical synchronisation G04C3/025; pendulum systems G04C13/028}	G04B17/02	G04B17/02		36
G04B17/04	8	Oscillators acting by spring tension	G04B17/04	G04B17/04		171
G04B17/045	9	{with oscillating blade springs (mechanical oscillations maintained by electro-magnetic means, e.g. tuning forks G04C3/10)}	G04B17/04	G04B17/04		339
G04B17/06	9	Oscillators with hairsprings, e.g. balance {(electrically driven balances G04C3/04; contacts actuated by a balance G04C13/065)}	G04B17/06	G04B17/06		425
G04B17/063	10	{Balance construction (balances with frequency adjustment screw G04B18/006; balances with temperature compensation G04B17/222; balancing devices G04B17/28)}	G04B17/06	G04B17/06		530
G04B17/066	10	{Manufacture of the spiral spring (locking of the spiral spring by the regulating lever G04B18/026; spiral spring with temperature compensation G04B17/227; fixation of the spiral spring on the collet G04B17/32; mainspring G04B1/14)}	G04B17/06	G04B17/06		502
G04B17/08	9	Oscillators with coil springs stretched and unstretched axially	G04B17/08	G04B17/08		24
G04B17/10	9	Oscillators with torsion strips or springs acting in the same manner as torsion strips, e.g. weight oscillating in a horizontal plane {(electrically driven torsion pendulum G04C3/033)}	G04B17/10	G04B17/10		158
G04B17/20	8	Compensation of mechanisms for stabilising frequency	G04B17/20	G04B17/20		149
G04B17/22	9	for the effect of variations of temperature {(alloys with small expansion coefficient C21C, C22C; adjustment of the regulator dependant on adjustment of the hands G04B18/028; depending on the difference in time with a comparison clockwork G04C11/007)}	G04B17/22	G04B17/22		140
G04B17/222	10	{with balances (construction of balances G04B17/063)}	G04B17/22	G04B17/22		153
G04B17/225	10	{with pendulums (construction of pendulums G04B17/02; setting frequency on the pendulum G04B18/003)}	G04B17/22	G04B17/22		75
G04B17/227	10	{composition and manufacture of the material used (composition and manufacture of hairsprings G04B17/066; of springs G04B1/145; anti-magnetic alloys G04B43/007; ferrous alloys C22C; non-ferrous alloys C22C, B22F)}	G04B17/22	G04B17/22		193
G04B17/24	9	for the effect of variations of atmospheric pressure	G04B17/24	G04B17/24		24
G04B17/26	9	for the effect of variations of the impulses	G04B17/26	G04B17/26		159
G04B17/28	9	for the effect of imbalance of the weights, e.g. tourbillon	G04B17/28	G04B17/28		148
G04B17/285	10	{Tourbillons or carrousels}	G04B17/28	G04B17/28		439
G04B17/30	8	Rotating governors, e.g. centrifugal governors, fan governors (for striking mechanism G04B21/06{; electrically driven G04C3/0335})	G04B17/30	G04B17/30		70
G04B17/32	8	Component parts or constructional details, e.g. collet, stud {, virole or piton}	G04B17/32	G04B17/32		408
G04B17/325	9	{for fastening the hairspring in a fixed position, e.g. using a block}	G04B17/32	G04B17/32		278
G04B17/34	9	for fastening the hairspring onto the balance	G04B17/34	G04B17/34		116
G04B17/345	10	{Details of the spiral roll}	G04B17/34	G04B17/34		242
G04B18/00	7	Mechanisms for setting frequency {(for stabilising frequency G04B17/00)}	G04B18/00	G04B18/00		99
G04B18/003	8	{by displacement of devices carried by the pendulum or by adjusting the pendulum length (pendulums and suspension G04B17/02; self- adjustment of the regulating lever G04B18/028, G04B17/22, G04C11/007; adjusting the stroke of the pendulum G04B18/04; time indicating by acoustic means G04B21/00; synchronisation with a standard clock G04C11/007; metronome with a variable length G04F5/027)}	G04B18/00	G04B18/00		71
G04B18/006	8	{by adjusting the devices fixed on the balance (construction of the pendulum G04B17/063; balancing G04B17/28)}	G04B18/00	G04B18/00		204
G04B18/02	8	Regulator {or adjustment} devices; Indexing devices {, e.g. raquettes}	G04B18/02	G04B18/02		388
G04B18/021	9	{adjusting the indexing device from the outside}	G04B18/02	G04B18/02		130
G04B18/023	9	{with means for fine adjustment of the indexing device}	G04B18/02	G04B18/02		314
G04B18/025	9	{Fixing of the indexing device}	G04B18/02	G04B18/02		159
G04B18/026	9	{Locking the hair spring in the indexing device, e.g. goupille of the raquette (hairsprings G04B17/066; locking the mainspring on the axle G04B1/18)}	G04B18/02	G04B18/02		256
G04B18/028	9	{Setting the regulator by means coupled to or depending on another device, e.g. by the time indication setting mechanism (automatic adjustment of the pendulum length G04B17/225, G04B18/003, G04C11/007; automatic adjustment of the regulator for temperature compensation G04B17/22; automatic adjustment of the regulator dependant on the tension of the mainspring G04B1/22)}	G04B18/02	G04B18/02		120
G04B18/04	8	Adjusting the beat of the pendulum, balance, or the like, e.g. putting into beat	G04B18/04	G04B18/04		176
G04B18/06	9	by setting the collet or the stud of a hairspring	G04B18/06	G04B18/06		149
G04B18/08	8	Component parts or constructional details {(G04B17/32 takes precedence)}	G04B18/08	G04B18/08		38
G04B19/00	7	Indicating the time by visual means ({indicating the time optically by electric means G04C17/00, e.g.} by electric lamps G04C17/02; display arrangements in general G09F)	G04B19/00	G04B19/00		395
G04B19/02	8	Back-gearing arrangements between gear train and hands {(transmissions in general G04B13/00)}	G04B19/02	G04B19/02		768
G04B19/025	9	{for simultaneous indicating on several dials (indicating means allowing simultaneous indication G04B19/048; with several separate dials G04B19/08; extra hands for indicating different local apparent times G04B19/23; with several clockworks G04B37/0083)}	G04B19/02	G04B19/02		141
G04B19/04	8	Hands; Discs with a single mark or the like {(moving indicating arrangements which have scales or numbers with stationary hands or reading means G04B19/20; optical projection of the position of the hands G04B19/34)}	G04B19/04	G04B19/04		518
G04B19/042	9	{Construction and manufacture of the hands; arrangements for increasing reading accuracy (hands with illumination G04B19/305; specially shaped hands, e.g. figures or pictures G04B45/0061; clockwork in the hands G04B45/043; invisible drive of the hands G04B45/046)}	G04B19/04	G04B19/04		486
G04B19/044	9	{Mounting and setting of the hands on the axle}	G04B19/04	G04B19/04		157
G04B19/046	9	{Indicating by means of a disc with a mark or window (for simultaneous indicating G04B19/048)}	G04B19/04	G04B19/04		240
G04B19/048	9	{having the possibility of indicating on more than one scale, e.g. hands with variable length which work on different scales (simultaneous indicating on several dials G04B19/025; indicating by discs used as hands G04B19/046; used as moving scales G04B19/202; different indications on several scales or dials, e.g. for different local apparent times G04B19/23)}	G04B19/04	G04B19/04		125
G04B19/06	8	Dials ({moving discs G04B19/20; illuminated dials or hands G04B19/30;} for time-pieces without clockwork G04B49/04{; machines and arrangements for the manufacture of dials or hands G04D3/0048})	G04B19/06	G04B19/06		648
G04B19/065	9	{with several parts}	G04B19/06	G04B19/06		260
G04B19/08	9	Geometrical arrangement of the graduations	G04B19/08	G04B19/08		177
G04B19/082	10	{varying from the normal closed scale}	G04B19/08	G04B19/08		283
G04B19/085	10	{varying from the normal 12 hour arrangement}	G04B19/08	G04B19/08		221
G04B19/087	10	{with several separate scales (for indicating the same or different times of the clockwork; indicating devices making several simultaneous indications possible G04B19/048)}	G04B19/08	G04B19/08		140
G04B19/10	9	Ornamental shape of the graduations or the surface of the dial; Attachment of the graduations to the dial {(cases for special purposes, e.g. ring or button watches G04B37/12; indicating means with special effects G04B45/00)}	G04B19/10	G04B19/10		843
G04B19/103	10	{attached or inlaid numbers (attaching of jewels or ornaments G04B47/042; arrangements for attaching bearing jewels, or the like G04D3/04)}	G04B19/10	G04B19/10		322
G04B19/106	10	{Special number markings}	G04B19/10	G04B19/10		88
G04B19/12	9	Selection of materials for dials or graduations {markings}	G04B19/12	G04B19/12		811
G04B19/14	9	Fastening the dials to the clock or watch plates {(tools, arrangements and machines for the manufacture of watch plates G04D3/0048)}	G04B19/14	G04B19/14		491
G04B19/16	9	Shiftable dials, e.g. indicating alternately from 1 to 12 and from 13 to 24 {(dials with a scale other than the normal 12 hour scale G04B19/085)}	G04B19/16	G04B19/16		163
G04B19/163	10	{numbers which are visible alternately from 1 to 12 and from 13 to 24 on the same dial G04B19/085}	G04B19/16	G04B19/16		198
G04B19/166	10	{with rotating scales}	G04B19/16	G04B19/16		107
G04B19/18	9	Graduations on the crystal or glass, on the bezel, or on the rim	G04B19/18	G04B19/18		269
G04B19/20	8	Indicating by numbered bands, drums, discs, or sheets {(indicating means without numbers or hands in general G04B19/04; illuminated G04B19/30; with optical projection G04B19/34; gearwork and linking in general G04B13/00; electrically driven G04C19/04; counter mechanisms G06M)}	G04B19/20	G04B19/20		206
G04B19/202	9	{by means of turning discs (disc-shaped indicating devices with a reference mark or a window G04B19/046; discs driven by clockwork and producing optical special effects G04B45/0007; with inscriptions or drawings driven by a clockwork G04B45/0023; with figures or parts of figures driven by clockwork G04B45/0038)}	G04B19/20	G04B19/20		499
G04B19/205	9	{by means of sheets}	G04B19/20	G04B19/20		101
G04B19/207	9	{by means of bands (bands as time indicating means with a reference mark or window G04B19/04)}	G04B19/20	G04B19/20		116
G04B19/21	9	Drums {(drum-shaped or spatial indicating devices G04B19/04; fixed scales or dials G04B19/06; scales disposed on a terrestrial globe for indicating local times in different places G04B19/22; clockwork combined with a lamp with no functional relationship G04B47/02)}	G04B19/21	G04B19/21		302
G04B19/22	8	Arrangements for indicating different local apparent times; Universal time pieces {(indicating by means of numbers or signs disposed on moving devices G04B19/20; illumination of dials or hands G04B19/30; combination with a terrestial globe in general G04B47/02; electronic time-zone watches G04G9/0076)}	G04B19/22	G04B19/22		213
G04B19/221	9	{mechanisms for correcting the hours hand only, i.e. independently for minutes and seconds hands}	G04B19/22	G04B19/22		81
G04B19/223	9	{with rotary disc, rotary bezel, or rotary dial}	G04B19/22	G04B19/22		517
G04B19/225	10	{driving mechanism for the bezel}	G04B19/22	G04B19/22		22
G04B19/226	9	{three-dimensionally shaped, e.g. terrestrial globes, cylinders and the like}	G04B19/22	G04B19/22		231
G04B19/228	9	{with linear time graduation}	G04B19/22	G04B19/22		48
G04B19/23	9	by means of additional hands or additional pairs of hands {(simultaneous indication on several dials G04B19/025; indicating devices giving several simultaneous indications G04B19/048)}	G04B19/23	G04B19/23		292
G04B19/235	10	{mechanisms for correcting the additional hand or hands (time setting G04B27/00)}	G04B19/23	G04B19/23		151
G04B19/24	8	Clocks or watches with date {or week-day} indicators {, i.e. calendar clocks or watches}; Clockwork calendars	G04B19/24	G04B19/24		501
G04B19/241	9	{the date is indicated by one or more hands}	G04B19/24	G04B19/24		213
G04B19/243	9	characterised by the shape of the date indicator	G04B19/243	G04B19/243		31
G04B19/24306	10	{combination of different shapes, e.g. bands and discs, discs and drums (for electrically driven timepieces G04C17/0041)}	G04B19/243	G04B19/243		9
G04B19/24313	11	{Independent date indicating devices activated by hand or by clockwork}	G04B19/243	G04B19/243		18
G04B19/2432	11	{Driving or releasing mechanisms wherein the date indicators are driven or released mechanically by a clockwork movement}	G04B19/243	G04B19/243		8
G04B19/24326	12	{driven or released stepwise by the clockwork movement}	G04B19/243	G04B19/243		30
G04B19/24333	12	{driven or released stepwise by an energy source which is released at determined moments by the clockwork movement}	G04B19/243	G04B19/243		36
G04B19/2434	12	{driven or released by their own energy source which is released at regular time intervals}	G04B19/243	G04B19/243		15
G04B19/24346	10	{band-shaped (G04B19/24306 takes precedence; for electrically driven timepieces G04C17/0016)}	G04B19/243	G04B19/243		7
G04B19/24353	11	{Independent date indicating devices activated by hand or by clockwork}	G04B19/243	G04B19/243		6
G04B19/2436	11	{Driving or releasing mechanisms wherein the date indicators are driven or released mechanically by a clockwork movement}	G04B19/243	G04B19/243		6
G04B19/24366	12	{driven or released stepwise by the clockwork movement}	G04B19/243	G04B19/243		27
G04B19/24373	12	{driven or released stepwise by an energy source which is released at determined moments by the clockwork movement}	G04B19/243	G04B19/243		18
G04B19/2438	12	{driven or released by their own energy source which is released at regular time intervals}	G04B19/243	G04B19/243		26
G04B19/24386	10	{sheet-shaped (G04B19/24306 takes precedence; flap-shaped for electrically driven timepieces G04C17/0033)}	G04B19/243	G04B19/243		32
G04B19/24393	11	{Driving or releasing mechanisms wherein the date indicators are driven or released mechanically by a clockwork movement}	G04B19/243	G04B19/243		26
G04B19/247	10	disc-shaped {(G04B19/24306 takes precedence; for electrically driven timepieces G04C17/0058)}	G04B19/247	G04B19/247		389
G04B19/25	11	Devices for setting the date indicators manually	G04B19/25	G04B19/25		436
G04B19/253	11	Driving or releasing mechanisms	G04B19/253	G04B19/253		117
G04B19/25306	12	{Independent date indicating devices activated by hand or by clockwork, e.g. calendar watches}	G04B19/253	G04B19/253		59
G04B19/25313	13	{driven or released by a steady movement}	G04B19/253	G04B19/253		11
G04B19/2532	14	{automatically corrected at the end of mounths having less than 31 days}	G04B19/253	G04B19/253		42
G04B19/25326	14	{manually corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		16
G04B19/25333	12	{wherein the date indicators are driven or released mechanically by a clockwork movement}	G04B19/253	G04B19/253		54
G04B19/2534	13	{driven or released continuously by the clockwork movement}	G04B19/253	G04B19/253		31
G04B19/25346	14	{manually corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		13
G04B19/25353	13	{driven or released stepwise by the clockwork movement}	G04B19/253	G04B19/253		205
G04B19/2536	14	{automatically corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		211
G04B19/25366	14	{manually corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		145
G04B19/25373	13	{driven or released stepwise by an energy source which is released at determined moments by the clockwork movement}	G04B19/253	G04B19/253		156
G04B19/2538	14	{automatically corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		101
G04B19/25386	14	{manually corrected at the end of months having less than 31 days}	G04B19/253	G04B19/253		64
G04B19/25393	13	{driven or released by their own energy source which is released at regular time intervals}	G04B19/253	G04B19/253		21
G04B19/257	10	drum-shaped {or three-dimensional shaped (G04B19/24306 takes precedence; for electrically driven timepieces G04C17/0083)}	G04B19/257	G04B19/257		20
G04B19/2571	11	{Independent date indicators activated by hand or by clockwork}	G04B19/257	G04B19/257		12
G04B19/2573	11	{Driving or releasing mechanisms wherein the date indicators are driven or released mechanically by a clockwork movement}	G04B19/257	G04B19/257		13
G04B19/2575	12	{driven or released stepwise by the clockwork movement}	G04B19/257	G04B19/257		27
G04B19/2576	12	{driven or released stepwise by an energy source which is released at determined moments by the clockwork movement}	G04B19/257	G04B19/257		20
G04B19/2578	12	{driven or released by their own energy source which is released at regular time intervals}	G04B19/257	G04B19/257		9
G04B19/26	8	Clocks or watches with indicators for tides, for the phases of the moon, or the like {(planetaria G09B27/00&#160;-&#160;G09B27/06; arrangements for table reference, e.g. menstrual tables G06C3/00)}	G04B19/26	G04B19/26		305
G04B19/262	9	{with indicators for astrological informations}	G04B19/26	G04B19/26		195
G04B19/264	9	{with indicators for biological cycles}	G04B19/26	G04B19/26		113
G04B19/266	9	{with indicators for tides}	G04B19/26	G04B19/26		97
G04B19/268	9	{with indicators for the phases of the moon}	G04B19/26	G04B19/26		364
G04B19/28	8	Adjustable guide marks or pointers for indicating determined points of time {(inscriptions or pictures moved by hand G04B45/003)}	G04B19/28	G04B19/28		263
G04B19/283	9	{on rotatable rings, i.e. bezel (for graduations on the bezels G04B19/18)}	G04B19/28	G04B19/28		519
G04B19/286	10	{with locking means to prevent undesired rotations in both directions}	G04B19/28	G04B19/28		102
G04B19/30	8	Illumination of dials or hands {(dials in general G04B19/06; moving indicating means with numbers or hands, in general G04B19/20; arrangements for indicating different local apparent times by means of a globe illuminated from inside G04B19/22; continuous indication of the time by non-electric light sources G04B25/00, e.g. by electric lamps G04C17/02; illumination by electric lamps which function at fixed times or periodically G04C19/02; illuminated panels G09F13/00)}	G04B19/30	G04B19/30		890
G04B19/305	9	{the hands carrying the light source (hands and manufacture thereof G04B19/042; projection of hands or dials G04B19/34; illumination of scales and/or hands on moving scales H03J1/02; on compasses G01C17/24; on weighing apparatus G01G23/18; on measuring instruments G01D11/28)}	G04B19/30	G04B19/30		126
G04B19/32	9	by luminescent substances {(disc or drum shaped indicating means with marks or windows G04B19/04; with numbers or number-marks G04B19/20; cases for housing the electrical parts G04G17/00; projection of hands and/or scales on weighing apparatus G01G19/00; on measuring instruments G01D5/262; for advertising G09F19/18)}	G04B19/32	G04B19/32		527
G04B19/34	8	Position of the hands projected optically {(for advertising G09F19/18; indicating by discs or drums with mark or window G04B19/04, with figures or signs G04B19/20; illumination of dials or hands G04B19/30, case for electrical components G04C3/008; optical projection of a pointer and/or scale for weighing apparatus G01G23/32; for measuring instruments G01D5/262)}	G04B19/34	G04B19/34		190
G04B21/00	7	Indicating the time by acoustic means (at preselected times G04B23/00; by electro-acoustic means G04C21/04; {indicating the time by means other than acoustically, or by combined means G04B25/00; indicating the time by visual means G04B19/00, G04C17/00; acoustic signalling arrangements G08B3/00})	G04B21/00	G04B21/00		226
G04B21/005	8	{Periodical acoustic signalling arrangements (G04B21/02 takes precedence); (adjustment of the frequencyby setting the length of the pendulum G04B18/003; metronomes G04F5/02)}	G04B21/00	G04B21/00		79
G04B21/02	8	Regular striking mechanisms giving the full hour, half hour or quarter hour {(electrically operating striking mechanism G04C21/06)}	G04B21/02	G04B21/02		209
G04B21/022	9	{with saw mechanism (with electric drive G04C21/08)}	G04B21/02	G04B21/02		144
G04B21/025	10	{with silent saw action}	G04B21/02	G04B21/02		11
G04B21/027	9	{with locking wheel (electrically driven G04C21/10)}	G04B21/02	G04B21/02		77
G04B21/04	9	Hour wheels; Racks or rakes; Snails or similar control mechanisms	G04B21/04	G04B21/04		89
G04B21/06	9	Details of striking mechanisms, e.g. hammer, fan governor {(escapements in general G04B15/00; mechanisms for stabilising frequency G04B17/00; resistance regulators G05D13/00; mechanical toys A63H)}	G04B21/06	G04B21/06		239
G04B21/08	9	Sounding bodies; Whistles; Musical apparatus (with electro-acoustical transmitters G04C21/00, {G04B23/08; sounding arrangements in alarm clocks G04B23/028; cases with arrangements for enhancing sound production G04B37/0075; carillons and sounding boards G10F1/08, G04B1/10, G10D13/08})	G04B21/08	G04B21/08		495
G04B21/10	9	Releasing or locking the regular stroke, e.g. for silence during the night	G04B21/10	G04B21/10		95
G04B21/12	9	Reiterating watches or clocks	G04B21/12	G04B21/12		453
G04B21/14	9	Winding-up the striking mechanism by the clockwork; winding up the clockwork by the striking mechanism {(winding up by hand or mechanically G04B3/00)}	G04B21/14	G04B21/14		55
G04B23/00	7	Arrangements producing acoustic signals at preselected times {(indicating the time by optical means G04B19/00, G04C17/00; indicating the time by acoustic means G04B21/00; indicating the time by means other than acoustic or optical, or by a combination of means G04B25/00; acoustic time signals produced electrically G04C21/00; coin-freed alarm clocks G07F17/0007; acoustic signalling means G08B3/00)}	G04B23/00	G04B23/00		127
G04B23/005	8	{by starting up musical boxes or other musical recordings (starting up and stopping of phonographs by means of clockwork apparatus G11B33/06)}	G04B23/00	G04B23/00		105
G04B23/02	8	Alarm clocks {(by other means&#160;G04B25/005; waking up by electric lamps&#160;G04C19/02; electrically released alarm signals&#160;G04C21/00; alarm clocks with electric contacts&#160;G04C23/06)}	G04B23/02	G04B23/02		337
G04B23/021	9	{Controls (winding up the alarm; adjusting and indicating the waking time)}	G04B23/02	G04B23/02		274
G04B23/023	9	{Driving, e.g. by springs or common drive with the clockwork; gears; escapements (escapements in general G04B15/00; regulating means for clockworks in general G04B17/00)}	G04B23/02	G04B23/02		91
G04B23/025	9	{Signal triggering (in alarm clocks which deliver also or only non-acoustic signals G04B25/005)}	G04B23/02	G04B23/02		95
G04B23/026	9	{Hammer driving; hammers; devices with several hammers or sounding bodies; vibrators}	G04B23/02	G04B23/02		127
G04B23/028	9	{Sounding bodies; boxes used as sounding cases; fixation on or in the case (sounding bodies G04B21/08; case enhancing transmission of sound waves G04B37/0075)}	G04B23/02	G04B23/02		195
G04B23/03	9	Alarm signal stop arrangements	G04B23/03	G04B23/03		407
G04B23/04	9	with coarse and fine setting of the preselected times	G04B23/04	G04B23/04		68
G04B23/06	9	adjustable for several preselected times with automatic stopping of the signal	G04B23/06	G04B23/06		150
G04B23/08	9	operating on successive days without resetting; operating only once in each 24 hours	G04B23/08	G04B23/08		161
G04B23/10	9	with presignal; with repeated signal; with changeable intensity of sound	G04B23/10	G04B23/10		280
G04B23/12	9	Alarm watches to be worn in pockets or on the wrist (giving signals by stimulating the skin G04B25/04)	G04B23/12	G04B23/12		362
G04B25/00	7	Indicating the time by other means or by combined means (electric or electromechanical indicating G04C{; illumination of dials or hands G04B19/30; indicating the time by acoustic means G04B21/00; arrangements producing acoustic signals at preselected times G04B23/00; continuously indicating the time optically by electric means G04C19/00; producing acoustic time signals by electrical means G04C21/00; devices for cooking eggs A47J29/00})	G04B25/00	G04B25/00		71
G04B25/005	8	{in alarm clocks (G04B25/04 takes precedence)}	G04B25/00	G04B25/00		168
G04B25/02	8	by feeling; Clocks or watches for blind persons	G04B25/02	G04B25/02		134
G04B25/04	9	Alarm clocks or watches with devices stimulating the skin {(normal pocket or wrist alarm clocks G04B23/12)}	G04B25/04	G04B25/04		226
G04B25/06	8	by moving figures, e.g. cuckoo clocks, trumpet clocks {(figures or part of figures set in motion by the clockwork and creating an optical special effect G04B45/0007; figures or parts of figures not used to indicate time G04B45/0038; clockworks driving inscriptions or figures G04B45/0023; time indication by means of plates or bands driven electrically G04C19/04)}	G04B25/06	G04B25/06		298
G04B27/00	7	Mechanical devices for setting the time indicating means	G04B27/00	G04B27/00		338
G04B27/001	8	{Internal gear therefor, e.g. for setting the second hand or for setting several clockworks}	G04B27/00	G04B27/00		158
G04B27/002	8	{The setting apparatus being crown shaped (G04B27/02 takes precedence)}	G04B27/00	G04B27/00		84
G04B27/004	8	{having several simultaneous functions, e.g. stopping or starting the clockwork or the hands (G04B27/02 takes precedence)}	G04B27/00	G04B27/00		201
G04B27/005	8	{stepwise or on determined values (G04B27/02 takes precedence)}	G04B27/00	G04B27/00		208
G04B27/007	8	{otherwise than manually (G04B27/02 takes precedence; oscillator weights in general G04B5/04)}	G04B27/00	G04B27/00		61
G04B27/008	8	{with parts which are put together with the winding parts, but are functionally separate from them}	G04B27/00	G04B27/00		20
G04B27/02	8	by making use of the winding means {(winding by hand or mechanically G04B3/00)}	G04B27/02	G04B27/02		277
G04B27/023	9	{changing of the winding position to the setting position and vice versa is done with an independant part of the winding or setting mechanism (G04B27/045 and G04B27/065 take precedence; by part of the case G04B27/086)}	G04B27/02	G04B27/02		54
G04B27/026	9	{for several clockworks or pairs of hands and/or supplementary functions}	G04B27/02	G04B27/02		141
G04B27/04	9	with clutch wheel {(support and displacement of the winding stem through the case, means for preventing the stem from going too far, fixation G04B37/06)}	G04B27/04	G04B27/04		495
G04B27/045	10	{Changing the winding position to the setting position and vice versa is done with an independant part of the winding or setting mechanism}	G04B27/04	G04B27/04		127
G04B27/06	9	with rocking bar {(support and displacement of the winding stem through the case, means preventing the stem from going too far, fixation G04B37/06)}	G04B27/06	G04B27/06		288
G04B27/065	10	{Changing the winding position to the setting position and vice versa is done with an independant part of the winding or setting mechanism}	G04B27/06	G04B27/06		111
G04B27/08	8	by using parts of the case {(winding by using parts of the case G04B3/08)}	G04B27/08	G04B27/08		92
G04B27/083	9	{which may be used for winding when changed form the normal position}	G04B27/08	G04B27/08		55
G04B27/086	9	{which, after displacing a supplementary part, may be used for winding (similar devices G04B27/023; in mechanisms with coupled pinions G04B27/045; in rocking mechanisms G04B27/065)}	G04B27/08	G04B27/08		56
G04B29/00	7	Frameworks	G04B29/00	G04B29/00		322
G04B29/02	8	Plates; Bridges; Cocks	G04B29/02	G04B29/02		216
G04B29/022	9	{Bridges}	G04B29/02	G04B29/02		99
G04B29/025	9	{Cocks}	G04B29/02	G04B29/02		55
G04B29/027	9	{Materials and manufacturing (alloys, in general C22C)}	G04B29/02	G04B29/02		237
G04B29/04	8	Connecting or supporting parts	G04B29/04	G04B29/04		241
G04B31/00	7	Bearings; Point suspensions or counter-point suspensions; Pivot bearings; Single parts therefor (bearings in general F16C{; manufacture and composition of springs G04B1/145; suspension of oscillating weights G04B5/18; suspension of a pendulum G04B17/02; bearings for electrical measurement apparatus G01R1/10, G01R1/12, G01R11/12, G01R11/14; inserting jewels A44C17/04; inserting cutting diamonds B23P5/00; devices for fixation of bearing jewels, bearing sleeves, or the like G04D3/04})	G04B31/00	G04B31/00		318
G04B31/004	8	characterised by the material used	G04B31/004	G04B31/004		96
G04B31/008	9	Jewel bearings (G04B31/04 takes precedence)	G04B31/008	G04B31/008		83
G04B31/0082	10	{with jewel hole and cap jewel (shock damping bearings with jewel hole and cap jewel G04B31/04)}	G04B31/008	G04B31/008		95
G04B31/0085	10	{with cap jewel only}	G04B31/008	G04B31/008		19
G04B31/0087	10	{with jewel hole only}	G04B31/008	G04B31/008		59
G04B31/012	9	Metallic bearings	G04B31/012	G04B31/012		62
G04B31/0123	10	{with metallic ball bearings and metallic roller bearings}	G04B31/012	G04B31/012		105
G04B31/0126	10	{Metallic step-bearings}	G04B31/012	G04B31/012		35
G04B31/016	9	Plastic bearings	G04B31/016	G04B31/016		93
G04B31/02	8	Shock-damping bearings {(shock damping in the case G04B37/052, G04B37/055, G04B37/0418)}	G04B31/02	G04B31/02		403
G04B31/04	9	with jewel hole and cap jewel {(jewel bearings with jewel hole and cap jewel G04B31/0082; tools for inserting jewel bearings G04D3/042)}	G04B31/04	G04B31/04		502
G04B31/06	8	Manufacture or mounting processes	G04B31/06	G04B31/06		210
G04B31/08	8	Lubrication {(self-lubricated plastic bearings G04B31/016; lubrication of the escape wheel G04B15/14; lubrication of synchronous clockworks G04C15/009; lubrication devices and lubricant containers G04D5/00)}	G04B31/08	G04B31/08		314
G04B33/00	7	Calibers {(disposition of components of the automatic winding mechanism in relation to the clockwork G04B5/18)}	G04B33/00	G04B33/00		204
G04B33/02	8	Circular calibers	G04B33/02	G04B33/02		225
G04B33/04	8	Non-circular calibers	G04B33/04	G04B33/04		121
G04B33/06	8	of extremely flat shape	G04B33/06	G04B33/06		95
G04B33/08	8	in which the gear train is arranged in different planes, e.g. parallel or inclined to each other (G04B33/10 takes precedence {case for special purposes, e.g. button or ring clockworks G04B37/12})	G04B33/08	G04B33/08		70
G04B33/10	8	with seconds hand arranged in the centre of the dial	G04B33/10	G04B33/10		250
G04B33/12	8	for extremely long running times	G04B33/12	G04B33/12		125
G04B33/14	8	Calibers of which the mainsprings or barrels are easily removable (mainsprings G04B1/14; barrels, arbors G04B1/16{; normal or mechanical winding G04B3/00})	G04B33/14	G04B33/14		153
G04B33/16	8	with arrangements affording protection of the clockwork against damage as a consequence of a rupture of the mainspring {(protection devices against the rupture of the mainspring or its over-tension, placed in the spring-drum or fixed on it against rupture if the mainspring is wound too far G04B1/20)}	G04B33/16	G04B33/16		3
G04B35/00	7	Adjusting the gear train, e.g. the backlash of the arbors, depth of meshing of the gears {(adjusting the escapement G04B15/12)}	G04B35/00	G04B35/00		245
G04B37/00	7	Cases {(cases with a special shape G04B45/0069; ornamentation of the case G04B47/04; cartridges A45C11/00&#160;-&#160;A45C11/38)}	G04B37/00	G04B37/00		360
G04B37/0008	8	{for pocket watches and wrist watches}	G04B37/00	G04B37/00		932
G04B37/0016	9	{with folding cover or folding bottom (hinge without spring)}	G04B37/00	G04B37/00		213
G04B37/0025	9	{with cover or bottom with a spring (savonette) bench watches opening or closing with spring action G04B37/0463}	G04B37/00	G04B37/00		241
G04B37/0033	9	{with cover or bottom which can slide or turn (without a spring action)}	G04B37/00	G04B37/00		127
G04B37/0041	9	{the cover or the bottom can slide or turn with a spring action}	G04B37/00	G04B37/00		88
G04B37/005	9	{with cover or protection device which can be completely removed, either by lifting off or by sliding, or by turning (protection covers, protection cases also against humidity)}	G04B37/00	G04B37/00		296
G04B37/0058	9	{for shaped watches}	G04B37/00	G04B37/00		246
G04B37/0066	8	{for wall clocks and balances (feet and stands for clocks G04B37/1473)}	G04B37/00	G04B37/00		411
G04B37/0075	8	{with means to enhance sound transmission (sonorous means for chimes G04B21/08; for alarm clocks G04B23/028; clockworks combined with musical devices G04B47/025)}	G04B37/00	G04B37/00		122
G04B37/0083	8	{for more than one clockwork}	G04B37/00	G04B37/00		119
G04B37/0091	8	{for clock parts, e.g. for the escapement or the electric motor (protection cases and air tight vacuum means for clockwork parts G04B37/088)}	G04B37/00	G04B37/00		40
G04B37/02	8	Evacuated cases; Cases filled with gas or liquids; Cases containing substances for absorbing or binding moisture or dust	G04B37/02	G04B37/02		187
G04B37/04	8	Mounting the clockwork in the case; Shock absorbing mountings	G04B37/04	G04B37/04		284
G04B37/0409	9	{Fixed mounting relating to wall clocks and pendulums}	G04B37/04	G04B37/04		186
G04B37/0418	10	{with shock damping means (shock damping bearings G04B31/02; protection against shocks with shields G04B43/002)}	G04B37/04	G04B37/04		44
G04B37/0427	9	{Mountings relative to pocket and wrist watches allowing a rocking movement about a hinge or any other movement (covers and protective cases which may be removed completely either by direct removal or by sliding or turning G04B37/005; ornamentation and interchangeable parts of cases, modifying the external appearance of the clockwork G04B47/046)}	G04B37/04	G04B37/04		150
G04B37/0436	10	{Clockwork movements coming out without springs, for allowing time reading or winding}	G04B37/04	G04B37/04		109
G04B37/0445	10	{Clockwork movements which come out by spring action for time reading and winding}	G04B37/04	G04B37/04		62
G04B37/0454	10	{Free standing watches (montre chevalet)}	G04B37/04	G04B37/04		79
G04B37/0463	10	{Free standing watches where the clockwork, on opening or closing the case, is ejected or returned by spring action, or possibly with a spring for opening or closing the case (cases with spring action cover G04B37/0025; wrist watches or pocket watches which can be used as free standing watches with the aid of certain parts of the case G04B37/148)}	G04B37/04	G04B37/04		105
G04B37/0472	10	{Rocking mounting of the clockwork}	G04B37/04	G04B37/04		104
G04B37/0481	9	{Mountings relative to wall-clockworks and to pendulums allowing certain movements}	G04B37/04	G04B37/04		58
G04B37/049	9	{Mountings for sound-damping}	G04B37/04	G04B37/04		50
G04B37/05	9	Fixed mountings for pocket or wrist watches	G04B37/05	G04B37/05		419
G04B37/052	10	{with shock damping means not related to the winding stem (shock damping bearings G04B31/02; shock protection G04B43/002)}	G04B37/05	G04B37/05		193
G04B37/055	10	{with shock damping means including the winding stem (shock damping bearings G04B31/02; shock protection G04B43/002)}	G04B37/05	G04B37/05		89
G04B37/057	10	{for shaped watches}	G04B37/05	G04B37/05		58
G04B37/06	8	Forming the passage for the winding stem through the case; Divided winding stems {(watertight protection means for the winding stem G04B37/10; fixing the knob to the case G04B37/1466; winding and setting the hands with the winding stem with clutch wheel G04B27/04, with rocking bar G04B27/06)}	G04B37/06	G04B37/06		129
G04B37/062	9	{Means for preventing the winding stem from being pulled out too far}	G04B37/06	G04B37/06		54
G04B37/064	10	{by a tirette}	G04B37/06	G04B37/06		85
G04B37/066	9	{Divided stem (tige brisee) (normal winding stems G04B3/041)}	G04B37/06	G04B37/06		124
G04B37/068	9	{Stem passage not being part of the layout of the clockwork}	G04B37/06	G04B37/06		86
G04B37/08	8	Hermetic sealing of openings, joints, passages or slits {(covers or protecting devices which can be directly removed, or by sliding or turning G04B37/005; hermetic sealing of watch or crystal with special pieces G04B39/02; hermetically-sealed electrical switches H01H23/06)}	G04B37/08	G04B37/08		481
G04B37/081	9	{Complete encasings for wrist or pocket watches also comprising means for hermetic sealing of the winding stem and crown (hermetic sealing of the stem or crown G04B37/10)}	G04B37/08	G04B37/08		284
G04B37/082	10	{without special hermetic sealing pieces}	G04B37/08	G04B37/08		66
G04B37/083	10	{for shaped watches}	G04B37/08	G04B37/08		82
G04B37/084	9	{Complete encasings for wrist or pocket watches without means for hermetic sealing of winding stem or crown}	G04B37/08	G04B37/08		420
G04B37/085	10	{without special hermetic sealing pieces}	G04B37/08	G04B37/08		89
G04B37/086	10	{for shaped watches}	G04B37/08	G04B37/08		142
G04B37/087	9	{Protection of wrist or pocket watch cases against dust}	G04B37/08	G04B37/08		206
G04B37/088	9	{Means affording hermetic sealing inside the case, e.g. protective case for the clockwork against dust, the escapement being in a hermetically sealed case (case for watch pieces G04B37/0091; synchronous motor lubrication G04C15/009)}	G04B37/08	G04B37/08		66
G04B37/10	9	of winding stems {(construction of winding crowns G04B3/041; in combination with hermetic sealing G04B37/081)}	G04B37/10	G04B37/10		647
G04B37/103	10	{by screwing the crown onto the case}	G04B37/10	G04B37/10		213
G04B37/106	10	{of push buttons (winding up by push button G04B3/001; crown in the form of push button G04B3/046; construction of push buttons G04B3/048)}	G04B37/10	G04B37/10		222
G04B37/11	9	of the back cover of pocket or wrist watches	G04B37/11	G04B37/11		394
G04B37/113	10	{without special hermetic sealing pieces}	G04B37/11	G04B37/11		42
G04B37/116	10	{for shaped watches}	G04B37/11	G04B37/11		38
G04B37/12	8	Cases for special purposes, e.g. watch combined with ring, watch combined with button (watch guards or protectors A45C11/10, A45C11/12; watches combined with cosmetic powder containers A45D33/30{; domed dial G04B19/10; calibers in which the clockwork is disposed on different planes G04B33/08; means for fixing watches on items of clothing G04B37/1433; cases having means for fixing onto a normal bracelet G04B37/1486; cases giving special affects due to their particular shape G04B45/0069; watches combined with various objects and therefore having a specially shaped case G04B47/00})	G04B37/12	G04B37/12		385
G04B37/122	9	{used as a mirror}	G04B37/12	G04B37/12		71
G04B37/125	9	{allowing note taking (cases with means for holding sheets of note-paper G04B37/127; adjustable guide marks or pointers for indicating determined points of time G04B19/28; changeable indicators G04B45/0092)}	G04B37/12	G04B37/12		39
G04B37/127	9	{used as containers or cartridges (means for incorporating a battery in the case G04G17/00)}	G04B37/12	G04B37/12		281
G04B37/14	8	Suspending devices, supports or stands for time-pieces insofar as they form part of the case {(wrist watch straps, fastening means therefor A44C5/00)}	G04B37/14	G04B37/14		340
G04B37/1406	9	{Means for fixing the clockwork pieces on other objects (possibly on walls)}	G04B37/14	G04B37/14		198
G04B37/1413	10	{Separable means}	G04B37/14	G04B37/14		155
G04B37/142	10	{Means which can be adjusted as a function of the clockwork piece}	G04B37/14	G04B37/14		24
G04B37/1426	10	{Means whereby the clockwork piece may move with regard to its suspension device}	G04B37/14	G04B37/14		90
G04B37/1433	10	{Fixation on items of clothing, e.g. with clips (button watches G04B37/12; brooches, or the like A44C1/00; other similar fixation means, in general A45F5/02)}	G04B37/14	G04B37/14		223
G04B37/144	10	{Fixation on flat support, e.g. on dashboard}	G04B37/14	G04B37/14		85
G04B37/1446	9	{Means for suspending pocket-, or other types of watches, e.g. on small chains (bracelet fixings G04B37/1486)}	G04B37/14	G04B37/14		129
G04B37/1453	10	{Construction and manufacture of case crown and clip}	G04B37/14	G04B37/14		14
G04B37/146	10	{with the case crown and a clip}	G04B37/14	G04B37/14		181
G04B37/1466	10	{Fixing the case crown onto the case}	G04B37/14	G04B37/14		37
G04B37/1473	9	{Supports and feet for supporting the clockwork (cases for standing clockworks in general G04B37/0066)}	G04B37/14	G04B37/14		248
G04B37/148	10	{formed by parts of the case (standing watches by bringing them out of the case or purse  G04B37/0463)}	G04B37/14	G04B37/14		152
G04B37/1486	9	{Arrangements for fixing to a bracelet (building watches into bracelets (montre marquise) G04B37/12; arrangements for hanging pocket- or other watches on chains G04B37/1446)}	G04B37/14	G04B37/14		1884
G04B37/1493	10	{by means of a feather spring (Barette &#225; ressort)}	G04B37/14	G04B37/14		251
G04B37/16	9	Fastening the case to the bracelet	G04B37/16	G04B37/16		77
G04B37/18	8	for pocket or wrist watches (G04B37/02 - G04B37/16 take precedence)	G04B37/18	G04B37/18		75
G04B37/20	9	with hinged covers or backs	G04B37/20	G04B37/20		7
G04B37/22	8	Materials or processes of manufacturing pocket watch or wrist watch cases {(machines or tools for the manufacture of clockwork cases G04D3/0064, G04D3/0097, G04D3/029; decoration or tools therefor G04B45/0076)}	G04B37/22	G04B37/22		1048
G04B37/223	9	{metallic cases coated with a nonmetallic layer}	G04B37/22	G04B37/22		108
G04B37/225	9	{Non-metallic cases}	G04B37/22	G04B37/22		441
G04B37/226	10	{coated with a metallic layer}	G04B37/22	G04B37/22		92
G04B37/228	10	{Wooden cases}	G04B37/22	G04B37/22		50
G04B39/00	7	Watch crystals; Fastening or sealing of crystals; Clock glasses	G04B39/00	G04B39/00		531
G04B39/002	8	{made of glass}	G04B39/00	G04B39/00		192
G04B39/004	8	{from a material other than glass}	G04B39/00	G04B39/00		130
G04B39/006	9	{out of wear resistant material, e.g. sapphire}	G04B39/00	G04B39/00		107
G04B39/008	8	{with means for magnified reading (combinations with a magnifying glass in general G04B47/00)}	G04B39/00	G04B39/00		91
G04B39/02	8	Sealing crystals or glasses {(sealing the case and the winding stem G04B37/08)}	G04B39/02	G04B39/02		480
G04B39/025	9	{without special sealing parts}	G04B39/02	G04B39/02		179
G04B41/00	7	Locking or holding devices for pendulums, chimes, or the like, for use during transport	G04B41/00	G04B41/00		37
G04B41/005	8	{holding and locking of the pendulum only}	G04B41/00	G04B41/00		67
G04B43/00	7	Protecting clockworks by shields or other means against external influences, e.g. magnetic fields {(demagnetising apparatus G04D9/00)}	G04B43/00	G04B43/00		185
G04B43/002	8	{Component shock protection arrangements (shock damping bearings G04B31/02; shock-damping in the case G04B37/04; protection of the pendulum or chime during transport G04B41/00)}	G04B43/00	G04B43/00		180
G04B43/005	8	{Protection against temperature influences}	G04B43/00	G04B43/00		47
G04B43/007	8	{Antimagnetic alloys (antimagnetic alloys with temperature compensation G04B17/227; apparatus for antimagnetising G04D9/00; alloys in general C22C)}	G04B43/00	G04B43/00		130
G04B45/00	7	Time pieces of which the indicating means or cases provoke special effects, e.g. aesthetic effects (ornamental shaping of dials G04B19/10){(lubrication of clockwork bearings G04B31/008; special effects and pictures in general B44F)}	G04B45/00	G04B45/00		547
G04B45/0007	8	{Light-, colour-, line-, or spot-effects caused by parts or pictures moved by the clockwork (disc-shaped indicating parts G04B19/046, G04B19/202; figures or parts thereof for indicating the time, moved by the clockwork G04B25/06)}	G04B45/00	G04B45/00		356
G04B45/0015	8	{Light-, colour-, line- or spot-effects caused by or on stationary parts (change of appearance by exchangeable case parts G04B47/046)}	G04B45/00	G04B45/00		356
G04B45/0023	8	{Inscriptions or pictures moved by the clockwork, e.g. for advertising (clocks with abrupt time indication G04B13/00; disc-shaped indicating elements G04B19/046, G04B19/202; advertising in general G09F)}	G04B45/00	G04B45/00		154
G04B45/003	8	{Inscriptions and pictures moved by hand (clockworks with abrupt time indication G04B13/00; adjustable hands or mechanisms G04B19/28; combination of clockwork with counter, e.g. for sports results G04B47/00; movable ornaments and decorations G04B47/044)}	G04B45/00	G04B45/00		73
G04B45/0038	8	{Figures or parts thereof moved by the clockwork (disc-shaped indicating means G04B19/046. G04B19/202; time indicating by moving figures G04B25/06; normal moving parts of the clockwork visible through a window, e.g. the escapement G04B45/02)}	G04B45/00	G04B45/00		201
G04B45/0046	9	{with oscillating motion, in pocket- or wrist watches}	G04B45/00	G04B45/00		94
G04B45/0053	9	{with oscillating motion in hanging or standing clockworks such as imitation of a real pendulum}	G04B45/00	G04B45/00		186
G04B45/0061	9	{Moving parts of the clockwork, e.g. pendulum, hands in special form, mostly constructed as a figure (cases and non moving parts of the clockwork in various forms G04B45/0069; decoration and manufacturing methods therefor, also for moving parts G04B45/0076; construction of normal pendulums G04B17/02; construction of normal hands G04B19/042)}	G04B45/00	G04B45/00		206
G04B45/0069	8	{Cases and fixed parts with a special shape (movable parts with a special shape G04B45/0061; decoration in general, and methods of manufacture thereof G04B45/0076; cases in general G04B37/00; combination with genuine utensils or mounting therein G04B47/00)}	G04B45/00	G04B45/00		436
G04B45/0076	8	{Decoration of the case and of parts thereof, e.g. as a method of manufacture thereof (specially shaped G04B45/0061, G04B45/0069; decoration with inscriptions and pictures G04B45/0084; construction of the hands G04B19/042; decoration by adding extra pieces to the clockwork G04B47/04; colouring by treatment of the surface, e.g. by oxidation C25D)}	G04B45/00	G04B45/00		604
G04B45/0084	8	{Pictures or inscriptions on the case or parts thereof, attaching complete pictures (decoration and manfuacture thereof G04B45/0076; special decorative parts which are attached to the case or other parts G04B47/04)}	G04B45/00	G04B45/00		281
G04B45/0092	9	{Changeable parts (cases or clockworks with holders or as holders G04B37/127)}	G04B45/00	G04B45/00		220
G04B45/02	8	Time pieces of which the clockwork is visible partly or wholly {(figures or parts thereof moved by the clockwork G04B45/0038)}	G04B45/02	G04B45/02		313
G04B45/04	8	Time pieces with invisible drive, e.g. with hands attached to a rotating glass disc {(for advertising G09F23/00; disc-shaped hands with marks or notches G04B19/046)}	G04B45/04	G04B45/04		147
G04B45/043	9	{the clockwork being positioned in the hands or pendulum (gearwork G04B1/00; pendulums G04B17/02; construction of the hands G04B19/042)}	G04B45/04	G04B45/04		47
G04B45/046	9	{the driving mechanism of the hands being invisible because of special shielding (construction of the hands G04B19/042)}	G04B45/04	G04B45/04		93
G04B47/00	7	Time-pieces combined with other articles which do not interfere with the running or the time-keeping of the time-piece ({clockwork cases for special purposes G04B37/12; clocks with magnifying glass built in the face G04B39/00; time-pieces in which parts or cases produce special effects, e.g. aesthetic effects, G04B45/00, particularly with inscriptions or pictures moved by hand G04B45/003, with specially shaped cases or parts G04B45/0069; combination of} writing or drawing implements with devices for indicating time B43K29/087; combined with cameras, projectors, or photographic printing apparatus G03B29/00)	G04B47/00	G04B47/00		1887
G04B47/001	8	{Mounting or fixing to the steering wheel of a vehicle}	G04B47/00	G04B47/00		24
G04B47/003	8	{Mounting in and combined with adjustable indicating means, e.g. date indicating means adjustable by hand, marks or counters (calendar clocks G04B19/24)}	G04B47/00	G04B47/00		194
G04B47/005	8	{combined with a key}	G04B47/00	G04B47/00		45
G04B47/006	8	{combined with a lighter}	G04B47/00	G04B47/00		173
G04B47/008	8	{combined with a thermometer}	G04B47/00	G04B47/00		69
G04B47/02	8	Installations within mirrors, pictures, furniture or other household articles {(clock-lamps, globe-clocks with a fixed dial, G04B19/04; clock in the form of a lamp with a dial mounted upon it, moved by the clockwork G04B19/21; clockwork in the form of a globe for indicating different local apparent times G04B19/22; illumination of the dial and the hands G04B19/30; clock-lamps with the lamp switched on and off by the clockwork mechanism G04C19/02, within keys G04B47/005, within lighters G04B47/006, within pens B43K29/087)}	G04B47/02	G04B47/02		441
G04B47/025	9	{in musical instruments or loudspeakers (sounding bodies with chimes G04B21/08; in alarm clocks G04B23/028; cases with arrangements for enhancing the sound production G04B37/0075)}	G04B47/02	G04B47/02		84
G04B47/04	8	with attached ornaments or amusement apparatus {(decorated cases seeG04B45/00)}	G04B47/04	G04B47/04		215
G04B47/042	9	{Fastening of jewels and the like (set on or into numbers G04B19/103; jewel bearings G04B31/008; setting of jewels and tools therefor A44C; devices for setting jewel bearings G04D3/04)}	G04B47/04	G04B47/04		215
G04B47/044	9	{Movable decorations and parts thereof (inscriptions and pictures moved by hand G04B45/003)}	G04B47/04	G04B47/04		190
G04B47/046	9	{Changeable decorations and parts thereof, decorations for the case which change the external appearance of the clockwork (clip-on -, sliding - or tilting protective lids or covers G04B37/005; with a clockwork which can be mounted on different cases for changing its external appearance G04B37/0427; clockworks which can be mounted in different cases for changing their purpose G04B37/14; decoration of the case or parts thereof G04B45/0076; changeable pictures or inscriptions G04B45/0092)}	G04B47/04	G04B47/04		256
G04B47/048	9	{Clockwork combined with toys (devices for teaching clock reading G09B19/12; indicating play time G07C1/28)}	G04B47/04	G04B47/04		102
G04B47/06	8	with attached measuring instruments, e.g. pedometer, barometer, thermometer or compass {(in combination with a tachometer which winds up the clockwork G04B5/206)}	G04B47/06	G04B47/06		532
G04B47/061	9	{calculating scales for indicating relationship between quantity and time (indicating or recording of quantity-time ratios G01D; meters for measuring average speed, measuring speed by chronograph G01P; slide rules and calculating wheels G06G)}	G04B47/06	G04B47/06		274
G04B47/063	9	{measuring physiological quantities, e.g. pedometers, heart-rate sensors, blood pressure gauges and the like}	G04B47/06	G04B47/06		295
G04B47/065	9	{with a compass (compasses G01C17/00)}	G04B47/06	G04B47/06		184
G04B47/066	9	{with a pressure sensor}	G04B47/06	G04B47/06		181
G04B47/068	9	{with a thermometer}	G04B47/06	G04B47/06		160
G04B49/00	7	Time-pieces using the position of the sun, moon or stars {(devices for fixing the place and time by astronomical observations G01C21/00)}	G04B49/00	G04B49/00		103
G04B49/02	8	Sundials {(normal dials G04B19/06)}	G04B49/02	G04B49/02		347
G04B49/04	9	Graduation or shaping of dials	G04B49/04	G04B49/04		66
G04B99/00	7	Subject matter not provided for in other groups of this subclass	G04B99/00	G04B99/00		45
