H04S   1/00		２チャンネル方式（Ｈ０４Ｓ５／００，Ｈ０４Ｓ７／００が優先）［３］	Two-channel systems(<b>H04S5/00</b>, <b>H04S7/00</b> take precedence)	7477
H04S   3/00		３チャンネル以上，例．４チャンネル，を用いる方式，（Ｈ０４Ｓ５／００，Ｈ０４Ｓ７／００が優先）［３］	Systems employing more than two channels, e.g. quadraphonic(<b>H04S5/00</b>, <b>H04S7/00</b> take precedence)	5584
H04S   3/02	・	マトリクス形式，すなわち．入力信号が代数学的に組み合わされるもの，例．互いに関して位相推移がなされた後組み合わされるもの［３］	of the matrix type, i.e. in which input signals are combined algebraically, e.g. after having been phase shifted with respect to each other	1037
H04S   5/00		擬似ステレオ方式，例．付加的なチャンネル信号が，モノラル信号から位相推移，時間遅延または残響によって生じる方式［３］	Pseudo-stereo systems, e.g. in which additional channel signals are derived from monophonic signals by means of phase shifting, time delay or reverberation	2224
H04S   5/02	・	擬似４チャンネル形式，例．後チャンネル信号が２チャンネルステレオ信号から生じるもの［３］	of the pseudo four-channel type, e.g. in which rear channel signals are derived from two-channel stereo signals	3623
H04S   7/00		指示装置；制御装置，例．バランス制御［３］	Indicating arrangements; Control arrangements, e.g. balance control	13236
