B29C31/00	7	Handling, e.g. feeding of the material to be shaped {, storage of plastics material before moulding; Automation, i.e. automated handling lines in plastics processing plants, e.g. using manipulators or robots (discharging moulded articles from the mould B29C37/0003; storage of prepregs or SMC after impregnation or during ageing B29C70/54; baling of rubber B29B15/02)}	B29C31/00	B29C31/00		1266
B29C31/002	8	{Handling tubes, e.g. transferring between shaping stations, loading on mandrels}	B29C31/00	B29C31/00		663
B29C31/004	8	{Arrangements for converting the motion of a material which is continuously fed to a working station in a stepwise motion}	B29C31/00	B29C31/00		162
B29C31/006	8	{Handling moulds, e.g. between a mould store and a moulding machine (movable moulds B29C33/34; for injection moulding B29C45/1756)}	B29C31/00	B29C31/00		531
B29C31/008	8	{Handling preformed parts, e.g. inserts (B29C37/001 takes precedence; for injection moulding B29C45/14008; for blow moulding B29C49/2408; for thermoforming B29C51/165)}	B29C31/00	B29C31/00		583
B29C31/02	8	Dispensing from vessels, e.g. hoppers {(into a mould cavity B29C31/04; large containers characterised by discharge means B65D88/28, B65D88/54)}	B29C31/02	B29C31/02		780
B29C31/04	8	Feeding {of the material to be moulded}, e.g. into a mould cavity {(B29C39/08 takes precedence; using a material distribution system to two or more fixed injection moulds B29C45/125)}	B29C31/04	B29C31/04		1132
B29C31/041	9	{using filling or dispensing heads placed in closed moulds or in contact with mould walls (B29C45/27 takes precedence)}	B29C31/04	B29C31/04		240
B29C31/042	9	{using dispensing heads, e.g. extruders, placed over or apart from the moulds (positioning extruded preforms on conveyors B29C31/085)}	B29C31/04	B29C31/04		194
B29C31/044	10	{with moving heads for distributing liquid or viscous material into the moulds}	B29C31/04	B29C31/04		124
B29C31/045	11	{moving along predetermined circuits or distributing the material according to predetermined patterns}	B29C31/04	B29C31/04		111
B29C31/047	10	{combined with moving moulds (B29C31/044, B29C31/048 take precedence)}	B29C31/04	B29C31/04		129
B29C31/048	10	{the material being severed at the dispensing head exit, e.g. as ring, drop or gob, and transported immediately into the mould, e.g. by gravity}	B29C31/04	B29C31/04		288
B29C31/06	9	in measured doses {, e.g. by weighting (feeding mixers with measured doses B01F35/714, B01F35/882, B29B7/24, B29B7/603)}	B29C31/06	B29C31/06		496
B29C31/061	10	{using stationary volumetric measuring chambers}	B29C31/06	B29C31/06		35
B29C31/063	11	{of the piston type}	B29C31/06	B29C31/06		107
B29C31/065	10	{using volumetric measuring chambers moving between a charging station and a discharge station}	B29C31/06	B29C31/06		45
B29C31/066	11	{using feed frames, e.g. for dry material}	B29C31/06	B29C31/06		128
B29C31/068	11	{of the piston type}	B29C31/06	B29C31/06		43
B29C31/08	9	of preforms {to be moulded, e.g. tablets, fibre reinforced preforms, extruded ribbons, tubes or profiles; Manipulating means specially adapted for feeding preforms, e.g. supports conveyors (B29C31/066, B29C37/001, B29C43/085 take precedence)}<br><br><u>NOTE</u><br><br> Documents describing feeding preforms, e.g. parisons, tubes, sheets in connection with shaping techniques described in groups B29C49/00&#160;-&#160;B29C65/00 are not classified in group B29C31/08, but in the relevant groups of these techniques 	B29C31/08	B29C31/08		1246
B29C31/085	10	{combined with positioning the preforms according to predetermined patterns, e.g. positioning extruded preforms on conveyors (B29C70/30 takes precedence; for building tyres B29D30/08)}	B29C31/08	B29C31/08		208
B29C31/10	9	of several materials	B29C31/10	B29C31/10		304
B29C33/00	7	Moulds or cores; Details thereof or accessories therefor	B29C33/00	B29C33/00		2789
B29C2033/0005	8	{with transparent parts, e.g. permitting visual inspection of the interior of the cavity}	B29C33/00	B29C33/00		141
B29C33/0011	8	{thin-walled moulds}	B29C33/00	B29C33/00		384
B29C33/0016	9	{Lost moulds, e.g. staying on the moulded object (flexible bags without particular shape filled with expandable material B29C44/182; single use mandrels for winding and forming B29C53/822)}	B29C33/00	B29C33/00		247
B29C33/0022	8	{Multi-cavity moulds (B29C33/301 takes precedence)}	B29C33/00	B29C33/00		605
B29C33/0027	9	{with deep narrow cavities, e.g. for making piles (non-woven pile fabrics D04H11/00)}	B29C33/00	B29C33/00		53
B29C33/0033	8	{constructed for making articles provided with holes}<br><br><u>NOTE</u><br><br>If the hole is made by cutting means associated with the mould, see the relevant moulding technique.	B29C33/00	B29C33/00		966
B29C33/0038	8	{with sealing means or the like (seals on envelopes used in tyre retreading B29D30/542; for injection moulding footwear B29D35/0045)}	B29C33/00	B29C33/00		882
B29C33/0044	9	{for sealing off parts of inserts projecting into the mould cavity}	B29C33/00	B29C33/00		311
B29C33/005	8	{characterised by the location of the parting line of the mould parts}	B29C33/00	B29C33/00		359
B29C33/0055	8	{with incorporated overflow cavities (in particular in injection moulds B29C45/2669)}	B29C33/00	B29C33/00		318
B29C33/0061	8	{characterised by the configuration of the material feeding channel (sprue channels for injection moulding B29C45/27)}	B29C33/00	B29C33/00		261
B29C33/0066	9	{with a subdivided channel for feeding the material to a plurality of locations}	B29C33/00	B29C33/00		77
B29C33/0072	9	{with a configuration promoting turbulency, e.g. for after-mixing in the mould}	B29C33/00	B29C33/00		95
B29C33/0077	8	{characterised by the configuration of the mould filling gate (mixing chambers situated in the mould opening B29B7/7471); accessories for connecting the mould filling gate with the filling spout}	B29C33/00	B29C33/00		146
B29C33/0083	8	{Electrical or fluid connection systems therefor}	B29C33/00	B29C33/00		148
B29C33/0088	8	{Multi-face stack moulds}	B29C33/00	B29C33/00		105
B29C2033/0094	8	{Means for masking a part of the moulding surface}	B29C33/00	B29C33/00		49
B29C33/02	8	with incorporated heating or cooling means	B29C33/02	B29C33/02		1887
B29C2033/023	9	{Thermal insulation of moulds or mould parts}	B29C33/02	B29C33/02		219
B29C33/026	9	{in rolls, calenders or drums}	B29C33/02	B29C33/02		76
B29C33/04	9	using liquids, gas or steam {(tyre moulds with incorporated heating or cooling means using liquids, gas or steam B29D30/0601)}	B29C33/04	B29C33/04		1950
B29C2033/042	10	{Meander or zig-zag shaped cooling channels, i.e. continuous cooling channels whereby a plurality of cooling channel sections are oriented in a substantial parallel direction}	B29C33/04	B29C33/04		214
B29C33/044	10	{in rolls calenders or drums}	B29C33/04	B29C33/04		193
B29C33/046	10	{using gas}	B29C33/04	B29C33/04		377
B29C33/048	10	{using steam}	B29C33/04	B29C33/04		299
B29C33/06	9	using radiation {, e.g. electro-magnetic waves, induction heating}	B29C33/06	B29C33/06		533
B29C33/065	10	{in rolls, calenders or drums}	B29C33/06	B29C33/06		27
B29C33/08	9	for dielectric heating	B29C33/08	B29C33/08		253
B29C33/085	10	{using rolls, calenders or drums}	B29C33/08	B29C33/08		3
B29C33/10	8	with incorporated venting means	B29C33/10	B29C33/10		1981
B29C33/12	8	with incorporated means for positioning inserts, e.g. labels {(positioning reinforcements B29C70/541)}	B29C33/12	B29C33/12		950
B29C33/123	9	{for centering the inserts}	B29C33/12	B29C33/12		495
B29C33/126	10	{using centering means forming part of the insert}	B29C33/12	B29C33/12		152
B29C33/14	9	against the mould wall	B29C33/14	B29C33/14		422
B29C33/16	10	using magnetic means	B29C33/16	B29C33/16		250
B29C33/18	10	using vacuum	B29C33/18	B29C33/18		301
B29C33/20	8	Opening, closing or clamping	B29C33/20	B29C33/20		1174
B29C33/202	9	{Clamping means operating on closed or nearly closed mould parts, the clamping means being independently movable of the opening or closing means (clamping devices for injection moulding machines B29C45/64)}	B29C33/20	B29C33/20		741
B29C2033/205	10	{mould clamping by membranes, e.g. inflatable membranes or cushions}	B29C33/20	B29C33/20		35
B29C2033/207	10	{mould clamping by pivoting members}	B29C33/20	B29C33/20		111
B29C33/22	9	by rectilinear movement	B29C33/22	B29C33/22		502
B29C33/24	10	using hydraulic or pneumatic means	B29C33/24	B29C33/24		323
B29C33/26	9	by pivotal movement	B29C33/26	B29C33/26		700
B29C33/28	10	using hydraulic or pneumatic means	B29C33/28	B29C33/28		140
B29C33/30	8	Mounting, exchanging or centering {(moulds, mould parts or cores; B29C33/485 takes precedence)}	B29C33/30	B29C33/30		1537
B29C33/301	9	{Modular mould systems [MMS], i.e. moulds built up by stacking mould elements, e.g. plates, blocks, rods (B29C33/0088 takes precedence)}	B29C33/30	B29C33/30		676
B29C33/302	10	{Assembling a large number of mould elements to constitute one cavity}	B29C33/30	B29C33/30		440
B29C33/303	9	{centering mould parts or halves, e.g. during mounting}	B29C33/30	B29C33/30		641
B29C33/304	10	{centering cores}	B29C33/30	B29C33/30		139
B29C33/305	9	{Mounting of moulds or mould support plates (handling of moulds B29C31/006; mounting of moulds for injection moulding B29C45/1742)}	B29C33/30	B29C33/30		981
B29C33/306	9	{Exchangeable mould parts, e.g. cassette moulds, mould inserts (moulds with exchangeable mould parts for injection moulding B29C45/2673; mounting of exchangeable mould inserts for injection moulding B29C45/2675)}	B29C33/30	B29C33/30		1084
B29C33/307	9	{Mould plates mounted on frames; Mounting the mould plates; Frame constructions therefor (shaping plates for making moulds B29C33/3842; thin walled moulds B29C33/0011)}	B29C33/30	B29C33/30		316
B29C33/308	9	{Adjustable moulds (for injection moulding B29C45/376)}	B29C33/30	B29C33/30		728
B29C33/32	9	using magnetic means	B29C33/32	B29C33/32		145
B29C33/34	8	movable, e.g. to or from the moulding station	B29C33/34	B29C33/34		675
B29C33/36	9	continuously movable {in one direction, e.g. in a closed circuit (B29C49/0021 takes precedence)}	B29C33/36	B29C33/36		819
B29C33/38	8	characterised by the material or the manufacturing process (B29C33/44 takes precedence)	B29C33/38	B29C33/38		1955
B29C33/3807	9	{Resin-bonded materials, e.g. inorganic particles}	B29C33/38	B29C33/38		222
B29C33/3814	9	{Porous moulds (adapted for vacuum forming B29C51/365)}	B29C33/38	B29C33/38		394
B29C33/3821	9	{composed of particles enclosed in a bag}	B29C33/38	B29C33/38		108
B29C33/3828	9	{Moulds made of at least two different materials having different thermal conductivities}	B29C33/38	B29C33/38		385
B29C33/3835	9	{Designing moulds, e.g. using CAD-CAM}	B29C33/38	B29C33/38		777
B29C33/3842	9	{Manufacturing moulds, e.g. shaping the mould surface by machining}	B29C33/38	B29C33/38		3606
B29C2033/385	10	{by laminating a plurality of layers}	B29C33/38	B29C33/38		276
B29C33/3857	10	{by making impressions of one or more parts of models, e.g. shaped articles and including possible subsequent assembly of the parts}	B29C33/38	B29C33/38		890
B29C2033/3864	11	{Spraying at least one layer to create the mould}	B29C33/38	B29C33/38		38
B29C2033/3871	11	{the models being organic material, e.g. living or dead bodies or parts thereof}	B29C33/38	B29C33/38		141
B29C33/3878	11	{used as masters for making successive impressions}	B29C33/38	B29C33/38		322
B29C33/3885	12	{the mould parts being co-operating impressions}	B29C33/38	B29C33/38		50
B29C33/3892	11	{Preparation of the model, e.g. by assembling parts}	B29C33/38	B29C33/38		169
B29C33/40	9	Plastics, e.g. foam or rubber	B29C33/40	B29C33/40		1539
B29C33/405	10	{Elastomers, e.g. rubber (B29C33/50 takes precedence)}	B29C33/40	B29C33/40		843
B29C33/42	8	characterised by the shape of the moulding surface, e.g. ribs or grooves	B29C33/42	B29C33/42		2172
B29C2033/422	9	{Moulding surfaces provided with a shape to promote flow of material in the mould cavity}	B29C33/42	B29C33/42		56
B29C33/424	9	{Moulding surfaces provided with means for marking or patterning (for injection moulding B29C45/372)}	B29C33/42	B29C33/42		1681
B29C2033/426	10	{Stampers}	B29C33/42	B29C33/42		121
B29C33/428	10	{For altering indicia, e.g. data, numbers (for injection moulding B29C45/374)}	B29C33/42	B29C33/42		121
B29C33/44	8	with means for, or specially constructed to facilitate, the removal of articles, e.g. of undercut articles	B29C33/44	B29C33/44		2027
B29C33/442	9	{with mechanical ejector or drive means therefor}	B29C33/44	B29C33/44		739
B29C33/444	10	{for stripping articles from a mould core, e.g. using stripper plates}	B29C33/44	B29C33/44		186
B29C33/446	11	{and using a rotating movement to unscrew articles (in particular in injection moulds B29C45/262)}	B29C33/44	B29C33/44		76
B29C33/448	9	{destructible (B29C33/52 takes precedence; in particular used in injection moulding B29C45/4457)}	B29C33/44	B29C33/44		249
B29C33/46	9	using fluid pressure	B29C33/46	B29C33/46		545
B29C33/48	9	with means for collapsing or disassembling	B29C33/48	B29C33/48		372
B29C33/485	10	{cores or mandrels (collapsible mandrels for shaping tube ends B29C57/02; collapsible mandrels for winding and joining B29C53/824)}	B29C33/48	B29C33/48		796
B29C33/50	10	elastic {or flexible (for isostatic pressing B29C43/3642)}	B29C33/50	B29C33/50		391
B29C33/505	11	{cores or mandrels, e.g. inflatable (B29C33/0016 takes precedence; for winding and joining B29C53/824; for supporting articles during joining B29C66/634; flexible cores for vulcanizing tyres B29D30/0654)}	B29C33/50	B29C33/50		604
B29C33/52	9	soluble or fusible {(in particular used in injection moulding B29C45/4457)}	B29C33/52	B29C33/52		993
B29C2033/525	10	{Cores made of frozen liquids, e.g. ice}	B29C33/52	B29C33/52		32
B29C33/54	9	made of powdered or granular material	B29C33/54	B29C33/54		100
B29C33/56	8	Coatings {, e.g. enameled or galvanised}; Releasing, lubricating or separating agents {(in-mould coating B29C37/0028; using or applying separating agents B29C37/0067)}	B29C33/56	B29C33/56		1346
B29C33/565	9	{Consisting of shell-like structures supported by backing material}	B29C33/56	B29C33/56		228
B29C33/58	9	Applying the releasing agents	B29C33/58	B29C33/58		1065
B29C33/60	9	Releasing, lubricating or separating agents {(in general C10M)}	B29C33/60	B29C33/60		1127
B29C33/62	10	based on polymers or oligomers	B29C33/62	B29C33/62		722
B29C33/64	11	Silicone	B29C33/64	B29C33/64		592
B29C33/66	11	Cellulose; Derivatives thereof	B29C33/66	B29C33/66		43
B29C33/68	9	Release sheets	B29C33/68	B29C33/68		1046
B29C33/70	8	Maintenance	B29C33/70	B29C33/70		144
B29C2033/705	9	{Mould inspection means, e.g. cameras}	B29C33/70	B29C33/70		62
B29C33/72	9	Cleaning {(extruder parts B29C48/27; in general B08B7/00)}	B29C33/72	B29C33/72		1654
B29C33/722	10	{Compositions for cleaning moulds}	B29C33/72	B29C33/72		181
B29C2033/725	10	{cleaning by plasma treatment}	B29C33/72	B29C33/72		33
B29C2033/727	10	{cleaning during moulding}	B29C33/72	B29C33/72		114
B29C33/74	9	Repairing	B29C33/74	B29C33/74		99
B29C33/76	8	Cores (B29C33/02&#160;-&#160;B29C33/70, {B29C41/40, B29C53/74, B29C53/82} take precedence)	B29C33/76	B29C33/76		1230
B29C35/00	7	Heating, cooling or curing, e.g. crosslinking or vulcanising; Apparatus therefor (moulds with incorporated heating or cooling means B29C33/02{; thermal after-treatment of shaped articles B29C71/02}; curing devices for plastics dental prostheses A61C13/14; before moulding B29B13/00)	B29C35/00	B29C35/00		801
B29C35/002	8	{Component parts, details or accessories; Auxiliary operations}	B29C35/00	B29C35/00		1277
B29C2035/005	9	{Enveloping the material to be cured, e.g. by helically winding a film around the material}	B29C35/00	B29C35/00		28
B29C35/007	8	{Tempering units for temperature control of moulds or cores, e.g. comprising heat exchangers, controlled valves, temperature-controlled circuits for fluids (B29C35/0294 takes precedence)}	B29C35/00	B29C35/00		635
B29C35/02	8	Heating or curing, e.g. crosslinking or vulcanizing {during moulding, e.g. in a mould}(cold vulcanisation B29C35/18{; vulcanising tyres, presses therefor B29D30/0601})	B29C35/02	B29C35/02		6956
B29C2035/0211	9	{resistance heating (B29C2035/0811 takes precedence)}	B29C35/02	B29C35/02		825
B29C2035/0216	9	{using Peltier-effect}	B29C35/02	B29C35/02		25
B29C35/0222	9	{the curing continuing after removal from the mould (B29C35/0233 takes precedence)}	B29C35/02	B29C35/02		159
B29C35/0227	9	{using pressure vessels, e.g. autoclaves, vulcanising pans (B29C35/065 takes precedence)}	B29C35/02	B29C35/02		543
B29C35/0233	10	{the curing continuing after removal from the mould}	B29C35/02	B29C35/02		111
B29C35/0238	10	{Presses provided with pressure vessels, e.g. steam chambers}	B29C35/02	B29C35/02		34
B29C35/0244	9	{using fluidised bed}	B29C35/02	B29C35/02		38
B29C35/025	10	{for articles of indefinite length}	B29C35/02	B29C35/02		33
B29C35/0255	9	{using friction}	B29C35/02	B29C35/02		58
B29C35/0261	9	{using ultrasonic or sonic vibrations}	B29C35/02	B29C35/02		274
B29C35/0266	9	{Local curing (for repairing B29C73/34)}	B29C35/02	B29C35/02		421
B29C35/0272	9	{using lost heating elements, i.e. heating means incorporated and remaining in the formed article (for preforms with internal stresses B29C61/0625; joining using lost heating elements B29C65/34; making electrically conductive articles B29C70/882)}	B29C35/02	B29C35/02		343
B29C35/0277	9	{Apparatus with continuous transport of the material to be cured (B29C35/025, B29C35/06, B29C35/10, B29C35/14 take precedence)}	B29C35/02	B29C35/02		478
B29C2035/0283	9	{Thermal pretreatment of the plastics material}	B29C35/02	B29C35/02		321
B29C35/0288	9	{Controlling heating or curing of polymers during moulding, e.g. by measuring temperatures or properties of the polymer and regulating the process (controlling or regulating chemical, physical or physico- chemical processes in general B01J19/0006)}	B29C35/02	B29C35/02		986
B29C35/0294	10	{using tempering units for temperature control of moulds or cores}	B29C35/02	B29C35/02		155
B29C35/04	9	using liquids, gas or steam	B29C35/04	B29C35/04		698
B29C35/041	10	{using liquids}	B29C35/04	B29C35/04		655
B29C2035/042	11	{other than water}	B29C35/04	B29C35/04		135
B29C2035/043	12	{oil}	B29C35/04	B29C35/04		184
B29C2035/044	12	{mercury}	B29C35/04	B29C35/04		8
B29C35/045	10	{using gas or flames}	B29C35/04	B29C35/04		1780
B29C2035/046	11	{dried air}	B29C35/04	B29C35/04		426
B29C2035/047	11	{other than air}	B29C35/04	B29C35/04		48
B29C2035/048	12	{inert gas}	B29C35/04	B29C35/04		83
B29C35/049	10	{using steam or damp}	B29C35/04	B29C35/04		1248
B29C35/06	10	for articles of indefinite length	B29C35/06	B29C35/06		637
B29C35/065	11	{in long tubular vessels}	B29C35/06	B29C35/06		257
B29C35/08	9	by wave energy or particle radiation {(B29C64/00, B29C71/04 take precedence)}	B29C35/08	B29C35/08		1453
B29C35/0805	10	{using electromagnetic radiation}	B29C35/08	B29C35/08		2578
B29C2035/0811	11	{using induction}	B29C35/08	B29C35/08		943
B29C2035/0816	12	{using eddy currents}	B29C35/08	B29C35/08		118
B29C2035/0822	11	{using IR radiation}	B29C35/08	B29C35/08		2293
B29C2035/0827	11	{using UV radiation}	B29C35/08	B29C35/08		3246
B29C2035/0833	11	{using actinic light}	B29C35/08	B29C35/08		395
B29C2035/0838	11	{using laser}	B29C35/08	B29C35/08		949
B29C2035/0844	11	{using X-ray}	B29C35/08	B29C35/08		202
B29C2035/085	11	{using gamma-ray}	B29C35/08	B29C35/08		312
B29C2035/0855	11	{using microwave}	B29C35/08	B29C35/08		1159
B29C2035/0861	11	{using radio frequency}	B29C35/08	B29C35/08		209
B29C35/0866	10	{using particle radiation}	B29C35/08	B29C35/08		222
B29C2035/0872	11	{using ion-radiation, e.g. alpha-rays}	B29C35/08	B29C35/08		207
B29C2035/0877	11	{using electron radiation, e.g. beta-rays}	B29C35/08	B29C35/08		867
B29C2035/0883	11	{using neutron radiation}	B29C35/08	B29C35/08		54
B29C35/0888	10	{using transparant moulds}	B29C35/08	B29C35/08		603
B29C35/0894	11	{provided with masks or diaphragms}	B29C35/08	B29C35/08		171
B29C35/10	10	for articles of indefinite length	B29C35/10	B29C35/10		789
B29C35/12	9	Dielectric heating	B29C35/12	B29C35/12		600
B29C35/14	10	for articles of indefinite length	B29C35/14	B29C35/14		114
B29C35/16	8	Cooling {(cooling extruded material B29C48/911; cooling preforms for blow moulding B29C49/6427; cooling blown articles B29C49/66; cooling tyres during post cure inflation B29D30/0643)}	B29C35/16	B29C35/16		4014
B29C2035/1608	9	{using Peltier-effect}	B29C35/16	B29C35/16		43
B29C2035/1616	9	{using liquids}	B29C35/16	B29C35/16		1807
B29C2035/1625	10	{other than water}	B29C35/16	B29C35/16		54
B29C2035/1633	11	{oil}	B29C35/16	B29C35/16		35
B29C2035/1641	11	{mercury}	B29C35/16	B29C35/16		2
B29C2035/165	11	{liquified gases}	B29C35/16	B29C35/16		146
B29C2035/1658	9	{using gas}	B29C35/16	B29C35/16		1470
B29C2035/1666	10	{dried air}	B29C35/16	B29C35/16		399
B29C2035/1675	10	{other than air}	B29C35/16	B29C35/16		27
B29C2035/1683	11	{inert gas}	B29C35/16	B29C35/16		41
B29C2035/1691	9	{using gas-liquid mixtures}	B29C35/16	B29C35/16		56
B29C35/18	8	Cold vulcanisation	B29C35/18	B29C35/18		92
B29C37/00	7	Component parts, details, accessories or auxiliary operations, not covered by group B29C33/00 or B29C35/00	B29C37/00	B29C37/00		1611
B29C37/0003	8	{Discharging moulded articles from the mould (constructions for removing the articles B29C33/44)}	B29C37/00	B29C37/00		646
B29C37/0007	9	{using means operable from outside the mould for moving between mould parts, e.g. robots}	B29C37/00	B29C37/00		406
B29C37/001	10	{combined with means for loading preforms to be moulded or inserts, e.g. preformed layers}	B29C37/00	B29C37/00		33
B29C37/0014	9	{by flexibly or permanently deforming undercut portions of the articles}	B29C37/00	B29C37/00		152
B29C37/0017	9	{by stripping articles from mould cores}	B29C37/00	B29C37/00		365
B29C37/0021	10	{and using a rotating movement to unscrew articles (in particular used in injection moulding B29C45/178)}	B29C37/00	B29C37/00		54
B29C37/0025	8	{Applying surface layers, e.g. coatings, decorative layers, printed layers, to articles during shaping, e.g. in-mould printing (moulding on preformed layers as inserts B29C70/68; applying fluent material to surfaces in general B05)}	B29C37/00	B29C37/00		567
B29C37/0028	9	{In-mould coating, e.g. by introducing the coating material into the mould after forming the article}	B29C37/00	B29C37/00		455
B29C37/0032	10	{the coating being applied upon the mould surface before introducing the moulding compound, e.g. applying a gelcoat (B29C44/14 and B29C44/32 take precedence)}	B29C37/00	B29C37/00		875
B29C2037/0035	10	{the coating being applied as liquid, gel, paste or the like}	B29C37/00	B29C37/00		315
B29C2037/0039	10	{the coating being applied in powder or particle form}	B29C37/00	B29C37/00		107
B29C2037/0042	10	{the coating being applied in solid sheet form, e.g. as meltable sheet}	B29C37/00	B29C37/00		203
B29C2037/0046	10	{In-mould printing, in-mould transfer printing}	B29C37/00	B29C37/00		116
B29C37/005	8	{Compensating volume or shape change during moulding, in general}	B29C37/00	B29C37/00		425
B29C37/0053	8	{Moulding articles characterised by the shape of the surface, e.g. ribs, high polish (mould construction therefor B29C33/42; surface shaping of articles B29C59/00; by incorporating filler in or near the surface B29C70/64)}	B29C37/00	B29C37/00		547
B29C37/0057	9	{Moulding single grooves or ribs, e.g. tear lines (folding lines B29C53/06)}	B29C37/00	B29C37/00		701
B29C37/006	8	{Degassing moulding material or draining off gas during moulding (venting means in moulds B29C33/10)}	B29C37/00	B29C37/00		542
B29C37/0064	9	{of reinforced material}	B29C37/00	B29C37/00		200
B29C37/0067	8	{Using separating agents during or after moulding; Applying separating agents on preforms or articles, e.g. to prevent sticking to each other (separating agents B29C33/60)}	B29C37/00	B29C37/00		608
B29C37/0071	9	{Dusting machines}	B29C37/00	B29C37/00		161
B29C37/0075	9	{using release sheets}	B29C37/00	B29C37/00		366
B29C37/0078	8	{Measures or configurations for obtaining anchoring effects in the contact areas between layers (surface shaping B29C59/00; B29C66/02 takes precedence)}	B29C37/00	B29C37/00		151
B29C37/0082	9	{Mechanical anchoring (B29C66/303 takes precedence)}	B29C37/00	B29C37/00		887
B29C37/0085	10	{by means of openings in the layers (joining through openings B29C66/304)}	B29C37/00	B29C37/00		325
B29C37/0089	8	{Sealing devices placed between articles and treatment installations during moulding or shaping, e.g. sealing off the entrance or exit of ovens or irradiation rooms, connections between rooms at different pressures}	B29C37/00	B29C37/00		81
B29C37/0092	8	{Drying moulded articles or half products, e.g. preforms, during or after moulding or cooling}	B29C37/00	B29C37/00		1469
B29C37/0096	8	{Trouble-shooting during starting or stopping moulding or shaping apparatus (B29C66/872 takes precedence)}	B29C37/00	B29C37/00		41
B29C37/02	8	Deburring or deflashing {(thermal deburring in general B23D79/005)}	B29C37/02	B29C37/02		2918
B29C37/04	9	of welded articles, e.g. deburring or deflashing in combination with welding {(shaping the burr B29C66/32)}<br><br><u>NOTE</u><br><br>Attention is drawn to Note (3) following the subclass title.	B29C37/04	B29C37/04		505
B29C2037/80	8	{Identifying, e.g. coding, dating, marking, numbering}	B29C37/00	B29C37/80		325
B29C2037/90	8	{Measuring, controlling or regulating}	B29C37/00	B29C37/90		1436
B29C2037/903	9	{by means of a computer}	B29C37/00	B29C37/90		345
B29C2037/906	9	{using visualisation means or linked accessories, e.g. screens, printers}	B29C37/00	B29C37/90		162
B29C2037/92	8	{Lubricating}	B29C37/00	B29C37/92		141
B29C2037/94	8	{Safety devices}	B29C37/00	B29C37/94		115
B29C2037/96	8	{Filters}	B29C37/00	B29C37/96		77
B29C39/00	7	Shaping by casting, i.e. introducing the moulding material into a mould or between confining surfaces without significant moulding pressure; Apparatus therefor (B29C41/00 takes precedence)	B29C39/00	B29C39/00		1052
B29C39/003	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest	B29C39/00	B29C39/00		1089
B29C39/006	9	{Monomers or prepolymers (by reaction injection moulding B29C67/246)}	B29C39/00	B29C39/00		859
B29C39/02	8	for making articles of definite length, i.e. discrete articles	B29C39/02	B29C39/02		1914
B29C39/021	9	{by casting in several steps}	B29C39/02	B29C39/02		288
B29C39/023	10	{for making multicoloured articles}	B29C39/02	B29C39/02		87
B29C39/025	10	{for making multilayered articles}	B29C39/02	B29C39/02		328
B29C39/026	9	{characterised by the shape of the surface}	B29C39/02	B29C39/02		622
B29C39/028	9	{having an axis of symmetry}	B29C39/02	B29C39/02		158
B29C39/04	9	using movable moulds (B29C41/02 takes precedence){not applied}	B29C39/04	B29C39/04		182
B29C39/06	10	continuously movable, e.g. along a production line	B29C39/06	B29C39/06		162
B29C39/08	10	Introducing the material into the mould by centrifugal force	B29C39/08	B29C39/08		219
B29C39/10	9	incorporating preformed parts or layers, e.g. casting around inserts or for coating articles {(coating a surface by casting in general B05D1/30, B29C39/126 takes precedence)}	B29C39/10	B29C39/10		3420
B29C39/12	9	Making multilayered or multicoloured articles {(B29C39/021 takes precedence)}	B29C39/12	B29C39/12		289
B29C39/123	10	{Making multilayered articles}	B29C39/12	B29C39/12		297
B29C39/126	11	{by casting between two preformed layers, e.g. deformable layers (between two glass layers B32B17/10917)}	B29C39/12	B29C39/12		109
B29C39/14	8	for making articles of indefinite length {(by depositing material on a substrate and stripping off the shaped article B29C41/24)}	B29C39/14	B29C39/14		179
B29C39/142	9	{by casting in serveral steps}	B29C39/14	B29C39/14		11
B29C39/144	10	{for making multicoloured articles}	B29C39/14	B29C39/14		1
B29C39/146	10	{for making multilayered articles}	B29C39/14	B29C39/14		24
B29C39/148	9	{characterised by the shape of the surface}	B29C39/14	B29C39/14		196
B29C39/16	9	between endless belts	B29C39/16	B29C39/16		103
B29C39/18	9	incorporating preformed parts or layers, e.g. casting around inserts or for coating articles {(B29C39/206 takes precedence)}	B29C39/18	B29C39/18		275
B29C39/20	9	Making multilayered or multicoloured articles {(B29C39/142 takes precedence)}	B29C39/20	B29C39/20		48
B29C39/203	10	{Making multilayered articles}	B29C39/20	B29C39/20		69
B29C39/206	11	{by casting between two preformed layers, e.g. deformable layers}	B29C39/20	B29C39/20		9
B29C39/22	8	Component parts, details or accessories; Auxiliary operations	B29C39/22	B29C39/22		1107
B29C39/24	9	Feeding the material into the mould	B29C39/24	B29C39/24		1334
B29C39/26	9	Moulds or cores	B29C39/26	B29C39/26		2000
B29C39/265	10	{comprising two large plates positioned at a small distance from each other, e.g. for making panels}	B29C39/26	B29C39/26		116
B29C39/28	10	with means to avoid flashes {(B29C39/30 takes precedence)}	B29C39/28	B29C39/28		43
B29C39/30	10	with means for cutting the article	B29C39/30	B29C39/30		68
B29C39/32	10	with joints or the like for making the mould impervious	B29C39/32	B29C39/32		72
B29C39/34	10	for undercut articles	B29C39/34	B29C39/34		134
B29C39/36	9	Removing moulded articles	B29C39/36	B29C39/36		780
B29C39/38	9	Heating or cooling	B29C39/38	B29C39/38		1211
B29C39/40	9	Compensating volume change, e.g. retraction {(in general B29C37/005)}	B29C39/40	B29C39/40		127
B29C39/405	10	{by applying pressure to the casting composition}	B29C39/40	B29C39/40		48
B29C39/42	9	Casting under special conditions, e.g. vacuum	B29C39/42	B29C39/42		1010
B29C39/44	9	Measuring, controlling or regulating	B29C39/44	B29C39/44		671
B29C41/00	7	Shaping by coating a mould, core or other substrate, i.e. by depositing material and stripping-off the shaped article; Apparatus therefor (with compacting pressure B29C43/00{; by lay-up of reinforcement of substantial or continuous length B29C70/30})	B29C41/00	B29C41/00		185
B29C41/003	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest	B29C41/00	B29C41/00		1336
B29C41/006	8	{using an electrostatic field for applying the material}	B29C41/00	B29C41/00		144
B29C41/02	8	for making articles of definite length, i.e. discrete articles	B29C41/02	B29C41/02		458
B29C41/025	9	{having hollow walls}	B29C41/02	B29C41/02		50
B29C41/04	9	Rotational or centrifugal casting, i.e. coating the inside of a mould by rotating the mould	B29C41/04	B29C41/04		1828
B29C41/042	10	{by rotating a mould around its axis of symmetry (for concrete B28B21/30)}	B29C41/04	B29C41/04		545
B29C41/045	11	{the axis being placed vertically, e.g. spin casting}	B29C41/04	B29C41/04		236
B29C41/047	11	{the mould cavity lying totally outside the axis, e.g. toroidal moulds}	B29C41/04	B29C41/04		38
B29C41/06	10	about two or more axes	B29C41/06	B29C41/06		779
B29C41/08	9	Coating a former, core or other substrate by spraying or fluidisation, e.g. spraying powder {(spray-up of reinforcing fibres B29C70/305)}	B29C41/08	B29C41/08		974
B29C41/085	10	{by rotating the former around its axis of symmetry}	B29C41/08	B29C41/08		200
B29C41/10	10	by fluidisation	B29C41/10	B29C41/10		117
B29C41/12	9	Spreading-out the material on a substrate {, e.g. on the surface of a liquid}	B29C41/12	B29C41/12		631
B29C41/14	9	Dipping a core {(B29C41/10 takes precedence)}	B29C41/14	B29C41/14		2732
B29C41/16	9	Slip casting, i.e. applying a slip or slurry on a perforated or porous or absorbent surface with the liquid being drained away	B29C41/16	B29C41/16		87
B29C41/18	9	Slush casting, i.e. pouring moulding material into a hollow mould with excess material being poured off	B29C41/18	B29C41/18		726
B29C41/20	9	incorporating preformed parts or layers, e.g. moulding inserts or for coating articles	B29C41/20	B29C41/20		1205
B29C41/22	9	Making multilayered or multicoloured articles	B29C41/22	B29C41/22		1244
B29C41/24	8	for making articles of indefinite length	B29C41/24	B29C41/24		750
B29C41/26	9	by depositing flowable material on a rotating drum	B29C41/26	B29C41/26		637
B29C41/265	10	{on the inside of the drum}	B29C41/26	B29C41/26		23
B29C41/28	9	by depositing flowable material on an endless belt	B29C41/28	B29C41/28		844
B29C41/30	9	incorporating preformed parts or layers, e.g. moulding around inserts or for coating articles	B29C41/30	B29C41/30		326
B29C41/32	9	Making multilayered or multicoloured articles	B29C41/32	B29C41/32		371
B29C41/34	8	Component parts, details or accessories; Auxiliary operations	B29C41/34	B29C41/34		1354
B29C41/36	9	Feeding the material on to the mould, core or other substrate	B29C41/36	B29C41/36		1004
B29C41/365	10	{Construction of spray-up equipment, e.g. spray-up guns (spraying apparatus in general B05B)}	B29C41/36	B29C41/36		199
B29C41/38	9	Moulds, cores or other substrates	B29C41/38	B29C41/38		960
B29C41/383	10	{with means for cutting the article}	B29C41/38	B29C41/38		34
B29C41/386	10	{for undercut articles}	B29C41/38	B29C41/38		73
B29C41/40	10	Cores	B29C41/40	B29C41/40		251
B29C41/42	9	Removing articles from moulds, cores or other substrates {(B29C33/444 and B29C37/0017 take precedence)}	B29C41/42	B29C41/42		620
B29C41/44	10	Articles of indefinite length	B29C41/44	B29C41/44		118
B29C41/46	9	Heating or cooling	B29C41/46	B29C41/46		1604
B29C41/48	9	Compensating volume change, e.g. retraction	B29C41/48	B29C41/48		30
B29C41/50	9	Shaping under special conditions, e.g. vacuum	B29C41/50	B29C41/50		247
B29C41/52	9	Measuring, controlling or regulating	B29C41/52	B29C41/52		811
B29C43/00	7	Compression moulding, i.e. applying external pressure to flow the moulding material; Apparatus therefor {(by liberation of internal stresses B29C61/006)}	B29C43/00	B29C43/00		3067
B29C43/003	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest	B29C43/00	B29C43/00		3227
B29C43/006	8	{Pressing and sintering powders, granules or fibres}	B29C43/00	B29C43/00		1390
B29C43/02	8	of articles of definite length, i.e. discrete articles {(B29C35/0227 takes precedence)}	B29C43/02	B29C43/02		4395
B29C43/021	9	{characterised by the shape of the surface}	B29C43/02	B29C43/02		2276
B29C2043/022	10	{having locally depressed lines, e.g. hinges}	B29C43/02	B29C43/02		84
B29C2043/023	10	{having a plurality of grooves}	B29C43/02	B29C43/02		418
B29C2043/024	11	{forming a threaded surface}	B29C43/02	B29C43/02		21
B29C2043/025	11	{forming a microstructure, i.e. fine patterning}	B29C43/02	B29C43/02		470
B29C2043/026	10	{having functional projections, e.g. fasteners}	B29C43/02	B29C43/02		84
B29C43/027	9	{having an axis of symmetry (B29C43/102 takes precedence)}	B29C43/02	B29C43/02		538
B29C2043/028	10	{using radial compression}	B29C43/02	B29C43/02		49
B29C2043/029	10	{using axial compression along a longitudinal axis}	B29C43/02	B29C43/02		82
B29C43/04	9	using movable moulds	B29C43/04	B29C43/04		682
B29C2043/043	10	{rotating on their own axis without linear displacement}	B29C43/04	B29C43/04		124
B29C2043/046	10	{travelling between different stations, e.g. feeding, moulding, curing stations}	B29C43/04	B29C43/04		241
B29C43/06	10	continuously movable {in one direction, e.g. mounted on chains, belts}	B29C43/06	B29C43/06		283
B29C43/08	11	with circular movement {, e.g. mounted on rolls, turntables}	B29C43/08	B29C43/08		776
B29C43/085	12	{and material fed in a continuous form, e.g. as a band}	B29C43/08	B29C43/08		81
B29C43/10	9	Isostatic pressing, i.e. using non-rigid pressure-exerting members against rigid parts or dies	B29C43/10	B29C43/10		683
B29C43/102	10	{using rigid mould parts specially adapted for moulding articles having an axis of symmetry}	B29C43/10	B29C43/10		65
B29C43/104	11	{the mould cavity lying totally outside the axis of symmetry, e.g. toroidal moulds}	B29C43/10	B29C43/10		92
B29C2043/106	10	{using powder material}	B29C43/10	B29C43/10		48
B29C2043/108	10	{using deformable metals, e.g. flowable metals, low melting point eutectic metals, liquified metals}	B29C43/10	B29C43/10		12
B29C43/12	10	using bags surrounding the moulding material {or using membranes contacting the moulding material}	B29C43/12	B29C43/12		1484
B29C43/14	9	in several steps	B29C43/14	B29C43/14		647
B29C2043/141	10	{for making single layer articles}	B29C43/14	B29C43/14		51
B29C2043/142	11	{by moving a single mould or the article progressively, i.e. portionwise}	B29C43/14	B29C43/14		44
B29C2043/143	11	{stepwise in a vertical direction, i.e. each time modifying the thickness}	B29C43/14	B29C43/14		12
B29C2043/144	11	{using different moulds, i.e. the layer is compressed in consecutive steps by using different moulds for each portion of the article}	B29C43/14	B29C43/14		38
B29C43/145	10	{for making multicoloured articles}	B29C43/14	B29C43/14		87
B29C43/146	10	{for making multilayered articles}	B29C43/14	B29C43/14		532
B29C2043/147	11	{by compressing after the laying of further material}	B29C43/14	B29C43/14		92
B29C2043/148	11	{using different moulds}	B29C43/14	B29C43/14		75
B29C43/16	9	Forging	B29C43/16	B29C43/16		213
B29C43/18	9	incorporating preformed parts or layers, e.g. compression moulding around inserts or for coating articles {(B29C43/206 takes precedence)}	B29C43/18	B29C43/18		3871
B29C2043/181	10	{encapsulated}	B29C43/18	B29C43/18		230
B29C2043/182	11	{completely}	B29C43/18	B29C43/18		173
B29C43/183	10	{the preformed layer being a lining, e.g. shaped in the mould before compression moulding, or a preformed shell adapted to the shape of the mould}	B29C43/18	B29C43/18		385
B29C43/184	11	{shaped by the compression of the material during moulding}	B29C43/18	B29C43/18		277
B29C2043/185	10	{using adhesives}	B29C43/18	B29C43/18		172
B29C2043/186	11	{hot-melt or heat activated adhesives}	B29C43/18	B29C43/18		77
B29C2043/187	11	{pressure activated or pressure sensitive adhesives}	B29C43/18	B29C43/18		11
B29C2043/188	11	{thermosetting adhesives, e.g.&#160;polyurethane adhesives}	B29C43/18	B29C43/18		43
B29C2043/189	10	{the parts being joined}	B29C43/18	B29C43/18		260
B29C43/20	9	Making multilayered or multicoloured articles {(B29C43/14 takes precedence)}	B29C43/20	B29C43/20		500
B29C43/203	10	{Making multilayered articles}	B29C43/20	B29C43/20		1471
B29C43/206	11	{by pressing the material between two preformed layers, e.g. deformable layers}	B29C43/20	B29C43/20		227
B29C43/22	8	of articles of indefinite length	B29C43/22	B29C43/22		1161
B29C43/222	9	{characterised by the shape of the surface}	B29C43/22	B29C43/22		1260
B29C43/224	9	{having a profiled section, e.g. tubes, rods}	B29C43/22	B29C43/22		211
B29C43/226	10	{having a corrugated section}	B29C43/22	B29C43/22		45
B29C43/228	9	{using endless belts feeding the material between non-rotating pressure members, e.g. vibrating pressure members}	B29C43/22	B29C43/22		164
B29C43/24	9	Calendering	B29C43/24	B29C43/24		3163
B29C43/245	10	{Adjusting calender parameters, e.g. bank quantity}	B29C43/24	B29C43/24		341
B29C43/26	9	in several steps (B29C43/30 takes precedence {not applied})	B29C43/26	B29C43/26		129
B29C43/265	10	{for making multilayered articles}	B29C43/26	B29C43/26		58
B29C43/28	9	incorporating preformed parts or layers, e.g. compression moulding around inserts or for coating articles	B29C43/28	B29C43/28		779
B29C43/30	9	Making multilayered or multicoloured articles {(B29C43/26 takes precedence)}	B29C43/30	B29C43/30		314
B29C43/305	10	{Making multilayered articles}	B29C43/30	B29C43/30		598
B29C43/32	8	Component parts, details or accessories; Auxiliary operations	B29C43/32	B29C43/32		2605
B29C2043/3205	9	{Particular pressure exerting means for making definite articles}	B29C43/32	B29C43/32		137
B29C2043/3211	10	{magnets}	B29C43/32	B29C43/32		26
B29C2043/3216	10	{deformable nets, meshes, lattices or fabrics, e.g. tubular ones}	B29C43/32	B29C43/32		16
B29C2043/3222	10	{pressurized gas, e.g. air}	B29C43/32	B29C43/32		96
B29C2043/3227	11	{inside the material, e.g. gas injection compression moulding}	B29C43/32	B29C43/32		20
B29C2043/3233	11	{exerting pressure on mould parts}	B29C43/32	B29C43/32		89
B29C2043/3238	10	{pressurized liquid acting directly or indirectly on the material to be formed}	B29C43/32	B29C43/32		80
B29C2043/3244	10	{retraction of an expanded member}	B29C43/32	B29C43/32		4
B29C2043/325	10	{screws}	B29C43/32	B29C43/32		16
B29C2043/3255	10	{springs}	B29C43/32	B29C43/32		61
B29C2043/3261	10	{thermal expansion}	B29C43/32	B29C43/32		38
B29C2043/3266	10	{vibrating tool means}	B29C43/32	B29C43/32		68
B29C2043/3272	9	{driving means}	B29C43/32	B29C43/32		238
B29C2043/3277	10	{for rotatable suports, e.g. carousels, drums}	B29C43/32	B29C43/32		47
B29C2043/3283	10	{for moving moulds or mould parts}	B29C43/32	B29C43/32		319
B29C2043/3288	11	{using cam drives}	B29C43/32	B29C43/32		108
B29C2043/3294	11	{using screw drives}	B29C43/32	B29C43/32		11
B29C43/34	9	Feeding the material to the mould or the compression means {(B29C43/085 takes precedence)}	B29C43/34	B29C43/34		2862
B29C2043/3405	10	{using carrying means}	B29C43/34	B29C43/34		146
B29C2043/3411	11	{mounted onto arms, e.g. grippers, fingers, clamping frame, suction means}	B29C43/34	B29C43/34		161
B29C2043/3416	11	{conveyor belts}	B29C43/34	B29C43/34		184
B29C2043/3422	11	{rollers}	B29C43/34	B29C43/34		148
B29C2043/3427	11	{hopper, vessel, chute, tube, conveying screw, for material in discrete form, e.g.&#160;particles or powder or fibres}	B29C43/34	B29C43/34		259
B29C2043/3433	10	{using dispensing heads, e.g.&#160;extruders, placed over or apart from the moulds}	B29C43/34	B29C43/34		549
B29C2043/3438	11	{moving during dispensing over the moulds, e.g.&#160;laying up}	B29C43/34	B29C43/34		104
B29C2043/3444	10	{using pressurising feeding means located in the mould, e.g.&#160;plungers or pistons}	B29C43/34	B29C43/34		232
B29C2043/345	10	{using gas, e.g. air, to transport non liquid material}	B29C43/34	B29C43/34		18
B29C2043/3455	11	{for particles, powder, fibres, e.g. fluidized or sprayed}	B29C43/34	B29C43/34		56
B29C2043/3461	11	{for foils, sheets, gobs, e.g. floated}	B29C43/34	B29C43/34		35
B29C2043/3466	10	{using rotating supports, e.g.&#160;turntables or drums}	B29C43/34	B29C43/34		171
B29C2043/3472	11	{using star wheels comprising arms}	B29C43/34	B29C43/34		47
B29C2043/3477	10	{centrally fed, e.g.&#160;feeding the material in the center of the mould turntables}	B29C43/34	B29C43/34		19
B29C2043/3483	10	{using band or film carriers}	B29C43/34	B29C43/34		64
B29C2043/3488	10	{uniformly distributed into the mould}	B29C43/34	B29C43/34		135
B29C2043/3494	11	{using vibrating means}	B29C43/34	B29C43/34		80
B29C43/36	9	Moulds for making articles of definite length, i.e. discrete articles	B29C43/36	B29C43/36		3635
B29C2043/3602	10	{with means for positioning, fastening or clamping the material to be formed or preforms inside the mould}	B29C43/36	B29C43/36		452
B29C2043/3605	11	{vacuum}	B29C43/36	B29C43/36		115
B29C43/3607	10	{with sealing means or the like}	B29C43/36	B29C43/36		262
B29C43/361	10	{with pressing members independently movable of the parts for opening or closing the mould, e.g. movable pistons (transfer moulding B29C45/02; injection-compression moulding B29C45/561)}	B29C43/36	B29C43/36		872
B29C2043/3613	11	{applying pressure locally}	B29C43/36	B29C43/36		154
B29C2043/3615	11	{Forming elements, e.g.&#160;mandrels or rams or stampers or pistons or plungers or punching devices}	B29C43/36	B29C43/36		506
B29C2043/3618	12	{plurality of counteracting elements}	B29C43/36	B29C43/36		299
B29C2043/3621	12	{a plurality of individual elements acting on the material in the same or diferent directions, e.g. making tubular T-joints, profiles}	B29C43/36	B29C43/36		78
B29C2043/3623	13	{coupled on a support, e.g. plate}	B29C43/36	B29C43/36		98
B29C2043/3626	12	{multi-part rams, plungers or mandrels}	B29C43/36	B29C43/36		97
B29C2043/3628	12	{moving inside a barrel or container like sleeve}	B29C43/36	B29C43/36		111
B29C2043/3631	12	{moving in a frame for pressing and stretching; material being subjected to compressing stretching}	B29C43/36	B29C43/36		65
B29C2043/3634	12	{having specific surface shape, e.g. grooves, projections, corrugations}	B29C43/36	B29C43/36		155
B29C2043/3636	11	{ultrasonically or sonically vibrating, e.g. sonotrodes}	B29C43/36	B29C43/36		54
B29C2043/3639	11	{hand operated}	B29C43/36	B29C43/36		26
B29C43/3642	10	{Bags, bleeder sheets or cauls for isostatic pressing}	B29C43/36	B29C43/36		756
B29C2043/3644	11	{Vacuum bags; Details thereof, e.g.&#160;fixing or clamping}	B29C43/36	B29C43/36		387
B29C2043/3647	11	{Membranes, diaphragms}	B29C43/36	B29C43/36		129
B29C2043/3649	11	{Inflatable bladders using gas or fluid and related details}	B29C43/36	B29C43/36		252
B29C2043/3652	11	{Elastic moulds or mould parts, e.g.&#160;cores or inserts}	B29C43/36	B29C43/36		201
B29C2043/3655	11	{Pressure transmitters, e.g.&#160;caul plates; pressure pads}	B29C43/36	B29C43/36		125
B29C2043/3657	11	{additional materials, e.g. permeable bleeder or breather sheets, cloths, blankets}	B29C43/36	B29C43/36		54
B29C2043/366	10	{plates pressurized by an actuator, e.g. ram drive, screw, vulcanizing presses}	B29C43/36	B29C43/36		90
B29C2043/3663	11	{confined in a chamber}	B29C43/36	B29C43/36		11
B29C2043/3665	10	{cores or inserts, e.g. pins, mandrels, sliders}	B29C43/36	B29C43/36		359
B29C2043/3668	11	{destructible or fusible}	B29C43/36	B29C43/36		40
B29C2043/3671	10	{preforms constituing part of the cavity mould wall}	B29C43/36	B29C43/36		4
B29C2043/3673	11	{preform constituting a mould half}	B29C43/36	B29C43/36		10
B29C2043/3676	10	{moulds mounted on rotating supporting constuctions}	B29C43/36	B29C43/36		53
B29C2043/3678	11	{on cylindrical supports with moulds or mould cavities provided on the periphery}	B29C43/36	B29C43/36		55
B29C2043/3681	12	{opening and closing axially, i.e. parallel to the rotation axis}	B29C43/36	B29C43/36		22
B29C2043/3684	12	{opening/closing or acting radially, i.e. vertical to the rotation axis}	B29C43/36	B29C43/36		53
B29C2043/3686	12	{opening and closing tangential to the rotation, i.e. vertical to the rotation axis and vertical to the radius}	B29C43/36	B29C43/36		3
B29C2043/3689	11	{on a support table, e.g. flat disk-like tables having moulds on the periphery}	B29C43/36	B29C43/36		235
B29C2043/3692	12	{cooperating with non rotating parts}	B29C43/36	B29C43/36		19
B29C2043/3694	11	{on rotating star wheels}	B29C43/36	B29C43/36		8
B29C43/3697	10	{comprising rollers or belts cooperating with non-rotating mould parts}	B29C43/36	B29C43/36		135
B29C43/38	10	with means to avoid flashes {(B29C43/40 takes precedence)}	B29C43/38	B29C43/38		192
B29C43/40	10	with means for cutting the article	B29C43/40	B29C43/40		492
B29C2043/403	11	{knife blades}	B29C43/40	B29C43/40		119
B29C2043/406	11	{laser cutting means}	B29C43/40	B29C43/40		13
B29C43/42	10	for undercut articles	B29C43/42	B29C43/42		399
B29C2043/425	11	{mould parts or sliders being movable independently from the mould halves for making undercut portions}	B29C43/42	B29C43/42		39
B29C43/44	9	Compression means for making articles of indefinite length	B29C43/44	B29C43/44		165
B29C43/46	10	Rollers	B29C43/46	B29C43/46		1325
B29C2043/461	11	{the rollers having specific surface features}	B29C43/46	B29C43/46		243
B29C2043/462	12	{smooth surface}	B29C43/46	B29C43/46		21
B29C2043/463	12	{corrugated, patterned or embossed surface}	B29C43/46	B29C43/46		322
B29C2043/464	12	{having projections or knives, e.g. for cutting-out or for forming local depressions}	B29C43/46	B29C43/46		114
B29C2043/465	12	{having one or more cavities, e.g. for forming distinct products}	B29C43/46	B29C43/46		198
B29C2043/466	11	{the rollers having specific shape, e.g. non cylindrical rollers, conical rollers}	B29C43/46	B29C43/46		62
B29C2043/467	11	{plurality of rollers arranged in a specific manner in relation to each other}	B29C43/46	B29C43/46		155
B29C2043/468	11	{take-off rollers, i.e.&#160;arranged adjacent a material feeding device}	B29C43/46	B29C43/46		53
B29C43/48	10	Endless belts	B29C43/48	B29C43/48		339
B29C2043/483	11	{cooperating with a second endless belt, i.e. double band presses}	B29C43/48	B29C43/48		330
B29C2043/486	11	{cooperating with rollers or drums}	B29C43/48	B29C43/48		150
B29C43/50	9	Removing moulded articles	B29C43/50	B29C43/50		1742
B29C2043/5007	10	{using cores, i.e. the cores forming part of the mould cavity}	B29C43/50	B29C43/50		49
B29C2043/5015	11	{having undercuts or being threaded}	B29C43/50	B29C43/50		17
B29C2043/5023	11	{moving away}	B29C43/50	B29C43/50		13
B29C2043/503	10	{using ejector pins, rods}	B29C43/50	B29C43/50		354
B29C2043/5038	11	{having an annular or tubular shape}	B29C43/50	B29C43/50		20
B29C2043/5046	10	{using vacuum}	B29C43/50	B29C43/50		72
B29C2043/5053	10	{using pressurised gas, e.g. air}	B29C43/50	B29C43/50		111
B29C2043/5061	10	{using means movable from outside the mould between mould parts}	B29C43/50	B29C43/50		71
B29C2043/5069	11	{take-off members or carriers for the moulded articles, e.g. grippers}	B29C43/50	B29C43/50		60
B29C2043/5076	10	{using belts}	B29C43/50	B29C43/50		60
B29C2043/5084	10	{using rotary devices, e.g.&#160;turntables or carousels}	B29C43/50	B29C43/50		72
B29C2043/5092	10	{using vibrations means}	B29C43/50	B29C43/50		19
B29C43/52	9	Heating or cooling	B29C43/52	B29C43/52		4089
B29C2043/522	10	{selectively heating a part of the mould to achieve partial heating, differential heating}	B29C43/52	B29C43/52		97
B29C2043/525	10	{at predetermined points for local melting, curing or bonding}	B29C43/52	B29C43/52		83
B29C2043/527	10	{selectively cooling, e.g. locally, on the surface of the material}	B29C43/52	B29C43/52		95
B29C43/54	9	Compensating volume change, e.g. retraction	B29C43/54	B29C43/54		115
B29C43/56	9	Compression moulding under special conditions, e.g. vacuum	B29C43/56	B29C43/56		824
B29C2043/561	10	{under vacuum conditions}	B29C43/56	B29C43/56		345
B29C2043/562	11	{combined with isostatic pressure, e.g. pressurising fluids, gases}	B29C43/56	B29C43/56		37
B29C2043/563	11	{combined with mechanical pressure, i.e. mould plates, rams, stampers}	B29C43/56	B29C43/56		98
B29C2043/565	10	{in a clean sterile environment, e.g. to avoid contamination}	B29C43/56	B29C43/56		11
B29C2043/566	10	{in a specific gas atmosphere, with or without pressure}	B29C43/56	B29C43/56		95
B29C2043/567	10	{in a liquid, i.e. the moulded parts being embedded in liquid}	B29C43/56	B29C43/56		14
B29C2043/568	10	{in a magnetic or electric field}	B29C43/56	B29C43/56		40
B29C43/58	9	Measuring, controlling or regulating {(for bank adjustment in calendering B29C43/245)}	B29C43/58	B29C43/58		2657
B29C2043/5808	10	{pressure or compressing force}	B29C43/58	B29C43/58		970
B29C2043/5816	10	{temperature}	B29C43/58	B29C43/58		1190
B29C2043/5825	10	{dimensions or shape, e.g. size, thickness}	B29C43/58	B29C43/58		265
B29C2043/5833	10	{movement of moulds or mould parts, e.g. opening or closing, actuating}	B29C43/58	B29C43/58		345
B29C2043/5841	11	{for accommodating variation in mould spacing or cavity volume during moulding}	B29C43/58	B29C43/58		116
B29C2043/585	10	{detecting defects, e.g. foreign matter between the moulds, inaccurate position, breakage}	B29C43/58	B29C43/58		98
B29C2043/5858	11	{for preventing tilting of movable mould plate during closing or clamping}	B29C43/58	B29C43/58		29
B29C2043/5866	10	{ejection of moulded articles}	B29C43/58	B29C43/58		22
B29C2043/5875	10	{the material feed to the moulds or mould parts, e.g. controlling feed flow, velocity, weight, doses}	B29C43/58	B29C43/58		203
B29C2043/5883	11	{ensuring cavity filling, e.g. providing overflow means}	B29C43/58	B29C43/58		78
B29C2043/5891	10	{using imaging devices, e.g. cameras}	B29C43/58	B29C43/58		74
B29C44/00	7	Shaping by internal pressure generated in the material, e.g. swelling or foaming {; Producing porous or cellular expanded plastics articles}	B29C44/00	B29C44/00		759
B29C44/005	8	{Avoiding skin formation; Making foams with porous surfaces}	B29C44/00	B29C44/00		80
B29C44/02	8	for articles of definite length, i.e. discrete articles	B29C44/02	B29C44/02		1897
B29C44/022	9	{Foaming unrestricted by cavity walls, e.g. without using moulds or using only internal cores}	B29C44/02	B29C44/02		220
B29C44/025	9	{Foaming in open moulds, followed by closing the moulds}	B29C44/02	B29C44/02		68
B29C44/027	9	{the foaming continuing or beginning when the mould is opened}	B29C44/02	B29C44/02		80
B29C44/04	9	consisting of at least two parts of chemically or physically different materials, e.g. having different densities	B29C44/04	B29C44/04		751
B29C44/0407	10	{by regulating the temperature of the mould or parts thereof, e.g. cold mould walls inhibiting foaming of an outer layer}	B29C44/04	B29C44/04		335
B29C44/0415	10	{by regulating the pressure of the material during or after filling of the mould, e.g. by local venting}	B29C44/04	B29C44/04		173
B29C44/0423	10	{by density separation}	B29C44/04	B29C44/04		9
B29C44/043	11	{using a rotating mould}	B29C44/04	B29C44/04		76
B29C44/0438	11	{using flotation}	B29C44/04	B29C44/04		1
B29C44/0446	10	{by increasing the density locally by compressing part of the foam while still in the mould}	B29C44/04	B29C44/04		90
B29C44/0453	10	{by joining the different materials using compression moulding before the foaming step}	B29C44/04	B29C44/04		7
B29C44/0461	10	{by having different chemical compositions in different places, e.g. having different concentrations of foaming agent, feeding one composition after the other}	B29C44/04	B29C44/04		517
B29C44/0469	11	{provided with physical separators between the different materials, e.g. separating layers, mould walls}	B29C44/04	B29C44/04		136
B29C44/0476	11	{by pouring more than one composition into an open mould}	B29C44/04	B29C44/04		58
B29C44/0484	10	{by having different solubility of the foaming agent}	B29C44/04	B29C44/04		7
B29C44/0492	10	{Devices for feeding the different materials}	B29C44/04	B29C44/04		135
B29C44/06	10	Making multilayered articles {(B29C44/0407 - B29C44/0492 take precedence)}	B29C44/06	B29C44/06		537
B29C44/065	11	{comprising at least one barrier layer}	B29C44/06	B29C44/06		48
B29C44/08	9	using several expanding {or moulding} steps	B29C44/08	B29C44/08		609
B29C44/083	10	{Increasing the size of the cavity after a first part has foamed, e.g. substituting one mould part with another}	B29C44/08	B29C44/08		89
B29C44/086	11	{and feeding more material into the enlarged cavity}	B29C44/08	B29C44/08		240
B29C44/10	9	Applying counter-pressure during expanding	B29C44/10	B29C44/10		627
B29C44/105	10	{the counterpressure being exerted by a fluid}	B29C44/10	B29C44/10		147
B29C44/12	9	Incorporating or moulding on preformed parts, e.g. inserts or reinforcements	B29C44/12	B29C44/12		2097
B29C44/1204	10	{and giving the material during expanding the shape of a particular article to be supported, e.g. a human body-part}	B29C44/12	B29C44/12		76
B29C44/1209	10	{by impregnating a preformed part, e.g. a porous lining}	B29C44/12	B29C44/12		384
B29C44/1214	10	{Anchoring by foaming into a preformed part, e.g. by penetrating through holes (anchoring by moulding in general B29C37/0078; outsert moulding B29C45/14344, B29C70/74)}	B29C44/12	B29C44/12		228
B29C44/1219	10	{Foaming between a movable mould part and the preformed part}	B29C44/12	B29C44/12		141
B29C44/1223	10	{Joining preformed parts which have previously been filled with foam}	B29C44/12	B29C44/12		52
B29C44/1228	10	{Joining preformed parts by the expanding material}	B29C44/12	B29C44/12		595
B29C44/1233	11	{the preformed parts being supported during expanding}	B29C44/12	B29C44/12		396
B29C44/1238	12	{and having flexible and solid areas}	B29C44/12	B29C44/12		91
B29C44/1242	11	{the preformed parts being concentric (B29C44/1233 takes precedence)}	B29C44/12	B29C44/12		208
B29C44/1247	12	{comprising dams or sealing arrangements}	B29C44/12	B29C44/12		56
B29C44/1252	10	{Removing portions of the preformed parts after the moulding step}	B29C44/12	B29C44/12		87
B29C44/1257	10	{Joining a preformed part and a lining, e.g. around the edges}	B29C44/12	B29C44/12		269
B29C44/1261	10	{Avoiding impregnation of a preformed part}	B29C44/12	B29C44/12		162
B29C44/1266	10	{the preformed part being completely encapsulated, e.g. for packaging purposes or as reinforcement}	B29C44/12	B29C44/12		421
B29C44/1271	10	{the preformed parts being partially covered}	B29C44/12	B29C44/12		805
B29C44/1276	10	{the preformed parts being three dimensional structures which are wholly or partially penetrated by the foam}	B29C44/12	B29C44/12		99
B29C44/128	10	{Internally reinforcing constructional elements, e.g. beams}	B29C44/12	B29C44/12		104
B29C44/1285	10	{the preformed part being foamed}	B29C44/12	B29C44/12		245
B29C44/129	10	{Enhancing adhesion to the preformed part using an interlayer}	B29C44/12	B29C44/12		75
B29C44/1295	10	{Foaming around pipe joints}	B29C44/12	B29C44/12		48
B29C44/14	10	the preformed part being a lining {(B29C44/1209 takes precedence)}	B29C44/14	B29C44/14		1329
B29C44/141	11	{Hiding joints in the lining}	B29C44/14	B29C44/14		95
B29C44/143	11	{Means for positioning the lining in the mould (in general B29C33/12)}	B29C44/14	B29C44/14		233
B29C44/145	11	{the lining being a laminate}	B29C44/14	B29C44/14		198
B29C44/146	11	{Shaping the lining before foaming}	B29C44/14	B29C44/14		508
B29C44/148	11	{Applying the foaming resin, moulding the lining or the like, with the lining turned inside out}	B29C44/14	B29C44/14		25
B29C44/16	11	shaped by the expansion of the material	B29C44/16	B29C44/16		285
B29C44/18	10	Filling preformed cavities {(B29C44/1204 takes precedence)}	B29C44/18	B29C44/18		1050
B29C44/181	11	{Filling unsupported soft shells having a particular shape}	B29C44/18	B29C44/18		55
B29C44/182	11	{Filling flexible bags not having a particular shape}	B29C44/18	B29C44/18		112
B29C44/183	12	{the components being kept apart in different containers within the bag, and mixed upon rupture of the containers (B29C44/184 takes precedence)}	B29C44/18	B29C44/18		26
B29C44/184	12	{and inserting the bags into preformed cavities}	B29C44/18	B29C44/18		57
B29C44/185	13	{Starting the expansion after rupturing or dissolving the bag}	B29C44/18	B29C44/18		34
B29C44/186	11	{Filling multiple cavities (B29C44/181, B29C44/182 and B29C44/188 takes precedence)}	B29C44/18	B29C44/18		162
B29C44/187	11	{Filling faulty voids in the foam}	B29C44/18	B29C44/18		21
B29C44/188	11	{Sealing off parts of the cavities}	B29C44/18	B29C44/18		220
B29C44/20	8	for articles of indefinite length	B29C44/20	B29C44/20		282
B29C44/203	9	{Expanding the moulding material in a vertical channel}	B29C44/20	B29C44/20		39
B29C44/206	9	{Using expandable particles or beads as starting material}	B29C44/20	B29C44/20		155
B29C44/22	9	consisting of at least two parts of chemically or physically different materials, e.g. having different densities	B29C44/22	B29C44/22		444
B29C44/24	10	Making multilayered articles	B29C44/24	B29C44/24		255
B29C44/26	9	using several expanding steps	B29C44/26	B29C44/26		111
B29C44/28	9	Expanding the moulding material on continuous moving surfaces {without restricting the upwards growth of the foam}	B29C44/28	B29C44/28		296
B29C44/285	10	{Rising trough lateral side members, e.g. following the foam expansion}	B29C44/28	B29C44/28		3
B29C44/30	9	Expanding the moulding material between endless belts or rollers {(B29C44/203 takes precedence)}	B29C44/30	B29C44/30		591
B29C44/302	10	{Expanding the moulding material in flexible endless moulds}	B29C44/30	B29C44/30		36
B29C44/304	10	{Adjusting the belt or roller pressure}	B29C44/30	B29C44/30		35
B29C44/306	10	{Longitudinally shaping, e.g. the belt}	B29C44/30	B29C44/30		63
B29C44/308	10	{Thickness separators and side seals}	B29C44/30	B29C44/30		50
B29C44/32	9	Incorporating or moulding on preformed parts, e.g. linings, inserts or reinforcements	B29C44/32	B29C44/32		169
B29C44/321	10	{the preformed part being a lining, e.g. a film or a support lining}	B29C44/32	B29C44/32		310
B29C44/3215	11	{Folding devices for the lining}	B29C44/32	B29C44/32		64
B29C44/322	10	{the preformed parts being elongated inserts, e.g. cables}	B29C44/32	B29C44/32		226
B29C44/324	11	{the preformed parts being tubular or folded to a tubular shape}	B29C44/32	B29C44/32		292
B29C44/326	10	{Joining the preformed parts, e.g. to make flat or profiled sandwich laminates}	B29C44/32	B29C44/32		474
B29C44/328	10	{the foamable components being mixed in the nip between the preformed parts}	B29C44/32	B29C44/32		30
B29C44/329	10	{the preformed parts being partially embedded}	B29C44/32	B29C44/32		96
B29C44/332	10	{the preformed parts being three-dimensional structures}	B29C44/32	B29C44/332		110
B29C44/334	10	{Filling the preformed spaces or cavities}	B29C44/32	B29C44/334		125
B29C44/34	8	Auxiliary operations	B29C44/34	B29C44/34		1026
B29C44/3402	9	{Details of processes or apparatus for reducing environmental damage or for working-up compositions comprising inert blowing agents or biodegradable components}	B29C44/34	B29C44/34		145
B29C44/3403	9	{Foaming under special conditions, e.g. in sub-atmospheric pressure, in or on a liquid}	B29C44/34	B29C44/34		483
B29C44/3407	10	{Vacuum extrusion using underwater barometric leg}	B29C44/34	B29C44/34		32
B29C44/3411	9	{Relieving stresses}	B29C44/34	B29C44/34		42
B29C44/3415	9	{Heating or cooling}	B29C44/34	B29C44/34		1877
B29C44/3419	10	{Quick cooling}	B29C44/34	B29C44/34		165
B29C44/3423	10	{by using a heated or cooled preformed part, e.g. in the mould}	B29C44/34	B29C44/34		54
B29C44/3426	10	{Heating by introducing steam in the mould}	B29C44/34	B29C44/34		1350
B29C44/343	11	{by using pipes to direct the steam inside the mould}	B29C44/34	B29C44/34		114
B29C44/3434	11	{by using a sheet, grid, etc. to distribute the steam in the mould}	B29C44/34	B29C44/34		38
B29C44/3438	9	{Bursting the cell walls by a sudden pressure release}	B29C44/34	B29C44/34		23
B29C44/3442	9	{Mixing, kneading or conveying the foamable material (mixing plastics B29B7/00; mixing in general B01F)}	B29C44/34	B29C44/34		1826
B29C44/3446	10	{Feeding the blowing agent}	B29C44/34	B29C44/34		735
B29C44/3449	11	{through the screw}	B29C44/34	B29C44/34		85
B29C44/3453	11	{Feeding the blowing agent to solid plastic material}	B29C44/34	B29C44/34		255
B29C44/3457	11	{Feeding the blowing agent in solid form to the plastic material}	B29C44/34	B29C44/34		27
B29C44/3461	9	{Making or treating expandable particles}	B29C44/34	B29C44/34		896
B29C44/3465	10	{by compressing particles in vacuum, followed by expansion in normal pressure}	B29C44/34	B29C44/34		17
B29C44/3469	9	{Cell or pore nucleation}	B29C44/34	B29C44/34		60
B29C44/3473	10	{by shearing forces}	B29C44/34	B29C44/34		22
B29C44/3476	10	{by, e.g. compression stress}	B29C44/34	B29C44/34		8
B29C44/348	10	{by regulating the temperature and/or the pressure, e.g. suppression of foaming until the pressure is rapidly decreased}	B29C44/34	B29C44/34		367
B29C44/3484	9	{Stopping the foaming reaction until the material is heated or re-heated}	B29C44/34	B29C44/34		122
B29C44/3488	9	{Vulcanizing the material before foaming}	B29C44/34	B29C44/34		51
B29C44/3492	9	{Expanding without a foaming agent}	B29C44/34	B29C44/34		38
B29C44/3496	10	{The foam being compressed and later released to expand (B29C44/3465 takes precedence)}	B29C44/34	B29C44/34		53
B29C44/35	9	{Component parts; Details or accessories}	B29C44/34	B29C44/35		1188
B29C44/351	10	{Means for preventing foam to leak out from the foaming device during foaming}	B29C44/34	B29C44/35		424
B29C44/352	10	{Means for giving the foam different characteristics in different directions}	B29C44/34	B29C44/35		106
B29C44/353	10	{Means for guiding the foaming in, e.g. a particular direction}	B29C44/34	B29C44/35		25
B29C44/354	10	{Means to prevent or reduce the effect of shrinking of the foamed article}	B29C44/34	B29C44/35		17
B29C44/355	10	{Characteristics of the foam, e.g. having particular surface properties or structure}	B29C44/34	B29C44/35		102
B29C44/356	11	{having a porous surface}	B29C44/34	B29C44/35		23
B29C44/357	11	{Auxetic foams, i.e. material with negative Poisson ratio; anti rubber; dilatational; re-entrant}	B29C44/34	B29C44/35		56
B29C44/358	11	{Foamed of foamable fibres}	B29C44/34	B29C44/35		27
B29C44/36	9	Feeding the material to be shaped {(B29C44/0492 takes precedence)}	B29C44/36	B29C44/36		305
B29C44/362	10	{Regulating the feed w.r.t. the foam layer thickness}	B29C44/36	B29C44/36		40
B29C44/365	10	{using elongate feed conduits provided with throttle devices}	B29C44/36	B29C44/36		30
B29C44/367	10	{using spray nozzles}	B29C44/36	B29C44/36		207
B29C44/38	10	into a closed space, i.e. to make articles of definite length {(B29C44/365 and B29C44/367 take precedence)}	B29C44/38	B29C44/38		355
B29C44/381	11	{Spreading the foamable material in the mould by pressing the mould halves together}	B29C44/38	B29C44/38		22
B29C44/383	11	{using spreading devices mounted in the mould, in front of the feed opening}	B29C44/38	B29C44/38		52
B29C44/385	11	{using manifolds or channels directing the flow in the mould}	B29C44/38	B29C44/38		101
B29C44/386	12	{using a movable, elongate nozzle, e.g. to reach deep into the mould}	B29C44/38	B29C44/38		126
B29C44/388	11	{into moving moulds}	B29C44/38	B29C44/38		143
B29C44/40	11	by gravity, e.g. by casting	B29C44/40	B29C44/40		156
B29C44/42	11	using pressure difference, e.g. by injection or by vacuum	B29C44/42	B29C44/42		1016
B29C44/421	12	{by plastizising the material into a shot cavity and injecting using a plunger}	B29C44/42	B29C44/42		75
B29C44/422	12	{by injecting by forward movement of the plastizising screw}	B29C44/42	B29C44/42		79
B29C44/424	12	{Details of machines}	B29C44/42	B29C44/42		128
B29C44/425	13	{Valve or nozzle constructions; Details of injection devices}	B29C44/42	B29C44/42		179
B29C44/427	14	{having several injection gates}	B29C44/42	B29C44/42		35
B29C44/428	12	{Mould constructions; Mould supporting equipment}	B29C44/42	B29C44/42		352
B29C44/44	11	{in solid form}	B29C44/44	B29C44/44		92
B29C44/445	12	{in the form of expandable granules, particles or beads}	B29C44/44	B29C44/44		1617
B29C44/46	10	into an open space or onto moving surfaces, i.e. to make articles of indefinite length {(B29C44/365, B29C44/367 take precedence)}	B29C44/46	B29C44/46		81
B29C44/461	11	{dispensing apparatus, e.g. dispensing foaming resin over the whole width of the moving surface}	B29C44/46	B29C44/46		455
B29C44/462	12	{provided with pre-foaming devices}	B29C44/46	B29C44/46		49
B29C44/464	12	{using centrifugal force}	B29C44/46	B29C44/46		11
B29C44/465	12	{with adjustable die gap}	B29C44/46	B29C44/46		17
B29C44/467	11	{Foam spreading or levelling devices}	B29C44/46	B29C44/46		170
B29C44/468	11	{in a plurality of parallel streams which unite during the foaming}	B29C44/46	B29C44/46		152
B29C44/48	11	by gravity, e.g. casting onto, or between, moving surfaces {(B29C44/468 takes precedence)}	B29C44/48	B29C44/48		17
B29C44/485	12	{the material being spread in the nip of two cooperating rollers}	B29C44/48	B29C44/48		29
B29C44/50	11	using pressure difference, e.g. by extrusion or by spraying {(B29C44/468 takes precedence)}	B29C44/50	B29C44/50		625
B29C44/505	12	{extruding the compound through a flat die (in general B29C48/03)}	B29C44/50	B29C44/50		506
B29C44/507	12	{extruding the compound through an annular die (in general B29C48/03)}	B29C44/50	B29C44/50		508
B29C44/52	12	between moving surfaces	B29C44/52	B29C44/52		21
B29C44/54	11	in the form of expandable particles or beads	B29C44/54	B29C44/54		52
B29C44/56	9	After-treatment of articles, e.g. for altering the shape	B29C44/56	B29C44/56		1063
B29C44/5609	10	{Purging of residual gas, e.g. noxious or explosive blowing agents}	B29C44/56	B29C44/56		165
B29C44/5618	10	{Impregnating foam articles}	B29C44/56	B29C44/56		243
B29C44/5627	10	{by mechanical deformation, e.g. crushing, embossing, stretching}	B29C44/56	B29C44/56		593
B29C44/5636	11	{with the addition of heat}	B29C44/56	B29C44/56		487
B29C44/5645	12	{Differential deformation by differential heating}	B29C44/56	B29C44/56		20
B29C44/5654	11	{Subdividing foamed articles to obtain particular surface properties, e.g. on multiple modules}	B29C44/56	B29C44/56		287
B29C44/5663	11	{by perforating the foam, e.g. to open the cells}	B29C44/56	B29C44/56		100
B29C44/5672	11	{by stretching the foam, e.g. to open the cells}	B29C44/56	B29C44/56		24
B29C44/5681	10	{Covering the foamed object with, e.g. a lining}	B29C44/56	B29C44/56		244
B29C44/569	10	{Shaping and joining components with different densities or hardness}	B29C44/56	B29C44/56		386
B29C44/58	9	Moulds	B29C44/58	B29C44/58		2323
B29C44/581	10	{Closure devices for pour holes}	B29C44/58	B29C44/58		181
B29C44/582	10	{for making undercut articles}	B29C44/58	B29C44/58		171
B29C44/583	10	{for making articles with cavities}	B29C44/58	B29C44/58		254
B29C44/585	10	{with adjustable size of the mould cavity}	B29C44/58	B29C44/58		223
B29C44/586	10	{with a cavity increasing in size during foaming}	B29C44/58	B29C44/58		367
B29C44/587	10	{with a membrane, e.g. for pressure control}	B29C44/58	B29C44/58		37
B29C44/588	10	{with means for venting, e.g. releasing foaming gas}	B29C44/58	B29C44/58		778
B29C44/60	9	Measuring, controlling or regulating	B29C44/60	B29C44/60		1963
B29C44/605	10	{Calibration following a shaping operation, e.g. extrusion}	B29C44/60	B29C44/60		52
B29C45/00	7	Injection moulding, i.e. forcing the required volume of moulding material through a nozzle into a closed mould; Apparatus therefor (injection blow-moulding B29C49/06)	B29C45/00	B29C45/00		4079
B29C45/0001	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C45/00	B29C45/00		4727
B29C45/0003	8	{of successively moulded portions rigidly joined to each other}	B29C45/00	B29C45/00		274
B29C45/0005	8	{using fibre reinforcements}	B29C45/00	B29C45/00		1598
B29C2045/0006	9	{the fibres being oriented in a direction perpendicular to the flow direction of the moulding material into the mould}	B29C45/00	B29C45/00		32
B29C2045/0008	9	{the fibres being oriented randomly}	B29C45/00	B29C45/00		72
B29C2045/001	9	{Bulk moulding compounds [BMC]}	B29C45/00	B29C45/00		51
B29C2045/0012	9	{Skin layers without fibres or with little fibres}	B29C45/00	B29C45/00		17
B29C45/0013	8	{using fillers dispersed in the moulding material, e.g. metal particles}	B29C45/00	B29C45/00		1238
B29C2045/0015	9	{Non-uniform dispersion of fillers}	B29C45/00	B29C45/00		61
B29C45/0017	8	{moulding interconnected elements which are movable with respect to one another, e.g. chains or hinges}	B29C45/00	B29C45/00		475
B29C2045/0018	9	{moulding containers with handle, e.g. buckets}	B29C45/00	B29C45/00		28
B29C2045/002	9	{using shrinkage}	B29C45/00	B29C45/00		40
B29C2045/0022	9	{using deformation of injected material to obtain interconnection}	B29C45/00	B29C45/00		11
B29C2045/0024	9	{using a mould core with a blind hole wherein the hinge shaft is moulded}	B29C45/00	B29C45/00		10
B29C45/0025	8	{Preventing defects on the moulded article, e.g. weld lines, shrinkage marks (preventing defects on the preformed parts or layers B29C45/14836)}	B29C45/00	B29C45/00		2674
B29C2045/0027	9	{Gate or gate mark locations}	B29C45/00	B29C45/00		548
B29C2045/0029	10	{gates on the central optical axis of lenses}	B29C45/00	B29C45/00		8
B29C2045/0031	9	{Movable mould wall parts in contact with weld lines, e.g. rotating pins for stirring the weld line}	B29C45/00	B29C45/00		23
B29C2045/0032	9	{sequential injection from multiple gates, e.g. to avoid weld lines}	B29C45/00	B29C45/00		174
B29C2045/0034	9	{Mould parting lines}	B29C45/00	B29C45/00		178
B29C2045/0036	9	{Submerged or recessed burrs}	B29C45/00	B29C45/00		115
B29C2045/0037	9	{Moulding articles or parts thereof without parting line}	B29C45/00	B29C45/00		40
B29C2045/0039	9	{intermixing the injected material front at the weld line, e.g. by applying vibrations to the melt front (B29C2045/0031 takes precedence)}	B29C45/00	B29C45/00		73
B29C2045/0041	9	{preventing initial material from entering the mould cavity}	B29C45/00	B29C45/00		28
B29C2045/0043	9	{preventing shrinkage by reducing the wall thickness of the moulded article}	B29C45/00	B29C45/00		97
B29C2045/0044	9	{expelling moulding material outside the mould cavity at the weld line location}	B29C45/00	B29C45/00		42
B29C45/0046	8	{Details relating to the filling pattern or flow paths or flow characteristics of moulding material in the mould cavity}	B29C45/00	B29C45/00		1028
B29C2045/0048	9	{Laminar flow}	B29C45/00	B29C45/00		11
B29C2045/0049	9	{the injected material flowing against a mould cavity protruding part}	B29C45/00	B29C45/00		114
B29C2045/0051	9	{Flow adjustment by throttles}	B29C45/00	B29C45/00		37
B29C45/0053	8	{combined with a final operation, e.g. shaping (injection-compression moulding B29C45/561)}	B29C45/00	B29C45/00		2427
B29C45/0055	9	{Shaping}	B29C45/00	B29C45/00		1418
B29C2045/0056	10	{folding back undercut forming parts, e.g. tabs of closures}	B29C45/00	B29C45/00		82
B29C2045/0058	10	{removing material}	B29C45/00	B29C45/00		470
B29C45/006	9	{Joining parts moulded in separate cavities}	B29C45/00	B29C45/00		895
B29C45/0062	10	{Joined by injection moulding}	B29C45/00	B29C45/00		492
B29C2045/0063	10	{facing before assembling, i.e. bringing the parts opposite to each other before assembling}	B29C45/00	B29C45/00		141
B29C2045/0065	10	{the parts being interconnected before assembling by a breaking or shearing point}	B29C45/00	B29C45/00		74
B29C2045/0067	10	{interposing an insert between the parts to be assembled}	B29C45/00	B29C45/00		73
B29C2045/0068	10	{using axially aligned and separated mould cavities}	B29C45/00	B29C45/00		22
B29C2045/007	10	{assembling a container and a handle}	B29C45/00	B29C45/00		23
B29C2045/0072	10	{the parts to be joined being moulded in a stack mould}	B29C45/00	B29C45/00		90
B29C2045/0074	10	{inserting a heating tool inside the mould}	B29C45/00	B29C45/00		21
B29C2045/0075	9	{curing or polymerising by irradiation}	B29C45/00	B29C45/00		126
B29C2045/0077	9	{removing burrs or flashes}	B29C45/00	B29C45/00		566
B29C2045/0079	9	{applying a coating or covering}	B29C45/00	B29C45/00		924
B29C45/0081	8	{of objects with parts connected by a thin section, e.g. hinge, tear line}	B29C45/00	B29C45/00		598
B29C45/0082	8	{Reciprocating the moulding material inside the mould cavity, e.g. push-pull injection moulding}	B29C45/00	B29C45/00		47
B29C45/0084	8	{General arrangement or lay-out of plants (B29C45/1468 takes precedence)}	B29C45/00	B29C45/00		301
B29C2045/0086	8	{Runner trees, i.e. several articles connected by a runner}	B29C45/00	B29C45/00		133
B29C2045/0087	8	{making hollow articles using a floating core movable in the mould cavity by fluid pressure and expelling molten excess material}	B29C45/00	B29C45/00		73
B29C2045/0089	8	{successive filling of parts of a mould cavity, i.e. one cavity part being filled before another part is filled (sequential filling to prevent weld lines B29C2045/0032)}	B29C45/00	B29C45/00		70
B29C2045/0091	8	{Pellets or granules, e.g. their structure, composition, length, height, width}	B29C45/00	B29C45/00		110
B29C2045/0093	8	{of articles provided with an attaching element}	B29C45/00	B29C45/00		267
B29C2045/0094	8	{injection moulding of small-sized articles, e.g. microarticles, ultra thin articles}	B29C45/00	B29C45/00		308
B29C2045/0096	8	{drying the moulding material before injection, e.g. by heating}	B29C45/00	B29C45/00		426
B29C2045/0098	8	{shearing of the moulding material, e.g. for obtaining molecular orientation or reducing the viscosity (B29C45/0082 takes precedence)}	B29C45/00	B29C45/00		97
B29C45/02	8	Transfer moulding, i.e. transferring the required volume of moulding material by a plunger from a "shot" cavity into a mould cavity	B29C45/02	B29C45/02		1490
B29C45/021	9	{Plunger drives; Pressure equalizing means for a plurality of transfer plungers}	B29C45/02	B29C45/02		157
B29C2045/022	9	{Stationary transfer plungers}	B29C45/02	B29C45/02		5
B29C2045/024	9	{Transfer plungers and pots with an oblong cross section}	B29C45/02	B29C45/02		13
B29C2045/025	9	{with the transfer plunger surface forming a part of the mould cavity wall at the end of the plunger transfer movement}	B29C45/02	B29C45/02		30
B29C2045/027	9	{heat insulated cold transfer moulding}	B29C45/02	B29C45/02		24
B29C2045/028	10	{using auxiliary curing or setting means}	B29C45/02	B29C45/02		10
B29C45/03	8	Injection moulding apparatus (transfer moulding B29C45/02)	B29C45/03	B29C45/03		2436
B29C2045/033	9	{horizontal injection units mounted on a mould half carrying plate}	B29C45/03	B29C45/03		28
B29C45/036	9	{Injection pistols}	B29C45/03	B29C45/03		74
B29C45/04	9	using movable moulds {or mould halves}(B29C45/08 takes precedence)	B29C45/04	B29C45/04		514
B29C45/0408	10	{involving at least a linear movement (B29C45/0433 takes precedence)}	B29C45/04	B29C45/04		346
B29C45/0416	11	{co-operating with fixed mould halves}	B29C45/04	B29C45/04		327
B29C2045/0425	12	{Book moulds, i.e. a mould half can be opened and closed like a book with regard to the other mould half, the mould halves being connected by a hinge}	B29C45/04	B29C45/04		49
B29C45/0433	10	{mounted on a conveyor belt or chain}	B29C45/04	B29C45/04		235
B29C45/0441	10	{involving a rotational movement (B29C45/06 takes precedence)}	B29C45/04	B29C45/04		457
B29C45/045	11	{mounted on the circumference of a rotating support having a rotating axis perpendicular to the mould opening, closing or clamping direction}	B29C45/04	B29C45/04		492
B29C2045/0458	12	{Drive means for the rotating support}	B29C45/04	B29C45/04		33
B29C2045/0466	10	{the axial movement of the mould being linked to the rotation of the mould or mould half}	B29C45/04	B29C45/04		24
B29C2045/0475	10	{continuously movable moulds}	B29C45/04	B29C45/04		34
B29C2045/0483	10	{pivotally mounted mould halves (B29C2045/0425 takes precedence)}	B29C45/04	B29C45/04		52
B29C2045/0491	10	{both mould halves being shifted to the injection unit for obtaining nozzle touch}	B29C45/04	B29C45/04		11
B29C45/06	10	{mounted} on a turntable {, i.e. on a rotating support having a rotating axis parallel to the mould opening, closing or clamping direction}	B29C45/06	B29C45/06		925
B29C45/062	11	{carrying mould halves co-operating with fixed mould halves}	B29C45/06	B29C45/06		388
B29C2045/065	11	{continuously rotating turntables}	B29C45/06	B29C45/06		107
B29C2045/067	11	{one mould being openable during clamping of the other moulds}	B29C45/06	B29C45/06		48
B29C45/07	9	using movable injection units	B29C45/07	B29C45/07		462
B29C2045/073	10	{pivotable horizontal injection unit with a nozzle pushed against a mould half}	B29C45/07	B29C45/07		13
B29C45/076	10	{cooperating with two or more moulds}	B29C45/07	B29C45/07		103
B29C45/08	10	moving with the mould during the injection operation	B29C45/08	B29C45/08		52
B29C45/10	9	using moulds or injection units usable in different arrangements or combinations to each other	B29C45/10	B29C45/10		290
B29C45/12	9	using two or more fixed moulds, e.g. in tandem {(B29C45/076 takes precedence)}	B29C45/12	B29C45/12		301
B29C45/125	10	{using a material distributing system}	B29C45/12	B29C45/12		150
B29C45/13	9	using two or more injection units co-operating with a single mould	B29C45/13	B29C45/13		338
B29C2045/135	10	{selectively injecting different materials in the same mould for making different articles in the same mould}	B29C45/13	B29C45/13		18
B29C45/14	8	incorporating preformed parts or layers, e.g. injection moulding around inserts or for coating articles {(B29C45/1671 takes precedence)}	B29C45/14	B29C45/14		7464
B29C45/14008	9	{Inserting articles into the mould (B29C45/14827 takes precedence)}	B29C45/14	B29C45/14		2857
B29C45/14016	10	{Intermittently feeding endless articles, e.g. transfer films, to the mould (B29C45/14262 takes precedence)}	B29C45/14	B29C45/14		353
B29C45/14024	11	{and punching or cutting a portion from the endless articles during mould closing}	B29C45/14	B29C45/14		109
B29C45/14032	10	{Transferring the inserts from a storage space inside the mould to the mould cavity}	B29C45/14	B29C45/14		76
B29C2045/1404	10	{feeding inserts cut out from an endless sheet outside the mould}	B29C45/14	B29C45/14		63
B29C2045/14049	10	{feeding inserts by a swing arm}	B29C45/14	B29C45/14		123
B29C2045/14057	10	{feeding inserts wrapped on a core}	B29C45/14	B29C45/14		91
B29C45/14065	9	{Positioning or centering articles in the mould}	B29C45/14	B29C45/14		4353
B29C45/14073	10	{using means being retractable during injection}	B29C45/14	B29C45/14		442
B29C2045/14081	11	{centering means retracted by the injection pressure}	B29C45/14	B29C45/14		68
B29C2045/1409	11	{using control means for retraction of the centering means}	B29C45/14	B29C45/14		56
B29C2045/14098	10	{fixing or clamping inserts having variable dimensions}	B29C45/14	B29C45/14		111
B29C2045/14106	10	{using electrostatic attraction or static electricity}	B29C45/14	B29C45/14		95
B29C2045/14114	10	{using an adhesive}	B29C45/14	B29C45/14		95
B29C2045/14122	10	{using fixed mould wall projections for centering the insert}	B29C45/14	B29C45/14		345
B29C2045/14131	10	{using positioning or centering means forming part of the insert}	B29C45/14	B29C45/14		339
B29C2045/14139	10	{positioning inserts having a part extending into a positioning cavity outside the mould cavity}	B29C45/14	B29C45/14		167
B29C2045/14147	10	{using pins or needles penetrating through the insert}	B29C45/14	B29C45/14		301
B29C2045/14155	10	{using vacuum or suction}	B29C45/14	B29C45/14		452
B29C2045/14163	10	{using springs being part of the positioning means}	B29C45/14	B29C45/14		174
B29C2045/14172	10	{using light to define the position of the insert}	B29C45/14	B29C45/14		13
B29C45/1418	9	{the inserts being deformed or preformed, e.g. by the injection pressure}	B29C45/14	B29C45/14		2612
B29C2045/14188	10	{trimming the article in the mould}	B29C45/14	B29C45/14		174
B29C45/14196	10	{the inserts being positioned around an edge of the injected part}	B29C45/14	B29C45/14		148
B29C2045/14204	11	{the edges formed by an intermediate mould part}	B29C45/14	B29C45/14		43
B29C2045/14213	10	{deforming by gas or fluid pressure in the mould cavity}	B29C45/14	B29C45/14		153
B29C45/14221	10	{by tools, e.g. cutting means}	B29C45/14	B29C45/14		843
B29C2045/14229	11	{deforming wire-like articles}	B29C45/14	B29C45/14		50
B29C2045/14237	10	{the inserts being deformed or preformed outside the mould or mould cavity}	B29C45/14	B29C45/14		523
B29C2045/14245	11	{using deforming or preforming means outside the mould cavity}	B29C45/14	B29C45/14		386
B29C2045/14254	11	{deforming or preforming endless articles outside the mould}	B29C45/14	B29C45/14		48
B29C45/14262	10	{Clamping or tensioning means for the insert}	B29C45/14	B29C45/14		263
B29C2045/1427	11	{controlling the slip of the insert}	B29C45/14	B29C45/14		49
B29C2045/14278	11	{controlling the tension of the insert}	B29C45/14	B29C45/14		25
B29C2045/14286	10	{means for heating the insert}	B29C45/14	B29C45/14		255
B29C2045/14295	11	{the heating means being used for feeding the insert into the mould}	B29C45/14	B29C45/14		29
B29C2045/14303	10	{progressively transferring the insert from one mould wall to the other mould wall of the mould cavity}	B29C45/14	B29C45/14		17
B29C45/14311	9	{using means for bonding the coating to the articles (B29C45/14795 takes precedence)}	B29C45/14	B29C45/14		1762
B29C2045/14319	10	{bonding by a fusion bond}	B29C45/14	B29C45/14		200
B29C2045/14327	10	{anchoring by forcing the material to pass through a hole in the article}	B29C45/14	B29C45/14		422
B29C45/14336	9	{Coating a portion of the article, e.g. the edge of the article (B29C45/14573 and B29C45/14598 take precedence)}	B29C45/14	B29C45/14		2692
B29C45/14344	10	{Moulding in or through a hole in the article, e.g. outsert moulding}	B29C45/14	B29C45/14		788
B29C2045/14352	11	{injecting into blind holes}	B29C45/14	B29C45/14		39
B29C2045/1436	11	{coating hollow articles having holes passing through the wall}	B29C45/14	B29C45/14		46
B29C2045/14368	11	{holes with means for anchoring the injected material}	B29C45/14	B29C45/14		36
B29C45/14377	10	{using an additional insert, e.g. a fastening element}	B29C45/14	B29C45/14		315
B29C45/14385	10	{Coating a portion of a bundle of inserts, e.g. making brushes}	B29C45/14	B29C45/14		282
B29C2045/14393	11	{preventing leakage of injected material into tuft insertion holes of the mould}	B29C45/14	B29C45/14		24
B29C2045/14401	11	{using a hot gas for forming a knob on the tuft end}	B29C45/14	B29C45/14		13
B29C45/14409	10	{Coating profiles or strips by injecting end or corner or intermediate parts}	B29C45/14	B29C45/14		205
B29C45/14418	10	{Sealing means between mould and article}	B29C45/14	B29C45/14		371
B29C45/14426	10	{Coating the end of wire-like or rod-like or cable-like or blade-like or belt-like articles}	B29C45/14	B29C45/14		277
B29C45/14434	10	{Coating brittle material, e.g. glass (B29C45/14377, B29C45/14418 take precedence)}	B29C45/14	B29C45/14		417
B29C2045/14442	10	{injecting a grill or grid on the insert}	B29C45/14	B29C45/14		59
B29C2045/1445	10	{injecting a part onto a blow moulded object}	B29C45/14	B29C45/14		95
B29C2045/14459	10	{injecting seal elements}	B29C45/14	B29C45/14		269
B29C45/14467	9	{Joining articles or parts of a single article (B29C45/14377, B29C45/14385, B29C45/14581, B29C45/14614 and B29C45/006 take precedence)}	B29C45/14	B29C45/14		2260
B29C45/14475	10	{Joining juxtaposed parts of a single article, e.g. edges of a folded container blank}	B29C45/14	B29C45/14		155
B29C2045/14483	11	{overlapping edges of the juxtaposed parts}	B29C45/14	B29C45/14		22
B29C45/14491	10	{Injecting material between coaxial articles, e.g. between a core and an outside sleeve for making a roll}	B29C45/14	B29C45/14		253
B29C2045/145	11	{making rolls}	B29C45/14	B29C45/14		27
B29C45/14508	10	{Joining juxtaposed sheet-like articles, e.g. for making trim panels}	B29C45/14	B29C45/14		229
B29C2045/14516	11	{the transition area of juxtaposed parts being hidden in a groove of the moulded article}	B29C45/14	B29C45/14		36
B29C2045/14524	10	{making hollow articles}	B29C45/14	B29C45/14		142
B29C2045/14532	10	{injecting between two sheets}	B29C45/14	B29C45/14		297
B29C2045/1454	10	{injecting between inserts not being in contact with each other}	B29C45/14	B29C45/14		193
B29C45/14549	9	{Coating rod-like, wire-like or belt-like articles (B29C45/14426 takes precedence)}	B29C45/14	B29C45/14		565
B29C2045/14557	10	{coating spliced fibres or cables, e.g. optical fiber splices or junctions}	B29C45/14	B29C45/14		48
B29C45/14565	10	{at spaced locations, e.g. coaxial-cable wires}	B29C45/14	B29C45/14		177
B29C45/14573	11	{Coating the edge of the article, e.g. for slide-fasteners}	B29C45/14	B29C45/14		197
B29C45/14581	11	{Coating the cross-over points of articles in the form of a network}	B29C45/14	B29C45/14		34
B29C45/1459	9	{Coating annular articles}	B29C45/14	B29C45/14		459
B29C45/14598	9	{Coating tubular articles}	B29C45/14	B29C45/14		935
B29C2045/14606	10	{Mould cavity sealing means}	B29C45/14	B29C45/14		42
B29C45/14614	10	{Joining tubular articles}	B29C45/14	B29C45/14		233
B29C45/14622	10	{Lining the inner or outer surface of tubular articles}	B29C45/14	B29C45/14		292
B29C45/14631	9	{Coating reinforcements (fibre reinforcements B29C45/0005)}	B29C45/14	B29C45/14		612
B29C45/14639	9	{for obtaining an insulating effect, e.g. for electrical components}	B29C45/14	B29C45/14		1931
B29C45/14647	10	{Making flat card-like articles with an incorporated IC or chip module, e.g. IC or chip cards}	B29C45/14	B29C45/14		224
B29C45/14655	10	{connected to or mounted on a carrier, e.g. lead frame}	B29C45/14	B29C45/14		1576
B29C2045/14663	11	{the mould cavity walls being lined with a film, e.g. release film}	B29C45/14	B29C45/14		93
B29C2045/14672	11	{moulding with different depths of the upper and lower mould cavity}	B29C45/14	B29C45/14		13
B29C45/1468	11	{Plants therefor}	B29C45/14	B29C45/14		111
B29C45/14688	9	{Coating articles provided with a decoration}	B29C45/14	B29C45/14		1189
B29C2045/14696	10	{transparent decorated inserts}	B29C45/14	B29C45/14		131
B29C2045/14704	10	{ink decorations}	B29C45/14	B29C45/14		210
B29C2045/14713	10	{decorations in contact with injected material}	B29C45/14	B29C45/14		196
B29C2045/14721	10	{decorations transferred by diffusion or sublimation}	B29C45/14	B29C45/14		23
B29C2045/14729	10	{decorations not in contact with injected material}	B29C45/14	B29C45/14		54
B29C2045/14737	10	{decorations printed on the insert by a digital imaging technique}	B29C45/14	B29C45/14		79
B29C2045/14745	10	{in-line printing}	B29C45/14	B29C45/14		39
B29C45/14754	9	{being in movable or releasable engagement with the coating, e.g. bearing assemblies}	B29C45/14	B29C45/14		442
B29C2045/14762	10	{using shrinkage}	B29C45/14	B29C45/14		39
B29C2045/1477	10	{Removable inserts, e.g. the insert being peeled off after moulding}	B29C45/14	B29C45/14		131
B29C45/14778	9	{the article consisting of a material with particular properties, e.g. porous, brittle}	B29C45/14	B29C45/14		1698
B29C45/14786	10	{Fibrous material or fibre containing material, e.g. fibre mats or fibre reinforced material}	B29C45/14	B29C45/14		898
B29C45/14795	10	{Porous or permeable material, e.g. foam}	B29C45/14	B29C45/14		353
B29C2045/14803	11	{the injected material entering minute pores}	B29C45/14	B29C45/14		86
B29C45/14811	10	{Multilayered articles (B29C45/14827 takes precedence)}	B29C45/14	B29C45/14		1674
B29C45/14819	9	{the inserts being completely encapsulated}	B29C45/14	B29C45/14		760
B29C45/14827	9	{using a transfer foil detachable from the insert}	B29C45/14	B29C45/14		469
B29C45/14836	9	{Preventing damage of inserts during injection, e.g. collapse of hollow inserts, breakage (B29C45/14434 takes precedence)}	B29C45/14	B29C45/14		570
B29C2045/14844	10	{Layers protecting the insert from injected material}	B29C45/14	B29C45/14		129
B29C2045/14852	9	{incorporating articles with a data carrier, e.g. chips}	B29C45/14	B29C45/14		223
B29C2045/1486	9	{Details, accessories and auxiliary operations}	B29C45/14	B29C45/14		275
B29C2045/14868	10	{Pretreatment of the insert, e.g. etching, cleaning}	B29C45/14	B29C45/14		993
B29C2045/14877	11	{preheating or precooling the insert for non-deforming purposes}	B29C45/14	B29C45/14		243
B29C2045/14885	11	{by plasma treatment}	B29C45/14	B29C45/14		73
B29C2045/14893	10	{Preventing defects relating to shrinkage of inserts or coating material}	B29C45/14	B29C45/14		108
B29C2045/14901	10	{Coating a sheet-like insert smaller than the dimensions of the adjacent mould wall}	B29C45/14	B29C45/14		173
B29C2045/14909	11	{the edge of the sheet-like insert being hidden, e.g. in a groove or protruding into the injected material}	B29C45/14	B29C45/14		62
B29C2045/14918	11	{in-mould-labelling}	B29C45/14	B29C45/14		468
B29C2045/14926	12	{multiple labels in the same cavity}	B29C45/14	B29C45/14		17
B29C2045/14934	10	{Preventing penetration of injected material between insert and adjacent mould wall}	B29C45/14	B29C45/14		169
B29C2045/14942	10	{Floating inserts, e.g. injecting simultaneously onto both sides of an insert through a pair of opposed gates}	B29C45/14	B29C45/14		57
B29C2045/1495	10	{Coating undercut inserts}	B29C45/14	B29C45/14		35
B29C2045/14959	10	{Flashing the injected material to the outside of the mould cavity for any purpose}	B29C45/14	B29C45/14		15
B29C2045/14967	10	{Injecting through an opening of the insert}	B29C45/14	B29C45/14		121
B29C2045/14975	11	{the injection nozzle penetrating through the insert}	B29C45/14	B29C45/14		32
B29C2045/14983	10	{Bursting or breakthrough of the insert by the injection pressure}	B29C45/14	B29C45/14		70
B29C2045/14991	10	{Submerged burrs, e.g. using protruding mould parts forming a cavity in which the burr on the insert is formed for preventing surface defects}	B29C45/14	B29C45/14		14
B29C45/16	8	Making multilayered or multicoloured articles {(B29C45/0062 takes precedence; feeding colouring materials into the injection unit B29C45/1816)}	B29C45/16	B29C45/16		3459
B29C2045/1601	9	{the injected materials not being adhered or bonded to each other (B29C45/0017 takes precedence)}	B29C45/16	B29C45/16		208
B29C45/1603	9	{Multi-way nozzles specially adapted therefor}	B29C45/16	B29C45/16		413
B29C45/1604	10	{using a valve urged by the injection pressure}	B29C45/16	B29C45/16		54
B29C45/1606	10	{using a rotatable valve}	B29C45/16	B29C45/16		43
B29C45/1607	10	{having at least three different ways}	B29C45/16	B29C45/16		110
B29C2045/1609	10	{having independent heating or cooling means for each way}	B29C45/16	B29C45/16		27
B29C2045/161	10	{using a hollow needle valve through which one material is injected}	B29C45/16	B29C45/16		46
B29C2045/1612	10	{using needle valves with at least four positions}	B29C45/16	B29C45/16		27
B29C2045/1614	10	{side-by-side flow of materials in the same channel}	B29C45/16	B29C45/16		22
B29C45/1615	9	{The materials being injected at different moulding stations}	B29C45/16	B29C45/16		1065
B29C2045/1617	10	{using stack moulds}	B29C45/16	B29C45/16		74
B29C45/1618	10	{using an auxiliary treatment station, e.g. for cooling or ejecting (B29C45/1628 takes precedence)}	B29C45/16	B29C45/16		125
B29C45/162	10	{using means, e.g. mould parts, for transferring an injected part between moulding stations}	B29C45/16	B29C45/16		592
B29C2045/1621	11	{the transfer means operating independently from the injection mould cavity, i.e. during injection the transfer means are completely outside the mould cavity}	B29C45/16	B29C45/16		46
B29C2045/1623	11	{transfer by a slidable element forming a part of both cavities}	B29C45/16	B29C45/16		19
B29C45/1625	10	{Injecting parison-like articles}	B29C45/16	B29C45/16		69
B29C2045/1626	11	{using a cooling station}	B29C45/16	B29C45/16		16
B29C45/1628	10	{using a mould carrier rotatable about an axis perpendicular to the opening and closing axis of the moulding stations}	B29C45/16	B29C45/16		446
B29C2045/1629	11	{turrets with incorporated ejection means}	B29C45/16	B29C45/16		30
B29C2045/1631	11	{turrets fixed with regard to the machine frame}	B29C45/16	B29C45/16		40
B29C2045/1632	11	{injection units supported by a movable mould plate}	B29C45/16	B29C45/16		20
B29C45/1634	9	{with a non-uniform dispersion of the moulding material in the article, e.g. resulting in a marble effect}	B29C45/16	B29C45/16		160
B29C45/1635	9	{using displaceable mould parts, e.g. retractable partition between adjacent mould cavities}	B29C45/16	B29C45/16		745
B29C2045/1637	10	{the first injected part and the movable mould part being movable together}	B29C45/16	B29C45/16		78
B29C45/1639	10	{Removable partitions between adjacent mould cavity portions}	B29C45/16	B29C45/16		157
B29C45/164	9	{The moulding materials being injected simultaneously}	B29C45/16	B29C45/16		260
B29C45/1642	9	{having a "sandwich" structure (B29C45/1603 takes precedence)}	B29C45/16	B29C45/16		770
B29C45/1643	10	{from at least three different materials or with at least four layers}	B29C45/16	B29C45/16		183
B29C45/1645	10	{Injecting skin and core materials from the same injection cylinder, e.g. mono-sandwich moulding}	B29C45/16	B29C45/16		77
B29C45/1646	10	{Injecting parison-like articles (B29C45/1643 takes precedence)}	B29C45/16	B29C45/16		130
B29C2045/1648	11	{the parison core layer being a barrier material}	B29C45/16	B29C45/16		66
B29C2045/165	11	{the parison core layer comprising recycled or scrap material}	B29C45/16	B29C45/16		21
B29C2045/1651	10	{Independent injection runners or nozzles}	B29C45/16	B29C45/16		42
B29C2045/1653	10	{using a core injection nozzle penetrating through the skin or into the mould cavity}	B29C45/16	B29C45/16		14
B29C2045/1654	10	{whereby the core material is penetrating through the skin}	B29C45/16	B29C45/16		48
B29C2045/1656	10	{Injecting the skin material through the central passage of the multiway nozzle}	B29C45/16	B29C45/16		34
B29C45/1657	9	{using means for adhering or bonding the layers or parts to each other (mechanical anchoring B29C37/0082)}	B29C45/16	B29C45/16		595
B29C2045/1659	10	{Fusion bonds}	B29C45/16	B29C45/16		134
B29C2045/166	10	{Roughened surface bonds}	B29C45/16	B29C45/16		28
B29C2045/1662	11	{plasma roughened surface bonds}	B29C45/16	B29C45/16		35
B29C2045/1664	10	{Chemical bonds}	B29C45/16	B29C45/16		63
B29C2045/1665	10	{Shrinkage bonds}	B29C45/16	B29C45/16		27
B29C2045/1667	10	{Deformation bonds}	B29C45/16	B29C45/16		20
B29C2045/1668	10	{Penetration bonds}	B29C45/16	B29C45/16		57
B29C2045/167	9	{injecting the second layer through the first layer}	B29C45/16	B29C45/16		117
B29C45/1671	9	{with an insert}	B29C45/16	B29C45/16		2280
B29C2045/1673	10	{injecting the first layer, then feeding the insert, then injecting the second layer}	B29C45/16	B29C45/16		302
B29C45/1675	9	{using exchangeable mould halves}	B29C45/16	B29C45/16		183
B29C45/1676	9	{using a soft material and a rigid material, e.g. making articles with a sealing part}	B29C45/16	B29C45/16		1536
B29C2045/1678	10	{first moulding the soft material}	B29C45/16	B29C45/16		74
B29C45/1679	9	{applying surface layers onto injection-moulded substrates inside the mould cavity, e.g. in-mould coating [IMC] (applying suface layers after ejection B29C45/0053)}	B29C45/16	B29C45/16		500
B29C2045/1681	9	{one layer penetrating at one or more areas through another layer}	B29C45/16	B29C45/16		93
B29C2045/1682	9	{preventing defects}	B29C45/16	B29C45/16		195
B29C45/1684	9	{Injecting parison-like articles (B29C45/1625, B29C45/1643 and B29C45/1646 take precedence)}	B29C45/16	B29C45/16		122
B29C2045/1685	9	{mounting of the additional injection unit}	B29C45/16	B29C45/16		87
B29C2045/1687	9	{preventing leakage of second injected material from the mould cavity}	B29C45/16	B29C45/16		111
B29C2045/1689	9	{injecting layers having identical injection cycle times}	B29C45/16	B29C45/16		6
B29C2045/169	9	{injecting electrical circuits, e.g. one layer being made of conductive material}	B29C45/16	B29C45/16		51
B29C2045/1692	9	{one layer comprising fibres}	B29C45/16	B29C45/16		71
B29C2045/1693	9	{shaping the first molding material before injecting the second molding material, e.g. by cutting, folding}	B29C45/16	B29C45/16		62
B29C2045/1695	9	{injecting ceramic powder layers and plastic material layers}	B29C45/16	B29C45/16		5
B29C2045/1696	9	{injecting metallic layers and plastic material layers}	B29C45/16	B29C45/16		79
B29C2045/1698	9	{multicoloured articles moulded in one step}	B29C45/16	B29C45/16		152
B29C45/17	8	Component parts, details or accessories; Auxiliary operations	B29C45/17	B29C45/17		4341
B29C45/1701	9	{using a particular environment during moulding, e.g. moisture-free or dust-free}	B29C45/17	B29C45/17		449
B29C2045/1702	10	{dissolving or absorbing a fluid in the plastic material}	B29C45/17	B29C45/17		68
B29C45/1703	9	{Introducing an auxiliary fluid into the mould (B29C45/1701 takes precedence)}	B29C45/17	B29C45/17		316
B29C45/1704	10	{the fluid being introduced into the interior of the injected material which is still in a molten state, e.g. for producing hollow articles (B29C45/1732 and B29C45/1734 take precedence; injection blow-moulding B29C49/06)}	B29C45/17	B29C45/17		1330
B29C45/1705	11	{using movable mould parts}	B29C45/17	B29C45/17		212
B29C45/1706	11	{using particular fluids or fluid generating substances}	B29C45/17	B29C45/17		189
B29C2045/1707	12	{using a liquid, e.g. water}	B29C45/17	B29C45/17		227
B29C2045/1708	13	{removing the liquid from the hollow}	B29C45/17	B29C45/17		30
B29C2045/1709	12	{using a cooling fluid}	B29C45/17	B29C45/17		48
B29C2045/171	12	{using an evaporating substance}	B29C45/17	B29C45/17		20
B29C45/1711	11	{and removing excess material from the mould cavity by the introduced fluid, e.g. to an overflow cavity}	B29C45/17	B29C45/17		236
B29C2045/1712	12	{plastic material flowing back into the injection unit}	B29C45/17	B29C45/17		41
B29C2045/1713	12	{using several overflow cavities}	B29C45/17	B29C45/17		21
B29C2045/1714	12	{overflow cavities provided with heating means}	B29C45/17	B29C45/17		4
B29C2045/1715	11	{Filled hollows}	B29C45/17	B29C45/17		42
B29C2045/1717	11	{Temperature controlled mould parts to control the location or configuration of the hollow}	B29C45/17	B29C45/17		26
B29C2045/1718	11	{sealing or closing the fluid injection opening}	B29C45/17	B29C45/17		62
B29C2045/1719	11	{making tubular articles}	B29C45/17	B29C45/17		103
B29C2045/172	11	{making roof racks for vehicles or parts thereof}	B29C45/17	B29C45/17		29
B29C2045/1721	11	{making wheels}	B29C45/17	B29C45/17		13
B29C2045/1722	11	{injecting fluids containing plastic material}	B29C45/17	B29C45/17		98
B29C2045/1723	11	{using fibre reinforcements}	B29C45/17	B29C45/17		68
B29C2045/1724	11	{hollows used as conduits}	B29C45/17	B29C45/17		111
B29C2045/1725	11	{making hollow seals}	B29C45/17	B29C45/17		5
B29C2045/1726	11	{moving the fluid through the hollow using a fluid inlet and a fluid outlet}	B29C45/17	B29C45/17		40
B29C2045/1727	11	{using short shots of moulding material}	B29C45/17	B29C45/17		31
B29C2045/1728	11	{injecting fluid from an end of the mould cavity and in the longitudinal direction thereof}	B29C45/17	B29C45/17		36
B29C2045/1729	11	{fluid venting means}	B29C45/17	B29C45/17		46
B29C2045/173	11	{using a plurality of fluid injection nozzles}	B29C45/17	B29C45/17		45
B29C2045/1731	11	{vacuum or underpressure for forming the hollow}	B29C45/17	B29C45/17		10
B29C45/1732	10	{Control circuits therefor}	B29C45/17	B29C45/17		191
B29C45/1734	10	{Nozzles therefor}	B29C45/17	B29C45/17		250
B29C45/1735	11	{Nozzles for introducing the fluid through the mould gate, e.g. incorporated in the injection nozzle}	B29C45/17	B29C45/17		132
B29C45/1736	11	{provided with small holes permitting the flow of gas therethrough, e.g. using a porous element of sintered material (B29C45/1735 takes precedence)}	B29C45/17	B29C45/17		49
B29C2045/1737	11	{Pin-in-sleeve devices}	B29C45/17	B29C45/17		48
B29C2045/1738	11	{using a valve mounted in movable valve sleeve}	B29C45/17	B29C45/17		8
B29C2045/1739	11	{controlling the temperature or heat-transfer in fluid injection nozzles}	B29C45/17	B29C45/17		16
B29C45/174	10	{Applying a pressurised fluid to the outer surface of the injected material inside the mould cavity, e.g. for preventing shrinkage marks}	B29C45/17	B29C45/17		254
B29C2045/1741	11	{Seals preventing pressurized fluid to escape from the mould cavity}	B29C45/17	B29C45/17		22
B29C45/1742	9	{Mounting of moulds; Mould supports (mounting of exchangeable mould inserts B29C45/2675)}	B29C45/17	B29C45/17		1781
B29C45/1743	10	{using mounting means projecting from the back side of the mould or from the front side of the mould support}	B29C45/17	B29C45/17		63
B29C45/1744	10	{Mould support platens}	B29C45/17	B29C45/17		447
B29C2045/1745	10	{using vacuum means}	B29C45/17	B29C45/17		29
B29C2045/1746	10	{using magnetic means}	B29C45/17	B29C45/17		98
B29C45/1747	9	{Tie-rod connections}	B29C45/17	B29C45/17		147
B29C45/1748	9	{Retractable tie-rods}	B29C45/17	B29C45/17		67
B29C2045/175	10	{using the movable mould plate for extracting a tie rod}	B29C45/17	B29C45/17		19
B29C45/1751	9	{Adjustment means allowing the use of moulds of different thicknesses}	B29C45/17	B29C45/17		318
B29C2045/1752	10	{using the mould clamping means for displacing the rear platen}	B29C45/17	B29C45/17		8
B29C45/1753	9	{Cleaning or purging, e.g. of the injection unit (B29C45/24 takes precedence)}	B29C45/17	B29C45/17		1982
B29C2045/1754	10	{purging cooling channels}	B29C45/17	B29C45/17		64
B29C45/1755	10	{Means for receiving or discharging purged material; Purge shields}	B29C45/17	B29C45/17		136
B29C45/1756	9	{Handling of moulds or mould parts, e.g. mould exchanging means (moulds per seB29C45/26)}	B29C45/17	B29C45/17		1445
B29C2045/1757	10	{common exchange means for several injection machines}	B29C45/17	B29C45/17		11
B29C2045/1758	10	{exchanging stampers}	B29C45/17	B29C45/17		46
B29C45/1759	9	{Removing sprues from sprue-channels}	B29C45/17	B29C45/17		276
B29C45/176	9	{Exchanging the injection unit or parts thereof}	B29C45/17	B29C45/17		163
B29C45/1761	9	{Means for guiding movable mould supports or injection units on the machine base or frame; Machine bases or frames (B29C45/1747 takes precedence)}	B29C45/17	B29C45/17		1167
B29C2045/1762	10	{compensating frame distortion proportional to the mould clamping force}	B29C45/17	B29C45/17		17
B29C2045/1763	10	{preventing distortion of the machine part guiding the movable mould}	B29C45/17	B29C45/17		60
B29C2045/1764	10	{Guiding means between the movable mould plate and tie rods}	B29C45/17	B29C45/17		57
B29C2045/1765	10	{Machine bases}	B29C45/17	B29C45/17		184
B29C2045/1767	11	{connecting means for machine base parts}	B29C45/17	B29C45/17		45
B29C2045/1768	10	{constructions of C-shaped frame elements}	B29C45/17	B29C45/17		163
B29C45/1769	9	{Handling of moulded articles or runners, e.g. sorting, stacking, grinding of runners}	B29C45/17	B29C45/17		2379
B29C2045/177	10	{stacking moulded articles}	B29C45/17	B29C45/17		368
B29C45/1771	10	{Means for guiding or orienting articles while dropped from the mould, e.g. guide rails or skirts}	B29C45/17	B29C45/17		148
B29C2045/1772	11	{sorting different articles}	B29C45/17	B29C45/17		34
B29C45/1773	9	{Means for adjusting or displacing the injection unit into different positions, e.g. for co-operating with different moulds (B29C45/1781 takes precedence)}	B29C45/17	B29C45/17		210
B29C45/1774	9	{Display units or mountings therefor; Switch cabinets}	B29C45/17	B29C45/17		190
B29C45/1775	9	{Connecting parts, e.g. injection screws, ejectors, to drive means}	B29C45/17	B29C45/17		401
B29C2045/1776	10	{magnetic connecting means}	B29C45/17	B29C45/17		20
B29C45/1777	9	{Nozzle touch mechanism}	B29C45/17	B29C45/17		193
B29C2045/1778	10	{separate drive means for moving and producing the touch force}	B29C45/17	B29C45/17		14
B29C2045/1779	10	{using chains or the like as drive transmission means for the movement of the injection unit}	B29C45/17	B29C45/17		9
B29C45/178	9	{Means disposed outside the mould for unscrewing threaded articles, e.g. chuck devices (moulds with incorporated unscrewing drive means B29C45/262)}	B29C45/17	B29C45/17		53
B29C45/1781	9	{Aligning injection nozzles with the mould sprue bush}	B29C45/17	B29C45/17		116
B29C45/1782	9	{Mounting or clamping means for heating elements or thermocouples}	B29C45/17	B29C45/17		123
B29C2045/1784	9	{Component parts, details or accessories not otherwise provided for; Auxiliary operations not otherwise provided for}	B29C45/17	B29C45/17		735
B29C2045/1785	10	{Movement of a part, e.g. opening or closing movement of the mould, generating fluid pressure in a built-in fluid pressure generator}	B29C45/17	B29C45/17		216
B29C2045/1786	10	{Electric wire or cable guides, e.g. for manifolds}	B29C45/17	B29C45/17		31
B29C2045/1787	10	{Mould parts driven by pressure of injected material (B29C2045/14081 takes precedence)}	B29C45/17	B29C45/17		24
B29C2045/1788	10	{Preventing tilting of movable mould plate during closing or clamping}	B29C45/17	B29C45/17		50
B29C2045/1789	11	{using weight compensating means for the movable mould half}	B29C45/17	B29C45/17		7
B29C2045/179	10	{Frames or machine parts made of concrete}	B29C45/17	B29C45/17		6
B29C2045/1791	10	{Means for spacing or distancing mould supporting plates, e.g. for mould exchange}	B29C45/17	B29C45/17		26
B29C2045/1792	10	{Machine parts driven by an electric motor, e.g. electric servomotor}	B29C45/17	B29C45/17		452
B29C2045/1793	11	{by an electric linear motor}	B29C45/17	B29C45/17		109
B29C2045/1794	11	{by a rotor or directly coupled electric motor, e.g. using a tubular shaft motor}	B29C45/17	B29C45/17		104
B29C2045/1795	10	{Means for detecting resin leakage or drooling from the injection nozzle}	B29C45/17	B29C45/17		26
B29C2045/1796	10	{Moulds carrying mould related information or codes, e.g. bar codes, counters}	B29C45/17	B29C45/17		147
B29C2045/1797	10	{Machine parts provided with a shroud or cover or shield, e.g. for preventing oil or dust scattering}	B29C45/17	B29C45/17		147
B29C2045/1798	10	{Using spring tension to drive movable machine parts}	B29C45/17	B29C45/17		89
B29C45/18	9	Feeding the material into the injection moulding apparatus {, i.e. feeding the non-plastified material into the injection unit}	B29C45/18	B29C45/18		2858
B29C45/1808	10	{Feeding measured doses}	B29C45/18	B29C45/18		451
B29C45/1816	10	{Feeding auxiliary material, e.g. colouring material}	B29C45/18	B29C45/18		563
B29C2045/1825	11	{feeding auxiliary material for either skin or core of the injected article}	B29C45/18	B29C45/18		14
B29C2045/1833	11	{recycling sprues or runners}	B29C45/18	B29C45/18		28
B29C2045/1841	11	{into runner channel or runner nozzle}	B29C45/18	B29C45/18		28
B29C2045/185	11	{controlling the amount of auxiliary material}	B29C45/18	B29C45/18		74
B29C45/1858	10	{Changing the kind or the source of material, e.g. using a plurality of hoppers}	B29C45/18	B29C45/18		72
B29C45/1866	10	{Feeding multiple materials (B29C45/1816 takes precedence)}	B29C45/18	B29C45/18		298
B29C2045/1875	10	{Hoppers connected to a feed screw}	B29C45/18	B29C45/18		197
B29C2045/1883	10	{directly injecting moulding material from the chemical production plant into the mould without granulating}	B29C45/18	B29C45/18		18
B29C2045/1891	10	{Means for detecting presence or level of raw material inside feeding ducts, e.g. level sensors inside hoppers}	B29C45/18	B29C45/18		72
B29C45/20	9	Injection nozzles {(B29C45/1603 takes precedence)}	B29C45/20	B29C45/20		1500
B29C2045/202	10	{Laterally adjustable nozzle or nozzle tip mountings}	B29C45/20	B29C45/20		83
B29C2045/205	10	{Elongated nozzle openings}	B29C45/20	B29C45/20		42
B29C2045/207	10	{Preventing stringing of the moulding material}	B29C45/20	B29C45/20		42
B29C45/22	10	Multiple nozzle systems	B29C45/22	B29C45/22		339
B29C45/23	10	Feed stopping equipment	B29C45/23	B29C45/23		458
B29C45/231	11	{Needle valve systems therefor}	B29C45/23	B29C45/23		465
B29C45/232	11	{comprising closing means disposed outside the nozzle}	B29C45/23	B29C45/23		78
B29C45/234	11	{Valves opened by the pressure of the moulding material (B29C45/231 takes precedence)}	B29C45/23	B29C45/23		127
B29C2045/235	11	{axially movable inclined or orthogonal valves}	B29C45/23	B29C45/23		55
B29C2045/237	11	{two or more cooperating valve elements}	B29C45/23	B29C45/23		27
B29C2045/238	11	{Injection nozzles extending into the sprue channel or vice versa}	B29C45/23	B29C45/23		15
B29C45/24	10	Cleaning equipment	B29C45/24	B29C45/24		311
B29C45/26	9	Moulds	B29C45/26	B29C45/26		8208
B29C45/2602	10	{Mould construction elements}	B29C45/26	B29C45/26		6651
B29C2045/2604	11	{Latching means for successive opening or closing of mould plates}	B29C45/26	B29C45/26		162
B29C45/2606	11	{Guiding or centering means}	B29C45/26	B29C45/26		2052
B29C45/2608	10	{Mould seals}	B29C45/26	B29C45/26		707
B29C45/261	10	{having tubular mould cavities}	B29C45/26	B29C45/26		890
B29C45/2612	11	{for manufacturing tubular articles with an annular groove}	B29C45/26	B29C45/26		153
B29C45/2614	11	{for manufacturing bent tubular articles using an undercut forming mould core}	B29C45/26	B29C45/26		194
B29C45/2616	10	{having annular mould cavities}	B29C45/26	B29C45/26		287
B29C45/2618	10	{having screw-threaded mould walls}	B29C45/26	B29C45/26		434
B29C45/262	11	{provided with unscrewing drive means (unscrewing means outside the mould B29C45/178)}	B29C45/26	B29C45/26		403
B29C45/2622	11	{for moulding interrupted screw threads}	B29C45/26	B29C45/26		67
B29C45/2624	10	{provided with a multiplicity of wall-like cavities connected to a common cavity, e.g. for battery cases}	B29C45/26	B29C45/26		135
B29C45/2626	10	{provided with a multiplicity of narrow cavities connected to a common cavity, e.g. for brushes, combs}	B29C45/26	B29C45/26		185
B29C45/2628	10	{with mould parts forming holes in or through the moulded article, e.g. for bearing cages}	B29C45/26	B29C45/26		835
B29C45/263	10	{with mould wall parts provided with fine grooves or impressions, e.g. for record discs}	B29C45/26	B29C45/26		1153
B29C45/2632	11	{Stampers; Mountings thereof}	B29C45/26	B29C45/26		381
B29C2045/2634	12	{mounting layers between stamper and mould or on the rear surface of the stamper}	B29C45/26	B29C45/26		36
B29C2045/2636	13	{insulating layers}	B29C45/26	B29C45/26		31
B29C2045/2638	12	{Magnetic means for mounting stampers}	B29C45/26	B29C45/26		16
B29C2045/264	12	{Holders retaining the inner periphery of the stamper}	B29C45/26	B29C45/26		85
B29C45/2642	11	{Heating or cooling means therefor}	B29C45/26	B29C45/26		155
B29C2045/2644	12	{for the outer peripheral ring}	B29C45/26	B29C45/26		11
B29C2045/2646	11	{Means for adjusting the axial dimension of the mould cavity}	B29C45/26	B29C45/26		24
B29C2045/2648	11	{Outer peripheral ring constructions}	B29C45/26	B29C45/26		77
B29C2045/2651	11	{using a plurality of mould cavities}	B29C45/26	B29C45/26		87
B29C2045/2653	11	{using two stampers}	B29C45/26	B29C45/26		48
B29C2045/2655	11	{Means for adjusting the radial dimension of the mould cavity}	B29C45/26	B29C45/26		13
B29C2045/2657	11	{Drive means for the outer peripheral ring}	B29C45/26	B29C45/26		27
B29C2045/2659	11	{for making substrates for laminated disks}	B29C45/26	B29C45/26		33
B29C2045/2661	11	{The thickness of the mould cavity being changeable in radial direction (B29C2045/2667 takes precedence)}	B29C45/26	B29C45/26		20
B29C2045/2663	11	{Maintaining the axial dimension of the mould cavity during injection}	B29C45/26	B29C45/26		4
B29C2045/2665	11	{using vacuum means for holding the disc on one of the mould walls during opening of the mould}	B29C45/26	B29C45/26		9
B29C2045/2667	11	{Particular inner or outer peripheral portions of the substrate}	B29C45/26	B29C45/26		36
B29C45/2669	10	{with means for removing excess material, e.g. with overflow cavities (B29C45/1711 takes precedence)}	B29C45/26	B29C45/26		483
B29C2045/2671	11	{Resin exit gates or bleeder passages}	B29C45/26	B29C45/26		91
B29C45/2673	10	{with exchangeable mould parts, e.g. cassette moulds (B29C45/1756 takes precedence)}	B29C45/26	B29C45/26		1210
B29C45/2675	11	{Mounting of exchangeable mould inserts}	B29C45/26	B29C45/26		463
B29C2045/2677	11	{The exchangeable mould parts being combinable or rearrangeable in different ways}	B29C45/26	B29C45/26		86
B29C2045/2679	11	{Simultaneously producing different products}	B29C45/26	B29C45/26		37
B29C45/2681	10	{with rotatable mould parts}	B29C45/26	B29C45/26		643
B29C2045/2683	10	{Plurality of independent mould cavities in a single mould}	B29C45/26	B29C45/26		983
B29C2045/2685	11	{filled with different materials}	B29C45/26	B29C45/26		63
B29C2045/2687	11	{controlling the filling thereof (B29C2045/2691 takes precedence)}	B29C45/26	B29C45/26		121
B29C2045/2689	11	{separate independent mould halves mounted on one plate}	B29C45/26	B29C45/26		44
B29C2045/2691	11	{sequentially filled}	B29C45/26	B29C45/26		73
B29C2045/2693	10	{Mould cores with a built-in injection nozzle}	B29C45/26	B29C45/26		38
B29C2045/2695	10	{injecting articles with varying wall thickness, e.g. for making a tear line}	B29C45/26	B29C45/26		52
B29C2045/2697	10	{Deformed geometry of the cavity}	B29C45/26	B29C45/26		108
B29C45/27	10	Sprue channels {; Runner channels or runner nozzles}	B29C45/27	B29C45/27		2922
B29C45/2701	11	{Details not specific to hot or cold runner channels (B29C45/2725 takes precedence)}	B29C45/27	B29C45/27		998
B29C45/2703	12	{Means for controlling the runner flow, e.g. runner switches, adjustable runners or gates}	B29C45/27	B29C45/27		416
B29C45/2704	13	{Controlling the filling rates or the filling times of two or more mould cavities by controlling the cross section or the length of the runners or the gates}	B29C45/27	B29C45/27		100
B29C2045/2706	13	{rotatable sprue bushings or runner channels for controlling runner flow in one cavity}	B29C45/27	B29C45/27		20
B29C45/2708	12	{Gates (B29C45/2703 takes precedence)}	B29C45/27	B29C45/27		2097
B29C2045/2709	13	{with a plurality of mould cavity inlets in close proximity}	B29C45/27	B29C45/27		241
B29C45/2711	13	{Gate inserts}	B29C45/27	B29C45/27		206
B29C2045/2712	13	{Serial gates for moulding articles in successively filled serial mould cavities}	B29C45/27	B29C45/27		72
B29C2045/2714	13	{elongated, e.g. film-like, annular}	B29C45/27	B29C45/27		180
B29C2045/2716	13	{The gate axis being perpendicular to main injection axis, e.g. injecting into side walls of a container}	B29C45/27	B29C45/27		47
B29C2045/2717	12	{Reconfigurable runner channels}	B29C45/27	B29C45/27		63
B29C2045/2719	12	{Fixing or locking of nozzles or sprue bushings in the mould}	B29C45/27	B29C45/27		88
B29C2045/272	12	{Part of the nozzle, bushing or runner in contact with the injected material being made from ceramic material}	B29C45/27	B29C45/27		21
B29C2045/2722	12	{Nozzles or runner channels provided with a pressure sensor}	B29C45/27	B29C45/27		72
B29C2045/2724	12	{Preventing stringing of the moulding material}	B29C45/27	B29C45/27		49
B29C45/2725	11	{Manifolds}	B29C45/27	B29C45/27		926
B29C45/2727	12	{Modular manifolds; Connections between spaced manifold elements}	B29C45/27	B29C45/27		96
B29C2045/2729	12	{with thermal expansion}	B29C45/27	B29C45/27		81
B29C2045/273	12	{stacked manifolds}	B29C45/27	B29C45/27		61
B29C2045/2732	13	{sealing means between them}	B29C45/27	B29C45/27		19
B29C2045/2733	12	{Inserts, plugs, bushings}	B29C45/27	B29C45/27		136
B29C45/2735	11	{for non-coaxial gates, e.g. for edge gates}	B29C45/27	B29C45/27		231
B29C45/2737	11	{Heating or cooling means therefor (B29C45/7331 takes precedence)}	B29C45/27	B29C45/27		1352
B29C45/2738	12	{specially adapted for manifolds}	B29C45/27	B29C45/27		225
B29C2045/274	12	{Thermocouples or heat sensors}	B29C45/27	B29C45/27		243
B29C2045/2741	13	{Plurality of independent thermocouples or heat sensors}	B29C45/27	B29C45/27		31
B29C2045/2743	12	{Electrical heating element constructions}	B29C45/27	B29C45/27		223
B29C2045/2745	13	{Film-like electrical heaters}	B29C45/27	B29C45/27		38
B29C2045/2746	13	{Multilayered electrical heaters}	B29C45/27	B29C45/27		27
B29C2045/2748	13	{Insulating layers covering the electrical heating element}	B29C45/27	B29C45/27		69
B29C2045/275	12	{Planar heating or cooling elements}	B29C45/27	B29C45/27		32
B29C2045/2751	12	{Electrical power supply connections}	B29C45/27	B29C45/27		43
B29C2045/2753	12	{Heating means and cooling means, e.g. heating the runner nozzle and cooling the nozzle tip}	B29C45/27	B29C45/27		156
B29C2045/2754	12	{Plurality of independent heating or cooling means, e.g. independently controlling the heating of several zones of the nozzle, (B29C2045/2753 takes precedence)}	B29C45/27	B29C45/27		102
B29C45/2756	11	{Cold runner channels}	B29C45/27	B29C45/27		290
B29C45/2758	11	{Means for preventing drooling by decompression of the moulding material}	B29C45/27	B29C45/27		59
B29C2045/2759	11	{Nozzle centering or guiding means}	B29C45/27	B29C45/27		81
B29C2045/2761	11	{Seals between nozzle and mould or gate}	B29C45/27	B29C45/27		186
B29C2045/2762	11	{Seals between nozzle and manifold}	B29C45/27	B29C45/27		69
B29C2045/2764	11	{Limited contact between nozzle and mould}	B29C45/27	B29C45/27		35
B29C2045/2766	11	{Heat insulation between nozzle and mould}	B29C45/27	B29C45/27		123
B29C2045/2767	12	{the heat insulation being provided with an axial opening being part of the melt flow channel}	B29C45/27	B29C45/27		25
B29C2045/2769	12	{Insulating layer of injected material}	B29C45/27	B29C45/27		19
B29C2045/277	11	{Spacer means or pressure pads between manifold and mould plates}	B29C45/27	B29C45/27		87
B29C2045/2772	11	{Means for fixing the nozzle to the manifold}	B29C45/27	B29C45/27		75
B29C2045/2774	11	{The nozzle head or the collar portion and central portion being made of different parts or materials}	B29C45/27	B29C45/27		28
B29C2045/2775	11	{Nozzles or parts thereof being mountable or exchangeable from the front side of the mould half}	B29C45/27	B29C45/27		33
B29C2045/2777	11	{Means for controlling heat flow or temperature distribution in the nozzle}	B29C45/27	B29C45/27		67
B29C2045/2779	11	{Nozzles with a plurality of outlets}	B29C45/27	B29C45/27		91
B29C45/278	11	{Nozzle tips (B29C45/2735 takes precedence)}	B29C45/27	B29C45/27		445
B29C2045/2782	12	{Nozzle tips metallurgically bonded to the nozzle body}	B29C45/27	B29C45/27		20
B29C2045/2783	12	{Nozzle tips with a non-axial outlet opening of the melt channel}	B29C45/27	B29C45/27		62
B29C2045/2785	12	{Nozzle tips with high thermal conductivity}	B29C45/27	B29C45/27		49
B29C2045/2787	12	{Nozzle tips made of at least 2 different materials}	B29C45/27	B29C45/27		72
B29C2045/2788	11	{Nozzles having a polygonal cross section}	B29C45/27	B29C45/27		44
B29C2045/279	11	{Controlling the flow of material of two or more nozzles or gates to a single mould cavity}	B29C45/27	B29C45/27		65
B29C2045/2791	11	{Alignment means between nozzle and manifold}	B29C45/27	B29C45/27		56
B29C2045/2793	11	{Means for providing access to the runner system}	B29C45/27	B29C45/27		26
B29C2045/2795	11	{Insulated runners}	B29C45/27	B29C45/27		34
B29C2045/2796	11	{Axially movable nozzles or nozzle tips}	B29C45/27	B29C45/27		81
B29C2045/2798	12	{for compensating thermal expansion}	B29C45/27	B29C45/27		41
B29C45/28	11	Closure devices therefor	B29C45/28	B29C45/28		607
B29C45/2803	12	{comprising a member with an opening or the injection nozzle movable into or out of alignment with the sprue channel or mould gate}	B29C45/28	B29C45/28		138
B29C45/2806	12	{consisting of needle valve systems (B29C45/2896 takes precedence)}	B29C45/28	B29C45/28		1365
B29C45/281	13	{Drive means therefor}	B29C45/28	B29C45/28		764
B29C2045/2813	14	{Common drive means for several needle valves}	B29C45/28	B29C45/28		173
B29C2045/2817	14	{Several valve pin drive cylinders connected to the fluid distributor}	B29C45/28	B29C45/28		43
B29C2045/282	14	{Needle valves driven by screw and nut means}	B29C45/28	B29C45/28		35
B29C2045/2824	14	{Needle valves driven by an electric motor}	B29C45/28	B29C45/28		114
B29C2045/2827	14	{Needle valves driven by an annular piston mounted around the nozzle}	B29C45/28	B29C45/28		45
B29C2045/2831	14	{Needle valves driven by a cam}	B29C45/28	B29C45/28		51
B29C2045/2834	14	{Needle valves driven by a lever}	B29C45/28	B29C45/28		73
B29C2045/2837	14	{Needle valves driven by rack and pinion}	B29C45/28	B29C45/28		28
B29C2045/2841	14	{Needle valves driven by a plurality of coaxial pistons}	B29C45/28	B29C45/28		20
B29C2045/2844	14	{Needle valves driven by racks only}	B29C45/28	B29C45/28		3
B29C2045/2848	13	{having an adjustable stroke length}	B29C45/28	B29C45/28		80
B29C2045/2851	13	{Lateral movement between drive piston and needle valve}	B29C45/28	B29C45/28		15
B29C2045/2855	13	{intersecting the nozzle or runner channel}	B29C45/28	B29C45/28		36
B29C2045/2858	13	{Materials or coatings therefor}	B29C45/28	B29C45/28		37
B29C2045/2862	13	{being tubular}	B29C45/28	B29C45/28		42
B29C2045/2865	13	{having position detecting means}	B29C45/28	B29C45/28		62
B29C2045/2868	13	{with an incorporated heat pipe}	B29C45/28	B29C45/28		15
B29C2045/2872	13	{with at least three positions, e.g. two different open positions to control the melt flow}	B29C45/28	B29C45/28		84
B29C2045/2875	13	{Preventing rotation of the needle valve}	B29C45/28	B29C45/28		29
B29C2045/2879	13	{Back flow of material into nozzle channel}	B29C45/28	B29C45/28		35
B29C2045/2882	13	{closing by a movement in the counterflow direction}	B29C45/28	B29C45/28		60
B29C2045/2886	13	{closing at a distance from the gate}	B29C45/28	B29C45/28		44
B29C2045/2889	13	{Sealing guide bushings therefor}	B29C45/28	B29C45/28		116
B29C2045/2893	13	{Multiple coaxial needle valves}	B29C45/28	B29C45/28		40
B29C45/2896	12	{extending in or through the mould cavity, e.g. valves mounted opposite the sprue channel}	B29C45/28	B29C45/28		82
B29C45/30	11	Flow control means disposed within the sprue channel, e.g. "torpedo" construction	B29C45/30	B29C45/30		613
B29C2045/302	12	{Torpedoes in the sprue channel for heating the melt of cross-linkable material}	B29C45/30	B29C45/30		10
B29C2045/304	12	{Adjustable torpedoes}	B29C45/30	B29C45/30		48
B29C2045/306	12	{Movable torpedoes}	B29C45/30	B29C45/30		51
B29C2045/308	12	{Mixing or stirring devices}	B29C45/30	B29C45/30		111
B29C45/32	10	having several axially spaced mould cavities {, i.e. for making several separated articles}	B29C45/32	B29C45/32		1097
B29C45/322	11	{Runner systems for distributing the moulding material to the stacked mould cavities}	B29C45/32	B29C45/32		281
B29C2045/324	11	{Linked ejection means}	B29C45/32	B29C45/32		54
B29C2045/326	11	{Supporting means for the central mould plate}	B29C45/32	B29C45/32		47
B29C2045/328	11	{having a movable mould plate between two fixed mould plates}	B29C45/32	B29C45/32		40
B29C45/33	10	having transversely, e.g. radially, movable mould parts	B29C45/33	B29C45/33		3652
B29C45/332	11	{Mountings or guides therefor; Drives therefor}	B29C45/33	B29C45/33		2965
B29C2045/334	12	{several transversely movable mould parts driven by a single drive means}	B29C45/33	B29C45/33		182
B29C2045/336	12	{Cam drives}	B29C45/33	B29C45/33		117
B29C2045/338	11	{Mould parts with combined axial and transversal movements}	B29C45/33	B29C45/33		330
B29C45/34	10	having venting means	B29C45/34	B29C45/34		2514
B29C45/345	11	{using a porous mould wall or a part thereof, e.g. made of sintered metal}	B29C45/34	B29C45/34		177
B29C45/36	10	having means for locating or centering cores	B29C45/36	B29C45/36		1345
B29C2045/363	11	{using a movable core or core part}	B29C45/36	B29C45/36		605
B29C2045/366	11	{using retractable pins}	B29C45/36	B29C45/36		65
B29C45/37	10	Mould cavity walls {, i.e. the inner surface forming the mould cavity, e.g. linings}	B29C45/37	B29C45/37		1039
B29C45/372	11	{provided with means for marking or patterning, e.g. numbering articles}	B29C45/37	B29C45/37		912
B29C45/374	12	{for displaying altering indicia, e.g. data, numbers}	B29C45/37	B29C45/37		173
B29C45/376	11	{adjustable (B29C45/374 takes precedence)}	B29C45/37	B29C45/37		251
B29C2045/378	11	{built by a stack of modular elements}	B29C45/37	B29C45/37		75
B29C45/38	9	Cutting-off equipment for sprues or ingates	B29C45/38	B29C45/38		1736
B29C45/382	10	{disposed outside the mould}	B29C45/38	B29C45/38		1179
B29C2045/384	10	{cutting the sprue by a plunger movable into the runner channel}	B29C45/38	B29C45/38		98
B29C2045/386	11	{returning the cutted sprue into the injection nozzle}	B29C45/38	B29C45/38		17
B29C2045/388	10	{Locking pins for retaining the sprue}	B29C45/38	B29C45/38		50
B29C45/40	9	Removing or ejecting moulded articles	B29C45/40	B29C45/40		2569
B29C45/4005	10	{Ejector constructions; Ejector operating mechanisms (B29C45/44 takes precedence)}	B29C45/40	B29C45/40		5875
B29C45/401	11	{Ejector pin constructions or mountings}	B29C45/40	B29C45/40		2250
B29C2045/4015	12	{Ejector pins provided with sealing means}	B29C45/40	B29C45/40		51
B29C2045/4021	12	{Adjustable ejector pins}	B29C45/40	B29C45/40		58
B29C2045/4026	12	{Ejectors with internal cooling}	B29C45/40	B29C45/40		54
B29C2045/4031	11	{driven by a lever}	B29C45/40	B29C45/40		32
B29C2045/4036	11	{driven by a screw and nut mechanism}	B29C45/40	B29C45/40		162
B29C2045/4042	11	{driven by rack and pinion means}	B29C45/40	B29C45/40		143
B29C2045/4047	11	{driven by a crank or eccentric}	B29C45/40	B29C45/40		41
B29C2045/4052	11	{Ejector boxes}	B29C45/40	B29C45/40		44
B29C2045/4057	10	{the ejecting surface being large with regard to the surface of the article}	B29C45/40	B29C45/40		37
B29C2045/4063	10	{preventing damage to articles caused by the ejector}	B29C45/40	B29C45/40		287
B29C2045/4068	10	{using an auxiliary mould part carrying the moulded article and removing it from the mould}	B29C45/40	B29C45/40		150
B29C2045/4073	10	{Ejection devices located outside the injection moulding machine}	B29C45/40	B29C45/40		47
B29C2045/4078	10	{using stripping means}	B29C45/40	B29C45/40		140
B29C2045/4084	10	{Progressive ejection}	B29C45/40	B29C45/40		170
B29C2045/4089	10	{Hollow articles retained in the female mould during mould opening}	B29C45/40	B29C45/40		34
B29C2045/4094	10	{Ejectors located on the fixed mould half}	B29C45/40	B29C45/40		68
B29C45/42	10	using means movable from outside the mould between mould parts {, e.g. robots}	B29C45/42	B29C45/42		1664
B29C45/4208	11	{and driven by the movable mould part}	B29C45/42	B29C45/42		145
B29C2045/4216	12	{releasable drive connections between the robot and the movable mould}	B29C45/42	B29C45/42		12
B29C45/4225	11	{Take-off members or carriers for the moulded articles, e.g. grippers}	B29C45/42	B29C45/42		1102
B29C2045/4233	12	{loading or holding moulded articles in take-off member by fluid ejection}	B29C45/42	B29C45/42		70
B29C2045/4241	11	{Auxiliary means for removing moulded articles from the robot}	B29C45/42	B29C45/42		116
B29C2045/425	11	{Single device for unloading moulded articles and loading inserts into the mould}	B29C45/42	B29C45/42		180
B29C2045/4258	11	{Article removing means movable into a closed mould}	B29C45/42	B29C45/42		8
B29C2045/4266	11	{Robot grippers movable along three orthogonal axes}	B29C45/42	B29C45/42		230
B29C2045/4275	11	{Related movements between the robot gripper and the movable mould or ejector}	B29C45/42	B29C45/42		48
B29C2045/4283	11	{Means for coupling robots to the injection moulding machine}	B29C45/42	B29C45/42		28
B29C2045/4291	12	{Robots mounted on a tie rod}	B29C45/42	B29C45/42		9
B29C45/43	10	using fluid under pressure	B29C45/43	B29C45/43		991
B29C45/435	11	{introduced between a mould core and a hollow resilient undercut article, e.g. bellows}	B29C45/43	B29C45/43		67
B29C45/44	10	for undercut articles	B29C45/44	B29C45/44		1910
B29C45/4407	11	{by flexible movement of undercut portions of the articles}	B29C45/44	B29C45/44		518
B29C2045/4414	12	{Flexible undercut parts divided into segments}	B29C45/44	B29C45/44		16
B29C45/4421	11	{using expansible or collapsible cores}	B29C45/44	B29C45/44		413
B29C2045/4428	12	{driven by the moulded article during ejection thereof}	B29C45/44	B29C45/44		5
B29C45/4435	11	{using inclined, tiltable or flexible undercut forming elements driven by the ejector means}	B29C45/44	B29C45/44		1175
B29C2045/4442	12	{Flexible undercut forming elements}	B29C45/44	B29C45/44		16
B29C2045/445	11	{using the movable undercut forming element for ejection of the moulded article}	B29C45/44	B29C45/44		252
B29C45/4457	11	{using fusible, soluble or destructible cores}	B29C45/44	B29C45/44		266
B29C2045/4464	12	{injecting the core and the undercut article in separate cavities}	B29C45/44	B29C45/44		21
B29C45/4471	11	{using flexible or pivotable undercut forming elements (B29C45/4435 takes precedence)}	B29C45/44	B29C45/44		155
B29C45/4478	11	{using non-rigid undercut forming elements, e.g. elastic or resilient}	B29C45/44	B29C45/44		160
B29C2045/4485	11	{the undercut forming mould part being rotatable into the space made available by the translation movement of another mould part}	B29C45/44	B29C45/44		48
B29C2045/4492	11	{preventing damage or deformation of undercut articles during ejection}	B29C45/44	B29C45/44		193
B29C45/46	9	Means for plasticising or homogenising the moulding material or forcing it into the mould {(combined with mould opening, closing or clamping devices B29C45/70)}	B29C45/46	B29C45/46		1037
B29C45/461	10	{Injection of measured doses}	B29C45/46	B29C45/46		178
B29C45/462	10	{Injection of preformed charges of material}	B29C45/46	B29C45/46		175
B29C45/463	11	{using packaged or wrapped charges}	B29C45/46	B29C45/46		45
B29C45/464	10	{using a rotating plasticising or injection disc}	B29C45/46	B29C45/46		139
B29C2045/465	10	{using pumps for injecting the material into the mould}	B29C45/46	B29C45/46		89
B29C2045/466	10	{supplying the injection unit directly by a compounder}	B29C45/46	B29C45/46		133
B29C2045/467	10	{injecting material into the mould by sudden expansion of compressed material in the injection unit}	B29C45/46	B29C45/46		23
B29C2045/468	10	{using a fluid as directly acting injection means}	B29C45/46	B29C45/46		46
B29C45/47	10	using screws (B29C45/54 takes precedence)	B29C45/47	B29C45/47		1029
B29C45/48	11	Plasticising screw and injection screw {comprising two separate screws}	B29C45/48	B29C45/48		115
B29C45/50	11	Axially movable screw	B29C45/50	B29C45/50		666
B29C2045/5004	12	{the forward screw end provided with an injection ram}	B29C45/50	B29C45/50		46
B29C45/5008	12	{Drive means therefor}	B29C45/50	B29C45/50		1109
B29C2045/5012	13	{screws axially driven by a toggle mechanism}	B29C45/50	B29C45/50		9
B29C2045/5016	13	{screws axially driven by a lever mechanism}	B29C45/50	B29C45/50		10
B29C2045/502	13	{screws axially driven by a crank or eccentric mechanism}	B29C45/50	B29C45/50		21
B29C2045/5024	13	{screws rotated by the coaxial rotor of an electric motor}	B29C45/50	B29C45/50		99
B29C2045/5028	13	{screws axially driven by the coaxial rotor of an electric motor}	B29C45/50	B29C45/50		85
B29C2045/5032	13	{using means for detecting injection or back pressures}	B29C45/50	B29C45/50		160
B29C2045/5036	14	{back pressure obtaining means}	B29C45/50	B29C45/50		32
B29C2045/504	13	{electric motors for rotary and axial movement of the screw being coaxial with the screw}	B29C45/50	B29C45/50		98
B29C2045/5044	13	{screws axially driven by rack and pinion means}	B29C45/50	B29C45/50		21
B29C2045/5048	13	{screws axially driven and rotated by a drive shaft having a screw threaded part and spline part}	B29C45/50	B29C45/50		33
B29C2045/5052	13	{screws axially driven by a rotatable nut cooperating with a fixed screw shaft}	B29C45/50	B29C45/50		25
B29C2045/5056	13	{screws axially driven by a rotatable screw shaft cooperating with a fixed nut}	B29C45/50	B29C45/50		61
B29C2045/506	13	{using a hydraulic transmission between drive motor and the axially movable screw}	B29C45/50	B29C45/50		35
B29C2045/5064	13	{coupling means between rotation motor and rectilinear drive motor}	B29C45/50	B29C45/50		15
B29C2045/5068	13	{mechanical drive means in series with hydraulic drive means for axially movable screw}	B29C45/50	B29C45/50		49
B29C2045/5072	13	{using a drive screw comprising screw parts having opposite thread directions}	B29C45/50	B29C45/50		6
B29C2045/5076	13	{using a single drive motor for rotary and for axial movements of the screw}	B29C45/50	B29C45/50		52
B29C2045/508	13	{idle or dead stroke elements between injection screw and drive means}	B29C45/50	B29C45/50		6
B29C2045/5084	13	{screws axially driven by roller elements}	B29C45/50	B29C45/50		14
B29C2045/5088	13	{screws axially and rotatably driven by a piston}	B29C45/50	B29C45/50		29
B29C45/5092	12	{Intrusion moulding, i.e. the screw rotates during injection}	B29C45/50	B29C45/50		58
B29C2045/5096	12	{decompression of the moulding material by retraction or opposite rotation of the screw}	B29C45/50	B29C45/50		67
B29C45/52	12	Non-return devices	B29C45/52	B29C45/52		586
B29C2045/522	13	{Spring biased check rings}	B29C45/52	B29C45/52		20
B29C2045/524	13	{Flexible valves}	B29C45/52	B29C45/52		11
B29C2045/526	13	{Abrasion resistant means in the screw head or non-return device}	B29C45/52	B29C45/52		53
B29C2045/528	13	{Mixing means forming part of or in close proximity to the non-return valve}	B29C45/52	B29C45/52		68
B29C45/53	10	using injection ram or piston	B29C45/53	B29C45/53		806
B29C45/531	11	{Drive means therefor}	B29C45/53	B29C45/53		357
B29C45/532	11	{using a hollow injection ram co-operating with a coaxial screw}	B29C45/53	B29C45/53		70
B29C2045/533	12	{using a continuously rotating plasticising screw}	B29C45/53	B29C45/53		13
B29C45/535	11	{using two or more cooperating injection rams, e.g. coaxially or alternately operating rams}	B29C45/53	B29C45/53		54
B29C2045/536	11	{rotatable injection plungers}	B29C45/53	B29C45/53		40
B29C2045/537	11	{the injection plunger cooperating with a coaxial hollow transfer plunger}	B29C45/53	B29C45/53		14
B29C2045/538	11	{the plunger being part of the mould cavity wall after injection}	B29C45/53	B29C45/53		20
B29C45/54	11	and plasticising screw {(B29C45/532 takes precedence)}	B29C45/54	B29C45/54		803
B29C45/541	12	{using a hollow plasticising screw co-operating with a coaxial injection ram}	B29C45/54	B29C45/54		83
B29C45/542	12	{using an accumulator between plasticising and injection unit, e.g. for a continuously operating plasticising screw}	B29C45/54	B29C45/54		116
B29C45/544	12	{the plasticising unit being connected to a transfer chamber in the injection unit at the upstream side of the injection piston}	B29C45/54	B29C45/54		78
B29C2045/545	12	{alternately operating injection plungers}	B29C45/54	B29C45/54		60
B29C2045/547	12	{continuously rotating plasticising screw cooperating with a single injection plunger (B29C45/542 takes precedence)}	B29C45/54	B29C45/54		72
B29C2045/548	12	{Reciprocating plasticising screws}	B29C45/54	B29C45/54		36
B29C45/56	10	using mould parts movable during or after injection, e.g. injection-compression moulding {(B29C45/1705 and B29C45/572 take precedence)}	B29C45/56	B29C45/56		662
B29C45/5605	11	{Rotatable mould parts}	B29C45/56	B29C45/56		115
B29C45/561	11	{Injection-compression moulding}	B29C45/56	B29C45/56		1542
B29C2045/5615	12	{Compression stroke, e.g. length thereof}	B29C45/56	B29C45/56		74
B29C2045/562	13	{Velocity profiles of the compression stroke}	B29C45/56	B29C45/56		42
B29C2045/5625	12	{Closing of the feed opening before or during compression}	B29C45/56	B29C45/56		77
B29C2045/563	12	{Enlarging the mould cavity during injection}	B29C45/56	B29C45/56		167
B29C2045/5635	12	{Mould integrated compression drive means}	B29C45/56	B29C45/56		109
B29C2045/564	12	{Compression drive means acting independently from the mould closing and clamping means}	B29C45/56	B29C45/56		83
B29C2045/5645	12	{Resilient compression means}	B29C45/56	B29C45/56		46
B29C2045/565	12	{Closing of the mould during injection}	B29C45/56	B29C45/56		64
B29C2045/5655	12	{using a screw mechanism as compression drive means}	B29C45/56	B29C45/56		16
B29C2045/566	12	{Reducing compression pressure during cooling of the moulded material}	B29C45/56	B29C45/56		12
B29C2045/5665	12	{Compression by transversely movable mould parts}	B29C45/56	B29C45/56		34
B29C2045/567	12	{Expelling resin through the gate}	B29C45/56	B29C45/56		26
B29C45/5675	11	{for making orifices in or through the moulded article}	B29C45/56	B29C45/56		162
B29C45/568	11	{Applying vibrations to the mould parts}	B29C45/56	B29C45/56		338
B29C2045/5685	12	{for eliminating internal voids in the moulding material}	B29C45/56	B29C45/56		82
B29C2045/569	11	{using a mould part for decreasing and a mould part for increasing the volume of the mould cavity}	B29C45/56	B29C45/56		36
B29C2045/5695	11	{using a movable mould part for continuously increasing the volume of the mould cavity to its final dimension during the whole injection step}	B29C45/56	B29C45/56		104
B29C45/57	10	Exerting after-pressure on the moulding material {(B29C45/174 takes precedence)}	B29C45/57	B29C45/57		358
B29C45/572	11	{using movable mould wall or runner parts}	B29C45/57	B29C45/57		248
B29C2045/575	12	{preventing backflow of moulding material to the injection means during after-pressure}	B29C45/57	B29C45/57		27
B29C2045/577	12	{pushing the material in the runner channel until a pin or slider reaches the mould cavity wall}	B29C45/57	B29C45/57		28
B29C45/58	10	Details	B29C45/58	B29C45/58		637
B29C45/581	11	{Devices for influencing the material flow, e.g. "torpedo constructions" or mixing devices}	B29C45/58	B29C45/58		536
B29C2045/583	12	{Mixing devices connected to drive means}	B29C45/58	B29C45/58		29
B29C45/585	11	{Vibration means for the injection unit or parts thereof}	B29C45/58	B29C45/58		96
B29C45/586	11	{Injection or transfer plungers}	B29C45/58	B29C45/58		307
B29C2045/588	12	{Means for retaining sprues on the end surface of the plunger}	B29C45/58	B29C45/58		15
B29C45/60	11	Screws	B29C45/60	B29C45/60		949
B29C2045/605	12	{comprising a zone or shape enhancing the degassing of the plastic material}	B29C45/60	B29C45/60		57
B29C45/62	11	Barrels or cylinders	B29C45/62	B29C45/62		733
B29C2045/623	12	{Cylinders and inner linings having different thermal expansion coefficients}	B29C45/62	B29C45/62		8
B29C2045/626	12	{Cylinders and inner linings having similar thermal expansion coefficients}	B29C45/62	B29C45/62		5
B29C45/63	11	Venting or degassing means	B29C45/63	B29C45/63		517
B29C45/64	9	Mould opening, closing or clamping devices {(combined with means for plasticising or homogenising B29C45/70)}	B29C45/64	B29C45/64		1124
B29C45/641	10	{Clamping devices using means for straddling or interconnecting the mould halves, e.g. jaws, straps, latches}	B29C45/64	B29C45/64		365
B29C2045/642	11	{using coupling rods for clamping}	B29C45/64	B29C45/64		30
B29C2045/644	10	{mould clamping by nozzle touch pressure}	B29C45/64	B29C45/64		3
B29C2045/645	10	{using magnetic means}	B29C45/64	B29C45/64		170
B29C2045/647	11	{using magnetostriction}	B29C45/64	B29C45/64		12
B29C2045/648	10	{Rack and pinion means for mould opening and closing a pair of mould halves}	B29C45/64	B29C45/64		62
B29C45/66	10	mechanical	B29C45/66	B29C45/66		1758
B29C45/661	11	{using a toggle mechanism for mould clamping}	B29C45/66	B29C45/66		467
B29C2045/662	12	{using toggles directly connected or linked to the fixed platen and indirectly to the movable platen}	B29C45/66	B29C45/66		32
B29C2045/664	11	{using mould clamping means operating independently from the mould closing means}	B29C45/66	B29C45/66		99
B29C2045/665	11	{using a screw or screws having differently threaded parts arranged in series}	B29C45/66	B29C45/66		91
B29C2045/667	11	{Cam drive for mould closing or clamping}	B29C45/66	B29C45/66		42
B29C2045/668	11	{using tilting elements for obtaining mould clamping}	B29C45/66	B29C45/66		24
B29C45/67	10	hydraulic	B29C45/67	B29C45/67		1543
B29C45/6707	11	{without relative movement between the piston and the cylinder of the clamping device during the mould opening or closing movement}	B29C45/67	B29C45/67		238
B29C45/6714	12	{using a separate element transmitting the mould clamping force from the clamping cylinder to the mould}	B29C45/67	B29C45/67		200
B29C45/6721	13	{the separate element being displaceable with respect to the mould or the clamping cylinder}	B29C45/67	B29C45/67		46
B29C45/6728	13	{the separate element consisting of coupling rods}	B29C45/67	B29C45/67		283
B29C2045/6735	14	{Rotatable means coaxial with the coupling rod for locking the coupling rod to the mould platen}	B29C45/67	B29C45/67		45
B29C2045/6742	14	{the coupling rods facilitating access between the mould halves}	B29C45/67	B29C45/67		12
B29C2045/675	12	{Rotatable means coaxial with the tie rod for locking the movable platen to the tie rod, e.g. bayonet couplings using teeth or splines interrupted by longitudinal grooves}	B29C45/67	B29C45/67		16
B29C2045/6757	12	{Hydraulic locking means}	B29C45/67	B29C45/67		55
B29C45/6764	11	{using hydraulically connectable chambers of the clamping cylinder during the mould opening and closing movement}	B29C45/67	B29C45/67		74
B29C45/6771	12	{the connection being provided within the clamping cylinder}	B29C45/67	B29C45/67		114
B29C45/6778	11	{Stroke adjusting or limiting means}	B29C45/67	B29C45/67		46
B29C2045/6785	11	{interconnecting two cylinders to supply fluid from one cylinder to the other during movement of the pistons}	B29C45/67	B29C45/67		27
B29C2045/6792	11	{Combined pneumatic-hydraulic cylinders}	B29C45/67	B29C45/67		80
B29C45/68	10	hydro-mechanical	B29C45/68	B29C45/68		628
B29C45/681	11	{using a toggle mechanism as mould clamping device}	B29C45/68	B29C45/68		306
B29C45/683	11	{using both a toggle mechanism as mould closing device and another mechanism as mould clamping device}	B29C45/68	B29C45/68		81
B29C2045/685	11	{using mechanical drive means for mould closing to obtain the hydraulic clamping pressure}	B29C45/68	B29C45/68		49
B29C2045/686	11	{using a screw and nut mechanism for mould closing and a mould clamping ram acting on another nut}	B29C45/68	B29C45/68		24
B29C2045/688	11	{using tie rods as separate elements for clamping}	B29C45/68	B29C45/68		73
B29C45/70	9	Means for plasticising or homogenising the moulding material or forcing it into the mould, combined with mould opening, closing or clamping devices	B29C45/70	B29C45/70		342
B29C2045/703	10	{using clamping and injection pressures that are proportional to each other}	B29C45/70	B29C45/70		8
B29C45/706	10	{using a single drive system providing both the mould closing and clamping pressure and also the injection pressure, e.g. using a fixed injection piston}	B29C45/70	B29C45/70		70
B29C45/72	9	Heating or cooling	B29C45/72	B29C45/72		1400
B29C45/7207	10	{of the moulded articles}	B29C45/72	B29C45/72		1570
B29C2045/7214	11	{Preform carriers for cooling preforms}	B29C45/72	B29C45/72		163
B29C2045/7221	12	{Means for ejecting the preforms}	B29C45/72	B29C45/72		25
B29C2045/7228	12	{turret-like}	B29C45/72	B29C45/72		24
B29C2045/7235	12	{Mechanical retaining means for preform ends}	B29C45/72	B29C45/72		11
B29C2045/7242	12	{Alignment means for preforms}	B29C45/72	B29C45/72		7
B29C2045/725	12	{Cooling circuits within the preform carriers}	B29C45/72	B29C45/72		35
B29C2045/7257	11	{Cooling or heating pins with temperature adjustment enhancing surface structure}	B29C45/72	B29C45/72		31
B29C2045/7264	11	{Cooling or heating the neck portion of preforms}	B29C45/72	B29C45/72		24
B29C2045/7271	10	{Cooling of drive motors}	B29C45/72	B29C45/72		70
B29C2045/7278	10	{Heating by friction of the moulding material}	B29C45/72	B29C45/72		18
B29C2045/7285	10	{using hydraulic oil as tempering medium}	B29C45/72	B29C45/72		13
B29C2045/7292	10	{Recovering waste heat}	B29C45/72	B29C45/72		130
B29C45/73	10	of the mould {(B29C45/2642 and B29C45/2737 take precedence)}	B29C45/73	B29C45/73		4267
B29C45/7306	11	{Control circuits therefor}	B29C45/73	B29C45/73		447
B29C45/7312	11	{Construction of heating or cooling fluid flow channels}	B29C45/73	B29C45/73		3230
B29C2045/7318	12	{multilayered fluid channel constructions}	B29C45/73	B29C45/73		260
B29C2045/7325	12	{Mould cavity linings for covering fluid channels or provided therewith}	B29C45/73	B29C45/73		46
B29C45/7331	11	{Heat transfer elements, e.g. heat pipes}	B29C45/73	B29C45/73		628
B29C45/7337	11	{using gas or steam (B29C45/7331 takes precedence)}	B29C45/73	B29C45/73		1167
B29C2045/7343	11	{heating or cooling different mould parts at different temperatures}	B29C45/73	B29C45/73		241
B29C2045/735	11	{heating a mould part and cooling another mould part during moulding}	B29C45/73	B29C45/73		78
B29C2045/7356	11	{the temperature of the mould being near or higher than the melting temperature or glass transition temperature of the moulding material}	B29C45/73	B29C45/73		111
B29C2045/7362	11	{turbulent flow of heating or cooling fluid}	B29C45/73	B29C45/73		91
B29C2045/7368	11	{combining a heating or cooling fluid and non-fluid means}	B29C45/73	B29C45/73		160
B29C2045/7375	11	{heating a mould surface by a heated gas}	B29C45/73	B29C45/73		56
B29C2045/7381	12	{heating by gas combustion}	B29C45/73	B29C45/73		19
B29C2045/7387	11	{jetting a cooling fluid onto the moulded article while still in the mould}	B29C45/73	B29C45/73		73
B29C2045/7393	11	{alternately heating and cooling}	B29C45/73	B29C45/73		217
B29C45/74	10	of the injection unit	B29C45/74	B29C45/74		1947
B29C45/76	9	Measuring, controlling or regulating {(measuring in general G01; controlling or regulating in general G05)}<br><br><u>NOTE</u><br><br> In groups B29C45/76&#160;-&#160;B29C45/80 it is desirable to add the indexing codes of B29C2945/76 relating to measuring, controlling or regulating in injection moulding 	B29C45/76	B29C45/76		6031
B29C2045/7606	10	{Controlling or regulating the display unit}	B29C45/76	B29C45/76		673
B29C45/7613	10	{the termination of flow of material into the mould}	B29C45/76	B29C45/76		265
B29C45/762	10	{the sequence of operations of an injection cycle}	B29C45/76	B29C45/76		284
B29C45/7626	10	{the ejection or removal of moulded articles}	B29C45/76	B29C45/76		560
B29C2045/7633	11	{Take out or gripping means}	B29C45/76	B29C45/76		217
B29C2045/764	11	{detecting or preventing overload of an ejector}	B29C45/76	B29C45/76		39
B29C45/7646	10	{viscosity}	B29C45/76	B29C45/76		176
B29C45/7653	10	{mould clamping forces}	B29C45/76	B29C45/76		617
B29C45/766	10	{the setting or resetting of moulding conditions, e.g. before starting a cycle}	B29C45/76	B29C45/76		710
B29C45/7666	10	{of power or energy, e.g. integral function of force}	B29C45/76	B29C45/76		259
B29C2045/7673	11	{Recovering energy or power from drive motors}	B29C45/76	B29C45/76		82
B29C45/768	10	{Detecting defective moulding conditions (B29C45/84 takes precedence)}	B29C45/76	B29C45/76		687
B29C45/7686	10	{the ejected articles, e.g. weight control}	B29C45/76	B29C45/76		419
B29C45/7693	10	{using rheological models of the material in the mould, e.g. finite elements method}	B29C45/76	B29C45/76		252
B29C45/77	10	of velocity or pressure of moulding material	B29C45/77	B29C45/77		3194
B29C2045/773	11	{Zero point correction}	B29C45/77	B29C45/77		36
B29C2045/776	11	{determining the switchover point to the holding pressure}	B29C45/77	B29C45/77		124
B29C45/78	10	of temperature	B29C45/78	B29C45/78		4419
B29C45/80	10	of relative position of mould parts	B29C45/80	B29C45/80		1030
B29C45/82	10	Hydraulic {or pneumatic} circuits	B29C45/82	B29C45/82		931
B29C2045/822	11	{Pneumatic circuits}	B29C45/82	B29C45/82		35
B29C2045/824	11	{Accumulators}	B29C45/82	B29C45/82		101
B29C2045/826	11	{Plurality of hydraulic actuators driven by one hydraulic pump}	B29C45/82	B29C45/82		41
B29C2045/828	11	{Bidirectional pumps}	B29C45/82	B29C45/82		22
B29C45/83	9	Lubricating means	B29C45/83	B29C45/83		485
B29C2045/835	10	{for ball screws or ball nuts}	B29C45/83	B29C45/83		49
B29C45/84	9	Safety devices {(B29C45/7626 takes precedence)}	B29C45/84	B29C45/84		1597
B29C45/842	10	{Detection of insert defects, e.g. inaccurate position, breakage}	B29C45/84	B29C45/84		100
B29C45/844	10	{Preventing damage caused by obstructions or foreign matter caught between mould halves during mould closing, e.g. moulded parts or runners}	B29C45/84	B29C45/84		175
B29C2045/846	10	{Windable safety screens}	B29C45/84	B29C45/84		15
B29C2045/848	10	{detecting or preventing overload of an injection plunger}	B29C45/84	B29C45/84		18
B29C48/00	7	Extrusion moulding, i.e. expressing the moulding material through a die or nozzle which imparts the desired form; Apparatus therefor (extrusion blow-moulding B29C49/04)	B29C48/00	B29C48/00		3712
B29C48/001	8	{Combinations of extrusion moulding with other shaping operations}	B29C48/00	B29C48/00		2182
B29C48/0011	9	{combined with compression moulding}	B29C48/00	B29C48/00		1964
B29C48/0012	9	{combined with shaping by internal pressure generated in the material, e.g. foaming}	B29C48/00	B29C48/00		1408
B29C48/0013	9	{Extrusion moulding in several steps, i.e. components merging outside the die (B29C48/15 takes precedence)}	B29C48/00	B29C48/00		129
B29C48/0014	10	{producing flat articles having components brought in contact outside the extrusion die}	B29C48/00	B29C48/00		379
B29C48/0015	10	{producing hollow articles having components brought in contact outside the extrusion die}	B29C48/00	B29C48/00		318
B29C48/0016	11	{using a plurality of extrusion dies}	B29C48/00	B29C48/00		314
B29C48/0017	9	{combined with blow-moulding or thermoforming}	B29C48/00	B29C48/00		1722
B29C48/0018	9	{combined with shaping by orienting, stretching or shrinking, e.g. film blowing (B29C48/0017 takes precedence)}	B29C48/00	B29C48/00		5642
B29C48/0019	9	{combined with shaping by flattening, folding or bending}	B29C48/00	B29C48/00		2322
B29C48/002	9	{combined with surface shaping}	B29C48/00	B29C48/00		914
B29C48/0021	9	{combined with joining, lining or laminating}	B29C48/00	B29C48/00		2038
B29C48/0022	9	{combined with cutting}	B29C48/00	B29C48/00		6465
B29C48/0023	9	{combined with printing or marking}	B29C48/00	B29C48/00		436
B29C48/02	8	Small extruding apparatus, e.g. handheld, toy or laboratory extruders	B29C48/02	B29C48/02		613
B29C48/022	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C48/00	B29C48/02		8557
B29C48/023	9	{Extruding materials comprising incompatible ingredients}	B29C48/00	B29C48/02		261
B29C48/025	8	General arrangement or layout of plant	B29C48/025	B29C48/025		461
B29C48/0255	9	{for extruding parallel streams of material, e.g. several separate parallel streams of extruded material forming separate articles (B29C48/0013, B29C48/345 takes precedence)}	B29C48/025	B29C48/025		144
B29C48/03	8	characterised by the shape of the extruded material at extrusion	B29C48/03	B29C48/03		9460
B29C48/04	9	Particle-shaped (making granules B29B9/00)	B29C48/04	B29C48/04		5400
B29C48/05	9	Filamentary, e.g. strands	B29C48/05	B29C48/05		8213
B29C48/06	9	Rod-shaped	B29C48/06	B29C48/06		5773
B29C48/07	9	Flat, e.g. panels	B29C48/07	B29C48/07		6912
B29C48/08	10	flexible, e.g. films	B29C48/08	B29C48/08		16633
B29C48/09	9	Articles with cross-sections having partially or fully enclosed cavities, e.g. pipes or channels	B29C48/09	B29C48/09		14836
B29C48/10	10	flexible, e.g. blown foils	B29C48/10	B29C48/10		8255
B29C48/11	10	comprising two or more partially or fully enclosed cavities, e.g. honeycomb-shaped	B29C48/11	B29C48/11		2132
B29C48/12	9	Articles with an irregular circumference when viewed in cross-section, e.g. window profiles	B29C48/12	B29C48/12		6307
B29C48/13	9	Articles with a cross-section varying in the longitudinal direction, e.g. corrugated pipes	B29C48/13	B29C48/13		3221
B29C48/131	9	{Curved articles}	B29C48/03	B29C48/13		473
B29C48/14	8	characterised by the particular extruding conditions, e.g. in a modified atmosphere or by using vibration	B29C48/14	B29C48/14		270
B29C48/141	9	{extruding in a clean room}	B29C48/14	B29C48/14		44
B29C48/142	9	{using force fields, e.g. gravity or electrical fields (B29C48/9165 takes precedence)}	B29C48/14	B29C48/14		142
B29C48/143	9	{at a location before or in the feed unit, e.g. influencing the material in the hopper}	B29C48/14	B29C48/14		63
B29C48/144	9	{at the plasticising zone}	B29C48/14	B29C48/14		72
B29C48/145	9	{at a venting zone}	B29C48/14	B29C48/14		34
B29C48/146	9	{in the die}	B29C48/14	B29C48/14		84
B29C48/147	9	{after the die nozzle}	B29C48/14	B29C48/14		48
B29C48/1472	10	{at the die nozzle exit zone}	B29C48/14	B29C48/14		270
B29C48/1474	10	{at a calibration zone}	B29C48/14	B29C48/14		51
B29C48/1476	10	{at a conveyor}	B29C48/14	B29C48/14		14
B29C48/1478	10	{at a storing zone}	B29C48/14	B29C48/14		3
B29C48/15	8	incorporating preformed parts or layers, e.g. extrusion moulding around inserts	B29C48/15	B29C48/15		2588
B29C48/151	9	Coating hollow articles	B29C48/151	B29C48/151		1500
B29C48/152	10	the inner surfaces thereof	B29C48/152	B29C48/152		201
B29C48/153	11	Coating both inner and outer surfaces	B29C48/153	B29C48/153		605
B29C48/154	9	Coating solid articles, i.e. non-hollow articles	B29C48/154	B29C48/154		2829
B29C48/155	10	Partial coating thereof	B29C48/155	B29C48/155		690
B29C48/156	9	Coating two or more articles simultaneously	B29C48/156	B29C48/156		773
B29C48/157	9	Coating linked inserts, e.g. chains	B29C48/157	B29C48/157		206
B29C48/16	8	Articles comprising two or more components, e.g. co-extruded layers	B29C48/16	B29C48/16		1029
B29C48/17	9	the components having different colours	B29C48/17	B29C48/17		838
B29C48/175	10	{comprising a multi-coloured single component, e.g. striated, marbled or wood-like patterned}	B29C48/17	B29C48/17		353
B29C48/18	9	the components being layers	B29C48/18	B29C48/18		3119
B29C48/185	10	{comprising six or more components, i.e. each component being counted once for each time it is present, e.g. in a layer}	B29C48/18	B29C48/18		244
B29C48/19	10	the layers being joined at their edges	B29C48/19	B29C48/19		918
B29C48/20	10	one of the layers being a strip, e.g. a partially embedded strip	B29C48/20	B29C48/20		372
B29C48/21	10	the layers being joined at their surfaces	B29C48/21	B29C48/21		7270
B29C48/22	10	with means connecting the layers, e.g. tie layers or undercuts	B29C48/22	B29C48/22		335
B29C48/23	10	with means for avoiding adhesion of the layers, e.g. for forming peelable layers	B29C48/23	B29C48/23		79
B29C48/25	8	Component parts, details or accessories; Auxiliary operations	B29C48/25	B29C48/25		1789
B29C48/251	9	{Design of extruder parts, e.g. by modelling based on mathematical theories or experiments}	B29C48/25	B29C48/25		82
B29C48/2511	10	{by modelling material flow, e.g. melt interaction with screw and barrel}	B29C48/25	B29C48/25		19
B29C48/2513	11	{in the plasticising zone}	B29C48/25	B29C48/25		16
B29C48/2515	11	{in the die zone}	B29C48/25	B29C48/25		16
B29C48/2517	10	{of intermeshing screws}	B29C48/25	B29C48/25		87
B29C48/2519	10	{by modelling of mechanical strength}	B29C48/25	B29C48/25		4
B29C48/252	9	{Drive or actuation means; Transmission means; Screw supporting means}	B29C48/25	B29C48/25		871
B29C48/2522	10	{Shaft or screw supports, e.g. bearings}	B29C48/25	B29C48/25		204
B29C48/2526	10	{Direct drives or gear boxes}	B29C48/25	B29C48/25		342
B29C48/2528	10	{Drive or actuation means for non-plasticising purposes, e.g. dosing unit}	B29C48/25	B29C48/25		242
B29C48/254	9	{Sealing means}	B29C48/25	B29C48/25		348
B29C48/2545	10	{for filters}	B29C48/25	B29C48/25		117
B29C48/255	9	Flow control means, e.g. valves (flow dividers B29C48/695)	B29C48/255	B29C48/255		228
B29C48/2552	10	{provided in the feeding, melting, plasticising or pumping zone, e.g. screw, barrel, gear-pump or ram}	B29C48/255	B29C48/255		206
B29C48/2554	10	{provided in or in the proximity of filter devices}	B29C48/255	B29C48/255		117
B29C48/2556	10	{provided in or in the proximity of dies (B29C48/302, B29C48/31, B29C48/325 take precedence)}	B29C48/255	B29C48/255		505
B29C48/256	9	{Exchangeable extruder parts (B29C48/691 takes precedence)}	B29C48/25	B29C48/25		318
B29C48/2561	10	{Mounting or handling of the screw}	B29C48/25	B29C48/25		158
B29C48/2562	10	{Mounting or handling of the die}	B29C48/25	B29C48/25		535
B29C48/2563	10	{Mounting or handling of the hopper or feeder}	B29C48/25	B29C48/25		35
B29C48/2564	10	{Screw parts}	B29C48/25	B29C48/25		292
B29C48/2565	10	{Barrel parts}	B29C48/25	B29C48/25		128
B29C48/2566	10	{Die parts}	B29C48/25	B29C48/25		357
B29C48/2567	10	{Hopper or feeder parts}	B29C48/25	B29C48/25		50
B29C48/2568	10	{Inserts}	B29C48/25	B29C48/25		11
B29C48/25682	11	{for screws}	B29C48/25	B29C48/25		23
B29C48/25684	11	{for barrels}	B29C48/25	B29C48/25		32
B29C48/25686	11	{for dies}	B29C48/25	B29C48/25		124
B29C48/265	9	Support structures or bases for apparatus, e.g. frames	B29C48/265	B29C48/265		376
B29C48/266	9	{Means for allowing relative movements between the apparatus parts, e.g. for twisting the extruded article or for moving the die along a surface to be coated}	B29C48/25	B29C48/266		448
B29C48/2665	10	{allowing small relative movement, e.g. adjustments for aligning the apparatus parts or for compensating for thermal expansion}	B29C48/25	B29C48/2665		110
B29C48/267	9	{Intermediate treatments, e.g. relaxation, annealing or decompression step for the melt (B29C48/76 takes precedence)}	B29C48/25	B29C48/267		117
B29C48/268	9	{Throttling of the flow, e.g. for cooperating with plasticising elements or for degassing (flow control means B29C48/255)}	B29C48/25	B29C48/268		331
B29C48/269	9	{Extrusion in non-steady condition, e.g. start-up or shut-down}	B29C48/25	B29C48/269		92
B29C48/2692	10	{Material change}	B29C48/25	B29C48/2692		96
B29C48/2694	10	{Intermittent extrusion}	B29C48/25	B29C48/2694		111
B29C48/27	9	Cleaning; Purging; Avoiding contamination	B29C48/27	B29C48/27		720
B29C48/271	10	{of feeding units}	B29C48/27	B29C48/27		211
B29C48/2715	10	{of plasticising units}	B29C48/27	B29C48/27		327
B29C48/272	10	{of dies}	B29C48/27	B29C48/27		347
B29C48/2725	10	{of filters}	B29C48/27	B29C48/27		210
B29C48/273	11	{using back flow}	B29C48/27	B29C48/27		130
B29C48/2735	11	{using scrapers}	B29C48/27	B29C48/27		137
B29C48/274	10	{of the extruded articles}	B29C48/27	B29C48/27		186
B29C48/275	9	Recovery or reuse of energy or materials	B29C48/275	B29C48/275		44
B29C48/276	10	{of energy}	B29C48/275	B29C48/27		227
B29C48/277	10	{of materials}	B29C48/275	B29C48/27		369
B29C48/278	11	{of additives or processing aids}	B29C48/275	B29C48/27		30
B29C48/28	9	Storing of extruded material, e.g. by winding up or stacking	B29C48/28	B29C48/28		988
B29C48/285	9	Feeding the extrusion material to the extruder	B29C48/285	B29C48/285		1576
B29C48/286	10	{Raw material dosing}	B29C48/285	B29C48/28		918
B29C48/287	10	{Raw material pre-treatment while feeding (B29C48/78 takes precedence)}	B29C48/285	B29C48/28		1413
B29C48/288	10	{in solid form, e.g. powder or granules}	B29C48/285	B29C48/28		1998
B29C48/2883	11	{of preformed parts, e.g. inserts, retaining their shape during the extrusion process}	B29C48/285	B29C48/28		345
B29C48/2886	11	{of fillers or of fibrous materials, e.g. short-fibre reinforcements}	B29C48/285	B29C48/28		963
B29C48/2888	11	{in thread form or in strip form, e.g. rubber strips}	B29C48/285	B29C48/28		423
B29C48/29	10	in liquid form	B29C48/29	B29C48/29		1425
B29C48/295	10	in gaseous form	B29C48/295	B29C48/295		150
B29C48/297	10	{at several locations, e.g. using several hoppers or using a separate additive feeding}	B29C48/285	B29C48/29		1039
B29C48/298	10	{in a location other than through a barrel, e.g. through a screw}	B29C48/285	B29C48/29		166
B29C48/30	9	Extrusion nozzles or dies (extrusion characterised by the shape or cross-section of the extruded article B29C48/03)	B29C48/30	B29C48/30		2906
B29C48/3001	10	{characterised by the material or their manufacturing process}	B29C48/30	B29C48/30		281
B29C48/3003	11	{Materials, coating or lining therefor}	B29C48/30	B29C48/30		244
B29C48/301	10	{having reciprocating, oscillating or rotating parts}	B29C48/30	B29C48/30		520
B29C48/302	10	{being adjustable, i.e. having adjustable exit sections}	B29C48/30	B29C48/30		537
B29C48/303	10	{using dies or die parts movable in a closed circuit, e.g. mounted on movable endless support (B29C48/35 takes precedence)}	B29C48/30	B29C48/30		588
B29C48/304	10	{specially adapted for bringing together components, e.g. melts within the die}	B29C48/30	B29C48/30		1053
B29C48/305	10	having a wide opening, e.g. for forming sheets	B29C48/305	B29C48/305		1886
B29C48/307	11	{specially adapted for bringing together components, e.g. melts within the die}	B29C48/305	B29C48/30		1183
B29C48/31	11	{being} adjustable {, i.e. having adjustable exit sections}	B29C48/31	B29C48/31		571
B29C48/313	12	{by positioning the die lips}	B29C48/31	B29C48/31		687
B29C48/315	11	with parts oscillating relative to each other	B29C48/315	B29C48/315		31
B29C48/32	10	with annular openings, e.g. for forming tubular articles	B29C48/32	B29C48/32		3376
B29C48/325	11	{being} adjustable {, i.e. having adjustable exit sections}	B29C48/325	B29C48/325		862
B29C48/327	12	{with centering means}	B29C48/325	B29C48/32		292
B29C48/33	11	with parts rotatable relative to each other	B29C48/33	B29C48/33		759
B29C48/335	11	Multiple annular extrusion nozzles in coaxial arrangement, e.g. for making multi-layered tubular articles	B29C48/335	B29C48/335		1181
B29C48/336	12	{the components merging one by one down streams in the die}	B29C48/335	B29C48/33		267
B29C48/3363	13	{using a layered die, e.g. stacked discs}	B29C48/335	B29C48/33		203
B29C48/3366	13	{using a die with concentric parts, e.g. rings, cylinders}	B29C48/335	B29C48/33		265
B29C48/337	12	{the components merging at a common location}	B29C48/335	B29C48/33		197
B29C48/338	13	{using a die with concentric parts, e.g. rings, cylinders}	B29C48/335	B29C48/33		366
B29C48/34	11	Cross-head annular extrusion nozzles, i.e. for simultaneously receiving moulding material and the preform to be coated	B29C48/34	B29C48/34		2270
B29C48/345	10	Extrusion nozzles comprising two or more adjacently arranged ports, for simultaneously extruding multiple strands, e.g. for pelletising	B29C48/345	B29C48/345		2093
B29C48/35	10	with rollers	B29C48/35	B29C48/35		799
B29C48/355	9	Conveyors for extruded articles	B29C48/355	B29C48/355		2369
B29C48/36	9	Means for plasticising or homogenising the moulding material or forcing it through the nozzle or die	B29C48/36	B29C48/36		354
B29C48/361	10	{with the barrel or with a part thereof rotating}	B29C48/36	B29C48/36		97
B29C48/362	10	{using static mixing devices}	B29C48/36	B29C48/36		771
B29C48/363	10	{using non-actuated dynamic mixing devices}	B29C48/36	B29C48/36		59
B29C48/365	10	using pumps, e.g. piston pumps	B29C48/365	B29C48/365		322
B29C48/37	11	Gear pumps	B29C48/37	B29C48/37		894
B29C48/375	10	Plasticisers, homogenisers or feeders comprising two or more stages	B29C48/375	B29C48/375		178
B29C48/38	11	using two or more serially arranged screws in the same barrel	B29C48/38	B29C48/38		692
B29C48/385	11	using two or more serially arranged screws in separate barrels	B29C48/385	B29C48/385		973
B29C48/387	11	{using a screw extruder and a gear pump}	B29C48/375	B29C48/38		687
B29C48/388	11	{using a screw extruder and a ram or piston}	B29C48/375	B29C48/38		233
B29C48/39	11	a first extruder feeding the melt into an intermediate location of a second extruder	B29C48/39	B29C48/39		756
B29C48/395	10	using screws surrounded by a cooperating barrel, e.g. single screw extruders	B29C48/395	B29C48/395		2928
B29C48/397	11	{using a single screw}	B29C48/395	B29C48/39		1798
B29C48/40	11	using two or more parallel screws {or at least two parallel non-intermeshing screws}, e.g. twin screw extruders	B29C48/40	B29C48/40		5988
B29C48/402	12	{the screws having intermeshing parts}	B29C48/40	B29C48/40		923
B29C48/404	12	{the screws having non-intermeshing parts}	B29C48/40	B29C48/40		133
B29C48/405	12	Intermeshing co-rotating screws	B29C48/405	B29C48/405		1234
B29C48/41	12	Intermeshing counter-rotating screws	B29C48/41	B29C48/41		717
B29C48/415	12	and having partially non-intermeshing screws	B29C48/415	B29C48/415		12
B29C48/42	12	Non-identical or non-mirrored screws	B29C48/42	B29C48/42		152
B29C48/425	12	using three or more screws (serially arranged screws B29C48/38, B29C48/385)	B29C48/425	B29C48/425		269
B29C48/43	13	Ring extruders	B29C48/43	B29C48/43		136
B29C48/435	12	Sub-screws	B29C48/435	B29C48/435		414
B29C48/44	13	Planetary screws	B29C48/44	B29C48/44		382
B29C48/445	11	Coaxially arranged screws, i.e. one within the other	B29C48/445	B29C48/445		171
B29C48/45	11	Axially movable screws	B29C48/45	B29C48/45		288
B29C48/455	11	Screws arranged to convey material towards each other, e.g. separate screws arranged after each other and feeding in opposite directions	B29C48/455	B29C48/455		137
B29C48/46	10	using vanes	B29C48/46	B29C48/46		140
B29C48/465	10	using rollers	B29C48/465	B29C48/465		355
B29C48/467	11	{using single rollers, e.g. provided with protrusions, closely surrounded by a housing with movement of the material in the axial direction}	B29C48/465	B29C48/46		67
B29C48/468	12	{Cavity transfer mixing devices, i.e. a roller and surrounding barrel both provided with cavities; Barrels and rollers therefor}	B29C48/465	B29C48/46		86
B29C48/47	10	using discs, e.g. plasticising the moulding material by passing it between a fixed and a rotating disc that are coaxially arranged	B29C48/47	B29C48/47		240
B29C48/475	10	using pistons, accumulators or press rams	B29C48/475	B29C48/475		1010
B29C48/48	11	Two or more rams or pistons	B29C48/48	B29C48/48		153
B29C48/485	11	Hydrostatic extrusion	B29C48/485	B29C48/485		18
B29C48/49	10	using two or more extruders to feed one die or nozzle	B29C48/49	B29C48/49		1400
B29C48/495	11	Feedblocks (extrusion moulding of multi-component articles B29C48/16)	B29C48/495	B29C48/495		264
B29C48/50	10	Details of extruders	B29C48/50	B29C48/50		426
B29C48/501	11	{Extruder feed section}	B29C48/50	B29C48/50		391
B29C48/503	11	{Extruder machines or parts thereof characterised by the material or by their manufacturing process (B29C48/256 takes precedence)}	B29C48/50	B29C48/50		99
B29C48/505	11	Screws	B29C48/505	B29C48/505		827
B29C48/507	12	{characterised by the material or their manufacturing process}	B29C48/505	B29C48/50		244
B29C48/509	13	{Materials, coating or lining therefor}	B29C48/505	B29C48/50		177
B29C48/51	12	with internal flow passages, e.g. for molten material	B29C48/51	B29C48/51		241
B29C48/515	13	for auxiliary fluids, e.g. foaming agents	B29C48/515	B29C48/515		354
B29C48/52	12	with an outer diameter varying along the longitudinal axis, e.g. for obtaining different thread clearance	B29C48/52	B29C48/52		391
B29C48/525	13	Conical screws	B29C48/525	B29C48/525		490
B29C48/53	12	having a varying channel depth, e.g. varying the diameter of the longitudinal screw trunk	B29C48/53	B29C48/53		1590
B29C48/535	12	with thread pitch varying along the longitudinal axis	B29C48/535	B29C48/535		943
B29C48/54	12	with additional forward-feeding elements	B29C48/54	B29C48/54		386
B29C48/55	12	having reverse-feeding elements	B29C48/55	B29C48/55		465
B29C48/56	12	having grooves or cavities other than the thread or the channel	B29C48/56	B29C48/56		546
B29C48/565	12	having projections other than the thread, e.g. pins	B29C48/565	B29C48/565		539
B29C48/57	12	provided with kneading disc-like elements, e.g. with oval-shaped elements	B29C48/57	B29C48/57		968
B29C48/575	12	provided with elements of a generally circular cross-section for shearing the melt, i.e. shear-ring elements	B29C48/575	B29C48/575		203
B29C48/58	12	provided with seal ring elements, i.e. elements of generally circular and tapered shape for preventing the back flow of the melt	B29C48/58	B29C48/58		102
B29C48/585	12	provided with gears interacting with the flow	B29C48/585	B29C48/585		182
B29C48/59	12	characterised by details of the thread, i.e. the shape of a single thread of the material-feeding screw	B29C48/59	B29C48/59		238
B29C48/595	13	the thread having non-uniform width	B29C48/595	B29C48/595		50
B29C48/60	13	Thread tops	B29C48/60	B29C48/60		165
B29C48/605	13	the thread being discontinuous	B29C48/605	B29C48/605		116
B29C48/61	13	Threads having wavy profiles	B29C48/61	B29C48/61		20
B29C48/615	13	Threads having varying helix angles	B29C48/615	B29C48/615		38
B29C48/62	12	characterised by the shape of the thread channel, e.g. U-shaped	B29C48/62	B29C48/62		249
B29C48/625	12	characterised by the ratio of the threaded length of the screw to its outside diameter [L/D ratio]	B29C48/625	B29C48/625		1003
B29C48/63	12	having sections without mixing elements or threads, i.e. having cylinder shaped sections	B29C48/63	B29C48/63		364
B29C48/635	12	Eccentrically rotating screws; Screws revolving around an axis other than their central axis	B29C48/635	B29C48/635		77
B29C48/64	12	Screws with two or more threads	B29C48/64	B29C48/64		291
B29C48/645	13	neighbouring threads and channels having identical configurations	B29C48/645	B29C48/645		128
B29C48/65	13	neighbouring threads or channels having different configurations, e.g. one thread being lower than its neighbouring thread	B29C48/65	B29C48/65		385
B29C48/655	13	having three or more threads	B29C48/655	B29C48/655		170
B29C48/66	13	Barrier threads, i.e. comprising primary and secondary threads whereby the secondary thread provides clearance to the barrel for material movement	B29C48/66	B29C48/66		77
B29C48/67	12	having incorporated mixing devices not provided for in groups B29C48/52 - B29C48/66	B29C48/67	B29C48/67		901
B29C48/68	11	Barrels or cylinders	B29C48/68	B29C48/68		450
B29C48/6801	12	{characterised by the material or their manufacturing process}	B29C48/68	B29C48/68		240
B29C48/6803	12	{Materials, coating or lining therefor}	B29C48/68	B29C48/68		91
B29C48/681	12	{for single screws}	B29C48/68	B29C48/68		231
B29C48/682	12	{for twin screws}	B29C48/68	B29C48/68		364
B29C48/683	12	{for more than two screws}	B29C48/68	B29C48/68		53
B29C48/684	12	{having adaptable feed or discharge locations, e.g. for varying the amount of kneading by changing hopper position or discharge exit}	B29C48/68	B29C48/68		35
B29C48/685	12	characterised by their inner surfaces, e.g. having grooves, projections or threads	B29C48/685	B29C48/685		89
B29C48/686	13	{having grooves or cavities}	B29C48/685	B29C48/68		422
B29C48/687	13	{having projections with a short length in the barrel direction, e.g. pins}	B29C48/685	B29C48/68		368
B29C48/688	13	{having threads}	B29C48/685	B29C48/68		141
B29C48/69	11	Filters or screens for the moulding material	B29C48/69	B29C48/69		821
B29C48/691	12	Arrangements for replacing filters, e.g. with two parallel filters for alternate use	B29C48/691	B29C48/691		169
B29C48/6912	13	{the filters being fitted on a single rectilinearly reciprocating slide (B29C48/692 takes precedence)}	B29C48/691	B29C48/691		304
B29C48/6914	13	{the filters being fitted on a rotatable or pivotable disc or on the circumference of a rotatable or pivotable cylinder}	B29C48/691	B29C48/691		141
B29C48/6916	14	{Continuously rotating cylindrical filters}	B29C48/691	B29C48/691		29
B29C48/692	12	in the form of webs displaceable for using adjacent areas consecutively	B29C48/692	B29C48/692		92
B29C48/693	12	Substantially flat filters mounted at the end of an extruder screw perpendicular to the feed axis	B29C48/693	B29C48/693		402
B29C48/694	12	Cylindrical or conical filters	B29C48/694	B29C48/694		260
B29C48/6945	13	{surrounding a rotating screw}	B29C48/694	B29C48/694		52
B29C48/695	11	Flow dividers, e.g. breaker plates	B29C48/695	B29C48/695		398
B29C48/70	12	comprising means for dividing, distributing and recombining melt flows	B29C48/70	B29C48/70		465
B29C48/705	13	{in the die zone, e.g. to create flow homogeneity}	B29C48/70	B29C48/70		498
B29C48/71	13	for layer multiplication (extrusion of multi-component articles B29C48/16)	B29C48/71	B29C48/71		228
B29C48/72	11	Feedback means, i.e. part of the molten material being fed back into upstream stages of the extruder	B29C48/72	B29C48/72		34
B29C48/725	12	{for plasticising or homogenising devices}	B29C48/72	B29C48/72		71
B29C48/74	11	Bypassing means, i.e. part of the molten material being diverted into downstream stages of the extruder	B29C48/74	B29C48/74		97
B29C48/745	12	{for plasticising or homogenising devices}	B29C48/74	B29C48/74		84
B29C48/76	11	Venting {, drying} means; Degassing means	B29C48/76	B29C48/76		874
B29C48/761	12	{the vented material being in liquid form}	B29C48/76	B29C48/76		118
B29C48/762	12	{Vapour stripping}	B29C48/76	B29C48/76		192
B29C48/763	12	{Vent constructions, e.g. venting means avoiding melt escape}	B29C48/76	B29C48/76		289
B29C48/765	12	{in the extruder apparatus}	B29C48/76	B29C48/76		82
B29C48/766	13	{in screw extruders}	B29C48/76	B29C48/76		489
B29C48/767	14	{through a degassing opening of a barrel}	B29C48/76	B29C48/76		815
B29C48/768	12	{outside the apparatus, e.g. after the die}	B29C48/76	B29C48/76		64
B29C48/78	9	Thermal treatment of the extrusion moulding material or of preformed parts or layers, e.g. by heating or cooling	B29C48/78	B29C48/78		232
B29C48/79	10	of preformed parts or layers	B29C48/79	B29C48/79		178
B29C48/793	10	upstream of the plasticising zone, e.g. heating in the hopper	B29C48/793	B29C48/793		787
B29C48/797	11	Cooling	B29C48/797	B29C48/797		169
B29C48/80	10	at the plasticising zone, e.g. by heating cylinders	B29C48/80	B29C48/80		151
B29C48/802	11	{Heating}	B29C48/80	B29C48/80		679
B29C48/82	11	Cooling (B29C48/84 takes precedence)	B29C48/82	B29C48/82		325
B29C48/83	11	{Heating or cooling the cylinders}	B29C48/80	B29C48/83		668
B29C48/832	12	{Heating}	B29C48/80	B29C48/832		2009
B29C48/834	12	{Cooling}	B29C48/80	B29C48/834		868
B29C48/84	11	by heating or cooling the feeding screws (for hollow screws B29C48/515)	B29C48/84	B29C48/84		264
B29C48/845	12	{Heating}	B29C48/84	B29C48/84		355
B29C48/85	12	Cooling	B29C48/85	B29C48/85		353
B29C48/86	10	at the nozzle zone	B29C48/86	B29C48/86		732
B29C48/865	11	{Heating}	B29C48/86	B29C48/86		1409
B29C48/87	11	Cooling	B29C48/87	B29C48/87		1058
B29C48/872	11	{characterised by differential heating or cooling}	B29C48/86	B29C48/87		114
B29C48/873	12	{in the direction of the stream of the material}	B29C48/86	B29C48/87		60
B29C48/875	10	for achieving a non-uniform temperature distribution, e.g. using barrels having both cooling and heating zones	B29C48/875	B29C48/875		1388
B29C48/88	9	Thermal treatment of the stream of extruded material, e.g. cooling<br><br><u>NOTE</u><br><br>When classifying in this group, forms or shapes of products are further classified in groups B29C48/03 - B29C48/13	B29C48/88	B29C48/88		338
B29C48/885	10	External treatment, e.g. by using air rings for cooling tubular films	B29C48/885	B29C48/885		3584
B29C48/89	10	Internal treatment, e.g. by applying an internal cooling fluid stream	B29C48/89	B29C48/89		354
B29C48/90	10	with calibration or sizing, i.e. combined with fixing or setting of the final dimensions of the extruded article	B29C48/90	B29C48/90		1015
B29C48/901	11	{of hollow bodies}	B29C48/90	B29C48/90		526
B29C48/902	12	{internally}	B29C48/90	B29C48/90		528
B29C48/903	12	{externally}	B29C48/90	B29C48/90		1184
B29C48/904	11	{using dry calibration, i.e. no quenching tank, e.g. with water spray for cooling or lubrication}	B29C48/90	B29C48/90		776
B29C48/905	11	{using wet calibration, i.e. in a quenching tank}	B29C48/90	B29C48/90		589
B29C48/906	11	{using roller calibration}	B29C48/90	B29C48/90		330
B29C48/907	11	{using adjustable calibrators, e.g. the dimensions of the calibrator being changeable}	B29C48/90	B29C48/90		296
B29C48/908	11	{characterised by calibrator surface, e.g. structure or holes for lubrication, cooling or venting}	B29C48/90	B29C48/90		1250
B29C48/91	10	Heating, e.g. for cross linking	B29C48/91	B29C48/91		1737
B29C48/9105	11	{of hollow articles}	B29C48/91	B29C48/91		183
B29C48/911	10	{Cooling}	B29C48/88	B29C48/91		2439
B29C48/9115	11	{of hollow articles}	B29C48/88	B29C48/91		1271
B29C48/912	12	{of tubular films}	B29C48/88	B29C48/91		2327
B29C48/9135	11	{of flat articles, e.g. using specially adapted supporting means}	B29C48/88	B29C48/91		1597
B29C48/914	12	{Cooling drums}	B29C48/88	B29C48/91		2674
B29C48/9145	12	{Endless cooling belts}	B29C48/88	B29C48/91		335
B29C48/915	12	{with means for improving the adhesion to the supporting means}	B29C48/88	B29C48/91		78
B29C48/9155	13	{Pressure rollers}	B29C48/88	B29C48/91		369
B29C48/916	13	{using vacuum}	B29C48/88	B29C48/91		389
B29C48/9165	13	{Electrostatic pinning}	B29C48/88	B29C48/91		363
B29C48/917	13	{by applying pressurised gas to the surface of the flat article}	B29C48/88	B29C48/91		277
B29C48/9175	12	{by interposing a fluid layer between the supporting means and the flat article}	B29C48/88	B29C48/91		156
B29C48/918	10	{characterized by differential heating or cooling}	B29C48/88	B29C48/91		146
B29C48/9185	11	{in the direction of the stream of the material}	B29C48/88	B29C48/91		363
B29C48/919	10	{using a bath, e.g. extruding into an open bath to coagulate or cool the material}	B29C48/88	B29C48/91		3478
B29C48/92	9	Measuring, controlling or regulating<br><br><u>NOTE</u><br><br>When classifying in group  B29C48/92 it is desirable to add the indexing codes of B29C2948/00 relating to measuring, controlling or regulating in extrusion moulding 	B29C48/92	B29C48/92		20628
B29C48/94	9	Lubricating	B29C48/94	B29C48/94		345
B29C48/95	10	by adding lubricant to the moulding material	B29C48/95	B29C48/95		190
B29C48/96	9	Safety devices	B29C48/96	B29C48/96		272
B29C48/965	10	{Personnel safety, e.g. safety for the operator}	B29C48/96	B29C48/96		65
B29C49/00	7	Blow-moulding, i.e. blowing a preform or parison to a desired shape within a mould; Apparatus therefor	B29C49/00	B29C49/00		578
B29C49/0005	8	{characterised by the material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest	B29C49/00	B29C49/00		1346
B29C49/0006	9	{for heating or cooling}	B29C49/00	B29C49/00		244
B29C49/0015	8	{Making articles of indefinite length, e.g. corrugated tubes}	B29C49/00	B29C49/00		130
B29C49/0021	9	{using moulds or mould parts movable in a closed path, e.g. mounted on movable endless supports}	B29C49/00	B29C49/00		357
B29C49/0022	10	{characterised by mould return means}	B29C49/00	B29C49/00		83
B29C49/0023	9	{using adjustable machine tables, e.g. to align extrusion nozzles with the moulds}	B29C49/00	B29C49/00		10
B29C49/0024	9	{using varying mould speed}	B29C49/00	B29C49/00		23
B29C49/0025	9	{subsequent mould cavities being different, e.g. for making bells}	B29C49/00	B29C49/00		58
B29C49/0027	9	{involving the change of moulds, e.g. in production processes without interrupting the production processes}	B29C49/00	B29C49/00		26
B29C49/0028	9	{using variable forming length, e.g. adapted to cooling needs}	B29C49/00	B29C49/00		11
B29C49/0029	9	{wherein the process is characterised by the pressure used, e.g. using varying pressure depending on sequence of cavity shapes}	B29C49/00	B29C49/00		54
B29C49/003	9	{wherein the process is characterised by temperature conditioning, e.g. using inside cooling by air}	B29C49/00	B29C49/00		33
B29C49/0031	8	{Making articles having hollow walls}	B29C49/00	B29C49/00		265
B29C49/0042	8	{without using a mould (B29C49/1602 takes precedence)}	B29C49/00	B29C49/00		114
B29C49/006	8	{Blow-moulding plants, e.g. using several blow-moulding apparatuses cooperating}	B29C49/00	B29C49/00		76
B29C49/0062	9	{using two or more parallel stations, e.g. two parallel heating or blowing stations}	B29C49/00	B29C49/00		23
B29C49/0064	10	{the number of preform manufacturing stations being different to the number of blowing stations}	B29C49/00	B29C49/00		27
B29C49/02	8	Combined blow-moulding and manufacture of the preform or the parison	B29C49/02	B29C49/02		288
B29C49/0208	9	{joining several separate preforms while blow-moulding, e.g. two cylindrical preforms welded together during blowing}	B29C49/02	B29C49/02		53
B29C2049/023	9	{using inherent heat of the preform, i.e. 1 step blow moulding}	B29C49/02	B29C49/02		2159
B29C2049/024	9	{not using inherent heat of the preform, i.e. 2 step blow moulding}	B29C49/02	B29C49/02		166
B29C49/04	9	Extrusion blow-moulding	B29C49/04	B29C49/04		3793
B29C49/041	10	{using an accumulator head}	B29C49/04	B29C49/04		265
B29C49/04102	10	{extruding the material continuously}	B29C49/04	B29C49/04		488
B29C49/04104	10	{extruding the material discontinuously}	B29C49/04	B29C49/04		144
B29C49/04106	10	{Means for moving the extruder head up and down, e.g. to continue extruding the next parison while blow-moulding the previous parison in the blow-mould}	B29C49/04	B29C49/04		40
B29C49/04108	10	{extruding several parisons parallel to each other at the same time}	B29C49/04	B29C49/04		170
B29C49/0411	10	{Means for defining the wall or layer thickness}	B29C49/04	B29C49/04		289
B29C49/04112	11	{for varying the thickness}	B29C49/04	B29C49/04		227
B29C49/04114	11	{for keeping constant thickness}	B29C49/04	B29C49/04		389
B29C49/04116	10	{characterised by the die}	B29C49/04	B29C49/04		218
B29C49/04118	10	{Means for supporting the extruded parison}	B29C49/04	B29C49/04		94
B29C49/0412	10	{Means for cutting the extruded preform}	B29C49/04	B29C49/04		133
B29C49/06	9	Injection blow-moulding	B29C49/06	B29C49/06		5652
B29C49/061	10	{with parison holding means displaceable between injection and blow stations}	B29C49/06	B29C49/06		120
B29C49/062	11	{following an arcuate path, e.g. rotary or oscillating-type}	B29C49/06	B29C49/06		227
B29C49/063	12	{with the parison axis held in the plane of rotation}	B29C49/06	B29C49/06		186
B29C49/064	11	{following a rectilinear path, e.g. shuttle-type}	B29C49/06	B29C49/06		131
B29C2049/065	10	{Means for compensating or avoiding the shrinking of preforms, e.g. in the injection mould or outside the injection mould}	B29C49/06	B29C49/06		21
B29C49/0665	10	{the injection mould cavity and the blow-mould cavity being displaceable to the geometrically fixed injection core mould}	B29C49/06	B29C49/06		35
B29C49/0685	9	{Compression blow-moulding}	B29C49/02	B29C49/06		159
B29C49/06905	9	{Using combined techniques for making the preform}	B29C49/02	B29C49/06		19
B29C49/0691	10	{using sheet like material, e.g. sheet blow-moulding from joined sheets}	B29C49/02	B29C49/06		681
B29C49/06912	11	{using folded sheets as a preform, e.g. folded into parallel sheets or rolled into cylindrical shape}	B29C49/02	B29C49/06		29
B29C49/06914	11	{using parallel sheets as a preform}	B29C49/02	B29C49/06		135
B29C49/06916	11	{Means for avoiding parts of the sheets to stick together, e.g. to provide blow opening}	B29C49/02	B29C49/06		95
B29C49/071	8	{Preforms or parisons characterised by their configuration, e.g. geometry, dimensions or physical properties}	B29C49/00	B29C49/071		2104
B29C49/08	8	Biaxial stretching during blow-moulding	B29C49/08	B29C49/08		414
B29C49/085	9	{without pre-stretching, e.g. simple blowing step}	B29C49/08	B29C49/08		21
B29C49/086	9	{mono-axial stretching, e.g. either length or width}	B29C49/08	B29C49/08		18
B29C49/087	9	{Means for providing controlled or limited stretch ratio}	B29C49/08	B29C49/08		261
B29C49/0871	10	{radial stretch ratio, i.e. hoop or tangential stretch ratio}	B29C49/08	B29C49/08		18
B29C49/0872	10	{axial stretch ratio}	B29C49/08	B29C49/08		34
B29C49/10	9	using mechanical means {for prestretching}	B29C49/10	B29C49/10		213
B29C49/12	10	Stretching rods	B29C49/12	B29C49/12		1247
B29C49/1202	11	{Means for fixing the stretching rod to the driving means, e.g. clamping means or bayonet connections}	B29C49/12	B29C49/12		39
B29C49/1205	11	{relative rotation between the preform and the stretch rod}	B29C49/12	B29C49/12		15
B29C49/1206	11	{using at least two stretching rods for stretching different parts of the preform}	B29C49/12	B29C49/12		10
B29C49/1208	11	{using additional means to clamp the preform bottom while stretching the preform}	B29C49/12	B29C49/12		69
B29C49/121	11	{Stretching rod configuration, e.g. geometry; Stretching rod material}	B29C49/12	B29C49/12		19
B29C49/1212	12	{the stretching rod comprising at least one opening on the surface, e.g. through which compressed air is blown into the preform to expand the same}	B29C49/12	B29C49/12		86
B29C49/1215	12	{Geometry of the stretching rod, e.g. specific stretching rod end shape}	B29C49/12	B29C49/12		103
B29C49/1216	12	{Material for stretching rods or parts thereof, e.g. heat insulating material}	B29C49/12	B29C49/12		18
B29C49/1218	11	{to stretch heated tubes}	B29C49/12	B29C49/12		12
B29C49/122	10	{Drive means therefor}	B29C49/10	B29C49/12		52
B29C49/1222	11	{Pneumatic}	B29C49/10	B29C49/12		106
B29C49/1224	11	{Hydraulic}	B29C49/10	B29C49/12		48
B29C49/1226	11	{Mechanical}	B29C49/10	B29C49/12		27
B29C49/1229	11	{being a cam mechanism}	B29C49/10	B29C49/12		103
B29C49/123	11	{Electric drives, e.g. linear motors}	B29C49/10	B29C49/12		128
B29C49/1232	11	{Magnetic}	B29C49/10	B29C49/12		23
B29C49/14	10	Clamps	B29C49/14	B29C49/14		204
B29C49/16	9	using pressure difference {for pre-stretching}, e.g. pre-blowing	B29C49/16	B29C49/16		257
B29C49/1602	10	{pre-blowing without using a mould}	B29C49/16	B29C49/16		94
B29C49/18	8	using several blowing steps (B29C49/16 takes precedence)	B29C49/18	B29C49/18		499
B29C49/1802	9	{the first mould cavity being bigger than a second mould cavity}	B29C49/18	B29C49/18		24
B29C49/20	8	of articles having inserts or reinforcements {; Handling of inserts or reinforcements}	B29C49/20	B29C49/20		1368
B29C2049/2008	9	{inside the article}	B29C49/20	B29C49/20		483
B29C2049/2013	10	{for connecting opposite walls, e.g. baffles in a fuel tank}	B29C49/20	B29C49/20		149
B29C2049/2017	9	{outside the article}	B29C49/20	B29C49/20		573
B29C2049/2021	9	{Inserts characterised by the material or type}	B29C49/20	B29C49/20		34
B29C2049/2026	10	{Neck portions}	B29C49/20	B29C49/20		134
B29C2049/203	10	{Carpets}	B29C49/20	B29C49/20		12
B29C2049/2034	10	{Attachments, e.g. hooks to hold or hang the blown article}	B29C49/20	B29C49/20		42
B29C2049/2039	11	{Handles, e.g. handles or grips on bottles}	B29C49/20	B29C49/20		158
B29C2049/2043	10	{comprising threads, e.g. screws or nuts}	B29C49/20	B29C49/20		73
B29C2049/2047	10	{Tubular inserts, e.g. tubes}	B29C49/20	B29C49/20		162
B29C2049/2052	10	{having means to avoid that the preform or parison gets into contact with parts of the insert}	B29C49/20	B29C49/20		7
B29C2049/2056	10	{being constructed in such a way that opposite preform or parison walls do not touch each other during extrusion or mould closing}	B29C49/20	B29C49/20		5
B29C2049/206	10	{being constructed in such a way that the joining between the insert and the preform or parison is avoided}	B29C49/20	B29C49/20		29
B29C2049/2065	10	{for reinforcing specific areas of the final blow moulded article}	B29C49/20	B29C49/20		64
B29C2049/2069	10	{moulded in combination, e.g. injection moulded in the same mould before or after blow-moulding}	B29C49/20	B29C49/20		68
B29C2049/2071	10	{comprising electronic elements or detection means, e.g. chips, RFIDs or barcodes}	B29C49/20	B29C49/20		31
B29C2049/2073	9	{Means for feeding the inserts into the mould, preform or parison, e.g. grippers}	B29C49/20	B29C49/20		148
B29C2049/2078	10	{being retractable during or after blow moulding}	B29C49/20	B29C49/20		40
B29C2049/2082	10	{Feeding the insert and the preform at the same time, e.g. using the same feeding means for the insert and the preform}	B29C49/20	B29C49/20		20
B29C2049/2086	9	{Means for verifying or keeping the position of the insert, e.g. sensors, or attachment on mould wall}	B29C49/20	B29C49/20		28
B29C2049/2095	9	{Means for preparing or treating the inserts, e.g. cutting, deforming, heating, cooling or applying adhesives}	B29C49/20	B29C49/20		43
B29C49/22	8	using multilayered preforms or parisons	B29C49/22	B29C49/22		1254
B29C2049/222	9	{only parts of the preforms or parisons are layered}	B29C49/22	B29C49/22		45
B29C49/24	8	Lining or labelling	B29C49/24	B29C49/24		570
B29C2049/2404	9	{inside the article}	B29C49/24	B29C49/24		201
B29C49/2408	9	{In-mould lining or labelling}	B29C49/24	B29C49/24		317
B29C2049/2412	9	{outside the article}	B29C49/24	B29C49/24		306
B29C2049/2414	9	{Linings or labels, e.g. specific geometry, multi-layered or material}	B29C49/24	B29C49/24		28
B29C2049/2422	10	{Cylindrical or sleeve shaped linings or labels}	B29C49/24	B29C49/24		32
B29C2049/2425	10	{Perforated, corrugated or embossed labels}	B29C49/24	B29C49/24		21
B29C2049/2429	10	{Multilayered labels}	B29C49/24	B29C49/24		27
B29C2049/24302	10	{Label materials}	B29C49/24	B29C49/24		33
B29C2049/24304	11	{using identical material for the label and the preform}	B29C49/24	B29C49/24		20
B29C2049/24306	11	{using different material for the label and the preform}	B29C49/24	B29C49/24		45
B29C2049/24308	10	{comprising electronic elements or detection means, e.g. chips, RFIDs or barcodes}	B29C49/24	B29C49/24		26
B29C2049/2431	9	{Means for preparing or treating the label or lining, e.g. cutting, deforming, heating or applying adhesive}	B29C49/24	B29C49/24		8
B29C2049/2433	10	{Heating or applying adhesive}	B29C49/24	B29C49/24		27
B29C2049/2435	11	{in a specific pattern}	B29C49/24	B29C49/24		8
B29C2049/2437	10	{Cutting}	B29C49/24	B29C49/24		24
B29C2049/2439	11	{by means in the mould cavity}	B29C49/24	B29C49/24		8
B29C2049/2441	10	{Deforming}	B29C49/24	B29C49/24		15
B29C2049/2442	11	{while blow-moulding, e.g. the preform expansion deforms the label or lining}	B29C49/24	B29C49/24		49
B29C2049/2443	9	{Means for feeding the lining or label into the mould, preform or parison, e.g. grippers}	B29C49/24	B29C49/24		20
B29C2049/2445	10	{holding the labels or linings by magnetic force}	B29C49/24	B29C49/24		2
B29C2049/2447	10	{holding the labels or linings by electrostatic force}	B29C49/24	B29C49/24		7
B29C2049/2449	10	{holding the labels or linings by vacuum}	B29C49/24	B29C49/24		59
B29C2049/2452	10	{being a transfer foil}	B29C49/24	B29C49/24		10
B29C2049/2454	10	{for placing labels at the same time in two opposite mould cavities}	B29C49/24	B29C49/24		65
B29C2049/2456	10	{and removing with the same means the final article}	B29C49/24	B29C49/24		9
B29C2049/2458	9	{Driving or transporting means related to lining or labelling}	B29C49/24	B29C49/24		4
B29C2049/246	10	{Cams}	B29C49/24	B29C49/24		1
B29C2049/2462	10	{Conveyor belts}	B29C49/24	B29C49/24		10
B29C2049/2464	9	{Means for verifying or keeping the position of the lining or label, e.g. sensors, or attachment on mould wall}	B29C49/24	B29C49/24		6
B29C2049/2466	10	{using electrostatic force}	B29C49/24	B29C49/24		16
B29C2049/2468	10	{using magnetic force}	B29C49/24	B29C49/24		4
B29C2049/247	10	{using needles}	B29C49/24	B29C49/24		2
B29C2049/2472	10	{using vacuum}	B29C49/24	B29C49/24		73
B29C2049/2474	10	{using adhesive}	B29C49/24	B29C49/24		8
B29C2049/2479	9	{Label or lining movements}	B29C49/24	B29C49/24		3
B29C2049/2481	10	{vertical only}	B29C49/24	B29C49/24		9
B29C2049/2483	10	{horizontal only}	B29C49/24	B29C49/24		27
B29C2049/2485	10	{multidirectional}	B29C49/24	B29C49/24		6
B29C2049/2487	10	{comprising a rotary movement}	B29C49/24	B29C49/24		5
B29C49/249	9	{explicit labelling}	B29C49/24	B29C49/24		14
B29C49/251	9	{explicit lining (B29C49/26 takes precedence)}	B29C49/24	B29C49/251		78
B29C49/26	9	inner lining of tubes	B29C49/26	B29C49/26		133
B29C49/28	8	Blow-moulding apparatus	B29C49/28	B29C49/28		723
B29C49/28002	9	{designed for reduced size or for experiments, e.g. lower inertia, transportable or experimental apparatus}	B29C49/28	B29C49/28		16
B29C49/28004	9	{designed for easy access by operator}	B29C49/28	B29C49/28		34
B29C49/28006	9	{having special frame}	B29C49/28	B29C49/28		81
B29C49/28008	9	{mounting, exchanging or centering machine parts, e.g. modular parts}	B29C49/28	B29C49/28		103
B29C49/28012	9	{using several moulds whereby at least one mould is different in at least one feature, e.g. size or shape (B29C49/0025 takes precedence)}	B29C49/28	B29C49/28		17
B29C49/30	9	having movable moulds or mould parts	B29C49/30	B29C49/30		191
B29C49/32	10	moving "to and fro"	B29C49/32	B29C49/32		327
B29C2049/325	11	{by using guide rails}	B29C49/32	B29C49/32		37
B29C49/34	11	the mould parts moving "hand-over-hand"	B29C49/34	B29C49/34		47
B29C49/36	10	rotatable about one axis	B29C49/36	B29C49/36		1262
B29C49/38	10	mounted on movable endless supports {(B29C49/0021 takes precedence)}	B29C49/38	B29C49/38		94
B29C49/40	11	on co-operating drums	B29C49/40	B29C49/40		19
B29C49/42	8	Component parts, details or accessories; Auxiliary operations	B29C49/42	B29C49/42		782
B29C49/4205	9	{Handling means, e.g. transfer, loading or discharging means (handling of inserts or reinforcements B29C49/20; handling of linings or labels B29C49/2408)}	B29C49/42	B29C49/42		673
B29C49/42051	10	{Means for stripping, aligning or de-stacking}	B29C49/42	B29C49/42		40
B29C49/42053	11	{Stripping preforms from moulds, e.g. from injection moulds or cores}	B29C49/42	B29C49/42		23
B29C49/42055	11	{De-stacking preforms, e.g. delivered in a stacked configuration}	B29C49/42	B29C49/42		19
B29C49/42057	11	{Aligning disorderly arranged preforms, e.g. delivered disorderly}	B29C49/42	B29C49/42		161
B29C49/42059	11	{Aligning of preforms getting stuck, unaligned or stacked during transport}	B29C49/42	B29C49/42		18
B29C49/42061	11	{Means for correcting, aligning or straighten preforms, e.g. gripper with correcting means}	B29C49/42	B29C49/42		19
B29C49/42063	12	{in relation to the mould, e.g. preform centring means in the mould}	B29C49/42	B29C49/42		28
B29C49/42065	10	{Means specially adapted for transporting preforms}	B29C49/42	B29C49/42		264
B29C49/42067	11	{Extruded preforms, e.g. providing means for avoiding deformation of the soft preform}	B29C49/42	B29C49/42		39
B29C49/42069	10	{Means explicitly adapted for transporting blown article}	B29C49/42	B29C49/42		564
B29C49/4207	11	{with stacking means, e.g. stacking the articles for further transport}	B29C49/42	B29C49/42		11
B29C49/42071	10	{Temperature conditioned transport, e.g. insulated or heated transport means}	B29C49/42	B29C49/42		19
B29C49/42073	10	{Grippers}	B29C49/42	B29C49/42		448
B29C49/42075	11	{with pivoting clamps}	B29C49/42	B29C49/42		147
B29C49/42077	11	{with U-shaped holder}	B29C49/42	B29C49/42		60
B29C49/42079	11	{using vacuum for gripping}	B29C49/42	B29C49/42		55
B29C49/42081	11	{adjustable for different preform size}	B29C49/42	B29C49/42		29
B29C49/42083	11	{being inflatable}	B29C49/42	B29C49/42		6
B29C49/42085	11	{holding inside the neck}	B29C49/42	B29C49/42		393
B29C49/42087	11	{holding outside the neck}	B29C49/42	B29C49/42		228
B29C49/42089	11	{holding body portion}	B29C49/42	B29C49/42		28
B29C49/42091	11	{holding bottom portion or sprue}	B29C49/42	B29C49/42		22
B29C49/42093	10	{Transporting apparatus, e.g. slides, wheels or conveyors}	B29C49/42	B29C49/42		183
B29C49/42095	11	{Rotating wheels or stars}	B29C49/42	B29C49/42		415
B29C49/42097	11	{Sliding rails, e.g. inclined}	B29C49/42	B29C49/42		133
B29C49/42099	12	{Pushing by air}	B29C49/42	B29C49/42		17
B29C49/42101	11	{Conveyors, e.g. flat conveyor or clamping between two bands}	B29C49/42	B29C49/42		434
B29C49/42103	11	{Vacuum suction pipes}	B29C49/42	B29C49/42		15
B29C49/42105	11	{for discontinuous or batch transport}	B29C49/42	B29C49/42		171
B29C49/42107	11	{with accumulator or temporary storage, e.g. while waiting for the blowing apparatus}	B29C49/42	B29C49/42		38
B29C49/42109	12	{keeping temperature of accumulated preforms or articles, e.g. the accumulator being an oven}	B29C49/42	B29C49/42		19
B29C49/42111	11	{with changeable transporting paths or lengths}	B29C49/42	B29C49/42		24
B29C49/42113	10	{Means for manipulating the objects&apos; position or orientation}	B29C49/42	B29C49/42		21
B29C49/42115	11	{Inversion, e.g. turning preform upside down}	B29C49/42	B29C49/42		68
B29C49/42117	11	{Translation e.g. telescopic movement to pick up a preform}	B29C49/42	B29C49/42		48
B29C49/42119	11	{Rotation, e.g. rotating a predetermined angle for asymmetric preform or with asymmetric heat profile}	B29C49/42	B29C49/42		128
B29C49/42121	11	{Changing the center-center distance}	B29C49/42	B29C49/42		30
B29C49/42122	12	{Adapting to blow-mould cavity center-center distance}	B29C49/42	B29C49/42		141
B29C49/42155	11	{Keeping center-center distance constant}	B29C49/42	B29C49/42		13
B29C49/4236	9	{Drive means}	B29C49/42	B29C49/42		198
B29C49/42362	10	{Electric drive means, e.g. servomotors}	B29C49/42	B29C49/42		139
B29C49/4237	10	{Pneumatic drive means}	B29C49/42	B29C49/42		41
B29C49/42372	10	{Hydraulic drive means}	B29C49/42	B29C49/42		45
B29C49/42374	10	{for the extruder, e.g. extruder moving up and down}	B29C49/42	B29C49/42		8
B29C49/42376	10	{for moulds other than opening, closing and clamping}	B29C49/42	B29C49/42		4
B29C49/42378	9	{Handling malfunction}	B29C49/42	B29C49/42		73
B29C49/4238	10	{Ejecting defective preforms or products}	B29C49/42	B29C49/42		159
B29C49/42382	10	{Stopping at least a part of the machine}	B29C49/42	B29C49/42		17
B29C49/42384	9	{Safety, e.g. operator safety}	B29C49/42	B29C49/42		46
B29C49/42386	9	{Improving flash formation, e.g. providing for easily removable flash from extrusion moulded articles}	B29C49/42	B29C49/42		15
B29C49/42388	9	{Eliminating electric charge}	B29C49/42	B29C49/42		9
B29C49/4239	9	{Avoiding condense, e.g. on cooled mould surfaces}	B29C49/42	B29C49/42		11
B29C49/42392	9	{Avoiding marks or scratches, e.g. mould marks}	B29C49/42	B29C49/42		18
B29C49/42394	9	{Providing specific wall thickness}	B29C49/42	B29C49/42		92
B29C49/42396	10	{Avoiding excessive thickness differences, e.g. thinning of corners}	B29C49/42	B29C49/42		31
B29C49/42398	9	{Simulation of the blow-moulding process}	B29C49/42	B29C49/42		34
B29C49/424	10	{Simulation of the preform conditioning process}	B29C49/42	B29C49/42		6
B29C49/42402	10	{Simulation of the shaping process}	B29C49/42	B29C49/42		17
B29C49/42403	9	{Purging or cleaning the blow-moulding apparatus}	B29C49/42	B29C49/42		85
B29C49/42405	10	{Sterilizing}	B29C49/42	B29C49/42		148
B29C49/42407	9	{Procedures for start-up or material change}	B29C49/42	B29C49/42		45
B29C49/42408	10	{Temperature conditioning, e.g. pre-heating of the moulds}	B29C49/42	B29C49/42		17
B29C49/42409	10	{Special pressurization during start-up of the machine}	B29C49/42	B29C49/42		
B29C49/4241	10	{Material change}	B29C49/42	B29C49/42		14
B29C49/42412	9	{Marking or printing}	B29C49/42	B29C49/42		46
B29C49/42413	10	{with a pattern for analysing deformation}	B29C49/42	B29C49/42		26
B29C49/42414	9	{Treatment of preforms, e.g. cleaning or spraying water for improved heat transfer}	B29C49/42	B29C49/42		77
B29C49/42416	10	{Purging or cleaning the preforms}	B29C49/42	B29C49/42		26
B29C49/42418	11	{for sterilizing}	B29C49/42	B29C49/42		166
B29C49/4242	9	{Means for deforming the parison prior to the blowing operation (B29C49/08 takes precedence)}	B29C49/42	B29C49/42		329
B29C49/42421	10	{before laying into the mould}	B29C49/42	B29C49/42		31
B29C49/42422	11	{by the preform transporting means}	B29C49/42	B29C49/42		54
B29C49/42424	11	{Deforming or closing the preform ends, e.g. pinching and welding}	B29C49/42	B29C49/42		47
B29C49/42426	11	{by pressure difference deforming parts of the preform}	B29C49/42	B29C49/42		20
B29C49/42428	11	{in a separate pre-moulding station}	B29C49/42	B29C49/42		7
B29C49/4244	10	{during or after laying preform into the final mould}	B29C49/42	B29C49/42		3
B29C49/42442	11	{by moving the extruder head}	B29C49/42	B29C49/42		23
B29C49/42444	11	{by moving the transport means}	B29C49/42	B29C49/42		30
B29C49/42446	11	{by using a robot arm or similar actuator}	B29C49/42	B29C49/42		12
B29C49/42448	11	{by moving the mould}	B29C49/42	B29C49/42		25
B29C49/4245	11	{aided by air floating}	B29C49/42	B29C49/42		53
B29C49/42452	11	{The mould opening plane being horizontal}	B29C49/42	B29C49/42		61
B29C49/42454	11	{The mould opening plane being vertical}	B29C49/42	B29C49/42		78
B29C49/4247	10	{using spreading or extending means}	B29C49/42	B29C49/42		150
B29C49/425	11	{rods or bars entering the preform}	B29C49/42	B29C49/42		94
B29C49/4251	10	{by foaming}	B29C49/42	B29C49/42		1
B29C49/4252	9	{Auxiliary operations prior to the blow-moulding operation not otherwise provided for}	B29C49/42	B29C49/42		324
B29C49/4268	9	{Auxiliary operations during the blow-moulding operation}	B29C49/42	B29C49/42		118
B29C49/427	10	{Auxiliary deformation, i.e. not caused by pre-stretching or blowing not otherwise provided for}	B29C49/42	B29C49/42		6
B29C49/4273	9	{Auxiliary operations after the blow-moulding operation not otherwise provided for}	B29C49/42	B29C49/42		518
B29C49/4278	10	{Cutting}	B29C49/42	B29C49/42		365
B29C49/428	10	{Joining}	B29C49/42	B29C49/42		13
B29C49/42802	11	{a closure or a sealing foil to the article or pincing the opening}	B29C49/42	B29C49/42		322
B29C49/42806	11	{auxiliary parts to the article, e.g. handle (B29C49/42802 takes precedence)}	B29C49/42	B29C49/42		32
B29C49/42808	10	{Filling the article}	B29C49/42	B29C49/42		358
B29C49/42809	11	{while in the mould, i.e. with other material than the blowing fluid}	B29C49/42	B29C49/42		36
B29C49/4281	11	{outside the mould}	B29C49/42	B29C49/42		34
B29C49/42811	11	{Introducing an auxiliary material not being the content, e.g. foamable material in a hollow wall section}	B29C49/42	B29C49/42		7
B29C49/42815	10	{Emptying the article, e.g. emptying hydraulic blowing fluid}	B29C49/42	B29C49/42		16
B29C49/42817	10	{Drying the article}	B29C49/42	B29C49/42		15
B29C49/4282	10	{Purging or cleaning the article}	B29C49/42	B29C49/42		11
B29C49/42822	11	{Sterilizing the article}	B29C49/42	B29C49/42		74
B29C49/42824	10	{Cooling the article outside the mould}	B29C49/42	B29C49/42		37
B29C49/42826	10	{Separating burr or other part from the article, e.g. using mechanical means}	B29C49/42	B29C49/42		27
B29C49/42828	10	{Coating or painting the article}	B29C49/42	B29C49/42		45
B29C49/4283	10	{Deforming the finished article}	B29C49/42	B29C49/42		124
B29C49/42832	11	{Moving or inverting sections, e.g. inverting bottom as vacuum panel}	B29C49/42	B29C49/42		86
B29C49/42834	11	{Foaming, expanding or stretching the article}	B29C49/42	B29C49/42		11
B29C49/42836	11	{Collapsing or folding the article, e.g. to save space for transport}	B29C49/42	B29C49/42		28
B29C49/4284	9	{Means for recycling or reusing auxiliaries or materials, e.g. blowing fluids or energy}	B29C49/42	B29C49/42		49
B29C49/42845	10	{Recycling or reusing of fluid, e.g. pressure}	B29C49/42	B29C49/42		39
B29C49/4285	11	{Reactive gases}	B29C49/42	B29C49/42		8
B29C49/42855	11	{Blowing fluids, e.g. reducing fluid consumption}	B29C49/42	B29C49/42		128
B29C49/4286	10	{Recycling or reusing of heat energy}	B29C49/42	B29C49/42		38
B29C49/42865	10	{Recycling or reusing of electric energy}	B29C49/42	B29C49/42		3
B29C49/4287	10	{for use outside the blow-moulding apparatus, e.g. generating power or as pressurized plant air}	B29C49/42	B29C49/42		10
B29C49/4289	9	{Valve constructions or configurations, e.g. arranged to reduce blowing fluid consumption}	B29C49/42	B29C49/42		321
B29C2049/4294	9	{Sealing means}	B29C49/42	B29C49/42		210
B29C2049/4296	10	{for avoiding blowing fluid from leaking, e.g. between the blowing means and the preform neck}	B29C49/42	B29C49/42		8
B29C2049/4298	10	{for sealing clean or sterile room or volume}	B29C49/42	B29C49/42		14
B29C2049/431	10	{for sealing moulds, e.g. for vacuum air floating}	B29C49/42	B29C2049/431		14
B29C49/44	9	for applying pressure through the walls of an inflated bag	B29C49/44	B29C49/44		223
B29C2049/445	10	{having wall areas with different elasticity}	B29C49/44	B29C49/44		4
B29C49/46	9	characterised by using particular environment or blow fluids other than air	B29C49/46	B29C49/46		750
B29C2049/4602	10	{Blowing fluids}	B29C49/46	B29C49/46		30
B29C2049/4605	11	{containing an inert gas, e.g. helium}	B29C49/46	B29C49/46		59
B29C2049/4608	12	{Nitrogen}	B29C49/46	B29C49/46		126
B29C2049/4611	11	{containing a reactive gas}	B29C49/46	B29C49/46		5
B29C2049/4614	12	{Chlorine}	B29C49/46	B29C49/46		3
B29C2049/4617	12	{Fluor}	B29C49/46	B29C49/46		41
B29C2049/462	12	{Oxygen}	B29C49/46	B29C49/46		12
B29C2049/4623	12	{the gas containing sulfur, e.g. sulfur trioxide}	B29C49/46	B29C49/46		35
B29C2049/4626	11	{containing carbon dioxide}	B29C49/46	B29C49/46		34
B29C2049/4629	11	{containing a polar gas}	B29C49/46	B29C49/46		4
B29C2049/4632	11	{being filtered air}	B29C49/46	B29C49/46		20
B29C2049/4635	11	{being sterile}	B29C49/46	B29C49/46		119
B29C2049/4638	11	{being a hot gas, i.e. gas with a temperature higher than ambient temperature}	B29C49/46	B29C49/46		64
B29C2049/4641	11	{being a cooled gas, i.e. gas with a temperature lower than ambient temperature}	B29C49/46	B29C49/46		13
B29C2049/4644	11	{created by evaporating material, e.g. solid powder}	B29C49/46	B29C49/46		26
B29C2049/4647	11	{created by an explosive gas mixture}	B29C49/46	B29C49/46		42
B29C2049/465	11	{being incompressible}	B29C49/46	B29C49/46		162
B29C2049/4652	12	{hot liquids}	B29C49/46	B29C49/46		53
B29C2049/4655	12	{water}	B29C49/46	B29C49/46		81
B29C2049/4658	12	{oil}	B29C49/46	B29C49/46		10
B29C2049/4661	12	{solid media, e.g. powder (B29C2049/4644 takes precedence)}	B29C49/46	B29C49/46		8
B29C2049/4664	12	{staying in the final article}	B29C49/46	B29C49/46		342
B29C2049/4667	11	{being foamable}	B29C49/46	B29C49/46		19
B29C2049/467	11	{created by thermal expansion of enclosed amount of gas, e.g. heating enclosed air in preforms or parisons}	B29C49/46	B29C49/46		8
B29C2049/4673	10	{Environments}	B29C49/46	B29C49/46		26
B29C2049/4676	11	{being dry air to surround or flush parts of the blow moulding apparatus, e.g. blow mould, preforms or parisons}	B29C49/46	B29C49/46		22
B29C2049/4679	11	{Sterile gas to surround or flush parts of the blow-moulding apparatus, e.g. blowing means, preforms or parisons}	B29C49/46	B29C49/46		81
B29C2049/4697	11	{Clean room}	B29C49/46	B29C49/46		234
B29C2049/4698	11	{Pressure difference, e.g. over pressure in room}	B29C49/46	B29C49/46		78
B29C2049/4699	11	{Air conditioned room}	B29C49/46	B29C49/46		7
B29C49/48	9	Moulds	B29C49/48	B29C49/48		1692
B29C49/4802	10	{with means for locally compressing part(s) of the parison in the main blowing cavity}	B29C49/48	B29C49/48		601
B29C2049/4805	11	{by closing the mould halves}	B29C49/48	B29C49/48		245
B29C2049/4807	11	{by movable mould parts in the mould halves}	B29C49/48	B29C49/48		383
B29C2049/481	12	{the movable mould parts moving outwardly, e.g. the mould size being increased due to the movement of the movable mould parts}	B29C49/48	B29C49/48		21
B29C49/4812	11	{and welding opposite wall parts of the parisons or preforms to each other}	B29C49/48	B29C49/48		199
B29C49/4815	12	{by means of movable mould parts}	B29C49/48	B29C49/48		58
B29C49/4817	11	{with means for closing off parison ends}	B29C49/48	B29C49/48		334
B29C49/48185	10	{with more than one separate mould cavity}	B29C49/48	B29C49/48		311
B29C49/4819	11	{having different sizes or shapes of the mould cavities}	B29C49/48	B29C49/48		59
B29C49/482	10	{with means for moulding parts of the parisons in an auxiliary cavity, e.g. moulding a handle}	B29C49/48	B29C49/48		188
B29C49/4823	10	{with incorporated heating or cooling means}	B29C49/48	B29C49/48		788
B29C2049/4825	11	{for cooling moulds or mould parts (B29C2049/5889 takes precedence)}	B29C49/48	B29C49/48		290
B29C2049/483	12	{in different areas of the mould at different temperatures, e.g. neck, shoulder or bottom}	B29C49/48	B29C49/48		34
B29C2049/4833	12	{the cooling means being connected to an external heat exchanger}	B29C49/48	B29C49/48		18
B29C2049/4835	12	{releasing the blowing fluid via the cooling channels of the moulds}	B29C49/48	B29C49/48		14
B29C2049/4838	11	{for heating moulds or mould parts}	B29C49/48	B29C49/48		155
B29C2049/4846	12	{in different areas of the mould at different temperatures, e.g. neck, shoulder or bottom}	B29C49/48	B29C49/48		43
B29C2049/4848	13	{Bottom}	B29C49/48	B29C49/48		76
B29C2049/4851	13	{Side walls}	B29C49/48	B29C49/48		22
B29C2049/4853	11	{with means for improving heat transfer between the mould cavity and the preform}	B29C49/48	B29C49/48		12
B29C2049/4854	11	{Heating or cooling from the inside of the cavity, e.g. using flames or other means}	B29C49/48	B29C49/48		15
B29C2049/4856	10	{Mounting, exchanging or centering moulds or parts thereof (B29C2049/5893 takes precedence)}	B29C49/48	B29C49/48		254
B29C2049/4858	11	{Exchanging mould parts, e.g. for changing the mould size or geometry for making different products in the same mould}	B29C49/48	B29C49/48		232
B29C2049/4861	12	{Neck portions of bottle producing moulds}	B29C49/48	B29C49/48		30
B29C2049/48615	11	{Aligning the mould assembly position e.g. adapting center to the extruded parison}	B29C49/48	B29C49/48		33
B29C2049/4862	11	{Aligning the mould part position e.g. left half to right half}	B29C49/48	B29C49/48		39
B29C2049/4863	11	{Mould identification, e.g. chip on mould with ID and process data}	B29C49/48	B29C49/48		26
B29C2049/4864	11	{Fixed by a special construction to the mould half carriers, e.g. using insulating material between the mould and the mould half carrier}	B29C49/48	B29C49/48		95
B29C2049/4866	12	{center the moulds with the mould half carriers}	B29C49/48	B29C49/48		9
B29C49/487105	10	{characterised by the manufacturing process}	B29C49/48	B29C49/48		57
B29C2049/4874	10	{characterised by the material, e.g. having different thermal conductivities or hardness}	B29C49/48	B29C49/48		55
B29C2049/4876	11	{one material being heat insulating material}	B29C49/48	B29C49/48		39
B29C2049/4879	10	{characterised by mould configurations}	B29C49/48	B29C49/48		111
B29C2049/4881	11	{having a mandrel or core e.g. two mould halves with a core in-between}	B29C49/48	B29C49/48		246
B29C2049/4882	11	{Mould cavity geometry}	B29C49/48	B29C49/48		117
B29C2049/48825	12	{Asymmetric moulds, i.e. the parison is not in the center of the mould}	B29C49/48	B29C49/48		63
B29C2049/4883	12	{having cavity parts avoiding preform contact, e.g. partial free blow}	B29C49/48	B29C49/48		3
B29C2049/4884	11	{Mould halves are made of one piece}	B29C49/48	B29C49/48		22
B29C2049/4887	11	{Mould halves consisting of an independent neck and main part}	B29C49/48	B29C49/48		54
B29C2049/4889	11	{Mould halves consisting of an independent neck, main and bottom part}	B29C49/48	B29C49/48		119
B29C2049/4892	11	{Mould halves consisting of an independent main and bottom part}	B29C49/48	B29C49/48		439
B29C2049/4894	11	{With at least a part of the mould cavity formed by a cylindrical mould}	B29C49/48	B29C49/48		27
B29C49/50	10	having cutting or deflashing means	B29C49/50	B29C49/50		625
B29C2049/503	11	{being independently movable during the mould closing}	B29C49/50	B29C49/50		45
B29C2049/506	11	{being heated}	B29C49/50	B29C49/50		11
B29C49/52	10	having decorating or printing means	B29C49/52	B29C49/52		141
B29C49/54	10	for undercut articles	B29C49/54	B29C49/54		227
B29C49/541	11	{having a recessed undersurface}	B29C49/54	B29C49/54		192
B29C2049/542	11	{having means to facilitate the removal of the blow moulded articles}	B29C49/54	B29C49/54		3
B29C2049/543	12	{at the neck portion}	B29C49/54	B29C49/54		24
B29C2049/545	12	{by rotationally actuating an auxiliary mould part while the mould is still in a closed position}	B29C49/54	B29C49/54		10
B29C2049/546	12	{by translatorilly actuating an auxiliary mould part while the mould is still in a closed position}	B29C49/54	B29C49/54		96
B29C2049/547	12	{which are self actuated during the removing of the blow moulded articles, e.g. the means are spring loaded or flexible}	B29C49/54	B29C49/54		33
B29C2049/548	12	{the movement of the mould parts during opening of the mould are interlinked}	B29C49/54	B29C49/54		55
B29C49/56	9	Opening, closing or clamping means	B29C49/56	B29C49/56		659
B29C49/5601	10	{Mechanically operated, i.e. closing or opening of the mould parts is done by mechanic means}	B29C49/56	B29C49/56		103
B29C49/5602	11	{using cams}	B29C49/56	B29C49/56		287
B29C49/5603	11	{using toggle mechanism}	B29C49/56	B29C49/56		157
B29C49/5604	11	{using spindle nut mechanism}	B29C49/56	B29C49/56		17
B29C49/5605	10	{Hydraulically operated, i.e. closing or opening of the mould parts is done by hydraulic means}	B29C49/56	B29C49/56		159
B29C49/5606	10	{Pneumatically operated, i.e. closing or opening of the mould parts is done by hydraulic means}	B29C49/56	B29C49/56		57
B29C49/5607	10	{Electrically operated, e.g. the closing or opening is done with an electrical motor direct drive}	B29C49/56	B29C49/56		87
B29C49/5608	10	{Asymmetric movement of mould parts, e.g. by moving only one mould part}	B29C49/56	B29C49/56		89
B29C49/561	10	{Characterised by speed, e.g. variable opening closing speed}	B29C49/56	B29C49/56		180
B29C49/5611	10	{Tilting movement, e.g. changing angle of the mould parts towards the vertical direction}	B29C49/56	B29C49/56		16
B29C49/5612	10	{characterised by bottom part movement}	B29C49/56	B29C49/56		57
B29C49/5613	10	{characterised by connected mould part movement, e.g. bottom part movement is linked to mould half movement}	B29C49/56	B29C49/56		42
B29C49/5614	10	{Safety means, e.g. during ejection or locking failure}	B29C49/56	B29C49/56		16
B29C2049/563	10	{Clamping means}	B29C49/56	B29C49/56		114
B29C2049/5631	11	{Hydraulic}	B29C49/56	B29C49/56		32
B29C2049/5632	11	{Magnetic}	B29C49/56	B29C49/56		3
B29C2049/5633	11	{Pneumatic}	B29C49/56	B29C49/56		43
B29C2049/5634	11	{Electric, e.g. electric motor}	B29C49/56	B29C49/56		11
B29C2049/5635	11	{Avoiding mould deformation}	B29C49/56	B29C49/56		35
B29C2049/5636	10	{using closing means as clamping means}	B29C49/56	B29C49/56		54
B29C2049/566	10	{Locking means}	B29C49/56	B29C49/56		164
B29C2049/5661	11	{Mechanical}	B29C49/56	B29C49/56		101
B29C2049/5662	12	{Latch}	B29C49/56	B29C49/56		26
B29C2049/5663	12	{Rotating locking pin}	B29C49/56	B29C49/56		27
B29C2049/5664	12	{Translating locking pin}	B29C49/56	B29C49/56		41
B29C2049/5665	11	{Magnetic}	B29C49/56	B29C49/56		5
B29C2049/5666	11	{Pneumatic}	B29C49/56	B29C49/56		4
B29C49/58	9	Blowing means	B29C49/58	B29C49/58		1266
B29C2049/5806	10	{Means for fixing the blowing means with the mould}	B29C49/58	B29C49/58		74
B29C2049/581	11	{Mechanical, e.g. fingers or toothed wheels}	B29C49/58	B29C49/58		61
B29C2049/5813	11	{Hydraulic}	B29C49/58	B29C49/58		11
B29C2049/5817	11	{Pneumatic}	B29C49/58	B29C49/58		10
B29C2049/582	11	{Magnetic, e.g. permanent magnets}	B29C49/58	B29C49/58		12
B29C2049/5824	12	{Electromagnetic means, e.g. electromagnets}	B29C49/58	B29C49/58		4
B29C2049/5827	10	{Blowing means not touching the preform}	B29C49/58	B29C49/58		67
B29C2049/5831	10	{Diaphragms or bellows protecting the blowing means against contamination}	B29C49/58	B29C49/58		25
B29C2049/5834	10	{Lost blowing means}	B29C49/58	B29C49/58		6
B29C2049/5837	10	{Plural independent blowing means}	B29C49/58	B29C49/58		49
B29C2049/5841	10	{Plural independent blowing paths}	B29C49/58	B29C49/58		49
B29C2049/5844	10	{Compacting means, e.g. to compact the neck portion of the blown article with the blowing means}	B29C49/58	B29C49/58		32
B29C2049/5848	10	{Cutting means, e.g. to cut parts of the preform or parison with the blowing means}	B29C49/58	B29C49/58		16
B29C2049/5851	10	{Means to avoid clogging of the blowing paths}	B29C49/58	B29C49/58		1
B29C2049/5855	10	{for injecting additional medium during the blowing operation, e.g. cooling medium}	B29C49/58	B29C49/58		11
B29C2049/5858	10	{Distributing blowing fluid to the moulds, e.g. rotative distributor or special connection}	B29C49/58	B29C49/58		55
B29C2049/5862	10	{Drive means therefore}	B29C49/58	B29C49/58		38
B29C2049/5865	11	{Pneumatic}	B29C49/58	B29C49/58		34
B29C2049/5868	11	{Hydraulic}	B29C49/58	B29C49/58		30
B29C2049/5872	11	{Mechanical}	B29C49/58	B29C49/58		18
B29C2049/5875	11	{Electric direct drives, e.g. linear electric motor}	B29C49/58	B29C49/58		27
B29C2049/5879	11	{Magnetic means, e.g. permanent magnets}	B29C49/58	B29C49/58		6
B29C2049/5882	12	{Electromagnetic means, e.g. electromagnets}	B29C49/58	B29C49/58		3
B29C2049/5886	10	{for introducing from below into the extruded parison, e.g. for reducing contamination of the preforms or parisons}	B29C49/58	B29C49/58		23
B29C2049/5889	10	{being cooled}	B29C49/58	B29C49/58		31
B29C2049/5893	10	{Mounting, exchanging or centering blowing means}	B29C49/58	B29C49/58		35
B29C2049/5896	11	{Centering means therefore}	B29C49/58	B29C49/58		32
B29C2049/5898	11	{Regulation of the blowing means clamp force}	B29C49/58	B29C49/58		18
B29C49/60	10	Blow-needles	B29C49/60	B29C49/60		346
B29C2049/6018	11	{Constructional features of the air outlet}	B29C49/60	B29C49/60		9
B29C2049/6027	12	{having several air outlets e.g. for directing the blowing fluid in different directions}	B29C49/60	B29C49/60		27
B29C2049/6036	12	{the air outlet being located distant from the end of the needle}	B29C49/60	B29C49/60		15
B29C2049/6045	12	{the air outlet being openable and closable}	B29C49/60	B29C49/60		4
B29C2049/6054	11	{Means for avoiding blowing fluid leakage between the blow needle and parisons or preforms}	B29C49/60	B29C49/60		13
B29C2049/6063	11	{having means which facilitate the puncturing of the parison}	B29C49/60	B29C49/60		25
B29C2049/6072	11	{being movable, e.g. blow needles move to pierce the parison}	B29C49/60	B29C49/60		80
B29C2049/6081	12	{being rotatable}	B29C49/60	B29C49/60		11
B29C2049/609	11	{Two or more blow-needles}	B29C49/60	B29C49/60		63
B29C2049/6091	11	{Avoiding needle marks, e.g. insertion in sprue}	B29C49/60	B29C49/60		33
B29C2049/6092	11	{Blow needle sterilization}	B29C49/60	B29C49/60		8
B29C49/62	9	Venting means	B29C49/62	B29C49/62		224
B29C2049/622	10	{for venting air between preform and cavity, e.g. using venting holes, gaps or patterned moulds}	B29C49/62	B29C49/62		21
B29C2049/627	11	{using vacuum means}	B29C49/62	B29C49/62		46
B29C2049/6271	10	{for venting blowing medium, e.g. using damper or silencer}	B29C49/62	B29C49/62		65
B29C2049/6272	11	{using vacuum means}	B29C49/62	B29C49/62		29
B29C49/64	9	Heating or cooling preforms, parisons or blown articles	B29C49/64	B29C49/64		697
B29C49/6409	10	{Thermal conditioning of preforms (B29C49/68 takes precedence)}	B29C49/64	B29C49/64		534
B29C49/6418	11	{Heating of preforms}	B29C49/64	B29C49/64		526
B29C49/6419	12	{from the inside}	B29C49/64	B29C49/64		28
B29C49/64195	12	{Heated by the mould}	B29C49/64	B29C49/64		30
B29C49/642	12	{and shrinking of the preform}	B29C49/64	B29C49/64		88
B29C49/6427	11	{Cooling of preforms}	B29C49/64	B29C49/64		346
B29C49/643	12	{from the inside}	B29C49/64	B29C49/64		68
B29C49/6435	12	{from the outside}	B29C49/64	B29C49/64		88
B29C49/6436	11	{characterised by temperature differential}	B29C49/64	B29C49/64		200
B29C49/6445	12	{through the preform length}	B29C49/64	B29C49/64		318
B29C49/645	13	{by cooling the neck}	B29C49/64	B29C49/64		75
B29C49/6452	13	{by heating the neck}	B29C49/64	B29C49/64		85
B29C49/6454	12	{through the preform thickness}	B29C49/64	B29C49/64		86
B29C49/6458	12	{tangentially, i.e. along circumference}	B29C49/64	B29C49/64		73
B29C49/6462	12	{by masking}	B29C49/64	B29C49/64		87
B29C49/6463	11	{by contact heating or cooling, e.g. mandrels or cores specially adapted for heating or cooling preforms}	B29C49/64	B29C49/64		134
B29C49/6464	12	{Heating}	B29C49/64	B29C49/64		87
B29C49/6465	12	{Cooling}	B29C49/64	B29C49/64		128
B29C49/6466	12	{on the inside}	B29C49/64	B29C49/64		65
B29C49/6467	12	{on the outside}	B29C49/64	B29C49/64		62
B29C49/6472	10	{in several stages}	B29C49/64	B29C49/64		291
B29C49/648	11	{of preforms or parisons}	B29C49/64	B29C49/64		86
B29C49/66	10	Cooling by refrigerant introduced into the blown article	B29C49/66	B29C49/66		296
B29C49/6604	10	{Thermal conditioning of the blown article (B29C49/66 takes precedence)}	B29C49/64	B29C49/66		77
B29C49/6605	11	{Heating the article, e.g. for hot fill}	B29C49/64	B29C49/66		412
B29C49/66055	12	{using special pressurizing during the heating, e.g. in order to control the shrinking}	B29C49/64	B29C49/66		30
B29C2049/6606	11	{Cooling the article}	B29C49/64	B29C49/66		156
B29C2049/6607	12	{Flushing blown articles}	B29C49/64	B29C49/66		26
B29C2049/6615	13	{and exhausting through the blowing means}	B29C49/64	B29C49/66		85
B29C2049/6623	13	{and exhausting through an opening in the blown article}	B29C49/64	B29C49/66		30
B29C2049/6646	13	{while keeping the final blowing pressure in the article}	B29C49/64	B29C49/66		43
B29C2049/6653	12	{the medium being other than cooled air}	B29C49/64	B29C49/66		15
B29C2049/6661	13	{Water}	B29C49/64	B29C49/66		25
B29C2049/6669	13	{Gas with water droplets}	B29C49/64	B29C49/66		14
B29C2049/6676	12	{the medium being oriented towards special areas of the blown article}	B29C49/64	B29C49/66		7
B29C2049/6684	13	{Neck area}	B29C49/64	B29C49/66		13
B29C2049/6692	13	{Bottom area}	B29C49/64	B29C49/66		71
B29C2049/671	11	{Conditioning the blown article outside the mould, e.g. while transporting it out of the mould}	B29C49/64	B29C2049/671		8
B29C49/68	10	Ovens specially adapted for heating preforms or parisons	B29C49/68	B29C49/68		288
B29C49/681	11	{using a conditioning receptacle, e.g. a cavity, e.g. having heated or cooled regions}	B29C49/68	B29C49/68		95
B29C49/682	11	{characterised by the path, e.g. sinusoidal path}	B29C49/68	B29C49/68		86
B29C49/6825	11	{Mounting exchanging or centering ovens or parts thereof}	B29C49/68	B29C49/68		38
B29C49/683	11	{Adjustable or modular conditioning means, e.g. position and number of heating elements}	B29C49/68	B29C49/68		53
B29C49/6835	11	{using reflectors}	B29C49/68	B29C49/68		351
B29C49/684	11	{using masking}	B29C49/68	B29C49/68		16
B29C49/6845	11	{using ventilation, e.g. a fan}	B29C49/68	B29C49/68		75
B29C49/685	11	{Rotating the preform in relation to heating means}	B29C49/68	B29C49/68		276
B29C49/6855	11	{Cooling of heating means, e.g. avoiding overheating}	B29C49/68	B29C49/68		55
B29C49/70	9	Removing or ejecting blown articles from the mould	B29C49/70	B29C49/70		540
B29C2049/701	10	{Ejecting means}	B29C49/70	B29C49/70		47
B29C2049/702	11	{Air pressure}	B29C49/70	B29C49/70		35
B29C2049/707	11	{Hydraulic driving means}	B29C49/70	B29C49/70		7
B29C2049/708	11	{Pneumatic driving means}	B29C49/70	B29C49/70		14
B29C2049/709	10	{Retaining means, e.g. means for retaining the article before it is removed or ejected}	B29C49/70	B29C49/70		20
B29C49/72	9	Deflashing outside the mould	B29C49/72	B29C49/72		334
B29C2049/725	10	{Means for removing the deflashed parts from the deflashing area, e.g. burrs being removed from the deflashing area by a conveyor}	B29C49/72	B29C49/72		37
B29C49/74	10	Deflashing the neck portion	B29C49/74	B29C49/74		206
B29C49/76	9	Neck calibration	B29C49/76	B29C49/76		191
B29C49/761	10	{Forming threads, e.g. shaping neck thread between blowing means and mould}	B29C49/76	B29C49/76		179
B29C49/78	9	Measuring, controlling or regulating	B29C49/78	B29C49/78		1118
B29C49/783	10	{blowing pressure}	B29C49/78	B29C49/78		483
B29C2049/7831	11	{characterised by pressure values or ranges}	B29C49/78	B29C49/78		397
B29C2049/7832	11	{Blowing with two or more pressure levels}	B29C49/78	B29C49/78		351
B29C2049/7833	12	{Blowing with three or more pressure levels}	B29C49/78	B29C49/78		72
B29C2049/7834	11	{Pressure increase speed, e.g. dependent on stretch or position}	B29C49/78	B29C49/78		43
B29C2049/7835	11	{Pressure reduction speed}	B29C49/78	B29C49/78		10
B29C49/786	10	{Temperature}	B29C49/78	B29C49/78		420
B29C2049/7861	11	{of the preform}	B29C49/78	B29C49/78		152
B29C2049/7862	12	{characterised by temperature values or ranges}	B29C49/78	B29C49/78		303
B29C2049/7863	12	{Cold blow-moulding, e.g. below Tg}	B29C49/78	B29C49/78		11
B29C2049/7864	11	{of the mould}	B29C49/78	B29C49/78		41
B29C2049/78645	12	{characterised by temperature values or ranges}	B29C49/78	B29C49/78		222
B29C2049/7865	11	{of the stretching means, e.g. stretch rod}	B29C49/78	B29C49/78		8
B29C2049/7866	11	{of the blowing medium}	B29C49/78	B29C49/78		30
B29C2049/7867	11	{of the heating or cooling means}	B29C49/78	B29C49/78		56
B29C2049/78675	12	{of the heating means}	B29C49/78	B29C49/78		96
B29C2049/7868	11	{of the articles}	B29C49/78	B29C49/78		39
B29C2049/787	10	{Thickness}	B29C49/78	B29C49/78		66
B29C2049/78705	11	{of a layer, e.g. intermediate layer}	B29C49/78	B29C49/78		17
B29C2049/7871	11	{of the extruded preform thickness}	B29C49/78	B29C49/78		77
B29C2049/78715	11	{of the blown article thickness}	B29C49/78	B29C49/78		70
B29C2049/7873	10	{Extrusion speed; Extruded preform position or length; Extrusion fall speed}	B29C49/78	B29C49/78		52
B29C2049/7874	10	{Preform or article shape, weight, defect or presence}	B29C49/78	B29C49/78		85
B29C2049/78745	11	{Weight or density}	B29C49/78	B29C49/78		12
B29C2049/7875	11	{Size or shape}	B29C49/78	B29C49/78		39
B29C2049/78755	11	{Optical properties}	B29C49/78	B29C49/78		27
B29C2049/7876	11	{Defects}	B29C49/78	B29C49/78		82
B29C2049/78765	11	{Presence, e.g. of the preform in the mould}	B29C49/78	B29C49/78		18
B29C2049/7878	10	{Preform or article handling, e.g. flow from station to station}	B29C49/78	B29C49/78		71
B29C2049/7879	10	{Stretching, e.g. stretch rod}	B29C49/78	B29C49/78		302
B29C2049/788	10	{Controller type or interface}	B29C49/78	B29C49/78		11
B29C2049/78805	11	{Computer or PLC control}	B29C49/78	B29C49/78		256
B29C2049/7881	11	{Mechanical control}	B29C49/78	B29C49/78		10
B29C2049/78815	11	{using wireless transmission}	B29C49/78	B29C49/78		33
B29C2049/7882	11	{Control interface, e.g. display}	B29C49/78	B29C49/78		47
B29C49/80	10	Testing, e.g. for leaks	B29C49/80	B29C49/80		244
B29C2049/801	11	{Taking preform or article samples, e.g. by cutting out pieces for analysis}	B29C49/80	B29C49/80		15
B29C51/00	7	Shaping by thermoforming {, i.e. shaping sheets or sheet like preforms after heating}, e.g. shaping sheets in matched moulds or by deep-drawing; Apparatus therefor {(blow moulding of tubular preforms B29C49/00, deforming of tubular or hollow preforms B29C67/0014)}	B29C51/00	B29C51/00		1324
B29C51/002	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C51/00	B29C51/00		1112
B29C51/004	9	{Textile or other fibrous material made from plastics fibres (combined with plastic layers B29C51/145; compression moulding of reinforced plastic articles in matched moulds B29C70/46; using pressure difference B29C70/44)}	B29C51/00	B29C51/00		411
B29C51/006	8	{for making articles having hollow walls}	B29C51/00	B29C51/00		159
B29C51/008	8	{without using a mould, e.g. ballooning (as prestretching step B29C51/06)}	B29C51/00	B29C51/00		113
B29C51/02	8	Combined thermoforming and manufacture of the preform	B29C51/02	B29C51/02		994
B29C51/04	8	Combined thermoforming and prestretching, e.g. biaxial stretching	B29C51/04	B29C51/04		907
B29C51/06	9	using pressure difference {for prestretching}	B29C51/06	B29C51/06		229
B29C51/08	8	Deep drawing or matched-mould forming, i.e. using mechanical means only	B29C51/08	B29C51/08		1433
B29C51/082	9	{by shaping between complementary mould parts}	B29C51/08	B29C51/08		1697
B29C51/085	10	{with at least one of the shaping surfaces being made of resilien material, e.g. rubber}	B29C51/08	B29C51/08		109
B29C51/087	10	{with at least one of the mould parts comprising independently movable sections (B29C51/32 and B29C51/34 take precedence)}	B29C51/08	B29C51/08		188
B29C51/10	8	Forming by pressure difference, e.g. vacuum	B29C51/10	B29C51/10		4462
B29C51/105	9	{Twin sheet thermoforming, i.e. deforming two parallel opposing sheets or foils at the same time by using one common mould cavity and without welding them together during thermoforming (B29C51/267, B29C49/0691 take precedence)}	B29C51/10	B29C51/10		121
B29C51/12	8	of articles having inserts or reinforcements	B29C51/12	B29C51/12		797
B29C51/14	8	using multilayered preforms or sheets	B29C51/14	B29C51/14		1768
B29C51/145	9	{having at least one layer of textile or fibrous material combined with at least one plastics layer}	B29C51/14	B29C51/14		626
B29C51/16	8	Lining or labelling	B29C51/16	B29C51/16		881
B29C51/162	9	{of deep containers or boxes}	B29C51/16	B29C51/16		206
B29C51/165	9	{combined with the feeding or the shaping of the lining or the labels (by injection moulding B29C45/14008, B29C45/1418)}	B29C51/16	B29C51/16		213
B29C51/167	10	{of a continuous strip}	B29C51/16	B29C51/16		119
B29C51/18	8	Thermoforming apparatus	B29C51/18	B29C51/18		1097
B29C51/20	9	having movable moulds or mould parts	B29C51/20	B29C51/20		323
B29C51/22	10	rotatable about an axis	B29C51/22	B29C51/22		384
B29C51/225	11	{mounted on a vacuum drum (for surface shaping B29C59/06)}	B29C51/22	B29C51/22		365
B29C51/24	10	mounted on movable endless supports	B29C51/24	B29C51/24		153
B29C51/26	8	Component parts, details or accessories; Auxiliary operations	B29C51/26	B29C51/26		886
B29C51/261	9	{Handling means, e.g. transfer means, feeding means (B29C51/44 takes precedence)}	B29C51/26	B29C51/26		1301
B29C51/262	10	{Clamping means for the sheets, e.g. clamping frames}	B29C51/26	B29C51/26		1127
B29C51/263	9	{characterised by using a particular environment, e.g. sterile}	B29C51/26	B29C51/26		59
B29C51/264	9	{Auxiliary operations prior to the thermoforming operation, e.g. cutting (B29C51/42, B29C51/46 take precedence)}	B29C51/26	B29C51/26		337
B29C51/265	9	{Auxiliary operations during the thermoforming operation (B29C51/42, B29C51/46 take precedence)}	B29C51/26	B29C51/26		135
B29C51/266	9	{Auxiliary operations after the thermoforming operation (B29C51/42, B29C51/44, B29C51/46 take precedence)}	B29C51/26	B29C51/26		541
B29C51/267	10	{Two sheets being thermoformed in separate mould parts and joined together while still in the mould (B29C49/0691 takes precedence)}	B29C51/26	B29C51/26		553
B29C51/268	10	{Cutting, rearranging and joining the cut parts}	B29C51/26	B29C51/26		386
B29C51/28	9	for applying pressure through the wall of an inflated bag or diaphragm	B29C51/28	B29C51/28		294
B29C51/30	9	Moulds	B29C51/30	B29C51/30		1221
B29C51/303	10	{with sealing means or the like}	B29C51/30	B29C51/30		92
B29C51/306	10	{with means for forming a rim (combined with cutting B29C51/325; rim rolling per seB29C53/34)}	B29C51/30	B29C51/30		110
B29C51/32	10	having cutting means	B29C51/32	B29C51/32		812
B29C51/325	11	{combined with means for forming a rim}	B29C51/32	B29C51/32		99
B29C51/34	10	for undercut articles	B29C51/34	B29C51/34		423
B29C51/343	11	{having recessed undersurfaces}	B29C51/34	B29C51/34		101
B29C51/346	11	{specially adapted to facilitate the destacking of nestable containers}	B29C51/34	B29C51/34		31
B29C51/36	10	specially adapted for vacuum forming {, Manufacture thereof}	B29C51/36	B29C51/36		912
B29C51/365	11	{Porous moulds}	B29C51/36	B29C51/36		164
B29C51/38	10	Opening, closing or clamping means	B29C51/38	B29C51/38		342
B29C51/40	10	Venting means	B29C51/40	B29C51/40		159
B29C51/42	9	Heating or cooling	B29C51/42	B29C51/42		773
B29C51/421	10	{of preforms, specially adapted for thermoforming (preheating sheets in general B29B13/023; B29C51/427 takes precedence)}	B29C51/42	B29C51/42		1022
B29C51/422	11	{to produce a temperature differential (B29C51/426 takes precedence)}	B29C51/42	B29C51/42		267
B29C51/423	12	{through the thickness of the preform}	B29C51/42	B29C51/42		44
B29C51/424	11	{using a heated fluid}	B29C51/42	B29C51/42		166
B29C51/425	11	{using movable heating devices}	B29C51/42	B29C51/42		198
B29C51/426	10	{Producing specific thermal regimes during thermoforming to obtain particular properties}	B29C51/42	B29C51/42		168
B29C51/427	10	{Cooling of the material with a fluid blast}	B29C51/42	B29C51/42		137
B29C51/428	10	{of moulds or mould parts}	B29C51/42	B29C51/42		791
B29C51/44	9	Removing or ejecting moulded articles	B29C51/44	B29C51/44		809
B29C51/445	10	{from a support after moulding, e.g. by cutting}	B29C51/44	B29C51/44		431
B29C51/46	9	Measuring, controlling or regulating	B29C51/46	B29C51/46		1069
B29C53/00	7	Shaping by bending, folding, twisting, straightening or flattening; Apparatus therefor (B29C61/10 takes precedence)	B29C53/00	B29C53/00		97
B29C53/005	8	{characterised by the choice of material (B29C53/36 and B29C53/56 take precedence)}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C53/00	B29C53/00		127
B29C53/02	8	Bending or folding (B29C53/22, B29C53/34, B29C53/36, B29C53/56 take precedence)	B29C53/02	B29C53/02		697
B29C53/025	9	{using a folding bag}	B29C53/02	B29C53/02		58
B29C53/04	9	of plates or sheets {(B29C63/04 takes precedence; bending or folding paper B31F1/0003; folding films B65H45/00)}	B29C53/04	B29C53/04		2087
B29C53/043	10	{using rolls or endless belts}	B29C53/04	B29C53/04		344
B29C53/046	10	{using centrifugal force}	B29C53/04	B29C53/04		19
B29C53/06	10	Forming folding lines by pressing or scoring	B29C53/06	B29C53/06		461
B29C53/063	11	{combined with folding}	B29C53/06	B29C53/06		370
B29C53/066	12	{and joining the sides of the folding line, e.g. "Abkantschweissen"}	B29C53/06	B29C53/06		162
B29C53/08	9	of tubes {or other profiled members}	B29C53/08	B29C53/08		304
B29C53/083	10	{bending longitudinally, i.e. modifying the curvature of the tube axis}	B29C53/08	B29C53/08		1067
B29C53/086	10	{bending radially, i.e. deformig the cross-section of the tube}	B29C53/08	B29C53/08		87
B29C53/10	9	of blown tubular films, e.g. gusseting {(flattening blown films during extrusion moulding B29C48/03)}	B29C53/10	B29C53/10		158
B29C53/12	9	helically, e.g. for making springs {(for textile fibres D02G1/00)}	B29C53/12	B29C53/12		346
B29C53/14	8	Twisting {(for textile fibres D01H)}	B29C53/14	B29C53/14		212
B29C53/16	8	Straightening or flattening	B29C53/16	B29C53/16		307
B29C53/18	9	of plates or sheets	B29C53/18	B29C53/18		553
B29C53/20	9	of tubes	B29C53/20	B29C53/20		300
B29C53/22	8	Corrugating	B29C53/22	B29C53/22		121
B29C53/24	9	of plates or sheets	B29C53/24	B29C53/24		442
B29C53/26	10	parallel with direction of feed	B29C53/26	B29C53/26		76
B29C53/265	11	{using rolls or endless bands}	B29C53/26	B29C53/26		107
B29C53/28	10	transverse to direction of feed	B29C53/28	B29C53/28		100
B29C53/285	11	{using rolls or endless bands}	B29C53/28	B29C53/28		181
B29C53/30	9	of tubes (by blow-moulding B29C49/00)	B29C53/30	B29C53/30		375
B29C53/305	10	{using a cording process}	B29C53/30	B29C53/30		53
B29C53/32	8	Coiling (B29C53/56 takes precedence)	B29C53/32	B29C53/32		365
B29C53/34	8	Rim rolling (of tube ends B29C57/12)	B29C53/34	B29C53/34		102
B29C53/36	8	Bending and joining, e.g. for making hollow articles (B29C53/56 takes precedence)	B29C53/36	B29C53/36		821
B29C2053/362	9	{for making hems}	B29C53/36	B29C53/36		36
B29C2053/365	10	{provided with a string}	B29C53/36	B29C53/36		11
B29C2053/367	10	{provided with a strip}	B29C53/36	B29C53/36		7
B29C53/38	9	by bending sheets or strips at right angles to the longitudinal axis of the article being formed and joining the edges	B29C53/38	B29C53/38		233
B29C53/382	10	{using laminated sheets}	B29C53/38	B29C53/38		136
B29C53/385	10	{using several sheets to form the circumference}	B29C53/38	B29C53/38		92
B29C53/387	10	{the joining being done from the inside}	B29C53/38	B29C53/38		43
B29C53/40	10	for articles of definite length, i.e. discrete articles	B29C53/40	B29C53/40		326
B29C53/42	11	using internal forming surfaces, e.g. mandrels	B29C53/42	B29C53/42		240
B29C53/44	12	rotatable about the axis of the article	B29C53/44	B29C53/44		57
B29C53/46	11	using external forming surfaces, e.g. sleeves	B29C53/46	B29C53/46		38
B29C53/48	10	for articles of indefinite length, i.e. bending a strip progressively	B29C53/48	B29C53/48		524
B29C53/50	11	using internal forming surfaces, e.g. mandrels	B29C53/50	B29C53/50		443
B29C53/52	11	using external forming surfaces, e.g. sleeves	B29C53/52	B29C53/52		129
B29C53/54	11	Guiding, aligning or shaping edges	B29C53/54	B29C53/54		33
B29C53/56	8	Winding and joining, e.g. winding spirally {(winding in general B65H)}	B29C53/56	B29C53/56		813
B29C53/562	9	{spirally}	B29C53/56	B29C53/56		438
B29C53/564	9	{for making non-tubular articles (for winding of reinforced articles having a non-circular cross-section followed by compression B29C70/347)}	B29C53/56	B29C53/56		267
B29C53/566	9	{for making tubular articles followed by compression}	B29C53/56	B29C53/56		435
B29C53/568	9	{without using a forming surface}	B29C53/56	B29C53/56		10
B29C53/58	9	helically	B29C53/58	B29C53/58		864
B29C53/581	10	{using sheets or strips consisting principally of plastics material (using profiled sheets or strips B29C53/78)}	B29C53/58	B29C53/58		427
B29C53/582	11	{comprising reinforcements, e.g. wires, threads}	B29C53/58	B29C53/58		488
B29C53/583	10	{for making tubular articles with particular features}	B29C53/58	B29C53/58		218
B29C53/584	11	{having a non-circular cross-section}	B29C53/58	B29C53/58		62
B29C53/585	11	{the cross-section varying along their axis, e.g. tapered, with ribs, or threads, with socket-ends}	B29C53/58	B29C53/58		300
B29C53/586	12	{having corrugations}	B29C53/58	B29C53/58		71
B29C53/587	11	{having a non-uniform wall-structure, e.g. with inserts, perforations, locally concentrated reinforcements}	B29C53/58	B29C53/58		205
B29C53/588	11	{having a non-linear axis, e.g. elbows, toroids}	B29C53/58	B29C53/58		76
B29C53/60	10	using internal forming surfaces, e.g. mandrels	B29C53/60	B29C53/60		1032
B29C53/602	11	{for tubular articles having closed or nearly closed ends, e.g. vessels, tanks, containers}	B29C53/60	B29C53/60		472
B29C53/605	12	{by polar winding}	B29C53/60	B29C53/60		90
B29C53/607	11	{having driving means for advancing the wound articles, e.g. belts, rolls (B29C53/74 takes precedence)}	B29C53/60	B29C53/60		204
B29C53/62	11	rotatable about the winding axis	B29C53/62	B29C53/62		188
B29C53/64	12	and moving axially	B29C53/64	B29C53/64		156
B29C53/66	12	with axially movable winding feed member {, e.g. lathe type winding}	B29C53/66	B29C53/66		340
B29C53/665	13	{Coordinating the movements of the winding feed member and the mandrel}	B29C53/66	B29C53/66		144
B29C53/68	11	with rotatable winding feed member	B29C53/68	B29C53/68		160
B29C53/70	12	and moving axially	B29C53/70	B29C53/70		85
B29C53/72	10	using external forming surfaces	B29C53/72	B29C53/72		95
B29C53/74	10	using a forming surface inthe shape of an endless belt which is recycled after the forming operation	B29C53/74	B29C53/74		92
B29C53/76	10	about more than one axis {, e.g. T-pieces, balls}	B29C53/76	B29C53/76		85
B29C53/78	10	using profiled sheets or strips	B29C53/78	B29C53/78		379
B29C53/785	11	{with reinforcements}	B29C53/78	B29C53/78		164
B29C53/80	8	Component parts, details or accessories; Auxiliary operations	B29C53/80	B29C53/80		1398
B29C53/8008	9	{specially adapted for winding and joining}	B29C53/80	B29C53/80		522
B29C53/8016	10	{Storing, feeding or applying winding materials, e.g. reels, thread guides, tensioners}	B29C53/80	B29C53/80		788
B29C2053/8025	11	{tensioning}	B29C53/80	B29C53/80		103
B29C2053/8033	11	{fixing the trailing edge of winding materials}	B29C53/80	B29C53/80		6
B29C53/8041	10	{Measuring, controlling or regulating (B29C53/665 takes precedence)}	B29C53/80	B29C53/80		245
B29C53/805	10	{Applying axial reinforcements}	B29C53/80	B29C53/80		146
B29C53/8058	11	{continuously}	B29C53/80	B29C53/80		120
B29C53/8066	10	{Impregnating (impregnating as pretreatment B29B15/10)}	B29C53/80	B29C53/80		299
B29C53/8075	11	{on the forming surfaces}	B29C53/80	B29C53/80		87
B29C53/8083	10	{Improving bonding of wound materials or layers}	B29C53/80	B29C53/80		131
B29C53/8091	10	{Cutting the ends, surface finishing}	B29C53/80	B29C53/80		134
B29C53/82	9	Cores or mandrels	B29C53/82	B29C53/82		397
B29C53/821	10	{Mandrels especially adapted for winding and joining}	B29C53/82	B29C53/82		450
B29C53/822	11	{Single use mandrels, e.g. destructible, becoming part of the wound articles (B29C53/825 takes precedence)}	B29C53/82	B29C53/82		202
B29C53/824	11	{collapsible, e.g. elastic or inflatable; with removable parts, e.g. for regular shaped, straight tubular articles (B29C53/825 takes precedence)}	B29C53/82	B29C53/82		357
B29C53/825	11	{for continuous winding}	B29C53/82	B29C53/82		98
B29C53/827	12	{formed by several elements rotating about their own axes}	B29C53/82	B29C53/82		144
B29C53/828	11	{Arrangements comprising a plurality of cores or mandrels, e.g. to increase production speed (B29C53/827 takes precedence)}	B29C53/82	B29C53/82		85
B29C53/84	9	Heating or cooling	B29C53/84	B29C53/84		1179
B29C53/845	10	{especially adapted for winding and joining}	B29C53/84	B29C53/84		592
B29C55/00	7	Shaping by stretching, e.g. drawing through a die; Apparatus therefor (B29C61/08 takes precedence)	B29C55/00	B29C55/00		813
B29C55/005	8	{characterised by the choice of materials}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C55/00	B29C55/00		1349
B29C55/02	8	of plates or sheets	B29C55/02	B29C55/02		1393
B29C55/023	9	{using multilayered plates or sheets}	B29C55/02	B29C55/02		849
B29C55/026	10	{of preformed plates or sheets coated with a solution, a dispersion or a melt of thermoplastic material}	B29C55/02	B29C55/02		221
B29C55/04	9	uniaxial, e.g. oblique	B29C55/04	B29C55/04		802
B29C55/045	10	{in a direction which is not parallel or transverse to the direction of feed, e.g. oblique}	B29C55/04	B29C55/04		167
B29C55/06	10	parallel with the direction of feed	B29C55/06	B29C55/06		1166
B29C55/065	11	{in several stretching steps}	B29C55/06	B29C55/06		342
B29C55/08	10	transverse to the direction of feed	B29C55/08	B29C55/08		774
B29C55/085	11	{in several stretching steps}	B29C55/08	B29C55/08		59
B29C55/10	9	multiaxial	B29C55/10	B29C55/10		195
B29C55/12	10	biaxial	B29C55/12	B29C55/12		1860
B29C55/14	11	successively	B29C55/14	B29C55/14		572
B29C55/143	12	{firstly parallel to the direction of feed and then transversely thereto}	B29C55/14	B29C55/14		890
B29C55/146	12	{firstly transversely to the direction of feed and then parallel thereto}	B29C55/14	B29C55/14		146
B29C55/16	11	simultaneously	B29C55/16	B29C55/16		439
B29C55/165	12	{Apparatus therefor}	B29C55/16	B29C55/16		427
B29C55/18	9	by squeezing between surfaces, e.g. rollers	B29C55/18	B29C55/18		793
B29C55/20	9	Edge clamps	B29C55/20	B29C55/20		632
B29C55/22	8	of tubes {(B29C61/08 takes precedence)}	B29C55/22	B29C55/22		286
B29C55/24	9	radial	B29C55/24	B29C55/24		370
B29C55/26	9	biaxial	B29C55/26	B29C55/26		220
B29C55/28	8	of blown tubular films, e.g. by inflation {(extrusion moulding of tubular films B29C48/03)}	B29C55/28	B29C55/28		2263
B29C55/285	9	{by using internal mechanical means}	B29C55/28	B29C55/28		54
B29C55/30	8	Drawing through a die {(pultrusion B29C70/52)}	B29C55/30	B29C55/30		309
B29C57/00	7	Shaping of tube ends, e.g. flanging, belling or closing; Apparatus therefor {, e.g. collapsible mandrels}	B29C57/00	B29C57/00		1264
B29C57/005	8	{the end of an internal lining (fixing the end of the lining B29C63/346)}	B29C57/00	B29C57/00		132
B29C57/02	8	Belling or enlarging, e.g. combined with forming a groove	B29C57/02	B29C57/02		318
B29C57/025	9	{combined with the introduction of a sealing ring, e.g. using the sealing element as forming element}	B29C57/02	B29C57/02		135
B29C57/04	9	using mechanical means {(B29C57/025 takes precedence)}	B29C57/04	B29C57/04		693
B29C57/045	10	{rotating}	B29C57/04	B29C57/04		89
B29C57/06	10	elastically deformable	B29C57/06	B29C57/06		112
B29C57/08	9	using pressure difference	B29C57/08	B29C57/08		146
B29C57/10	8	Closing	B29C57/10	B29C57/10		491
B29C57/12	8	Rim rolling	B29C57/12	B29C57/12		358
B29C57/125	9	{using tools with helical grooves}	B29C57/12	B29C57/12		65
B29C59/00	7	Surface shaping {of articles}, e.g. embossing; Apparatus therefor {(in-mould printing B29C37/0025; by using liquids B29C71/0009; by using gases without chemical reaction B29C71/009; for decorating in general B44; abrasive blasting B24C; chemical aspects C08J7/00)}	B29C59/00	B29C59/00		534
B29C59/002	8	{Component parts, details or accessories; Auxiliary operations}	B29C59/00	B29C59/00		1118
B29C59/005	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br> Documents in which moulding materials are mentioned are indexed using indexing codes of subclass B29K. However, when, for example, documents concerning the choice of moulding material having a particular influence on the moulding technique cannot be satisfactorily indexed, the documents may be classified in this group if of interest. 	B29C59/00	B29C59/00		297
B29C59/007	8	{Forming single grooves or ribs, e.g. tear lines, weak spots (by moulding B29C37/0057; folding lines B29C53/06; in metal articles B21D17/00; by cutting B26D3/08)}	B29C59/00	B29C59/00		640
B29C59/02	8	by mechanical means, e.g. pressing {(B29C59/007 takes precedence; embossing expanded porous articles B29C44/5627)}	B29C59/02	B29C59/02		2670
B29C59/021	9	{of profiled articles, e.g. hollow or tubular articles, beams}	B29C59/02	B29C59/02		341
B29C59/022	9	{characterised by the disposition or the configuration, e.g. dimensions, of the embossments or the shaping tools therefor}	B29C59/02	B29C59/02		1774
B29C2059/023	10	{Microembossing}	B29C59/02	B29C59/02		1291
B29C59/025	10	{Fibrous surfaces with piles or similar fibres substantially perpendicular to the surface}	B29C59/02	B29C59/02		218
B29C59/026	9	{of layered or coated substantially flat surfaces}	B29C59/02	B29C59/02		685
B29C2059/027	9	{Grinding; Polishing}	B29C59/02	B29C59/02		259
B29C2059/028	9	{Incorporating particles by impact in the surface, e.g. using fluid jets or explosive forces to implant particles}	B29C59/02	B29C59/02		81
B29C59/04	9	using rollers or endless belts	B29C59/04	B29C59/04		3180
B29C59/043	10	{for profiled articles}	B29C59/04	B29C59/04		350
B29C59/046	10	{for layered or coated substantially flat surfaces}	B29C59/04	B29C59/04		909
B29C59/06	9	using vacuum drums {(for thermoforming B29C51/225)}	B29C59/06	B29C59/06		147
B29C59/08	8	by flame treatment {; using hot gases}	B29C59/08	B29C59/08		303
B29C59/085	9	{of profiled articles, e.g. hollow or tubular articles}	B29C59/08	B29C59/08		94
B29C59/10	8	by electric discharge treatment	B29C59/10	B29C59/10		806
B29C59/103	9	{of profiled articles, e.g. hollow or tubular articles}	B29C59/10	B29C59/10		162
B29C59/106	9	{the electrodes being placed on the same side of the material to be treated}	B29C59/10	B29C59/10		46
B29C59/12	9	in an environment other than air	B29C59/12	B29C59/12		182
B29C59/14	8	by plasma treatment {(plasma tubes per seH01J)}	B29C59/14	B29C59/14		1136
B29C59/142	9	{of profiled articles, e.g. hollow or tubular articles}	B29C59/14	B29C59/14		182
B29C2059/145	9	{Atmospheric plasma}	B29C59/14	B29C59/14		132
B29C2059/147	9	{Low pressure plasma; Glow discharge plasma}	B29C59/14	B29C59/14		61
B29C59/16	8	by wave energy or particle radiation {, e.g. infrared heating (B29C59/007 takes precedence)}	B29C59/16	B29C59/16		1118
B29C59/165	9	{of profiled articles, e.g. hollow or tubular articles}	B29C59/16	B29C59/16		74
B29C59/18	8	by liberation of internal stresses, e.g. plastic memory	B29C59/18	B29C59/18		80
B29C61/00	7	Shaping by liberation of internal stresses; Making preforms having internal stresses; Apparatus therefor (for surface shaping B29C59/18; for lining articles B29C63/38; for joining preformed parts B29C65/66{; for packaging B65B53/00; connecting arrangements or other fittings for plastics pipes using shrink-down material F16L47/22, electrical connections insulated using heat shrinking insulating sleeves H01R4/72; cable junctions protected by sleeves H02G15/18})	B29C61/00	B29C61/00		250
B29C61/003	8	{characterised by the choice of material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C61/00	B29C61/00		484
B29C61/006	8	{the force created by the liberation of the internal stresses being used for compression moulding or for pressing preformed material}	B29C61/00	B29C61/00		162
B29C61/02	8	Thermal shrinking	B29C61/02	B29C61/02		672
B29C61/025	9	{for the production of hollow or tubular articles}	B29C61/02	B29C61/02		436
B29C61/04	8	Thermal expansion	B29C61/04	B29C61/04		103
B29C61/06	8	Making preforms having internal stresses, e.g. plastic memory	B29C61/06	B29C61/06		478
B29C61/0608	9	{characterised by the configuration or structure of the preforms}	B29C61/06	B29C61/06		405
B29C61/0616	10	{layered or partially layered preforms, e.g. preforms with layers of adhesive or sealing compositions (B29C61/0625 and B29C61/065 take precedence)}	B29C61/06	B29C61/06		456
B29C61/0625	10	{Preforms comprising incorporated or associated heating means}	B29C61/06	B29C61/06		132
B29C61/0633	10	{Preforms comprising reinforcing elements (B29C61/0625 takes precedence)}	B29C61/06	B29C61/06		93
B29C61/0641	10	{Clips for dividing preforms or forming branch-offs (clips in general F16B2/20)}	B29C61/06	B29C61/06		90
B29C61/065	10	{Preforms held in a stressed condition by means of a removable support; Supports therefor}	B29C61/06	B29C61/06		131
B29C61/0658	10	{consisting of fibrous plastics material, e.g. woven}	B29C61/06	B29C61/06		128
B29C61/0666	10	{comprising means indicating that the shrinking temperature is reached}	B29C61/06	B29C61/06		70
B29C2061/0675	11	{the means being a material exuding outside the preform when the temperature is reached}	B29C61/06	B29C61/06		3
B29C2061/0683	11	{the means being a thermochromic painting or coating}	B29C61/06	B29C61/06		25
B29C2061/0691	11	{the means being protrusions on the preform surface disappearing when the temperature is reached}	B29C61/06	B29C61/06		8
B29C61/08	9	by stretching tubes {(in general B29C55/22, B29C55/28)}	B29C61/08	B29C61/08		399
B29C61/10	9	by bending plates or sheets {(in general B29C53/36)}	B29C61/10	B29C61/10		363
B29C63/00	7	Lining or sheathing, i.e. applying preformed layers or sheathings of plastics; Apparatus therefor (B29C73/00 takes precedence; by blowing B29C49/00; by thermoforming B29C51/00)	B29C63/00	B29C63/00		944
B29C63/0004	8	{Component parts, details or accessories; Auxiliary operations}	B29C63/00	B29C63/00		3004
B29C2063/0008	9	{Registering, centering the lining material on the substrate}	B29C63/00	B29C63/00		210
B29C63/0013	9	{Removing old coatings}	B29C63/00	B29C63/00		817
B29C63/0017	8	{characterised by the choice of the material}<br><br><u>NOTE</u><br><br>When classifying in this group, it is desirable to add the indexing codes of subclass B29K to identify the moulding materials and their properties. Documents concerning the choice of moulding materials having a particular influence on the moulding technique should be classified in this group if of interest.	B29C63/00	B29C63/00		320
B29C63/0021	9	{with coherent impregnated reinforcing layers}	B29C63/00	B29C63/00		218
B29C63/0026	8	{an edge face with strip material, e.g. a panel edge (securing a veneer strip to a panel edge B27D5/003)}	B29C63/00	B29C63/00		244
B29C63/003	9	{continuously}	B29C63/00	B29C63/00		154
B29C63/0034	9	{the strip material being folded}	B29C63/00	B29C63/00		157
B29C63/0039	10	{continuously}	B29C63/00	B29C63/00		106
B29C63/0043	8	{Fixing the layers by electrostatic charges, by the use of structured surfaces or by mechanical means}	B29C63/00	B29C63/00		79
B29C63/0047	8	{Preventing air-inclusions}	B29C63/00	B29C63/00		556
B29C63/0052	8	{Testing, e.g. testing for the presence of pinholes}	B29C63/00	B29C63/00		76
B29C63/0056	8	{Provisional sheathings}	B29C63/00	B29C63/00		295
B29C2063/006	8	{of surfaces having irregularities or roughness}	B29C63/00	B29C63/00		39
B29C63/0065	8	{Heat treatment}	B29C63/00	B29C63/00		641
B29C63/0069	9	{of tubular articles}	B29C63/00	B29C63/00		465
B29C63/0073	8	{of non-flat surfaces, e.g. curved, profiled (B29C63/042 takes precedence)}	B29C63/00	B29C63/00		462
B29C63/0078	9	{having local protrusions, e.g. rivet heads}	B29C63/00	B29C63/00		17
B29C63/0082	8	{Finishing the edges of holes or perforations in the lined product}	B29C63/00	B29C63/00		76
B29C63/0086	9	{and removing the portion of the lining covering the holes}	B29C63/00	B29C63/00		32
B29C63/0091	8	{in particular atmospheres}	B29C63/00	B29C63/00		102
B29C63/0095	8	{using a provisional carrier}	B29C63/00	B29C63/00		85
B29C63/02	8	using sheet or web-like material (B29C63/26{and B29C63/38} take precedence)	B29C63/02	B29C63/02		5010
B29C2063/021	9	{characterized by the junction of material sections}	B29C63/02	B29C63/02		76
B29C2063/022	10	{the junction being located in a groove}	B29C63/02	B29C63/02		56
B29C63/024	9	{the sheet or web-like material being supported by a moving carriage}	B29C63/02	B29C63/02		264
B29C63/025	9	{applied by a die matching with the profile of the surface of resilient articles, e.g. cushions, seat pads}	B29C63/02	B29C63/02		110
B29C2063/027	9	{applied by a squeegee}	B29C63/02	B29C63/02		128
B29C2063/028	9	{applied by a fluid jet}	B29C63/02	B29C63/02		31
B29C63/04	9	by folding, winding, bending or the like	B29C63/04	B29C63/04		769
B29C63/042	10	{of L- or Z- shaped surfaces, e.g. for counter-tops}	B29C63/04	B29C63/04		49
B29C63/044	10	{continuously (B29C63/065, B29C63/105 take precedence)}	B29C63/04	B29C63/04		278
B29C63/046	10	{using a folding shoulder}	B29C63/04	B29C63/04		21
B29C63/048	10	{specially adapted for articles having local protrusions, e.g. tubes having a bead weld}	B29C63/04	B29C63/04		38
B29C63/06	10	around tubular articles	B29C63/06	B29C63/06		388
B29C63/065	11	{continuously}	B29C63/06	B29C63/06		187
B29C63/08	10	by winding helically	B29C63/08	B29C63/08		124
B29C63/10	11	around tubular articles	B29C63/10	B29C63/10		388
B29C63/105	12	{continuously}	B29C63/10	B29C63/10		322
B29C63/12	10	by winding spirally	B29C63/12	B29C63/12		28
B29C63/14	11	around tubular articles	B29C63/14	B29C63/14		107
B29C63/145	12	{the tubular articles being mounted on transfer means}	B29C63/14	B29C63/14		4
B29C63/16	9	applied by "rubber" bag or diaphragm	B29C63/16	B29C63/16		203
B29C63/18	8	using tubular layers or sheathings (B29C63/26{and B29C63/38} take precedence; {placing tubular labels around rigid containers B65C3/065})	B29C63/18	B29C63/18		680
B29C63/182	9	{applied by a "rubber" bag or diaphragm}	B29C63/18	B29C63/18		20
B29C63/185	9	{by turning inside-out or by derolling}	B29C63/18	B29C63/18		41
B29C63/187	9	{by removing a shirred or pleated hose from a support}	B29C63/18	B29C63/18		12
B29C63/20	9	using pressure difference, e.g. vacuum	B29C63/20	B29C63/20		194
B29C63/22	8	using layers or sheathings having a shape adapted to the shape of the article (B29C63/26{and B29C63/38} take precedence)	B29C63/22	B29C63/22		570
B29C63/24	8	using threads	B29C63/24	B29C63/24		265
B29C63/26	8	Lining or sheathing of internal surfaces (B29C63/38 takes precedence)	B29C63/26	B29C63/26		422
B29C63/28	9	applied by "rubber" bag or diaphragm	B29C63/28	B29C63/28		125
B29C63/30	9	using sheet or web-like material	B29C63/30	B29C63/30		175
B29C63/32	10	by winding helically	B29C63/32	B29C63/32		117
B29C63/34	9	using tubular layers or sheathings	B29C63/34	B29C63/34		710
B29C63/341	10	{pressed against the wall by mechanical means}	B29C63/34	B29C63/34		225
B29C63/343	10	{the tubular sheathing having a deformed non-circular cross-section prior to introduction}	B29C63/34	B29C63/34		168
B29C63/345	10	{whilst rotating the article}	B29C63/34	B29C63/34		19
B29C63/346	10	{Fixing the end of the lining (shaping tube ends B29C57/005)}	B29C63/34	B29C63/34		138
B29C2063/348	10	{combined with reducing the diameter of the substrate to be lined}	B29C63/34	B29C63/34		15
B29C63/36	10	being turned inside out {(for platic tubes in general B29C67/0018)}	B29C63/36	B29C63/36		448
B29C63/38	8	by liberation of internal stresses	B29C63/38	B29C63/38		67
B29C63/40	9	using sheet or web-like material	B29C63/40	B29C63/40		143
B29C63/42	9	using tubular layers or sheathings	B29C63/42	B29C63/42		698
B29C63/423	10	{specially applied to the mass-production of externally coated articles, e.g. bottles}	B29C63/42	B29C63/42		222
B29C63/426	11	{in combination with the in situ shaping of the external tubular layer}	B29C63/42	B29C63/42		96
B29C63/44	9	the shape of the layers or sheathings being adapted to the shape of the articles	B29C63/44	B29C63/44		45
B29C63/46	9	of internal surfaces	B29C63/46	B29C63/46		126
B29C63/48	8	Preparation of the surfaces	B29C63/48	B29C63/48		498
B29C63/481	9	{mechanically}	B29C63/48	B29C63/48		187
B29C2063/483	9	{by applying a liquid}	B29C63/48	B29C63/48		96
B29C2063/485	10	{the liquid being an adhesive}	B29C63/48	B29C63/48		240
B29C63/486	9	{of metal surfaces (B29C63/481 takes precedence)}	B29C63/48	B29C63/48		94
B29C2063/488	9	{providing the surface with fixing elements on which the plastic liner is bonded}	B29C63/48	B29C63/48		20
B29C64/00	7	Additive manufacturing, i.e. manufacturing of three-dimensional [3D] objects by additive deposition, additive agglomeration or additive layering, e.g. by 3D printing, stereolithography or selective laser sintering<br><br><u>WARNING</u><br>Groups B29C64/00 - B29C64/40 are incomplete pending reclassification of documents from group G03F7/70416. <br>All groups listed in this Warning should be considered in order to perform a complete search.	B29C64/00	B29C64/00		602
B29C64/10	8	Processes of additive manufacturing	B29C64/10	B29C64/10		1605
B29C64/106	9	using only liquids or viscous materials, e.g. depositing a continuous bead of viscous material	B29C64/106	B29C64/106		4815
B29C64/112	10	using individual droplets, e.g. from jetting heads	B29C64/112	B29C64/112		3188
B29C64/118	10	using filamentary material being melted, e.g. fused deposition modelling [FDM]	B29C64/118	B29C64/118		6639
B29C64/124	10	using layers of liquid which are selectively solidified	B29C64/124	B29C64/124		3205
B29C64/129	11	characterised by the energy source therefor, e.g. by global irradiation combined with a mask	B29C64/129	B29C64/129		1458
B29C64/135	12	the energy source being concentrated, e.g. scanning lasers or focused light sources	B29C64/135	B29C64/135		2195
B29C64/141	9	using only solid materials	B29C64/141	B29C64/141		729
B29C64/147	10	using sheet material, e.g. laminated object manufacturing [LOM] or laminating sheet material precut to local cross sections of the 3D object	B29C64/147	B29C64/147		432
B29C64/153	10	using layers of powder being selectively joined, e.g. by selective laser sintering or melting	B29C64/153	B29C64/153		6593
B29C64/159	9	using only gaseous substances, e.g. vapour deposition	B29C64/159	B29C64/159		46
B29C64/165	9	using a combination of solid and fluid materials, e.g. a powder selectively bound by a liquid binder, catalyst, inhibitor or energy absorber	B29C64/165	B29C64/165		3282
B29C64/171	9	specially adapted for manufacturing multiple 3D objects	B29C64/171	B29C64/171		296
B29C64/176	10	Sequentially	B29C64/176	B29C64/176		227
B29C64/182	10	in parallel batches	B29C64/182	B29C64/182		332
B29C64/188	9	involving additional operations performed on the added layers, e.g. smoothing, grinding or thickness control (surface shaping B29C59/00; after-treatment of articles without altering their shape B29C71/00)	B29C64/188	B29C64/188		1288
B29C64/194	10	during lay-up	B29C64/194	B29C64/194		470
B29C64/20	8	Apparatus for additive manufacturing; Details thereof or accessories therefor	B29C64/20	B29C64/20		5117
B29C64/205	9	Means for applying layers	B29C64/205	B29C64/205		1269
B29C64/209	10	Heads; Nozzles	B29C64/209	B29C64/209		6309
B29C64/214	10	Doctor blades	B29C64/214	B29C64/214		872
B29C64/218	10	Rollers	B29C64/218	B29C64/218		556
B29C64/223	10	Foils or films, e.g. for transferring layers of building material from one working station to another	B29C64/223	B29C64/223		200
B29C64/227	9	Driving means	B29C64/227	B29C64/227		1585
B29C64/232	10	for motion along the axis orthogonal to the plane of a layer	B29C64/232	B29C64/232		1461
B29C64/236	10	for motion in a direction within the plane of a layer	B29C64/236	B29C64/236		1392
B29C64/241	10	for rotary motion	B29C64/241	B29C64/241		1072
B29C64/245	9	Platforms or substrates (support structures intended to be sacrificed after manufacture B29C64/40)	B29C64/245	B29C64/245		4504
B29C64/25	9	Housings, e.g. machine housings	B29C64/25	B29C64/25		915
B29C64/255	9	Enclosures for the building material, e.g. powder containers	B29C64/255	B29C64/255		1834
B29C64/259	10	Interchangeable	B29C64/259	B29C64/259		315
B29C64/264	9	Arrangements for irradiation	B29C64/264	B29C64/264		1802
B29C64/268	10	using laser beams; using electron beams [EB]	B29C64/268	B29C64/268		1968
B29C64/273	11	pulsed; frequency modulated	B29C64/273	B29C64/273		152
B29C64/277	10	using multiple radiation means, e.g. micromirrors or multiple light-emitting diodes [LED]	B29C64/277	B29C64/277		682
B29C64/282	11	of the same type, e.g. using different energy levels	B29C64/282	B29C64/282		372
B29C64/286	10	Optical filters, e.g. masks	B29C64/286	B29C64/286		308
B29C64/291	10	for operating globally, e.g. together with selectively applied activators or inhibitors	B29C64/291	B29C64/291		177
B29C64/295	9	Heating elements	B29C64/295	B29C64/295		2881
B29C64/30	8	Auxiliary operations or equipment	B29C64/30	B29C64/30		2622
B29C64/307	9	Handling of material to be used in additive manufacturing	B29C64/307	B29C64/307		615
B29C64/314	10	Preparation	B29C64/314	B29C64/314		2199
B29C64/321	10	Feeding	B29C64/321	B29C64/321		2887
B29C64/329	11	using hoppers	B29C64/329	B29C64/329		432
B29C64/336	11	of two or more materials	B29C64/336	B29C64/336		1401
B29C64/343	10	Metering	B29C64/343	B29C64/343		466
B29C64/35	9	Cleaning	B29C64/35	B29C64/35		2571
B29C64/357	9	Recycling	B29C64/357	B29C64/357		1022
B29C64/364	9	Conditioning of environment	B29C64/364	B29C64/364		890
B29C64/371	10	using an environment other than air, e.g. inert gas	B29C64/371	B29C64/371		614
B29C64/379	9	Handling of additively manufactured objects, e.g. using robots	B29C64/379	B29C64/379		1731
B29C64/386	9	Data acquisition or data processing for additive manufacturing	B29C64/386	B29C64/386		6465
B29C64/393	10	for controlling or regulating additive manufacturing processes	B29C64/393	B29C64/393		10556
B29C64/40	8	Structures for supporting 3D objects during manufacture and intended to be sacrificed after completion thereof	B29C64/40	B29C64/40		2450
B29C65/00	7	Joining {or sealing} of preformed parts {, e.g. welding of plastics materials}; Apparatus therefor {(general aspects of processes or apparatus for joining preformed parts B29C66/00; using porous material formed by internal pressure generated therein for joining preformed parts B29C44/1228, B29C44/326)}	B29C65/00	B29C65/00		4200
B29C65/002	8	{Joining methods not otherwise provided for}	B29C65/00	B29C65/00		161
B29C65/004	9	{Cold joining}	B29C65/00	B29C65/00		84
B29C65/006	9	{Diffusion joining (measures for intermixing the material of the joint interlayer B29C66/341)}	B29C65/00	B29C65/00		34
B29C65/008	9	{making use of electrostatic charges (holding means using electrostatic forces to hold at least one of the parts to be joined B29C65/7852)}	B29C65/00	B29C65/00		66
B29C65/02	8	by heating, with or without pressure	B29C65/02	B29C65/02		11531
B29C65/022	9	{Particular heating or welding methods not otherwise provided for}	B29C65/02	B29C65/02		239
B29C65/024	10	{making use of combustible material, i.e. the combustible material is in contact with the material to be joined}	B29C65/02	B29C65/02		20
B29C65/026	10	{making use of hot liquids, i.e. the liquid is in direct contact with the material to be joined}	B29C65/02	B29C65/02		32
B29C65/028	10	{making use of inherent heat, i.e. the heat for the joining comes from the moulding process of one of the parts to be joined}	B29C65/02	B29C65/02		477
B29C65/04	9	Dielectric heating, e.g. high-frequency welding {, i.e. radio frequency welding of plastic materials having dielectric properties, e.g. PVC}	B29C65/04	B29C65/04		3572
B29C65/06	9	using friction, e.g. spin welding {(non-plastics elements to plastic elements B29C65/645)}	B29C65/06	B29C65/06		1227
B29C65/0609	10	{characterised by the movement of the parts to be joined (B29C65/0672 takes precedence)}	B29C65/06	B29C65/06		30
B29C65/0618	11	{Linear}	B29C65/06	B29C65/06		438
B29C65/0627	11	{Angular, i.e. torsional (B29C65/082 takes precedence)}	B29C65/06	B29C65/06		86
B29C65/0636	11	{Orbital}	B29C65/06	B29C65/06		75
B29C65/0645	12	{Circular}	B29C65/06	B29C65/06		25
B29C65/0654	12	{Elliptical}	B29C65/06	B29C65/06		10
B29C65/0663	12	{Other specific orbital movements not provided for in B29C65/0645&#160;-&#160;B29C65/0654, e.g. Lissajous}	B29C65/06	B29C65/06		7
B29C65/0672	10	{Spin welding}	B29C65/06	B29C65/06		878
B29C65/0681	10	{created by a tool}	B29C65/06	B29C65/06		283
B29C65/069	10	{the welding tool cooperating with specially formed features of at least one of the parts to be joined, e.g. cooperating with holes or ribs of at least one of the parts to be joined}	B29C65/06	B29C65/06		225
B29C65/08	9	using ultrasonic vibrations {(non-plastics element to plastics elements B29C65/645)}	B29C65/08	B29C65/08		8816
B29C65/081	10	{having a component of vibration not perpendicular to the welding surface}	B29C65/08	B29C65/08		329
B29C65/082	11	{Angular, i.e. torsional ultrasonic welding}	B29C65/08	B29C65/08		88
B29C65/083	10	{using a rotary sonotrode or a rotary anvil}	B29C65/08	B29C65/08		26
B29C65/085	11	{using a rotary sonotrode}	B29C65/08	B29C65/08		261
B29C65/086	11	{using a rotary anvil}	B29C65/08	B29C65/08		964
B29C65/087	11	{using both a rotary sonotrode and a rotary anvil}	B29C65/08	B29C65/08		494
B29C65/088	10	{using several cooperating sonotrodes, i.e. interacting with each other, e.g. for realising the same joint}	B29C65/08	B29C65/08		179
B29C65/10	9	using hot gases {(e.g. combustion gases) or flames coming in contact with at least one of the parts to be joined}	B29C65/10	B29C65/10		2405
B29C65/103	10	{direct heating both surfaces to be joined}	B29C65/10	B29C65/10		875
B29C65/106	10	{using flames coming in contact with at least one of the parts to be joined}	B29C65/10	B29C65/10		343
B29C65/12	10	and welding bar	B29C65/12	B29C65/12		293
B29C65/125	11	{characterised by the composition of the welding bar}	B29C65/12	B29C65/12		67
B29C65/14	9	using wave energy {, i.e. electromagnetic radiation,} or particle radiation {(using mechanical waves B29C65/06; using ultrasonic waves B29C65/08; pressing means transparent to electromagnetic radiation B29C66/81267)}	B29C65/14	B29C65/14		1091
B29C65/1403	10	{characterised by the type of electromagnetic or particle radiation (B29C65/1603 takes precedence)}	B29C65/14	B29C65/14		190
B29C65/1406	11	{Ultraviolet [UV] radiation}	B29C65/14	B29C65/14		750
B29C65/1409	11	{Visible light radiation}	B29C65/14	B29C65/14		157
B29C65/1412	11	{Infrared [IR] radiation}	B29C65/14	B29C65/14		1418
B29C65/1416	12	{Near-infrared radiation [NIR]}	B29C65/14	B29C65/14		184
B29C65/1419	12	{Mid-infrared radiation [MIR]}	B29C65/14	B29C65/14		46
B29C65/1422	12	{Far-infrared radiation [FIR]}	B29C65/14	B29C65/14		81
B29C65/1425	11	{Microwave radiation}	B29C65/14	B29C65/14		493
B29C65/1429	10	{characterised by the way of heating the interface (B29C65/1629 takes precedence)}	B29C65/14	B29C65/14		17
B29C65/1432	11	{direct heating of the surfaces to be joined}	B29C65/14	B29C65/14		728
B29C65/1435	11	{at least passing through one of the parts to be joined, i.e. transmission welding}	B29C65/14	B29C65/14		551
B29C65/1438	12	{focusing the wave energy or particle radiation on the interface}	B29C65/14	B29C65/14		25
B29C65/1441	12	{making use of a reflector on the opposite side, e.g. a polished mandrel or a mirror (pressing means reflective to electromagnetic radiation B29C66/81268)}	B29C65/14	B29C65/14		39
B29C65/1445	11	{heating both sides of the joint}	B29C65/14	B29C65/14		196
B29C65/1448	11	{radiating the edges of the parts to be joined, e.g. for curing a layer of adhesive placed between two flat parts to be joined, e.g. for making CDs or DVDs}	B29C65/14	B29C65/14		178
B29C65/1451	12	{radiating the edges of holes or perforations}	B29C65/14	B29C65/14		19
B29C65/1454	11	{scanning at least one of the parts to be joined}	B29C65/14	B29C65/14		154
B29C65/1458	12	{once, i.e. contour welding}	B29C65/14	B29C65/14		104
B29C65/1461	12	{repeatedly, i.e. quasi-simultaneous welding}	B29C65/14	B29C65/14		8
B29C65/1464	11	{making use of several radiators}	B29C65/14	B29C65/14		244
B29C65/1467	12	{at the same time, i.e. simultaneous welding}	B29C65/14	B29C65/14		508
B29C65/1477	10	{making use of an absorber or impact modifier (B29C65/1677 takes precedence)}	B29C65/14	B29C65/14		100
B29C65/148	11	{placed at the interface}	B29C65/14	B29C65/14		136
B29C65/1483	11	{coated on the article}	B29C65/14	B29C65/14		440
B29C65/1487	10	{making use of light guides (B29C65/1687 takes precedence)}	B29C65/14	B29C65/14		116
B29C65/149	11	{being a part of the joined article}	B29C65/14	B29C65/14		18
B29C65/1493	12	{in the form of a cavity}	B29C65/14	B29C65/14		4
B29C65/1496	10	{making use of masks (B29C65/1696 takes precedence)}	B29C65/14	B29C65/14		197
B29C65/16	10	Laser beams	B29C65/16	B29C65/16		1643
B29C65/1603	11	{characterised by the type of electromagnetic radiation}	B29C65/16	B29C65/16		14
B29C65/1606	12	{Ultraviolet [UV] radiation, e.g. by ultraviolet excimer lasers}	B29C65/16	B29C65/16		219
B29C65/1609	12	{Visible light radiation, e.g. by visible light lasers}	B29C65/16	B29C65/16		100
B29C65/1612	12	{Infrared [IR] radiation, e.g. by infrared lasers}	B29C65/16	B29C65/16		240
B29C65/1616	13	{Near infrared radiation [NIR], e.g. by YAG lasers}	B29C65/16	B29C65/16		1051
B29C65/1619	13	{Mid infrared radiation [MIR], e.g. by CO or CO2 lasers}	B29C65/16	B29C65/16		355
B29C65/1622	13	{Far infrared radiation [FIR], e.g. by FIR lasers}	B29C65/16	B29C65/16		23
B29C65/1629	11	{characterised by the way of heating the interface}	B29C65/16	B29C65/16		206
B29C65/1632	12	{direct heating the surfaces to be joined}	B29C65/16	B29C65/16		257
B29C65/1635	12	{at least passing through one of the parts to be joined, i.e. laser transmission welding}	B29C65/16	B29C65/16		1984
B29C65/1638	13	{focusing the laser beam on the interface}	B29C65/16	B29C65/16		209
B29C65/1641	13	{making use of a reflector on the opposite side, e.g. a polished mandrel or a mirror (pressing means reflective to electromagnetic radiation B29C66/81268)}	B29C65/16	B29C65/16		58
B29C65/1645	12	{heating both sides of the joint, e.g. by using two lasers or a split beam}	B29C65/16	B29C65/16		74
B29C65/1648	12	{radiating the edges of the parts to be joined}	B29C65/16	B29C65/16		109
B29C65/1651	13	{radiating the edges of holes or perforations}	B29C65/16	B29C65/16		13
B29C65/1654	12	{scanning at least one of the parts to be joined}	B29C65/16	B29C65/16		1011
B29C65/1658	13	{scanning once, e.g. contour laser welding}	B29C65/16	B29C65/16		350
B29C65/1661	13	{scanning repeatedly, e.g. quasi-simultaneous laser welding}	B29C65/16	B29C65/16		264
B29C65/1664	12	{making use of several radiators}	B29C65/16	B29C65/16		295
B29C65/1667	13	{at the same time, i.e. simultaneous laser welding}	B29C65/16	B29C65/16		283
B29C65/167	14	{using laser diodes}	B29C65/16	B29C65/16		69
B29C65/1674	12	{making use of laser diodes (B29C65/167 takes precedence)}	B29C65/16	B29C65/16		386
B29C65/1677	11	{making use of an absorber or impact modifier}	B29C65/16	B29C65/16		757
B29C65/168	12	{placed at the interface}	B29C65/16	B29C65/16		288
B29C65/1683	12	{coated on the article}	B29C65/16	B29C65/16		362
B29C65/1687	11	{making use of light guides}	B29C65/16	B29C65/16		411
B29C65/169	12	{being a part of the joined article}	B29C65/16	B29C65/16		70
B29C65/1693	13	{in the form of a cavity}	B29C65/16	B29C65/16		21
B29C65/1696	11	{making use of masks}	B29C65/16	B29C65/16		271
B29C65/18	9	using heated tools	B29C65/18	B29C65/18		10835
B29C65/20	10	with direct contact, e.g. using "mirror"	B29C65/20	B29C65/20		2784
B29C65/2007	11	{characterised by the type of welding mirror}	B29C65/20	B29C65/20		75
B29C65/2015	12	{being a single welding mirror comprising several separate heating surfaces in different planes, e.g. said heating surfaces having different temperatures}	B29C65/20	B29C65/20		96
B29C65/2023	12	{said welding mirror comprising several sectors}	B29C65/20	B29C65/20		42
B29C65/203	12	{being several single mirrors, e.g. not mounted on the same tool}	B29C65/20	B29C65/20		405
B29C65/2038	12	{being a wire}	B29C65/20	B29C65/20		38
B29C65/2046	11	{using a welding mirror which also cuts the parts to be joined, e.g. for sterile welding}	B29C65/20	B29C65/20		234
B29C65/2053	11	{characterised by special ways of bringing the welding mirrors into position}	B29C65/20	B29C65/20		21
B29C65/2061	12	{by sliding}	B29C65/20	B29C65/20		416
B29C65/2069	13	{with an angle with respect to the plane comprising the parts to be joined}	B29C65/20	B29C65/20		21
B29C65/2076	14	{perpendicularly to the plane comprising the parts to be joined}	B29C65/20	B29C65/20		385
B29C65/2084	12	{by pivoting}	B29C65/20	B29C65/20		176
B29C65/2092	11	{and involving the use of a facer}	B29C65/20	B29C65/20		262
B29C65/22	10	Heated wire {resistive ribbon, resistive band or resistive strip (electrical insulating support therefor B29C66/81871)}	B29C65/22	B29C65/22		201
B29C65/221	11	{characterised by the type of heated wire, resistive ribbon, band or strip (specific electrical or thermal properties also to be classified in B29C66/81262 or B29C66/81261)}	B29C65/22	B29C65/22		46
B29C65/222	12	{comprising at least a single heated wire}	B29C65/22	B29C65/22		769
B29C65/223	13	{comprising several heated wires}	B29C65/22	B29C65/22		330
B29C65/224	12	{being a resistive ribbon, a resistive band or a resistive strip}	B29C65/22	B29C65/22		954
B29C65/225	12	{being a coating or being printed, e.g. being applied as a paint or forming a printed circuit}	B29C65/22	B29C65/22		69
B29C65/226	12	{characterised by the cross-section of said heated wire, resistive ribbon, resistive band or resistive strip, e.g. being triangular}	B29C65/22	B29C65/22		169
B29C65/227	13	{said cross-section being hollow}	B29C65/22	B29C65/22		25
B29C65/228	11	{characterised by the means for electrically connecting the ends of said heated wire, resistive ribbon, resistive band or resistive strip}	B29C65/22	B29C65/22		634
B29C65/229	11	{characterised by the means for tensioning said heated wire, resistive ribbon, resistive band or resistive strip (means for compensating for the thermal expansion of welding jaws in general B29C66/8185)}	B29C65/22	B29C65/22		340
B29C65/24	10	characterised by the means for heating the tool {(by impulse heating B29C65/38)}<br><br><u>NOTE</u><br><br> Classification is made in groups B29C65/24&#160;-&#160;B29C65/32 only if the details or adaptations of the heating means are of interest. <br> When classifying in this group, heated tools are additionally classified in groups B29C65/18, B29C65/20 or B29C65/22	B29C65/24	B29C65/24		158
B29C65/242	11	{the heat transfer being achieved by contact, i.e. a heated tool being brought into contact with the welding tool and afterwards withdrawn from it}	B29C65/24	B29C65/24		197
B29C65/245	11	{the heat transfer being achieved contactless, e.g. by radiation (B29C65/32 takes precedence)}	B29C65/24	B29C65/24		307
B29C65/247	11	{the heat resulting from a chemical reaction}	B29C65/24	B29C65/24		12
B29C65/26	11	Hot fluid	B29C65/26	B29C65/26		487
B29C65/28	11	Flame or combustible material	B29C65/28	B29C65/28		126
B29C65/30	11	Electrical means {(B29C65/38 takes precedence)}	B29C65/30	B29C65/30		1231
B29C65/305	12	{involving the use of cartridge heaters}	B29C65/30	B29C65/30		1958
B29C65/32	12	Induction	B29C65/32	B29C65/32		539
B29C65/34	9	using heated elements which remain in the joint, e.g. "verlorenes Schweisselement"	B29C65/34	B29C65/34		424
B29C65/3404	10	{characterised by the type of heated elements which remain in the joint (B29C65/3604 takes precedence)}	B29C65/34	B29C65/34		23
B29C65/3408	11	{comprising single particles, e.g. fillers or discontinuous fibre-reinforcements}	B29C65/34	B29C65/34		21
B29C65/3412	12	{comprising fillers}	B29C65/34	B29C65/34		121
B29C65/3416	12	{comprising discontinuous fibre-reinforcements}	B29C65/34	B29C65/34		54
B29C65/342	11	{comprising at least a single wire, e.g. in the form of a winding}	B29C65/34	B29C65/34		1713
B29C65/3424	12	{said at least a single wire having the form of a coil spring}	B29C65/34	B29C65/34		88
B29C65/3428	12	{said at least a single wire having a waveform, e.g. a sinusoidal form}	B29C65/34	B29C65/34		235
B29C65/3432	12	{comprising several wires, e.g. in the form of several independent windings (B29C65/3436, B29C65/344 take precedence)}	B29C65/34	B29C65/34		417
B29C65/3436	11	{comprising independent continuous fibre-reinforcements}	B29C65/34	B29C65/34		70
B29C65/344	11	{being a woven or non-woven fabric or being a mesh}	B29C65/34	B29C65/34		314
B29C65/3444	11	{being a ribbon, band or strip}	B29C65/34	B29C65/34		233
B29C65/3448	12	{said ribbon, band or strip being perforated}	B29C65/34	B29C65/34		104
B29C65/3452	12	{forming a sleeve, e.g. a wrap-around sleeve}	B29C65/34	B29C65/34		113
B29C65/3456	11	{being a layer of a multilayer part to be joined, e.g. for joining plastic-metal laminates}	B29C65/34	B29C65/34		47
B29C65/346	11	{being a coating or being printed, e.g. being applied as a paint or forming a printed circuit}	B29C65/34	B29C65/34		71
B29C65/3464	11	{characterised by the cross-section of said heated elements which remain in the joint or by the cross-section of their coating, e.g. being triangular}	B29C65/34	B29C65/34		101
B29C65/3468	10	{characterised by the means for supplying heat to said heated elements which remain in the join, e.g. special electrical connectors of windings (B29C65/3668 takes precedence)}	B29C65/34	B29C65/34		1297
B29C65/3472	10	{characterised by the composition of the heated elements which remain in the joint (B29C65/3672 takes precedence)}	B29C65/34	B29C65/34		5
B29C65/3476	11	{being metallic}	B29C65/34	B29C65/34		1658
B29C65/348	12	{with a polymer coating}	B29C65/34	B29C65/34		498
B29C65/3484	11	{being non-metallic}	B29C65/34	B29C65/34		51
B29C65/3488	12	{being an electrically conductive polymer}	B29C65/34	B29C65/34		99
B29C65/3492	12	{being carbon}	B29C65/34	B29C65/34		246
B29C65/3496	12	{with a coating, e.g. a metallic or a carbon coating}	B29C65/34	B29C65/34		59
B29C65/36	10	heated by induction	B29C65/36	B29C65/36		286
B29C65/3604	11	{characterised by the type of elements heated by induction which remain in the joint}	B29C65/36	B29C65/36		143
B29C65/3608	12	{comprising single particles, e.g. fillers or discontinuous fibre-reinforcements}	B29C65/36	B29C65/36		59
B29C65/3612	13	{comprising fillers}	B29C65/36	B29C65/36		388
B29C65/3616	13	{comprising discontinuous fibre-reinforcements}	B29C65/36	B29C65/36		127
B29C65/362	12	{comprising at least a single wire, e.g. in the form of a winding}	B29C65/36	B29C65/36		285
B29C65/3624	13	{said at least a single wire having the form of a coil spring}	B29C65/36	B29C65/36		19
B29C65/3628	13	{said at least a single wire having a waveform, e.g. a sinusoidal form}	B29C65/36	B29C65/36		35
B29C65/3632	13	{comprising several wires, e.g. in the form of several independent windings (B29C65/364 takes precedence)}	B29C65/36	B29C65/36		85
B29C65/3636	12	{comprising independent continuous fibre-reinforcements}	B29C65/36	B29C65/36		73
B29C65/364	12	{being a woven or non-woven fabric or being a mesh}	B29C65/36	B29C65/36		283
B29C65/3644	12	{being a ribbon, band or strip}	B29C65/36	B29C65/36		507
B29C65/3648	13	{said strip being perforated}	B29C65/36	B29C65/36		80
B29C65/3652	13	{forming a sleeve, e.g. a wrap-around sleeve}	B29C65/36	B29C65/36		21
B29C65/3656	12	{being a layer of a multilayer part to be joined, e.g. for joining plastic-metal laminates}	B29C65/36	B29C65/36		713
B29C65/366	12	{being a coating or being printed, e.g. being applied as a paint or forming a printed circuit}	B29C65/36	B29C65/36		54
B29C65/3668	11	{characterised by the means for supplying heat to said heated elements which remain in the join, e.g. special induction coils}	B29C65/36	B29C65/36		557
B29C65/3672	11	{characterised by the composition of the elements heated by induction which remain in the joint}	B29C65/36	B29C65/36		8
B29C65/3676	12	{being metallic}	B29C65/36	B29C65/36		611
B29C65/368	13	{with a polymer coating}	B29C65/36	B29C65/36		946
B29C65/3684	12	{being non-metallic}	B29C65/36	B29C65/36		187
B29C65/3696	13	{with a coating}	B29C65/36	B29C65/36		118
B29C65/38	9	Impulse heating<br><br><u>NOTE</u><br><br> When classifying in this group, heated tools are additionally classified in the relevant groups, e.g. B29C65/22	B29C65/38	B29C65/38		745
B29C65/40	9	Applying molten plastics, e.g. hot melt (using welding bar {combined with hot gases}B29C65/12; by moulding B29C65/70)	B29C65/40	B29C65/40		608
B29C65/405	10	{characterised by the composition of the applied molten plastics (B29C65/425 takes precedence)}	B29C65/40	B29C65/40		75
B29C65/42	10	between pre-assembled parts {(B29C65/605 takes precedence)}	B29C65/42	B29C65/42		529
B29C65/425	11	{characterised by the composition of the molten plastics applied between pre-assembled parts}	B29C65/42	B29C65/42		107
B29C65/44	9	Joining a heated non plastics element to a plastics element<br><br><u>NOTE</u><br><br> When classifying in this group, compositions of the non-plastics element are additionally classified in the relevant groups, i.e. in B29C66/74 and subgroups 	B29C65/44	B29C65/44		861
B29C65/46	10	heated by induction<br><br><u>NOTE</u><br><br> When classifying in this group, compositions of the non-plastics element are additionally classified in the relevant groups, i.e. in B29C66/74 and subgroups 	B29C65/46	B29C65/46		387
B29C65/48	8	using adhesives {, i.e. using supplementary joining material; solvent bonding}<br><br><u>NOTE</u><br><br> When classifying in this group, heat-activated adhesives are further classified in group B29C65/02. When classifying in this group, applying molten plastics is further classified in group B29C65/40. 	B29C65/48	B29C65/48		7261
B29C65/4805	9	{characterised by the type of adhesives}	B29C65/48	B29C65/48		232
B29C65/481	10	{Non-reactive adhesives, e.g. physically hardening adhesives}	B29C65/48	B29C65/48		108
B29C65/4815	11	{Hot melt adhesives, e.g. thermoplastic adhesives}	B29C65/48	B29C65/48		3996
B29C65/482	11	{Drying adhesives, e.g. solvent based adhesives}	B29C65/48	B29C65/48		367
B29C65/4825	11	{Pressure sensitive adhesives}	B29C65/48	B29C65/48		546
B29C65/483	10	{Reactive adhesives, e.g. chemically curing adhesives}	B29C65/48	B29C65/48		1641
B29C65/4835	11	{Heat curing adhesives}	B29C65/48	B29C65/48		1620
B29C65/484	11	{Moisture curing adhesives}	B29C65/48	B29C65/48		245
B29C65/4845	11	{Radiation curing adhesives, e.g. UV light curing adhesives}	B29C65/48	B29C65/48		1007
B29C65/485	11	{Multi-component adhesives, i.e. chemically curing as a result of the mixing of said multi-components}	B29C65/48	B29C65/48		539
B29C65/4855	9	{characterised by their physical properties, e.g. being electrically-conductive}	B29C65/48	B29C65/48		294
B29C65/486	9	{characterised by their physical form being non-liquid, e.g. in the form of granules or powders (B29C65/50 takes precedence)}	B29C65/48	B29C65/48		287
B29C65/4865	9	{containing additives (C09J11/00 and subgroups take precedence)}	B29C65/48	B29C65/48		246
B29C65/487	10	{characterised by their shape, e.g. being fibres or being spherical}	B29C65/48	B29C65/48		12
B29C65/4875	11	{being spherical, e.g. particles or powders}	B29C65/48	B29C65/48		233
B29C65/488	11	{being longitudinal, e.g. fibres}	B29C65/48	B29C65/48		124
B29C65/4885	10	{characterised by their composition being non-plastics}	B29C65/48	B29C65/48		170
B29C65/489	11	{being metals}	B29C65/48	B29C65/48		117
B29C65/4895	9	{Solvent bonding, i.e. the surfaces of the parts to be joined being treated with solvents, swelling or softening agents, without adhesives}	B29C65/48	B29C65/48		647
B29C65/50	9	using adhesive tape {, e.g. thermoplastic tape; using threads or the like (B29C65/3444 takes precedence)}	B29C65/50	B29C65/50		616
B29C65/5007	10	{characterised by the structure of said adhesive tape, threads or the like}	B29C65/50	B29C65/50		113
B29C65/5014	11	{being fibre-reinforced (B29C65/5028 takes precedence)}	B29C65/50	B29C65/50		306
B29C65/5021	11	{being multi-layered}	B29C65/50	B29C65/50		727
B29C65/5028	11	{being textile in woven or non-woven form}	B29C65/50	B29C65/50		386
B29C65/5035	11	{being in thread form, i.e. in the form of a single filament, e.g. in the form of a single coated filament}	B29C65/50	B29C65/50		213
B29C65/5042	10	{covering both elements to be joined}	B29C65/50	B29C65/50		1444
B29C65/505	11	{and placed in a recess formed in the parts to be joined, e.g. in order to obtain a continuous surface}	B29C65/50	B29C65/50		139
B29C65/5057	10	{positioned between the surfaces to be joined (B29C65/5035 takes precedence)}	B29C65/50	B29C65/50		2145
B29C65/5064	10	{of particular form, e.g. being C-shaped, T-shaped}	B29C65/50	B29C65/50		39
B29C65/5071	11	{and being composed by one single element}	B29C65/50	B29C65/50		425
B29C65/5078	11	{and being composed by several elements}	B29C65/50	B29C65/50		111
B29C65/5085	11	{and comprising grooves, e.g. being E-shaped, H-shaped}	B29C65/50	B29C65/50		247
B29C65/5092	10	{characterised by the tape handling mechanisms, e.g. using vacuum}	B29C65/50	B29C65/50		662
B29C65/52	9	{characterised by the way of} applying the adhesive {(B29C65/50 takes precedence; apparatus for applying liquids in general B05C; processes for applying liquids in general B05D)}	B29C65/52	B29C65/52		1333
B29C65/521	10	{by spin coating}	B29C65/52	B29C65/52		344
B29C65/522	10	{by spraying, e.g. by flame spraying}	B29C65/52	B29C65/52		636
B29C65/523	10	{by dipping}	B29C65/52	B29C65/52		93
B29C65/524	10	{by applying the adhesive from an outlet device in contact with, or almost in contact with, the surface of the part to be joined}	B29C65/52	B29C65/52		634
B29C65/525	11	{by extrusion coating}	B29C65/52	B29C65/52		135
B29C65/526	10	{by printing or by transfer from the surfaces of elements carrying the adhesive, e.g. using brushes, pads, rollers, stencils or silk screens}	B29C65/52	B29C65/52		652
B29C65/527	10	{by gravity only, e.g. by pouring}	B29C65/52	B29C65/52		60
B29C65/528	10	{by CVD or by PVD, i.e. by chemical vapour deposition or by physical vapour deposition}	B29C65/52	B29C65/52		23
B29C65/54	10	between pre-assembled parts	B29C65/54	B29C65/54		663
B29C65/542	11	{by injection}	B29C65/54	B29C65/54		544
B29C65/544	11	{by suction}	B29C65/54	B29C65/54		91
B29C65/546	11	{by gravity, e.g. by pouring}	B29C65/54	B29C65/54		89
B29C65/548	11	{by capillarity}	B29C65/54	B29C65/54		88
B29C65/56	8	using mechanical means {or mechanical connections, e.g. form-fits}	B29C65/56	B29C65/56		2758
B29C65/561	9	{using screw-threads being integral at least to one of the parts to be joined}	B29C65/56	B29C65/56		406
B29C65/562	9	{using extra joining elements, i.e. which are not integral with the parts to be joined (using plastic snap elements B29C65/58; using plastic rivets B29C65/601)}	B29C65/56	B29C65/56		1131
B29C65/564	10	{hidden in the joint, e.g. dowels or Z-pins (B29C65/603 takes precedence)}	B29C65/56	B29C65/56		386
B29C65/565	9	{involving interference fits, e.g. force-fits or press-fits (B29C65/66 takes precedence)}	B29C65/56	B29C65/56		812
B29C65/567	9	{using a tamping or a swaging operation, i.e. at least partially deforming the edge or the rim of a first part to be joined to clamp a second part to be joined}	B29C65/56	B29C65/56		155
B29C65/568	10	{using a swaging operation, i.e. totally deforming the edge or the rim of a first part to be joined to clamp a second part to be joined}	B29C65/56	B29C65/56		419
B29C65/58	9	Snap connection	B29C65/58	B29C65/58		932
B29C65/60	9	Riveting {or staking}	B29C65/60	B29C65/60		355
B29C65/601	10	{using extra riveting elements, i.e. the rivets being non-integral with the parts to be joined}	B29C65/60	B29C65/60		408
B29C65/602	11	{using hollow rivets (B29C65/607 takes precedence)}	B29C65/60	B29C65/60		121
B29C65/603	11	{the rivets being pushed in blind holes}	B29C65/60	B29C65/60		77
B29C65/604	12	{in both parts}	B29C65/60	B29C65/60		17
B29C65/605	11	{the rivets being molded in place, e.g. by injection}	B29C65/60	B29C65/60		73
B29C65/606	10	{the rivets being integral with one of the parts to be joined, i.e. staking}	B29C65/60	B29C65/60		766
B29C65/607	11	{the integral rivets being hollow}	B29C65/60	B29C65/60		226
B29C65/608	11	{the integral rivets being pushed in blind holes}	B29C65/60	B29C65/60		98
B29C65/609	11	{the integral rivets being plunge-formed}	B29C65/60	B29C65/60		113
B29C65/62	9	Stitching	B29C65/62	B29C65/62		783
B29C65/64	9	Joining a non-plastics element to a plastics element, e.g. by force (B29C65/44 takes precedence)<br><br><u>NOTE</u><br><br> When classifying in this group, compositions of the non-plastics element are additionally classified in the relevant groups, i.e. in B29C66/74 and subgroups 	B29C65/64	B29C65/64		1437
B29C65/645	10	{using friction or ultrasonic vibrations}<br><br><u>NOTE</u><br><br>When classifying in this group, compositions of the non-plastics element are additionally classified in the relevant groups, i.e. in B29C66/74 and subgroups. 	B29C65/64	B29C65/64		359
B29C65/66	8	by liberation of internal stresses, e.g. shrinking of one of the parts to be joined	B29C65/66	B29C65/66		487
B29C65/665	9	{using shrinking during cooling}	B29C65/66	B29C65/66		149
B29C65/68	9	using auxiliary shrinkable elements	B29C65/68	B29C65/68		381
B29C65/70	8	by moulding (using a particular moulding technique, see the relevant technique {, e.g. by injection B29C45/14467})<br><br><u>NOTE</u><br><br>This group covers only techniques involving the use of a mould	B29C65/70	B29C65/70		1086
B29C65/72	8	by combined operations {or combined techniques}, e.g. welding and stitching	B29C65/72	B29C65/72		2229
B29C65/74	8	by welding and severing {, or by joining and severing, the severing being performed in the area to be joined, next to the area to be joined, in the joint area or next to the joint area}<br><br><u>NOTE</u><br><br> When classifying in this group, joining techniques are additionally classified in the relevant groups, e.g. in B29C65/02 and subgroups 	B29C65/74	B29C65/74		2203
B29C65/741	9	{characterised by the relationships between the joining step and the severing step (cutting as mechanical pre-treatment B29C66/02241; cutting as thermal pre-treatment B29C66/0246; cutting as mechanical after-treatment B29C66/0326; cutting as thermal after-treatment B29C66/0346)}	B29C65/74	B29C65/74		126
B29C65/7411	10	{characterised by the temperature relationship between the joining step and the severing step}	B29C65/74	B29C65/74		3
B29C65/7412	11	{the joining step and the severing step being performed at different temperatures}	B29C65/74	B29C65/74		72
B29C65/7415	10	{characterised by the pressure relationship between the joining step and the severing step}	B29C65/74	B29C65/74		1
B29C65/7416	11	{the joining step and the severing step being performed at different pressures}	B29C65/74	B29C65/74		16
B29C65/7419	10	{characterised by the time relationship between the joining step and the severing step, said joining step and said severing step being performed by the same tool but at different times}	B29C65/74	B29C65/74		38
B29C65/743	9	{using the same tool for both joining and severing, said tool being monobloc or formed by several parts mounted together and forming a monobloc (B29C65/2046 takes precedence)}	B29C65/74	B29C65/74		746
B29C65/7433	10	{the tool being a wire}	B29C65/74	B29C65/74		329
B29C65/7435	10	{the tool being a roller}	B29C65/74	B29C65/74		226
B29C65/7437	10	{the tool being a perforating tool (perforating as mechanical pre-treatment B29C66/02242)}	B29C65/74	B29C65/74		351
B29C65/7439	10	{for continuously and longitudinally welding and severing webs (B29C65/7435 takes precedence)}	B29C65/74	B29C65/74		164
B29C65/7441	10	{for making welds and cuts of other than simple rectilinear form}	B29C65/74	B29C65/74		654
B29C65/7443	10	{by means of ultrasonic vibrations}	B29C65/74	B29C65/74		526
B29C65/745	9	{using a single unit having both a severing tool and a welding tool}	B29C65/74	B29C65/74		532
B29C65/7451	10	{the severing tool and the welding tool being movable with respect to one-another}	B29C65/74	B29C65/74		870
B29C65/7453	10	{the severing tool being a wire}	B29C65/74	B29C65/74		82
B29C65/7455	10	{the unit being a roller}	B29C65/74	B29C65/74		67
B29C65/7457	10	{comprising a perforating tool}	B29C65/74	B29C65/74		137
B29C65/7459	10	{for continuously and longitudinally welding and severing webs (B29C65/7455 takes precedence)}	B29C65/74	B29C65/74		52
B29C65/7461	10	{for making welds and cuts of other than simple rectilinear form}	B29C65/74	B29C65/74		194
B29C65/747	9	{using other than mechanical means}	B29C65/74	B29C65/74		20
B29C65/7471	10	{using a fluid, e.g. hot gases}	B29C65/74	B29C65/74		35
B29C65/7473	10	{using radiation, e.g. laser, for simultaneously welding and severing}	B29C65/74	B29C65/74		194
B29C65/749	9	{Removing scrap (deburring welded articles B29C37/04)}	B29C65/74	B29C65/74		394
B29C65/76	8	Making non-permanent or releasable joints	B29C65/76	B29C65/76		919
B29C65/78	8	Means for handling the parts to be joined, e.g. for making containers or hollow articles {, e.g. means for handling sheets, plates, web-like materials, tubular articles, hollow articles or elements to be joined therewith; Means for discharging the joined articles from the joining apparatus}<br><br><u>WARNING</u><br> Subgroups of B29C65/78 are not complete, pending a reorganisation; see also this group and its subgroups and B29C65/20 and its subgroups 	B29C65/78	B29C65/78		1954
B29C65/7802	9	{Positioning the parts to be joined, e.g. aligning, indexing or centring}	B29C65/78	B29C65/78		2725
B29C65/7805	10	{the parts to be joined comprising positioning features}	B29C65/78	B29C65/78		731
B29C65/7808	11	{in the form of holes or slots (B29C65/7814 takes precedence; holding or clamping means cooperating with specially formed features of at least one of the parts to be joined B29C65/7844)}	B29C65/78	B29C65/78		192
B29C65/7811	12	{for centring purposes}	B29C65/78	B29C65/78		220
B29C65/7814	11	{in the form of inter-cooperating positioning features (holding or clamping means cooperating with specially formed features of at least one of the parts to be joined B29C65/7844), e.g. tenons and mortises (tenon and mortise joints B29C66/126; tongue and groove joints B29C66/124)}	B29C65/78	B29C65/78		313
B29C65/7817	11	{in the form of positioning marks}	B29C65/78	B29C65/78		75
B29C65/782	10	{by setting the gap between the parts to be joined (controlling or regulating the gap between the joining tools B29C66/92611)}	B29C65/78	B29C65/78		86
B29C65/7823	11	{by using distance pieces, i.e. by using spacers positioned between the parts to be joined and forming a part of the joint}	B29C65/78	B29C65/78		18
B29C65/7826	12	{said distance pieces being non-integral with the parts to be joined, e.g. particles}	B29C65/78	B29C65/78		135
B29C65/7829	12	{said distance pieces being integral with at least one of the parts to be joined}	B29C65/78	B29C65/78		213
B29C65/7832	10	{by setting the overlap between the parts to be joined, e.g. the overlap between sheets, plates or web-like materials}	B29C65/78	B29C65/78		288
B29C65/7835	10	{by using stops (B29C65/7823, B29C66/92651 take precedence; tongue and groove joints B29C66/124; tenon and mortise joints B29C66/126)}	B29C65/78	B29C65/78		150
B29C65/7838	10	{from the inside, e.g. of tubular or hollow articles (B29C66/3242 takes precedence)}	B29C65/78	B29C65/78		181
B29C65/7841	9	{Holding or clamping means for handling purposes (clamping means for the purpose of applying pressure on the parts to be joined, in the area to be joined B29C66/81; work holders in general B25B; devices for holding or positioning work for welding metal B23K37/04)}	B29C65/78	B29C65/78		5564
B29C65/7844	10	{cooperating with specially formed features of at least one of the parts to be joined, e.g. cooperating with holes or ribs of at least one of the parts to be joined (parts to be joined comprising holes or slots for the purpose of positioning said parts B29C65/7808; parts to be joined comprising inter-cooperating positioning features B29C65/7814;  welding using friction, the welding tool cooperating with specially formed features of at least one of the parts to be joined, e.g. cooperating with holes or ribs of at least one of the parts to be joined B29C65/069)}	B29C65/78	B29C65/78		275
B29C65/7847	10	{using vacuum to hold at least one of the parts to be joined (vacuum work holders in general B25B11/005)}	B29C65/78	B29C65/78		1830
B29C65/785	10	{using magnetic forces to hold at least one of the parts to be joined (magnetic work holders in general B25B11/002)}	B29C65/78	B29C65/78		69
B29C65/7852	10	{using electrostatic forces to hold at least one of the parts to be joined}	B29C65/78	B29C65/78		59
B29C65/7855	9	{Provisory fixing}	B29C65/78	B29C65/78		444
B29C65/7858	9	{characterised by the feeding movement of the parts to be joined}	B29C65/78	B29C65/78		2229
B29C65/7861	10	{In-line machines, i.e. feeding, joining and discharging are in one production line (B29C65/7879, B29C65/7888 take precedence)}	B29C65/78	B29C65/78		1007
B29C65/7864	11	{using a feeding table which moves to and fro (oscillating around an axis B29C65/7876)}	B29C65/78	B29C65/78		124
B29C65/7867	11	{using carriers, provided with holding means, said carriers moving in a closed path}	B29C65/78	B29C65/78		158
B29C65/787	11	{using conveyor belts or conveyor chains (B29C66/83421, B29C66/83521, B29C66/83531 take precedence)}	B29C65/78	B29C65/78		619
B29C65/7873	12	{using cooperating conveyor belts or cooperating conveyor chains (B29C66/83423, B29C66/83523, B29C66/83533 take precedence)}	B29C65/78	B29C65/78		288
B29C65/7876	10	{oscillating around an axis (B29C65/7888 takes precedence)}	B29C65/78	B29C65/78		75
B29C65/7879	10	{said parts to be joined moving in a closed path, e.g. a rectangular path (B29C65/7888 takes precedence)}	B29C65/78	B29C65/78		40
B29C65/7882	11	{said parts to be joined moving in a circular path}	B29C65/78	B29C65/78		452
B29C65/7885	12	{Rotary turret joining machines, i.e. having several joining tools moving around an axis}<br><br><u>WARNING</u><br> Group B29C65/7885 is incomplete pending reclassification of documents from B29C65/0672.<br> Groups B29C65/0672 and B29C65/7885 should be considered in order to perform a complete search. 	B29C65/78	B29C65/78		302
B29C65/7888	10	{Means for handling of moving sheets or webs}	B29C65/78	B29C65/78		295
B29C65/7891	11	{of discontinuously moving sheets or webs}	B29C65/78	B29C65/78		650
B29C65/7894	11	{of continuously moving sheets or webs}	B29C65/78	B29C65/78		1098
B29C65/7897	9	{Means for discharging the joined articles from the joining apparatus (B29C66/005 takes precedence; discharging moulded articles from moulds B29C37/0003)}	B29C65/78	B29C65/78		516
B29C65/80	9	Rotatable transfer means {for loading or unloading purposes, i.e. turret transfer means (B29C65/7879 takes precedence; in-line machines using carriers, provided with holding means, said carriers moving in a closed path B29C65/7867; in-line machines using conveyor belts or conveyor chains B29C65/787)}	B29C65/80	B29C65/80		655
B29C65/82	8	Testing the joint	B29C65/82	B29C65/82		363
B29C65/8207	9	{by mechanical methods}	B29C65/82	B29C65/82		278
B29C65/8215	10	{Tensile tests}	B29C65/82	B29C65/82		544
B29C65/8223	10	{Peel tests}	B29C65/82	B29C65/82		189
B29C65/823	10	{Bend tests}	B29C65/82	B29C65/82		28
B29C65/8238	10	{Impact tests}	B29C65/82	B29C65/82		26
B29C65/8246	10	{Pressure tests, e.g. hydrostatic pressure tests}	B29C65/82	B29C65/82		359
B29C65/8253	9	{by the use of waves or particle radiation, e.g. visual examination, scanning electron microscopy, or X-rays (B29C65/8292 takes precedence)}	B29C65/82	B29C65/82		621
B29C65/8261	9	{by the use of thermal means}	B29C65/82	B29C65/82		49
B29C65/8269	9	{by the use of electric or magnetic means}	B29C65/82	B29C65/82		16
B29C65/8276	10	{by the use of electric means}	B29C65/82	B29C65/82		72
B29C65/8284	10	{by the use of magnetic means}	B29C65/82	B29C65/82		25
B29C65/8292	9	{by the use of ultrasonic, sonic or infrasonic waves}	B29C65/82	B29C65/82		118
B29C66/00	7	{General aspects of processes or apparatus for joining preformed parts (means for handling the parts to be joined B29C65/78; testing the joint B29C65/82)}	B29C65/00	B29C66/00		213
B29C66/001	8	{Joining in special atmospheres}<br><br><u>WARNING</u><br> Subgroups of B29C66/001 are not complete, pending a reorganisation; see also this group 	B29C65/00	B29C66/001		268
B29C66/0012	9	{characterised by the type of environment}	B29C65/00	B29C66/0012		8
B29C66/0014	10	{Gaseous environments}	B29C65/00	B29C66/0014		79
B29C66/00141	11	{Protective gases}	B29C65/00	B29C66/00141		239
B29C66/00143	11	{Active gases}	B29C65/00	B29C66/00143		36
B29C66/00145	11	{Vacuum, e.g. partial vacuum}	B29C65/00	B29C66/00145		433
B29C66/0016	10	{Liquid environments, i.e. the parts to be joined being submerged in a liquid}	B29C65/00	B29C66/0016		63
B29C66/0018	10	{being sterile}	B29C65/00	B29C66/0018		204
B29C66/002	8	{Removing toxic gases}	B29C65/00	B29C66/002		179
B29C66/003	8	{Protecting areas of the parts to be joined from overheating (B29C66/348, B29C66/8744 take precedence)}	B29C65/00	B29C66/003		343
B29C66/004	8	{Preventing sticking together, e.g. of some areas of the parts to be joined}	B29C65/00	B29C66/004		500
B29C66/0042	9	{of the joining tool and the parts to be joined (B29C66/0046 takes precedence; joining tool characterized by its composition B29C66/8122; joining tool characterized by its microstructure B29C66/8124)}	B29C65/00	B29C66/0042		634
B29C66/0044	10	{using a separating sheet, e.g. fixed on the joining tool}	B29C65/00	B29C66/0044		737
B29C66/00441	11	{movable, e.g. mounted on reels}	B29C65/00	B29C66/00441		258
B29C66/0046	9	{by the use of a lubricant, e.g. fluid, powder}	B29C65/00	B29C66/0046		51
B29C66/00461	10	{being liquid, e.g. oil based}	B29C65/00	B29C66/00461		76
B29C66/00463	10	{being solid, e.g. a powder}	B29C65/00	B29C66/00463		22
B29C66/005	8	{Detaching the article from the joining tool}	B29C65/00	B29C66/005		207
B29C66/006	8	{Preventing damaging, e.g. of the parts to be joined (B29C66/003, B29C66/004, B29C66/348 take precedence)}<br><br><u>WARNING</u><br> Group B29C66/006 and subgroups are not complete, pending a reorganisation; see also B29C65/00 and subgroups 	B29C65/00	B29C66/006		187
B29C66/0062	9	{of the joining tool, e.g. avoiding wear of the joining tool}	B29C65/00	B29C66/0062		126
B29C66/01	8	{General aspects dealing with the joint area or with the area to be joined (B29C65/76, B29C65/82 take precedence)}	B29C65/00	B29C66/01		61
B29C66/02	9	{Preparation of the material, in the area to be joined, prior to joining or welding (B29C66/32 takes precedence)}	B29C65/00	B29C66/02		525
B29C66/022	10	{Mechanical pre-treatments, e.g. reshaping}	B29C65/00	B29C66/022		527
B29C66/0222	11	{without removal of material, e.g. cleaning by air blowing or using brushes}	B29C65/00	B29C66/0222		864
B29C66/0224	11	{with removal of material}	B29C65/00	B29C66/0224		261
B29C66/02241	12	{Cutting, e.g. by using waterjets, or sawing (using heat B29C66/0246; cutting-off or cutting-out a part of a strip-like or sheet-like material, transferring that part and fixing it to an article B29C69/005)}	B29C65/00	B29C66/02241		1289
B29C66/02242	13	{Perforating or boring}	B29C65/00	B29C66/02242		276
B29C66/02245	12	{Abrading, e.g. grinding, sanding, sandblasting or scraping}	B29C65/00	B29C66/02245		649
B29C66/024	10	{Thermal pre-treatments}	B29C65/00	B29C66/024		63
B29C66/0242	11	{Heating, or preheating, e.g. drying (B29C66/3464 takes precedence)}	B29C65/00	B29C66/0242		1716
B29C66/0244	11	{Cooling}	B29C65/00	B29C66/0244		124
B29C66/0246	11	{Cutting or perforating, e.g. burning away by using a laser or using hot air (simultaneously welding and severing using a fluid B29C65/7471; simultaneously welding and severing using radiation B29C65/7473; cutting-off or cutting-out a part of a strip-like or sheet-like material, transferring that part and fixing it to an article B29C69/005)}	B29C65/00	B29C66/0246		279
B29C66/026	10	{Chemical pre-treatments (B29C66/028 takes precedence)}	B29C65/00	B29C66/026		550
B29C66/028	10	{Non-mechanical surface pre-treatments, i.e. by flame treatment, electric discharge treatment, plasma treatment, wave energy or particle radiation (B29C65/14 takes precedence; non-mechanical surface treatment of plastics in general B29C59/08&#160;-&#160;B29C59/16)}	B29C65/00	B29C66/028		503
B29C66/03	9	{After-treatments in the joint area (B29C66/3262 takes precedence)}	B29C65/00	B29C66/03		151
B29C66/032	10	{Mechanical after-treatments (deburring welded articles B29C37/04)}	B29C65/00	B29C66/032		295
B29C66/0322	11	{Post-pressing without reshaping, i.e. keeping the joint under pressure after joining}	B29C65/00	B29C66/0322		424
B29C66/0324	11	{Reforming or reshaping the joint, e.g. folding over (reshaping the burr B29C66/326)}	B29C65/00	B29C66/0324		300
B29C66/03241	12	{Flattening}	B29C65/00	B29C66/03241		188
B29C66/03242	13	{of sheets being positioned in abutment, e.g. after folding open of an overlap joint}	B29C65/00	B29C66/03242		76
B29C66/0326	11	{Cutting, e.g. by using waterjets, or perforating (using heat B29C66/0346)}<br><br><u>WARNING</u><br> Not complete, pending a reorganisation; see also B29C66/032	B29C65/00	B29C66/0326		702
B29C66/034	10	{Thermal after-treatments}	B29C65/00	B29C66/034		287
B29C66/0342	11	{Cooling, e.g. transporting through welding and cooling zone}	B29C65/00	B29C66/0342		1474
B29C66/0344	11	{Annealing}<br><br><u>WARNING</u><br> Not complete, pending a reorganisation; see also B29C66/034	B29C65/00	B29C66/0344		37
B29C66/0346	11	{Cutting or perforating, e.g. burning away by using a laser or using hot air (simultaneously joining and severing using a fluid B29C65/7471; simultaneously welding and severing using radiation B29C65/7473)}<br><br><u>WARNING</u><br> Not complete, pending a reorganisation; see also B29C66/034	B29C65/00	B29C66/0346		49
B29C66/038	10	{Covering the joint by a coating material}	B29C65/00	B29C66/038		82
B29C66/0382	11	{the coating material being in liquid or paste form (joining by applying molten plastics B29C65/40)}	B29C65/00	B29C66/0382		56
B29C66/0384	11	{the coating material being in tape, strip or band form (joining using adhesive tapes covering both elements to be joined B29C65/5042)}	B29C65/00	B29C66/0384		168
B29C66/05	9	{Particular design of joint configurations}<br><br><u>NOTE</u><br><br> In this group the possible supplementary joining material, e.g. adhesive or adhesive tape, is not taken into account for the joint configuration. The use of supplementary joining material, e.g. adhesive or adhesive tape, has to be additionally classified as such, e.g. in B29C65/48 and subgroups or B29C65/50 and subgroups <br><br><u>WARNING</u><br> Group B29C66/05 and subgroups are not complete, pending a reorganisation; see also B29C65/00 and its subgroups 	B29C65/00	B29C66/05		94
B29C66/10	10	{particular design of the joint cross-sections}<br><br><u>NOTE</u><br><br>The scope of the subgroups is defined by the drawings in the Definitions	B29C65/00	B29C66/10		30
B29C66/11	11	{Joint cross-sections comprising a single joint-segment, i.e. one of the parts to be joined comprising a single joint-segment in the joint cross-section (B29C66/12 and subgroups take precedence)}	B29C65/00	B29C66/11		26
B29C66/112	12	{Single lapped joints}	B29C65/00	B29C66/112		5278
B29C66/1122	13	{Single lap to lap joints, i.e. overlap joints (B29C66/45, B29C66/472, B29C66/52272 take precedence)}	B29C65/00	B29C66/1122		24421
B29C66/114	12	{Single butt joints}	B29C65/00	B29C66/114		1805
B29C66/1142	13	{Single butt to butt joints}	B29C65/00	B29C66/1142		5605
B29C66/116	12	{Single bevelled joints, i.e. one of the parts to be joined being bevelled in the joint area}	B29C65/00	B29C66/116		298
B29C66/1162	13	{Single bevel to bevel joints, e.g. mitre joints}	B29C65/00	B29C66/1162		1567
B29C66/118	12	{Single monotone curved joints}	B29C65/00	B29C66/118		104
B29C66/1182	13	{the joint being C-shaped}	B29C65/00	B29C66/1182		53
B29C66/12	11	{Joint cross-sections combining only two joint-segments; Tongue and groove joints; Tenon and mortise joints; Stepped joint cross-sections}	B29C65/00	B29C66/12		9
B29C66/122	12	{Joint cross-sections combining only two joint-segments, i.e. one of the parts to be joined comprising only two joint-segments in the joint cross-section (B29C66/124 takes precedence)}	B29C65/00	B29C66/122		18
B29C66/1222	13	{comprising at least a lapped joint-segment}	B29C65/00	B29C66/1222		2500
B29C66/12221	14	{the two joint-segments being lapped}	B29C65/00	B29C66/12221		29
B29C66/1224	13	{comprising at least a butt joint-segment}	B29C65/00	B29C66/1224		2472
B29C66/12241	14	{the two joint-segments being butt}	B29C65/00	B29C66/12241		20
B29C66/1226	13	{comprising at least one bevelled joint-segment}	B29C65/00	B29C66/1226		506
B29C66/12261	14	{the two joint-segments being bevelled, e.g. the two joint-segments forming a V}	B29C65/00	B29C66/12261		116
B29C66/1228	13	{comprising at least one monotone curved joint-segment}	B29C65/00	B29C66/1228		76
B29C66/12281	14	{the two joint-segments being monotone curved}	B29C65/00	B29C66/12281		5
B29C66/124	12	{Tongue and groove joints}	B29C65/00	B29C66/124		330
B29C66/1242	13	{comprising interlocking undercuts}	B29C65/00	B29C66/1242		19
B29C66/12421	14	{Teardrop-like, waterdrop-like or mushroom-like interlocking undercuts}	B29C65/00	B29C66/12421		127
B29C66/12423	14	{Dovetailed interlocking undercuts}	B29C65/00	B29C66/12423		118
B29C66/12425	14	{Other specific interlocking undercuts not provided for in B29C66/12421&#160;-&#160;B29C66/12423}	B29C65/00	B29C66/12425		52
B29C66/1244	13	{characterised by the male part, i.e. the part comprising the tongue}	B29C65/00	B29C66/1244		7
B29C66/12441	14	{being a single wall}	B29C65/00	B29C66/12441		941
B29C66/12443	14	{having the tongue substantially in the middle}	B29C65/00	B29C66/12443		338
B29C66/12445	14	{having the tongue on the side}	B29C65/00	B29C66/12445		191
B29C66/12449	14	{being asymmetric (B29C66/12445 takes precedence)}	B29C65/00	B29C66/12449		246
B29C66/1246	13	{characterised by the female part, i.e. the part comprising the groove}	B29C65/00	B29C66/1246		9
B29C66/12461	14	{being rounded, i.e. U-shaped or C-shaped}	B29C65/00	B29C66/12461		228
B29C66/12463	14	{being tapered}	B29C65/00	B29C66/12463		380
B29C66/12464	15	{being V-shaped}	B29C65/00	B29C66/12464		177
B29C66/12469	14	{being asymmetric}	B29C65/00	B29C66/12469		614
B29C66/1248	13	{Interpenetrating groove joints (interpenetrating fingered joints B29C66/139)}	B29C65/00	B29C66/1248		174
B29C66/126	12	{Tenon and mortise joints (tenons and mortises for positioning purposes B29C65/7814)}	B29C65/00	B29C66/126		317
B29C66/128	12	{Stepped joint cross-sections}	B29C65/00	B29C66/128		91
B29C66/1282	13	{comprising at least one overlap joint-segment}	B29C65/00	B29C66/1282		786
B29C66/12821	14	{comprising at least two overlap joint-segments}	B29C65/00	B29C66/12821		344
B29C66/12822	15	{comprising at least three overlap joint-segments}	B29C65/00	B29C66/12822		92
B29C66/1284	13	{comprising at least one butt joint-segment}	B29C65/00	B29C66/1284		262
B29C66/12841	14	{comprising at least two butt joint-segments}	B29C65/00	B29C66/12841		777
B29C66/12842	15	{comprising at least three butt joint-segments}	B29C65/00	B29C66/12842		142
B29C66/1286	13	{comprising at least one bevelled joint-segment}	B29C65/00	B29C66/1286		296
B29C66/12861	14	{comprising at least two bevelled joint-segments}	B29C65/00	B29C66/12861		97
B29C66/12862	15	{comprising at least three bevelled joint-segments}	B29C65/00	B29C66/12862		33
B29C66/1288	13	{comprising at least one monotone curved joint-segment}	B29C65/00	B29C66/1288		30
B29C66/12881	14	{comprising at least two monotone curved joint-segments}	B29C65/00	B29C66/12881		32
B29C66/12882	15	{comprising at least three monotone curved joint-segments}	B29C65/00	B29C66/12882		3
B29C66/13	11	{Single flanged joints; Fin-type joints; Single hem joints; Edge joints; Interpenetrating fingered joints; Other specific particular designs of joint cross-sections not provided for in groups B29C66/11&#160;-&#160;B29C66/12}	B29C65/00	B29C66/13		80
B29C66/131	12	{Single flanged joints, i.e. one of the parts to be joined being rigid and flanged in the joint area}	B29C65/00	B29C66/131		3953
B29C66/1312	13	{Single flange to flange joints, the parts to be joined being rigid (the parts to be joined being flexible B29C66/133)}	B29C65/00	B29C66/1312		1845
B29C66/133	12	{Fin-type joints, the parts to be joined being flexible (the parts to be joined being rigid B29C66/1312)}	B29C65/00	B29C66/133		1401
B29C66/135	12	{Single hemmed joints, i.e. one of the parts to be joined being hemmed in the joint area}	B29C65/00	B29C66/135		852
B29C66/1352	13	{Single hem to hem joints}	B29C65/00	B29C66/1352		245
B29C66/137	12	{Beaded-edge joints or bead seals (for sealing or securing package folds or closures B65B51/24)}	B29C65/00	B29C66/137		770
B29C66/139	12	{Interpenetrating fingered joints}	B29C65/00	B29C66/139		38
B29C66/14	11	{the joint having the same thickness as the thickness of the parts to be joined (B29C66/1142 takes precedence)}	B29C65/00	B29C66/14		809
B29C66/20	10	{particular design of the joint lines, e.g. of the weld lines}<br><br><u>NOTE</u><br><br>The scope of the subgroups is defined by the drawings in the Definitions	B29C65/00	B29C66/20		85
B29C66/21	11	{said joint lines being formed by a single dot or dash or by several dots or dashes, i.e. spot joining or spot welding}	B29C65/00	B29C66/21		3057
B29C66/22	11	{said joint lines being in the form of recurring patterns (B29C66/234 takes precedence)}	B29C65/00	B29C66/22		21
B29C66/221	12	{being in the form of a sinusoidal wave (B29C66/2272 takes precedence)}	B29C65/00	B29C66/221		282
B29C66/223	12	{being in the form of a triangle wave or of a sawtooth wave, e.g. zigzagged}	B29C65/00	B29C66/223		247
B29C66/225	12	{being castellated, e.g. in the form of a square wave or of a rectangular wave (B29C66/2276 takes precedence)}	B29C65/00	B29C66/225		116
B29C66/227	12	{being in the form of repetitive interlocking undercuts, e.g. in the form of puzzle cuts (tongue and groove joints or tenon and mortise joints comprising interlocking undercuts B29C66/1242)}	B29C65/00	B29C66/227		5
B29C66/2272	13	{Teardrop-like, waterdrop-like or mushroom-like interlocking undercuts (tongue and groove joints or tenon and mortise joints comprising teardrop-like, waterdrop-like or mushroom-like interlocking undercuts B29C66/12421)}	B29C65/00	B29C66/2272		114
B29C66/2274	13	{Dovetailed interlocking undercuts (tongue and groove joints or tenon and mortise joints comprising dovetailed interlocking undercuts B29C66/12423)}	B29C65/00	B29C66/2274		72
B29C66/2276	13	{Other specific local geometries of interlocking undercuts not provided for in B29C66/2272&#160;-&#160;B29C66/2274(tongue and groove joints or tenon and mortise joints comprising other specific interlocking undercuts B29C66/12425)}	B29C65/00	B29C66/2276		61
B29C66/229	12	{Other specific patterns not provided for in B29C66/221&#160;-&#160;B29C66/227}	B29C65/00	B29C66/229		86
B29C66/23	11	{said joint lines being multiple and parallel or being in the form of tessellations}	B29C65/00	B29C66/23		2
B29C66/232	12	{said joint lines being multiple and parallel, i.e. the joint being formed by several parallel joint lines}	B29C65/00	B29C66/232		1492
B29C66/234	12	{said joint lines being in the form of tessellations}	B29C65/00	B29C66/234		182
B29C66/24	11	{said joint lines being closed or non-straight}	B29C65/00	B29C66/24		70
B29C66/242	12	{said joint lines being closed, i.e. forming closed contours}	B29C65/00	B29C66/242		435
B29C66/2422	13	{being circular, oval or elliptical}	B29C65/00	B29C66/2422		7
B29C66/24221	14	{being circular (B29C66/51 takes precedence)}	B29C65/00	B29C66/24221		1315
B29C66/24223	14	{being oval}	B29C65/00	B29C66/24223		76
B29C66/24225	14	{being elliptical}	B29C65/00	B29C66/24225		31
B29C66/2424	13	{being a closed polygonal chain}	B29C65/00	B29C66/2424		22
B29C66/24241	14	{forming a triangle}	B29C65/00	B29C66/24241		45
B29C66/24243	14	{forming a quadrilateral}	B29C65/00	B29C66/24243		23
B29C66/24244	15	{forming a rectangle}	B29C65/00	B29C66/24244		845
B29C66/24245	16	{forming a square}	B29C65/00	B29C66/24245		165
B29C66/24249	14	{forming a specific polygon not provided for in B29C66/24241&#160;-&#160;B29C66/24243}	B29C65/00	B29C66/24249		66
B29C66/244	12	{said joint lines being non-straight, e.g. forming non-closed contours}	B29C65/00	B29C66/244		718
B29C66/2442	13	{in the form of a single arc of circle}	B29C65/00	B29C66/2442		128
B29C66/246	12	{said joint lines forming figures, e.g. animals, flowers, hearts}	B29C65/00	B29C66/246		104
B29C66/301	10	{Three-dimensional joints, i.e. the joined area being substantially non-flat (B29C66/5223, B29C66/5224, B29C66/5225 take precedence)}	B29C65/00	B29C66/301		988
B29C66/302	10	{the area to be joined comprising melt initiators}	B29C65/00	B29C66/302		7
B29C66/3022	11	{said melt initiators being integral with at least one of the parts to be joined}	B29C65/00	B29C66/3022		247
B29C66/30221	12	{said melt initiators being point-like}	B29C65/00	B29C66/30221		250
B29C66/30223	12	{said melt initiators being rib-like}	B29C65/00	B29C66/30223		1230
B29C66/3024	11	{said melt initiators being non-integral with the parts to be joined}	B29C65/00	B29C66/3024		71
B29C66/303	10	{the joint involving an anchoring effect (B29C66/341, B29C65/56 and subgroups take precedence)}	B29C65/00	B29C66/303		158
B29C66/3032	11	{making use of protrusions or cavities belonging to at least one of the parts to be joined (B29C66/3034 takes precedence)}	B29C65/00	B29C66/3032		99
B29C66/30321	12	{making use of protrusions belonging to at least one of the parts to be joined}	B29C65/00	B29C66/30321		335
B29C66/30322	13	{in the form of rugosity}	B29C65/00	B29C66/30322		177
B29C66/30325	12	{making use of cavities belonging to at least one of the parts to be joined}	B29C65/00	B29C66/30325		596
B29C66/30326	13	{in the form of porosity}	B29C65/00	B29C66/30326		185
B29C66/3034	11	{making use of additional elements, e.g. meshes}	B29C65/00	B29C66/3034		165
B29C66/30341	12	{non-integral with the parts to be joined, e.g. making use of extra elements (B29C65/562 takes precedence)}	B29C65/00	B29C66/30341		259
B29C66/304	10	{Joining through openings in an intermediate part of the article (B29C66/3034 takes precedence)}	B29C65/00	B29C66/304		277
B29C66/305	10	{Decorative or coloured joints (optical properties of the material of the parts to be joined B29C66/733)}	B29C65/00	B29C66/305		327
B29C66/306	10	{Applying a mark during joining}	B29C65/00	B29C66/306		173
B29C66/3062	11	{in the form of letters or numbers}	B29C65/00	B29C66/3062		14
B29C66/30621	12	{in the form of letters}	B29C65/00	B29C66/30621		157
B29C66/30623	12	{in the form of numbers}	B29C65/00	B29C66/30623		54
B29C66/32	9	{Measures for keeping the burr form under control; Avoiding burr formation; Shaping the burr (deburring welded articles B29C37/04)}	B29C65/00	B29C66/32		179
B29C66/322	10	{Providing cavities in the joined article to collect the burr}	B29C65/00	B29C66/322		1077
B29C66/324	10	{Avoiding burr formation}	B29C65/00	B29C66/324		387
B29C66/3242	11	{on the inside of a tubular or hollow article}	B29C65/00	B29C66/3242		259
B29C66/326	10	{Shaping the burr, e.g. by the joining tool}	B29C65/00	B29C66/326		326
B29C66/3262	11	{as after-treatment, e.g. by a separate tool}	B29C65/00	B29C66/3262		127
B29C66/328	10	{Leaving the burrs unchanged for providing particular properties to the joint, e.g. as decorative effect}	B29C65/00	B29C66/328		22
B29C66/3282	11	{for reinforcing the joint}	B29C65/00	B29C66/3282		145
B29C66/3284	11	{for weakening the joint}	B29C65/00	B29C66/3284		16
B29C66/341	9	{Measures for intermixing the material of the joint interlayer}	B29C65/00	B29C66/341		174
B29C66/342	9	{Preventing air-inclusions}	B29C65/00	B29C66/342		536
B29C66/343	9	{Making tension-free or wrinkle-free joints}	B29C65/00	B29C66/343		194
B29C66/3432	10	{by holding the material loose or tension-free during joining}	B29C65/00	B29C66/3432		74
B29C66/344	9	{Stretching or tensioning the joint area during joining}	B29C65/00	B29C66/344		550
B29C66/345	9	{Progressively making the joint, e.g. starting from the middle (B29C66/8341, B29C65/12, B29C65/14, B29C65/16 take precedence)}	B29C65/00	B29C66/345		194
B29C66/3452	10	{Making complete joints by combining partial joints}	B29C65/00	B29C66/3452		932
B29C66/346	9	{Making joints having variable thicknesses in the joint area, e.g. by using jaws having an adapted configuration}	B29C65/00	B29C66/346		335
B29C66/3462	10	{by differentially heating the zones of different thickness}	B29C65/00	B29C66/3462		63
B29C66/3464	10	{by preheating}	B29C65/00	B29C66/3464		22
B29C66/347	9	{using particular temperature distributions or gradients; using particular heat distributions or gradients}	B29C65/00	B29C66/347		77
B29C66/3472	10	{in the plane of the joint, e.g. along the joint line in the plane of the joint or perpendicular to the joint line in the plane of the joint}	B29C65/00	B29C66/3472		395
B29C66/3474	10	{perpendicular to the plane of the joint}	B29C65/00	B29C66/3474		117
B29C66/348	9	{Avoiding melting or weakening of the zone directly next to the joint area, e.g. by cooling}	B29C65/00	B29C66/348		347
B29C66/349	9	{Cooling the welding zone on the welding spot}<br><br><u>WARNING</u><br> Subgroups of B29C66/349 are not complete, pending a reorganisation; see also this group 	B29C65/00	B29C66/349		259
B29C66/3492	10	{by means placed on the side opposed to the welding tool}	B29C65/00	B29C66/3492		60
B29C66/3494	10	{while keeping the welding zone under pressure}	B29C65/00	B29C66/3494		370
B29C66/40	8	{General aspects of joining substantially flat articles, e.g. plates, sheets or web-like materials; Making flat seams in tubular or hollow articles; Joining single elements to substantially flat surfaces}	B29C65/00	B29C66/40		132
B29C66/41	9	{Joining substantially flat articles (B29C66/47 and subgroups take precedence); Making flat seams in tubular or hollow articles (B29C66/51 and subgroups take precedence)}	B29C65/00	B29C66/41		1676
B29C66/43	10	{Joining a relatively small portion of the surface of said articles (B29C66/45 takes precedence)}	B29C65/00	B29C66/43		9076
B29C66/431	11	{Joining the articles to themselves (B29C66/4322 and B29C66/4332 take precedence)}	B29C65/00	B29C66/431		1682
B29C66/4312	12	{for making flat seams in tubular or hollow articles, e.g. transversal seams}	B29C65/00	B29C66/4312		3035
B29C66/43121	13	{Closing the ends of tubular or hollow single articles, e.g. closing the ends of bags (closing tube ends B29C57/10)}	B29C65/00	B29C66/43121		1885
B29C66/43122	14	{Closing the top of gable top containers (gable top containers B65D5/067)}	B29C65/00	B29C66/43122		254
B29C66/43123	14	{Closing the ends of squeeze tubes, e.g. for toothpaste or cosmetics (producing flexible squeeze tubes by combined operations B29D23/20; collapsible tubes B65D35/00)}	B29C65/00	B29C66/43123		219
B29C66/43129	13	{said flat seams being transversal but non-orthogonal with respect to the tubular or hollow articles, i.e. oblique}	B29C65/00	B29C66/43129		129
B29C66/432	11	{for making tubular articles or closed loops, e.g. by joining several sheets (B29C66/547 takes precedence; bending and joining sheets at right angles to the longitudinal axis of the article being formed and joining the edges B29C53/38); for making hollow articles or hollow preforms}	B29C65/00	B29C66/432		617
B29C66/4322	12	{by joining a single sheet to itself (B29C66/4332 takes precedence)}	B29C65/00	B29C66/4322		3932
B29C66/4324	12	{for making closed loops, e.g. belts}	B29C65/00	B29C66/4324		882
B29C66/4326	12	{for making hollow articles or hollow-preforms, e.g. half-shells}	B29C65/00	B29C66/4326		468
B29C66/4329	12	{the joint lines being transversal but non-orthogonal with respect to the axis of said tubular articles, i.e. being oblique}	B29C65/00	B29C66/4329		318
B29C66/433	11	{Casing-in, i.e. enclosing an element between two sheets by an outlined seam (for bookbinding B42C11/06; for packaging B65B; by laminating B32B37/00; enclosing tubular articles between substantially flat elements B29C66/53261)}	B29C65/00	B29C66/433		1199
B29C66/4332	12	{by folding a sheet over}	B29C65/00	B29C66/4332		243
B29C66/434	11	{Joining substantially flat articles for forming corner connections, fork connections or cross connections}	B29C65/00	B29C66/434		24
B29C66/4342	12	{Joining substantially flat articles for forming corner connections, e.g. for making V-shaped pieces}	B29C65/00	B29C66/4342		65
B29C66/43421	13	{with a right angle, e.g. for making L-shaped pieces}	B29C65/00	B29C66/43421		317
B29C66/4344	12	{Joining substantially flat articles for forming fork connections, e.g. for making Y-shaped pieces}	B29C65/00	B29C66/4344		35
B29C66/43441	13	{with two right angles, e.g. for making T-shaped pieces, H-shaped pieces}	B29C65/00	B29C66/43441		356
B29C66/4346	12	{Joining substantially flat articles for forming cross connections, e.g. for making X-shaped pieces}	B29C65/00	B29C66/4346		10
B29C66/43461	13	{with four right angles, e.g. for making +-shaped pieces}	B29C65/00	B29C66/43461		41
B29C66/435	11	{Making large sheets by joining smaller ones or strips together}	B29C65/00	B29C66/435		648
B29C66/436	11	{Joining sheets for making articles comprising cushioning or padding materials, the weld being performed through the cushioning material, e.g. car seats (joining through openings B29C66/304)}	B29C65/00	B29C66/436		314
B29C66/437	11	{Joining plastics plates for making venetian blinds (making venetian blinds in general E06B9/266)}	B29C65/00	B29C66/437		82
B29C66/438	11	{Joining sheets for making hollow-walled, channelled structures or multi-tubular articles}	B29C65/00	B29C66/438		474
B29C66/439	11	{Joining sheets for making inflated articles without using a mould}	B29C65/00	B29C66/439		228
B29C66/45	10	{Joining of substantially the whole surface of the articles (methods or apparatus for laminating B32B37/00)}	B29C65/00	B29C66/45		4629
B29C66/452	11	{the article having a disc form, e.g. making CDs or DVDs}	B29C65/00	B29C66/452		475
B29C66/47	9	{Joining single elements to sheets, plates or other substantially flat surfaces (B29C66/5326 takes precedence)}	B29C65/00	B29C66/47		545
B29C66/472	10	{said single elements being substantially flat}	B29C65/00	B29C66/472		1425
B29C66/4722	11	{Fixing strips to surfaces other than edge faces (fixing strips to edge faces B29C63/0026)}	B29C65/00	B29C66/4722		958
B29C66/4724	11	{said single elements being appliques, e.g. in the form of a text or drawing}	B29C65/00	B29C66/4724		183
B29C66/474	10	{said single elements being substantially non-flat}	B29C65/00	B29C66/474		1790
B29C66/4742	11	{said single elements being spouts}	B29C65/00	B29C66/4742		38
B29C66/47421	12	{said spouts comprising flanges}	B29C65/00	B29C66/47421		173
B29C66/49	9	{Internally supporting the, e.g. tubular, article during joining (B29C66/63 takes precedence)}	B29C65/00	B29C66/49		1661
B29C66/492	10	{using a fluid}	B29C65/00	B29C66/492		18
B29C66/494	10	{using an inflatable core}	B29C65/00	B29C66/494		37
B29C66/496	10	{using a support which remains in the joined object}	B29C65/00	B29C66/496		163
B29C66/50	8	{General aspects of joining tubular articles; General aspects of joining long products, i.e. bars or profiled elements; General aspects of joining single elements to tubular articles, hollow articles or bars; General aspects of joining several hollow-preforms to form hollow or tubular articles}<br><br><u>WARNING</u><br> Group B29C66/50 and subgroups are not complete, pending a reorganisation; see also B29C65/00 and its subgroups 	B29C65/00	B29C66/50		140
B29C66/51	9	{Joining tubular articles, profiled elements or bars; Joining single elements to tubular articles, hollow articles or bars; Joining several hollow-preforms to form hollow or tubular articles}	B29C65/00	B29C66/51		56
B29C66/52	10	{Joining tubular articles, bars or profiled elements}	B29C65/00	B29C66/52		47
B29C66/522	11	{Joining tubular articles (B29C66/53241 takes precedence)}	B29C65/00	B29C66/522		667
B29C66/5221	12	{for forming coaxial connections, i.e. the tubular articles to be joined forming a zero angle relative to each other}	B29C65/00	B29C66/5221		4503
B29C66/52211	13	{for making endless tubular articles, e.g. endless inner tubes}	B29C65/00	B29C66/52211		162
B29C66/5223	12	{for forming corner connections or elbows, e.g. for making V-shaped pieces}	B29C65/00	B29C66/5223		215
B29C66/52231	13	{with a right angle, e.g. for making L-shaped pieces}	B29C65/00	B29C66/52231		319
B29C66/5224	12	{for forming fork-shaped connections, e.g. for making Y-shaped pieces}	B29C65/00	B29C66/5224		192
B29C66/52241	13	{with two right angles, e.g. for making T-shaped pieces}	B29C65/00	B29C66/52241		838
B29C66/5225	12	{for forming cross-shaped connections, e.g. for making X-shaped pieces}	B29C65/00	B29C66/5225		29
B29C66/52251	13	{with four right angles, e.g. for making +-shaped pieces}	B29C65/00	B29C66/52251		76
B29C66/5227	12	{for forming multi-tubular articles by longitudinally joining elementary tubular articles wall-to-wall (e.g. joining the wall of a first tubular article to the wall of a second tubular article) or for forming multilayer tubular articles}	B29C65/00	B29C66/5227		233
B29C66/52271	13	{one tubular article being placed inside the other}	B29C65/00	B29C66/52271		33
B29C66/52272	14	{concentrically, e.g. for forming multilayer tubular articles}	B29C65/00	B29C66/52272		212
B29C66/5229	12	{involving the use of a socket}	B29C65/00	B29C66/5229		1383
B29C66/52291	13	{said socket comprising a stop}	B29C65/00	B29C66/52291		170
B29C66/52292	14	{said stop being internal}	B29C65/00	B29C66/52292		1058
B29C66/52293	14	{said stop being external}	B29C65/00	B29C66/52293		189
B29C66/52294	14	{said stop being heated}	B29C65/00	B29C66/52294		66
B29C66/52295	13	{said socket comprising reinforcements}	B29C65/00	B29C66/52295		98
B29C66/52296	13	{said socket comprising sealing elements, e.g. gaskets}	B29C65/00	B29C66/52296		230
B29C66/52297	13	{said socket comprising slip-off prevention means (B29C66/52296 takes precedence)}	B29C65/00	B29C66/52297		202
B29C66/52298	13	{said socket being composed by several elements}	B29C65/00	B29C66/52298		553
B29C66/524	11	{Joining profiled elements}	B29C65/00	B29C66/524		542
B29C66/5241	12	{for forming coaxial connections, i.e. the profiled elements to be joined forming a zero angle relative to each other}	B29C65/00	B29C66/5241		372
B29C66/5243	12	{for forming corner connections, e.g. for making window frames or V-shaped pieces (welded corner joints for window frames E06B3/9604)}	B29C65/00	B29C66/5243		118
B29C66/52431	13	{with a right angle, e.g. for making L-shaped pieces}	B29C65/00	B29C66/52431		620
B29C66/5244	12	{for forming fork-shaped connections, e.g. for making window frames or Y-shaped pieces}	B29C65/00	B29C66/5244		19
B29C66/52441	13	{with two right angles, e.g. for making T-shaped pieces}	B29C65/00	B29C66/52441		116
B29C66/5245	12	{for forming cross-shaped connections, e.g. for making window frames or X-shaped pieces}	B29C65/00	B29C66/5245		10
B29C66/52451	13	{with four right angles, e.g. for making +-shaped pieces}	B29C65/00	B29C66/52451		33
B29C66/526	11	{Joining bars}	B29C65/00	B29C66/526		173
B29C66/5261	12	{for forming coaxial connections, i.e. the bars to be joined forming a zero angle relative to each other}	B29C65/00	B29C66/5261		209
B29C66/5263	12	{for forming corner connections, e.g. for making V-shaped pieces}	B29C65/00	B29C66/5263		6
B29C66/52631	13	{with a right angle, e.g. for making L-shaped pieces}	B29C65/00	B29C66/52631		15
B29C66/5264	12	{for forming fork-shaped connections, e.g. for making Y-shaped pieces}	B29C65/00	B29C66/5264		11
B29C66/52641	13	{with two right angles, e.g. for making T-shaped pieces}	B29C65/00	B29C66/52641		15
B29C66/5265	12	{for forming cross-shaped connections, e.g. for making X-shaped pieces}	B29C65/00	B29C66/5265		11
B29C66/52651	13	{with four right angles, e.g. for making +-shaped pieces}	B29C65/00	B29C66/52651		8
B29C66/5268	12	{characterised by their solid cross sections being non-circular, e.g. being elliptical, square or rectangular}	B29C65/00	B29C66/5268		63
B29C66/53	10	{Joining single elements to tubular articles, hollow articles or bars}	B29C65/00	B29C66/53		152
B29C66/532	11	{Joining single elements to the wall of tubular articles, hollow articles or bars}	B29C65/00	B29C66/532		1315
B29C66/5324	12	{said single elements being substantially annular, i.e. of finite length (B29C66/5326 takes precedence)}	B29C65/00	B29C66/5324		121
B29C66/53241	13	{said articles being tubular and said substantially annular single elements being of finite length relative to the infinite length of said tubular articles (making T-shaped pieces by joining tubular articles B29C66/52241)}	B29C65/00	B29C66/53241		333
B29C66/53242	14	{said single elements being spouts, e.g. joining spouts to tubes}	B29C65/00	B29C66/53242		28
B29C66/53243	15	{said spouts comprising flanges}	B29C65/00	B29C66/53243		57
B29C66/53245	13	{said articles being hollow}	B29C65/00	B29C66/53245		202
B29C66/53246	14	{said single elements being spouts, e.g. joining spouts to containers}	B29C65/00	B29C66/53246		88
B29C66/53247	15	{said spouts comprising flanges}	B29C65/00	B29C66/53247		378
B29C66/5326	12	{said single elements being substantially flat}	B29C65/00	B29C66/5326		1099
B29C66/53261	13	{Enclosing tubular articles between substantially flat elements}	B29C65/00	B29C66/53261		43
B29C66/53262	14	{Enclosing spouts between the walls of bags, e.g. of medical bags}	B29C65/00	B29C66/53262		340
B29C66/53263	15	{said spouts comprising wings, e.g. said spouts being of ship-like or canoe-like form to avoid leaks in the corners}	B29C65/00	B29C66/53263		159
B29C66/534	11	{Joining single elements to open ends of tubular or hollow articles or to the ends of bars}	B29C65/00	B29C66/534		789
B29C66/5342	12	{a substantially flat extra element being placed between and clamped by the joined single elements and the end of said tubular or hollow articles}	B29C65/00	B29C66/5342		26
B29C66/53421	13	{said substantially flat extra element being flexible, e.g. a membrane (B29C66/53425 takes precedence)}	B29C65/00	B29C66/53421		44
B29C66/53423	13	{said substantially flat extra element being rigid, e.g. a plate (B29C66/53425 takes precedence)}	B29C65/00	B29C66/53423		17
B29C66/53425	13	{said substantially flat extra element being perforated, e.g. a screen}	B29C65/00	B29C66/53425		13
B29C66/5344	12	{said single elements being substantially annular, i.e. of finite length, e.g. joining flanges to tube ends (B29C66/5346 takes precedence)}	B29C65/00	B29C66/5344		2093
B29C66/5346	12	{said single elements being substantially flat}	B29C65/00	B29C66/5346		747
B29C66/53461	13	{joining substantially flat covers and/or substantially flat bottoms to open ends of container bodies}	B29C65/00	B29C66/53461		2216
B29C66/53462	14	{joining substantially flat covers and substantially flat bottoms to open ends of container bodies}	B29C65/00	B29C66/53462		166
B29C66/53465	13	{said single flat elements being provided with holes facing the tube ends, e.g. for making heat-exchangers}	B29C65/00	B29C66/53465		131
B29C66/536	11	{Joining substantially flat single elements to hollow articles to form tubular articles}	B29C65/00	B29C66/536		44
B29C66/54	10	{Joining several hollow-preforms, e.g. half-shells, to form hollow articles, e.g. for making balls, containers; Joining several hollow-preforms, e.g. half-cylinders, to form tubular articles}	B29C65/00	B29C66/54		3706
B29C66/541	11	{a substantially flat extra element being placed between and clamped by the joined hollow-preforms}	B29C65/00	B29C66/541		34
B29C66/5412	12	{said substantially flat extra element being flexible, e.g. a membrane (B29C66/5416 takes precedence)}	B29C65/00	B29C66/5412		144
B29C66/5414	12	{said substantially flat extra element being rigid, e.g. a plate (B29C66/5416 takes precedence)}	B29C65/00	B29C66/5414		114
B29C66/5416	12	{said substantially flat extra element being perforated, e.g. a screen}	B29C65/00	B29C66/5416		48
B29C66/542	11	{joining hollow covers or hollow bottoms to open ends of container bodies}	B29C65/00	B29C66/542		2147
B29C66/543	11	{joining more than two hollow-preforms to form said hollow articles}	B29C65/00	B29C66/543		1020
B29C66/5432	12	{joining hollow covers and hollow bottoms to open ends of container bodies}	B29C65/00	B29C66/5432		272
B29C66/545	11	{one hollow-preform being placed inside the other}	B29C65/00	B29C66/545		1142
B29C66/5452	12	{joining hollow bottoms to bottom of bottles}	B29C65/00	B29C66/5452		60
B29C66/547	11	{Joining several hollow-preforms, e.g. half-cylinders, to form tubular articles, e.g. endless tubes}	B29C65/00	B29C66/547		376
B29C66/5472	12	{for making elbows or V-shaped pieces}	B29C65/00	B29C66/5472		59
B29C66/54721	13	{for making L-shaped pieces}	B29C65/00	B29C66/54721		45
B29C66/5474	12	{for making fork-shaped pieces, i.e. with 3 branches, e.g. Y-shaped pieces}	B29C65/00	B29C66/5474		34
B29C66/54741	13	{for making T-shaped pieces}	B29C65/00	B29C66/54741		25
B29C66/5476	12	{for making cross-shaped pieces, e.g. with 4 branches, e.g. X-shaped pieces}	B29C65/00	B29C66/5476		3
B29C66/54761	13	{for making +-shaped pieces}	B29C65/00	B29C66/54761		4
B29C66/549	11	{said hollow-preforms being interconnected during their moulding process, e.g. by a hinge}	B29C65/00	B29C66/549		172
B29C66/55	10	{sealing elements being incorporated into the joints, e.g. gaskets (B29C66/52296 takes precedence)}	B29C65/00	B29C66/55		303
B29C66/61	9	{Joining from or joining on the inside (for making tubes by bending sheets and joining from the inside B29C53/387)}	B29C65/00	B29C66/61		1577
B29C66/612	10	{Making circumferential joints}	B29C65/00	B29C66/612		1308
B29C66/63	9	{Internally supporting the article during joining (B29C66/49 takes precedence)}	B29C65/00	B29C66/63		1031
B29C66/632	10	{using a fluid}	B29C65/00	B29C66/632		102
B29C66/634	10	{using an inflatable core}	B29C65/00	B29C66/634		163
B29C66/636	10	{using a support which remains in the joined object}	B29C65/00	B29C66/636		611
B29C66/65	9	{with a relative motion between the article and the welding tool (B29C65/10, B29C65/12 take precedence)}	B29C65/00	B29C66/65		420
B29C66/652	10	{moving the welding tool around the fixed article}	B29C65/00	B29C66/652		336
B29C66/69	8	{General aspects of joining&#160;filaments&#160; (bundling&#160;articles&#160; B65B13/00; interconnecting&#160;successive&#160;lengths&#160;of&#160;material B65H69/00)}	B29C65/00	B29C66/69		851
B29C66/70	8	{characterised by the composition, physical properties or the structure of the material of the parts to be joined; Joining with non-plastics material (chemical aspects C08J5/12, C09J)}	B29C65/00	B29C66/70		55
B29C66/71	9	{characterised by the composition of the plastics material of the parts to be joined (welding bar compositions B29C65/125)}	B29C65/00	B29C66/71		21255
B29C66/712	10	{the composition of one of the parts to be joined being different from the composition of the other part}	B29C65/00	B29C66/712		1636
B29C66/72	9	{characterised by the structure of the material of the parts to be joined}	B29C65/00	B29C66/72		126
B29C66/721	10	{Fibre-reinforced materials (B29C66/729 takes precedence)}	B29C65/00	B29C66/721		2777
B29C66/7212	11	{characterised by the composition of the fibres}	B29C65/00	B29C66/7212		3030
B29C66/7214	11	{characterised by the length of the fibres}	B29C65/00	B29C66/7214		9
B29C66/72141	12	{Fibres of continuous length}	B29C65/00	B29C66/72141		1311
B29C66/72143	12	{Fibres of discontinuous lengths}	B29C65/00	B29C66/72143		523
B29C66/723	10	{being multi-layered (B29C66/7292, B29C66/72941 take precedence)}	B29C65/00	B29C66/723		3248
B29C66/7232	11	{comprising a non-plastics layer}	B29C65/00	B29C66/7232		25
B29C66/72321	12	{consisting of metals or their alloys}	B29C65/00	B29C66/72321		2553
B29C66/72322	12	{consisting of elements other than metals, e.g. boron}	B29C65/00	B29C66/72322		2
B29C66/72323	13	{Carbon}	B29C65/00	B29C66/72323		32
B29C66/72324	12	{consisting of inorganic materials not provided for in B29C66/72321&#160;-&#160;B29C66/72322}	B29C65/00	B29C66/72324		6
B29C66/72325	13	{Ceramics}	B29C65/00	B29C66/72325		117
B29C66/72326	13	{Glass}	B29C65/00	B29C66/72326		129
B29C66/72327	12	{consisting of natural products or their composites, not provided for in B29C66/72321&#160;-&#160;B29C66/72324}	B29C65/00	B29C66/72327		68
B29C66/72328	13	{Paper}	B29C65/00	B29C66/72328		1453
B29C66/72329	13	{Wood}	B29C65/00	B29C66/72329		72
B29C66/7234	11	{comprising a barrier layer}	B29C65/00	B29C66/7234		774
B29C66/72341	12	{for gases}	B29C65/00	B29C66/72341		629
B29C66/72343	12	{for liquids}	B29C65/00	B29C66/72343		531
B29C66/725	10	{being hollow-walled or honeycombs}	B29C65/00	B29C66/725		14
B29C66/7252	11	{hollow-walled}	B29C65/00	B29C66/7252		99
B29C66/72521	12	{comprising corrugated cores}	B29C65/00	B29C66/72521		42
B29C66/72523	12	{multi-channelled or multi-tubular (B29C66/438, B29C66/5227 take precedence)}	B29C65/00	B29C66/72523		392
B29C66/72525	12	{comprising honeycomb cores}	B29C65/00	B29C66/72525		194
B29C66/7254	11	{honeycomb structures}	B29C65/00	B29C66/7254		189
B29C66/727	10	{being porous, e.g. foam}	B29C65/00	B29C66/727		2142
B29C66/729	10	{Textile or other fibrous material made from plastics}	B29C65/00	B29C66/729		2218
B29C66/7292	11	{coated (B29C66/72941 takes precedence)}	B29C65/00	B29C66/7292		433
B29C66/7294	11	{Non woven mats, e.g. felt}	B29C65/00	B29C66/7294		1016
B29C66/72941	12	{coated}	B29C65/00	B29C66/72941		149
B29C66/73	9	{characterised by the intensive physical properties of the material of the parts to be joined, by the optical properties of the material of the parts to be joined, by the extensive physical properties of the parts to be joined, by the state of the material of the parts to be joined or by the material of the parts to be joined being a thermoplastic or a thermoset}	B29C65/00	B29C66/73		49
B29C66/731	10	{characterised by the intensive physical properties of the material of the parts to be joined}	B29C65/00	B29C66/731		101
B29C66/7311	11	{Thermal properties}	B29C65/00	B29C66/7311		54
B29C66/73111	12	{Thermal expansion coefficient}	B29C65/00	B29C66/73111		76
B29C66/73112	13	{of different thermal expansion coefficient, i.e. the thermal expansion coefficient of one of the parts to be joined being different from the thermal expansion coefficient of the other part}	B29C65/00	B29C66/73112		134
B29C66/73113	12	{Thermal conductivity}	B29C65/00	B29C66/73113		66
B29C66/73114	13	{of different thermal conductivity, i.e. the thermal conductivity of one of the parts to be joined being different from the thermal conductivity of the other part}	B29C65/00	B29C66/73114		15
B29C66/73115	12	{Melting point}	B29C65/00	B29C66/73115		423
B29C66/73116	13	{of different melting point, i.e. the melting point of one of the parts to be joined being different from the melting point of the other part}	B29C65/00	B29C66/73116		383
B29C66/73117	12	{Tg, i.e. glass transition temperature}	B29C65/00	B29C66/73117		253
B29C66/73118	13	{of different glass transition temperature, i.e. the glass transition temperature of one of the parts to be joined being different from the glass transition temperature of the other part}	B29C65/00	B29C66/73118		41
B29C66/7312	11	{Rheological properties}	B29C65/00	B29C66/7312		3
B29C66/73121	12	{Viscosity}	B29C65/00	B29C66/73121		61
B29C66/73122	13	{of different viscosity, i.e. the viscosity of one of the parts to be joined being different from the viscosity of the other part}	B29C65/00	B29C66/73122		18
B29C66/7313	11	{Density}	B29C65/00	B29C66/7313		63
B29C66/73132	12	{of different density, i.e. the density of one of the parts to be joined being different from the density of the other part}	B29C65/00	B29C66/73132		55
B29C66/7314	11	{Electrical and dielectric properties}	B29C65/00	B29C66/7314		16
B29C66/73141	12	{Electrical conductivity}	B29C65/00	B29C66/73141		71
B29C66/73143	12	{Dielectric properties}	B29C65/00	B29C66/73143		159
B29C66/7315	11	{Mechanical properties}	B29C65/00	B29C66/7315		169
B29C66/73151	12	{Hardness}	B29C65/00	B29C66/73151		108
B29C66/73152	13	{of different hardness, i.e. the hardness of one of the parts to be joined being different from the hardness of the other part}	B29C65/00	B29C66/73152		130
B29C66/7316	11	{Surface properties}	B29C65/00	B29C66/7316		11
B29C66/73161	12	{Roughness or rugosity}	B29C65/00	B29C66/73161		620
B29C66/73162	13	{of different roughness or rugosity, i.e. the roughness or rugosity of the surface of one of the parts to be joined being different from the roughness or rugosity of the surface of the other part}	B29C65/00	B29C66/73162		31
B29C66/7317	11	{Hydrophilicity or hydrophobicity}	B29C65/00	B29C66/7317		4
B29C66/73171	12	{Hydrophilicity}	B29C65/00	B29C66/73171		21
B29C66/73172	13	{of different hydrophilicity, i.e. the hydrophilicity of one of the parts to be joined being different from the hydrophilicity of the other part}	B29C65/00	B29C66/73172		3
B29C66/73175	12	{Hydrophobicity}	B29C65/00	B29C66/73175		24
B29C66/73176	13	{of different hydrophobicity, i.e. the hydrophobicity of one of the parts to be joined being different from the hydrophobicity of the other part}	B29C65/00	B29C66/73176		1
B29C66/7318	11	{Permeability to gases or liquids}	B29C65/00	B29C66/7318		
B29C66/73181	12	{permeable}	B29C65/00	B29C66/73181		1
B29C66/73182	13	{to gases}	B29C65/00	B29C66/73182		33
B29C66/73183	13	{to liquids}	B29C65/00	B29C66/73183		13
B29C66/73185	12	{non-permeable}	B29C65/00	B29C66/73185		12
B29C66/73186	13	{to gases}	B29C65/00	B29C66/73186		23
B29C66/73187	13	{to liquids}	B29C65/00	B29C66/73187		88
B29C66/733	10	{characterised by the optical properties of the material of the parts to be joined, e.g. fluorescence, phosphorescence}	B29C65/00	B29C66/733		43
B29C66/7332	11	{at least one of the parts to be joined being coloured}	B29C65/00	B29C66/7332		170
B29C66/73321	12	{both parts to be joined being coloured}	B29C65/00	B29C66/73321		69
B29C66/73322	13	{both parts to be joined having a different colour}	B29C65/00	B29C66/73322		63
B29C66/7334	11	{at least one of the parts to be joined being glossy or matt, reflective or refractive}	B29C65/00	B29C66/7334		1
B29C66/73341	12	{at least one of the parts to be joined being glossy or reflective}	B29C65/00	B29C66/73341		49
B29C66/73343	12	{at least one of the parts to be joined being matt or refractive}	B29C65/00	B29C66/73343		35
B29C66/7336	11	{at least one of the parts to be joined being opaque, transparent or translucent to visible light}	B29C65/00	B29C66/7336		6
B29C66/73361	12	{at least one of the parts to be joined being opaque to visible light}	B29C65/00	B29C66/73361		90
B29C66/73362	13	{both parts to be joined being opaque to visible light}	B29C65/00	B29C66/73362		25
B29C66/73365	12	{at least one of the parts to be joined being transparent or translucent to visible light}	B29C65/00	B29C66/73365		263
B29C66/73366	13	{both parts to be joined being transparent or translucent to visible light}	B29C65/00	B29C66/73366		148
B29C66/7338	11	{at least one of the parts to be joined being polarising}	B29C65/00	B29C66/7338		40
B29C66/735	10	{characterised by the extensive physical properties of the parts to be joined}	B29C65/00	B29C66/735		51
B29C66/7352	11	{Thickness, e.g. very thin}	B29C65/00	B29C66/7352		692
B29C66/73521	12	{of different thickness, i.e. the thickness of one of the parts to be joined being different from the thickness of the other part}	B29C65/00	B29C66/73521		279
B29C66/737	10	{characterised by the state of the material of the parts to be joined}	B29C65/00	B29C66/737		20
B29C66/7371	11	{oriented or heat-shrinkable}	B29C65/00	B29C66/7371		128
B29C66/73711	12	{oriented}	B29C65/00	B29C66/73711		413
B29C66/73712	13	{mono-axially}	B29C65/00	B29C66/73712		154
B29C66/73713	13	{bi-axially or multi-axially}	B29C65/00	B29C66/73713		265
B29C66/73715	12	{heat-shrinkable}	B29C65/00	B29C66/73715		723
B29C66/7373	11	{Joining soiled or oxidised materials}	B29C65/00	B29C66/7373		461
B29C66/7375	11	{uncured, partially cured or fully cured}	B29C65/00	B29C66/7375		88
B29C66/73751	12	{the to-be-joined area of at least one of the parts to be joined being uncured, i.e. non cross-linked, non vulcanized}	B29C65/00	B29C66/73751		296
B29C66/73752	13	{the to-be-joined areas of both parts to be joined being uncured}	B29C65/00	B29C66/73752		433
B29C66/73753	12	{the to-be-joined area of at least one of the parts to be joined being partially cured, i.e. partially cross-linked, partially vulcanized}	B29C65/00	B29C66/73753		135
B29C66/73754	13	{the to-be-joined areas of both parts to be joined being partially cured}	B29C65/00	B29C66/73754		170
B29C66/73755	12	{the to-be-joined area of at least one of the parts to be joined being fully cured, i.e. fully cross-linked, fully vulcanized}	B29C65/00	B29C66/73755		251
B29C66/73756	13	{the to-be-joined areas of both parts to be joined being fully cured}	B29C65/00	B29C66/73756		259
B29C66/7377	11	{amorphous, semi-crystalline or crystalline}	B29C65/00	B29C66/7377		11
B29C66/73771	12	{the to-be-joined area of at least one of the parts to be joined being amorphous}	B29C65/00	B29C66/73771		156
B29C66/73772	13	{the to-be-joined areas of both parts to be joined being amorphous}	B29C65/00	B29C66/73772		175
B29C66/73773	12	{the to-be-joined area of at least one of the parts to be joined being semi-crystalline}	B29C65/00	B29C66/73773		123
B29C66/73774	13	{the to-be-joined areas of both parts to be joined being semi-crystalline}	B29C65/00	B29C66/73774		185
B29C66/73775	12	{the to-be-joined area of at least one of the parts to be joined being crystalline}	B29C65/00	B29C66/73775		82
B29C66/73776	13	{the to-be-joined areas of both parts to be joined being crystalline}	B29C65/00	B29C66/73776		161
B29C66/7379	11	{degradable}	B29C65/00	B29C66/7379		15
B29C66/73791	12	{biodegradable}	B29C65/00	B29C66/73791		81
B29C66/73793	12	{soluble, e.g. water-soluble}	B29C65/00	B29C66/73793		106
B29C66/739	10	{characterised by the material of the parts to be joined being a thermoplastic or a thermoset}	B29C65/00	B29C66/739		16
B29C66/7392	11	{characterised by the material of at least one of the parts being a thermoplastic}	B29C65/00	B29C66/7392		3676
B29C66/73921	12	{characterised by the materials of both parts being thermoplastics}	B29C65/00	B29C66/73921		11120
B29C66/7394	11	{characterised by the material of at least one of the parts being a thermoset}	B29C65/00	B29C66/7394		1267
B29C66/73941	12	{characterised by the materials of both parts being thermosets}	B29C65/00	B29C66/73941		940
B29C66/74	9	{Joining plastics material to non-plastics material}<br><br><u>NOTE</u><br><br> When classifying in this group, joining techniques are additionally classified in the relevant groups, i.e. in B29C65/44 and subgroups or in B29C65/64 and subgroups 	B29C65/00	B29C66/74		258
B29C66/742	10	{to metals or their alloys}	B29C65/00	B29C66/742		2878
B29C66/7422	11	{Aluminium or alloys of aluminium}	B29C65/00	B29C66/7422		779
B29C66/7424	11	{Lead or alloys of lead}	B29C65/00	B29C66/7424		8
B29C66/7426	11	{Tin or alloys of tin}	B29C65/00	B29C66/7426		19
B29C66/7428	11	{Transition metals or their alloys}	B29C65/00	B29C66/7428		90
B29C66/74281	12	{Copper or alloys of copper}	B29C65/00	B29C66/74281		204
B29C66/74283	12	{Iron or alloys of iron, e.g. steel}	B29C65/00	B29C66/74283		613
B29C66/74285	12	{Noble metals, e.g. silver, gold, platinum or their alloys}	B29C65/00	B29C66/74285		30
B29C66/744	10	{to elements other than metals}	B29C65/00	B29C66/744		22
B29C66/7442	11	{Boron}	B29C65/00	B29C66/7442		2
B29C66/7444	11	{Carbon}	B29C65/00	B29C66/7444		45
B29C66/746	10	{to inorganic materials not provided for in groups B29C66/742&#160;-&#160;B29C66/744}	B29C65/00	B29C66/746		30
B29C66/7461	11	{Ceramics}	B29C65/00	B29C66/7461		162
B29C66/74611	12	{Carbides; Nitrides}	B29C65/00	B29C66/74611		12
B29C66/7463	11	{Concrete}	B29C65/00	B29C66/7463		28
B29C66/7465	11	{Glass}	B29C65/00	B29C66/7465		442
B29C66/7467	11	{Mica}	B29C65/00	B29C66/7467		3
B29C66/7469	11	{Asbestos}	B29C65/00	B29C66/7469		1
B29C66/748	10	{to natural products or their composites, not provided for in groups B29C66/742&#160;-&#160;B29C66/746}	B29C65/00	B29C66/748		35
B29C66/7481	11	{Cork}	B29C65/00	B29C66/7481		3
B29C66/7482	11	{Linoleum}	B29C65/00	B29C66/7482		1
B29C66/7483	11	{Bone, horn, ivory}	B29C65/00	B29C66/7483		8
B29C66/7484	11	{Leather}	B29C65/00	B29C66/7484		56
B29C66/7485	11	{Natural fibres, e.g. wool, cotton}	B29C65/00	B29C66/7485		119
B29C66/7486	11	{Paper, e.g. cardboard}	B29C65/00	B29C66/7486		261
B29C66/7487	11	{Wood}	B29C65/00	B29C66/7487		195
B29C66/80	8	{General aspects of machine operations or constructions and parts thereof}	B29C65/00	B29C66/80		4700
B29C66/81	9	{General aspects of the pressing elements, i.e. the elements applying pressure on the parts to be joined in the area to be joined, e.g. the welding jaws or clamps (holding or clamping means for handling purposes B29C65/7841)}	B29C65/00	B29C66/81		273
B29C66/812	10	{characterised by the composition, by the structure, by the intensive physical properties or by the optical properties of the material constituting the pressing elements, e.g. constituting the welding jaws or clamps}	B29C65/00	B29C66/812		10
B29C66/8122	11	{characterised by the composition of the material constituting the pressing elements, e.g. constituting the welding jaws or clamps}	B29C65/00	B29C66/8122		2525
B29C66/8124	11	{characterised by the structure of the material constituting the pressing elements, e.g. constituting the welding jaws or clamps}	B29C65/00	B29C66/8124		29
B29C66/81241	12	{being porous or sintered}	B29C65/00	B29C66/81241		228
B29C66/8126	11	{characterised by the intensive physical properties or by the optical properties of the material constituting the pressing elements, e.g. constituting the welding jaws or clamps}	B29C65/00	B29C66/8126		66
B29C66/81261	12	{Thermal properties, e.g. thermal conductivity, thermal expansion coefficient}	B29C65/00	B29C66/81261		489
B29C66/81262	12	{Electrical and dielectric properties, e.g. electrical conductivity}	B29C65/00	B29C66/81262		159
B29C66/81263	13	{Dielectric properties}	B29C65/00	B29C66/81263		200
B29C66/81264	12	{Mechanical properties, e.g. hardness}	B29C65/00	B29C66/81264		257
B29C66/81265	12	{Surface properties, e.g. surface roughness or rugosity}	B29C65/00	B29C66/81265		151
B29C66/81266	12	{Optical properties, e.g. transparency, reflectivity}	B29C65/00	B29C66/81266		21
B29C66/81267	13	{Transparent to electromagnetic radiation, e.g. to visible light}	B29C65/00	B29C66/81267		587
B29C66/81268	13	{Reflective to electromagnetic radiation, e.g. to visible light}	B29C65/00	B29C66/81268		48
B29C66/814	10	{characterised by the design of the pressing elements, e.g. of the welding jaws or clamps}	B29C65/00	B29C66/814		59
B29C66/8141	11	{characterised by the surface geometry of the part of the pressing elements, e.g. welding jaws or clamps, coming into contact with the parts to be joined}	B29C65/00	B29C66/8141		40
B29C66/81411	12	{characterised by its cross-section, e.g. transversal or longitudinal, being non-flat}	B29C65/00	B29C66/81411		36
B29C66/81413	13	{being non-symmetrical (B29C66/81415 takes precedence)}	B29C65/00	B29C66/81413		136
B29C66/81415	13	{being bevelled}	B29C65/00	B29C66/81415		415
B29C66/81417	14	{being V-shaped}	B29C65/00	B29C66/81417		870
B29C66/81419	14	{and flat}	B29C65/00	B29C66/81419		835
B29C66/81421	13	{being convex or concave}	B29C65/00	B29C66/81421		31
B29C66/81422	14	{being convex}	B29C65/00	B29C66/81422		1360
B29C66/81423	14	{being concave}	B29C65/00	B29C66/81423		1552
B29C66/81425	13	{being stepped, e.g. comprising a shoulder}	B29C65/00	B29C66/81425		390
B29C66/81427	12	{comprising a single ridge, e.g. for making a weakening line; comprising a single tooth}	B29C65/00	B29C66/81427		2413
B29C66/81429	13	{comprising a single tooth}	B29C65/00	B29C66/81429		796
B29C66/81431	12	{comprising a single cavity, e.g. a groove}	B29C65/00	B29C66/81431		2612
B29C66/81433	12	{being toothed, i.e. comprising several teeth or pins (comprising a single tooth B29C66/81429), or being patterned}	B29C65/00	B29C66/81433		1399
B29C66/81435	13	{comprising several parallel ridges, e.g. for crimping (comprising a single ridge B29C66/81427)}	B29C65/00	B29C66/81435		719
B29C66/8145	11	{characterised by the constructional aspects of the pressing elements, e.g. of the welding jaws or clamps (B29C66/816 and B29C66/818 take precedence; adaptable for making articles or joints of different dimensions B29C66/841)}	B29C65/00	B29C66/8145		324
B29C66/81451	12	{being adaptable to the surface of the joint (B29C66/81453, B29C66/81455, B29C66/81457, B29C66/81459, B29C66/81461 take precedence)}	B29C65/00	B29C66/81451		73
B29C66/81453	12	{being made of flexible slats, flexible fins, flexible bristles or springs, e.g. coiled springs}	B29C65/00	B29C66/81453		75
B29C66/81455	12	{being a fluid inflatable bag or bladder, a diaphragm or a vacuum bag for applying isostatic pressure (inflatable element positioned between the joining tool and a backing-up part B29C66/82421)}	B29C65/00	B29C66/81455		597
B29C66/81457	12	{comprising a block or layer of deformable material, e.g. sponge, foam, rubber (pressing elements supported or backed-up by resilient material B29C66/8161)}	B29C65/00	B29C66/81457		1254
B29C66/81459	12	{being a filled deformable bladder, e.g. bladder filled with oil, with granules or with a meltable solid material (B29C66/81455 takes precedence)}	B29C65/00	B29C66/81459		42
B29C66/81461	12	{being multi-lamellar or segmented, i.e. comprising a plurality of strips, plates or stacked elements}	B29C65/00	B29C66/81461		205
B29C66/81463	12	{comprising a plurality of single pressing elements, e.g. a plurality of sonotrodes, or comprising a plurality of single counter-pressing elements, e.g. a plurality of anvils, said plurality of said single elements being suitable for making a single joint}	B29C65/00	B29C66/81463		737
B29C66/81465	13	{one placed behind the other in a single row in the feed direction}	B29C65/00	B29C66/81465		577
B29C66/81467	13	{arranged in an offset pattern}	B29C65/00	B29C66/81467		53
B29C66/81469	13	{one placed next to the other in a single line transverse to the feed direction, e.g. shoulder to shoulder sonotrodes}	B29C65/00	B29C66/81469		301
B29C66/81471	12	{being a wrap-around tape or band}	B29C65/00	B29C66/81471		114
B29C66/816	10	{characterised by the mounting of the pressing elements, e.g. of the welding jaws or clamps}	B29C65/00	B29C66/816		185
B29C66/8161	11	{said pressing elements being supported or backed-up by springs or by resilient material}	B29C65/00	B29C66/8161		2829
B29C66/81611	12	{by resilient material}	B29C65/00	B29C66/81611		117
B29C66/8163	11	{Self-aligning to the joining plane, e.g. mounted on a ball and socket}	B29C65/00	B29C66/8163		271
B29C66/8165	11	{Carrier plates for mounting joining tool parts, e.g. for re-arranging the tool parts to make other forms}	B29C65/00	B29C66/8165		72
B29C66/8167	11	{Quick change joining tools or surfaces}	B29C65/00	B29C66/8167		2092
B29C66/8169	11	{the mounting of said pressing elements being laterally movable, e.g. adjustable (B29C66/836, B29C66/841, B29C66/863 take precedence)}	B29C65/00	B29C66/8169		128
B29C66/818	10	{characterised by the cooling constructional aspects, or by the thermal or electrical insulating or conducting constructional aspects of the welding jaws or of the clamps (characterised by the heating means B29C65/24); comprising means for compensating for the thermal expansion of the welding jaws or of the clamps}	B29C65/00	B29C66/818		360
B29C66/8181	11	{characterised by the cooling constructional aspects}	B29C65/00	B29C66/8181		952
B29C66/81811	12	{of the welding jaws}	B29C65/00	B29C66/81811		1045
B29C66/81812	13	{the welding jaws being cooled from the outside, e.g. by blowing a gas or spraying a liquid}	B29C65/00	B29C66/81812		290
B29C66/81815	12	{of the clamps}	B29C65/00	B29C66/81815		156
B29C66/8182	11	{characterised by the thermal insulating constructional aspects}	B29C65/00	B29C66/8182		34
B29C66/81821	12	{of the welding jaws}	B29C65/00	B29C66/81821		954
B29C66/81825	12	{of the clamps}	B29C65/00	B29C66/81825		23
B29C66/8183	11	{characterised by the thermal conducting constructional aspects}	B29C65/00	B29C66/8183		8
B29C66/81831	12	{of the welding jaws}	B29C65/00	B29C66/81831		144
B29C66/81835	12	{of the clamps}	B29C65/00	B29C66/81835		5
B29C66/8185	11	{comprising means for compensating for the thermal expansion of the welding jaws or of the clamps (means for tensioning resistive elements B29C65/229)}	B29C65/00	B29C66/8185		92
B29C66/8187	11	{characterised by the electrical insulating constructional aspects}	B29C65/00	B29C66/8187		18
B29C66/81871	12	{of the welding jaws}	B29C65/00	B29C66/81871		903
B29C66/81875	12	{of the clamps}	B29C65/00	B29C66/81875		16
B29C66/8188	11	{characterised by the electrical conducting constructional aspects}	B29C65/00	B29C66/8188		2
B29C66/81881	12	{of the welding jaws}	B29C65/00	B29C66/81881		40
B29C66/81885	12	{of the clamps}	B29C65/00	B29C66/81885		1
B29C66/82	9	{Pressure application arrangements, e.g. transmission or actuating mechanisms for joining tools or clamps}<br><br><u>WARNING</u><br> Group B29C66/82 and subgroups are not complete, pending a reorganisation; see also B29C65/00 and its subgroups 	B29C65/00	B29C66/82		117
B29C66/822	10	{Transmission mechanisms}	B29C65/00	B29C66/822		67
B29C66/8221	11	{Scissor or lever mechanisms, i.e. involving a pivot point}	B29C65/00	B29C66/8221		2835
B29C66/8222	11	{Pinion or rack mechanisms}	B29C65/00	B29C66/8222		343
B29C66/8223	11	{Worm or spindle mechanisms}	B29C65/00	B29C66/8223		709
B29C66/8224	11	{Chain or sprocket drives}	B29C65/00	B29C66/8224		67
B29C66/8225	11	{Crank mechanisms}	B29C65/00	B29C66/8225		393
B29C66/8226	11	{Cam mechanisms; Wedges; Eccentric mechanisms}	B29C65/00	B29C66/8226		793
B29C66/82261	12	{Wedges}	B29C65/00	B29C66/82261		130
B29C66/82263	12	{Follower pin or roller cooperating with a groove}	B29C65/00	B29C66/82263		346
B29C66/82265	12	{Eccentric mechanisms}	B29C65/00	B29C66/82265		243
B29C66/8227	11	{using springs}	B29C65/00	B29C66/8227		973
B29C66/824	10	{Actuating mechanisms}	B29C65/00	B29C66/824		103
B29C66/8242	11	{Pneumatic or hydraulic drives (using fluid pressure directly acting on the parts to be joined B29C66/8266)}	B29C65/00	B29C66/8242		3964
B29C66/82421	12	{using an inflatable element positioned between the joining tool and a backing-up part}	B29C65/00	B29C66/82421		218
B29C66/82423	12	{using vacuum (using vacuum directly acting on the parts to be joined B29C66/82661)}	B29C65/00	B29C66/82423		56
B29C66/8244	11	{magnetically driven}	B29C65/00	B29C66/8244		330
B29C66/8246	11	{Servomechanisms, e.g. servomotors}	B29C65/00	B29C66/8246		346
B29C66/8248	11	{Pressure application by weights (by the own weight of the joining tool B29C66/8282)}	B29C65/00	B29C66/8248		159
B29C66/826	10	{without using a separate pressure application tool, e.g. the own weight of the parts to be joined (B29C65/66 takes precedence)}	B29C65/00	B29C66/826		36
B29C66/8262	11	{using "pressure means" which are associated with at least one of the parts to be joined and remain in or on it}	B29C65/00	B29C66/8262		65
B29C66/8264	11	{using the thermal expansion of the parts to be joined}	B29C65/00	B29C66/8264		88
B29C66/8266	11	{using fluid pressure directly acting on the parts to be joined}	B29C65/00	B29C66/8266		252
B29C66/82661	12	{by means of vacuum}	B29C65/00	B29C66/82661		263
B29C66/828	10	{Other pressure application arrangements}	B29C65/00	B29C66/828		65
B29C66/8282	11	{using the own weight of the joining tool}	B29C65/00	B29C66/8282		58
B29C66/8284	11	{using the thermal expansion of the joining tool}	B29C65/00	B29C66/8284		31
B29C66/8286	11	{Hand placed clamps (wrap-around tapes or bands B29C66/81471)}	B29C65/00	B29C66/8286		157
B29C66/83	9	{characterised by the movement of the joining or pressing tools}	B29C65/00	B29C66/83		99
B29C66/832	10	{Reciprocating joining or pressing tools (B29C66/834 takes precedence)}	B29C65/00	B29C66/832		530
B29C66/8322	11	{Joining or pressing tools reciprocating along one axis}	B29C65/00	B29C66/8322		11566
B29C66/83221	12	{cooperating reciprocating tools, each tool reciprocating along one axis}	B29C65/00	B29C66/83221		2844
B29C66/8324	11	{Joining or pressing tools pivoting around one axis (scissor or lever transmission mechanisms B29C66/8221; tools self-aligning to the joining plane B29C66/8163)}	B29C65/00	B29C66/8324		1178
B29C66/83241	12	{cooperating pivoting tools}	B29C65/00	B29C66/83241		411
B29C66/834	10	{moving with the parts to be joined}	B29C65/00	B29C66/834		55
B29C66/8341	11	{Roller, cylinder or drum types; Band or belt types; Ball types (B29C66/8351 takes precedence)}	B29C65/00	B29C66/8341		112
B29C66/83411	12	{Roller, cylinder or drum types (B29C66/83431 takes precedence; rollers, cylinders or drums moving relative to and tangentially to the parts to be joined B29C66/8362)}	B29C65/00	B29C66/83411		1981
B29C66/83413	13	{cooperating rollers, cylinders or drums}	B29C65/00	B29C66/83413		3348
B29C66/83415	13	{the contact angle between said rollers, cylinders or drums and said parts to be joined being a non-zero angle (B29C66/83433 takes precedence)}	B29C65/00	B29C66/83415		763
B29C66/83417	13	{said rollers, cylinders or drums being hollow}	B29C65/00	B29C66/83417		255
B29C66/83421	12	{band or belt types (B29C66/83431 takes precedence)}	B29C65/00	B29C66/83421		329
B29C66/83423	13	{cooperating bands or belts}	B29C65/00	B29C66/83423		432
B29C66/83431	12	{rollers, cylinders or drums cooperating with bands or belts}	B29C65/00	B29C66/83431		128
B29C66/83433	13	{the contact angle between said rollers, cylinders or drums and said bands or belts being a non-zero angle}	B29C65/00	B29C66/83433		188
B29C66/83435	13	{said rollers, cylinders or drums being hollow}	B29C65/00	B29C66/83435		55
B29C66/83441	12	{Ball types}	B29C65/00	B29C66/83441		52
B29C66/8351	11	{Jaws mounted on rollers, cylinders, drums, bands, belts or chains; Flying jaws}	B29C65/00	B29C66/8351		68
B29C66/83511	12	{jaws mounted on rollers, cylinders or drums}	B29C65/00	B29C66/83511		972
B29C66/83513	13	{cooperating jaws mounted on rollers, cylinders or drums and moving in a closed path}	B29C65/00	B29C66/83513		622
B29C66/83517	13	{said rollers, cylinders or drums being hollow}	B29C65/00	B29C66/83517		117
B29C66/83521	12	{jaws mounted on bands or belts}	B29C65/00	B29C66/83521		44
B29C66/83523	13	{Cooperating jaws mounted on cooperating bands or belts and moving in a closed path}	B29C65/00	B29C66/83523		57
B29C66/83531	12	{jaws mounted on chains}	B29C65/00	B29C66/83531		64
B29C66/83533	13	{Cooperating jaws mounted on cooperating chains and moving in a closed path}	B29C65/00	B29C66/83533		162
B29C66/83541	12	{flying jaws, e.g. jaws mounted on crank mechanisms or following a hand over hand movement}	B29C65/00	B29C66/83541		165
B29C66/83543	13	{cooperating flying jaws}	B29C65/00	B29C66/83543		617
B29C66/836	10	{Moving relative to and tangentially to the parts to be joined, e.g. transversely to the displacement of the parts to be joined, e.g. using a X-Y table (B29C66/65 takes precedence)}	B29C65/00	B29C66/836		2388
B29C66/8362	11	{Rollers, cylinders or drums moving relative to and tangentially to the parts to be joined}	B29C65/00	B29C66/8362		1347
B29C66/84	9	{Specific machine types or machines suitable for specific applications}	B29C65/00	B29C66/84		402
B29C66/841	10	{Machines or tools adaptable for making articles of different dimensions or shapes or for making joints of different dimensions}	B29C65/00	B29C66/841		219
B29C66/8412	11	{of different length, width or height}	B29C65/00	B29C66/8412		243
B29C66/84121	12	{of different width}	B29C65/00	B29C66/84121		204
B29C66/84123	12	{of different height}	B29C65/00	B29C66/84123		86
B29C66/8414	11	{of different diameter}	B29C65/00	B29C66/8414		192
B29C66/8416	11	{of different thickness}	B29C65/00	B29C66/8416		111
B29C66/843	10	{Machines for making separate joints at the same time in different planes; Machines for making separate joints at the same time mounted in parallel or in series}	B29C65/00	B29C66/843		517
B29C66/8432	11	{Machines for making separate joints at the same time mounted in parallel or in series}	B29C65/00	B29C66/8432		1187
B29C66/845	10	{C-clamp type or sewing machine type}	B29C65/00	B29C66/845		482
B29C66/847	10	{Drilling standard machine type}	B29C65/00	B29C66/847		155
B29C66/849	10	{Packaging machines}	B29C65/00	B29C66/849		3087
B29C66/8491	11	{welding through a filled container, e.g. tube or bag}	B29C65/00	B29C66/8491		475
B29C66/851	10	{Bag or container making machines}	B29C65/00	B29C66/851		198
B29C66/8511	11	{Bag making machines}	B29C65/00	B29C66/8511		755
B29C66/853	10	{Machines for changing web rolls or filaments, e.g. for joining a replacement web to an expiring web}	B29C65/00	B29C66/853		117
B29C66/855	10	{Belt splicing machines}	B29C65/00	B29C66/855		183
B29C66/857	10	{Medical tube welding machines}	B29C65/00	B29C66/857		347
B29C66/861	10	{Hand-held&#160;tools}	B29C65/00	B29C66/861		1610
B29C66/8612	11	{Ironing tool type}	B29C65/00	B29C66/8612		103
B29C66/8614	11	{Tongs, pincers or scissors}	B29C65/00	B29C66/8614		262
B29C66/8616	11	{Pen or pencil like}	B29C65/00	B29C66/8616		43
B29C66/8618	11	{being battery operated}	B29C65/00	B29C66/8618		309
B29C66/863	10	{Robotised, e.g. mounted on a robot arm}	B29C65/00	B29C66/863		632
B29C66/865	10	{Independently movable welding apparatus, e.g. on wheels}	B29C65/00	B29C66/865		85
B29C66/8652	11	{being pushed by hand or being self-propelling}	B29C65/00	B29C66/8652		128
B29C66/86521	12	{being self-propelling}	B29C65/00	B29C66/86521		185
B29C66/86523	13	{the traction being made on the seam}	B29C65/00	B29C66/86523		75
B29C66/86531	12	{being guided}	B29C65/00	B29C66/86531		21
B29C66/86533	13	{by rails}	B29C65/00	B29C66/86533		111
B29C66/86535	13	{by the edge of one of the parts to be joined or by a groove between the parts to be joined, e.g. using a roller}	B29C65/00	B29C66/86535		74
B29C66/87	9	{Auxiliary operations or devices}	B29C65/00	B29C66/87		740
B29C66/872	10	{Starting or stopping procedures}	B29C65/00	B29C66/872		379
B29C66/874	10	{Safety measures or devices}	B29C65/00	B29C66/874		108
B29C66/8742	11	{for operators (B29C66/002 takes precedence)}	B29C65/00	B29C66/8742		227
B29C66/8744	11	{Preventing overheating of the parts to be joined, e.g. if the machine stops or slows down}	B29C65/00	B29C66/8744		61
B29C66/87441	12	{by lowering or shutting down the power supply}	B29C65/00	B29C66/87441		47
B29C66/87443	12	{by withdrawing the heating tools}	B29C65/00	B29C66/87443		146
B29C66/87445	12	{by introducing protection shields}	B29C65/00	B29C66/87445		44
B29C66/8746	11	{Detecting the absence of the articles to be joined}	B29C65/00	B29C66/8746		143
B29C66/8748	11	{involving the use of warnings}	B29C65/00	B29C66/8748		194
B29C66/876	10	{Maintenance or cleaning}	B29C65/00	B29C66/876		367
B29C66/8762	11	{Cleaning of the joining tools}	B29C65/00	B29C66/8762		206
B29C66/90	8	{Measuring or controlling the joining process}	B29C65/00	B29C66/90		394
B29C66/91	9	{by measuring or controlling the temperature, the heat or the thermal flux}	B29C65/00	B29C66/91		351
B29C66/912	10	{by measuring the temperature, the heat or the thermal flux}	B29C65/00	B29C66/912		17
B29C66/9121	11	{by measuring the temperature}	B29C65/00	B29C66/9121		484
B29C66/91211	12	{with special temperature measurement means or methods}	B29C65/00	B29C66/91211		58
B29C66/91212	13	{involving measurement means being part of the welding jaws, e.g. integrated in the welding jaws}	B29C65/00	B29C66/91212		778
B29C66/91213	14	{and measuring the electrical resistance of a resistive element belonging to said welding jaws, said element being, e.g. a thermistor}	B29C65/00	B29C66/91213		146
B29C66/91214	13	{by measuring the electrical resistance of a resistive element belonging to one of the parts to be welded, said element acting, e.g. as a thermistor}	B29C65/00	B29C66/91214		112
B29C66/91216	13	{enabling contactless temperature measurements, e.g. using a pyrometer}	B29C65/00	B29C66/91216		486
B29C66/91218	13	{using colour change, e.g. using separate colour indicators}	B29C65/00	B29C66/91218		143
B29C66/91221	12	{of the parts to be joined}	B29C65/00	B29C66/91221		901
B29C66/91231	12	{of the joining tool}	B29C65/00	B29C66/91231		1228
B29C66/9131	11	{by measuring the heat or the thermal flux, i.e. the heat flux}	B29C65/00	B29C66/9131		70
B29C66/91311	12	{by measuring the heat generated by Joule heating or induction heating}	B29C65/00	B29C66/91311		58
B29C66/91313	13	{by measuring the voltage, i.e. the electric potential difference or electric tension}	B29C65/00	B29C66/91313		150
B29C66/91315	13	{by measuring the current intensity}	B29C65/00	B29C66/91315		179
B29C66/91317	13	{by measuring the electrical resistance}	B29C65/00	B29C66/91317		161
B29C66/914	10	{by controlling or regulating the temperature, the heat or the thermal flux}	B29C65/00	B29C66/914		32
B29C66/9141	11	{by controlling or regulating the temperature}	B29C65/00	B29C66/9141		785
B29C66/91411	12	{of the parts to be joined, e.g. the joining process taking the temperature of the parts to be joined into account}	B29C65/00	B29C66/91411		1597
B29C66/91413	13	{the parts to be joined having different temperatures}	B29C65/00	B29C66/91413		85
B29C66/91421	12	{of the joining tools}	B29C65/00	B29C66/91421		2122
B29C66/91423	13	{using joining tools having different temperature zones or using several joining tools with different temperatures}	B29C65/00	B29C66/91423		420
B29C66/91431	12	{the temperature being kept constant over time}	B29C65/00	B29C66/91431		1330
B29C66/91441	12	{the temperature being non-constant over time}	B29C65/00	B29C66/91441		45
B29C66/91443	13	{following a temperature-time profile (B29C65/38 takes precedence)}	B29C65/00	B29C66/91443		316
B29C66/91445	14	{by steps}	B29C65/00	B29C66/91445		350
B29C66/9161	11	{by controlling or regulating the heat or the thermal flux, i.e. the heat flux}	B29C65/00	B29C66/9161		595
B29C66/91631	12	{the heat or the thermal flux being kept constant over time}	B29C65/00	B29C66/91631		53
B29C66/91641	12	{the heat or the thermal flux being non-constant over time}	B29C65/00	B29C66/91641		757
B29C66/91643	13	{following a heat-time profile (B29C65/38 takes precedence)}	B29C65/00	B29C66/91643		154
B29C66/91645	14	{by steps}	B29C65/00	B29C66/91645		559
B29C66/91651	12	{by controlling or regulating the heat generated by Joule heating or induction heating}	B29C65/00	B29C66/91651		740
B29C66/91653	13	{by controlling or regulating the voltage, i.e. the electric potential difference or electric tension}	B29C65/00	B29C66/91653		393
B29C66/91655	13	{by controlling or regulating the current intensity}	B29C65/00	B29C66/91655		712
B29C66/919	10	{characterised by specific temperature, heat or thermal flux values or ranges (specific electrical resistance values B29C66/81262)}	B29C65/00	B29C66/919		2481
B29C66/9192	11	{in explicit relation to another variable, e.g. temperature diagrams}	B29C65/00	B29C66/9192		189
B29C66/91921	12	{in explicit relation to another temperature, e.g. to the softening temperature or softening point, to the thermal degradation temperature or to the ambient temperature}	B29C65/00	B29C66/91921		434
B29C66/91931	13	{in explicit relation to the fusion temperature or melting point of the material of one of the parts to be joined}	B29C65/00	B29C66/91931		225
B29C66/91933	14	{higher than said fusion temperature}	B29C65/00	B29C66/91933		321
B29C66/91935	14	{lower than said fusion temperature}	B29C65/00	B29C66/91935		360
B29C66/91941	13	{in explicit relation to Tg, i.e. the glass transition temperature, of the material of one of the parts to be joined}	B29C65/00	B29C66/91941		67
B29C66/91943	14	{higher than said glass transition temperature}	B29C65/00	B29C66/91943		157
B29C66/91945	14	{lower than said glass transition temperature}	B29C65/00	B29C66/91945		90
B29C66/91951	12	{in explicit relation to time, e.g. temperature-time diagrams}	B29C65/00	B29C66/91951		365
B29C66/92	9	{by measuring or controlling the pressure, the force, the mechanical power or the displacement of the joining tools}	B29C65/00	B29C66/92		99
B29C66/922	10	{by measuring the pressure, the force, the mechanical power or the displacement of the joining tools}	B29C65/00	B29C66/922		28
B29C66/9221	11	{by measuring the pressure, the force or the mechanical power}	B29C65/00	B29C66/9221		435
B29C66/92211	12	{with special measurement means or methods}	B29C65/00	B29C66/92211		222
B29C66/9231	11	{by measuring the displacement of the joining tools}	B29C65/00	B29C66/9231		199
B29C66/92311	12	{with special measurement means or methods}	B29C65/00	B29C66/92311		105
B29C66/924	10	{by controlling or regulating the pressure, the force, the mechanical power or the displacement of the joining tools}	B29C65/00	B29C66/924		96
B29C66/9241	11	{by controlling or regulating the pressure, the force or the mechanical power}	B29C65/00	B29C66/9241		1185
B29C66/92431	12	{the pressure, the force or the mechanical power being kept constant over time (B29C66/92613 takes precedence)}	B29C65/00	B29C66/92431		139
B29C66/92441	12	{the pressure, the force or the mechanical power being non-constant over time}	B29C65/00	B29C66/92441		43
B29C66/92443	13	{following a pressure-time profile}	B29C65/00	B29C66/92443		117
B29C66/92445	14	{by steps}	B29C65/00	B29C66/92445		194
B29C66/92451	12	{using joining tools having different pressure zones or using several joining tools with different pressures}	B29C65/00	B29C66/92451		102
B29C66/9261	11	{by controlling or regulating the displacement of the joining tools}	B29C65/00	B29C66/9261		299
B29C66/92611	12	{by controlling or regulating the gap between the joining tools}	B29C65/00	B29C66/92611		365
B29C66/92613	13	{the gap being kept constant over time}	B29C65/00	B29C66/92613		74
B29C66/92615	13	{the gap being non-constant over time}	B29C65/00	B29C66/92615		73
B29C66/92651	12	{by using stops}	B29C65/00	B29C66/92651		159
B29C66/92653	13	{said stops being adjustable}	B29C65/00	B29C66/92653		233
B29C66/92655	13	{by using several stops}	B29C65/00	B29C66/92655		149
B29C66/929	10	{characterized by specific pressure, force, mechanical power or displacement values or ranges}	B29C65/00	B29C66/929		1211
B29C66/9292	11	{in explicit relation to another variable, e.g. pressure diagrams}	B29C65/00	B29C66/9292		91
B29C66/92921	12	{in specific relation to time, e.g. pressure-time diagrams}	B29C65/00	B29C66/92921		254
B29C66/93	9	{by measuring or controlling the speed}	B29C65/00	B29C66/93		20
B29C66/932	10	{by measuring the speed}	B29C65/00	B29C66/932		189
B29C66/9321	11	{with special speed measurement means or methods}	B29C65/00	B29C66/9321		23
B29C66/934	10	{by controlling or regulating the speed}	B29C65/00	B29C66/934		652
B29C66/93411	11	{the parts to be joined having different speeds}	B29C65/00	B29C66/93411		46
B29C66/93431	11	{the speed being kept constant over time}	B29C65/00	B29C66/93431		171
B29C66/93441	11	{the speed being non-constant over time}	B29C65/00	B29C66/93441		315
B29C66/93451	11	{by controlling or regulating the rotational speed, i.e. the speed of revolution}	B29C65/00	B29C66/93451		482
B29C66/939	10	{characterised by specific speed values or ranges}	B29C65/00	B29C66/939		656
B29C66/9392	11	{in explicit relation to another variable, e.g. speed diagrams}	B29C65/00	B29C66/9392		132
B29C66/94	9	{by measuring or controlling the time}	B29C65/00	B29C66/94		441
B29C66/942	10	{by measuring the time}	B29C65/00	B29C66/942		77
B29C66/9421	11	{with special time measurement means or methods}	B29C65/00	B29C66/9421		5
B29C66/944	10	{by controlling or regulating the time}	B29C65/00	B29C66/944		642
B29C66/9441	11	{the time being controlled or regulated as a function of another parameter}	B29C65/00	B29C66/9441		86
B29C66/949	10	{characterised by specific time values or ranges}	B29C65/00	B29C66/949		1362
B29C66/9492	11	{in explicit relation to another variable}	B29C65/00	B29C66/9492		17
B29C66/95	9	{by measuring or controlling specific variables not covered by groups B29C66/91&#160;-&#160;B29C66/94}	B29C65/00	B29C66/95		377
B29C66/951	10	{by measuring or controlling the vibration frequency and/or the vibration amplitude of vibrating joining tools, e.g. of ultrasonic welding tools}	B29C65/00	B29C66/951		54
B29C66/9511	11	{by measuring their vibration frequency}	B29C65/00	B29C66/9511		63
B29C66/9512	11	{by controlling their vibration frequency}	B29C65/00	B29C66/9512		292
B29C66/9513	11	{characterised by specific vibration frequency values or ranges}	B29C65/00	B29C66/9513		657
B29C66/9515	11	{by measuring their vibration amplitude}	B29C65/00	B29C66/9515		55
B29C66/9516	11	{by controlling their vibration amplitude}	B29C65/00	B29C66/9516		360
B29C66/9517	11	{characterised by specific vibration amplitude values or ranges}	B29C65/00	B29C66/9517		347
B29C66/952	10	{by measuring or controlling the wavelength}	B29C65/00	B29C66/952		36
B29C66/953	10	{by measuring or controlling the humidity}	B29C65/00	B29C66/953		14
B29C66/9532	11	{of the parts to be joined, i.e. taking the humidity of the parts to be joined into account}	B29C65/00	B29C66/9532		22
B29C66/9534	11	{of the atmosphere, i.e. taking the ambient humidity into account}	B29C65/00	B29C66/9534		37
B29C66/954	10	{by measuring or controlling the thickness of the parts to be joined}	B29C65/00	B29C66/954		188
B29C66/959	10	{characterised by specific values or ranges of said specific variables}	B29C65/00	B29C66/959		31
B29C66/9592	11	{in explicit relation to another variable, e.g. X-Y diagrams}	B29C65/00	B29C66/9592		541
B29C66/96	9	{characterised by the method for implementing the controlling of the joining process}	B29C65/00	B29C66/96		242
B29C66/961	10	{involving a feedback loop mechanism, e.g. comparison with a desired value}	B29C65/00	B29C66/961		1731
B29C66/962	10	{using proportional controllers, e.g. PID controllers [proportional&#8211;integral&#8211;derivative controllers]}	B29C65/00	B29C66/962		91
B29C66/963	10	{using stored or historical data sets, e.g. using expert systems}	B29C65/00	B29C66/963		78
B29C66/964	10	{involving trial and error}	B29C65/00	B29C66/964		75
B29C66/965	10	{using artificial neural networks}	B29C65/00	B29C66/965		19
B29C66/966	10	{using fuzzy logic}	B29C65/00	B29C66/966		7
B29C66/967	10	{involving special data inputs or special data outputs, e.g. for monitoring purposes}	B29C65/00	B29C66/967		37
B29C66/9672	11	{involving special data inputs, e.g. involving barcodes, RFID tags}	B29C65/00	B29C66/9672		675
B29C66/9674	11	{involving special data outputs, e.g. special data display means (B29C66/8748 takes precedence)}	B29C65/00	B29C66/9674		338
B29C66/97	9	{Checking completion of joining or correct joining by using indications on at least one of the joined parts}	B29C65/00	B29C66/97		120
B29C66/972	10	{by extrusion of molten material}	B29C65/00	B29C66/972		135
B29C66/974	10	{by checking the bead or burr form}	B29C65/00	B29C66/974		42
B29C66/976	10	{by the use of an indicator pin, e.g. being integral with one of the parts to be joined}	B29C65/00	B29C66/976		119
B29C66/98	9	{Determining the joining area by using markings on at least one of the parts to be joined}	B29C65/00	B29C66/98		167
B29C67/00	7	Shaping techniques not covered by groups B29C39/00&#160;-&#160;B29C65/00, B29C70/00 or B29C73/00	B29C67/00	B29C67/00		2112
B29C67/0003	8	{Moulding articles between moving mould surfaces, e.g. turning surfaces}	B29C67/00	B29C67/00		207
B29C67/0007	8	{Manufacturing coloured articles not otherwise provided for, e.g. by colour change}	B29C67/00	B29C67/00		205
B29C67/0011	8	{for shaping plates or sheets}	B29C67/00	B29C67/00		361
B29C67/0014	8	{for shaping tubes or blown tubular films}	B29C67/00	B29C67/00		433
B29C67/0018	9	{Turning tubes inside out (for lining internal surfaces B29C63/36)}	B29C67/00	B29C67/00		198
B29C67/0022	9	{using an internal mandrel}	B29C67/00	B29C67/00		50
B29C67/0025	10	{and pressure difference}	B29C67/00	B29C67/00		19
B29C67/0029	8	{Cold deforming of thermoplastics material (B29C43/16, B29C59/00 take precedence)}	B29C67/00	B29C67/00		204
B29C67/0033	8	{by shock-waves}	B29C67/00	B29C67/00		29
B29C67/0037	8	{Forming articles from a moulding composition enclosed in a deformable bag (making moulds composed of particles enclosed in a bag B29C33/3821; from expandable material in flexible bags B29C44/182; with reinforcements placed in a covering element B29C70/542)}	B29C67/00	B29C67/00		64
B29C67/004	8	{Closing perforations or small holes, e.g. using additional moulding material}	B29C67/00	B29C67/00		122
B29C67/0044	8	{for shaping edges or extremities (B29C57/00 takes precedence)}	B29C67/00	B29C67/00		791
B29C67/0048	8	{Local deformation of formed objects}	B29C67/00	B29C67/00		92
B29C67/02	8	Moulding by agglomerating {(B29C67/20 takes precedence)}	B29C67/02	B29C67/02		144
B29C67/04	9	Sintering (combined with compression B29C43/00)	B29C67/04	B29C67/04		673
B29C67/06	9	Coagulating	B29C67/06	B29C67/06		53
B29C67/08	8	Screen moulding, e.g. forcing the moulding material through a perforated screen on to a moulding surface	B29C67/08	B29C67/08		99
B29C67/20	8	for porous or cellular articles, e.g. of foam plastics, coarse-pored {(chemical aspects of working up macro-molecular substances to porous or cellular articles C08J9/00)}	B29C67/20	B29C67/20		1092
B29C67/202	9	{comprising elimination of a solid or a liquid ingredient}	B29C67/20	B29C67/20		471
B29C67/205	9	{comprising surface fusion, and bonding of particles to form voids, e.g. sintering}	B29C67/20	B29C67/20		408
B29C67/207	9	{comprising impregnating expanded particles or fragments with a binder}	B29C67/20	B29C67/20		186
B29C67/24	8	characterised by the choice of material	B29C67/24	B29C67/24		1088
B29C67/241	9	{Moulding wax}	B29C67/24	B29C67/24		337
B29C67/242	9	{Moulding mineral aggregates bonded with resin, e.g. resin concrete (shaping ceramic compositions without binder or water-setting cementitious material B28B; compositions per seC04B)}	B29C67/24	B29C67/24		266
B29C67/243	10	{for making articles of definite length}	B29C67/24	B29C67/24		728
B29C67/244	11	{by vibrating the composition before or during moulding}	B29C67/24	B29C67/24		290
B29C67/245	10	{for making articles of indefinite length}	B29C67/24	B29C67/24		115
B29C67/246	9	{Moulding high reactive monomers or prepolymers, e.g. by reaction injection moulding [RIM], liquid injection moulding [LIM] (casting monomers B29C39/006, mixing construction B29B7/74)}	B29C67/24	B29C67/24		1378
B29C67/247	9	{Moulding polymers or prepolymers containing ingredients in a frangible packaging, e.g. microcapsules (expandable components kept in frangible containers within a flexible bag B29C44/183)}	B29C67/24	B29C67/24		49
B29C67/248	9	{Moulding mineral fibres or particles bonded with resin, e.g. for insulating or roofing board (articles from wood or lignocellulosic material with binding agents B27N; mineral aggregates bonded with resin B29C67/242; thermal insulation in general F16L59/00)}	B29C67/24	B29C67/24		179
B29C67/249	10	{for making articles of indefinite length}	B29C67/24	B29C67/24		135
B29C69/00	7	Combinations of shaping techniques not provided for in a single one of main groups B29C39/00&#160;-&#160;B29C67/00, e.g. associations of moulding and joining techniques; Apparatus therefore {(B29C48/001 takes precedence)}	B29C69/00	B29C69/00		3139
B29C69/001	8	{a shaping technique combined with cutting, e.g. in parts or slices combined with rearranging and joining the cut parts (for reinforced material B29C70/545; B29C49/4278, B29C51/268 take precedence)}	B29C69/00	B29C69/00		2657
B29C69/002	9	{Winding (cutting of individual length B26D)}	B29C69/00	B29C69/00		171
B29C69/003	10	{and cutting longitudinally, e.g. for making O-rings; chain links, insulation tubes}	B29C69/00	B29C69/00		163
B29C69/004	8	{making articles by joining parts moulded in separate cavities, said parts being in said separate cavities during said joining (B29C45/006, B29C51/267 take precedence)}	B29C69/00	B29C69/00		291
B29C69/005	8	{cutting-off or cutting-out a part of a strip-like or sheet-like material, transferring that part and fixing it to an article (if labeling seeB65C, in combination with box-making B31B50/81; labelling in general B65C)}	B29C69/00	B29C69/00		257
B29C69/006	9	{rotating transfer means}	B29C69/00	B29C69/00		105
B29C69/007	8	{Lining or sheathing in combination with forming the article to be lined}	B29C69/00	B29C69/00		95
B29C69/008	9	{of tubular articles}	B29C69/00	B29C69/00		50
B29C69/02	8	of moulding techniques only	B29C69/02	B29C69/02		1741
B29C69/025	9	{Deforming articles in a simpler intermediate shape without internal stresses for packaging transporting or storage and reshaping and fixing the original configuration on the place of use (shaping by liberation of internal stresses B29C61/00)}	B29C69/02	B29C69/02		51
B29C70/00	7	Shaping composites, i.e. plastics material comprising reinforcements, fillers or preformed parts, e.g. inserts<br><br><u>NOTE</u><br><br> In this group, the following terms or expressions are used with the meanings indicated: <br>"reinforcement" means a structure in the form of fibres, wires, rods, bars, sections, plates or blocks, which improves the strength of an article;<br>"filler" means a relatively inert substance in the form of particles, powder, beads, flakes or spheres, which improves the physical properties or increases the bulk or weight of an article;<br>"preformed part" means a part made of any material, being completely shaped to have a determined form and which is not used as a reinforcement, e.g. wires or nets forced only into the surface of an article;<br>"insert" means a preformed part incorporated in an article during moulding.	B29C70/00	B29C70/00		807
B29C70/003	8	{characterised by the matrix material, e.g. material composition or physical properties}	B29C70/00	B29C70/00		660
B29C70/0035	9	{comprising two or more matrix materials}	B29C70/00	B29C70/00		266
B29C70/02	8	comprising combinations of reinforcements, {e.g. non-specified reinforcements, fibrous reinforcing inserts} and fillers, {e.g. particulate fillers}, incorporated in matrix material, forming one or more layers and with or without non-reinforced or non-filled layers {(combinations of fibrous reinforcement only B29C70/04; combinations of fillers only B29C70/58; combinations with non reinforcing inserts, e.g. foam blocks, B29C70/68)}	B29C70/02	B29C70/02		291
B29C70/021	9	{Combinations of fibrous reinforcement and non-fibrous material}	B29C70/02	B29C70/02		291
B29C70/023	10	{with reinforcing inserts}	B29C70/02	B29C70/02		185
B29C70/025	10	{with particular filler}	B29C70/02	B29C70/02		919
B29C70/026	9	{and with one or more layers of pure plastics material, e.g. foam layers (applying a non-preformed coating, e.g. a gel-coat B29C37/0025; with foam blocks B29C70/86)}	B29C70/02	B29C70/02		184
B29C70/028	9	{and with one or more layers of non-plastics material or non-specified material, e.g. supports}	B29C70/02	B29C70/02		81
B29C70/04	8	comprising reinforcements only, e.g. self-reinforcing plastics	B29C70/04	B29C70/04		488
B29C70/06	9	Fibrous reinforcements only	B29C70/06	B29C70/06		1470
B29C70/08	10	comprising combinations of different forms of fibrous reinforcements incorporated in matrix material, forming one or more layers, and with or without non-reinforced layers	B29C70/08	B29C70/08		1244
B29C70/081	11	{Combinations of fibres of continuous or substantial length and short fibres}	B29C70/08	B29C70/08		576
B29C70/083	11	{Combinations of continuous fibres or fibrous profiled structures oriented in one direction and reinforcements forming a two dimensional structure, e.g. mats (B29D24/00, B29D99/001 take precedence)}	B29C70/08	B29C70/08		368
B29C70/085	12	{the structure being deformed in a three dimensional configuration (B29C53/805 takes precedence)}	B29C70/08	B29C70/08		178
B29C70/086	11	{and with one or more layers of pure plastics material, e.g. foam layers (applying a non-preformed coating, e.g. a gel-coat, B29C37/0025; with foam blocks B29C70/86)}	B29C70/08	B29C70/08		1501
B29C70/088	11	{and with one or more layers of non-plastics material or non-specified material, e.g. supports}	B29C70/08	B29C70/08		633
B29C70/10	10	characterised by the structure of fibrous reinforcements {, e.g. hollow fibres}	B29C70/10	B29C70/10		831
B29C70/12	11	using fibres of short length, e.g. in the form of a mat {(non-woven fabrics per seD04H1/00)}	B29C70/12	B29C70/12		1347
B29C70/14	12	oriented	B29C70/14	B29C70/14		482
B29C70/16	11	using fibres of substantial or continuous length {(non-woven fabrics per seD04H3/00)}	B29C70/16	B29C70/16		1226
B29C70/18	12	in the form of a mat, e.g. sheet moulding compound [SMC]	B29C70/18	B29C70/18		349
B29C70/20	12	oriented in a single direction, e.g. roofing or other parallel fibres {(B29C70/083, B29C70/226 take precedence)}	B29C70/20	B29C70/20		1068
B29C70/202	13	{arranged in parallel planes or structures of fibres crossing at substantial angles, e.g. cross-moulding compound [XMC] (B29C70/207 takes precedence)}	B29C70/20	B29C70/20		660
B29C70/205	13	{the structure being shaped to form a three-dimensional configuration}	B29C70/20	B29C70/20		384
B29C70/207	14	{arranged in parallel planes of fibres crossing at substantial angles}	B29C70/20	B29C70/20		267
B29C70/22	12	oriented in at least two directions forming a two-dimensional [2D] structure	B29C70/22	B29C70/22		1022
B29C70/222	13	{the structure being shaped to form a three dimensional configuration}	B29C70/22	B29C70/22		760
B29C70/224	13	{the structure being a net (B29C70/688 takes precedence)}	B29C70/22	B29C70/22		158
B29C70/226	13	{the structure comprising mainly parallel filaments interconnected by a small number of cross threads}	B29C70/22	B29C70/22		194
B29C70/228	13	{the structure being stacked in parallel layers with fibres of adjacent layers crossing at substantial angles}	B29C70/22	B29C70/22		232
B29C70/24	12	oriented in at least three directions forming a three-dimensional [3D] structure	B29C70/24	B29C70/24		1453
B29C70/26	9	Non-fibrous reinforcements only {(B29C35/0272, B29C61/0625, B29C70/887 take precedence; combined with fibres B29C70/023)}	B29C70/26	B29C70/26		288
B29C70/28	9	Shaping operations therefor<br><br><u>NOTE</u><br><br> This group covers: <br>the shaping of a coherent fibrous reinforcements which are pre-impregnated or without binder; or of non-coherent reinforcements of fibres in a mould or on a support;<br>the impregnation or introduction of a plastics matrix in reinforcements during shaping;<br>This group does not cover:<br>the moulding by a single technique of plastics matrix material mixed with and containing reinforcing fibres of short length, which is covered by the appropriate place for that technique;<br>the pretreatment, e.g. impregnation, of reinforcements per se, i.e. independently of their shaping, which is covered by group B29B15/08	B29C70/28	B29C70/28		801
B29C70/30	10	Shaping by lay-up, i.e. applying fibres, tape or broadsheet on a mould, former or core; Shaping by spray-up, i.e. spraying of fibres on a mould, former or core	B29C70/30	B29C70/30		3468
B29C70/302	11	{Details of the edges of fibre composites, e.g. edge finishing or means to avoid delamination}	B29C70/30	B29C70/30		400
B29C70/304	11	{In-plane lamination by juxtaposing or interleaving of plies, e.g. scarf joining}	B29C70/30	B29C70/30		194
B29C70/305	11	{Spray-up of reinforcing fibres with or without matrix to form a non-coherent mat in or on a mould (B29C41/365, B29C70/32, B29C70/34, B29C70/502, B29C70/508 take precedence; coating a former by spraying plastics B29C41/08)}	B29C70/30	B29C70/30		333
B29C70/32	11	on a rotating mould, former or core	B29C70/32	B29C70/32		2345
B29C70/323	12	{on the inner surface of a rotating mould}	B29C70/32	B29C70/32		72
B29C70/326	13	{by rotating the mould around its axis of symmetry}	B29C70/32	B29C70/32		209
B29C70/34	11	and shaping or impregnating by compression {, i.e. combined with compressing after the lay-up operation}	B29C70/34	B29C70/34		2831
B29C70/342	12	{using isostatic pressure}	B29C70/34	B29C70/34		2909
B29C70/345	12	{using matched moulds}	B29C70/34	B29C70/34		1933
B29C70/347	12	{combined with compressing after the winding of lay-ups having a non-circular cross-section, e.g. flat spiral windings}	B29C70/34	B29C70/34		381
B29C70/36	11	and impregnating by casting, e.g. vacuum casting	B29C70/36	B29C70/36		1176
B29C70/38	11	Automated lay-up, e.g. using robots, laying filaments according to predetermined patterns {(application heads for tyres B29D30/28)}	B29C70/38	B29C70/38		1388
B29C70/382	12	{Automated fiber placement [AFP]}	B29C70/38	B29C70/38		872
B29C70/384	13	{Fiber placement heads, e.g. component parts, details or accessories}	B29C70/38	B29C70/38		579
B29C70/386	12	{Automated tape laying [ATL]}	B29C70/38	B29C70/38		839
B29C70/388	13	{Tape placement heads, e.g. component parts, details or accessories}	B29C70/38	B29C70/38		542
B29C70/40	10	Shaping or impregnating by compression (B29C70/34 takes precedence){not applied}	B29C70/40	B29C70/40		492
B29C70/42	11	for producing articles of definite length, i.e. discrete articles	B29C70/42	B29C70/42		1250
B29C70/44	12	using isostatic pressure, e.g. pressure difference-moulding, vacuum bag-moulding, autoclave-moulding or expanding rubber-moulding	B29C70/44	B29C70/44		2525
B29C70/443	13	{and impregnating by vacuum or injection}	B29C70/44	B29C70/44		1940
B29C70/446	13	{Moulding structures having an axis of symmetry or at least one channel, e.g. tubular structures, frames}	B29C70/44	B29C70/44		1148
B29C70/46	12	using matched moulds, e.g. for deforming sheet moulding compounds [SMC] or prepregs	B29C70/46	B29C70/46		2656
B29C70/461	13	{Rigid movable compressing mould parts acting independently from opening or closing action of the main mould}	B29C70/46	B29C70/46		182
B29C70/462	13	{Moulding structures having an axis of symmetry or at least one channel, e.g. tubular structures, frames}	B29C70/46	B29C70/46		548
B29C70/465	13	{and impregnating by melting a solid material, e.g. sheets, powders of fibres}	B29C70/46	B29C70/46		535
B29C70/467	13	{and impregnating the reinforcements during mould closing (B29C70/465 takes precedence)}	B29C70/46	B29C70/46		295
B29C70/48	13	and impregnating the reinforcements in the closed mould, e.g. resin transfer moulding [RTM] {, e.g. by vacuum}	B29C70/48	B29C70/48		3133
B29C70/50	11	for producing articles of indefinite length, e.g. prepregs, sheet moulding compounds [SMC] or cross moulding compounds [XMC]	B29C70/50	B29C70/50		1362
B29C70/502	12	{by first forming a mat composed of short fibres}	B29C70/50	B29C70/50		161
B29C70/504	12	{using rollers or pressure bands (for corrugating B29C53/22)}	B29C70/50	B29C70/50		1078
B29C70/506	13	{and impregnating by melting a solid material, e.g. sheet, powder, fibres (B29C70/508 takes precedence)}	B29C70/50	B29C70/50		406
B29C70/508	13	{and first forming a mat composed of short fibres}	B29C70/50	B29C70/50		172
B29C70/52	12	Pultrusion, i.e. forming and compressing by continuously pulling through a die	B29C70/52	B29C70/52		1441
B29C70/521	13	{and impregnating the reinforcement before the die}	B29C70/52	B29C70/52		1027
B29C70/522	14	{the transport direction being vertical}	B29C70/52	B29C70/52		75
B29C70/523	13	{and impregnating the reinforcement in the die}	B29C70/52	B29C70/52		426
B29C70/524	14	{the transport direction being vertical}	B29C70/52	B29C70/52		30
B29C70/525	13	{Component parts, details or accessories; Auxiliary operations}	B29C70/52	B29C70/52		1135
B29C70/526	14	{Pultrusion dies, e.g. dies with moving or rotating parts (B29C70/523 takes precedence)}	B29C70/52	B29C70/52		466
B29C70/527	14	{Pulling means}	B29C70/52	B29C70/52		195
B29C70/528	14	{Heating or cooling}	B29C70/52	B29C70/52		573
B29C70/54	10	Component parts, details or accessories; Auxiliary operations {, e.g. feeding or storage of prepregs or SMC after impregnation or during ageing}	B29C70/54	B29C70/54		8482
B29C70/541	11	{Positioning reinforcements in a mould, e.g. using clamping means for the reinforcement (positioning inserts in moulds B29C33/12; lay-up on a mould B29C70/30)}	B29C70/54	B29C70/54		1061
B29C70/542	11	{Placing or positioning the reinforcement in a covering or packaging element before or during moulding, e.g. drawing in a sleeve}	B29C70/54	B29C70/54		430
B29C70/543	11	{Fixing the position or configuration of fibrous reinforcements before or during moulding (for non-woven fabrics D04H3/08)}	B29C70/54	B29C70/54		1258
B29C70/544	11	{Details of vacuum bags, e.g. materials or shape}	B29C70/54	B29C70/54		309
B29C70/545	11	{Perforating, cutting or machining during or after moulding}	B29C70/54	B29C70/54		2760
B29C70/546	11	{Measures for feeding or distributing the matrix material in the reinforcing structure}	B29C70/54	B29C70/54		454
B29C70/547	12	{using channels or porous distribution layers incorporated in or associated with the product}	B29C70/54	B29C70/54		311
B29C70/548	12	{using distribution constructions, e.g. channels incorporated in or associated with the mould}	B29C70/54	B29C70/54		277
B29C70/549	11	{Details of caul plates, e.g. materials or shape}	B29C70/54	B29C70/54		234
B29C70/56	11	Tensioning reinforcements before or during shaping	B29C70/56	B29C70/56		796
B29C70/58	8	comprising fillers only {, e.g. particles, powder, beads, flakes, spheres (B29C70/025 takes precedence, agglomerating hollow spheres to produce synthetic foam B29C70/66; compounding ingredients per seC08K)}<br><br><u>NOTE</u><br><br>Moulding of plastics matrix material mixed with fillers by a single technique is classified in the appropriate place for that technique.	B29C70/58	B29C70/58		1195
B29C70/585	9	{incorporation of light reflecting filler, e.g. lamellae to obtain pearlescent effet (partially embedding reflective elements into the surface of or support B29D11/00615)}	B29C70/58	B29C70/58		99
B29C70/60	9	comprising a combination of distinct filler types incorporated in matrix material, forming one or more layers, and with or without non-filled layers	B29C70/60	B29C70/60		90
B29C70/603	10	{and with one or more layers of pure plastics material, e.g. foam layers (applying a non-preformed coating, e.g. a gel-coat B29C37/0025; with foam blocks B29C70/86)}	B29C70/60	B29C70/60		52
B29C70/606	10	{and with one or more layers of non-plastics material or non-specified material, e.g. supports}	B29C70/60	B29C70/60		23
B29C70/62	9	the filler being oriented during moulding (for short fibres B29C70/14)	B29C70/62	B29C70/62		244
B29C70/64	9	the filler influencing the surface characteristics of the material, e.g. by concentrating near the surface or by incorporating in the surface by force	B29C70/64	B29C70/64		418
B29C70/66	9	the filler comprising hollow constituents, e.g. syntactic foam	B29C70/66	B29C70/66		438
B29C70/68	8	by incorporating or moulding on preformed parts, e.g. inserts or layers {, e.g. foam blocks (mould constructions therefor B29C33/12; joining preformed parts by moulding B29C65/70)}<br><br><u>NOTE</u><br><br> This group does not cover: <br>incorporating, or moulding on, preformed parts by a single technique, which is covered by the appropriate place for that technique;<br>pretreatment of preformed parts per se, i.e. independently of their shaping, which is covered by group B29B15/00	B29C70/68	B29C70/68		1758
B29C70/681	9	{Component parts, details or accessories; Auxiliary operations}	B29C70/68	B29C70/68		731
B29C70/682	10	{Preformed parts characterised by their structure, e.g. form}	B29C70/68	B29C70/68		583
B29C70/683	10	{Pretreatment of the preformed part, e.g. insert}	B29C70/68	B29C70/68		514
B29C70/685	9	{by laminating inserts between two plastic films or plates}	B29C70/68	B29C70/68		145
B29C70/686	10	{the inserts being sheets or documents, e.g. ID cards}	B29C70/68	B29C70/68		35
B29C70/687	10	{the inserts being oriented, e.g. nets or meshes}	B29C70/68	B29C70/68		272
B29C70/688	9	{the inserts being meshes or lattices (B29C70/82, B29C70/683 take precedence)}	B29C70/68	B29C70/68		172
B29C70/70	9	Completely encapsulating inserts {(B29C70/86 takes precedence)}	B29C70/70	B29C70/70		1297
B29C70/72	9	Encapsulating inserts having non-encapsulated projections, e.g. extremities or terminal portions of electrical components {(B29C70/742 takes precedence)}	B29C70/72	B29C70/72		932
B29C70/74	9	Moulding material on a relatively small portion of the preformed part, e.g. outsert moulding {(B29C70/845 takes precedence)}	B29C70/74	B29C70/74		792
B29C70/742	10	{Forming a hollow body around the preformed part}	B29C70/74	B29C70/74		105
B29C70/745	10	{Filling cavities in the preformed part (for joining B29C70/84)}	B29C70/74	B29C70/74		308
B29C70/747	10	{Applying material, e.g. foam, only in a limited number of places or in a pattern, e.g. to create a decorative effect}	B29C70/74	B29C70/74		85
B29C70/76	10	Moulding on edges or extremities of the preformed part	B29C70/76	B29C70/76		312
B29C70/763	11	{the edges being disposed in a substantial flat plane}	B29C70/76	B29C70/76		416
B29C70/766	11	{on the end part of a tubular article}	B29C70/76	B29C70/76		271
B29C70/78	9	Moulding material on one side only of the preformed part	B29C70/78	B29C70/78		1277
B29C70/80	10	Moulding sealing material into closure members {(placing sealings in closures B21D51/46)}	B29C70/80	B29C70/80		265
B29C70/82	9	Forcing wires, nets or the like partially or completely into the surface of an article, e.g. by cutting and pressing	B29C70/82	B29C70/82		344
B29C70/84	9	by moulding material on preformed parts to be joined {(joining plastic parts by moulding B29C65/70)}	B29C70/84	B29C70/84		776
B29C70/845	10	{by moulding material on a relative small portion of the preformed parts}	B29C70/84	B29C70/84		348
B29C70/86	9	Incorporated in coherent impregnated reinforcing layers, {e.g. by winding}	B29C70/86	B29C70/86		1617
B29C70/865	10	{completely encapsulated}	B29C70/86	B29C70/86		960
B29C70/88	8	characterised primarily by possessing specific properties, e.g. electrically conductive or locally reinforced	B29C70/88	B29C70/88		646
B29C70/882	9	{partly or totally electrically conductive, e.g. for EMI shielding (conductive floors or floor coverings H05F3/025; EMI shielding in general H05K9/00)}	B29C70/88	B29C70/88		724
B29C70/885	10	{with incorporated metallic wires, nets, films or plates (as lost heating elements B29C35/0272, B29C61/0625)}	B29C70/88	B29C70/88		643
B29C70/887	9	{locally reinforced, e.g. by fillers (filler concentrated near the surface B29C70/64)}	B29C70/88	B29C70/88		348
B29C71/00	7	After-treatment of articles without altering their shape; Apparatus therefor (B29C44/56, B29C73/00 take precedence; surface shaping B29C59/00{; for joined or sealed parts B29C66/03; after-treatment specially adapted for vulcanising tyres B29D30/0633})	B29C71/00	B29C71/00		1015
B29C71/0009	8	{using liquids, e.g. solvents, swelling agents (spectacle cases, e.g. for cleaning contact lenses A45C11/04; disinfecting  or sterilising contact lenses A61L12/00, using liquid substances A61L2/20; cleaning involving the use of liquid in general B08B3/00; for hydrating contact lenses B29D11/00067)}	B29C71/00	B29C71/00		1269
B29C2071/0018	9	{Absorbing ingredients, e.g. drugs, flavourings, UV screeners, embedded in the articles}	B29C71/00	B29C71/00		99
B29C2071/0027	9	{Removing undesirable residual components, e.g. solvents, unreacted monomers}	B29C71/00	B29C71/00		173
B29C2071/0036	9	{Extracting, degassing, removing gases from moulded articles}	B29C71/00	B29C71/00		35
B29C2071/0045	9	{Washing using non-reactive liquids}	B29C71/00	B29C71/00		123
B29C2071/0054	9	{Supercritical fluid treatment, i.e. using a liquid in which distinct liquid and gas phases do not exist}	B29C71/00	B29C71/00		33
B29C71/0063	8	{for changing crystallisation}	B29C71/00	B29C71/00		354
B29C71/0072	8	{for changing orientation}	B29C71/00	B29C71/00		130
B29C71/0081	8	{using an electric field, e.g. for electrostatic charging (electrostatic pinning of extruded material B29C48/9165; fixing linings by electrostatic charges B29C63/0043)}	B29C71/00	B29C71/00		276
B29C71/009	8	{using gases without chemical reaction (C08J7/12 takes precedence; in combination with blow-moulding B29C49/46; surface treatment using plasma B29C59/14, ionised gas B29C59/16)}	B29C71/00	B29C71/00		133
B29C71/02	8	Thermal after-treatment {(B29C71/0063 and B29C71/0072 take precedence)}	B29C71/02	B29C71/02		2604
B29C2071/022	9	{Annealing}	B29C71/02	B29C71/02		774
B29C2071/025	9	{Quenching, i.e. rapid cooling of an object}	B29C71/02	B29C71/02		107
B29C2071/027	9	{Tempering, i.e. heating an object to a high temperature and quenching it}	B29C71/02	B29C71/02		92
B29C71/04	8	by wave energy or particle radiation {, e.g. for curing or vulcanising preformed articles (during moulding, e.g. in a mould B29C35/08)}	B29C71/04	B29C71/04		1359
B29C73/00	7	Repairing of articles made from plastics or substances in a plastic state, e.g. of articles shaped or produced by using techniques covered by this subclass or subclass B29D({linings for tyres acting locally B60C5/142;} retreading tyres B29D30/54; devices for covering leaks in pipes or hoses F16L55/16)	B29C73/00	B29C73/00		336
B29C73/02	8	using liquid or paste-like material (B29C73/16 takes precedence)	B29C73/02	B29C73/02		822
B29C73/025	9	{fed under pressure}	B29C73/02	B29C73/02		433
B29C73/04	8	using preformed elements	B29C73/04	B29C73/04		459
B29C73/06	9	using plugs sealing in the hole	B29C73/06	B29C73/06		376
B29C73/063	10	{expandable}	B29C73/06	B29C73/06		17
B29C73/066	11	{by mechanical means provided on the plug}	B29C73/06	B29C73/06		14
B29C73/08	10	Apparatus therefor, e.g. for inserting	B29C73/08	B29C73/08		343
B29C73/10	9	using patches sealing on the surface of the article (B29C73/14 takes precedence)	B29C73/10	B29C73/10		1764
B29C73/105	10	{provided with a centering element}	B29C73/10	B29C73/10		17
B29C73/12	10	Apparatus therefor, e.g. for applying (B29C73/30 takes precedence)	B29C73/12	B29C73/12		315
B29C73/14	9	using elements composed of two parts joined together after having been placed one on each side of the article	B29C73/14	B29C73/14		114
B29C73/16	8	Auto-repairing or self-sealing arrangements or agents {(incorporating auto-repairing or self-sealing arrangements or agents on or into tyres B29D30/0685)}	B29C73/16	B29C73/16		85
B29C73/163	9	{Sealing compositions or agents, e.g. combined with propellant agents}	B29C73/16	B29C73/16		858
B29C73/166	9	{Devices or methods for introducing sealing compositions into articles}	B29C73/16	B29C73/16		720
B29C73/18	9	the article material itself being self-sealing, e.g. by compression	B29C73/18	B29C73/18		117
B29C73/20	10	the article material only consisting in part of a deformable sealing material	B29C73/20	B29C73/20		156
B29C73/22	9	the article containing elements including a sealing composition, e.g. powder being liberated when the article is damaged	B29C73/22	B29C73/22		428
B29C73/24	8	Apparatus or accessories not otherwise provided for	B29C73/24	B29C73/24		490
B29C73/245	9	{for removing the element having caused the damage}	B29C73/24	B29C73/24		54
B29C73/26	9	for mechanical pretreatment	B29C73/26	B29C73/26		620
B29C2073/262	10	{for polishing, roughening, buffing or sanding the area to be repaired}	B29C73/26	B29C73/26		304
B29C2073/264	10	{for cutting out or grooving the area to be repaired}	B29C73/26	B29C73/26		268
B29C2073/266	10	{for cutting out an undercut for anchoring the repairing material}	B29C73/26	B29C73/26		40
B29C2073/268	10	{for drilling holes in the area to be repaired}	B29C73/26	B29C73/26		65
B29C73/28	9	for clamping and stretching flexible material, e.g. inner tubes	B29C73/28	B29C73/28		51
B29C73/30	9	for local pressing or local heating	B29C73/30	B29C73/30		814
B29C73/305	10	{specially adapted for toroidal articles, e.g. tyres (B29C73/325 takes precedence)}	B29C73/30	B29C73/30		388
B29C73/32	10	using an elastic element, e.g. inflatable bag	B29C73/32	B29C73/32		113
B29C73/325	11	{specially adapted for toroidal articles, e.g. tyres}	B29C73/32	B29C73/32		200
B29C73/34	10	for local heating	B29C73/34	B29C73/34		496
B29C2791/00	7	Shaping characteristics in general	CPCONLY	B29C2791/00		15
B29C2791/001	8	Shaping in several steps	CPCONLY	B29C2791/001		2214
B29C2791/002	8	Making articles of definite length, i.e. discrete articles (B29C53/40 takes precedence)	CPCONLY	B29C2791/002		178
B29C2791/003	8	Making articles of indefinite length (B29C53/48 takes precedence)	CPCONLY	B29C2791/003		116
B29C2791/004	8	Shaping under special conditions	CPCONLY	B29C2791/004		68
B29C2791/005	9	Using a particular environment, e.g. sterile fluids other than air	CPCONLY	B29C2791/005		269
B29C2791/006	9	Using vacuum	CPCONLY	B29C2791/006		3139
B29C2791/007	9	Using fluid under pressure	CPCONLY	B29C2791/007		1199
B29C2791/008	9	Using vibrations during moulding	CPCONLY	B29C2791/008		417
B29C2791/009	9	Using laser	CPCONLY	B29C2791/009		480
B29C2793/00	7	Shaping techniques involving a cutting or machining operation	CPCONLY	B29C2793/00		1118
B29C2793/0009	8	Cutting out	CPCONLY	B29C2793/0009		441
B29C2793/0018	9	for making a hole	CPCONLY	B29C2793/0018		449
B29C2793/0027	8	Cutting off	CPCONLY	B29C2793/0027		1424
B29C2793/0036	8	Slitting	CPCONLY	B29C2793/0036		270
B29C2793/0045	8	Perforating	CPCONLY	B29C2793/0045		970
B29C2793/0054	8	partially cutting through the material	CPCONLY	B29C2793/0054		309
B29C2793/0063	8	Cutting longitudinally	CPCONLY	B29C2793/0063		734
B29C2793/0072	8	combined with rearranging and joining the cut parts	CPCONLY	B29C2793/0072		104
B29C2793/0081	8	before shaping	CPCONLY	B29C2793/0081		1531
B29C2793/009	8	after shaping	CPCONLY	B29C2793/009		3039
B29C2795/00	7	Printing on articles made from plastics or substances in a plastic state	CPCONLY	B29C2795/00		185
B29C2795/002	8	before shaping	CPCONLY	B29C2795/002		488
B29C2795/005	8	during shaping	CPCONLY	B29C2795/005		55
B29C2795/007	8	after shaping	CPCONLY	B29C2795/007		266
B29C2945/00	7	Indexing scheme relating to injection moulding, i.e. forcing the required volume of moulding material through a nozzle into a closed mould	CPCONLY	B29C2945/00		8
B29C2945/76	8	Measuring, controlling or regulating	CPCONLY	B29C2945/76		28
B29C2945/76003	9	Measured parameter	CPCONLY	B29C2945/76003		94
B29C2945/76006	10	Pressure	CPCONLY	B29C2945/76006		1160
B29C2945/7601	11	derivative, change thereof	CPCONLY	B29C2945/7601		41
B29C2945/76013	10	Force	CPCONLY	B29C2945/76013		214
B29C2945/76016	11	derivative, change thereof	CPCONLY	B29C2945/76016		12
B29C2945/7602	10	Torque	CPCONLY	B29C2945/7602		96
B29C2945/76023	11	derivative, change thereof	CPCONLY	B29C2945/76023		6
B29C2945/76026	10	Energy, power	CPCONLY	B29C2945/76026		39
B29C2945/7603	11	Power	CPCONLY	B29C2945/7603		21
B29C2945/76033	10	Electric current or voltage	CPCONLY	B29C2945/76033		102
B29C2945/76036	10	Frequency	CPCONLY	B29C2945/76036		20
B29C2945/7604	10	Temperature	CPCONLY	B29C2945/7604		1144
B29C2945/76043	11	derivative, change thereof	CPCONLY	B29C2945/76043		24
B29C2945/76046	11	Heat flux, heat transfer	CPCONLY	B29C2945/76046		6
B29C2945/7605	10	Viscosity	CPCONLY	B29C2945/7605		66
B29C2945/76053	11	derivative, change thereof	CPCONLY	B29C2945/76053		2
B29C2945/76056	10	Flow rate	CPCONLY	B29C2945/76056		130
B29C2945/7606	11	derivative, change thereof	CPCONLY	B29C2945/7606		10
B29C2945/76063	11	MFI, MFR	CPCONLY	B29C2945/76063		19
B29C2945/76066	10	Time	CPCONLY	B29C2945/76066		101
B29C2945/7607	11	start	CPCONLY	B29C2945/7607		13
B29C2945/76073	11	termination	CPCONLY	B29C2945/76073		11
B29C2945/76076	11	duration	CPCONLY	B29C2945/76076		91
B29C2945/7608	11	pause, wilful interruption	CPCONLY	B29C2945/7608		4
B29C2945/76083	10	Position	CPCONLY	B29C2945/76083		473
B29C2945/76086	11	Start position	CPCONLY	B29C2945/76086		14
B29C2945/7609	11	End position	CPCONLY	B29C2945/7609		23
B29C2945/76093	11	Angular position	CPCONLY	B29C2945/76093		42
B29C2945/76096	11	Distance	CPCONLY	B29C2945/76096		126
B29C2945/761	10	Dimensions, e.g. thickness	CPCONLY	B29C2945/761		149
B29C2945/76103	11	shrinkage, dilation, dimensional change, warpage	CPCONLY	B29C2945/76103		66
B29C2945/76107	11	volume	CPCONLY	B29C2945/76107		36
B29C2945/7611	10	Velocity	CPCONLY	B29C2945/7611		155
B29C2945/76113	11	linear movement	CPCONLY	B29C2945/76113		64
B29C2945/76117	12	derivative, change thereof	CPCONLY	B29C2945/76117		15
B29C2945/7612	11	rotational movement	CPCONLY	B29C2945/7612		73
B29C2945/76123	12	derivative, change thereof	CPCONLY	B29C2945/76123		1
B29C2945/76127	10	Density	CPCONLY	B29C2945/76127		16
B29C2945/7613	10	Weight	CPCONLY	B29C2945/7613		122
B29C2945/76133	10	Crystallinity	CPCONLY	B29C2945/76133		7
B29C2945/76137	10	Degree of crosslinking, solidification	CPCONLY	B29C2945/76137		9
B29C2945/7614	10	Humidity, moisture	CPCONLY	B29C2945/7614		59
B29C2945/76143	10	Volatiles	CPCONLY	B29C2945/76143		8
B29C2945/76147	10	Contaminants	CPCONLY	B29C2945/76147		25
B29C2945/7615	10	Electrical properties	CPCONLY	B29C2945/7615		20
B29C2945/76153	10	Optical properties	CPCONLY	B29C2945/76153		61
B29C2945/76157	10	Magnetic properties	CPCONLY	B29C2945/76157		12
B29C2945/7616	10	Surface properties	CPCONLY	B29C2945/7616		35
B29C2945/76163	10	Errors, malfunctioning	CPCONLY	B29C2945/76163		223
B29C2945/76167	10	Presence, absence of objects	CPCONLY	B29C2945/76167		129
B29C2945/7617	10	Sequence, e.g. the order in which operations are conducted	CPCONLY	B29C2945/7617		20
B29C2945/76177	9	Location of measurement	CPCONLY	B29C2945/76177		21
B29C2945/7618	10	Injection unit	CPCONLY	B29C2945/7618		126
B29C2945/76183	11	hopper	CPCONLY	B29C2945/76183		56
B29C2945/76187	11	screw	CPCONLY	B29C2945/76187		269
B29C2945/7619	11	barrel	CPCONLY	B29C2945/7619		139
B29C2945/76193	12	barrel-chamber	CPCONLY	B29C2945/76193		38
B29C2945/76197	13	screw ante-chamber	CPCONLY	B29C2945/76197		23
B29C2945/762	11	injection piston	CPCONLY	B29C2945/762		34
B29C2945/76204	11	injection piston cylinder	CPCONLY	B29C2945/76204		35
B29C2945/76207	11	accumulators	CPCONLY	B29C2945/76207		6
B29C2945/7621	11	nozzle	CPCONLY	B29C2945/7621		107
B29C2945/76214	11	drive means	CPCONLY	B29C2945/76214		139
B29C2945/76217	11	nozzle-touch mechanism	CPCONLY	B29C2945/76217		6
B29C2945/76224	10	Closure or clamping unit	CPCONLY	B29C2945/76224		99
B29C2945/76227	11	mould platen	CPCONLY	B29C2945/76227		80
B29C2945/7623	11	clamping or closing drive means	CPCONLY	B29C2945/7623		100
B29C2945/76234	11	tie-bars	CPCONLY	B29C2945/76234		60
B29C2945/7624	10	Ejection unit	CPCONLY	B29C2945/7624		24
B29C2945/76244	11	ejectors	CPCONLY	B29C2945/76244		50
B29C2945/76247	12	drive means thereof	CPCONLY	B29C2945/76247		34
B29C2945/76254	10	Mould	CPCONLY	B29C2945/76254		417
B29C2945/76257	11	cavity	CPCONLY	B29C2945/76257		325
B29C2945/7626	12	cavity walls	CPCONLY	B29C2945/7626		92
B29C2945/76264	13	movable	CPCONLY	B29C2945/76264		23
B29C2945/76267	11	non-cavity forming parts	CPCONLY	B29C2945/76267		19
B29C2945/7627	12	movable	CPCONLY	B29C2945/7627		10
B29C2945/76274	11	runners, nozzles	CPCONLY	B29C2945/76274		77
B29C2945/76277	12	nozzles	CPCONLY	B29C2945/76277		85
B29C2945/7628	12	manifolds	CPCONLY	B29C2945/7628		45
B29C2945/76287	10	Moulding material	CPCONLY	B29C2945/76287		201
B29C2945/7629	10	Moulded articles	CPCONLY	B29C2945/7629		337
B29C2945/76294	10	Inserts	CPCONLY	B29C2945/76294		108
B29C2945/76297	10	Fluids	CPCONLY	B29C2945/76297		29
B29C2945/76301	11	auxiliary fluids introduced into the cavity	CPCONLY	B29C2945/76301		19
B29C2945/76304	11	temperature control fluids	CPCONLY	B29C2945/76304		57
B29C2945/76307	11	hydraulic fluids	CPCONLY	B29C2945/76307		65
B29C2945/76311	11	environment	CPCONLY	B29C2945/76311		3
B29C2945/76314	10	Auxiliary devices	CPCONLY	B29C2945/76314		21
B29C2945/76317	11	robots, grippers	CPCONLY	B29C2945/76317		38
B29C2945/76321	11	conveyors	CPCONLY	B29C2945/76321		16
B29C2945/76324	11	pre-treatment devices	CPCONLY	B29C2945/76324		1
B29C2945/76327	11	post-treatment devices	CPCONLY	B29C2945/76327		6
B29C2945/76331	11	raw material feeding devices	CPCONLY	B29C2945/76331		24
B29C2945/76334	11	auxiliary fluid supplying devices	CPCONLY	B29C2945/76334		12
B29C2945/76344	9	Phase or stage of measurement	CPCONLY	B29C2945/76344		14
B29C2945/76347	10	Pre-treatment	CPCONLY	B29C2945/76347		12
B29C2945/76351	10	Feeding	CPCONLY	B29C2945/76351		33
B29C2945/76354	11	raw materials	CPCONLY	B29C2945/76354		61
B29C2945/76357	11	inserts	CPCONLY	B29C2945/76357		41
B29C2945/76361	11	auxiliary fluids, e.g. gas, liquid	CPCONLY	B29C2945/76361		10
B29C2945/76367	10	Metering	CPCONLY	B29C2945/76367		138
B29C2945/76371	10	Intrusion	CPCONLY	B29C2945/76371		3
B29C2945/76374	10	Pre-compression prior to injection	CPCONLY	B29C2945/76374		6
B29C2945/76377	10	De-compression after injection	CPCONLY	B29C2945/76377		9
B29C2945/76381	10	Injection	CPCONLY	B29C2945/76381		454
B29C2945/76384	10	Holding, dwelling	CPCONLY	B29C2945/76384		94
B29C2945/76387	10	Mould closing	CPCONLY	B29C2945/76387		138
B29C2945/76391	10	Mould clamping, compression of the cavity	CPCONLY	B29C2945/76391		118
B29C2945/76394	10	Mould opening	CPCONLY	B29C2945/76394		66
B29C2945/76397	10	Switch-over	CPCONLY	B29C2945/76397		8
B29C2945/76401	11	metering-injection	CPCONLY	B29C2945/76401		14
B29C2945/76404	11	injection-holding	CPCONLY	B29C2945/76404		30
B29C2945/76408	11	holding-metering	CPCONLY	B29C2945/76408		8
B29C2945/76414	10	Solidification, setting phase	CPCONLY	B29C2945/76414		29
B29C2945/76418	10	Ejection	CPCONLY	B29C2945/76418		58
B29C2945/76421	10	Removing or handling ejected articles	CPCONLY	B29C2945/76421		87
B29C2945/76424	10	After-treatment	CPCONLY	B29C2945/76424		7
B29C2945/76428	10	Purging	CPCONLY	B29C2945/76428		17
B29C2945/76431	10	Calibration, e.g. zero-point correction	CPCONLY	B29C2945/76431		11
B29C2945/76434	10	Parameter setting	CPCONLY	B29C2945/76434		34
B29C2945/76438	10	Start up	CPCONLY	B29C2945/76438		17
B29C2945/76441	10	Shut down	CPCONLY	B29C2945/76441		2
B29C2945/76444	11	in case of emergency	CPCONLY	B29C2945/76444		2
B29C2945/76451	9	Measurement means	CPCONLY	B29C2945/76451		44
B29C2945/76454	10	Electrical, e.g. thermocouples	CPCONLY	B29C2945/76454		148
B29C2945/76458	11	piezoelectric	CPCONLY	B29C2945/76458		51
B29C2945/76461	10	Optical, e.g. laser	CPCONLY	B29C2945/76461		213
B29C2945/76464	11	cameras	CPCONLY	B29C2945/76464		181
B29C2945/76468	10	Manual	CPCONLY	B29C2945/76468		6
B29C2945/76471	10	Acoustic	CPCONLY	B29C2945/76471		26
B29C2945/76474	10	Ultrasonic	CPCONLY	B29C2945/76474		41
B29C2945/76478	10	Mechanical	CPCONLY	B29C2945/76478		24
B29C2945/76481	10	Strain gauges	CPCONLY	B29C2945/76481		86
B29C2945/76484	10	Fluid type	CPCONLY	B29C2945/76484		10
B29C2945/76488	10	Magnetic, electro-magnetic	CPCONLY	B29C2945/76488		44
B29C2945/76494	9	Controlled parameter	CPCONLY	B29C2945/76494		76
B29C2945/76498	10	Pressure	CPCONLY	B29C2945/76498		1518
B29C2945/76501	11	derivative, change thereof	CPCONLY	B29C2945/76501		21
B29C2945/76505	10	Force	CPCONLY	B29C2945/76505		143
B29C2945/76508	11	derivative, change thereof	CPCONLY	B29C2945/76508		3
B29C2945/76511	10	Torque	CPCONLY	B29C2945/76511		41
B29C2945/76515	11	derivative, change thereof	CPCONLY	B29C2945/76515		1
B29C2945/76518	10	Energy, power	CPCONLY	B29C2945/76518		55
B29C2945/76521	11	power	CPCONLY	B29C2945/76521		39
B29C2945/76525	10	Electric current or voltage	CPCONLY	B29C2945/76525		105
B29C2945/76528	10	Frequency	CPCONLY	B29C2945/76528		13
B29C2945/76531	10	Temperature	CPCONLY	B29C2945/76531		2265
B29C2945/76535	11	derivative, change thereof	CPCONLY	B29C2945/76535		12
B29C2945/76538	10	Viscosity	CPCONLY	B29C2945/76538		46
B29C2945/76541	11	derivative, change thereof	CPCONLY	B29C2945/76541		2
B29C2945/76545	10	Flow rate	CPCONLY	B29C2945/76545		355
B29C2945/76548	11	derivative, change thereof	CPCONLY	B29C2945/76548		12
B29C2945/76551	10	Time	CPCONLY	B29C2945/76551		199
B29C2945/76555	11	start	CPCONLY	B29C2945/76555		44
B29C2945/76558	11	termination	CPCONLY	B29C2945/76558		28
B29C2945/76561	11	duration	CPCONLY	B29C2945/76561		312
B29C2945/76565	11	pause, wilful interruption	CPCONLY	B29C2945/76565		10
B29C2945/76568	10	Position	CPCONLY	B29C2945/76568		407
B29C2945/76571	11	start position	CPCONLY	B29C2945/76571		13
B29C2945/76575	11	end position	CPCONLY	B29C2945/76575		33
B29C2945/76578	11	angular position	CPCONLY	B29C2945/76578		17
B29C2945/76581	11	distance	CPCONLY	B29C2945/76581		63
B29C2945/76585	10	Dimensions, e.g. thickness	CPCONLY	B29C2945/76585		64
B29C2945/76588	11	shrinkage, dilation, dimensional change, warpage	CPCONLY	B29C2945/76588		36
B29C2945/76591	11	volume	CPCONLY	B29C2945/76591		53
B29C2945/76595	10	Velocity	CPCONLY	B29C2945/76595		424
B29C2945/76598	11	linear movement	CPCONLY	B29C2945/76598		138
B29C2945/76602	12	derivative, change thereof	CPCONLY	B29C2945/76602		24
B29C2945/76605	11	rotational movement	CPCONLY	B29C2945/76605		167
B29C2945/76608	12	derivative, change thereof	CPCONLY	B29C2945/76608		6
B29C2945/76612	10	Density	CPCONLY	B29C2945/76612		9
B29C2945/76615	10	Weight	CPCONLY	B29C2945/76615		41
B29C2945/76618	10	Crystallinity	CPCONLY	B29C2945/76618		8
B29C2945/76622	10	Degree of crosslinking, solidification	CPCONLY	B29C2945/76622		7
B29C2945/76625	10	Humidity, moisture	CPCONLY	B29C2945/76625		23
B29C2945/76628	10	Volatiles	CPCONLY	B29C2945/76628		1
B29C2945/76632	10	Contaminants	CPCONLY	B29C2945/76632		6
B29C2945/76635	10	Electrical properties	CPCONLY	B29C2945/76635		13
B29C2945/76638	10	Optical properties	CPCONLY	B29C2945/76638		10
B29C2945/76642	10	Magnetic properties	CPCONLY	B29C2945/76642		8
B29C2945/76645	10	Surface properties	CPCONLY	B29C2945/76645		13
B29C2945/76648	10	Sequence, e.g. the order in which operations are conducted	CPCONLY	B29C2945/76648		102
B29C2945/76655	9	Location of control	CPCONLY	B29C2945/76655		14
B29C2945/76658	10	Injection unit	CPCONLY	B29C2945/76658		180
B29C2945/76662	11	hopper	CPCONLY	B29C2945/76662		91
B29C2945/76665	11	screw	CPCONLY	B29C2945/76665		259
B29C2945/76668	11	barrel	CPCONLY	B29C2945/76668		154
B29C2945/76672	12	barrel-chamber	CPCONLY	B29C2945/76672		16
B29C2945/76675	13	screw ante-chamber	CPCONLY	B29C2945/76675		11
B29C2945/76678	11	injection piston	CPCONLY	B29C2945/76678		46
B29C2945/76682	11	injection piston cylinder	CPCONLY	B29C2945/76682		31
B29C2945/76685	11	accumulators	CPCONLY	B29C2945/76685		6
B29C2945/76688	11	nozzle	CPCONLY	B29C2945/76688		114
B29C2945/76692	11	drive means	CPCONLY	B29C2945/76692		92
B29C2945/76695	11	nozzle-touch mechanism	CPCONLY	B29C2945/76695		11
B29C2945/76702	10	Closure or clamping device	CPCONLY	B29C2945/76702		116
B29C2945/76705	11	mould platen	CPCONLY	B29C2945/76705		42
B29C2945/76709	11	clamping or closing drive means	CPCONLY	B29C2945/76709		122
B29C2945/76712	11	tie-bars	CPCONLY	B29C2945/76712		15
B29C2945/76719	10	Ejection unit	CPCONLY	B29C2945/76719		20
B29C2945/76722	11	ejectors	CPCONLY	B29C2945/76722		32
B29C2945/76725	12	drive means thereof	CPCONLY	B29C2945/76725		24
B29C2945/76732	10	Mould	CPCONLY	B29C2945/76732		580
B29C2945/76735	11	cavity	CPCONLY	B29C2945/76735		146
B29C2945/76739	12	cavity walls	CPCONLY	B29C2945/76739		20
B29C2945/76742	13	movable	CPCONLY	B29C2945/76742		41
B29C2945/76745	11	non-cavity forming parts	CPCONLY	B29C2945/76745		10
B29C2945/76749	12	movable	CPCONLY	B29C2945/76749		11
B29C2945/76752	11	runners, nozzles	CPCONLY	B29C2945/76752		129
B29C2945/76755	12	nozzles	CPCONLY	B29C2945/76755		93
B29C2945/76759	12	manifolds	CPCONLY	B29C2945/76759		24
B29C2945/76765	10	Moulding material	CPCONLY	B29C2945/76765		174
B29C2945/76769	10	Moulded articles	CPCONLY	B29C2945/76769		89
B29C2945/76772	10	Inserts	CPCONLY	B29C2945/76772		36
B29C2945/76775	10	Fluids	CPCONLY	B29C2945/76775		30
B29C2945/76779	11	auxiliary fluids introduced into the cavity	CPCONLY	B29C2945/76779		27
B29C2945/76782	11	temperature control fluids	CPCONLY	B29C2945/76782		81
B29C2945/76785	11	hydraulic fluids	CPCONLY	B29C2945/76785		124
B29C2945/76789	11	environment	CPCONLY	B29C2945/76789		3
B29C2945/76792	10	Auxiliary devices	CPCONLY	B29C2945/76792		42
B29C2945/76795	11	robots, grippers	CPCONLY	B29C2945/76795		73
B29C2945/76799	11	conveyors	CPCONLY	B29C2945/76799		7
B29C2945/76802	11	pre-treatment devices	CPCONLY	B29C2945/76802		4
B29C2945/76806	11	post-treatment devices	CPCONLY	B29C2945/76806		16
B29C2945/76809	11	raw material feeding devices	CPCONLY	B29C2945/76809		29
B29C2945/76812	11	Auxiliary fluid supplying devices	CPCONLY	B29C2945/76812		30
B29C2945/76822	9	Phase or stage of control	CPCONLY	B29C2945/76822		19
B29C2945/76826	10	Pre-treatment	CPCONLY	B29C2945/76826		19
B29C2945/76829	10	Feeding	CPCONLY	B29C2945/76829		61
B29C2945/76832	11	raw materials	CPCONLY	B29C2945/76832		105
B29C2945/76836	11	inserts	CPCONLY	B29C2945/76836		24
B29C2945/76839	11	auxiliary fluids, e.g. gas, liquid	CPCONLY	B29C2945/76839		21
B29C2945/76846	10	Metering	CPCONLY	B29C2945/76846		99
B29C2945/76849	10	Intrusion	CPCONLY	B29C2945/76849		3
B29C2945/76852	10	Pre-compression prior to injection	CPCONLY	B29C2945/76852		14
B29C2945/76856	10	De-compression after injection	CPCONLY	B29C2945/76856		23
B29C2945/76859	10	Injection	CPCONLY	B29C2945/76859		641
B29C2945/76862	10	Holding, dwelling	CPCONLY	B29C2945/76862		156
B29C2945/76866	10	Mould closing	CPCONLY	B29C2945/76866		170
B29C2945/76869	10	Mould clamping, compression of the cavity	CPCONLY	B29C2945/76869		147
B29C2945/76872	10	Mould opening	CPCONLY	B29C2945/76872		108
B29C2945/76876	10	Switch-over	CPCONLY	B29C2945/76876		25
B29C2945/76879	11	metering-injection	CPCONLY	B29C2945/76879		13
B29C2945/76882	11	injection-holding	CPCONLY	B29C2945/76882		34
B29C2945/76886	11	holding-metering	CPCONLY	B29C2945/76886		3
B29C2945/76892	10	Solidification, setting phase	CPCONLY	B29C2945/76892		49
B29C2945/76896	10	Ejection	CPCONLY	B29C2945/76896		69
B29C2945/76899	10	Removing or handling ejected articles	CPCONLY	B29C2945/76899		121
B29C2945/76903	10	After-treatment	CPCONLY	B29C2945/76903		21
B29C2945/76906	10	Purging	CPCONLY	B29C2945/76906		19
B29C2945/76909	10	Calibration, e.g. zero-point correction	CPCONLY	B29C2945/76909		3
B29C2945/76913	10	Parameter setting	CPCONLY	B29C2945/76913		96
B29C2945/76916	10	Start up	CPCONLY	B29C2945/76916		17
B29C2945/76919	10	Shut down	CPCONLY	B29C2945/76919		14
B29C2945/76923	11	in case of emergency	CPCONLY	B29C2945/76923		12
B29C2945/76929	9	Controlling method	CPCONLY	B29C2945/76929		55
B29C2945/76933	10	The operating conditions are corrected immediately, during the same phase or cycle	CPCONLY	B29C2945/76933		213
B29C2945/76936	10	The operating conditions are corrected in the next phase or cycle	CPCONLY	B29C2945/76936		190
B29C2945/76939	10	Using stored or historical data sets	CPCONLY	B29C2945/76939		412
B29C2945/76943	11	compare with thresholds	CPCONLY	B29C2945/76943		388
B29C2945/76946	11	using an expert system, i.e. the system possesses a database in which human experience is stored, e.g. to help interfering the possible cause of a fault	CPCONLY	B29C2945/76946		79
B29C2945/76949	11	using a learning system, i.e. the system accumulates experience from previous occurrences, e.g. adaptive control	CPCONLY	B29C2945/76949		190
B29C2945/76953	10	Distributed, i.e. several control units perform different tasks	CPCONLY	B29C2945/76953		23
B29C2945/76956	10	Proportional	CPCONLY	B29C2945/76956		13
B29C2945/76959	11	and derivative, i.e. PD regulation	CPCONLY	B29C2945/76959		6
B29C2945/76963	12	using a second derivative, e.g. determination of inflexion points	CPCONLY	B29C2945/76963		3
B29C2945/76966	11	and integral, i.e. Pl regulation	CPCONLY	B29C2945/76966		11
B29C2945/76969	12	derivative and integral, i.e. PID regulation	CPCONLY	B29C2945/76969		57
B29C2945/76973	10	By counting	CPCONLY	B29C2945/76973		256
B29C2945/76976	10	By trial and error, trial tests	CPCONLY	B29C2945/76976		21
B29C2945/76979	10	Using a neural network	CPCONLY	B29C2945/76979		90
B29C2945/76983	10	Using fuzzy logic	CPCONLY	B29C2945/76983		18
B29C2945/76986	10	Interpolating	CPCONLY	B29C2945/76986		10
B29C2945/76989	10	Extrapolating	CPCONLY	B29C2945/76989		19
B29C2945/76993	10	Remote, e.g. LAN, wireless LAN	CPCONLY	B29C2945/76993		243
B29C2948/00	7	Indexing scheme relating to extrusion moulding	CPCONLY	B29C2948/00		9
B29C2948/92	8	Measuring, controlling or regulating	CPCONLY	B29C2948/92		23
B29C2948/92009	9	Measured parameter	CPCONLY	B29C2948/92009		42
B29C2948/92019	10	Pressure	CPCONLY	B29C2948/92019		1227
B29C2948/92028	10	Force; Tension	CPCONLY	B29C2948/92028		100
B29C2948/92038	10	Torque	CPCONLY	B29C2948/92038		118
B29C2948/92047	10	Energy, power, electric current or voltage	CPCONLY	B29C2948/92047		107
B29C2948/92057	10	Frequency	CPCONLY	B29C2948/92057		25
B29C2948/92066	10	Time, e.g. start, termination, duration or interruption	CPCONLY	B29C2948/92066		92
B29C2948/92076	10	Position, e.g. linear or angular	CPCONLY	B29C2948/92076		426
B29C2948/92085	10	Velocity	CPCONLY	B29C2948/92085		290
B29C2948/92095	11	Angular velocity	CPCONLY	B29C2948/92095		296
B29C2948/92104	11	Flow or feed rate	CPCONLY	B29C2948/92104		411
B29C2948/92114	10	Dimensions	CPCONLY	B29C2948/92114		246
B29C2948/92123	11	Diameter or circumference	CPCONLY	B29C2948/92123		346
B29C2948/92133	11	Width or height	CPCONLY	B29C2948/92133		169
B29C2948/92142	11	Length	CPCONLY	B29C2948/92142		163
B29C2948/92152	11	Thickness	CPCONLY	B29C2948/92152		1036
B29C2948/92161	11	Volume or quantity	CPCONLY	B29C2948/92161		170
B29C2948/92171	11	Distortion, shrinkage, dilatation, swell or warpage	CPCONLY	B29C2948/92171		111
B29C2948/9218	10	Weight	CPCONLY	B29C2948/9218		351
B29C2948/9219	10	Density, e.g. per unit length or area	CPCONLY	B29C2948/9219		61
B29C2948/922	10	Viscosity; Melt flow index [MFI]; Molecular weight	CPCONLY	B29C2948/922		245
B29C2948/92209	10	Temperature	CPCONLY	B29C2948/92209		1793
B29C2948/92219	10	Degree of crosslinking, solidification, crystallinity or homogeneity	CPCONLY	B29C2948/92219		56
B29C2948/92228	10	Content, e.g. percentage of humidity, volatiles, contaminants or degassing	CPCONLY	B29C2948/92228		113
B29C2948/92238	10	Electrical properties	CPCONLY	B29C2948/92238		87
B29C2948/92247	10	Optical properties	CPCONLY	B29C2948/92247		124
B29C2948/92257	11	Colour	CPCONLY	B29C2948/92257		50
B29C2948/92266	10	Mechanical properties	CPCONLY	B29C2948/92266		85
B29C2948/92276	10	Magnetic properties	CPCONLY	B29C2948/92276		15
B29C2948/92285	10	Surface properties	CPCONLY	B29C2948/92285		75
B29C2948/92295	10	Errors or malfunctioning, e.g. for quality control	CPCONLY	B29C2948/92295		174
B29C2948/92304	10	Presence or absence; Sequence; Counting	CPCONLY	B29C2948/92304		80
B29C2948/92314	10	Particular value claimed	CPCONLY	B29C2948/92314		247
B29C2948/92323	9	Location or phase of measurement	CPCONLY	B29C2948/92323		3
B29C2948/92333	10	Raw material handling or dosing, e.g. active hopper or feeding device	CPCONLY	B29C2948/92333		284
B29C2948/92342	10	Raw material pre-treatment, e.g. drying or cleaning	CPCONLY	B29C2948/92342		29
B29C2948/92352	10	Inserts	CPCONLY	B29C2948/92352		39
B29C2948/92361	10	Extrusion unit	CPCONLY	B29C2948/92361		118
B29C2948/92371	11	Inlet shaft or slot, e.g. passive hopper; Injector, e.g. injector nozzle on barrel	CPCONLY	B29C2948/92371		65
B29C2948/9238	11	Feeding, melting, plasticising or pumping zones, e.g. the melt itself	CPCONLY	B29C2948/9238		396
B29C2948/9239	12	Screw or gear	CPCONLY	B29C2948/9239		258
B29C2948/924	12	Barrel or housing	CPCONLY	B29C2948/924		533
B29C2948/92409	11	Die; Nozzle zone	CPCONLY	B29C2948/92409		836
B29C2948/92419	11	Degassing unit	CPCONLY	B29C2948/92419		45
B29C2948/92428	10	Calibration, after-treatment, or cooling zone	CPCONLY	B29C2948/92428		876
B29C2948/92438	10	Conveying, transporting or storage of articles	CPCONLY	B29C2948/92438		607
B29C2948/92447	10	Moulded article	CPCONLY	B29C2948/92447		504
B29C2948/92457	10	Drive section, e.g. gearbox, motor or drive fluids	CPCONLY	B29C2948/92457		122
B29C2948/92466	10	Auxiliary unit, e.g. for external melt filtering, re-combining or transfer between units	CPCONLY	B29C2948/92466		232
B29C2948/92476	10	Fluids, e.g. for temperature control or of environment	CPCONLY	B29C2948/92476		68
B29C2948/92485	10	Start-up, shut-down or parameter setting phase; Emergency shut-down; Material change; Test or laboratory equipment or studies	CPCONLY	B29C2948/92485		163
B29C2948/92495	10	Treatment of equipment, e.g. purging, cleaning, lubricating or filter exchange	CPCONLY	B29C2948/92495		26
B29C2948/92504	9	Controlled parameter	CPCONLY	B29C2948/92504		38
B29C2948/92514	10	Pressure	CPCONLY	B29C2948/92514		2463
B29C2948/92523	10	Force; Tension	CPCONLY	B29C2948/92523		186
B29C2948/92533	10	Torque	CPCONLY	B29C2948/92533		90
B29C2948/92542	10	Energy, power, electric current or voltage	CPCONLY	B29C2948/92542		250
B29C2948/92552	10	Frequency	CPCONLY	B29C2948/92552		57
B29C2948/92561	10	Time, e.g. start, termination, duration or interruption	CPCONLY	B29C2948/92561		695
B29C2948/92571	10	Position, e.g. linear or angular	CPCONLY	B29C2948/92571		679
B29C2948/9258	10	Velocity	CPCONLY	B29C2948/9258		2436
B29C2948/9259	11	Angular velocity	CPCONLY	B29C2948/9259		3803
B29C2948/926	11	Flow or feed rate	CPCONLY	B29C2948/926		1866
B29C2948/92609	10	Dimensions	CPCONLY	B29C2948/92609		329
B29C2948/92619	11	Diameter or circumference	CPCONLY	B29C2948/92619		379
B29C2948/92628	11	Width or height	CPCONLY	B29C2948/92628		250
B29C2948/92638	11	Length	CPCONLY	B29C2948/92638		231
B29C2948/92647	11	Thickness	CPCONLY	B29C2948/92647		1647
B29C2948/92657	11	Volume or quantity	CPCONLY	B29C2948/92657		279
B29C2948/92666	11	Distortion, shrinkage, dilatation, swell or warpage	CPCONLY	B29C2948/92666		127
B29C2948/92676	10	Weight	CPCONLY	B29C2948/92676		237
B29C2948/92685	10	Density, e.g. per unit length or area	CPCONLY	B29C2948/92685		72
B29C2948/92695	10	Viscosity; Melt flow index [MFI]; Molecular weight	CPCONLY	B29C2948/92695		275
B29C2948/92704	10	Temperature	CPCONLY	B29C2948/92704		12300
B29C2948/92714	10	Degree of crosslinking, solidification, crystallinity or homogeneity	CPCONLY	B29C2948/92714		111
B29C2948/92723	10	Content, e.g. percentage of humidity, volatiles, contaminants or degassing	CPCONLY	B29C2948/92723		197
B29C2948/92733	10	Electrical properties	CPCONLY	B29C2948/92733		55
B29C2948/92742	10	Optical properties	CPCONLY	B29C2948/92742		45
B29C2948/92752	11	Colour	CPCONLY	B29C2948/92752		65
B29C2948/92761	10	Mechanical properties	CPCONLY	B29C2948/92761		91
B29C2948/92771	10	Magnetic properties	CPCONLY	B29C2948/92771		6
B29C2948/9278	10	Surface properties	CPCONLY	B29C2948/9278		39
B29C2948/9279	10	Errors or malfunctioning, e.g. for quality control	CPCONLY	B29C2948/9279		177
B29C2948/928	10	Presence or absence; Sequence; Counting	CPCONLY	B29C2948/928		29
B29C2948/92809	10	Particular value claimed	CPCONLY	B29C2948/92809		273
B29C2948/92819	9	Location or phase of control	CPCONLY	B29C2948/92819		4
B29C2948/92828	10	Raw material handling or dosing, e.g. active hopper or feeding device	CPCONLY	B29C2948/92828		796
B29C2948/92838	10	Raw material pre-treatment, e.g. drying or cleaning	CPCONLY	B29C2948/92838		88
B29C2948/92847	10	Inserts	CPCONLY	B29C2948/92847		63
B29C2948/92857	10	Extrusion unit	CPCONLY	B29C2948/92857		297
B29C2948/92866	11	Inlet shaft or slot, e.g. passive hopper; Injector, e.g. injector nozzle on barrel	CPCONLY	B29C2948/92866		194
B29C2948/92876	11	Feeding, melting, plasticising or pumping zones, e.g. the melt itself	CPCONLY	B29C2948/92876		708
B29C2948/92885	12	Screw or gear	CPCONLY	B29C2948/92885		2632
B29C2948/92895	12	Barrel or housing	CPCONLY	B29C2948/92895		4512
B29C2948/92904	11	Die; Nozzle zone	CPCONLY	B29C2948/92904		3178
B29C2948/92914	11	Degassing unit	CPCONLY	B29C2948/92914		63
B29C2948/92923	10	Calibration, after-treatment or cooling zone	CPCONLY	B29C2948/92923		1673
B29C2948/92933	10	Conveying, transporting or storage of articles	CPCONLY	B29C2948/92933		892
B29C2948/92942	10	Moulded article	CPCONLY	B29C2948/92942		422
B29C2948/92952	10	Drive section, e.g. gearbox, motor or drive fluids	CPCONLY	B29C2948/92952		624
B29C2948/92961	10	Auxiliary unit, e.g. for external melt filtering, re-combining or transfer between units	CPCONLY	B29C2948/92961		326
B29C2948/92971	10	Fluids, e.g. for temperature control or of environment	CPCONLY	B29C2948/92971		324
B29C2948/9298	10	Start-up, shut-down or parameter setting phase; Emergency shut-down; Material change; Test or laboratory equipment or studies	CPCONLY	B29C2948/9298		234
B29C2948/9299	10	Treatment of equipment, e.g. purging, cleaning, lubricating or filter exchange	CPCONLY	B29C2948/9299		40
B29C2949/00	7	Indexing scheme relating to blow-moulding	CPCONLY	B29C2949/00		10
B29C2949/07	8	Preforms or parisons characterised by their configuration	CPCONLY	B29C2949/07		10
B29C2949/071	9	the preform being a tube, i.e. with both ends open	CPCONLY	B29C2949/071		37
B29C2949/0715	9	the preform having one end closed	CPCONLY	B29C2949/0715		5040
B29C2949/072	9	having variable wall thickness	CPCONLY	B29C2949/072		827
B29C2949/0721	10	Tangentially varying thickness	CPCONLY	B29C2949/0721		79
B29C2949/0722	10	at neck portion	CPCONLY	B29C2949/0722		201
B29C2949/0723	10	at flange portion	CPCONLY	B29C2949/0723		243
B29C2949/0724	10	at body portion	CPCONLY	B29C2949/0724		364
B29C2949/0725	10	at bottom portion	CPCONLY	B29C2949/0725		211
B29C2949/073	9	having variable diameter	CPCONLY	B29C2949/073		755
B29C2949/0731	10	at neck portion	CPCONLY	B29C2949/0731		240
B29C2949/0732	10	at flange portion	CPCONLY	B29C2949/0732		252
B29C2949/0733	10	at body portion	CPCONLY	B29C2949/0733		451
B29C2949/0734	10	at bottom portion	CPCONLY	B29C2949/0734		33
B29C2949/074	9	having ribs or protrusions	CPCONLY	B29C2949/074		202
B29C2949/0741	10	longitudinal, e.g. from top to bottom	CPCONLY	B29C2949/0741		53
B29C2949/0742	10	Circumferential	CPCONLY	B29C2949/0742		24
B29C2949/0744	10	at neck portion	CPCONLY	B29C2949/0744		80
B29C2949/0745	10	at flange portion	CPCONLY	B29C2949/0745		42
B29C2949/0746	10	at body portion	CPCONLY	B29C2949/0746		79
B29C2949/0747	10	at bottom portion	CPCONLY	B29C2949/0747		67
B29C2949/075	9	having at least one internal separating wall	CPCONLY	B29C2949/075		60
B29C2949/0751	10	at neck portion	CPCONLY	B29C2949/0751		14
B29C2949/0752	10	at flange portion	CPCONLY	B29C2949/0752		12
B29C2949/0753	10	at body portion	CPCONLY	B29C2949/0753		27
B29C2949/0754	10	at bottom portion	CPCONLY	B29C2949/0754		23
B29C2949/076	9	characterised by the shape	CPCONLY	B29C2949/076		10
B29C2949/0761	10	characterised by overall the shape	CPCONLY	B29C2949/0761		47
B29C2949/0762	11	Conical	CPCONLY	B29C2949/0762		106
B29C2949/0763	11	Axially asymmetrical	CPCONLY	B29C2949/0763		74
B29C2949/0764	11	Elliptic or oval cross-section shape	CPCONLY	B29C2949/0764		37
B29C2949/0765	11	Rectangular cross-section shape	CPCONLY	B29C2949/0765		13
B29C2949/0766	11	Hexagonal cross-section shape	CPCONLY	B29C2949/0766		18
B29C2949/0767	11	the shape allowing stacking or nesting	CPCONLY	B29C2949/0767		31
B29C2949/0768	10	characterised by the shape of specific parts of preform	CPCONLY	B29C2949/0768		2
B29C2949/0769	11	characterised by the lip, i.e. very top of preform neck	CPCONLY	B29C2949/0769		199
B29C2949/077	11	characterised by the neck	CPCONLY	B29C2949/077		295
B29C2949/0771	12	Wide-mouth	CPCONLY	B29C2949/0771		150
B29C2949/0772	12	Closure retaining means	CPCONLY	B29C2949/0772		63
B29C2949/0773	13	Threads	CPCONLY	B29C2949/0773		679
B29C2949/0774	14	Interrupted threads	CPCONLY	B29C2949/0774		108
B29C2949/0775	14	Inner threads	CPCONLY	B29C2949/0775		26
B29C2949/0776	13	not containing threads	CPCONLY	B29C2949/0776		126
B29C2949/0777	12	Tamper-evident band retaining ring	CPCONLY	B29C2949/0777		399
B29C2949/0778	11	characterised by the flange	CPCONLY	B29C2949/0778		184
B29C2949/0779	11	characterised by the body	CPCONLY	B29C2949/0779		82
B29C2949/078	11	characterised by the bottom	CPCONLY	B29C2949/078		349
B29C2949/0781	12	characterised by the sprue, i.e. injection mark	CPCONLY	B29C2949/0781		76
B29C2949/0782	12	characterised by the pinch-off portion	CPCONLY	B29C2949/0782		8
B29C2949/079	9	Auxiliary parts or inserts	CPCONLY	B29C2949/079		122
B29C2949/0791	10	Handle	CPCONLY	B29C2949/0791		70
B29C2949/0792	10	Closure	CPCONLY	B29C2949/0792		37
B29C2949/0793	10	Transport means	CPCONLY	B29C2949/0793		31
B29C2949/0794	10	Dispensing spout	CPCONLY	B29C2949/0794		31
B29C2949/0795	10	Parts to assist orientation of preform, e.g. in mould	CPCONLY	B29C2949/0795		6
B29C2949/0796	11	at neck portion	CPCONLY	B29C2949/0796		21
B29C2949/0797	11	at flange portion	CPCONLY	B29C2949/0797		20
B29C2949/0798	11	at body portion	CPCONLY	B29C2949/0798		4
B29C2949/0799	11	at bottom portion	CPCONLY	B29C2949/0799		6
B29C2949/08	10	Preforms made of several individual parts, e.g. by welding or gluing parts together	CPCONLY	B29C2949/08		578
B29C2949/0801	11	Finish neck ring	CPCONLY	B29C2949/0801		51
B29C2949/081	9	Specified dimensions, e.g. values or ranges	CPCONLY	B29C2949/081		8
B29C2949/0811	10	Wall thickness	CPCONLY	B29C2949/0811		336
B29C2949/0812	11	of the lip, i.e. the very top of the preform neck	CPCONLY	B29C2949/0812		14
B29C2949/0813	11	of the neck	CPCONLY	B29C2949/0813		73
B29C2949/0814	11	of the threads	CPCONLY	B29C2949/0814		9
B29C2949/0815	11	of the tamper-evident band retaining ring	CPCONLY	B29C2949/0815		2
B29C2949/0816	11	of the flange	CPCONLY	B29C2949/0816		31
B29C2949/0817	11	of the body	CPCONLY	B29C2949/0817		191
B29C2949/0818	11	of the bottom	CPCONLY	B29C2949/0818		90
B29C2949/0819	11	of a layer	CPCONLY	B29C2949/0819		136
B29C2949/082	10	Diameter	CPCONLY	B29C2949/082		167
B29C2949/0821	11	of the lip, i.e. the very top of the preform neck	CPCONLY	B29C2949/0821		40
B29C2949/0822	11	of the neck	CPCONLY	B29C2949/0822		98
B29C2949/0823	11	of the threads	CPCONLY	B29C2949/0823		8
B29C2949/0824	11	of the tamper-evident band retaining ring	CPCONLY	B29C2949/0824		2
B29C2949/0825	11	of the flange	CPCONLY	B29C2949/0825		35
B29C2949/0826	11	of the body	CPCONLY	B29C2949/0826		105
B29C2949/0827	11	of the bottom	CPCONLY	B29C2949/0827		32
B29C2949/0828	11	of a layer	CPCONLY	B29C2949/0828		4
B29C2949/0829	10	Height, length	CPCONLY	B29C2949/0829		229
B29C2949/083	11	of the lip, i.e. the very top of the preform neck	CPCONLY	B29C2949/083		15
B29C2949/0831	11	of the neck	CPCONLY	B29C2949/0831		67
B29C2949/0832	11	of the threads	CPCONLY	B29C2949/0832		6
B29C2949/0833	11	of the tamper-evident band retaining ring	CPCONLY	B29C2949/0833		5
B29C2949/0834	11	of the flange	CPCONLY	B29C2949/0834		15
B29C2949/0835	11	of the body	CPCONLY	B29C2949/0835		70
B29C2949/0836	11	of the bottom	CPCONLY	B29C2949/0836		34
B29C2949/0837	11	of a layer	CPCONLY	B29C2949/0837		3
B29C2949/0838	10	Ratio between length and diameter	CPCONLY	B29C2949/0838		21
B29C2949/0839	10	Angle	CPCONLY	B29C2949/0839		7
B29C2949/084	11	of the lip, i.e. the very top of the preform neck	CPCONLY	B29C2949/084		6
B29C2949/0841	11	of the neck	CPCONLY	B29C2949/0841		9
B29C2949/0842	11	of the threads	CPCONLY	B29C2949/0842		4
B29C2949/0843	11	of the tamper-evident band retaining ring	CPCONLY	B29C2949/0843		2
B29C2949/0844	11	of the flange	CPCONLY	B29C2949/0844		7
B29C2949/0845	11	of the body	CPCONLY	B29C2949/0845		22
B29C2949/0846	11	of the bottom	CPCONLY	B29C2949/0846		13
B29C2949/0847	11	of a layer	CPCONLY	B29C2949/0847		
B29C2949/0849	10	Curvature, e.g. radius	CPCONLY	B29C2949/0849		3
B29C2949/085	11	of the lip, i.e. the very top of the preform neck	CPCONLY	B29C2949/085		5
B29C2949/0851	11	of the neck	CPCONLY	B29C2949/0851		7
B29C2949/0852	11	of the threads	CPCONLY	B29C2949/0852		6
B29C2949/0853	11	of the tamper-evident band retaining ring	CPCONLY	B29C2949/0853		1
B29C2949/0854	11	of the flange	CPCONLY	B29C2949/0854		7
B29C2949/0855	11	of the body	CPCONLY	B29C2949/0855		8
B29C2949/0856	11	of the bottom	CPCONLY	B29C2949/0856		21
B29C2949/086	11	of a layer	CPCONLY	B29C2949/086		
B29C2949/0861	9	Other specified values, e.g. values or ranges	CPCONLY	B29C2949/0861		5
B29C2949/0862	10	Crystallinity	CPCONLY	B29C2949/0862		153
B29C2949/0863	11	at the neck portion	CPCONLY	B29C2949/0863		31
B29C2949/0864	11	at the flange portion	CPCONLY	B29C2949/0864		3
B29C2949/0865	11	at the body portion	CPCONLY	B29C2949/0865		23
B29C2949/0866	11	at the bottom portion	CPCONLY	B29C2949/0866		20
B29C2949/0867	10	Surface roughness	CPCONLY	B29C2949/0867		8
B29C2949/0868	11	at the neck portion	CPCONLY	B29C2949/0868		5
B29C2949/0869	11	at the flange portion	CPCONLY	B29C2949/0869		3
B29C2949/087	11	at the body portion	CPCONLY	B29C2949/087		6
B29C2949/0871	11	at the bottom portion	CPCONLY	B29C2949/0871		4
B29C2949/0872	10	Weight	CPCONLY	B29C2949/0872		217
B29C2949/20	8	Preforms or parisons whereby a specific part is made of only one component, e.g. only one layer	CPCONLY	B29C2949/20		65
B29C2949/22	9	at neck portion	CPCONLY	B29C2949/22		1486
B29C2949/24	9	at flange portion	CPCONLY	B29C2949/24		1382
B29C2949/26	9	at body portion	CPCONLY	B29C2949/26		1286
B29C2949/28	9	at bottom portion	CPCONLY	B29C2949/28		1302
B29C2949/30	8	Preforms or parisons made of several components	CPCONLY	B29C2949/30		37
B29C2949/3004	9	having longitudinally different components within one layer, e.g. tubes with longitudinal stratified layering	CPCONLY	B29C2949/3004		59
B29C2949/3006	9	having tangentially different components within one layer, e.g. longitudinal stripes	CPCONLY	B29C2949/3006		63
B29C2949/3008	9	at neck portion	CPCONLY	B29C2949/3008		639
B29C2949/3009	10	partially	CPCONLY	B29C2949/3009		134
B29C2949/3012	9	at flange portion	CPCONLY	B29C2949/3012		686
B29C2949/3014	10	partially	CPCONLY	B29C2949/3014		59
B29C2949/3016	9	at body portion	CPCONLY	B29C2949/3016		865
B29C2949/3018	10	partially	CPCONLY	B29C2949/3018		110
B29C2949/302	9	at bottom portion	CPCONLY	B29C2949/302		836
B29C2949/3022	10	partially	CPCONLY	B29C2949/3022		76
B29C2949/3024	9	characterised by the number of components or by the manufacturing technique	CPCONLY	B29C2949/3024		771
B29C2949/3026	10	having two or more components	CPCONLY	B29C2949/3026		549
B29C2949/3028	11	having three or more components	CPCONLY	B29C2949/3028		463
B29C2949/303	12	having more than three components	CPCONLY	B29C2949/303		267
B29C2949/3032	9	having components being injected	CPCONLY	B29C2949/3032		1295
B29C2949/3034	10	having two or more components being injected	CPCONLY	B29C2949/3034		351
B29C2949/3036	11	having three or more components being injected	CPCONLY	B29C2949/3036		272
B29C2949/3038	12	having more than three components being injected	CPCONLY	B29C2949/3038		161
B29C2949/3041	9	having components being extruded	CPCONLY	B29C2949/3041		311
B29C2949/3042	10	having two or more components being extruded	CPCONLY	B29C2949/3042		81
B29C2949/3044	11	having three or more components being extruded	CPCONLY	B29C2949/3044		47
B29C2949/3046	12	having more than three components being extruded	CPCONLY	B29C2949/3046		37
B29C2949/3048	9	having components being thermoformed	CPCONLY	B29C2949/3048		30
B29C2949/3051	10	having two or more components being thermoformed	CPCONLY	B29C2949/3051		14
B29C2949/3052	11	having three or more components being thermoformed	CPCONLY	B29C2949/3052		6
B29C2949/3054	12	having more than three components being thermoformed	CPCONLY	B29C2949/3054		2
B29C2949/3056	9	having components being compression moulded	CPCONLY	B29C2949/3056		137
B29C2949/3058	10	having two or more components being compression moulded	CPCONLY	B29C2949/3058		40
B29C2949/306	11	having three or more components being compression moulded	CPCONLY	B29C2949/306		60
B29C2949/3062	12	having more than three components being compression moulded	CPCONLY	B29C2949/3062		39
B29C2949/3064	9	having at least one components being applied using techniques not covered by B29C2949/3032 - B29C2949/3062	CPCONLY	B29C2949/3064		163
B29C2949/3066	10	having two or more components being applied using said techniques	CPCONLY	B29C2949/3066		57
B29C2949/3068	11	having three or more components being applied using said techniques	CPCONLY	B29C2949/3068		16
B29C2949/307	12	having more than three components being applied using said techniques	CPCONLY	B29C2949/307		11
B29C2949/3074	10	said at least one component obtained by coating	CPCONLY	B29C2949/3074		71
B29C2949/3076	11	on the inside	CPCONLY	B29C2949/3076		45
B29C2949/3078	11	by spray coating	CPCONLY	B29C2949/3078		64
B29C2949/308	11	by dip coating	CPCONLY	B29C2949/308		62
B29C2949/3082	11	by powder coating	CPCONLY	B29C2949/3082		17
B29C2949/3084	10	said at least one component obtained by casting	CPCONLY	B29C2949/3084		21
B29C2949/3086	9	Interaction between two or more components, e.g. type of or lack of bonding	CPCONLY	B29C2949/3086		29
B29C2949/3088	10	Bonding	CPCONLY	B29C2949/3088		32
B29C2949/309	11	by welding	CPCONLY	B29C2949/309		9
B29C2949/3092	11	by using adhesives	CPCONLY	B29C2949/3092		44
B29C2949/3094	10	preform having at least partially loose components, e.g. at least partially loose layers	CPCONLY	B29C2949/3094		172
