B60Q1/00	7	Arrangement of optical signalling or lighting devices, the mounting or supporting thereof or circuits therefor (for lighting vehicle interior B60Q3/00)	B60Q1/00	B60Q1/00		1348
B60Q1/0005	8	{Devices preventing the lights from becoming dirty or damaged, e.g. protection grids or cleaning by air flow (windshield wipers for cleaning optical devices of vehicles B60S1/04)}	B60Q1/00	B60Q1/00		545
B60Q1/0011	8	{with light guides for distributing the light between several lighting or signalling devices}	B60Q1/00	B60Q1/00		452
B60Q1/0017	8	{Devices integrating an element dedicated to another function}	B60Q1/00	B60Q1/00		568
B60Q1/0023	9	{the element being a sensor, e.g. distance sensor, camera}	B60Q1/00	B60Q1/00		3029
B60Q1/0029	8	{Spatial arrangement}	B60Q1/00	B60Q1/00		88
B60Q1/0035	9	{relative to the vehicle}	B60Q1/00	B60Q1/00		1108
B60Q1/0041	9	{of several lamps in relation to each other}	B60Q1/00	B60Q1/00		1302
B60Q1/0047	10	{Signalling unit mounted on a headlamp unit}	B60Q1/00	B60Q1/00		198
B60Q1/0052	10	{concentric}	B60Q1/00	B60Q1/00		413
B60Q1/0058	10	{Stacked, i.e. one lamp located behind the other in the optical axis direction}	B60Q1/00	B60Q1/00		400
B60Q1/0064	8	{with provision for maintenance, e.g. changing the light bulb (swivel arrangements &#160;B60Q1/0425)}	B60Q1/00	B60Q1/00		296
B60Q1/007	9	{via a removable cap}	B60Q1/00	B60Q1/00		365
B60Q1/0076	8	{Switches therefor (B60Q1/1446, B60Q1/343, B60Q1/40 take precedence)}	B60Q1/00	B60Q1/00		1893
B60Q1/0082	9	{mounted on the steering wheel}	B60Q1/00	B60Q1/00		401
B60Q1/0088	8	{Details of electrical connections (B60Q1/305 takes precedence; electrical connection of the light source itself F21S41/192, F21S43/195)}	B60Q1/00	B60Q1/00		1949
B60Q1/0094	9	{Arrangement of electronic circuits separated from the light source, e.g. mounting of housings for starter circuits for discharge lamps (arrangements being part of the light source holder F21V17/06, F21S43/195)}	B60Q1/00	B60Q1/00		597
B60Q1/02	8	the devices being primarily intended to illuminate the way ahead or to illuminate other areas of way or environments	B60Q1/02	B60Q1/02		623
B60Q1/04	9	the devices being headlights	B60Q1/04	B60Q1/04		2363
B60Q1/0408	10	{built into the vehicle body, e.g. details concerning the mounting of the headlamps on the vehicle body (B60Q1/0491, B60Q1/05 take precedence, integrated front ends B62D25/00)}	B60Q1/04	B60Q1/04		677
B60Q1/0416	11	{the housing being mounted on the vehicle body using rails}	B60Q1/04	B60Q1/04		84
B60Q1/0425	11	{the housing being swivel mounted on the vehicle body}	B60Q1/04	B60Q1/04		71
B60Q1/0433	11	{the housing being fastened onto the vehicle body using screws (adjustable headlamp by rotation of a screw B60Q1/0683)}	B60Q1/04	B60Q1/04		696
B60Q1/0441	11	{the housing being fastened onto the vehicle body using means other than screws}	B60Q1/04	B60Q1/04		506
B60Q1/045	11	{with provision for adjusting the alignment of the headlamp housing with respect to the vehicle body}	B60Q1/04	B60Q1/04		404
B60Q1/0458	11	{the front cover being directly mounted onto the vehicle body}	B60Q1/04	B60Q1/04		135
B60Q1/0466	11	{with arrangement for sealing the headlamp with respect to the vehicle body, or for concealling gaps between the headlamp and the vehicle body}	B60Q1/04	B60Q1/04		293
B60Q1/0475	11	{with provisions for pre-mounting, for temporary holding the headlamp before or during final mounting}	B60Q1/04	B60Q1/04		94
B60Q1/0483	10	{mounted on a bracket, e.g. details concerning the mouting of the lamps on the vehicle body}	B60Q1/04	B60Q1/04		1186
B60Q1/0491	10	{Shock absorbing devices therefor}	B60Q1/04	B60Q1/04		471
B60Q1/0495	11	{Frangible brackets}	B60Q1/04	B60Q1/04		179
B60Q1/05	10	retractable	B60Q1/05	B60Q1/05		412
B60Q1/06	10	adjustable, e.g. remotely-controlled from inside vehicle (B60Q1/05 takes precedence)	B60Q1/06	B60Q1/06		699
B60Q1/064	11	by fluid means	B60Q1/064	B60Q1/064		127
B60Q1/068	11	by mechanical means	B60Q1/068	B60Q1/068		815
B60Q1/0683	12	{Adjustable by rotation of a screw}	B60Q1/068	B60Q1/068		1511
B60Q1/0686	13	{using a position indicator mounted on the headlight and permanently attached thereto}	B60Q1/068	B60Q1/068		118
B60Q1/072	12	comprising a flexible element, e.g. chain	B60Q1/072	B60Q1/072		71
B60Q1/076	11	by electrical means {including means to transmit the movements, e.g. shafts or joints}	B60Q1/076	B60Q1/076		1751
B60Q1/08	11	automatically	B60Q1/08	B60Q1/08		1317
B60Q1/085	12	{due to special conditions, e.g. adverse weather, type of road, badly illuminated road signs or potential dangers (B60Q1/10, B60Q1/12, B60Q1/1423 take precedence)}	B60Q1/08	B60Q1/08		2118
B60Q1/10	12	due to vehicle inclination, e.g. due to load distribution	B60Q1/10	B60Q1/10		532
B60Q1/105	13	by fluid means	B60Q1/105	B60Q1/105		126
B60Q1/11	13	by mechanical means	B60Q1/11	B60Q1/11		121
B60Q1/115	13	by electric means {(details of the electric drive components, e.g. motors, shafts, ball joints B60Q1/076)}	B60Q1/115	B60Q1/115		678
B60Q1/12	12	due to steering position	B60Q1/12	B60Q1/12		1052
B60Q1/121	13	{with fluid actuating means}	B60Q1/12	B60Q1/12		35
B60Q1/122	13	{with electrical actuating means (details of the electric drive components, e.g. motors, shafts, ball joints B60Q1/076)}	B60Q1/12	B60Q1/12		522
B60Q1/124	13	by mechanical means	B60Q1/124	B60Q1/124		2455
B60Q1/14	10	having dimming means	B60Q1/14	B60Q1/14		1435
B60Q1/1407	11	{General lighting circuits comprising dimming circuits}	B60Q1/14	B60Q1/14		407
B60Q1/1415	11	{Dimming circuits}	B60Q1/14	B60Q1/14		827
B60Q1/1423	12	{Automatic dimming circuits, i.e. switching between high beam and low beam due to change of ambient light or light level in road traffic}	B60Q1/14	B60Q1/14		2252
B60Q1/143	13	{combined with another condition, e.g. using vehicle recognition from camera images or activation of wipers}	B60Q1/14	B60Q1/14		2655
B60Q1/1438	11	{Actuating means for dimming masks or screens}	B60Q1/14	B60Q1/14		971
B60Q1/1446	11	{controlled by mechanically actuated switches}	B60Q1/14	B60Q1/14		43
B60Q1/1453	12	{Hand actuated switches}	B60Q1/14	B60Q1/14		114
B60Q1/1461	13	{Multifunction switches for dimming headlights and controlling additional devices, e.g. for controlling direction indicating lights}	B60Q1/14	B60Q1/14		423
B60Q1/1469	14	{controlled by or attached to a single lever, e.g. steering column stalk switches}	B60Q1/14	B60Q1/14		650
B60Q1/1476	15	{comprising switch controlling means located near the free end of the lever, e.g. press buttons, rotatable rings}	B60Q1/14	B60Q1/14		448
B60Q1/1484	14	{mounted on the steering wheel}	B60Q1/14	B60Q1/14		454
B60Q1/1492	12	{Foot actuated switches}	B60Q1/14	B60Q1/14		63
B60Q1/16	10	illuminating the way asymmetrically	B60Q1/16	B60Q1/16		193
B60Q1/18	10	being additional front lights {(bracket mounted headlights B60Q1/0483)}	B60Q1/18	B60Q1/18		1170
B60Q1/20	11	Fog lights	B60Q1/20	B60Q1/20		1011
B60Q1/22	9	for reverse drive	B60Q1/22	B60Q1/22		1125
B60Q1/24	9	for lighting other areas than only the way ahead	B60Q1/24	B60Q1/24		929
B60Q1/245	10	{Searchlights, e.g. adjustable from within the vehicle (adjustable headlights B60Q1/06)}	B60Q1/24	B60Q1/24		954
B60Q1/247	10	{for illuminating the close surroundings of the vehicle, e.g. to facilitate entry or exit (for reverse drive B60Q1/22; by opening a side door B60Q1/323)}	B60Q1/24	B60Q1/24		855
B60Q1/249	10	{for illuminating the field of view of a sensor or camera}	B60Q1/24	B60Q1/24		181
B60Q1/26	8	the devices being primarily intended to indicate the vehicle, or parts thereof, or to give signals, to other traffic	B60Q1/26	B60Q1/26		2261
B60Q1/2603	9	{Attenuation of the light according to ambient luminiosity, e.g. for braking or direction indicating lamps}	B60Q1/26	B60Q1/26		485
B60Q1/2607	9	{comprising at least two indicating lamps}	B60Q1/26	B60Q1/26		2163
B60Q1/2611	9	{Indicating devices mounted on the roof of the vehicle}	B60Q1/26	B60Q1/26		1727
B60Q1/2615	9	{mounted on the vehicle body, e.g. with magnets}	B60Q1/26	B60Q1/26		1224
B60Q1/2619	9	{built in the vehicle body}	B60Q1/26	B60Q1/26		318
B60Q1/2623	10	{Details of the fastening means}	B60Q1/26	B60Q1/26		282
B60Q1/2626	11	{Screw-nut fasteners}	B60Q1/26	B60Q1/26		412
B60Q1/263	11	{Snap-in fasteners}	B60Q1/26	B60Q1/26		363
B60Q1/2634	11	{Fastening by rotating the device housing about its longitudinal axis, e.g. bayonet fasteners}	B60Q1/26	B60Q1/26		26
B60Q1/2638	10	{Positioning the device housing by indexing means separate from the fastening means, e.g. pins, rails}	B60Q1/26	B60Q1/26		204
B60Q1/2642	10	{with provision for adjusting the alignment of the device housing with respect to the vehicle body}	B60Q1/26	B60Q1/26		114
B60Q1/2646	11	{using dowels or expansible elements}	B60Q1/26	B60Q1/26		17
B60Q1/2649	10	{with provision for pre-mounting or temporary holding the device before or during final mounting}	B60Q1/26	B60Q1/26		59
B60Q1/2653	10	{with arrangement for sealing the device with respect to the vehicle body, or for concealing gaps between the device and the vehicle body}	B60Q1/26	B60Q1/26		270
B60Q1/2657	9	{mounted on a shaft, e.g. telescopic}	B60Q1/26	B60Q1/26		607
B60Q1/2661	9	{mounted on parts having other functions (on wheels B60Q1/326)}	B60Q1/26	B60Q1/26		1301
B60Q1/2665	10	{on rear-view mirrors (lighting devices for vehicle interior on or for rear-view mirrors B60Q3/258)}	B60Q1/26	B60Q1/26		1600
B60Q1/2669	10	{on door or boot handles (lighting devices for vehicle interior on door handles B60Q3/267)}	B60Q1/26	B60Q1/26		470
B60Q1/2673	10	{on parts worn by the driver, e.g. clothes, gloves or bags, specially adapted to provide auxiliary vehicle signalling}	B60Q1/26	B60Q1/26		208
B60Q1/2676	11	{Helmets}	B60Q1/26	B60Q1/26		198
B60Q1/268	10	{on windscreens or windows (B60Q1/302 takes precedence; lighting devices for vehicle interior on or for windows B60Q3/208)}	B60Q1/26	B60Q1/26		632
B60Q1/2684	10	{on wipers or windscreen washers}	B60Q1/26	B60Q1/26		64
B60Q1/2688	10	{on exhaust pipes}	B60Q1/26	B60Q1/26		55
B60Q1/2692	9	{retractable lights (retractable headlights B60Q1/05)}	B60Q1/26	B60Q1/26		411
B60Q1/2696	9	{Mounting of devices using LEDs}	B60Q1/26	B60Q1/26		1632
B60Q1/28	9	for indicating front of vehicle	B60Q1/28	B60Q1/28		969
B60Q1/30	9	for indicating rear of vehicle, e.g. by means of reflecting surfaces	B60Q1/30	B60Q1/30		1989
B60Q1/301	10	{by means of surfaces, e.g. metal plate, reflecting the light of an external light source}	B60Q1/30	B60Q1/30		118
B60Q1/3015	11	{combined with a lamp}	B60Q1/30	B60Q1/30		180
B60Q1/302	10	{mounted in the vicinity, e.g. in the middle, of a rear window}	B60Q1/30	B60Q1/30		1724
B60Q1/303	10	{Rear fog lamps}	B60Q1/30	B60Q1/30		139
B60Q1/304	10	{Adaptations of signalling devices having a part on the vehicle body and another on the boot door}	B60Q1/30	B60Q1/30		310
B60Q1/305	10	{Indicating devices for towed vehicles}	B60Q1/30	B60Q1/30		1027
B60Q1/307	10	{mounted on loading platforms}	B60Q1/30	B60Q1/30		212
B60Q1/32	9	for indicating vehicle sides {, e.g. clearance lights}	B60Q1/32	B60Q1/32		1429
B60Q1/323	10	{on or for doors (illuminated exterior door handles B60Q1/2669; illuminated door locks E05B17/10)}	B60Q1/32	B60Q1/32		562
B60Q1/324	11	{for signalling that a door is open or intended to be opened}	B60Q1/32	B60Q1/32		523
B60Q1/325	10	{on or for running boards or steps}	B60Q1/32	B60Q1/32		245
B60Q1/326	10	{on or for wheels}	B60Q1/32	B60Q1/32		612
B60Q1/34	9	for indicating change of drive direction (B60Q1/22 takes precedence)	B60Q1/34	B60Q1/34		6694
B60Q1/343	10	{Manually actuated switching arrangements therefor (hand actuated multifunction switches B60Q1/1461; B60Q1/40 takes precedence)}	B60Q1/34	B60Q1/34		888
B60Q1/346	10	{with automatic actuation}	B60Q1/34	B60Q1/34		882
B60Q1/36	10	using movable members, e.g. arms with built-in flashing lamps	B60Q1/36	B60Q1/36		1028
B60Q1/38	10	using immovably-mounted light sources, e.g. fixed flashing lamps	B60Q1/38	B60Q1/38		1054
B60Q1/381	11	{with several light sources activated in sequence, e.g. to create a sweep effect}	B60Q1/38	B60Q1/38		714
B60Q1/382	11	{Electronic temporisation with semiconductor amplification}	B60Q1/38	B60Q1/38		96
B60Q1/385	11	{Electronic temporisation with relay amplification}	B60Q1/38	B60Q1/38		265
B60Q1/387	11	{Mechanical temporisation}	B60Q1/38	B60Q1/38		862
B60Q1/40	10	having {mechanical, electric or electronic} automatic return to inoperative position	B60Q1/40	B60Q1/40		435
B60Q1/42	11	{having mechanical automatic return to inoperative position} due to steering-wheel position {, e.g. with roller wheel control}	B60Q1/42	B60Q1/42		165
B60Q1/425	12	{using a latching element for resetting a switching element}	B60Q1/42	B60Q1/42		1040
B60Q1/44	9	for indicating braking action {or preparation for braking, e.g. by detection of the foot approaching the brake pedal}	B60Q1/44	B60Q1/44		3214
B60Q1/441	10	{Electric switches operable by the driver&apos;s pedals}	B60Q1/44	B60Q1/44		1405
B60Q1/442	10	{visible on the front side of the vehicle, e.g. for pedestrians}	B60Q1/44	B60Q1/44		308
B60Q1/444	10	{with indication of the braking strength or speed changes, e.g. by changing shape or intensity of the indication (B60Q1/1407, B60Q1/442, B60Q1/447 take precedence)}	B60Q1/44	B60Q1/44		1386
B60Q1/445	10	{controlled by inertial devices}	B60Q1/44	B60Q1/44		391
B60Q1/447	11	{with indication of the braking strength or speed changes, e.g. by changing the shape or intensity of the indication}	B60Q1/44	B60Q1/44		248
B60Q1/448	10	{specially adapted for vehicles with ABS}	B60Q1/44	B60Q1/44		119
B60Q1/46	9	for giving flashing caution signals during drive, other than signalling change of direction, e.g. flashing the headlights {or hazard lights}	B60Q1/46	B60Q1/46		2387
B60Q1/48	9	for parking purposes	B60Q1/48	B60Q1/48		450
B60Q1/482	10	{for locating vehicle in parking lot}	B60Q1/48	B60Q1/48		155
B60Q1/484	10	{for showing outline of vehicle}	B60Q1/48	B60Q1/48		208
B60Q1/486	10	{for indicating that vehicle is in a parked state}	B60Q1/48	B60Q1/48		283
B60Q1/488	10	{for indicating intention to park}	B60Q1/48	B60Q1/48		174
B60Q1/50	9	for indicating other intentions or conditions, e.g. request for waiting or overtaking	B60Q1/50	B60Q1/50		2443
B60Q1/503	10	{using luminous text or symbol displays in or on the vehicle, e.g. static text}	B60Q1/50	B60Q1/50		1333
B60Q1/5035	11	{electronic displays}	B60Q1/50	B60Q1/50		894
B60Q1/5037	12	{the display content changing automatically, e.g. depending on traffic situation}	B60Q1/50	B60Q1/50		427
B60Q1/506	10	{specific to silent vehicles, e.g. for warning that a hybrid or electric vehicle is approaching}	B60Q1/50	B60Q1/50		63
B60Q1/507	10	{specific to autonomous vehicles}	B60Q1/50	B60Q1/50		861
B60Q1/508	10	{specific to vehicles driving in fleets or convoys}	B60Q1/50	B60Q1/50		147
B60Q1/509	10	{specific to unauthorised use, e.g. for indicating stolen vehicles or infringements of traffic rules}	B60Q1/50	B60Q1/50		154
B60Q1/52	10	for indicating emergencies	B60Q1/52	B60Q1/52		3653
B60Q1/525	10	{automatically indicating risk of collision between vehicles in traffic or with pedestrians, e.g. after risk&#160;assessment using the vehicle sensor data}	B60Q1/50	B60Q1/52		1491
B60Q1/535	11	{to prevent rear-end collisions, e.g. by indicating safety distance at the rear of the vehicle}	B60Q1/50	B60Q1/535		922
B60Q1/54	10	for indicating speed {outside of the vehicle}	B60Q1/54	B60Q1/54		1096
B60Q1/543	10	{for indicating other states or conditions of the vehicle (indicating taxis&apos; state of hire or fare G07B13/045)}	B60Q1/50	B60Q1/54		1311
B60Q1/544	10	{for indicating other states or conditions of the vehicle occupants, e.g. for indicating disabled occupants}	B60Q1/50	B60Q1/54		476
B60Q1/545	10	{for indicating other traffic conditions, e.g. fog, heavy traffic}	B60Q1/50	B60Q1/54		377
B60Q1/547	10	{for issuing requests to other traffic participants; for confirming to other traffic participants they can proceed, e.g. they can overtake}	B60Q1/50	B60Q1/54		644
B60Q1/549	10	{for expressing greetings, gratitude or emotions}	B60Q1/50	B60Q1/54		403
B60Q1/56	9	for illuminating registrations or the like {, e.g. for licence plates}	B60Q1/56	B60Q1/56		1573
B60Q3/00	7	Arrangement of lighting devices for vehicle interiors; Lighting devices specially adapted for vehicle interiors	B60Q3/00	B60Q3/00		168
B60Q3/10	8	for dashboards	B60Q3/10	B60Q3/10		459
B60Q3/12	9	lighting onto the surface to be illuminated	B60Q3/12	B60Q3/12		376
B60Q3/14	9	lighting through the surface to be illuminated	B60Q3/14	B60Q3/14		1730
B60Q3/16	9	Circuits; Control arrangements	B60Q3/16	B60Q3/16		596
B60Q3/18	10	for varying the light intensity	B60Q3/18	B60Q3/18		450
B60Q3/20	8	for lighting specific fittings of passenger or driving compartments; mounted on specific fittings of passenger or driving compartments (lighting for dashboards B60Q3/10)	B60Q3/20	B60Q3/20		1064
B60Q3/208	9	Sun roofs; Windows	B60Q3/208	B60Q3/208		872
B60Q3/217	9	Doors, e.g. door sills; Steps	B60Q3/217	B60Q3/217		879
B60Q3/225	9	Small compartments, e.g. glove compartments	B60Q3/225	B60Q3/225		448
B60Q3/229	10	{Cup holders}	B60Q3/225	B60Q3/229		170
B60Q3/233	9	Seats; Arm rests; Head rests	B60Q3/233	B60Q3/233		529
B60Q3/242	9	Safety belts; Body harnesses	B60Q3/242	B60Q3/242		145
B60Q3/252	9	Sun visors	B60Q3/252	B60Q3/252		392
B60Q3/258	9	Rear-view mirrors	B60Q3/258	B60Q3/258		179
B60Q3/267	9	Door handles; Hand grips	B60Q3/267	B60Q3/267		292
B60Q3/275	9	Smoking-related fittings, e.g. cigarette lighters or ashtrays	B60Q3/275	B60Q3/275		193
B60Q3/283	9	Steering wheels; Gear levers	B60Q3/283	B60Q3/283		466
B60Q3/292	9	Ignition locks	B60Q3/292	B60Q3/292		54
B60Q3/30	8	for compartments other than passenger or driving compartments, e.g. luggage or engine compartments	B60Q3/30	B60Q3/30		997
B60Q3/35	9	Portable lighting devices	B60Q3/35	B60Q3/35		125
B60Q3/40	8	specially adapted for specific vehicle types	B60Q3/40	B60Q3/40		73
B60Q3/41	9	for mass transit vehicles, e.g. buses	B60Q3/41	B60Q3/41		144
B60Q3/43	10	General lighting	B60Q3/43	B60Q3/43		507
B60Q3/44	10	Spotlighting, e.g. reading lamps	B60Q3/44	B60Q3/44		327
B60Q3/46	10	Emergency lighting, e.g. for escape routes	B60Q3/46	B60Q3/46		128
B60Q3/47	10	Circuits; Control arrangements	B60Q3/47	B60Q3/47		275
B60Q3/49	9	for vehicles with non-fixed roofs, e.g. convertibles	B60Q3/49	B60Q3/49		39
B60Q3/50	8	Mounting arrangements (for compartments other than passenger or driving compartments B60Q3/30; specially adapted for specific vehicle types B60Q3/40)	B60Q3/50	B60Q3/50		128
B60Q3/51	9	for mounting lighting devices onto vehicle interior, e.g. onto ceiling or floor	B60Q3/51	B60Q3/51		1339
B60Q3/53	10	Modular mounting systems, e.g. using tracks, rails or multiple plugs	B60Q3/53	B60Q3/53		182
B60Q3/54	9	Lighting devices embedded in interior trim, e.g. in roof liners	B60Q3/54	B60Q3/54		1175
B60Q3/56	9	Lighting devices mounted on elongate supports, e.g. on flexible arms	B60Q3/56	B60Q3/56		114
B60Q3/57	9	Retractable or concealable lighting devices	B60Q3/57	B60Q3/57		185
B60Q3/59	9	Lighting devices mounted in the vehicle interior and adapted for portability	B60Q3/59	B60Q3/59		243
B60Q3/60	8	characterised by optical aspects	B60Q3/60	B60Q3/60		704
B60Q3/62	9	using light guides	B60Q3/62	B60Q3/62		619
B60Q3/64	10	for a single lighting device	B60Q3/64	B60Q3/64		1944
B60Q3/66	10	for distributing light among several lighting devices	B60Q3/66	B60Q3/66		234
B60Q3/68	9	using ultraviolet light	B60Q3/68	B60Q3/68		347
B60Q3/70	8	characterised by the purpose	B60Q3/70	B60Q3/70		868
B60Q3/72	9	for preventing the driver from being dazzled	B60Q3/72	B60Q3/72		181
B60Q3/731	9	{for autonomous vehicle travel}	B60Q3/70	B60Q3/731		32
B60Q3/735	10	{for preventing discomfort, e.g. for preventing motion sickness or for anticipating motion}	B60Q3/70	B60Q3/735		102
B60Q3/74	9	for overall compartment lighting; for overall compartment lighting in combination with specific lighting, e.g. room lamps with reading lamps (general lighting mounted on specific fittings B60Q3/20; general lighting for mass transit vehicles B60Q3/43)	B60Q3/74	B60Q3/74		1155
B60Q3/745	10	{using lighting panels or mats, e.g. electro-luminescent panels, LED mats}	B60Q3/74	B60Q3/74		630
B60Q3/76	9	for spotlighting, e.g. reading lamps (spotlighting on or for specific fittings B60Q3/20; spotlighting in mass transit vehicles B60Q3/44)	B60Q3/76	B60Q3/76		786
B60Q3/78	9	for generating luminous strips, e.g. for marking trim component edges	B60Q3/78	B60Q3/78		873
B60Q3/80	8	Circuits; Control arrangements (for dashboards B60Q3/16; for mass transit vehicles B60Q3/47)	B60Q3/80	B60Q3/80		3449
B60Q3/82	9	Switches specially adapted for vehicle interior lighting, e.g. switching by tilting the lens	B60Q3/82	B60Q3/82		1124
B60Q3/85	9	for manual control of the light, e.g. of colour, orientation or intensity	B60Q3/85	B60Q3/85		668
B60Q3/88	9	Means for plugging to the electrical power supply of the vehicle, e.g. by using cigarette lighter sockets	B60Q3/88	B60Q3/88		364
B60Q5/00	7	Arrangement or adaptation of acoustic signal devices	B60Q5/00	B60Q5/00		2667
B60Q5/001	8	{Switches therefor}	B60Q5/00	B60Q5/00		294
B60Q5/003	9	{mounted on the steering wheel}	B60Q5/00	B60Q5/00		1256
B60Q5/005	8	{automatically actuated}	B60Q5/00	B60Q5/00		1906
B60Q5/006	9	{indicating risk of collision between vehicles or with pedestrians}	B60Q5/00	B60Q5/00		1578
B60Q5/008	9	{for signaling silent vehicles, e.g. for warning that a hybrid or electric vehicle is approaching}	B60Q5/00	B60Q5/00		1099
B60Q7/00	7	Arrangement or adaptation of portable emergency signal devices on vehicles	B60Q7/00	B60Q7/00		2463
B60Q7/005	8	{Devices without lamps}	B60Q7/00	B60Q7/00		1040
B60Q7/02	8	to be attached to overhanging loads or extending parts of vehicle	B60Q7/02	B60Q7/02		308
B60Q9/00	7	Arrangement or adaptation of signal devices not provided for in one of main groups B60Q1/00 - B60Q7/00{, e.g. haptic signalling}	B60Q9/00	B60Q9/00		10180
B60Q9/001	8	{Alarm devices when the motor is stopped and the lights are on}	B60Q9/00	B60Q9/00		372
B60Q9/002	8	{for parking purposes, e.g. for warning the driver that his vehicle has contacted or is about to contact an obstacle (warning arrangements in garages E04H6/42)}	B60Q9/00	B60Q9/00		287
B60Q9/003	9	{using physical contactors, e.g. arms that trigger alarm upon contact with obstacle}	B60Q9/00	B60Q9/00		192
B60Q9/004	9	{using wave sensors (radar designed for anti-collision purposes between land vehicles or between land vehicles and fixed obstacles G01S13/931)}	B60Q9/00	B60Q9/00		164
B60Q9/005	10	{using a video camera}	B60Q9/00	B60Q9/00		301
B60Q9/006	10	{using a distance sensor}	B60Q9/00	B60Q9/00		503
B60Q9/007	9	{providing information about the distance to an obstacle, e.g. varying sound}	B60Q9/00	B60Q9/00		378
B60Q9/008	8	{for anti-collision purposes}	B60Q9/00	B60Q9/00		5623
B60Q11/00	7	Arrangement of monitoring devices for devices provided for in groups B60Q1/00 - B60Q9/00	B60Q11/00	B60Q11/00		1357
B60Q11/002	8	{Emergency driving lights in the event of failure of the principal lighting circuit}	B60Q11/00	B60Q11/00		336
B60Q11/005	8	{for lighting devices, e.g. indicating if lamps are burning or not}	B60Q11/00	B60Q11/00		1949
B60Q11/007	9	{the lighting devices indicating change of drive direction}	B60Q11/00	B60Q11/00		422
B60Q2200/00	7	Special features or arrangements of vehicle headlamps	CPCONLY	B60Q2200/00		26
B60Q2200/30	8	Special arrangements for adjusting headlamps, e.g. means for transmitting the movements for adjusting the lamps	CPCONLY	B60Q2200/30		339
B60Q2200/32	9	Ball-joints	CPCONLY	B60Q2200/32		319
B60Q2200/34	9	Deformable parts, i.e. the adjustment is performed by bending or stretching a part	CPCONLY	B60Q2200/34		29
B60Q2200/36	9	Conjoint adjustments, i.e. a mechanical link allows conjoint adjustment of several units	CPCONLY	B60Q2200/36		234
B60Q2200/38	9	Automatic calibration of motor-driven means for adjusting headlamps, i.e. when switching on the headlamps, not during mounting at factories	CPCONLY	B60Q2200/38		322
B60Q2300/00	7	Indexing codes for automatically adjustable headlamps or automatically dimmable headlamps	CPCONLY	B60Q2300/00		21
B60Q2300/05	8	Special features for controlling or switching of the light beam	CPCONLY	B60Q2300/05		186
B60Q2300/052	9	Switching delay, i.e. the beam is not switched or changed instantaneously upon occurrence of a condition change	CPCONLY	B60Q2300/052		370
B60Q2300/054	9	Variable non-standard intensity, i.e. emission of various beam intensities different from standard intensities, e.g. continuous or stepped transitions of intensity	CPCONLY	B60Q2300/054		726
B60Q2300/056	9	Special anti-blinding beams, e.g. a standard beam is chopped or moved in order not to blind	CPCONLY	B60Q2300/056		1026
B60Q2300/10	8	Indexing codes relating to particular vehicle conditions	CPCONLY	B60Q2300/10		50
B60Q2300/11	9	Linear movements of the vehicle	CPCONLY	B60Q2300/11		25
B60Q2300/112	10	Vehicle speed	CPCONLY	B60Q2300/112		1557
B60Q2300/114	10	Vehicle acceleration or deceleration	CPCONLY	B60Q2300/114		408
B60Q2300/116	10	Vehicle at a stop	CPCONLY	B60Q2300/116		283
B60Q2300/12	9	Steering parameters	CPCONLY	B60Q2300/12		93
B60Q2300/122	10	Steering angle	CPCONLY	B60Q2300/122		992
B60Q2300/124	10	Steering speed	CPCONLY	B60Q2300/124		54
B60Q2300/126	10	Hysteresis behavior based on steering	CPCONLY	B60Q2300/126		31
B60Q2300/128	10	Steering dead zone	CPCONLY	B60Q2300/128		78
B60Q2300/13	9	Attitude of the vehicle body	CPCONLY	B60Q2300/13		111
B60Q2300/132	10	Pitch	CPCONLY	B60Q2300/132		616
B60Q2300/134	10	Yaw	CPCONLY	B60Q2300/134		213
B60Q2300/136	10	Roll	CPCONLY	B60Q2300/136		236
B60Q2300/14	9	Other vehicle conditions	CPCONLY	B60Q2300/14		174
B60Q2300/142	10	Turn signal actuation	CPCONLY	B60Q2300/142		212
B60Q2300/144	10	Rearward ratio actuation	CPCONLY	B60Q2300/144		49
B60Q2300/146	10	Abnormalities, e.g. fail-safe	CPCONLY	B60Q2300/146		256
B60Q2300/20	8	Indexing codes relating to the driver or the passengers	CPCONLY	B60Q2300/20		91
B60Q2300/21	9	Manual control	CPCONLY	B60Q2300/21		418
B60Q2300/22	9	Seat occupation	CPCONLY	B60Q2300/22		33
B60Q2300/23	9	Driver&apos;s line of sight	CPCONLY	B60Q2300/23		148
B60Q2300/30	8	Indexing codes relating to the vehicle environment	CPCONLY	B60Q2300/30		118
B60Q2300/305	9	Calendar date or clock time	CPCONLY	B60Q2300/305		64
B60Q2300/31	9	Atmospheric conditions	CPCONLY	B60Q2300/31		117
B60Q2300/312	10	Adverse weather	CPCONLY	B60Q2300/312		670
B60Q2300/314	10	Ambient light	CPCONLY	B60Q2300/314		1518
B60Q2300/32	9	Road surface or travel path	CPCONLY	B60Q2300/32		386
B60Q2300/322	10	Road curvature	CPCONLY	B60Q2300/322		387
B60Q2300/324	10	Road inclination, e.g. uphill or downhill	CPCONLY	B60Q2300/324		251
B60Q2300/33	9	Driving situation	CPCONLY	B60Q2300/33		187
B60Q2300/331	10	characterised by the driving side, e.g. on the left or right hand side	CPCONLY	B60Q2300/331		81
B60Q2300/332	10	on city roads	CPCONLY	B60Q2300/332		169
B60Q2300/3321	11	Detection of streetlights	CPCONLY	B60Q2300/3321		161
B60Q2300/333	10	on suburban or country roads	CPCONLY	B60Q2300/333		104
B60Q2300/334	10	on motorways	CPCONLY	B60Q2300/334		178
B60Q2300/335	10	Number or size of road lanes	CPCONLY	B60Q2300/335		68
B60Q2300/336	10	Crossings	CPCONLY	B60Q2300/336		142
B60Q2300/337	10	Tunnels or bridges	CPCONLY	B60Q2300/337		247
B60Q2300/338	10	Overtaking	CPCONLY	B60Q2300/338		51
B60Q2300/40	8	Indexing codes relating to other road users or special conditions	CPCONLY	B60Q2300/40		114
B60Q2300/41	9	preceding vehicle	CPCONLY	B60Q2300/41		978
B60Q2300/42	9	oncoming vehicle	CPCONLY	B60Q2300/42		1809
B60Q2300/43	9	following vehicle	CPCONLY	B60Q2300/43		442
B60Q2300/45	9	Special conditions, e.g. pedestrians, road signs or potential dangers	CPCONLY	B60Q2300/45		1220
B60Q2300/47	9	Direct command from other road users, i.e. the command for switching or changing the beam is sent by other vehicles or road devices	CPCONLY	B60Q2300/47		222
B60Q2400/00	7	Special features or arrangements of exterior signal lamps for vehicles	CPCONLY	B60Q2400/00		77
B60Q2400/10	8	Electro- or photo- luminescent surfaces, e.g. signalling by way of electroluminescent strips or panels	CPCONLY	B60Q2400/10		189
B60Q2400/20	8	Multi-color single source or LED matrix, e.g. yellow blinker and red brake lamp generated by single lamp	CPCONLY	B60Q2400/20		1026
B60Q2400/30	8	Daytime running lights [DRL], e.g. circuits or arrangements therefor	CPCONLY	B60Q2400/30		758
B60Q2400/40	8	Welcome lights, i.e. specific or existing exterior lamps to assist leaving or approaching the vehicle	CPCONLY	B60Q2400/40		740
B60Q2400/50	8	Projected symbol or information, e.g. onto the road or car body	CPCONLY	B60Q2400/50		2172
B60Q2500/00	7	Special features or arrangements of vehicle interior lamps	CPCONLY	B60Q2500/00		99
B60Q2500/20	8	associated with air conditioning arrangements	CPCONLY	B60Q2500/20		246
B60Q2500/30	8	Arrangements for illuminating different zones in the vehicle, e.g. front/rear, different seats	CPCONLY	B60Q2500/30		235
B60Q2800/00	7	Features related to particular types of vehicles not otherwise provided for	CPCONLY	B60Q2800/00		6
B60Q2800/10	8	Autonomous vehicles	CPCONLY	B60Q2800/10		167
B60Q2800/20	8	Utility vehicles, e.g. for agriculture, construction work	CPCONLY	B60Q2800/20		685
B60Q2800/30	8	Mass transport vehicles	CPCONLY	B60Q2800/30		29
B60Q2900/00	7	Features of lamps not covered by other groups in B60Q	CPCONLY	B60Q2900/00		7
B60Q2900/10	8	Retrofit arrangements	CPCONLY	B60Q2900/10		435
B60Q2900/20	8	Arrangements for easy recycling, e.g. for easy dismantling or use of special materials	CPCONLY	B60Q2900/20		86
B60Q2900/30	8	Lamps commanded by wireless transmissions	CPCONLY	B60Q2900/30		953
B60Q2900/40	8	Several lamps activated in sequence, e.g. sweep effect, progressive activation	CPCONLY	B60Q2900/40		463
B60Q2900/50	8	Arrangements to reconfigure features of lighting or signalling devices, or to choose from a list of pre-defined settings	CPCONLY	B60Q2900/50		262
