E05D1/00	7	Pinless hinges; Substitutes for hinges	E05D1/00	E05D1/00		270
E05D1/02	8	made of one piece	E05D1/02	E05D1/02		848
E05D1/04	8	with guide members shaped as circular arcs	E05D1/04	E05D1/04		870
E05D2001/045	9	{for telescopic hinges}	E05D1/04	E05D1/04		40
E05D1/06	8	consisting of two easily-separable parts	E05D1/06	E05D1/06		368
E05D3/00	7	Hinges with pins {(E05D7/08 takes precedence)}	E05D3/00	E05D3/00		216
E05D3/02	8	with one pin	E05D3/02	E05D3/02		5256
E05D3/022	9	{allowing an additional lateral movement, e.g. for sealing}	E05D3/02	E05D3/02		823
E05D2003/025	9	{having three knuckles}	E05D3/02	E05D3/02		269
E05D2003/027	10	{the end knuckles being mutually connected}	E05D3/02	E05D3/02		337
E05D3/04	9	engaging three or more parts, e.g. sleeves, movable relatively to one another for connecting two or more wings to another member	E05D3/04	E05D3/04		279
E05D3/06	8	with two or more pins (E05D7/08 takes precedence)	E05D3/06	E05D3/06		1744
E05D3/08	9	for swing-doors, i.e. openable by pushing from either side	E05D3/08	E05D3/08		191
E05D3/10	9	with non-parallel pins	E05D3/10	E05D3/10		413
E05D3/12	9	with two parallel pins and one arm	E05D3/12	E05D3/12		1140
E05D3/122	10	{Gear hinges}	E05D3/12	E05D3/12		515
E05D3/125	10	{specially adapted for vehicles}	E05D3/12	E05D3/12		109
E05D3/127	11	{for vehicle doors}	E05D3/12	E05D3/12		272
E05D3/14	9	with four parallel pins and two arms	E05D3/14	E05D3/14		435
E05D3/142	10	{with at least one of the hinge parts having a cup-shaped fixing part, e.g. for attachment to cabinets or furniture (E05D11/1021 takes precedence)}	E05D3/14	E05D3/14		390
E05D3/145	10	{specially adapted for vehicles}	E05D3/14	E05D3/14		337
E05D3/147	11	{for vehicle doors}	E05D3/14	E05D3/14		157
E05D3/16	9	with seven parallel pins and four arms	E05D3/16	E05D3/16		581
E05D2003/163	10	{Horizontal pivot-axis}	E05D3/16	E05D3/16		143
E05D2003/166	10	{Vertical pivot-axis}	E05D3/16	E05D3/16		204
E05D3/18	9	with sliding pins or guides	E05D3/18	E05D3/18		981
E05D3/183	10	{with at least one of the hinge parts having a cup-shaped fixing part, e.g. for attachment to cabinets or furniture}	E05D3/18	E05D3/18		155
E05D3/186	10	{Scissors hinges, with two crossing levers and five parallel pins}	E05D3/18	E05D3/18		351
E05D5/00	7	Construction of single parts, e.g. the parts for attachment	E05D5/00	E05D5/00		282
E05D5/02	8	Parts for attachment, e.g. flaps	E05D5/02	E05D5/02		2146
E05D5/0207	9	{for attachment to vehicles (E05D5/043, E05D5/062 take precedence)}	E05D5/02	E05D5/02		860
E05D5/0215	9	{for attachment to profile members or the like}	E05D5/02	E05D5/02		391
E05D5/0223	10	{with parts, e.g. screws, extending through the profile wall or engaging profile grooves}	E05D5/02	E05D5/02		255
E05D5/023	11	{with parts extending through the profile wall}	E05D5/02	E05D5/02		669
E05D5/0238	11	{with parts engaging profile grooves}	E05D5/02	E05D5/02		647
E05D5/0246	9	{for attachment to glass panels}	E05D5/02	E05D5/02		1318
E05D2005/0253	10	{the panels having conical or stepped recesses}	E05D5/02	E05D5/02		120
E05D2005/0261	10	{connecting two or more glass panels}	E05D5/02	E05D5/02		24
E05D2005/0269	11	{the panels being coplanar}	E05D5/02	E05D5/02		94
E05D5/0276	9	{for attachment to cabinets or furniture, the hinge having two or more pins (E05D5/046, E05D5/065, E05D7/125 take precedence)}	E05D5/02	E05D5/02		635
E05D2005/0284	9	{for embedding in concrete or masonry}	E05D5/02	E05D5/02		66
E05D2005/0292	9	{for passing through insulating layers}	E05D5/02	E05D5/02		40
E05D5/04	9	Flat flaps	E05D5/04	E05D5/04		1257
E05D5/043	10	{specially adapted for vehicles}	E05D5/04	E05D5/04		186
E05D5/046	10	{specially adapted for cabinets or furniture}	E05D5/04	E05D5/04		180
E05D5/06	9	Bent flaps	E05D5/06	E05D5/06		1286
E05D5/062	10	{specially adapted for vehicles}	E05D5/06	E05D5/06		1006
E05D5/065	10	{specially adapted for cabinets or furniture}	E05D5/06	E05D5/06		370
E05D2005/067	10	{gooseneck shaped}	E05D5/06	E05D5/06		439
E05D5/08	9	of cylindrical shape	E05D5/08	E05D5/08		789
E05D5/10	8	Pins, sockets or sleeves; Removable pins (E05D15/522 takes precedence)	E05D5/10	E05D5/10		1130
E05D2005/102	9	{Pins}	E05D5/10	E05D5/10		591
E05D2005/104	10	{characterised by the materials}	E05D5/10	E05D5/10		108
E05D2005/106	10	{with non-cylindrical portions}	E05D5/10	E05D5/10		280
E05D2005/108	10	{with elastically deformable parts}	E05D5/10	E05D5/10		107
E05D5/12	9	Securing pins in sockets, movably or not	E05D5/12	E05D5/12		544
E05D5/121	10	{Screw-threaded pins}	E05D5/12	E05D5/12		312
E05D2005/122	11	{externally threaded}	E05D5/12	E05D5/12		99
E05D2005/124	11	{internally threaded}	E05D5/12	E05D5/12		43
E05D5/125	10	{Non-removable, snap-fitted pins (removable snap-fitted pins E05D7/1022, E05D7/1055)}	E05D5/12	E05D5/12		102
E05D5/127	10	{by forcing the pin into the socket (E05D5/125 takes precedence)}	E05D5/12	E05D5/12		161
E05D5/128	10	{the pin having a recess or through-hole engaged by a securing member}	E05D5/12	E05D5/12		462
E05D5/14	9	Construction of sockets or sleeves	E05D5/14	E05D5/14		932
E05D2005/145	10	{with elastically deformable parts}	E05D5/14	E05D5/14		136
E05D5/16	10	to be secured without special attachment parts on the socket or sleeve	E05D5/16	E05D5/16		212
E05D7/00	7	Hinges or pivots of special construction (used for special suspension arrangements E05D15/00; so as to be self-closing E05F1/06, E05F1/12; with means for raising wings before being turned E05F7/02)	E05D7/00	E05D7/00		1210
E05D7/0009	8	{Adjustable hinges (E05D7/04 takes precedence)}	E05D7/00	E05D7/00		325
E05D7/0018	9	{at the hinge axis}	E05D7/00	E05D7/00		122
E05D7/0027	10	{in an axial direction}	E05D7/00	E05D7/00		888
E05D2007/0036	11	{with axially fixed hinge pins}	E05D7/00	E05D7/00		96
E05D7/0045	10	{in a radial direction}	E05D7/00	E05D7/00		247
E05D7/0054	11	{by means of eccentric parts}	E05D7/00	E05D7/00		339
E05D2007/0063	12	{Eccentric hinge pins}	E05D7/00	E05D7/00		63
E05D2007/0072	11	{with sliding sleeves}	E05D7/00	E05D7/00		28
E05D2007/0081	11	{with swinging or rolling sleeves}	E05D7/00	E05D7/00		30
E05D7/009	8	{Elongate hinges, e.g. piano-hinges}	E05D7/00	E05D7/00		326
E05D7/02	8	for use on the right-hand as well as the left-hand side; Convertible right-hand or left-hand hinges	E05D7/02	E05D7/02		650
E05D7/04	8	Hinges adjustable relative to the wing or the frame	E05D7/04	E05D7/04		2102
E05D7/0407	9	{the hinges having two or more pins and being specially adapted for cabinets or furniture}	E05D7/04	E05D7/04		669
E05D7/0415	9	{with adjusting drive means}	E05D7/04	E05D7/04		763
E05D7/0423	10	{Screw-and-nut mechanisms (E05D7/0407, E05D7/043 take precedence)}	E05D7/04	E05D7/04		1281
E05D7/043	9	{by means of dowel attachments}	E05D7/04	E05D7/04		389
E05D2007/0438	10	{with bolts fixedly mounted on the hinge part}	E05D7/04	E05D7/04		49
E05D2007/0446	10	{with threaded bolts fixedly mounted on the hinge part}	E05D7/04	E05D7/04		113
E05D2007/0453	10	{with threaded sleeves}	E05D7/04	E05D7/04		21
E05D2007/0461	9	{in angular arrangement to the wing or the frame}	E05D7/04	E05D7/04		254
E05D2007/0469	9	{in an axial direction}	E05D7/04	E05D7/04		482
E05D2007/0476	9	{Pocket hinges}	E05D7/04	E05D7/04		303
E05D2007/0484	9	{in a radial direction}	E05D7/04	E05D7/04		649
E05D2007/0492	9	{in three directions}	E05D7/04	E05D7/04		195
E05D7/06	8	to allow tilting of the members	E05D7/06	E05D7/06		347
E05D7/08	8	for use in suspensions comprising two spigots placed at opposite edges of the wing, especially at the top and the bottom, e.g. trunnions {(E05D15/266 takes precedence)}	E05D7/08	E05D7/08		281
E05D7/081	9	the pivot axis of the wing being situated near one edge of the wing, especially at the top and bottom, e.g. trunnions	E05D7/081	E05D7/081		2793
E05D7/082	9	the pivot axis of the wing being situated at a considerable distance from the edges of the wing {, e.g. for balanced wings}	E05D7/082	E05D7/082		81
E05D7/083	10	with a fixed pivot axis	E05D7/083	E05D7/083		467
E05D7/084	10	with a movable pivot axis	E05D7/084	E05D7/084		102
E05D7/085	11	with two or more pivot axes, e.g. used at the same time	E05D7/085	E05D7/085		220
E05D7/086	10	Braking devices structurally combined with hinges (braking devices for windows per seE05F5/00)	E05D7/086	E05D7/086		246
E05D7/10	8	to allow easy separation {or connection} of the parts at the hinge axis ({E05D5/12 and E05D15/50 take precedence } ; substitutes for hinges E05D1/06)	E05D7/10	E05D7/10		482
E05D7/1005	9	{by axially moving free pins, balls or sockets}	E05D7/10	E05D7/10		500
E05D7/1011	10	{biased by free springs (E05D7/1016 takes precedence)}	E05D7/10	E05D7/10		229
E05D7/1016	10	{requiring a specific angular position}	E05D7/10	E05D7/10		100
E05D7/1022	10	{with snap-fitted pins}	E05D7/10	E05D7/10		123
E05D2007/1027	10	{by axially moving free pins}	E05D7/10	E05D7/10		108
E05D2007/1033	10	{by axially moving free balls}	E05D7/10	E05D7/10		18
E05D2007/1038	10	{by axially moving free sockets}	E05D7/10	E05D7/10		29
E05D7/1044	9	{in an axial direction (E05D7/1005 takes precedence)}	E05D7/10	E05D7/10		385
E05D7/105	10	{requiring a specific angular position}	E05D7/10	E05D7/10		219
E05D7/1055	10	{with snap-fitted pins}	E05D7/10	E05D7/10		110
E05D7/1061	9	{in a radial direction (E05D7/1005 takes precedence)}	E05D7/10	E05D7/10		307
E05D7/1066	10	{requiring a specific angular position}	E05D7/10	E05D7/10		204
E05D7/1072	11	{the pin having a non-circular cross-section}	E05D7/10	E05D7/10		172
E05D7/1077	10	{with snap-fitted pins}	E05D7/10	E05D7/10		273
E05D7/1083	9	{facilitating simultaneous assembly of a plurality of hinges, e.g. for mounting heavy wings}	E05D7/10	E05D7/10		114
E05D2007/1088	10	{using hinge pins having different lengths}	E05D7/10	E05D7/10		44
E05D2007/1094	9	{Guiding devices therefor}	E05D7/10	E05D7/10		53
E05D7/12	8	to allow easy detachment of the hinge from the wing or the frame {(E05D15/507 takes precedence)}	E05D7/12	E05D7/12		890
E05D7/121	9	{specially adapted for vehicles}	E05D7/12	E05D7/12		200
E05D7/123	9	{specially adapted for cabinets or furniture}	E05D7/12	E05D7/12		271
E05D7/125	10	{the hinge having two or more pins}	E05D7/12	E05D7/12		294
E05D2007/126	9	{in an axial direction}	E05D7/12	E05D7/12		80
E05D2007/128	9	{in a radial direction}	E05D7/12	E05D7/12		163
E05D7/14	8	Hinges for safes	E05D7/14	E05D7/14		201
E05D9/00	7	Flaps or sleeves specially designed for making from particular material, e.g. hoop-iron, sheet metal, plastics	E05D9/00	E05D9/00		558
E05D9/005	8	{from plastics (E05D1/02 takes precedence)}	E05D9/00	E05D9/00		399
E05D11/00	7	Additional features or accessories of hinges {(edge protecting devices E06B3/88)}	E05D11/00	E05D11/00		2485
E05D11/0009	8	{Templates for marking the position of fittings on wings or frames (implements for making doors, windows or frames E04F21/003)}	E05D11/00	E05D11/00		423
E05D11/0018	8	{Anti-tamper devices}	E05D11/00	E05D11/00		321
E05D11/0027	9	{arranged on or near the hinge and comprising parts interlocking as the wing closes, e.g. security studs}	E05D11/00	E05D11/00		356
E05D2011/0036	10	{near the hinge}	E05D11/00	E05D11/00		85
E05D2011/0045	10	{on the hinge}	E05D11/00	E05D11/00		86
E05D11/0054	8	{Covers, e.g. for protection}	E05D11/00	E05D11/00		1388
E05D2011/0063	9	{for screw-heads or bolt-heads}	E05D11/00	E05D11/00		85
E05D2011/0072	9	{for the gap between hinge parts}	E05D11/00	E05D11/00		200
E05D11/0081	8	{for transmitting energy, e.g. electrical cable routing}	E05D11/00	E05D11/00		785
E05D2011/009	8	{Impact absorbing hinges for vehicle doors}	E05D11/00	E05D11/00		202
E05D11/02	8	Lubricating arrangements	E05D11/02	E05D11/02		499
E05D11/04	8	relating to the use of free balls as bearing-surfaces (E05D7/06 takes precedence)	E05D11/04	E05D11/04		550
E05D2011/045	9	{located in line with the hinge axis}	E05D11/04	E05D11/04		145
E05D11/06	8	Devices for limiting the opening movement of hinges	E05D11/06	E05D11/06		2173
E05D11/08	8	Friction devices between relatively-movable hinge parts (E05D7/086 takes precedence)	E05D11/08	E05D11/08		493
E05D11/081	9	{with both radial and axial friction, e.g. conical friction surfaces}	E05D11/08	E05D11/08		240
E05D11/082	9	{with substantially radial friction, e.g. cylindrical friction surfaces}	E05D11/08	E05D11/08		847
E05D11/084	10	{the friction depending on direction of rotation or opening angle of the hinge}	E05D11/08	E05D11/08		252
E05D2011/085	10	{the friction depending on the opening angle}	E05D11/08	E05D11/08		69
E05D11/087	9	{with substantially axial friction, e.g. friction disks}	E05D11/08	E05D11/08		668
E05D2011/088	9	{with automatic disengagement}	E05D11/08	E05D11/08		30
E05D11/10	8	Devices for preventing movement between relatively-movable hinge parts	E05D11/10	E05D11/10		1053
E05D11/1007	9	{with positive locking}	E05D11/10	E05D11/10		1294
E05D11/1014	9	{for maintaining the hinge in only one position, e.g. closed}	E05D11/10	E05D11/10		1198
E05D11/1021	10	{the hinge having two or more pins and being specially adapted for cabinets or furniture}	E05D11/10	E05D11/10		458
E05D11/1028	9	{for maintaining the hinge in two or more positions, e.g. intermediate or fully open}	E05D11/10	E05D11/10		773
E05D2011/1035	10	{with circumferential and evenly distributed detents around the pivot-axis}	E05D11/10	E05D11/10		208
E05D11/1042	10	{the maintaining means being a cam and a torsion bar, e.g. motor vehicle hinge mechanisms}	E05D11/10	E05D11/10		260
E05D11/105	10	{the maintaining means acting perpendicularly to the pivot axis}	E05D11/10	E05D11/10		650
E05D11/1057	11	{specially adapted for vehicles (E05D11/1064 takes precedence)}	E05D11/10	E05D11/10		323
E05D11/1064	11	{with a coil spring perpendicular to the pivot axis}	E05D11/10	E05D11/10		610
E05D11/1071	12	{specially adapted for vehicles}	E05D11/10	E05D11/10		178
E05D11/1078	10	{the maintaining means acting parallel to the pivot}	E05D11/10	E05D11/10		796
E05D11/1085	11	{specially adapted for vehicles}	E05D11/10	E05D11/10		264
E05D2011/1092	9	{the angle between the hinge parts being adjustable}	E05D11/10	E05D11/10		187
E05D13/00	7	Accessories for sliding or lifting wings, e.g. pulleys, safety catches ({closers or openers for horizontally sliding wings E05F1/02, E05F1/08}; counterbalance devices {for swinging wings}E05F1/00, E05F3/00)	E05D13/00	E05D13/00		3167
E05D13/003	8	{Anti-dropping devices (E05D13/1223, E05D13/1246, E05D13/1269, E05D13/1292 take precedence)}	E05D13/00	E05D13/00		397
E05D13/006	9	{fixed to the wing, i.e. safety catches}	E05D13/00	E05D13/00		313
E05D13/04	8	{Fasteners specially adapted for holding sliding wings open (for holding wings closed E05C)}	E05C17/60	E05D13/04		457
E05D13/06	9	{with notches for vertically sliding wings}	E05C17/62	E05D13/06		493
E05D13/08	9	{acting by friction for vertically sliding wings}	E05C17/64	E05D13/08		294
E05D13/10	8	{Counterbalance devices}	E05D13/00	E05D13/10		247
E05D13/12	9	{with springs}	E05D13/00	E05D13/12		361
E05D13/1207	10	{with tension springs}	E05D13/00	E05D13/12		320
E05D13/1215	11	{specially adapted for overhead wings (E05D13/1223 takes precedence)}	E05D13/00	E05D13/12		413
E05D13/1223	11	{Spring safety devices}	E05D13/00	E05D13/12		84
E05D13/123	10	{with compression springs}	E05D13/00	E05D13/12		113
E05D13/1238	11	{specially adapted for overhead wings (E05D13/1246 takes precedence)}	E05D13/00	E05D13/12		70
E05D13/1246	11	{Spring safety devices}	E05D13/00	E05D13/12		34
E05D13/1253	10	{with canted-coil torsion springs}	E05D13/00	E05D13/12		228
E05D13/1261	11	{specially adapted for overhead wings (E05D13/1269 takes precedence)}	E05D13/00	E05D13/12		491
E05D13/1269	11	{Spring safety devices}	E05D13/00	E05D13/12		93
E05D13/1276	10	{with coiled ribbon springs, e.g. constant force springs (E05D13/1253 takes precedence)}	E05D13/00	E05D13/12		226
E05D13/1284	11	{specially adapted for overhead wings (E05D13/1292 takes precedence)}	E05D13/00	E05D13/12		33
E05D13/1292	11	{Spring safety devices}	E05D13/00	E05D13/12		54
E05D13/14	9	{with weights}	E05D13/00	E05D13/14		524
E05D13/145	10	{specially adapted for overhead wings}	E05D13/00	E05D13/14		238
E05D15/00	7	Suspension arrangements for wings (arrangements of wings not characterised by the construction of the supporting means E06B3/32)	E05D15/00	E05D15/00		536
E05D15/02	8	for revolving wings	E05D15/02	E05D15/02		429
E05D15/04	8	with arms fixed on the wing pivoting about an axis outside of the wing	E05D15/04	E05D15/04		136
E05D15/06	8	for wings sliding horizontally more or less in their own plane	E05D15/06	E05D15/06		1315
E05D15/0604	9	{allowing an additional movement (E05D15/10 takes precedence; raising wings before sliding E05D15/565)}	E05D15/06	E05D15/06		487
E05D15/0608	10	{caused by track lay-out}	E05D15/06	E05D15/06		363
E05D15/0613	11	{with multi-directional trolleys}	E05D15/06	E05D15/06		160
E05D15/0617	9	{of cantilever type}	E05D15/06	E05D15/06		185
E05D15/0621	9	{Details, e.g. suspension or supporting guides (E05D15/0604, E05D15/08&#160;-&#160;E05D15/14 take precedence)}	E05D15/06	E05D15/06		1093
E05D15/0626	10	{for wings suspended at the top}	E05D15/06	E05D15/06		908
E05D15/063	11	{on wheels with fixed axis}	E05D15/06	E05D15/06		2271
E05D15/0634	12	{with height adjustment}	E05D15/06	E05D15/06		653
E05D15/0639	13	{by vertical bolts}	E05D15/06	E05D15/06		199
E05D15/0643	11	{on balls or floating rollers}	E05D15/06	E05D15/06		384
E05D15/0647	11	{on sliding blocks}	E05D15/06	E05D15/06		263
E05D15/0652	11	{Tracks (E05D15/063&#160;-&#160;E05D15/0647 and E05D15/0656 take precedence)}	E05D15/06	E05D15/06		1738
E05D15/0656	11	{Bottom guides}	E05D15/06	E05D15/06		795
E05D15/066	10	{for wings supported at the bottom}	E05D15/06	E05D15/06		462
E05D15/0665	11	{on wheels with fixed axis}	E05D15/06	E05D15/06		984
E05D15/0669	12	{with height adjustment}	E05D15/06	E05D15/06		528
E05D15/0673	13	{by vertical bolts}	E05D15/06	E05D15/06		90
E05D15/0678	11	{on balls or floating rollers}	E05D15/06	E05D15/06		223
E05D15/0682	11	{on sliding blocks}	E05D15/06	E05D15/06		154
E05D15/0686	11	{Tracks (E05D15/0665&#160;-&#160;E05D15/0682 and E05D15/0691 take precedence)}	E05D15/06	E05D15/06		909
E05D15/0691	11	{Top guides}	E05D15/06	E05D15/06		337
E05D2015/0695	10	{Magnetic suspension or supporting means}	E05D15/06	E05D15/06		154
E05D15/08	9	consisting of two or more independent parts movable each in its own guides	E05D15/08	E05D15/08		587
E05D15/10	9	movable out of one plane into a second parallel plane	E05D15/10	E05D15/10		550
E05D15/1002	10	{specially adapted for use in railway-cars or mass transit vehicles (E05D15/1007, E05D15/1023, E05D15/1044, E05D15/1068 take precedence)}	E05D15/10	E05D15/10		197
E05D15/1005	10	{the wing being supported on arms movable in horizontal planes}	E05D15/10	E05D15/10		156
E05D15/1007	11	{specially adapted for use in railway-cars or mass transit vehicles}	E05D15/10	E05D15/10		162
E05D15/101	11	{specially adapted for vehicles (E05D15/1007 takes precedence)}	E05D15/10	E05D15/10		376
E05D15/1013	11	{specially adapted for windows}	E05D15/10	E05D15/10		173
E05D15/1015	12	{with an intermediate tilt position}	E05D15/10	E05D15/10		90
E05D2015/1018	10	{with the track rotating around its axis}	E05D15/10	E05D15/10		10
E05D15/1021	10	{involving movement in a third direction, e.g. vertically}	E05D15/10	E05D15/10		238
E05D15/1023	11	{specially adapted for use in railway-cars or mass transit vehicles}	E05D15/10	E05D15/10		25
E05D2015/1026	10	{accessories, e.g. sliding or rolling guides, latches}	E05D15/10	E05D15/10		331
E05D2015/1028	10	{with only the wing moving transversely}	E05D15/10	E05D15/10		82
E05D2015/1031	11	{the wing supported on arms extending from the carriage}	E05D15/10	E05D15/10		285
E05D2015/1034	12	{the carriage having means for preventing rotation of the wing}	E05D15/10	E05D15/10		33
E05D2015/1036	12	{the arms being movable in vertical, e.g. transverse, planes}	E05D15/10	E05D15/10		72
E05D2015/1039	11	{the wing sliding transversely on the carriage}	E05D15/10	E05D15/10		176
E05D15/1042	10	{with transversely moving carriage (E05D15/1065 takes precedence)}	E05D15/10	E05D15/10		321
E05D15/1044	11	{specially adapted for use in railway-cars or mass transit vehicles}	E05D15/10	E05D15/10		135
E05D15/1047	11	{specially adapted for vehicles (E05D15/1044 takes precedence)}	E05D15/10	E05D15/10		457
E05D2015/1049	11	{the carriage swinging or rotating in a transverse plane}	E05D15/10	E05D15/10		105
E05D2015/1052	11	{transversely over-dimensioned track sections or carriage}	E05D15/10	E05D15/10		64
E05D2015/1055	11	{with slanted or curved track sections or cams}	E05D15/10	E05D15/10		619
E05D2015/1057	12	{the carriage swinging or rotating in those track sections}	E05D15/10	E05D15/10		145
E05D2015/106	11	{transversely orientated track sections}	E05D15/10	E05D15/10		55
E05D2015/1063	11	{disconnecting the carriage from the track}	E05D15/10	E05D15/10		89
E05D15/1065	10	{with transversely moving track}	E05D15/10	E05D15/10		161
E05D15/1068	11	{specially adapted for use in railway-cars or mass transit vehicles}	E05D15/10	E05D15/10		254
E05D2015/1071	11	{the track being directly linked to the fixed frame, e.g. slidingly}	E05D15/10	E05D15/10		120
E05D2015/1073	12	{rocking transversely}	E05D15/10	E05D15/10		6
E05D2015/1076	12	{swinging transversely, e.g. on arms}	E05D15/10	E05D15/10		100
E05D2015/1078	12	{swinging or rotating in a horizontal plane}	E05D15/10	E05D15/10		39
E05D15/1081	11	{specially adapted for vehicles (E05D15/1068 takes precedence)}	E05D15/10	E05D15/10		198
E05D2015/1084	11	{the carriage being directly linked to the fixed frame, e.g. slidingly}	E05D15/10	E05D15/10		50
E05D2015/1086	12	{swingingly, e.g. on arms}	E05D15/10	E05D15/10		157
E05D2015/1089	13	{the carriage having means for preventing rotation of the wing}	E05D15/10	E05D15/10		58
E05D2015/1092	13	{the carriage swinging or rotating in curved track sections}	E05D15/10	E05D15/10		26
E05D2015/1094	13	{disconnecting itself from the track}	E05D15/10	E05D15/10		3
E05D2015/1097	11	{with the carriage and track forming a telescopic element}	E05D15/10	E05D15/10		62
E05D15/12	9	consisting of parts connected at their edges	E05D15/12	E05D15/12		238
E05D15/14	9	with movable arms situated in the plane of the wing	E05D15/14	E05D15/14		144
E05D15/16	8	for wings sliding vertically more or less in their own plane	E05D15/16	E05D15/16		236
E05D15/165	9	{Details, e.g. sliding or rolling guides (E05D15/18&#160;-&#160;E05D15/24 take precedence)}	E05D15/16	E05D15/16		994
E05D15/18	9	consisting of two or more independent parts, movable each in its own guides	E05D15/18	E05D15/18		103
E05D15/20	9	movable out of one plane into a second parallel plane	E05D15/20	E05D15/20		168
E05D15/22	9	allowing an additional movement {(E05D15/20 takes precedence)}	E05D15/22	E05D15/22		510
E05D2015/225	10	{specially adapted for overhead wings}	E05D15/22	E05D15/22		50
E05D15/24	9	consisting of parts connected at their edges	E05D15/24	E05D15/24		916
E05D15/242	10	{Hinge connections between the parts}	E05D15/24	E05D15/24		426
E05D15/244	10	{Upper part guiding means}	E05D15/24	E05D15/24		49
E05D15/246	11	{with additional guide rail for producing an additional movement}	E05D15/24	E05D15/24		176
E05D15/248	11	{with lever arms for producing an additional movement}	E05D15/24	E05D15/24		98
E05D15/26	8	for folding wings	E05D15/26	E05D15/26		1087
E05D15/262	9	{folding vertically}	E05D15/26	E05D15/26		468
E05D15/264	9	{for bi-fold wings}	E05D15/26	E05D15/26		750
E05D15/266	10	{comprising two pivots placed at opposite edges of the wing}	E05D15/26	E05D15/26		168
E05D2015/268	9	{the wings being successively folded}	E05D15/26	E05D15/26		185
E05D15/28	8	supported on arms movable in horizontal plane	E05D15/28	E05D15/28		295
E05D15/30	9	with pivoted arms and sliding guides	E05D15/30	E05D15/30		935
E05D15/32	9	with two pairs of pivoted arms	E05D15/32	E05D15/32		197
E05D15/34	10	with wings opening parallel to themselves	E05D15/34	E05D15/34		180
E05D15/36	8	moving along slide-ways so arranged that one guide-member of the wing moves in a direction substantially perpendicular to the movement of another guide member	E05D15/36	E05D15/36		104
E05D15/38	9	for upwardly-moving wings, e.g. up-and-over doors	E05D15/38	E05D15/38		364
E05D15/40	8	supported on arms movable in vertical planes	E05D15/40	E05D15/40		348
E05D15/401	9	{specially adapted for overhead wings (E05D15/403&#160;-&#160;E05D15/46 take precedence)}	E05D15/40	E05D15/40		150
E05D15/403	9	{with arms fixed on the wing pivoting about an axis outside the wing}	E05D15/40	E05D15/40		163
E05D15/405	9	{with curved arms fixed on the wing, rolling on a support}	E05D15/40	E05D15/40		46
E05D15/406	9	{with pivoted arms and sliding guides (E05D15/42, E05D15/44 take precedence)}	E05D15/40	E05D15/40		101
E05D15/408	10	{with sliding guides fixed to the wing}	E05D15/40	E05D15/40		68
E05D15/42	9	with pivoted arms and horizontally-sliding guides	E05D15/42	E05D15/42		90
E05D15/425	10	{specially adapted for overhead wings}	E05D15/42	E05D15/42		239
E05D15/44	9	with pivoted arms and vertically-sliding guides	E05D15/44	E05D15/44		673
E05D15/445	10	{specially adapted for overhead wings}	E05D15/44	E05D15/44		275
E05D15/46	9	with two pairs of pivoted arms	E05D15/46	E05D15/46		309
E05D15/463	10	{specially adapted for overhead wings}	E05D15/46	E05D15/46		185
E05D15/466	10	{specially adapted for windows}	E05D15/46	E05D15/46		137
E05D15/48	8	allowing alternative movements ({E05D15/0604 takes precedence } ; for vertically-sliding wings E05D15/22)	E05D15/48	E05D15/48		737
E05D2015/482	9	{for panic doors}	E05D15/48	E05D15/48		73
E05D2015/485	9	{Swinging or sliding movements}	E05D15/48	E05D15/48		253
E05D2015/487	9	{Tilting or swinging movements}	E05D15/48	E05D15/48		86
E05D15/50	9	for opening at either of two opposite edges {(hinges or pivots of special construction to allow easy separation or connection of the parts at the hinge axis E05D7/10; to allow easy detachment of the hinge from the wing or the frame E05D7/12)}	E05D15/50	E05D15/50		264
E05D15/502	10	{by axial separation of the hinge parts at the hinge axis}	E05D15/50	E05D15/50		248
E05D15/505	10	{by radial separation of the hinge parts at the hinge axis}	E05D15/50	E05D15/50		250
E05D15/507	10	{by detachment of the hinge from the wing or the frame}	E05D15/50	E05D15/50		125
E05D15/52	9	for opening about a vertical as well as a horizontal axis	E05D15/52	E05D15/52		1316
E05D15/5202	10	{with non-horizontally extending checks}	E05D15/52	E05D15/52		89
E05D15/5205	10	{with horizontally-extending checks}	E05D15/52	E05D15/52		559
E05D15/5208	10	{with means for transmitting movements between vertical and horizontal sliding bars, rods or cables}	E05D15/52	E05D15/52		146
E05D15/5211	10	{Concealed suspension fittings}	E05D15/52	E05D15/52		226
E05D15/5214	10	{Corner supports}	E05D15/52	E05D15/52		301
E05D15/5217	10	{Tilt-lock devices}	E05D15/52	E05D15/52		117
E05D15/522	10	with disconnecting means for the appropriate pivoting parts	E05D15/522	E05D15/522		72
E05D15/523	11	using movable rods	E05D15/523	E05D15/523		65
E05D15/524	12	Actuating mechanisms	E05D15/524	E05D15/524		78
E05D15/526	10	Safety devices {(E05D15/5217 takes precedence)}	E05D15/526	E05D15/526		243
E05D2015/5263	11	{acting parallel to the plane of the wing}	E05D15/526	E05D15/526		17
E05D2015/5266	11	{acting perpendicular to the plane of the wing}	E05D15/526	E05D15/526		34
E05D15/54	9	for opening both inwards and outwards	E05D15/54	E05D15/54		270
E05D15/56	8	with successive different movements {(raising wings before being turned E05F7/02)}	E05D15/56	E05D15/56		316
E05D15/565	9	{for raising wings before sliding}	E05D15/56	E05D15/56		521
E05D15/58	9	with both swinging and sliding movements	E05D15/58	E05D15/58		1154
E05D15/581	10	{the swinging axis laying in the sliding direction (E05D15/1015 takes precedence)}	E05D15/58	E05D15/58		182
E05D15/582	10	{with horizontal swinging axis (E05D15/581 takes precedence)}	E05D15/58	E05D15/58		234
E05D15/583	11	{specially adapted for overhead wings}	E05D15/58	E05D15/58		141
E05D2015/585	10	{with stationary hinge parts}	E05D15/58	E05D15/58		49
E05D2015/586	10	{with travelling hinge parts}	E05D15/58	E05D15/58		303
E05D2015/587	10	{with axially separating hinge parts}	E05D15/58	E05D15/58		26
E05D2015/588	10	{with radially separating hinge parts}	E05D15/58	E05D15/58		49
E05D2700/00	7	Hinges or other suspension devices especially for doors or windows	CPCONLY	E05D2700/00		15
E05D2700/02	8	Hinges with one pivot axis and one bearing surface	CPCONLY	E05D2700/02		226
E05D2700/04	8	Hinges with one pivot axis and more than one bearing surface	CPCONLY	E05D2700/04		388
E05D2700/10	8	Various door and window fittings, e.g. suspension devices for double hung windows or screens	CPCONLY	E05D2700/10		274
E05D2700/12	8	Suspension devices for doors or windows movable in a direction perpendicular to their plane or pivotable about an axis being situated at a considerable distance from the edge of the wing by means of pivot arms	CPCONLY	E05D2700/12		211
