B25B1/00	7	Vices (specially adapted for tying flies for angling A01K97/28; specially adapted for machine tools B23Q3/00{; rope or cable splicing vices D07B7/162})	B25B1/00	B25B1/00		120
B25B1/02	8	with sliding jaws	B25B1/02	B25B1/02		825
B25B1/04	8	with pivoted jaws	B25B1/04	B25B1/04		207
B25B1/06	8	Arrangements for positively actuating jaws	B25B1/06	B25B1/06		297
B25B1/08	9	using cams	B25B1/08	B25B1/08		619
B25B1/10	9	using screws	B25B1/10	B25B1/10		528
B25B1/103	10	{with one screw perpendicular to the jaw faces, e.g. a differential or telescopic screw}	B25B1/10	B25B1/10		1519
B25B1/106	10	{with mechanical or hydraulic power amplifiers}	B25B1/10	B25B1/10		187
B25B1/12	10	with provision for disengagement	B25B1/12	B25B1/12		252
B25B1/125	11	{with one screw perpendicular to the jaw faces}	B25B1/12	B25B1/12		867
B25B1/14	9	using toggle links	B25B1/14	B25B1/14		100
B25B1/16	9	by pedal, with or without provision for additional manual actuation	B25B1/16	B25B1/16		127
B25B1/18	9	motor driven, e.g. with fluid drive, with or without provision for manual actuation	B25B1/18	B25B1/18		724
B25B1/20	8	Vices for clamping work of special profile, e.g. pipes	B25B1/20	B25B1/20		748
B25B1/205	9	{Vices of the chain or strip type}	B25B1/20	B25B1/20		340
B25B1/22	8	Arrangements for turning or tilting vices	B25B1/22	B25B1/22		918
B25B1/24	8	Details, e.g. jaws of special shape, slideways	B25B1/24	B25B1/24		787
B25B1/2405	9	{Construction of the jaws}	B25B1/24	B25B1/24		798
B25B1/241	10	{characterised by surface features or material}	B25B1/24	B25B1/24		336
B25B1/2415	11	{being composed of a plurality of parts adapting to the shape of the workpiece}	B25B1/24	B25B1/24		68
B25B1/2421	12	{the parts having a linear movement}	B25B1/24	B25B1/24		289
B25B1/2426	12	{the parts having a pivotal movement}	B25B1/24	B25B1/24		124
B25B1/2431	10	{the whole jaw being pivotable around an axis perpendicular to the actioning direction of the vice}	B25B1/24	B25B1/24		20
B25B1/2436	11	{around a vertical axis (B25B1/2447 takes precedence)}	B25B1/24	B25B1/24		131
B25B1/2442	11	{around a horizontal axis (B25B1/2447 takes precedence)}	B25B1/24	B25B1/24		41
B25B1/2447	11	{to put one of the jaw faces in a position opposite to the second jaw}	B25B1/24	B25B1/24		51
B25B1/2452	10	{with supplementary jaws}	B25B1/24	B25B1/24		622
B25B1/2457	10	{with auxiliary attachments}	B25B1/24	B25B1/24		271
B25B1/2463	11	{Supports for the workpiece}	B25B1/24	B25B1/24		193
B25B1/2468	11	{Lateral positioning arms}	B25B1/24	B25B1/24		87
B25B1/2473	10	{with pull-down action on the workpiece}	B25B1/24	B25B1/24		274
B25B1/2478	10	{with more than one pair of jaws}	B25B1/24	B25B1/24		281
B25B1/2484	9	{Supports}	B25B1/24	B25B1/24		614
B25B1/2489	9	{Slideways}	B25B1/24	B25B1/24		422
B25B1/2494	9	{Means indicating the distance between jaws or their angular position}	B25B1/24	B25B1/24		87
B25B3/00	7	Hand vices, i.e. vices intended to be held by hand; Pin vices	B25B3/00	B25B3/00		170
B25B5/00	7	Clamps (for holding or positioning work for welding, soldering, or cutting by applying heat locally B23K37/04)	B25B5/00	B25B5/00		319
B25B5/003	8	{Combinations of clamps}	B25B5/00	B25B5/00		1025
B25B5/006	8	{Supporting devices for clamps}	B25B5/00	B25B5/00		1131
B25B5/02	8	with sliding jaws	B25B5/02	B25B5/02		598
B25B5/04	8	with pivoted jaws	B25B5/04	B25B5/04		722
B25B5/06	8	Arrangements for positively actuating jaws	B25B5/06	B25B5/06		1194
B25B5/061	9	{with fluid drive (B25B5/087, B25B5/122 take precedence)}	B25B5/06	B25B5/06		1007
B25B5/062	10	{with clamping means pivoting around an axis parallel to the pressing direction}	B25B5/06	B25B5/06		218
B25B5/064	10	{with clamping means pivoting around an axis perpendicular to the pressing direction (B25B5/122 takes precedence)}	B25B5/06	B25B5/06		305
B25B5/065	10	{involving the use of flexible pressure bags or diaphragms}	B25B5/06	B25B5/06		211
B25B5/067	9	{C-clamps (B25B5/061, B25B5/082, B25B5/101, B25B5/125 take precedence)}	B25B5/06	B25B5/06		142
B25B5/068	9	{with at least one jaw sliding along a bar (B25B5/061, B25B5/085, B25B5/102, B25B5/127 take precedence)}	B25B5/06	B25B5/06		646
B25B5/08	9	using cams	B25B5/08	B25B5/08		1046
B25B5/082	10	{C-clamps}	B25B5/08	B25B5/08		59
B25B5/085	10	{with at least one jaw sliding along a bar}	B25B5/08	B25B5/08		211
B25B5/087	10	{actuated by a hydraulic or pneumatic piston}	B25B5/08	B25B5/08		417
B25B5/10	9	using screws	B25B5/10	B25B5/10		1386
B25B5/101	10	{C-clamps}	B25B5/10	B25B5/10		697
B25B5/102	10	{with at least one jaw sliding along a bar}	B25B5/10	B25B5/10		879
B25B5/103	10	{with a hinge}	B25B5/10	B25B5/10		232
B25B5/104	10	{with one screw and one clamping lever and one fulcrum element}	B25B5/10	B25B5/10		85
B25B5/105	11	{with one end of the lever resting on a table and the screw being positioned between the ends of the lever}	B25B5/10	B25B5/10		87
B25B5/106	11	{with one end of the lever resting on an additional block and the screw being positioned between the ends of the lever}	B25B5/10	B25B5/10		188
B25B5/107	12	{Blocks therefor}	B25B5/10	B25B5/10		103
B25B5/108	11	{the screw contacting one of the ends of the lever}	B25B5/10	B25B5/10		119
B25B5/109	10	{with two screws, e.g. parallel screw clamps}	B25B5/10	B25B5/10		183
B25B5/12	9	using toggle links	B25B5/12	B25B5/12		755
B25B5/122	10	{with fluid drive}	B25B5/12	B25B5/12		555
B25B5/125	10	{C-clamps}	B25B5/12	B25B5/12		49
B25B5/127	10	{with at least one jaw sliding along a bar}	B25B5/12	B25B5/12		116
B25B5/14	8	Clamps for work of special profile {(using chains or strips B25B1/205)}	B25B5/14	B25B5/14		860
B25B5/142	9	{for windows and frames}	B25B5/14	B25B5/14		659
B25B5/145	9	{for plates}	B25B5/14	B25B5/14		385
B25B5/147	9	{for pipes}	B25B5/14	B25B5/14		991
B25B5/16	8	Details, e.g. jaws, jaw attachments	B25B5/16	B25B5/16		1180
B25B5/163	9	{Jaws or jaw attachments}	B25B5/16	B25B5/16		1679
B25B5/166	9	{Slideways; Guiding and/or blocking means for jaws thereon}	B25B5/16	B25B5/16		503
B25B7/00	7	Pliers; Other hand-held gripping tools with jaws on pivoted limbs; Details applicable generally to pivoted-limb hand tools (implements for fastening, connecting, or tensioning wire or strip B25B25/00; adapted for other fitting or separating purposes B25B27/00; for marking animals A01K11/00; dentists&apos; forceps A61C3/00; bending wire eyes B21F1/06; hand-held metal-shearing or metal-cutting devices B23D29/00; hand cutting tools B26B; for punching or perforating B26F1/36; devices for securing ends of binding material in bundling machines B65B13/24; specially designed for watch-making or comparable work G04D1/00)	B25B7/00	B25B7/00		1305
B25B7/02	8	Jaws	B25B7/02	B25B7/02		3012
B25B7/04	9	adjustable	B25B7/04	B25B7/04		982
B25B7/06	8	Joints	B25B7/06	B25B7/06		274
B25B7/08	9	with fixed fulcrum	B25B7/08	B25B7/08		506
B25B7/10	9	with adjustable fulcrum	B25B7/10	B25B7/10		1150
B25B7/12	8	involving special transmission means between the handles and the jaws, e.g. toggle levers, gears	B25B7/12	B25B7/12		1593
B25B7/123	9	{with self-locking toggle levers}	B25B7/12	B25B7/12		752
B25B7/126	9	{with fluid drive}	B25B7/12	B25B7/12		170
B25B7/14	8	Locking means {(B25B7/123 takes precedence)}	B25B7/14	B25B7/14		520
B25B7/16	9	combined with means for tightening the operating arms of jaws	B25B7/16	B25B7/16		271
B25B7/18	8	Adjusting means for the operating arms	B25B7/18	B25B7/18		486
B25B7/20	8	Pliers for sealing	B25B7/20	B25B7/20		222
B25B7/22	8	Pliers provided with auxiliary tool elements, e.g. cutting edges, nail extractors (for removing insulation or armouring from electric cables H02G1/12)	B25B7/22	B25B7/22		1316
B25B9/00	7	Hand-held gripping tools other than those covered by group B25B7/00(wrenches B25B13/00; specially adapted for watchmakers&apos; or like use G04D)	B25B9/00	B25B9/00		1489
B25B9/02	8	without sliding or pivotal connections, e.g. tweezers, onepiece tongs	B25B9/02	B25B9/02		1204
B25B9/04	8	with sliding jaws	B25B9/04	B25B9/04		83
B25B11/00	7	Work holders not covered by any preceding group in the subclass, e.g. magnetic work holders, vacuum work holders (for holding or positioning work for welding, soldering, or cutting by applying heat locally B23K37/04; specially adapted to machine tools B23Q3/00)	B25B11/00	B25B11/00		21497
B25B11/002	8	{Magnetic work holders}	B25B11/00	B25B11/00		1095
B25B11/005	8	{Vacuum work holders}	B25B11/00	B25B11/00		2421
B25B11/007	9	{portable, e.g. handheld}	B25B11/00	B25B11/00		725
B25B11/02	8	Assembly jigs	B25B11/02	B25B11/02		10386
B25B13/00	7	Spanners; Wrenches (hand-driven gear-operated B25B17/00; impact wrenches B25B19/00; portable power-driven B25B21/00{; spanners or wrenches pecially adapted for osteosynthesis A61B17/8875}; machines for fitting together or separating metal parts B23P19/00{; for mounting or dismounting wheels B60B29/003})	B25B13/00	B25B13/00		578
B25B13/005	8	{Cross wrenches}	B25B13/00	B25B13/00		166
B25B13/02	8	with rigid jaws (B25B13/46, B25B13/48 take precedence)	B25B13/02	B25B13/02		529
B25B13/04	9	of ring jaw type	B25B13/04	B25B13/04		1208
B25B13/06	9	of socket type	B25B13/06	B25B13/06		3100
B25B13/065	10	{characterised by the cross-section of the socket}	B25B13/06	B25B13/06		893
B25B13/08	9	of open jaw type	B25B13/08	B25B13/08		1810
B25B13/10	8	with adjustable jaws (B25B13/46, B25B13/48{B25B13/5041} take precedence)	B25B13/10	B25B13/10		428
B25B13/102	9	{composed of a plurality of sockets slidable in each other}	B25B13/10	B25B13/10		249
B25B13/105	9	{composed of a plurality of slidable pins}	B25B13/10	B25B13/10		94
B25B13/107	9	{composed of a main body with exchangeable inserts}	B25B13/10	B25B13/10		189
B25B13/12	9	the jaws being slidable	B25B13/12	B25B13/12		1659
B25B13/14	10	by rack and pinion, worm or gear	B25B13/14	B25B13/14		1820
B25B13/16	10	by screw or nut	B25B13/16	B25B13/16		1691
B25B13/18	10	by cam, wedge, or lever	B25B13/18	B25B13/18		550
B25B13/20	10	Arrangements for locking the jaws	B25B13/20	B25B13/20		250
B25B13/22	11	by ratchet action or toothed bars	B25B13/22	B25B13/22		1502
B25B13/24	11	by cam, wedge, or friction means	B25B13/24	B25B13/24		345
B25B13/26	11	by toggle links	B25B13/26	B25B13/26		69
B25B13/28	9	the jaws being pivotally movable	B25B13/28	B25B13/28		827
B25B13/30	10	by screw or nut	B25B13/30	B25B13/30		120
B25B13/32	10	by cam, wedge or lever	B25B13/32	B25B13/32		191
B25B13/34	10	Arrangements for locking the jaws	B25B13/34	B25B13/34		55
B25B13/36	11	by ratchet action	B25B13/36	B25B13/36		58
B25B13/38	11	by cam, wedge, or friction means	B25B13/38	B25B13/38		27
B25B13/40	11	by toggle links	B25B13/40	B25B13/40		17
B25B13/42	11	with self-locking action	B25B13/42	B25B13/42		14
B25B13/44	8	of the chuck type	B25B13/44	B25B13/44		620
B25B13/46	8	of the ratchet type, for providing a free return stroke of the handle	B25B13/46	B25B13/46		1696
B25B13/461	9	{with concentric driving and driven member}	B25B13/46	B25B13/46		723
B25B13/462	10	{the ratchet parts engaging in a direction radial to the tool operating axis}	B25B13/46	B25B13/46		709
B25B13/463	11	{a pawl engaging an externally toothed wheel}	B25B13/46	B25B13/46		3096
B25B13/465	11	{a pawl engaging an internally toothed ring}	B25B13/46	B25B13/46		560
B25B13/466	10	{the ratchet parts engaging in an axial direction}	B25B13/46	B25B13/46		259
B25B13/467	10	{which are gear-operated}	B25B13/46	B25B13/46		441
B25B13/468	10	{with possibility of locking the ratchet mechanism}	B25B13/46	B25B13/46		201
B25B13/48	8	for special purposes	B25B13/48	B25B13/48		3507
B25B13/481	9	{for operating in areas having limited access}	B25B13/48	B25B13/48		1891
B25B13/483	9	{for spark plugs}	B25B13/48	B25B13/48		159
B25B13/485	9	{for theft-proof screws, bolts or nuts}	B25B13/48	B25B13/48		337
B25B13/486	10	{using a threaded connection between screw and tool}	B25B13/48	B25B13/48		39
B25B13/488	9	{for connections where two parts must be turned in opposite directions by one tool}	B25B13/48	B25B13/48		307
B25B13/50	9	for operating on work of special profile, e.g. pipes	B25B13/50	B25B13/50		908
B25B13/5008	10	{for operating on pipes or cylindrical objects (B25B13/52 takes precedence)}	B25B13/50	B25B13/50		137
B25B13/5016	11	{by externally gripping the pipe}	B25B13/50	B25B13/50		245
B25B13/5025	12	{using a pipe wrench type tool}	B25B13/50	B25B13/50		43
B25B13/5033	13	{with fixed jaws}	B25B13/50	B25B13/50		54
B25B13/5041	13	{with movable or adjustable jaws}	B25B13/50	B25B13/50		67
B25B13/505	14	{Pivotally moving or adjustable}	B25B13/50	B25B13/50		610
B25B13/5058	14	{Linearly moving or adjustable, e.g. with an additional small tilting or rocking movement}	B25B13/50	B25B13/50		1110
B25B13/5066	12	{using rollers moving along radial cams in a cage structure at least partially surrounding the pipe}	B25B13/50	B25B13/50		45
B25B13/5075	12	{using jaws moving along radial cams or by excentric disks in a cage structure at least partially surrounding the pipe}	B25B13/50	B25B13/50		68
B25B13/5083	11	{by internally gripping the pipe}	B25B13/50	B25B13/50		100
B25B13/5091	10	{for operating on wing nuts, hooks, eye hooks or the like}	B25B13/50	B25B13/50		410
B25B13/52	10	Chain or strap wrenches	B25B13/52	B25B13/52		1003
B25B13/54	10	Internal grip wrenches {(B25B13/5083 takes precedence)}	B25B13/54	B25B13/54		241
B25B13/56	8	Spanner sets	B25B13/56	B25B13/56		1136
B25B13/58	8	Jaw attachments	B25B13/58	B25B13/58		390
B25B15/00	7	Screwdrivers (hand-driven gear-operated B25B17/00; impact screwdrivers B25B19/00; portable power-driven B25B21/00{; screwdrivers specially adapted for osteosynthesis A61B17/8875})	B25B15/00	B25B15/00		886
B25B15/001	8	{characterised by material or shape of the tool bit}	B25B15/00	B25B15/00		795
B25B15/002	9	{characterised by material used or surface finishing}	B25B15/00	B25B15/00		149
B25B15/004	9	{characterised by cross-section}	B25B15/00	B25B15/00		320
B25B15/005	10	{with cross- or star-shaped cross-section}	B25B15/00	B25B15/00		805
B25B15/007	10	{with blade of flat or substantially flat cross-section}	B25B15/00	B25B15/00		491
B25B15/008	10	{Allen-type keys}	B25B15/00	B25B15/00		823
B25B15/02	8	operated by rotating the handle	B25B15/02	B25B15/02		2297
B25B15/04	9	with ratchet action	B25B15/04	B25B15/04		997
B25B15/06	8	operated by axial movement of the handle	B25B15/06	B25B15/06		380
B25B17/00	7	Hand-driven gear-operated wrenches or screwdrivers (ratchet-operated B25B13/46{B25B13/467}, B25B15/04; {for mounting or dismounting wheels B60B29/005})	B25B17/00	B25B17/00		1191
B25B17/02	8	providing for torque amplification	B25B17/02	B25B17/02		436
B25B19/00	7	Impact wrenches or screwdrivers (portable power-driven B25B21/02)	B25B19/00	B25B19/00		507
B25B21/00	7	Portable power-driven screw or nut setting or loosening tools; (details or components, e.g. casings, bodies, of portable power-driven tools not particularly related to the operation performed B25F5/00; {for mounting or dismounting wheels B60B29/006}); Attachments for drilling apparatus serving the same purpose (machines B23P19/06)	B25B21/00	B25B21/00		4913
B25B21/001	8	{Combined nut setting and crimping}	B25B21/00	B25B21/00		156
B25B21/002	8	{for special purposes}	B25B21/00	B25B21/00		1465
B25B21/004	8	{of the ratchet type}	B25B21/00	B25B21/00		523
B25B21/005	9	{driven by a radially acting hydraulic or pneumatic piston}	B25B21/00	B25B21/00		498
B25B21/007	8	{Attachments for drilling apparatus for screw or nut setting or loosening}	B25B21/00	B25B21/00		527
B25B21/008	8	{with automatic change-over from high speed-low torque mode to low speed-high torque mode}	B25B21/00	B25B21/00		258
B25B21/02	8	with means for imparting impact to screwdriver blade or nut socket	B25B21/02	B25B21/02		1758
B25B21/023	9	{for imparting an axial impact, e.g. for self-tapping screws}	B25B21/02	B25B21/02		219
B25B21/026	9	{Impact clutches}	B25B21/02	B25B21/02		665
B25B23/00	7	Details of, or accessories for, spanners, wrenches, screwdrivers (bolt tensioners B25B29/02)	B25B23/00	B25B23/00		3333
B25B23/0007	8	{Connections or joints between tool parts}	B25B23/00	B25B23/00		777
B25B23/0014	9	{Screwdriver- or wrench-heads provided with cardan joints or the like}	B25B23/00	B25B23/00		326
B25B23/0021	9	{Prolongations interposed between handle and tool}	B25B23/00	B25B23/00		790
B25B23/0028	9	{Angular adjustment means between tool head and handle}	B25B23/00	B25B23/00		847
B25B23/0035	9	{Connection means between socket or screwdriver bit and tool}	B25B23/00	B25B23/00		3155
B25B23/0042	9	{Connection means between screwdriver handle and screwdriver shaft}	B25B23/00	B25B23/00		503
B25B23/005	8	{Screw guiding means}	B25B23/00	B25B23/00		280
B25B23/0057	8	{Socket or nut ejector means}	B25B23/00	B25B23/00		248
B25B23/0064	8	{Means for adjusting screwing depth}	B25B23/00	B25B23/00		337
B25B23/0071	8	{Abutment for screws or nuts}	B25B23/00	B25B23/00		189
B25B23/0078	8	{Reaction arms}	B25B23/00	B25B23/00		395
B25B23/0085	8	{Counterholding devices}	B25B23/00	B25B23/00		428
B25B23/0092	8	{Tools for placing nut or screw lock wires}	B25B23/00	B25B23/00		21
B25B23/02	8	Arrangements for handling screws or nuts	B25B23/02	B25B23/02		290
B25B23/04	9	for feeding screws or nuts	B25B23/04	B25B23/04		657
B25B23/045	10	{using disposable strips or discs carrying the screws or nuts}	B25B23/04	B25B23/04		389
B25B23/06	10	using built-in magazine (B25B23/045 takes precedence)	B25B23/06	B25B23/06		303
B25B23/065	11	{the magazine being coaxial with the tool axis}	B25B23/06	B25B23/06		162
B25B23/08	9	for holding or positioning screw or nut prior to or during its rotation	B25B23/08	B25B23/08		477
B25B23/10	10	using mechanical gripping means	B25B23/10	B25B23/10		1102
B25B23/101	11	{for hand-driven screw-drivers (B25B23/105 takes precedence)}	B25B23/10	B25B23/10		672
B25B23/103	11	{for gripping threaded studs}	B25B23/10	B25B23/10		408
B25B23/105	11	{the gripping device being an integral part of the driving bit}	B25B23/10	B25B23/10		229
B25B23/106	12	{the driving bit being a blade}	B25B23/10	B25B23/10		258
B25B23/108	12	{the driving bit being a Philips type bit, an Allen type bit or a socket}	B25B23/10	B25B23/10		456
B25B23/12	10	using magnetic means	B25B23/12	B25B23/12		1118
B25B23/14	8	Arrangement of torque limiters or torque indicators in wrenches or screwdrivers (couplings for transmitting rotation or clutches F16D; devices for measuring torque per seG01L)	B25B23/14	B25B23/14		1561
B25B23/1405	9	{for impact wrenches or screwdrivers}	B25B23/14	B25B23/14		212
B25B23/141	9	{Mechanical overload release couplings}	B25B23/14	B25B23/14		1113
B25B23/1415	9	{Break members; Arrangements specially adapted for break-bolts (break-bolts per seF16B31/00)}	B25B23/14	B25B23/14		191
B25B23/142	9	specially adapted for hand operated wrenches or screwdrivers	B25B23/142	B25B23/142		432
B25B23/1422	10	{torque indicators or adjustable torque limiters}	B25B23/142	B25B23/142		251
B25B23/1425	11	{by electrical means}	B25B23/142	B25B23/142		775
B25B23/1427	11	{by mechanical means}	B25B23/142	B25B23/142		1753
B25B23/145	9	specially adapted for fluid operated wrenches or screwdrivers	B25B23/145	B25B23/145		593
B25B23/1453	10	{for impact wrenches or screwdrivers}	B25B23/145	B25B23/145		316
B25B23/1456	10	{having electrical components}	B25B23/145	B25B23/145		268
B25B23/147	9	specially adapted for electrically operated wrenches or screwdrivers	B25B23/147	B25B23/147		1220
B25B23/1475	10	{for impact wrenches or screwdrivers}	B25B23/147	B25B23/147		374
B25B23/15	9	having a mechanism to mark the work when the selected torque is applied to the work	B25B23/15	B25B23/15		107
B25B23/16	8	Handles (in general B25G)	B25B23/16	B25B23/16		1898
B25B23/18	8	Devices for illuminating the head of the screw or the nut	B25B23/18	B25B23/18		957
B25B25/00	7	Implements for fastening, connecting or tensioning of wire or strip	B25B25/00	B25B25/00		1057
B25B25/005	8	{for applying wire clasps to hose couplings}	B25B25/00	B25B25/00		622
B25B27/00	7	Hand tools, specially adapted for fitting together or separating parts or objects whether or not involving some deformation, not otherwise provided for (machines for simply fitting together or separating metal parts or objects B23P19/00)	B25B27/00	B25B27/00		6237
B25B27/0007	8	{Tools for fixing internally screw-threaded tubular fasteners}	B25B27/00	B25B27/00		243
B25B27/0014	9	{motor-driven}	B25B27/00	B25B27/00		328
B25B27/0021	8	{Tools for bonding or debonding brake linings}	B25B27/00	B25B27/00		162
B25B27/0028	8	{Tools for removing or installing seals (B25B27/0092 takes precedence)}	B25B27/00	B25B27/00		1467
B25B27/0035	8	{for motor-vehicles (wrenches for mounting or dismounting wheels B60B29/003)}	B25B27/00	B25B27/00		2145
B25B27/0042	9	{Tools for removing or replacing filters or for draining oil; Tools for setting or loosening closure means for radiators, batteries, or the like}	B25B27/00	B25B27/00		401
B25B27/005	9	{for pulling off battery terminals}	B25B27/00	B25B27/00		76
B25B27/0057	9	{for screwing or unscrewing tyre valve caps}	B25B27/00	B25B27/00		99
B25B27/0064	9	{for assembling or disassembling clutches}	B25B27/00	B25B27/00		152
B25B27/0071	8	{for bicycles}	B25B27/00	B25B27/00		380
B25B27/0078	8	{Tools for wheel weights}	B25B27/00	B25B27/00		46
B25B27/0085	8	{explosive-powered}	B25B27/00	B25B27/00		157
B25B27/0092	8	{Tools moving along strips, e.g. decorating or sealing strips, to insert them in, or remove them from, grooves or profiles (machines therefor B23P19/047)}	B25B27/00	B25B27/00		381
B25B27/02	8	for connecting objects by press fit or detaching same {(B25D1/16 takes precedence)}	B25B27/02	B25B27/02		4966
B25B27/023	9	{using screws}	B25B27/02	B25B27/02		2410
B25B27/026	9	{fluid driven}	B25B27/02	B25B27/02		1601
B25B27/04	9	inserting or withdrawing keys	B25B27/04	B25B27/04		531
B25B27/06	9	inserting or withdrawing sleeves or bearing races	B25B27/06	B25B27/06		1358
B25B27/062	10	{using screws}	B25B27/06	B25B27/06		1292
B25B27/064	10	{fluid driven}	B25B27/06	B25B27/06		481
B25B27/08	9	inserting or withdrawing cotter pins	B25B27/08	B25B27/08		269
B25B27/10	9	inserting fittings into hoses	B25B27/10	B25B27/10		1914
B25B27/12	9	mounting or demounting piston rings	B25B27/12	B25B27/12		578
B25B27/14	8	for assembling objects other than by press fit or detaching same	B25B27/14	B25B27/14		4531
B25B27/143	9	{for installing wire thread inserts or tubular threaded inserts}	B25B27/14	B25B27/14		899
B25B27/146	9	{Clip clamping hand tools}	B25B27/14	B25B27/14		863
B25B27/16	9	abutted flanges	B25B27/16	B25B27/16		380
B25B27/18	9	withdrawing broken threaded parts or twist drills	B25B27/18	B25B27/18		740
B25B27/20	9	inserting or withdrawing split pins or circlips	B25B27/20	B25B27/20		606
B25B27/205	10	{Pliers or tweezer type tools with tow actuated jaws}	B25B27/20	B25B27/20		385
B25B27/22	9	positioning sprocket chains, endless tracks, antiskid chains (tools or implements for repairing chains using metal-working operations B21L21/00)	B25B27/22	B25B27/22		563
B25B27/24	9	mounting or demounting valves (for tyre valves B60C25/18)	B25B27/24	B25B27/24		933
B25B27/26	10	compressing the springs	B25B27/26	B25B27/26		1017
B25B27/28	9	positioning or withdrawing resilient bushings or the like	B25B27/28	B25B27/28		492
B25B27/30	9	positioning or withdrawing springs, e.g. coil or leaf springs (B25B27/26 takes precedence; watchmakers&apos; or watch-repairers&apos; tools G04D)	B25B27/30	B25B27/30		597
B25B27/302	10	{coil springs other than torsion coil springs}	B25B27/30	B25B27/30		45
B25B27/304	11	{by compressing coil springs}	B25B27/30	B25B27/30		475
B25B27/306	11	{by tensioning coil springs}	B25B27/30	B25B27/30		107
B25B27/308	10	{leaf springs}	B25B27/30	B25B27/30		91
B25B28/00	7	Portable power-driven joining or separation tools (B25B21/00 takes precedence)	B25B28/00	B25B28/00		172
B25B29/00	7	Accessories (specially for spanners, wrenches, screwdrivers B25B23/00; tool boxes, tool positioning stands B25H)	B25B29/00	B25B29/00		215
B25B29/02	8	Bolt tensioners	B25B29/02	B25B29/02		757
B25B31/00	7	Hand tools for applying fasteners (nailing or stapling tools B25C)	B25B31/00	B25B31/00		1037
B25B31/005	8	{for temporarily connecting sheets before or during assembly operations}	B25B31/00	B25B31/00		603
B25B33/00	7	Hand tools not covered by any other group in this subclass	B25B33/00	B25B33/00		1083
B25B33/005	8	{Chuck keys}	B25B33/00	B25B33/00		179
