B60J1/00	7	Windows; Windscreens; Accessories therefor (B60J10/00 takes precedence; air curtains instead of windows B60J9/04{; sealing strips for windshields B60J10/70; sealing sash guides for sliding window panes B60J10/74; glass partitions inside vehicles to protect occupants against personal attack B60R21/12})	B60J1/00	B60J1/00		1469
B60J1/001	8	{Double glazing for vehicles}	B60J1/00	B60J1/00		972
B60J1/002	8	{with means for clear vision, e.g. anti-frost or defog panes, rain shields (window heating in H05B3/84, H05B3/86)}	B60J1/00	B60J1/00		1068
B60J1/003	8	{Rear seat windscreens}	B60J1/00	B60J1/00		428
B60J1/004	8	{Mounting of windows}	B60J1/00	B60J1/00		426
B60J1/005	9	{using positioning means during mounting}	B60J1/00	B60J1/00		400
B60J1/006	9	{characterised by fixation means such as clips, adhesive, etc. (incorporated in seal B60J10/70)}	B60J1/00	B60J1/00		959
B60J1/007	9	{received in frames to be attached to vehicle}	B60J1/00	B60J1/00		380
B60J1/008	8	{of special shape, e.g. beveled edges, holes for attachment, bent windows, peculiar curvatures such as when being integrally formed with roof, door, etc.}	B60J1/00	B60J1/00		424
B60J1/02	8	arranged at the vehicle front {, e.g. structure of the glazing, mounting of the glazing (on windscreen mounted antenna wire H01Q1/1271)}	B60J1/02	B60J1/02		2225
B60J1/025	9	{Temporary windscreens}	B60J1/02	B60J1/02		66
B60J1/04	9	adjustable	B60J1/04	B60J1/04		1104
B60J1/06	10	comprising more than one pane	B60J1/06	B60J1/06		348
B60J1/08	8	arranged at vehicle sides	B60J1/08	B60J1/08		799
B60J1/085	9	{removably mounted}	B60J1/08	B60J1/08		598
B60J1/10	9	fixedly mounted {(B60J1/085 takes precedence)}	B60J1/10	B60J1/10		868
B60J1/12	9	adjustable	B60J1/12	B60J1/12		364
B60J1/14	10	with pivotal or rotary movement	B60J1/14	B60J1/14		1200
B60J1/16	10	slidable	B60J1/16	B60J1/16		729
B60J1/17	11	vertically	B60J1/17	B60J1/17		3913
B60J1/18	8	arranged at the vehicle rear {(optical viewing arrangements integrated in rear windows, e.g. Fresnel lenses B60R1/001)}	B60J1/18	B60J1/18		650
B60J1/1807	9	{movable for vehicles with convertible top}	B60J1/18	B60J1/18		24
B60J1/1815	10	{non-adjustably mounted in and moving with the soft-top cover}	B60J1/18	B60J1/18		374
B60J1/1823	10	{adjustable relative to hard- or soft-top, e.g. pivotable}	B60J1/18	B60J1/18		327
B60J1/183	11	{slidable}	B60J1/18	B60J1/18		156
B60J1/1838	9	{movable for non-convertible vehicles, including vehicles with versatile load area}	B60J1/18	B60J1/18		36
B60J1/1846	10	{where the window can slide}	B60J1/18	B60J1/18		47
B60J1/1853	11	{horizontally in direction transverse to vehicle longitudinal axis}	B60J1/18	B60J1/18		195
B60J1/1861	11	{vertically, e.g. into lower part of rear door before opening rear door}	B60J1/18	B60J1/18		142
B60J1/1869	11	{to an end position parallel to roof}	B60J1/18	B60J1/18		27
B60J1/1876	10	{where the window is pivotable relative to a stationary axis}	B60J1/18	B60J1/18		60
B60J1/1884	11	{about a horizontal axis}	B60J1/18	B60J1/18		205
B60J1/1892	10	{where the window is translated by a linkage system}	B60J1/18	B60J1/18		15
B60J1/20	8	Accessories, e.g. wind deflectors, blinds (antiglare provisions B60J3/00; wind deflectors associated with roof openings B60J7/22; removable external protective coverings for windows or windscreens B60J11/08{; aerodynamical spoiler for vehicles B62D35/00;} heating arrangements specially adapted for transparent or reflecting areas H05B3/84)	B60J1/20	B60J1/20		1789
B60J1/2002	9	{Wind deflectors specially adapted for preventing soiling, e.g. for side windows (integral with sealing arrangements B60J10/72)}	B60J1/20	B60J1/20		197
B60J1/2005	10	{for windscreens}	B60J1/20	B60J1/20		245
B60J1/2008	10	{for rear windows}	B60J1/20	B60J1/20		87
B60J1/2011	9	{Blinds; curtains or screens reducing heat or light intensity (means against intense light blinding the driver or passengers B60J3/00)}	B60J1/20	B60J1/20		1990
B60J1/2013	10	{Roller blinds (for roofs B60J7/0015; for luggage covering B60R5/047; for openings in buildings E06B9/40)}	B60J1/20	B60J1/20		315
B60J1/2016	11	{Control means for actuating the roller blind, e.g. using electronic control}	B60J1/20	B60J1/20		232
B60J1/2019	11	{powered, e.g. by electric, hydraulic or pneumatic actuators}	B60J1/20	B60J1/20		625
B60J1/2022	12	{with screw rods or extensible rods acting on the draw bar for pushing or push-pulling (pivoting arms B60J1/2055)}	B60J1/20	B60J1/20		88
B60J1/2025	12	{with flexible actuating elements connected to the draw bar for pulling only, e.g. cords, wires or cables}	B60J1/20	B60J1/20		168
B60J1/2027	12	{with a buckle-proof guided flexible actuating element acting on the draw bar for pushing or push-pulling, e.g. a Bowden cable}	B60J1/20	B60J1/20		205
B60J1/203	11	{Mechanism for actuation by hand, e.g. cranks or curtain cords}	B60J1/20	B60J1/20		296
B60J1/2033	11	{characterised by the spring motor}	B60J1/20	B60J1/20		197
B60J1/2036	11	{characterised by structural elements}	B60J1/20	B60J1/20		265
B60J1/2038	12	{Storage boxes}	B60J1/20	B60J1/20		288
B60J1/2041	12	{Blind sheets, e.g. shape of sheets, reinforcements in sheets, materials therefor}	B60J1/20	B60J1/20		396
B60J1/2044	12	{Draw bars, including elements attached to it, e.g. sliding shoes, gripping elements or pull cords}	B60J1/20	B60J1/20		473
B60J1/2047	12	{End position holding means, e.g. suction cups, hooks on a vehicle, indentations on guides}	B60J1/20	B60J1/20		414
B60J1/205	12	{Winding tubes, e.g. telescopic tubes or conically shaped tubes}	B60J1/20	B60J1/20		248
B60J1/2052	12	{Guides}	B60J1/20	B60J1/20		400
B60J1/2055	12	{Pivoting arms}	B60J1/20	B60J1/20		203
B60J1/2058	12	{Springs for compensating the number of windings of the blind on the tube in case winding tube and draw bar are driven together}	B60J1/20	B60J1/20		35
B60J1/2061	12	{Tensioning systems for keeping the blind taut when in use, other than spring motors}	B60J1/20	B60J1/20		212
B60J1/2063	11	{Mounting arrangements for roller blind or its storage box, e.g. integration into beltline or window frame}	B60J1/20	B60J1/20		570
B60J1/2066	11	{Arrangement of blinds in vehicles}	B60J1/20	B60J1/20		109
B60J1/2069	12	{of multiple blinds, e.g. more than one blind per window or per actuation system}	B60J1/20	B60J1/20		176
B60J1/2072	12	{Blinds with inclined or vertical orientation of the winding axis}	B60J1/20	B60J1/20		132
B60J1/2075	12	{specially adapted for fixed windows}	B60J1/20	B60J1/20		60
B60J1/2077	13	{for windshields}	B60J1/20	B60J1/20		395
B60J1/208	13	{for rear windows}	B60J1/20	B60J1/20		376
B60J1/2083	13	{for side windows, e.g. quarter windows}	B60J1/20	B60J1/20		96
B60J1/2086	12	{specially adapted for openable windows, e.g. side window}	B60J1/20	B60J1/20		582
B60J1/2088	10	{Lamellar or like blinds}	B60J1/20	B60J1/20		350
B60J1/2091	10	{Foldable sunscreens (B60J1/2088 takes precedence)}	B60J1/20	B60J1/20		503
B60J1/2094	9	{Protective means for window, e.g. additional panel or foil, against vandalism, dirt, wear, shattered glass, etc.}	B60J1/20	B60J1/20		452
B60J1/2097	9	{means to prevent rattling of vehicle windows (anti-rattling means for vehicle doors E05F7/02)}	B60J1/20	B60J1/20		220
B60J3/00	7	Antiglare equipment associated with windows or windscreens (optical viewing arrangements for vehicles B60R1/00); Sun visors for vehicles (sun visors having appliances for storing or holding personal property B60R7/05)	B60J3/00	B60J3/00		525
B60J3/002	8	{External sun shield, e.g. awning or visor}	B60J3/00	B60J3/00		1080
B60J3/005	9	{for side windows}	B60J3/00	B60J3/00		464
B60J3/007	8	{Sunglare reduction by coatings, interposed foils in laminar windows, or permanent screens (layered glass products B32B17/00; process of coating windows C03C17/00)}	B60J3/00	B60J3/00		437
B60J3/02	8	adjustable in position {(B60J3/002, B60J3/005 take precedence)}	B60J3/02	B60J3/02		1760
B60J3/0204	9	{Sun visors}	B60J3/02	B60J3/02		1273
B60J3/0208	10	{combined with auxiliary visor}	B60J3/02	B60J3/02		1662
B60J3/0213	10	{characterised by the mounting means (B60J3/0208 takes precedence)}	B60J3/02	B60J3/02		637
B60J3/0217	11	{Brackets for mounting the sun visor support arm to the vehicle}	B60J3/02	B60J3/02		472
B60J3/0221	12	{self mounting, i.e. no tools or screws required}	B60J3/02	B60J3/02		113
B60J3/0226	12	{comprising a ball joint or at least two axes of rotation}	B60J3/02	B60J3/02		104
B60J3/023	11	{Additional support bracket releasably holding the sun visor}	B60J3/02	B60J3/02		299
B60J3/0234	11	{Mounted slidably}	B60J3/02	B60J3/02		264
B60J3/0239	12	{and pivoting on a support arm (bearing members regulating the rotational friction on the support arm B60J3/0265)}	B60J3/02	B60J3/02		226
B60J3/0243	12	{sliding out from ceiling}	B60J3/02	B60J3/02		139
B60J3/0247	11	{using a suction cup}	B60J3/02	B60J3/02		104
B60J3/0252	11	{Structure of the support arm}	B60J3/02	B60J3/02		162
B60J3/0256	12	{telescopic}	B60J3/02	B60J3/02		46
B60J3/026	12	{articulated, e.g. comprising pivot joints or lazy-tong structure}	B60J3/02	B60J3/02		161
B60J3/0265	11	{Attachments of sun visors to mounting means including details of sun visor bearing member regulating the rotational friction on the support arm}	B60J3/02	B60J3/02		361
B60J3/0269	12	{in middle region of sun visor}	B60J3/02	B60J3/02		72
B60J3/0273	12	{on both end regions of sun visor}	B60J3/02	B60J3/02		130
B60J3/0278	10	{structure of the body (B60J3/0208, B60J3/0213 take precedence)}	B60J3/02	B60J3/02		1095
B60J3/0282	11	{specially adapted for a courtesy mirror}	B60J3/02	B60J3/02		745
B60J3/0286	9	{Sunglare reduction by temporary translucent screens or foils removably attached to window}	B60J3/02	B60J3/02		160
B60J3/0291	9	{Preventing dazzlement during driving in the dark}	B60J3/02	B60J3/02		163
B60J3/0295	10	{due to reflections in side or rear mirror}	B60J3/02	B60J3/02		34
B60J3/04	8	adjustable in transparency	B60J3/04	B60J3/04		2150
B60J3/06	8	using polarising effect	B60J3/06	B60J3/06		386
B60J5/00	7	Doors (B60J10/00 takes precedence; window aspects B60J1/00{; side board or tailgate structures for open load compartments B62D33/023})	B60J5/00	B60J5/00		944
B60J5/02	8	arranged at the vehicle front {(lids or bonnets B62D25/10)}	B60J5/02	B60J5/02		140
B60J5/04	8	arranged at the vehicle sides {(panel mounted arm-rests B60N2/78; wall liners B60R13/02; door edge guards B60R13/043; padded linings associated with the side doors B60R21/0428)}	B60J5/04	B60J5/04		2134
B60J5/0401	9	{Upper door structure}	B60J5/04	B60J5/04		238
B60J5/0402	10	{window frame details, including sash guides and glass runs}	B60J5/04	B60J5/04		1570
B60J5/0404	10	{Outside rear view mirror support}	B60J5/04	B60J5/04		274
B60J5/0405	10	{Inboard or outboard side of window frame formed integrally with the lower door structure}	B60J5/04	B60J5/04		139
B60J5/0406	10	{window frame formed separately as module}	B60J5/04	B60J5/04		119
B60J5/0408	10	{fastening window frame or parts of window frame to lower door structure}	B60J5/04	B60J5/04		161
B60J5/0409	10	{mechanism preventing outward displacement of window frame at high speeds (ventilation valves B60H)}	B60J5/04	B60J5/04		33
B60J5/0411	9	{Beltline}	B60J5/04	B60J5/04		306
B60J5/0412	9	{Lower door structure}	B60J5/04	B60J5/04		1081
B60J5/0413	10	{Inner panel, e.g. characterised by carrying components}	B60J5/04	B60J5/04		1033
B60J5/0415	10	{Outer panel}	B60J5/04	B60J5/04		600
B60J5/0416	10	{Assembly panels to be installed in doors as a module with components, e.g. lock or window lifter, attached thereto}	B60J5/04	B60J5/04		2179
B60J5/0418	10	{Water or sound barrier, e.g. watershields or seals between dry/wet compartment, sound or vibration dampers}	B60J5/04	B60J5/04		493
B60J5/0419	10	{Windows in lower door structures}	B60J5/04	B60J5/04		67
B60J5/042	9	{Reinforcement elements}	B60J5/04	B60J5/04		481
B60J5/0422	10	{Elongated type elements, e.g. beams, cables, belts or wires}	B60J5/04	B60J5/04		142
B60J5/0423	11	{characterised by position in the lower door structure}	B60J5/04	B60J5/04		102
B60J5/0425	12	{the elements being arranged essentially horizontal in the centre of the lower door structure (B60J5/0426&#160;-&#160;B60J5/0448 take precedence)}	B60J5/04	B60J5/04		436
B60J5/0426	12	{the elements being arranged at the beltline}	B60J5/04	B60J5/04		327
B60J5/0427	12	{the elements being arranged along the lower edge of door}	B60J5/04	B60J5/04		187
B60J5/0429	12	{the elements being arranged diagonally}	B60J5/04	B60J5/04		277
B60J5/043	12	{the elements being arranged vertically}	B60J5/04	B60J5/04		111
B60J5/0431	12	{the elements being arranged at the hinge area}	B60J5/04	B60J5/04		270
B60J5/0433	12	{the elements being arranged at the lock area}	B60J5/04	B60J5/04		189
B60J5/0434	12	{the elements being arranged at the handle area}	B60J5/04	B60J5/04		72
B60J5/0436	12	{the elements being arranged at the mirror area}	B60J5/04	B60J5/04		29
B60J5/0437	11	{characterised by the attachment means to the door, e.g. releasable attachment means}	B60J5/04	B60J5/04		715
B60J5/0438	11	{characterised by the type of elongated elements}	B60J5/04	B60J5/04		41
B60J5/044	12	{the elements being flexible, e.g. belts, cables or wires}	B60J5/04	B60J5/04		73
B60J5/0441	12	{the elements having a grid-like structure, i.e. interconnected or interwoven elements}	B60J5/04	B60J5/04		77
B60J5/0443	12	{Beams}	B60J5/04	B60J5/04		667
B60J5/0444	13	{characterised by a special cross section}	B60J5/04	B60J5/04		512
B60J5/0445	13	{formed of several elements arranged in series}	B60J5/04	B60J5/04		87
B60J5/0447	13	{formed of several elements arranged in parallel}	B60J5/04	B60J5/04		255
B60J5/0448	13	{with branched structures}	B60J5/04	B60J5/04		82
B60J5/045	10	{Panel type elements (B60J5/0455 takes precedence)}	B60J5/04	B60J5/04		546
B60J5/0451	10	{Block or short strip-type elements (beams B60J5/0443, position thereof B60J5/0423)}	B60J5/04	B60J5/04		519
B60J5/0452	10	{including foams or expanded materials}	B60J5/04	B60J5/04		339
B60J5/0454	11	{being expanded onto door panel and forming a laminar structure with door panel, e.g. a rib}	B60J5/04	B60J5/04		35
B60J5/0455	10	{integrated in door structure or other door elements, e.g. beam-like shapes stamped in inner door panel}	B60J5/04	B60J5/04		395
B60J5/0456	10	{Behaviour during impact}	B60J5/04	B60J5/04		218
B60J5/0458	11	{Passive coupling of the reinforcement elements to the door or to the vehicle body}	B60J5/04	B60J5/04		328
B60J5/0459	11	{Active coupling of the reinforcement elements to the door or to the vehicle body, e.g. through releasing of pressurized gas}	B60J5/04	B60J5/04		69
B60J5/0461	11	{characterised by a pre-defined mode of deformation or displacement in order to absorb impact}	B60J5/04	B60J5/04		315
B60J5/0462	11	{the impact being a frontal impact}	B60J5/04	B60J5/04		41
B60J5/0463	9	{Conceptual assembling of door, i.e. how door frame parts should be fitted together to form door}	B60J5/04	B60J5/04		395
B60J5/0465	10	{using tailored blanks}	B60J5/04	B60J5/04		31
B60J5/0466	10	{using cast parts}	B60J5/04	B60J5/04		49
B60J5/0468	9	{Fixation or mounting means specific for door components (fasteners in general F16B21/00)}	B60J5/04	B60J5/04		2038
B60J5/0469	10	{for door panels, e.g. hemming (hemming equipment B21D39/00)}	B60J5/04	B60J5/04		440
B60J5/047	9	{characterised by the opening or closing movement}	B60J5/04	B60J5/04		1404
B60J5/0472	10	{the door having a hinge axis in horizontal direction transverse to vehicle longitudinal axis}	B60J5/04	B60J5/04		233
B60J5/0473	10	{the door having a hinge axis in the direction of the vehicle longitudinal axis}	B60J5/04	B60J5/04		292
B60J2005/0475	10	{due to absence of the B-pillar}	B60J5/04	B60J5/04		58
B60J5/0476	10	{convertible doors, e.g. window frame is stored in lower door structure}	B60J5/04	B60J5/04		100
B60J5/0477	10	{with two doors opening in opposite direction}	B60J5/04	B60J5/04		146
B60J5/0479	11	{without B-pillar or releasable B-pillar, i.e. the pillar is moving with door}	B60J5/04	B60J5/04		330
B60J5/048	9	{characterised by the material}	B60J5/04	B60J5/04		183
B60J5/0481	10	{plastic}	B60J5/04	B60J5/04		375
B60J5/0483	10	{lightweight metal, e.g. aluminum, magnesium}	B60J5/04	B60J5/04		177
B60J5/0484	10	{hybrid, i.e. plastic moulded onto metal parts}	B60J5/04	B60J5/04		125
B60J5/0486	9	{Special type}	B60J5/04	B60J5/04		164
B60J5/0487	10	{simplified doors related to cabins of, e.g. golf carts, tractors, jeeps, cranes, forklifts, etc.}	B60J5/04	B60J5/04		473
B60J5/0488	10	{rectangular of shape, e.g. as found in old fashioned cars and coaches}	B60J5/04	B60J5/04		104
B60J5/049	10	{caravan door}	B60J5/04	B60J5/04		68
B60J5/0491	10	{lid, e.g. for luggage compartment accessible at vehicle side (B60J5/0498 takes precedence)}	B60J5/04	B60J5/04		146
B60J5/0493	9	{Appurtenances}	B60J5/04	B60J5/04		904
B60J5/0494	10	{Rain covers deployed upon opening door}	B60J5/04	B60J5/04		457
B60J5/0495	10	{Finger guards (for doors in general E06B7/36, with sensors E05F15/42)}	B60J5/04	B60J5/04		54
B60J5/0497	9	{for load transporting vehicles or public transport, e.g. lorries, trucks, buses}	B60J5/04	B60J5/04		611
B60J5/0498	10	{with rigid panels pivoting about a horizontal axis}	B60J5/04	B60J5/04		366
B60J5/06	9	slidable; foldable	B60J5/06	B60J5/06		2288
B60J5/062	10	{for utility vehicles or public transport (B60J5/08 takes precedence)}	B60J5/06	B60J5/06		1042
B60J5/065	11	{with non-rigid elements, e.g. side curtains (B60J7/062, B60J7/068 take precedence)}	B60J5/06	B60J5/06		503
B60J5/067	12	{vertically movable}	B60J5/06	B60J5/06		87
B60J5/08	10	of roller-blind type {made of rigid elements}	B60J5/08	B60J5/08		222
B60J5/10	8	arranged at the vehicle rear (B60J5/04 takes precedence {; bonnets or lids B62D25/10; tail gates for pick-up trucks B62D33/0273; counterbalancing E05F; springs, e.g. pneumatic F16F})	B60J5/10	B60J5/10		1055
B60J5/101	9	{for non-load transporting vehicles, i.e. family cars including vans}	B60J5/10	B60J5/10		1095
B60J5/102	10	{comprising door or part of door being pivotable downwards about horizontal axis to open position}	B60J5/10	B60J5/10		207
B60J5/103	11	{where lower door part moves independently from other door structures, e.g. by being hinged on the vehicle body}	B60J5/10	B60J5/10		223
B60J5/104	11	{where lower door part optionally moves independently, or follows as component the movement of the entire door structure, e.g. by being hinged in a door frame or releasably connected to upper door part}	B60J5/10	B60J5/10		66
B60J5/105	10	{comprising door or part of door being pivotable about vertical axis}	B60J5/10	B60J5/10		202
B60J5/106	10	{comprising door or part of door being moveable by a linkage system to open/close position}	B60J5/10	B60J5/10		264
B60J5/107	10	{constructional details, e.g. about door frame, panels, materials used, reinforcements}	B60J5/10	B60J5/10		1108
B60J5/108	9	{for load transporting vehicles or public transport, e.g. lorries, trucks, buses}	B60J5/10	B60J5/10		763
B60J5/12	9	slidable; foldable	B60J5/12	B60J5/12		259
B60J5/125	10	{for utility vehicles or public transport (B60J5/14 takes precedence)}	B60J5/12	B60J5/12		164
B60J5/14	10	of roller-blind type {made of rigid elements}	B60J5/14	B60J5/14		249
B60J7/00	7	Non-fixed roofs; Roofs with movable panels {, e.g. rotary sunroofs}(B60J10/00 takes precedence; window aspects B60J1/00; fixed roofs B62D25/06; mechanisms for operating wings E05F11/00, E05F15/00)	B60J7/00	B60J7/00		1099
B60J7/0007	8	{moveable head-liners, screens, curtains or blinds for ceilings}	B60J7/00	B60J7/00		407
B60J7/0015	9	{roller blind}	B60J7/00	B60J7/00		1051
B60J7/0023	9	{flexible and foldable}	B60J7/00	B60J7/00		201
B60J7/003	9	{one or more sliding rigid plate or lammellae}	B60J7/00	B60J7/00		418
B60J7/0038	10	{stored in stacked fashion}	B60J7/00	B60J7/00		61
B60J7/0046	9	{side blind between roof and panel in vent mode}	B60J7/00	B60J7/00		103
B60J7/0053	8	{Collapsible lateral roof side beams}	B60J7/00	B60J7/00		90
B60J7/0061	9	{where the beam moves inwardly during folding of roof, e.g. by swiveling, sliding or translation, to disconnect the beam from windshield header}	B60J7/00	B60J7/00		82
B60J7/0069	9	{where the beam itself is folded and moves inwardly, e.g. concertina type}	B60J7/00	B60J7/00		71
B60J7/0076	8	{separately collapsible C-pillars, e.g. by folding inwardly or sliding (B60J7/126 takes precedence)}	B60J7/00	B60J7/00		71
B60J7/0084	8	{Water draining for non-fixed roofs or roof panels (for fixed roofs not integral with roof structure B60R13/06, for fixed roofs integral with roof structure B62D25/07)}	B60J7/00	B60J7/00		446
B60J7/0092	9	{by inflating the roof (inflatable soft tops B60J7/1256)}	B60J7/00	B60J7/00		34
B60J7/02	8	of sliding type {, e.g. comprising guide shoes}	B60J7/02	B60J7/02		681
B60J7/022	9	{Sliding roof trays or assemblies}	B60J7/02	B60J7/02		656
B60J7/024	9	{characterised by the height regulating mechanism of the sliding panel (B60J7/043&#160;-&#160;B60J7/053 take precedence)}	B60J7/02	B60J7/02		415
B60J7/026	9	{with rigid non plate-like elements, e.g. for convertible vehicles}	B60J7/02	B60J7/02		209
B60J7/028	10	{the sliding movement being combined with a pivoting movement}	B60J7/02	B60J7/02		229
B60J7/04	9	with rigid plate-like element or elements {, e.g. open roofs with harmonica-type folding rigid panels (B60J7/061 takes precedence)}	B60J7/04	B60J7/04		735
B60J7/041	10	{for utility vehicles, e.g. with slidable and foldable rigid panels}	B60J7/04	B60J7/04		330
B60J7/042	11	{with a vertical lifting or folding movement (non-sliding roof panels movable for lifting B60J7/1614)}	B60J7/04	B60J7/04		82
B60J7/043	10	Sunroofs (B60J7/047&#160;-&#160;B60J7/053 take precedence){e.g. sliding above the roof}	B60J7/043	B60J7/043		1529
B60J7/0435	11	{pivoting upwardly to vent mode and moving at the outside of the roof to fully open mode}	B60J7/043	B60J7/043		661
B60J7/047	10	movable to overlapping or nested relationship {(B60J7/041 takes precedence)}	B60J7/047	B60J7/047		532
B60J7/05	10	pivoting upwardly to vent mode and moving downward before sliding to fully open mode	B60J7/05	B60J7/05		331
B60J7/053	10	sliding with final closing motion having vertical component to attain closed and sealed condition {, e.g. sliding under the roof}	B60J7/053	B60J7/053		300
B60J7/057	10	Driving or actuating arrangements (B60J7/047&#160;-&#160;B60J7/053 take precedence){e.g. manually operated levers or knobs}	B60J7/057	B60J7/057		734
B60J7/0573	11	{power driven arrangements, e.g. electrical}	B60J7/057	B60J7/057		1538
B60J7/0576	12	{fluid}	B60J7/057	B60J7/057		64
B60J7/06	9	with non-rigid element or elements	B60J7/06	B60J7/06		108
B60J7/061	10	{sliding and folding}	B60J7/06	B60J7/06		488
B60J7/062	11	{for utility vehicles (B60J7/065 takes precedence)}	B60J7/06	B60J7/06		641
B60J7/063	11	{for public transport (B60J7/066 takes precedence)}	B60J7/06	B60J7/06		96
B60J7/064	11	{using folding arms sliding in longitudinal tracks for supporting the soft roof}	B60J7/06	B60J7/06		123
B60J7/065	12	{for utility vehicles}	B60J7/06	B60J7/06		206
B60J7/066	12	{for public transport}	B60J7/06	B60J7/06		24
B60J7/067	10	{sliding and winding up}	B60J7/06	B60J7/06		201
B60J7/068	11	{for utility vehicles, e.g. of tarpaulin or roller-blind type}	B60J7/06	B60J7/06		245
B60J7/08	8	of non-sliding type, i.e. movable or removable roofs or panels, e.g. let-down tops or roofs capable of being easily detached or of assuming a collapsed or inoperative position	B60J7/08	B60J7/08		414
B60J7/085	9	{winding up, e.g. for utility vehicles}	B60J7/08	B60J7/08		724
B60J7/10	9	readily detachable, e.g. tarpaulins with frames, or fastenings for tarpaulins (covering of loads on vehicles by tarpaulins B60P7/04)	B60J7/10	B60J7/10		338
B60J7/102	10	{Readily detachable tarpaulins, e.g. for utility vehicles; Frames therefor}	B60J7/10	B60J7/10		571
B60J7/104	11	{Fastening means for tarpaulins}	B60J7/10	B60J7/10		752
B60J7/106	10	{readily detachable hard-tops (storage compartment for collapsible flexible tops B60J7/20)}	B60J7/10	B60J7/10		403
B60J7/108	11	{Foldable rear hoods therefor}	B60J7/10	B60J7/10		49
B60J7/11	10	Removable panels, e.g. sunroofs	B60J7/11	B60J7/11		337
B60J7/12	9	foldable; Tensioning mechanisms therefor, e.g. struts (B60J7/10, {B60J7/20} take precedence)	B60J7/12	B60J7/12		235
B60J7/1204	10	{Control devices, e.g. for compensating tolerances, for defining movement or end position of top, for tensioning the top or for switching to an emergency mode}	B60J7/12	B60J7/12		415
B60J7/1226	10	{Soft tops for convertible vehicles}	B60J7/12	B60J7/12		414
B60J7/123	11	{characterised by means for fastening the soft top cloth to the arches or vehicle body work}	B60J7/12	B60J7/12		204
B60J7/1234	11	{characterised by arches, e.g. shape or material}	B60J7/12	B60J7/12		285
B60J7/1239	12	{Front bow}	B60J7/12	B60J7/12		68
B60J7/1243	12	{Intermediate bows}	B60J7/12	B60J7/12		81
B60J7/1247	12	{Tensioning bow at rear of soft top}	B60J7/12	B60J7/12		138
B60J7/1252	12	{characterised by lateral arches (foldable side roof beams B60J7/0053; linkage arms B60J7/1265)}	B60J7/12	B60J7/12		81
B60J7/1256	11	{Inflatable soft tops}	B60J7/12	B60J7/12		73
B60J7/126	11	{for landaulet-type vehicles, i.e. using a collapsible upper structure of the vehicle body}	B60J7/12	B60J7/12		282
B60J7/1265	11	{characterised by kinematic movements, e.g. using parallelogram linkages (B60J7/126 takes precedence)}	B60J7/12	B60J7/12		742
B60J7/1269	12	{with remote power control}	B60J7/12	B60J7/12		218
B60J7/1273	13	{using hydraulic means}	B60J7/12	B60J7/12		201
B60J7/1278	12	{the complete top rotating around a single main axis on the vehicle body (B60J7/1282 takes precedence)}	B60J7/12	B60J7/12		199
B60J7/1282	12	{foldable against a main arch before attaining fully open mode}	B60J7/12	B60J7/12		446
B60J7/1286	12	{including folding of the quarter windows}	B60J7/12	B60J7/12		35
B60J7/1291	10	{Soft tops for closed vehicle bodies}	B60J7/12	B60J7/12		207
B60J7/1295	10	{Temporary soft tops for seats outside passenger compartments, e.g. rumble seats, chauffeur seats}	B60J7/12	B60J7/12		154
B60J7/14	10	with a plurality of {rigid} plate-like elements {or rigid non plate-like elements, e.g. with non-slidable, but pivotable or foldable movement}	B60J7/14	B60J7/14		41
B60J7/141	11	{for covering load areas, e.g. for pick-up trucks}	B60J7/14	B60J7/14		570
B60J7/143	11	{for covering the passenger compartment}	B60J7/14	B60J7/14		167
B60J7/145	12	{at least two elements being folded in clamp-shell fashion}	B60J7/14	B60J7/14		435
B60J7/146	12	{all elements being folded in same orientation and stacked fashion}	B60J7/14	B60J7/14		348
B60J7/148	12	{at least one element being stored in vertical fashion}	B60J7/14	B60J7/14		98
B60J7/16	9	non-foldable {and rigid, e.g. a one-piece hard-top or a single rigid roof panel}(B60J7/10 takes precedence)	B60J7/16	B60J7/16		87
B60J7/1607	10	{for covering load areas, e.g. rigid panels for pick-up truck beds}	B60J7/16	B60J7/16		222
B60J7/1614	11	{with a vertical lifting movement maintaining the inclination of the roof or panel}	B60J7/16	B60J7/16		196
B60J7/1621	11	{hinged on one side}	B60J7/16	B60J7/16		388
B60J7/1628	10	{for covering the passenger compartment}	B60J7/16	B60J7/16		44
B60J7/1635	11	{of non-convertible vehicles}	B60J7/16	B60J7/16		39
B60J7/1642	12	{Roof panels, e.g. sunroofs or hatches, movable relative to the main roof structure, e.g. by lifting or pivoting}	B60J7/16	B60J7/16		779
B60J7/165	12	{at least a major part of the roof being lifted on all corners}	B60J7/16	B60J7/16		184
B60J7/1657	12	{at least a major part of the roof pivoting about a stationary axis}	B60J7/16	B60J7/16		188
B60J7/1664	11	{of convertible vehicles (foldable rear hoods for readily detachable hard-tops B60J7/108)}	B60J7/16	B60J7/16		36
B60J7/1671	12	{the roof pivoting about a stationary axis}	B60J7/16	B60J7/16		2
B60J7/1678	13	{the axis being horizontal}	B60J7/16	B60J7/16		66
B60J7/1685	13	{the axis being vertical}	B60J7/16	B60J7/16		12
B60J7/1692	12	{the roof being movable by a linkage system}	B60J7/16	B60J7/16		75
B60J7/185	8	Locking arrangements (locks in general E05B)	B60J7/185	B60J7/185		210
B60J7/1851	9	{for locking the foldable soft- or hard-top to the windshield header}	B60J7/185	B60J7/185		476
B60J7/1853	10	{locking mechanism arranged in windshield header}	B60J7/185	B60J7/185		44
B60J7/1855	9	{for locking or immobilising roof elements when stored}	B60J7/185	B60J7/185		307
B60J7/1856	9	{for interlocking the roof linkage system when deployed}	B60J7/185	B60J7/185		89
B60J7/1858	9	{for locking soft tops to a surrounding rigid roof structure, e.g. to a closed vehicle body (B60J7/1291 takes precedence)}	B60J7/185	B60J7/185		74
B60J7/19	9	for rigid panels {(B60J7/1851&#160;-&#160;B60J7/1856 take precedence)}	B60J7/19	B60J7/19		171
B60J7/192	10	{for locking the sunroof panel to the roof}	B60J7/19	B60J7/19		181
B60J7/194	10	{for locking detachable hard-tops or removable roof panels to the vehicle body}	B60J7/19	B60J7/19		131
B60J7/196	10	{for locking or interconnecting rigid roof panels to each other}	B60J7/19	B60J7/19		89
B60J7/198	10	{for locking tonneau covers such as covers for roof storage compartments or for pick-up truck beds}	B60J7/19	B60J7/19		279
B60J7/20	8	Vehicle storage compartments for roof parts {or for collapsible flexible tops}	B60J7/20	B60J7/20		359
B60J7/201	9	{being outside of vehicle, e.g. onto boot lid, or into a storage compartment to be closed by one of the roof panels itself}	B60J7/20	B60J7/20		246
B60J7/202	9	{being characterised by moveable cover parts for closing the gap between boot lid and rearmost seats}	B60J7/20	B60J7/20		417
B60J7/203	10	{the cover part comprising cover side flaps}	B60J7/20	B60J7/20		200
B60J7/205	9	{where the boot lid opens in rearward direction to receive the roof and in forward direction to receive luggage}	B60J7/20	B60J7/20		237
B60J7/206	9	{being arranged at the vehicle front}	B60J7/20	B60J7/20		23
B60J7/207	9	{being adjustable in volume, i.e. collapsible in order to increase luggage space in boot when roof is not stored}	B60J7/20	B60J7/20		144
B60J7/208	9	{with improved trunk access by moving the folded roof package when opening the trunk lid for loading or unloading luggage}	B60J7/20	B60J7/20		55
B60J7/22	8	Wind deflectors for open roofs	B60J7/22	B60J7/22		976
B60J7/223	9	{specially adapted for convertible cars}	B60J7/22	B60J7/22		593
B60J7/226	9	{immovably attached to vehicle roof section}	B60J7/22	B60J7/22		134
B60J9/00	7	Devices not provided for in one of main groups B60J1/00&#160;-&#160;B60J7/00(B60J10/00 takes precedence)	B60J9/00	B60J9/00		109
B60J9/02	8	Entrance or exit closures other than windows, doors, or in roofs, e.g. emergency escape closures in vehicle bottom {(emergency exits for rail vehicles B61D19/023)}	B60J9/02	B60J9/02		260
B60J9/04	8	Air curtains (in general F24F)	B60J9/04	B60J9/04		175
B60J10/00	7	Sealing arrangements	B60J10/00	B60J10/00		562
B60J10/15	8	characterised by the material	B60J10/15	B60J10/15		552
B60J10/16	9	consisting of two or more plastic materials having different physical or chemical properties (B60J10/17 takes precedence)	B60J10/16	B60J10/16		1062
B60J10/17	9	provided with a low-friction material on the surface	B60J10/17	B60J10/17		552
B60J10/18	9	provided with reinforcements or inserts	B60J10/18	B60J10/18		1003
B60J10/20	8	characterised by the shape	B60J10/20	B60J10/20		456
B60J10/21	9	having corner parts or bends	B60J10/21	B60J10/21		707
B60J10/22	9	having varying cross-section in the longitudinal direction	B60J10/22	B60J10/22		234
B60J10/23	9	assembled from two or more parts (B60J10/21 takes precedence)	B60J10/23	B60J10/23		194
B60J10/233	10	{Modular sealing arrangements, i.e. arrangements built up from a large number of joined modules}	B60J10/23	B60J10/23		66
B60J10/2335	11	{with joint end members, e.g. abutting ends}	B60J10/23	B60J10/23		114
B60J10/235	10	the parts being joined along their longitudinal direction	B60J10/235	B60J10/235		324
B60J10/24	9	having tubular parts	B60J10/24	B60J10/24		1581
B60J10/242	10	with vent holes	B60J10/242	B60J10/242		122
B60J10/244	10	inflatable or deflatable	B60J10/244	B60J10/244		334
B60J10/246	10	having projections, e.g. ribs, within the tubular parts	B60J10/246	B60J10/246		289
B60J10/248	10	having two or more tubular cavities, e.g. formed by partition walls	B60J10/248	B60J10/248		626
B60J10/25	9	characterised by water drainage means	B60J10/25	B60J10/25		614
B60J10/26	9	characterised by the surface shape	B60J10/26	B60J10/26		82
B60J10/265	10	the surface being primarily decorative	B60J10/265	B60J10/265		969
B60J10/27	9	having projections, grooves or channels in the longitudinal direction (for separately inserted fastening means, e.g. beads or strips, B60J10/36)	B60J10/27	B60J10/27		538
B60J10/273	10	for enclosing or housing devices for purposes other than sealing, e.g. cables	B60J10/273	B60J10/273		94
B60J10/277	10	for facilitating specific deformation of sealing parts, e.g. for ensuring proper folding	B60J10/277	B60J10/277		235
B60J10/30	8	characterised by the fastening means	B60J10/30	B60J10/30		1902
B60J10/32	9	using integral U-shaped retainers	B60J10/32	B60J10/32		799
B60J10/33	10	characterised by the configuration of the retaining lips	B60J10/33	B60J10/33		569
B60J10/34	9	using adhesives	B60J10/34	B60J10/34		427
B60J10/345	10	{with formless adhesives, e.g. hot melt}	B60J10/34	B60J10/34		67
B60J10/35	10	using adhesive tapes, e.g. double-sided tapes	B60J10/35	B60J10/35		259
B60J10/36	9	using separately inserted fastening means, e.g. using clips, beads or strips	B60J10/36	B60J10/36		654
B60J10/365	10	{comprising beads}	B60J10/36	B60J10/36		190
B60J10/38	9	using magnetic means	B60J10/38	B60J10/38		87
B60J10/40	8	characterised by contact between two or more cooperating sealing arrangements	B60J10/40	B60J10/40		356
B60J10/45	8	{Assembling sealing arrangements with vehicle parts}	B60J10/00	B60J10/45		967
B60J10/50	8	characterised by means for prevention or reduction of noise, e.g. of rattling or vibration of windows	B60J10/50	B60J10/50		936
B60J10/60	8	characterised by defrosting arrangements	B60J10/60	B60J10/60		73
B60J10/70	8	specially adapted for windows or windscreens	B60J10/70	B60J10/70		3315
B60J10/72	9	with integral wind-deflecting means, e.g. for preventing soiling	B60J10/72	B60J10/72		105
B60J10/74	9	for sliding window panes, e.g. sash guides	B60J10/74	B60J10/74		1573
B60J10/75	10	for sealing the lower part of the panes	B60J10/75	B60J10/75		1172
B60J10/76	10	for window sashes; for glass run channels	B60J10/76	B60J10/76		1192
B60J10/763	11	for preventing outward displacement of windows when at high speed	B60J10/763	B60J10/763		25
B60J10/767	11	for reducing air resistance due to the panes not being flush with the sash guide or glass run channel	B60J10/767	B60J10/767		20
B60J10/77	10	for sashless windows, i.e. for frameless windows forming a seal directly with the vehicle body	B60J10/77	B60J10/77		177
B60J10/773	11	for preventing outward displacement of windows when at high speed	B60J10/773	B60J10/773		10
B60J10/777	11	the sealing arrangement being between the edges of adjacent panes	B60J10/777	B60J10/777		48
B60J10/7775	12	{mounted on the pillar}	B60J10/777	B60J10/777		48
B60J10/78	10	adjacent to corner pieces, mirror supports or quarter windows	B60J10/78	B60J10/78		247
B60J10/79	10	for flush-glass windows, i.e. for windows flush with the vehicle body or the window frame	B60J10/79	B60J10/79		684
B60J10/80	8	specially adapted for opening panels, e.g. doors (for non-fixed roofs B60J10/90)	B60J10/80	B60J10/80		2122
B60J10/82	9	for movable panels in roofs	B60J10/82	B60J10/82		759
B60J10/84	9	arranged on the vehicle body	B60J10/84	B60J10/84		1059
B60J10/85	10	{with additional seals on the body side}	B60J10/84	B60J10/85		149
B60J10/86	9	arranged on the opening panel	B60J10/86	B60J10/86		1341
B60J10/87	10	{with additional seals on the panel side}	B60J10/86	B60J10/87		201
B60J10/88	10	mounted on, or integral with, the glass-run seals	B60J10/88	B60J10/88		349
B60J10/90	8	specially adapted for non-fixed roofs, e.g. foldable roofs or removable hard-tops	B60J10/90	B60J10/90		477
B60J11/00	7	Removable external protective coverings specially adapted for vehicles or parts of vehicles, e.g. parking covers (covering of load on vehicles B60P7/00; guard strips for body finishing, identifying or decorating B60R13/04; tents for use as garages E04H15/00)<br><br><u>NOTE</u><br><br>In groups B60J11/02 - B60J11/10, the first place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the first appropriate place. This Note corresponds to IPC Note (1) relating to B60J11/02 - B60J11/06.	B60J11/00	B60J11/00		1660
B60J11/02	8	Covers wound on rollers	B60J11/02	B60J11/02		853
B60J11/025	9	{specially adapted for covering vehicle parts, e.g. for doors, windows or windscreens}	B60J11/02	B60J11/02		376
B60J11/04	8	for covering at least the roof of the vehicle, e.g. for covering the whole vehicle	B60J11/04	B60J11/04		1538
B60J11/06	8	for covering only specific parts of the vehicle, e.g. for doors (covers or guards for traction couplings, hitches, draw-gear or towing devices B60D1/60; guards for wheels, radiators or bumpers B60R19/00)	B60J11/06	B60J11/06		821
B60J11/08	9	for windows or windscreens (antiglare equipment B60J3/00)	B60J11/08	B60J11/08		1197
B60J11/10	9	for wheels (hub caps or the like B60B7/00; external spare wheel stowing, holding or mounting arrangements B62D43/02)	B60J11/10	B60J11/10		132
