B02C1/00	7	Crushing or disintegrating by reciprocating members	B02C1/00	B02C1/00		2671
B02C1/005	8	{hydraulically or pneumatically operated}	B02C1/00	B02C1/00		1246
B02C1/02	8	Jaw crushers or pulverisers	B02C1/02	B02C1/02		911
B02C1/025	9	{Jaw clearance or overload control}	B02C1/02	B02C1/02		304
B02C1/04	9	with single-acting jaws	B02C1/04	B02C1/04		1789
B02C1/043	10	{with cooperating single acting jaws}	B02C1/04	B02C1/04		303
B02C1/046	10	{of the plural stage type}	B02C1/04	B02C1/04		64
B02C1/06	9	with double-acting jaws	B02C1/06	B02C1/06		319
B02C1/08	9	with jaws coacting with rotating roller	B02C1/08	B02C1/08		169
B02C1/10	9	Shape or construction of jaws	B02C1/10	B02C1/10		777
B02C1/12	8	Mills with non-rotating spiked members	B02C1/12	B02C1/12		322
B02C1/14	8	Stamping mills	B02C1/14	B02C1/14		3683
B02C2/00	7	Crushing or disintegrating by gyratory or cone crushers {(with non-coaxial discs with intersecting axes B02C7/005)}	B02C2/00	B02C2/00		647
B02C2002/002	8	{the bowl being a driven element for providing a crushing effect}	B02C2/00	B02C2/00		50
B02C2/005	8	{Lining}	B02C2/00	B02C2/00		531
B02C2/007	8	{Feeding devices}	B02C2/00	B02C2/00		331
B02C2/02	8	eccentrically moved	B02C2/02	B02C2/02		110
B02C2/04	9	with vertical axis	B02C2/04	B02C2/04		923
B02C2/042	10	{Moved by an eccentric weight}	B02C2/04	B02C2/04		141
B02C2/045	10	{and with bowl adjusting or controlling mechanisms (B02C2/042, B02C2/06 take precedence)}	B02C2/04	B02C2/04		444
B02C2/047	10	{and with head adjusting or controlling mechanisms (B02C2/042, B02C2/06 take precedence)}	B02C2/04	B02C2/04		272
B02C2/06	10	and with top bearing {(B02C2/042 takes precedence)}	B02C2/06	B02C2/06		630
B02C2/08	9	with horizontal axis	B02C2/08	B02C2/08		42
B02C2/10	8	concentrically moved; Bell crushers	B02C2/10	B02C2/10		2951
B02C4/00	7	Crushing or disintegrating by roller mills (with milling members in the form of rollers or balls co-operating with rings or discs B02C15/00; roller mills or roll refiners exclusively for chocolate A23G1/10, A23G1/12)	B02C4/00	B02C4/00		822
B02C4/02	8	with two or more rollers	B02C4/02	B02C4/02		6712
B02C4/04	9	specially adapted for milling paste-like material, e.g. paint, chocolate, colloids	B02C4/04	B02C4/04		278
B02C4/06	9	specially adapted for milling grain	B02C4/06	B02C4/06		915
B02C4/08	9	with co-operating corrugated or toothed crushing-rollers	B02C4/08	B02C4/08		12298
B02C4/10	8	with a roller co-operating with a stationary member	B02C4/10	B02C4/10		2470
B02C4/12	9	in the form of a plate	B02C4/12	B02C4/12		1132
B02C4/14	10	specially adapted for milling paste-like material, e.g. paint, chocolate, colloids	B02C4/14	B02C4/14		23
B02C4/16	10	specially adapted for milling grain	B02C4/16	B02C4/16		166
B02C4/18	9	in the form of a bar	B02C4/18	B02C4/18		61
B02C4/20	10	wherein the roller is corrugated or toothed	B02C4/20	B02C4/20		175
B02C4/22	10	specially adapted for milling paste-like material, e.g. paint, chocolate, colloids	B02C4/22	B02C4/22		231
B02C4/24	10	specially adapted for milling grain	B02C4/24	B02C4/24		22
B02C4/26	9	in the form of a grid or grating	B02C4/26	B02C4/26		762
B02C4/28	8	Details	B02C4/28	B02C4/28		6434
B02C4/283	9	{Lateral sealing shields}	B02C4/28	B02C4/28		254
B02C4/286	9	{Feeding devices}	B02C4/28	B02C4/28		4374
B02C4/30	9	Shape or construction of rollers	B02C4/30	B02C4/30		5003
B02C4/305	10	{Wear resistant rollers}	B02C4/30	B02C4/30		489
B02C4/32	9	Adjusting, applying pressure to, or controlling the distance between, milling members	B02C4/32	B02C4/32		2352
B02C4/34	10	in mills wherein a roller co-operates with a stationary member	B02C4/34	B02C4/34		432
B02C4/36	10	in mills specially adapted for paste-like materials	B02C4/36	B02C4/36		184
B02C4/38	10	in grain mills	B02C4/38	B02C4/38		270
B02C4/40	9	Detachers, e.g. scrapers	B02C4/40	B02C4/40		1726
B02C4/42	9	Driving mechanisms; Roller speed control	B02C4/42	B02C4/42		7135
B02C4/423	10	{with vibrating or oscillating mechanisms}	B02C4/42	B02C4/42		170
B02C4/426	10	{Torque counterbalancing mechanisms}	B02C4/42	B02C4/42		33
B02C4/44	9	Cooling or heating rollers or bars	B02C4/44	B02C4/44		542
B02C7/00	7	Crushing or disintegrating by disc mills (apparatus specially adapted for manufacture or treatment of cocoa or cocoa products exclusively A23G1/04)	B02C7/00	B02C7/00		289
B02C7/005	8	{Crushers with non-coaxial toothed discs with intersecting axes}	B02C7/00	B02C7/00		62
B02C7/02	8	with coaxial discs	B02C7/02	B02C7/02		267
B02C7/04	9	with concentric circles of intermeshing teeth	B02C7/04	B02C7/04		415
B02C7/06	9	with horizontal axis (B02C7/04 takes precedence)	B02C7/06	B02C7/06		1142
B02C7/08	9	with vertical axis (B02C7/04 takes precedence)	B02C7/08	B02C7/08		2605
B02C7/10	8	with eccentric discs	B02C7/10	B02C7/10		150
B02C7/11	8	Details	B02C7/11	B02C7/11		1365
B02C7/12	9	Shape or construction of discs	B02C7/12	B02C7/12		1893
B02C7/13	10	for grain mills	B02C7/13	B02C7/13		241
B02C7/14	9	Adjusting, applying pressure to, or controlling distance between, discs	B02C7/14	B02C7/14		969
B02C7/16	9	Driving mechanisms	B02C7/16	B02C7/16		1138
B02C7/17	9	Cooling or heating of discs	B02C7/17	B02C7/17		228
B02C7/175	8	Disc mills specially adapted for paste-like material, e.g. paint, chocolate, colloids	B02C7/175	B02C7/175		101
B02C7/18	8	Disc mills specially adapted for grain	B02C7/18	B02C7/18		113
B02C7/182	9	{with horizontal axis}	B02C7/18	B02C7/18		140
B02C7/184	9	{with vertical axis}	B02C7/18	B02C7/18		413
B02C7/186	9	{Adjusting, applying pressure to, or controlling distance between, discs}	B02C7/18	B02C7/18		134
B02C7/188	9	{Driving mechanisms}	B02C7/18	B02C7/18		185
B02C9/00	7	Other milling methods or mills specially adapted for grain	B02C9/00	B02C9/00		748
B02C9/02	8	Cutting or splitting grain	B02C9/02	B02C9/02		484
B02C9/04	8	Systems or sequences of operations; Plant	B02C9/04	B02C9/04		865
B02C11/00	7	Other auxiliary devices or accessories specially adapted for grain mills	B02C11/00	B02C11/00		702
B02C11/02	8	Breaking up amassed particles, e.g. flakes	B02C11/02	B02C11/02		72
B02C11/04	8	Feeding devices	B02C11/04	B02C11/04		522
B02C11/06	8	Arrangements for preventing fire or explosion (methods for preventing or extinguishing fires, devices therefor A62C)	B02C11/06	B02C11/06		15
B02C11/08	8	Cooling, heating, ventilating, conditioning with respect to temperature or water content (conditioning grain before milling B02B1/08; air-conditioning or ventilating in general F24F)	B02C11/08	B02C11/08		514
B02C13/00	7	Disintegrating by mills having rotary beater elements {; Hammer mills}	B02C13/00	B02C13/00		832
B02C13/02	8	with horizontal rotor shaft (with axial flow B02C13/10)	B02C13/02	B02C13/02		1437
B02C13/04	9	with beaters hinged to the rotor; Hammer mills	B02C13/04	B02C13/04		958
B02C13/06	9	with beaters rigidly connected to the rotor	B02C13/06	B02C13/06		1598
B02C13/08	10	and acting as a fan	B02C13/08	B02C13/08		235
B02C13/09	10	and throwing the material against an anvil or impact plate {(with vertical axis B02C13/1807)}	B02C13/09	B02C13/09		787
B02C13/095	11	{with an adjustable anvil or impact plate}	B02C13/09	B02C13/09		371
B02C13/10	8	with horizontal rotor shaft and axial flow	B02C13/10	B02C13/10		213
B02C13/12	9	with vortex chamber	B02C13/12	B02C13/12		61
B02C13/13	8	with horizontal rotor shaft and combined with sifting devices, e.g. for making powdered fuel	B02C13/13	B02C13/13		1673
B02C13/14	8	with vertical rotor shaft, e.g. combined with sifting devices	B02C13/14	B02C13/14		1786
B02C2013/145	9	{with fast rotating vanes generating vortexes effecting material on material impact}	B02C13/14	B02C13/14		112
B02C13/16	9	with beaters hinged to the rotor	B02C13/16	B02C13/16		293
B02C13/18	9	with beaters rigidly connected to the rotor	B02C13/18	B02C13/18		1917
B02C13/1807	10	{the material to be crushed being thrown against an anvil or impact plate (with horizontal axis B02C13/09; centrifugal acceleration of material through radially extending channels B02C19/0025; centrifugal acceleration of material by means of an open top rotor B02C19/0031)}	B02C13/18	B02C13/18		239
B02C13/1814	11	{by means of beater or impeller elements fixed on top of a disc type rotor}	B02C13/18	B02C13/18		253
B02C13/1821	12	{the beater or impeller elements being rotatably fixed around their own axis}	B02C13/18	B02C13/18		20
B02C13/1828	12	{with dead bed protected beater or impeller elements}	B02C13/18	B02C13/18		16
B02C13/1835	11	{by means of beater or impeller elements fixed in between an upper and lower rotor disc}	B02C13/18	B02C13/18		231
B02C13/1842	12	{with dead bed protected beater or impeller elements}	B02C13/18	B02C13/18		123
B02C13/185	11	{Construction or shape of anvil or impact plate}	B02C13/18	B02C13/18		119
B02C2013/1857	11	{rotating coaxially around the rotor shaft}	B02C13/18	B02C13/18		56
B02C2013/1864	11	{rotatable around its own axis}	B02C13/18	B02C13/18		32
B02C2013/1871	11	{vertically adjustable}	B02C13/18	B02C13/18		34
B02C2013/1878	11	{radially adjustable}	B02C13/18	B02C13/18		33
B02C2013/1885	11	{of dead bed type}	B02C13/18	B02C13/18		82
B02C2013/1892	11	{cooled or heated}	B02C13/18	B02C13/18		9
B02C13/20	8	with two or more co-operating rotors	B02C13/20	B02C13/20		1138
B02C13/205	9	{arranged concentrically}	B02C13/20	B02C13/20		235
B02C13/22	8	with intermeshing pins {; Pin Disk Mills}	B02C13/22	B02C13/22		523
B02C13/24	9	arranged around a vertical axis	B02C13/24	B02C13/24		86
B02C13/26	8	Details	B02C13/26	B02C13/26		2612
B02C13/28	9	Shape or construction of beater elements	B02C13/28	B02C13/28		3267
B02C13/2804	10	{the beater elements being rigidly connected to the rotor}	B02C13/28	B02C13/28		1831
B02C2013/2808	10	{the beater elements are attached to disks mounted on a shaft}	B02C13/28	B02C13/28		382
B02C2013/2812	10	{the beater elements are attached to a hollow cylindrical rotor}	B02C13/28	B02C13/28		81
B02C2013/2816	10	{of chain, rope or cable type}	B02C13/28	B02C13/28		214
B02C13/282	9	Shape or inner surface of mill-housings	B02C13/282	B02C13/282		1663
B02C2013/2825	10	{with fastening means for fixing lining members to the inner surface of mill-housings}	B02C13/282	B02C13/282		131
B02C13/284	10	Built-in screens	B02C13/284	B02C13/284		1874
B02C13/286	9	Feeding or discharge	B02C13/286	B02C13/286		2931
B02C2013/28609	10	{Discharge means}	B02C13/286	B02C13/286		1146
B02C2013/28618	10	{Feeding means}	B02C13/286	B02C13/286		671
B02C2013/28627	11	{of ram or pusher type}	B02C13/286	B02C13/286		37
B02C2013/28636	11	{of conveyor belt type}	B02C13/286	B02C13/286		194
B02C2013/28645	11	{of conveyor belt and cooperating roller type}	B02C13/286	B02C13/286		25
B02C2013/28654	11	{of screw type}	B02C13/286	B02C13/286		163
B02C2013/28663	11	{using rollers}	B02C13/286	B02C13/286		73
B02C2013/28672	11	{Feed chute arrangements}	B02C13/286	B02C13/286		318
B02C2013/28681	11	{Feed distributor plate for vertical mill}	B02C13/286	B02C13/286		76
B02C2013/2869	10	{Arrangements of feed and discharge means in relation to each other}	B02C13/286	B02C13/286		126
B02C13/288	9	Ventilating, or influencing air circulation	B02C13/288	B02C13/288		964
B02C2013/29	9	{devices for manipulating beater elements}	B02C13/26	B02C13/29		107
B02C13/30	9	Driving mechanisms	B02C13/30	B02C13/30		2705
B02C13/31	9	Safety devices or measures	B02C13/31	B02C13/31		532
B02C15/00	7	Disintegrating by milling members in the form of rollers or balls co-operating with rings or discs {(high-speed drum mills B02C19/11)}	B02C15/00	B02C15/00		1492
B02C15/001	8	{Air flow directing means positioned on the periphery of the horizontally rotating milling surface}	B02C15/00	B02C15/00		233
B02C2015/002	8	{combined with a classifier}	B02C15/00	B02C15/00		832
B02C15/003	8	{Shape or construction of discs or rings}	B02C15/00	B02C15/00		391
B02C15/004	8	{Shape or construction of rollers or balls}	B02C15/00	B02C15/00		459
B02C15/005	9	{Rollers or balls of composite construction}	B02C15/00	B02C15/00		169
B02C15/006	8	{Ring or disc drive gear arrangement}	B02C15/00	B02C15/00		173
B02C15/007	8	{Mills with rollers pressed against a rotary horizontal disc (with pendularly mounted rollers B02C15/04)}	B02C15/00	B02C15/00		441
B02C2015/008	8	{Roller drive arrangements}	B02C15/00	B02C15/00		358
B02C15/02	8	Centrifugal pendulum-type mills	B02C15/02	B02C15/02		405
B02C15/04	8	Mills with pressed pendularly-mounted rollers, e.g. spring pressed	B02C15/04	B02C15/04		484
B02C15/045	9	{pressed against the interior of a ring rotating in a vertical plane}	B02C15/04	B02C15/04		100
B02C15/06	8	Mills with rollers forced against the interior of a rotary ring, e.g. under spring action (B02C15/04 takes precedence)	B02C15/06	B02C15/06		241
B02C15/08	8	Mills with balls or rollers centrifugally forced against the inner surface of a ring, the balls or rollers of which are driven by a centrally arranged member (B02C15/02 takes precedence)	B02C15/08	B02C15/08		669
B02C15/10	8	Mills with balls or rollers centrifugally forced against the inner surface of a ring, the balls or rollers of which are driven by other means than a centrally-arranged member	B02C15/10	B02C15/10		69
B02C15/12	8	Mills with at least two discs {or rings} and interposed balls or rollers mounted like ball or roller bearings	B02C15/12	B02C15/12		442
B02C15/123	9	{with rings and interposed rollers}	B02C15/12	B02C15/12		88
B02C2015/126	9	{of the plural stage type}	B02C15/12	B02C15/12		172
B02C15/14	8	Edge runners, e.g. Chile mills	B02C15/14	B02C15/14		973
B02C2015/143	9	{each runner pivot carrying more than one runner}	B02C15/14	B02C15/14		57
B02C2015/146	9	{Step-shaped runners}	B02C15/14	B02C15/14		5
B02C15/16	8	with milling members essentially having different peripheral speeds and in the form of a hollow cylinder or cone and an internal roller or cone	B02C15/16	B02C15/16		288
B02C17/00	7	Disintegrating by tumbling mills, i.e. mills having a container charged with the material to be disintegrated with or without special disintegrating members such as pebbles or balls (high-speed drum mills B02C19/11{; drums for polishing or grinding B24B})	B02C17/00	B02C17/00		594
B02C17/002	8	{with rotary cutting or beating elements}	B02C17/00	B02C17/00		394
B02C17/005	8	{the charge being turned over by magnetic forces}	B02C17/00	B02C17/00		109
B02C17/007	8	{specially adapted for disintegrating refuse}	B02C17/00	B02C17/00		190
B02C17/02	8	with perforated container	B02C17/02	B02C17/02		476
B02C17/04	8	with unperforated container	B02C17/04	B02C17/04		567
B02C17/06	9	with several compartments	B02C17/06	B02C17/06		664
B02C2017/065	10	{with several compartments in the form of multiwell blocks}	B02C17/06	B02C17/06		27
B02C17/07	10	in radial arrangement	B02C17/07	B02C17/07		100
B02C17/08	9	with containers performing a planetary movement	B02C17/08	B02C17/08		405
B02C17/10	8	with one or a few disintegrating members arranged in the container	B02C17/10	B02C17/10		3559
B02C17/14	8	Mills in which the charge to be ground is turned over by movements of the container other than by rotating, e.g. by swinging, vibrating, tilting {(mills provided with vibrators in general B02C19/16)}	B02C17/14	B02C17/14		938
B02C17/16	8	Mills in which a fixed container houses stirring means tumbling the charge	B02C17/16	B02C17/16		1509
B02C17/161	9	{Arrangements for separating milling media and ground material}	B02C17/16	B02C17/16		394
B02C17/163	9	{Stirring means}	B02C17/16	B02C17/16		1030
B02C2017/165	9	{with stirring means comprising more than one agitator}	B02C17/16	B02C17/16		123
B02C17/166	9	{of the annular gap type}	B02C17/16	B02C17/16		126
B02C17/168	9	{with a basket media milling device arranged in or on the container, involving therein a circulatory flow of the material to be milled}	B02C17/16	B02C17/16		79
B02C17/18	8	Details	B02C17/18	B02C17/18		3015
B02C17/1805	9	{Monitoring devices for tumbling mills}	B02C17/18	B02C17/18		606
B02C17/181	9	{Bearings specially adapted for tumbling mills}	B02C17/18	B02C17/18		169
B02C17/1815	9	{Cooling or heating devices}	B02C17/18	B02C17/18		698
B02C17/182	9	{Lids}	B02C17/18	B02C17/18		114
B02C17/1825	9	{Lifting devices (lifting devices associated with the lining for containers B02C17/22)}	B02C17/18	B02C17/18		113
B02C17/183	9	{Feeding or discharging devices}	B02C17/18	B02C17/18		1366
B02C17/1835	10	{Discharging devices combined with sorting or separating of material (B02C17/186 takes precedence)}	B02C17/18	B02C17/18		190
B02C17/184	11	{with separator arranged in discharge path of crushing zone}	B02C17/18	B02C17/18		279
B02C17/1845	12	{with return of oversize material to crushing zone}	B02C17/18	B02C17/18		166
B02C17/185	11	{with more than one separator}	B02C17/18	B02C17/18		183
B02C17/1855	11	{with separator defining termination of crushing zone, e.g. screen denying egress of oversize material}	B02C17/18	B02C17/18		559
B02C17/186	10	{Adding fluid, other than for crushing by fluid energy}	B02C17/18	B02C17/18		219
B02C17/1865	11	{after crushing}	B02C17/18	B02C17/18		73
B02C17/187	12	{with recirculation of material to crushing zone}	B02C17/18	B02C17/18		27
B02C17/1875	11	{passing gas through crushing zone}	B02C17/18	B02C17/18		94
B02C17/188	12	{characterised by point of gas entry or exit or by gas flow path}	B02C17/18	B02C17/18		33
B02C17/1885	12	{the applied gas acting to effect material separation (B02C17/1895 takes precedence)}	B02C17/18	B02C17/18		69
B02C17/189	12	{with return of oversize material to crushing zone (B02C17/1895 takes precedence)}	B02C17/18	B02C17/18		34
B02C17/1895	12	{gas being recirculated to crushing zone}	B02C17/18	B02C17/18		11
B02C17/20	9	Disintegrating members	B02C17/20	B02C17/20		1402
B02C17/205	10	{Adding disintegrating members to the tumbling mill}	B02C17/20	B02C17/20		259
B02C17/22	9	Lining for containers	B02C17/22	B02C17/22		1487
B02C17/225	10	{using rubber or elastomeric material}	B02C17/22	B02C17/22		261
B02C17/24	9	Driving mechanisms	B02C17/24	B02C17/24		1874
B02C18/00	7	Disintegrating by knives or other cutting or tearing members which chop material into fragments {(tree stump comminutors A01G23/067)}	B02C18/00	B02C18/00		835
B02C18/0007	8	{specially adapted for disintegrating documents}	B02C18/00	B02C18/00		2187
B02C2018/0015	9	{for disintegrating CDs, DVDs and/or credit cards}	B02C18/00	B02C18/00		109
B02C2018/0023	9	{Switching devices}	B02C18/00	B02C18/00		223
B02C2018/003	9	{Removing clips, pins or staples before disintegrating}	B02C18/00	B02C18/00		29
B02C2018/0038	9	{Motor drives}	B02C18/00	B02C18/00		327
B02C2018/0046	9	{Shape or construction of frames, housings or casings}	B02C18/00	B02C18/00		355
B02C2018/0053	9	{hand-operated}	B02C18/00	B02C18/00		34
B02C2018/0061	9	{with compacting devices for the disintegrated material}	B02C18/00	B02C18/00		185
B02C2018/0069	9	{with stripping devices}	B02C18/00	B02C18/00		242
B02C18/0076	8	{with cutting or tearing members fixed on endless flexible members (without cutting or tearing members B02C19/0006)}	B02C18/00	B02C18/00		61
B02C18/0084	8	{specially adapted for disintegrating garbage, waste or sewage}	B02C18/00	B02C18/00		3740
B02C18/0092	9	{for waste water or for garbage}	B02C18/00	B02C18/00		4194
B02C18/02	8	with reciprocating knives	B02C18/02	B02C18/02		1744
B02C18/04	9	Details	B02C18/04	B02C18/04		1169
B02C18/06	8	with rotating knives	B02C18/06	B02C18/06		2368
B02C18/062	9	{with rotor elements extending axially in close radial proximity of a concentrically arranged slotted or perforated ring}	B02C18/06	B02C18/06		231
B02C18/065	9	{within rotatable bowls, e.g. meat cutters}	B02C18/06	B02C18/06		426
B02C18/067	9	{Tub-grinders}	B02C18/06	B02C18/06		321
B02C18/08	9	within vertical containers {(B02C18/062, B02C18/065 take precedence)}	B02C18/08	B02C18/08		1033
B02C18/083	10	{with a disc rotor having generally radially extending slots or openings bordered with cutting knives}	B02C18/08	B02C18/08		134
B02C18/086	10	{specially adapted for disintegrating plastics, e.g. cinematographic films (for plastic bottles B02C19/0093, disintegrating plastics B29B17/00)}	B02C18/08	B02C18/08		147
B02C18/10	10	with drive arranged above container {(B02C18/083 takes precedence)}	B02C18/10	B02C18/10		5511
B02C18/12	10	with drive arranged below container {(B02C18/083 takes precedence)}	B02C18/12	B02C18/12		3854
B02C18/14	9	within horizontal containers {(B02C18/062, B02C18/065 take precedence)}	B02C18/14	B02C18/14		7665
B02C18/141	10	{with axial flow}	B02C18/14	B02C18/14		230
B02C18/142	10	{with two or more inter-engaging rotatable cutter assemblies}	B02C18/14	B02C18/14		3881
B02C18/143	10	{with a disc rotor having generally radially extending slots or openings bordered with cutting knives}	B02C18/14	B02C18/14		303
B02C18/144	10	{with axially elongated knives}	B02C18/14	B02C18/14		413
B02C18/145	10	{with knives spaced axially and circumferentially on the periphery of a cylindrical rotor unit}	B02C18/14	B02C18/14		1475
B02C18/146	10	{with a rotor comprising a plurality of axially contiguous disc-like segments each having at least one radially extending cutting element}	B02C18/14	B02C18/14		230
B02C2018/147	10	{of the plural stage type}	B02C18/14	B02C18/14		673
B02C18/148	10	{specially adapted for disintegrating plastics, e.g. cinematographic films (for plastic bottles B02C19/0093, disintegrating plastics B29B17/00)}	B02C18/14	B02C18/14		871
B02C18/16	9	Details	B02C18/16	B02C18/16		6383
B02C2018/162	10	{Shape or inner surface of shredder-housings}	B02C18/16	B02C18/16		708
B02C2018/164	10	{Prevention of jamming and/or overload}	B02C18/16	B02C18/16		638
B02C2018/166	10	{Lubricating the knives of the cutting mechanisms}	B02C18/16	B02C18/16		56
B02C2018/168	10	{User safety devices or measures in shredders}	B02C18/16	B02C18/16		470
B02C18/18	10	Knives; Mountings thereof	B02C18/18	B02C18/18		8595
B02C18/182	11	{Disc-shaped knives}	B02C18/18	B02C18/18		1153
B02C18/184	12	{with peripherally arranged demountable cutting tips or elements}	B02C18/18	B02C18/18		311
B02C18/186	11	{Axially elongated knives}	B02C18/18	B02C18/18		462
B02C2018/188	11	{Stationary counter-knives;  Mountings thereof}	B02C18/18	B02C18/18		644
B02C18/20	11	Sickle-shaped knives	B02C18/20	B02C18/20		429
B02C18/22	10	Feed or discharge means	B02C18/22	B02C18/22		820
B02C2018/2208	11	{for weblike material}	B02C18/22	B02C18/22		110
B02C18/2216	11	{Discharge means}	B02C18/22	B02C18/22		3677
B02C18/2225	11	{Feed means}	B02C18/22	B02C18/22		2040
B02C18/2233	12	{of ram or pusher type}	B02C18/22	B02C18/22		296
B02C18/2241	12	{of conveyor belt type (B02C18/225 takes precedence)}	B02C18/22	B02C18/22		484
B02C18/225	12	{of conveyor belt and cooperating roller type}	B02C18/22	B02C18/22		155
B02C18/2258	12	{of screw type}	B02C18/22	B02C18/22		538
B02C18/2266	12	{of revolving drum type}	B02C18/22	B02C18/22		44
B02C18/2275	12	{using a rotating arm}	B02C18/22	B02C18/22		72
B02C18/2283	12	{using rollers (B02C18/225 takes precedence)}	B02C18/22	B02C18/22		485
B02C18/2291	12	{Feed chute arrangements}	B02C18/22	B02C18/22		920
B02C18/24	10	Drives	B02C18/24	B02C18/24		7471
B02C18/26	8	with knives which both reciprocate and rotate	B02C18/26	B02C18/26		490
B02C18/28	8	with spiked cylinders	B02C18/28	B02C18/28		314
B02C18/30	8	Mincing machines with perforated discs and feeding worms	B02C18/30	B02C18/30		390
B02C18/301	9	{with horizontal axis}	B02C18/30	B02C18/30		319
B02C18/302	10	{with a knife-perforated disc unit}	B02C18/30	B02C18/30		584
B02C18/304	10	{with several axially aligned knife-perforated disc units}	B02C18/30	B02C18/30		107
B02C18/305	9	{Details}	B02C18/30	B02C18/30		445
B02C2018/307	10	{Cooling arrangements in mincing machines}	B02C18/30	B02C18/30		48
B02C2018/308	9	{with separating devices for hard material, e.g. bone}	B02C18/30	B02C18/30		93
B02C18/32	9	with sharpening devices	B02C18/32	B02C18/32		12
B02C18/34	9	with means for cleaning the perforated discs	B02C18/34	B02C18/34		80
B02C18/36	9	Knives or perforated discs	B02C18/36	B02C18/36		249
B02C18/362	10	{Knives}	B02C18/36	B02C18/36		335
B02C18/365	10	{Perforated discs}	B02C18/36	B02C18/36		162
B02C2018/367	10	{Resiliently mounted knives or discs}	B02C18/36	B02C18/36		56
B02C18/38	9	Drives	B02C18/38	B02C18/38		198
B02C19/00	7	Other disintegrating devices or methods (for grain B02C9/00)	B02C19/00	B02C19/00		3424
B02C19/0006	8	{Crushing by endless flexible members (with cutting or tearing members B02C18/0076)}	B02C19/00	B02C19/00		73
B02C19/0012	8	{Devices for disintegrating materials by collision of these materials against a breaking surface or breaking body and/or by friction between the material particles (also for grain)}	B02C19/00	B02C19/00		455
B02C19/0018	9	{using a rotor accelerating the materials centrifugally against a circumferential breaking surface (rotors with beater elements B02C13/09, B02C13/1807)}	B02C19/00	B02C19/00		461
B02C19/0025	10	{by means of a rotor with radially extending channels}	B02C19/00	B02C19/00		68
B02C19/0031	10	{by means of an open top rotor}	B02C19/00	B02C19/00		46
B02C19/0037	11	{with concentrically arranged open top rotors}	B02C19/00	B02C19/00		14
B02C19/0043	9	{the materials to be pulverised being projected against a breaking surface or breaking body by a pressurised fluid (jet mills B02C19/06)}	B02C19/00	B02C19/00		126
B02C19/005	9	{the materials to be pulverised being disintegrated by collision of, or friction between, the material particles (jet mills B02C19/06)}	B02C19/00	B02C19/00		604
B02C19/0056	8	{specially adapted for specific materials not otherwise provided for}	B02C19/00	B02C19/00		2809
B02C19/0062	9	{specially adapted for shredding scrap metal, e.g. automobile bodies}	B02C19/00	B02C19/00		168
B02C19/0068	9	{specially adapted for breaking-up fluorescent tubes}	B02C19/00	B02C19/00		95
B02C19/0075	9	{specially adapted for disintegrating medical waste (sterilisation of refuse A61L11/00; disposal of medical waste B09B3/00)}	B02C19/00	B02C19/00		387
B02C19/0081	9	{specially adapted for breaking-up bottles}	B02C19/00	B02C19/00		205
B02C19/0087	10	{for glass bottles}	B02C19/00	B02C19/00		354
B02C19/0093	10	{for plastic bottles}	B02C19/00	B02C19/00		163
B02C19/06	8	Jet mills	B02C19/06	B02C19/06		1367
B02C19/061	9	{of the cylindrical type (B02C19/068 takes precedence)}	B02C19/06	B02C19/06		252
B02C19/063	9	{of the toroidal type (B02C19/068 takes precedence)}	B02C19/06	B02C19/06		105
B02C19/065	9	{of the opposed-jet type (B02C19/068 takes precedence)}	B02C19/06	B02C19/06		175
B02C19/066	9	{of the jet-anvil type (B02C19/068 takes precedence)}	B02C19/06	B02C19/06		242
B02C19/068	9	{of the fluidised-bed type}	B02C19/06	B02C19/06		144
B02C19/08	8	Pestle and mortar	B02C19/08	B02C19/08		595
B02C19/10	8	Mills in which a friction block is towed along the surface of a cylindrical or annular member	B02C19/10	B02C19/10		519
B02C19/11	8	High-speed drum mills (for separating B04B)	B02C19/11	B02C19/11		98
B02C19/16	8	Mills provided with vibrators ({roller mills B02C4/423}; tumbling mills B02C17/14)	B02C19/16	B02C19/16		1126
B02C19/18	8	Use of auxiliary physical effects, e.g. ultrasonic waves or irradiation, for disintegrating	B02C19/18	B02C19/18		1224
B02C2019/183	9	{Crushing by discharge of high electrical energy}	B02C19/18	B02C19/18		326
B02C19/186	9	{Use of cold or heat for disintegrating (B02C4/44, B02C7/17, B02C11/08 take precedence)}	B02C19/18	B02C19/18		1216
B02C19/20	8	Disintegrating by grating {(domestic food grating devices A47J43/25)}	B02C19/20	B02C19/20		898
B02C19/22	8	Crushing mills with screw-shaped crushing means	B02C19/22	B02C19/22		2229
B02C21/00	7	Disintegrating plant with or without drying of the material (for grain B02C9/04)	B02C21/00	B02C21/00		13592
B02C21/002	8	{using a combination of a roller mill and a drum mill}	B02C21/00	B02C21/00		58
B02C21/005	9	{the roller mill having cooperating rollers}	B02C21/00	B02C21/00		90
B02C21/007	8	{using a combination of two or more drum or tube mills}	B02C21/00	B02C21/00		105
B02C21/02	8	Transportable disintegrating plant	B02C21/02	B02C21/02		3125
B02C2021/023	9	{for disintegrating material on the surface of the ground}	B02C21/02	B02C21/02		313
B02C21/026	9	{self-propelled}	B02C21/02	B02C21/02		677
B02C23/00	7	Auxiliary methods or auxiliary devices or accessories specially adapted for crushing or disintegrating not provided for in preceding groups or not specially adapted to apparatus covered by a single preceding group ({specially adapted for grain mills B02C11/00;} separating or sorting in general B03, B04, B07)	B02C23/00	B02C23/00		10460
B02C23/02	8	Feeding devices ({for grain mills B02C11/04; for roller mills B02C4/286}; transport devices in general B65G)	B02C23/02	B02C23/02		8240
B02C23/04	8	Safety devices (in general F16P{; for rotary mills B02C13/31})	B02C23/04	B02C23/04		3003
B02C23/06	8	Selection or use of additives to aid disintegrating	B02C23/06	B02C23/06		621
B02C23/08	8	Separating or sorting of material, associated with crushing or disintegrating (B02C23/18 takes precedence {; beater mills combined with sifting devices B02C13/13, B02C13/14; for tumbling mills B02C17/1835})	B02C23/08	B02C23/08		7290
B02C23/10	9	with separator arranged in discharge path of crushing or disintegrating zone	B02C23/10	B02C23/10		6766
B02C23/12	10	with return of oversize material to crushing or disintegrating zone	B02C23/12	B02C23/12		3160
B02C23/14	9	with more than one separator	B02C23/14	B02C23/14		7173
B02C23/16	9	with separator defining termination of crushing or disintegrating zone, e.g. screen denying egress of oversize material	B02C23/16	B02C23/16		10758
B02C2023/165	10	{Screen denying egress of oversize material}	B02C23/16	B02C23/16		8278
B02C23/18	8	Adding fluid, other than for crushing or disintegrating by fluid energy ({for tumbling mills B02C17/186;} feeding devices B02C23/02)	B02C23/18	B02C23/18		3941
B02C23/20	9	after crushing or disintegrating	B02C23/20	B02C23/20		2085
B02C23/22	10	with recirculation of material to crushing or disintegrating zone	B02C23/22	B02C23/22		409
B02C23/24	9	Passing gas through crushing or disintegrating zone ({B02C15/001}, B02C23/38, B02C23/40 take precedence)	B02C23/24	B02C23/24		1752
B02C23/26	10	characterised by point of gas entry or exit or by gas flow path	B02C23/26	B02C23/26		235
B02C23/28	10	gas moving means being integral with, or attached to, crushing or disintegrating element	B02C23/28	B02C23/28		284
B02C23/30	10	the applied gas acting to effect material separation (B02C23/34 takes precedence)	B02C23/30	B02C23/30		887
B02C23/32	10	with return of oversize material to crushing or disintegrating zone (B02C23/34 takes precedence)	B02C23/32	B02C23/32		514
B02C23/34	10	gas being recirculated to crushing or disintegrating zone	B02C23/34	B02C23/34		144
B02C23/36	9	the crushing or disintegrating zone being submerged in liquid	B02C23/36	B02C23/36		327
B02C23/38	9	in apparatus having multiple crushing or disintegrating zones	B02C23/38	B02C23/38		146
B02C23/40	9	with more than one means for adding fluid to the material being crushed or disintegrated	B02C23/40	B02C23/40		573
B02C25/00	7	Control arrangements specially adapted for crushing or disintegrating	B02C25/00	B02C25/00		6004
B02C2201/00	7	Codes relating to disintegrating devices adapted for specific materials	CPCONLY	B02C2201/00		61
B02C2201/02	8	for reinforced concrete	CPCONLY	B02C2201/02		787
B02C2201/04	8	for used tyres	CPCONLY	B02C2201/04		289
B02C2201/06	8	for garbage, waste or sewage	CPCONLY	B02C2201/06		11847
B02C2201/063	9	for waste water or sewage	CPCONLY	B02C2201/063		759
B02C2201/066	9	for garden waste	CPCONLY	B02C2201/066		874
B02C2210/00	7	Codes relating to different types of disintegrating devices	CPCONLY	B02C2210/00		10
B02C2210/01	8	Indication of wear on beaters, knives, rollers, anvils, linings and the like	CPCONLY	B02C2210/01		149
B02C2210/02	8	Features for generally used wear parts on beaters, knives, rollers, anvils, linings and the like	CPCONLY	B02C2210/02		443
