F17C1/00	7	Pressure vessels, e.g. gas cylinder, gas tank, replaceable cartridge (pressurised apparatus for purposes other than storage, see the relevant subclasses such as A62C, B05B; associated with vehicles, see the appropriate subclass of classes B60&#160;-&#160;B64; pressure vessels in general F16J12/00{; autoclaves B01J3/04; tank vehicles B60P3/22; railway tank wagons for carrying fluent materials B61D5/00; accumulators for supplying fluid under pressure F15B1/04; liquefied gas stoves F24C3/00})	F17C1/00	F17C1/00		3628
F17C1/002	8	{Storage in barges or on ships}	F17C1/00	F17C1/00		445
F17C1/005	8	{Storage of gas or gaseous mixture at high pressure and at high density condition, e.g. in the single state phase}	F17C1/00	F17C1/00		262
F17C1/007	8	{Underground or underwater storage}	F17C1/00	F17C1/00		476
F17C1/02	8	involving reinforcing arrangements {(F17C1/14, F17C1/16 take precedence)}	F17C1/02	F17C1/02		822
F17C1/04	9	Protecting sheathings	F17C1/04	F17C1/04		539
F17C1/06	10	built-up from wound-on bands or filamentary material, e.g. wires	F17C1/06	F17C1/06		1369
F17C1/08	9	Integral reinforcements, e.g. ribs	F17C1/08	F17C1/08		435
F17C1/10	8	with provision for protection against corrosion, e.g. due to gaseous acid ({F17C1/14, F17C1/16 take precedence}; inhibiting corrosion of metallic material or incrustation in general C23F)	F17C1/10	F17C1/10		321
F17C1/12	8	with provision for thermal insulation ({F17C1/14, F17C1/16 take precedence}; thermal insulation in general F16L59/00)	F17C1/12	F17C1/12		1515
F17C1/14	8	constructed of aluminium; constructed of non-magnetic steel	F17C1/14	F17C1/14		632
F17C1/16	8	constructed of plastics materials {(shaping of plastics B29C)}	F17C1/16	F17C1/16		1511
F17C3/00	7	Vessels not under pressure	F17C3/00	F17C3/00		999
F17C3/005	8	{Underground or underwater containers or vessels (storing in natural or artificial cavities in the earth in general B65G5/00)}	F17C3/00	F17C3/00		434
F17C3/02	8	with provision for thermal insulation (thermal insulation in general F16L59/00{; refrigerators F25D; insulation specially adapted for cryogenic vessels F17C13/001; tank vehicles B60P3/22; railway tank wagons B61D5/00})	F17C3/02	F17C3/02		556
F17C3/022	9	{Land-based bulk storage containers (civil engineering aspects E04H7/00)}	F17C3/02	F17C3/02		525
F17C3/025	9	{Bulk storage in barges or on ships (constructive aspects B63B25/16)}	F17C3/02	F17C3/02		1426
F17C3/027	10	{Wallpanels for so-called membrane tanks}	F17C3/02	F17C3/02		1280
F17C3/04	9	by insulating layers (F17C3/08 takes precedence)	F17C3/04	F17C3/04		1035
F17C3/06	10	on the inner surface, i.e. in contact with the stored fluid	F17C3/06	F17C3/06		180
F17C3/08	9	by vacuum spaces, e.g. Dewar flask (for household use A47J41/02)	F17C3/08	F17C3/08		1117
F17C3/085	10	{Cryostats}	F17C3/08	F17C3/08		723
F17C3/10	9	by liquid-circulating or vapour-circulating jackets	F17C3/10	F17C3/10		255
F17C3/12	8	with provision for protection against corrosion, e.g. due to gaseous acid (protection against corrosion in general C23F)	F17C3/12	F17C3/12		67
F17C5/00	7	Methods or apparatus for filling containers with liquefied, solidified, or compressed gases under pressures (adding propellants to aerosol containers B65B31/00)<br><br><u>NOTE</u><br><br>This group includes not only the filling of vessels for storage of compressed or liquefied gases, but also the filling of pressurised apparatus insofar as it is not covered by a single other subclass, e.g. A62C, B05B.	F17C5/00	F17C5/00		1133
F17C5/002	8	{Automated filling apparatus}	F17C5/00	F17C5/00		214
F17C5/005	9	{for gas bottles, such as on a continuous belt or on a merry-go-round}	F17C5/00	F17C5/00		283
F17C5/007	9	{for individual gas tanks or containers, e.g. in vehicles (filling with liquid fuel not under pressure, B60S5/02, B67D7/00)}	F17C5/00	F17C5/00		887
F17C5/02	8	for filling with liquefied gases	F17C5/02	F17C5/02		1762
F17C5/04	9	requiring the use of refrigeration, e.g. filling with helium or hydrogen	F17C5/04	F17C5/04		374
F17C5/06	8	for filling with compressed gases	F17C5/06	F17C5/06		4018
F17C6/00	7	Methods and apparatus for filling vessels not under pressure with liquefied or solidified gases	F17C6/00	F17C6/00		1883
F17C7/00	7	Methods or apparatus for discharging liquefied, solidified, or compressed gases from pressure vessels, not covered by another subclass	F17C7/00	F17C7/00		2325
F17C7/02	8	Discharging liquefied gases	F17C7/02	F17C7/02		1162
F17C7/04	9	with change of state, e.g. vaporisation	F17C7/04	F17C7/04		2351
F17C9/00	7	Methods or apparatus for discharging liquefied or solidified gases from vessels not under pressure	F17C9/00	F17C9/00		2165
F17C9/02	8	with change of state, e.g. vaporisation	F17C9/02	F17C9/02		3381
F17C9/04	9	Recovery of thermal energy	F17C9/04	F17C9/04		942
F17C11/00	7	Use of gas-solvents or gas-sorbents in vessels {(absorbing compositions for acetylene C10L3/04; absorbing compositions for hydrogen C01B3/0005)}	F17C11/00	F17C11/00		682
F17C11/002	8	{for acetylene}	F17C11/00	F17C11/00		131
F17C11/005	8	{for hydrogen}	F17C11/00	F17C11/00		1924
F17C11/007	8	{for hydrocarbon gases, such as methane or natural gas, propane, butane or mixtures thereof [LPG]}	F17C11/00	F17C11/00		469
F17C13/00	7	Details of vessels or of the filling or discharging of vessels	F17C13/00	F17C13/00		5934
F17C13/001	8	{Thermal insulation specially adapted for cryogenic vessels (vessels not under pressure with insulation F17C3/02; thermal insulation in general F16L59/00)}	F17C13/00	F17C13/00		1611
F17C13/002	8	{for vessels under pressure (F17C13/008 and F17C13/02&#160;-&#160;F17C13/12 take precedence)}	F17C13/00	F17C13/00		2602
F17C13/003	9	{Means for coding or identifying them and/or their contents}	F17C13/00	F17C13/00		256
F17C13/004	8	{for large storage vessels not under pressure (F17C13/008 and F17C13/02&#160;-&#160;F17C13/12 take precedence)}	F17C13/00	F17C13/00		1556
F17C13/005	8	{for medium-size and small storage vessels not under pressure (F17C13/008 and F17C13/02&#160;-&#160;F17C13/12 take precedence)}	F17C13/00	F17C13/00		389
F17C13/006	9	{for Dewar vessels or cryostats}	F17C13/00	F17C13/00		193
F17C13/007	10	{used for superconducting phenomena (investigating by nuclear magnetic resonance G01N24/08; magnets having superconductive winding H01F6/00)}	F17C13/00	F17C13/00		83
F17C13/008	8	{for use under microgravity conditions}	F17C13/00	F17C13/00		143
F17C13/02	8	Special adaptations of indicating, measuring, or monitoring equipment (measuring in general G01)	F17C13/02	F17C13/02		3577
F17C13/021	9	{having the height as the parameter}	F17C13/02	F17C13/02		785
F17C13/023	9	{having the mass as the parameter}	F17C13/02	F17C13/02		477
F17C13/025	9	{having the pressure as the parameter}	F17C13/02	F17C13/02		3945
F17C13/026	9	{having the temperature as the parameter}	F17C13/02	F17C13/02		2073
F17C13/028	9	{having the volume as the parameter}	F17C13/02	F17C13/02		337
F17C13/04	8	Arrangement or mounting of valves (valves per seF16K{; snap-coupling of nipples F16L37/00})	F17C13/04	F17C13/04		9574
F17C13/045	9	{Automatic change-over switching assembly for bottled gas systems with two (or more) gas containers}	F17C13/04	F17C13/04		405
F17C13/06	8	Closures, e.g. cap, breakable member ({for autoclaves B01J3/03}; closures for {large} containers in general B65D{B65D90/54}; {for pressure vessels in general F16J13/00})	F17C13/06	F17C13/06		2291
F17C13/08	8	Mounting arrangements for vessels	F17C13/08	F17C13/08		1902
F17C13/081	9	{for large land-based storage vessels (supports for large containers in general B65D90/12)}	F17C13/08	F17C13/08		272
F17C13/082	9	{for large sea-borne storage vessels (load-accommodating arrangements for ships or waterborne vessels B63B25/12)}	F17C13/08	F17C13/08		661
F17C13/083	9	{for medium-sized mobile storage vessels, e.g. tank vehicles or railway tank vehicles}	F17C13/08	F17C13/08		354
F17C13/084	9	{for small-sized storage vessels, e.g. compressed gas cylinders or bottles, disposable gas vessels, vessels adapted for automotive use}	F17C13/08	F17C13/08		1982
F17C13/085	10	{on wheels (hand carts B62B)}	F17C13/08	F17C13/08		472
F17C13/086	9	{for Dewar vessels or cryostats}	F17C13/08	F17C13/08		158
F17C13/087	10	{used for superconducting phenomena}	F17C13/08	F17C13/08		82
F17C13/088	9	{for use under microgravity conditions}	F17C13/08	F17C13/08		41
F17C13/10	8	Arrangements for preventing freezing	F17C13/10	F17C13/10		415
F17C13/12	8	Arrangements or mounting of devices for preventing or minimising the effect of explosion (flame traps A62C4/00){; Other safety measures}	F17C13/12	F17C13/12		2462
F17C13/123	9	{for gas bottles, cylinders or reservoirs for tank vehicles or for railway tank wagons}	F17C13/12	F17C13/12		1181
F17C13/126	9	{for large storage containers for liquefied gas (for large containers in general B65D90/22)}	F17C13/12	F17C13/12		606
F17C2201/00	7	Vessel construction, in particular geometry, arrangement or size	CPCONLY	F17C2201/00		25
F17C2201/01	8	Shape	CPCONLY	F17C2201/01		90
F17C2201/0104	9	cylindrical	CPCONLY	F17C2201/0104		2173
F17C2201/0109	10	with exteriorly curved end-piece	CPCONLY	F17C2201/0109		7386
F17C2201/0114	10	with interiorly curved end-piece	CPCONLY	F17C2201/0114		354
F17C2201/0119	10	with flat end-piece	CPCONLY	F17C2201/0119		2457
F17C2201/0123	10	with variable thickness or diameter	CPCONLY	F17C2201/0123		283
F17C2201/0128	9	spherical or elliptical	CPCONLY	F17C2201/0128		1220
F17C2201/0133	9	toroidal	CPCONLY	F17C2201/0133		144
F17C2201/0138	9	tubular	CPCONLY	F17C2201/0138		448
F17C2201/0142	9	conical	CPCONLY	F17C2201/0142		62
F17C2201/0147	9	complex	CPCONLY	F17C2201/0147		317
F17C2201/0152	10	Lobes	CPCONLY	F17C2201/0152		248
F17C2201/0157	10	Polygonal	CPCONLY	F17C2201/0157		1160
F17C2201/0161	10	Honeycomb	CPCONLY	F17C2201/0161		48
F17C2201/0166	10	divided in several chambers	CPCONLY	F17C2201/0166		574
F17C2201/0171	10	comprising a communication hole between chambers	CPCONLY	F17C2201/0171		306
F17C2201/0176	9	variable	CPCONLY	F17C2201/0176		129
F17C2201/018	10	with bladders	CPCONLY	F17C2201/018		238
F17C2201/0185	10	with separating membrane	CPCONLY	F17C2201/0185		135
F17C2201/019	10	with pistons	CPCONLY	F17C2201/019		96
F17C2201/0195	10	with bellows	CPCONLY	F17C2201/0195		53
F17C2201/03	8	Orientation	CPCONLY	F17C2201/03		4
F17C2201/032	9	with substantially vertical main axis	CPCONLY	F17C2201/032		2779
F17C2201/035	9	with substantially horizontal main axis	CPCONLY	F17C2201/035		1986
F17C2201/037	9	with sloping main axis	CPCONLY	F17C2201/037		72
F17C2201/05	8	Size	CPCONLY	F17C2201/05		7
F17C2201/052	9	large (&gt;1000 m3)	CPCONLY	F17C2201/052		2363
F17C2201/054	9	medium (&gt;1 m3)	CPCONLY	F17C2201/054		2014
F17C2201/056	9	Small (&lt;1 m3)	CPCONLY	F17C2201/056		4342
F17C2201/058	9	portable (&lt;30 l)	CPCONLY	F17C2201/058		2939
F17C2201/06	8	Vessel construction using filling material in contact with the handled fluid	CPCONLY	F17C2201/06		102
F17C2203/00	7	Vessel construction, in particular walls or details thereof	CPCONLY	F17C2203/00		29
F17C2203/01	8	Reinforcing or suspension means	CPCONLY	F17C2203/01		141
F17C2203/011	9	Reinforcing means	CPCONLY	F17C2203/011		452
F17C2203/012	10	on or in the wall, e.g. ribs	CPCONLY	F17C2203/012		1164
F17C2203/013	10	in the vessel, e.g. columns	CPCONLY	F17C2203/013		481
F17C2203/014	9	Suspension means	CPCONLY	F17C2203/014		390
F17C2203/015	10	Bars	CPCONLY	F17C2203/015		201
F17C2203/016	10	Cords	CPCONLY	F17C2203/016		107
F17C2203/017	10	Magnetic means	CPCONLY	F17C2203/017		22
F17C2203/018	10	by attachment at the neck	CPCONLY	F17C2203/018		219
F17C2203/03	8	Thermal insulations	CPCONLY	F17C2203/03		1268
F17C2203/0304	9	by solid means	CPCONLY	F17C2203/0304		694
F17C2203/0308	10	Radiation shield	CPCONLY	F17C2203/0308		244
F17C2203/0312	11	cooled by external means	CPCONLY	F17C2203/0312		49
F17C2203/0316	11	cooled by vaporised gas from the interior	CPCONLY	F17C2203/0316		76
F17C2203/032	11	Multi-sheet layers	CPCONLY	F17C2203/032		369
F17C2203/0325	10	Aerogel	CPCONLY	F17C2203/0325		244
F17C2203/0329	10	Foam	CPCONLY	F17C2203/0329		575
F17C2203/0333	11	Polyurethane	CPCONLY	F17C2203/0333		837
F17C2203/0337	10	Granular	CPCONLY	F17C2203/0337		252
F17C2203/0341	11	Perlite	CPCONLY	F17C2203/0341		398
F17C2203/0345	10	Fibres	CPCONLY	F17C2203/0345		323
F17C2203/035	11	Glass wool	CPCONLY	F17C2203/035		501
F17C2203/0354	10	Wood	CPCONLY	F17C2203/0354		447
F17C2203/0358	10	in form of panels	CPCONLY	F17C2203/0358		1175
F17C2203/0362	9	by liquid means	CPCONLY	F17C2203/0362		74
F17C2203/0366	10	Cryogen	CPCONLY	F17C2203/0366		114
F17C2203/037	10	Water	CPCONLY	F17C2203/037		47
F17C2203/0375	9	by gas	CPCONLY	F17C2203/0375		108
F17C2203/0379	10	Inert	CPCONLY	F17C2203/0379		207
F17C2203/0383	10	Air	CPCONLY	F17C2203/0383		73
F17C2203/0387	10	Cryogen	CPCONLY	F17C2203/0387		61
F17C2203/0391	9	by vacuum	CPCONLY	F17C2203/0391		1990
F17C2203/0395	10	Getter	CPCONLY	F17C2203/0395		101
F17C2203/06	8	Materials for walls or layers thereof; Properties or structures of walls or their materials	CPCONLY	F17C2203/06		30
F17C2203/0602	9	Wall structures; Special features thereof	CPCONLY	F17C2203/0602		148
F17C2203/0604	10	Liners	CPCONLY	F17C2203/0604		2197
F17C2203/0607	10	Coatings	CPCONLY	F17C2203/0607		656
F17C2203/0609	10	Straps, bands or ribbons	CPCONLY	F17C2203/0609		233
F17C2203/0612	10	Wall structures	CPCONLY	F17C2203/0612		133
F17C2203/0614	11	Single wall	CPCONLY	F17C2203/0614		153
F17C2203/0617	12	with one layer	CPCONLY	F17C2203/0617		1409
F17C2203/0619	12	with two layers	CPCONLY	F17C2203/0619		1644
F17C2203/0621	12	with three layers	CPCONLY	F17C2203/0621		654
F17C2203/0624	12	with four or more layers	CPCONLY	F17C2203/0624		458
F17C2203/0626	11	Multiple walls	CPCONLY	F17C2203/0626		108
F17C2203/0629	12	Two walls	CPCONLY	F17C2203/0629		2839
F17C2203/0631	12	Three or more walls	CPCONLY	F17C2203/0631		850
F17C2203/0634	9	Materials for walls or layers thereof	CPCONLY	F17C2203/0634		81
F17C2203/0636	10	Metals	CPCONLY	F17C2203/0636		1751
F17C2203/0639	11	Steels	CPCONLY	F17C2203/0639		1657
F17C2203/0641	12	Non-magnetic steels	CPCONLY	F17C2203/0641		26
F17C2203/0643	12	Stainless steels	CPCONLY	F17C2203/0643		1072
F17C2203/0646	11	Aluminium	CPCONLY	F17C2203/0646		1552
F17C2203/0648	11	Alloys or compositions of metals	CPCONLY	F17C2203/0648		973
F17C2203/0651	12	Invar	CPCONLY	F17C2203/0651		171
F17C2203/0653	11	Lead	CPCONLY	F17C2203/0653		12
F17C2203/0656	11	in form of filaments	CPCONLY	F17C2203/0656		144
F17C2203/0658	10	Synthetics	CPCONLY	F17C2203/0658		363
F17C2203/066	11	Plastics	CPCONLY	F17C2203/066		1714
F17C2203/0663	11	in form of fibers or filaments	CPCONLY	F17C2203/0663		2128
F17C2203/0665	12	radially wound	CPCONLY	F17C2203/0665		324
F17C2203/0668	12	axially wound	CPCONLY	F17C2203/0668		156
F17C2203/067	12	helically wound	CPCONLY	F17C2203/067		413
F17C2203/0673	12	Polymers	CPCONLY	F17C2203/0673		714
F17C2203/0675	11	with details of composition	CPCONLY	F17C2203/0675		235
F17C2203/0678	10	Concrete	CPCONLY	F17C2203/0678		748
F17C2203/068	9	Special properties of materials for vessel walls	CPCONLY	F17C2203/068		124
F17C2203/0682	10	with liquid or gas layer	CPCONLY	F17C2203/0682		128
F17C2203/0685	10	flexible	CPCONLY	F17C2203/0685		252
F17C2203/0687	10	superconducting	CPCONLY	F17C2203/0687		163
F17C2203/069	10	Break point in the wall	CPCONLY	F17C2203/069		82
F17C2203/0692	10	transparent	CPCONLY	F17C2203/0692		78
F17C2203/0695	10	pre-constrained	CPCONLY	F17C2203/0695		71
F17C2203/0697	10	comprising nanoparticles	CPCONLY	F17C2203/0697		72
F17C2205/00	7	Vessel construction, in particular mounting arrangements, attachments or identifications means	CPCONLY	F17C2205/00		30
F17C2205/01	8	Mounting arrangements	CPCONLY	F17C2205/01		117
F17C2205/0103	9	Exterior arrangements	CPCONLY	F17C2205/0103		565
F17C2205/0107	10	Frames	CPCONLY	F17C2205/0107		1120
F17C2205/0111	10	Boxes	CPCONLY	F17C2205/0111		737
F17C2205/0115	10	Dismountable protective hulls	CPCONLY	F17C2205/0115		280
F17C2205/0119	10	Vessel walls form part of another structure	CPCONLY	F17C2205/0119		128
F17C2205/0123	9	characterised by number of vessels	CPCONLY	F17C2205/0123		5
F17C2205/0126	10	One vessel	CPCONLY	F17C2205/0126		828
F17C2205/013	10	Two or more vessels	CPCONLY	F17C2205/013		1274
F17C2205/0134	11	characterised by the presence of fluid connection between vessels	CPCONLY	F17C2205/0134		366
F17C2205/0138	12	bundled in series	CPCONLY	F17C2205/0138		197
F17C2205/0142	12	bundled in parallel	CPCONLY	F17C2205/0142		1128
F17C2205/0146	12	with details of the manifold	CPCONLY	F17C2205/0146		533
F17C2205/0149	11	Vessel mounted inside another one	CPCONLY	F17C2205/0149		222
F17C2205/0153	9	Details of mounting arrangements	CPCONLY	F17C2205/0153		492
F17C2205/0157	10	for transport	CPCONLY	F17C2205/0157		360
F17C2205/0161	11	with wheels	CPCONLY	F17C2205/0161		610
F17C2205/0165	11	with handgrip	CPCONLY	F17C2205/0165		658
F17C2205/0169	10	stackable	CPCONLY	F17C2205/0169		178
F17C2205/0173	10	lockable	CPCONLY	F17C2205/0173		174
F17C2205/0176	10	with ventilation	CPCONLY	F17C2205/0176		239
F17C2205/018	10	Supporting feet	CPCONLY	F17C2205/018		1866
F17C2205/0184	10	Attachments to the ground, e.g. mooring or anchoring	CPCONLY	F17C2205/0184		240
F17C2205/0188	10	Hanging up devices	CPCONLY	F17C2205/0188		272
F17C2205/0192	10	with external bearing means	CPCONLY	F17C2205/0192		524
F17C2205/0196	10	with shock absorbing means	CPCONLY	F17C2205/0196		520
F17C2205/03	8	Fluid connections, filters, valves, closure means or other attachments	CPCONLY	F17C2205/03		131
F17C2205/0302	9	Fittings, valves, filters, or components in connection with the gas storage device	CPCONLY	F17C2205/0302		681
F17C2205/0305	10	Bosses, e.g. boss collars	CPCONLY	F17C2205/0305		1333
F17C2205/0308	10	Protective caps	CPCONLY	F17C2205/0308		1305
F17C2205/0311	10	Closure means	CPCONLY	F17C2205/0311		923
F17C2205/0314	11	breakable, e.g. with burst discs	CPCONLY	F17C2205/0314		354
F17C2205/0317	11	fusing or melting	CPCONLY	F17C2205/0317		185
F17C2205/032	11	pierceable	CPCONLY	F17C2205/032		333
F17C2205/0323	10	Valves	CPCONLY	F17C2205/0323		4931
F17C2205/0326	11	electrically actuated	CPCONLY	F17C2205/0326		1964
F17C2205/0329	11	manually actuated	CPCONLY	F17C2205/0329		1797
F17C2205/0332	11	Safety valves or pressure relief valves	CPCONLY	F17C2205/0332		3213
F17C2205/0335	11	Check-valves or non-return valves	CPCONLY	F17C2205/0335		1706
F17C2205/0338	10	Pressure regulators	CPCONLY	F17C2205/0338		1928
F17C2205/0341	10	Filters	CPCONLY	F17C2205/0341		734
F17C2205/0344	11	Sinter type	CPCONLY	F17C2205/0344		33
F17C2205/0347	11	Active charcoal type	CPCONLY	F17C2205/0347		27
F17C2205/035	10	Flow reducers	CPCONLY	F17C2205/035		283
F17C2205/0352	10	Pipes	CPCONLY	F17C2205/0352		1551
F17C2205/0355	11	Insulation thereof	CPCONLY	F17C2205/0355		264
F17C2205/0358	11	coaxial	CPCONLY	F17C2205/0358		141
F17C2205/0361	11	corrugated	CPCONLY	F17C2205/0361		37
F17C2205/0364	11	flexible or articulated, e.g. a hose	CPCONLY	F17C2205/0364		569
F17C2205/0367	11	Arrangements in parallel	CPCONLY	F17C2205/0367		238
F17C2205/037	10	Quick connecting means, e.g. couplings	CPCONLY	F17C2205/037		741
F17C2205/0373	11	Adapters	CPCONLY	F17C2205/0373		211
F17C2205/0376	10	Dispensing pistols	CPCONLY	F17C2205/0376		308
F17C2205/0379	10	Manholes or access openings for human beings	CPCONLY	F17C2205/0379		237
F17C2205/0382	10	Constructional details of valves, regulators	CPCONLY	F17C2205/0382		1723
F17C2205/0385	11	in blocks or units	CPCONLY	F17C2205/0385		837
F17C2205/0388	9	Arrangement of valves, regulators, filters	CPCONLY	F17C2205/0388		396
F17C2205/0391	10	inside the pressure vessel	CPCONLY	F17C2205/0391		476
F17C2205/0394	10	in direct contact with the pressure vessel	CPCONLY	F17C2205/0394		1564
F17C2205/0397	11	on both sides of the pressure vessel	CPCONLY	F17C2205/0397		483
F17C2205/05	8	Vessel or content identifications, e.g. labels	CPCONLY	F17C2205/05		213
F17C2205/051	9	by coating	CPCONLY	F17C2205/051		48
F17C2205/052	9	by stickers	CPCONLY	F17C2205/052		61
F17C2205/054	9	by bar codes	CPCONLY	F17C2205/054		97
F17C2205/055	9	by magnetic means	CPCONLY	F17C2205/055		40
F17C2205/057	9	by chips	CPCONLY	F17C2205/057		56
F17C2205/058	9	by Radio Frequency Identification	CPCONLY	F17C2205/058		174
F17C2209/00	7	Vessel construction, in particular methods of manufacturing	CPCONLY	F17C2209/00		63
F17C2209/21	8	Shaping processes	CPCONLY	F17C2209/21		148
F17C2209/2109	9	Moulding	CPCONLY	F17C2209/2109		287
F17C2209/2118	10	by injection	CPCONLY	F17C2209/2118		252
F17C2209/2127	10	by blowing	CPCONLY	F17C2209/2127		291
F17C2209/2136	10	using wax moulds	CPCONLY	F17C2209/2136		12
F17C2209/2145	10	by rotation	CPCONLY	F17C2209/2145		107
F17C2209/2154	9	Winding	CPCONLY	F17C2209/2154		841
F17C2209/2163	10	with a mandrel	CPCONLY	F17C2209/2163		334
F17C2209/2172	9	Polishing	CPCONLY	F17C2209/2172		64
F17C2209/2181	9	Metal working processes, e.g. deep drawing, stamping or cutting	CPCONLY	F17C2209/2181		355
F17C2209/219	9	Working processes for non metal materials, e.g. extruding	CPCONLY	F17C2209/219		130
F17C2209/22	8	Assembling processes	CPCONLY	F17C2209/22		437
F17C2209/221	9	Welding	CPCONLY	F17C2209/221		1996
F17C2209/222	10	by friction	CPCONLY	F17C2209/222		65
F17C2209/224	9	Press-fitting; Shrink-fitting	CPCONLY	F17C2209/224		187
F17C2209/225	9	Spraying	CPCONLY	F17C2209/225		157
F17C2209/227	9	by adhesive means	CPCONLY	F17C2209/227		809
F17C2209/228	9	by screws, bolts or rivets	CPCONLY	F17C2209/228		1050
F17C2209/23	8	Manufacturing of particular parts or at special locations	CPCONLY	F17C2209/23		173
F17C2209/232	9	of walls	CPCONLY	F17C2209/232		1204
F17C2209/234	9	of closing end pieces, e.g. caps	CPCONLY	F17C2209/234		609
F17C2209/236	10	Apparatus therefore	CPCONLY	F17C2209/236		60
F17C2209/238	9	Filling of insulants	CPCONLY	F17C2209/238		174
F17C2221/00	7	Handled fluid, in particular type of fluid	CPCONLY	F17C2221/00		25
F17C2221/01	8	Pure fluids	CPCONLY	F17C2221/01		546
F17C2221/011	9	Oxygen	CPCONLY	F17C2221/011		2481
F17C2221/012	9	Hydrogen	CPCONLY	F17C2221/012		7732
F17C2221/013	9	Carbon dioxide	CPCONLY	F17C2221/013		1596
F17C2221/014	9	Nitrogen	CPCONLY	F17C2221/014		2614
F17C2221/015	9	Carbon monoxide	CPCONLY	F17C2221/015		102
F17C2221/016	9	Noble gases (Ar, Kr, Xe)	CPCONLY	F17C2221/016		665
F17C2221/017	10	Helium	CPCONLY	F17C2221/017		1239
F17C2221/018	9	Acetylene	CPCONLY	F17C2221/018		227
F17C2221/03	8	Mixtures	CPCONLY	F17C2221/03		664
F17C2221/031	9	Air	CPCONLY	F17C2221/031		1459
F17C2221/032	9	Hydrocarbons	CPCONLY	F17C2221/032		903
F17C2221/033	10	Methane, e.g. natural gas, CNG, LNG, GNL, GNC, PLNG	CPCONLY	F17C2221/033		8719
F17C2221/035	10	Propane butane, e.g. LPG, GPL	CPCONLY	F17C2221/035		2994
F17C2221/036	10	Hydrates	CPCONLY	F17C2221/036		36
F17C2221/037	9	Containing pollutant, e.g. H2S, Cl	CPCONLY	F17C2221/037		220
F17C2221/038	9	Refrigerants	CPCONLY	F17C2221/038		158
F17C2221/05	8	Ultrapure fluid	CPCONLY	F17C2221/05		142
F17C2221/07	8	Hyperpolarised gases	CPCONLY	F17C2221/07		14
F17C2221/08	8	Ergols, e.g. hydrazine	CPCONLY	F17C2221/08		75
F17C2223/00	7	Handled fluid before transfer, i.e. state of fluid when stored in the vessel or before transfer from the vessel	CPCONLY	F17C2223/00		35
F17C2223/01	8	characterised by the phase	CPCONLY	F17C2223/01		5
F17C2223/0107	9	Single phase	CPCONLY	F17C2223/0107		14
F17C2223/0115	10	dense or supercritical, i.e. at high pressure and high density	CPCONLY	F17C2223/0115		170
F17C2223/0123	10	gaseous, e.g. CNG, GNC	CPCONLY	F17C2223/0123		7329
F17C2223/013	10	liquid	CPCONLY	F17C2223/013		739
F17C2223/0138	10	solid	CPCONLY	F17C2223/0138		211
F17C2223/0146	9	Two-phase	CPCONLY	F17C2223/0146		45
F17C2223/0153	10	Liquefied gas, e.g. LPG, GPL	CPCONLY	F17C2223/0153		5202
F17C2223/0161	11	cryogenic, e.g. LNG, GNL, PLNG	CPCONLY	F17C2223/0161		9245
F17C2223/0169	11	subcooled	CPCONLY	F17C2223/0169		152
F17C2223/0176	10	Solids and gas	CPCONLY	F17C2223/0176		101
F17C2223/0184	10	Liquids and solids	CPCONLY	F17C2223/0184		26
F17C2223/0192	9	Three-phase, e.g. CO2 at triple point	CPCONLY	F17C2223/0192		35
F17C2223/03	8	characterised by the pressure level	CPCONLY	F17C2223/03		28
F17C2223/031	9	Not under pressure, i.e. containing liquids or solids only	CPCONLY	F17C2223/031		98
F17C2223/033	9	Small pressure, e.g. for liquefied gas	CPCONLY	F17C2223/033		5942
F17C2223/035	9	High pressure (&gt;10 bar)	CPCONLY	F17C2223/035		2449
F17C2223/036	9	Very high pressure (&gt;80 bar)	CPCONLY	F17C2223/036		4180
F17C2223/038	9	Subatmospheric pressure	CPCONLY	F17C2223/038		67
F17C2223/04	8	characterised by other properties of handled fluid before transfer	CPCONLY	F17C2223/04		4
F17C2223/041	9	Stratification	CPCONLY	F17C2223/041		77
F17C2223/042	9	Localisation of the removal point	CPCONLY	F17C2223/042		12
F17C2223/043	10	in the gas	CPCONLY	F17C2223/043		452
F17C2223/045	11	with a dip tube	CPCONLY	F17C2223/045		264
F17C2223/046	10	in the liquid	CPCONLY	F17C2223/046		439
F17C2223/047	11	with a dip tube	CPCONLY	F17C2223/047		1008
F17C2223/048	10	in the solid	CPCONLY	F17C2223/048		10
F17C2225/00	7	Handled fluid after transfer, i.e. state of fluid after transfer from the vessel	CPCONLY	F17C2225/00		3
F17C2225/01	8	characterised by the phase	CPCONLY	F17C2225/01		3
F17C2225/0107	9	Single phase	CPCONLY	F17C2225/0107		7
F17C2225/0115	10	dense or supercritical, i.e. at high pressure and high density	CPCONLY	F17C2225/0115		81
F17C2225/0123	10	gaseous, e.g. CNG, GNC	CPCONLY	F17C2225/0123		3238
F17C2225/013	10	liquid	CPCONLY	F17C2225/013		127
F17C2225/0138	10	solid	CPCONLY	F17C2225/0138		26
F17C2225/0146	9	Two-phase	CPCONLY	F17C2225/0146		13
F17C2225/0153	10	Liquefied gas, e.g. LPG, GPL	CPCONLY	F17C2225/0153		403
F17C2225/0161	11	cryogenic, e.g. LNG, GNL, PLNG	CPCONLY	F17C2225/0161		1288
F17C2225/0169	11	subcooled	CPCONLY	F17C2225/0169		86
F17C2225/0176	10	Solids and gas	CPCONLY	F17C2225/0176		11
F17C2225/0184	10	Liquids and solids	CPCONLY	F17C2225/0184		11
F17C2225/0192	9	Three-phase, e.g. CO2 at triple point	CPCONLY	F17C2225/0192		17
F17C2225/03	8	characterised by the pressure level	CPCONLY	F17C2225/03		13
F17C2225/031	9	Not under pressure, i.e. containing liquids or solids only	CPCONLY	F17C2225/031		12
F17C2225/033	9	Small pressure, e.g. for liquefied gas	CPCONLY	F17C2225/033		817
F17C2225/035	9	High pressure, i.e. between 10 and 80 bars	CPCONLY	F17C2225/035		876
F17C2225/036	9	Very high pressure, i.e. above 80 bars	CPCONLY	F17C2225/036		1034
F17C2225/038	9	Subatmospheric pressure	CPCONLY	F17C2225/038		25
F17C2225/04	8	characterised by other properties of handled fluid after transfer	CPCONLY	F17C2225/04		5
F17C2225/041	9	Stratification	CPCONLY	F17C2225/041		20
F17C2225/042	9	Localisation of the filling point	CPCONLY	F17C2225/042		8
F17C2225/043	10	in the gas	CPCONLY	F17C2225/043		144
F17C2225/044	11	at several points, e.g. with a device for recondensing gas	CPCONLY	F17C2225/044		144
F17C2225/045	11	with a dip tube	CPCONLY	F17C2225/045		96
F17C2225/046	10	in the liquid	CPCONLY	F17C2225/046		115
F17C2225/047	11	with a dip tube	CPCONLY	F17C2225/047		259
F17C2225/048	10	in the solid	CPCONLY	F17C2225/048		7
F17C2227/00	7	Transfer of fluids, i.e. method or means for transferring the fluid; Heat exchange with the fluid	CPCONLY	F17C2227/00		21
F17C2227/01	8	Propulsion of the fluid	CPCONLY	F17C2227/01		89
F17C2227/0107	9	by pressurising the ullage	CPCONLY	F17C2227/0107		398
F17C2227/0114	9	with vacuum injectors, e.g. venturi	CPCONLY	F17C2227/0114		130
F17C2227/0121	9	by gravity	CPCONLY	F17C2227/0121		181
F17C2227/0128	9	with pumps or compressors	CPCONLY	F17C2227/0128		104
F17C2227/0135	10	Pumps	CPCONLY	F17C2227/0135		2774
F17C2227/0142	11	with specified pump type, e.g. piston or impulsive type	CPCONLY	F17C2227/0142		321
F17C2227/015	11	with cooling of the pump	CPCONLY	F17C2227/015		83
F17C2227/0157	10	Compressors	CPCONLY	F17C2227/0157		1917
F17C2227/0164	11	with specified compressor type, e.g. piston or impulsive type	CPCONLY	F17C2227/0164		230
F17C2227/0171	10	Arrangement	CPCONLY	F17C2227/0171		22
F17C2227/0178	11	in the vessel	CPCONLY	F17C2227/0178		392
F17C2227/0185	11	comprising several pumps or compressors	CPCONLY	F17C2227/0185		669
F17C2227/0192	9	by using a working fluid	CPCONLY	F17C2227/0192		362
F17C2227/03	8	Heat exchange with the fluid	CPCONLY	F17C2227/03		300
F17C2227/0302	9	by heating	CPCONLY	F17C2227/0302		1402
F17C2227/0304	10	using an electric heater	CPCONLY	F17C2227/0304		743
F17C2227/0306	10	using the same fluid	CPCONLY	F17C2227/0306		268
F17C2227/0309	10	using another fluid	CPCONLY	F17C2227/0309		692
F17C2227/0311	11	Air heating	CPCONLY	F17C2227/0311		372
F17C2227/0313	12	by forced circulation, e.g. using a fan	CPCONLY	F17C2227/0313		127
F17C2227/0316	11	Water heating	CPCONLY	F17C2227/0316		492
F17C2227/0318	12	using seawater	CPCONLY	F17C2227/0318		308
F17C2227/032	12	using geothermal water	CPCONLY	F17C2227/032		10
F17C2227/0323	11	in a closed loop	CPCONLY	F17C2227/0323		366
F17C2227/0325	10	by expansion using "Joule-Thompson" effect	CPCONLY	F17C2227/0325		48
F17C2227/0327	10	with recovery of heat	CPCONLY	F17C2227/0327		202
F17C2227/033	10	using solar energy	CPCONLY	F17C2227/033		44
F17C2227/0332	10	by burning a combustible	CPCONLY	F17C2227/0332		128
F17C2227/0334	10	by radiation means	CPCONLY	F17C2227/0334		18
F17C2227/0337	9	by cooling	CPCONLY	F17C2227/0337		936
F17C2227/0339	10	using the same fluid	CPCONLY	F17C2227/0339		655
F17C2227/0341	10	using another fluid	CPCONLY	F17C2227/0341		805
F17C2227/0344	11	Air cooling	CPCONLY	F17C2227/0344		118
F17C2227/0346	12	by forced circulation, e.g. using a fan	CPCONLY	F17C2227/0346		78
F17C2227/0348	11	Water cooling	CPCONLY	F17C2227/0348		288
F17C2227/0351	12	using seawater	CPCONLY	F17C2227/0351		63
F17C2227/0353	11	using cryocooler	CPCONLY	F17C2227/0353		190
F17C2227/0355	11	in a closed loop	CPCONLY	F17C2227/0355		307
F17C2227/0358	10	by expansion	CPCONLY	F17C2227/0358		128
F17C2227/036	11	"Joule-Thompson" effect	CPCONLY	F17C2227/036		123
F17C2227/0362	11	in a turbine	CPCONLY	F17C2227/0362		38
F17C2227/0365	10	with recovery of heat	CPCONLY	F17C2227/0365		93
F17C2227/0367	9	Localisation of heat exchange	CPCONLY	F17C2227/0367		38
F17C2227/0369	10	in or on a vessel	CPCONLY	F17C2227/0369		179
F17C2227/0372	11	in the gas	CPCONLY	F17C2227/0372		149
F17C2227/0374	11	in the liquid	CPCONLY	F17C2227/0374		282
F17C2227/0376	11	in wall contact	CPCONLY	F17C2227/0376		53
F17C2227/0379	12	inside the vessel	CPCONLY	F17C2227/0379		194
F17C2227/0381	12	integrated in the wall	CPCONLY	F17C2227/0381		189
F17C2227/0383	12	outside the vessel	CPCONLY	F17C2227/0383		233
F17C2227/0386	13	with a jacket	CPCONLY	F17C2227/0386		89
F17C2227/0388	10	separate	CPCONLY	F17C2227/0388		467
F17C2227/039	11	on the pipes	CPCONLY	F17C2227/039		539
F17C2227/0393	11	using a vaporiser	CPCONLY	F17C2227/0393		1400
F17C2227/0395	11	using a submerged heat exchanger	CPCONLY	F17C2227/0395		71
F17C2227/0397	10	characterised by fins	CPCONLY	F17C2227/0397		139
F17C2227/04	8	Methods for emptying or filling	CPCONLY	F17C2227/04		1462
F17C2227/041	9	vessel by vessel	CPCONLY	F17C2227/041		215
F17C2227/042	10	with change-over from one vessel to another	CPCONLY	F17C2227/042		197
F17C2227/043	9	by pressure cascade	CPCONLY	F17C2227/043		273
F17C2227/044	9	by purging	CPCONLY	F17C2227/044		571
F17C2227/045	9	by vacuum	CPCONLY	F17C2227/045		165
F17C2227/046	9	by even emptying or filling	CPCONLY	F17C2227/046		240
F17C2227/047	9	by repeating a process cycle	CPCONLY	F17C2227/047		114
F17C2227/048	9	by maintaining residual pressure	CPCONLY	F17C2227/048		275
F17C2250/00	7	Accessories; Control means; Indicating, measuring or monitoring of parameters	CPCONLY	F17C2250/00		39
F17C2250/01	8	Intermediate tanks	CPCONLY	F17C2250/01		574
F17C2250/03	8	Control means	CPCONLY	F17C2250/03		657
F17C2250/032	9	using computers	CPCONLY	F17C2250/032		2295
F17C2250/034	9	using wireless transmissions	CPCONLY	F17C2250/034		781
F17C2250/036	9	using alarms	CPCONLY	F17C2250/036		911
F17C2250/038	9	using cameras	CPCONLY	F17C2250/038		93
F17C2250/04	8	Indicating or measuring of parameters as input values	CPCONLY	F17C2250/04		233
F17C2250/0404	9	Parameters indicated or measured	CPCONLY	F17C2250/0404		255
F17C2250/0408	10	Level of content in the vessel	CPCONLY	F17C2250/0408		912
F17C2250/0413	11	with floats	CPCONLY	F17C2250/0413		392
F17C2250/0417	11	with electrical means	CPCONLY	F17C2250/0417		203
F17C2250/0421	10	Mass or weight of the content of the vessel	CPCONLY	F17C2250/0421		540
F17C2250/0426	10	Volume	CPCONLY	F17C2250/0426		266
F17C2250/043	10	Pressure	CPCONLY	F17C2250/043		4321
F17C2250/0434	11	Pressure difference	CPCONLY	F17C2250/0434		314
F17C2250/0439	10	Temperature	CPCONLY	F17C2250/0439		2656
F17C2250/0443	10	Flow or movement of content	CPCONLY	F17C2250/0443		857
F17C2250/0447	10	Composition; Humidity	CPCONLY	F17C2250/0447		196
F17C2250/0452	11	Concentration of a product	CPCONLY	F17C2250/0452		394
F17C2250/0456	11	Calorific or heating value	CPCONLY	F17C2250/0456		32
F17C2250/046	11	Humidity	CPCONLY	F17C2250/046		67
F17C2250/0465	10	Vibrations, e.g. of acoustic type	CPCONLY	F17C2250/0465		81
F17C2250/0469	10	Constraints, e.g. by gauges	CPCONLY	F17C2250/0469		122
F17C2250/0473	10	Time or time periods	CPCONLY	F17C2250/0473		221
F17C2250/0478	10	Position or presence	CPCONLY	F17C2250/0478		347
F17C2250/0482	10	Acceleration	CPCONLY	F17C2250/0482		104
F17C2250/0486	9	Indicating or measuring characterised by the location	CPCONLY	F17C2250/0486		50
F17C2250/0491	10	Parameters measured at or inside the vessel	CPCONLY	F17C2250/0491		711
F17C2250/0495	10	the indicated parameter is a converted measured parameter	CPCONLY	F17C2250/0495		331
F17C2250/06	8	Controlling or regulating of parameters as output values	CPCONLY	F17C2250/06		31
F17C2250/0605	9	Parameters	CPCONLY	F17C2250/0605		29
F17C2250/061	10	Level of content in the vessel	CPCONLY	F17C2250/061		278
F17C2250/0615	10	Mass or weight of the content of the vessel	CPCONLY	F17C2250/0615		115
F17C2250/0621	10	Volume	CPCONLY	F17C2250/0621		117
F17C2250/0626	10	Pressure	CPCONLY	F17C2250/0626		1616
F17C2250/0631	10	Temperature	CPCONLY	F17C2250/0631		897
F17C2250/0636	10	Flow or movement of content	CPCONLY	F17C2250/0636		1400
F17C2250/0642	10	Composition; Humidity	CPCONLY	F17C2250/0642		50
F17C2250/0647	11	Concentration of a product	CPCONLY	F17C2250/0647		81
F17C2250/0652	11	Calorific or heating value	CPCONLY	F17C2250/0652		16
F17C2250/0657	11	Humidity	CPCONLY	F17C2250/0657		22
F17C2250/0663	10	Vibrations, e.g. of acoustic type	CPCONLY	F17C2250/0663		22
F17C2250/0668	10	Constraints, e.g. by gauges	CPCONLY	F17C2250/0668		16
F17C2250/0673	10	Time or time periods	CPCONLY	F17C2250/0673		58
F17C2250/0678	10	Position or presence	CPCONLY	F17C2250/0678		76
F17C2250/0684	10	Acceleration	CPCONLY	F17C2250/0684		5
F17C2250/0689	9	Methods for controlling or regulating	CPCONLY	F17C2250/0689		190
F17C2250/0694	10	with calculations	CPCONLY	F17C2250/0694		295
F17C2250/07	8	Actions triggered by measured parameters	CPCONLY	F17C2250/07		85
F17C2250/072	9	Action when predefined value is reached	CPCONLY	F17C2250/072		555
F17C2250/075	10	when full	CPCONLY	F17C2250/075		254
F17C2250/077	10	when empty	CPCONLY	F17C2250/077		139
F17C2260/00	7	Purposes of gas storage and gas handling	CPCONLY	F17C2260/00		14
F17C2260/01	8	Improving mechanical properties or manufacturing	CPCONLY	F17C2260/01		192
F17C2260/011	9	Improving strength	CPCONLY	F17C2260/011		1532
F17C2260/012	9	Reducing weight	CPCONLY	F17C2260/012		829
F17C2260/013	9	Reducing manufacturing time or effort	CPCONLY	F17C2260/013		773
F17C2260/015	9	Facilitating maintenance	CPCONLY	F17C2260/015		526
F17C2260/016	9	Preventing slosh	CPCONLY	F17C2260/016		571
F17C2260/017	9	by calculation	CPCONLY	F17C2260/017		139
F17C2260/018	9	Adapting dimensions	CPCONLY	F17C2260/018		452
F17C2260/02	8	Improving properties related to fluid or fluid transfer	CPCONLY	F17C2260/02		424
F17C2260/021	9	Avoiding over pressurising	CPCONLY	F17C2260/021		457
F17C2260/022	9	Avoiding overfilling	CPCONLY	F17C2260/022		210
F17C2260/023	9	Avoiding overheating	CPCONLY	F17C2260/023		411
F17C2260/024	9	Improving metering	CPCONLY	F17C2260/024		376
F17C2260/025	9	Reducing transfer time	CPCONLY	F17C2260/025		471
F17C2260/026	9	by calculation	CPCONLY	F17C2260/026		174
F17C2260/027	9	Making transfer independent of vessel orientation	CPCONLY	F17C2260/027		47
F17C2260/028	9	Avoiding unauthorised transfer	CPCONLY	F17C2260/028		164
F17C2260/03	8	Dealing with losses	CPCONLY	F17C2260/03		78
F17C2260/031	9	due to heat transfer	CPCONLY	F17C2260/031		284
F17C2260/032	10	Avoiding freezing or defrosting	CPCONLY	F17C2260/032		379
F17C2260/033	10	by enhancing insulation	CPCONLY	F17C2260/033		659
F17C2260/035	9	of fluid	CPCONLY	F17C2260/035		262
F17C2260/036	10	Avoiding leaks	CPCONLY	F17C2260/036		1247
F17C2260/037	10	Handling leaked fluid	CPCONLY	F17C2260/037		588
F17C2260/038	10	Detecting leaked fluid	CPCONLY	F17C2260/038		751
F17C2260/04	8	Reducing risks and environmental impact	CPCONLY	F17C2260/04		645
F17C2260/042	9	Reducing risk of explosion	CPCONLY	F17C2260/042		2224
F17C2260/044	9	Avoiding pollution or contamination	CPCONLY	F17C2260/044		492
F17C2260/046	9	Enhancing energy recovery	CPCONLY	F17C2260/046		360
F17C2260/048	9	Refurbishing	CPCONLY	F17C2260/048		91
F17C2260/05	8	Improving chemical properties	CPCONLY	F17C2260/05		36
F17C2260/053	9	Reducing corrosion	CPCONLY	F17C2260/053		346
F17C2260/056	9	Improving fluid characteristics	CPCONLY	F17C2260/056		169
F17C2265/00	7	Effects achieved by gas storage or gas handling	CPCONLY	F17C2265/00		8
F17C2265/01	8	Purifying the fluid	CPCONLY	F17C2265/01		122
F17C2265/012	9	by filtering	CPCONLY	F17C2265/012		277
F17C2265/015	9	by separating	CPCONLY	F17C2265/015		466
F17C2265/017	10	different phases of a same fluid	CPCONLY	F17C2265/017		451
F17C2265/02	8	Mixing fluids	CPCONLY	F17C2265/02		36
F17C2265/022	9	identical fluid	CPCONLY	F17C2265/022		239
F17C2265/025	9	different fluids	CPCONLY	F17C2265/025		304
F17C2265/027	10	with odorizing	CPCONLY	F17C2265/027		39
F17C2265/03	8	Treating the boil-off	CPCONLY	F17C2265/03		278
F17C2265/031	9	by discharge	CPCONLY	F17C2265/031		983
F17C2265/032	9	by recovery	CPCONLY	F17C2265/032		409
F17C2265/033	10	with cooling	CPCONLY	F17C2265/033		615
F17C2265/034	11	with condensing the gas phase	CPCONLY	F17C2265/034		607
F17C2265/035	11	with subcooling the liquid phase	CPCONLY	F17C2265/035		96
F17C2265/036	10	with heating	CPCONLY	F17C2265/036		143
F17C2265/037	10	with pressurising	CPCONLY	F17C2265/037		689
F17C2265/038	10	with expanding	CPCONLY	F17C2265/038		336
F17C2265/04	8	using an independent energy source, e.g. battery	CPCONLY	F17C2265/04		261
F17C2265/05	8	Regasification	CPCONLY	F17C2265/05		1272
F17C2265/06	8	Fluid distribution	CPCONLY	F17C2265/06		1015
F17C2265/061	9	for supply of supplying vehicles	CPCONLY	F17C2265/061		346
F17C2265/063	9	for supply of refuelling stations	CPCONLY	F17C2265/063		338
F17C2265/065	9	for refuelling vehicle fuel tanks	CPCONLY	F17C2265/065		1488
F17C2265/066	9	for feeding engines for propulsion	CPCONLY	F17C2265/066		1621
F17C2265/068	9	Distribution pipeline networks	CPCONLY	F17C2265/068		178
F17C2265/07	8	Generating electrical power as side effect	CPCONLY	F17C2265/07		432
F17C2270/00	7	Applications	CPCONLY	F17C2270/00		11
F17C2270/01	8	for fluid transport or storage	CPCONLY	F17C2270/01		287
F17C2270/0102	9	on or in the water	CPCONLY	F17C2270/0102		275
F17C2270/0105	10	Ships	CPCONLY	F17C2270/0105		5432
F17C2270/0107	11	Wall panels	CPCONLY	F17C2270/0107		1438
F17C2270/011	10	Barges	CPCONLY	F17C2270/011		128
F17C2270/0113	11	floating	CPCONLY	F17C2270/0113		203
F17C2270/0115	11	immerged	CPCONLY	F17C2270/0115		18
F17C2270/0118	10	Offshore	CPCONLY	F17C2270/0118		61
F17C2270/0121	11	Platforms	CPCONLY	F17C2270/0121		119
F17C2270/0123	11	Terminals	CPCONLY	F17C2270/0123		165
F17C2270/0126	11	Buoys	CPCONLY	F17C2270/0126		51
F17C2270/0128	11	Storage in depth	CPCONLY	F17C2270/0128		121
F17C2270/0131	10	Submarines	CPCONLY	F17C2270/0131		66
F17C2270/0134	9	placed above the ground	CPCONLY	F17C2270/0134		326
F17C2270/0136	10	Terminals	CPCONLY	F17C2270/0136		397
F17C2270/0139	10	Fuel stations	CPCONLY	F17C2270/0139		1030
F17C2270/0142	9	placed underground	CPCONLY	F17C2270/0142		365
F17C2270/0144	10	Type of cavity	CPCONLY	F17C2270/0144		47
F17C2270/0147	11	by burying vessels	CPCONLY	F17C2270/0147		296
F17C2270/0149	11	by digging cavities	CPCONLY	F17C2270/0149		148
F17C2270/0152	12	Salt caverns	CPCONLY	F17C2270/0152		69
F17C2270/0155	11	by using natural cavities	CPCONLY	F17C2270/0155		77
F17C2270/0157	10	Location of cavity	CPCONLY	F17C2270/0157		3
F17C2270/016	11	onshore	CPCONLY	F17C2270/016		105
F17C2270/0163	11	offshore	CPCONLY	F17C2270/0163		41
F17C2270/0165	9	on the road	CPCONLY	F17C2270/0165		90
F17C2270/0168	10	by vehicles	CPCONLY	F17C2270/0168		3075
F17C2270/0171	11	Trucks	CPCONLY	F17C2270/0171		1201
F17C2270/0173	11	Railways	CPCONLY	F17C2270/0173		371
F17C2270/0176	11	Buses	CPCONLY	F17C2270/0176		237
F17C2270/0178	11	Cars	CPCONLY	F17C2270/0178		1519
F17C2270/0181	10	Airbags	CPCONLY	F17C2270/0181		102
F17C2270/0184	10	Fuel cells	CPCONLY	F17C2270/0184		2026
F17C2270/0186	9	in the air or in space	CPCONLY	F17C2270/0186		184
F17C2270/0189	10	Planes	CPCONLY	F17C2270/0189		689
F17C2270/0192	10	Hot air balloons	CPCONLY	F17C2270/0192		20
F17C2270/0194	10	for use under microgravity conditions, e.g. space	CPCONLY	F17C2270/0194		272
F17C2270/0197	10	Rockets	CPCONLY	F17C2270/0197		262
F17C2270/02	8	for medical applications	CPCONLY	F17C2270/02		486
F17C2270/025	9	Breathing	CPCONLY	F17C2270/025		593
F17C2270/05	8	for industrial use	CPCONLY	F17C2270/05		1053
F17C2270/0509	9	"Dewar" vessels	CPCONLY	F17C2270/0509		456
F17C2270/0518	9	Semiconductors	CPCONLY	F17C2270/0518		584
F17C2270/0527	9	Superconductors	CPCONLY	F17C2270/0527		97
F17C2270/0536	10	Magnetic resonance imaging	CPCONLY	F17C2270/0536		90
F17C2270/0545	9	Tools	CPCONLY	F17C2270/0545		164
F17C2270/0554	9	Hydraulic applications	CPCONLY	F17C2270/0554		39
F17C2270/0563	9	Pneumatic applications	CPCONLY	F17C2270/0563		84
F17C2270/0572	9	Isostatic presses	CPCONLY	F17C2270/0572		4
F17C2270/0581	9	Power plants	CPCONLY	F17C2270/0581		251
F17C2270/059	9	Mass bottling, e.g. merry belts	CPCONLY	F17C2270/059		260
F17C2270/07	8	for household use	CPCONLY	F17C2270/07		358
F17C2270/0709	9	Camping gas	CPCONLY	F17C2270/0709		368
F17C2270/0718	9	Aerosols	CPCONLY	F17C2270/0718		115
F17C2270/0727	9	Thermos flasks	CPCONLY	F17C2270/0727		2
F17C2270/0736	9	Capsules, e.g. CO2	CPCONLY	F17C2270/0736		370
F17C2270/0745	9	Gas bottles	CPCONLY	F17C2270/0745		827
F17C2270/0754	9	Fire extinguishers	CPCONLY	F17C2270/0754		247
F17C2270/0763	9	Fuel cells	CPCONLY	F17C2270/0763		193
F17C2270/0772	9	Inflation devices, e.g. for rescue vests or tyres	CPCONLY	F17C2270/0772		183
F17C2270/0781	9	Diving equipments	CPCONLY	F17C2270/0781		175
F17C2270/079	9	Respiration devices for rescuing	CPCONLY	F17C2270/079		129
