F23Q1/00	7	Mechanical igniters (lighters containing fuel F23Q2/00; matches C06F)	F23Q1/00	F23Q1/00		119
F23Q1/02	8	using friction or shock effects	F23Q1/02	F23Q1/02		136
F23Q1/04	9	on a part moved by the fuel-controlling member, e.g. by a tap on a gas cooker	F23Q1/04	F23Q1/04		19
F23Q1/06	9	Portable igniters	F23Q1/06	F23Q1/06		244
F23Q2/00	7	Lighters containing fuel, e.g. for cigarettes	F23Q2/00	F23Q2/00		87
F23Q2/02	8	Lighters with liquid fuel {fuel which is fluid at atmospheric pressure}	F23Q2/02	F23Q2/02		386
F23Q2/04	9	with cerium-iron alloy and wick {with friction ignition}	F23Q2/04	F23Q2/04		11
F23Q2/06	10	with friction wheel	F23Q2/06	F23Q2/06		667
F23Q2/08	11	with ignition by spring action of the cover	F23Q2/08	F23Q2/08		1167
F23Q2/10	10	with other friction member	F23Q2/10	F23Q2/10		58
F23Q2/12	9	with cerium-iron alloy without wick	F23Q2/12	F23Q2/12		
F23Q2/14	9	with cerium-iron alloy and torch ignited by striking or pushing	F23Q2/14	F23Q2/14		330
F23Q2/16	8	Lighters with gaseous fuel, e.g. the gas being stored in liquid phase	F23Q2/16	F23Q2/16		616
F23Q2/161	9	{with friction wheel}	F23Q2/16	F23Q2/16		387
F23Q2/162	9	{with non-adjustable gas flame (if electrically ignited F23Q2/28)}	F23Q2/16	F23Q2/16		454
F23Q2/163	10	{Burners (gas valves)}	F23Q2/16	F23Q2/16		360
F23Q2/164	9	{Arrangements for preventing undesired ignition}	F23Q2/16	F23Q2/16		678
F23Q2/165	9	{with more than one flame}	F23Q2/16	F23Q2/16		44
F23Q2/167	9	with adjustable flame	F23Q2/167	F23Q2/167		285
F23Q2/173	9	Valves therefor (valves in general F16K)	F23Q2/173	F23Q2/173		351
F23Q2/18	8	Lighters with solid fuel	F23Q2/18	F23Q2/18		78
F23Q2/20	9	with cerium-iron alloy and friction wheel	F23Q2/20	F23Q2/20		6
F23Q2/22	9	with cerium-iron alloy and tinder	F23Q2/22	F23Q2/22		59
F23Q2/24	9	ignition pills or strips with inflammable parts {(ignition pills C06C9/00, C06C15/00; corresponding lighters with fluid fuel F23Q2/10)}	F23Q2/24	F23Q2/24		138
F23Q2/26	9	combined with liquid fuel lighters	F23Q2/26	F23Q2/26		15
F23Q2/28	8	Lighters characterised by electrical ignition of the fuel (lighter with electrically-produced sparks but without fuel F23Q3/00)	F23Q2/28	F23Q2/28		128
F23Q2/282	9	{with incandescent ignition (lighters with incandescent ignition but without fuel F23Q7/00)}	F23Q2/28	F23Q2/28		124
F23Q2/285	9	{with spark ignition}	F23Q2/28	F23Q2/28		460
F23Q2/287	10	{piezoelectric}	F23Q2/28	F23Q2/28		653
F23Q2/30	8	Lighters characterised by catalytic ignition of fuel (catalytic igniters without fuel C06C)	F23Q2/30	F23Q2/30		340
F23Q2/32	8	Lighters characterised by being combined with other objects (combinations with smokers&apos; equipment A24F)	F23Q2/32	F23Q2/32		1146
F23Q2/325	9	{combined with clock, timer or counter}	F23Q2/32	F23Q2/32		105
F23Q2/34	8	Component parts or accessories	F23Q2/34	F23Q2/34		832
F23Q2/345	9	{Scent-distribution or flame-colouring devices}	F23Q2/34	F23Q2/34		62
F23Q2/36	9	Casings	F23Q2/36	F23Q2/36		463
F23Q2/365	10	{Tabletop lighters}	F23Q2/36	F23Q2/36		207
F23Q2/38	10	with containers for flints or tools	F23Q2/38	F23Q2/38		30
F23Q2/40	9	Cover fastenings	F23Q2/40	F23Q2/40		202
F23Q2/42	9	Fuel containers; Closures for fuel containers	F23Q2/42	F23Q2/42		330
F23Q2/44	9	Wicks; Wick guides or fastenings	F23Q2/44	F23Q2/44		318
F23Q2/46	9	Friction wheels; Arrangement of friction wheels	F23Q2/46	F23Q2/46		381
F23Q2/48	9	Flint (composition, manufacture C06C15/00); Guides for, or arrangements of, flints	F23Q2/48	F23Q2/48		407
F23Q2/50	9	Protecting coverings	F23Q2/50	F23Q2/50		250
F23Q2/52	9	Filling devices (in general B67D)	F23Q2/52	F23Q2/52		577
F23Q3/00	7	Igniters using electrically-produced sparks (sparking-plugs H01T13/00)	F23Q3/00	F23Q3/00		1198
F23Q3/002	8	{using piezoelectric elements}	F23Q3/00	F23Q3/00		824
F23Q3/004	8	{Using semiconductor elements}	F23Q3/00	F23Q3/00		311
F23Q3/006	8	{Details (sparking-plugs H01T13/00)}	F23Q3/00	F23Q3/00		630
F23Q3/008	8	{Structurally associated with fluid-fuel burners}	F23Q3/00	F23Q3/00		698
F23Q3/01	8	Hand-held lighters, e.g. for cigarettes	F23Q3/01	F23Q3/01		254
F23Q5/00	7	Make-and-break ignition, i.e. with spark generated between electrodes by breaking contact therebetween (specially adapted for internal-combustion engines F02P15/00)	F23Q5/00	F23Q5/00		143
F23Q7/00	7	Incandescent ignition; Igniters using electrically-produced heat, e.g. lighters for cigarettes (circuits therefor H01T15/00); Electrically-heated glowing plugs	F23Q7/00	F23Q7/00		1297
F23Q7/001	8	{Glowing plugs for internal-combustion engines}	F23Q7/00	F23Q7/00		1807
F23Q2007/002	9	{with sensing means}	F23Q7/00	F23Q7/00		253
F23Q2007/004	9	{Manufacturing or assembling methods}	F23Q7/00	F23Q7/00		274
F23Q2007/005	10	{pressure sensors}	F23Q7/00	F23Q7/00		43
F23Q2007/007	10	{ion current sensors}	F23Q7/00	F23Q7/00		4
F23Q2007/008	10	{temperature sensors}	F23Q7/00	F23Q7/00		18
F23Q7/02	8	for igniting solid fuel	F23Q7/02	F23Q7/02		304
F23Q7/04	9	with fans for transfer of heat to fuel	F23Q7/04	F23Q7/04		136
F23Q7/06	8	structurally associated with fluid-fuel burners (lighters containing fuel F23Q2/00)	F23Q7/06	F23Q7/06		182
F23Q7/08	9	for evaporating and igniting liquid fuel, e.g. in hurricane lanterns	F23Q7/08	F23Q7/08		200
F23Q7/10	9	for gaseous fuel, e.g. in welding appliances	F23Q7/10	F23Q7/10		242
F23Q7/12	10	actuated by gas-controlling device	F23Q7/12	F23Q7/12		117
F23Q7/14	8	Portable igniters	F23Q7/14	F23Q7/14		105
F23Q7/16	9	with built-in battery	F23Q7/16	F23Q7/16		356
F23Q7/18	9	with built-in generator	F23Q7/18	F23Q7/18		57
F23Q7/20	9	with built-in mains transformer	F23Q7/20	F23Q7/20		24
F23Q7/22	8	Details	F23Q7/22	F23Q7/22		555
F23Q7/24	9	Safety arrangements	F23Q7/24	F23Q7/24		117
F23Q7/26	10	Provision for re-ignition	F23Q7/26	F23Q7/26		31
F23Q9/00	7	Pilot flame igniters	F23Q9/00	F23Q9/00		786
F23Q9/02	8	without interlock with main fuel supply	F23Q9/02	F23Q9/02		334
F23Q9/04	9	for upright burners, e.g. gas-cooker burners	F23Q9/04	F23Q9/04		259
F23Q9/045	10	{Structurally associated with a main-burner}	F23Q9/04	F23Q9/04		171
F23Q9/06	9	for inverted burners, e.g. gas lamps	F23Q9/06	F23Q9/06		21
F23Q9/08	8	with interlock with main fuel supply	F23Q9/08	F23Q9/08		111
F23Q9/10	9	to determine the sequence of supply of fuel to pilot and main burners	F23Q9/10	F23Q9/10		109
F23Q9/12	9	to permit the supply to the main burner in dependence upon existence of pilot flame	F23Q9/12	F23Q9/12		289
F23Q9/14	10	using electric means, e.g. by light-sensitive elements	F23Q9/14	F23Q9/14		266
F23Q11/00	7	Arrangement of catalytic igniters (catalytic igniters per seC06C)	F23Q11/00	F23Q11/00		62
F23Q11/04	8	at the burner	F23Q11/04	F23Q11/04		21
F23Q11/06	8	remote from the burner, e.g. on the chimney of a lamp	F23Q11/06	F23Q11/06		9
F23Q11/08	8	on a part moved by the fuel controlling member	F23Q11/08	F23Q11/08		1
F23Q11/10	9	and moving out of the flame after ignition	F23Q11/10	F23Q11/10		1
F23Q13/00	7	Igniters not otherwise provided for	F23Q13/00	F23Q13/00		571
F23Q13/005	8	{using light, e.g. sunlight or laser}	F23Q13/00	F23Q13/00		104
F23Q13/02	8	using gas burners, e.g. gas pokers	F23Q13/02	F23Q13/02		227
F23Q13/04	8	using portable burners, e.g. torches, fire pots	F23Q13/04	F23Q13/04		241
F23Q21/00	7	Devices for effecting ignition from a remote location	F23Q21/00	F23Q21/00		503
F23Q23/00	7	Testing of ignition installations (peculiar to internal-combustion engines F02P17/00)	F23Q23/00	F23Q23/00		77
F23Q23/02	8	Testing of ignition timing	F23Q23/02	F23Q23/02		12
F23Q23/08	8	Testing of components (of sparking plugs H01T13/58, F02P17/12)	F23Q23/08	F23Q23/08		21
F23Q23/10	9	electrically	F23Q23/10	F23Q23/10		30
F23Q25/00	7	Extinguishing-devices, e.g. for blowing-out or snuffing candle flames (for cigarettes A24F)	F23Q25/00	F23Q25/00		990
