B01F21/00	7	Dissolving (separating by dissolving B01D; dissolving to effect cooling F25D5/00)	B01F21/00	B01F21/00		961
B01F21/02	8	{Methods}	B01F21/00	B01F21/02		473
B01F21/10	8	using driven stirrers	B01F21/10	B01F21/10		2055
B01F21/15	8	{comprising constructions for blocking or redispersing undissolved solids, e.g. sieves, separators or guiding constructions (B01F21/221 takes precedence)}	B01F21/00	B01F21/15		357
B01F21/20	8	using flow mixing	B01F21/20	B01F21/20		874
B01F21/22	9	{using additional holders in conduits, containers or pools for keeping the solid material in place, e.g. supports or receptacles}	B01F21/20	B01F21/22		722
B01F21/221	10	{comprising constructions for blocking or redispersing undissolved solids}	B01F21/20	B01F21/221		301
B01F21/30	8	{Workflow diagrams or layout of plants, e.g. flow charts; Details of workflow diagrams or layout of plants, e.g. controlling means}	B01F21/00	B01F21/30		588
B01F21/40	8	{characterised by the state of the material being dissolved}	B01F21/00	B01F21/40		25
B01F21/401	9	{Molten solids}	B01F21/00	B01F21/401		18
B01F21/402	9	{characterised by the configuration, form or shape of the solid material, e.g. in the form of tablets or blocks}	B01F21/00	B01F21/402		58
B01F21/4021	10	{in the form of tablets stored in containers, canisters or receptacles}	B01F21/00	B01F21/4021		63
B01F21/403	9	{Solid carbon dioxide or dry ice}	B01F21/00	B01F21/403		16
B01F21/50	8	{Elements used for separating or keeping undissolved material in the mixer}	B01F21/00	B01F21/50		12
B01F21/501	9	{Tablet canisters provided with perforated walls, sieves, grids or filters}	B01F21/00	B01F21/501		35
B01F21/502	9	{Baffles}	B01F21/00	B01F21/502		39
B01F21/503	9	{Filters}	B01F21/00	B01F21/503		168
B01F21/504	9	{Sieves, i.e. perforated plates or walls}	B01F21/00	B01F21/504		87
B01F23/00	7	Mixing according to the phases to be mixed, e.g. dispersing or emulsifying<br><br><u>NOTE</u><br><br>In this group, the following term is used with the meaning indicated:<br>"gases" covers also vapours.	B01F23/00	B01F23/00		303
B01F23/02	8	{Maintaining the aggregation state of the mixed materials}	B01F23/00	B01F23/02		11
B01F23/021	9	{Maintaining mixed ingredients in movement to prevent crystalisation of the ingredients after mixing}	B01F23/00	B01F23/021		4
B01F23/022	9	{Preventing precipitation of solid ingredients during or after mixing by adding a solvent}	B01F23/00	B01F23/022		12
B01F23/023	9	{Preventing sedimentation, conglomeration or agglomeration of solid ingredients during or after mixing by maintaining mixed ingredients in movement}	B01F23/00	B01F23/023		161
B01F23/024	9	{Maintaining mixed ingredients in movement to prevent separation of the ingredients after mixing}	B01F23/00	B01F23/024		33
B01F23/04	8	{Specific aggregation state of one or more of the phases to be mixed}	B01F23/00	B01F23/04		7
B01F23/041	9	{Mixing ingredients in more than two different agglomeration states, phases}	B01F23/00	B01F23/041		20
B01F23/042	9	{Mixing cryogenic aerosols, i.e. mixtures of gas with solid particles in cryogenic condition, with other ingredients}	B01F23/00	B01F23/042		7
B01F23/043	9	{Mixing fluids or with fluids in a supercritical state, in supercritical conditions or variable density fluids}	B01F23/00	B01F23/043		68
B01F23/06	8	{Mixing phases by adding a very small quantity of one of the phases or microdosing}	B01F23/00	B01F23/06		4
B01F23/061	9	{Adding a small quantity or concentration of an additional phase in a main phase, e.g. acting as a carrier phase}	B01F23/00	B01F23/061		29
B01F23/062	9	{Mixing ingredients in very small quantity, adding microingredients or microconcentration, e.g. adding vitamins, minerals, proteins, enzymes, hormones, antibiotics or worm medicines}	B01F23/00	B01F23/062		14
B01F23/09	8	{Mixing systems, i.e. flow charts or diagrams for components having more than two different of undetermined agglomeration states, e.g. supercritical states}	B01F23/00	B01F23/09		181
B01F23/10	8	Mixing gases with gases	B01F23/10	B01F23/10		1247
B01F23/12	9	{with vaporisation of a liquid (disinfection, sterilisation or deodorisation of air A61L9/00)}	B01F23/10	B01F23/12		335
B01F23/14	9	{with moving mixing elements, e.g. with liquid seal}	B01F23/10	B01F23/14		163
B01F23/19	9	{Mixing systems, i.e. flow charts or diagrams; Arrangements, e.g. comprising controlling means}	B01F23/10	B01F23/19		581
B01F23/191	10	{characterised by the construction of the controlling means}	B01F23/10	B01F23/191		336
B01F23/20	8	Mixing gases with liquids	B01F23/20	B01F23/20		1370
B01F23/21	9	by introducing liquids into gaseous media	B01F23/21	B01F23/21		402
B01F23/211	10	{Methods}	B01F23/21	B01F23/21		91
B01F23/213	10	by spraying or atomising of the liquids	B01F23/213	B01F23/213		249
B01F23/2131	11	{using rotating elements, e.g. rolls or brushes}	B01F23/213	B01F23/213		94
B01F23/21311	12	{for spraying the liquid radially by centrifugal force}	B01F23/213	B01F23/213		129
B01F23/21312	12	{with additional rotating elements mounted on the same axis, e.g. fans, for moving the gas}	B01F23/213	B01F23/213		51
B01F23/2132	11	{using nozzles}	B01F23/213	B01F23/213		1025
B01F23/21321	12	{High pressure atomization, i.e. the liquid is atomized and sprayed by a jet at high pressure}	B01F23/213	B01F23/213		80
B01F23/21322	12	{Internal mixer atomization, i.e. liquid and gas are mixed and atomized in a jet nozzle before spraying}	B01F23/213	B01F23/213		43
B01F23/2133	11	{using electric, sonic or ultrasonic energy}	B01F23/213	B01F23/213		125
B01F23/214	10	{using a gas-liquid mixing column or tower}	B01F23/21	B01F23/21		99
B01F23/215	10	{by forcing the gas through absorbent pads containing the liquid}	B01F23/21	B01F23/21		112
B01F23/216	10	{by using liquefied or cryogenic gases as liquid component}	B01F23/21	B01F23/21		10
B01F23/23	9	by introducing gases into liquid media, e.g. for producing aerated liquids	B01F23/23	B01F23/23		2000
B01F23/231	10	by bubbling (mixers with gas or liquid agitation, e.g. with air supply tubes B01F33/40)	B01F23/231	B01F23/231		705
B01F23/23105	11	{Arrangement or manipulation of the gas bubbling devices}	B01F23/231	B01F23/231		208
B01F23/2311	12	{Mounting the bubbling devices or the diffusers}	B01F23/231	B01F23/231		412
B01F23/23112	13	{comprising the use of flow guiding elements adjacent or above the gas stream}	B01F23/231	B01F23/231		8
B01F23/231121	14	{the flow guiding elements being baffles, tubes or walls}	B01F23/231	B01F23/231		88
B01F23/231122	14	{the flow guiding elements being dome-shaped elements, i.e. for trapping air, e.g. cap-, umbrella- or inversed cone-shaped}	B01F23/231	B01F23/231		30
B01F23/23113	13	{characterised by the disposition of the bubbling elements in particular configurations, patterns or arrays}	B01F23/231	B01F23/231		210
B01F23/23114	13	{characterised by the way in which the different elements of the bubbling installation are mounted}	B01F23/231	B01F23/231		20
B01F23/231141	14	{Mounting auxiliary devices, e.g. pumps or compressors in a particular place on the bubbling installation, e.g. under water}	B01F23/231	B01F23/231		69
B01F23/231142	14	{Mounting the gas transporting elements, i.e. connections between conduits}	B01F23/231	B01F23/231		141
B01F23/231143	14	{Mounting the bubbling elements or diffusors, e.g. on conduits, using connecting elements; Connections therefor}	B01F23/231	B01F23/231		189
B01F23/23115	13	{characterised by the way in which the bubbling devices are mounted within the receptacle}	B01F23/231	B01F23/231		24
B01F23/231151	14	{the bubbling devices being fixed or anchored in the bottom}	B01F23/231	B01F23/231		74
B01F23/231152	14	{the bubbling devices being supported, e.g. on cables or laying on the bottom}	B01F23/231	B01F23/231		45
B01F23/231153	14	{the bubbling devices being suspended on a supporting construction, i.e. not on a floating construction}	B01F23/231	B01F23/231		41
B01F23/231154	14	{the bubbling devices being provided with ballast to keep them floating under the surface, i.e. when the bubbling devices are lighter than the liquid}	B01F23/231	B01F23/231		50
B01F23/231155	14	{the bubbling devices floating and having a pendulum movement, going to and from or moving in alternating directions}	B01F23/231	B01F23/231		12
B01F23/231156	14	{the bubbling devices floating and having a rotating movement around a central vertical axis}	B01F23/231	B01F23/231		5
B01F23/23116	13	{Means for manipulating the bubbling constructions or elements, e.g. for raising or lowering them}	B01F23/231	B01F23/231		71
B01F23/2312	12	{Diffusers}	B01F23/231	B01F23/231		358
B01F23/23121	13	{having injection means, e.g. nozzles with circumferential outlet}	B01F23/231	B01F23/231		812
B01F23/23122	13	{having elements opening under air pressure, e.g. valves}	B01F23/231	B01F23/231		117
B01F23/23123	13	{consisting of rigid porous or perforated material}	B01F23/231	B01F23/231		816
B01F23/231231	14	{the outlets being in the form of perforations}	B01F23/231	B01F23/231		242
B01F23/231232	15	{in the form of slits or cut-out openings}	B01F23/231	B01F23/231		66
B01F23/231233	14	{comprising foam-like gas outlets}	B01F23/231	B01F23/231		27
B01F23/23124	13	{consisting of flexible porous or perforated material, e.g. fabric}	B01F23/231	B01F23/231		620
B01F23/231241	14	{the outlets being in the form of perforations}	B01F23/231	B01F23/231		68
B01F23/231242	15	{in the form of slits or cut-out openings}	B01F23/231	B01F23/231		67
B01F23/231243	14	{comprising foam-like gas outlets}	B01F23/231	B01F23/231		6
B01F23/231244	14	{Dissolving, hollow fiber membranes}	B01F23/231	B01F23/231		141
B01F23/231245	14	{Fabric in the form of woven, knitted, braided, non-woven or flocculated fibers or filaments}	B01F23/231	B01F23/231		68
B01F23/23125	13	{characterised by the way in which they are assembled or mounted; Fabricating the parts of the diffusers}	B01F23/231	B01F23/231		238
B01F23/23126	13	{characterised by the shape of the diffuser element}	B01F23/231	B01F23/231		31
B01F23/231261	14	{having a box- or block-shape, being in the form of aeration stones}	B01F23/231	B01F23/231		80
B01F23/231262	14	{having disc shape}	B01F23/231	B01F23/231		268
B01F23/231263	14	{having dome-, cap- or inversed cone-shape}	B01F23/231	B01F23/231		73
B01F23/231264	14	{being in the form of plates, flat beams, flat membranes or films}	B01F23/231	B01F23/231		178
B01F23/231265	14	{being tubes, tubular elements, cylindrical elements or set of tubes}	B01F23/231	B01F23/231		847
B01F23/231266	14	{being in the form of rings or annular elements}	B01F23/231	B01F23/231		72
B01F23/231267	14	{being axially stacked discs, rings or plates}	B01F23/231	B01F23/231		29
B01F23/231268	14	{being helically wound, coiled and joined bands or wires}	B01F23/231	B01F23/231		40
B01F23/231269	14	{being spirally wound, coiled tubes or spirally wound, coiled and joined bands or wires}	B01F23/231	B01F23/231		35
B01F23/23127	14	{Screens, nets, grades or grids}	B01F23/231	B01F23/231		43
B01F23/23128	13	{having specific properties or elements attached thereto}	B01F23/231	B01F23/231		21
B01F23/231281	14	{made of or comprising a biocide}	B01F23/231	B01F23/231		13
B01F23/231282	14	{made of or comprising a material able to store a gas which is released when water flows through it}	B01F23/231	B01F23/231		2
B01F23/231283	14	{having elements to protect the parts of the diffusers, e.g. from clogging when not in use}	B01F23/231	B01F23/231		24
B01F23/2319	10	{Methods of introducing gases into liquid media}	B01F23/23	B01F23/231		352
B01F23/232	10	using flow-mixing means for introducing the gases, e.g. baffles	B01F23/232	B01F23/232		1215
B01F23/2321	11	{by moving liquid and gas in counter current}	B01F23/232	B01F23/232		158
B01F23/23211	12	{the liquid flowing in a thin film to absorb the gas}	B01F23/232	B01F23/232		69
B01F23/232111	13	{the liquid film or layer flowing over a horizontal or inclined surface, e.g. perforated}	B01F23/232	B01F23/232		13
B01F23/232112	13	{the liquid film or layer flowing over a vertical surface, e.g. a mesh}	B01F23/232	B01F23/232		7
B01F23/2322	11	{using columns, e.g. multi-staged columns}	B01F23/232	B01F23/232		219
B01F23/2323	11	{by circulating the flow in guiding constructions or conduits}	B01F23/232	B01F23/232		731
B01F23/23231	12	{being at least partially immersed in the liquid, e.g. in a closed circuit}	B01F23/232	B01F23/232		322
B01F23/232311	13	{the conduits being vertical draft pipes with a lower intake end and an upper exit end}	B01F23/232	B01F23/232		331
B01F23/232312	13	{the guiding constructions being baffles for guiding the flow up-and-down or from left-to-right}	B01F23/232	B01F23/232		50
B01F23/2326	11	adding the flowing main component by suction means, e.g. using an ejector	B01F23/2326	B01F23/2326		377
B01F23/233	10	using driven stirrers with completely immersed stirring elements	B01F23/233	B01F23/233		700
B01F23/2331	11	{characterised by the introduction of the gas along the axis of the stirrer or along the stirrer elements}	B01F23/233	B01F23/233		1008
B01F23/23311	12	{through a hollow stirrer axis}	B01F23/233	B01F23/233		556
B01F23/23312	12	{through a conduit surrounding the stirrer axis}	B01F23/233	B01F23/233		156
B01F23/23313	12	{through a separate conduit substantially parallel with the stirrer axis}	B01F23/233	B01F23/233		84
B01F23/23314	12	{through a hollow stirrer element}	B01F23/233	B01F23/233		423
B01F23/23315	12	{through a hollow guide surrounding the stirrer element}	B01F23/233	B01F23/233		25
B01F23/23316	12	{through a separate hollow guide substantially parallel with the stirrer element}	B01F23/233	B01F23/233		12
B01F23/2332	11	{the stirrer rotating about a horizontal axis; Stirrers therefor}	B01F23/233	B01F23/233		233
B01F23/2333	11	{Single stirrer-drive aerating units, e.g. with the stirrer-head pivoting around an horizontal axis}	B01F23/233	B01F23/233		113
B01F23/2334	11	{provided with stationary guiding means surrounding at least partially the stirrer}	B01F23/233	B01F23/233		99
B01F23/23341	12	{with tubes surrounding the stirrer}	B01F23/233	B01F23/233		431
B01F23/23342	12	{the stirrer being of the centrifugal type, e.g. with a surrounding stator}	B01F23/233	B01F23/233		230
B01F23/2335	11	{characterised by the direction of introduction of the gas relative to the stirrer}	B01F23/233	B01F23/233		6
B01F23/23351	12	{the gas moving along the axis of rotation}	B01F23/233	B01F23/233		48
B01F23/23352	12	{the gas moving perpendicular to the axis of rotation}	B01F23/233	B01F23/233		92
B01F23/23353	12	{the gas being sucked towards the rotating stirrer}	B01F23/233	B01F23/233		129
B01F23/23354	12	{the gas being driven away from the rotating stirrer}	B01F23/233	B01F23/233		77
B01F23/2336	11	{characterised by the location of the place of introduction of the gas relative to the stirrer}	B01F23/233	B01F23/233		11
B01F23/23361	12	{the gas being introduced in a guide tube surrounding at least partially the axis of the stirrer}	B01F23/233	B01F23/233		12
B01F23/23362	12	{the gas being introduced under the stirrer}	B01F23/233	B01F23/233		310
B01F23/23363	12	{the gas being introduced above the stirrer}	B01F23/233	B01F23/233		187
B01F23/23364	12	{the gas being introduced between the stirrer elements}	B01F23/233	B01F23/233		89
B01F23/233641	13	{at the stirrer axis}	B01F23/233	B01F23/233		20
B01F23/233642	13	{at the stirrer elements}	B01F23/233	B01F23/233		38
B01F23/23365	12	{the gas being introduced at the radial periphery of the stirrer}	B01F23/233	B01F23/233		54
B01F23/23366	12	{the gas being introduced in front of the stirrer}	B01F23/233	B01F23/233		58
B01F23/23367	12	{the gas being introduced behind the stirrer}	B01F23/233	B01F23/233		60
B01F23/234	10	Surface aerating	B01F23/234	B01F23/234		469
B01F23/2341	11	{by cascading, spraying or projecting a liquid into a gaseous atmosphere (B01F23/2342 takes precedence)}	B01F23/234	B01F23/234		62
B01F23/23411	12	{by cascading the liquid}	B01F23/234	B01F23/234		124
B01F23/23412	12	{using liquid falling from orifices in a gaseous atmosphere, the orifices being exits from perforations, tubes or chimneys}	B01F23/234	B01F23/234		103
B01F23/23413	12	{using nozzles for projecting the liquid into the gas atmosphere}	B01F23/234	B01F23/234		243
B01F23/2342	11	{with stirrers near to the liquid surface, e.g. partially immersed, for spraying the liquid in the gas or for sucking gas into the liquid, e.g. using stirrers rotating around a horizontal axis or using centrifugal force}	B01F23/234	B01F23/234		245
B01F23/23421	12	{the stirrers rotating about a vertical axis}	B01F23/234	B01F23/234		366
B01F23/234211	13	{Stirrers thereof}	B01F23/234	B01F23/234		182
B01F23/235	10	for making foam	B01F23/235	B01F23/235		1040
B01F23/2351	11	{using driven stirrers}	B01F23/235	B01F23/235		286
B01F23/236	10	specially adapted for aerating or carbonating beverages	B01F23/236	B01F23/236		441
B01F23/2361	11	within small containers, e.g. within bottles	B01F23/2361	B01F23/2361		528
B01F23/23611	12	{Portable appliances comprising a gas cartridge}	B01F23/2361	B01F23/2361		317
B01F23/2362	11	{for aerating or carbonating within receptacles or tanks, e.g. distribution machines (B01F23/2361 takes precedence)}	B01F23/236	B01F23/236		1004
B01F23/2363	11	{Mixing systems, i.e. flow charts or diagrams; Arrangements, e.g. comprising controlling means}	B01F23/236	B01F23/236		475
B01F23/2364	11	{using security elements, e.g. valves, for relieving overpressure}	B01F23/236	B01F23/236		80
B01F23/2366	10	{Parts; Accessories}	B01F23/23	B01F23/236		367
B01F23/2368	11	{Mixing receptacles, e.g. tanks, vessels or reactors, being completely closed, e.g. hermetically closed}	B01F23/23	B01F23/236		417
B01F23/237	10	characterised by the physical or chemical properties of gases or vapours introduced in the liquid media	B01F23/237	B01F23/237		105
B01F23/2373	11	for obtaining fine bubbles, i.e. bubbles with a size below 100 &#181;m	B01F23/2373	B01F23/2373		880
B01F23/2375	12	for obtaining bubbles with a size below 1 &#181;m	B01F23/2375	B01F23/2375		398
B01F23/2376	11	{characterised by the gas being introduced}	B01F23/237	B01F23/237		69
B01F23/23761	12	{Aerating, i.e. introducing oxygen containing gas in liquids}	B01F23/237	B01F23/237		274
B01F23/237611	13	{Air}	B01F23/237	B01F23/237		494
B01F23/237612	13	{Oxygen}	B01F23/237	B01F23/237		648
B01F23/237613	13	{Ozone}	B01F23/237	B01F23/237		622
B01F23/23762	12	{Carbon dioxide}	B01F23/237	B01F23/237		347
B01F23/237621	13	{in beverages}	B01F23/237	B01F23/237		395
B01F23/23763	12	{Chlorine or chlorine containing gases}	B01F23/237	B01F23/237		50
B01F23/23764	12	{Hydrogen}	B01F23/237	B01F23/237		186
B01F23/23765	12	{Nitrogen}	B01F23/237	B01F23/237		126
B01F23/23766	12	{Sulphur containing gas}	B01F23/237	B01F23/237		12
B01F23/23767	12	{Introducing steam or damp in liquids}	B01F23/237	B01F23/237		53
B01F23/238	10	{using vibrations, electrical or magnetic energy, radiations}	B01F23/23	B01F23/23		257
B01F23/29	9	{Mixing systems, i.e. flow charts or diagrams}	B01F23/20	B01F23/29		506
B01F23/291	10	{for obtaining foams or aerosols}	B01F23/20	B01F23/291		231
B01F23/30	8	Mixing gases with solids	B01F23/30	B01F23/30		293
B01F23/32	9	{by introducing solids in gas volumes}	B01F23/30	B01F23/32		53
B01F23/34	9	{by introducing gases in solid materials, e.g. in masses of powder or particles}	B01F23/30	B01F23/34		58
B01F23/341	10	{by introducing steam, e.g. for wetting the solids}	B01F23/30	B01F23/341		18
B01F23/36	9	{by mixing in fluidised bed state}	B01F23/30	B01F23/36		12
B01F23/39	9	{Mixing systems, i.e. flow charts or diagrams}	B01F23/30	B01F23/39		37
B01F23/40	8	Mixing liquids with liquids; Emulsifying	B01F23/40	B01F23/40		1160
B01F23/405	9	{Methods of mixing liquids with liquids (B01F23/4105 takes precedence)}	B01F23/40	B01F23/40		677
B01F23/41	9	Emulsifying	B01F23/41	B01F23/41		2050
B01F23/4105	10	{Methods of emulsifying}	B01F23/41	B01F23/41		817
B01F23/411	10	using electrical or magnetic fields, heat or vibrations	B01F23/411	B01F23/411		180
B01F23/4111	11	{using vibrations}	B01F23/411	B01F23/411		251
B01F23/413	10	{Homogenising a raw emulsion or making monodisperse or fine emulsions}	B01F23/41	B01F23/41		114
B01F23/414	10	{characterised by the internal structure of the emulsion}	B01F23/41	B01F23/41		35
B01F23/4141	11	{High internal phase ratio [HIPR] emulsions, e.g. having high percentage of internal phase, e.g. higher than 60-90 % of water in oil [W/O]}	B01F23/41	B01F23/41		32
B01F23/4142	11	{Inversed-type emulsions}	B01F23/41	B01F23/41		23
B01F23/4143	11	{Microemulsions}	B01F23/41	B01F23/41		145
B01F23/4144	11	{Multiple emulsions, in particular double emulsions, e.g. water in oil in water; Three-phase emulsions}	B01F23/41	B01F23/41		99
B01F23/4145	11	{Emulsions of oils, e.g. fuel, and water}	B01F23/41	B01F23/41		269
B01F23/4146	11	{Emulsions including solid particles, e.g. as solution or dispersion, i.e. molten material or material dissolved in a solvent or dispersed in a liquid}	B01F23/41	B01F23/41		85
B01F23/43	9	using driven stirrers	B01F23/43	B01F23/43		1486
B01F23/431	10	{the liquids being introduced from the outside through or along the axis of a rotating stirrer, e.g. the stirrer rotating due to the reaction of the introduced liquid}	B01F23/43	B01F23/43		109
B01F23/45	9	using flow mixing	B01F23/45	B01F23/45		705
B01F23/451	10	by injecting one liquid into another	B01F23/451	B01F23/451		716
B01F23/452	10	{by uniting flows taken from different parts of a receptacle or silo; Sandglass-type mixing (for particulate material B01F25/80)}	B01F23/45	B01F23/45		87
B01F23/453	10	{by moving the liquids in countercurrent}	B01F23/45	B01F23/45		71
B01F23/454	10	by injecting a mixture of liquid and gas	B01F23/454	B01F23/454		662
B01F23/47	9	involving high-viscosity liquids, e.g. asphalt	B01F23/47	B01F23/47		714
B01F23/471	10	{using a very viscous liquid and a liquid of low viscosity}	B01F23/47	B01F23/47		112
B01F23/48	9	{characterised by the nature of the liquids (B01F23/47 takes precedence)}	B01F23/40	B01F23/48		81
B01F23/481	10	{using liquefied or cryogenic gases}	B01F23/40	B01F23/481		53
B01F23/482	10	{using molten solids}	B01F23/40	B01F23/482		38
B01F23/483	10	{using water for diluting a liquid ingredient, obtaining a predetermined concentration or making an aqueous solution of a concentrate}	B01F23/40	B01F23/483		329
B01F23/49	9	{Mixing systems, i.e. flow charts or diagrams}	B01F23/40	B01F23/49		1240
B01F23/50	8	Mixing liquids with solids (displacing one liquid by another in dispersions of solids in liquids B01D12/00)	B01F23/50	B01F23/50		1188
B01F23/51	9	{Methods thereof}	B01F23/50	B01F23/51		640
B01F23/511	10	{characterised by the composition of the liquids or solids}	B01F23/50	B01F23/511		530
B01F23/53	9	using driven stirrers	B01F23/53	B01F23/53		2168
B01F23/54	9	{wetting solids}	B01F23/50	B01F23/54		342
B01F23/55	9	{the mixture being submitted to electrical, sonic or similar energy}	B01F23/50	B01F23/55		65
B01F23/551	10	{using vibrations}	B01F23/50	B01F23/551		171
B01F23/56	9	{by introducing solids in liquids, e.g. dispersing or dissolving}	B01F23/50	B01F23/56		780
B01F23/565	9	{by introducing liquids in solid material, e.g. to obtain slurries}	B01F23/50	B01F23/565		490
B01F23/566	10	{by introducing liquids in a fluidised bed}	B01F23/50	B01F23/566		18
B01F23/57	9	Mixing high-viscosity liquids with solids	B01F23/57	B01F23/57		238
B01F23/58	9	{characterised by the nature of the liquid (B01F23/57 takes precedence)}	B01F23/50	B01F23/58		28
B01F23/581	10	{Mixing liquids with solids, slurries or sludge, for obtaining a diluted slurry}	B01F23/50	B01F23/581		80
B01F23/582	10	{Mixing foam with solids}	B01F23/50	B01F23/582		10
B01F23/59	9	{Mixing systems, i.e. flow charts or diagrams}	B01F23/50	B01F23/59		881
B01F23/60	8	Mixing solids with solids	B01F23/60	B01F23/60		1368
B01F23/62	9	using a receptacle with a bottom discharge with oscillating or vibrating opening and closing elements; using a receptacle with a bottom discharge with elements fitted on moving chains	B01F23/62	B01F23/62		48
B01F23/64	9	using rotatable mixing elements at the lower end of discharge hoppers	B01F23/64	B01F23/64		78
B01F23/66	9	{by evaporating or liquefying at least one of the components; using a fluid which is evaporated after mixing}	B01F23/60	B01F23/66		29
B01F23/69	9	{Mixing systems, i.e. flow charts or diagrams; Arrangements, e.g. comprising controlling means}	B01F23/60	B01F23/69		342
B01F23/70	8	Pre-treatment of the materials to be mixed	B01F23/70	B01F23/70		937
B01F23/701	9	{Coating solid materials}	B01F23/70	B01F23/70		3
B01F23/702	9	{Cooling materials}	B01F23/70	B01F23/70		61
B01F23/703	9	{Degassing or de-aerating materials; Replacing one gas within the materials by another gas}	B01F23/70	B01F23/70		87
B01F23/704	9	{Drying materials, e.g. in order to mix them in solid state}	B01F23/70	B01F23/70		144
B01F23/705	9	{Submitting materials to electrical energy fields to charge or ionize them}	B01F23/70	B01F23/70		24
B01F23/706	9	{Evaporating solvents or dispersion liquids, e.g. water, at least partially}	B01F23/70	B01F23/70		23
B01F23/707	9	{Extracting materials to be mixed from a stream of fluid or from a solid containing them, e.g. by adsorption, absorption or distillation}	B01F23/70	B01F23/70		16
B01F23/708	9	{Filtering materials}	B01F23/70	B01F23/70		814
B01F23/709	9	{Freezing materials, e.g. to mix them in solid state}	B01F23/70	B01F23/70		11
B01F23/71	9	{Grinding materials}	B01F23/70	B01F23/71		546
B01F23/711	9	{Heating materials, e.g. melting}	B01F23/70	B01F23/711		301
B01F23/712	9	{Irradiating materials}	B01F23/70	B01F23/712		22
B01F23/713	9	{Sieving materials}	B01F23/70	B01F23/713		735
B01F23/80	8	After-treatment of the mixture	B01F23/80	B01F23/80		591
B01F23/801	9	{Coating the solid mixture}	B01F23/80	B01F23/80		4
B01F23/802	9	{Cooling the mixture}	B01F23/80	B01F23/80		117
B01F23/803	9	{Venting, degassing or ventilating of gases, fumes or toxic vapours from the mixture}	B01F23/80	B01F23/80		114
B01F23/804	9	{Drying the mixture}	B01F23/80	B01F23/80		198
B01F23/805	9	{Submitting a mixture to electrical energy fields, e.g. corona discharge}	B01F23/80	B01F23/80		12
B01F23/806	9	{Evaporating a carrier, e.g. liquid carbon dioxide used to dissolve, disperse, emulsify or other components that are difficult to be mixed; Evaporating liquid components}	B01F23/80	B01F23/80		38
B01F23/807	9	{Extracting components from the mixture, e.g. by adsorption, absorption or distillation}	B01F23/80	B01F23/80		35
B01F23/808	9	{Filtering the mixture}	B01F23/80	B01F23/80		1076
B01F23/809	9	{Freezing the mixture}	B01F23/80	B01F23/80		16
B01F23/81	9	{Grinding the mixture}	B01F23/80	B01F23/81		96
B01F23/811	9	{Heating the mixture}	B01F23/80	B01F23/811		107
B01F23/812	9	{Irradiating the mixture}	B01F23/80	B01F23/812		18
B01F25/00	7	Flow mixers; Mixers for falling materials, e.g. solid particles (centrifugal mixers B04)	B01F25/00	B01F25/00		759
B01F25/10	8	Mixing by creating a vortex flow, e.g. by tangential introduction of flow components	B01F25/10	B01F25/10		1470
B01F25/101	9	{wherein the vortex flows in a spherical shaped receptacle or chamber}	B01F25/10	B01F25/10		54
B01F25/102	9	{wherein the vortex is created by two or more jets introduced tangentially in separate mixing chambers or consecutively in the same mixing chamber}	B01F25/10	B01F25/10		187
B01F25/103	9	{with additional mixing means other than vortex mixers, e.g. the vortex chamber being positioned in another mixing chamber}	B01F25/10	B01F25/10		303
B01F25/104	9	{characterised by the arrangement of the discharge opening}	B01F25/10	B01F25/10		189
B01F25/1041	10	{the mixing chamber being vertical with the outlet tube at its upper side}	B01F25/10	B01F25/10		61
B01F25/1042	10	{the mixing chamber being vertical and having an outlet tube at its bottom whose inlet is at a higher level than the inlet of the vortex creating jet, e.g. the jet being introduced at the bottom of the mixing chamber}	B01F25/10	B01F25/10		35
B01F25/105	8	{Mixing heads, i.e. compact mixing units or modules, using mixing valves for feeding and mixing at least two components}	B01F25/00	B01F25/10		305
B01F25/1051	9	{of the mixing valve type}	B01F25/00	B01F25/10		114
B01F25/12	8	{Interdigital mixers, i.e. the substances to be mixed are divided in sub-streams which are rearranged in an interdigital or interspersed manner (micromixers using interdigital streams B01F33/3012)}	B01F25/00	B01F25/12		78
B01F25/14	8	{Mixing drops, droplets or bodies of liquid which flow together or contact each other (micromixers using where the materials to be mixed are in the form of droplets B01F33/302)}	B01F25/00	B01F25/14		82
B01F25/20	8	Jet mixers, i.e. mixers using high-speed fluid streams (using jets to create vortex flow B01F25/10)	B01F25/20	B01F25/20		914
B01F25/21	9	with submerged injectors, e.g. nozzles, for injecting high-pressure jets into a large volume or into mixing chambers	B01F25/21	B01F25/21		751
B01F25/211	10	{the injectors being surrounded by guiding tubes}	B01F25/21	B01F25/21		299
B01F25/212	10	{the injectors being movable, e.g. rotating}	B01F25/21	B01F25/21		202
B01F25/2121	11	{Pivoting or oscillating in a multidirectional way during jetting}	B01F25/21	B01F25/21		22
B01F25/2122	11	{Rotating during jetting}	B01F25/21	B01F25/21		142
B01F25/2123	11	{being vertically moved to bring the injector in or out of operative position}	B01F25/21	B01F25/21		18
B01F25/2124	11	{being moved or transported between different locations during jetting}	B01F25/21	B01F25/21		26
B01F25/2125	11	{Moving to adjust the direction of jetting, the injectors being fixed during operation}	B01F25/21	B01F25/21		40
B01F25/23	9	Mixing by intersecting jets	B01F25/23	B01F25/23		656
B01F25/231	10	{the intersecting jets having the configuration of sheets, cylinders or cones}	B01F25/23	B01F25/23		64
B01F25/25	9	Mixing by jets impinging against collision plates	B01F25/25	B01F25/25		548
B01F25/27	9	Mixing by jetting components into a conduit for agitating its contents	B01F25/27	B01F25/27		174
B01F25/28	9	{characterised by the specific design of the jet injector}	B01F25/20	B01F25/28		115
B01F25/281	10	{the jet injector being of the explosive rapid expansion of supercritical solutions [RESS] or fluid injection of molecular spray [FIMS] type, i.e. the liquid is jetted in an environment (gas or liquid) by nozzles, in conditions of significant pressure drop, with the possible generation of shock waves}	B01F25/20	B01F25/281		17
B01F25/282	10	{the jet injector being of Coanda-type, i.e. having a surface to attract the jet for adjusting its direction}	B01F25/20	B01F25/282		13
B01F25/30	8	Injector mixers (mixing by creating vortex flow B01F25/10)	B01F25/30	B01F25/30		666
B01F25/305	9	{the additional component being axially fed and radially discharged through a circumferential outlet}	B01F25/30	B01F25/30		55
B01F25/31	9	in conduits or tubes through which the main component flows	B01F25/31	B01F25/31		584
B01F25/311	10	{for mixing more than two components; Devices specially adapted for generating foam}	B01F25/31	B01F25/31		289
B01F25/3111	11	{Devices specially adapted for generating foam, e.g. air foam}	B01F25/31	B01F25/31		246
B01F25/31112	12	{with additional mixing means other than injector mixers, e.g. screen or baffles (B01F25/31113 takes precedence)}	B01F25/31	B01F25/31		150
B01F25/31113	12	{with rotating elements, e.g. driven by one of the components for feeding or by the resulting mixture for additional mixing}	B01F25/31	B01F25/31		39
B01F25/31114	12	{with means for introducing an additional component, e.g. in predetermined proportion or in the main component}	B01F25/31	B01F25/31		51
B01F25/312	10	with Venturi elements; Details thereof	B01F25/312	B01F25/312		1611
B01F25/3121	11	{with additional mixing means other than injector mixers, e.g. screens, baffles or rotating elements}	B01F25/312	B01F25/312		658
B01F25/3122	11	{the material flowing at a supersonic velocity thereby creating shock waves}	B01F25/312	B01F25/312		65
B01F25/3123	11	{with two or more Venturi elements}	B01F25/312	B01F25/312		50
B01F25/31231	12	{used alternatively}	B01F25/312	B01F25/312		21
B01F25/31232	12	{used simultaneously}	B01F25/312	B01F25/312		157
B01F25/31233	12	{used successively}	B01F25/312	B01F25/312		138
B01F25/3124	11	{characterised by the place of introduction of the main flow}	B01F25/312	B01F25/312		10
B01F25/31241	12	{the main flow being injected in the circumferential area of the venturi, creating an aspiration in the central part of the conduit}	B01F25/312	B01F25/312		163
B01F25/31242	12	{the main flow being injected in the central area of the venturi, creating an aspiration in the circumferential part of the conduit (B01F25/31243 takes precedence)}	B01F25/312	B01F25/312		1008
B01F25/31243	12	{Eductor or eductor-type venturi, i.e. the main flow being injected through the venturi with high speed in the form of a jet}	B01F25/312	B01F25/312		518
B01F25/3125	11	{characteristics of the Venturi parts}	B01F25/312	B01F25/312		83
B01F25/31251	12	{Throats}	B01F25/312	B01F25/312		40
B01F25/312511	13	{Adjustable Venturi throat}	B01F25/312	B01F25/312		45
B01F25/312512	13	{Profiled, grooved, ribbed throat, or being provided with baffles}	B01F25/312	B01F25/312		54
B01F25/31252	12	{Nozzles}	B01F25/312	B01F25/312		64
B01F25/312521	13	{Adjustable Venturi nozzle}	B01F25/312	B01F25/312		49
B01F25/312522	13	{Profiled, grooved, ribbed nozzle, or being provided with baffles}	B01F25/312	B01F25/312		34
B01F25/31253	12	{Discharge}	B01F25/312	B01F25/312		5
B01F25/312531	13	{Adjustable discharge conduit or barrel, e.g. adjustable in width}	B01F25/312	B01F25/312		14
B01F25/312532	13	{Profiled, grooved, ribbed discharge conduit, or being provided with baffles}	B01F25/312	B01F25/312		38
B01F25/312533	13	{Constructional characteristics of the diverging discharge conduit or barrel, e.g. with zones of changing conicity}	B01F25/312	B01F25/312		73
B01F25/313	10	wherein additional components are introduced in the centre of the conduit	B01F25/313	B01F25/313		672
B01F25/3131	11	{with additional mixing means other than injector mixers, e.g. screens, baffles or rotating elements}	B01F25/313	B01F25/313		1030
B01F25/3132	11	{by using two or more injector devices}	B01F25/313	B01F25/313		253
B01F25/31321	12	{used alternatively}	B01F25/313	B01F25/313		
B01F25/31322	12	{used simultaneously}	B01F25/313	B01F25/313		193
B01F25/31323	12	{used successively}	B01F25/313	B01F25/313		48
B01F25/31324	12	{arranged concentrically}	B01F25/313	B01F25/313		49
B01F25/3133	11	{characterised by the specific design of the injector}	B01F25/313	B01F25/313		75
B01F25/31331	12	{Perforated, multi-opening, with a plurality of holes}	B01F25/313	B01F25/313		330
B01F25/313311	13	{Porous injectors}	B01F25/313	B01F25/313		119
B01F25/31332	12	{Ring, torus, toroidal or coiled configurations}	B01F25/313	B01F25/313		69
B01F25/31333	12	{Rotatable injectors}	B01F25/313	B01F25/313		22
B01F25/31334	12	{the opening for introducing the supplementary stream being a slit}	B01F25/313	B01F25/313		14
B01F25/314	10	wherein additional components are introduced at the circumference of the conduit	B01F25/314	B01F25/314		493
B01F25/3141	11	{with additional mixing means other than injector mixers}	B01F25/314	B01F25/314		721
B01F25/3142	11	{the conduit having a plurality of openings in the axial direction or in the circumferential direction}	B01F25/314	B01F25/314		372
B01F25/31421	12	{the conduit being porous}	B01F25/314	B01F25/314		205
B01F25/31422	12	{with a plurality of perforations in the axial direction only}	B01F25/314	B01F25/314		82
B01F25/31423	12	{with a plurality of perforations in the circumferential direction only and covering the whole circumference}	B01F25/314	B01F25/314		203
B01F25/314231	13	{the perforations being a complete cut-out in the circumferential direction covering the whole diameter of the tube, i.e. having two consecutive tubes placed consecutively, the additional component being introduced between them}	B01F25/314	B01F25/314		12
B01F25/31424	12	{with a plurality of perforations aligned in a row perpendicular to the flow direction}	B01F25/314	B01F25/314		37
B01F25/31425	12	{with a plurality of perforations in the axial and circumferential direction covering the whole surface}	B01F25/314	B01F25/314		158
B01F25/3143	11	{characterised by the specific design of the injector}	B01F25/314	B01F25/314		48
B01F25/31431	12	{being a slit extending in the longitudinal direction only}	B01F25/314	B01F25/314		4
B01F25/31432	12	{being a slit extending in the circumferential direction only}	B01F25/314	B01F25/314		50
B01F25/31433	12	{being rotatable, e.g. placed on a rotatable housing or conduit}	B01F25/314	B01F25/314		13
B01F25/31434	12	{being a bundle of similar tubes, each of them having feedings on the circumferential wall, e.g. as mixer for a reactor}	B01F25/314	B01F25/314		29
B01F25/315	10	wherein a difference of pressure at different points of the conduit causes introduction of the additional component into the main component (B01F25/316 takes precedence)	B01F25/315	B01F25/315		155
B01F25/316	10	with containers for additional components fixed to the conduit	B01F25/316	B01F25/316		661
B01F25/32	9	wherein the additional components are added in a by-pass of the main flow	B01F25/32	B01F25/32		217
B01F25/40	8	Static mixers (colloid-mills B02C; mixing valves F16K11/00)	B01F25/40	B01F25/40		726
B01F25/41	9	Mixers of the fractal type	B01F25/41	B01F25/41		132
B01F25/42	9	in which the mixing is affected by moving the components jointly in changing directions, e.g. in tubes provided with baffles or obstructions	B01F25/42	B01F25/42		668
B01F25/421	10	by moving the components in a convoluted or labyrinthine path (B01F25/433 takes precedence)	B01F25/421	B01F25/421		281
B01F25/422	11	between stacked plates, e.g. grooved or perforated plates	B01F25/422	B01F25/422		259
B01F25/423	11	{by means of elements placed in the receptacle for moving or guiding the components}	B01F25/421	B01F25/42		78
B01F25/4231	12	{using baffles}	B01F25/421	B01F25/42		322
B01F25/4232	12	{using dams}	B01F25/421	B01F25/42		15
B01F25/4233	12	{using plates with holes, the holes being displaced from one plate to the next one to force the flow to make a bending movement}	B01F25/421	B01F25/42		145
B01F25/43	10	Mixing tubes, e.g. wherein the material is moved in a radial or partly reversed direction	B01F25/43	B01F25/43		208
B01F25/431	11	Straight mixing tubes with baffles or obstructions that do not cause substantial pressure drop; Baffles therefor	B01F25/431	B01F25/431		596
B01F25/4311	12	{the baffles being adjustable}	B01F25/431	B01F25/431		103
B01F25/4312	12	{having different kinds of baffles, e.g. plates alternating with screens}	B01F25/431	B01F25/431		116
B01F25/4313	12	{comprising a plurality of stacked ducts having their axes parallel to the tube axis}	B01F25/431	B01F25/431		55
B01F25/4314	12	with helical baffles	B01F25/4314	B01F25/4314		491
B01F25/43141	13	{composed of consecutive sections of helical formed elements}	B01F25/4314	B01F25/4314		560
B01F25/4315	12	{the baffles being deformed flat pieces of material (B01F25/4314 takes precedence)}	B01F25/431	B01F25/431		349
B01F25/43151	13	{composed of consecutive sections of deformed flat pieces of material}	B01F25/431	B01F25/431		194
B01F25/4316	12	{the baffles being flat pieces of material, e.g. intermeshing, fixed to the wall or fixed on a central rod}	B01F25/431	B01F25/431		393
B01F25/43161	13	{composed of consecutive sections of flat pieces of material}	B01F25/431	B01F25/431		347
B01F25/43162	13	{Assembled flat elements}	B01F25/431	B01F25/431		40
B01F25/43163	13	{in the form of small flat plate-like elements}	B01F25/431	B01F25/431		55
B01F25/4317	12	{Profiled elements, e.g. profiled blades, bars, pillars, columns or chevrons}	B01F25/431	B01F25/431		222
B01F25/43171	13	{Profiled blades, wings, wedges, i.e. plate-like element having one side or part thicker than the other}	B01F25/431	B01F25/431		95
B01F25/43172	13	{Profiles, pillars, chevrons, i.e. long elements having a polygonal cross-section}	B01F25/431	B01F25/431		80
B01F25/4318	12	{Ring-shaped blades or strips}	B01F25/431	B01F25/431		20
B01F25/4319	12	{Tubular elements}	B01F25/431	B01F25/431		105
B01F25/43195	12	{Wires or coils}	B01F25/431	B01F25/431		49
B01F25/431951	13	{Spirally-shaped baffle}	B01F25/431	B01F25/431		27
B01F25/431952	14	{Conical or pyramidal elements}	B01F25/431	B01F25/431		40
B01F25/43197	12	{characterised by the mounting of the baffles or obstructions}	B01F25/431	B01F25/431		56
B01F25/431971	13	{Mounted on the wall}	B01F25/431	B01F25/431		430
B01F25/431972	13	{Mounted on an axial support member, e.g. a rod or bar}	B01F25/431	B01F25/431		219
B01F25/431973	13	{Mounted on a support member extending transversally through the mixing tube}	B01F25/431	B01F25/431		64
B01F25/431974	13	{Support members, e.g. tubular collars, with projecting baffles fitted inside the mixing tube or adjacent to the inner wall}	B01F25/431	B01F25/431		281
B01F25/432	11	with means for dividing the material flow into separate sub-flows and for repositioning and recombining these sub-flows; Cross-mixing, e.g. conducting the outer layer of the material nearer to the axis of the tube or vice-versa	B01F25/432	B01F25/432		318
B01F25/4321	12	{the subflows consisting of at least two flat layers which are recombined, e.g. using means having restriction or expansion zones}	B01F25/432	B01F25/432		199
B01F25/43211	13	{using a simple by-pass for separating and recombining the flow, e.g. by using branches of different length}	B01F25/432	B01F25/432		44
B01F25/4322	12	{essentially composed of stacks of sheets, e.g. corrugated sheets}	B01F25/432	B01F25/432		96
B01F25/4323	12	{using elements provided with a plurality of channels or using a plurality of tubes which can either be placed between common spaces or collectors}	B01F25/432	B01F25/432		300
B01F25/43231	13	{the channels or tubes crossing each other several times}	B01F25/432	B01F25/432		69
B01F25/433	11	Mixing tubes wherein the shape of the tube influences the mixing, e.g. mixing tubes with varying cross-section or provided with inwardly extending profiles	B01F25/433	B01F25/433		745
B01F25/4331	12	{Mixers with bended, curved, coiled, wounded mixing tubes or comprising elements for bending the flow}	B01F25/433	B01F25/433		670
B01F25/4332	12	{Mixers with a strong change of direction in the conduit for homogenizing the flow}	B01F25/433	B01F25/433		109
B01F25/4333	12	{Mixers with scallop-shaped tubes or surfaces facing each other}	B01F25/433	B01F25/433		35
B01F25/4334	12	{Mixers with a converging cross-section}	B01F25/433	B01F25/433		100
B01F25/4335	12	{Mixers with a converging-diverging cross-section}	B01F25/433	B01F25/433		253
B01F25/4336	12	{Mixers with a diverging cross-section}	B01F25/433	B01F25/433		107
B01F25/4337	12	{Mixers with a diverging-converging cross-section}	B01F25/433	B01F25/433		93
B01F25/4338	12	{Mixers with a succession of converging-diverging cross-sections, i.e. undulating cross-section}	B01F25/433	B01F25/433		225
B01F25/434	11	Mixing tubes comprising cylindrical or conical inserts provided with grooves or protrusions	B01F25/434	B01F25/434		201
B01F25/4341	12	{the insert being provided with helical grooves}	B01F25/434	B01F25/434		44
B01F25/4342	12	{the insert being provided with a labyrinth of grooves or a distribution of protrusions}	B01F25/434	B01F25/434		22
B01F25/435	11	Mixing tubes composed of concentric tubular members	B01F25/435	B01F25/435		144
B01F25/438	9	{with movable slits formed between reciprocating surfaces}	B01F25/40	B01F25/43		35
B01F25/44	9	Mixers in which the components are pressed through slits	B01F25/44	B01F25/44		91
B01F25/441	10	characterised by the configuration of the surfaces forming the slits	B01F25/441	B01F25/441		43
B01F25/4412	11	{the slits being formed between opposed planar surfaces, e.g. pushed again each other by springs}	B01F25/441	B01F25/441		208
B01F25/44121	12	{with a plurality of parallel slits, e.g. formed between stacked plates}	B01F25/441	B01F25/441		47
B01F25/4413	11	{the slits being formed between opposed conical or cylindrical surfaces}	B01F25/441	B01F25/441		216
B01F25/4414	11	{the slits being formed between the balls and the seats of a bearing-like construction}	B01F25/441	B01F25/441		36
B01F25/4415	11	{the slits being formed between the helical windings of a spring-like construction or by deforming a spring}	B01F25/441	B01F25/441		31
B01F25/4416	11	{the opposed surfaces being provided with grooves}	B01F25/441	B01F25/441		6
B01F25/44161	12	{Axial grooves formed on opposed surfaces, e.g. on cylinders or cones}	B01F25/441	B01F25/441		21
B01F25/44162	12	{Circumferential grooves formed on opposed surfaces, e.g. on planar surfaces or on cylinders or cones}	B01F25/441	B01F25/441		25
B01F25/44163	12	{Helical grooves formed on opposed surfaces, e.g. on cylinders or cones}	B01F25/441	B01F25/441		44
B01F25/44164	12	{Crossing sets of grooves forming a labyrinth formed on opposed surfaces, e.g. on planar surfaces or on cylinders or cones}	B01F25/441	B01F25/441		14
B01F25/44165	12	{Radial grooves formed on opposed surfaces, e.g. on planar surfaces}	B01F25/441	B01F25/441		7
B01F25/44166	12	{Spiral grooves formed on opposed surfaces, e.g. on planar surfaces}	B01F25/441	B01F25/441		3
B01F25/44167	12	{the grooves being formed on the outer surface of the cylindrical or conical core of the slits}	B01F25/441	B01F25/441		48
B01F25/44168	12	{the grooves being formed on the inner surface of the cylindrical or conical housing of the slits}	B01F25/441	B01F25/441		16
B01F25/442	10	characterised by the relative position of the surfaces during operation	B01F25/442	B01F25/442		4
B01F25/4421	11	{the surfaces being maintained in a fixed position, spaced from each other, therefore maintaining the slit always open}	B01F25/442	B01F25/442		47
B01F25/4422	11	{the surfaces being maintained in a fixed but adjustable position, spaced from each other, therefore allowing the slit spacing to be varied (B01F25/4423 takes precedence)}	B01F25/442	B01F25/442		146
B01F25/4423	11	{the surfaces being part of a valve construction, formed by opposed members in contact, e.g. automatic positioning caused by spring pressure}	B01F25/442	B01F25/442		143
B01F25/45	9	Mixers in which the materials to be mixed are pressed together through orifices or interstitial spaces, e.g. between beads (B01F25/44 takes precedence)	B01F25/45	B01F25/45		637
B01F25/451	10	characterised by means for moving the materials to be mixed or the mixture	B01F25/451	B01F25/451		139
B01F25/4511	11	{with a rotor surrounded by a stator provided with orifices}	B01F25/451	B01F25/451		48
B01F25/4512	11	{with reciprocating pistons}	B01F25/451	B01F25/451		162
B01F25/452	10	characterised by elements provided with orifices or interstitial spaces	B01F25/452	B01F25/452		100
B01F25/4521	11	{the components being pressed through orifices in elements, e.g. flat plates or cylinders, which obstruct the whole diameter of the tube}	B01F25/452	B01F25/452		629
B01F25/45211	12	{the elements being cylinders or cones which obstruct the whole diameter of the tube, the flow changing from axial in radial and again in axial}	B01F25/452	B01F25/452		217
B01F25/45212	12	{the elements comprising means for adjusting the orifices}	B01F25/452	B01F25/452		34
B01F25/4522	11	{the components being pressed through porous bodies, e.g. flat plates, blocks or cylinders, which obstruct the whole diameter of the tube (B01F25/45243 takes precedence)}	B01F25/452	B01F25/452		137
B01F25/45221	12	{the porous bodies being cylinders or cones which obstruct the whole diameter of the tube, the flow changing from axial in radial and again in axial}	B01F25/452	B01F25/452		28
B01F25/4523	11	{the components being pressed through sieves, screens or meshes which obstruct the whole diameter of the tube}	B01F25/452	B01F25/452		271
B01F25/45231	12	{the sieves, screens or meshes being cylinders or cones which obstruct the whole diameter of the tube, the flow changing from axial in radial and again in axial}	B01F25/452	B01F25/452		63
B01F25/4524	11	{the components being pressed through foam-like inserts or through a bed of loose bodies, e.g. balls}	B01F25/452	B01F25/452		96
B01F25/45241	12	{through a bed of balls}	B01F25/452	B01F25/452		169
B01F25/45242	12	{through a bed of fibres, steel wool or wood chips}	B01F25/452	B01F25/452		57
B01F25/45243	12	{through a foam or expanded material body}	B01F25/452	B01F25/452		25
B01F25/46	9	Homogenising or emulsifying nozzles	B01F25/46	B01F25/46		140
B01F25/50	8	Circulation mixers, e.g. wherein at least part of the mixture is discharged from and reintroduced into a receptacle	B01F25/50	B01F25/50		1773
B01F25/51	9	in which the mixture is circulated through a set of tubes, e.g. with gradual introduction of a component into the circulating flow	B01F25/51	B01F25/51		682
B01F25/52	9	with a rotary stirrer in the recirculation tube	B01F25/52	B01F25/52		660
B01F25/53	9	in which the mixture is discharged from and reintroduced into a receptacle through a recirculation tube, into which an additional component is introduced	B01F25/53	B01F25/53		744
B01F25/54	9	provided with a pump inside the receptacle to recirculate the material within the receptacle	B01F25/54	B01F25/54		209
B01F25/60	8	Pump mixers, i.e. mixing within a pump	B01F25/60	B01F25/60		503
B01F25/62	9	of the gear type	B01F25/62	B01F25/62		160
B01F25/621	10	{Wankel pump}	B01F25/62	B01F25/62		3
B01F25/64	9	of the centrifugal-pump type, i.e. turbo-mixers	B01F25/64	B01F25/64		310
B01F25/641	10	{Multi-staged turbo-mixers}	B01F25/64	B01F25/64		48
B01F25/642	10	{consisting of a stator-rotor system with intermeshing teeth or cages}	B01F25/64	B01F25/64		54
B01F25/643	10	{with axial access to the mixing device at both its sides}	B01F25/64	B01F25/64		19
B01F25/70	8	Spray-mixers, e.g. for mixing intersecting sheets of material	B01F25/70	B01F25/70		98
B01F25/72	9	with nozzles	B01F25/72	B01F25/72		479
B01F25/721	10	for spraying a fluid on falling particles or on a liquid curtain	B01F25/721	B01F25/721		319
B01F25/74	9	with rotating parts, e.g. discs	B01F25/74	B01F25/74		178
B01F25/741	10	{with a disc or a set of discs mounted on a shaft rotating about a vertical axis, on top of which the material to be thrown outwardly is fed}	B01F25/74	B01F25/74		90
B01F25/7411	11	{with repeated action, i.e. the material thrown outwardly being guided, by means provided on the surrounding casing or on top of the next lower disc}	B01F25/74	B01F25/74		63
B01F25/742	10	{for spraying a liquid on falling particles or on a liquid curtain (B01F25/7411 takes precedence)}	B01F25/74	B01F25/74		50
B01F25/743	10	{the material being fed on both sides of a part rotating about a vertical axis}	B01F25/74	B01F25/74		43
B01F25/744	10	{the rotating part being composed of at least two cooperating members rotating independently about the same vertical axis}	B01F25/74	B01F25/74		24
B01F25/80	8	Falling particle mixers, e.g. with repeated agitation along a vertical axis	B01F25/80	B01F25/80		135
B01F25/82	9	uniting flows of material taken from different parts of a receptacle or from a set of different receptacles	B01F25/82	B01F25/82		79
B01F25/821	10	{by means of conduits having inlet openings at different levels}	B01F25/82	B01F25/82		76
B01F25/8211	11	{by means of a central conduit or central set of conduits}	B01F25/82	B01F25/82		53
B01F25/822	10	{the receptacle being divided into compartments for receiving or storing the different components}	B01F25/82	B01F25/82		57
B01F25/823	10	{Flow collectors therefor}	B01F25/82	B01F25/82		26
B01F25/83	9	with receptacles provided with fixed guiding elements therein, e.g. baffles; Cross-mixers comprising crossing channels for guiding the falling particles	B01F25/83	B01F25/83		185
B01F25/84	9	{Falling-particle mixers comprising superimposed receptacles, the material flowing from one to the other, e.g. of the sandglass type}	B01F25/80	B01F25/84		83
B01F25/85	9	wherein the particles fall onto a film that flows along the inner wall of a mixer	B01F25/85	B01F25/85		107
B01F25/90	9	with moving or vibrating means, e.g. stirrers, for enhancing the mixing	B01F25/90	B01F25/90		128
B01F25/901	10	{using one central conveyor or several separate conveyors, e.g. belt, screw conveyors or vibrating tables, for discharging flows from receptacles, e.g. in layers}	B01F25/90	B01F25/90		65
B01F2025/91	8	{Direction of flow or arrangement of feed and discharge openings}	B01F25/00	B01F2025/91		264
B01F2025/911	9	{Axial flow}	B01F25/00	B01F2025/911		237
B01F2025/912	9	{Radial flow}	B01F25/00	B01F2025/912		394
B01F2025/9121	10	{from the center to the circumference, i.e. centrifugal flow}	B01F25/00	B01F2025/9121		72
B01F2025/9122	10	{from the circumference to the center}	B01F25/00	B01F2025/9122		29
B01F2025/913	9	{Vortex flow, i.e. flow spiraling in a tangential direction and moving in an axial direction}	B01F25/00	B01F2025/913		356
B01F2025/914	9	{Tangential flow, i.e. flow spiraling in a tangential direction in a flat plane or belt-like area}	B01F25/00	B01F2025/914		103
B01F2025/915	9	{Reverse flow, i.e. flow changing substantially 180&#176; in direction}	B01F25/00	B01F2025/915		121
B01F2025/916	9	{Turbulent flow, i.e. every point of the flow moves in a random direction and intermixes}	B01F25/00	B01F2025/916		168
B01F2025/917	9	{Laminar or parallel flow, i.e. every point of the flow moves in layers which do not intermix}	B01F25/00	B01F2025/917		32
B01F2025/9171	10	{Parallel flow, i.e. every point of the flow moves in parallel layers where intermixing can occur by diffusion or which do not intermix; Focusing, i.e. compressing parallel layers without intermixing them}	B01F25/00	B01F2025/9171		33
B01F2025/918	9	{Counter current flow, i.e. flows moving in opposite direction and colliding}	B01F25/00	B01F2025/918		196
B01F2025/919	9	{characterised by the disposition of the feed and discharge openings}	B01F25/00	B01F2025/919		31
B01F2025/9191	10	{characterised by the arrangement of the feed openings for one or more flows, e.g. for the mainflow and the flow of an additional component}	B01F25/00	B01F2025/9191		118
B01F2025/91911	11	{with feed openings in the center of the main flow}	B01F25/00	B01F2025/91911		30
B01F2025/91912	11	{with feed openings at the circumference of the main flow}	B01F25/00	B01F2025/91912		22
B01F2025/919121	12	{with feed openings around the complete circumference of the main flow, e.g. being a perforated or porous part}	B01F25/00	B01F2025/919121		13
B01F2025/919125	11	{with feed openings in the center and at the circumference of the main flow}	B01F25/00	B01F2025/919125		36
B01F2025/91913	11	{with feed openings facing each other, e.g. for creating counter flows, for creating a series of vortex flows}	B01F25/00	B01F2025/91913		17
B01F2025/93	8	{Arrangements, nature or configuration of flow guiding elements}	B01F25/00	B01F2025/93		72
B01F2025/931	9	{Flow guiding elements surrounding feed openings, e.g. jet nozzles}	B01F25/00	B01F2025/931		290
B01F2025/932	9	{Nature of the flow guiding elements}	B01F25/00	B01F2025/932		21
B01F2025/9321	10	{Surface characteristics, e.g. coated or rough}	B01F25/00	B01F2025/9321		33
B01F27/00	7	Mixers with rotary stirring devices in fixed receptacles (magnetic mixers B01F33/45); Kneaders	B01F27/00	B01F27/00		1163
B01F27/05	8	Stirrers	B01F27/05	B01F27/05		514
B01F27/051	9	characterised by their elements, materials or mechanical properties	B01F27/051	B01F27/051		255
B01F27/052	10	Stirrers with replaceable wearing elements; Wearing elements therefor	B01F27/052	B01F27/052		220
B01F27/053	10	characterised by their materials	B01F27/053	B01F27/053		368
B01F27/0531	11	{with particular surface characteristics, e.g. coated or rough}	B01F27/053	B01F27/053		219
B01F27/054	10	Deformable stirrers, e.g. deformed by a centrifugal force applied during operation	B01F27/054	B01F27/054		546
B01F27/0541	11	{with mechanical means to alter the position of the stirring elements}	B01F27/054	B01F27/054		767
B01F27/0542	11	{deformable by centrifugal force}	B01F27/054	B01F27/054		421
B01F27/0543	11	{the position of the stirring elements depending on the direction of rotation of the stirrer}	B01F27/054	B01F27/054		85
B01F27/06	10	{Stirrers made by deforming a plate}	B01F27/051	B01F27/06		16
B01F27/07	9	characterised by their mounting on the shaft	B01F27/07	B01F27/07		239
B01F27/071	10	{Fixing of the stirrer to the shaft}	B01F27/07	B01F27/07		841
B01F27/072	10	characterised by the disposition of the stirrers with respect to the rotating axis	B01F27/072	B01F27/072		119
B01F27/0721	11	{parallel with respect to the rotating axis}	B01F27/072	B01F27/072		272
B01F27/0722	11	{perpendicular with respect to the rotating axis}	B01F27/072	B01F27/072		716
B01F27/0723	11	{oblique with respect to the rotating axis}	B01F27/072	B01F27/072		370
B01F27/0724	11	{directly mounted on the rotating axis}	B01F27/072	B01F27/072		598
B01F27/0725	11	{on the free end of the rotating axis}	B01F27/072	B01F27/072		361
B01F27/0726	11	{having stirring elements connected to the stirrer shaft each by a single radial rod, other than open frameworks}	B01F27/072	B01F27/072		465
B01F27/07261	12	{of the anchor type, i.e. the stirring elements being connected to the rods by one end and extending parallel to the shaft axis}	B01F27/072	B01F27/072		88
B01F27/0727	11	{having stirring elements connected to the stirrer shaft each by two or more radial rods, e.g. the shaft being interrupted between the rods, or of crankshaft type}	B01F27/072	B01F27/072		224
B01F27/073	10	{with stirring elements moving with respect to the stirrer shaft, e.g. floating or comprising contracting chambers}	B01F27/07	B01F27/07		275
B01F27/074	10	{having two or more mixing elements being concentrically mounted on the same shaft}	B01F27/07	B01F27/07		1869
B01F27/09	9	characterised by the mounting of the stirrers with respect to the receptacle	B01F27/09	B01F27/09		126
B01F27/091	10	with elements co-operating with receptacle wall or bottom, e.g. for scraping the receptacle wall	B01F27/091	B01F27/091		2000
B01F27/092	10	{occupying substantially the whole interior space of the receptacle}	B01F27/09	B01F27/09		690
B01F27/093	10	eccentrically arranged	B01F27/093	B01F27/093		72
B01F27/11	9	characterised by the configuration of the stirrers	B01F27/11	B01F27/11		571
B01F27/111	10	Centrifugal stirrers, i.e. stirrers with radial outlets; Stirrers of the turbine type, e.g. with means to guide the flow	B01F27/111	B01F27/111		418
B01F27/1111	11	with a flat disc or with a disc-like element equipped with blades, e.g. Rushton turbine	B01F27/1111	B01F27/1111		74
B01F27/112	10	with arms, paddles, vanes or blades	B01F27/112	B01F27/112		2897
B01F27/1121	11	pin-shaped	B01F27/1121	B01F27/1121		269
B01F27/1122	11	anchor-shaped	B01F27/1122	B01F27/1122		196
B01F27/1123	11	sickle-shaped, i.e. curved in at least one direction	B01F27/1123	B01F27/1123		616
B01F27/1124	11	rake-shaped or grid-shaped	B01F27/1124	B01F27/1124		131
B01F27/1125	11	with vanes or blades extending parallel or oblique to the stirrer axis	B01F27/1125	B01F27/1125		1170
B01F27/11251	12	{having holes in the surface}	B01F27/1125	B01F27/1125		998
B01F27/11252	12	{paddle wheels}	B01F27/1125	B01F27/1125		103
B01F27/11253	12	{the blades extending oblique to the stirrer axis}	B01F27/1125	B01F27/1125		104
B01F27/1126	11	the stirrer being a bent rod supported at one end only	B01F27/1126	B01F27/1126		107
B01F27/1127	11	spoon-shaped	B01F27/1127	B01F27/1127		35
B01F27/113	10	Propeller-shaped stirrers for producing an axial flow, e.g. shaped like a ship or aircraft propeller	B01F27/113	B01F27/113		943
B01F27/1131	11	with holes in the propeller blade surface	B01F27/1131	B01F27/1131		90
B01F27/1132	11	with guiding tubes or tubular segments fixed to and surrounding the tips of the propeller blades, e.g. for supplementary mixing	B01F27/1132	B01F27/1132		90
B01F27/1133	11	{the impeller being of airfoil or aerofoil type}	B01F27/113	B01F27/113		37
B01F27/1134	11	{the impeller being of hydrofoil type}	B01F27/113	B01F27/113		30
B01F27/114	10	Helically shaped stirrers, i.e. stirrers comprising a helically shaped band or helically shaped band sections	B01F27/114	B01F27/114		843
B01F27/1141	11	{having holes in the surface}	B01F27/114	B01F27/114		90
B01F27/1142	11	of the corkscrew type	B01F27/1142	B01F27/1142		193
B01F27/1143	11	screw-shaped, e.g. worms	B01F27/1143	B01F27/1143		811
B01F27/1144	11	with a plurality of blades following a helical path on a shaft or a blade support	B01F27/1144	B01F27/1144		262
B01F27/1145	11	ribbon shaped with an open space between the helical ribbon flight and the rotating axis	B01F27/1145	B01F27/1145		331
B01F27/11451	12	{forming open frameworks or cages}	B01F27/1145	B01F27/1145		116
B01F27/115	10	comprising discs or disc-like elements essentially perpendicular to the stirrer shaft axis	B01F27/115	B01F27/115		454
B01F27/1151	11	with holes on the surface	B01F27/1151	B01F27/1151		232
B01F27/1152	11	with separate elements other than discs fixed on the discs, e.g. vanes fixed on the discs	B01F27/1152	B01F27/1152		424
B01F27/1153	11	{the discs being made by deforming flat discs}	B01F27/115	B01F27/115		107
B01F27/1154	11	{the discs being cup shaped, e.g. semi sphere}	B01F27/115	B01F27/115		42
B01F27/1155	11	{with interconnected discs, forming open frameworks or cages}	B01F27/115	B01F27/115		79
B01F27/116	10	Stirrers shaped as cylinders, balls or rollers	B01F27/116	B01F27/116		238
B01F27/1161	11	{having holes in the surface}	B01F27/116	B01F27/116		98
B01F27/1162	11	{Balls}	B01F27/116	B01F27/116		86
B01F27/1163	11	{Rollers}	B01F27/116	B01F27/116		44
B01F27/11631	12	{comprising paddles fixed thereon, e.g. with a total a diameter close to that of the surrounding receptacle}	B01F27/116	B01F27/116		33
B01F27/117	10	Stirrers provided with conical-shaped elements, e.g. funnel-shaped	B01F27/117	B01F27/117		136
B01F27/1171	11	{having holes in the surface}	B01F27/117	B01F27/117		36
B01F27/118	10	Stirrers in the form of brushes, sieves, grids, chains or springs	B01F27/118	B01F27/118		534
B01F27/119	10	Stirrers with rigid wires or flexible rods	B01F27/119	B01F27/119		73
B01F27/1191	11	{with a bent rod of non-helical configuration supported at one end}	B01F27/119	B01F27/119		26
B01F27/13	10	Openwork frame or cage stirrers not provided for in other groups of this subclass	B01F27/13	B01F27/13		636
B01F27/15	10	Stirrers with tubes for guiding the material	B01F27/15	B01F27/15		476
B01F27/17	10	Stirrers with additional elements mounted on the stirrer, for purposes other than mixing	B01F27/17	B01F27/17		535
B01F27/171	11	for disintegrating, e.g. for milling	B01F27/171	B01F27/171		596
B01F27/172	11	for cutting, e.g. with knives	B01F27/172	B01F27/172		437
B01F27/19	10	Stirrers with two or more mixing elements mounted in sequence on the same axis	B01F27/19	B01F27/19		279
B01F27/191	11	with similar elements	B01F27/191	B01F27/191		7128
B01F27/192	11	with dissimilar elements	B01F27/192	B01F27/192		2695
B01F27/1921	12	{comprising helical elements and paddles}	B01F27/192	B01F27/192		1005
B01F27/21	8	characterised by their rotating shafts	B01F27/21	B01F27/21		70
B01F27/211	9	characterised by the material of the shaft	B01F27/211	B01F27/211		73
B01F27/2111	10	Flexible shafts	B01F27/2111	B01F27/2111		24
B01F27/212	9	{Construction of the shaft (B01F27/2121, B01F27/2122, B01F27/2123, B01F27/2124 take precedence)}	B01F27/21	B01F27/21		256
B01F27/2121	9	composed of interconnected parts	B01F27/2121	B01F27/2121		228
B01F27/2122	9	Hollow shafts	B01F27/2122	B01F27/2122		833
B01F27/2123	9	Shafts with both stirring means and feeding or discharging means	B01F27/2123	B01F27/2123		623
B01F27/2124	9	Shafts with adjustable length, e.g. telescopic shafts	B01F27/2124	B01F27/2124		180
B01F27/213	9	characterised by the connection with the drive	B01F27/213	B01F27/213		1041
B01F27/23	8	characterised by the orientation or disposition of the rotor axis	B01F27/23	B01F27/23		165
B01F27/231	9	with a variable orientation during mixing operation, e.g. with tiltable rotor axis	B01F27/231	B01F27/231		115
B01F27/2311	10	{the orientation of the rotating shaft being adjustable in the interior of the receptacle, e.g. by tilting the stirrer shaft during the mixing}	B01F27/231	B01F27/231		131
B01F27/2312	10	{the position of the rotating shaft being adjustable in the interior of the receptacle, e.g. to locate the stirrer in different locations during the mixing}	B01F27/231	B01F27/231		572
B01F27/232	9	with two or more rotation axes	B01F27/232	B01F27/232		341
B01F27/2321	10	{having different inclinations, e.g. non parallel}	B01F27/232	B01F27/232		341
B01F27/2322	10	with parallel axes	B01F27/2322	B01F27/2322		2539
B01F27/2323	10	with perpendicular axes	B01F27/2323	B01F27/2323		481
B01F27/2324	10	{planetary}	B01F27/232	B01F27/232		724
B01F27/25	8	Mixers with both stirrer and drive unit submerged in the material being mixed	B01F27/25	B01F27/25		427
B01F27/251	9	{Vertical beam constructions therefor}	B01F27/25	B01F27/25		141
B01F27/27	8	Mixers with stator-rotor systems, e.g. with intermeshing teeth or cylinders or having orifices (the stirrers having a central axial inflow and a substantially radial outflow B01F27/81)	B01F27/27	B01F27/27		220
B01F27/271	9	with means for moving the materials to be mixed radially between the surfaces of the rotor and the stator	B01F27/271	B01F27/271		439
B01F27/2711	10	{provided with intermeshing elements}	B01F27/271	B01F27/271		519
B01F27/2712	10	{provided with ribs, ridges or grooves on one surface}	B01F27/271	B01F27/271		184
B01F27/2713	10	{the surfaces having a conical shape}	B01F27/271	B01F27/271		70
B01F27/2714	10	{the relative position of the stator and the rotor, gap in between or gap with the walls being adjustable}	B01F27/271	B01F27/271		139
B01F27/272	9	with means for moving the materials to be mixed axially between the surfaces of the rotor and the stator, e.g. the stator rotor system formed by conical or cylindrical surfaces	B01F27/272	B01F27/272		347
B01F27/2721	10	{provided with intermeshing elements}	B01F27/272	B01F27/272		154
B01F27/2722	10	{provided with ribs, ridges or grooves on one surface}	B01F27/272	B01F27/272		385
B01F27/2723	10	{the surfaces having a conical shape}	B01F27/272	B01F27/272		166
B01F27/2724	10	{the relative position of the stator and the rotor, gap in between or gap with the walls being adjustable}	B01F27/272	B01F27/272		102
B01F27/276	9	{the mixer being composed of a stator-rotor system being formed by bearing elements, e.g. roller bearings}	B01F27/27	B01F27/27		50
B01F27/40	8	Mixers with rotor-rotor system, e.g. with intermeshing teeth	B01F27/40	B01F27/40		86
B01F27/41	9	with the mutually rotating surfaces facing each other	B01F27/41	B01F27/41		62
B01F27/411	10	{provided with intermeshing elements}	B01F27/41	B01F27/41		65
B01F27/412	10	{provided with ribs, ridges or grooves on one surface}	B01F27/41	B01F27/41		16
B01F27/42	9	with rotating surfaces next to each other, i.e. on substantially parallel axes	B01F27/42	B01F27/42		49
B01F27/421	10	{provided with intermeshing elements}	B01F27/42	B01F27/42		67
B01F27/422	10	{provided with ribs, ridges or grooves on one surface}	B01F27/42	B01F27/42		5
B01F27/50	8	Pipe mixers, i.e. mixers wherein the materials to be mixed flow continuously through pipes, e.g. column mixers	B01F27/50	B01F27/50		594
B01F27/55	8	with stirrers driven by the moving material	B01F27/55	B01F27/55		421
B01F27/60	8	with stirrers rotating about a horizontal or inclined axis	B01F27/60	B01F27/60		1952
B01F27/61	9	about an inclined axis	B01F27/61	B01F27/61		765
B01F27/62	9	{comprising liquid feeding, e.g. spraying means}	B01F27/60	B01F27/62		331
B01F27/621	10	{the liquid being fed through the shaft of the stirrer}	B01F27/60	B01F27/621		87
B01F27/625	9	{the receptacle being divided into compartments, e.g. with porous divisions}	B01F27/60	B01F27/625		159
B01F27/627	9	{the receptacles being tiltable, e.g. for emptying}	B01F27/60	B01F27/627		107
B01F27/63	9	co-operating with deflectors or baffles fixed to the receptacle	B01F27/63	B01F27/63		25
B01F27/65	9	with buckets	B01F27/65	B01F27/65		62
B01F27/70	9	with paddles, blades or arms	B01F27/70	B01F27/70		5445
B01F27/701	10	comprising two or more shafts, e.g. in consecutive mixing chambers	B01F27/701	B01F27/701		409
B01F27/702	11	with intermeshing paddles	B01F27/702	B01F27/702		610
B01F27/703	11	with stirrers rotating at different speeds	B01F27/703	B01F27/703		145
B01F27/704	11	with stirrers facing each other, i.e. supported by opposite walls of the receptacle	B01F27/704	B01F27/704		142
B01F27/705	11	with stirrers rotating in opposite directions about the same axis, e.g. with a first stirrer surrounded by a tube inside a second stirrer	B01F27/705	B01F27/705		55
B01F27/706	11	with all the shafts in the same receptacle (B01F27/702-B01F27/705 take precedence)	B01F27/706	B01F27/706		1059
B01F27/707	10	the paddles co-operating, e.g. intermeshing, with elements on the receptacle wall	B01F27/707	B01F27/707		277
B01F27/708	10	characterised by the shape of the stirrer as a whole, i.e. of Z- or S-shape	B01F27/708	B01F27/708		108
B01F27/71	9	with propellers	B01F27/71	B01F27/71		413
B01F27/711	10	{co-operating with stationary guiding means, e.g. baffles}	B01F27/71	B01F27/71		43
B01F27/7111	11	{the guiding means being tubes surrounding the propellers}	B01F27/71	B01F27/71		38
B01F27/72	9	with helices or sections of helices	B01F27/72	B01F27/72		1719
B01F27/721	10	with two or more helices in the same receptacle	B01F27/721	B01F27/721		573
B01F27/722	11	the helices closely surrounded by a casing	B01F27/722	B01F27/722		156
B01F27/7221	12	{the stirrers being composed of helices and paddles on the same shaft, e.g. helically arranged ovally shaped paddles}	B01F27/722	B01F27/722		62
B01F27/723	11	the helices intermeshing to knead the mixture	B01F27/723	B01F27/723		171
B01F27/724	10	with a single helix closely surrounded by a casing	B01F27/724	B01F27/724		283
B01F27/725	10	{with two or more helices in respective separate casings, e.g. one casing inside the other}	B01F27/72	B01F27/72		75
B01F27/726	10	with two helices with opposite pitch on the same shaft; with two helices on the same axis, driven in opposite directions or at different speeds	B01F27/726	B01F27/726		354
B01F27/73	9	with rotary discs	B01F27/73	B01F27/73		271
B01F27/731	10	{with two or more parallel shafts provided with perpendicularly mounted discs, e.g. lens shaped, one against the other on each shaft and in circumferential contact with the discs on the other shafts, e.g. for cleaning}	B01F27/73	B01F27/73		72
B01F27/74	9	with rotary cylinders	B01F27/74	B01F27/74		136
B01F27/75	9	with stirrers having planetary motion, i.e. rotating about their own axis and about a sun axis	B01F27/75	B01F27/75		294
B01F27/755	10	{the stirrers being cylinders, balls or gears}	B01F27/75	B01F27/75		44
B01F27/80	8	with stirrers rotating about a substantially vertical axis	B01F27/80	B01F27/80		4445
B01F27/805	9	wherein the stirrers or the receptacles are moved in order to bring them into operative position; Means for fixing the receptacle	B01F27/805	B01F27/805		819
B01F27/806	10	with vertical displacement of the stirrer, e.g. in combination with means for pivoting the stirrer about a vertical axis in order to co-operate with different receptacles	B01F27/806	B01F27/806		1917
B01F27/807	10	with the stirrer-head pivoting about a horizontal axis to bring it in and out of operative position, e.g. with receptacles pivoting about a horizontal axis for emptying	B01F27/807	B01F27/807		163
B01F27/808	9	with stirrers driven from the bottom of the receptacle	B01F27/808	B01F27/808		2990
B01F27/81	9	the stirrers having central axial inflow and substantially radial outflow	B01F27/81	B01F27/81		283
B01F27/811	10	{with the inflow from one side only, e.g. stirrers placed on the bottom of the receptacle, or used as a bottom discharge pump}	B01F27/81	B01F27/81		171
B01F27/8111	11	{the stirrers co-operating with stationary guiding elements, e.g. surrounding stators or intermeshing stators (B01F27/812 takes precedence)}	B01F27/81	B01F27/81		234
B01F27/812	10	{the stirrers co-operating with surrounding stators, or with intermeshing stators, e.g. comprising slits, orifices or screens}	B01F27/81	B01F27/81		268
B01F27/813	10	{the stirrers co-operating with stationary guiding elements (B01F27/812 takes precedence)}	B01F27/81	B01F27/81		49
B01F27/82	9	Pan-type mixers, i.e. mixers in which the stirring elements move along the bottom of a pan-shaped receptacle (with stirring elements moving along the wall or bottom of the receptacle B01F27/091)	B01F27/82	B01F27/82		383
B01F27/83	9	the stirrers being additionally moved radially, or oscillating about an axis perpendicular to the stirrer axis	B01F27/83	B01F27/83		434
B01F27/84	9	with two or more stirrers rotating at different speeds or in opposite directions about the same axis	B01F27/84	B01F27/84		1079
B01F27/85	9	with two or more stirrers on separate shafts	B01F27/85	B01F27/85		2883
B01F27/851	10	{the receptacle being subdivided in adjacent compartments}	B01F27/85	B01F27/85		121
B01F27/86	9	co-operating with deflectors or baffles fixed to the receptacle	B01F27/86	B01F27/86		584
B01F27/861	10	{the baffles being of cylindrical shape, e.g. a mixing chamber surrounding the stirrer, the baffle being displaced axially to form an interior mixing chamber}	B01F27/86	B01F27/86		199
B01F27/862	10	{the baffles being adjustable or movable (B01F27/861 takes precedence)}	B01F27/86	B01F27/86		113
B01F27/87	9	the receptacle being divided into superimposed compartments	B01F27/87	B01F27/87		267
B01F27/88	9	with a separate receptacle-stirrer unit that is adapted to be coupled to a drive mechanism	B01F27/88	B01F27/88		773
B01F27/90	9	with paddles or arms&#160;	B01F27/90	B01F27/90		21122
B01F27/902	10	cooperating with intermeshing elements fixed on the receptacle walls	B01F27/902	B01F27/902		244
B01F27/9021	11	{the elements being vertically arranged, e.g. fixed on the bottom}	B01F27/902	B01F27/902		128
B01F27/906	10	with fixed axis	B01F27/906	B01F27/906		1471
B01F27/91	9	with propellers	B01F27/91	B01F27/91		1514
B01F27/911	10	{forcing the material through orifices or slits, e.g. in a stationary part}	B01F27/91	B01F27/91		59
B01F27/92	9	with helices or screws	B01F27/92	B01F27/92		2227
B01F27/921	10	with helices centrally mounted in the receptacle	B01F27/921	B01F27/921		470
B01F27/9211	11	{the helices being surrounded by a guiding tube}	B01F27/921	B01F27/921		287
B01F27/92112	12	{combined with means for uniting flows of material taken from different parts of the receptacle}	B01F27/921	B01F27/921		27
B01F27/9212	11	with conical helices	B01F27/9212	B01F27/9212		238
B01F27/9213	11	{the helices having a diameter only slightly less than the diameter of the receptacle}	B01F27/921	B01F27/921		96
B01F27/9214	11	{with additional mixing elements other than helices; having inner and outer helices; with helices surrounding a guiding tube}	B01F27/921	B01F27/921		205
B01F27/922	10	with two or more helices, e.g. with intermeshing helices	B01F27/922	B01F27/922		664
B01F27/923	10	{the material flowing continuously through the receptacle}	B01F27/92	B01F27/92		70
B01F27/93	9	with rotary discs	B01F27/93	B01F27/93		1315
B01F27/94	9	with rotary cylinders or cones	B01F27/94	B01F27/94		191
B01F27/941	10	{being hollow, perforated or having special stirring elements thereon}	B01F27/94	B01F27/94		244
B01F27/95	9	with stirrers having planetary motion, i.e. rotating about their own axis and about a sun axis	B01F27/95	B01F27/95		1789
B01F27/951	10	{with at least one stirrer mounted on the sun axis}	B01F27/95	B01F27/95		1044
B01F27/952	10	the stirrers being cylinders with their circumference in contact with the bottom of the receptacle and rotating about an axis at an angle to the sun axis, e.g. mixers of the Muller type	B01F27/952	B01F27/952		36
B01F27/953	10	{using only helical stirrers}	B01F27/95	B01F27/95		387
B01F27/96	9	with openwork frames or cages	B01F27/96	B01F27/96		1291
B01F29/00	7	Mixers with rotating receptacles	B01F29/00	B01F29/00		192
B01F29/10	8	with receptacles rotated about two different axes, e.g. receptacles having planetary motion	B01F29/10	B01F29/10		551
B01F29/15	8	Use of centrifuges for mixing	B01F29/15	B01F29/15		186
B01F29/20	8	with receptacles rotating about an axis at an angle to their longitudinal axis (B01F29/62 takes precedence)	B01F29/20	B01F29/20		211
B01F29/25	8	with material flowing continuously through the receptacles from inlet to discharge	B01F29/25	B01F29/25		224
B01F29/251	9	{with at least one screw inside the receptacle for feeding or discharging, e.g. the axis of screw and receptacle being parallel}	B01F29/25	B01F29/25		47
B01F29/252	9	{the feed and discharge openings being at opposite ends of the receptacle}	B01F29/25	B01F29/25		68
B01F29/253	9	{the feed and discharge openings being at the same side of the receptacle}	B01F29/25	B01F29/25		12
B01F29/30	8	Mixing the contents of individual packages or containers, e.g. by rotating tins or bottles	B01F29/30	B01F29/30		197
B01F29/31	9	the containers being supported by driving means, e.g. by rotating rollers	B01F29/31	B01F29/31		266
B01F29/32	9	Containers specially adapted for coupling to rotating frames or the like; Coupling means therefor	B01F29/32	B01F29/32		163
B01F29/321	10	of test-tubes or the like	B01F29/321	B01F29/321		231
B01F29/322	10	of two or more containers supported for simultaneous mixing, e.g. for bottles in crates	B01F29/322	B01F29/322		219
B01F29/33	9	by imparting a combination of movements to two or more containers	B01F29/33	B01F29/33		51
B01F29/331	10	{by means of a rotary table provided with a plurality of bottle grippers at its periphery, an additional movement being imparted to the grippers}	B01F29/33	B01F29/33		64
B01F29/332	10	{the bottles being submitted to a screw-motion about an axis perpendicular to the axis of the bottles and lying intermediate the ends of the bottles}	B01F29/33	B01F29/33		8
B01F29/333	10	{essentially by rotating bottles about an axis perpendicular to the bottle axis and lying outside the bottles, using a rotating drum provided with pockets for the bottles at its periphery}	B01F29/33	B01F29/33		31
B01F29/34	9	Constructional details of holders for the individual packages or containers	B01F29/34	B01F29/34		195
B01F29/40	8	{Parts or components, e.g. receptacles, feeding or discharging means (B01F29/251 takes precedence)}	B01F29/00	B01F29/40		408
B01F29/401	9	{Receptacles, e.g. provided with liners}	B01F29/00	B01F29/401		193
B01F29/4011	10	{characterised by the shape or cross-section of the receptacle, e.g. of Y-, Z -, S -, or X shape}	B01F29/00	B01F29/4011		154
B01F29/40111	11	{Non-cylindrical sections, e.g. elliptical or irregular}	B01F29/00	B01F29/40111		34
B01F29/40112	11	{Polygonal sections, e.g. triangularor square}	B01F29/00	B01F29/40112		49
B01F29/40113	11	{Conical, double-conicalor diabolo shapes}	B01F29/00	B01F29/40113		96
B01F29/40114	11	{Cubic, cubical or polyhedronical shapes}	B01F29/00	B01F29/40114		17
B01F29/40115	11	{S shapes}	B01F29/00	B01F29/40115		6
B01F29/40116	11	{Spherical shapes}	B01F29/00	B01F29/40116		19
B01F29/40117	11	{Toroidal shapes}	B01F29/00	B01F29/40117		106
B01F29/40118	11	{V or W shapes}	B01F29/00	B01F29/40118		75
B01F29/40119	11	{X shapes}	B01F29/00	B01F29/40119		7
B01F29/401195	11	{Y or double Y shapes}	B01F29/00	B01F29/401195		20
B01F29/402	10	{characterised by the relative disposition or configuration of the interior of the receptacles}	B01F29/00	B01F29/402		135
B01F29/4021	11	{Multi-compartment receptacles}	B01F29/00	B01F29/4021		128
B01F29/4022	11	{Configuration of the interior}	B01F29/00	B01F29/4022		79
B01F29/40221	12	{provided with baffles, plates or bars on the wall or the bottom}	B01F29/00	B01F29/40221		192
B01F29/40222	12	{provided with guide tubes on the wall or the bottom}	B01F29/00	B01F29/40222		13
B01F29/4023	11	{Nature of the receptacle}	B01F29/00	B01F29/4023		22
B01F29/40231	10	{Surface characteristics, e.g. coated, rough}	B01F29/00	B01F29/40231		24
B01F29/403	9	{Disposition of the rotor axis}	B01F29/00	B01F29/403		13
B01F29/4031	10	{horizontal}	B01F29/00	B01F29/4031		217
B01F29/4032	10	{vertical}	B01F29/00	B01F29/4032		449
B01F29/4033	10	{inclined}	B01F29/00	B01F29/4033		298
B01F29/4034	10	{variable, e.g. tiltable during the operation}	B01F29/00	B01F29/4034		73
B01F29/4035	10	{with a receptacle rotating around two or more axes}	B01F29/00	B01F29/4035		11
B01F29/40351	11	{having different, non-perpendicular inclinations, e.g. skew axes}	B01F29/00	B01F29/40351		24
B01F29/40352	11	{being parallel axes}	B01F29/00	B01F29/40352		6
B01F29/40353	11	{being perpendicular axes}	B01F29/00	B01F29/40353		109
B01F29/40354	11	{arranged for planetary motion}	B01F29/00	B01F29/40354		44
B01F29/4036	10	{with a plurality of rotating receptacles}	B01F29/00	B01F29/4036		14
B01F29/40361	11	{having axes of different, non-perpendicular inclinations}	B01F29/00	B01F29/40361		18
B01F29/40362	11	{having parallel axes}	B01F29/00	B01F29/40362		19
B01F29/40363	11	{having perpendicular axes}	B01F29/00	B01F29/40363		39
B01F29/40364	11	{being concentrically arranged}	B01F29/00	B01F29/40364		14
B01F29/40365	11	{arranged for planetary motion}	B01F29/00	B01F29/40365		33
B01F29/60	8	rotating about a horizontal or inclined axis, e.g. drum mixers	B01F29/60	B01F29/60		631
B01F29/61	9	{comprising liquid spraying devices}	B01F29/60	B01F29/61		116
B01F29/62	9	without bars, i.e. without mixing elements; characterised by the shape or cross section of the receptacle, e.g. of Y-, Z-, S- or X- shape; with cylindrical receptacles rotating about an axis at an angle to their longitudinal axis	B01F29/62	B01F29/62		514
B01F29/63	9	with fixed bars, i.e. stationary, or fixed on the receptacle	B01F29/63	B01F29/63		906
B01F29/64	9	with stirring devices moving in relation to the receptacle, e.g. rotating	B01F29/64	B01F29/64		1266
B01F29/80	8	rotating about a substantially vertical axis	B01F29/80	B01F29/80		542
B01F29/81	9	with stationary mixing elements	B01F29/81	B01F29/81		333
B01F29/82	9	{the receptacle comprising a rotary part, e.g. the bottom, and a stationary part, e.g. the wall, with optional use of a stirrer; the receptacle comprising parts moving in opposite directions}	B01F29/80	B01F29/82		288
B01F29/83	9	with rotary paddles or arms, e.g. movable out of the receptacle	B01F29/83	B01F29/83		1294
B01F29/835	10	{Pan-type mixers, i.e. having stirrers moving along the bottom of a pan-shaped receptacle}	B01F29/83	B01F29/83		36
B01F29/84	9	with propellers	B01F29/84	B01F29/84		28
B01F29/85	9	with helices, e.g. rotating about an inclined axis	B01F29/85	B01F29/85		152
B01F29/86	9	with rotary discs	B01F29/86	B01F29/86		56
B01F29/87	9	with rotary cylinders	B01F29/87	B01F29/87		69
B01F29/90	8	with stirrers having planetary motion	B01F29/90	B01F29/90		133
B01F31/00	7	Mixers with shaking, oscillating, or vibrating mechanisms	B01F31/00	B01F31/00		1576
B01F31/10	8	with a mixing receptacle rotating alternately in opposite directions	B01F31/10	B01F31/10		425
B01F31/20	8	Mixing the contents of independent containers, e.g. test tubes	B01F31/20	B01F31/20		873
B01F31/201	9	{Holders therefor}	B01F31/20	B01F31/20		980
B01F31/202	9	{for beverage bottles, e.g. within crates or with feeding means for the bottles}	B01F31/20	B01F31/20		42
B01F31/22	9	with supporting means moving in a horizontal plane, e.g. describing an orbital path for moving the containers about an axis which intersects the receptacle axis at an angle	B01F31/22	B01F31/22		412
B01F31/23	9	by pivoting the containers about an axis	B01F31/23	B01F31/23		392
B01F31/231	10	{the containers being of the sandglass-type or being linked with their openings}	B01F31/23	B01F31/23		10
B01F31/24	9	the containers being submitted to a rectilinear movement	B01F31/24	B01F31/24		480
B01F31/25	9	the containers being submitted to a combination of movements other than within a horizontal plane, e.g. rectilinear and pivoting movement (with a receptacle submitted to a combination of movements, i.e. at least one movement being vibratory or oscillatory B01F31/50)	B01F31/25	B01F31/25		342
B01F31/26	9	{the containers being submitted to a wobbling movement}	B01F31/20	B01F31/26		373
B01F31/265	9	{the vibrations being caused by an unbalanced rotating member}	B01F31/20	B01F31/265		135
B01F31/27	9	{the vibrations being caused by electromagnets}	B01F31/20	B01F31/27		94
B01F31/275	9	{with means for transporting test tubes to and from the stirring device}	B01F31/20	B01F31/275		86
B01F31/28	9	{the vibrations being caused by piezoelectric elements}	B01F31/20	B01F31/28		18
B01F31/29	8	Mixing by periodically deforming flexible tubular members through which the material is flowing	B01F31/29	B01F31/29		108
B01F31/30	8	comprising a receptacle to only a part of which the shaking, oscillating, or vibrating movement is imparted	B01F31/30	B01F31/30		13
B01F31/31	9	using receptacles with deformable parts, e.g. membranes, to which a motion is imparted	B01F31/31	B01F31/31		129
B01F31/311	10	{the motion being a linear movement to one part of the receptacle}	B01F31/31	B01F31/31		22
B01F31/312	10	{the motion being a transversal movement to one part of the receptacle, e.g. by moving alternatively up and down the opposite edges of a closing lid to cause a pumping action}	B01F31/31	B01F31/31		27
B01F31/40	8	with an axially oscillating rotary stirrer	B01F31/40	B01F31/40		1965
B01F31/401	9	{for material flowing continuously axially therethrough}	B01F31/40	B01F31/40		54
B01F31/42	8	with pendulum stirrers, i.e. with stirrers suspended so as to oscillate about fixed points or axes	B01F31/42	B01F31/42		214
B01F31/44	8	with stirrers performing an oscillatory, vibratory or shaking movement (B01F31/40, B01F31/42 take precedence)	B01F31/44	B01F31/44		774
B01F31/441	9	performing a rectilinear reciprocating movement	B01F31/441	B01F31/441		2557
B01F31/443	9	{performing a superposed additional movement other than oscillation, vibration or shaking}	B01F31/44	B01F31/44		1105
B01F31/445	9	performing an oscillatory movement about an axis	B01F31/445	B01F31/445		720
B01F31/449	9	{Stirrers constructions}	B01F31/44	B01F31/44		840
B01F31/46	8	with an annular vibrating trough	B01F31/46	B01F31/46		30
B01F31/50	8	with a receptacle submitted to a combination of movements, i.e. at least one vibratory or oscillatory movement	B01F31/50	B01F31/50		474
B01F31/55	8	the materials to be mixed being contained in a flexible bag submitted to periodical deformation	B01F31/55	B01F31/55		356
B01F31/56	8	{having a vibrating receptacle provided with stirring elements, e.g. independent stirring elements}	B01F31/00	B01F31/56		994
B01F31/57	8	{for material continuously moving therethrough (B01F31/29, B01F31/30, B01F31/401, B01F31/46, B01F31/84 take precedence)}	B01F31/00	B01F31/57		123
B01F31/60	8	with a vibrating receptacle (B01F31/10, B01F31/20, B01F31/50 take precedence)	B01F31/60	B01F31/60		597
B01F31/65	8	the materials to be mixed being directly submitted to a pulsating movement, e.g. by means of an oscillating piston or air column	B01F31/65	B01F31/65		412
B01F31/651	9	{Mixing by successively aspirating a part of the mixture in a conduit, e.g. a piston, and reinjecting it through the same conduit into the receptacle}	B01F31/65	B01F31/65		141
B01F31/70	8	{Drives therefor, e.g. crank mechanisms}	B01F31/00	B01F31/70		1238
B01F31/80	8	Mixing by means of high-frequency vibrations above one kHz, e.g. ultrasonic vibrations	B01F31/80	B01F31/80		778
B01F31/81	9	by vibrations generated inside a mixing device not coming from an external drive, e.g. by the flow of material causing a knife to vibrate or by vibrating nozzles	B01F31/81	B01F31/81		190
B01F31/82	9	{the material being forced through a narrow vibrating slit}	B01F31/80	B01F31/82		65
B01F31/83	9	{comprising a supplementary stirring element}	B01F31/80	B01F31/83		271
B01F31/831	10	{the vibrations being generated by the rotation of the stirring element}	B01F31/80	B01F31/831		134
B01F31/84	9	{for material continuously moving through a tube, e.g. by deforming the tube}	B01F31/80	B01F31/84		128
B01F31/841	10	{with a vibrating element inside the tube}	B01F31/80	B01F31/841		92
B01F31/85	9	with a vibrating element inside the receptacle	B01F31/85	B01F31/85		493
B01F31/86	9	with vibration of the receptacle or part of it	B01F31/86	B01F31/86		405
B01F31/861	10	{caused by hitting or striking the receptacle}	B01F31/86	B01F31/86		26
B01F31/87	9	transmitting the vibratory energy by means of a fluid, e.g. by means of air shock waves	B01F31/87	B01F31/87		171
B01F31/89	9	{Methodical aspects; Controlling}	B01F31/80	B01F31/89		114
B01F33/00	7	Other mixers; Mixing plants; Combinations of mixers	B01F33/00	B01F33/00		641
B01F33/05	8	Mixers using radiation, e.g. magnetic fields or microwaves to mix the material ({B01F23/2133, B01F23/238, B01F23/55,}B01F33/3031, B01F33/3032 take precedence)	B01F33/05	B01F33/05		249
B01F33/051	9	{the energy being electrical energy working on the ingredients or compositions for mixing them}	B01F33/05	B01F33/05		39
B01F33/052	9	{the energy being electric fields for electrostatically charging of the ingredients or compositions for mixing them}	B01F33/05	B01F33/05		53
B01F33/053	9	{the energy being magnetic or electromagnetic energy, radiation working on the ingredients or compositions for or during mixing them}	B01F33/05	B01F33/05		130
B01F33/054	9	{the energy being in the form of a laser to modify the characteristics or conditions of the products, e.g. for heating}	B01F33/05	B01F33/05		13
B01F33/055	9	{the energy being particle radiation working on the ingredients or compositions for or during mixing them}	B01F33/05	B01F33/05		21
B01F33/12	8	Mixers in which the mixing of the components is achieved by natural convection	B01F33/12	B01F33/12		32
B01F33/25	8	Mixers with loose mixing elements, e.g. loose balls in a receptacle	B01F33/25	B01F33/25		205
B01F33/251	9	{using balls as loose mixing element}	B01F33/25	B01F33/25		296
B01F33/252	9	{using bubbles as loose mixing element}	B01F33/25	B01F33/25		13
B01F33/253	9	{using sliders or cylindrical elements as loose mixing element}	B01F33/25	B01F33/25		33
B01F33/254	9	{using springs as loose mixing element}	B01F33/25	B01F33/25		33
B01F33/26	8	{Mixers with an endless belt for transport of the material, e.g. in layers or with mixing means above or at the end of the belt}	B01F33/00	B01F33/26		221
B01F33/27	8	{Mixers having moving endless chains or belts, e.g. provided with paddles, as mixing elements}	B01F33/00	B01F33/27		153
B01F33/30	8	Micromixers	B01F33/30	B01F33/30		1821
B01F33/301	9	using specific means for arranging the streams to be mixed, e.g. channel geometries or dispositions	B01F33/301	B01F33/301		219
B01F33/3011	10	using a sheathing stream of a fluid surrounding a central stream of a different fluid, e.g. for reducing the cross-section of the central stream or to produce droplets from the central stream	B01F33/3011	B01F33/3011		312
B01F33/3012	10	Interdigital streams, e.g. lamellae	B01F33/3012	B01F33/3012		129
B01F33/30121	11	{the interdigital streams being concentric lamellae}	B01F33/3012	B01F33/3012		17
B01F33/3017	10	{Mixing chamber}	B01F33/301	B01F33/301		172
B01F33/302	9	the materials to be mixed flowing in the form of droplets	B01F33/302	B01F33/302		38
B01F33/3021	10	{the components to be mixed being combined in a single independent droplet, e.g. these droplets being divided by a non-miscible fluid or consisting of independent droplets}	B01F33/302	B01F33/302		325
B01F33/3022	10	{the components being formed by independent droplets which are alternated, the mixing of the components being achieved by diffusion between droplets}	B01F33/302	B01F33/302		31
B01F33/3031	9	using electro-hydrodynamic [EHD] or electro-kinetic [EKI] phenomena to mix or move the fluids	B01F33/3031	B01F33/3031		253
B01F33/3032	9	using magneto-hydrodynamic [MHD] phenomena to mix or move the fluids	B01F33/3032	B01F33/3032		67
B01F33/3033	9	using heat to mix or move the fluids	B01F33/3033	B01F33/3033		66
B01F33/3034	9	{using induced convection or movement in the mixture to mix or move the fluids without mechanical means, e.g. thermodynamic instability, strong gradients, etc.}	B01F33/30	B01F33/30		24
B01F33/3035	9	{using surface tension to mix, move or hold the fluids}	B01F33/30	B01F33/30		27
B01F33/30351	10	{using hydrophilic/hydrophobic surfaces}	B01F33/30	B01F33/30		78
B01F33/30352	10	{using roughness of the surfaces}	B01F33/30	B01F33/30		21
B01F33/3036	9	{using a biological motor, i.e. biological molecules which are activated and movement is induced to stir a fluid}	B01F33/30	B01F33/30		3
B01F33/3037	9	{using coupled electrorotation [CER] phenomena to mix or move fluids, or to sense properties of the mixture}	B01F33/30	B01F33/30		
B01F33/3038	9	{using ciliary stirrers to move or stir the fluids}	B01F33/30	B01F33/30		29
B01F33/3039	9	with mixing achieved by diffusion between layers	B01F33/3039	B01F33/3039		115
B01F33/304	9	{the mixing being performed in a mixing chamber where the products are brought into contact}	B01F33/30	B01F33/30		84
B01F33/3045	9	{using turbulence on microscale}	B01F33/30	B01F33/30		38
B01F33/305	9	{using mixing means not otherwise provided for (B01F25/00, B01F27/00, B01F29/00, B01F31/00, B01F33/301 - B01F33/3045, B01F33/40 and B01F33/45 take precedence)}	B01F33/30	B01F33/30		59
B01F33/35	8	Mixing after turning the mixing vessel upside down	B01F33/35	B01F33/35		96
B01F33/40	8	Mixers using gas or liquid agitation, e.g. with air supply tubes<br><br><u>NOTE</u><br><br>The agitating fluid is not meant to mix with the material.	B01F33/40	B01F33/40		614
B01F33/401	9	{Methods}	B01F33/40	B01F33/40		156
B01F33/402	9	{comprising supplementary stirring elements}	B01F33/40	B01F33/40		1045
B01F33/4021	10	{the gas being introduced through the shaft of the stirring element}	B01F33/40	B01F33/40		415
B01F33/403	9	{for mixing liquids (B01F33/402, B01F33/405, B01F33/406 take precedence)}	B01F33/40	B01F33/40		291
B01F33/404	9	{for mixing material moving continuously therethrough, e.g. using impinging jets}	B01F33/40	B01F33/40		114
B01F33/405	9	{in receptacles having guiding conduits therein, e.g. for feeding the gas to the bottom of the receptacle}	B01F33/40	B01F33/40		236
B01F33/4051	10	{with vertical conduits through which the material is being moved upwardly driven by the fluid}	B01F33/40	B01F33/40		43
B01F33/40511	11	{with a central conduit or a central set of conduits}	B01F33/40	B01F33/40		126
B01F33/40512	11	{involving gas diffusers at the bottom}	B01F33/40	B01F33/40		67
B01F33/406	9	{in receptacles with gas supply only at the bottom (B01F33/405 takes precedence)}	B01F33/40	B01F33/40		480
B01F33/4061	10	{through orifices arranged around a central cone (B01F33/4062 takes precedence)}	B01F33/40	B01F33/40		44
B01F33/4062	10	{with means for modifying the gas pressure or for supplying gas at different pressures or in different volumes at different parts of the bottom}	B01F33/40	B01F33/40		88
B01F33/407	9	{by blowing gas on the material from above}	B01F33/40	B01F33/40		111
B01F33/408	9	{Controlling}	B01F33/40	B01F33/40		107
B01F33/409	9	{Parts, e.g. diffusion elements; Accessories}	B01F33/40	B01F33/40		697
B01F33/4092	9	{Storing receptacles provided with separate mixing chambers}	B01F33/40	B01F33/40		62
B01F33/4094	9	{Plants}	B01F33/40	B01F33/40		674
B01F33/45	8	Magnetic mixers; Mixers with magnetically driven stirrers	B01F33/45	B01F33/45		943
B01F33/451	9	wherein the mixture is directly exposed to an electromagnetic field without use of a stirrer, e.g. for material comprising ferromagnetic particles or for molten metal	B01F33/451	B01F33/451		468
B01F33/452	9	using independent floating stirring elements	B01F33/452	B01F33/452		973
B01F33/453	9	using supported or suspended stirring elements	B01F33/453	B01F33/453		782
B01F33/4531	10	{using an axis supported in several points for mounting the stirring element}	B01F33/453	B01F33/453		80
B01F33/4532	10	{using a bearing, tube, opening or gap for internally supporting the stirring element}	B01F33/453	B01F33/453		156
B01F33/4533	10	{supporting the stirring element in one point}	B01F33/453	B01F33/453		68
B01F33/4534	10	{using a rod for supporting the stirring element, e.g. stirrer sliding on a rod or mounted on a rod sliding in a tube}	B01F33/453	B01F33/453		169
B01F33/4535	10	{using a stud for supporting the stirring element}	B01F33/453	B01F33/453		158
B01F33/4536	10	{using a wire for supporting or suspending the stirring element, e.g. stirrer sliding on a wire}	B01F33/453	B01F33/453		7
B01F33/4537	10	{the stirring element being suspended by one point}	B01F33/453	B01F33/453		54
B01F33/50	8	Movable or transportable mixing devices or plants	B01F33/50	B01F33/50		225
B01F33/501	9	Movable mixing devices, i.e. readily shifted or displaced from one place to another, e.g. portable during use	B01F33/501	B01F33/501		1717
B01F33/5011	10	{portable during use, e.g. hand-held}	B01F33/501	B01F33/501		2563
B01F33/50111	11	{Small portable bottles, flasks, vials, e.g. with means for mixing ingredients or for homogenizing their content, e.g. by hand shaking}	B01F33/501	B01F33/501		424
B01F33/50112	11	{of the syringe or cartridge type}	B01F33/501	B01F33/501		576
B01F33/50113	11	{of the pipette type}	B01F33/501	B01F33/501		13
B01F33/50114	11	{of the hand-held gun type}	B01F33/501	B01F33/501		163
B01F33/50115	11	{Stirring devices adapted to be connected to a standard boring machine or other kind of domestic tool}	B01F33/501	B01F33/501		122
B01F33/5012	10	{adapted to be mounted during use on a standard, base or support}	B01F33/501	B01F33/501		93
B01F33/5013	10	{movable by mechanical means, e.g. hoisting systems, grippers or lift trucks}	B01F33/501	B01F33/501		136
B01F33/5014	10	{movable by human force, e.g. kitchen or table devices}	B01F33/501	B01F33/501		556
B01F33/502	9	Vehicle-mounted mixing devices	B01F33/502	B01F33/502		1065
B01F33/5021	10	{the vehicle being self-propelled, e.g. truck mounted, provided with a motor, driven by tracks (B01F33/5022 - B01F33/5027 take precedence)}	B01F33/502	B01F33/502		256
B01F33/5022	10	{the vehicle being a carriage moving or driving along fixed or movable beams or bridges}	B01F33/502	B01F33/502		36
B01F33/5023	10	{the vehicle being a trailer which is hand moved or coupled to self-propelling vehicles}	B01F33/502	B01F33/502		364
B01F33/5024	10	{the vehicle being moved by human force}	B01F33/502	B01F33/502		99
B01F33/5025	10	{using rails for guiding the mixing installation during moving or displacing}	B01F33/502	B01F33/502		36
B01F33/5026	10	{using sledges or skids for moving or displacing the mixing installation}	B01F33/502	B01F33/502		31
B01F33/5027	10	{using driven tracks, caterpillars or crawler for moving or displacing the mixing installation}	B01F33/502	B01F33/502		19
B01F33/503	9	Floating mixing devices	B01F33/503	B01F33/503		716
B01F33/70	8	Mixers specially adapted for working at sub- or super-atmospheric pressure, e.g. combined with de-foaming	B01F33/70	B01F33/70		1305
B01F33/71	9	working at super-atmospheric pressure, e.g. in pressurised vessels	B01F33/71	B01F33/71		457
B01F33/80	8	Mixing plants; Combinations of mixers	B01F33/80	B01F33/80		1306
B01F33/805	9	{for granular material}	B01F33/80	B01F33/80		166
B01F33/8051	10	{with several silos arranged in a row or around a central delivery point, e.g. provided with proportioning means}	B01F33/80	B01F33/80		113
B01F33/80514	11	{the silos being arranged in a circular configuration, i.e. in a circle around a central delivery point}	B01F33/80	B01F33/80		26
B01F33/8052	10	{involving other than mixing operations, e.g. milling, sieving or drying}	B01F33/80	B01F33/80		176
B01F33/81	9	Combinations of similar mixers, e.g. with rotary stirring devices in two or more receptacles	B01F33/81	B01F33/81		1290
B01F33/811	10	{in two or more consecutive, i.e. successive, mixing receptacles or being consecutively arranged}	B01F33/81	B01F33/81		1500
B01F33/812	10	{in two or more alternative mixing receptacles, e.g. mixing in one receptacle and dispensing from another receptacle}	B01F33/81	B01F33/81		194
B01F33/813	10	{mixing simultaneously in two or more mixing receptacles}	B01F33/81	B01F33/81		1130
B01F33/82	9	Combinations of dissimilar mixers	B01F33/82	B01F33/82		2285
B01F33/821	10	{with consecutive receptacles}	B01F33/82	B01F33/82		2726
B01F33/8212	11	{with moving and non-moving stirring devices}	B01F33/82	B01F33/82		560
B01F33/822	10	{with moving and non-moving stirring devices in the same receptacle}	B01F33/82	B01F33/82		407
B01F33/823	10	{in two or more alternative mixing receptacles, e.g. mixing in one receptacle and dispensing from another receptacle}	B01F33/82	B01F33/82		56
B01F33/824	10	{mixing simultaneously in two or more mixing receptacles}	B01F33/82	B01F33/82		115
B01F33/83	9	Mixing plants specially adapted for mixing in combination with disintegrating operations	B01F33/83	B01F33/83		2675
B01F33/8305	10	{Devices with one shaft, provided with mixing and milling tools, e.g. using balls or rollers as working tools; Devices with two or more tools rotating about the same axis}	B01F33/83	B01F33/83		1161
B01F33/831	10	{Devices with consecutive working receptacles, e.g. with two intermeshing tools in one of the receptacles (B01F33/8305 takes precedence)}	B01F33/83	B01F33/83		2117
B01F33/833	10	{Devices with several tools rotating about different axis in the same receptacle}	B01F33/83	B01F33/83		517
B01F33/834	9	{Mixing in several steps, e.g. successive steps (B01F33/81, B01F33/82 and B01F33/85 take precedence)}	B01F33/80	B01F33/83		495
B01F33/836	9	{combining mixing with other treatments}	B01F33/80	B01F33/83		830
B01F33/8361	10	{with disintegrating}	B01F33/80	B01F33/83		88
B01F33/83611	11	{by cutting}	B01F33/80	B01F33/83		725
B01F33/83612	11	{by crushing or breaking}	B01F33/80	B01F33/83		2426
B01F33/83613	11	{by grinding or milling}	B01F33/80	B01F33/83		1524
B01F33/83614	11	{with irradiating}	B01F33/80	B01F33/83		13
B01F33/8362	10	{with chemical reactions}	B01F33/80	B01F33/83		584
B01F33/8363	10	{with coating}	B01F33/80	B01F33/83		58
B01F33/8364	10	{with drying}	B01F33/80	B01F33/83		408
B01F33/84	9	Mixing plants with mixing receptacles receiving material dispensed from several component receptacles, e.g. paint tins	B01F33/84	B01F33/84		876
B01F33/841	10	with component receptacles fixed in a circular configuration on a horizontal table, e.g. the table being able to be indexed about a vertical axis	B01F33/841	B01F33/841		405
B01F33/844	10	{with means for customizing the mixture on the point of sale, e.g. by sensing, receiving or analysing information about the characteristics of the mixture to be made}	B01F33/84	B01F33/84		85
B01F33/8442	11	{using a computer for controlling information and converting it in a formula and a set of operation instructions, e.g. on the point of sale}	B01F33/84	B01F33/84		280
B01F33/846	10	{using stored recipes for determining the composition of the mixture to be produced, i.e. for determining the amounts of the basic components to be dispensed from the component receptacles}	B01F33/84	B01F33/84		280
B01F33/848	10	{using data, i.e. barcodes, 3D codes or similar type of tagging information, as instruction or identification codes for controlling the dispensing and mixing operations}	B01F33/84	B01F33/84		146
B01F33/85	9	Mixing plants with mixing receptacles or mixing tools that can be indexed into different working positions	B01F33/85	B01F33/85		311
B01F33/86	8	{Mixing heads comprising a driven stirrer}	B01F33/00	B01F33/86		763
B01F33/862	9	{the stirrer being provided with a surrounding stator}	B01F33/00	B01F33/862		140
B01F33/87	8	Roll-type mixers	B01F33/87	B01F33/87		18
B01F35/00	7	Accessories for mixers; Auxiliary operations or auxiliary devices; Parts or details of general application	B01F35/00	B01F35/00		2433
B01F35/10	8	Maintenance of mixers	B01F35/10	B01F35/10		1358
B01F35/11	9	using fluids	B01F35/11	B01F35/11		1229
B01F35/12	9	using mechanical means	B01F35/12	B01F35/12		1216
B01F35/121	10	{using a brush for cleaning out rests of products}	B01F35/12	B01F35/12		1022
B01F35/122	10	{using pushers, i.e. a piston, for pushing out rests of products}	B01F35/12	B01F35/12		62
B01F35/123	10	{using scrapers for cleaning mixers}	B01F35/12	B01F35/12		5219
B01F35/13	9	using one or more of the components of the mixture to wash-out the mixer	B01F35/13	B01F35/13		70
B01F35/145	9	{Washing or cleaning mixers not provided for in other groups in this subclass; Inhibiting build-up of material on machine parts using other means}	B01F35/10	B01F35/145		564
B01F35/1452	10	{using fluids}	B01F35/10	B01F35/1452		685
B01F35/1453	11	{by means of jets of fluid, e.g. air}	B01F35/10	B01F35/1453		1167
B01F35/146	10	{Working under sterile conditions; Sterilizing the mixer or parts thereof}	B01F35/10	B01F35/146		201
B01F35/165	8	{Making mixers or parts thereof}	B01F35/00	B01F35/165		103
B01F35/181	8	{Preventing generation of dust or dirt; Sieves; Filters (B01F35/145, B01F35/43 take precedence)}	B01F35/00	B01F35/181		641
B01F35/184	9	{Preventing generation of dust}	B01F35/00	B01F35/184		700
B01F35/186	9	{using splash guards in mixers for avoiding dirt or projection of material}	B01F35/00	B01F35/186		85
B01F35/187	9	{using filters in mixers, e.g. during venting}	B01F35/00	B01F35/187		2097
B01F35/1872	10	{Filters for micro-living organisms, i.e. filtering of the mixture}	B01F35/00	B01F35/1872		14
B01F35/188	9	{using sieves in mixers for purposes other than mixing, e.g. eliminating dust during venting}	B01F35/00	B01F35/188		619
B01F35/189	9	{Venting, degassing or ventilating of gases, fumes or toxic vapours during mixing}	B01F35/00	B01F35/189		840
B01F35/20	8	Measuring; Control or regulation	B01F35/20	B01F35/20		1185
B01F35/21	9	Measuring	B01F35/21	B01F35/21		513
B01F35/211	10	{of the operational parameters (B01F35/212 and B01F35/213 take precedence)}	B01F35/21	B01F35/21		272
B01F35/2111	11	{Flow rate}	B01F35/21	B01F35/21		634
B01F35/21111	12	{Mass flow rate}	B01F35/21	B01F35/21		75
B01F35/21112	12	{Volumetric flow rate}	B01F35/21	B01F35/21		161
B01F35/2112	11	{Level of material in a container or the position or shape of the upper surface of the material}	B01F35/21	B01F35/21		1085
B01F35/2113	11	{Pressure}	B01F35/21	B01F35/21		897
B01F35/2114	11	{Speed of feeding material, e.g. bands or strips}	B01F35/21	B01F35/21		34
B01F35/2115	11	{Temperature}	B01F35/21	B01F35/21		1310
B01F35/21151	12	{using infrared radiation thermometer or pyrometer or infrared sensors for temperature measurement without contact}	B01F35/21	B01F35/21		40
B01F35/2116	11	{Volume}	B01F35/21	B01F35/21		105
B01F35/2117	11	{Weight}	B01F35/21	B01F35/21		995
B01F35/212	10	of the driving system data, e.g. torque, speed or power data	B01F35/212	B01F35/212		568
B01F35/213	10	of the properties of the mixtures, e.g. temperature, density or colour	B01F35/213	B01F35/213		1155
B01F35/2131	10	{Colour or luminescence}	B01F35/21	B01F35/213		163
B01F35/2132	10	{Concentration, pH, pOH, p(ION) or oxygen-demand (B01F35/2133 takes precedence)}	B01F35/21	B01F35/213		1000
B01F35/2133	10	{Electrical conductivity or dielectric constant of the mixture}	B01F35/21	B01F35/213		155
B01F35/2134	10	{Density or solids or particle number}	B01F35/21	B01F35/213		200
B01F35/2135	10	{Humidity, e.g. moisture content}	B01F35/21	B01F35/213		193
B01F35/2136	10	{Viscosity}	B01F35/21	B01F35/213		336
B01F35/214	10	characterised by the means for measuring	B01F35/214	B01F35/214		175
B01F35/2142	11	{using wireless sensors introduced in the mixture, e.g. transponders or RFID tags, for measuring the parameters of the mixture or components to be mixed}	B01F35/214	B01F35/214		69
B01F35/2144	11	{using radiation for measuring the parameters of the mixture or components to be mixed}	B01F35/214	B01F35/214		72
B01F35/22	9	Control or regulation	B01F35/22	B01F35/22		905
B01F35/2201	10	{characterised by the type of control technique used}	B01F35/22	B01F35/22		237
B01F35/2202	11	{Controlling the mixing process by feed-back, i.e. a measured parameter of the mixture is measured, compared with the set-value and the feed values are corrected}	B01F35/22	B01F35/22		593
B01F35/2203	11	{Controlling the mixing process by feed-forward, i.e. a parameter of the components to be mixed is measured and the feed values are calculated}	B01F35/22	B01F35/22		115
B01F35/2204	11	{Controlling the mixing process by fuzzy control, i.e. a prescribed fuzzy rule}	B01F35/22	B01F35/22		26
B01F35/2205	11	{Controlling the mixing process from a remote server, e.g. by sending commands using radio, telephone, internet, local network, GPS or other means}	B01F35/22	B01F35/22		231
B01F35/2206	11	{Use of stored recipes for controlling the computer programs, e.g. for manipulation, handling, production or composition in mixing plants (B01F33/846 takes precedence)}	B01F35/22	B01F35/22		331
B01F35/2207	11	{Use of data, i.e. barcodes, 3D codes or similar type of tagging information, as instruction or identification codes for controlling the computer programs, e.g. for manipulation, handling, production or compounding in mixing plants (B01F33/848 takes precedence)}	B01F35/22	B01F35/22		198
B01F35/2208	11	{Controlling using ultrasonic waves during the operation}	B01F35/22	B01F35/22		18
B01F35/2209	11	{Controlling the mixing process as a whole, i.e. involving a complete monitoring and controlling of the mixing process during the whole mixing cycle}	B01F35/22	B01F35/22		931
B01F35/221	10	of operational parameters, e.g. level of material in the mixer, temperature or pressure	B01F35/221	B01F35/221		621
B01F35/2211	11	{Amount of delivered fluid during a period}	B01F35/221	B01F35/221		1180
B01F35/2212	11	{Level of the material in the mixer}	B01F35/221	B01F35/221		307
B01F35/2213	11	{Pressure}	B01F35/221	B01F35/221		650
B01F35/2214	11	{Speed during the operation}	B01F35/221	B01F35/221		156
B01F35/22141	12	{Speed of feeding of at least one component to be mixed}	B01F35/221	B01F35/221		292
B01F35/22142	12	{Speed of the mixing device during the operation}	B01F35/221	B01F35/221		295
B01F35/221421	13	{Linear speed of the tip of a moving stirrer during the operation}	B01F35/221	B01F35/221		27
B01F35/221422	13	{Speed of rotation of the mixing axis, stirrer or receptacle during the operation}	B01F35/221	B01F35/221		495
B01F35/2215	11	{Temperature}	B01F35/221	B01F35/221		1441
B01F35/2216	11	{Time, i.e. duration, of at least one parameter during the operation}	B01F35/221	B01F35/221		188
B01F35/22161	12	{duration of the mixing process or parts of it}	B01F35/221	B01F35/221		268
B01F35/22162	12	{Time of feeding of at least one of the components to be mixed}	B01F35/221	B01F35/221		105
B01F35/2217	11	{Volume of at least one component to be mixed}	B01F35/221	B01F35/221		170
B01F35/2218	11	{Weight of at least one component to be mixed}	B01F35/221	B01F35/221		399
B01F35/222	10	of the operation of the driving system, e.g. torque, speed or power of motors; of the position of mixing devices or elements	B01F35/222	B01F35/222		436
B01F35/2221	11	{the position of baffles used to modify the flow in a conduit or a container}	B01F35/222	B01F35/222		7
B01F35/30	8	Driving arrangements; Transmissions; Couplings; Brakes	B01F35/30	B01F35/30		2183
B01F35/31	9	Couplings	B01F35/31	B01F35/31		1170
B01F35/32	9	Driving arrangements	B01F35/32	B01F35/32		520
B01F35/32005	10	{Type of drive}	B01F35/32	B01F35/32		378
B01F35/3201	11	{by using acoustic force, e.g. acoustically induced bubbles, acoustic windmill, acoustic scallop}	B01F35/32	B01F35/32		16
B01F35/32015	11	{Flow driven}	B01F35/32	B01F35/32		492
B01F35/3202	11	{Hand driven}	B01F35/32	B01F35/32		1092
B01F35/32021	12	{Shaking by hand a portable receptacle or stirrer for mixing}	B01F35/32	B01F35/32		295
B01F35/32025	11	{Battery driven}	B01F35/32	B01F35/32		179
B01F35/3203	11	{Gas driven}	B01F35/32	B01F35/32		437
B01F35/32035	11	{Gravity driven, e.g. by means of weights out of balance or plunger-weights moving in a cylinder}	B01F35/32	B01F35/32		33
B01F35/3204	11	{Motor driven, i.e. by means of an electric or IC motor}	B01F35/32	B01F35/32		4876
B01F35/32045	11	{Hydraulically driven}	B01F35/32	B01F35/32		227
B01F35/3205	11	{by using optical pressure force, e.g. produced by a laser beam}	B01F35/32	B01F35/32		9
B01F35/32055	11	{by using solar energy}	B01F35/32	B01F35/32		99
B01F35/3206	11	{by the rotation of the wheels during movement}	B01F35/32	B01F35/32		64
B01F35/32065	11	{Wind driven}	B01F35/32	B01F35/32		72
B01F35/321	10	{Disposition of the drive}	B01F35/32	B01F35/32		241
B01F35/3211	11	{independent from the receptacle}	B01F35/32	B01F35/32		144
B01F35/3212	11	{mounted on the receptacle}	B01F35/32	B01F35/32		73
B01F35/3213	11	{at the lower side of the axis, e.g. driving the stirrer from the bottom of a receptacle}	B01F35/32	B01F35/32		467
B01F35/3214	11	{at the upper side of the axis, e.g. driving the stirrer from the top of a receptacle}	B01F35/32	B01F35/32		379
B01F35/3215	11	{the driving system comprising more than one motor, e.g. having an auxiliary motor or comprising independently driven elements}	B01F35/32	B01F35/32		730
B01F35/32151	12	{Driving the stirrer axis from both ends of the axis, i.e. using at least two motors per shaft}	B01F35/32	B01F35/32		17
B01F35/322	10	{Construction of driving shafts}	B01F35/32	B01F35/32		526
B01F35/323	10	{for vertical stirrer shafts (B01F35/324 takes precedence)}	B01F35/32	B01F35/32		361
B01F35/3231	11	{Driving several stirrer shafts, e.g. about the same axis}	B01F35/32	B01F35/32		469
B01F35/324	10	{Driving independent stirrer shafts, i.e. not fitted on the container}	B01F35/32	B01F35/32		158
B01F35/325	10	{Driving reciprocating or oscillating stirrers}	B01F35/32	B01F35/32		603
B01F35/33	9	Transmissions; Means for modifying the speed or direction of rotation	B01F35/33	B01F35/33		1038
B01F35/331	10	{alternately changing the speed of rotation}	B01F35/33	B01F35/33		171
B01F35/332	10	{alternately changing the direction of rotation}	B01F35/33	B01F35/33		521
B01F35/333	10	{the rotation sense being changeable, e.g. to mix or aerate, to move a fluid forward or backward or to suck or blow}	B01F35/33	B01F35/33		100
B01F35/34	9	{Brake mechanisms}	B01F35/30	B01F35/34		39
B01F2035/35	9	{Use of other general mechanical engineering elements in mixing devices}	B01F35/30	B01F2035/35		100
B01F2035/351	10	{Sealings}	B01F35/30	B01F2035/351		1526
B01F2035/3511	11	{for laboratory mixers}	B01F35/30	B01F2035/3511		69
B01F2035/3512	11	{Fluid sealings, e.g. using liquids or air under pressure which is leaking into the mixing receptacle}	B01F35/30	B01F2035/3512		122
B01F2035/3513	11	{comprising a stationary member in frontal contact with a movable member}	B01F35/30	B01F2035/3513		159
B01F2035/352	10	{Bearings}	B01F35/30	B01F2035/352		576
B01F2035/353	10	{Lubricating systems}	B01F35/30	B01F2035/353		80
B01F35/40	8	Mounting or supporting mixing devices or receptacles; Clamping or holding arrangements therefor	B01F35/40	B01F35/40		1106
B01F35/41	9	Mounting or supporting stirrer shafts or stirrer units on receptacles	B01F35/41	B01F35/41		226
B01F35/411	10	{by supporting only one extremity of the shaft}	B01F35/41	B01F35/41		35
B01F35/4111	11	{at the top of the receptacle}	B01F35/41	B01F35/41		708
B01F35/4112	11	{at the bottom of the receptacle, e.g. by studs}	B01F35/41	B01F35/41		192
B01F35/4113	11	{at a side wall of the receptacle}	B01F35/41	B01F35/41		132
B01F35/412	10	{by supporting both extremities of the shaft}	B01F35/41	B01F35/41		75
B01F35/4121	11	{at the top and at the bottom of the receptacle, e.g. for performing a conical orbital movement about a vertical axis}	B01F35/41	B01F35/41		208
B01F35/4122	11	{at the side walls of the receptacle}	B01F35/41	B01F35/41		135
B01F35/413	10	{by means of clamps or clamping arrangements for fixing attached stirrers or independent stirrer units}	B01F35/41	B01F35/41		171
B01F35/414	10	{using inflatable arrangements for supporting a stirring element}	B01F35/41	B01F35/41		4
B01F35/42	9	Clamping or holding arrangements for mounting receptacles on mixing devices	B01F35/42	B01F35/42		1745
B01F35/421	10	{having a cup-shaped or cage-type form}	B01F35/42	B01F35/42		209
B01F35/422	10	{having a jaw-type or finger-type shape}	B01F35/42	B01F35/42		196
B01F35/423	10	{of the vertically movable, two-plates type}	B01F35/42	B01F35/42		218
B01F35/424	10	{by means of an air cushion used for supporting the mixing receptacle}	B01F35/42	B01F35/42		6
B01F35/425	10	{Holding arrangements for retaining loose elements of the mixing receptacle, e.g. for holding the handle of a can, while it is being shaken}	B01F35/42	B01F35/42		78
B01F35/43	9	Supporting receptacles on frames or stands	B01F35/43	B01F35/43		3374
B01F35/45	8	Closures or doors specially adapted for mixing receptacles; Operating mechanisms therefor	B01F35/45	B01F35/45		1611
B01F35/451	9	{by rotating them about an axis parallel to the plane of the opening}	B01F35/45	B01F35/45		419
B01F35/452	9	{by moving them in the plane of the opening (B01F35/454 takes precedence)}	B01F35/45	B01F35/45		120
B01F35/4521	10	{by rotating them about an axis perpendicular to the plane of the opening}	B01F35/45	B01F35/45		59
B01F35/453	9	{by moving them perpendicular to the plane of the opening}	B01F35/45	B01F35/45		425
B01F35/4531	10	{and moving them afterwards in another direction}	B01F35/45	B01F35/45		63
B01F35/454	9	{Moving covers on a cylindrical drum in a circular path along the drum}	B01F35/45	B01F35/45		19
B01F35/50	8	Mixing receptacles	B01F35/50	B01F35/50		938
B01F35/51	9	characterised by their material	B01F35/51	B01F35/51		844
B01F35/511	9	provided with liners, e.g. wear resistant or flexible liners	B01F35/511	B01F35/511		269
B01F35/512	9	characterised by surface properties, e.g. coated or rough	B01F35/512	B01F35/512		188
B01F35/513	9	Flexible receptacles, e.g. bags supported by rigid containers	B01F35/513	B01F35/513		443
B01F35/514	9	{the mixing receptacle or conduit being transparent or comprising transparent parts}	B01F35/50	B01F35/51		462
B01F35/52	9	Receptacles with two or more compartments	B01F35/52	B01F35/52		329
B01F35/522	10	{comprising compartments keeping the materials to be mixed separated until the mixing is initiated (containers or packages for packaging two or more different materials which must be maintained separate prior to use in admixture B65D81/32)}	B01F35/52	B01F35/52		235
B01F35/53	9	characterised by the configuration of the interior, e.g. baffles for facilitating the mixing of components	B01F35/53	B01F35/53		529
B01F35/531	10	{with baffles, plates or bars on the wall or the bottom}	B01F35/53	B01F35/53		655
B01F35/5311	11	{with horizontal baffles mounted on the walls}	B01F35/53	B01F35/53		193
B01F35/5312	11	{with vertical baffles mounted on the walls}	B01F35/53	B01F35/53		209
B01F35/532	10	{with guide tubes on the wall or the bottom}	B01F35/53	B01F35/53		76
B01F35/54	9	{Closely surrounding the rotating element}	B01F35/50	B01F35/54		66
B01F35/55	8	{Baffles; Flow breakers (B01F35/531 takes precedence)}	B01F35/00	B01F35/55		359
B01F35/56	8	{General build-up of the mixers}	B01F35/00	B01F35/56		168
B01F35/561	9	{the mixer being built-up from a plurality of modules or stacked plates comprising complete or partial elements of the mixer}	B01F35/00	B01F35/561		169
B01F35/562	9	{the mixer or mixing elements being collapsible, i.e. when discharging the products}	B01F35/00	B01F35/562		46
B01F35/5621	10	{the complete mixer being collapsible, i.e. the housing can be collapsed}	B01F35/00	B01F35/5621		8
B01F35/60	8	Safety arrangements	B01F35/60	B01F35/60		609
B01F35/602	9	{with a safety or relief valve}	B01F35/60	B01F35/60		79
B01F35/605	9	{Safety devices concerning the operation of the mixer}	B01F35/60	B01F35/60		299
B01F35/6052	10	{with locking, blocking or interlocking mechanisms for preventing operation of the actuation mechanism of the mixing device}	B01F35/60	B01F35/60		138
B01F35/71	8	Feed mechanisms (with proportioning B01F35/80)	B01F35/71	B01F35/71		4635
B01F35/711	9	{for feeding a mixture of components, i.e. solids in liquid, solids in a gas stream}	B01F35/71	B01F35/71		315
B01F35/712	9	{for feeding fluids}	B01F35/71	B01F35/71		3920
B01F35/713	9	{comprising breaking packages or parts thereof, e.g. piercing or opening sealing elements between compartments or cartridges (containers or packages per seB65D)}	B01F35/71	B01F35/71		393
B01F35/7131	10	{Breaking or perforating packages, containers or vials}	B01F35/71	B01F35/71		428
B01F35/7132	10	{the package containing one of the components dissolves when in contact with the other component of the mixture (disintegrable, dissolvable or edible packaging materials B65D65/46)}	B01F35/71	B01F35/71		26
B01F35/7133	10	{Opening clips which seal openings between the compartments}	B01F35/71	B01F35/71		16
B01F35/7134	10	{Dissolving the seal when in contact with one of the products to be mixed, thereby bringing the compartments in communication}	B01F35/71	B01F35/71		5
B01F35/7135	10	{Opening the seal between the compartments by application of heat}	B01F35/71	B01F35/71		12
B01F35/7136	10	{Opening hooks which lock or close-off openings between compartments}	B01F35/71	B01F35/71		3
B01F35/7137	10	{Piercing, perforating or melting membranes or closures which seal the compartments}	B01F35/71	B01F35/71		267
B01F35/7138	10	{Opening valves which close-off openings between compartments}	B01F35/71	B01F35/71		42
B01F35/7139	10	{Removing separation walls, plugs which close off the different compartments, e.g. by rotation or axially sliding}	B01F35/71	B01F35/71		94
B01F35/714	9	{for feeding predetermined amounts (B01F35/88 takes precedence)}	B01F35/71	B01F35/71		1678
B01F35/7141	10	{using measuring chambers moving between a loading and unloading position, e.g. reciprocating feed frames}	B01F35/71	B01F35/71		153
B01F35/71411	11	{rotating or oscillating about an axis}	B01F35/71	B01F35/71		63
B01F35/714111	12	{the measuring chambers being pockets on the circumference of a drum rotating about a horizontal axis with discharging by gravity}	B01F35/71	B01F35/71		63
B01F35/714112	12	{the measuring chambers being channels extending between both front faces of a rotating cylinder or disc}	B01F35/71	B01F35/71		43
B01F35/715	9	{Feeding the components in several steps, e.g. successive steps}	B01F35/71	B01F35/71		371
B01F35/716	9	{characterised by the relative arrangement of the containers for feeding or mixing the components}	B01F35/71	B01F35/71		308
B01F35/7161	10	{the containers being connected coaxially before contacting the contents}	B01F35/71	B01F35/71		177
B01F35/7162	10	{A container being placed inside the other before contacting the contents}	B01F35/71	B01F35/71		185
B01F35/7163	10	{the containers being connected in a mouth-to-mouth, end-to-end disposition, i.e. the openings are juxtaposed before contacting the contents}	B01F35/71	B01F35/71		397
B01F35/7164	10	{the containers being placed in parallel before contacting the contents}	B01F35/71	B01F35/71		693
B01F35/717	9	{characterised by the means for feeding the components to the mixer}	B01F35/71	B01F35/71		3716
B01F35/71705	10	{using belts}	B01F35/71	B01F35/71		710
B01F35/7171	10	{using boxes, closable containers, sacks or carts}	B01F35/71	B01F35/71		202
B01F35/71715	10	{using buckets, cups or open containers}	B01F35/71	B01F35/71		163
B01F35/7172	10	{using capillary forces}	B01F35/71	B01F35/71		69
B01F35/71725	10	{using centrifugal forces}	B01F35/71	B01F35/71		269
B01F35/7173	10	{using gravity, e.g. from a hopper}	B01F35/71	B01F35/71		633
B01F35/71731	11	{using a hopper}	B01F35/71	B01F35/71		1901
B01F35/71735	10	{using grippers}	B01F35/71	B01F35/71		16
B01F35/7174	10	{using pistons, plungers or syringes}	B01F35/71	B01F35/71		1214
B01F35/71745	10	{using pneumatic pressure, overpressure, gas or air pressure in a closed receptacle or circuit system}	B01F35/71	B01F35/71		447
B01F35/7175	10	{using propellers}	B01F35/71	B01F35/71		163
B01F35/71755	10	{using means for feeding components in a pulsating or intermittent manner}	B01F35/71	B01F35/71		339
B01F35/717551	11	{using electrical pulses}	B01F35/71	B01F35/71		20
B01F35/7176	10	{using pumps}	B01F35/71	B01F35/71		1483
B01F35/71761	11	{Membrane pumps}	B01F35/71	B01F35/71		61
B01F35/717611	11	{Peristaltic pumps}	B01F35/71	B01F35/71		101
B01F35/717612	11	{Piezoelectric pumps}	B01F35/71	B01F35/71		23
B01F35/717613	11	{Piston pumps}	B01F35/71	B01F35/71		209
B01F35/717614	11	{Venturi pumps}	B01F35/71	B01F35/71		27
B01F35/71765	10	{using rakes or plain plates with raking movement}	B01F35/71	B01F35/71		52
B01F35/7177	10	{using rollers}	B01F35/71	B01F35/71		49
B01F35/71775	10	{using helical screws}	B01F35/71	B01F35/71		1529
B01F35/7178	10	{using shovels or scoops}	B01F35/71	B01F35/71		35
B01F35/71785	10	{using slides or vibrating tables}	B01F35/71	B01F35/71		44
B01F35/7179	10	{using sprayers, nozzles or jets}	B01F35/71	B01F35/71		1962
B01F35/71791	11	{using ink jet heads or cartridges, e.g. of the thermal bubble jet or piezoelectric type}	B01F35/71	B01F35/71		36
B01F35/71795	10	{Squeezing a flexible container}	B01F35/71	B01F35/71		90
B01F35/718	10	{using vacuum, under pressure in a closed receptacle or circuit system}	B01F35/71	B01F35/71		503
B01F35/71801	11	{using a syphon to create a suction of a component}	B01F35/71	B01F35/71		24
B01F35/71805	10	{using valves, gates, orifices or openings}	B01F35/71	B01F35/71		3090
B01F35/718051	11	{being adjustable}	B01F35/71	B01F35/71		590
B01F35/7181	10	{using fans or turbines}	B01F35/71	B01F35/71		135
B01F35/71815	10	{using vibrations, e.g. standing waves or ultrasonic vibrations}	B01F35/71	B01F35/71		396
B01F35/7182	10	{with means for feeding the material with a fractal or tree-type distribution in a surface}	B01F35/71	B01F35/71		129
B01F35/71825	10	{using means for feeding one phase surrounded by another phase without mixing during the feeding}	B01F35/71	B01F35/71		51
B01F35/75	8	Discharge mechanisms	B01F35/75	B01F35/75		2284
B01F35/751	9	{Discharging by opening a gate, e.g. using discharge paddles}	B01F35/75	B01F35/75		399
B01F35/7511	10	{the gate carrying a stirrer acting as discharge pump}	B01F35/75	B01F35/75		31
B01F35/752	9	{with arrangements for converting the mechanism from mixing to discharging, e.g. by either guiding a mixture back into a receptacle or discharging it}	B01F35/75	B01F35/75		273
B01F35/753	9	{Discharging at the upper side of the receptacle, e.g. by pressurising the liquid in the receptacle or by centrifugal force}	B01F35/75	B01F35/75		195
B01F35/754	9	{characterised by the means for discharging the components from the mixer}	B01F35/75	B01F35/75		1723
B01F35/7541	10	{using belts}	B01F35/75	B01F35/75		136
B01F35/75415	10	{using gravity}	B01F35/75	B01F35/75		205
B01F35/7542	10	{Discharging the components by overflow}	B01F35/75	B01F35/75		30
B01F35/75425	10	{using pistons or plungers}	B01F35/75	B01F35/75		298
B01F35/754251	11	{reciprocating in the mixing receptacle}	B01F35/75	B01F35/75		362
B01F35/7543	10	{using pneumatic pressure, overpressure or gas pressure in a closed receptacle or circuit system}	B01F35/75	B01F35/75		234
B01F35/75435	10	{using means for discharging the mixture in a pulsating or intermittent manner}	B01F35/75	B01F35/75		51
B01F35/754351	11	{using electrical pulses}	B01F35/75	B01F35/75		3
B01F35/7544	10	{using pumps}	B01F35/75	B01F35/75		479
B01F35/75441	11	{Venturi pumps}	B01F35/75	B01F35/75		6
B01F35/75445	10	{using pushers}	B01F35/75	B01F35/75		107
B01F35/7545	10	{using slides}	B01F35/75	B01F35/75		120
B01F35/75455	10	{using a rotary discharge means, e.g. a screw beneath the receptacle (B01F35/751 takes precedence)}	B01F35/75	B01F35/75		628
B01F35/754551	11	{using helical screws}	B01F35/75	B01F35/75		956
B01F35/7546	10	{using squeezing means on a deformable container}	B01F35/75	B01F35/75		62
B01F35/75465	10	{using suction, vacuum, e.g. with a pipette}	B01F35/75	B01F35/75		167
B01F35/7547	10	{using valves, gates, orifices or openings}	B01F35/75	B01F35/75		2128
B01F35/75471	11	{being adjustable}	B01F35/75	B01F35/75		244
B01F35/75475	10	{using fans or ventilators}	B01F35/75	B01F35/75		23
B01F35/7548	10	{using tilting or pivoting means for emptying the mixing receptacle}	B01F35/75	B01F35/75		741
B01F35/75485	10	{the mixing receptacle rotating in opposite directions for mixing and for discharging}	B01F35/75	B01F35/75		52
B01F35/7549	10	{using distributing means, e.g. manifold valves or multiple fittings for supplying the discharge components to a plurality of dispensing places}	B01F35/75	B01F35/75		73
B01F35/79	8	{Preventing lumping, or comminuting lumps, during feeding or discharging, e.g. by means of vibrations, or by scrapers}	B01F35/00	B01F35/79		502
B01F35/80	8	Forming a predetermined ratio of the substances to be mixed (controlling ratio of two or more flows of fluid or fluent material G05D11/02)	B01F35/80	B01F35/80		1761
B01F35/81	9	Forming mixtures with changing ratios or gradients	B01F35/81	B01F35/81		310
B01F35/82	9	by adding a material to be mixed to a mixture in response to a detected feature, e.g. density, radioactivity, consumed power or colour	B01F35/82	B01F35/82		754
B01F35/83	9	by controlling the ratio of two or more flows, e.g. using flow sensing or flow controlling devices	B01F35/83	B01F35/83		1147
B01F35/831	10	{using one or more pump or other dispensing mechanisms for feeding the flows in predetermined proportion, e.g. one of the pumps being driven by one of the flows (B01F35/832 takes precedence)}	B01F35/83	B01F35/83		370
B01F35/8311	11	{with means for controlling the motor driving the pumps or the other dispensing mechanisms}	B01F35/83	B01F35/83		194
B01F35/832	10	{Flow control by weighing}	B01F35/83	B01F35/83		376
B01F35/833	10	{Flow control by valves, e.g. opening intermittently}	B01F35/83	B01F35/83		930
B01F35/8331	11	{the flow of one component operating the actuator of the valve, e.g. by deforming a membrane which operates de valve actuator}	B01F35/83	B01F35/83		38
B01F35/834	10	{the flow of substances to be mixed circulating in a closed circuit, e.g. from a container through valve, driving means, metering means or dispensing means, e.g. 3-way valve, and back to the container}	B01F35/83	B01F35/83		89
B01F35/88	9	by feeding the materials batchwise	B01F35/88	B01F35/88		971
B01F35/881	10	{by weighing, e.g. with automatic discharge}	B01F35/88	B01F35/88		1394
B01F35/8811	11	{the weighing being effected by material receiving containers rotating or tilting under the influence of the weight of the material in those containers}	B01F35/88	B01F35/88		60
B01F35/882	10	{using measuring chambers, e.g. volumetric pumps, for feeding the substances}	B01F35/88	B01F35/88		543
B01F35/8821	11	{involving controlling}	B01F35/88	B01F35/88		184
B01F35/8822	11	{using measuring chambers of the piston or plunger type (B01F35/8823 takes precedence)}	B01F35/88	B01F35/88		390
B01F35/88221	12	{with double acting pistons (B01F35/88222 takes precedence)}	B01F35/88	B01F35/88		53
B01F35/88222	12	{without external means for driving the piston, e.g. the piston being driven by one of the components}	B01F35/88	B01F35/88		61
B01F35/8823	11	{using diaphragms or bellows}	B01F35/88	B01F35/88		57
B01F35/883	10	{using flow rate controls for feeding the substances}	B01F35/88	B01F35/88		580
B01F35/892	9	{for solid materials, e.g. using belts, vibrations, hoppers with variable outlets or hoppers with rotating elements, e.g. screws, at their outlet (B01F35/82 - B01F35/88 take precedence)}	B01F35/80	B01F35/892		175
B01F35/8921	10	{the material after falling on a, e.g. rotatable, plate being wiped from this plate by means of a scraper}	B01F35/80	B01F35/8921		25
B01F35/894	9	{Measuring receptacles therefor}	B01F35/80	B01F35/894		98
B01F35/896	9	{characterised by the build-up of the device}	B01F35/80	B01F35/896		166
B01F35/90	8	Heating or cooling systems	B01F35/90	B01F35/90		1510
B01F35/91	9	using gas or liquid injected into the material, e.g. using liquefied carbon dioxide or steam	B01F35/91	B01F35/91		843
B01F35/92	9	for heating the outside of the receptacle, e.g. heated jackets or burners	B01F35/92	B01F35/92		4566
B01F35/93	9	arranged inside the receptacle	B01F35/93	B01F35/93		2448
B01F35/94	9	using radiation, e.g. microwaves or electromagnetic radiation	B01F35/94	B01F35/94		155
B01F35/95	9	using heated or cooled stirrers	B01F35/95	B01F35/95		1163
B01F2035/98	9	{Cooling}	B01F35/90	B01F2035/98		1817
B01F2035/99	9	{Heating}	B01F35/90	B01F2035/99		5858
B01F2101/00	7	Mixing characterised by the nature of the mixed materials or by the application field	B01F101/00	B01F101/00		52
B01F2101/005	8	{Mixing or agitating manure, dung}	B01F101/00	B01F101/00		287
B01F2101/02	8	Mixing or agitating during harvesting or mowing, e.g. mixing with solid harvested products or particles	B01F101/02	B01F101/02		8
B01F2101/04	8	Mixing biocidal, pesticidal or herbicidal ingredients used in agriculture or horticulture, e.g. for spraying	B01F101/04	B01F101/04		1113
B01F2101/06	8	Mixing of food ingredients	B01F101/06	B01F101/06		3031
B01F2101/07	9	Mixing ingredients into milk or cream, e.g. aerating	B01F101/07	B01F101/07		228
B01F2101/08	9	Mixing of dough	B01F101/08	B01F101/08		91
B01F2101/09	9	Mixing of cereals, grains or seeds materials	B01F101/09	B01F101/09		206
B01F2101/10	9	Mixing of butter or margarine ingredients	B01F101/10	B01F101/10		19
B01F2101/11	9	Mixing of cheese ingredients	B01F101/11	B01F101/11		24
B01F2101/12	9	Mixing of chocolate ingredients	B01F101/12	B01F101/12		46
B01F2101/13	9	Mixing of ice-cream ingredients	B01F101/13	B01F101/13		112
B01F2101/14	9	Mixing of ingredients for non-alcoholic beverages; Dissolving sugar in water	B01F101/14	B01F101/14		912
B01F2101/15	9	Mixing of beer ingredients	B01F101/15	B01F101/15		50
B01F2101/16	9	Mixing wine or other alcoholic beverages; Mixing ingredients thereof	B01F101/16	B01F101/16		261
B01F2101/17	10	Aeration of wine	B01F101/17	B01F101/17		284
B01F2101/18	9	Mixing animal food ingredients	B01F101/18	B01F101/18		2410
B01F2101/1805	8	{Kitchen, household equipment for mixing}	B01F101/00	B01F101/18		144
B01F2101/19	8	Mixing dentistry compositions	B01F101/19	B01F101/19		161
B01F2101/20	8	Mixing of ingredients for bone cement	B01F101/20	B01F101/20		362
B01F2101/21	8	Mixing of ingredients for cosmetic or perfume compositions	B01F101/21	B01F101/21		1484
B01F2101/22	8	Mixing of ingredients for pharmaceutical or medical compositions	B01F101/22	B01F101/22		3528
B01F2101/2202	8	{Mixing compositions or mixers in the medical or veterinary field}	B01F101/00	B01F101/22		1001
B01F2101/2204	8	{Mixing chemical components in generals in order to improve chemical treatment or reactions, independently from the specific application}	B01F101/00	B01F101/22		1261
B01F2101/23	8	Mixing of laboratory samples e.g. in preparation of analysing or testing properties of materials	B01F101/23	B01F101/23		2475
B01F2101/2305	8	{Mixers of the two-component package type, i.e. where at least two components are separately stored, and are mixed in the moment of application}	B01F101/00	B01F101/23		412
B01F2101/24	8	Mixing of ingredients for cleaning compositions	B01F101/24	B01F101/24		460
B01F2101/25	8	Mixing waste with other ingredients	B01F101/25	B01F101/25		429
B01F2101/26	8	Mixing ingredients for casting metals	B01F101/26	B01F101/26		214
B01F2101/27	8	Mixing ingredients for grinding, polishing or lapping materials	B01F101/27	B01F101/27		64
B01F2101/28	8	Mixing cement, mortar, clay, plaster or concrete ingredients	B01F101/28	B01F101/28		862
B01F2101/2805	8	{Mixing plastics, polymer material ingredients, monomers or oligomers}	B01F101/00	B01F101/28		772
B01F2101/30	8	Mixing paints or paint ingredients, e.g. pigments, dyes, colours, lacquers or enamel	B01F101/30	B01F101/30		5909
B01F2101/305	8	{Treatment of water, waste water or sewage}	B01F101/00	B01F101/30		4045
B01F2101/32	8	Mixing fertiliser ingredients	B01F101/32	B01F101/32		1710
B01F2101/33	9	Mixing compost ingredients or organic waste	B01F101/33	B01F101/33		510
B01F2101/34	8	Mixing fuel and prill, i.e. water or other fluids mixed with solid explosives, to obtain liquid explosive fuel emulsions or slurries	B01F101/34	B01F101/34		65
B01F2101/35	8	Mixing inks or toners	B01F101/35	B01F101/35		650
B01F2101/36	8	Mixing of ingredients for adhesives or glues; Mixing adhesives and gas	B01F101/36	B01F101/36		1500
B01F2101/38	8	Mixing of asphalt, bitumen, tar or pitch or their ingredients	B01F101/38	B01F101/38		554
B01F2101/39	8	Mixing of ingredients for grease or lubricating compositions	B01F101/39	B01F101/39		577
B01F2101/40	8	Mixing of ingredients for oils, fats or waxes	B01F101/40	B01F101/40		288
B01F2101/44	8	Mixing of ingredients for microbiology, enzymology, in vitro culture or genetic manipulation	B01F101/44	B01F101/44		576
B01F2101/45	8	Mixing in metallurgical processes of ferrous or non-ferrous materials	B01F101/45	B01F101/45		355
B01F2101/4505	8	{Mixing ingredients comprising detergents, soaps, for washing, e.g. washing machines}	B01F101/00	B01F101/45		228
B01F2101/47	8	Mixing of ingredients for making paper pulp, e.g. wood fibres or wood pulp	B01F101/47	B01F101/47		385
B01F2101/48	8	Mixing water in water-taps with other ingredients, e.g. air, detergents or disinfectants	B01F101/48	B01F101/48		772
B01F2101/49	8	Mixing drilled material or ingredients for well-drilling, earth-drilling or deep-drilling compositions with liquids to obtain slurries	B01F101/49	B01F101/49		367
B01F2101/50	8	Mixing mined ingredients and liquid to obtain slurries	B01F101/50	B01F101/50		108
B01F2101/501	8	{Mixing combustion ingredients, e.g. gases, for burners or combustion chambers}	B01F101/00	B01F101/50		176
B01F2101/503	8	{Mixing fuel or propellant and water or gas, e.g. air, or other fluids, e.g. liquid additives to obtain fluid fuel}	B01F101/00	B01F101/50		120
B01F2101/505	8	{Mixing fuel and water or other fluids to obtain liquid fuel emulsions}	B01F101/00	B01F101/50		182
B01F2101/54	8	Mixing liquid fragrances with air	B01F101/54	B01F101/54		37
B01F2101/55	8	Mixing liquid air humidifiers with air	B01F101/55	B01F101/55		25
B01F2101/56	8	Mixing photosensitive chemicals or photographic base materials	B01F101/56	B01F101/56		56
B01F2101/57	8	Mixing radioactive materials, e.g. nuclear materials	B01F101/57	B01F101/57		43
B01F2101/58	8	Mixing semiconducting materials, e.g. during semiconductor or wafer manufacturing processes	B01F101/58	B01F101/58		136
B01F2101/59	8	Mixing reaction ingredients for fuel cells	B01F101/59	B01F101/59		246
B01F2215/00	7	Auxiliary or complementary information in relation with mixing	CPCONLY	B01F2215/00		5
B01F2215/04	8	Technical information in relation with mixing	CPCONLY	B01F2215/04		1
B01F2215/0404	9	theories or general explanations of phenomena associated with mixing or generalizations of a concept by comparison of equivalent methods	CPCONLY	B01F2215/0404		40
B01F2215/0409	9	Relationships between different variables defining features or parameters of the apparatus or process	CPCONLY	B01F2215/0409		120
B01F2215/0413	9	Numerical information	CPCONLY	B01F2215/0413		6
B01F2215/0418	10	Geometrical information	CPCONLY	B01F2215/0418		3
B01F2215/0422	11	Numerical values of angles	CPCONLY	B01F2215/0422		364
B01F2215/0427	11	Numerical distance values, e.g. separation, position	CPCONLY	B01F2215/0427		158
B01F2215/0431	11	Numerical size values, e.g. diameter of a hole or conduit, area, volume, length, width, or ratios thereof	CPCONLY	B01F2215/0431		903
B01F2215/0436	10	Operational information	CPCONLY	B01F2215/0436		12
B01F2215/044	11	Numerical composition values of components or mixtures, e.g. percentage of components	CPCONLY	B01F2215/044		106
B01F2215/0445	11	Numerical electrical values, e.g. intensity, voltage	CPCONLY	B01F2215/0445		12
B01F2215/045	11	Numerical flow-rate values	CPCONLY	B01F2215/045		188
B01F2215/0454	11	Numerical frequency values	CPCONLY	B01F2215/0454		116
B01F2215/0459	11	Numerical values of dimensionless numbers, i.e. Re, Pr, Nu, transfer coefficients	CPCONLY	B01F2215/0459		34
B01F2215/0463	11	Numerical power values	CPCONLY	B01F2215/0463		37
B01F2215/0468	11	Numerical pressure values	CPCONLY	B01F2215/0468		235
B01F2215/0472	11	Numerical temperature values	CPCONLY	B01F2215/0472		133
B01F2215/0477	11	Numerical time values	CPCONLY	B01F2215/0477		130
B01F2215/0481	11	Numerical speed values	CPCONLY	B01F2215/0481		283
B01F2215/0486	10	Material property information	CPCONLY	B01F2215/0486		20
B01F2215/049	11	Numerical values of density of substances	CPCONLY	B01F2215/049		11
B01F2215/0495	11	Numerical values of viscosity of substances	CPCONLY	B01F2215/0495		78
