C10H1/00	7	Acetylene gas generators with dropwise, gravity, non-automatic water feed (valves, cocks F16K)	C10H1/00	C10H1/00		687
C10H1/02	8	Valves	C10H1/02	C10H1/02		2
C10H1/04	9	Screw valves	C10H1/04	C10H1/04		1
C10H1/06	9	Cocks	C10H1/06	C10H1/06		2
C10H1/08	8	Other means for controlling the water feed	C10H1/08	C10H1/08		5
C10H1/10	8	Water feed from above through a central or lateral pipe	C10H1/10	C10H1/10		7
C10H1/12	8	Water feed from above through porous materials	C10H1/12	C10H1/12		57
C10H3/00	7	Acetylene gas generators with automatic water feed regulation by means independent of the gas-holder	C10H3/00	C10H3/00		10
C10H3/02	8	with membranes	C10H3/02	C10H3/02		1
C10H3/04	8	with floats	C10H3/04	C10H3/04		1
C10H3/06	8	with pistons	C10H3/06	C10H3/06		
C10H5/00	7	Acetylene gas generators with automatic water feed regulation by the gas-holder	C10H5/00	C10H5/00		592
C10H5/02	8	with overflow for the water	C10H5/02	C10H5/02		1
C10H5/04	8	by drop-by-drop water valves connected with the gas-holder	C10H5/04	C10H5/04		
C10H5/06	9	by drop-by-drop water cocks connected with the gas-holder	C10H5/06	C10H5/06		
C10H5/08	8	with gas-holder-connected water valves or cocks according to the submersion system	C10H5/08	C10H5/08		
C10H7/00	7	Acetylene gas generators with water feed by Kipp&apos;s principle	C10H7/00	C10H7/00		2
C10H7/02	8	with water feed from below	C10H7/02	C10H7/02		
C10H7/04	8	with water feed from above	C10H7/04	C10H7/04		
C10H9/00	7	Acetylene gas generators according to Dobereiner&apos;s principle with fixed carbide bell	C10H9/00	C10H9/00		576
C10H9/02	8	with water feed from below through porous materials (by capillary feed)	C10H9/02	C10H9/02		2
C10H9/04	8	with gas cock actuated by the gas holder	C10H9/04	C10H9/04		
C10H9/06	8	with the depth of the gas outlet pipe regulated by the gas-holder	C10H9/06	C10H9/06		
C10H9/08	8	with movable gas-holder	C10H9/08	C10H9/08		
C10H9/10	8	by wetting the carbide only at the bottom	C10H9/10	C10H9/10		
C10H11/00	7	Acetylene gas generators with submersion of the carbide in water	C10H11/00	C10H11/00		20
C10H11/02	8	inside the gas-holder	C10H11/02	C10H11/02		2
C10H11/04	8	with sealing and reaction water separated from each other	C10H11/04	C10H11/04		
C10H13/00	7	Acetylene gas generation with combined dipping and drop-by-drop system	C10H13/00	C10H13/00		204
C10H15/00	7	Acetylene gas generators with carbide feed, with or without regulation by the gas pressure	C10H15/00	C10H15/00		49
C10H15/02	8	with non-automatic carbide feed	C10H15/02	C10H15/02		93
C10H15/04	9	Closure means at the filling-hopper	C10H15/04	C10H15/04		
C10H15/06	8	with automatic carbide feed by valves	C10H15/06	C10H15/06		713
C10H15/08	9	by flap or slide valves	C10H15/08	C10H15/08		1
C10H15/10	9	by float valves	C10H15/10	C10H15/10		
C10H15/12	9	by measuring valves, including pocket-wheels	C10H15/12	C10H15/12		257
C10H15/14	8	with feed worm or feed conveyors	C10H15/14	C10H15/14		7
C10H15/16	8	with feed drums	C10H15/16	C10H15/16		1
C10H15/18	8	with movable feed disc and fixed carbide-receptacle	C10H15/18	C10H15/18		1
C10H15/20	8	with carbide feed by cartridges or other packets	C10H15/20	C10H15/20		36
C10H15/22	8	with carbide feed of pulverous carbide from receptacles or through the gas-holder	C10H15/22	C10H15/22		31
C10H15/24	8	with carbide feed by pistons	C10H15/24	C10H15/24		
C10H17/00	7	High-pressure acetylene gas generators	C10H17/00	C10H17/00		2
C10H19/00	7	Other acetylene gas generators	C10H19/00	C10H19/00		41
C10H19/02	8	Rotary carbide receptacles	C10H19/02	C10H19/02		2
C10H21/00	7	Details of acetylene generators; Accessory equipment for, or features of, the wet production of acetylene	C10H21/00	C10H21/00		375
C10H21/02	8	Packages of carbide for use in generators, e.g. cartridges	C10H21/02	C10H21/02		71
C10H21/04	9	Placing packages in the generator	C10H21/04	C10H21/04		2
C10H21/06	10	Opening devices for packages in the generator	C10H21/06	C10H21/06		1
C10H21/08	8	Safety devices for acetylene generators	C10H21/08	C10H21/08		100
C10H21/10	8	Carbide compositions	C10H21/10	C10H21/10		15
C10H21/12	8	Gas-tight sealing means, e.g. liquid seals in generators	C10H21/12	C10H21/12		5
C10H21/14	8	Ventilation means; Cooling devices	C10H21/14	C10H21/14		7
C10H21/16	8	Removing sludge from generators	C10H21/16	C10H21/16		155
