F42B1/00	7	Explosive charges characterised by form or shape but not dependent on shape of container	F42B1/00	F42B1/00		303
F42B1/02	8	Shaped or hollow charges (blasting cartridges with cavities in the charge F42B3/08; oil winning using shaped-charge perforators E21B43/116)	F42B1/02	F42B1/02		585
F42B1/024	9	provided with embedded bodies of inert material	F42B1/024	F42B1/024		161
F42B1/028	9	characterised by the form of the liner	F42B1/028	F42B1/028		427
F42B1/032	9	characterised by the material of the liner	F42B1/032	F42B1/032		356
F42B1/036	9	Manufacturing processes therefor {(F42B33/0214&#160;-&#160;F42B33/0292 take precedence)}	F42B1/036	F42B1/036		241
F42B1/04	8	Detonator charges not forming part of the fuze	F42B1/04	F42B1/04		61
F42B3/00	7	Blasting cartridges, i.e. case and explosive (fuse cords, e.g. detonating fuse cords C06C5/00; chemical aspects of detonators, blasting caps or primers C06C7/00)	F42B3/00	F42B3/00		754
F42B3/003	8	{Liquid-oxygen cartridges}	F42B3/00	F42B3/00		45
F42B3/006	8	{Explosive bolts; Explosive actuators (explosive valves F16K13/06; explosive cutting B23D15/145; explosive switches H01H39/00; pyrotechnical actuators F15B15/19)}	F42B3/00	F42B3/00		432
F42B3/02	8	adapted to be united into assemblies	F42B3/02	F42B3/02		349
F42B3/04	8	for producing gas under pressure {(generators of inflation fluid especially adapted for vehicle air bags B60R21/26)}	F42B3/04	F42B3/04		902
F42B3/045	9	{Hybrid systems with previously pressurised gas using blasting to increase the pressure, e.g. causing the gas to be released from its sealed container}	F42B3/04	F42B3/04		189
F42B3/06	9	with re-utilisable case	F42B3/06	F42B3/06		275
F42B3/08	8	with cavities in the charge, e.g. hollow-charge blasting cartridges	F42B3/08	F42B3/08		383
F42B3/087	8	Flexible or deformable blasting cartridges, e.g. bags or hoses {for slurries}(loaded cartridge bags F42B5/38)	F42B3/087	F42B3/087		194
F42B3/093	9	in mat or tape form	F42B3/093	F42B3/093		78
F42B3/10	8	Initiators therefor (percussion fuzes F42C7/00; percussion caps F42C19/10; electric primers F42C19/12)<br><br><u>NOTE</u><br><br>Group F42B3/18 takes precedence over groups F42B3/103&#160;-&#160;F42B3/16.	F42B3/10	F42B3/10		847
F42B3/103	9	Mounting initiator heads in initiators; Sealing-plugs	F42B3/103	F42B3/103		616
F42B3/107	10	Sealing-plugs characterised by the material used	F42B3/107	F42B3/107		51
F42B3/11	9	characterised by the material used, e.g. for initiator case or electric leads (F42B3/107 takes precedence)	F42B3/11	F42B3/11		287
F42B3/113	9	activated by optical means, e.g. laser, flashlight	F42B3/113	F42B3/113		278
F42B3/117	9	activated by friction	F42B3/117	F42B3/117		69
F42B3/12	9	Bridge initiators {(F42B3/103, F42B3/11, F42B3/195 take precedence; electric ignitors in propellant charges F42C19/12)}	F42B3/12	F42B3/12		297
F42B3/121	10	{Initiators with incorporated integrated circuit}	F42B3/12	F42B3/12		197
F42B3/122	11	{Programmable electronic delay initiators}	F42B3/12	F42B3/12		73
F42B3/124	10	{characterised by the configuration or material of the bridge (F42B3/13 takes precedence)}	F42B3/12	F42B3/12		360
F42B3/125	10	{characterised by the configuration of the bridge initiator case (F42B3/11 takes precedence)}	F42B3/12	F42B3/12		153
F42B3/127	11	{the case having burst direction defining elements}	F42B3/12	F42B3/12		57
F42B3/128	10	{characterised by the composition of the pyrotechnic material}	F42B3/12	F42B3/12		100
F42B3/13	10	with semiconductive bridge	F42B3/13	F42B3/13		180
F42B3/14	9	Spark initiators {(F42B3/195 takes precedence)}	F42B3/14	F42B3/14		132
F42B3/16	9	{Pyrotechnic} delay initiators (F42B3/195 takes precedence; {programmable electronic delay initiators F42C11/065})	F42B3/16	F42B3/16		330
F42B3/18	9	Safety initiators resistant to premature firing by static electricity or stray currents	F42B3/18	F42B3/18		333
F42B3/182	10	having shunting means {(F42B3/185 takes precedence; details of shunting devices H01R13/7032)}	F42B3/182	F42B3/182		144
F42B3/185	10	having semi-conductive {means, e.g.} sealing plugs	F42B3/185	F42B3/185		45
F42B3/188	10	having radio-frequency filters {, e.g. containing ferrite cores or inductances (F42B3/185 takes precedence)}	F42B3/188	F42B3/188		80
F42B3/192	9	designed for neutralisation on contact with water	F42B3/192	F42B3/192		42
F42B3/195	9	Manufacture	F42B3/195	F42B3/195		348
F42B3/198	10	of electric initiator heads {e.g., testing, machines}	F42B3/198	F42B3/198		214
F42B3/22	8	Elements for controlling or guiding the detonation wave, e.g. tubes (using inert bodies embedded in shaped or hollow charges F42B1/024)	F42B3/22	F42B3/22		211
F42B3/24	8	Cartridge closures or seals (top closures for shotgun ammunition cartridges F42B7/12)	F42B3/24	F42B3/24		125
F42B3/26	8	Arrangements for mounting initiators; Accessories therefor, e.g. tools	F42B3/26	F42B3/26		410
F42B3/28	8	Cartridge cases characterised by the material used, e.g. coatings (for initiator cases F42B3/11)	F42B3/28	F42B3/28		353
F42B4/00	7	Fireworks, i.e. pyrotechnic devices for amusement, display, illumination or signal purposes (signalling by explosives G08B; advertising by fireworks G09F13/46; {signalling by pyrotechnics in railway systems B61L5/20})	F42B4/00	F42B4/00		630
F42B4/02	8	in cartridge form, i.e. shell, propellant and primer	F42B4/02	F42B4/02		168
F42B4/04	8	Firecrackers	F42B4/04	F42B4/04		385
F42B4/06	8	Aerial display rockets (rockets in general F42B15/00)	F42B4/06	F42B4/06		174
F42B4/08	9	characterised by having vanes, wings, parachutes or balloons	F42B4/08	F42B4/08		27
F42B4/10	9	characterised by having means to separate article or charge from casing without destroying the casing	F42B4/10	F42B4/10		17
F42B4/12	10	Parachute or flare separation	F42B4/12	F42B4/12		32
F42B4/14	9	characterised by having plural successively-ignited charges	F42B4/14	F42B4/14		45
F42B4/16	8	Hand-thrown impact-exploded noise makers; {Other noise-makers generating noise via a pyrotechnic charge}(cap pistols F41C3/06)	F42B4/16	F42B4/16		128
F42B4/18	8	Simulations, e.g. pine cone, house that is destroyed, warship, volcano	F42B4/18	F42B4/18		204
F42B4/20	8	characterised by having holder or support other than casing, e.g. whirler or spike support {(supports for flares or torches F42B4/26)}	F42B4/20	F42B4/20		353
F42B4/22	8	characterised by having means to separate article or charge from casing without destroying the casing (in aerial display rockets F42B4/10)	F42B4/22	F42B4/22		118
F42B4/24	8	characterised by having plural successively-ignited charges (in aerial display rockets F42B4/14)	F42B4/24	F42B4/24		200
F42B4/26	8	Flares; Torches {(mines for practice or training containing flares or illuminating charges F42B8/28; projectiles of illuminating type F42B12/42)}	F42B4/26	F42B4/26		606
F42B4/28	9	Parachute flares (F42B4/12 takes precedence)	F42B4/28	F42B4/28		111
F42B4/30	8	Manufacture	F42B4/30	F42B4/30		976
F42B5/00	7	Cartridge ammunition, e.g. separately-loaded propellant charges (shotgun ammunition F42B7/00; practice or training ammunition F42B8/00; missiles therefor F42B12/00, F42B14/00, F42B15/00)	F42B5/00	F42B5/00		65
F42B5/02	8	Cartridges, i.e. cases with charge and missile	F42B5/02	F42B5/02		621
F42B5/025	9	{characterised by the dimension of the case or the missile}	F42B5/02	F42B5/02		386
F42B5/03	9	containing more than one missile	F42B5/03	F42B5/03		139
F42B5/035	10	{the cartridge or barrel assembly having a plurality of axially stacked projectiles each having a separate propellant charge}	F42B5/03	F42B5/03		164
F42B5/045	9	of telescopic type (F42B5/184 takes precedence)	F42B5/045	F42B5/045		204
F42B5/05	9	for recoilless guns (recoilless guns using a counter-projectile to balance recoil F41A1/10)	F42B5/05	F42B5/05		94
F42B5/067	9	Mounting or locking missiles in cartridge cases (F42B5/18 takes precedence)	F42B5/067	F42B5/067		198
F42B5/073	10	using an auxiliary locking element	F42B5/073	F42B5/073		108
F42B5/08	9	modified for electric ignition	F42B5/08	F42B5/08		294
F42B5/10	9	with self-propelled bullet	F42B5/10	F42B5/10		146
F42B5/105	10	{propelled by two propulsive charges, the rearwardly situated one being separated from the rest of the projectile during flight or in the barrel; Projectiles with self-ejecting cartridge cases}	F42B5/10	F42B5/10		95
F42B5/145	9	for dispensing gases, vapours, powders, particles or chemically-reactive substances (from projectiles F42B12/46)	F42B5/145	F42B5/145		164
F42B5/15	10	for creating a screening or decoy effect, e.g. using radar chaff or infrared material (infrared flares F42B4/26)	F42B5/15	F42B5/15		189
F42B5/155	11	Smoke-pot projectors, e.g. arranged on vehicles	F42B5/155	F42B5/155		107
F42B5/16	9	characterised by composition or physical dimensions or form of propellant charge, {with or without projectile,} or powder (chemical composition C06B; {F42B5/24 takes precedence})	F42B5/16	F42B5/16		651
F42B5/18	9	Caseless ammunition; Cartridges having combustible cases	F42B5/18	F42B5/18		290
F42B5/181	10	{consisting of a combustible casing wall and a metal base; Connectors therefor}	F42B5/18	F42B5/18		137
F42B5/182	10	{Caseless cartridges characterised by their shape}	F42B5/18	F42B5/18		29
F42B5/184	10	telescopic	F42B5/184	F42B5/184		54
F42B5/188	10	Manufacturing processes therefor	F42B5/188	F42B5/188		137
F42B5/192	10	Cartridge cases characterised by the material {of the casing wall (cartridge bags F42B5/38)}	F42B5/192	F42B5/192		95
F42B5/196	11	Coatings	F42B5/196	F42B5/196		44
F42B5/24	9	for cleaning; for cooling; for lubricating {; for wear reducing}	F42B5/24	F42B5/24		196
F42B5/26	8	Cartridge cases (F42B5/18 takes precedence {; manufacturing of cartridge cases B21K21/04})	F42B5/26	F42B5/26		552
F42B5/28	9	of metal {, i.e. the cartridge-case tube is of metal}	F42B5/28	F42B5/28		190
F42B5/285	10	formed by assembling several elements	F42B5/285	F42B5/285		199
F42B5/29	11	wound from sheets or strips	F42B5/29	F42B5/29		36
F42B5/295	10	coated	F42B5/295	F42B5/295		71
F42B5/297	11	with plastics	F42B5/297	F42B5/297		13
F42B5/30	9	of plastics {, i.e. the cartridge-case tube is of plastics}	F42B5/30	F42B5/30		275
F42B5/307	10	formed by assembling several elements	F42B5/307	F42B5/307		252
F42B5/313	11	all elements made of plastics	F42B5/313	F42B5/313		107
F42B5/32	9	for rim fire	F42B5/32	F42B5/32		92
F42B5/34	9	with provision for varying the length	F42B5/34	F42B5/34		20
F42B5/36	9	modified for housing an integral firing-cap	F42B5/36	F42B5/36		263
F42B5/38	8	Separately-loaded propellant charges, e.g. cartridge bags {(F42B5/16, F42B5/192 take precedence)}	F42B5/38	F42B5/38		319
F42B6/00	7	Projectiles or missiles specially adapted for projection without use of explosive or combustible propellant charge, e.g. for blow guns, bows or crossbows, hand-held spring or air guns (for delivering hypodermic charges F42B12/54; projectiles or missiles incorporating springs as the projecting means F41B7/02; {Arrows or darts for dispensing materials, for producing chemical or physical reaction, or for signalling F42B12/362})	F42B6/00	F42B6/00		225
F42B6/003	8	{Darts}	F42B6/00	F42B6/00		643
F42B6/006	8	{Projectiles for electromagnetic or plasma guns}	F42B6/00	F42B6/00		72
F42B6/02	8	Arrows; Crossbow bolts; Harpoons for hand-held spring or air guns	F42B6/02	F42B6/02		169
F42B6/04	9	Archery arrows (F42B6/08, F41B5/06, {F42B12/362} take precedence)	F42B6/04	F42B6/04		506
F42B6/06	10	Tail ends, e.g. nocks, fletching	F42B6/06	F42B6/06		406
F42B6/08	9	Arrow heads; Harpoon heads	F42B6/08	F42B6/08		792
F42B6/10	8	Air gun pellets {; Ammunition for air guns, e.g. propellant-gas containers}	F42B6/10	F42B6/10		307
F42B7/00	7	Shotgun ammunition	F42B7/00	F42B7/00		58
F42B7/02	8	Cartridges, i.e. cases with propellant charge and missile	F42B7/02	F42B7/02		107
F42B7/04	9	of pellet type	F42B7/04	F42B7/04		394
F42B7/043	10	{with shot-scattering means}	F42B7/04	F42B7/04		60
F42B7/046	10	{Pellets or shot therefor}	F42B7/04	F42B7/04		192
F42B7/06	9	with cartridge case of plastics {(F42B5/30 takes precedence)}	F42B7/06	F42B7/06		131
F42B7/08	9	Wads, {i.e. projectile or shot carrying devices,} therefor	F42B7/08	F42B7/08		743
F42B7/10	9	Ball or slug shotgun cartridges	F42B7/10	F42B7/10		258
F42B7/12	9	Cartridge top closures, i.e. for the missile side (closures for blasting cartridges F42B3/24)	F42B7/12	F42B7/12		200
F42B8/00	7	Practice or training ammunition	F42B8/00	F42B8/00		80
F42B8/02	8	Cartridges {(F41A33/02, F42B7/12 take precedence)}	F42B8/02	F42B8/02		270
F42B8/04	9	Blank cartridges, i.e. primed cartridges without projectile but containing an explosive or combustible powder charge	F42B8/04	F42B8/04		254
F42B8/06	10	for cap-firing pistols	F42B8/06	F42B8/06		83
F42B8/08	9	Dummy cartridges, i.e. inert cartridges containing neither primer nor explosive or combustible powder charge	F42B8/08	F42B8/08		89
F42B8/10	9	with sub-calibre adaptor	F42B8/10	F42B8/10		166
F42B8/12	8	Projectiles or missiles (F42B10/48, F42B12/36, F42B19/36 take precedence)	F42B8/12	F42B8/12		270
F42B8/14	9	disintegrating in flight or upon impact<br><br><u>NOTE</u><br><br>Group F42B8/14 takes precedence over groups F42B8/18&#160;-&#160;F42B8/26	F42B8/14	F42B8/14		191
F42B8/16	10	containing an inert filler in powder or granular form	F42B8/16	F42B8/16		145
F42B8/18	9	Rifle grenades	F42B8/18	F42B8/18		71
F42B8/20	9	Mortar grenades	F42B8/20	F42B8/20		90
F42B8/22	9	Fall bombs	F42B8/22	F42B8/22		69
F42B8/24	9	Rockets	F42B8/24	F42B8/24		102
F42B8/26	9	Hand grenades	F42B8/26	F42B8/26		292
F42B8/28	8	Land or marine mines; Depth charges	F42B8/28	F42B8/28		164
F42B10/00	7	Means for influencing, e.g. improving, the aerodynamic properties of projectiles or missiles; Arrangements on projectiles or missiles for stabilising, steering, range-reducing, range-increasing or fall-retarding (F42B6/00 takes precedence)	F42B10/00	F42B10/00		126
F42B10/02	8	Stabilising arrangements	F42B10/02	F42B10/02		260
F42B10/025	9	{using giratory or oscillating masses for stabilising projectile trajectory}	F42B10/02	F42B10/02		38
F42B10/04	9	using fixed fins (F42B10/22 takes precedence)	F42B10/04	F42B10/04		116
F42B10/06	10	Tail fins	F42B10/06	F42B10/06		559
F42B10/08	11	Flechette-type projectiles	F42B10/08	F42B10/08		76
F42B10/10	11	the fins being formed in the barrel by deformation or the projectile body	F42B10/10	F42B10/10		10
F42B10/12	9	using fins longitudinally-slidable with respect to the projectile or missile	F42B10/12	F42B10/12		98
F42B10/14	9	using fins spread or deployed after launch, e.g. after leaving the barrel	F42B10/14	F42B10/14		989
F42B10/143	10	{Lattice or grid fins}	F42B10/14	F42B10/14		44
F42B10/146	10	{Fabric fins, i.e. fins comprising at least one spar and a fin cover made of flexible sheet material}	F42B10/14	F42B10/14		41
F42B10/16	10	Wrap-around fins	F42B10/16	F42B10/16		296
F42B10/18	10	using a longitudinally slidable support member	F42B10/18	F42B10/18		79
F42B10/20	10	deployed by combustion gas pressure, or by pneumatic or hydraulic forces	F42B10/20	F42B10/20		139
F42B10/22	9	Projectiles of cannelured type	F42B10/22	F42B10/22		115
F42B10/24	10	with inclined grooves	F42B10/24	F42B10/24		78
F42B10/26	9	using spin (F42B10/04, F42B10/12, F42B10/14, F42B10/24, F42B14/02 take precedence)	F42B10/26	F42B10/26		345
F42B10/28	10	induced by gas action	F42B10/28	F42B10/28		54
F42B10/30	11	using rocket motor nozzles	F42B10/30	F42B10/30		246
F42B10/32	8	Range-reducing or range-increasing arrangements; Fall-retarding means	F42B10/32	F42B10/32		39
F42B10/34	9	Tubular projectiles	F42B10/34	F42B10/34		181
F42B10/36	10	Ring-foil projectiles	F42B10/36	F42B10/36		36
F42B10/38	9	Range-increasing arrangements (F42B10/34, F42B14/06{and F42B15/105} take precedence)	F42B10/38	F42B10/38		314
F42B10/40	10	with combustion of a slow-burning charge, e.g. fumers, base-bleed projectiles	F42B10/40	F42B10/40		163
F42B10/42	10	Streamlined projectiles	F42B10/42	F42B10/42		160
F42B10/44	11	Boat-tails specially adapted for drag reduction	F42B10/44	F42B10/44		138
F42B10/46	11	Streamlined nose cones; Windshields; Radomes {(F42B12/105 takes precedence)}	F42B10/46	F42B10/46		438
F42B10/48	9	Range-reducing, destabilising or braking arrangements, {e.g. impact-braking arrangements}; Fall-retarding means, {e.g. balloons, rockets for braking or fall-retarding}(F42B10/34 takes precedence)	F42B10/48	F42B10/48		344
F42B10/50	10	Brake flaps {, e.g. inflatable}	F42B10/50	F42B10/50		214
F42B10/52	10	Nose cones	F42B10/52	F42B10/52		58
F42B10/54	10	Spin braking means	F42B10/54	F42B10/54		90
F42B10/56	10	of parachute {or paraglider} type	F42B10/56	F42B10/56		589
F42B10/58	10	of rotochute type	F42B10/58	F42B10/58		70
F42B10/60	8	Steering arrangements (F42B19/01 takes precedence)	F42B10/60	F42B10/60		176
F42B10/62	9	Steering by movement of flight surfaces	F42B10/62	F42B10/62		167
F42B10/64	10	of fins	F42B10/64	F42B10/64		747
F42B10/66	9	Steering by varying intensity or direction of thrust (thrust vector control of rocket engine plants F02K9/80{; guiding or controlling apparatus using jets adapted for cosmonautic vehicles B64G1/26})	F42B10/66	F42B10/66		174
F42B10/661	10	{using several transversally acting rocket motors, each motor containing an individual propellant charge, e.g. solid charge}	F42B10/66	F42B10/66		184
F42B10/663	10	{using a plurality of transversally acting auxiliary nozzles, which are opened or closed by valves}	F42B10/66	F42B10/66		249
F42B10/665	10	{characterised by using a nozzle provided with at least a deflector mounted within the nozzle}	F42B10/66	F42B10/66		107
F42B10/666	10	{characterised by using a nozzle rotatable about an axis transverse to the axis of the projectile}	F42B10/66	F42B10/66		89
F42B10/668	10	{Injection of a fluid, e.g. a propellant, into the gas shear in a nozzle or in the boundary layer at the outer surface of a missile, e.g. to create a shock wave in a supersonic flow}	F42B10/66	F42B10/66		56
F42B12/00	7	Projectiles, missiles or mines characterised by the warhead, the intended effect, or the material (F42B6/00, F42B10/00, F42B14/00 take precedence; for practice or training F42B8/12, F42B8/28; self-propulsion or guidance aspects F42B15/00)	F42B12/00	F42B12/00		121
F42B12/02	8	characterised by the warhead or the intended effect	F42B12/02	F42B12/02		373
F42B12/04	9	of armour-piercing type	F42B12/04	F42B12/04		171
F42B12/06	10	with hard or heavy core; Kinetic energy penetrators (F42B12/16, F42B12/74 take precedence)	F42B12/06	F42B12/06		743
F42B12/08	10	with armour-piercing caps; with armoured cupola	F42B12/08	F42B12/08		152
F42B12/10	10	with shaped or hollow charge (shaped or hollow charges per seF42B1/02{; mines having hollow charges F42B23/04})	F42B12/10	F42B12/10		413
F42B12/105	11	{Protruding target distance or stand-off members therefor, e.g. slidably mounted (fuze aspects F42C1/14)}	F42B12/10	F42B12/10		88
F42B12/12	11	rotatably mounted with respect to missile housing	F42B12/12	F42B12/12		52
F42B12/14	11	the symmetry axis of the hollow charge forming an angle with the longitudinal axis of the projectile	F42B12/14	F42B12/14		110
F42B12/16	11	in combination with an additional projectile or charge, acting successively on the target {(see also F42B12/625)}	F42B12/16	F42B12/16		172
F42B12/18	12	Hollow charges in tandem arrangement	F42B12/18	F42B12/18		149
F42B12/20	9	of high-explosive type (F42B12/44 takes precedence)	F42B12/20	F42B12/20		295
F42B12/201	10	{characterised by target class}	F42B12/20	F42B12/20		24
F42B12/202	11	{for attacking land area or area targets, e.g. airburst}	F42B12/20	F42B12/20		67
F42B12/204	11	{for attacking structures, e.g. specific buildings or fortifications, ships or vehicles}	F42B12/20	F42B12/20		563
F42B12/205	11	{for attacking aerial targets}	F42B12/20	F42B12/20		50
F42B12/207	10	{characterised by the explosive material or the construction of the high explosive warhead, e.g. insensitive ammunition}	F42B12/20	F42B12/20		210
F42B12/208	10	{characterised by a plurality of charges within a single high explosive warhead}	F42B12/20	F42B12/20		160
F42B12/22	10	with fragmentation-hull construction	F42B12/22	F42B12/22		393
F42B12/24	11	with grooves, recesses or other wall weakenings {(F42B12/26, F42B12/28 take precedence)}	F42B12/24	F42B12/24		211
F42B12/26	11	the projectile wall being formed by a spirally-wound element	F42B12/26	F42B12/26		48
F42B12/28	11	the projectile wall being built from annular elements	F42B12/28	F42B12/28		46
F42B12/30	11	Continuous-rod warheads	F42B12/30	F42B12/30		34
F42B12/32	11	the hull or case comprising a plurality of discrete bodies, e.g. steel balls, embedded therein {or disposed around the explosive charge}	F42B12/32	F42B12/32		562
F42B12/34	9	expanding before or on impact, i.e. of dumdum or mushroom type	F42B12/34	F42B12/34		770
F42B12/36	9	for dispensing materials; for producing chemical or physical reaction; for signalling {; for transmitting information}	F42B12/36	F42B12/36		618
F42B12/362	10	{Arrows or darts (F42B12/38 takes precedence, having means for implantation, e.g. hypodermic projectiles F42B12/54; arrows or darts in general F42B6/00)}	F42B12/36	F42B12/36		221
F42B12/365	10	{Projectiles transmitting information to a remote location using optical or electronic means (F42B12/385 takes precedence)}	F42B12/36	F42B12/36		304
F42B12/367	10	{Projectiles fragmenting upon impact without the use of explosives, the fragments creating a wounding or lethal effect (practice or training projectiles disintegrating upon impact F42B8/14; projectiles of high-explosive type with fragmentation-hull construction F42B12/22)}	F42B12/36	F42B12/36		147
F42B12/38	10	of tracer type	F42B12/38	F42B12/38		378
F42B12/382	11	{emitting an electromagnetic radiation, e.g. laser beam or infrared emission}	F42B12/38	F42B12/38		156
F42B12/385	12	{Arrow or dart carrying a radio transmitter for signalling}	F42B12/38	F42B12/38		106
F42B12/387	11	{Passive tracers, e.g. using a reflector mounted on the projectile}	F42B12/38	F42B12/38		39
F42B12/40	10	of target-marking, i.e. impact-indicating type (F42B12/48, {F42B12/50} take precedence)	F42B12/40	F42B12/40		592
F42B12/42	10	of illuminating type, e.g. carrying flares	F42B12/42	F42B12/42		334
F42B12/44	10	of incendiary type (F42B12/46 takes precedence)	F42B12/44	F42B12/44		560
F42B12/46	10	for dispensing gases, vapours, powders or chemically-reactive substances (F42B12/70 takes precedence)	F42B12/46	F42B12/46		596
F42B12/48	11	smoke-producing {, e.g. infrared clouds}	F42B12/48	F42B12/48		413
F42B12/50	11	by dispersion	F42B12/50	F42B12/50		634
F42B12/52	12	Fuel-air explosive devices	F42B12/52	F42B12/52		101
F42B12/54	11	by implantation, e.g. hypodermic projectiles	F42B12/54	F42B12/54		208
F42B12/56	10	for dispensing discrete solid bodies (F42B12/70 takes precedence)	F42B12/56	F42B12/56		172
F42B12/58	11	Cluster or cargo ammunition, i.e. projectiles containing one or more submissiles (F42B12/32 takes precedence)	F42B12/58	F42B12/58		588
F42B12/60	12	the submissiles being ejected radially	F42B12/60	F42B12/60		270
F42B12/62	12	the submissiles being ejected parallel to the longitudinal axis of the projectile	F42B12/62	F42B12/62		310
F42B12/625	13	{a single submissile arranged in a carrier missile for being launched or accelerated coaxially; Coaxial tandem arrangement of missiles which are active in the target one after the other (with shaped or hollow charges F42B12/16)}	F42B12/62	F42B12/62		169
F42B12/64	13	the submissiles being of shot- or flechette-type	F42B12/64	F42B12/64		189
F42B12/66	12	Chain-shot, i.e. the submissiles being interconnected by chains or the like {(ballistically deployed systems for restraining persons or animals F41H13/0006)}	F42B12/66	F42B12/66		302
F42B12/68	11	Line-carrying missiles, e.g. for life-saving (harpoons F42B30/14{, mine-clearing snakes F41H11/14})	F42B12/68	F42B12/68		431
F42B12/70	11	for dispensing radar chaff or infrared material (radar-reflector targets, active targets transmitting infrared radiation F41J2/00; radar-reflecting surfaces H01Q15/14)	F42B12/70	F42B12/70		327
F42B12/72	8	characterised by the material (heat treatment for explosive shells C21D9/16)	F42B12/72	F42B12/72		212
F42B12/74	9	of the core or solid body	F42B12/74	F42B12/74		821
F42B12/745	10	{the core being made of plastics; Compounds or blends of plastics and other materials, e.g. fillers}	F42B12/74	F42B12/74		267
F42B12/76	9	of the casing	F42B12/76	F42B12/76		459
F42B12/78	10	of jackets for smallarm bullets {; Jacketed bullets or projectiles}	F42B12/78	F42B12/78		384
F42B12/80	10	Coatings	F42B12/80	F42B12/80		146
F42B12/82	11	reducing friction	F42B12/82	F42B12/82		38
F42B14/00	7	Projectiles or missiles characterised by arrangements for guiding or sealing them inside barrels, or for lubricating or cleaning barrels	F42B14/00	F42B14/00		121
F42B14/02	8	Driving bands; Rotating bands (F42B14/04 takes precedence)	F42B14/02	F42B14/02		759
F42B14/04	8	Lubrication means in missiles (coatings for reducing friction F42B12/82)	F42B14/04	F42B14/04		140
F42B14/06	8	Sub-calibre projectiles having sabots; Sabots therefor	F42B14/06	F42B14/06		243
F42B14/061	9	{Sabots for long rod fin stabilised kinetic energy projectiles, i.e. multisegment sabots attached midway on the projectile}	F42B14/06	F42B14/06		319
F42B14/062	10	{characterised by contact surfaces between projectile and sabot}	F42B14/06	F42B14/06		56
F42B14/064	9	{Sabots enclosing the rear end of a kinetic energy projectile, i.e. having a closed disk shaped obturator base and petals extending forward from said base}	F42B14/06	F42B14/06		435
F42B14/065	9	{Sabots carrying several projectiles}	F42B14/06	F42B14/06		33
F42B14/067	9	{Sealing aspects in sabots, e.g. sealing between individual segments of the sabots or sealing between the outer surface of the sabot and the inner surface of the barrel}	F42B14/06	F42B14/06		82
F42B14/068	9	{Sabots characterised by the material (F42B14/067 takes precedence)}	F42B14/06	F42B14/06		77
F42B14/08	9	Sabots filled with propulsive charges; Removing sabots by combustion of pyrotechnic elements or by propulsive-gas pressure (arrangements on barrels for removing sabots from projectiles F41A21/46)	F42B14/08	F42B14/08		56
F42B15/00	7	Self-propelled projectiles or missiles, e.g. rockets; Guided missiles (F42B10/00, F42B12/00, F42B14/00 take precedence; for practice or training F42B8/12; rocket torpedoes F42B17/00; marine torpedoes F42B19/00; cosmonautic vehicles B64G; jet-propulsion plants F02K)	F42B15/00	F42B15/00		1754
F42B15/01	8	Arrangements thereon for guidance or control ({steering arrangements F42B10/60}; aircraft flight control B64C; guidance systems other than those installed aboard F41G7/00, F41G9/00; locating by use of radio or other waves G01S; flight control in general G05D1/00; computer aspects G06])	F42B15/01	F42B15/01		1960
F42B15/04	9	using wire, e.g. for guiding ground-to-ground rockets	F42B15/04	F42B15/04		186
F42B15/08	8	for carrying measuring instruments; {Arrangements for mounting sensitive cargo within a projectile}(adaptations for meteorology G01W1/08); {Arrangements for acoustic sensitive cargo within a projectile}	F42B15/08	F42B15/08		160
F42B15/10	8	Missiles having a trajectory only in the air	F42B15/10	F42B15/10		218
F42B15/105	9	{Air torpedoes, e.g. projectiles with or without propulsion, provided with supporting air foil surfaces}	F42B15/10	F42B15/10		124
F42B15/12	9	Intercontinental ballistic missiles (F42B15/01 takes precedence)	F42B15/12	F42B15/12		26
F42B15/20	8	Missiles having a trajectory beginning below water surface (having additional propulsion means for movement through water F42B17/00)	F42B15/20	F42B15/20		77
F42B15/22	8	Missiles having a trajectory finishing below water surface (having additional propulsion means for movement through water F42B17/00)	F42B15/22	F42B15/22		103
F42B15/34	8	Protection against overheating or radiation, e.g. heat shields; Additional cooling arrangements {(thermal protection fitted in or to cosmonautic vehicles B64G1/58)}	F42B15/34	F42B15/34		290
F42B15/36	8	Means for interconnecting rocket-motor and body section; Multi-stage connectors; Disconnecting means	F42B15/36	F42B15/36		988
F42B15/38	9	Ring-shaped explosive elements for the separation of rocket parts {(systems for coupling or separating cosmonautic vehicles or parts thereof B64G1/64)}	F42B15/38	F42B15/38		157
F42B17/00	7	Rocket torpedoes, i.e. missiles provided with separate propulsion means for movement through air and through water (F42B12/00 takes precedence)	F42B17/00	F42B17/00		130
F42B19/00	7	Marine torpedoes, e.g. launched by surface vessels or submarines (having additional propulsion means for movement through air F42B17/00); Sea mines having self-propulsion means (F42B12/00 takes precedence; launching means F41F; locating by use of radio or other waves G01S; automatic control of course G05D1/00; firing directors or calculators G06G)	F42B19/00	F42B19/00		374
F42B19/005	8	{Nose caps for torpedoes; Coupling torpedo-case parts together}	F42B19/00	F42B19/00		90
F42B19/01	8	Steering control	F42B19/01	F42B19/01		453
F42B19/04	9	Depth control	F42B19/04	F42B19/04		134
F42B19/06	9	Directional control	F42B19/06	F42B19/06		104
F42B19/08	9	with means for preventing rolling or pitching	F42B19/08	F42B19/08		28
F42B19/10	9	remotely controlled, e.g. by sonic or radio control (control systems using wire F41G7/32)	F42B19/10	F42B19/10		122
F42B19/12	8	Propulsion specially adapted for torpedoes (having additional propulsion means for movement through air F42B17/00; marine propulsion in general B63H)	F42B19/12	F42B19/12		153
F42B19/125	9	{Torpedoes provided with drag-reducing means (projectiles with drag-reducing means F42B10/38)}	F42B19/12	F42B19/12		101
F42B19/14	9	by compressed-gas motors	F42B19/14	F42B19/14		25
F42B19/16	10	of cylinder type	F42B19/16	F42B19/16		14
F42B19/18	10	of turbine type	F42B19/18	F42B19/18		48
F42B19/20	10	characterised by the composition of propulsive gas; Manufacture or heating thereof in torpedoes	F42B19/20	F42B19/20		171
F42B19/22	9	by internal-combustion engines	F42B19/22	F42B19/22		29
F42B19/24	9	by electric motors	F42B19/24	F42B19/24		73
F42B19/26	9	by jet propulsion	F42B19/26	F42B19/26		104
F42B19/28	9	with means for avoiding visible wake	F42B19/28	F42B19/28		19
F42B19/30	9	with timing control of propulsion	F42B19/30	F42B19/30		16
F42B19/36	8	adapted to be used for exercise purposes, e.g. indicating position or course	F42B19/36	F42B19/36		53
F42B19/38	9	with means for causing torpedoes to surface at end of run	F42B19/38	F42B19/38		24
F42B19/40	10	by expelling liquid ballast	F42B19/40	F42B19/40		55
F42B19/42	10	by releasing solid ballast	F42B19/42	F42B19/42		13
F42B19/44	10	by enlarging displacement	F42B19/44	F42B19/44		14
F42B19/46	8	adapted to be launched from aircraft	F42B19/46	F42B19/46		91
F42B21/00	7	Depth charges (F42B12/00 takes precedence; for practice or training F42B8/28; laying aspects B63G)	F42B21/00	F42B21/00		100
F42B22/00	7	Marine mines, e.g. launched by surface vessels or submarines (F42B12/00 takes precedence; for practice or training F42B8/28; mine laying or sweeping B63G)	F42B22/00	F42B22/00		126
F42B22/02	8	Contact mines {, e.g. antenne-type mines}(contact fuzes F42C7/02)	F42B22/02	F42B22/02		45
F42B22/04	8	Influenced mines, e.g. by magnetic or acoustic effect	F42B22/04	F42B22/04		136
F42B22/06	8	Ground mines	F42B22/06	F42B22/06		42
F42B22/08	8	Drifting mines (with propulsion means F42B19/00)	F42B22/08	F42B22/08		93
F42B22/10	8	Moored mines	F42B22/10	F42B22/10		278
F42B22/12	9	at a fixed depth setting	F42B22/12	F42B22/12		27
F42B22/14	9	at a variable depth setting	F42B22/14	F42B22/14		9
F42B22/16	10	using mechanical means, e.g. plummet and float	F42B22/16	F42B22/16		50
F42B22/18	10	using hydrostatic means	F42B22/18	F42B22/18		39
F42B22/20	10	using magnetic or acoustic depth-control means	F42B22/20	F42B22/20		10
F42B22/22	8	having self-contained sinking means	F42B22/22	F42B22/22		26
F42B22/24	8	Arrangement of mines in fields or barriers (net barriers for harbour defence F41H11/05)	F42B22/24	F42B22/24		64
F42B22/42	8	with anti-sweeping means, e.g. electrical	F42B22/42	F42B22/42		39
F42B22/44	8	adapted to be launched from aircraft	F42B22/44	F42B22/44		22
F42B23/00	7	Land mines {; Land torpedoes}(F42B12/00 takes precedence; for practice or training F42B8/28)	F42B23/00	F42B23/00		189
F42B23/005	8	{Selfpropelled land mines}	F42B23/00	F42B23/00		25
F42B23/04	8	anti-vehicle {, e.g. anti-aircraft or anti tank (hollow charges per seF42B1/02; artillery projectiles having hollow charges F42B12/10)}	F42B23/04	F42B23/04		144
F42B23/08	9	non-metallic	F42B23/08	F42B23/08		22
F42B23/10	8	anti-personnel	F42B23/10	F42B23/10		77
F42B23/14	9	non-metallic	F42B23/14	F42B23/14		21
F42B23/16	9	of missile type, i.e. {all kinds of mines launched} for detonation after ejection from ground (fuzes for initiating mine ejection F42C1/09)	F42B23/16	F42B23/16		127
F42B23/24	8	Details	F42B23/24	F42B23/24		212
F42B25/00	7	Fall bombs (F42B10/00, F42B12/00 take precedence; for practice or training F42B8/12{; gliding type bombs F42B15/105})	F42B25/00	F42B25/00		232
F42B27/00	7	Hand grenades (F42B12/00 takes precedence; for practice or training F42B8/12)	F42B27/00	F42B27/00		481
F42B27/08	8	with handle	F42B27/08	F42B27/08		152
F42B29/00	7	Noiseless, smokeless, or flashless missiles launched by their own explosive propellant	F42B29/00	F42B29/00		53
F42B30/00	7	Projectiles or missiles, not otherwise provided for, characterised by the ammunition class or type, e.g. by the launching apparatus or weapon used (F42B10/00, F42B12/00, F42B14/00 take precedence)	F42B30/00	F42B30/00		122
F42B30/003	8	{Closures or baseplates therefor (closures for blasting cartridges F42B3/24, for shotgun cartridges F42B7/12)}	F42B30/00	F42B30/00		52
F42B30/006	8	{Mounting of sensors, antennas or target trackers on projectiles}	F42B30/00	F42B30/00		134
F42B30/02	8	Bullets	F42B30/02	F42B30/02		418
F42B30/04	8	Rifle grenades	F42B30/04	F42B30/04		363
F42B30/06	9	Bullet traps or bullet decelerators therefor	F42B30/06	F42B30/06		90
F42B30/08	8	Ordnance projectiles or missiles, e.g. shells	F42B30/08	F42B30/08		259
F42B30/10	9	Mortar projectiles	F42B30/10	F42B30/10		206
F42B30/12	10	with provision for additional propulsive charges, or for varying the length	F42B30/12	F42B30/12		102
F42B30/14	8	Harpoons (for hand-held spring or air guns F42B6/02)	F42B30/14	F42B30/14		211
F42B33/00	7	Manufacture of ammunition; Dismantling of ammunition; Apparatus therefor (F42B5/188 takes precedence; manufacturing processes for hollow charges F42B1/036; manufacture of blasting cartridge initiators F42B3/195)	F42B33/00	F42B33/00		612
F42B33/001	8	{Devices or processes for assembling ammunition, cartridges or cartridge elements from parts}	F42B33/00	F42B33/00		664
F42B33/002	8	{Orienting or guiding means for cartridges or cartridge parts during the manufacturing or packaging process; Feeding cartridge elements to automatic machines}	F42B33/00	F42B33/00		314
F42B33/004	8	{Cartridge loaders of the rotatable-turret type}	F42B33/00	F42B33/00		217
F42B33/005	8	{Crimping cartridge cases on projectiles}	F42B33/00	F42B33/00		59
F42B33/007	8	{Making cavities in an explosive or propulsive charge}	F42B33/00	F42B33/00		17
F42B33/008	8	{Cutting explosive or propulsive charges}	F42B33/00	F42B33/00		27
F42B33/02	8	Filling cartridges, missiles, or fuzes; Inserting propellant or explosive charges {(F42B33/004 takes precedence)}	F42B33/02	F42B33/02		414
F42B33/0207	9	{Processes for loading or filling propulsive or explosive charges in containers}	F42B33/02	F42B33/02		307
F42B33/0214	9	{by casting (F42B33/004 takes precedence)}	F42B33/02	F42B33/02		110
F42B33/0221	10	{by centrifugal casting}	F42B33/02	F42B33/02		15
F42B33/0228	10	{Funnel arrangements therefor}	F42B33/02	F42B33/02		39
F42B33/0235	10	{Heating of casting equipment or explosive charge containers during the loading process}	F42B33/02	F42B33/02		21
F42B33/0242	10	{by pressure casting}	F42B33/02	F42B33/02		26
F42B33/025	9	{by compacting (F42B33/004 takes precedence)}	F42B33/02	F42B33/02		296
F42B33/0257	10	{by vibration compacting}	F42B33/02	F42B33/02		21
F42B33/0264	9	{by using screw-type feeders (F42B33/004 takes precedence)}	F42B33/02	F42B33/02		32
F42B33/0271	10	{for extruding blasting cartridges}	F42B33/02	F42B33/02		37
F42B33/0278	9	{Safety arrangements therefor (F42B33/004 takes precedence)}	F42B33/02	F42B33/02		41
F42B33/0285	9	{Measuring explosive-charge levels in containers or cartridge cases; Methods or devices for controlling the quantity of material fed or filled (F42B33/004 takes precedence; controlling the quantity of material fed in packaging B65B3/26)}	F42B33/02	F42B33/02		77
F42B33/0292	10	{by volumetric measurement, i.e. the volume of the material being determined before filling}	F42B33/02	F42B33/02		157
F42B33/04	8	Fitting or extracting primers in or from fuzes or charges {(F42B33/004 takes precedence)}	F42B33/04	F42B33/04		409
F42B33/06	8	Dismantling fuzes, cartridges, projectiles, missiles, rockets or bombs ({F42B33/004 and}F42B33/04 take precedence; {elimination of undesirable components of explosives C06B21/0091})	F42B33/06	F42B33/06		664
F42B33/062	9	{by high-pressure water jet means}	F42B33/06	F42B33/06		163
F42B33/065	9	{by laser means}	F42B33/06	F42B33/06		18
F42B33/067	9	{by combustion (incineration apparatuses or processes for used articles F23G7/003)}	F42B33/06	F42B33/06		161
F42B33/10	8	Reconditioning used cartridge cases {(F42B33/004 takes precedence)}	F42B33/10	F42B33/10		269
F42B33/12	8	Crimping shotgun cartridges {(F42B33/004 takes precedence)}	F42B33/12	F42B33/12		141
F42B33/14	8	Surface treatment of cartridges or cartridge cases {(F42B33/004 takes precedence)}	F42B33/14	F42B33/14		170
F42B35/00	7	Testing or checking of ammunition {(apparatus for measuring the energy of projectiles G01L5/14)}	F42B35/00	F42B35/00		1456
F42B35/02	8	Gauging, sorting, trimming or shortening cartridges or missiles	F42B35/02	F42B35/02		465
F42B39/00	7	Packaging or storage of ammunition or explosive charges; Safety features thereof; Cartridge belts or bags	F42B39/00	F42B39/00		880
F42B39/002	8	{Cartridge containers provided with cartridge-dispensing means}	F42B39/00	F42B39/00		140
F42B39/005	8	{Protection for driving bands}	F42B39/00	F42B39/00		33
F42B39/007	8	{Packaging or storage of arrows or darts (quivers for arrows F41B5/06)}	F42B39/00	F42B39/00		84
F42B39/02	8	Cartridge bags; Bandoleers	F42B39/02	F42B39/02		691
F42B39/08	8	Cartridge belts	F42B39/08	F42B39/08		410
F42B39/082	9	{for caseless ammunition}	F42B39/08	F42B39/08		25
F42B39/085	9	{for blank cartridges}	F42B39/08	F42B39/08		79
F42B39/087	9	{Feed belts manufactured from fabric or plastics material}	F42B39/08	F42B39/08		53
F42B39/10	9	Machines for charging or for extracting cartridges from feed belts	F42B39/10	F42B39/10		132
F42B39/14	8	Explosion or fire protection arrangements on packages or ammunition (F42B39/20{and F42B39/24} take precedence; {wall or panel structure of fireproof safes or storage containers E05G1/024})	F42B39/14	F42B39/14		390
F42B39/16	9	Fire-extinguishing	F42B39/16	F42B39/16		33
F42B39/18	9	Heat shields; Thermal insulation	F42B39/18	F42B39/18		56
F42B39/20	8	Packages or ammunition having valves for pressure-equalising; Packages or ammunition having plugs for pressure release, e.g. meltable {; Blow-out panels; Venting arrangements (ventilating arrangements on packages formed from foldable or erectable blanks B65D5/4295; packages with pressure-relief valves incorporated in a container wall B65D77/225)}	F42B39/20	F42B39/20		343
F42B39/22	8	Locking of ammunition in transport containers	F42B39/22	F42B39/22		234
F42B39/24	8	Shock-absorbing arrangements in packages {, e.g. for shock waves}	F42B39/24	F42B39/24		152
F42B39/26	8	Packages or containers for a plurality of ammunition, e.g. cartridges (F42B39/14&#160;-&#160;F42B39/24, F42B39/28 take precedence)	F42B39/26	F42B39/26		547
F42B39/28	8	Ammunition racks, e.g. in vehicles	F42B39/28	F42B39/28		130
F42B39/30	8	Containers for detonators or fuzes (F42B39/14, F42B39/20 take precedence)	F42B39/30	F42B39/30		175
F42B99/00	7	Subject matter not provided for in other groups of this subclass	F42B99/00	F42B99/00		32
