H		電気<br><br><b><ul>注</ul></b><br>（利用にあたっての基本原則と一般的指示）<br>Ｉ．セクションＨは以下のものを包含する：<br>（ａ）基本的電気素子，これは全ての電気ユニットと，装置や回路の一般的な機械的構成を包含しており，その中にはプリント配線と称されるものに各種の基本素子を組み立てたものも含まれる。またこれは他に包含されない場合には，ある程度までこれらの素子の製造をも包含する；<br>（ｂ）発電，これは，発電，変換および配電と共にそのための装置の制御を包含する；<br>（ｃ）電気の応用，これは以下のものを包含する：<br>（ｉ）一般的な利用技術，すなわち．電気加熱と電気照明回路の利用技術；<br>（ｉｉ）厳密な意味で電気的か電子的かいずれかの特定の利用技術で国際特許分類の他のセクションに包含されないもの，これは以下のものを含んでいる：<br>（１）電気的光源，これはレーザーを含む；<br>（２）電気的なＸ線技術；<br>（３）電気的なプラズマ技術，および帯電粒子または中性子の発生および加速；<br>（ｄ）基本電子回路およびその制御；<br>（ｅ）電気通信技術；これは電気―機械変換器一般を含む；<br>（ｆ）物品や上記素子を作るための特定の材料の使用，この点については指針の８８項から９０項を参照されたい。<br>ＩＩ．このセクションにおいては，下記の一般規則が適用される：<br>（ａ）上記Ｉ（ｃ）で述べた例外を除いて，国際特許分類のセクションＨ以外のいずれかのセクションに分類される特殊な操作，方法，装置，物体または物品に特有の電気的観点または部分は，常にその操作，方法，装置，物体または物品のためのサブクラスに分類されるか，または類似の性質を有する技術主題に関する共通的な特徴がクラス・レベルで展開されている場合には，それは，該技術主題のための一般的電気的な応用を完全に包含するサブクラスに，その操作，方法，装置，物体または物品と関連して分類される；<br>（ｂ）この様な電気的な応用には，一般的なものであれ特殊なものであれ，次の事項が含まれる。<br>（ｉ）Ａ６１における治療方法および装置；<br>（ｉｉ）Ｂ０１，Ｂ０３およびＢ２３Ｋにおける各種の実験室または工業的操作に用いられる電気的方法および装置；<br>（ｉｉｉ）セクションＢの“運輸”のサブセクションにおける車両一般および特殊な車両への電気の供給，電気的推進および電気照明；<br>（ｉｖ）Ｆ０２Ｐにおける内燃機関の電気点火系，およびＦ２３Ｑにおける燃焼装置一般のもの；<br>（ｖ）セクションＧにおける全ての電気的部分，すなわち，電気変量の測定器を含む測定装置，検査，信号および計算。このＧセクションにおいて電気とは，一般に手段として扱われるものでそれ自体目的として扱われるものではない；<br>（ｃ）全ての電気的な応用は一般的なものであれ特殊なものであれ，それが含んでいる電気的“基本的素子”に関して言えば，“基本的な電気”の観点がセクションＨ（上記Ｉ（ａ）参照）にあることを前提としている。この規則は，セクションＨ自身にある上記Ｉ（ｃ）で示した電気の応用に対しても有効である。	ELECTRICITY; <br><br><b><u>Note(s)</u></b><br><br><ul><li>These Notes cover the basic principles and general instructions for use of section <b>H</b>.<ul><li>Section <b>H</b> <u>covers</u>: <ul><li>basic electric elements, which cover all electric units and the general mechanical structure of apparatus and circuits, including the assembly of various basic elements into what are called printed circuits and also cover to a certain extent the manufacture of these elements (when not covered elsewhere);</li><li>generation of electricity, which covers the generation, conversion and distribution of electricity together with the controlling of the corresponding gear;</li><li>applied electricity, which <u>covers</u>: <ul><li>general utilisation techniques, viz. those of electric heating and electric lighting circuits;</li><li>some special utilisation techniques, either electric or electronic in the strict sense, which are not covered by other sections of the Classification, including: <ul><li>electric light sources, including lasers;</li><li>electric X-ray technique;</li><li>electric plasma technique and the generation and acceleration of electrically charged particles or neutrons;</li></ul></li></ul></li><li>basic electronic circuits and their control;</li><li>radio or electric communication technique;</li><li>the use of a specified material for the manufacture of the article or element described. In this connection, paragraphs 88 to 90 of the Guide should be referred to.</li></ul></li><li>In this section, the following general rules apply: <ul><li>Subject to the exceptions stated in I(c), above, any electric aspect or part peculiar to a particular operation, process, apparatus, object or article, classified in one of the sections of the Classification other than section <b>H</b>, is always classified in the subclass for that operation, process, apparatus, object or article. Where common characteristics concerning technical subjects of similar nature have been brought out at class level, the electric aspect or part is classified, in conjunction with the operation, process, apparatus, object or article, in a subclass which covers entirely the general electrical applications for the technical subject in question;</li><li>The electrical applications referred to under (a), above, either general or particular, include: <ul><li>the therapeutic processes and apparatus, in class <b>A61</b>;</li><li>the electric processes and apparatus used in various laboratory or industrial operations, in classes <b>B01</b> and <b>B03</b> and in subclass <b>B23K</b>;</li><li>the electricity supply, electric propulsion and electric lighting of vehicles in general and of particular vehicles, in the subsection "Transporting" of section <b>B</b>;</li><li>the electric ignition systems of internal-combustion engines, in subclass <b>F02P</b>, and of combustion apparatus in general, in subclass <b>F23Q</b>;</li><li>the whole electrical part of section <b>G</b>, i.e. measuring devices including apparatus for measuring electric variables, checking, signalling and calculating. Electricity in that section is generally dealt with as a means and not as an end in itself;</li></ul></li><li>All electrical applications, both general and particular, presuppose that the "basic electricity" aspect appears in section <b>H</b> (see I(a) above) as regards the electric "basic elements" which they comprise. This rule is also valid for applied electricity, referred to in I(c), above, which appears in section <b>H</b> itself.</li></ul></li></ul></li></ul>	
H01		電気素子<br><br><b><ul>注</ul></b><br>（１）他に項目が存在する単一の技術のみを含む方法，例．乾燥，被覆，はその技術に関連するクラスに分類される。<br>（２）“マイクロ構造の装置”および“マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。［７］	ELECTRIC ELEMENTS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>Processes involving only a single technical art, e.g. drying, coating, for which provision exists elsewhere are classified in the relevant class for that art.</li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to "microstructural devices" and "microstructural systems".</li></ul>	
H01B		ケーブル；導体；絶縁体；導電性，絶縁性または誘導性特性に対する材料の選択（磁気特性に対する選択Ｈ０１Ｆ１／００；導波管Ｈ０１Ｐ）<br><br><b><ul>サブクラス内の索引</ul></b><br>導体またはケーブル<br>材料を特徴とするもの　１／００<br>構造を特徴とするもの　５／００，７／００<br>通信，電力または超電導ケーブルのための特殊なタイプ　１１／００，９／００，１２／００<br>製造，廃物利用　１３／００，１５／００<br>絶縁物または絶縁材<br>材料を特徴とするもの　３／００<br>構造を特徴とするもの　１７／００<br>製造　１９／００	CABLES; CONDUCTORS; INSULATORS; SELECTION OF MATERIALS FOR THEIR CONDUCTIVE, INSULATING OR DIELECTRIC PROPERTIES(selection for magnetic properties <b>H01F1/00</b>; waveguides <b>H01P</b>);<br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CONDUCTORS OR CABLES<tr><td width="70%">Characterised by the material </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Characterised by the construction </td><td><b><b>5/00</b>, <b>7/00</b></b></td></tr></tr><tr><td width="70%">Special types for: communication; power; superconductive cables </td><td><b><b>11/00</b>; <b>9/00</b>; <b>12/00</b></b></td></tr></tr><tr><td width="70%">Manufacture; salvaging </td><td><b><b>13/00</b>; <b>15/00</b></b></td></tr></tr></tr><tr><td width="70%">INSULATORS OR INSULATING BODIES<tr><td width="70%">Characterised by the material </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">Characterised by the construction </td><td><b><b>17/00</b></b></td></tr></tr><tr><td width="70%">Manufacture </td><td><b><b>19/00</b></b></td></tr></tr></tr></table>	2876
H01C		抵抗器<br><br><b><ul>注</ul></b><br>（１）このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“可調整”とは，機械的に調整が可能なことを意味する。［２］<br>（２）抵抗値を機械的に変化できない可変抵抗器，例．電圧または熱によるものはグループ７／００に分類される。［２］<br><br><b><ul>サブクラス内の索引</ul></b><br>固定抵抗器　３／００，７／００，８／００，１１／００<br>可変抵抗器　１０／００<br>他の抵抗器　１３／００<br>細部　１／００<br>製造　１７／００	RESISTORS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following term is used with the meaning indicated:<ul><li>"adjustable" means mechanically adjustable. </li></ul></li><li>Variable resistors, the value of which is changed non-mechanically, e.g. by voltage or temperature, are classified in group <b>H01C7/00</b>. </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">NON-ADJUSTABLE RESISTORS </td><td><b><b>3/00</b>, <b>7/00</b>, <b>8/00</b>, <b>11/00</b></b></td></tr></tr><tr><td width="70%">ADJUSTABLE RESISTORS </td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">OTHER RESISTORS </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>17/00</b></b></td></tr></tr></table>	506
H01F		磁石；インダクタンス；変成器；それらの磁気特性による材料の選択［２］<br><br><b><ul>サブクラス内の索引</ul></b><br>磁石，電磁石<br>磁性材料を特徴とするもの　１／００<br>コア，ヨーク，アーマチュア　３／００<br>コイル　５／００<br>超電導コイルまたは磁石　６／００<br>磁石　７／００<br>磁化，消磁　１３／００<br>製造　４１／００<br>薄膜　１０／００<br>固定インダクタンスまたは変成器<br>信号用　１７／００，１９／００<br>信号用以外　３０／００，３７／００<br>製造　４１／００<br>可変インダクタンスまたは変成器<br>信号用　２１／００<br>信号用以外　２９／００<br>製造　４１／００<br>変成器またはインダクタンスの細部一般　２７／００<br>超電導巻線または低温で動作する巻線を有する変成器　３６／００<br>特定の応用や機能のための変成器またはインダクタンスの適用　３８／００	MAGNETS; INDUCTANCES; TRANSFORMERS; SELECTION OF MATERIALS FOR THEIR MAGNETIC PROPERTIES; <br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">MAGNETS, ELECTROMAGNETS<tr><td width="70%">Characterised by the magnetic material </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Cores, yokes, armatures </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">Coils </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">Superconducting coils or magnets </td><td><b><b>6/00</b></b></td></tr></tr><tr><td width="70%">Magnets </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">Magnetising, demagnetising </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">Manufacture </td><td><b><b>41/00</b></b></td></tr></tr></tr><tr><td width="70%">THIN FILMS </td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">FIXED INDUCTANCES OR TRANSFORMERS<tr><td width="70%">Of the signal type </td><td><b><b>17/00</b>, <b>19/00</b></b></td></tr></tr><tr><td width="70%">Other than of the signal type </td><td><b><b>30/00</b>, <b>37/00</b></b></td></tr></tr><tr><td width="70%">Manufacture </td><td><b><b>41/00</b></b></td></tr></tr></tr><tr><td width="70%">VARIABLE INDUCTANCES OR TRANSFORMERS<tr><td width="70%">Of the signal type </td><td><b><b>21/00</b></b></td></tr></tr><tr><td width="70%">Other than of the signal type </td><td><b><b>29/00</b></b></td></tr></tr><tr><td width="70%">Manufacture </td><td><b><b>41/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS OF TRANSFORMERS OR INDUCTANCES, IN GENERAL </td><td><b><b>27/00</b></b></td></tr></tr><tr><td width="70%">SUPERCONDUCTIVE OR CRYOGENIC TRANSFORMERS </td><td><b><b>36/00</b></b></td></tr></tr><tr><td width="70%">ADAPTATIONS OF TRANSFORMERS OR INDUCTANCES FOR SPECIFIC APPLICATIONS OR FUNCTIONS </td><td><b><b>38/00</b></b></td></tr></tr></table>	1886
H01G		コンデンサ；電解型のコンデンサ，整流器，検波器，開閉装置，感光装置また感温装置（誘電体としての特定の材料の選択Ｈ０１Ｂ３／００；電位障壁を有するコンデンサＨ１０Ｄ１／６２，Ｈ１０Ｋ１０／１０）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，グループＨ０１Ｇ１１／００はグループＨ０１Ｇ４／００およびＨ０１Ｇ９／００に優先する。［２０１３．０１］<br><br><b><ul>サブクラス内の索引</ul></b><br>コンデンサ<br>固定コンデンサ　４／００<br>可変コンデンサ：機械的手段によるもの；非機械的手段によるもの　５／００，７／００<br>ハイブリッド　１１／００<br>細部　２／００<br>電解型装置　９／００<br>構造的組み合わせ　１５／００，１７／００<br>製造　４／００，５／００，７／００，９／００，１３／００	CAPACITORS; CAPACITORS, RECTIFIERS, DETECTORS, SWITCHING DEVICES, LIGHT-SENSITIVE OR TEMPERATURE-SENSITIVE DEVICES OF THE ELECTROLYTIC TYPE (selection of specified materials as dielectric <b>H01B3/00</b>;  capacitors having potential barriers <b>H10D1/62</b>, <b>H10K10/10</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, group <b>H01G11/00</b> takes precedence over groups <b>H01G4/00</b> and <b>H01G9/00</b>. </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CAPACITORS<tr><td width="70%">With fixed capacitance</td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">With variable capacitance: by mechanical means; by non-mechanical means</td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr><tr><td width="70%">Hybrid</td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">Details</td><td><b><b>2/00</b></b></td></tr></tr></tr><tr><td width="70%">ELECTROLYTIC APPARATUS</td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">STRUCTURAL COMBINATIONS</td><td><b><b>15/00</b>, <b>17/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE</td><td><b><b>4/00</b>, <b>5/00</b>, <b>7/00</b>, <b>9/00</b>, <b>13/00</b></b></td></tr></tr></table>	1156
H01H		電気的スイッチ；継電器；セレクタ；非常保護装置（接触ケーブルＨ０１Ｂ７／１０；電解自己遮断装置Ｈ０１Ｇ９／１８；非常保護回路装置Ｈ０２Ｈ；無接点電子手段による開閉Ｈ０３Ｋ１７／００）<br><br><b><ul>注</ul></b><br>１．このサブクラスは，正常な電気的作動状態から不所望の状態に変化する電線，電気機械又は電気器具を保護するための装置で，その電気的状態が前記装置に直接入力として作用する装置を，グループＨ０１Ｈ６９／００〜Ｈ０１Ｈ８７／００内に，包含する。<br>２．このサブクラスは，２つ以上の開閉器を収容するか，又は開閉器と共に他の電気的構成物，例．バスバー，コネクタ，を収容するための基台，ケース，又はカバーを包含しない。これらの基台，ケース又はカバーはグループＨ０２Ｂ１／２６に包含される。<br>３．このサブクラスにおいては，下記の用語又は表現は以下に示す意味で用いる：<br>・“継電器”とは，接点の開閉を引き起こすに必要な機械的エネルギーの全てを，直接的又は間接的に供給する電気的入力によって操作される接点をもつ開閉器を意味する；<br>・“駆動機構”とは，スイッチに与えられた操作力が，可動接点に伝達される手段をいう；<br>・“操作（ｏｐｅｒａｔｉｎｇ）”は，スイッチ動作を手動で行なわない部分に対して用いられる“作動（ａｃｔｕａｔｉｎｇ）”よりも広い意味に使われる；<br>・“動作（ａｃｔｉｎｇ）”又は“動き（ａｃｔｉｏｎ）”とは，スイッチングの一段階において，ある部分が自ら誘起する運動を意味する。これらの意味は，“操作する（ｔｏ　ｏｐｅｒａｔｅ）“作動する（ｔｏ　ａｃｔｕａｔｅ）“動く（ｔｏ　ａｃｔ）”の動詞のすべての部分に適用され，そこから導かれる語，例．“作動（ａｃｔｕａｔｉｏｎ）”，にも適用される。<br>４．このサブクラスにおいては，細部は下記のように分類される：<br>・不特定型式の開閉器の細部，又はスイッチ，継電器，セレクタスイッチおよび非常保護装置という用語又は表現によって指示された二種以上の開閉器に適用し得るように開示されているものの細部はグループＨ０１Ｈ１／００〜Ｈ０１Ｈ９／００に分類される；<br>・不特定型式のスイッチの細部，又はグループＨ０１Ｈ１３／００〜Ｈ０１Ｈ４３／００ならびにサブグループＨ０１Ｈ３５／０２，Ｈ０１Ｈ３５／０６，Ｈ０１Ｈ３５／１４，Ｈ０１Ｈ３５／１８，Ｈ０１Ｈ３５／２４およびＨ０１Ｈ３５／４２によって規定された二つ以上の型式のスイッチに適用し得るように開示されているものの細部，以下基本型と称するすべてのものはグループＨ０１Ｈ１／００〜Ｈ０１Ｈ９／００に分類される；<br>・不特定型式の継電器の細部，又はグループＨ０１Ｈ５１／００〜Ｈ０１Ｈ６１／００によって規定された二つ以上の型式の継電器に適用し得るように開示されているものの細部，以下基本型と称するものはグループＨ０１Ｈ４５／００に分類される；<br>・不特定な保護装置の細部，又はグループＨ０１Ｈ７３／００〜Ｈ０１Ｈ８３／００によって規定された二つ以上の型式の保護装置に適用し得るものの細部，以下基本型と称するものはＨ０１Ｈ７１／００に分類される。<br>・しかしながら，単一の基本型の開閉器に関して単に述べられた細部またはその開閉器のみに適用されることが明らかな細部はその基本型の開閉器に適切なグループ，例．Ｈ０１Ｈ１９／０２，Ｈ０１Ｈ７５／０４，に分類される；<br>・作動される要素に対して力を伝達するためのキー，押ボタン，レバー又はその他の機構のような，スイッチ又はキーボードの制御部材の機械的な構造の細部は，それが電子的スイッチを制御するために使用される場合でも，このサブクラスに分類される；<br>しかしながら，電子的効果を直接的に生じさせる機械的な細部はグループＨ０３Ｋ１７／９４に分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>電気スイッチ<br>制御原理によって特徴づけられるもの：<br>機械的なもの：<br>直線移動によるもの：一方向；二方向　１３／００；１５／００<br>角変位によるもの：制限されない角度で；制限された角度で　１９／００；２１／００<br>引張りによるもの；タンブラースイッチ　１７／００；２３／００<br>複合運動するもの　２５／００<br>着脱部材によるもの　２７／００<br>物理的なもの：<br>一般；電界または磁界によるもの；加熱；爆発　３５／００；３６／００；３７／００；３９／００<br>接点によって特徴づけられるもの：<br>液体　２９／００<br>電圧または強さによって特徴づけられるもの：<br>消弧手段をもたないもの；消弧手段をもつもの　３１／００；３３／００<br>始動，持続によって特徴づけられるもの：<br>手動；プログラム　４１／００；４３／００<br>製造　１１／００<br>継電器<br>電磁型；動電型；磁わい型　５１／００；５３／００；５５／００<br>電わい型または圧電型；静電型；電熱型　５７／００；５９／００；６１／００<br>細部：<br>一般；電気機械的；回路　４５／００；５０／００；４７／００<br>製造　４９／００<br>セレクタ<br>型式　６７／００<br>細部　６３／００<br>製造　６５／００<br>セクショナライザ<br>刃形接片をもつ低応力のもの　２１／５４<br>高応力のためのもの　３１／００<br>ヒューズと結合したもの　８５／５４<br>保護装置<br>回路遮断スイッチ：<br>リセット機構を持つもの：手動；電動機によるもの；別の作動を要するもの　７３／００；７５／００；７７／００<br>保護スイッチ：<br>短絡の；開閉を繰り返すもの；異常状態　７９／００；８１／００；８３／００<br>ヒューズ；蒸発装置　８５／００；８７／００<br>保護スイッチまたは保護継電器の細部　７１／００<br>製造　６９／００<br>組合せ　８９／００<br>一般的細部<br>接点　１／００<br>機構：<br>接点の操作機構一般；速動装置；遅延　３／００；５／００；７／００<br>他の細部　９／００	ELECTRIC SWITCHES; RELAYS; SELECTORS; EMERGENCY PROTECTIVE DEVICES(contact cables <b>H01B7/10</b>;  electrolytic self-interrupters <b>H01G9/18</b>;  emergency protective circuit arrangements <b>H02H</b>;  switching by electronic means without contact-making <b>H03K17/00</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers,</u> in groups <b>H01H69/00 to H01H87/00</b>  devices for the protection of electric lines or electric machines or apparatus in the event of undesired change from normal electric working conditions, the electrical condition serving directly as the input to the device.</li><li>This subclass <u>does not cover</u> bases, casings, or covers accommodating two or more switching devices or for accommodating a switching device as well as another electric component, e.g. bus-bar, line connector. Those bases, casings or covers are covered by group <b>H02B1/26</b>.</li><li>In this subclass, the following terms or expressions are used with the meanings indicated: <ul><li>"relay" means a switching device having contacts which are operated from electric inputs which supply, directly or indirectly, all the mechanical energy necessary to cause both the closure and the opening of the contacts;</li><li>"driving mechanism" refers to the means by which an operating force applied to the switch is transmitted to the moving contact or contacts;</li><li>"operating" is used in a broader sense than "actuating" which is reserved for those parts not touched by hand to effect switching;</li><li>"acting" or "action" means a self-induced movements of parts at one stage of the switching. These connotations apply to all parts of the verbs "to operate"; "to actuate", and "to act", and to words derived therefrom, e.g. to "actuation".</li></ul></li><li>In this subclass, details are classified as follows: <ul><li>details of an unspecified type of switching device, or disclosed as applicable to two or more kinds of switching devices designated by the terms or expressions "switches", "relays", "selector switches", and "emergency protective devices", are classified in groups <b>H01H1/00 to H01H9/00</b> ;</li><li>details of an unspecified type of switch, or disclosed as applicable to two or more types of switches as defined by groups <b>H01H13/00 to H01H43/00</b>  and subgroups <b>H01H35/02</b>, <b>H01H35/06</b>, <b>H01H35/14</b>, <b>H01H35/18</b>, <b>H01H35/24</b>, and <b>H01H35/42</b>, all hereinafter called basic types, are classified in groups <b>H01H1/00 to H01H9/00</b> ;</li><li>details of an unspecified type of relay, or disclosed as applicable to two or more types of relays as defined by groups <b>H01H51/00 to H01H61/00</b> , hereinafter called basic types, are classified in group <b>H01H45/00</b>;</li><li>details of an unspecified protective device, or applicable to two or more types of protective devices as defined by groups <b>H01H73/00 to H01H83/00</b> , hereinafter called basic types, are classified in group <b>H01H71/00</b>.</li><li>However, details only described with reference to, or clearly only applicable to, switching devices of a single basic type, are classified in the group appropriate to switching devices of that basic type, e.g. <b>H01H19/02</b>, <b>H01H75/04</b>;</li><li>mechanical structural details of control members of switches or of keyboards such as keys, push-buttons, levers or other mechanisms for transferring the force to the activated elements are classified in this subclass, even when they are used for controlling electronic switches.</li></ul>However, mechanical details directly producing electronic effects are classified in group <b>H03K17/94</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">ELECTRIC SWITCHES<tr><td width="70%">Characterised by the principle of control<tr><td width="70%">mechanical<tr><td width="70%">rectilinearly movable: one direction; two directions</td><td><b><b>13/00</b>; <b>15/00</b></b></td></tr></tr><tr><td width="70%">with angular displacement: unlimited angle; limited angle</td><td><b><b>19/00</b>; <b>21/00</b></b></td></tr></tr><tr><td width="70%">by pulling; by tumbling</td><td><b><b>17/00</b>; <b>23/00</b></b></td></tr></tr><tr><td width="70%">with compound movements</td><td><b><b>25/00</b></b></td></tr></tr><tr><td width="70%">by removable members</td><td><b><b>27/00</b></b></td></tr></tr></tr><tr><td width="70%">physical<tr><td width="70%">general; electric or magnetic field; heat; explosion</td><td><b><b>35/00</b>; <b>36/00</b>; <b>37/00</b>; <b>39/00</b></b></td></tr></tr></tr></tr><tr><td width="70%">Characterised by the contacts<tr><td width="70%">liquid</td><td><b><b>29/00</b></b></td></tr></tr></tr><tr><td width="70%">Characterised by the voltage or the intensity<tr><td width="70%">without arc-extinguishing means; with such means</td><td><b><b>31/00</b>; <b>33/00</b></b></td></tr></tr></tr><tr><td width="70%">Characterised by the actuation duration<tr><td width="70%">manual; programme</td><td><b><b>41/00</b>; <b>43/00</b></b></td></tr></tr></tr><tr><td width="70%">Manufacture</td><td><b><b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">RELAYS<tr><td width="70%">Electromagnetic; dynamo-electric; magnetostrictive</td><td><b><b>51/00</b>; <b>53/00</b>; <b>55/00</b></b></td></tr></tr><tr><td width="70%">Electrostrictive or piezoelectric; electrostatic; electrothermal</td><td><b><b>57/00</b>; <b>59/00</b>; <b>61/00</b></b></td></tr></tr><tr><td width="70%">Details<tr><td width="70%">general; electromechanical; circuits</td><td><b><b>45/00</b>; <b>50/00</b>; <b>47/00</b></b></td></tr></tr></tr><tr><td width="70%">Manufacture</td><td><b><b>49/00</b></b></td></tr></tr></tr><tr><td width="70%">SELECTORS<tr><td width="70%">Types</td><td><b><b>67/00</b></b></td></tr></tr><tr><td width="70%">Details</td><td><b><b>63/00</b></b></td></tr></tr><tr><td width="70%">Manufacture</td><td><b><b>65/00</b></b></td></tr></tr></tr><tr><td width="70%">SECTIONALISERS<tr><td width="70%">low-tension with blade-type contact</td><td><b><b>21/54</b></b></td></tr></tr><tr><td width="70%">for high tension</td><td><b><b>31/00</b></b></td></tr></tr><tr><td width="70%">combined with fuses</td><td><b><b>85/54</b></b></td></tr></tr></tr><tr><td width="70%">PROTECTIVE DEVICES<tr><td width="70%">Circuit-breaking switches<tr><td width="70%">with resetting: manual; by motor; separate</td><td><b><b>73/00</b>; <b>75/00</b>; <b>77/00</b></b></td></tr></tr></tr><tr><td width="70%">Protective switches<tr><td width="70%">by short-circuit; opening and closing; particular</td><td><b><b>79/00</b>; <b>81/00</b>; <b>83/00</b></b></td></tr></tr></tr><tr><td width="70%">Fuses; evaporation devices</td><td><b><b>85/00</b>; <b>87/00</b></b></td></tr></tr><tr><td width="70%">Details of protective switches and relays</td><td><b><b>71/00</b></b></td></tr></tr><tr><td width="70%">Manufacture</td><td><b><b>69/00</b></b></td></tr></tr></tr><tr><td width="70%">COMBINATIONS</td><td><b><b>89/00</b></b></td></tr></tr><tr><td width="70%">GENERAL DETAILS<tr><td width="70%">Contacts</td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Mechanisms<tr><td width="70%">operating contacts in general; snap-action; delay</td><td><b><b>3/00</b>; <b>5/00</b>; <b>7/00</b></b></td></tr></tr></tr><tr><td width="70%">Other details</td><td><b><b>9/00</b></b></td></tr></tr></tr></table>	5542
H01J		放電管または放電ランプ（スパークギャップＨ０１Ｔ；電気アークランプＨ０５Ｂ３１／００；粒子加速器Ｈ０５Ｈ）<br><br><b><ul>注</ul></b><br>注［４］<br>１．このサブクラスは電子流またはイオン流を発生し，誘導しまたは使用する装置，例．電流を制御し，指示しまたは開閉し，電気パルスを計数し，光またはＸ線のような他の電磁振動を発生し，または放射線あるいは粒子を分離しまたは分析するものであって，装置の特性を定める圧力および性質に基づき選択されたガス，蒸気を含むまたは真空の，密閉されまたは実質上密閉されたケースをもつもののみを包含する。<br>２．このサブクラスは，Ｈ０５Ｂ３５／００に包含される，放電型の光源および他の光源型式の組み合わせを用いる光源を，グループＨ０１Ｊ６１／９６に包含される光源を除いては，包含しない。<br>３．このサブクラスにおいては，グループＨ０１Ｊ１／００〜Ｈ０１Ｊ７／００は，以下の（ｉ）（ｉｉ）のみに関する：<br>ｉ．電子管または放電ランプの種類を特定していないものの細部，または<br>ｉｉ．以下に基本型と称するグループＨ０１Ｊ１１／００，Ｈ０１Ｊ１３／００，Ｈ０１Ｊ１５／００，Ｈ０１Ｊ１７／００，Ｈ０１Ｊ２１／００，Ｈ０１Ｊ２５／００，Ｈ０１Ｊ２７／００，Ｈ０１Ｊ３１／００，Ｈ０１Ｊ３３／００，Ｈ０１Ｊ３５／００，Ｈ０１Ｊ３７／００，Ｈ０１Ｊ４０／００，Ｈ０１Ｊ４１／００，Ｈ０１Ｊ４７／００，Ｈ０１Ｊ４９／００，Ｈ０１Ｊ６１／００，Ｈ０１Ｊ６３／００またはＨ０１Ｊ６５／００に定義される型の電子管またはランプのうちの２あるいはそれ以上のものに適用することができると明細書の中で述べられているものの細部。唯１つの基本型の電子管またはランプに対してのみ記載され，あるいは適用し得ることが明らかなものの細部は，その基本型の電子管またはランプの適当な細部グループ，例．Ｈ０１Ｊ１７／０４，に分類される。<br>４．このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>・“ランプ”は紫外線または赤外線の光を放射する管を含む。<br>５．サブクラスＨ０１Ｔのタイトルに続く注で与えられる表現“スパークギャップ”の定義に注意すること。<br>６．電子管，放電ランプまたはそれらの部品の製造に特に適合する装置または方法はグループＨ０１Ｊ９／００に分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>ガス入り管<br>管内に電極をもたないもの；液体陰極；ガス状陰極；固体陰極　１１／００；１３／００；１５／００；１７／００<br>真空管<br>古典的な真空管：管；細部　２１／００；１９／００<br>走行時間型電子管：管；細部　２５／００；２３／００<br>イオンビーム管　２７／００<br>陰極線管：管；細部　３１／００；２９／００<br>Ｘ線管　３５／００<br>材料または目的物を処理または試験するための管　３７／００<br>特殊な管<br>電子またはイオンを取り出すための；粒子分光器または粒子分離管　３３／００；４９／００<br>真空ゲージ，イオンの拡散による排気；二次電　子管；電子増倍管；熱イオン発生器　４１／００；４３／００；４５／００<br>光電管；輻射および粒子の検出器　４０／００；４７／００<br>放電ランプ<br>ガス放電ランプ；陰極線または電子流ランプ；管内に電　極をもたないランプ　６１／００；６３／００；６５／００<br>細部<br>電極；電子光学；容器；その他の細部　１／００；３／００；５／００；７／００<br>製造；修理；再生；材料の回収　９／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	ELECTRIC DISCHARGE TUBES OR DISCHARGE LAMPS(spark-gaps <b>H01T</b>; electric arc lamps <b>H05B31/00</b>; particle accelerators <b>H05H</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> only devices for producing, influencing, or using a flow of electrons or ions, e.g. for controlling, indicating, or switching of electric current, counting electric pulses, producing light or other electromagnetic oscillations, such as X-rays, or for separating or analysing radiation or particles, and having a closed or substantially closed casing containing a chosen gas, vapour, or vacuum, upon the pressure and nature of which the characteristics of the device depend.</li><li>This subclass <u>does not cover</u> light sources using combinations of discharge-type light sources and other types of light sources, which are covered by group <b>H05B35/00</b>, except for those light sources covered by group <b>H01J61/96</b>.</li><li>In this subclass, groups <b>H01J1/00 to H01J7/00</b>  relate only to: <ul><li>details of an unspecified kind of discharge tube or lamp, or</li><li>details mentioned in a specification as applicable to two or more kinds of tubes or lamps as defined by groups <b>H01J11/00</b>, <b>H01J13/00</b>, <b>H01J15/00</b>, <b>H01J17/00</b>, <b>H01J21/00</b>, <b>H01J25/00</b>, <b>H01J27/00</b>, <b>H01J31/00</b>, <b>H01J33/00</b>, <b>H01J35/00</b>, <b>H01J37/00</b>, <b>H01J40/00</b>, <b>H01J41/00</b>, <b>H01J47/00</b>, <b>H01J49/00</b>, <b>H01J61/00</b>, <b>H01J63/00</b> or <b>H01J65/00</b>, hereinafter called basic kinds. A detail only described with reference to, or clearly only applicable to, tubes or lamps of a single basic kind is classified in the detail group appropriate to tubes or lamps of that basic kind, e.g. <b>H01J17/04</b>.</li></ul></li><li>In this subclass, the following term is used with the meaning indicated: <ul><li>"lamp" includes tubes emitting ultraviolet or infrared light.</li></ul></li><li>Attention is drawn to the definition of the expression "spark gaps" given in the Note following the title of subclass <b>H01T</b>.</li><li>Apparatus or processes specially adapted for the manufacture of electric discharge tubes, discharge lamps, or parts thereof are classified in group <b>H01J9/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">GAS-FILLED TUBES<tr><td width="70%">Without electrode inside; liquid cathode; gaseous cathode; solid cathode </td><td><b><b>11/00</b>; <b>13/00</b>; <b>15/00</b>; <b>17/00</b></b></td></tr></tr></tr><tr><td width="70%">VACUUM TUBES<tr><td width="70%">Classical tubes: tubes; details </td><td><b><b>21/00</b>; <b>19/00</b></b></td></tr></tr><tr><td width="70%">Transit-time tubes: tubes; details </td><td><b><b>25/00</b>; <b>23/00</b></b></td></tr></tr><tr><td width="70%">Ion beam tubes </td><td><b><b>27/00</b></b></td></tr></tr><tr><td width="70%">Cathode ray tubes: tubes; details </td><td><b><b>31/00</b>; <b>29/00</b></b></td></tr></tr><tr><td width="70%">X-ray tubes </td><td><b><b>35/00</b></b></td></tr></tr></tr><tr><td width="70%">TUBES FOR PROCESSING OR EXAMINATION OF MATERIALS OR OBJECTS </td><td><b><b>37/00</b></b></td></tr></tr><tr><td width="70%">SPECIAL TUBES<tr><td width="70%">For emergence of electrons or ions; particle spectrometers or separator tubes </td><td><b><b>33/00</b>; <b>49/00</b></b></td></tr></tr><tr><td width="70%">Vacuum gauges, evacuation by ion diffusion; secondary-emission tubes, electron multipliers; thermionic generators </td><td><b><b>41/00</b>; <b>43/00</b>; <b>45/00</b></b></td></tr></tr><tr><td width="70%">Photoelectric; radiation and particle detectors </td><td><b><b>40/00</b>; <b>47/00</b></b></td></tr></tr></tr><tr><td width="70%">DISCHARGE LAMPS<tr><td width="70%">Gas discharge lamps; cathode ray or electron stream lamps; without electrode inside </td><td><b><b>61/00</b>; <b>63/00</b>; <b>65/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS<tr><td width="70%">Electrodes; electron optics; vessels; other details </td><td><b><b>1/00</b>; <b>3/00</b>; <b>5/00</b>; <b>7/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE; REPAIR; REGENERATION; RECOVERY OF MATERIAL </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS </td><td><b><b>99/00</b></b></td></tr></tr></table>	1676
H01K		白熱ランプ（放電装置と白熱ランプの両方に使用できる細部，製造装置と製造方法Ｈ０１Ｊ；白熱発光体と他の発光体とを組み合わせた光源Ｈ０１Ｊ６１／９６，Ｈ０５Ｂ３５／００）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>―“ランプ”は，紫外線または赤外線を照射するものを含む。<br><br><b><ul>サブクラス内の索引</ul></b><br>利用によって特徴づけられるもの<br>一般照明用；他の照明用　５／００；７／００<br>白熱体によって特徴づけられるもの<br>非導電体；低温では非導電体のもの；複数の白熱体をもつもの　１１／００；１３／００；９／００<br>細部　１／００<br>製造　３／００	ELECTRIC INCANDESCENT LAMPS(details, apparatus or processes for manufacture applicable to both discharge devices and incandescent lamps <b>H01J</b>;  light sources using a combination of incandescent and other types of light generation <b>H01J61/96</b>, <b>H05B35/00</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following term is used with the meaning indicated:<ul><li>"lamp" includes tubes emitting ultraviolet or infrared light.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CHARACTERISED BY UTILISATION<tr><td width="70%">General lighting; other lighting </td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr></tr><tr><td width="70%">CHARACTERISED BY THE INCANDESCENT BODY<tr><td width="70%">Non-conductive; non-conductive in the cold state; multiple </td><td><b><b>11/00</b>; <b>13/00</b>; <b>9/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>3/00</b></b></td></tr></tr></table>	456
H01M		化学的エネルギーを電気的エネルギーに直接変換するための方法または手段，例．電池［２］<br><br><b><ul>注</ul></b><br>化学的エネルギーを電気的エネルギーに直接変換するための方法または手段，例．電池［２］<br>このサブクラスは一次電池または二次電池，燃料電池またはスタックを包含する。<br>型による電池<br>一次電池　Ｈ０１Ｍ６／００<br>燃料電池　Ｈ０１Ｍ８／００<br>二次電池　Ｈ０１Ｍ１０／００<br>混成電池；他に分類されない電気化学的発電装置；異なる型式の電気化学的発電装置の構造的組み合わせ　Ｈ０１Ｍ１２／００；Ｈ０１Ｍ１４／００；Ｈ０１Ｍ１６／００<br>種々の型の電池に共通する細部<br>電極　Ｈ０１Ｍ４／００<br>燃料電池以外の電気化学的電池の，発電要素以外の部分の構造の細部または製造方法　Ｈ０１Ｍ５０／００<br><br><b><ul>サブクラス内の索引</ul></b><br>型による電池<br>一次電池　Ｈ０１Ｍ６／００<br>燃料電池　Ｈ０１Ｍ８／００<br>二次電池　Ｈ０１Ｍ１０／００<br>混成電池；他に分類されない電気化学的発電装置；異なる型式の電気化学的発電装置の構造的組み合わせ　Ｈ０１Ｍ１２／００；Ｈ０１Ｍ１４／００；Ｈ０１Ｍ１６／００<br><br>種々の型の電池に共通する細部<br>電極Ｈ０１Ｍ４／００<br>燃料電池以外の電気化学的電池の，発電要素以外の部分の構造の細部または製造方法Ｈ０１Ｍ５０／００	PROCESSES OR MEANS, e.g. BATTERIES, FOR THE DIRECT CONVERSION OF CHEMICAL ENERGY INTO ELECTRICAL ENERGY; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> galvanic primary or secondary cells or batteries, fuel cells or stacks.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CELLS ACCORDING TO TYPE<tr><td width="70%">Primary cells</td><td><b><b>6/00</b></b></td></tr></tr><tr><td width="70%">Fuel cells</td><td><b><b>8/00</b></b></td></tr></tr><tr><td width="70%">Secondary cells</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Hybrid cells; electrochemical generators not provided for otherwise; combinations of different types of electrochemical generators</td><td><b><b>12/00</b>; <b>14/00</b>; <b>16/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS COMMON TO DIFFERENT TYPES OF CELLS<tr><td width="70%">Electrodes</td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">Constructional details or processes of manufacture of the non-active parts of electrochemical cells other than fuel cells</td><td><b><b>50/00</b></b></td></tr></tr></tr></table>	3116
H01P		導波管；導波管型の共振器，線路または他の装置（光周波数で動作するものＧ０２Ｂ）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―伝送線路に適用される“導波管型”は，高周波同軸ケーブルまたはレッヘル線のみを含み，共振器，遅延線路または他の装置に適用される“導波管型”は，分布インダクタンスと分布キャパシタンスをもつすべての装置を含む。<br><br><b><ul>サブクラス内の索引</ul></b><br>導波管，伝送線路　３／００<br>導波管型の装置：<br>補助装置；結合装置；共振器；遅延線路　１／００；５／００；７／００；９／００<br>製造　１１／００	WAVEGUIDES; RESONATORS, LINES OR OTHER DEVICES OF THE WAVEGUIDE TYPE(operating at optical frequencies <b>G02B</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following expression is used with the meaning indicated:<ul><li>"waveguide type" as applied to transmission lines includes only high-frequency coaxial cables or Lecher lines, and as applied to resonators, delay lines, or other devices includes all devices having distributed inductance and capacitance.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">WAVEGUIDES, TRANSMISSION LINES </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">DEVICES OF THE WAVEGUIDE TYPE<tr><td width="70%">Auxiliary devices; coupling devices; resonators; delay lines </td><td><b><b>1/00</b>; <b>5/00</b>; <b>7/00</b>; <b>9/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>11/00</b></b></td></tr></tr></table>	526
H01Q		アンテナ，すなわち空中線（マイクロ波加熱用の放射器またはアンテナＨ０５Ｂ６／７２）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―１次輻射素子のほかに，<br>（ｉ）アンテナから放射された電波を吸収するための２次装置または指向性または偏波を変えるための２次装置，および<br>（ｉｉ）接地スイッチ，導入線装置や避雷器などの補助装置との組合せ；<br>―送信用および受信用アンテナ［３］<br>（２）このサブクラスは導波管型の共振器や線路で，輻射素子として設計されていない装置を包含しない。ただし，これらはＨ０１Ｐに包含される。<br>（３）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“輻射器”は受信用アンテナの対応する部分を包含する。［３］<br><br><b><ul>サブクラス内の索引</ul></b><br>アンテナの型：<br>ループ型　７／００<br>導波管型　１３／００<br>他の型：短；長　９／００；１１／００<br>放射された電波に影響を与える装置：<br>準光学的；吸収　１５／００；１７／００<br>一次輻射要素と２次装置との組み合せ　１９／００<br>能動回路または回路素子を有するアンテナの組合せ　２３／００<br>２個以上の放射パターンを作るための構成　２５／００<br>アンテナ配列または系　２１／００<br>特殊な構成<br>細部；指向性；異なる周波数帯での同時動作　１／００；３／００；５／００	ANTENNAS, i.e. RADIO AERIALS(radiators or antennas for microwave heating <b>H05B6/72</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>in addition to the primary active radiating elements, <ul><li>secondary devices for absorbing or for modifying the direction or polarisation of waves radiated from antennas, and</li><li>combinations with auxiliary devices such as earthing switches, lead-in devices, and lightning protectors;</li></ul></li><li>both transmitting and receiving antennas.</li></ul></li><li>This subclass <u>does not cover</u> devices of the waveguide type, such as resonators or lines, not designed as radiating elements, which are covered by subclass <b>H01P</b>.</li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"active radiating element" covers corresponding parts of a receiving antenna.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">TYPES OF ANTENNAS<tr><td width="70%">Loop type</td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">Waveguide type</td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">Other type: short; long</td><td><b><b>9/00</b>; <b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">DEVICES FOR INFLUENCING RADIATED WAVES<tr><td width="70%">Quasi-optical; absorbing</td><td><b><b>15/00</b>; <b>17/00</b></b></td></tr></tr></tr><tr><td width="70%">COMBINATIONS OF PRIMARY ACTIVE ELEMENTS WITH SECONDARY DEVICES</td><td><b><b>19/00</b></b></td></tr></tr><tr><td width="70%">COMBINATIONS OF ANTENNAS  WITH ACTIVE CIRCUITS OR CIRCUIT ELEMENTS</td><td><b><b>23/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS PROVIDING MORE THAN ONE RADIATION PATTERN</td><td><b><b>25/00</b></b></td></tr></tr><tr><td width="70%">ANTENNA  ARRAYS OR SYSTEMS</td><td><b><b>21/00</b></b></td></tr></tr><tr><td width="70%">SPECIAL ARRANGEMENTS<tr><td width="70%">Details; orientation; simultaneity</td><td><b><b>1/00</b>; <b>3/00</b>; <b>5/00</b></b></td></tr></tr></tr></table>	2016
H01R		導電接続；互いに絶縁された多数の電気接続要素の構造的な集合体；嵌合装置；集電装置<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―全ての種類の取りはずし可能，および取りはずし不可能な電線接続装置，嵌合装置，ランプまたは類似物のホルダ，あるいは全ての種類の電線，ケーブル，または装置に対する集電装置；<br>―印刷回路への，または印刷回路間の，電気接続のための印刷されない手段<br>（２）このサブクラスは特殊な装置内，または装置上の接続部の取付けを包含しない。このような取付けはその装置に関連のあるサブクラスに包含される。例．接続箱または配電箱内の取付けは，Ｈ０２ＢまたはＨ０２Ｇに包含され，加熱素子に対する高温接続部はＨ０５Ｂ３／０８に包含される。特殊な電気装置と嵌合装置の一部の構造的な集合体はその装置と共に分類される。例．白熱電球と口金との関連はサブクラスＨ０１Ｋに分類される。<br>（３）このサブクラスでは，下記の表現は以下に示す意味で用いる：［７］<br>―“ピン”とは，接触を得るために適切な形のソケットにかみあうようになっている，剛性，または柔軟性のある導体のことである。［７］<br>―“ソケット”とは，電気的接触を得るために，当該のピンを受け入れるようになっている，剛性，または柔軟性のある導体のことである。［７］<br>―“嵌合装置”とは，電気の通り道を設けたり解除したりするために，他の道具を用いずに，繰り返し物理的なはめ合わせや取り外しができるように用いられる２つ又は２つ以上の部品を持つ装置のことである。２つ以上の部品を持つ，こうした装置の例としては，ａ）二つの嵌合部品を結びつけるアダプタ；及び，ｂ）対応するもう片方との，複数の目立たない接続部を持つレールまたはバスバー［７］<br>（４）一般的な細部はグループ４／００，９／００，１１／００，１２／００に分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>接続；接続要素<br>直接；絶縁体−突き刺し　４／００<br>構造的な集合体：<br>相互絶縁される導電部材用の，間隔をあけた２つ以上の接続箇所を有する複数の電気接続部材の　９／００<br>印刷回路基板，フラットまたはリボン・ケーブルに　１２／００<br>互いに接続される導電部材用の，間隔をあけた２つ以上の接続箇所を有する個々の接続部材　１１／００<br>端子　９／００；１２／００<br>他の接続　３／００<br>嵌合<br>導体と導電部材間の直接接触　４／００<br>他の細部　１３／００<br>２つの部品からなる嵌合の全体構造　２４／００<br>複数の相手方部品と共働するのに適した嵌合部品　２５／００；２７／００；２９／００<br>相手方部品に支持された嵌合部品　３１／００<br>装置を支持するためのホルダを有する嵌合　３３／００<br>可撓性または屈曲可能な電線接続器　３５／００<br>集電装置<br>回転型；非回転型　３９／００；４１／００<br>製造　４３／００	ELECTRICALLY-CONDUCTIVE CONNECTIONS; STRUCTURAL ASSOCIATIONS OF A PLURALITY OF MUTUALLY-INSULATED ELECTRICAL CONNECTING ELEMENTS; COUPLING DEVICES; CURRENT COLLECTORS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>all kinds of contact-making disconnectable and non-disconnectable electric line connecting devices, coupling devices, lamp or similar holders or current collectors for all kinds of electric lines, cables or apparatus;</li><li>non-printed means for electric connections to or between printed circuits.</li></ul></li><li>This subclass <u>does not cover</u> mounting of connections in or on specified apparatus. Such mounting is covered by the relevant subclass for such apparatus, e.g. mounting in junction or distribution boxes is covered by subclass <b>H02B</b> or <b>H02G</b>, high-temperature connections for heating elements is covered by group <b>H05B3/08</b>. Structural association of one part of a coupling device with specific electric apparatus is classified with the apparatus, e.g. association of cap with incandescent lamp is covered by subclass <b>H01K</b>.</li><li>In this subclass, the following expressions are used with the meaning indicated: <ul><li>"pin" is a rigid or flexible conductor for engagement with an appropriately shaped socket to establish contact therewith;</li><li>"socket" is a rigid or flexible conductor for receiving an appropriate pin to establish electrical contact therewith;</li><li>"coupling devices" are devices having two or more parts specially adapted so as to be capable of ready and repeated physical engagement or disengagement, without the use of a tool, for the purpose of establishing or breaking an electrical path. Examples of such devices having more than two parts: <ul><li>adapters for linking two coupling parts;</li><li>rails or bus-bars provided with a plurality of discrete connecting locations for counterparts.</li></ul></li></ul></li><li>General details are classified in groups <b>H01R4/00</b>, <b>H01R9/00</b>, <b>H01R11/00</b>, <b>H01R12/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CONNECTIONS; CONNECTING ELEMENTS<tr><td width="70%">Direct; Insulation-penetrating </td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">Structural associations:<tr><td width="70%">of a plurality of mutually-insulated connecting elements </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">for printed circuits, flat or ribbon cables </td><td><b><b>12/00</b></b></td></tr></tr></tr><tr><td width="70%">Individual connecting elements providing two or more spaced connecting locations </td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">Terminals </td><td><b><b>9/00</b>; <b>12/00</b></b></td></tr></tr><tr><td width="70%">Other connections </td><td><b><b>3/00</b></b></td></tr></tr></tr><tr><td width="70%">COUPLINGS<tr><td width="70%">Direct connections between conductors and conductive members of coupling </td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">Other details </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">Overall structure of two-part couplings </td><td><b><b>24/00</b></b></td></tr></tr><tr><td width="70%">Coupling parts for multiple or alternative co-operation with counterparts </td><td><b><b>25/00</b>, <b>27/00</b>, <b>29/00</b></b></td></tr></tr><tr><td width="70%">Coupling parts supported by counterpart </td><td><b><b>31/00</b></b></td></tr></tr><tr><td width="70%">Couplings having holders for supporting apparatus </td><td><b><b>33/00</b></b></td></tr></tr></tr><tr><td width="70%">FLEXIBLE OR TURNABLE LINE CONNECTORS </td><td><b><b>35/00</b></b></td></tr></tr><tr><td width="70%">CURRENT COLLECTORS<tr><td width="70%">Rotary; non-rotary </td><td><b><b>39/00</b>; <b>41/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>43/00</b></b></td></tr></tr></table>	4935
H01S		光を増幅または生成するために，放射の誘導放出による光増幅［レーザ］を用いた装置；光領域以外の電磁放射の誘導放出を用いた装置［２０１９．０１］<br><br><b><ul>注</ul></b><br>このサブクラスは以下のものを包含する：<br>　ａ．単色でコヒーレントな電磁放射を増幅または生成するための励起原子または分子による放射の誘導放出を用いた装置；<br>　ｂ．このような単色でコヒーレントな電磁放射を変調，復調，制御または安定化するような機能。<br><br><b><ul>サブクラス内の索引</ul></b><br>メーザ　１／００<br>半導体レーザ　５／００<br>半導体レーザ以外のレーザ　３／００<br>誘導放出を用いたその他の装置　４／００	DEVICES USING THE PROCESS OF LIGHT AMPLIFICATION BY STIMULATED EMISSION OF RADIATION [LASER] TO AMPLIFY OR GENERATE LIGHT; DEVICES USING STIMULATED EMISSION OF ELECTROMAGNETIC RADIATION IN WAVE RANGES OTHER THAN OPTICAL; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>devices using the stimulated emission of radiation by excited atoms or molecules to amplify or generate coherent monochromatic electromagnetic radiation;</li><li>functions as modulating, demodulating, controlling or stabilising such coherent monochromatic electromagnetic radiation.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">MASERS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">SEMICONDUCTOR LASERS </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">LASERS OTHER THAN SEMICONDUCTOR LASERS </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">OTHER DEVICES USING STIMULATED EMISSION </td><td><b><b>4/00</b></b></td></tr></tr></table>	741
H01T		スパークギャップ；スパークギャップを用いる過電圧避雷器；スパークプラグ；コロナ放電装置；密閉されない気体中へ導入されるイオンの発生（過電圧保護回路Ｈ０２Ｈ）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“スパークギャップ”とは，冷電極を有し，かつ，短時間に多量の電気エネルギーを放電するために限って用いられる密閉型または非密閉型の放電装置を意味する。［４］<br><br><b><ul>サブクラス内の索引</ul></b><br>スパークギャップ<br>回転するもの　７／００<br>補助的なトリガ手段を含むもの　２／００<br>特殊な適用：発振のための；整流のための　９／００；１１／００<br>過電圧避雷器；アークホーン　４／００<br>その他のスパークギャップ　１４／００<br>細部　１／００<br>スパークプラグ　１３／００<br>回路　１５／００<br>コロナ放電用装置　１９／００<br>製造，保守　２１／００<br>イオン発生装置　２３／００	SPARK GAPS; OVERVOLTAGE ARRESTERS USING SPARK GAPS; SPARKING PLUGS; CORONA DEVICES; GENERATING IONS TO BE INTRODUCED INTO NON-ENCLOSED GASES(overvoltage protection circuits <b>H02H</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following expression is used with the meaning indicated:<ul><li>"spark gaps" means enclosed or non-enclosed discharge device having cold electrodes and used exclusively to discharge a quantity of electrical energy in a small time duration. </li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">SPARK GAPS<tr><td width="70%">Rotary </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">Comprising auxiliary triggering means </td><td><b><b>2/00</b></b></td></tr></tr><tr><td width="70%">Special adaptations: for oscillations; for rectifiers </td><td><b><b>9/00</b>; <b>11/00</b></b></td></tr></tr><tr><td width="70%">Overvoltage arresters; arcing horns </td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">Other spark gaps </td><td><b><b>14/00</b></b></td></tr></tr><tr><td width="70%">Details </td><td><b><b>1/00</b></b></td></tr></tr></tr><tr><td width="70%">SPARKING PLUGS </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">CIRCUITS </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">DEVICES FOR CORONA DISCHARGE </td><td><b><b>19/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE, MAINTENANCE </td><td><b><b>21/00</b></b></td></tr></tr><tr><td width="70%">APPARATUS FOR GENERATING IONS </td><td><b><b>23/00</b></b></td></tr></tr></table>	304
H02		電力の発電，変換，配電	GENERATION, CONVERSION, OR DISTRIBUTION OF ELECTRIC POWER	
H02B		電力の供給または配電のための盤，変電所または開閉装置<br><br><b><ul>注</ul></b><br>このサブクラスは，配電盤，開閉所，開閉装置あるいはそれらの据え付け，または開閉器相互の組合せあるいは開閉器と他の装置（例．変圧器，ヒューズ，メーターまたは配電盤；変電所または配電点を構成するかかる組立体）との組合せを包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>配電盤；変電所または開閉装置の細部　１／００<br>変電所　５／００，７／００<br>開閉装置　１１／００，１３／００<br>監視机または板　１５／００<br>製造　３／００	BOARDS, SUBSTATIONS OR SWITCHING ARRANGEMENTS FOR THE SUPPLY OR DISTRIBUTION OF ELECTRIC POWER; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> boards, switchyards, switchgear or their installation, or the association of switching devices with each other or with other devices, e.g. transformers, fuses, meters or distribution boards; such associations constitute substations or distribution points.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">BOARDS, OR DETAILS OF SUBSTATIONS OR SWITCHING ARRANGEMENTS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">SUBSTATIONS </td><td><b><b>5/00</b>, <b>7/00</b></b></td></tr></tr><tr><td width="70%">SWITCHGEAR </td><td><b><b>11/00</b>, <b>13/00</b></b></td></tr></tr><tr><td width="70%">SUPERVISORY DESKS OR PANELS </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>3/00</b></b></td></tr></tr></table>	1364
H02G		電気ケーブルまたは電線の，もしくは光と電気の複合ケーブルまたは電線の据付け<br><br><b><ul>注</ul></b><br>（１）このサブクラスは，電力ケーブルまたは電力線，もしくは光と電気の複合ケーブルまたは電線の据え付けのほかに，通信ケーブル，通信線または避雷用導体の据え付けを包含する。<br>（２）このサブクラスは純粋の光ケーブルを包含せず，それはグループＧ０２Ｂ６／４６に包含する。［６］<br>（３）このサブクラスにおいて，下記の表現は以下に示す意味で用いる：<br>―“電気ケーブル”は電気導体と組み合わせた光導体，例．ファイバー，からなるケーブルを含む。［６］<br><br><b><ul>サブクラス内の索引</ul></b><br>据え付けの主要な型<br>内側；頭上；地下または水中　３／００；７／００；９／００<br>特殊な据え付け<br>ブスバー；避雷用導体；移動部分　５／００；１３／００；１１／００<br>ケーブル付属品　１５／００<br>据え付け，保守，修理　１／００	INSTALLATION OF ELECTRIC CABLES OR LINES, OR OF COMBINED OPTICAL AND ELECTRIC CABLES OR LINES; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> installation of communication cables or lines, including those comprising a combination of optical and electrical conductors, or of lightning conductors as well as installation of power cables or lines.</li><li>This subclass <u>does not cover</u> installation of purely optical cables, which is covered by group <b>G02B6/46</b>. </li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"electric cable" includes cables comprising optical conductors, e.g. fibres, in combination with electrical conductors. </li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">PRINCIPAL TYPES OF INSTALLATIONS<tr><td width="70%">Inside; overhead; underground or underwater </td><td><b><b>3/00</b>; <b>7/00</b>; <b>9/00</b></b></td></tr></tr></tr><tr><td width="70%">SPECIAL INSTALLATIONS<tr><td width="70%">Of bus-bars; of lightning conductors; of movable parts </td><td><b><b>5/00</b>; <b>13/00</b>; <b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">CABLE FITTINGS </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">INSTALLING, MAINTAINING, REPAIRING </td><td><b><b>1/00</b></b></td></tr></tr></table>	2935
H02H		非常保護回路装置（正常でない動作状態の指示または警報Ｇ０１Ｒ，例．Ｇ０１Ｒ３１／００，Ｇ０８Ｂ；線路に沿った故障点測定Ｇ０１Ｒ３１／０８；非常保護装置Ｈ０１Ｈ）<br><br><b><ul>注</ul></b><br>このサブクラスは，正常動作状態から異常状態へ変化する場合における電線，電気機械または電気装置の自動保護のための回路装置のみを包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>非常保護回路装置<br>状況の変化に応じて自動的に開放またはスイッチングするもの<br>電気的；検知された非電気的；模擬された非電気的　３／００；５／００；６／００<br>特殊な機器またはケーブルまたは線路の区間保護に適用されるもの　７／００<br>過電流または過電圧の制限　９／００<br>望ましくない状況のときの通電防止　１１／００<br>細部　１／００	EMERGENCY PROTECTIVE CIRCUIT ARRANGEMENTS(indicating or signalling undesired working conditions <b>G01R</b>, e.g. <b>G01R31/00</b>, <b>G08B</b>; locating faults along lines <b>G01R31/08</b>; emergency protective devices <b>H01H</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> only circuit arrangements for the automatic protection of electric lines or electric machines or apparatus in the event of an undesired change from normal working conditions.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">EMERGENCY PROTECTIVE CIRCUIT ARRANGEMENTS<tr><td width="70%">For automatic disconnection or switching responsive to variation of conditions:<tr><td width="70%">electric; sensed non-electric; simulated non-electric </td><td><b><b>3/00</b>; <b>5/00</b>; <b>6/00</b></b></td></tr></tr><tr><td width="70%">adapted for specific machines or for sectionalised protection of cables or lines </td><td><b><b>7/00</b></b></td></tr></tr></tr><tr><td width="70%">For limiting excess current or voltage </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">For preventing switching-on in case of undesired conditions </td><td><b><b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr></table>	1459
H02J		電力網；電力給電または電力配電のための回路装置または方式；電気エネルギーを蓄積するための方式<br><br><b><ul>注</ul></b><br>注<br>１．このサブクラスは以下のものを包含する：<br>・直流，交流または不特定の幹線または配電網；<br>・直流，交流または不特定の電力網の遠隔操作；<br>・負荷が回路装置に対して何らの特殊な制限効果をもたない時に電池を充電または放電するための回路装置；<br>・直流または交流の動力網と相互作用のある，他に分類されない長期エネルギー蓄積方式<br>・ワイヤレスで電力給電または電力配電を行うための回路装置または方式；<br>・スマートグリッドの運用の観点，すなわち，改良電力インフラストラクチャのための電力，通信および情報各技術の統合がエンドユースアプリケーションの進化を促しながら負荷に電力を供給すること。<br>２．このサブクラスは以下のものを包含しない：<br>・サブクラスＨ０１ＦまたはＨ０２Ｋに包含される型式の単一の電動機，発電機または回転変換機の制御，ただし，これはサブクラスＨ０２Ｐに包含される；<br>・サブクラスＨ０２Ｎに包含される型式の単一の電動機または発電機の制御，ただし，これはサブクラスＨ０２Ｎに包含される。<br>３．このサブクラスでは，グループＨ０２Ｊ１０１／００〜Ｈ０２Ｊ１０７／００のインデキシングコードを付加することが望ましい。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>回路装置<br>配電網のためのもの：<br>直流；交流　１／００；３／００<br>結合されるもの；特定されないもの　４／００<br>電池のためのもの　７／００<br>非常用または待機用の給電のためのもの　９／００<br>局の補助設備への電力供給のためのもの　１１／００<br>回路状態の遠隔指示のためのもの　１３／００<br>電気エネルギーを蓄積する方式　１５／００<br>ワイヤレスで電力給電または電力配電を行うための回路装置または方式　５０／００	ELECTRIC POWER NETWORKS; CIRCUIT ARRANGEMENTS OR SYSTEMS FOR SUPPLYING OR DISTRIBUTING ELECTRIC POWER; SYSTEMS FOR STORING ELECTRIC ENERGY; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>AC, DC or unspecified mains or power distribution networks;</li><li>remote operation of AC, DC or unspecified power networks;</li><li>circuit arrangements for charging or discharging batteries when the load has no particular limiting effect on the circuit arrangement;</li><li>long-term energy storage systems not otherwise provided for, having an interaction with AC or DC power networks;</li><li>circuit arrangements or systems for wireless supply or distribution of electric power;</li><li>operational aspects of smart grids, namely the integration of power, communications and information technologies for an improved electric power infrastructure serving loads while providing for evolution of end-use applications.</li></ul></li><li>This subclass <u>does not cover</u>: <ul><li>the control of a single motor, generator or dynamo-electric converter of the types covered by subclasses <b>H01F</b> or <b>H02K</b>, which is covered by subclass <b>H02P</b>;</li><li>the control of a single motor or generator of the types covered by subclass <b>H02N</b>, which is covered by subclass <b>H02N</b>.</li></ul></li><li>In this subclass, it is desirable to add the indexing codes of groups <b>H02J101/00 to H02J107/00</b> .</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CIRCUIT ARRANGEMENTS<tr><td width="70%">for distribution networks:<tr><td width="70%">Direct current; alternative current</td><td><b><b>1/00</b>; <b>3/00</b></b></td></tr></tr><tr><td width="70%">combined; not specified</td><td><b><b>4/00</b></b></td></tr></tr></tr><tr><td width="70%">for batteries</td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">for emergency or stand-by power supply</td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">for power supply to auxiliaries of stations</td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">for providing remote indication of network conditions</td><td><b><b>13/00</b></b></td></tr></tr></tr><tr><td width="70%">SYSTEMS FOR STORING ELECTRIC ENERGY</td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">CIRCUIT ARRANGEMENTS OR SYSTEMS FOR WIRELESS SUPPLY OR DISTRIBUTION OF ELECTRIC POWER</td><td><b><b>50/00</b></b></td></tr></tr></table>	2051
H02K		発電機，電動機（動電型継電器Ｈ０１Ｈ５３／００；直流または交流入力−サージ出力変換Ｈ０２Ｍ９／００）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは制御を目的とする発電機または電動機の構造を包含する。<br>（２）このサブクラスは電動機，発電機または回転変換機の起動，調整，電子的整流，制動，またはその他の制御，一般を包含しない，ただし，これらはサブクラスＨ０２Ｐに包含される。<br>（３）“マイクロ構造の装置”および“マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。［７］<br><br><b><ul>サブクラス内の索引</ul></b><br>電動機または発電機<br>連続的に回転するもの<br>交流機：非同期機；同期機；機械的整流子を有するもの　１７／００，１９／００，２１／００，２７／００<br>直流機または交直両用機：機械的整流子を有するもの；断続器を有するもの　２３／００，２５／００<br>非機械的整流子を有するもの　２９／００<br>非周期的な電機；振動電機；ステップ回転電動機　３１／００；３３／００，３５／００，３７／００<br>非正弦波形を発生する発電機　３９／００<br>２以上の回転子または固定子を有する電機　１６／００<br>特殊な電動装置<br>回転角位置を伝送する電機；トルク電動機　２４／００，２６／００<br>プラズマまたは導電性液体の流れまたは導電性または磁性粒子との機械―電気相互作用による機械　４４／００<br>固体を経路に沿って移動させる方式　４１／００<br>変換機　４７／００<br>電動クラッチまたはブレーキ；電動歯車　４９／００；５１／００<br>永久運動と称されるもの　５３／００<br>低温で作動する電機　５５／００<br>細部<br>磁気回路；巻線；外枠　１／００，３／００，５／００<br>機械エネルギーを取扱うための機械と構造的に結合した装置；冷却；測定または保護装置；集電または整流　７／００，９／００，１１／００，１３／００<br>製造　１５／００  <br>このサブクラスの他のグループに包含されない事項　９９／００	DYNAMO-ELECTRIC MACHINES(dynamo-electric relays <b>H01H53/00</b>; conversion of DC or AC input power into surge output power <b>H02M9/00</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> the structural adaptation of dynamo-electric machines for the purpose of their control.</li><li>This subclass <u>does not cover</u> starting, regulating, electronically commutating, braking, or otherwise controlling motors, generators or dynamo-electric converters, in general, which is covered by subclass <b>H02P</b>.</li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to "microstructural devices" and "microstructural systems".   </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">MOTORS OR GENERATORS<tr><td width="70%">Continuously rotating<tr><td width="70%">AC machines: asynchronous; synchronous; with mechanical commutators</td><td><b><b>17/00</b>; <b>19/00</b>, <b>21/00</b>; <b>27/00</b></b></td></tr></tr><tr><td width="70%">DC machines or universal AC/DC motors: with mechanical commutators; with interrupters</td><td><b><b>23/00</b>; <b>25/00</b></b></td></tr></tr><tr><td width="70%">with non-mechanical commutating devices</td><td><b><b>29/00</b></b></td></tr></tr></tr><tr><td width="70%">Acyclic machines; oscillating machines; motors rotating step by step</td><td><b><b>31/00</b>; <b>33/00</b>, <b>35/00</b>; <b>37/00</b></b></td></tr></tr><tr><td width="70%">Generators producing a non-sinusoidal waveform</td><td><b><b>39/00</b></b></td></tr></tr><tr><td width="70%">Machines with more than one rotor or stator</td><td><b><b>16/00</b></b></td></tr></tr></tr><tr><td width="70%">SPECIAL DYNAMO-ELECTRIC APPARATUS<tr><td width="70%">Machines for transmitting angular displacements; torque motors</td><td><b><b>24/00</b>; <b>26/00</b></b></td></tr></tr><tr><td width="70%">Machines involving dynamo-electric interaction with a plasma or a flow of conductive liquid or of fluid-borne conductive or magnetic particles</td><td><b><b>44/00</b></b></td></tr></tr><tr><td width="70%">Systems for propulsing a rigid body along a path</td><td><b><b>41/00</b></b></td></tr></tr><tr><td width="70%">Converters</td><td><b><b>47/00</b></b></td></tr></tr><tr><td width="70%">Dynamo-electric clutches or brakes; dynamo-electric gears</td><td><b><b>49/00</b>; <b>51/00</b></b></td></tr></tr><tr><td width="70%">Alleged <u>perpetua mobilia</u></td><td><b><b>53/00</b></b></td></tr></tr><tr><td width="70%">Machines operating at cryogenic temperatures</td><td><b><b>55/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS<tr><td width="70%">Magnetic circuits; windings; casings</td><td><b><b>1/00</b>; <b>3/00</b>; <b>5/00</b></b></td></tr></tr><tr><td width="70%">Arrangements structurally associated with the machine for handling mechanical energy; cooling; measuring or protective devices; current collection or commutation</td><td><b><b>7/00</b>; <b>9/00</b>; <b>11/00</b>; <b>13/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE</td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	3454
H02M		交流−交流，交流−直流または直流−直流変換装置，および主要な，または類似の電力供給システムと共に使用するための装置：直流または交流入力−サージ出力変換；そのための制御または調整（変成器Ｈ０１Ｆ；回転変換機Ｈ０２Ｋ４７／００；変成器，リアクトルまたはチョークコイルの制御，電動機，発電機または回転変換機の制御または調整Ｈ０２Ｐ）<br><br><b><ul>注</ul></b><br>注［４］<br>１．このサブクラスは電力の変換のための回路または装置，またはこのような回路または装置の制御または調整のための装置のみを包含する。<br>２．このサブクラスは電力を変換するときに用いられる個々の電気装置を包含しない。これらの装置は関連するサブクラス，例．インダクタ，変圧器Ｈ０１Ｆ，蓄電器，電解整流器Ｈ０１Ｇ，水銀整流器または他の放電管Ｈ０１Ｊ，電力の伝送に主として関係のないインピーダンス回路網または共振回路Ｈ０３Ｈ，半導体装置Ｈ１０に包含される。<br>３．このサブクラスにおいては，下記の用語は以下に示す意味で用いる：<br>・“変換”とは，電気変量に関して，変量のパラメータ，例．振幅，周波数，位相，極性，の１または２以上の変更を意味する。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>細部　１／００<br>変換の様式<br>直流から直流へ　３／００<br>交流から交流へ　５／００<br>交流から直流および直流から交流へ　７／００<br>直流または交流からサージ出力へ　９／００<br>その他の電力変換システム　１１／００	APPARATUS FOR CONVERSION BETWEEN AC AND AC, BETWEEN AC AND DC, OR BETWEEN DC AND DC, AND FOR USE WITH MAINS OR SIMILAR POWER SUPPLY SYSTEMS; CONVERSION OF DC OR AC INPUT POWER INTO SURGE OUTPUT POWER; CONTROL OR REGULATION THEREOF (transformers <b>H01F</b>;  dynamo-electric converters <b>H02K47/00</b>;  controlling transformers, reactors or choke coils, control or regulation of electric motors, generators or dynamo-electric converters <b>H02P</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> only circuits or apparatus for the conversion of electric power, or arrangements for control or regulation of such circuits or apparatus.</li><li>This subclass <u>does not cover</u> the individual electro-technical devices employed when converting electric power. Such devices are covered by the relevant subclasses, e.g. inductors, transformers <b>H01F</b>, capacitors, electrolytic rectifiers <b>H01G</b>, mercury-vapour rectifying or other discharge tubes <b>H01J</b>, impedance networks or resonant circuits not primarily concerned with the transfer of electric power <b>H03H</b>, semiconductor devices <b>H10</b>.</li><li>In this subclass, the following term is used with the meaning indicated: <ul><li>"conversion", in respect of an electric variable, e.g. voltage or current, means the change of one or more of the parameters of the variable, e.g. amplitude, frequency, phase, polarity.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">DETAILS</td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">TYPES OF CONVERSION<tr><td width="70%">DC to DC</td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">AC to AC</td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">AC to DC and <u>vice versa</u></td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">DC or AC to surge output power</td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">other power conversion systems</td><td><b><b>11/00</b></b></td></tr></tr></tr></table>	1707
H02N		他類に属しない電機<br><br><b><ul>注</ul></b><br>注［７］<br>１．このサブクラスは以下のものを包含する：<br>・静電発電機，電動機，クラッチまたは把持装置；<br>・他の非動電的発電機または電動機；<br>・磁気的吸引または反発力を用いる支持または浮上装置；<br>・第２の電機を結合して運転するものを除いた前記のような電機の始動，調整，ブレーキあるいは制御のための装置。<br>２．“マイクロ構造の装置”および“マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。<br>３．発電機，電動機または電気と他の形態のエネルギとを変換するその他の手段の特殊設備は，他のサブクラス中に，例．クラスＨ１０及びサブクラスＨ０１Ｍ，Ｈ０２Ｋ，Ｈ０４Ｒ中に，同様に存在する。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>発電機，電動機<br>静電的なもの　１／００<br>熱によるイオン化および電荷の除去を用いた発電機；熱効果を用いた電動機　３／００；１０／００<br>光輻射を電気エネルギに変換するもの　６／００<br>その他　１１／００<br>圧電効果，電歪または磁歪を用いる電機一般　２／００<br>静電クラッチまたは把持装置　１３／００<br>磁気による支持または浮上装置　１５／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	ELECTRIC MACHINES NOT OTHERWISE PROVIDED FOR; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>electrostatic generators, motors, clutches, or holding devices;</li><li>other non-dynamo-electric generators or motors;</li><li>holding or levitation devices using magnetic attraction or repulsion;</li><li>arrangements for starting, regulating, braking, or otherwise controlling such machines unless in conjoint operation with a second machine.</li></ul></li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to "microstructural devices" and "microstructural systems".</li><li>Specific provision for generators, motors, or other means for converting between electric and other forms of energy also exists in other subclasses, e.g. in class <b>H10</b> and subclasses <b>H01M</b>, <b>H02K</b>, <b>H04R</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">GENERATORS, MOTORS<tr><td width="70%">With electrostatic effect</td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Generators using thermal ionisation and removal of charge; electric motors using thermal effects</td><td><b><b>3/00</b>; <b>10/00</b></b></td></tr></tr><tr><td width="70%">Others</td><td><b><b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">ELECTRIC MACHINES IN GENERAL USING PIEZOELECTRIC EFFECT, ELECTROSTRICTION OR MAGNETOSTRICTION</td><td><b><b>2/00</b></b></td></tr></tr><tr><td width="70%">ELECTROSTATIC CLUTCHES OR HOLDING DEVICES</td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">MAGNETIC HOLDING OR LEVITATING DEVICES</td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	496
H02P		電動機，発電機，回転変換機の制御または調整；変圧器，リアクトルまたはチョークコイルの制御［４］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは，関連サブクラス，例．Ｈ０１Ｆ，Ｈ０２Ｋに分類される型の電動機，発電機，回転変換機，クラッチ，ブレーキ，歯車，変圧器，リアクトルまたはチョークコイルを起動，調整，電子的整流，ブレーキまたはその他の方法で制御する装置を包含する。<br>（２）このサブクラスは，サブクラスＨ０２Ｎに分類される型の機器に対する同様な装置は包含しない。ただし，これらの装置はそのサブクラスに包含される。<br>（３）このサブクラスでは，グループＨ０２Ｐ１０１／００およびＨ０２Ｐ１０３／００のインデキシングコードを付加することが望ましい。［２０１５．０１］<br><br><b><ul>サブクラス内の索引</ul></b><br>起動装置；減速，停止　１／００；３／００<br>異なる供給源に接続可能な電動機を制御する装置　４／００<br>２以上の電動機を制御するための装置　５／００<br>回転子の位置に依存する電子整流子を有する同期電動機または他の電動機の制御装置　６／００<br>直流電動機の制御装置　７／００<br>ステップ回転電動機の制御装置　８／００<br>発電機から所望出力を得る装置　９／００<br>変換器から所望出力を得る装置；電機的なもの；静止型のもの　１１／００；１３／００<br>ブレーキまたはクラッチの制御装置　１５／００<br>電動歯車の制御装置　１７／００<br>ベクトル制御による発電機の制御装置　２１／００<br>ベクトル制御以外の方法による交流発動機の制御装置　２３／００<br>交流電動機の種類または構造的細部に特徴があるもの　２５／００<br>供給電圧の種類に特徴があるもの　２７／００<br>交流発動機および直流発動機双方に適した制御装置　２９／００<br>他に分類されない制御装置　３１／００	CONTROL OR REGULATION OF ELECTRIC MOTORS, ELECTRIC GENERATORS OR DYNAMO-ELECTRIC CONVERTERS; CONTROLLING TRANSFORMERS, REACTORS OR CHOKE COILS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> arrangements for starting, regulating, electronically commutating, braking, or otherwise controlling motors, generators, dynamo-electric converters, clutches, brakes, gears, transformers, reactors or choke coils, of the types classified in the relevant subclasses, e.g. <b>H01F</b>, <b>H02K</b>.</li><li>This subclass <u>does not cover</u> similar arrangements for the apparatus of the types classified in subclass <b>H02N</b>, which arrangements are covered by that subclass.</li><li>In this subclass, it is desirable to add the indexing codes of groups <b>H02P101/00</b> and <b>H02P103/00</b>.  </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">ARRANGEMENTS FOR STARTING; FOR SLOWING, STOPPING </td><td><b><b>1/00</b>; <b>3/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING ELECTRIC MOTORS THAT CAN BE CONNECTED TO DIFFERENT POWER SUPPLIES </td><td><b><b>4/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING TWO OR MORE ELECTRIC MOTORS </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING SYNCHRONOUS MOTORS OR OTHER DYNAMO-ELECTRIC MOTORS WITH ELECTRONIC COMMUTATORS IN DEPENDENCE ON THE ROTOR POSITION </td><td><b><b>6/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING DC MOTORS </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING DYNAMO-ELECTRIC MOTORS ROTATING STEP BY STEP </td><td><b><b>8/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR OBTAINING DESIRED OUTPUT OF GENERATOR </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR OBTAINING DESIRED OUTPUT OF CONVERTERS: DYNAMO-ELECTRIC; STATIC </td><td><b><b>11/00</b>; <b>13/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING BRAKES OR CLUTCHES </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING DYNAMO-ELECTRIC GEARS </td><td><b><b>17/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING ELECTRIC MACHINES BY VECTOR CONTROL </td><td><b><b>21/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING AC MOTORS BY METHODS OTHER THAN VECTOR CONTROL </td><td><b><b>23/00</b></b></td></tr></tr><tr><td width="70%">CHARACTERISED BY THE KIND OF AC MOTORS OR BY STRUCTURAL DETAILS </td><td><b><b>25/00</b></b></td></tr></tr><tr><td width="70%">CHARACTERISED BY THE KIND OF SUPPLY VOLTAGE </td><td><b><b>27/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING APPROPRIATE FOR BOTH AC AND DC MOTORS </td><td><b><b>29/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR CONTROLLING NOT OTHERWISE PROVIDED FOR </td><td><b><b>31/00</b></b></td></tr></tr></table>	1654
H02S		赤外線，可視光または紫外光の変換による電力発電，例．光起電［ＰＶ］モジュールを使用するもの（放射線源からの電気的エネルギーの取得Ｇ２１Ｈ１／１２；光に感応する無機半導体装置Ｈ１０Ｆ；光に感応する有機半導体装置Ｈ１０Ｋ３０／００；熱電装置Ｈ１０Ｎ１０／００；焦電装置Ｈ１０Ｎ１５／００）［２０１４．０１］	GENERATION OF ELECTRIC POWER BY CONVERSION OF INFRARED RADIATION, VISIBLE LIGHT OR ULTRAVIOLET LIGHT, e.g. USING PHOTOVOLTAIC [PV] MODULES  (obtaining electrical energy from radioactive sources <b>G21H1/12</b>;   light sensitive inorganic semiconductor devices <b>H10F</b>;  light sensitive organic semiconductor devices <b>H10K30/00</b>; thermoelectric devices <b>H10N10/00</b>;   pyroelectric devices <b>H10N15/00</b>)	146
H03		電子回路	ELECTRONIC CIRCUITRY	
H03B		振動の発生，直接のまたは周波数変換による振動の発生，スイッチング動作を行なわない能動素子を用いた回路による振動の発生；このような回路による雑音の発生（電気機械的手段による楽器に特別に適合する発生器Ｇ１０Ｈ；メーザまたはレーザＨ０１Ｓ；プラズマにおける振動の発生Ｈ０５Ｈ）<br><br><b><ul>サブクラス内の索引</ul></b><br>周波数変換によらない発生<br>増巾と帰還による手段；負性抵抗　５／００；７／００<br>電子走行時間による手段；電子ビーム管　９／００；１３／００<br>衝撃励振によるもの；ホール効果；放射源と検出器の組み合わせ　１１／００；１５／００；１７／００<br>周波数変換による発生<br>信号の逓倍または逓降によるもの　１９／００<br>非変調信号の結合によるもの　２１／００<br>発生した振動の特殊性<br>周波数範囲の掃引；多重周波数；多重位相；雑音　２３／００；２５／００；２７／００；２９／００<br>その他の発生方法　２８／００<br>細部　１／００	GENERATION OF OSCILLATIONS, DIRECTLY OR BY FREQUENCY-CHANGING, BY CIRCUITS EMPLOYING ACTIVE ELEMENTS WHICH OPERATE IN A NON-SWITCHING MANNER; GENERATION OF NOISE BY SUCH CIRCUITS(generators specially adapted for electrophonic musical instruments <b>G10H</b>; masers or lasers <b>H01S</b>;  generation of oscillations in plasma <b>H05H</b>);<br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">GENERATION WITHOUT FREQUENCY-CHANGING<tr><td width="70%">By means of amplification and feedback; negative resistance </td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr><tr><td width="70%">By means of transit-time tubes; electron-beam tubes </td><td><b><b>9/00</b>; <b>13/00</b></b></td></tr></tr><tr><td width="70%">By shock-exciting; Hall effect; radiation source and detectors </td><td><b><b>11/00</b>; <b>15/00</b>; <b>17/00</b></b></td></tr></tr></tr><tr><td width="70%">GENERATION WITH FREQUENCY- CHANGING<tr><td width="70%">By multiplication or division of a signal </td><td><b><b>19/00</b></b></td></tr></tr><tr><td width="70%">By combining unmodulated signals </td><td><b><b>21/00</b></b></td></tr></tr></tr><tr><td width="70%">PARTICULARITIES OF GENERATED OSCILLATIONS<tr><td width="70%">Swept-over frequency range; multi-frequency; multiphase; noise </td><td><b><b>23/00</b>; <b>25/00</b>; <b>27/00</b>; <b>29/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER METHODS OF GENERATION </td><td><b><b>28/00</b></b></td></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr></table>	427
H03C		変調（メーザまたはレーザＨ０１Ｓ；符号化，復号化または符号変換Ｈ０３Ｍ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは正弦波振動または電磁波についての変調，キーイングまたは断続のみを包含する。変調信号は所望の波形でよい。<br>（２）このサブグラスにおいては，変調器としても復調器としても用いることができる回路は，その種の変調器を扱うグループに分類される。	MODULATION(masers or lasers <b>H01S</b>; coding, decoding or code conversion <b>H03M</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> only modulation, keying, or interruption of sinusoidal oscillations or electromagnetic waves, the modulating signal having any desired waveform.</li><li>In this subclass, circuits usable both as modulator and demodulator are classified in the group dealing with the type of modulator involved.</li></ul>	140
H03D		一つの搬送波から他の搬送波への変換または変調の復調（メーザ，レーザＨ０１Ｓ；変調器としても復調器としても動作する回路Ｈ０３Ｃ，例．平衡変調器Ｈ０３Ｃ１／５４；変調器にも周波数変換器にも適用できる細部Ｈ０３Ｃ；パルス復調で常時変化する信号を変調したものＨ０３Ｋ９／００；パルス変調形式の変換Ｈ０３Ｋ１１／００；継電器システム，例．中継器Ｈ０４Ｂ７／１４；デジタル搬送波変調方式に適した復調器Ｈ０４Ｌ２７／００；カラーテレビジョンに適合した同期復調器Ｈ０４Ｎ９／６６）<br><br><b><ul>注</ul></b><br>このサブクラスは以下のもののみを包含する：<br>―１つの正弦波，搬送波または電磁波上に変調された信号の復調または変換；<br>―互いに独立な２つの振動の位相または周波数の比較<br><br><b><ul>サブクラス内の索引</ul></b><br>復調<br>振幅；角度；複合；超再生　１／００；３／００；５／００，９／００；１１／００<br>変換　７／００，９／００<br>位相または周波数の比較　１３／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	DEMODULATION OR TRANSFERENCE OF MODULATION FROM ONE CARRIER TO ANOTHER(masers, lasers <b>H01S</b>; circuits capable of acting both as modulator and demodulator <b>H03C</b>, e.g. balanced modulators <b>H03C1/54</b>; details applicable to both modulators and frequency-changers <b>H03C</b>; demodulating pulses which have been modulated with a continuously-variable signal <b>H03K9/00</b>; transforming types of pulse modulation <b>H03K11/00</b>; relay systems, e.g. repeater stations <b>H04B7/14</b>; demodulators adapted for digitally modulated-carrier systems <b>H04L27/00</b>; synchronous demodulators adapted for colour television <b>H04N9/66</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> only:<ul><li>demodulation or transference of signals modulated on a sinusoidal carrier or on electromagnetic waves;</li><li>comparing phase or frequency of two mutually-independent oscillations.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">DEMODULATION<tr><td width="70%">Amplitude; angle; combined; super-regenerative </td><td><b><b>1/00</b>; <b>3/00</b>; <b>5/00</b>, <b>9/00</b>; <b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">TRANSFERENCE </td><td><b><b>7/00</b>, <b>9/00</b></b></td></tr></tr><tr><td width="70%">COMPARING PHASE OR FREQUENCY </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS </td><td><b><b>99/00</b></b></td></tr></tr></table>	169
H03F		増幅器<br><br><b><ul>注</ul></b><br>このサブクラスは以下のものを包含する：<br>―線形増幅器，すなわち入力と出力の振幅の間に線形関係があるもの，出力が入力とほぼ同じ波形をもつもの；<br>―誘電体増幅器，磁気増幅器，および発振器または周波数変換器として使われる場合のパラメトリック増幅器；<br>―誘電体増幅器およびパラメトリック増幅器の能動素子の構造で，他に分類されないもの<br><br><b><ul>サブクラス内の索引</ul></b><br>電子管または半導体を用いる増幅器；細部　３／００，５／００；１／００<br>パラメトリック増幅器　７／００<br>磁気増幅器；誘電体増幅器　９／００；１１／００<br>特別な素子を用いる増幅器<br>機械的または音響的；ホール効果を用いるもの；エレクトロルミネセントを用いるもの；超伝導を用いるもの　１３／００；１５／００；１７／００；１９／００<br>その他の増幅器　９９／００	AMPLIFIERS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>linear amplification, there being linear relationship between the amplitudes of input and output, and the output having substantially the same waveform as the input;</li><li>dielectric amplifiers, magnetic amplifiers, and parametric amplifiers when used as oscillators or frequency-changers;</li><li>constructions of active elements of dielectric amplifiers and parametric amplifiers if no provision exists elsewhere.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">AMPLIFIERS USING TUBES OR SEMICONDUCTORS; DETAILS </td><td><b><b>3/00</b>, <b>5/00</b>; <b>1/00</b></b></td></tr></tr><tr><td width="70%">PARAMETRIC AMPLIFIERS </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">MAGNETIC; DIELECTRIC AMPLIFIERS </td><td><b><b>9/00</b>; <b>11/00</b></b></td></tr></tr><tr><td width="70%">AMPLIFIERS USING SPECIAL ELEMENTS<tr><td width="70%">Mechanical or acoustic; using Hall effect; electroluminescent; superconductive </td><td><b><b>13/00</b>; <b>15/00</b>; <b>17/00</b>; <b>19/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER AMPLIFIERS </td><td><b><b>99/00</b></b></td></tr></tr></table>	813
H03G		増幅の制御<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する。<br>―増幅器または周波数変換器の利得の制御；<br>―増幅器の周波数範囲の制御；<br>―振幅の制限または振幅の変化率の制限<br>（２）サブクラスＨ０３Ｆのタイトルに続く注に注意すること。［３］<br><br><b><ul>サブクラス内の索引</ul></b><br>利得調整　３／００<br>音質調整　５／００<br>圧縮器または伸張器；リミッタ　７／００；１１／００<br>２種以上の形式の制御の結合　９／００<br>細部　１／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	CONTROL OF AMPLIFICATION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>control of gain of amplifiers or frequency-changers;</li><li>control of frequency range of amplifiers;</li><li>limiting amplitude or rate of change of amplitude.</li></ul></li><li>Attention is drawn to the Note following the title of subclass <b>H03F</b>. </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">GAIN CONTROL </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">TONE CONTROL </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">COMPRESSORS OR EXPANDERS; LIMITERS </td><td><b><b>7/00</b>; <b>11/00</b></b></td></tr></tr><tr><td width="70%">COMBINATION OF TWO OR MORE TYPES OF CONTROL </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS </td><td><b><b>99/00</b></b></td></tr></tr></table>	309
H03H		インピーダンス回路網，例．共振回路；共振器（導波管，導波管型の共振器，線路または他の装置Ｈ０１Ｐ）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―集中定数インピーダンス素子を含む回路網；<br>―集中定数インピーダンスと共に分布定数インピーダンス素子を含む回路網；<br>―電気機械的または電気音響的素子を含む回路網；<br>―リアクタンスを擬似し，放電管または半導体装置を含む回路網；<br>―電気機械的共振器の構造<br>（２）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“受動素子”とは抵抗器，容量素子，インダクター，相互インダクターまたはダイオードを意味する。［３］<br>（３）“マイクロ構造の装置”および“マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。［７］<br>（４）このサブクラスにおいては上位番号のメイングループが優先する。［３］<br><br><b><ul>サブクラス内の索引</ul></b><br>回路<br>適応型のもの　２１／００<br>デイジタル技術を用いるもの　１７／００<br>トランスバーサルフィルター　１５／００<br>受動素子のみを用いるもの：<br>一端子対；多端子対　５／００；７／００<br>電気機械的または電気音響的素子を用いるもの　９／００<br>能動素子を用いるもの　１１／００<br>時間変化要素を用いるもの　１９／００<br>他の素子または技術を用いるもの　２／００<br>細部　１／００<br>製造　３／００	IMPEDANCE NETWORKS, e.g. RESONANT CIRCUITS; RESONATORS  (waveguides, resonators, lines or other devices of the waveguide type <b>H01P</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>networks comprising lumped impedance elements;</li><li>networks comprising distributed impedance elements together with lumped impedance elements;</li><li>networks comprising electromechanical or electro-acoustic elements;</li><li>networks simulating reactances and comprising discharge tubes or semiconductor devices;</li><li>constructions of electromechanical resonators.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated:<ul><li>"passive elements" means resistors, capacitors, inductors, mutual inductors, or diodes. </li></ul></li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to "microstructural devices" and "microstructural systems".</li><li>In this subclass, main groups with a higher number take precedence. </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">NETWORKS<tr><td width="70%">Adaptive </td><td><b><b>21/00</b></b></td></tr></tr><tr><td width="70%">Using digital techniques </td><td><b><b>17/00</b></b></td></tr></tr><tr><td width="70%">Transversal filters </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">Using passive elements only:<tr><td width="70%">one port; multi-port </td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr></tr><tr><td width="70%">Using electromechanical or electro-acoustical elements </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">Using active elements </td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">Using time varying elements </td><td><b><b>19/00</b></b></td></tr></tr><tr><td width="70%">Using other elements or techniques </td><td><b><b>2/00</b></b></td></tr></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE </td><td><b><b>3/00</b></b></td></tr></tr></table>	590
H03J		同調共振回路；選択共振回路<br><br><b><ul>注</ul></b><br>このサブクラスは，同調と他の機能の結合した制御，例．同調の制御と音量と制御との結合，局部発振器の制御と付加的共振回路の制御との結合も含めて，同調の制御も包含する。［３］<br><br><b><ul>サブクラス内の索引</ul></b><br>同調<br>連続　３／００<br>非連続　５／００<br>自動周波数制御　７／００<br>遠隔制御　９／００<br>自動周波数掃引　７／００<br>細部　１／００	TUNING RESONANT CIRCUITS; SELECTING RESONANT CIRCUITS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> also the control of tuning, including the combined control of tuning and other functions, e.g. combinations of tuning control and volume control, combinations of control of local oscillator and of supplementary resonant circuits. </li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">TUNING<tr><td width="70%">Continuous </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">Discontinuous </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">Automatic frequency control </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">Remote control </td><td><b><b>9/00</b></b></td></tr></tr></tr><tr><td width="70%">AUTOMATIC FREQUENCY SCANNING </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr></table>	268
H03K		パルス技術（パルス特性の測定Ｇ０１Ｒ；パルスによる正弦波振動の変調Ｈ０３Ｃ；デジタル情報の伝送Ｈ０４Ｌ；振動の周期を計数または積分することによって２つの信号の間の位相差を検出する弁別器回路Ｈ０３Ｄ３／０４；自動制御，発生器の形に関係しないまたは特定されていない電子振動またはパルス発生器の起動，同期または安定化Ｈ０３Ｌ；符号化，復号化または符号変換一般Ｈ０３Ｍ）［４］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―信号の発生，計数，増幅，整形，変調，復調，またはその他の操作を行うために非連続またはスイッチング方法で作動する能動素子を使用する方法，回路，装置，または機器；<br>―メークおよびブレークする接点を含まない電子的スイッチング；<br>―電気的パルスを取り扱う論理回路<br>（２）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“能動素子”は振動またはエネルギーの不連続な流れへの入力エネルギの変換についての制御を行う。<br>（３）このサブクラスにおいては，特許文献の請求事項が特定の回路素子が限定されていない場合，その文献は，文献中に記された実施態様において使われた素子に基づいて分類する。［６］<br><br><b><ul>サブクラス内の索引</ul></b><br>パルスの発生<br>回路；有限の傾斜またはステップ部分を持つパルス　３／００；４／００<br>正弦波からのパルスの発生　１２／００<br>計数以外のパルスの操作<br>変調；復調；変換　７／００；９／００；１１／００<br>その他　５／００，６／００<br>パルス計数器，周波数分割器<br>計数連鎖を持つもの；積算するもの；閉ループをもつもの；多安定素子をもつもの　２３／００；２５／００；２７／００；２９／００<br>細部　２１／００<br>特殊な応用<br>電子的スイッチング；論理回路　１７／００；１９／００	PULSE TECHNIQUE(measuring pulse characteristics <b>G01R</b>; modulating sinusoidal oscillations with pulses <b>H03C</b>;  transmission of digital information <b>H04L</b>; discriminator circuits detecting phase difference between two signals by counting or integrating cycles of oscillation <b>H03D3/04</b>; automatic control, starting, synchronisation or stabilisation of generators of electronic oscillations or pulses where the type of generator is irrelevant or unspecified <b>H03L</b>; coding, decoding or code conversion, in general <b>H03M</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> : <ul><li>methods, circuits, devices or apparatus using active elements operating in a discontinuous or switching manner for generating, counting, amplifying, shaping, modulating, demodulating or otherwise manipulating signals;</li><li>electronic switching not involving contact-making and breaking;</li><li>logic circuits handling electric pulses.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"active element" exercises control over the conversion of input energy into an oscillation or a discontinuous flow of energy.</li></ul></li><li>In this subclass, where the claims of a patent document are not limited to a specific circuit element, the document is classified at least according to the elements used in the described embodiment.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">GENERATING PULSES<tr><td width="70%">Circuits; with finite slope or stepped portions </td><td><b><b>3/00</b>; <b>4/00</b></b></td></tr></tr></tr><tr><td width="70%">PRODUCING PULSES FROM SINEWAVES </td><td><b><b>12/00</b></b></td></tr></tr><tr><td width="70%">MANIPULATING PULSES OTHER THAN WHEN COUNTING<tr><td width="70%">Modulating; demodulating; transfer </td><td><b><b>7/00</b>; <b>9/00</b>; <b>11/00</b></b></td></tr></tr><tr><td width="70%">Other </td><td><b><b>5/00</b>, <b>6/00</b></b></td></tr></tr></tr><tr><td width="70%">PULSE COUNTERS, FREQUENCY DIVIDERS<tr><td width="70%">With counting chains; with integration; with a closed loop; with multistable elements </td><td><b><b>23/00</b>; <b>25/00</b>; <b>27/00</b>; <b>29/00</b></b></td></tr></tr><tr><td width="70%">Details </td><td><b><b>21/00</b></b></td></tr></tr></tr><tr><td width="70%">SPECIAL APPLICATIONS<tr><td width="70%">Electronic switching; logic circuits </td><td><b><b>17/00</b>; <b>19/00</b></b></td></tr></tr></tr></table>	1801
H03L		電子的振動またはパルス発生器の自動制御，起動，同期または安定化（振動の発生Ｈ０３Ｂ）<br><br><b><ul>注</ul></b><br>１．このサブクラスは以下のものを包含する：<br>・電子的振動またはパルス発生器に対する自動制御回路；<br>・発生器の形成が関係しないまたは特定されていない発生器に対する起動，同期または安定化<br>２．このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“自動制御”は閉ルーブ系のみを包含する。	AUTOMATIC CONTROL, STARTING, SYNCHRONISATION OR STABILISATION OF GENERATORS OF ELECTRONIC OSCILLATIONS OR PULSES(generation of oscillations <b>H03B</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>automatic control circuits for generators of electronic oscillations or pulses;</li><li>starting, synchronisation or stabilisation circuits for generators where the type of generator is irrelevant or unspecified.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"automatic control" covers only closed loop systems.</li></ul></li></ul>	199
H03M		符号化，復号化または符号変換一般（流体的手段を用いるものＦ１５Ｃ４／００；光学的アナログ／デジタル変換器Ｇ０２Ｆ７／００；特殊な用途に特に適した符号化，復号化または符号変換は，関連するサブクラス，例．Ｇ０１Ｄ，Ｇ０１Ｒ，Ｇ０６Ｆ，Ｇ０６Ｔ，Ｇ０９Ｇ，Ｇ１０Ｌ，Ｇ１１Ｂ，Ｇ１１Ｃ，Ｈ０４Ｂ，Ｈ０４Ｌ，Ｈ０４Ｍ，Ｈ０４Ｎ，を参照；秘密の必要性を含む暗号または他の目的のための暗号化または暗号解読Ｇ０９Ｃ）［４］<br><br><b><ul>サブクラス内の索引</ul></b><br>符号化および復号化<br>一般　１／００<br>異なった変調へまたは異なった変調からの　３／００<br>キーボードに関連するもの　１１／００<br>変換<br>個々のデジットの形式の　５／００<br>デジットの順序の　７／００<br>並列／直列またはその逆　９／００<br>誤りの検出または誤りの訂正　１３／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	CODING, DECODING OR CODE CONVERSION, IN GENERAL(using fluidic means <b>F15C4/00</b>; optical analogue/digital converters <b>G02F7/00</b>; coding, decoding or code conversion, specially adapted for particular applications, <u>see</u> the relevant subclasses, e.g. <b>G01D</b>, <b>G01R</b>, <b>G06F</b>, <b>G06T</b>, <b>G09G</b>, <b>G10L</b>, <b>G11B</b>, <b>G11C</b>, <b>H04B</b>, <b>H04L</b>, <b>H04M</b>, <b>H04N</b>; ciphering or deciphering for cryptography or other purposes involving the need for secrecy <b>G09C</b>);<br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CODING AND DECODING<tr><td width="70%">in general </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">to or from differential modulation </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">in connection with keyboards </td><td><b><b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">CONVERSION<tr><td width="70%">of the form of individual digits </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">of the sequence of digits </td><td><b><b>7/00</b></b></td></tr></tr><tr><td width="70%">parallel/series or vice versa </td><td><b><b>9/00</b></b></td></tr></tr></tr><tr><td width="70%">ERROR DETECTION OR ERROR CORRECTION </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS </td><td><b><b>99/00</b></b></td></tr></tr></table>	562
H04		電気通信技術<br><br><b><ul>注</ul></b><br>このクラスは，伝搬路として，微粒子放射線，音波または電磁波を使用する電気通信方式，例，無線または光通信，を包含する。［４］	ELECTRIC COMMUNICATION TECHNIQUE; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This class <u>covers</u> electrical communication systems with propagation paths employing beams of corpuscular radiation, acoustic waves or electromagnetic waves, e.g. radio or optical communication. </li></ul>	
H04B		伝送［４］<br><br><b><ul>注</ul></b><br>このサブクラスは情報を搬送する信号の伝送，情報の性質に依存しない伝送を包含し，そして監視および試験用装置ならびに雑音および妨害の抑圧および制限を含む。<br><br><b><ul>サブクラス内の索引</ul></b><br>細部　１／００<br>伝送に利用される媒体によって特徴づけられた方式<br>導体を利用するもの　３／００<br>自由空間を利用するもの　５／００〜１１／００<br>その他　１３／００<br>伝送媒体によって特徴づけられない方式　１４／００<br>雑音または妨害の抑圧または制限　１５／００<br>監視；試験　１７／００	TRANSMISSION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> the transmission of information-carrying signals, the transmission being independent of the nature of the information, and includes monitoring and testing arrangements and the suppression and limitation of noise and interference.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">SYSTEMS CHARACTERISED BY THE MEDIUM USED FOR TRANSMISSION<tr><td width="70%">Using conductors </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">Using free-space propagation </td><td><b><b>5/00 to 11/00</b> </b></td></tr></tr><tr><td width="70%">Others </td><td><b><b>13/00</b></b></td></tr></tr></tr><tr><td width="70%">SYSTEMS NOT CHARACTERISED BY THE MEDIUM USED FOR TRANSMISSION </td><td><b><b>14/00</b></b></td></tr></tr><tr><td width="70%">SUPPRESSION OR LIMITATION OF NOISE OR INTERFERENCE </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">MONITORING, TESTING </td><td><b><b>17/00</b></b></td></tr></tr></table>	3997
H04H		放送通信（多重通信Ｈ０４Ｊ；放送方式における画像通信の観点Ｈ０４Ｎ）<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>・“放送”とは，複数の受信局への同一信号の同時配信である。“放送”には，受信局自身からの要求または応答によって制御される受信局への配信は含まれない。<br>・“放送情報”とは，放送システムを使って配信されるあらゆる種類の情報を包含する。<br>・“放送関連情報”とは，放送情報ではないが，放送システムを介して提供されるサービスのために必要な情報である。<br>・“放送時間”とは，特定の放送情報が存在し，利用可能となっている時間である。<br>・“放送チャネル”とは，放送情報を配送する際に介するチャネル，例．搬送波，放送時間帯，ケーブルまたは無線放送サービスエリア，である。<br>・“放送空間”とは，特定の放送情報が存在し利用可能となっている放送チャネルの集合か，または，その放送チャネルの集合によって決定される地理的範囲である。<br>・“放送時空”とは，特定の放送情報が存在し利用可能となっている放送空間および放送時間によって決定される時空である。<br>・“放送システム”とは，放送のための送信機，中継器および受信機からなるシステムである。<br>・“放送関連システム”とは，放送情報の作成，放送，受信または利用による影響を直接受けるシステムである。<br>・“放送サービス”とは，放送システムによって直接提供されるサービス，すなわち，放送情報の分配サービスである。<br>・“放送関連サービス”とは，放送関連システムによって提供されるサービスである。<br>・“ＡがＢに直接結合する”とは，ＡがＢに直接影響を与えるか，または，ＡがＢから直接影響を受けることである。	BROADCAST COMMUNICATION(multiplex communication <b>H04J</b>; pictorial communication aspects of broadcast systems <b>H04N</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following terms or expressions are used with the meaning indicated:<ul><li>&ldquo;broadcast&rdquo; is simultaneous distribution of identical signals to plural receiving stations. The term "broadcast" does not include distribution to receiving stations which is controlled by requests or responses from the receiving stations;</li><li>&ldquo;broadcast information&rdquo; covers all kinds of information distributed by broadcast systems;</li><li>&ldquo;broadcast-related information&rdquo; is information required by services provided via broadcast systems, other than broadcast information;</li><li>&ldquo;broadcast time&rdquo; is a time when particular broadcast information exists and is available;</li><li>&ldquo;broadcast channel&rdquo; is a channel via which broadcast information is distributed, e.g. carrier waves, time slots, cables or wireless broadcast service areas;</li><li>&ldquo;broadcast space&rdquo; is either a set of broadcast channels in which particular broadcast information exists and is available or a geographical area determined by the set of broadcast channels;</li><li>&ldquo;broadcast space-time&rdquo; is space-time determined by broadcast space and broadcast time in which particular broadcast information exists and is available;</li><li>&ldquo;broadcast system&rdquo; is a system which consists of transmitter, transponder and receiver for broadcast;</li><li>&ldquo;broadcast-related system&rdquo; is a system which is directly affected by generation, broadcast, reception or use of broadcast information;</li><li>&ldquo;broadcast service&rdquo; is a service directly provided by a broadcast system, i.e. distribution service of broadcast information;</li><li>&ldquo;broadcast-related service&rdquo; is a service provided by broadcast-related systems;</li><li>&ldquo;A with a direct linkage to B&rdquo; means that A directly affects B or that A is directly affected by B.</li></ul></li></ul>	433
H04J		多重通信（デジタル情報の伝送に特有のものＨ０４Ｌ５／００；２以上のテレビジョン信号の同時伝送または順次伝送のための方式Ｈ０４Ｎ７／０８；交換におけるものＨ０４Ｑ１１／００）<br><br><b><ul>注</ul></b><br>このサブクラスは以下のものを包含する：<br>―同一伝送路上に複数個の信号を同時的または順次的に伝送する目的でそれらの信号を結合または分離するための回路または装置；<br>―そのための監視装置	MULTIPLEX COMMUNICATION(peculiar to transmission of digital information <b>H04L5/00</b>; systems for the simultaneous or sequential transmission of more than one television signal <b>H04N7/08</b>; in exchanges <b>H04Q11/00</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>circuits or apparatus for combining or dividing signals for the purpose of transmitting them simultaneously or sequentially over the same transmission path;</li><li>monitoring arrangements therefor.</li></ul></li></ul>	644
H04K		秘密通信；通信妨害<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“秘密通信”は有線および無線の秘密伝送方式，すなわち，送信局の装置で信号を変形し，受信局でそれに対応して修正する装置なしでは情報を明瞭に受信できないような伝送方式を含む。	SECRET COMMUNICATION; JAMMING OF COMMUNICATION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following expression is used with the meaning indicated:<ul><li>"secret communication" includes secret line and radiation transmission systems, i.e. those in which apparatus at the transmitting station modifies the signal in such a way that the information cannot be intelligibly received without corresponding modifying apparatus at the receiving station.</li></ul></li></ul>	145
H04L		デジタル情報の伝送，例．電信通信（電信通信と電話通信に共通の装置Ｈ０４Ｍ）［４］<br><br><b><ul>注</ul></b><br>１．このサブクラスはデジタル形式で供給された信号の伝送を包含し，そしてデータ伝送，電信通信または監視のための方法もしくは配置を包含する<br>２．このサブクラスに分類する場合は，グループＨ０４Ｌ１０１／００のインデキシングコードを付加することが望ましい<br><br><b><ul>サブクラス内の索引</ul></b><br>用いる符号によるもの：長短符号；等長符号；細部　１５／００；１７／００；１３／００<br>その他の観点から：ステップバイステップ；モザイク印刷機；他の方式　１９／００；２１／００；２３／００<br>ベースバンド・システム　２５／００<br>変調された搬送方式　２７／００<br>データ交換ネットワーク　１２／００<br>一般に適用される配置<br>保護：誤り；秘密　１／００；９／００<br>多重通信；同期　５／００；７／００<br>データ交換ネットワークの保守，運用または管理のための配置　Ｈ０４Ｌ４１／００<br>データ交換ネットワークを監視または試験するための配置　Ｈ０４Ｌ４３／００<br>データ交換ネットワーク内のパケットのルーティングまたはパス探索　Ｈ０４Ｌ４５／００<br>データ交換ネットワークにおけるトラフィック制御　Ｈ０４Ｌ４７／００<br>パケット交換要素　Ｈ０４Ｌ４９／００<br>ストアアンドフォワード転送またはリアルタイム転送プロトコルによる，パケット交換ネットワーク内のユーザ間のメッセージ転送　Ｈ０４Ｌ５１／００<br>アドレッシングまたはネーミングのためのネットワーク配置，プロトコルまたはサービス　Ｈ０４Ｌ６１／００<br>データパケット通信におけるリアルタイムアプリケーションを支援するためのネットワーク配置，プロトコルまたはサービス　Ｈ０４Ｌ６５／００<br>ネットワークサービスまたはネットワークアプリケーションを支援するためのネットワークの配置またはプロトコル　Ｈ０４Ｌ６７／００<br>他のグループに包含されない配置，装置または方式　Ｈ０４Ｌ６９／００	TRANSMISSION OF DIGITAL INFORMATION, e.g. TELEGRAPHIC COMMUNICATION(arrangements common to telegraphic and telephonic communication <b>H04M</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> transmission of signals having been supplied in digital form and includes data transmission, telegraphic communication, or methods or arrangements for monitoring.</li><li>In this subclass it is desirable to add the indexing codes of group <b>H04L101/00</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">SYSTEMS CHARACTERISED BY:<tr><td width="70%">The code used: Morse; Baudot; details</td><td><b><b>15/00</b>; <b>17/00</b>; <b>13/00</b></b></td></tr></tr><tr><td width="70%">Otherwise: step by step; mosaic printers; other systems</td><td><b><b>19/00</b>; <b>21/00</b>; <b>23/00</b></b></td></tr></tr></tr><tr><td width="70%">BASEBAND SYSTEMS</td><td><b><b>25/00</b></b></td></tr></tr><tr><td width="70%">MODULATED-CARRIER SYSTEMS</td><td><b><b>27/00</b></b></td></tr></tr><tr><td width="70%">DATA SWITCHING NETWORKS</td><td><b><b>12/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS OF GENERAL APPLICATION<tr><td width="70%">Cryptography; Security, Errors; Network security</td><td><b><b>1/00</b>; <b>9/00</b></b></td></tr></tr><tr><td width="70%">Multiple communications; synchronising</td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr><tr><td width="70%">Arrangements for maintenance, administration or management of data switching networks</td><td><b><b>41/00</b></b></td></tr></tr><tr><td width="70%">Arrangements for monitoring or testing data switching networks</td><td><b><b>43/00</b></b></td></tr></tr><tr><td width="70%">Routing or path finding of packets in data switching networks</td><td><b><b>45/00</b></b></td></tr></tr><tr><td width="70%">Traffic control in data switching networks</td><td><b><b>47/00</b></b></td></tr></tr><tr><td width="70%">Packet switching elements</td><td><b><b>49/00</b></b></td></tr></tr><tr><td width="70%">User-to-user messaging in packet-switching networks, transmitted according to store-and-forward or real-time protocols</td><td><b><b>51/00</b></b></td></tr></tr><tr><td width="70%">Network arrangements, protocols or services for addressing or naming</td><td><b><b>61/00</b></b></td></tr></tr><tr><td width="70%">Network arrangements, protocols or services for supporting real-time applications in data packet communication</td><td><b><b>65/00</b></b></td></tr></tr><tr><td width="70%">Network arrangements or protocols for supporting network services or applications</td><td><b><b>67/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER ARRANGEMENTS, APPARATUS OR SYSTEMS</td><td><b><b>69/00</b></b></td></tr></tr></table>	7484
H04M		電話通信（電話ケーブルを通して他の装置を制御するための回路であって電話機開閉装置に関わらないものＧ０８）<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―サブステーションの装置<br>―他の電気的方式と結合された電話通信方式；<br>―電話通信方式に特に適用される試験装置<br>（２）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“加入者”とは，端末装置，例．固定電話，無線電話，携帯電話またはセルラー方式の無線携帯電話の総称，または端末装置の利用者の総称である；　<br>―“サブステーション”とは，単一の加入者をあれこれと区別せずに回線に接続できる端末装置または監視装置を意味する；<br>―“従局”とは，交換局の一形式であってその動作が監視交換局から受信された制御信号に依存するものである；<br>―“交換点”とは，交換局および従局を包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>電話方式<br>他の電気システムとの結合；共同線方式；料金前納方式　１１／００；１３／００；１７／００<br>装置と配置<br>装置　１／００<br>交換：自動：手動　３／００；５／００<br>相互接続配置：中央集中交換；中央集中交換でないもの　７／００；９／００<br>監視および制御；電流供給配置　１５／００；１９／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	TELEPHONIC COMMUNICATION(circuits for controlling other apparatus <u>via</u> a telephone cable and not involving telephone switching apparatus <b>G08</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>substation equipment;</li><li>telephonic communication systems combined with other electrical systems;</li><li>testing arrangements specially adapted for telephonic communication systems.</li></ul></li><li>In this subclass, the following terms or expressions are used with the meanings indicated: <ul><li>"subscriber" is a general term for terminal equipment, e.g. fixed, wireless, mobile or cellular phones, or for a user of terminal equipment;</li><li>"substation" means subscriber or monitoring equipment which may connect a single subscriber to a line without choice as to subscriber;</li><li>"satellite" is a type of exchange the operation of which depends upon control signals received from a supervisory exchange;</li><li>"switching centres" include exchanges and satellites.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">TELEPHONIC SYSTEMS<tr><td width="70%">Combined; party-line systems; prepayment systems </td><td><b><b>11/00</b>; <b>13/00</b>; <b>17/00</b></b></td></tr></tr></tr><tr><td width="70%">EQUIPMENT AND ARRANGEMENTS<tr><td width="70%">Equipment </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Exchanges: automatic; manual </td><td><b><b>3/00</b>; <b>5/00</b></b></td></tr></tr><tr><td width="70%">Interconnection arrangements: centralised; non-centralised </td><td><b><b>7/00</b>; <b>9/00</b></b></td></tr></tr><tr><td width="70%">Monitoring and control; supply arrangements </td><td><b><b>15/00</b>; <b>19/00</b></b></td></tr></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS </td><td><b><b>99/00</b></b></td></tr></tr></table>	5195
H04N		画像通信，例．テレビジョン［４］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する。<br>―下記の二つの手順により，局所的あるいは離れた地点間での画像の伝送またはその瞬時的あるいは恒久的再生：<br>ステップ（ａ）：画像の走査，すなわち．画像を含む全領域を個々の画素に分解し，同時的または順次的に画像を現わす電気信号を引き出すこと；<br>ステップ（ｂ）：個々の画素に分解された画像を現わす電気信号によって，同時的または順次的に画像を含む全領域を再生すること；［４］<br>―グループＨ０４Ｎ１／００において，画像を形成している部分的な光の変化が経時的変化をしない画像またはパターン，例．文書（手書きのものおよび印刷されたもの），地図，図表，映画用フィルムを除く写真，の伝送方式または再生方式；<br>―単に特殊な周波数帯域をもつような信号とは区別されるような画像通信信号，例．テレビジョン信号を処理するように特別に設計された回路<br>（２）このサブクラスは以下のものを包含しない：<br>―他のサブクラスの主題を形成する方式の回路またはその他の部品，ただし，これらは対応するサブクラス，例．Ｈ０３Ｃ，Ｈ０３Ｆ，Ｈ０３Ｊ，Ｈ０４Ｂ，Ｈ０４Ｈに包含される；<br>―アルファベット，文字，数字などの読み易い文字を注（１）のステップ（ａ）により分解して電気信号を取り出し，これを蓄積されている情報と比較することにより上記文字を認識する方式，ただし，これらはサブクラスＧ０６Ｋに包含される；<br>―画像を現わす電気信号を前記ステップ（ａ）により取り出し，これを操作，例．露出の制御，信号として用いる原画の直接写真複写のための方式，ただし，これらはクラスＧ０３に包含される；<br>―アルファベット，文字，数字などの文字形を含む画像を注（１）のステップ（ｂ）により再生する方式であって，例．カム，パンチカードまたはテープ，符号化信号制御，その他の手段によって，上述のステップ（ａ）により取り出される信号と等価な信号の発生を含む方式，ただし，これらは応用分野のためのサブクラス，例．Ｇ０１Ｄ，Ｇ０６Ｔ，Ｈ０４Ｌ，に包含される；<br>―アファベッド，文字，数字などの文字形からなる画像を上述のステップ（ｂ）により再生する方法であって，画像を現わす電気信号を，方式の不可欠部分を構成する文字群またはその記録から上述のステップ（ａ）により発生させる方式，ただし，これらはこのサブクラスに包含されるそれらの応用を条件として，応用のためのサブクラス，例．Ｂ４１Ｂ，Ｇ０６Ｋ，に包含される；<br>―印刷，複製またはマーキング処理，またはそれに用いる材料，ただし，これらは関連するサブクラス，例．Ｂ４１Ｃ，Ｂ４１Ｊ，Ｂ４１Ｍ，Ｇ０３Ｃ，Ｇ０３Ｆ，Ｇ０３Ｇ，に包含される。［４］<br>（３）このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“テレビジョン方式”とは，画像を形成する部分的な光の変化が経時的に変わる画像，例．自然の生の景色や映画のフィルムのような生の景色の記録，を伝送し，再生する方式を意味する。	PICTORIAL COMMUNICATION, e.g. TELEVISION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>transmission of pictures or their transient or permanent reproduction either locally or remotely, by methods involving both the following steps: <ul><li>step (a): the scanning of a picture, i.e. resolving the whole picture-containing area into individual picture-elements and the derivation of picture-representative electric signals related thereto, simultaneously or in sequence;</li><li>step (b): the reproduction of the whole picture-containing area by the reproduction of individual picture-elements into which the picture is resolved by means of picture-representative electric signals derived therefrom, simultaneously or in sequence;</li></ul></li><li>in group <b>H04N1/00</b>, systems for the transmission or the reproduction of arbitrarily composed pictures or patterns in which the local light variations composing a picture are <u>not</u> subject to variation with time, e.g. documents, maps, charts, photographs other than cinematograph films;</li><li>circuits specially designed for dealing with pictorial communication signals, e.g. television signals, as distinct from merely signals of a particular frequency range.</li></ul></li><li>This subclass <u>does not cover</u>: <ul><li>circuits or other parts of systems which form the subject of other subclasses, which are covered by the corresponding subclasses, e.g. <b>H03C</b>, <b>H03F</b>, <b>H03J</b>, <b>H04B</b>, <b>H04H</b>;</li><li>systems in which legible alphanumeric or like character forms are analysed according to step (a) of Note (1) to derive an electric signal from which the character is recognised by comparison with stored information, which are covered by subclass <b>G06K</b>;</li><li>systems for the direct photographic copying of an original picture in which an electric signal representative of the picture is derived according to the said step (a) and employed to modify the operation of the system, e.g. to control exposure, which are covered by class <b>G03</b>;</li><li>systems for the reproduction according to step (b) of Note (1) of pictures comprising alphanumeric or like character forms but involving the production of the <u>equivalent</u> of a signal which would be derived according to the above-mentioned step (a), e.g. by cams, punched card or tape, coded control signal, or other means, which are covered by the subclass for the application, e.g. <b>G01D</b>, <b>G06T</b>, <b>H04L</b>;</li><li>systems for the reproduction according to the above-mentioned step (b) of pictures comprising alphanumeric or like character forms and involving the generation according to the above-mentioned step (a) of picture-representative electric signals from a pre-arranged assembly of such characters, or records thereof, forming an integral part of the systems, which are covered by the subclass for the application, e.g. <b>B41B</b>, <b>G06K</b>, subject to those applications which are covered by this subclass;</li><li>printing, duplication or marking processes, or materials therefor, which are covered by the relevant subclasses, e.g. <b>B41C</b>, <b>B41J</b>, <b>B41M</b>, <b>G03C</b>, <b>G03F</b>, <b>G03G</b>.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"television systems" means those systems for the transmission and reproduction of arbitrarily composed pictures in which the local light variations composing a picture <u>may</u> change with time, e.g. natural "live" scenes, recordings of such scenes such as cinematograph films.</li></ul></li></ul>	4645
H04Q		選択（スイッチ，リレー，セレクタＨ０１Ｈ；無線通信ネットワークＨ０４Ｗ）［１，２００９．０１］<br><br><b><ul>注</ul></b><br>（１）このサブクラスは以下のものを包含する：<br>―接続完成後に情報を伝送するために，多数の（通常２つの）所望局間または主局と多数の（通常１つの）所望サブステーション間の選択接続を行う方法，回路または装置；<br>―すでに完成された接続に沿う選択呼出装置［２００９．０１］<br>（２）このサブクラスにおいては，下記の用語または表現は以下に示す意味で用いる：<br>―“加入者”とは，端末装置，例．加入電話機，の総称である；<br>―“サブステーション”とは，加入者，または加入者をあれこれと区別せずに単一の加入者を回線に接続しうる装置を意味する；<br>―“従局”とは，交換局の一形式であって，その動作が監視交換局から受信された制御信号に依存するものである；<br>―“交換点”とは，交換局および従局を包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>選択配置<br>一般；線路の；多重化系の　３／００；５／００；１１／００<br>遠隔制御または遠隔計測の処理　９／００<br>細部　１／００	SELECTING(switches, relays, selectors <b>H01H</b>;  wireless communication networks <b>H04W</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers </u>: <ul><li>methods, circuits, or apparatus for establishing selectively a connection between a desired number of stations (normally two), or between a main station and a desired number of substations (normally one) for the purpose of transferring information <u>via</u> this connection after it has been established;</li><li>selective calling arrangements over connections already established. </li></ul></li><li>In this subclass, the following terms or expressions are used with the meanings indicated: <ul><li>"subscriber" is a general term for terminal equipment, e.g. telephone for public use;</li><li>"substation" means a subscriber or monitoring equipment which may connect a single subscriber to a line without choice as to subscriber;</li><li>"satellite" is a kind of exchange the operation of which depends upon control signals received from a supervisory exchange;</li><li>"switching centres" includes exchanges and satellites.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">SELECTING ARRANGEMENTS<tr><td width="70%">General; by line; multiplex </td><td><b><b>3/00</b>; <b>5/00</b>;  <b>11/00</b></b></td></tr></tr></tr><tr><td width="70%">DISPOSITIONS FOR TELECONTROL OR TELEMETRY </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">DETAILS </td><td><b><b>1/00</b></b></td></tr></tr></table>	1417
H04R		スピーカ，マイクロホン，蓄音機ピックアップまたは類似の音響電気機械変換器；電気的な補聴器；パブリックアドレスシステム（供給周波数で決まらない周波数を有する音の生成Ｇ１０Ｋ）［６］<br><br><b><ul>注</ul></b><br>注［７］<br>１．このサブクラスは以下のものを包含する。<br>・音響波または電流電圧変化を生ずる，スピーカ，マイクロホン，蓄音機ピックアップまたは類似の変換器；<br>・音盤に溝を切るために電流電圧変化によって駆動される装置；<br>・前記の装置のための回路；<br>・監視または試験<br>２．“マイクロ構造の装置”および“マイクロ構造のシステム”に関する，クラスＢ８１およびサブクラスＢ８１Ｂの両タイトルの後の注に注意すること。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>変換器の型式<br>磁気回路をもつもの：<br>可動線輪型；可動接極子型；磁性材料の振動板をもつもの；磁歪型　９／００；１１／００；１３／００；１５／００<br>磁気回路をもたないもの：<br>圧電型；静電型；可変抵抗型　１７／００；１９／００；２１／００<br>その他の型式　２３／００<br>細部<br>一般；回路；振動板またはコーン　１／００；３／００；７／００<br>応用<br>ステレオ配置；電気的な補聴器；パブリックアドレスシステム　５／００；２５／００；２７／００<br>監視，試験；製造　２９／００；３１／００	LOUDSPEAKERS, MICROPHONES, GRAMOPHONE PICK-UPS OR LIKE ACOUSTIC ELECTROMECHANICAL TRANSDUCERS; ELECTRIC HEARING AIDS; PUBLIC ADDRESS SYSTEMS (producing sounds with frequency not determined by supply frequency <b>G10K</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>:<ul><li>loudspeakers, microphones, gramophone pick-ups or like transducers producing acoustic waves or variations of electric current or voltage;</li><li>arrangements actuated by variations of electric current or voltage for cutting grooves in records;</li><li>circuits for the above-mentioned arrangements;</li><li>monitoring or testing the above-mentioned equipment.</li></ul></li><li>Attention is drawn to the Notes following the titles of class <b>B81</b> and subclass <b>B81B</b> relating to "microstructural devices" and "microstructural systems".</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">TYPES OF TRANSDUCER<tr><td width="70%">With magnetic circuit:<tr><td width="70%">moving coil; moving armature; magnetisable diaphragm; magnetostriction</td><td><b><b>9/00</b>; <b>11/00</b>; <b>13/00</b>; <b>15/00</b></b></td></tr></tr></tr><tr><td width="70%">Without magnetic circuit:<tr><td width="70%">piezoelectric; electrostatic; with variable resistance</td><td><b><b>17/00</b>; <b>19/00</b>; <b>21/00</b></b></td></tr></tr></tr><tr><td width="70%">Other types</td><td><b><b>23/00</b></b></td></tr></tr><tr><td width="70%">Details<tr><td width="70%">general; circuits; diaphragms and cones</td><td><b><b>1/00</b>; <b>3/00</b>; <b>7/00</b></b></td></tr></tr></tr></tr><tr><td width="70%">APPLICATIONS<tr><td width="70%">Stereophonic arrangements; electric hearing aids; public address systems</td><td><b><b>5/00</b>; <b>25/00</b>; <b>27/00</b></b></td></tr></tr></tr><tr><td width="70%">MONITORING, TESTING; MANUFACTURE</td><td><b><b>29/00</b>; <b>31/00</b></b></td></tr></tr></table>	1598
H04S		ステレオ方式［３］<br><br><b><ul>注</ul></b><br>このクラスにおいては，下記の表現は以下に示す意味で用いる：<br>―“ステレオ方式”は４チャンネル方式またはそれと類似の方式を包含する。［３］	STEREOPHONIC SYSTEMS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the following expression is used with the meaning indicated:<ul><li>"stereophonic systems" covers quadraphonic or similar systems. </li></ul></li></ul>	219
H04W		無線通信ネットワーク（放送通信Ｈ０４Ｈ；選択式通信によらない無線接続を用いる通信システム，例．ワイヤレスエクステンションＨ０４Ｍ１／７２）［２００９．０１］<br><br><b><ul>注</ul></b><br>１．このサブクラスは以下のものを包含する。<br>―無線通信回線を介した情報伝達を目的として，希望する数のユーザ間またはユーザとネットワーク装置間で，１つまたはそれ以上の数の無線通信回線を選択的に確立するための通信ネットワーク；<br>―通信ネットワークと接続している無線通信回線のユーザーのモビリティ管理を行うための基盤施設を配備したネットワーク，例．セルラーネットワーク，ＷＬＡＮ［無線ＬＡＮ］，ワイヤレスアクセスネットワーク，例．ＷＬＬ［ワイヤレスローカルループ］または自律分散型ネットワーク，例．アドホックネットワーク；<br>―上述の無線ネットワークに特に適した設計または配置；<br>―上述の無線通信に特に適したサービスまたは設備；<br>―上述の無線通信の運営に特に適した装置または技術；<br>２．このサブクラスは以下のものを包含しない：<br>―無線拡張した通信システム，すなわち，選択式通信によらない無線接続，例．グループＨ０４Ｍ１／７２に包含されるコードレスフォン；<br>―サブクラスＨ０４Ｈに包含される放送通信。このサブクラスでは，ファーストプレイス優先ルールが適用される，すなわち各階層レベルにおいて，相反する指示がない限り，最初の適切な箇所に分類する。［２００９．０１］	WIRELESS COMMUNICATION NETWORKS(broadcast communication <b>H04H</b>; communication systems using wireless links for non-selective communication, e.g. wireless extensions <b>H04M1/72</b>);<br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> : <ul><li>communication networks for selectively establishing one or a plurality of wireless communication links between a desired number of users or between users and network equipment, for the purpose of transferring information via these wireless communication links;</li><li>networks deploying an infrastructure for mobility management of wireless users connected thereto, e.g. cellular networks, WLAN [Wireless Local Area Network], wireless access networks, e.g. WLL [Wireless Local Loop] or self-organising wireless communication networks, e.g. <u>ad hoc</u> networks;</li><li>planning or deployment specially adapted for the above-mentioned wireless networks;</li><li>services or facilities specially adapted for the above-mentioned wireless networks;</li><li>arrangements or techniques specially adapted for the operation of the above-mentioned wireless networks.</li></ul></li><li>This subclass <u>does not cover</u> : <ul><li>communication systems using wireless extensions, i.e. wireless links without selective communication, e.g. cordless telephones, which are covered by group <b>H04M1/72</b>;</li><li>broadcast communication, which is covered by subclass <b>H04H</b>.</li></ul></li></ul>	2316
H05		他に分類されない電気技術	ELECTRIC TECHNIQUES NOT OTHERWISE PROVIDED FOR	
H05B		電気加熱：他に分類されない電気的光源；電気的光源一般の回路装置<br><br><b><ul>注</ul></b><br>このサブクラスにおいては，下記の特別なケースが存在する：<br>ａ．セクションＨ以外のセクションに包含される一般的な応用の中で，電気的な加熱一般がサブクラスＦ２４ＤまたはＦ２４ＨまたはクラスＦ２７に包含されること，および電気的な照明一般が，クラスＦ２１にいくらか包含されることに注意すべきである。それは，セクションＨのＨ０５Ｂに，同じ技術主題を包含する箇所があるからである（セクションＨのタイトルに続く注Ｉ（ｃ）を参照）；<br>ｂ．上記注ａで述べられている２つのケースにおいて，それぞれの主題を扱うセクションＦのサブクラスは，本質的には，第１に装置またはデバイスの全機械的な観点を包含するが，このような装置またはデバイスの電気的観点はサブクラスＨ０５Ｂに包含される；<br>ｃ．照明の場合，この機械的観点は各種の電気的素子の実質的な配置，すなわち，それらの幾何的，または物理的な相対位置を包含することを理解すべきである；これはクラスＦ２１のサブクラスに包含される，素子自体および基本的な回路はセクションＨに残る。同じことは，電気的光源についても，異なる種類の光源を組み合わせる場合に適用される。これらはサブクラスＨ０５Ｂに包含されるが，これらの結合が構成する物理的な配置はクラスＦ２１のサブクラスに包含される；<br>ｄ．加熱に関しては，電気的素子および回路設計のみだけでなく，一般的な応用に関する場合にはそれらの配置の電気的観点もまた，そのようなものとしてサブクラスＨ０５Ｂに包含される；電気炉がそのようなものとして考えられる。炉における電気的素子の物理的配列はセクションＦに包含される，溶接に関して，電気的溶接回路がサブクラスＢ２３Ｋに包含されることと比較してみるならば，電気加熱はセクションＨのタイトルに続く注ＩＩで述べた一般規則に包含されないことが理解できる。<br><br><b><ul>サブクラス内の索引</ul></b><br>電気加熱<br>抵抗によるもの；電界，磁界または電磁界によるもの；放電によるもの　３／００，６／００，７／００<br>組合せた型式のもの　１１／００<br>細部　１／００<br>電気的光源<br>アーク　３１／００<br>エレクトロルミネッセンス　３３／００<br>組合せた型式のもの　３５／００<br>回路装置：<br>白熱光源を制御するためのもの　３９／００<br>放電灯を制御または点弧するためのもの　４１／００<br>エレクトロルミネッセンス光源を制御するためのもの　４４／００<br>発光ダイオード［ＬＥＤ］を制御するためのもの　４５／００<br>可燃性物質を充填使用する光源を制御するためのもの　４６／００<br>一般的な光源を制御するためのもの　４７／００	ELECTRIC HEATING;  ELECTRIC LIGHT SOURCES NOT OTHERWISE PROVIDED FOR; CIRCUIT ARRANGEMENTS FOR ELECTRIC LIGHT SOURCES, IN GENERAL; <br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">ELECTRIC HEATING<tr><td width="70%">Produced by: resistance; electric, magnetic or electromagnetic fields; discharge</td><td><b><b>3/00</b>; <b>6/00</b>; <b>7/00</b></b></td></tr></tr><tr><td width="70%">Combined types</td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">Details</td><td><b><b>1/00</b></b></td></tr></tr></tr><tr><td width="70%">ELECTRIC LIGHT SOURCES<tr><td width="70%">Arc</td><td><b><b>31/00</b></b></td></tr></tr><tr><td width="70%">Electroluminescent</td><td><b><b>33/00</b></b></td></tr></tr><tr><td width="70%">Combined types</td><td><b><b>35/00</b></b></td></tr></tr><tr><td width="70%">Circuit arrangements:<tr><td width="70%">for operating incandescent light sources</td><td><b><b>39/00</b></b></td></tr></tr><tr><td width="70%">for operating or igniting discharge lamps</td><td><b><b>41/00</b></b></td></tr></tr><tr><td width="70%">for operating electroluminescent light sources</td><td><b><b>44/00</b></b></td></tr></tr><tr><td width="70%">for operating light-emitting diodes [LED]</td><td><b><b>45/00</b></b></td></tr></tr><tr><td width="70%">for operating light sources using a charge of combustible material</td><td><b><b>46/00</b></b></td></tr></tr><tr><td width="70%">for operating light sources in general</td><td><b><b>47/00</b></b></td></tr></tr></tr></tr></table>	2965
H05C		生物を殺し，気絶させ，囲い，または導くための装置用に特別に設計された電気回路または電気装置（電気的手段によって昆虫を捕獲，あるいは殺除するための定置式装置Ａ０１Ｍ１／２２；昆虫以外の有害な動物を電気的に駆除する装置Ａ０１Ｍ１９／００；電気仕掛わなＡ０１Ｍ２３／３８；電流による屠殺または気絶Ａ２２Ｂ３／０６）	ELECTRIC CIRCUITS OR APPARATUS SPECIALLY DESIGNED FOR USE IN EQUIPMENT FOR KILLING, STUNNING, ENCLOSING OR GUIDING LIVING BEINGS(stationary means for catching or killing insects by electric means <b>A01M1/22</b>; apparatus for the destruction of noxious animals, other than insects, by electricity <b>A01M19/00</b>; electric traps for animals <b>A01M23/38</b>; slaughtering or stunning by electric current <b>A22B3/06</b>)	137
H05F		静電気；自然に発生する電気<br><br><b><ul>注</ul></b><br>（１）このサブクラスは，物体上の静電荷の形成を防止するための，または静電荷形成後これらの電荷を除去するための方法または装置を包含する。<br>（２）このサブクラスは，前記方法または装置の特殊な応用を包含しない。<br>該装置，例．大型容器における装置Ｂ６５Ｄ９０／４６，は関連のサブクラスに包含される。	STATIC ELECTRICITY; NATURALLY-OCCURRING ELECTRICITY; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> methods or arrangements for preventing the formation of electrostatic charges on bodies or for carrying-off these charges after their formation.</li><li>This subclass <u>does not cover</u> specific applications of the above-mentioned methods or arrangements. Such arrangements are covered by the relevant subclasses, e.g. arrangements in large containers <b>B65D90/46</b>.</li></ul>	74
H05G		Ｘ線技術（Ｘ線の使用による材料の調査または分析Ｇ０１Ｎ２３／００；Ｘ線写真のための装置Ｇ０３Ｂ４２／０２；Ｘ線管Ｈ０１Ｊ３５／００；Ｘ線入力をもつＴＶシステムＨ０４Ｎ５／３２１）	X-RAY TECHNIQUE(investigating or analysing materials by the use of X-rays <b>G01N23/00</b>; apparatus for X-ray photography <b>G03B42/02</b>; X-ray tubes <b>H01J35/00</b>; TV systems having X-ray input <b>H04N5/321</b>)	176
H05H		プラズマ技術（Ｘ線の発生に特に適した装置と方法Ｈ０５Ｇ２／００）；加速された荷電粒子のまたは中性子の発生；中性分子または原子ビームの発生または加速<br><br><b><ul>注</ul></b><br>注［３］<br>（１）このサブクラスは，以下のものを包含する：<br>（ａ）プラズマの発生または取扱い；<br>（ｂ）電子，イオンビームまたは中性粒子を加速する装置；<br>（ｃ）中性粒子ビームを発生させるための装置；<br>（ｄ）（ａ），（ｂ），または（ｃ）のためのターゲット<br>（２）このサブクラスは、サブクラスＨ０１Ｊが包含する放電管または放電ランプ内で電子またはイオンの流れを生成、加速、影響、または利用するための装置を包含しない。<br><br><b><ul>サブクラス内の索引</ul></b><br>プラズマ技術　１／００<br>中性粒子ビームの発生と加速　３／００<br>核反応を起すためのターゲット　６／００<br>粒子加速器<br>直流電圧型加速器；単一パルスを用いる加速器　５／００<br>線型；磁気誘導型；磁気共振型　９／００；１１／００；１３／００<br>その他　１５／００<br>細部　７／００	PLASMA TECHNIQUE (apparatus or processes specially adapted for producing X-rays <b>H05G2/00</b>);PRODUCTION OF ACCELERATED ELECTRICALLY-CHARGED PARTICLES OR OF NEUTRONS; PRODUCTION OR ACCELERATION OF NEUTRAL MOLECULAR OR ATOMIC BEAMS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>generating or handling plasma;</li><li>devices for accelerating electrons, ion beams or neutral particles;</li><li>devices for producing neutral particle beams;</li><li>targets for (a), (b) or (c).</li></ul></li><li>This subclass <u>does not cover</u> devices for producing, accelerating, influencing or using a flow of electrons or ions within electric discharge tubes or discharge lamps, which are covered by subclass <b>H01J</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">PLASMA TECHNIQUE </td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">PRODUCTION OR ACCELERATION OF NEUTRAL PARTICLE BEAMS </td><td><b><b>3/00</b></b></td></tr></tr><tr><td width="70%">TARGETS FOR NUCLEAR REACTIONS </td><td><b><b>6/00</b></b></td></tr></tr><tr><td width="70%">PARTICLE ACCELERATORS<tr><td width="70%">Direct voltage accelerators, accelerators using single pulses </td><td><b><b>5/00</b></b></td></tr></tr><tr><td width="70%">Linear; magnetic induction; magnetic resonance </td><td><b><b>9/00</b>; <b>11/00</b>; <b>13/00</b></b></td></tr></tr><tr><td width="70%">Others </td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">Details </td><td><b><b>7/00</b></b></td></tr></tr></tr></table>	254
H05K		印刷回路；電気装置の箱体または構造的細部，電気部品の組立体の製造<br><br><b><ul>注</ul></b><br>注<br>１．このサブクラスは，以下のものを包含する：<br>・主要な機能を異にする装置とラジオ受信機またはテレビ受像機との組合せ；<br>・印刷によらない電気部品と構造的に結合した印刷回路。<br>２．このサブクラスにおいては，下記の表現は以下に示す意味で用いる：<br>・“印刷回路”は，導体を有する絶縁基板または支持部材からなり，特に平面において分離しないように基板に固定されている導体と構造的に結合している回路の機械的構成のすべてを包含し，さらにその構成を製造，例．絶縁支持部材上での導電性の薄片，ペーストもしくは薄膜の機械的または化学的処理による回路の形成，するための方法または装置も包含する。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>印刷されたものでない電気素子の有無に関しない印刷回路<br>型式，製造　１／００；３／００<br>ケーシング，キャビネットまたはひき出し；構造的細部　５／００；７／００<br>遮蔽　９／００<br>ラジオ受信機またはテレビジョン受像機と他の装置との組み合せ　１１／００<br>電子的組み立て体の製造　１３／００<br>動作の信頼性を改善するための装置　１０／００	PRINTED CIRCUITS; CASINGS OR CONSTRUCTIONAL DETAILS OF ELECTRIC APPARATUS; MANUFACTURE OF ASSEMBLAGES OF ELECTRICAL COMPONENTS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>combinations of a radio or television receiver with apparatus having a different main function;</li><li>printed circuits structurally associated with non-printed electric components.</li></ul></li><li>In this subclass, the following expression is used with the meaning indicated: <ul><li>"printed circuits" covers all kinds of mechanical constructions of circuits that consist of an insulating base or support carrying the conductor and are combined structurally with the conductor throughout their length, especially in a two-dimensional [2D] plane, the conductors of which are secured to the base in a non-dismountable manner, and also covers the processes or apparatus for manufacturing such constructions, e.g. forming the circuit by mechanical or chemical treatment of a conductive foil, paste or film on an insulating support.</li></ul></li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">PRINTED CIRCUITS ASSOCIATED OR NOT ASSOCIATED WITH NON-PRINTED ELECTRIC COMPONENTS<tr><td width="70%">Types; manufacture </td><td><b><b>1/00</b>; <b>3/00</b></b></td></tr></tr></tr><tr><td width="70%">CASINGS, CABINETS OR DRAWERS; CONSTRUCTIONAL DETAILS </td><td><b><b>5/00</b>; <b>7/00</b></b></td></tr></tr><tr><td width="70%">SCREENING </td><td><b><b>9/00</b></b></td></tr></tr><tr><td width="70%">COMBINATIONS OF A RADIO OR TELEVISION RECEIVER WITH OTHER APPARATUS </td><td><b><b>11/00</b></b></td></tr></tr><tr><td width="70%">MANUFACTURE OF ELECTRONIC ASSEMBLAGES </td><td><b><b>13/00</b></b></td></tr></tr><tr><td width="70%">ARRANGEMENTS FOR IMPROVING THE OPERATING RELIABILITY </td><td><b><b>10/00</b></b></td></tr></tr></table>	2951
H10		半導体装置；他に分類されない電気的固体装置［２０２３．０１］	SEMICONDUCTOR DEVICES; ELECTRIC SOLID-STATE DEVICES NOT OTHERWISE PROVIDED FOR	
H10B		電子記憶装置［２０２３．０１］<br><br><b><ul>注</ul></b><br>このサブクラスでは、セクションＣの注（３）の周期表中に示されたＩ〜ＶＩＩＩ族のシステムが用いられる。<br><br><b><ul>サブクラス内の索引</ul></b><br>揮発性記憶装置<br>ＳＲＡＭ　１０／００<br>ＤＲＡＭ　１２／００<br>不揮発性記憶装置<br>ＲＯＭ；ＰＲＯＭ；ＥＰＲＯＭ　２０／００<br>フローティングゲートを含むＥＥＰＲＯＭ　４１／００<br>電荷トラッピングゲート絶縁体を含むＥＥＰＲＯＭ　４３／００<br>強誘電性のメモリトランジスタを含むＦｅＲＡＭ　５１／００<br>強誘電性のメモリキャパシタを含むＦｅＲＡＭ　５３／００<br>ＭＲＡＭ　６１／００<br>抵抗変化メモリ　６３／００<br>他のＥＰＲＯＭ　６９／００<br>複数の装置の組立体　８０／００<br>他の電子記憶装置<br>このサブクラスの他のグループに分類されない主題事項　９９／００<br>	ELECTRONIC MEMORY DEVICES; <br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">VOLATILE MEMORY DEVICES<tr><td width="70%">SRAMs</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">DRAMs</td><td><b><b>12/00</b></b></td></tr></tr></tr><tr><td width="70%">NON-VOLATILE MEMORY DEVICES<tr><td width="70%">ROMs; PROMs; EPROMs</td><td><b><b>20/00</b></b></td></tr></tr><tr><td width="70%">EEPROMs with floating gates</td><td><b><b>41/00</b></b></td></tr></tr><tr><td width="70%">EEPROMs with charge-trapping gate insulators</td><td><b><b>43/00</b></b></td></tr></tr><tr><td width="70%">FeRAMs with ferroelectric memory transistors</td><td><b><b>51/00</b></b></td></tr></tr><tr><td width="70%">FeRAMs with ferroelectric memory capacitors</td><td><b><b>53/00</b></b></td></tr></tr><tr><td width="70%">MRAMs</td><td><b><b>61/00</b></b></td></tr></tr><tr><td width="70%">Resistance change RAMs</td><td><b><b>63/00</b></b></td></tr></tr><tr><td width="70%">Other EPROMs</td><td><b><b>69/00</b></b></td></tr></tr></tr><tr><td width="70%">ASSEMBLIES OF MULTIPLE DEVICES</td><td><b><b>80/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	
H10D		無機電気的半導体装置［２０２５．０１］<br><br><b><ul>注</ul></b><br>注［２０２５．０１］<br>１．このサブクラスは無機半導体本体を有する電気的半導体装置を包含する。この装置は以下の種類の装置を含む；<br>・整流，増幅，発振またはスイッチングに特に適した無機半導体装置，例．トランジスタまたはダイオード；<br>・電位障壁を有する個々の無機抵抗器またはキャパシタ；<br>・電位障壁を有さず，他の半導体構成部品との集積に特に適した，個々の抵抗器，キャパシタまたはインダクタ；<br>・このサブクラスに包含される装置の半導体本体，またはその領域；<br>・このサブクラスに包含される装置の電極；<br>・集積装置，例．ＣＭＯＳ集積装置；<br>・当該装置の製造または処理に特に適した方法または装置<br>２．このサブクラスは以下を包含しない。<br>・サブクラスＨ１０Ｂに包含される，電子記憶装置；<br>・サブクラスＨ１０Ｆに包含される，赤外線，可視光，短波長電磁波または粒子線の輻射に感応する半導体装置；<br>・サブクラスＨ１０Ｈに包含される，電位障壁を有する，発光半導体装置；<br>・サブクラスＨ１０Ｎに包含される，熱電装置，熱磁気装置，圧電装置，電歪装置，磁歪装置，磁気効果装置，超電導装置またはその他の電気的固体装置；<br>・グループＨ１０Ｗに包含される，半導体本体または電極以外の構造上の細部<br>３．このサブクラスでは，セクションＣの注（３）の周期表中に示されたＩ〜ＶＩＩＩ族のシステムが用いられる。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>個々の装置<br>抵抗器；キャパシタ；インダクタ　１／００<br>ダイオード　８／００<br>バイポーラトランジスタ　１０／００<br>電界効果により制御されるバイポーラ装置　１２／００<br>サイリスタ　１８／００<br>電界効果トランジスタ［ＦＥＴ］　３０／００<br>電荷転送装置　４４／００<br>その他の個々の装置　４８／００<br>構造上の細部<br>本体　６２／００<br>電極　６４／００<br>集積装置；複数の装置の組立体<br>複数の装置の組立体　８０／００<br>半導体層のみを備える半導体基板内または上に形成される集積装置　８４／００<br>絶縁性または導電性基板内または上に形成される集積装置　８６／００<br>同一基板上のバルク構成部品とＳＯＩまたはＳＯＳ構成部品を備える集積装置　８７／００<br>３次元集積装置　８８／００<br>集積装置の他の観点　８９／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	INORGANIC ELECTRIC SEMICONDUCTOR DEVICES; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> electric semiconductor devices having inorganic semiconductor bodies. This includes the following kind of devices: <ul><li>inorganic semiconductor devices specially adapted for rectifying, amplifying, oscillating or switching, e.g. transistors or diodes;</li><li>individual inorganic resistors or capacitors having potential barriers;</li><li>individual resistors, capacitors or inductors having no potential barriers, and specially adapted for integration with other semiconductor components;</li><li>semiconductor bodies, or regions thereof, of devices covered by this subclass;</li><li>electrodes of devices covered by this subclass;</li><li>integrated devices, e.g. CMOS integrated devices;</li><li>processes or apparatus specially adapted for the manufacture or treatment of such devices.</li></ul></li><li>This subclass <u>does not cover</u>: <ul><li>electronic memory devices, which are covered by subclass <b>H10B</b>;</li><li>semiconductor devices sensitive to infrared radiation, light, electromagnetic radiation of shorter wavelength or corpuscular radiation, which are covered by subclass <b>H10F</b>;</li><li>light-emitting semiconductor devices having at least one potential barrier, which are covered by subclass <b>H10H</b>;</li><li>thermoelectric, thermomagnetic, piezoelectric, electrostrictive, magnetostrictive, magnetic-effect, superconducting or other electric solid-state devices, which are covered by subclass <b>H10N</b>;</li><li>constructional details other than semiconductor bodies or electrodes, which are covered by subclass <b>H10W</b>.</li></ul></li><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">INDIVIDUAL DEVICES<tr><td width="70%">Resistors; capacitors; inductors</td><td><b><b>1/00</b></b></td></tr></tr><tr><td width="70%">Diodes</td><td><b><b>8/00</b></b></td></tr></tr><tr><td width="70%">Bipolar junction transistors</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Bipolar devices controlled by the field-effect</td><td><b><b>12/00</b></b></td></tr></tr><tr><td width="70%">Thyristors</td><td><b><b>18/00</b></b></td></tr></tr><tr><td width="70%">FETs</td><td><b><b>30/00</b></b></td></tr></tr><tr><td width="70%">Charge transfer devices</td><td><b><b>44/00</b></b></td></tr></tr><tr><td width="70%">Other individual devices</td><td><b><b>48/00</b></b></td></tr></tr></tr><tr><td width="70%">CONSTRUCTIONAL DETAILS<tr><td width="70%">Bodies</td><td><b><b>62/00</b></b></td></tr></tr><tr><td width="70%">Electrodes</td><td><b><b>64/00</b></b></td></tr></tr></tr><tr><td width="70%">INTEGRATED DEVICES; ASSEMBLIES OF MULTIPLE DEVICES<tr><td width="70%">Assemblies of multiple devices</td><td><b><b>80/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices formed in or on semiconductor substrates that comprise only semiconducting layers</td><td><b><b>84/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices formed in or on insulating or conducting substrates</td><td><b><b>86/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices comprising both bulk devices and either SOI or SOS devices on the same substrate</td><td><b><b>87/00</b></b></td></tr></tr><tr><td width="70%">3D integrated devices</td><td><b><b>88/00</b></b></td></tr></tr><tr><td width="70%">Other aspects of integrated devices</td><td><b><b>89/00</b></b></td></tr></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	
H10F		赤外線，可視光，短波長電磁波または粒子線の輻射に感応する無機半導体装置［２０２５．０１］<br><br><b><ul>注</ul></b><br>１．　無機輻射線感応半導体装置が以下に特に適している場合に限り，このサブクラスは当該装置を包含する。：<br>・輻射線エネルギーの電気的エネルギーへの変換；　または<br>・輻射線による電気的エネルギーの制御<br>２．このサブクラスでは，「赤外線」は，約７００ｎｍから約１ｍｍの間の波長を含む。<br>３．このサブクラスでは，セクションＣの注（３）の周期表中で示されたＩ〜ＶＩＩＩ族の周期系が用いられる。［２０２５．０１］<br><br><b><ul>サブクラス内の索引</ul></b><br>光起電<br>個々の光起電セル　Ｈ１０Ｆ１０／００<br>光起電モジュールまたは集積装置　Ｈ１０Ｆ１９／００<br>輻射線によって制御される装置<br>個々のフォトレジスタ，フォトダイオード，フォトトランジスタまたは類似の装置　Ｈ１０Ｆ３０／００<br>集積装置または複数の装置の組立体　Ｈ１０Ｆ３９／００<br>他の装置<br>電気光源と結合された輻射線感応装置　Ｈ１０Ｆ５５／００<br>製造または処理；構造的細部<br>製造または処理　Ｈ１０Ｆ７１／００<br>構造的細部　Ｈ１０Ｆ７７／００<br>このサブクラスの他のグループに分類されない主題事項　Ｈ１０Ｆ９９／００［２０２５．０１］	INORGANIC SEMICONDUCTOR DEVICES SENSITIVE TO INFRARED RADIATION, LIGHT, ELECTROMAGNETIC RADIATION OF SHORTER WAVELENGTH OR CORPUSCULAR RADIATION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass covers inorganic radiation-sensitive semiconductor devices insofar as these devices are specially adapted for: <ul><li>the conversion of the radiation energy into electrical energy; or</li><li>the control of electrical energy by such radiation.</li></ul></li><li>In this subclass, &ldquo;infrared radiation&rdquo; includes wavelengths between about 700 nm and about 1 mm.</li><li>In this subclass, the periodic system used is the I to VIII Group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">PHOTOVOLTAICS<tr><td width="70%">Individual photovoltaic cells</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Photovoltaic modules or integrated devices</td><td><b><b>19/00</b></b></td></tr></tr></tr><tr><td width="70%">RADIATION-CONTROLLED DEVICES<tr><td width="70%">Individual photoresistors, photodiodes, phototransistors or like devices</td><td><b><b>30/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>39/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER DEVICES<tr><td width="70%">Radiation-sensitive devices coupled to electric light sources</td><td><b><b>55/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE OR TREATMENT; CONSTRUCTIONAL DETAILS<tr><td width="70%">Manufacture or treatment</td><td><b><b>71/00</b></b></td></tr></tr><tr><td width="70%">Constructional details</td><td><b><b>77/00</b></b></td></tr></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	
H10H		電位障壁を有する，無機発光半導体装置［２０２５．０１］<br><br><b><ul>注</ul></b><br>１．　このサブクラスは可視，赤外［ＩＲ］または紫外［ＵＶ］の光を発する，無機発光半導体装置を包含する。これは発光ダイオード［ＬＥＤ］およびスーパールミネッセントダイオード［ＳＬＤ］を含む。<br>２．　このサブクラスは半導体レーザーを包含しない，半導体レーザーはグループＨ０１Ｓ５／００に包含される。<br>３．　このサブクラスでは、セクションＣの注（３）の周期表中に示されたＩ〜ＶＩＩＩ族の周期系が用いられる。［２０２５．０１］	INORGANIC LIGHT-EMITTING SEMICONDUCTOR DEVICES HAVING POTENTIAL BARRIERS; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> inorganic light-emitting semiconductor devices that emit visible, infrared [IR] or ultraviolet [UV] light. This includes light-emitting diodes [LED] and superluminescent diodes [SLD].</li><li>This subclass <u>does not cover</u> semiconductor lasers, which are covered by group <b>H01S5/00</b>.</li><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul>	
H10K		有機電気的固体装置［２０２３．０１］<br><br><b><ul>注</ul></b><br>１．このサブクラスは以下を包含する。：<br>個々の有機電気的固体装置，すなわち電気的固体装置の能動部分が有機材料からなるもの；<br>有機電気的素子を備える，集積装置または複数の装置の組立体<br>２．このサブクラスは以下を包含しない。：<br>サブクラスＨ１０Ｂに包含される，有機電子記憶装置<br>サブクラスＨ１０Ｎに包含される，有機熱電装置，有機熱磁気装置，有機圧電装置，有機電歪装置，有機磁歪装置，有機電流磁気装置，有機ホール効果装置，有機超電導装置または電位障壁を有しない，整流，増幅，発振またはスイッチングに特に適した有機固体装置<br>電位障壁を有しない有機抵抗器で，集積装置に特に適合していないものはサブクラスＨ０１Ｃに包含される。<br>電位障壁を有しない有機コンデンサで，集積装置に特に適合していないものはサブクラスＨ０１Ｇに包含される。<br>３．このサブクラスでは、セクションＣの注（３）の周期表中に示されたＩ〜ＶＩＩＩ族のシステムが用いられる。<br>４．このサブクラスでは，グループＨ１０Ｋ１０１／００〜Ｈ０１Ｋ１０２／００のインデキシングコードを付するのが望ましい。<br><br><b><ul>サブクラス内の索引</ul></b><br>整流，増幅，発振またはスイッチングに特に適した有機装置<br>装置　１０／００<br>集積装置または複数の装置の組立体　１９／００<br>有機輻射線感応装置<br>装置　３０／００<br>集積装置または複数の装置の組立体　３９／００<br>有機発光装置<br>装置　５０／００<br>集積装置または複数の装置の組立体　５９／００<br>少なくとも１つの有機輻射線感応素子および少なくとも１つの有機発光素子を備える，集積装置または複数の装置の組立体　６５／００<br>製造または処理；構造的細部<br>製造または処理　７１／００<br>構造的細部　７７／００<br>有機活性材料　８５／００<br>このサブクラスの他のグループに包含されない主題事項　９９／００<br>インデキシング系列<br>インデキシング系列　１０１／００，１０２／００	ORGANIC ELECTRIC SOLID-STATE DEVICES; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>individual organic electric solid-state devices, i.e. electric solid-state devices comprising organic material in the active part;</li><li>integrated devices, or assemblies of multiple devices, comprising such elements.</li></ul></li><li>This subclass <u>does not cover</u>: <ul><li>organic electronic memory devices, which are covered by subclass <b>H10B</b>;</li><li>organic thermoelectric devices, organic thermomagnetic devices, organic piezoelectric devices, organic electrostrictive devices, organic magnetostrictive devices, organic galvanomagnetic devices, organic Hall-effect devices, organic superconducting devices or organic solid-state devices having no potential barriers, and specially adapted for rectifying, amplifying, oscillating or switching, which are covered by subclass <b>H10N</b>;</li><li>organic resistors having no potential barriers and not specially adapted for integrated devices, which are covered by subclass <b>H01C</b>;</li><li>organic capacitors having no potential barriers and not specially adapted for integrated devices, which are covered by subclass <b>H01G</b>.</li></ul></li><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li><li>In this subclass, it is desirable to add the indexing codes of groups <b>H10K101/00 to H10K102/00</b> .</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">ORGANIC DEVICES SPECIALLY ADAPTED FOR RECTIFYING, AMPLIFYING, OSCILLATING OR SWITCHING<tr><td width="70%">Devices</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>19/00</b></b></td></tr></tr></tr><tr><td width="70%">ORGANIC RADIATION-SENSITIVE DEVICES<tr><td width="70%">Devices</td><td><b><b>30/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>39/00</b></b></td></tr></tr></tr><tr><td width="70%">ORGANIC LIGHT-EMITTING DEVICES<tr><td width="70%">Devices</td><td><b><b>50/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>59/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices, or assemblies of multiple devices, comprising at least one organic radiation-sensitive element and at least one organic light-emitting element</td><td><b><b>65/00</b></b></td></tr></tr></tr><tr><td width="70%">MANUFACTURE OR TREATMENT; CONSTRUCTIONAL DETAILS<tr><td width="70%">Manufacture or treatment    </td><td><b><b>71/00</b></b></td></tr></tr><tr><td width="70%">Constructional details</td><td><b><b>77/00</b></b></td></tr></tr><tr><td width="70%">Organic active materials</td><td><b><b>85/00</b></b></td></tr></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr><tr><td width="70%">INDEXING SCHEMES<tr><td width="70%">Indexing schemes</td><td><b><b>101/00</b>, <b>102/00</b></b></td></tr></tr></tr></table>	
H10N		他に分類されない電気的固体装置［２０２３．０１］<br><br><b><ul>注</ul></b><br>このサブクラスでは、セクションＣの注（３）の周期表中に示されたＩ〜ＶＩＩＩ族のシステムが用いられる。<br><br><b><ul>サブクラス内の索引</ul></b><br>熱電装置または熱磁気装置<br>熱電装置　１０／００，１５／００<br>熱磁気装置　１５／００<br>集積装置または複数の装置の組立体　１９／００<br>圧電装置，電歪装置または磁歪装置<br>圧電装置または電歪装置　３０／００<br>磁歪装置　３５／００<br>集積装置または複数の装置の組立体　３９／００<br>電流磁気装置または類似の磁気効果装置電流<br>磁気装置　５０／００<br>ホール効果装置　５２／００<br>集積装置または複数の装置の組立体　５９／００<br>超電導装置<br>超電導装置　６０／００<br>集積装置または複数の装置の組立体　６９／００<br>他の電気的固体装置<br>電位障壁を有しない，整流，増幅，発振またはスイッチングに特に適した，電位障壁または表面障壁を有しない固体装置　７０／００<br>集積装置または複数の装置の組立体　７９／００<br>バルク負性抵抗効果装置　８０／００<br>集積装置または複数の装置の組立体　８９／００<br>他に分類されない電気的固体薄膜または厚膜装置　９７／００<br>このサブクラスの他のグループに分類されない主題事項　９９／００	ELECTRIC SOLID-STATE DEVICES NOT OTHERWISE PROVIDED FOR; <br><br><b><u>Note(s)</u></b><br><br><ul><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">THERMOELECTRIC OR THERMOMAGNETIC DEVICES<tr><td width="70%">Thermoelectric devices</td><td><b><b>10/00</b>, <b>15/00</b></b></td></tr></tr><tr><td width="70%">Thermomagnetic devices</td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>19/00</b></b></td></tr></tr></tr><tr><td width="70%">PIEZOELECTRIC, ELECTROSTRICTIVE OR MAGNETOSTRICTIVE DEVICES<tr><td width="70%">Piezoelectric or electrostrictive devices</td><td><b><b>30/00</b></b></td></tr></tr><tr><td width="70%">Magnetostrictive devices</td><td><b><b>35/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>39/00</b></b></td></tr></tr></tr><tr><td width="70%">GALVANOMAGNETIC OR SIMILAR MAGNETIC-EFFECT DEVICES<tr><td width="70%">Galvanomagnetic devices</td><td><b><b>50/00</b></b></td></tr></tr><tr><td width="70%">Hall-effect devices</td><td><b><b>52/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>59/00</b></b></td></tr></tr></tr><tr><td width="70%">SUPERCONDUCTING DEVICES<tr><td width="70%">Superconducting devices</td><td><b><b>60/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>69/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER ELECTRIC SOLID-STATE DEVICES<tr><td width="70%">Solid-state devices having no potential barriers and specially adapted for rectifying, amplifying, oscillating or switching</td><td><b><b>70/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>79/00</b></b></td></tr></tr><tr><td width="70%">Bulk negative-resistance effect devices</td><td><b><b>80/00</b></b></td></tr></tr><tr><td width="70%">Integrated devices or assemblies of multiple devices</td><td><b><b>89/00</b></b></td></tr></tr></tr><tr><td width="70%">ELECTRIC SOLID-STATE THIN-FILM OR THICK-FILM DEVICES, NOT OTHERWISE PROVIDED FOR</td><td><b><b>97/00</b></b></td></tr></tr><tr><td width="70%">SUBJECT MATTER NOT PROVIDED FOR IN OTHER GROUPS OF THIS SUBCLASS</td><td><b><b>99/00</b></b></td></tr></tr></table>	
H10P		クラスＨ１０に包含される装置を製造または処理するための一般的な方法または装置［２０２６．０１］<br><br><b><ul>注</ul></b><br>注［２０２６．０１］<br>１．このサブクラスはクラスＨ１０に包含される装置，またはその部品，に一般的に適用し得る製造または処理に特に適合する方法または装置を包含する。<br>２．以下の点に注意すること：<br>ａ．Ｈ１０Ｂ−Ｈ１０Ｎの単一のサブクラスに包含される，装置，またはその部品，の製造または処理に特に適合する方法または装置は当該サブクラスに分類される。例えば，トランジスタの製造はサブクラスＨ１０Ｄに分類される；<br>ｂ．サブクラスＨ１０Ｗに包含される，装置の一般的なパッケージ，相互接続，コネクタまたは他の構造上の細部の製造または処理に特に適合する方法または装置は，当該サブクラスに分類される。例えば，銅ピラーバンプコネクタの形成はサブクラスＨ１０Ｗに分類される。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>層，構造または材料の構築<br>ボンディング　１０／００<br>材料の形成　１４／００<br>層，構造または材料の加工<br>イオン注入　３０／００<br>ドーパントの拡散　３２／００<br>電磁輻射線または粒子輻射線の照射　３４／００<br>ゲッタリング　３６／００<br>層，構造または材料の除去<br>エッチング　５０／００<br>研削，ラッピングまたは研磨　５２／００<br>切断または分離　５４／００<br>ディボンディング　５６／００<br>ウェハまたは基板を複数のチップに個片化するもの，すなわちダイシング　５８／００<br>その他の製造または処理<br>洗浄　７０／００<br>ウェハ，基板または装置の製造または処理中にこれらを取り扱うまたは保持するもの　７２／００<br>ウェハ，基板または装置の製造または処理中の試験または測定　７４／００<br>半導体本体上のマスクの製造または処理　７６／００<br>ウェハの製造　９０／００<br>製造または処理のための他の一般的な方法または装置　９５／００	GENERIC PROCESSES OR APPARATUS FOR THE MANUFACTURE OR TREATMENT OF DEVICES COVERED BY CLASS <b>H10</b>; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>co</u><u>vers</u> processes or apparatus specially adapted for the manufacture or treatment of devices, or parts thereof, covered by class <b>H10</b>, which are generically applicable to these devices.</li><li>Attention is drawn to the following: <ul><li>processes or apparatus specially adapted for the manufacture or treatment of devices, or parts thereof, which are covered by a single subclass of <b>H10B to H10N</b> , are classified in the subclass in question. For example, the manufacture of a transistor is classified in subclass <b>H10D</b>;</li><li>processes or apparatus specially adapted for the manufacture or treatment of generic packages, interconnections, connectors or other constructional details of devices, which are covered by subclass <b>H10W</b>, are classified in the subclass in question. For example, the formation of a copper pillar bump connector is classified in subclass <b>H10W</b>.</li></ul></li><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">BUILDING UP OF LAYERS, STRUCTURES OR MATERIALS<tr><td width="70%">Bonding</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Formation of materials</td><td><b><b>14/00</b></b></td></tr></tr></tr><tr><td width="70%">MODIFICATION OF LAYERS, STRUCTURES OR MATERIALS<tr><td width="70%">Ion implantation</td><td><b><b>30/00</b></b></td></tr></tr><tr><td width="70%">Diffusion of dopants</td><td><b><b>32/00</b></b></td></tr></tr><tr><td width="70%">Irradiation with electromagnetic or particle radiation</td><td><b><b>34/00</b></b></td></tr></tr><tr><td width="70%">Gettering</td><td><b><b>36/00</b></b></td></tr></tr></tr><tr><td width="70%">REMOVAL OF LAYERS, STRUCTURES OR MATERIALS<tr><td width="70%">Etching</td><td><b><b>50/00</b></b></td></tr></tr><tr><td width="70%">Grinding, lapping or polishing</td><td><b><b>52/00</b></b></td></tr></tr><tr><td width="70%">Cutting or separating</td><td><b><b>54/00</b></b></td></tr></tr><tr><td width="70%">Debonding</td><td><b><b>56/00</b></b></td></tr></tr><tr><td width="70%">Singulating wafers or substrates into multiple chips, i.e. dicing</td><td><b><b>58/00</b></b></td></tr></tr></tr><tr><td width="70%">OTHER MANUFACTURE OR TREATMENT<tr><td width="70%">Cleaning</td><td><b><b>70/00</b></b></td></tr></tr><tr><td width="70%">Handling or holding of wafers, substrates or devices during manufacture or treatment thereof</td><td><b><b>72/00</b></b></td></tr></tr><tr><td width="70%">Testing or measuring during manufacture or treatment of wafers, substrates or devices </td><td><b><b>74/00</b></b></td></tr></tr><tr><td width="70%">Manufacture or treatment of masks on semiconductor bodies</td><td><b><b>76/00</b></b></td></tr></tr><tr><td width="70%">Preparation of wafers</td><td><b><b>90/00</b></b></td></tr></tr><tr><td width="70%">Other generic processes or apparatus for manufacture or treatments</td><td><b><b>95/00</b></b></td></tr></tr></tr></table>	
H10W		クラスＨ１０に包含される装置の一般的なパッケージ，相互接続，コネクタまたは他の構造上の細部［２０２６．０１］<br><br><b><ul>注</ul></b><br>注［２０２６．０１］<br>１．このサブクラスは以下のものを包含する：<br>ａ．装置のパッケージおよびそのパッケージの部品；<br>ｂ．チップ，ウェハ，基板またはパッケージ内の装置の相互接続；<br>ｃ．パッケージ内の装置のコネクタ；<br>ｄ．チップ，ウェハ，基板またはパッケージ内の装置のその他の構造上の細部，例．集積装置の構成部品間における分離領域；<br>ｅ．動作中のパッケージを支持するための分離可能な保持具；<br>ｆ．以下の（ａ）−（ｅ）の観点の製造または処理；<br>（１）サブクラスＨ１０Ｂに包含される装置に適用可能な場合；<br>（２）サブクラスＨ１０Ｄに包含される装置に適用可能な場合，ただしサブグループＨ１０Ｄ６２／００またはＨ１０Ｄ６４／００に包含される半導体本体またはその電極を除く；<br>（３）サブクラスＨ１０Ｂ，Ｈ１０Ｄ，Ｈ１０Ｆ，Ｈ１０Ｈ，Ｈ１０ＫまたはＨ１０Ｎに包含される装置に一般的に適用可能な場合。<br><br><b><ul>サブクラス内の索引</ul></b><br>サブクラス内の索引<br>スチップ，ウェハまたは基板内の集積装置の構造上の細部<br>集積装置の構成部品間における半導体本体内の分離領域　１０／００<br>集積装置の高濃度にドープされた埋め込み領域　１５／００<br>チップ，ウェハまたは基板内の相互接続　２０／００<br>他に分類されない，集積装置の一般的な部品　２９／００<br>チップ，ウェハ，基板またはパッケージに関する構造上の細部<br>熱保護または熱制御のための構成　４０／００<br>装置の保護のための構成　４２／００<br>インピーダンスを制御または整合させるための電気的構成　４４／００<br>装置に適用されるマーク　４６／００<br>パッケージに関する観点<br>パッケージ基板；インターポーザ；再配線層　７０／００<br>パッケージ内の相互接続またはコネクタ　７２／００<br>封緘　７４／００<br>容器；充填物；シール　７６／００<br>動作中のパッケージ化されたチップを支持するための，分離可能な保持具　７８／００<br>チップ，ウェハまたは基板のダイレクトボンディング　８０／００<br>パッケージの配置　９０／００<br>このサブクラスの他のグループに包含されないパッケージング方法　９５／００<br>このサブクラスの他のグループに包含されない主題事項　９９／００	GENERIC PACKAGES, INTERCONNECTIONS, CONNECTORS OR OTHER CONSTRUCTIONAL DETAILS OF DEVICES COVERED BY CLASS <b>H10</b>; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u>: <ul><li>packages of devices and parts of such packages;</li><li>interconnections of devices in chips, wafers, substrates or packages;</li><li>connectors of devices in packages;</li><li>other constructional details of devices in chips, wafers, substrates or packages, e.g. isolation regions between components of integrated devices;</li><li>detachable holders for supporting packaged chips in operation;</li><li>the manufacture or treatment of aspects (a)-(e); <ul><li>when aspects (a)-(e) are</li><li>(1) applicable to devices covered by subclass <b>H10B</b>;</li><li>(2) applicable to devices covered by subclass <b>H10D</b>, except for semiconductor bodies or electrodes thereof, which are covered by subgroups <b>H10D62/00</b> or <b>H10D64/00</b>; or</li><li>(3) generically applicable to devices covered by subclasses <b>H10B</b>, <b>H10D</b>, <b>H10F</b>, <b>H10H</b>, <b>H10K</b> or <b>H10N</b>.</li></ul></li></ul></li><li>In this subclass, the periodic system used is the I to VIII group system indicated in the Periodic Table under Note (3) of section <b>C</b>.</li></ul><br><br><b><u>Subclass indexes</u></b><br><br><table><tr><td width="70%">CONSTRUCTIONAL DETAILS OF INTEGRATED DEVICES IN CHIPS, WAFERS OR SUBSTRATES<tr><td width="70%">Isolation regions in semiconductor bodies between components of integrated devices</td><td><b><b>10/00</b></b></td></tr></tr><tr><td width="70%">Highly-doped buried regions of integrated devices</td><td><b><b>15/00</b></b></td></tr></tr><tr><td width="70%">Interconnections in chips, wafers or substrates</td><td><b><b>20/00</b></b></td></tr></tr><tr><td width="70%">Generic parts of integrated devices, not otherwise provided for</td><td><b><b>29/00</b></b></td></tr></tr></tr><tr><td width="70%">CONSTRUCTIONAL DETAILS RELATED TO CHIPS, WAFERS, SUBSTRATES OR PACKAGES<tr><td width="70%">Arrangements for thermal protection or control</td><td><b><b>40/00</b></b></td></tr></tr><tr><td width="70%">Arrangements for protection of devices</td><td><b><b>42/00</b></b></td></tr></tr><tr><td width="70%">Electrical arrangements for controlling or matching impedance</td><td><b><b>44/00</b></b></td></tr></tr><tr><td width="70%">Marks applied to devices</td><td><b><b>46/00</b></b></td></tr></tr></tr><tr><td width="70%">ASPECTS OF PACKAGES<tr><td width="70%">Package substrates; Interposers; Redistribution layers</td><td><b><b>70/00</b></b></td></tr></tr><tr><td width="70%">Interconnections or connectors in packages</td><td><b><b>72/00</b></b></td></tr></tr><tr><td width="70%">Encapsulations</td><td><b><b>74/00</b></b></td></tr></tr><tr><td width="70%">Containers; Fillings; Seals</td><td><b><b>76/00</b></b></td></tr></tr><tr><td width="70%">Detachable holders for supporting packaged chips in operation</td><td><b><b>78/00</b></b></td></tr></tr><tr><td width="70%">Direct bonding of chips, wafers or substrates</td><td><b><b>80/00</b></b></td></tr></tr><tr><td width="70%">Package configurations</td><td><b><b>90/00</b></b></td></tr></tr><tr><td width="70%">Packaging processes not covered by the other groups of this subclass</td><td><b><b>95/00</b></b></td></tr></tr><tr><td width="70%">Subject matter not provided for in other groups of this subclass</td><td><b><b>99/00</b></b></td></tr></tr></tr></table>	
H99		このセクションの中で他に分類されない主題事項［８］	SUBJECT MATTER NOT OTHERWISE PROVIDED FOR IN THIS SECTION	
H99Z		このセクションの中で他に分類されない主題事項［８］<br><br><b><ul>注</ul></b><br>このサブクラスは，以下の主題事項を包含する：［８］<br>（ａ）このセクションのサブクラスに包含される主題事項に分類されないが，これに最も関連しているもの，［８］<br>（ｂ）別のセクションの何れのサブクラスにも明示的に包含されないもの［８］	SUBJECT MATTER NOT OTHERWISE PROVIDED FOR IN THIS SECTION; <br><br><b><u>Note(s)</u></b><br><br><ul><li>This subclass <u>covers</u> subject matter that:<ul><li>is not provided for, but is most closely related to, the subject matter covered by the subclasses of this section, and</li><li>is not explicitly covered by any subclass of another section.</li></ul></li></ul>	3
