F16M1/00	7	Frames or casings of engines, machines or apparatus; Frames serving as machinery beds	F16M1/00	F16M1/00		1109
F16M1/02	8	for reciprocating engines or similar machines	F16M1/02	F16M1/02		139
F16M1/021	9	for housing crankshafts	F16M1/021	F16M1/021		75
F16M1/022	10	of tunnel type, i.e. wherein the crankshaft can only be introduced axially (for engines or machines with star-shaped cylinder arrangement F16M1/023)	F16M1/022	F16M1/022		3
F16M1/023	10	specially adapted for engines or machines with star-shaped cylinder arrangement	F16M1/023	F16M1/023		2
F16M1/024	10	facilitating assembly of power-transmitting parts of engines or machines, e.g. of connecting-rods	F16M1/024	F16M1/024		10
F16M1/025	10	Assembling bearings in casings, e.g. having anchor bolts	F16M1/025	F16M1/025		54
F16M1/026	9	for housing movable engine or machine parts other than crankshafts, e.g. valve-gear housings	F16M1/026	F16M1/026		117
F16M1/04	8	for rotary engines or similar machines	F16M1/04	F16M1/04		179
F16M1/08	8	characterised by being built-up of sheet material or welded parts	F16M1/08	F16M1/08		179
F16M3/00	7	Portable or wheeled frames or beds, e.g. for emergency power-supply aggregates, compressor sets (construction of vehicles in general B60&#160;-&#160;B62)	F16M3/00	F16M3/00		1950
F16M5/00	7	Engine beds, i.e. means for supporting engines or machines on foundations	F16M5/00	F16M5/00		2157
F16M7/00	7	Details of attaching or adjusting engine beds, frames, or supporting-legs on foundation or base; Attaching non-moving engine parts, e.g. cylinder blocks (elastic or equivalent mounting for absorbing vibrations F16F, especially F16F15/04)	F16M7/00	F16M7/00		4962
F16M9/00	7	Special layout of foundations with respect to machinery to be supported (foundations for machinery E02D27/44)	F16M9/00	F16M9/00		276
F16M11/00	7	Stands or trestles as supports for apparatus or articles placed thereon {; Stands for scientific apparatus such as gravitational force meters}(without heads F16M13/00; easels or stands for blackboards or the like A47B97/04; show-stands A47F7/00; for workmen E04G1/32; {sockets or holders for poles or posts E04H12/22;} supporting or suspending for lighting devices F21V21/00)	F16M11/00	F16M11/00		1208
F16M11/02	8	Heads	F16M11/02	F16M11/02		400
F16M11/04	9	Means for attachment of apparatus; Means allowing adjustment of the apparatus relatively to the stand	F16M11/04	F16M11/04		17529
F16M11/041	10	{Allowing quick release of the apparatus}	F16M11/04	F16M11/04		6917
F16M11/043	10	{Allowing translations}	F16M11/04	F16M11/04		4451
F16M11/045	11	{adapted to left-right translation movement}	F16M11/04	F16M11/04		2426
F16M11/046	11	{adapted to upward-downward translation movement}	F16M11/04	F16M11/04		9953
F16M11/048	11	{adapted to forward-backward translation movement}	F16M11/04	F16M11/04		1753
F16M11/06	10	allowing pivoting	F16M11/06	F16M11/06		4082
F16M11/08	11	around a vertical axis {, e.g. panoramic heads (F16M11/12 takes precedence)}	F16M11/08	F16M11/08		8793
F16M11/10	11	around a horizontal axis {(F16M11/12 takes precedence)}	F16M11/10	F16M11/10		15144
F16M11/105	12	{the horizontal axis being the roll axis, e.g. for creating a landscape-portrait rotation}	F16M11/10	F16M11/10		1443
F16M11/12	11	in more than one direction	F16M11/12	F16M11/12		3786
F16M11/121	12	{constituted of several dependent joints}	F16M11/12	F16M11/12		1453
F16M11/123	13	{the axis of rotation intersecting in a single point, e.g. by using gimbals}	F16M11/12	F16M11/12		670
F16M11/125	12	{for tilting and rolling (F16M11/14 takes precedence)}	F16M11/12	F16M11/12		462
F16M11/126	12	{for tilting and panning (F16M11/14 takes precedence)}	F16M11/12	F16M11/12		524
F16M11/128	12	{for panning and rolling (F16M11/14 takes precedence)}	F16M11/12	F16M11/12		45
F16M11/14	12	with ball-joint (ball-jointed hinges F16C11/06{; adjustable mountings employing universal joints for lighting devices F21V21/26&#160;-&#160;F21V21/30})	F16M11/14	F16M11/14		4191
F16M11/16	9	Details concerning attachment of head-supporting legs, with or without actuation of locking members thereof	F16M11/16	F16M11/16		5727
F16M11/18	9	with mechanism for moving the apparatus relatively to the stand	F16M11/18	F16M11/18		23215
F16M11/20	8	Undercarriages with or without wheels	F16M11/20	F16M11/20		1373
F16M11/2007	9	{comprising means allowing pivoting adjustment}	F16M11/20	F16M11/20		360
F16M11/2014	10	{around a vertical axis (F16M11/2035 takes precedence)}	F16M11/20	F16M11/20		3786
F16M11/2021	10	{around a horizontal axis (F16M11/2035 takes precedence)}	F16M11/20	F16M11/20		2387
F16M11/2028	11	{for rolling, i.e. for creating a landscape-portrait rotation}	F16M11/20	F16M11/20		222
F16M11/2035	10	{in more than one direction}	F16M11/20	F16M11/20		360
F16M11/2042	11	{constituted of several dependent joints}	F16M11/20	F16M11/20		133
F16M11/205	12	{the axis of rotation intersecting in a single point, e.g. gimbals}	F16M11/20	F16M11/20		123
F16M11/2057	11	{for tilting and rolling (F16M11/2078 takes precedence)}	F16M11/20	F16M11/20		270
F16M11/2064	11	{for tilting and panning (F16M11/2078 takes precedence)}	F16M11/20	F16M11/20		915
F16M11/2071	11	{for panning and rolling (F16M11/2078 takes precedence)}	F16M11/20	F16M11/20		249
F16M11/2078	11	{with ball-joint (ball-jointed hinges F16C11/06)}	F16M11/20	F16M11/20		870
F16M11/2085	9	{comprising means allowing sideward adjustment, i.e. left-right translation of the head relatively to the undercarriage}	F16M11/20	F16M11/20		813
F16M11/2092	9	{comprising means allowing depth adjustment, i.e. forward-backward translation of the head relatively to the undercarriage}	F16M11/20	F16M11/20		1878
F16M11/22	9	with approximately constant height, e.g. with constant length of column or of legs (F16M11/42 takes precedence)	F16M11/22	F16M11/22		5611
F16M11/24	9	changeable in height or length of legs, also for transport only, {e.g. by means of tubes screwed into each other}(F16M11/42 takes precedence)	F16M11/24	F16M11/24		5899
F16M11/242	10	{by spreading of the legs (F16M11/32 takes precedence)}	F16M11/24	F16M11/24		1546
F16M11/245	11	{Members limiting spreading of legs, e.g. "umbrella legs" (for supports with three or more telescoping legs F16M11/34)}	F16M11/24	F16M11/24		808
F16M11/247	11	{Members preventing slipping of the feet (for supports with three or more telescoping legs F16M11/36)}	F16M11/24	F16M11/24		336
F16M11/26	10	by telescoping, with or without folding (details concerning the constructional features of telescoping parts only F16B7/10)	F16M11/26	F16M11/26		2381
F16M11/28	11	Undercarriages for supports with one single telescoping pillar	F16M11/28	F16M11/28		6175
F16M11/30	12	with co-moving side-struts	F16M11/30	F16M11/30		220
F16M11/32	11	Undercarriages for supports with three or more telescoping legs	F16M11/32	F16M11/32		3088
F16M11/34	12	Members limiting spreading of legs {, e.g. "umbrella legs"}	F16M11/34	F16M11/34		741
F16M11/36	12	Members preventing slipping of the feet	F16M11/36	F16M11/36		838
F16M11/38	10	by folding {, e.g. pivoting or scissors tong mechanisms}	F16M11/38	F16M11/38		3498
F16M11/40	10	by means of coilable or bendable legs {or spiral shaped legs}	F16M11/40	F16M11/40		846
F16M11/42	8	with arrangement for propelling the support {stands on wheels}	F16M11/42	F16M11/42		8314
F16M11/425	9	{along guiding means}	F16M11/42	F16M11/42		1778
F16M13/00	7	Other supports for positioning apparatus or articles (heads thereof F16M11/02{; undercarriages thereof F16M11/20} ; adapted to be stuck in the ground A45F3/44{; sockets or holders for poles or posts E04H12/22}); Means for steadying hand-held apparatus or articles {(supports for measuring instruments G01D11/30; supports for casings of remote control switching devices H01H9/025)}	F16M13/00	F16M13/00		5150
F16M13/005	8	{integral with the apparatus or articles to be supported}	F16M13/00	F16M13/00		781
F16M13/02	8	for supporting on, or attaching to, an object, e.g. tree, gate, window-frame, cycle	F16M13/02	F16M13/02		17203
F16M13/022	9	{repositionable}	F16M13/02	F16M13/02		6240
F16M13/025	9	{Corner supports}	F16M13/02	F16M13/02		190
F16M13/027	9	{Ceiling supports}	F16M13/02	F16M13/02		1977
F16M13/04	8	for supporting on, or holding steady relative to, a person, e.g. by chains {, e.g. rifle butt or pistol grip supports, supports attached to the chest or head (apparatus or arrangements for taking photographs or for projecting or viewing them G03B)}	F16M13/04	F16M13/04		3719
F16M13/06	8	also serviceable for other purposes, e.g. to be used as spade, chair, ski-stick	F16M13/06	F16M13/06		160
F16M13/08	9	for use as a walking-cane	F16M13/08	F16M13/08		115
F16M2200/00	7	Details of stands or supports	CPCONLY	F16M2200/00		151
F16M2200/02	8	Locking means	CPCONLY	F16M2200/02		806
F16M2200/021	9	for rotational movement	CPCONLY	F16M2200/021		463
F16M2200/022	10	by friction	CPCONLY	F16M2200/022		2595
F16M2200/024	10	by positive interaction, e.g. male-female connections	CPCONLY	F16M2200/024		1905
F16M2200/025	9	for translational movement	CPCONLY	F16M2200/025		247
F16M2200/027	10	by friction	CPCONLY	F16M2200/027		1408
F16M2200/028	10	by positive interaction, e.g. male-female connections	CPCONLY	F16M2200/028		1225
F16M2200/04	8	Balancing means	CPCONLY	F16M2200/04		566
F16M2200/041	9	for balancing rotational movement of the head	CPCONLY	F16M2200/041		1611
F16M2200/042	10	for panning movement	CPCONLY	F16M2200/042		69
F16M2200/044	9	for balancing rotational movement of the undercarriage	CPCONLY	F16M2200/044		1359
F16M2200/045	10	for panning movement	CPCONLY	F16M2200/045		30
F16M2200/047	9	for balancing translational movement of the head	CPCONLY	F16M2200/047		402
F16M2200/048	9	for balancing translational movement of the undercarriage	CPCONLY	F16M2200/048		425
F16M2200/06	8	Arms	CPCONLY	F16M2200/06		327
F16M2200/061	9	Scissors arms	CPCONLY	F16M2200/061		384
F16M2200/063	9	Parallelogram arms	CPCONLY	F16M2200/063		852
F16M2200/065	9	with a special structure, e.g. reinforced or adapted for space reduction	CPCONLY	F16M2200/065		795
F16M2200/066	9	being part of the head	CPCONLY	F16M2200/066		323
F16M2200/068	9	being part of the undercarriage	CPCONLY	F16M2200/068		551
F16M2200/08	8	Foot or support base	CPCONLY	F16M2200/08		4767
