H01H1/00	7	Contacts (liquid contacts H01H29/04)	H01H1/00	H01H1/00		711
H01H2001/0005	8	{Redundant contact pairs in one switch for safety reasons}	H01H1/00	H01H1/00		128
H01H2001/001	8	{providing easy replacement of contacts}	H01H1/00	H01H1/00		48
H01H1/0015	8	{Means for testing or for inspecting contacts, e.g. wear indicator (measuring circuits G01R31/3274)}	H01H1/00	H01H1/00		627
H01H2001/0021	9	{Camera or endoscope for monitoring contacts, their position or mechanism}	H01H1/00	H01H1/00		51
H01H2001/0026	9	{wherein one or both contacts contain embedded contact wear signal material, e.g. radioactive material being released as soon as the contact wear reaches the embedded layer}	H01H1/00	H01H1/00		17
H01H2001/0031	9	{by analysing radiation emitted by arc or trace material}	H01H1/00	H01H1/00		33
H01H1/0036	8	{Switches making use of microelectromechanical systems [MEMS] (for electromagnetic relays H01H50/005; for electrostatic relays H01H59/0009)}	H01H1/00	H01H1/00		897
H01H2001/0042	9	{Bistable switches, i.e. having two stable positions requiring only actuating energy for switching between them, e.g. with snap membrane or by permanent magnet}	H01H1/00	H01H1/00		172
H01H2001/0047	10	{operable only by mechanical latching}	H01H1/00	H01H1/00		58
H01H2001/0052	9	{Special contact materials used for MEMS}	H01H1/00	H01H1/00		66
H01H2001/0057	10	{the contact materials containing refractory materials, e.g. tungsten}	H01H1/00	H01H1/00		30
H01H2001/0063	9	{having electrostatic latches, i.e. the activated position is kept by electrostatic forces other than the activation force}	H01H1/00	H01H1/00		59
H01H2001/0068	9	{with multi dimensional movement, i.e. the movable actuator performing movements in at least two different directions}	H01H1/00	H01H1/00		40
H01H2001/0073	9	{Solutions for avoiding the use of expensive silicon technologies in micromechanical switches}	H01H1/00	H01H1/00		27
H01H2001/0078	9	{with parallel movement of the movable contact relative to the substrate}	H01H1/00	H01H1/00		138
H01H2001/0084	9	{with perpendicular movement of the movable contact relative to the substrate}	H01H1/00	H01H1/00		174
H01H2001/0089	9	{Providing protection of elements to be released by etching of sacrificial element;  Avoiding stiction problems, e.g. of movable element to substrate}	H01H1/00	H01H1/00		24
H01H1/0094	8	{Switches making use of nanoelectromechanical systems [NEMS]}	H01H1/00	H01H1/00		150
H01H1/02	8	characterised by the material thereof {(containing gas-evolving material H01H33/765)}	H01H1/02	H01H1/02		460
H01H1/0201	9	{Materials for reed contacts}	H01H1/02	H01H1/02		174
H01H1/0203	9	{specially adapted for vacuum switches}	H01H1/02	H01H1/02		431
H01H2001/0205	10	{Conditioning of the contact material through arcing during manufacturing, e.g. vacuum-depositing of layer on contact surface}	H01H1/02	H01H1/02		32
H01H1/0206	10	{containing as major components Cu and Cr}	H01H1/02	H01H1/02		196
H01H2001/0208	9	{containing rhenium}	H01H1/02	H01H1/02		27
H01H1/021	9	Composite material<br><br><u>NOTE</u><br><br>In this group, the following expression is used with the meaning indicated :<br>"composite material" is a material made of two or more different materials, e.g. coated material, layered materials or carbon fibres in a copper base or matrix<br>Subject matter classifiable in more than one of groups H01H1/023 - H01H1/029 should be classified in all relevant groups.	H01H1/021	H01H1/021		451
H01H1/023	10	having a noble metal as the basic material	H01H1/023	H01H1/023		809
H01H1/0231	11	{provided with a solder layer}	H01H1/023	H01H1/023		167
H01H1/0233	11	and containing carbides	H01H1/0233	H01H1/0233		170
H01H1/0237	11	and containing oxides	H01H1/0237	H01H1/0237		260
H01H1/02372	12	{containing as major components one or more oxides of the following elements only: Cd, Sn, Zn, In, Bi, Sb or Te}	H01H1/0237	H01H1/0237		151
H01H1/02374	13	{containing as major component CdO}	H01H1/0237	H01H1/0237		111
H01H1/02376	13	{containing as major component SnO2}	H01H1/0237	H01H1/0237		166
H01H2001/02378	12	{containing iron-oxide as major component}	H01H1/0237	H01H1/0237		18
H01H1/025	10	having copper as the basic material	H01H1/025	H01H1/025		454
H01H1/027	10	containing carbon particles or fibres	H01H1/027	H01H1/027		342
H01H1/029	10	comprising conducting material dispersed in an elastic support or binding material	H01H1/029	H01H1/029		295
H01H1/04	9	Co-operating contacts of different material	H01H1/04	H01H1/04		270
H01H1/06	8	characterised by the shape or structure of the contact-making surface, e.g. grooved	H01H1/06	H01H1/06		833
H01H1/065	9	{formed by freely suspended particles, e.g. magnetic dust or balls}	H01H1/06	H01H1/06		37
H01H1/08	9	wetted with mercury	H01H1/08	H01H1/08		201
H01H1/10	9	Laminated contacts with divided contact surface	H01H1/10	H01H1/10		122
H01H1/12	8	characterised by the manner in which co-operating contacts engage	H01H1/12	H01H1/12		129
H01H2001/125	9	{whereby the contacts of the switch are formed by teeth of a zipper}	H01H1/12	H01H1/12		31
H01H1/14	9	by abutting	H01H1/14	H01H1/14		363
H01H2001/145	10	{by crossing each other, the cooperating contacts each having a contact making ridge perpendicular to each other}	H01H1/14	H01H1/14		82
H01H1/16	10	by rolling; by wrapping; Roller or ball contacts	H01H1/16	H01H1/16		685
H01H1/18	10	with subsequent sliding	H01H1/18	H01H1/18		489
H01H1/20	10	Bridging contacts {(for circuit breakers H01H73/045)}	H01H1/20	H01H1/20		1253
H01H1/2008	11	{Facilitate mounting or replacing contact bridge and pressure spring on carrier (H01H11/0012 takes precedence)}	H01H1/20	H01H1/20		161
H01H1/2016	11	{in which the two contact pairs commutate at substantially different moments}	H01H1/20	H01H1/20		97
H01H1/2025	11	{comprising two-parallel bridges}	H01H1/20	H01H1/20		167
H01H2001/2033	12	{with a contact bridge on both opposite sides of a fixed contact pair, each contact bridge being moved to close or open the circuit}	H01H1/20	H01H1/20		37
H01H1/2041	11	{Rotating bridge}	H01H1/20	H01H1/20		298
H01H1/205	12	{Details concerning the elastic mounting of the rotating bridge in the rotor}	H01H1/20	H01H1/20		126
H01H1/2058	12	{Rotating bridge being assembled in a cassette, which can be placed as a complete unit into a circuit breaker}	H01H1/20	H01H1/20		203
H01H1/2066	11	{Fork-shaped bridge; Two transversally connected contact arms bridging two fixed contacts}	H01H1/20	H01H1/20		98
H01H1/2075	11	{T-shaped bridge; bridging contact has lateral arm for mounting resiliently or on a pivot}	H01H1/20	H01H1/20		53
H01H1/2083	11	{Bridging contact surfaces directed at an oblique angle with respect to the movement of the bridge}	H01H1/20	H01H1/20		151
H01H2001/2091	11	{having two pivotally and electrically connected halve bridges}	H01H1/20	H01H1/20		51
H01H1/22	10	with rigid pivoted member carrying the moving contact	H01H1/22	H01H1/22		234
H01H1/221	11	{and a contact pressure spring acting between the pivoted member and a supporting member}	H01H1/22	H01H1/22		87
H01H2001/223	12	{using a torsion spring}	H01H1/22	H01H1/22		155
H01H1/225	12	{the supporting member being pivotable}	H01H1/22	H01H1/22		178
H01H1/226	12	{having a plurality of parallel contact bars}	H01H1/22	H01H1/22		316
H01H2001/228	13	{with insulating spacers between the contact bars}	H01H1/22	H01H1/22		35
H01H1/24	10	with resilient mounting	H01H1/24	H01H1/24		329
H01H1/242	11	{the contact forming a part of a coil spring}	H01H1/24	H01H1/24		290
H01H1/245	11	{Spring wire contacts}	H01H1/24	H01H1/24		185
H01H2001/247	11	{using an elastic hinge, the contact being composed of rigid parts connected by thinned flexible hinge parts}	H01H1/24	H01H1/24		29
H01H1/26	11	with spring blade support	H01H1/26	H01H1/26		672
H01H2001/265	12	{having special features for supporting, locating or pre-stressing the contact blade springs}	H01H1/26	H01H1/26		121
H01H1/28	12	Assembly of three or more contact-supporting spring blades	H01H1/28	H01H1/28		180
H01H1/30	11	within supporting guides	H01H1/30	H01H1/30		38
H01H1/32	10	Self-aligning contacts	H01H1/32	H01H1/32		111
H01H1/34	10	with provision for adjusting position of contact relative to its co-operating contact	H01H1/34	H01H1/34		190
H01H1/36	9	by sliding	H01H1/36	H01H1/36		397
H01H1/365	10	{Bridging contacts}	H01H1/36	H01H1/36		399
H01H1/38	10	Plug-and-socket contacts	H01H1/38	H01H1/38		411
H01H1/385	11	{Contact arrangements for high voltage gas blast circuit breakers}	H01H1/38	H01H1/38		437
H01H1/40	10	Contact mounted so that its contact-making surface is flush with adjoining insulation	H01H1/40	H01H1/40		116
H01H1/403	11	{Contacts forming part of a printed circuit (multilayer keyboard switches H01H13/702; thumbwheel switches H01H19/001; for rotary switches with axial contact pressure H01H19/585)}	H01H1/40	H01H1/40		498
H01H2001/406	11	{with holes or recesses between adjacent contacts, e.g. to collect abrasion powder}	H01H1/40	H01H1/40		34
H01H1/42	10	Knife-and-clip contacts	H01H1/42	H01H1/42		1046
H01H2001/425	11	{with separate contact pressure spring confined between two contact knifes and urging the knifes onto a mating contact}	H01H1/42	H01H1/42		48
H01H1/44	10	with resilient mounting	H01H1/44	H01H1/44		295
H01H1/46	10	self-aligning contacts	H01H1/46	H01H1/46		106
H01H1/48	10	with provision for adjusting position of contact relative to its co-operating contact	H01H1/48	H01H1/48		53
H01H1/50	8	Means for increasing contact pressure, preventing vibration of contacts, holding contacts together after engagement, or biasing contacts to the open position	H01H1/50	H01H1/50		1517
H01H1/502	9	{the action of the contact pressure spring becoming active only after engagement of the contacts}	H01H1/50	H01H1/50		147
H01H1/504	9	{by thermal means}	H01H1/50	H01H1/50		195
H01H2001/506	9	{Fail safe contacts, i.e. the contacts being kept in a safe position, usually in an open circuit position, at end of life time of switch}	H01H1/50	H01H1/50		23
H01H2001/508	9	{with mechanical means to prevent return/reverse movement of movable contact once opening or closing cycle has started}	H01H1/50	H01H1/50		60
H01H1/52	9	Contacts adapted to act as latches	H01H1/52	H01H1/52		190
H01H1/54	9	by magnetic force {(combined with electrodynamic opening H01H77/101)}	H01H1/54	H01H1/54		823
H01H2001/545	10	{having permanent magnets directly associated with the contacts}	H01H1/54	H01H1/54		150
H01H1/56	8	Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing	H01H1/56	H01H1/56		129
H01H1/58	8	Electric connections to or between contacts; Terminals {(for high tension switches H01H33/025; for electromagnetic relays H01H50/14; for circuit breakers H01H71/08)}	H01H1/58	H01H1/58		1771
H01H1/5805	9	{Connections to printed circuits (for slide switches H01H15/005; for tumbler switches H01H23/006)}	H01H1/58	H01H1/58		774
H01H2001/5811	10	{both fixed and movable contacts being formed by blank stamping and mounted or soldered on printed circuit board without any other housing elements}	H01H1/58	H01H1/58		38
H01H2001/5816	10	{Connections to flexible or curved printed circuit boards}	H01H1/58	H01H1/58		82
H01H1/5822	9	{Flexible connections between movable contact and terminal}	H01H1/58	H01H1/58		529
H01H2001/5827	10	{Laminated connections, i.e. the flexible conductor is composed of a plurality of thin flexible conducting layers}	H01H1/58	H01H1/58		107
H01H1/5833	9	{comprising an articulating, sliding or rolling contact between movable contact and terminal}	H01H1/58	H01H1/58		423
H01H2001/5838	10	{using electrodynamic forces for enhancing the contact pressure between the sliding surfaces}	H01H1/58	H01H1/58		49
H01H1/5844	9	{making use of wire-gripping clips or springs}	H01H1/58	H01H1/58		286
H01H1/585	10	{and piercing the wire insulation}	H01H1/58	H01H1/58		80
H01H1/5855	9	{characterised by the use of a wire clamping screw or nut}	H01H1/58	H01H1/58		277
H01H2001/5861	10	{Box connector with a collar or lug for clamping internal rail and external conductor together by a tightening screw}	H01H1/58	H01H1/58		124
H01H1/5866	9	{characterised by the use of a plug and socket connector}	H01H1/58	H01H1/58		390
H01H2001/5872	10	{including means for preventing incorrect coupling}	H01H1/58	H01H1/58		20
H01H2001/5877	9	{with provisions for direct mounting on a battery pole}	H01H1/58	H01H1/58		181
H01H2001/5883	9	{the extension of the contact being crimped around a wire}	H01H1/58	H01H1/58		49
H01H2001/5888	9	{Terminals of surface mounted devices [SMD]}	H01H1/58	H01H1/58		279
H01H2001/5894	9	{the extension of the contact being welded to a wire or a bus}	H01H1/58	H01H1/58		18
H01H1/60	8	Auxiliary means structurally associated with the switch for cleaning or lubricating contact-making surfaces (cleaning by normal sliding of contacts H01H1/18, H01H1/36)	H01H1/60	H01H1/60		364
H01H1/605	9	{Cleaning of contact-making surfaces by relatively high voltage pulses}	H01H1/60	H01H1/60		155
H01H1/62	8	Heating or cooling of contacts	H01H1/62	H01H1/62		427
H01H1/64	8	Protective enclosures, baffle plates, or screens for contacts	H01H1/64	H01H1/64		282
H01H1/645	9	{containing getter material (for explosion inhibiting in explosion-proofcases H01H9/046; for vacuum switches H01H33/6683)}	H01H1/64	H01H1/64		48
H01H1/66	9	Contacts sealed in an evacuated or gas-filled envelope, e.g. magnetic dry-reed contacts	H01H1/66	H01H1/66		317
H01H3/00	7	Mechanisms for operating contacts ({for tap changers H01H9/0027;} thermal actuating or release means H01H37/02)	H01H3/00	H01H3/00		184
H01H3/001	8	{Means for preventing or breaking contact-welding}	H01H3/00	H01H3/00		620
H01H2003/002	9	{with lockout, e.g. two contact pairs in series}	H01H3/00	H01H3/00		28
H01H3/004	8	{for operating contacts periodically}	H01H3/00	H01H3/00		453
H01H3/005	8	{making use of superconductivity, e.g. levitation switch}	H01H3/00	H01H3/00		41
H01H2003/007	8	{the contacts being actuated by deformation of a flexible housing}	H01H3/00	H01H3/00		70
H01H2003/008	8	{with a haptic or a tactile feedback controlled by electrical means, e.g. a motor or magnetofriction}	H01H3/00	H01H3/00		416
H01H3/02	8	Operating parts, i.e. for operating driving mechanism by a mechanical force external to the switch	H01H3/02	H01H3/02		1581
H01H3/0206	9	{Combined operation of electric switch and of fluid control device}	H01H3/02	H01H3/02		322
H01H3/0213	9	{Combined operation of electric switch and variable impedance, e.g. resistor, capacitor (H01H9/061 takes precedence)}	H01H3/02	H01H3/02		336
H01H3/022	9	{Emergency operating parts, e.g. for stop-switch in dangerous conditions}	H01H3/02	H01H3/02		620
H01H3/0226	10	{operated by a pull cord}	H01H3/02	H01H3/02		162
H01H2003/0233	10	{for alarm triggering, e.g. fire alarm, emergency off switches operated by breaking a glass}	H01H3/02	H01H3/02		108
H01H2003/024	10	{Resetting of bistable emergency operating part by pulling it}	H01H3/02	H01H3/02		53
H01H2003/0246	10	{Resetting of bistable emergency operating part by rotating itself or an accessory}	H01H3/02	H01H3/02		79
H01H3/0253	9	{two co-operating contacts actuated independently (for combined circuit-breaker-contactors H01H89/10)}	H01H3/02	H01H3/02		135
H01H2003/026	9	{specially adapted to avoid injury to occupants of a car during an accident}	H01H3/02	H01H3/02		87
H01H2003/0266	9	{Operating part bringable in an inoperative position by an electrical drive}	H01H3/02	H01H3/02		39
H01H2003/0273	9	{Manually irreversibly actuated switch}	H01H3/02	H01H3/02		38
H01H2003/028	9	{Rotating knob or lever or tumbler that can be turned or pushed by hand in only one direction, e.g. by making inaccessible one side of a tumbler}	H01H3/02	H01H3/02		49
H01H2003/0286	9	{having a weak point breaking or uncoupling on abnormal external force}	H01H3/02	H01H3/02		58
H01H2003/0293	9	{with an integrated touch switch}	H01H3/02	H01H3/02		339
H01H3/04	9	Levers (tumblers H01H23/14)	H01H3/04	H01H3/04		482
H01H3/06	10	Means for securing to shaft of driving mechanism	H01H3/06	H01H3/06		84
H01H3/08	9	Turn knobs	H01H3/08	H01H3/08		573
H01H2003/085	10	{Retractable turn knobs, e.g. flush mounted}	H01H3/08	H01H3/08		189
H01H3/10	10	Means for securing to shaft of driving mechanism	H01H3/10	H01H3/10		304
H01H2003/105	11	{with compensation of misalignment in the link between the operating part, the driving mechanism and the switch, e.g. misalignment between two axis}	H01H3/10	H01H3/10		78
H01H3/12	9	Push-buttons	H01H3/12	H01H3/12		904
H01H3/122	10	{with enlarged actuating area, e.g. of the elongated bar-type; Stabilising means therefor}	H01H3/12	H01H3/12		500
H01H3/125	11	{using a scissor mechanism as stabiliser}	H01H3/12	H01H3/12		1297
H01H2003/127	10	{Details of the key cap concerning the actuation by fingernails or having provision to allow usage with long fingernails}	H01H3/12	H01H3/12		45
H01H3/14	9	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H3/14	H01H3/14		658
H01H3/141	10	{Cushion or mat switches}	H01H3/14	H01H3/14		604
H01H3/142	11	{of the elongated strip type}	H01H3/14	H01H3/14		479
H01H2003/143	12	{provisions for avoiding the contact actuation when the elongated strip is bended}	H01H3/14	H01H3/14		21
H01H2003/145	11	{provisions for avoiding closure or contact damage during manufacturing or mounting}	H01H3/14	H01H3/14		5
H01H2003/146	11	{being normally closed}	H01H3/14	H01H3/14		55
H01H2003/147	11	{Special aspects regarding the peripheral edges of the mat switches}	H01H3/14	H01H3/14		42
H01H2003/148	11	{the mat switch being composed by independently juxtaposed contact tiles, e.g. for obtaining a variable protected area}	H01H3/14	H01H3/14		31
H01H3/16	9	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. for a door switch, a limit switch, a floor-levelling switch of a lift	H01H3/16	H01H3/16		1138
H01H3/161	10	{for actuation by moving a closing member, e.g. door, cover or lid (the switch controlling enclosed equipment H01H9/226; switches operated by a removable member, wherein one single insertion movement of a key comprises an unlocking stroke and a switch actuating stroke, e.g. security switch for safety guards H01H27/002)}	H01H3/16	H01H3/16		656
H01H3/162	11	{associated with a hinge of the closing member}	H01H3/16	H01H3/16		157
H01H3/163	11	{associated with locking or manipulating means of the closing member}	H01H3/16	H01H3/16		154
H01H2003/165	11	{associated with an edge of the closing member}	H01H3/16	H01H3/16		32
H01H3/166	10	{Self-adjusting mountings, transmissions and the like}	H01H3/16	H01H3/16		138
H01H2003/167	11	{with locking of the adjusted parts in the adjusted position by a separate action}	H01H3/16	H01H3/16		23
H01H3/168	10	{operated by movement in any direction}	H01H3/16	H01H3/16		63
H01H3/18	10	the movement in one direction being intentionally by hand, e.g. for setting automatically cancelled trafficators	H01H3/18	H01H3/18		23
H01H3/20	9	wherein an auxiliary movement thereof, or of an attachment thereto, is necessary before the main movement is possible or effective, e.g. for unlatching, for coupling	H01H3/20	H01H3/20		814
H01H3/22	8	Power arrangements internal to the switch for operating the driving mechanism	H01H3/22	H01H3/22		281
H01H3/222	9	{using electrodynamic repulsion}	H01H3/22	H01H3/22		183
H01H2003/225	10	{with coil contact, i.e. the movable contact itself forms a secondary coil in which the repulsing current is induced by an operating current in a stationary coil}	H01H3/22	H01H3/22		33
H01H3/227	9	{Interlocked hand- and power-operating mechanisms}	H01H3/22	H01H3/22		192
H01H3/24	9	using pneumatic or hydraulic actuator {(for storing energy in a spring motor H01H3/301)}	H01H3/24	H01H3/24		631
H01H3/26	9	using dynamo-electric motor (for storing energy in a spring motor H01H3/30)	H01H3/26	H01H3/26		1553
H01H3/262	10	{using a centrifugal mechanism}	H01H3/26	H01H3/26		26
H01H3/264	10	{using a travelling nut mechanism}	H01H3/26	H01H3/26		100
H01H2003/266	10	{having control circuits for motor operating switches, e.g. controlling the opening or closing speed of the contacts}	H01H3/26	H01H3/26		280
H01H2003/268	10	{using a linear motor}	H01H3/26	H01H3/26		63
H01H3/28	9	using electromagnet (for storing energy in a spring motor H01H3/30; for operating relays H01H45/00)	H01H3/28	H01H3/28		1220
H01H3/30	9	using spring motor	H01H3/30	H01H3/30		1136
H01H3/3005	10	{Charging means}	H01H3/30	H01H3/30		199
H01H3/301	11	{using a fluid actuator}	H01H3/30	H01H3/30		51
H01H3/3015	11	{using cam devices}	H01H3/30	H01H3/30		228
H01H3/3021	11	{using unidirectional coupling}	H01H3/30	H01H3/30		103
H01H3/3026	11	{in which the closing spring charges the opening spring or vice versa}	H01H3/30	H01H3/30		84
H01H3/3031	10	{Means for locking the spring in a charged state}	H01H3/30	H01H3/30		428
H01H2003/3036	11	{using of balls or rollers in the locking device}	H01H3/30	H01H3/30		63
H01H3/3042	10	{using a torsion spring}	H01H3/30	H01H3/30		242
H01H3/3047	10	{adapted for operation of a three-position switch, e.g. on-off-earth}	H01H3/30	H01H3/30		111
H01H3/3052	10	{Linear spring motors}	H01H3/30	H01H3/30		149
H01H2003/3057	10	{provisions for avoiding idling, e.g. preventing release of stored energy when a breaker is closed, or when the springs are not fully charged}	H01H3/30	H01H3/30		45
H01H2003/3063	10	{Decoupling charging handle or motor at end of charging cycle or during charged condition}	H01H3/30	H01H3/30		77
H01H2003/3068	10	{Housing support frame for energy accumulator and cooperating mechanism}	H01H3/30	H01H3/30		45
H01H2003/3073	10	{Indication of the charge on the spring motor}	H01H3/30	H01H3/30		43
H01H2003/3078	10	{using an inertia element, e.g. a flywheel, to controll the energy released by the spring}	H01H3/30	H01H3/30		31
H01H2003/3084	10	{Kinetic energy of moving parts recuperated by transformation into potential energy in closing or opening spring to be used in next operation}	H01H3/30	H01H3/30		44
H01H2003/3089	10	{Devices for manual releasing of locked charged spring motor;  Devices for remote releasing}	H01H3/30	H01H3/30		80
H01H2003/3094	10	{allowing an opening - closing - opening [OCO] sequence}	H01H3/30	H01H3/30		61
H01H3/32	8	Driving mechanisms, i.e. for transmitting driving force to the contacts (snap-action arrangements H01H5/00; introducing a predetermined time delay H01H7/00)	H01H3/32	H01H3/32		1562
H01H2003/323	9	{the mechanisms being adjustable}	H01H3/32	H01H3/32		167
H01H2003/326	9	{using bearings}	H01H3/32	H01H3/32		144
H01H3/34	9	using ratchet	H01H3/34	H01H3/34		149
H01H3/36	9	using belt, chain, or cord	H01H3/36	H01H3/36		259
H01H3/38	9	using spring or other flexible shaft coupling	H01H3/38	H01H3/38		625
H01H3/40	9	using friction, toothed, or screw-and-nut gearing	H01H3/40	H01H3/40		1171
H01H2003/405	10	{using a walking nut}	H01H3/40	H01H3/40		69
H01H3/42	9	using cam or eccentric	H01H3/42	H01H3/42		1077
H01H3/44	9	using Geneva movement	H01H3/44	H01H3/44		173
H01H3/46	9	using rod or lever linkage, e.g. toggle	H01H3/46	H01H3/46		1288
H01H2003/463	10	{using a blade spring lever for perpendicular force transmission}	H01H3/46	H01H3/46		36
H01H2003/466	10	{using a living hinge to connect the levers}	H01H3/46	H01H3/46		76
H01H3/48	9	using lost-motion device	H01H3/48	H01H3/48		129
H01H3/50	9	with indexing or locating means, e.g. indexing by ball and spring	H01H3/50	H01H3/50		397
H01H3/503	10	{making use of electromagnets}	H01H3/50	H01H3/50		359
H01H2003/506	10	{making use of permanent magnets}	H01H3/50	H01H3/50		136
H01H3/52	9	with means to ensure stopping at intermediate operative positions	H01H3/52	H01H3/52		105
H01H3/54	8	Mechanisms for coupling or uncoupling operating parts, driving mechanisms, or contacts	H01H3/54	H01H3/54		213
H01H3/56	9	using electromagnetic clutch	H01H3/56	H01H3/56		99
H01H3/58	9	using friction, toothed, or other mechanical clutch	H01H3/58	H01H3/58		374
H01H3/60	8	Mechanical arrangements for preventing or damping vibration or shock	H01H3/60	H01H3/60		1030
H01H3/605	9	{making use of a fluid damper}	H01H3/60	H01H3/60		273
H01H3/62	8	Lubricating means structurally associated with the switch (for lubricating contact-making surfaces H01H1/60)	H01H3/62	H01H3/62		114
H01H5/00	7	Snap-action arrangements, i.e. in which during a single opening operation or a single closing operation energy is first stored and then released to produce or assist the contact movement	H01H5/00	H01H5/00		78
H01H5/02	8	Energy stored by the attraction or repulsion of magnetic parts	H01H5/02	H01H5/02		565
H01H5/04	8	Energy stored by deformation of elastic members (by deformation of bimetallic element in thermally-actuated switches H01H37/54)	H01H5/04	H01H5/04		241
H01H5/045	9	{making use of cooperating spring loaded wedging or camming parts between operating member and contact structure}	H01H5/04	H01H5/04		289
H01H5/06	9	by compression or extension of coil springs	H01H5/06	H01H5/06		545
H01H5/08	10	one end of spring transmitting movement to the contact member when the other end is moved by the operating part	H01H5/08	H01H5/08		61
H01H5/10	10	one end of spring being fixedly connected to the stationary or movable part of the switch and the other end reacting with a movable or stationary rigid member respectively through pins, cams, toothed or other shaped surfaces	H01H5/10	H01H5/10		46
H01H5/12	10	having two or more snap-action motions in succession	H01H5/12	H01H5/12		26
H01H5/14	9	by twisting of torsion members	H01H5/14	H01H5/14		31
H01H5/16	10	with auxiliary means for temporarily holding parts until torsion member is sufficiently strained	H01H5/16	H01H5/16		79
H01H5/18	9	by flexing of blade springs	H01H5/18	H01H5/18		525
H01H5/20	10	single blade moved across dead-centre position	H01H5/20	H01H5/20		44
H01H5/22	10	blade spring with at least one snap-acting leg and at least one separate contact-carrying or contact-actuating leg	H01H5/22	H01H5/22		25
H01H5/24	11	having three legs	H01H5/24	H01H5/24		17
H01H5/26	10	having two or more snap-action motions in succession	H01H5/26	H01H5/26		5
H01H5/28	10	two separate blade springs forming a toggle	H01H5/28	H01H5/28		6
H01H5/30	9	by buckling of disc springs	H01H5/30	H01H5/30		146
H01H7/00	7	Devices for introducing a predetermined time delay between the initiation of the switching operation and the opening or closing of the contacts (time or time-programme switches H01H43/00)	H01H7/00	H01H7/00		161
H01H7/02	8	with fluid timing means	H01H7/02	H01H7/02		82
H01H7/03	9	with dash-pots	H01H7/03	H01H7/03		111
H01H7/04	9	with flies, i.e. fan governors	H01H7/04	H01H7/04		10
H01H7/06	8	with thermal timing means	H01H7/06	H01H7/06		15
H01H7/08	8	with timing by mechanical speed-control devices	H01H7/08	H01H7/08		91
H01H7/10	9	by escapement	H01H7/10	H01H7/10		13
H01H7/12	10	mechanical	H01H7/12	H01H7/12		57
H01H7/14	10	electromagnetic	H01H7/14	H01H7/14		39
H01H7/16	8	Devices for ensuring operation of the switch at a predetermined point in the AC cycle (circuit arrangements&#160;H01H9/56)	H01H7/16	H01H7/16		41
H01H9/00	7	Details of switching devices, not covered by groups H01H1/00&#160;-&#160;H01H7/00	H01H9/00	H01H9/00		766
H01H9/0005	8	{Tap change devices}	H01H9/00	H01H9/00		927
H01H9/0011	9	{Voltage selector switches}	H01H9/00	H01H9/00		181
H01H9/0016	9	{Contact arrangements for tap changers}	H01H9/00	H01H9/00		613
H01H2009/0022	10	{Mounting of the fixed contacts or taps on cylindrical wall of oil vessel containing the tap changer;  Details of screening}	H01H9/00	H01H9/00		55
H01H9/0027	9	{Operating mechanisms}	H01H9/00	H01H9/00		701
H01H9/0033	10	{with means for indicating the selected tap or limiting the number of selectable taps}	H01H9/00	H01H9/00		86
H01H9/0038	9	{making use of vacuum switches}	H01H9/00	H01H9/00		329
H01H9/0044	9	{Casings; Mountings; Disposition in transformer housing}	H01H9/00	H01H9/00		264
H01H2009/005	10	{Details concerning the sealing of the oil filled casings}	H01H9/00	H01H9/00		55
H01H2009/0055	9	{Oil filters for tap change devices}	H01H9/00	H01H9/00		39
H01H2009/0061	9	{Monitoring tap change switching devices}	H01H9/00	H01H9/00		193
H01H9/0066	8	{Auxiliary contact devices (for arc transfer H01H9/38; for electromagnetic relays H01H50/541)}	H01H9/00	H01H9/00		433
H01H9/0072	8	{particular to three-phase switches (synchronous switching H01H9/563)}	H01H9/00	H01H9/00		158
H01H2009/0077	8	{using recyclable materials, e.g. for easier recycling or minimising the packing material}	H01H9/00	H01H9/00		67
H01H2009/0083	8	{using redundant components, e.g. two pressure tubes for pressure switch}	H01H9/00	H01H9/00		170
H01H2009/0088	8	{Details of rotatable shafts common to more than one pole or switch unit}	H01H9/00	H01H9/00		85
H01H2009/0094	8	{Details of rotatable shafts which are subdivided;  details of the coupling means thereof}	H01H9/00	H01H9/00		93
H01H9/02	8	Bases, casings, or covers (accommodating more than one switch or a switch and another electrical component H02B1/26)	H01H9/02	H01H9/02		2903
H01H9/0207	9	{Adjustable mounting of casings}	H01H9/02	H01H9/02		238
H01H9/0214	9	{Hand-held casings}	H01H9/02	H01H9/02		448
H01H2009/0221	10	{the switches being fixed to the operator&apos;s hand, e.g. integrated in a glove or fixed to a ring}	H01H9/02	H01H9/02		78
H01H9/0228	10	{Line cord switches}	H01H9/02	H01H9/02		270
H01H9/0235	10	{specially adapted for remote control, e.g. of audio or video apparatus}	H01H9/02	H01H9/02		692
H01H9/0242	11	{Protective enclosures; Cushioning means}	H01H9/02	H01H9/02		145
H01H9/025	11	{Stands or organisers to facilitate location or operation}	H01H9/02	H01H9/02		173
H01H2009/0257	11	{Multisided remote control, comprising control or display elements on at least two sides, e.g. front and back surface}	H01H9/02	H01H9/02		89
H01H9/0264	9	{Protective covers for terminals}	H01H9/02	H01H9/02		587
H01H9/0271	9	{structurally combining a switch and an electronic component (for relays H01H50/021)}	H01H9/02	H01H9/02		559
H01H2009/0278	9	{Casings containing special noise reduction means, e.g. elastic foam between inner and outer casing}	H01H9/02	H01H9/02		94
H01H2009/0285	9	{Casings overmoulded over assembled switch or relay}	H01H9/02	H01H9/02		45
H01H2009/0292	9	{Transparent window or opening, e.g. for allowing visual inspection of contact position or contact condition}	H01H9/02	H01H9/02		302
H01H9/04	9	Dustproof, splashproof, drip-proof, waterproof, or flameproof casings	H01H9/04	H01H9/04		1923
H01H9/041	10	{Casings hermetically closed by a diaphragm through which passes an actuating member (vacuum switches H01H33/66)}	H01H9/04	H01H9/04		109
H01H9/042	10	{Explosion-proof cases}	H01H9/04	H01H9/04		448
H01H9/043	11	{with pressure-relief devices}	H01H9/04	H01H9/04		67
H01H9/045	11	{with interlocking mechanism between cover and operating mechanism}	H01H9/04	H01H9/04		126
H01H9/046	11	{with internal explosion inhibiting means}	H01H9/04	H01H9/04		44
H01H9/047	10	{provided with venting means}	H01H9/04	H01H9/04		223
H01H2009/048	10	{using a sealing boot, e.g. the casing having separate elastic body surrounding the operating member and hermetically closing the opening for it}	H01H9/04	H01H9/04		375
H01H9/06	9	Casing of switch constituted by a handle serving a purpose other than the actuation of the switch, e.g. by the handle of a vacuum cleaner	H01H9/06	H01H9/06		1043
H01H9/061	10	{enclosing a continuously variable impedance}	H01H9/06	H01H9/06		293
H01H9/063	10	{enclosing a reversing switch}	H01H9/06	H01H9/06		199
H01H2009/065	10	{Battery operated hand tools in which the battery and the switch are directly connected}	H01H9/06	H01H9/06		64
H01H2009/066	10	{having switches mounted on a control handle, e.g. gear shift lever}	H01H9/06	H01H9/06		167
H01H2009/068	10	{with switches mounted on a handlebar, e.g. for motorcycles, fork lift trucks, etc.}	H01H9/06	H01H9/06		326
H01H9/08	8	Arrangements to facilitate replacement of a switch, e.g. cartridge housing	H01H9/08	H01H9/08		407
H01H9/085	9	{contact separation effected by removing contact carrying element}	H01H9/08	H01H9/08		223
H01H9/10	8	Adaptation for built-in fuses (mounting switch and fuse separately on, or in, common support H02B1/18)	H01H9/10	H01H9/10		795
H01H9/102	9	{Fuses mounted on or constituting the movable contact parts of the switch}	H01H9/10	H01H9/10		608
H01H9/104	9	{with interlocking mechanism between switch and fuse}	H01H9/10	H01H9/10		511
H01H9/106	9	{fuse and switch being connected in parallel}	H01H9/10	H01H9/10		165
H01H2009/108	9	{Building a sliding and/or a removable bridging connector for batteries}	H01H9/10	H01H9/10		53
H01H9/12	8	Means for earthing parts of switch not normally conductively connected to the contacts	H01H9/12	H01H9/12		176
H01H9/14	8	Adaptation for built-in safety spark gaps	H01H9/14	H01H9/14		78
H01H9/16	8	Indicators for switching condition, e.g. "on" or "off"	H01H9/16	H01H9/16		1884
H01H9/161	9	{comprising light emitting elements}	H01H9/16	H01H9/16		1144
H01H9/162	10	{Means to facilitate removal or replacement of light-emitting elements}	H01H9/16	H01H9/16		163
H01H2009/164	10	{the light emitting elements being incorporated in and movable with the operating part}	H01H9/16	H01H9/16		105
H01H9/165	9	{comprising numbered dials (thumb-wheel switches H01H19/001)}	H01H9/16	H01H9/16		129
H01H9/167	9	{Circuits for remote indication}	H01H9/16	H01H9/16		814
H01H9/168	9	{making use of an electromagnetic wave communication}	H01H9/16	H01H9/16		394
H01H9/18	8	Distinguishing marks on switches, e.g. for indicating switch location in the dark; Adaptation of switches to receive distinguishing marks	H01H9/18	H01H9/18		934
H01H9/181	9	{using a programmable display, e.g. LED or LCD}	H01H9/18	H01H9/18		428
H01H9/182	9	{Illumination of the symbols or distinguishing marks (H01H9/181 takes precedence)}	H01H9/18	H01H9/18		806
H01H2009/183	10	{Provisions for enhancing the contrast between the illuminated symbol and the background or between juxtaposed symbols}	H01H9/18	H01H9/18		79
H01H2009/184	10	{Illumination of symbols by using laser light}	H01H9/18	H01H9/18		18
H01H9/185	9	{Fluorescent or phosphorescent symbols or distinguishing marks (H01H9/181 takes precedence)}	H01H9/18	H01H9/18		238
H01H2009/186	9	{using an electroluminiscent panel}	H01H9/18	H01H9/18		106
H01H2009/187	9	{having symbols engraved or printed by laser}	H01H9/18	H01H9/18		166
H01H2009/188	9	{with indication of rating}	H01H9/18	H01H9/18		44
H01H2009/189	9	{with a tactile symbol or indication, e.g. for blind people}	H01H9/18	H01H9/18		131
H01H9/20	8	Interlocking, locking, or latching mechanisms	H01H9/20	H01H9/20		1457
H01H9/22	9	for interlocking between casing, cover, or protective shutter and mechanism for operating contacts {(explosion-proof cases H01H9/045; built-in fuses and interlocking mechanisms H01H9/104; by automatic release of circuit breakers H01H71/126)}	H01H9/22	H01H9/22		1298
H01H9/223	10	{Defeatable locking means}	H01H9/22	H01H9/22		142
H01H9/226	10	{the casing containing electrical equipment other than and operated by the switch}	H01H9/22	H01H9/22		319
H01H9/24	9	for interlocking two or more parts of the mechanism for operating contacts	H01H9/24	H01H9/24		474
H01H9/26	9	for interlocking two or more switches ({H01H13/568 takes precedence;} by a detachable member H01H9/28{; for electromagnetic relays H01H50/323})	H01H9/26	H01H9/26		1906
H01H9/262	10	{using flexible transmission elements, e.g. Bowden cable}	H01H9/26	H01H9/26		79
H01H2009/265	10	{with interlocking of more than two switches}	H01H9/26	H01H9/26		169
H01H2009/267	10	{with interlocking of two out of three switches, e.g. two switches each connecting a power supply to a busbar and a bus coupling switch interlocked in such a way that the power supplies are never connected in parallel}	H01H9/26	H01H9/26		40
H01H9/28	9	for locking switch parts by a key or equivalent removable member (switches operated by a key H01H27/00; locking by removable part of two-part coupling device H01R)	H01H9/28	H01H9/28		299
H01H9/281	10	{making use of a padlock (H01H9/287 takes precedence)}	H01H9/28	H01H9/28		274
H01H9/282	11	{and a separate part mounted or mountable on the switch assembly and movable between an unlocking position and a locking position where it can be secured by the padlock}	H01H9/28	H01H9/28		312
H01H9/283	12	{the part being removable}	H01H9/28	H01H9/28		179
H01H9/285	10	{Locking mechanisms incorporated in the switch assembly and operable by a key or a special tool}	H01H9/28	H01H9/28		227
H01H9/286	10	{making use of a removable locking part acting directly on the operating part (H01H9/281 takes precedence)}	H01H9/28	H01H9/28		172
H01H9/287	10	{wherein the operating part is made inaccessible or more difficult to access by a lid, cover or guard, e.g. lockable covers}	H01H9/28	H01H9/28		309
H01H2009/288	10	{Provisions relating to welded contacts}	H01H9/28	H01H9/28		52
H01H9/30	8	Means for extinguishing or preventing arc between current-carrying parts	H01H9/30	H01H9/30		1119
H01H9/302	9	{wherein arc-extinguishing gas is evolved from stationary parts}	H01H9/30	H01H9/30		305
H01H2009/305	9	{including means for screening for arc gases as protection of mechanism against hot arc gases or for keeping arc gases in the arc chamber}	H01H9/30	H01H9/30		198
H01H2009/307	9	{with slow break, e.g. for AC current waiting for a zero crossing}	H01H9/30	H01H9/30		57
H01H9/32	9	Insulating body insertable between contacts	H01H9/32	H01H9/32		571
H01H9/34	9	Stationary parts for restricting or subdividing the arc, e.g. barrier plate	H01H9/34	H01H9/34		1269
H01H9/341	10	{Barrier plates carrying electrodes}	H01H9/34	H01H9/34		78
H01H9/342	10	{Venting arrangements for arc chutes}	H01H9/34	H01H9/34		807
H01H2009/343	11	{with variable venting aperture function of arc chute internal pressure, e.g. resilient flap-valve or check-valve}	H01H9/34	H01H9/34		116
H01H9/345	10	{Mounting of arc chutes}	H01H9/34	H01H9/34		173
H01H9/346	10	{Details concerning the arc formation chamber}	H01H9/34	H01H9/34		260
H01H2009/347	10	{using lids for closing the arc chamber after assembly}	H01H9/34	H01H9/34		38
H01H2009/348	10	{Provisions for recirculation of arcing gasses to improve the arc extinguishing, e.g. move the arc quicker into the arcing chamber}	H01H9/34	H01H9/34		85
H01H9/36	10	Metal parts	H01H9/36	H01H9/36		590
H01H9/362	11	{Mounting of plates in arc chamber}	H01H9/36	H01H9/36		237
H01H2009/365	11	{using U-shaped plates}	H01H9/36	H01H9/36		128
H01H2009/367	11	{defining a recurrent path, e.g. the subdivided arc is moved in a closed path between each pair of splitter plates}	H01H9/36	H01H9/36		23
H01H9/38	9	Auxiliary contacts on to which the arc is transferred from the main contacts (using arcing-horns H01H9/46)	H01H9/38	H01H9/38		511
H01H9/383	10	{Arcing contact pivots relative to the movable contact assembly}	H01H9/38	H01H9/38		122
H01H9/386	10	{Arcing contact pivots relative to the fixed contact assembly}	H01H9/38	H01H9/38		59
H01H9/40	9	Multiple main contacts for the purpose of dividing the current through, or potential drop along, the arc	H01H9/40	H01H9/40		309
H01H9/42	9	Impedances connected with contacts	H01H9/42	H01H9/42		325
H01H9/44	9	using blow-out magnet	H01H9/44	H01H9/44		920
H01H9/443	10	{using permanent magnets}	H01H9/44	H01H9/44		791
H01H9/446	10	{using magnetisable elements associated with the contacts}	H01H9/44	H01H9/44		255
H01H9/46	9	using arcing horns (using blow-out magnet H01H9/44)	H01H9/46	H01H9/46		486
H01H9/465	10	{Shunt circuit closed by transferring the arc onto an auxiliary electrode}	H01H9/46	H01H9/46		45
H01H9/48	8	Means for preventing discharge to non-current-carrying parts, e.g. using corona ring	H01H9/48	H01H9/48		123
H01H9/50	8	Means for detecting the presence of an arc or discharge	H01H9/50	H01H9/50		161
H01H9/52	8	Cooling of switch parts (cooling of contacts H01H1/62)	H01H9/52	H01H9/52		1607
H01H2009/523	9	{by using heat pipes}	H01H9/52	H01H9/52		134
H01H2009/526	9	{of the high voltage switches}	H01H9/52	H01H9/52		356
H01H9/54	8	Circuit arrangements not adapted to a particular application of the switching device and for which no provision exists elsewhere	H01H9/54	H01H9/54		1821
H01H9/541	9	{Contacts shunted by semiconductor devices}	H01H9/54	H01H9/54		374
H01H9/542	10	{Contacts shunted by static switch means}	H01H9/54	H01H9/54		938
H01H2009/543	11	{third parallel branch comprising an energy absorber, e.g. MOV, PTC, Zener}	H01H9/54	H01H9/54		245
H01H2009/544	11	{the static switching means being an insulated gate bipolar transistor, e.g. IGBT, Darlington configuration of FET and bipolar transistor}	H01H9/54	H01H9/54		212
H01H2009/545	11	{comprising a parallel semiconductor switch being fired optically, e.g. using a photocoupler,}	H01H9/54	H01H9/54		108
H01H2009/546	11	{the static switching means being triggered by the voltage over the mechanical switch contacts}	H01H9/54	H01H9/54		110
H01H9/547	9	{Combinations of mechanical switches and static switches, the latter being controlled by the former}	H01H9/54	H01H9/54		328
H01H9/548	9	{Electromechanical and static switch connected in series}	H01H9/54	H01H9/54		448
H01H9/56	9	for ensuring operation of the switch at a predetermined point in the AC cycle	H01H9/56	H01H9/56		643
H01H9/563	10	{for multipolar switches, e.g. different timing for different phases, selecting phase with first zero-crossing}	H01H9/56	H01H9/56		243
H01H2009/566	10	{with self learning, e.g. measured delay is used in later actuations}	H01H9/56	H01H9/56		104
H01H11/00	7	Apparatus or processes specially adapted for the manufacture of electric switches (processes specially adapted for manufacture of rectilinearly movable switches having a plurality of operating members associated with different sets of contacts, e.g. keyboards, H01H13/88)	H01H11/00	H01H11/00		2314
H01H11/0006	8	{for converting electric switches (H01H13/564 takes precedence)}	H01H11/00	H01H11/00		609
H01H11/0012	9	{for converting normally open to normally closed switches and vice versa}	H01H11/00	H01H11/00		242
H01H11/0018	9	{for allowing different operating parts}	H01H11/00	H01H11/00		257
H01H2011/0025	10	{with provisions for allowing different orientation of the operating part, e.g. turning knob can be mounted in different positions}	H01H11/00	H01H11/00		43
H01H11/0031	9	{for allowing different types or orientation of connections to contacts}	H01H11/00	H01H11/00		263
H01H2011/0037	10	{with removable or replaceable terminal blocks}	H01H11/00	H01H11/00		99
H01H2011/0043	9	{for modifying the number or type of operating positions, e.g. momentary and stable}	H01H11/00	H01H11/00		110
H01H11/005	8	{of reed switches}	H01H11/00	H01H11/00		206
H01H11/0056	8	{comprising a successive blank-stamping, insert-moulding and severing operation}	H01H11/00	H01H11/00		404
H01H11/0062	8	{Testing or measuring non-electrical properties of switches, e.g. contact velocity (monitoring contacts H01H1/0015; monitoring gas density H01H33/563; monitoring vacuum H01H33/668; calibrating H01H69/01; adjusting H01H71/74; testing of electrical properties G01R31/333)}	H01H11/00	H01H11/00		491
H01H2011/0068	9	{measuring the temperature of the switch or parts thereof}	H01H11/00	H01H11/00		126
H01H2011/0075	8	{calibrating mechanical switching properties, e.g. "snap or switch moment", by mechanically deforming a part of the switch, e.g. elongating a blade spring by puncturing it with a laser}	H01H11/00	H01H11/00		105
H01H2011/0081	8	{using double shot moulding, e.g. for forming elastomeric sealing elements on form stable casing}	H01H11/00	H01H11/00		145
H01H2011/0087	8	{Welding switch parts by use of a laser beam}	H01H11/00	H01H11/00		173
H01H2011/0093	8	{Standardization, e.g. limiting the factory stock by limiting the number of unique, i.e. different components}	H01H11/00	H01H11/00		90
H01H11/02	8	for mercury switches	H01H11/02	H01H11/02		65
H01H11/04	8	of switch contacts	H01H11/04	H01H11/04		942
H01H11/041	9	{by bonding of a contact marking face to a contact body portion}	H01H11/04	H01H11/04		334
H01H11/042	10	{by mechanical deformation}	H01H11/04	H01H11/04		161
H01H11/043	10	{by resistance welding}	H01H11/04	H01H11/04		234
H01H11/045	10	{with the help of an intermediate layer (contacts provided with a solder layer H01H1/0231)}	H01H11/04	H01H11/04		100
H01H2011/046	10	{by plating}	H01H11/04	H01H11/04		94
H01H2011/047	10	{on both sides of the contact body portion}	H01H11/04	H01H11/04		38
H01H11/048	9	{by powder-metallurgical processes}	H01H11/04	H01H11/04		511
H01H11/06	9	Fixing of contacts to carrier {; Fixing of contacts to insulating carrier}	H01H11/06	H01H11/06		724
H01H2011/062	10	{by inserting only}	H01H11/06	H01H11/06		108
H01H2011/065	10	{by plating metal or conductive rubber on insulating substrate, e.g. Molded Interconnect Devices [MID]}	H01H11/06	H01H11/06		45
H01H2011/067	10	{by deforming, e.g. bending, folding or caulking, part of the contact or terminal which is being mounted}	H01H11/06	H01H11/06		95
H01H13/00	7	Switches having rectilinearly-movable operating part or parts adapted for pushing or pulling in one direction only, e.g. push-button switch (wherein the operating part is flexible H01H17/00)	H01H13/00	H01H13/00		704
H01H13/02	8	Details	H01H13/02	H01H13/02		1527
H01H13/023	9	{Light-emitting indicators (for multi-layer switches H01H13/83)}	H01H13/02	H01H13/02		2195
H01H2013/026	10	{with two or more independent lighting elements located inside the push button switch that illuminate separate zones of push buttons}	H01H13/02	H01H13/02		180
H01H13/04	9	Cases; Covers	H01H13/04	H01H13/04		1797
H01H13/06	10	Dustproof, splashproof, drip-proof, waterproof or flameproof casings	H01H13/06	H01H13/06		2035
H01H13/063	11	{Casings hermetically closed by a diaphragm through which passes an actuating member (vacuum switches H01H33/66)}	H01H13/06	H01H13/06		413
H01H2013/066	11	{using bellows}	H01H13/06	H01H13/06		80
H01H13/08	10	Casing of switch constituted by a handle serving a purpose other than the actuation of the switch	H01H13/08	H01H13/08		316
H01H13/10	9	Bases; Stationary contacts mounted thereon	H01H13/10	H01H13/10		1355
H01H13/12	9	Movable parts; Contacts mounted thereon	H01H13/12	H01H13/12		1295
H01H13/14	10	Operating parts, e.g. push-button	H01H13/14	H01H13/14		7335
H01H13/16	11	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H13/16	H01H13/16		523
H01H13/18	11	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H13/18	H01H13/18		684
H01H13/183	12	{for actuation by moving a closing member, e.g. door, cover (H01H13/186, H01H27/002 take precedence; the switch controlling enclosed equipment H01H9/226)}	H01H13/18	H01H13/18		385
H01H13/186	12	{wherein the pushbutton is rectilinearly actuated by a lever pivoting on the housing of the switch}	H01H13/18	H01H13/18		275
H01H13/20	10	Driving mechanisms	H01H13/20	H01H13/20		1245
H01H13/22	11	acting with snap action (depending upon deformation of elastic members H01H13/26)	H01H13/22	H01H13/22		75
H01H13/24	11	with means for introducing a predetermined time delay	H01H13/24	H01H13/24		38
H01H13/26	9	Snap-action arrangements depending upon deformation of elastic members	H01H13/26	H01H13/26		904
H01H13/28	10	using compression or extension of coil springs	H01H13/28	H01H13/28		1206
H01H13/285	11	{having a symmetrical configuration (H01H13/30&#160;-&#160;H01H13/34 take precedence)}	H01H13/28	H01H13/28		76
H01H13/30	11	one end of spring transmitting movement to the contact member when the other end is moved by the operating part	H01H13/30	H01H13/30		96
H01H13/32	11	one end of spring being fixedly connected to the stationary or movable part of the switch and the other end reacting with a movable or stationary rigid member respectively through pins, cams, toothed, or other shaped surfaces	H01H13/32	H01H13/32		65
H01H13/34	11	having two or more snap-action motions in succession	H01H13/34	H01H13/34		24
H01H13/36	10	using flexing of blade springs	H01H13/36	H01H13/36		789
H01H13/365	11	{having a symmetrical configuration (H01H13/38&#160;-&#160;H01H13/46 take precedence)}	H01H13/36	H01H13/36		123
H01H13/38	11	Single blade moved across dead-centre position	H01H13/38	H01H13/38		72
H01H13/40	11	Blade spring with at least one snap-acting leg and at least one separate contact-carrying or contact-actuating leg	H01H13/40	H01H13/40		35
H01H13/42	12	having three legs	H01H13/42	H01H13/42		61
H01H13/44	11	having two or more snap-action motions in succession	H01H13/44	H01H13/44		31
H01H13/46	11	two separate blade springs forming a toggle	H01H13/46	H01H13/46		70
H01H13/48	10	using buckling of disc springs	H01H13/48	H01H13/48		1146
H01H13/50	8	having a single operating member	H01H13/50	H01H13/50		289
H01H13/503	9	{Stacked switches}	H01H13/50	H01H13/50		190
H01H13/506	9	{with a make-break action in a single operation}	H01H13/50	H01H13/50		136
H01H13/52	9	the contact returning to its original state immediately upon removal of operating force, e.g. bell-push switch	H01H13/52	H01H13/52		1137
H01H2013/525	10	{using a return spring acting perpendicular to the actuating direction}	H01H13/52	H01H13/52		140
H01H13/54	9	the contact returning to its original state a predetermined time interval after removal of operating force, e.g. for staircase lighting	H01H13/54	H01H13/54		82
H01H13/56	9	the contact returning to its original state upon the next application of operating force	H01H13/56	H01H13/56		321
H01H13/562	10	{making use of a heart shaped cam}	H01H13/56	H01H13/56		408
H01H13/564	11	{convertible to momentary push button switches}	H01H13/56	H01H13/56		41
H01H2013/566	12	{by removable or exchangeable parts}	H01H13/56	H01H13/56		15
H01H13/568	11	{the contact also returning by some external action, e.g. interlocking, protection, remote control}	H01H13/56	H01H13/56		92
H01H13/58	10	with contact-driving member rotated step-wise in one direction	H01H13/58	H01H13/58		412
H01H13/585	11	{wherein the movable contact rotates around the axis of the push button}	H01H13/58	H01H13/58		202
H01H13/60	10	with contact-driving member moved alternately in opposite directions	H01H13/60	H01H13/60		432
H01H13/62	9	the contact returning to its original state upon manual release of a latch (latch released by second push-button H01H13/68)	H01H13/62	H01H13/62		267
H01H13/64	9	wherein the switch has more than two electrically distinguishable positions, e.g. multi-position push-button switches	H01H13/64	H01H13/64		556
H01H13/66	10	the operating member having only two positions	H01H13/66	H01H13/66		87
H01H13/68	8	having two operating members, one for opening and one for closing the same set of contacts (single operating member protruding from different sides of switch casing for alternate pushing upon opposite ends H01H15/22)	H01H13/68	H01H13/68		275
H01H13/70	8	having a plurality of operating members associated with different sets of contacts, e.g. keyboard (mounting together a plurality of independent switches H02B)	H01H13/70	H01H13/70		2228
H01H13/7006	9	{comprising a separate movable contact element for each switch site, all other elements being integrated in layers}	H01H13/70	H01H13/70		392
H01H13/7013	9	{in which the movable contacts of each switch site or of a row of switch sites are formed in a single plate}	H01H13/70	H01H13/70		111
H01H13/702	9	with contacts carried by or formed from layers in a multilayer structure, e.g. membrane switches	H01H13/702	H01H13/702		2338
H01H13/703	10	characterised by spacers between contact carrying layers	H01H13/703	H01H13/703		479
H01H13/704	10	characterised by the layers, e.g. by their material or structure (H01H13/703 takes precedence)	H01H13/704	H01H13/704		1075
H01H13/705	10	characterised by construction, mounting or arrangement of operating parts, e.g. push-buttons or keys	H01H13/705	H01H13/705		2790
H01H13/7057	11	characterised by the arrangement of operating parts in relation to each other, e.g. pre-assembled groups of keys	H01H13/7057	H01H13/7057		182
H01H13/7065	11	characterised by the mechanism between keys and layered keyboards	H01H13/7065	H01H13/7065		789
H01H13/7073	12	characterised by springs, e.g. Euler springs	H01H13/7073	H01H13/7073		266
H01H13/72	9	wherein the switch has means for limiting the number of operating members that can concurrently be in the actuated position	H01H13/72	H01H13/72		432
H01H13/74	10	each contact set returning to its original state only upon actuation of another of the operating members	H01H13/74	H01H13/74		326
H01H13/76	9	wherein some or all of the operating members actuate different combinations of the contact sets, e.g. ten operating members actuating different combinations of four contact sets	H01H13/76	H01H13/76		47
H01H13/78	9	characterised by the contacts or the contact sites	H01H13/78	H01H13/78		145
H01H13/785	10	characterised by the material of the contacts, e.g. conductive polymers	H01H13/785	H01H13/785		628
H01H13/79	10	characterised by the form of the contacts, e.g. interspersed fingers or helical networks	H01H13/79	H01H13/79		118
H01H13/80	10	characterised by the manner of cooperation of the contacts, e.g. with both contacts movable or with bounceless contacts	H01H13/80	H01H13/80		126
H01H13/803	10	characterised by the switching function thereof, e.g. normally closed contacts or consecutive operation of contacts	H01H13/803	H01H13/803		62
H01H13/807	10	characterised by the spatial arrangement of the contact sites, e.g. superimposed sites	H01H13/807	H01H13/807		503
H01H13/81	9	characterised by electrical connections to external devices	H01H13/81	H01H13/81		126
H01H13/82	9	characterised by contact space venting means	H01H13/82	H01H13/82		88
H01H13/83	9	characterised by legends, e.g. Braille, liquid crystal displays, light emitting or optical elements	H01H13/83	H01H13/83		2773
H01H13/84	9	characterised by ergonomic functions, e.g. for miniature keyboards; characterised by operational sensory functions, e.g. sound feedback (legends H01H13/83)	H01H13/84	H01H13/84		1006
H01H13/85	10	characterised by tactile feedback features	H01H13/85	H01H13/85		849
H01H13/86	9	characterised by the casing, e.g. sealed casings or casings reducible in size	H01H13/86	H01H13/86		1044
H01H13/88	9	Processes specially adapted for manufacture of rectilinearly movable switches having a plurality of operating members associated with different sets of contacts, e.g. keyboards	H01H13/88	H01H13/88		1052
H01H15/00	7	Switches having rectilinearly-movable operating part or parts adapted for actuation in opposite directions, e.g. slide switch	H01H15/00	H01H15/00		232
H01H15/005	8	{adapted for connection with printed circuit boards}	H01H15/00	H01H15/00		303
H01H15/02	8	Details	H01H15/02	H01H15/02		721
H01H15/025	9	{Light-emitting indicators}	H01H15/02	H01H15/02		56
H01H15/04	9	Stationary parts; Contacts mounted thereon	H01H15/04	H01H15/04		233
H01H15/06	9	Movable parts; Contacts mounted thereon	H01H15/06	H01H15/06		611
H01H15/08	10	Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing	H01H15/08	H01H15/08		93
H01H15/10	10	Operating parts	H01H15/10	H01H15/10		526
H01H15/102	11	{comprising cam devices}	H01H15/10	H01H15/10		688
H01H15/105	12	{Adjustable cams}	H01H15/10	H01H15/10		53
H01H15/107	12	{actuating conventional selfcontained microswitches (H01H15/105 takes precedence)}	H01H15/10	H01H15/10		138
H01H15/12	11	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H15/12	H01H15/12		11
H01H15/14	11	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H15/14	H01H15/14		91
H01H15/16	10	Driving mechanisms	H01H15/16	H01H15/16		164
H01H15/18	11	acting with snap action	H01H15/18	H01H15/18		263
H01H15/20	11	with means for introducing a predetermined time delay	H01H15/20	H01H15/20		5
H01H15/22	8	having a single operating part protruding from different sides of switch casing for alternate actuation from opposite ends	H01H15/22	H01H15/22		35
H01H15/24	8	having a single operating part only protruding from one side of the switch casing for alternate pushing and pulling	H01H15/24	H01H15/24		94
H01H17/00	7	Switches having flexible operating part adapted only for pulling, e.g. cord, chain {(for emergency stop switches H01H3/0226)}	H01H17/00	H01H17/00		621
H01H17/02	8	Details	H01H17/02	H01H17/02		31
H01H17/04	9	Stationary parts (guides H01H17/14)	H01H17/04	H01H17/04		6
H01H17/06	9	Movable parts (guides H01H17/14)	H01H17/06	H01H17/06		20
H01H17/08	10	Operating part, e.g. cord	H01H17/08	H01H17/08		117
H01H17/10	11	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H17/10	H01H17/10		3
H01H17/12	11	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H17/12	H01H17/12		32
H01H17/14	9	Guiding means for flexible operating part	H01H17/14	H01H17/14		8
H01H17/16	8	having a single flexible operating part adapted for pulling at one end only	H01H17/16	H01H17/16		18
H01H17/165	9	{secured to a part of the switch mechanism that has only rectilinear movement}	H01H17/16	H01H17/16		93
H01H17/18	9	secured to part of the switch driving mechanism that has only angular movement	H01H17/18	H01H17/18		14
H01H17/20	10	the contact returning to its original state immediately upon removal of operating force	H01H17/20	H01H17/20		8
H01H17/22	10	the contact returning to its original state upon the next application of operating force	H01H17/22	H01H17/22		46
H01H17/24	9	secured to a part of the switch driving mechanism that has both angular and rectilinear motion	H01H17/24	H01H17/24		2
H01H17/26	8	having two flexible operating parts; having a single operating part adapted for pulling at both ends	H01H17/26	H01H17/26		16
H01H17/28	9	secured to part or parts of the switch driving mechanism having only rectilinear motion	H01H17/28	H01H17/28		4
H01H17/30	9	secured to a part or parts of the switch driving mechanism having only angular motion	H01H17/30	H01H17/30		5
H01H19/00	7	Switches operated by an operating part which is rotatable about a longitudinal axis thereof and which is acted upon directly by a solid body external to the switch, e.g. by a hand	H01H19/00	H01H19/00		277
H01H19/001	8	{Thumb wheel switches}	H01H19/00	H01H19/00		266
H01H19/003	9	{having a pushbutton actuator}	H01H19/00	H01H19/00		210
H01H19/005	8	{Electromechanical pulse generators}	H01H19/00	H01H19/00		231
H01H2019/006	9	{being rotation direction sensitive, e.g. the generated pulse or code depends on the direction of rotation of the operating part}	H01H19/00	H01H19/00		143
H01H2019/008	8	{with snap mounting of rotatable part on fixed part, e.g. rotor on stator, operating knob on switch panel}	H01H19/00	H01H19/00		73
H01H19/02	8	Details	H01H19/02	H01H19/02		692
H01H19/025	9	{Light-emitting indicators}	H01H19/02	H01H19/02		654
H01H19/03	9	Means for limiting the angle of rotation of the operating part	H01H19/03	H01H19/03		276
H01H19/04	9	Cases; Covers	H01H19/04	H01H19/04		512
H01H19/06	10	Dustproof, splashproof, drip-proof, waterproof, or flameproof casings	H01H19/06	H01H19/06		290
H01H19/065	11	{Casings hermetically closed by a diaphragm through which passes an actuating member (vacuum switches H01H33/66)}	H01H19/06	H01H19/06		24
H01H19/08	9	Bases; Stationary contacts mounted thereon	H01H19/08	H01H19/08		544
H01H19/10	9	Movable parts; Contacts mounted thereon	H01H19/10	H01H19/10		637
H01H19/11	10	with indexing means	H01H19/11	H01H19/11		1139
H01H19/115	11	{using molded elastic parts only}	H01H19/11	H01H19/11		94
H01H19/12	10	Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing	H01H19/12	H01H19/12		81
H01H19/14	10	Operating parts, e.g. turn knob	H01H19/14	H01H19/14		2224
H01H2019/143	11	{having at least two concentric turn knobs}	H01H19/14	H01H19/14		140
H01H2019/146	11	{Roller type actuators}	H01H19/14	H01H19/14		210
H01H19/16	11	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H19/16	H01H19/16		18
H01H19/18	11	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H19/18	H01H19/18		155
H01H19/183	12	{adapted for operation by the simultaneous action of two cam plates, rotating at different speeds}	H01H19/18	H01H19/18		60
H01H19/186	12	{with travelling nuts}	H01H19/18	H01H19/18		134
H01H19/20	10	Driving mechanisms allowing angular displacement of the operating part to be effective in either direction	H01H19/20	H01H19/20		248
H01H19/22	11	incorporating lost motion	H01H19/22	H01H19/22		26
H01H19/24	11	acting with snap action	H01H19/24	H01H19/24		463
H01H19/26	11	with means for introducing a predetermined time delay	H01H19/26	H01H19/26		3
H01H19/28	10	Driving mechanisms allowing angular displacement of the operating part to be effective or possible in only one direction	H01H19/28	H01H19/28		95
H01H19/30	11	incorporating lost motion	H01H19/30	H01H19/30		6
H01H19/32	11	acting with snap action	H01H19/32	H01H19/32		86
H01H19/34	11	with means for introducing a predetermined time delay	H01H19/34	H01H19/34		8
H01H19/36	8	the operating part having only two operative positions, e.g. relatively displaced by 180 degrees	H01H19/36	H01H19/36		85
H01H19/38	9	Change-over switches	H01H19/38	H01H19/38		66
H01H19/40	10	having only axial contact pressure	H01H19/40	H01H19/40		26
H01H19/42	9	providing more than two electrically different conditions, e.g. for closing either or both of two circuits	H01H19/42	H01H19/42		24
H01H19/44	10	having only axial contact pressure	H01H19/44	H01H19/44		
H01H19/46	8	the operating part having three operative positions, e.g. off/star/delta	H01H19/46	H01H19/46		173
H01H19/48	9	having only axial contact pressure	H01H19/48	H01H19/48		23
H01H19/50	8	the operating part having four operative positions, e.g. off/two-in-series/one-only/two-in-parallel	H01H19/50	H01H19/50		81
H01H19/52	9	having only axial contact pressure	H01H19/52	H01H19/52		16
H01H19/54	8	the operating part having at least five or an unspecified number of operative positions	H01H19/54	H01H19/54		192
H01H19/56	9	Angularly-movable actuating part carrying contacts, e.g. drum switch	H01H19/56	H01H19/56		686
H01H19/563	10	{with an initial separation movement perpendicular to the switching movement}	H01H19/56	H01H19/56		139
H01H19/566	10	{in which the contact making surfaces are inclined, i.e. not perpendicular, to the axial or radial direction}	H01H19/56	H01H19/56		36
H01H19/58	10	having only axial contact pressure, e.g. disc switch, wafer switch	H01H19/58	H01H19/58		1151
H01H19/585	11	{provided with printed circuit contacts}	H01H19/58	H01H19/58		556
H01H19/60	9	Angularly-movable actuating part carrying no contacts	H01H19/60	H01H19/60		87
H01H19/605	10	{in which the actuation of the contacts depends on the direction of rotation}	H01H19/60	H01H19/60		37
H01H19/62	10	Contacts actuated by radial cams	H01H19/62	H01H19/62		1261
H01H19/623	11	{Adjustable cams}	H01H19/62	H01H19/62		201
H01H19/626	11	{actuating bridging contacts (H01H19/623 takes precedence)}	H01H19/62	H01H19/62		96
H01H19/63	10	Contacts actuated by axial cams {(H01H19/6355 takes precedence)}	H01H19/63	H01H19/63		388
H01H19/635	10	Contacts actuated by rectilinearly-movable member linked to operating part, e.g. by pin and slot	H01H19/635	H01H19/635		478
H01H19/6355	11	{using axial cam devices for transforming the angular movement into linear movement along the axis of rotation}	H01H19/635	H01H19/635		108
H01H19/64	8	Encased switches adapted for ganged operation when assembled in a line with identical switches, e.g. stacked switches	H01H19/64	H01H19/64		585
H01H21/00	7	Switches operated by an operating part in the form of a pivotable member acted upon directly by a solid body, e.g. by a hand (tumbler or rocker switches H01H23/00; switches having an operating part movable angularly in more than one plane H01H25/04)	H01H21/00	H01H21/00		160
H01H21/02	8	Details	H01H21/02	H01H21/02		402
H01H21/025	9	{Light-emitting indicators}	H01H21/02	H01H21/02		234
H01H21/04	9	Cases; Covers	H01H21/04	H01H21/04		272
H01H21/06	10	interlocked with operating mechanism	H01H21/06	H01H21/06		156
H01H21/08	10	Dustproof, splashproof, drip-proof, waterproof, or flameproof casings	H01H21/08	H01H21/08		179
H01H21/085	11	{Casings hermetically closed by a diaphragm through which passes an actuating member (vacuum switches H01H33/66)}	H01H21/08	H01H21/08		72
H01H21/10	10	Casing of switch constituted by a handle serving a purpose other than the actuation of the switch	H01H21/10	H01H21/10		172
H01H21/12	9	Bases; Stationary contacts mounted thereon	H01H21/12	H01H21/12		222
H01H21/14	9	Means for increasing contact pressure	H01H21/14	H01H21/14		92
H01H21/16	9	Adaptation for built-in fuse	H01H21/16	H01H21/16		112
H01H21/165	10	{Fuses mounted on, or constituting the movable contact parts of, the switch}	H01H21/16	H01H21/16		80
H01H21/18	9	Movable parts; Contacts mounted thereon	H01H21/18	H01H21/18		268
H01H21/20	10	Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing	H01H21/20	H01H21/20		26
H01H21/22	10	Operating parts, e.g. handle	H01H21/22	H01H21/22		975
H01H2021/225	11	{with push-pull operation, e.g. which can be pivoted in both directions by pushing or pulling on the same extremity of the operating member}	H01H21/22	H01H21/22		187
H01H21/24	11	biased to return to normal position upon removal of operating force	H01H21/24	H01H21/24		427
H01H21/245	12	{the contact returning to its original state upon the next application of operating force}	H01H21/24	H01H21/24		90
H01H21/26	12	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H21/26	H01H21/26		439
H01H21/28	12	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H21/28	H01H21/28		258
H01H21/282	13	{for actuation by moving a closing member, e.g. door, cover (the switch controlling enclosed equipment H01H9/226)}	H01H21/28	H01H21/28		74
H01H21/285	13	{having an operating arm actuated by the movement of the body and mounted on an axis converting its rotating movement into a rectilinear switch activating movement}	H01H21/28	H01H21/28		217
H01H2021/287	13	{with adjustable head, e.g. the actuator head can have different positions in relation to the limit switch itself}	H01H21/28	H01H21/28		50
H01H21/30	11	not biased to return to a normal position upon removal of operating force	H01H21/30	H01H21/30		51
H01H21/32	12	adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H21/32	H01H21/32		10
H01H21/34	12	adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H21/34	H01H21/34		92
H01H21/36	10	Driving mechanisms	H01H21/36	H01H21/36		313
H01H21/38	11	incorporating lost motion	H01H21/38	H01H21/38		46
H01H21/40	11	having snap action	H01H21/40	H01H21/40		100
H01H21/42	12	produced by compression or extension of coil spring	H01H21/42	H01H21/42		498
H01H21/44	12	produced by flexing blade springs	H01H21/44	H01H21/44		53
H01H21/46	12	with two or more snap-action motions in succession	H01H21/46	H01H21/46		13
H01H21/48	11	incorporating a ratchet mechanism	H01H21/48	H01H21/48		20
H01H21/50	11	with indexing or latching means, e.g. indexing by ball and spring; with means to ensure stopping at intermediate operative positions	H01H21/50	H01H21/50		360
H01H21/52	11	with means for introducing a predetermined time delay	H01H21/52	H01H21/52		26
H01H21/54	8	Lever switches with blade-type contact co-operating with one or two spring-clip contacts, e.g. knife switch	H01H21/54	H01H21/54		496
H01H21/56	9	making contact in one position only	H01H21/56	H01H21/56		83
H01H21/58	9	Change-over switches without stable intermediate position	H01H21/58	H01H21/58		120
H01H21/60	9	Change-over switches with stable intermediate position	H01H21/60	H01H21/60		35
H01H21/86	8	Switches with abutting contact carried by operating part, e.g. telegraph tapping key	H01H21/86	H01H21/86		96
H01H21/88	9	with intermediate position of rest	H01H21/88	H01H21/88		2
H01H23/00	7	Tumbler or rocker switches, i.e. switches characterised by being operated by rocking an operating member in the form of a rocker button<br><br><u>NOTE</u><br><br><br>In this group, the term "rocking" is defined as pivotal motion in one plane about an axis parallel to the switch faceplate and located substantially centrally between the ends of the rocker button	H01H23/00	H01H23/00		459
H01H23/003	8	{with more than one electrically distinguishable condition in one or both positions}	H01H23/00	H01H23/00		195
H01H23/006	8	{adapted for connection with printed circuit boards}	H01H23/00	H01H23/00		143
H01H23/02	8	Details	H01H23/02	H01H23/02		724
H01H23/025	9	{Light-emitting indicators}	H01H23/02	H01H23/02		633
H01H23/04	9	Cases; Covers	H01H23/04	H01H23/04		791
H01H23/06	10	Dustproof, splashproof, drip-proof, waterproof, or flameproof casings	H01H23/06	H01H23/06		396
H01H23/065	11	{Casings hermetically closed by a diaphragm through which passes an actuating member (vacuum switches H01H33/66)}	H01H23/06	H01H23/06		90
H01H23/08	9	Bases; Stationary contacts mounted thereon	H01H23/08	H01H23/08		423
H01H23/10	9	Adaptation for built-in fuse	H01H23/10	H01H23/10		42
H01H23/105	10	{Fuses mounted on, or constituting the movable part of, the switch}	H01H23/10	H01H23/10		23
H01H23/12	9	Movable parts; Contacts mounted thereon	H01H23/12	H01H23/12		943
H01H23/14	10	Tumblers	H01H23/14	H01H23/14		765
H01H23/141	11	{provided with extensions, e.g. for actuation by a child}	H01H23/14	H01H23/14		200
H01H23/143	11	{having a generally flat elongated shape}	H01H23/14	H01H23/14		305
H01H23/145	12	{the actuating surface having two slightly inclined areas extending from the middle outward}	H01H23/14	H01H23/14		168
H01H23/146	11	{having a generally tubular or conical elongated shape, e.g. dolly}	H01H23/14	H01H23/14		206
H01H23/148	11	{actuated by superimposed sliding element (H01H23/141 takes precedence)}	H01H23/14	H01H23/14		61
H01H23/16	10	Driving mechanisms	H01H23/16	H01H23/16		679
H01H23/162	11	{incorporating links interconnecting tumbler and contact arm}	H01H23/16	H01H23/16		267
H01H23/164	11	{with rectilinearly movable member carrying the contacts}	H01H23/16	H01H23/16		270
H01H23/166	11	{with positive action}	H01H23/16	H01H23/16		61
H01H23/168	11	{using cams}	H01H23/16	H01H23/16		353
H01H23/18	11	incorporating lost motion	H01H23/18	H01H23/18		15
H01H23/20	11	having snap action	H01H23/20	H01H23/20		349
H01H23/205	12	{using a compression spring between tumbler and an articulated contact plate}	H01H23/20	H01H23/20		323
H01H23/22	11	with means for introducing a predetermined time delay	H01H23/22	H01H23/22		21
H01H23/24	8	with two operating positions	H01H23/24	H01H23/24		302
H01H23/26	9	one of which positions is unstable	H01H23/26	H01H23/26		42
H01H23/28	8	with three operating positions	H01H23/28	H01H23/28		172
H01H23/30	9	with stable centre positions and one or both end positions unstable	H01H23/30	H01H23/30		256
H01H25/00	7	Switches with compound movement of handle or other operating part	H01H25/00	H01H25/00		421
H01H25/002	8	{having an operating member rectilinearly slidable in different directions}	H01H25/00	H01H25/00		294
H01H2025/004	9	{the operating member being depressable perpendicular to the other directions}	H01H25/00	H01H25/00		137
H01H25/006	8	{having an operating member slidable in a plane in one direction and pivotable around an axis located in the sliding plane perpendicular to the sliding direction}	H01H25/00	H01H25/00		81
H01H25/008	8	{Operating part movable both angularly and rectilinearly, the rectilinear movement being perpendicular to the axis of angular movement}	H01H25/00	H01H25/00		608
H01H25/04	8	Operating part movable angularly in more than one plane, e.g. joystick	H01H25/04	H01H25/04		964
H01H25/041	9	{having a generally flat operating member depressible at different locations to operate different controls}	H01H25/04	H01H25/04		1087
H01H2025/043	10	{the operating member being rotatable around wobbling axis for additional switching functions}	H01H25/04	H01H25/04		171
H01H2025/045	10	{having a rotating dial around the operating member for additional switching functions}	H01H25/04	H01H25/04		104
H01H2025/046	10	{having a spherical bearing between operating member and housing or bezel}	H01H25/04	H01H25/04		78
H01H2025/048	9	{having a separate central push, slide or tumbler button which is not integral with the operating part that surrounds it}	H01H25/04	H01H25/04		257
H01H25/06	8	Operating part movable both angularly and rectilinearly, the rectilinear movement being along the axis of angular movement	H01H25/06	H01H25/06		1334
H01H25/065	9	{using separate operating parts, e.g. a push button surrounded by a rotating knob}	H01H25/06	H01H25/06		448
H01H27/00	7	Switches operated by a removable member, e.g. key, plug or plate; Switches operated by setting members according to a single predetermined combination out of several possible settings (combined with plug-and-socket connectors H01R13/70; with current-carrying plug H01R31/08)	H01H27/00	H01H27/00		500
H01H27/002	8	{wherein one single insertion movement of a key comprises an unlocking stroke and a switch actuating stroke, e.g. security switch for safety guards}	H01H27/00	H01H27/00		305
H01H2027/005	9	{the key receiving part having multiple openings to allow keys from different directions to operate the switch}	H01H27/00	H01H27/00		75
H01H27/007	9	{the switch being lockable by remote control, e.g. by electromagnet}	H01H27/00	H01H27/00		108
H01H27/04	8	Insulating plug or plate inserted between normally closed contacts	H01H27/04	H01H27/04		93
H01H27/06	8	Key inserted and then turned to effect operation of the switch	H01H27/06	H01H27/06		802
H01H27/063	9	{wherein the switch cannot be moved to a third position, e.g. start position, unless the preceding movement was from a first position to a second position, e.g. ignition position}	H01H27/06	H01H27/06		127
H01H2027/066	9	{having anti-tamper provisions, e.g. avoiding the removal of the lock cylinder}	H01H27/06	H01H27/06		58
H01H27/08	9	wherein the key cannot be removed until the switch is returned to its original position {(H01H27/063 takes precedence)}	H01H27/08	H01H27/08		101
H01H27/10	8	Switch operated by setting members according to a single predetermined combination out of several possible settings	H01H27/10	H01H27/10		249
H01H29/00	7	Switches having at least one liquid contact (solid contacts wetted or soaked with mercury H01H1/08)	H01H29/00	H01H29/00		178
H01H29/002	8	{Inertia switches}	H01H29/00	H01H29/00		134
H01H29/004	8	{Operated by deformation of container}	H01H29/00	H01H29/00		79
H01H29/006	8	{Self interrupters, e.g. with periodic or other repetitive opening and closing of contacts}	H01H29/00	H01H29/00		113
H01H2029/008	8	{using micromechanics, e.g. micromechanical liquid contact switches or [LIMMS]}	H01H29/00	H01H29/00		170
H01H29/02	8	Details	H01H29/02	H01H29/02		57
H01H29/04	9	Contacts; Containers for liquid contacts	H01H29/04	H01H29/04		195
H01H29/06	10	Liquid contacts characterised by the material thereof	H01H29/06	H01H29/06		92
H01H29/08	9	Means for introducing a predetermined time delay	H01H29/08	H01H29/08		30
H01H29/10	10	by constricting the flow of the contact liquid	H01H29/10	H01H29/10		120
H01H29/12	9	Operating mechanisms adapted for operation by a part of the human body other than the hand, e.g. by foot	H01H29/12	H01H29/12		13
H01H29/14	9	Operating mechanisms adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift	H01H29/14	H01H29/14		19
H01H29/16	8	operated by dipping soil contact into stationary contact liquid	H01H29/16	H01H29/16		128
H01H29/18	8	with level of surface of contact liquid displaced by non-electrical contact-making plunger	H01H29/18	H01H29/18		320
H01H29/20	8	operated by tilting contact-liquid container	H01H29/20	H01H29/20		515
H01H29/22	9	wherein contact is made and broken between liquid and solid	H01H29/22	H01H29/22		374
H01H29/24	9	wherein contact is made and broken between liquid and liquid	H01H29/24	H01H29/24		175
H01H29/26	8	with level of surface of contact liquid displaced by centrifugal action	H01H29/26	H01H29/26		129
H01H29/28	8	with level of surface of contact liquid displaced by fluid pressure	H01H29/28	H01H29/28		278
H01H29/30	8	with level of surface of contact liquid displaced by expansion or evaporation thereof	H01H29/30	H01H29/30		118
H01H29/32	8	with contact made by a liquid jet, e.g. earthing switch with contact made by jet of water	H01H29/32	H01H29/32		23
H01H31/00	7	Air-break switches for high tension without arc-extinguishing or arc-preventing means (in combination with high tension or heavy-current switches with arc-extinguishing or arc-preventing means H01H33/00)	H01H31/00	H01H31/00		236
H01H31/003	8	{Earthing switches (H01H31/02&#160;-&#160;H01H31/26 take precedence; contact made by liquid jet H01H29/32; for substations H02B1/16, H02B5/01; for withdrawable switchgear H02B11/28; for gas-insulated switchgear H02B13/075)}	H01H31/00	H01H31/00		1425
H01H31/006	8	{adapted to be operated by a hot stick; Hot sticks therefor}	H01H31/00	H01H31/00		199
H01H31/02	8	Details	H01H31/02	H01H31/02		1720
H01H31/023	9	{Base and stationary contacts mounted thereon}	H01H31/02	H01H31/02		704
H01H31/026	9	{Movable parts and contacts mounted thereon}	H01H31/02	H01H31/02		827
H01H31/04	9	Interlocking mechanisms	H01H31/04	H01H31/04		331
H01H31/06	10	for interlocking between casing, cover, or protective shutter and mechanism for operating contacts	H01H31/06	H01H31/06		276
H01H31/08	10	for interlocking two or more parts of the mechanism for operating contacts	H01H31/08	H01H31/08		183
H01H31/10	10	for interlocking two or more switches	H01H31/10	H01H31/10		353
H01H31/12	9	Adaptation for built-in fuse	H01H31/12	H01H31/12		145
H01H31/122	10	{Fuses mounted on, or constituting the movable contact parts of, the switch}	H01H31/12	H01H31/12		440
H01H31/125	11	{with a pivotally supported fuse, hanging on a fixed contact in the open position of the switch (H01H31/127 takes precedence)}	H01H31/12	H01H31/12		99
H01H31/127	11	{Drop-out fuses}	H01H31/12	H01H31/12		473
H01H31/14	8	with bridging contact that is not electrically connected to either line contact in open position of switch	H01H31/14	H01H31/14		19
H01H31/16	9	with angularly-movable bridging contact or contact-carrying member	H01H31/16	H01H31/16		114
H01H31/18	10	actuated through the movement of one or more insulators	H01H31/18	H01H31/18		27
H01H31/20	11	at least one insulator being rotatable about its own geometrical axis	H01H31/20	H01H31/20		76
H01H31/22	10	wherein the contact or contacts are rectilinearly movable with respect to the carrying member	H01H31/22	H01H31/22		27
H01H31/24	9	with rectilinearly-movable bridging contact	H01H31/24	H01H31/24		89
H01H31/26	8	with movable contact that remains electrically connected to one line in open position of switch	H01H31/26	H01H31/26		93
H01H31/28	9	with angularly-movable contact	H01H31/28	H01H31/28		842
H01H31/283	10	{wherein the contact or contacts are rectilinearly movable with respect to the carrying member}	H01H31/28	H01H31/28		126
H01H2031/286	10	{wherein the contact is rotatable around its own longitudinal axis}	H01H31/28	H01H31/28		130
H01H31/30	10	actuated through the movement of one or more insulators	H01H31/30	H01H31/30		133
H01H31/32	9	with rectilinearly-movable contact	H01H31/32	H01H31/32		463
H01H31/34	8	with movable contact adapted to engage an overhead transmission line, e.g. for branching	H01H31/34	H01H31/34		96
H01H31/36	9	Contact moved by pantograph	H01H31/36	H01H31/36		173
H01H33/00	7	High-tension or heavy-current switches with arc-extinguishing or arc-preventing means	H01H33/00	H01H33/00		270
H01H33/002	8	{Very heavy-current switches (H01H33/02&#160;-&#160;H01H33/98 take precedence)}	H01H33/00	H01H33/00		304
H01H33/004	9	{making use of superconducting contacts (current limitation using superconducting elements H02H9/023; power cryotrons H10N60/355)}	H01H33/00	H01H33/00		41
H01H33/006	8	{adapted for interrupting fault currents with delayed zero crossings}	H01H33/00	H01H33/00		70
H01H33/008	8	{Pedestal mounted switch gear combinations}	H01H33/00	H01H33/00		307
H01H33/02	8	Details	H01H33/02	H01H33/02		1044
H01H33/021	9	{Use of solid insulating compounds resistant to the contacting fluid dielectrics and their decomposition products, e.g. to SF6}	H01H33/02	H01H33/02		219
H01H33/022	9	{particular to three-phase circuit breakers (synchronous switching H01H9/563)}	H01H33/02	H01H33/02		729
H01H2033/024	10	{with a triangular setup of circuit breakers}	H01H33/02	H01H33/02		114
H01H33/025	9	{Terminal arrangements (for vacuum switches H01H33/6606)}	H01H33/02	H01H33/02		379
H01H33/027	9	{Integrated apparatus for measuring current or voltage}	H01H33/02	H01H33/02		325
H01H2033/028	9	{the cooperating contacts being both actuated simultaneously in opposite directions}	H01H33/02	H01H33/02		172
H01H33/04	9	Means for extinguishing or preventing arc between current-carrying parts	H01H33/04	H01H33/04		504
H01H33/045	10	{for arcs formed during closing}	H01H33/04	H01H33/04		103
H01H33/06	10	Insulating body insertable between contacts	H01H33/06	H01H33/06		234
H01H33/08	10	Stationary parts for restricting or subdividing the arc, e.g. barrier plate	H01H33/08	H01H33/08		502
H01H2033/085	11	{using a flat arc chute, the width of arc chamber being only slightly greater then thickness of switch blade}	H01H33/08	H01H33/08		79
H01H33/10	11	Metal parts	H01H33/10	H01H33/10		128
H01H33/12	10	Auxiliary contacts on to which the arc is transferred from the main contacts (using arcing horns H01H33/20)	H01H33/12	H01H33/12		686
H01H33/121	11	{Load break switches}	H01H33/12	H01H33/12		494
H01H33/122	12	{both breaker and sectionaliser being enclosed, e.g. in SF6-filled container}	H01H33/12	H01H33/12		235
H01H33/123	12	{in which the auxiliary contact pivots on the main contact-arm and performs a delayed and accelerated movement}	H01H33/12	H01H33/12		103
H01H33/124	13	{the auxiliary contact being a whip contact}	H01H33/12	H01H33/12		66
H01H33/125	12	{comprising a separate circuit breaker (H01H33/122 takes precedence)}	H01H33/12	H01H33/12		134
H01H33/126	13	{being operated by the distal end of a sectionalising contact arm}	H01H33/12	H01H33/12		137
H01H33/127	13	{movable with a sectionalising contact arm and operated by such movement}	H01H33/12	H01H33/12		122
H01H33/128	13	{being operated by a separate mechanism interlocked with the sectionalising mechanism}	H01H33/12	H01H33/12		145
H01H33/14	10	Multiple main contacts for the purpose of dividing the current through, or potential drop along, the arc	H01H33/14	H01H33/14		705
H01H33/143	11	{of different construction or type}	H01H33/14	H01H33/14		101
H01H2033/146	11	{using capacitors, e.g. for the voltage division over the different switches}	H01H33/14	H01H33/14		97
H01H33/16	10	Impedances connected with contacts	H01H33/16	H01H33/16		541
H01H33/161	11	{Variable impedances}	H01H33/16	H01H33/16		200
H01H33/162	12	{Liquid resistors}	H01H33/16	H01H33/16		79
H01H2033/163	12	{using PTC elements}	H01H33/16	H01H33/16		71
H01H33/164	11	{the impedance being inserted in the circuit by blowing the arc onto an auxiliary electrode}	H01H33/16	H01H33/16		107
H01H33/165	11	{Details concerning the impedances (H01H33/161 takes precedence)}	H01H33/16	H01H33/16		96
H01H33/166	11	{the impedance being inserted only while closing the switch}	H01H33/16	H01H33/16		142
H01H33/167	11	{the impedance being inserted only while opening the switch}	H01H33/16	H01H33/16		109
H01H33/168	11	{the impedance being inserted both while closing and while opening the switch}	H01H33/16	H01H33/16		64
H01H33/18	10	using blow-out magnet {(for vacuum switches H01H33/664)}	H01H33/18	H01H33/18		370
H01H33/182	11	{using permanent magnets (H01H33/187 takes precedence)}	H01H33/18	H01H33/18		183
H01H33/185	11	{using magnetisable elements associated with the contacts (H01H33/187 takes precedence)}	H01H33/18	H01H33/18		88
H01H33/187	11	{comprising a hollow annular arc runner and a central contact between which a radially drawn arc rotates}	H01H33/18	H01H33/18		58
H01H33/20	10	using arcing horns (using blow-out magnet H01H33/18)	H01H33/20	H01H33/20		72
H01H33/22	10	Selection of fluids for arc-extinguishing	H01H33/22	H01H33/22		434
H01H33/24	9	Means for preventing discharge to non-current-carrying parts, e.g. using corona ring	H01H33/24	H01H33/24		535
H01H33/245	10	{using movable field electrodes}	H01H33/24	H01H33/24		75
H01H33/26	9	Means for detecting the presence of an arc or other discharge	H01H33/26	H01H33/26		176
H01H33/28	9	Power arrangements internal to the switch for operating the driving mechanism	H01H33/28	H01H33/28		214
H01H33/285	10	{using electro-dynamic repulsion (assisting the movement of pistons by accelerating coil H01H33/882)}	H01H33/28	H01H33/28		179
H01H33/30	10	using fluid actuator	H01H33/30	H01H33/30		223
H01H33/302	11	{for fluid insulated switchgear, wherein the insulating fluid is also the working fluid}	H01H33/30	H01H33/30		62
H01H33/304	11	{Working fluid supplies}	H01H33/30	H01H33/30		45
H01H2033/306	11	{monitoring the pressure of the working fluid, e.g. for protection measures}	H01H33/30	H01H33/30		54
H01H2033/308	11	{comprising control and pilot valves}	H01H33/30	H01H33/30		81
H01H33/32	11	pneumatic	H01H33/32	H01H33/32		912
H01H33/34	11	hydraulic	H01H33/34	H01H33/34		492
H01H33/36	10	using dynamo-electric motor	H01H33/36	H01H33/36		264
H01H33/38	10	using electromagnet	H01H33/38	H01H33/38		407
H01H33/40	10	using spring motor	H01H33/40	H01H33/40		291
H01H33/42	9	Driving mechanisms	H01H33/42	H01H33/42		1634
H01H33/423	10	{making use of an electromagnetic wave communication}	H01H33/42	H01H33/42		82
H01H2033/426	10	{Details concerning the connection of the isolating driving rod to a metallic part}	H01H33/42	H01H33/42		107
H01H33/44	9	Devices for ensuring operation of the switch at a predetermined point in the AC cycle (circuit arrangements&#160;H01H33/59)	H01H33/44	H01H33/44		140
H01H33/46	9	Interlocking mechanisms	H01H33/46	H01H33/46		191
H01H33/48	10	for interlocking between casing or cover and mechanism for operating contacts	H01H33/48	H01H33/48		120
H01H33/50	10	for interlocking two or more parts of the mechanism for operating contacts	H01H33/50	H01H33/50		95
H01H33/52	10	for interlocking two or more switches	H01H33/52	H01H33/52		293
H01H33/53	9	Cases (for switchgear H02B1/26); Reservoirs, tanks, piping or valves, for arc-extinguishing fluid; Accessories therefor, e.g. safety arrangements, pressure relief devices	H01H33/53	H01H33/53		692
H01H33/55	10	Oil reservoirs or tanks; Lowering means therefor (associated with withdrawal mechanism for isolation of switch H02B11/08)	H01H33/55	H01H33/55		523
H01H33/555	11	{Protective arrangements responsive to abnormal fluid pressure, liquid level or liquid displacement, e.g. Buchholz relays (circuits H02H5/08; specially adapted for transformers H01F27/402)}	H01H33/55	H01H33/55		258
H01H33/56	10	Gas reservoirs	H01H33/56	H01H33/56		935
H01H33/561	11	{composed of different independent pressurised compartments put in communication only after their assemblage}	H01H33/56	H01H33/56		44
H01H33/562	11	{Means for avoiding liquefaction or for disposing of liquefaction products}	H01H33/56	H01H33/56		122
H01H33/563	11	{comprising means for monitoring the density of the insulating gas}	H01H33/56	H01H33/56		192
H01H33/565	11	{Gas-tight sealings for moving parts penetrating into the reservoir}	H01H33/56	H01H33/56		121
H01H2033/566	11	{Avoiding the use of SF6}	H01H33/56	H01H33/56		225
H01H2033/567	11	{Detection of decomposition products of the gas}	H01H33/56	H01H33/56		34
H01H2033/568	11	{with overpressure release, e.g. rupture membranes}	H01H33/56	H01H33/56		177
H01H33/57	10	Recuperation of liquid or gas	H01H33/57	H01H33/57		217
H01H33/58	10	Silencers for suppressing noise of switch operation	H01H33/58	H01H33/58		90
H01H33/59	9	Circuit arrangements not adapted to a particular application of the switch and not otherwise provided for, e.g. for ensuring operation of the switch at a predetermined point in the AC cycle	H01H33/59	H01H33/59		393
H01H33/593	10	{for ensuring operation of the switch at a predetermined point of the AC cycle (for multipolar switches&#160;H01H9/563)}	H01H33/59	H01H33/59		201
H01H33/596	10	{for interrupting DC}	H01H33/59	H01H33/59		906
H01H33/60	8	Switches wherein the means for extinguishing or preventing the arc do not include separate means for obtaining or increasing flow of arc-extinguishing fluid	H01H33/60	H01H33/60		54
H01H33/64	9	wherein the break is in gas (vacuum switches H01H33/66)	H01H33/64	H01H33/64		218
H01H33/65	10	wherein the break is in air at atmospheric pressure, e.g. in open air	H01H33/65	H01H33/65		23
H01H33/66	9	Vacuum switches	H01H33/66	H01H33/66		1895
H01H33/6606	10	{Terminal arrangements}	H01H33/66	H01H33/66		658
H01H2033/6613	11	{Cooling arrangements directly associated with the terminal arrangements}	H01H33/66	H01H33/66		163
H01H33/662	10	Housings or protective screens	H01H33/662	H01H33/662		845
H01H33/66207	11	{Specific housing details, e.g. sealing, soldering or brazing}	H01H33/662	H01H33/662		1197
H01H2033/66215	12	{Details relating to the soldering or brazing of vacuum switch housings}	H01H33/662	H01H33/662		203
H01H2033/66223	12	{Details relating to the sealing of vacuum switch housings}	H01H33/662	H01H33/662		395
H01H2033/6623	12	{Details relating to the encasing or the outside layers of the vacuum switch housings}	H01H33/662	H01H33/662		438
H01H33/66238	11	{Specific bellows details}	H01H33/662	H01H33/662		329
H01H2033/66246	12	{Details relating to the guiding of the contact rod in vacuum switch belows}	H01H33/662	H01H33/662		189
H01H2033/66253	12	{Details relating to the prevention of unwanted rotation of the contact rod in vacuum switch bellows}	H01H33/662	H01H33/662		61
H01H33/66261	11	{Specific screen details, e.g. mounting, materials, multiple screens or specific electrical field considerations}	H01H33/662	H01H33/662		630
H01H2033/66269	12	{Details relating to the materials used for screens in vacuum switches}	H01H33/662	H01H33/662		143
H01H2033/66276	12	{Details relating to the mounting of screens in vacuum switches}	H01H33/662	H01H33/662		288
H01H2033/66284	12	{Details relating to the electrical field properties of screens in vacuum switches}	H01H33/662	H01H33/662		142
H01H2033/66292	12	{Details relating to the use of multiple screens in vacuum switches}	H01H33/662	H01H33/662		189
H01H33/664	10	Contacts; Arc-extinguishing means, e.g. arcing rings	H01H33/664	H01H33/664		2072
H01H33/6641	11	{making use of a separate coil}	H01H33/664	H01H33/664		112
H01H33/6642	11	{having cup-shaped contacts, the cylindrical wall of which being provided with inclined slits to form a coil}	H01H33/664	H01H33/664		265
H01H33/6643	11	{having disc-shaped contacts subdivided in petal-like segments, e.g. by helical grooves}	H01H33/664	H01H33/664		252
H01H33/6644	11	{having coil-like electrical connections between contact rod and the proper contact}	H01H33/664	H01H33/664		190
H01H33/6645	12	{in which the coil like electrical connections encircle at least once the contact rod}	H01H33/664	H01H33/664		67
H01H33/6646	11	{having non flat disc-like contact surface}	H01H33/664	H01H33/664		208
H01H33/6647	11	{having fixed middle contact and two movable contacts}	H01H33/664	H01H33/664		58
H01H2033/6648	11	{Contacts containing flexible parts, e.g. to improve contact pressure}	H01H33/664	H01H33/664		68
H01H33/666	10	Operating arrangements	H01H33/666	H01H33/666		2888
H01H33/6661	11	{Combination with other type of switch, e.g. for load break switches (H01H33/143, H01H33/6662 take precedence)}	H01H33/666	H01H33/666		706
H01H33/6662	11	{using bistable electromagnetic actuators, e.g. linear polarised electromagnetic actuators}	H01H33/666	H01H33/666		343
H01H33/6664	11	{with pivoting movable contact structure}	H01H33/666	H01H33/666		174
H01H2033/6665	11	{Details concerning the mounting or supporting of the individual vacuum bottles}	H01H33/666	H01H33/666		201
H01H2033/6667	11	{Details concerning lever type driving rod arrangements}	H01H33/666	H01H33/666		310
H01H2033/6668	11	{with a plurality of interruptible circuit paths in single vacuum chamber}	H01H33/666	H01H33/666		99
H01H33/668	10	Means for obtaining or monitoring the vacuum	H01H33/668	H01H33/668		401
H01H33/6683	11	{by gettering}	H01H33/668	H01H33/668		83
H01H2033/6686	11	{by emitting and receiving reflected sound or ultrasound signals}	H01H33/668	H01H33/668		14
H01H33/68	9	Liquid-break switches, e.g. oil-break	H01H33/68	H01H33/68		140
H01H33/70	8	Switches with separate means for directing, obtaining, or increasing flow of arc-extinguishing fluid	H01H33/70	H01H33/70		405
H01H33/7007	9	{wherein the flow is a function of the current being interrupted}	H01H33/70	H01H33/70		135
H01H33/7015	9	{characterised by flow directing elements associated with contacts (electrical or mechanical properties of the contact system H01H1/385)}	H01H33/70	H01H33/70		245
H01H33/7023	10	{characterised by an insulating tubular gas flow enhancing nozzle (H01H33/7038 takes precedence)}	H01H33/70	H01H33/70		385
H01H33/703	11	{having special gas flow directing elements, e.g. grooves, extensions}	H01H33/70	H01H33/70		153
H01H33/7038	10	{characterised by a conducting tubular gas flow enhancing nozzle}	H01H33/70	H01H33/70		146
H01H33/7046	11	{having special gas flow directing elements, e.g. grooves, extensions (H01H33/7053 takes precedence)}	H01H33/70	H01H33/70		80
H01H33/7053	11	{having a bridging element around two hollow tubular contacts}	H01H33/70	H01H33/70		69
H01H33/7061	10	{characterised by use of special mounting means (H01H33/7023&#160;-&#160;H01H33/7038 take precedence)}	H01H33/70	H01H33/70		60
H01H33/7069	10	{characterised by special dielectric or insulating properties or by special electric or magnetic field control properties (H01H33/7023&#160;-&#160;H01H33/7061 take precedence)}	H01H33/70	H01H33/70		87
H01H33/7076	10	{characterised by the use of special materials (H01H33/7023&#160;-&#160;H01H33/7069 take precedence)}	H01H33/70	H01H33/70		113
H01H33/7084	10	{characterised by movable parts influencing the gas flow (H01H33/7023&#160;-&#160;H01H33/7076 take precedence)}	H01H33/70	H01H33/70		58
H01H33/7092	10	{characterised by several arcing chambers in series (H01H33/7023&#160;-&#160;H01H33/7084 take precedence)}	H01H33/70	H01H33/70		38
H01H33/72	9	having stationary parts for directing the flow of arc-extinguishing fluid, e.g. arc-extinguishing chamber	H01H33/72	H01H33/72		222
H01H33/73	10	wherein the break is in air at atmospheric pressure, e.g. in open air	H01H33/73	H01H33/73		38
H01H33/74	10	wherein the break is in gas (in air at atmospheric pressure H01H33/73)	H01H33/74	H01H33/74		209
H01H33/75	10	Liquid-break switches, e.g. oil-break	H01H33/75	H01H33/75		719
H01H33/76	9	wherein arc-extinguishing gas is evolved from stationary parts; Selection of material therefor	H01H33/76	H01H33/76		486
H01H33/765	10	{the gas-evolving material being incorporated in the contact material}	H01H33/76	H01H33/76		44
H01H33/77	10	wherein the break is in air at atmospheric pressure	H01H33/77	H01H33/77		140
H01H33/78	10	wherein the break is in gas (in air at atmospheric pressure H01H33/77)	H01H33/78	H01H33/78		53
H01H33/80	9	flow of arc-extinguishing fluid from a pressure source being controlled by a valve	H01H33/80	H01H33/80		42
H01H33/82	10	the fluid being air or gas	H01H33/82	H01H33/82		280
H01H33/83	11	wherein the contacts are opened by the flow of air or gas	H01H33/83	H01H33/83		165
H01H33/84	10	the fluid being liquid, e.g. oil	H01H33/84	H01H33/84		14
H01H33/85	11	wherein the contacts are opened by the flow of liquid	H01H33/85	H01H33/85		6
H01H33/86	9	the flow of arc-extinguishing fluid under pressure from the contact space being controlled by a valve	H01H33/86	H01H33/86		180
H01H33/88	9	the flow of arc-extinguishing fluid being produced or increased by movement of pistons or other pressure-producing parts	H01H33/88	H01H33/88		132
H01H33/882	10	{the movement being assisted by accelerating coils}	H01H33/88	H01H33/88		48
H01H33/884	10	{with variable-area piston}	H01H33/88	H01H33/88		14
H01H33/886	10	{by movement of rotating pistons}	H01H33/88	H01H33/88		44
H01H2033/888	10	{Deflection of hot gasses and arcing products}	H01H33/88	H01H33/88		210
H01H33/90	10	this movement being effected by or in conjunction with the contact-operating mechanism	H01H33/90	H01H33/90		109
H01H33/901	11	{making use of the energy of the arc or an auxiliary arc}	H01H33/90	H01H33/90		223
H01H2033/902	12	{with the gases from hot space and compression volume following different paths to arc space or nozzle, i.e. the compressed gases do not pass through hot volume}	H01H33/90	H01H33/90		27
H01H33/903	12	{and assisting the operating mechanism}	H01H33/90	H01H33/90		72
H01H33/904	11	{characterised by the transmission between operating mechanism and piston or movable contact}	H01H33/90	H01H33/90		169
H01H33/905	11	{the compression volume being formed by a movable cylinder and a semi-mobile piston}	H01H33/90	H01H33/90		105
H01H2033/906	11	{with pressure limitation in the compression volume, e.g. by valves or bleeder openings}	H01H33/90	H01H33/90		81
H01H2033/907	11	{using tandem pistons, e.g. several compression volumes being modified in conjunction or sequential}	H01H33/90	H01H33/90		37
H01H2033/908	11	{using valves for regulating communication between, e.g. arc space, hot volume, compression volume, surrounding volume}	H01H33/90	H01H33/90		144
H01H33/91	11	the arc-extinguishing fluid being air or gas	H01H33/91	H01H33/91		940
H01H2033/912	12	{Liquified gases, e.g. liquified SF6}	H01H33/91	H01H33/91		48
H01H33/92	11	the arc-extinguishing fluid being liquid, e.g. oil	H01H33/92	H01H33/92		288
H01H33/94	10	this movement being effected solely due to the pressure caused by the arc itself or by an auxiliary arc {(H01H33/903 takes precedence)}	H01H33/94	H01H33/94		12
H01H33/95	11	the arc-extinguishing fluid being air or gas	H01H33/95	H01H33/95		23
H01H33/96	11	the arc-extinguishing fluid being liquid, e.g. oil	H01H33/96	H01H33/96		182
H01H33/98	9	the flow of arc-extinguishing fluid being initiated by an auxiliary arc or a section of the arc, without any moving parts for producing or increasing the flow {(H01H33/901 takes precedence)}	H01H33/98	H01H33/98		334
H01H33/982	10	{in which the pressure-generating arc is rotated by a magnetic field}	H01H33/98	H01H33/98		86
H01H35/00	7	Switches operated by change of a physical condition (operated by change of magnetic or electric field H01H36/00; thermally-actuated switches H01H37/00)<br><br><u>NOTE</u><br><br>A switching device is classified according to that physical condition which, when changed, acts as input to the device, e.g. external explosion causing pressure wave to act upon switch is classified in group H01H35/24, an explosion produced within the switch in group H01H37/00 if initiated by heat, in group H01H39/00 if initiated electrically, and in group H01H35/14 if initiated by an external blow.	H01H35/00	H01H35/00		748
H01H35/003	8	{Switches operated by other part of human body than hands (push-button switches H01H13/16; slide switches H01H15/20; cord switches H01H17/10; other switches H01H19/16 and H01H21/26)}	H01H35/00	H01H35/00		120
H01H35/006	8	{Switches operated by mechanical overload condition, e.g. transmitted force or torque becoming too high}	H01H35/00	H01H35/00		150
H01H35/02	8	Switches operated by change of position, inclination or orientation of the switch itself in relation to gravitational field (tilting mercury container H01H29/20; change of position due to change of liquid level H01H35/18)	H01H35/02	H01H35/02		658
H01H35/022	9	{the switch being of the reed switch type}	H01H35/02	H01H35/02		69
H01H35/025	9	{the switch being discriminative in different directions}	H01H35/02	H01H35/02		88
H01H35/027	9	{the inertia mass activating the switch mechanically, e.g. through a lever}	H01H35/02	H01H35/02		174
H01H35/06	8	Switches operated by change of speed (operated by change of fluid flow H01H35/24)	H01H35/06	H01H35/06		138
H01H35/10	9	Centrifugal switches (level of mercury displaced by centrifugal action H01H29/26)	H01H35/10	H01H35/10		1227
H01H35/12	9	operated by reversal of direction of movement	H01H35/12	H01H35/12		136
H01H35/14	8	Switches operated by change of acceleration, e.g. by shock or vibration, inertia switch {(wherein the liquid constitutes a contact of the switch H01H29/002)}	H01H35/14	H01H35/14		1416
H01H35/141	9	{Details}	H01H35/14	H01H35/14		113
H01H35/142	10	{Damping means to avoid unwanted response}	H01H35/14	H01H35/14		124
H01H35/143	10	{Resetting means}	H01H35/14	H01H35/14		88
H01H35/144	9	{operated by vibration}	H01H35/14	H01H35/14		333
H01H35/145	9	{operated by a particular acceleration-time function}	H01H35/14	H01H35/14		66
H01H35/146	9	{operated by plastic deformation or rupture of structurally associated elements}	H01H35/14	H01H35/14		103
H01H35/147	9	{the switch being of the reed switch type}	H01H35/14	H01H35/14		217
H01H35/148	9	{making use of a rolamite sensor}	H01H35/14	H01H35/14		29
H01H35/18	8	Switches operated by change of liquid level or of liquid density, e.g. float switch (by magnet carried on a float H01H36/02)	H01H35/18	H01H35/18		988
H01H35/183	9	{making use of a thermal switch}	H01H35/18	H01H35/18		45
H01H35/186	9	{making use of a cable suspended floater containing an inclination sensing switch}	H01H35/18	H01H35/18		183
H01H35/24	8	Switches operated by change of fluid pressure, by fluid pressure waves, or by change of fluid flow (wherein the change of pressure is caused by change of temperature H01H37/36)	H01H35/24	H01H35/24		878
H01H35/242	9	{operated by one particular pressure-time function}	H01H35/24	H01H35/24		47
H01H35/245	9	{actuated by the deformation of a body of elastic material}	H01H35/24	H01H35/24		98
H01H35/247	9	{the switch being of the reed switch type}	H01H35/24	H01H35/24		80
H01H35/26	9	Details	H01H35/26	H01H35/26		555
H01H35/2607	10	{Means for adjustment of "ON" or "OFF" operating pressure (means for adjustment of "ON" or "OFF" operating temperature of thermally actuated switches by varying bias on the thermal element due to a separate spring H01H37/18)}	H01H35/26	H01H35/26		326
H01H35/2614	11	{by varying the bias on the pressure sensitive element}	H01H35/26	H01H35/26		433
H01H35/2621	12	{the bias being magnetic}	H01H35/26	H01H35/26		48
H01H35/2628	11	{by varying the relative position of switch-casing and pressure sensitive element}	H01H35/26	H01H35/26		86
H01H35/2635	11	{by adjustment of a motion transmitting system}	H01H35/26	H01H35/26		254
H01H35/2642	12	{comprising a lost-motion connection}	H01H35/26	H01H35/26		23
H01H35/265	11	{by adjustment of one of the co-operating contacts}	H01H35/26	H01H35/26		62
H01H35/2657	10	{with different switches operated at substantially different pressures}	H01H35/26	H01H35/26		259
H01H35/2664	11	{making use of a balance plate pivoting about different axes}	H01H35/26	H01H35/26		26
H01H35/2671	10	{Means to detect leaks in the pressure sensitive element}	H01H35/26	H01H35/26		91
H01H35/2678	10	{Means to isolate oscillating component of pressure}	H01H35/26	H01H35/26		24
H01H35/2685	10	{Means to protect pressure sensitive element against over pressure}	H01H35/26	H01H35/26		39
H01H35/2692	10	{comprising pneumatic snap-action}	H01H35/26	H01H35/26		20
H01H35/28	10	Compensation for variation of ambient pressure or temperature	H01H35/28	H01H35/28		169
H01H35/30	10	Means for transmitting pressure to pressure-responsive operating part, e.g. by capsule and capillary tube	H01H35/30	H01H35/30		123
H01H35/32	9	actuated by bellows	H01H35/32	H01H35/32		367
H01H35/34	9	actuated by diaphragm	H01H35/34	H01H35/34		1459
H01H35/343	10	{by snap acting diaphragm}	H01H35/34	H01H35/34		104
H01H35/346	10	{in which the movable contact is formed or directly supported by the diaphragm}	H01H35/34	H01H35/34		197
H01H35/36	9	actuated by curled flexible tube, e.g. Bourdon tube	H01H35/36	H01H35/36		142
H01H35/38	9	actuated by piston and cylinder	H01H35/38	H01H35/38		632
H01H35/40	9	actuated by devices allowing continual flow of fluid, e.g. vane	H01H35/40	H01H35/40		452
H01H35/405	10	{the switch being of the reed switch type}	H01H35/40	H01H35/40		161
H01H35/42	8	Switches operated by change of humidity	H01H35/42	H01H35/42		268
H01H36/00	7	Switches actuated by change of magnetic field or of electric field, e.g. by change of relative position of magnet and switch, by shielding	H01H36/00	H01H36/00		1542
H01H36/0006	8	{Permanent magnet actuating reed switches (H01H35/147 takes precedence)}	H01H36/00	H01H36/00		637
H01H36/0013	9	{characterised by the co-operation between reed switch and permanent magnet; Magnetic circuits}	H01H36/00	H01H36/00		225
H01H36/002	10	{Actuation by moving ferromagnetic material, switch and magnet being fixed}	H01H36/00	H01H36/00		131
H01H36/0026	10	{comprising a biasing, helping or polarising magnet}	H01H36/00	H01H36/00		90
H01H36/0033	9	{Mountings; Housings; Connections}	H01H36/00	H01H36/00		309
H01H36/004	9	{push-button-operated, e.g. for keyboards}	H01H36/00	H01H36/00		238
H01H36/0046	9	{Limit switches, also fail-safe operation or anti-tamper considerations}	H01H36/00	H01H36/00		350
H01H36/0053	9	{periodically operated}	H01H36/00	H01H36/00		60
H01H36/006	9	{comprising a plurality of reed switches, e.g. selectors or joystick-operated}	H01H36/00	H01H36/00		198
H01H36/0066	9	{magnet being removable, e.g. part of key pencil}	H01H36/00	H01H36/00		99
H01H36/0073	8	{actuated by relative movement between two magnets}	H01H36/00	H01H36/00		574
H01H36/008	8	{Change of magnetic field wherein the magnet and switch are fixed, e.g. by shielding or relative movements of armature (for reed switches H01H36/002)}	H01H36/00	H01H36/00		282
H01H2036/0086	8	{Movable or fixed contacts formed by permanent magnets}	H01H36/00	H01H36/00		77
H01H2036/0093	8	{Micromechanical switches actuated by a change of the magnetic field}	H01H36/00	H01H36/00		90
H01H36/02	8	actuated by movement of a float carrying a magnet	H01H36/02	H01H36/02		720
H01H37/00	7	Thermally-actuated switches	H01H37/00	H01H37/00		286
H01H37/002	8	{combined with protective means}	H01H37/00	H01H37/00		423
H01H37/004	8	{with thermal image}	H01H37/00	H01H37/00		115
H01H37/006	8	{with different switches operated at substantially different temperatures}	H01H37/00	H01H37/00		70
H01H2037/008	8	{Micromechanical switches operated thermally}	H01H37/00	H01H37/00		80
H01H37/02	8	Details	H01H37/02	H01H37/02		313
H01H37/04	9	Bases; Housings; Mountings {(H01H37/5427 takes precedence)}	H01H37/04	H01H37/04		775
H01H37/043	10	{Mountings on controlled apparatus}	H01H37/04	H01H37/04		272
H01H2037/046	10	{being soldered on the printed circuit to be protected}	H01H37/04	H01H37/04		102
H01H37/06	10	to facilitate replacement, e.g. cartridge housing	H01H37/06	H01H37/06		46
H01H37/08	9	Indicators; Distinguishing marks	H01H37/08	H01H37/08		145
H01H37/10	9	Compensation for variation of ambient temperature or pressure	H01H37/10	H01H37/10		228
H01H37/12	9	Means for adjustment of "on" or "off" operating temperature	H01H37/12	H01H37/12		531
H01H37/14	10	by anticipatory electric heater	H01H37/14	H01H37/14		232
H01H37/16	10	by varying the proportion of input heat received by the thermal element, e.g. by displacement of a shield	H01H37/16	H01H37/16		37
H01H37/18	10	by varying bias on the thermal element due to a separate spring	H01H37/18	H01H37/18		86
H01H37/20	10	by varying the position of the thermal element in relation to switch base or casing	H01H37/20	H01H37/20		115
H01H37/22	10	by adjustment of a member transmitting motion from the thermal element to contacts or latch	H01H37/22	H01H37/22		155
H01H37/24	10	by adjustment of position of the movable contact on its driving member	H01H37/24	H01H37/24		16
H01H37/26	10	by adjustment of abutment for "off" position of the movable contact	H01H37/26	H01H37/26		39
H01H37/28	10	by adjustment of the position of the fixed contact	H01H37/28	H01H37/28		150
H01H37/30	10	by varying the position of the contact unit in relation to switch base or casing	H01H37/30	H01H37/30		53
H01H37/32	9	Thermally-sensitive members	H01H37/32	H01H37/32		325
H01H37/323	10	{making use of shape memory materials (in thermal relays H01H61/0107; release mechanism H01H71/145; treatment of SMF alloys C22F1/006; for control of temperature G05D23/024)}	H01H37/32	H01H37/32		272
H01H2037/326	10	{with radiative heat transfer to the switch, e.g. special absorption surfaces}	H01H37/32	H01H37/32		51
H01H37/34	10	Means for transmitting heat thereto, e.g. capsule remote from contact member	H01H37/34	H01H37/34		182
H01H37/36	10	actuated due to expansion or contraction of a fluid with or without vaporisation (the fluid forming a contact of the switch H01H29/04, H01H29/30)	H01H37/36	H01H37/36		597
H01H37/38	11	with bellows	H01H37/38	H01H37/38		66
H01H37/40	11	with diaphragm	H01H37/40	H01H37/40		92
H01H37/42	11	with curled flexible tube, e.g. Bourdon tube	H01H37/42	H01H37/42		11
H01H37/44	11	with piston and cylinder	H01H37/44	H01H37/44		34
H01H37/46	10	actuated due to expansion or contraction of a solid (deflection of a bimetallic element H01H37/52)	H01H37/46	H01H37/46		387
H01H37/48	11	with extensible rigid rods or tubes	H01H37/48	H01H37/48		517
H01H37/50	11	with extensible wires under tension	H01H37/50	H01H37/50		164
H01H37/52	10	actuated due to deflection of bimetallic element	H01H37/52	H01H37/52		1329
H01H37/521	11	{comprising a plurality of bimetals acting in the same direction}	H01H37/52	H01H37/52		72
H01H2037/523	11	{using a corrugated bimetal}	H01H37/52	H01H37/52		35
H01H2037/525	11	{Details of manufacturing of the bimetals, e.g. connection to non bimetallic elements or insulating coatings}	H01H37/52	H01H37/52		98
H01H2037/526	11	{Materials for bimetals}	H01H37/52	H01H37/52		150
H01H2037/528	11	{the bimetallic element being composed of more than two layers}	H01H37/52	H01H37/52		56
H01H37/54	11	wherein the bimetallic element is inherently snap acting	H01H37/54	H01H37/54		1008
H01H37/5409	12	{Bistable switches; Resetting means}	H01H37/54	H01H37/54		178
H01H37/5418	12	{using cantilevered bimetallic snap elements}	H01H37/54	H01H37/54		295
H01H37/5427	12	{encapsulated in sealed miniaturised housing}	H01H37/54	H01H37/54		397
H01H37/5436	13	{mounted on controlled apparatus}	H01H37/54	H01H37/54		134
H01H2037/5445	12	{with measures for avoiding slow break of contacts during the creep phase of the snap bimetal}	H01H37/54	H01H37/54		76
H01H2037/5454	12	{with separate spring biasing the bimetal snap element against the heat transfer surface}	H01H37/54	H01H37/54		24
H01H2037/5463	12	{the bimetallic snap element forming part of switched circuit}	H01H37/54	H01H37/54		266
H01H2037/5472	12	{having an omega form, e.g. the bimetallic snap element having a ring shape with a central tongue}	H01H37/54	H01H37/54		58
H01H2037/5481	12	{the bimetallic snap element being mounted on the contact spring}	H01H37/54	H01H37/54		89
H01H2037/549	12	{Details of movement transmission between bimetallic snap element and contact}	H01H37/54	H01H37/54		86
H01H37/56	11	having spirally wound or helically wound bimetallic element	H01H37/56	H01H37/56		342
H01H37/58	10	actuated due to thermally controlled change of magnetic permeability	H01H37/58	H01H37/58		201
H01H37/585	11	{the switch being of the reed switch type}	H01H37/58	H01H37/58		74
H01H37/60	9	Means for producing snap action (inherent in bimetallic element H01H37/54; caused by a magnet H01H37/66)	H01H37/60	H01H37/60		615
H01H37/62	9	Means other than thermal means for introducing a predetermined time delay	H01H37/62	H01H37/62		23
H01H37/64	9	Contacts	H01H37/64	H01H37/64		248
H01H37/66	10	Magnetic reinforcement of contact pressure; Magnet causing snap action	H01H37/66	H01H37/66		336
H01H37/68	10	sealed in evacuated or gas-filled tube	H01H37/68	H01H37/68		121
H01H37/70	10	Resetting means {(H01H37/5409 takes precedence)}	H01H37/70	H01H37/70		169
H01H2037/705	11	{wherein the switch cannot be closed when the temperature is above a certain value}	H01H37/70	H01H37/70		60
H01H37/72	8	Switches in which the opening movement and the closing movement of a contact are effected respectively by heating and cooling or vice versa	H01H37/72	H01H37/72		65
H01H37/74	8	Switches in which only the opening movement or only the closing movement of a contact is effected by heating or cooling	H01H37/74	H01H37/74		109
H01H37/76	9	Contact member actuated by melting of fusible material, actuated due to burning of combustible material or due to explosion of explosive material	H01H37/76	H01H37/76		915
H01H37/761	10	{with a fusible element forming part of the switched circuit (H01H37/767 takes precedence)}	H01H37/76	H01H37/76		883
H01H2037/762	11	{using a spring for opening the circuit when the fusible element melts}	H01H37/76	H01H37/76		239
H01H2037/763	12	{the spring being a blade spring}	H01H37/76	H01H37/76		174
H01H37/764	10	{in which contacts are held closed by a thermal pellet}	H01H37/76	H01H37/76		111
H01H37/765	11	{using a sliding contact between a metallic cylindrical housing and a central electrode}	H01H37/76	H01H37/76		187
H01H37/766	11	{using a bridging contact}	H01H37/76	H01H37/76		30
H01H37/767	10	{Normally open}	H01H37/76	H01H37/76		189
H01H2037/768	10	{characterised by the composition of the fusible material}	H01H37/76	H01H37/76		258
H01H2037/769	10	{characterised by the composition of insulating fusible materials, e.g. for use in the thermal pellets}	H01H37/76	H01H37/76		42
H01H39/00	7	Switching devices actuated by an explosion produced within the device and initiated by an electric current	H01H39/00	H01H39/00		584
H01H39/002	8	{provided with a cartridge-magazine}	H01H39/00	H01H39/00		57
H01H39/004	8	{Closing switches}	H01H39/00	H01H39/00		244
H01H39/006	8	{Opening by severing a conductor}	H01H39/00	H01H39/00		579
H01H2039/008	8	{using the switch for a battery cutoff}	H01H39/00	H01H39/00		421
H01H41/00	7	Switches providing a selected number of consecutive operations of the contacts by a single manual actuation of the operating part	H01H41/00	H01H41/00		476
H01H41/04	8	Switches without means for setting or mechanically storing a multidigit number	H01H41/04	H01H41/04		4
H01H41/06	9	dial or slide operated	H01H41/06	H01H41/06		3
H01H41/08	9	keyboard operated	H01H41/08	H01H41/08		8
H01H41/10	8	Switches with means for setting or mechanically storing a multidigit number	H01H41/10	H01H41/10		
H01H41/12	9	dial or slide operated	H01H41/12	H01H41/12		2
H01H41/14	9	keyboard operated	H01H41/14	H01H41/14		2
H01H43/00	7	Time or time-programme switches providing a choice of time-intervals for executing one or more switching actions and automatically terminating their operation after the programme is completed	H01H43/00	H01H43/00		815
H01H43/005	8	{with timing of the actuation of contacts due to a part rotating at variable speed}	H01H43/00	H01H43/00		28
H01H43/02	8	Details	H01H43/02	H01H43/02		292
H01H43/022	9	{Bases; Housings; Mountings}	H01H43/02	H01H43/02		164
H01H43/024	9	{Terminal arrangements}	H01H43/02	H01H43/02		81
H01H43/026	9	{Contact arrangements}	H01H43/02	H01H43/02		73
H01H43/028	9	{Means for manually actuating the contacts or interfering with the cooperation between timer mechanism and contacts}	H01H43/02	H01H43/02		73
H01H43/04	9	Means for time setting	H01H43/04	H01H43/04		423
H01H43/06	10	comprising separately adjustable parts for each programme step, e.g. with tappets	H01H43/06	H01H43/06		160
H01H43/065	11	{using cams or discs supporting a plurality of individually programmable elements (Schaltreiter)}	H01H43/06	H01H43/06		111
H01H43/08	10	comprising an interchangeable programme part which is common for all programme steps, e.g. with a punched card	H01H43/08	H01H43/08		65
H01H43/10	8	with timing of actuation of contacts due to a part rotating at substantially constant speed	H01H43/10	H01H43/10		438
H01H43/101	9	{Driving mechanisms}	H01H43/10	H01H43/10		203
H01H43/102	10	{using a pawl and ratchet wheel mechanism}	H01H43/10	H01H43/10		189
H01H43/103	9	{stopping automatically after one preselected time interval}	H01H43/10	H01H43/10		57
H01H43/104	10	{by mechanical coupling device}	H01H43/10	H01H43/10		31
H01H43/105	10	{by electromechanical coupling device}	H01H43/10	H01H43/10		23
H01H43/106	9	{Manual programme selecting means}	H01H43/10	H01H43/10		119
H01H2043/107	10	{Bidirectional selecting means, e.g. the programme selecting knob being turnable in both directions}	H01H43/10	H01H43/10		51
H01H2043/108	9	{where at least some contacts of electromechanical timer give instructions to electronic timer and/or the timing motor is under control of electronic timer, e.g. hybrid timer}	H01H43/10	H01H43/10		65
H01H43/12	9	stopping automatically after a single cycle of operation	H01H43/12	H01H43/12		134
H01H43/121	10	{using a drum}	H01H43/12	H01H43/12		145
H01H43/122	11	{with provision for adjustment of the intervals by a non-rotating member}	H01H43/12	H01H43/12		6
H01H43/124	10	{using a disc}	H01H43/12	H01H43/12		176
H01H43/125	10	{using a cam}	H01H43/12	H01H43/12		325
H01H43/127	11	{with provision for adjustment of the intervals by means carried by the cam}	H01H43/12	H01H43/12		28
H01H43/128	11	{with provision for adjustment of the intervals by a non-rotating member}	H01H43/12	H01H43/12		15
H01H43/14	10	wherein repetition of operation necessitates resetting of time intervals	H01H43/14	H01H43/14		2
H01H43/16	9	stopping automatically after a predetermined plurality of cycles of operation	H01H43/16	H01H43/16		74
H01H43/24	8	with timing of actuation of contacts due to a non-rotatable moving part	H01H43/24	H01H43/24		219
H01H43/26	9	the actuation being produced by a substance flowing due to gravity, e.g. sand, water	H01H43/26	H01H43/26		22
H01H43/28	9	the actuation being produced by a part, the speed of which is controlled by fluid-pressure means, e.g. by piston and cylinder	H01H43/28	H01H43/28		180
H01H43/285	10	{adjusting the time interval by means of an adjustable orifice, e.g. needle valve}	H01H43/28	H01H43/28		66
H01H43/30	8	with timing of actuation of contacts due to thermal action	H01H43/30	H01H43/30		111
H01H43/301	9	{based on the expansion or contraction of a material (thermometers based on the expansion or contraction of a material G01K5/00)}	H01H43/30	H01H43/30		1
H01H43/302	10	{of solid bodies}	H01H43/30	H01H43/30		31
H01H43/303	11	{of one single solid body, e.g. hot wire}	H01H43/30	H01H43/30		61
H01H43/304	11	{of two bodies expanding or contracting in a different manner, e.g. bimetallic elements}	H01H43/30	H01H43/30		411
H01H43/305	12	{actuating the contacts by commanding a mechanical device, e.g. thermal motor}	H01H43/30	H01H43/30		14
H01H43/306	10	{of liquids}	H01H43/30	H01H43/30		7
H01H43/307	10	{of gases}	H01H43/30	H01H43/30		11
H01H43/308	9	{based on the change of electrical properties, e.g. thermistors (thermometers based on the use of electric or magnetic elements directly sensitive to heat G01K7/00)}	H01H43/30	H01H43/30		71
H01H43/309	9	{based on the change of magnetic properties (thermometers based on the use of electric or magnetic elements directly sensitive to heat G01K7/00)}	H01H43/30	H01H43/30		6
H01H43/32	8	with timing of actuation of contacts due to electrolytic processes; with timing of actuation of contacts due to chemical processes	H01H43/32	H01H43/32		86
H01H43/322	9	{Electrolytic decomposition of liquids, e.g. actuation of contacts due to action of the products of reaction}	H01H43/32	H01H43/32		1
H01H43/325	9	{Electrolytic decomposition of solid bodies, e.g. action by rupture}	H01H43/32	H01H43/32		4
H01H43/327	9	{acting by coulometric transfer of material}	H01H43/32	H01H43/32		7
H01H45/00	7	Details of relays (electric circuit arrangements H01H47/00; of electromagnetic relays H01H50/00; details of electrically-operated selector switches H01H63/00)	H01H45/00	H01H45/00		165
H01H45/02	8	Bases; Casings; Covers (frames for mounting two or more relays or for mounting a relay and another electric component H02B1/01, H04Q1/08, H05K)	H01H45/02	H01H45/02		264
H01H45/04	9	Mounting complete relay or separate parts of relay on a base or inside a case	H01H45/04	H01H45/04		207
H01H45/06	9	having windows; Transparent cases or covers	H01H45/06	H01H45/06		9
H01H45/08	8	Indicators; Distinguishing marks	H01H45/08	H01H45/08		49
H01H45/10	8	Electromagnetic or electrostatic shielding (casings H01H45/02)	H01H45/10	H01H45/10		14
H01H45/12	8	Ventilating; Cooling; Heating (for operating electrothermal relays H01H61/013)	H01H45/12	H01H45/12		130
H01H45/14	8	Terminal arrangements	H01H45/14	H01H45/14		158
H01H47/00	7	Circuit arrangements not adapted to a particular application of the relay and designed to obtain desired operating characteristics or to provide energising current	H01H47/00	H01H47/00		912
H01H47/001	8	{Functional circuits, e.g. logic, sequencing, interlocking circuits}	H01H47/00	H01H47/00		785
H01H47/002	8	{Monitoring or fail-safe circuits}	H01H47/00	H01H47/00		1782
H01H2047/003	9	{Detecting welded contacts and applying weld break pulses to coil}	H01H47/00	H01H47/00		77
H01H47/004	9	{using plural redundant serial connected relay operated contacts in controlled circuit}	H01H47/00	H01H47/00		173
H01H47/005	10	{Safety control circuits therefor, e.g. chain of relays mutually monitoring each other}	H01H47/00	H01H47/00		161
H01H2047/006	9	{Detecting unwanted movement of contacts and applying pulses to coil for restoring to normal status}	H01H47/00	H01H47/00		51
H01H47/007	8	{with galvanic isolation between controlling and controlled circuit, e.g. transformer relay}	H01H47/00	H01H47/00		69
H01H2047/008	8	{with a drop in current upon closure of armature or change of inductance}	H01H47/00	H01H47/00		82
H01H2047/009	8	{with self learning features, e.g. measuring the attracting current for a relay and memorising it}	H01H47/00	H01H47/00		55
H01H47/02	8	for modifying the operation of the relay	H01H47/02	H01H47/02		880
H01H2047/025	9	{with taking into account of the thermal influences, e.g. change in resistivity of the coil or being adapted to high temperatures}	H01H47/02	H01H47/02		89
H01H47/04	9	for holding armature in attracted position, e.g. when initial energising circuit is interrupted; for maintaining armature in attracted position, e.g. with reduced energising current {(with switching regulator H01H47/325)}	H01H47/04	H01H47/04		385
H01H47/043	10	{making use of an energy accumulator (for bistable relays H01H47/226)}	H01H47/04	H01H47/04		156
H01H2047/046	10	{with measuring of the magnetic field, e.g. of the magnetic flux, for the control of coil current}	H01H47/04	H01H47/04		48
H01H47/06	10	by changing number of serially-connected turns or windings	H01H47/06	H01H47/06		55
H01H47/08	10	by changing number of parallel-connected turns or windings	H01H47/08	H01H47/08		49
H01H47/10	10	by switching-in or -out impedance external to the relay winding	H01H47/10	H01H47/10		84
H01H47/12	9	for biasing the electromagnet	H01H47/12	H01H47/12		50
H01H47/14	9	for differential operation of the relay	H01H47/14	H01H47/14		82
H01H47/16	9	for conjoint, e.g. additive, operation of the relay	H01H47/16	H01H47/16		90
H01H47/18	9	for introducing delay in the operation of the relay (short-circuited conducting sleeves, bands or discs H01H50/46)	H01H47/18	H01H47/18		718
H01H47/20	9	for producing frequency-selective operation of the relay	H01H47/20	H01H47/20		93
H01H47/22	8	for supplying energising current for relay coil	H01H47/22	H01H47/22		652
H01H47/223	9	{adapted to be supplied by AC}	H01H47/22	H01H47/22		182
H01H47/226	9	{for bistable relays}	H01H47/22	H01H47/22		295
H01H47/24	9	having light-sensitive input	H01H47/24	H01H47/24		308
H01H47/26	9	having thermo-sensitive input	H01H47/26	H01H47/26		100
H01H47/28	9	Energising current supplied by discharge tube	H01H47/28	H01H47/28		12
H01H47/30	10	by gas-filled discharge tube	H01H47/30	H01H47/30		1
H01H47/32	9	Energising current supplied by semiconductor device	H01H47/32	H01H47/32		521
H01H47/325	10	{by switching regulator}	H01H47/32	H01H47/32		827
H01H47/34	9	Energising current supplied by magnetic amplifier	H01H47/34	H01H47/34		57
H01H47/36	9	Relay coil or coils forming part of a bridge circuit	H01H47/36	H01H47/36		48
H01H49/00	7	Apparatus or processes specially adapted to the manufacture of relays or parts thereof	H01H49/00	H01H49/00		1108
H01H50/00	7	Details of electromagnetic relays ({H01H51/28 takes precedence;} electric circuit arrangements H01H47/00; details of electrically-operated selector switches H01H63/00)	H01H50/00	H01H50/00		295
H01H50/002	8	{particular to three-phase electromagnetic relays (synchronous switching H01H9/563)}	H01H50/00	H01H50/00		101
H01H50/005	8	{using micromechanics}	H01H50/00	H01H50/00		225
H01H2050/007	9	{Relays of the polarised type, e.g. the MEMS relay beam having a preferential magnetisation direction}	H01H50/00	H01H50/00		85
H01H50/02	8	Bases; Casings; Covers (frames for mounting two or more relays or for mounting a relay and another electric component H02B1/01, H04Q1/08, H05K)	H01H50/02	H01H50/02		1404
H01H50/021	9	{structurally combining a relay and an electronic component, e.g. varistor, RC circuit (auxiliary switch inserting resistor during closure H01H50/543)}	H01H50/02	H01H50/02		564
H01H50/023	9	{Details concerning sealing, e.g. sealing casing with resin}	H01H50/02	H01H50/02		666
H01H2050/025	10	{containing inert or dielectric gasses, e.g. SF6, for arc prevention or arc extinction}	H01H50/02	H01H50/02		263
H01H50/026	9	{Details concerning isolation between driving and switching circuit}	H01H50/02	H01H50/02		294
H01H2050/028	9	{Means to improve the overall withstanding voltage, e.g. creepage distances}	H01H50/02	H01H50/02		203
H01H50/04	9	Mounting complete relay or separate parts of relay on a base or inside a case	H01H50/04	H01H50/04		582
H01H50/041	10	{Details concerning assembly of relays}	H01H50/04	H01H50/04		562
H01H50/042	11	{Different parts are assembled by insertion without extra mounting facilities like screws, in an isolated mounting part, e.g. stack mounting on a coil-support}	H01H50/04	H01H50/04		323
H01H50/043	11	{Details particular to miniaturised relays (H01H50/042 takes precedence)}	H01H50/04	H01H50/04		194
H01H2050/044	12	{Special measures to minimise the height of the relay}	H01H50/04	H01H50/04		69
H01H50/045	11	{Details particular to contactors (H01H50/042 takes precedence)}	H01H50/04	H01H50/04		540
H01H2050/046	11	{Assembling parts of a relay by using snap mounting techniques}	H01H50/04	H01H50/04		117
H01H50/047	10	{Details concerning mounting a relays}	H01H50/04	H01H50/04		315
H01H50/048	11	{Plug-in mounting or sockets}	H01H50/04	H01H50/04		291
H01H2050/049	10	{Assembling or mounting multiple relays in one common housing}	H01H50/04	H01H50/04		182
H01H50/06	9	having windows; Transparent cases or covers	H01H50/06	H01H50/06		69
H01H50/08	8	Indicators; Distinguishing marks	H01H50/08	H01H50/08		468
H01H50/10	8	Electromagnetic or electrostatic shielding (casings H01H50/02)	H01H50/10	H01H50/10		184
H01H50/12	8	Ventilating; Cooling; Heating (for operating electrothermal relays H01H61/013)	H01H50/12	H01H50/12		549
H01H50/14	8	Terminal arrangements {(for coils H01H50/443)}	H01H50/14	H01H50/14		1784
H01H50/16	8	Magnetic circuit arrangements	H01H50/16	H01H50/16		1217
H01H50/163	9	{Details concerning air-gaps, e.g. anti-remanence, damping, anti-corrosion}	H01H50/16	H01H50/16		313
H01H2050/166	9	{wherein the magnetic circuit parts are molded in a magnetic plastic material}	H01H50/16	H01H50/16		18
H01H50/18	9	Movable parts of magnetic circuits, e.g. armature	H01H50/18	H01H50/18		930
H01H50/20	10	movable inside coil and substantially lengthwise with respect to axis thereof; movable coaxially with respect to coil	H01H50/20	H01H50/20		905
H01H50/22	11	wherein the magnetic circuit is substantially closed	H01H50/22	H01H50/22		459
H01H2050/225	12	{with yoke and armature formed by identical stacked laminates, e.g. punched in one and the same tool}	H01H50/22	H01H50/22		29
H01H50/24	10	Parts rotatable or rockable outside coil	H01H50/24	H01H50/24		583
H01H50/26	11	Parts movable about a knife edge	H01H50/26	H01H50/26		306
H01H50/28	11	Parts movable due to bending of a blade spring or reed	H01H50/28	H01H50/28		311
H01H50/30	10	Mechanical arrangements for preventing or damping vibration or shock, e.g. by balancing of armature	H01H50/30	H01H50/30		766
H01H50/305	11	{damping vibration due to functional movement of armature (in air-gap H01H50/163)}	H01H50/30	H01H50/30		504
H01H50/32	10	Latching movable parts mechanically	H01H50/32	H01H50/32		393
H01H50/321	11	{the mechanical latch being controlled directly by the magnetic flux or part of it}	H01H50/32	H01H50/32		75
H01H50/323	11	{for interlocking two or more relays}	H01H50/32	H01H50/32		269
H01H2050/325	12	{Combined electrical and mechanical interlocking, e.g. usually for auxiliary contacts}	H01H50/32	H01H50/32		31
H01H50/326	11	{with manual intervention, e.g. for testing, resetting or mode selection}	H01H50/32	H01H50/32		192
H01H2050/328	12	{with manual locking means having three positions, e.g. on-off-automatic}	H01H50/32	H01H50/32		25
H01H50/34	10	Means for adjusting limits of movement; Mechanical means for adjusting returning force	H01H50/34	H01H50/34		438
H01H50/36	9	Stationary parts of magnetic circuit, e.g. yoke	H01H50/36	H01H50/36		947
H01H2050/362	10	{Part of the magnetic circuit conducts current to be switched or coil current, e.g. connector and magnetic circuit formed of one single part}	H01H50/36	H01H50/36		47
H01H2050/365	10	{formed from a single sheet of magnetic material by punching, bending, plying}	H01H50/36	H01H50/36		37
H01H2050/367	10	{Methods for joining separate core and L-shaped yoke}	H01H50/36	H01H50/36		75
H01H50/38	10	Part of main magnetic circuit shaped to suppress arcing between the contacts of the relay	H01H50/38	H01H50/38		399
H01H50/40	10	Branched or multiple-limb main magnetic circuits	H01H50/40	H01H50/40		148
H01H50/42	10	Auxiliary magnetic circuits, e.g. for maintaining armature in, or returning armature to, position of rest, for damping or accelerating movement	H01H50/42	H01H50/42		224
H01H50/44	8	Magnetic coils or windings	H01H50/44	H01H50/44		1134
H01H50/443	9	{Connections to coils}	H01H50/44	H01H50/44		567
H01H2050/446	9	{Details of the insulating support of the coil, e.g. spool, bobbin, former}	H01H50/44	H01H50/44		454
H01H50/46	9	Short-circuited conducting sleeves, bands, or discs {(for electromagnets H01F7/1205)}	H01H50/46	H01H50/46		168
H01H50/54	8	Contact arrangements	H01H50/54	H01H50/54		2685
H01H50/541	9	{Auxiliary contact devices}	H01H50/54	H01H50/54		595
H01H50/543	10	{Auxiliary switch inserting resistor during closure of contactor}	H01H50/54	H01H50/54		83
H01H50/545	10	{Self-contained, easily replaceable microswitches}	H01H50/54	H01H50/54		177
H01H50/546	9	{for contactors having bridging contacts}	H01H50/54	H01H50/54		1377
H01H50/548	9	{for miniaturised relays}	H01H50/54	H01H50/54		154
H01H50/56	9	Contact spring sets	H01H50/56	H01H50/56		1149
H01H50/58	10	Driving arrangements structurally associated therewith; Mounting of driving arrangements on armature	H01H50/58	H01H50/58		673
H01H50/60	9	moving contact being rigidly combined with movable part of magnetic circuit {(for polarised relays H01H51/2254, H01H51/2281)}	H01H50/60	H01H50/60		431
H01H50/62	9	Co-operating movable contacts operated by separate electrical actuating means	H01H50/62	H01H50/62		86
H01H50/64	8	Driving arrangements between movable part of magnetic circuit and contact (structurally associated with contact spring sets H01H50/58)	H01H50/64	H01H50/64		764
H01H50/641	9	{intermediate part performing a rectilinear movement (H01H50/645, H01H50/66&#160;-&#160;H01H50/74 take precedence)}	H01H50/64	H01H50/64		378
H01H50/642	10	{intermediate part being generally a slide plate, e.g. a card}	H01H50/64	H01H50/64		261
H01H50/643	9	{intermediate part performing a rotating or pivoting movement (H01H50/645, H01H50/66&#160;-&#160;H01H50/74 take precedence)}	H01H50/64	H01H50/64		299
H01H50/644	10	{having more than one rotating or pivoting part}	H01H50/64	H01H50/64		143
H01H50/645	9	{intermediate part making a resilient or flexible connection (H01H50/66&#160;-&#160;H01H50/74 take precedence)}	H01H50/64	H01H50/64		142
H01H50/646	10	{intermediate part being a blade spring}	H01H50/64	H01H50/64		68
H01H50/647	9	{intermediate part comprising interlocking means for different contact pairs (H01H50/66&#160;-&#160;H01H50/74 take precedence; for two separate relays H01H50/323; for ratchets H01H51/08)}	H01H50/64	H01H50/64		30
H01H50/648	9	{intermediate part being rigidly combined with armature (H01H50/66&#160;-&#160;H01H50/74 take precedence)}	H01H50/64	H01H50/64		110
H01H50/66	9	with lost motion	H01H50/66	H01H50/66		45
H01H50/68	9	with snap action	H01H50/68	H01H50/68		118
H01H50/70	9	operating contact momentarily during stroke of armature	H01H50/70	H01H50/70		20
H01H50/72	9	for mercury contact	H01H50/72	H01H50/72		85
H01H50/74	9	Mechanical means for producing a desired natural frequency of operation of the contacts, e.g. for self-interrupter	H01H50/74	H01H50/74		24
H01H50/76	10	using reed or blade spring	H01H50/76	H01H50/76		487
H01H50/78	10	using diaphragm; using stretched wire or ribbon vibrating sideways	H01H50/78	H01H50/78		9
H01H50/80	10	using torsionally-vibrating member, e.g. wire, strip	H01H50/80	H01H50/80		4
H01H50/82	10	using spring-loaded pivoted inertia member	H01H50/82	H01H50/82		31
H01H50/84	10	with means for adjustment of frequency or of make-to-break ratio	H01H50/84	H01H50/84		8
H01H50/86	8	Means for introducing a predetermined time delay between the initiation of the switching operation and the opening or closing of the contacts (circuit arrangements for introducing delay H01H47/18; short-circuited conducting sleeves, bands, or discs H01H50/46)	H01H50/86	H01H50/86		68
H01H50/88	9	Mechanical means, e.g. dash-pot	H01H50/88	H01H50/88		351
H01H50/90	10	the delay effective in both directions of operation	H01H50/90	H01H50/90		4
H01H50/92	9	Thermal means (inherent in electrothermal relays H01H61/00)	H01H50/92	H01H50/92		5
H01H51/00	7	Electromagnetic relays (relays using the dynamo-electric effect H01H53/00)	H01H51/00	H01H51/00		132
H01H51/005	8	{Inversing contactors (H01H50/323 takes precedence)}	H01H51/00	H01H51/00		145
H01H51/01	8	Relays in which the armature is maintained in one position by a permanent magnet and freed by energisation of a coil producing an opposing magnetic field {(H01H51/02&#160;-&#160;H01H51/26 take precedence)}	H01H51/01	H01H51/01		505
H01H51/02	8	Non-polarised relays	H01H51/02	H01H51/02		56
H01H51/04	9	with single armature; with single set of ganged armatures	H01H51/04	H01H51/04		56
H01H51/06	10	Armature is movable between two limit positions of rest and is moved in one direction due to energisation of an electromagnet and after the electromagnet is de-energised is returned by energy stored during the movement in the first direction, e.g. by using a spring, by using a permanent magnet, by gravity	H01H51/06	H01H51/06		583
H01H51/065	11	{Relays having a pair of normally open contacts rigidly fixed to a magnetic core movable along the axis of a solenoid, e.g. relays for starting automobiles (details H01H50/20)}	H01H51/06	H01H51/06		852
H01H51/08	11	Contacts alternately opened and closed by successive cycles of energisation and de-energisation of the electromagnet, e.g. by use of a ratchet	H01H51/08	H01H51/08		208
H01H51/082	12	{using rotating ratchet mechanism}	H01H51/08	H01H51/08		111
H01H51/084	13	{with axial ratchet elements}	H01H51/08	H01H51/08		52
H01H51/086	13	{with radial ratchet elements}	H01H51/08	H01H51/08		254
H01H51/088	14	{moved alternately in opposite directions}	H01H51/08	H01H51/08		141
H01H51/10	11	Contacts retained open or closed by a latch which is controlled by an electromagnet	H01H51/10	H01H51/10		251
H01H51/12	10	Armature is movable between two limit positions of rest and is moved in both directions due to the energisation of one or the other of two electromagnets without the storage of energy to effect the return movement	H01H51/12	H01H51/12		488
H01H51/14	11	without intermediate neutral position of rest	H01H51/14	H01H51/14		12
H01H51/16	11	with intermediate neutral position of rest	H01H51/16	H01H51/16		7
H01H51/18	10	Armature is rotatable through an unlimited number of revolutions	H01H51/18	H01H51/18		17
H01H51/20	9	with two or more independent armatures	H01H51/20	H01H51/20		250
H01H51/22	8	Polarised relays {(H01H51/284 takes precedence)}	H01H51/22	H01H51/22		297
H01H51/2209	9	{with rectilinearly movable armature}	H01H51/22	H01H51/22		421
H01H2051/2218	10	{having at least one movable permanent magnet}	H01H51/22	H01H51/22		144
H01H51/2227	9	{in which the movable part comprises at least one permanent magnet, sandwiched between pole-plates, each forming an active air-gap with parts of the stationary magnetic circuit (H01H51/2209 takes precedence)}	H01H51/22	H01H51/22		226
H01H51/2236	9	{comprising pivotable armature, pivoting at extremity or bending point of armature (H01H51/2227 takes precedence)}	H01H51/22	H01H51/22		202
H01H51/2245	10	{Armature inside coil}	H01H51/22	H01H51/22		37
H01H51/2254	11	{Contact forms part of armature}	H01H51/22	H01H51/22		73
H01H51/2263	9	{comprising rotatable armature, rotating around central axis perpendicular to the main plane of the armature (H01H51/2227 takes precedence)}	H01H51/22	H01H51/22		92
H01H51/2272	9	{comprising rockable armature, rocking movement around central axis parallel to the main plane of the armature (H01H51/2227 takes precedence)}	H01H51/22	H01H51/22		297
H01H51/2281	10	{Contacts rigidly combined with armature}	H01H51/22	H01H51/22		214
H01H51/229	11	{Blade-spring contacts alongside armature}	H01H51/22	H01H51/22		103
H01H51/24	9	without intermediate neutral position of rest	H01H51/24	H01H51/24		31
H01H51/26	9	with intermediate neutral position of rest	H01H51/26	H01H51/26		10
H01H51/27	8	Relays with armature having two stable magnetic states and operated by change from one state to the other	H01H51/27	H01H51/27		123
H01H51/28	8	Relays having both armature and contacts within a sealed casing outside which the operating coil is located, e.g. contact carried by a magnetic leaf spring or reed (H01H51/27 takes precedence)	H01H51/28	H01H51/28		431
H01H51/281	9	{Mounting of the relay; Encapsulating; Details of connections}	H01H51/28	H01H51/28		448
H01H51/282	9	{Constructional details not covered by H01H51/281}	H01H51/28	H01H51/28		73
H01H51/284	9	{Polarised relays}	H01H51/28	H01H51/28		223
H01H51/285	10	{for latching of contacts}	H01H51/28	H01H51/28		108
H01H51/287	9	{Details of the shape of the contact springs}	H01H51/28	H01H51/28		342
H01H51/288	9	{Freely suspended contacts}	H01H51/28	H01H51/28		111
H01H51/29	8	Relays having armature, contacts, and operating coil within a sealed casing (H01H51/27 takes precedence)	H01H51/29	H01H51/29		133
H01H51/30	8	specially adapted for actuation by AC	H01H51/30	H01H51/30		190
H01H51/32	9	Frequency relays; Mechanically-tuned relays	H01H51/32	H01H51/32		565
H01H51/34	8	Self-interrupters, i.e. with periodic or other repetitive opening and closing of contacts	H01H51/34	H01H51/34		217
H01H51/36	9	wherein the make-to-break ratio is varied by hand setting or current strength	H01H51/36	H01H51/36		1
H01H53/00	7	Relays using the dynamo-electric effect, i.e. relays in which contacts are opened or closed due to relative movement of current-carrying conductor and magnetic field caused by force of interaction between them	H01H53/00	H01H53/00		24
H01H53/01	8	Details	H01H53/01	H01H53/01		10
H01H53/015	9	Moving coils; Contact-driving arrangements associated therewith	H01H53/015	H01H53/015		289
H01H53/02	8	Electrodynamic relays, i.e. relays in which the interaction is between two current-carrying conductors	H01H53/02	H01H53/02		33
H01H53/04	9	Ferrodynamic relays, i.e. relays in which the magnetic field is concentrated in ferromagnetic parts	H01H53/04	H01H53/04		10
H01H53/06	8	Magnetodynamic relays, i.e. relays in which the magnetic field is produced by a permanent magnet	H01H53/06	H01H53/06		32
H01H53/08	8	wherein a mercury contact constitutes the current-carrying conductor	H01H53/08	H01H53/08		36
H01H53/10	8	Induction relays, i.e. relays in which the interaction is between a magnetic field and current induced thereby in a conductor	H01H53/10	H01H53/10		234
H01H53/12	9	Ferraris relays	H01H53/12	H01H53/12		66
H01H53/14	8	Contacts actuated by an electric motor through fluid-pressure transmission, e.g. using a motor-driven pump	H01H53/14	H01H53/14		4
H01H55/00	7	Magnetostrictive relays	H01H55/00	H01H55/00		65
H01H57/00	7	Electrostrictive relays; Piezoelectric relays	H01H57/00	H01H57/00		447
H01H2057/003	8	{the relay being latched in actuated position by magnet}	H01H57/00	H01H57/00		31
H01H2057/006	8	{Micromechanical piezoelectric relay}	H01H57/00	H01H57/00		232
H01H59/00	7	Electrostatic relays; Electro-adhesion relays	H01H59/00	H01H59/00		284
H01H59/0009	8	{making use of micromechanics}	H01H59/00	H01H59/00		1370
H01H2059/0018	9	{Special provisions for avoiding charge trapping, e.g. insulation layer between actuating electrodes being permanently polarised by charge trapping so that actuating or release voltage is altered}	H01H59/00	H01H59/00		53
H01H2059/0027	9	{Movable electrode connected to ground in the open position, for improving isolation}	H01H59/00	H01H59/00		32
H01H2059/0036	9	{Movable armature with higher resonant frequency for faster switching}	H01H59/00	H01H59/00		32
H01H2059/0045	9	{with s-shaped movable electrode, positioned and connected between two driving fixed electrodes, e.g. movable electrodes moving laterally when driving voltage being applied}	H01H59/00	H01H59/00		11
H01H2059/0054	9	{Rocking contacts or actuating members}	H01H59/00	H01H59/00		51
H01H2059/0063	9	{with stepped actuation, e.g. actuation voltages applied to different sets of electrodes at different times or different spring constants during actuation}	H01H59/00	H01H59/00		41
H01H2059/0072	9	{with stoppers or protrusions for maintaining a gap, reducing the contact area or for preventing stiction between the movable and the fixed electrode in the attracted position}	H01H59/00	H01H59/00		93
H01H2059/0081	9	{with a tapered air-gap between fixed and movable electrodes}	H01H59/00	H01H59/00		65
H01H2059/009	8	{using permanently polarised dielectric layers}	H01H59/00	H01H59/00		49
H01H61/00	7	Electrothermal relays (thermal switches not operated by electrical input, thermal switches with anticipating electrical input H01H37/00; thermally-sensitive members H01H37/32)	H01H61/00	H01H61/00		131
H01H61/002	8	{Structural combination of a time delay electrothermal relay with an electrothermal protective relay, e.g. a start relay}	H01H61/00	H01H61/00		212
H01H2061/004	9	{PTC resistor in series with start winding, e.g. adapted for being switched off after starting for limiting power dissipation}	H01H61/00	H01H61/00		21
H01H2061/006	8	{Micromechanical thermal relay}	H01H61/00	H01H61/00		197
H01H2061/008	9	{Micromechanical actuator with a cold and a hot arm, coupled together at one end}	H01H61/00	H01H61/00		42
H01H61/01	8	Details	H01H61/01	H01H61/01		118
H01H61/0107	9	{making use of shape memory materials}	H01H61/01	H01H61/01		177
H01H2061/0115	10	{Shape memory alloy [SMA] actuator formed by coil spring}	H01H61/01	H01H61/01		97
H01H2061/0122	10	{Two SMA actuators, e.g. one for closing or resetting contacts and one for opening them}	H01H61/01	H01H61/01		72
H01H61/013	9	Heating arrangements for operating relays	H01H61/013	H01H61/013		113
H01H61/017	10	Heating by glow discharge or arc in confined space	H01H61/017	H01H61/017		38
H01H61/02	8	wherein the thermally-sensitive member is heated indirectly, e.g. resistively, inductively	H01H61/02	H01H61/02		604
H01H61/04	8	wherein the thermally-sensitive member is only heated directly	H01H61/04	H01H61/04		138
H01H61/06	8	Self-interrupters, i.e. with periodic or other repetitive opening and closing of contacts	H01H61/06	H01H61/06		147
H01H61/063	9	{making use of a bimetallic element}	H01H61/06	H01H61/06		238
H01H61/066	9	{making use of an extensible wire, rod or strips}	H01H61/06	H01H61/06		291
H01H61/08	9	wherein the make-to-break ratio is varied by hand setting or current strength	H01H61/08	H01H61/08		36
H01H63/00	7	Details of electrically-operated selector switches	H01H63/00	H01H63/00		110
H01H63/02	8	Contacts; Wipers; Connections thereto	H01H63/02	H01H63/02		213
H01H63/04	9	Contact-making or contact-breaking wipers; Position indicators therefor	H01H63/04	H01H63/04		129
H01H63/06	9	Contact banks	H01H63/06	H01H63/06		259
H01H63/08	10	cylindrical	H01H63/08	H01H63/08		8
H01H63/10	10	plane	H01H63/10	H01H63/10		3
H01H63/12	9	Multiplying connections to contact banks, e.g. using ribbon cables	H01H63/12	H01H63/12		10
H01H63/14	10	without soldering	H01H63/14	H01H63/14		1
H01H63/16	8	Driving arrangements for multi-position wipers	H01H63/16	H01H63/16		23
H01H63/18	9	with step-by-step motion of wiper to a selector position	H01H63/18	H01H63/18		23
H01H63/20	10	using stepping magnet and ratchet	H01H63/20	H01H63/20		125
H01H63/22	10	using step-by-step electromagnetic drive without ratchet, e.g. self-interrupting driving magnet	H01H63/22	H01H63/22		139
H01H63/24	9	with continuous motion of wiper until a selected position is reached	H01H63/24	H01H63/24		71
H01H63/26	10	with an individual clutch-drive from a shaft common to more than one selector switch	H01H63/26	H01H63/26		
H01H63/28	10	with an individual motor for each selector switch	H01H63/28	H01H63/28		2
H01H63/30	11	Pneumatic motor for moving wiper to selected position	H01H63/30	H01H63/30		70
H01H63/32	11	Spring motor for moving wiper to selected position	H01H63/32	H01H63/32		8
H01H63/33	8	Constructional details of co-ordinate-type selector switches not having relays at cross-points	H01H63/33	H01H63/33		12
H01H63/34	8	Bases; Cases; Covers; Mountings (racks for mounting selectors with or without other exchange equipment H04Q1/04); Mounting of fuses on selector switch	H01H63/34	H01H63/34		34
H01H63/36	8	Circuit arrangements for ensuring correct or desired operation and not adapted to a particular application of the selector switch	H01H63/36	H01H63/36		61
H01H63/38	9	for multi-position wiper switches	H01H63/38	H01H63/38		28
H01H63/40	9	for multi-position switches without wipers	H01H63/40	H01H63/40		12
H01H63/42	10	for co-ordinate-type selector switches not having relays at cross-points	H01H63/42	H01H63/42		12
H01H65/00	7	Apparatus or processes specially adapted to the manufacture of selector switches or parts thereof	H01H65/00	H01H65/00		15
H01H67/00	7	Electrically-operated selector switches	H01H67/00	H01H67/00		21
H01H67/02	8	Multi-position wiper switches	H01H67/02	H01H67/02		26
H01H67/04	9	having wipers movable only in one direction for purpose of selection	H01H67/04	H01H67/04		3
H01H67/06	10	Rotary switches, i.e. having angularly movable wipers	H01H67/06	H01H67/06		616
H01H67/08	11	with wiper selection	H01H67/08	H01H67/08		9
H01H67/10	11	with coarse and fine positioning of wipers	H01H67/10	H01H67/10		
H01H67/12	10	Linear-motion switches	H01H67/12	H01H67/12		305
H01H67/14	9	having wipers movable in two mutually perpendicular directions for purpose of selection	H01H67/14	H01H67/14		1
H01H67/16	10	one motion being rotary and the other being parallel to the axis of rotation, e.g. Strowger or "up and around" switches	H01H67/16	H01H67/16		203
H01H67/18	10	one motion being rotary and the other being perpendicular to the axis of rotation, e.g. "round and in" switches	H01H67/18	H01H67/18		2
H01H67/20	10	both motions being linear	H01H67/20	H01H67/20		1
H01H67/22	8	Switches without multi-position wipers	H01H67/22	H01H67/22		162
H01H67/24	9	Co-ordinate-type relay switches having an individual electromagnet at each cross-point	H01H67/24	H01H67/24		214
H01H67/26	9	Co-ordinate-type selector switches not having relays at cross-points but involving mechanical movement, e.g. cross-bar switch, code-bar switch	H01H67/26	H01H67/26		1017
H01H67/30	9	Co-ordinate-type selector switches with field of co-ordinate coil acting directly upon magnetic leaf spring or reed-type contact member	H01H67/30	H01H67/30		96
H01H67/32	9	having a multiplicity of interdependent armatures operated in succession by a single coil and each controlling one contact or set of contacts, e.g. counting relay	H01H67/32	H01H67/32		33
H01H69/00	7	Apparatus or processes for the manufacture of emergency protective devices	H01H69/00	H01H69/00		610
H01H69/01	8	for calibrating or setting of devices to function under predetermined conditions	H01H69/01	H01H69/01		195
H01H2069/013	9	{with calibrating screws in trip bar}	H01H69/01	H01H69/01		34
H01H2069/016	9	{with single separate parts mountable or insertable in different orientations or positions, e.g. to obtain desired trip conditions}	H01H69/01	H01H69/01		23
H01H69/02	8	Manufacture of fuses	H01H69/02	H01H69/02		1121
H01H69/022	9	{of printed circuit fuses}	H01H69/02	H01H69/02		187
H01H2069/025	9	{using lasers}	H01H69/02	H01H69/02		49
H01H2069/027	9	{using ultrasonic techniques}	H01H69/02	H01H69/02		34
H01H71/00	7	Details of the protective switches or relays covered by groups H01H73/00&#160;-&#160;H01H83/00	H01H71/00	H01H71/00		405
H01H71/002	8	{with provision for switching the neutral conductor}	H01H71/00	H01H71/00		221
H01H2071/004	9	{with a tripping or current sensing device in the neutral wire, e.g. for third harmonics in a three fase system}	H01H71/00	H01H71/00		22
H01H2071/006	8	{Provisions for user interfaces for electrical protection devices}	H01H71/00	H01H71/00		270
H01H2071/008	8	{Protective switches or relays using micromechanics}	H01H71/00	H01H71/00		55
H01H71/02	8	Housings; Casings; Bases; Mountings	H01H71/02	H01H71/02		1948
H01H71/0207	9	{Mounting or assembling the different parts of the circuit breaker}	H01H71/02	H01H71/02		1442
H01H71/0214	10	{Housing or casing lateral walls containing guiding grooves or special mounting facilities (H01H71/0221 takes precedence)}	H01H71/02	H01H71/02		422
H01H71/0221	10	{Majority of parts mounted on central frame or wall}	H01H71/02	H01H71/02		145
H01H71/0228	10	{having provisions for interchangeable or replaceable parts}	H01H71/02	H01H71/02		515
H01H71/0235	10	{Contacts and the arc extinguishing space inside individual separate cases, which are positioned inside the housing of the circuit breaker (casettes for rotating bridges seeH01H1/2058)}	H01H71/02	H01H71/02		110
H01H2071/0242	10	{Assembling parts of a circuit breaker by using snap mounting techniques}	H01H71/02	H01H71/02		159
H01H71/025	9	{Constructional details of housings or casings not concerning the mounting or assembly of the different internal parts}	H01H71/02	H01H71/02		485
H01H71/0257	10	{Strength considerations}	H01H71/02	H01H71/02		104
H01H71/0264	9	{Mountings or coverplates for complete assembled circuit breakers, e.g. snap mounting in panel}	H01H71/02	H01H71/02		380
H01H71/0271	10	{Mounting several complete assembled circuit breakers together (interconnected mechanisms H01H71/1009)}	H01H71/02	H01H71/02		373
H01H2071/0278	11	{with at least one of juxtaposed casings dedicated to an auxiliary device, e.g. for undervoltage or shunt trip}	H01H71/02	H01H71/02		167
H01H2071/0285	11	{Provisions for an intermediate device between two adjacent circuit breakers having the same general contour but an auxiliary function, e.g. cooling, isolation, wire guiding, magnetic isolation or screening}	H01H71/02	H01H71/02		47
H01H2071/0292	9	{Housing or frames containing grooves or slots for guiding movable parts}	H01H71/02	H01H71/02		116
H01H71/04	8	Means for indicating condition of the switching device {(by means of an auxiliary contact H01H71/46)}	H01H71/04	H01H71/04		2276
H01H2071/042	9	{with different indications for different conditions, e.g. contact position, overload, short circuit or earth leakage}	H01H71/04	H01H71/04		471
H01H2071/044	9	{Monitoring, detection or measuring systems to establish the end of life of the switching device, can also contain other on-line monitoring systems, e.g. for detecting mechanical failures}	H01H71/04	H01H71/04		461
H01H2071/046	9	{exclusively by position of operating part, e.g. with additional labels or marks but no other movable indicators}	H01H71/04	H01H71/04		184
H01H2071/048	9	{containing non-mechanical switch position sensor, e.g. HALL sensor}	H01H71/04	H01H71/04		204
H01H71/06	8	Distinguishing marks, e.g. colour coding	H01H71/06	H01H71/06		128
H01H71/08	8	Terminals; Connections	H01H71/08	H01H71/08		2559
H01H71/082	9	{Connections between juxtaposed circuit breakers}	H01H71/08	H01H71/08		373
H01H2071/084	9	{specially adapted for avoiding decalibration of trip unit, e.g. bimetal, when fixing conductor wire to connector}	H01H71/08	H01H71/08		25
H01H2071/086	9	{Low power connections for auxiliary switches, e.g. shunt trip}	H01H71/08	H01H71/08		210
H01H2071/088	9	{Terminals for switching devices which make the devices interchangeable, e.g. with fuses}	H01H71/08	H01H71/08		115
H01H71/10	8	Operating or release mechanisms	H01H71/10	H01H71/10		2793
H01H71/1009	9	{Interconnected mechanisms (H01H71/1045 takes precedence; operated by excess current and other electrical conditions H01H83/20)}	H01H71/10	H01H71/10		993
H01H71/1018	10	{with only external interconnections}	H01H71/10	H01H71/10		216
H01H71/1027	10	{comprising a bidirectional connecting member actuated by the opening movement of one pole to trip a neighbour pole}	H01H71/10	H01H71/10		219
H01H2071/1036	10	{having provisions for four or more poles}	H01H71/10	H01H71/10		134
H01H71/1045	9	{Multiple circuits-breaker, e.g. for the purpose of dividing current or potential drop}	H01H71/10	H01H71/10		250
H01H71/1054	9	{Means for avoiding unauthorised release}	H01H71/10	H01H71/10		382
H01H2071/1063	10	{making use of an equilibrating mass}	H01H71/10	H01H71/10		40
H01H71/1072	9	{Release mechanisms which are reset by opening movement of contacts}	H01H71/10	H01H71/10		113
H01H71/1081	9	{Modifications for selective or back-up protection; Correlation between feeder and branch circuit breaker (circuits H02H3/06, H02H7/26)}	H01H71/10	H01H71/10		236
H01H2071/109	9	{with provisions for selecting between automatic or manual reset}	H01H71/10	H01H71/10		129
H01H71/12	9	Automatic release mechanisms with or without manual release	H01H71/12	H01H71/12		989
H01H71/121	10	{Protection of release mechanisms (with auxiliary contact H01H71/48)}	H01H71/12	H01H71/12		206
H01H71/122	10	{actuated by blowing of a fuse}	H01H71/12	H01H71/12		235
H01H71/123	10	{using a solid-state trip unit (circuits H02H)}	H01H71/12	H01H71/12		1129
H01H2071/124	11	{with a hybrid structure, the solid state trip device being combined with a thermal or a electromagnetic trip}	H01H71/12	H01H71/12		116
H01H71/125	11	{characterised by sensing elements, e.g. current transformers (for differential protection H01H83/144)}	H01H71/12	H01H71/12		398
H01H71/126	10	{actuated by dismounting of circuit breaker or removal of part of circuit breaker}	H01H71/12	H01H71/12		119
H01H71/127	10	{using piezoelectric, electrostrictive or magnetostrictive trip units}	H01H71/12	H01H71/12		74
H01H71/128	10	{Manual release or trip mechanisms, e.g. for test purposes (two similar push buttons for closing or resetting and opening or tripping H01H71/58; test switches for earth fault circuit breakers H01H83/04)}	H01H71/12	H01H71/12		461
H01H71/14	10	Electrothermal mechanisms {(combined with a electro-thermal time delay relay H01H61/002)}	H01H71/14	H01H71/14		345
H01H71/142	11	{actuated due to change of magnetic permeability}	H01H71/14	H01H71/14		118
H01H71/145	11	{using shape memory materials (H01H71/16 takes precedence)}	H01H71/14	H01H71/14		140
H01H2071/147	11	{Thermal release by expansion of a fluid}	H01H71/14	H01H71/14		44
H01H71/16	11	with bimetal element {(combined with detection of imbalance of two or more currents H01H83/223)}	H01H71/16	H01H71/16		1305
H01H71/161	12	{with helically or spirally wound bimetal}	H01H71/16	H01H71/16		71
H01H71/162	12	{with compensation for ambient temperature}	H01H71/16	H01H71/16		305
H01H71/164	12	{Heating elements}	H01H71/16	H01H71/16		323
H01H2071/165	13	{the bimetal being inductively heated, e.g. load current does not pass through bimetal}	H01H71/16	H01H71/16		25
H01H2071/167	12	{Multiple bimetals working in parallel together, e.g. laminated together}	H01H71/16	H01H71/16		24
H01H2071/168	12	{Provisions for avoiding permanent deformation and thus decalibration of bimetal, e.g. due to overheating or action of a magnet}	H01H71/16	H01H71/16		20
H01H71/18	11	with expanding rod, strip, or wire	H01H71/18	H01H71/18		208
H01H71/20	11	with fusible mass	H01H71/20	H01H71/20		404
H01H71/205	12	{using a ratchet wheel kept against rotation by solder}	H01H71/20	H01H71/20		259
H01H71/22	11	with compensation for variation of ambient temperature {(H01H71/162 takes precedence)}	H01H71/22	H01H71/22		43
H01H71/24	10	Electromagnetic mechanisms	H01H71/24	H01H71/24		1603
H01H71/2409	11	{combined with an electromagnetic current limiting mechanism}	H01H71/24	H01H71/24		279
H01H71/2418	11	{combined with an electrodynamic current limiting mechanism}	H01H71/24	H01H71/24		95
H01H2071/2427	12	{with blow-off movement tripping mechanism, e.g. electrodynamic effect on contacts trips the traditional trip device before it can unlatch the spring mechanism by itself}	H01H71/24	H01H71/24		64
H01H71/2436	11	{with a holding and a releasing magnet, the holding force being limited due to saturation of the holding magnet}	H01H71/24	H01H71/24		78
H01H71/2445	11	{using a reed switch (for current measuring G01R19/16509)}	H01H71/24	H01H71/24		101
H01H71/2454	11	{characterised by the magnetic circuit or active magnetic elements}	H01H71/24	H01H71/24		400
H01H71/2463	11	{with plunger type armatures}	H01H71/24	H01H71/24		631
H01H71/2472	11	{with rotatable armatures}	H01H71/24	H01H71/24		602
H01H71/2481	11	{characterised by the coil design}	H01H71/24	H01H71/24		144
H01H2071/249	11	{with part of the magnetic circuit being in the normal current path in the circuit breaker, e.g. yoke, fixed contact and arc-runner are made out of one single conductive element}	H01H71/24	H01H71/24		75
H01H71/26	11	with windings acting in opposition {(H01H71/2436 takes precedence)}	H01H71/26	H01H71/26		160
H01H71/28	11	with windings acting in conjunction	H01H71/28	H01H71/28		58
H01H71/30	11	having additional short-circuited winding	H01H71/30	H01H71/30		24
H01H71/32	11	having permanently magnetised part	H01H71/32	H01H71/32		429
H01H71/321	12	{characterised by the magnetic circuit or active magnetic elements}	H01H71/32	H01H71/32		119
H01H71/322	13	{with plunger type armature}	H01H71/32	H01H71/32		163
H01H71/323	13	{with rotatable armature}	H01H71/32	H01H71/32		155
H01H71/325	12	{Housings, assembly or disposition of different elements in the housing}	H01H71/32	H01H71/32		35
H01H71/326	13	{Sealed housings}	H01H71/32	H01H71/32		15
H01H71/327	12	{Manufacturing or calibrating methods, e.g. air gap treatments}	H01H71/32	H01H71/32		46
H01H2071/328	12	{using a spring for having minimal force on armature while maximal force on trip pin}	H01H71/32	H01H71/32		23
H01H71/34	11	having two or more armatures controlled by a common winding	H01H71/34	H01H71/34		71
H01H71/345	12	{having a delayed movable core and a movable armature}	H01H71/34	H01H71/34		124
H01H71/36	11	frequency selective	H01H71/36	H01H71/36		8
H01H71/38	11	wherein the magnet coil also acts as arc blow-out device	H01H71/38	H01H71/38		103
H01H71/40	10	Combined electrothermal and electromagnetic mechanisms	H01H71/40	H01H71/40		953
H01H71/402	11	{in which the thermal mechanism influences the magnetic circuit of the electromagnetic mechanism}	H01H71/40	H01H71/40		57
H01H71/405	11	{in which a bimetal forms the inductor for the electromagnetic mechanism}	H01H71/40	H01H71/40		135
H01H2071/407	11	{the thermal element being heated by the coil of the electromagnetic mechanism}	H01H71/40	H01H71/40		68
H01H71/42	10	Induction-motor, induced-current, or electrodynamic release mechanisms	H01H71/42	H01H71/42		151
H01H71/43	11	Electrodynamic release mechanisms	H01H71/43	H01H71/43		281
H01H71/44	10	having means for introducing a predetermined time delay (by short-circuited winding H01H71/30; by additional armature H01H71/34)	H01H71/44	H01H71/44		468
H01H71/443	11	{with dash-pot}	H01H71/44	H01H71/44		120
H01H71/446	11	{making use of an inertia mass}	H01H71/44	H01H71/44		54
H01H71/46	10	having means for operating auxiliary contacts additional to the main contacts	H01H71/46	H01H71/46		577
H01H71/462	11	{housed in a separate casing, juxtaposed to and having the same general contour as the main casing (for neutral conductor H01H71/002)}	H01H71/46	H01H71/46		152
H01H71/465	11	{Self-contained, easily replaceable microswitches}	H01H71/46	H01H71/46		161
H01H2071/467	11	{with history indication, e.g. of trip and/or kind of trip, number of short circuits etc.}	H01H71/46	H01H71/46		84
H01H71/48	11	with provision for short-circuiting the electrical input to the release mechanism after release of the switch, e.g. for protection of heating wire	H01H71/48	H01H71/48		79
H01H71/50	9	Manual reset mechanisms {which may be also used for manual release}	H01H71/50	H01H71/50		633
H01H71/501	10	{Means for breaking welded contacts; Indicating contact welding or other malfunction of the circuit breaker}	H01H71/50	H01H71/50		296
H01H2071/502	11	{with direct contact between manual operator and welded contact structure}	H01H71/50	H01H71/50		25
H01H71/503	10	{Means for increasing the opening stroke of the contacts}	H01H71/50	H01H71/50		50
H01H71/504	10	{provided with anti-rebound means}	H01H71/50	H01H71/50		156
H01H71/505	10	{Latching devices between operating and release mechanism}	H01H71/50	H01H71/50		698
H01H2071/506	11	{using balls or rollers in the latching device}	H01H71/50	H01H71/50		113
H01H2071/507	11	{being collapsible, e.g. yielding elastically, when the opening force is higher than a predetermined value}	H01H71/50	H01H71/50		22
H01H2071/508	11	{with serial latches, e.g. primary latch latched by secondary latch for requiring a smaller trip force}	H01H71/50	H01H71/50		93
H01H71/52	10	actuated by lever	H01H71/52	H01H71/52		892
H01H71/521	11	{Details concerning the lever handle}	H01H71/52	H01H71/52		280
H01H71/522	11	{comprising a cradle-mechanism}	H01H71/52	H01H71/52		161
H01H71/523	12	{the contact arm being pivoted on cradle and mechanism spring acting between handle and contact arm}	H01H71/52	H01H71/52		31
H01H71/524	12	{the contact arm being pivoted on handle and mechanism spring acting between cradle and contact arm}	H01H71/52	H01H71/52		92
H01H71/525	12	{comprising a toggle between cradle and contact arm and mechanism spring acting between handle and toggle knee}	H01H71/52	H01H71/52		280
H01H71/526	11	{the lever forming a toggle linkage with a second lever, the free end of which is directly and releasably engageable with a contact structure}	H01H71/52	H01H71/52		325
H01H71/527	11	{making use of a walking beam with one extremity latchable, the other extremity actuating or supporting the movable contact and an intermediate part co-operating with the actuator}	H01H71/52	H01H71/52		74
H01H71/528	11	{comprising a toggle or collapsible link between handle and contact arm, e.g. sear pin mechanism}	H01H71/52	H01H71/52		148
H01H71/529	11	{comprising an electroresponsive element forming part of the transmission chain between handle and contact arm}	H01H71/52	H01H71/52		56
H01H71/54	10	actuated by tumbler	H01H71/54	H01H71/54		88
H01H71/56	10	actuated by rotatable knob or wheel	H01H71/56	H01H71/56		440
H01H2071/565	11	{using a add on unit, e.g. a separate rotary actuator unit, mounted on lever actuated circuit breakers}	H01H71/56	H01H71/56		127
H01H71/58	10	actuated by push-button, pull-knob, or slide	H01H71/58	H01H71/58		579
H01H71/60	10	actuated by closure of switch casing	H01H71/60	H01H71/60		9
H01H71/62	10	with means for preventing resetting while abnormal condition persists, e.g. loose handle arrangement	H01H71/62	H01H71/62		141
H01H71/64	11	incorporating toggle linkage	H01H71/64	H01H71/64		22
H01H71/66	9	Power reset mechanisms	H01H71/66	H01H71/66		173
H01H2071/665	10	{the reset mechanism operating directly on the normal manual operator, e.g. electromagnet pushes manual release lever back into "ON" position}	H01H71/66	H01H71/66		213
H01H71/68	10	actuated by electromagnet	H01H71/68	H01H71/68		535
H01H71/685	11	{in which the excitation of the electromagnet is interrupted by abnormal conditions}	H01H71/68	H01H71/68		61
H01H71/70	10	actuated by electric motor	H01H71/70	H01H71/70		654
H01H71/72	10	actuated automatically a limited number of times	H01H71/72	H01H71/72		8
H01H71/74	8	Means for adjusting the conditions under which the device will function to provide protection	H01H71/74	H01H71/74		347
H01H71/7409	9	{Interchangeable elements}	H01H71/74	H01H71/74		223
H01H71/7418	9	{Adjusting both electrothermal and electromagnetic mechanism}	H01H71/74	H01H71/74		107
H01H71/7427	9	{Adjusting only the electrothermal mechanism}	H01H71/74	H01H71/74		230
H01H71/7436	10	{Adjusting the position (or prestrain) of the bimetal (H01H71/7445 takes precedence)}	H01H71/74	H01H71/74		193
H01H71/7445	10	{Poly-phase adjustment}	H01H71/74	H01H71/74		108
H01H2071/7454	10	{with adjustable axis of transmission lever between bimetal element and trip lever}	H01H71/74	H01H71/74		39
H01H71/7463	9	{Adjusting only the electromagnetic mechanism}	H01H71/74	H01H71/74		391
H01H2071/7472	9	{with antitamper means for avoiding unauthorised setting}	H01H71/74	H01H71/74		47
H01H2071/7481	9	{with indexing means for magnetic or thermal tripping adjustment knob}	H01H71/74	H01H71/74		92
H01H2071/749	9	{with a shunt element connected in parallel to magnetic or thermal trip elements, e.g. for adjusting trip current}	H01H71/74	H01H71/74		53
H01H73/00	7	Protective overload circuit-breaking switches in which excess current opens the contacts by automatic release of mechanical energy stored by previous operation of a hand reset mechanism	H01H73/00	H01H73/00		94
H01H73/02	8	Details	H01H73/02	H01H73/02		143
H01H73/04	9	Contacts	H01H73/04	H01H73/04		1212
H01H73/045	10	{Bridging contacts}	H01H73/04	H01H73/04		488
H01H73/06	9	Housings; Casings; Bases; Mountings	H01H73/06	H01H73/06		256
H01H73/08	10	Plug-in housings	H01H73/08	H01H73/08		135
H01H73/10	10	Cartridge housings, e.g. screw-in housing	H01H73/10	H01H73/10		68
H01H73/12	9	Means for indicating condition of the switch	H01H73/12	H01H73/12		76
H01H73/14	10	Indicating lamp structurally associated with the switch	H01H73/14	H01H73/14		157
H01H73/16	9	Distinguishing marks, e.g. colour coding	H01H73/16	H01H73/16		6
H01H73/18	9	Means for extinguishing or suppressing arc {(magnet coil acting as blow-out device H01H71/38)}	H01H73/18	H01H73/18		2155
H01H73/20	9	Terminals; Connections	H01H73/20	H01H73/20		148
H01H73/22	8	having electrothermal release and no other automatic release (cartridge type H01H73/62)	H01H73/22	H01H73/22		48
H01H73/24	9	reset by lever	H01H73/24	H01H73/24		217
H01H73/26	9	reset by tumbler	H01H73/26	H01H73/26		162
H01H73/28	9	reset by rotatable knob or wheel	H01H73/28	H01H73/28		90
H01H73/30	9	reset by push-button, pull-knob or slide	H01H73/30	H01H73/30		585
H01H73/303	10	{with an insulating body insertable between the contacts when released by a bimetal element}	H01H73/30	H01H73/30		102
H01H73/306	10	{the push-button supporting pivotally a combined contact-latch lever}	H01H73/30	H01H73/30		94
H01H73/32	9	reset by closure of switch casing	H01H73/32	H01H73/32		3
H01H73/34	9	reset action requiring replacement or reconditioning of a fusible or explosive part	H01H73/34	H01H73/34		37
H01H73/36	8	having electromagnetic release and no other automatic release (cartridge type H01H73/64)	H01H73/36	H01H73/36		94
H01H73/38	9	reset by lever	H01H73/38	H01H73/38		172
H01H73/40	9	reset by tumbler	H01H73/40	H01H73/40		22
H01H73/42	9	reset by rotatable knob or wheel	H01H73/42	H01H73/42		139
H01H73/44	9	reset by push-button, pull-knob or slide	H01H73/44	H01H73/44		171
H01H73/46	9	reset by closure of switch casing	H01H73/46	H01H73/46		1
H01H73/48	8	having both electrothermal and electromagnetic automatic release (cartridge type H01H73/66)	H01H73/48	H01H73/48		35
H01H73/50	9	reset by lever	H01H73/50	H01H73/50		213
H01H73/52	9	reset by tumbler	H01H73/52	H01H73/52		20
H01H73/54	9	reset by rotatable knob or wheel	H01H73/54	H01H73/54		23
H01H73/56	9	reset by push-button, pull-knob or slide	H01H73/56	H01H73/56		195
H01H73/58	9	reset by closure of switch casing	H01H73/58	H01H73/58		
H01H73/60	8	cartridge type, e.g. screw-in cartridge	H01H73/60	H01H73/60		278
H01H73/62	9	having only electrothermal release	H01H73/62	H01H73/62		16
H01H73/64	9	having only electromagnetic release	H01H73/64	H01H73/64		14
H01H73/66	9	having combined electrothermal and electromagnetic release	H01H73/66	H01H73/66		12
H01H75/00	7	Protective overload circuit-breaking switches in which excess current opens the contacts by automatic release of mechanical energy stored by previous operation of power reset mechanism	H01H75/00	H01H75/00		31
H01H75/02	8	Details	H01H75/02	H01H75/02		15
H01H75/04	9	Reset mechanisms for automatically reclosing a limited number of times (circuit arrangements H02H3/06)	H01H75/04	H01H75/04		644
H01H75/06	10	effecting one reclosing action only	H01H75/06	H01H75/06		53
H01H75/08	8	having only electrothermal release	H01H75/08	H01H75/08		10
H01H75/10	8	having only electromagnetic release	H01H75/10	H01H75/10		22
H01H75/12	8	having combined electrothermal and electromagnetic release	H01H75/12	H01H75/12		5
H01H77/00	7	Protective overload circuit-breaking switches operated by excess current and requiring separate action for resetting (H01H73/00, H01H75/00 take precedence)	H01H77/00	H01H77/00		22
H01H77/02	8	in which the excess current itself provides the energy for opening the contacts, and having a separate reset mechanism	H01H77/02	H01H77/02		46
H01H2077/025	9	{with pneumatic means, e.g. by arc pressure}	H01H77/02	H01H77/02		78
H01H77/04	9	with electrothermal opening	H01H77/04	H01H77/04		169
H01H77/06	9	with electromagnetic opening {(combined with electromagnetic release mechanism H01H71/2409)}	H01H77/06	H01H77/06		111
H01H77/08	10	retained closed by permanent or remanent magnetism and opened by windings acting in opposition	H01H77/08	H01H77/08		38
H01H77/10	9	with electrodynamic opening {(combined with electromagnetic release mechanism H01H71/2418)}	H01H77/10	H01H77/10		236
H01H77/101	10	{with increasing of contact pressure by electrodynamic forces before opening}	H01H77/10	H01H77/10		71
H01H77/102	10	{characterised by special mounting of contact arm, allowing blow-off movement}	H01H77/10	H01H77/10		126
H01H77/104	11	{with a stable blow-off position}	H01H77/10	H01H77/10		232
H01H77/105	11	{whereby the blow-off movement unlatches the contact from a contact holder}	H01H77/10	H01H77/10		37
H01H77/107	10	{characterised by the blow-off force generating means, e.g. current loops}	H01H77/10	H01H77/10		78
H01H77/108	11	{comprising magnetisable elements, e.g. flux concentrator, linear slot motor}	H01H77/10	H01H77/10		112
H01H79/00	7	Protective switches in which excess current causes the closing of contacts, e.g. for short-circuiting the apparatus to be protected {(H01H39/004 takes precedence)}	H01H79/00	H01H79/00		371
H01H81/00	7	Protective switches in which contacts are normally closed but are repeatedly opened and reclosed as long as a condition causing excess current persists, e.g. for current limiting	H01H81/00	H01H81/00		31
H01H81/02	8	electrothermally operated	H01H81/02	H01H81/02		193
H01H81/04	8	electromagnetically operated	H01H81/04	H01H81/04		45
H01H83/00	7	Protective switches, e.g. circuit-breaking switches, or protective relays operated by abnormal electrical conditions otherwise than solely by excess current	H01H83/00	H01H83/00		204
H01H83/02	8	operated by earth fault currents (H01H83/14 takes precedence)	H01H83/02	H01H83/02		675
H01H83/04	9	with testing means for indicating the ability of the switch or relay to function properly	H01H83/04	H01H83/04		838
H01H2083/045	10	{Auxiliary switch opening testing circuit in synchronism with the main circuit}	H01H83/04	H01H83/04		111
H01H83/06	8	operated by current falling below a predetermined value	H01H83/06	H01H83/06		72
H01H83/08	8	operated by reversal of DC	H01H83/08	H01H83/08		141
H01H83/10	8	operated by excess voltage, e.g. for lightning protection	H01H83/10	H01H83/10		288
H01H83/12	8	operated by voltage falling below a predetermined value, e.g. for no-volt protection	H01H83/12	H01H83/12		480
H01H83/14	8	operated by imbalance of two or more currents or voltages, e.g. for differential protection	H01H83/14	H01H83/14		252
H01H83/142	9	{with bimetal elements}	H01H83/14	H01H83/14		27
H01H83/144	9	{with differential transformer}	H01H83/14	H01H83/14		433
H01H2083/146	10	{Provisions for avoiding disadvantages of having asymetrical primaries, e.g. induction of a magnetic field even by zero difference current}	H01H83/14	H01H83/14		34
H01H2083/148	10	{with primary windings formed of rigid copper conductors}	H01H83/14	H01H83/14		48
H01H83/16	8	operated by abnormal ratio of voltage and current, e.g. distance relay	H01H83/16	H01H83/16		17
H01H83/18	8	operated by abnormal product of, or abnormal phase angle between, voltage and current, e.g. directional relay	H01H83/18	H01H83/18		18
H01H83/20	8	operated by excess current as well as by some other abnormal electrical condition	H01H83/20	H01H83/20		685
H01H2083/201	9	{the other abnormal electrical condition being an arc fault}	H01H83/20	H01H83/20		212
H01H2083/203	9	{with shunt trip circuits, e.g. NC contact in an undervoltage coil circuit}	H01H83/20	H01H83/20		75
H01H2083/205	9	{having shunt or UVR tripping device with integrated mechanical energy accumulator}	H01H83/20	H01H83/20		70
H01H2083/206	9	{with thermal shunt trip}	H01H83/20	H01H83/20		31
H01H2083/208	9	{Converting under voltage release [UVR] and shunt release}	H01H83/20	H01H83/20		52
H01H83/22	9	the other condition being imbalance of two or more currents or voltages	H01H83/22	H01H83/22		104
H01H83/223	10	{with bimetal elements}	H01H83/22	H01H83/22		296
H01H83/226	10	{with differential transformer}	H01H83/22	H01H83/22		255
H01H85/00	7	Protective devices in which the current flows through a part of fusible material and this current is interrupted by displacement of the fusible material when this current becomes excessive (switches actuated by melting of fusible material H01H37/76; disposition or arrangement of fuses on boards H02B1/18)	H01H85/00	H01H85/00		270
H01H2085/0004	8	{making use of shape-memory material}	H01H85/00	H01H85/00		47
H01H2085/0008	8	{making use of heat shrinkable material}	H01H85/00	H01H85/00		37
H01H85/0013	8	{Means for preventing damage, e.g. by ambient influences to the fuse}	H01H85/00	H01H85/00		83
H01H85/0017	9	{due to vibration or other mechanical forces, e.g. centrifugal forces}	H01H85/00	H01H85/00		81
H01H85/0021	9	{water or dustproof devices}	H01H85/00	H01H85/00		75
H01H85/0026	10	{casings for the fuse and its base contacts}	H01H85/00	H01H85/00		158
H01H85/003	10	{casings for the fusible element}	H01H85/00	H01H85/00		188
H01H2085/0034	10	{with molded casings}	H01H85/00	H01H85/00		86
H01H85/0039	8	{Means for influencing the rupture process of the fusible element}	H01H85/00	H01H85/00		84
H01H85/0043	9	{Boiling of a material associated with the fusible element, e.g. surrounding fluid}	H01H85/00	H01H85/00		19
H01H85/0047	9	{Heating means}	H01H85/00	H01H85/00		93
H01H85/0052	10	{Fusible element and series heating means or series heat dams}	H01H85/00	H01H85/00		117
H01H85/0056	10	{Heat conducting or heat absorbing means associated with the fusible member, e.g. for providing time delay}	H01H85/00	H01H85/00		53
H01H85/006	10	{Heat reflective or insulating layer on the casing or on the fuse support}	H01H85/00	H01H85/00		29
H01H85/0065	10	{Heat reflective or insulating layer on the fusible element}	H01H85/00	H01H85/00		19
H01H85/0069	10	{Heat reflective or insulating filler, support, or block forming the casing}	H01H85/00	H01H85/00		21
H01H85/0073	9	{Expansion or rupture of the insulating support for the fusible element}	H01H85/00	H01H85/00		42
H01H85/0078	8	{Security-related arrangements}	H01H85/00	H01H85/00		71
H01H85/0082	9	{preventing explosion of the cartridge}	H01H85/00	H01H85/00		50
H01H85/0086	10	{use of a flexible body, e.g. inside the casing}	H01H85/00	H01H85/00		14
H01H85/0091	9	{providing disconnection of the neutral line}	H01H85/00	H01H85/00		31
H01H85/0095	9	{Earthing means}	H01H85/00	H01H85/00		18
H01H85/02	8	Details	H01H85/02	H01H85/02		585
H01H85/0208	9	{Tools for inserting and removing fuses}	H01H85/02	H01H85/02		613
H01H2085/0216	9	{Tools for controlling fuses or the line associated with the fuses}	H01H85/02	H01H85/02		98
H01H2085/0225	9	{Means for preventing discharge, e.g. corona ring}	H01H85/02	H01H85/02		113
H01H2085/0233	9	{with common casing for fusible elements inserted in more than one phase or more than one circuit}	H01H85/02	H01H85/02		59
H01H85/0241	9	{Structural association of a fuse and another component or apparatus (switches with built-in fuses H01H9/10, spark-gap arresters H01H85/44, transformers and inductances H01F27/402, capacitors H01G2/14, lamps H01K1/66, semiconductors H10W20/493 or H10W42/80)}	H01H85/02	H01H85/02		1055
H01H2085/025	10	{Structural association with a binding post of a storage battery}	H01H85/02	H01H85/02		288
H01H2085/0258	10	{Structural association of a fuse or a fuse holder with a bimetallic element}	H01H85/02	H01H85/02		77
H01H2085/0266	10	{Structural association with a measurement device, e.g. a shunt}	H01H85/02	H01H85/02		145
H01H2085/0275	10	{Structural association with a printed circuit board}	H01H85/02	H01H85/02		183
H01H2085/0283	10	{Structural association with a semiconductor device}	H01H85/02	H01H85/02		123
H01H2085/0291	10	{Structural association with a current transformer}	H01H85/02	H01H85/02		100
H01H85/04	9	Fuses, i.e. expendable parts of the protective device, e.g. cartridges	H01H85/04	H01H85/04		497
H01H85/041	10	characterised by the type	H01H85/041	H01H85/041		157
H01H85/0411	11	{Miniature fuses}	H01H85/041	H01H85/041		382
H01H2085/0412	12	{specially adapted for being mounted on a printed circuit board}	H01H85/041	H01H85/041		131
H01H2085/0414	12	{Surface mounted fuses}	H01H85/041	H01H85/041		236
H01H85/0415	12	{cartridge type}	H01H85/041	H01H85/041		33
H01H85/0417	13	{with parallel side contacts}	H01H85/041	H01H85/041		398
H01H85/0418	13	{with ferrule type end contacts}	H01H85/041	H01H85/041		77
H01H85/042	11	General constructions or structure of high voltage fuses, i.e. above 1000 V	H01H85/042	H01H85/042		597
H01H85/044	11	General constructions or structure of low voltage fuses, i.e. below 1000 V, or of fuses where the applicable voltage is not specified (H01H85/046&#160;-&#160;H01H85/048 take precedence)	H01H85/044	H01H85/044		598
H01H85/0445	12	fast or slow type (H01H85/045&#160;-&#160;H01H85/048 take precedence)	H01H85/0445	H01H85/0445		27
H01H85/045	12	cartridge type	H01H85/045	H01H85/045		38
H01H85/0452	13	{with parallel side contacts}	H01H85/045	H01H85/045		127
H01H85/0454	13	{with screw-in type contacts}	H01H85/045	H01H85/045		283
H01H85/0456	13	{with knife-blade end contacts}	H01H85/045	H01H85/045		184
H01H85/0458	13	{with ferrule type end contacts}	H01H85/045	H01H85/045		129
H01H85/046	11	Fuses formed as printed circuits	H01H85/046	H01H85/046		655
H01H85/047	11	Vacuum fuses	H01H85/047	H01H85/047		66
H01H85/048	11	Fuse resistors	H01H85/048	H01H85/048		207
H01H2085/0483	12	{with temperature dependent resistor, e.g. thermistor}	H01H85/048	H01H85/048		83
H01H2085/0486	12	{with voltage dependent resistor, e.g. varistor}	H01H85/048	H01H85/048		79
H01H85/05	10	Component parts thereof	H01H85/05	H01H85/05		234
H01H85/055	11	Fusible members	H01H85/055	H01H85/055		933
H01H2085/0555	12	{Input terminal connected to a plurality of output terminals, e.g. multielectrode}	H01H85/055	H01H85/055		221
H01H85/06	12	characterised by the fusible material (H01H85/11 takes precedence)	H01H85/06	H01H85/06		667
H01H85/08	12	characterised by the shape or form of the fusible member	H01H85/08	H01H85/08		615
H01H85/10	13	with constriction for localised fusing (H01H85/11 takes precedence)	H01H85/10	H01H85/10		547
H01H85/11	13	with applied local area of a metal which, on melting, forms a eutectic with the main material of the fusible member, i.e. M-effect devices	H01H85/11	H01H85/11		167
H01H85/12	12	Two or more separate fusible members in parallel	H01H85/12	H01H85/12		367
H01H85/143	11	Electrical contacts; Fastening fusible members to such contacts	H01H85/143	H01H85/143		881
H01H85/147	12	Parallel-side contacts	H01H85/147	H01H85/147		112
H01H85/15	12	Screw-in contacts	H01H85/15	H01H85/15		81
H01H85/153	12	Knife-blade-end contacts	H01H85/153	H01H85/153		383
H01H85/157	12	Ferrule-end contacts	H01H85/157	H01H85/157		363
H01H85/165	11	Casings	H01H85/165	H01H85/165		757
H01H85/17	12	characterised by the casing material	H01H85/17	H01H85/17		175
H01H85/175	12	characterised by the casing shape or form	H01H85/175	H01H85/175		447
H01H85/1755	13	{composite casing}	H01H85/175	H01H85/175		123
H01H85/18	11	Casing fillings, e.g. powder	H01H85/18	H01H85/18		401
H01H85/185	12	{Insulating members for supporting fusible elements inside a casing, e.g. for helically wound fusible elements}	H01H85/18	H01H85/18		164
H01H85/20	9	Bases for supporting the fuse; Separate parts thereof	H01H85/20	H01H85/20		1703
H01H85/2005	10	{for use with screw-in type fuse}	H01H85/20	H01H85/20		372
H01H85/201	10	{for connecting a fuse in a lead and adapted to be supported by the lead alone}	H01H85/20	H01H85/20		290
H01H85/2015	10	{for plug-in type fuses}	H01H85/20	H01H85/20		132
H01H85/202	10	{for fuses with ferrule type end contacts}	H01H85/20	H01H85/20		354
H01H85/2025	10	{for fuses with conical end contacts, e.g. fuses used on motor vehicles}	H01H85/20	H01H85/20		73
H01H85/203	10	{for fuses with blade type terminals}	H01H85/20	H01H85/20		184
H01H85/2035	11	{for miniature fuses with parallel side contacts}	H01H85/20	H01H85/20		294
H01H85/204	11	{for low voltage fuses with knife-blade end contacts}	H01H85/20	H01H85/20		376
H01H85/2045	10	{Mounting means or insulating parts of the base, e.g. covers, casings}	H01H85/20	H01H85/20		928
H01H85/205	10	{Electric connections to contacts on the base}	H01H85/20	H01H85/20		579
H01H2085/2055	11	{Connections to bus bars in an installation with screw in type fuses or knife blade fuses}	H01H85/20	H01H85/20		172
H01H2085/206	11	{being tappable, e.g. terminals on the fuse or base being arranged so as to permit an additional connector to be engaged therewith}	H01H85/20	H01H85/20		122
H01H2085/2065	10	{with base contacts adapted or adaptable to fuses of different lenghts;  bases with self-aligning contacts;  intermediate adaptation pieces}	H01H85/20	H01H85/20		98
H01H2085/207	10	{Bases adapted to fuses with different end contacts or to other components, e.g. circuit breakers;  intermediate adaptation pieces}	H01H85/20	H01H85/20		60
H01H2085/2075	10	{Junction box, having holders integrated with several other holders in a particular wiring layout}	H01H85/20	H01H85/20		210
H01H2085/208	11	{specially adapted for vehicles}	H01H85/20	H01H85/20		659
H01H2085/2085	10	{Holders for mounting a fuse on a printed circuit}	H01H85/20	H01H85/20		139
H01H2085/209	10	{Modular assembly of fuses or holders, e.g. side by side;  combination of a plurality of identical fuse units}	H01H85/20	H01H85/20		153
H01H2085/2095	10	{Triangular setup of fuses, e.g. for space saving}	H01H85/20	H01H85/20		27
H01H85/22	9	Intermediate or auxiliary parts for carrying, holding, or retaining fuse, co-operating with base or fixed holder, and removable therefrom for renewing the fuse	H01H85/22	H01H85/22		626
H01H85/24	9	Means for preventing insertion of incorrect fuse	H01H85/24	H01H85/24		462
H01H85/25	9	Safety arrangements preventing or inhibiting contact with live parts, including operation of isolation on removal of cover	H01H85/25	H01H85/25		229
H01H85/26	9	Magazine arrangements	H01H85/26	H01H85/26		712
H01H85/263	10	{with spare printed circuit fuse}	H01H85/26	H01H85/26		32
H01H2085/266	10	{with replacement of a fuse which is part of a printed circuit}	H01H85/26	H01H85/26		29
H01H85/28	10	effecting automatic replacement	H01H85/28	H01H85/28		262
H01H85/30	9	Means for indicating condition of fuse structurally associated with the fuse	H01H85/30	H01H85/30		747
H01H85/303	10	{Movable indicating elements}	H01H85/30	H01H85/30		468
H01H85/306	11	{acting on an auxiliary switch or contact}	H01H85/30	H01H85/30		275
H01H85/32	10	Indicating lamp structurally associated with the protective device	H01H85/32	H01H85/32		562
H01H85/34	9	Distinguishing marks, e.g. colour coding	H01H85/34	H01H85/34		120
H01H85/36	9	Means for applying mechanical tension to fusible member	H01H85/36	H01H85/36		565
H01H85/38	9	Means for extinguishing or suppressing arc (by powder filling H01H85/18; by mechanical tension applied to fusible member H01H85/36)	H01H85/38	H01H85/38		870
H01H2085/381	10	{with insulating body insertable between the end contacts of the fusible element}	H01H85/38	H01H85/38		45
H01H2085/383	10	{with insulating stationary parts}	H01H85/38	H01H85/38		111
H01H2085/385	10	{Impedances connected with the end contacts of the fusible element}	H01H85/38	H01H85/38		15
H01H2085/386	10	{with magnetic or electrodynamic arc-blowing}	H01H85/38	H01H85/38		83
H01H2085/388	10	{using special materials}	H01H85/38	H01H85/38		173
H01H85/40	10	using an arc-extinguishing liquid (characterised by the composition of the liquid H01H33/22)	H01H85/40	H01H85/40		127
H01H85/42	10	using an arc-extinguishing gas (characterised by the composition of the gas H01H33/22)	H01H85/42	H01H85/42		497
H01H85/43	9	Means for exhausting or absorbing gases liberated by fusing arc, or for ventilating excess pressure generated by heating	H01H85/43	H01H85/43		146
H01H85/44	9	Structural association with a spark-gap arrester	H01H85/44	H01H85/44		299
H01H85/46	9	Circuit arrangements not adapted to a particular application of the protective device	H01H85/46	H01H85/46		331
H01H85/463	10	{with printed circuit fuse}	H01H85/46	H01H85/46		66
H01H2085/466	10	{with remote controlled forced fusing}	H01H85/46	H01H85/46		236
H01H85/47	9	Means for cooling	H01H85/47	H01H85/47		331
H01H85/48	8	Protective devices wherein the fuse is carried or held directly by the base	H01H85/48	H01H85/48		110
H01H85/485	9	{the fuse being provided with bayonet-type locking means}	H01H85/48	H01H85/48		14
H01H85/50	9	the fuse having contacts at opposite ends for co-operation with the base	H01H85/50	H01H85/50		28
H01H85/52	9	the fuse being adapted for screwing into the base	H01H85/52	H01H85/52		20
H01H85/54	8	Protective devices wherein the fuse is carried, held, or retained by an intermediate or auxiliary part removable from the base, or used as sectionalisers	H01H85/54	H01H85/54		387
H01H85/542	9	{the intermediate or auxiliary part being provided with bayonet-type locking means}	H01H85/54	H01H85/54		175
H01H85/545	9	{with pivoting fuse carrier (tumbler switch with built-in fuse H01H23/10)}	H01H85/54	H01H85/54		165
H01H85/547	9	{with sliding fuse carrier}	H01H85/54	H01H85/54		239
H01H85/56	9	the intermediate or auxiliary part having side contacts for plugging into the base, e.g. bridge-carrier type	H01H85/56	H01H85/56		122
H01H85/58	10	with intermediate auxiliary part and base shaped to interfit and thereby enclose the fuse	H01H85/58	H01H85/58		12
H01H85/60	9	the intermediate or auxiliary part having contacts at opposite ends for co-operation with the base	H01H85/60	H01H85/60		20
H01H85/62	9	the intermediate or auxiliary part being adapted for screwing into the base	H01H85/62	H01H85/62		226
H01H87/00	7	Protective devices in which a current flowing through a liquid or solid is interrupted by the evaporation of the liquid or by the melting and evaporation of the solid when the current becomes excessive, the circuit continuity being reestablished on cooling	H01H87/00	H01H87/00		266
H01H89/00	7	Combinations of two or more different basic types of electric switches, relays, selectors and emergency protective devices, not covered by any single one of the other main groups of this subclass	H01H89/00	H01H89/00		400
H01H2089/005	8	{Multi-purpose combinations, e.g. LS/DI, LS/FI, of normal protective circuit breakers with known other forms of protection, e.g. earthfaults, differential, imbalance}	H01H89/00	H01H89/00		43
H01H89/02	8	Combination of a key operated switch with a manually operated switch, e.g. ignition and lighting switches	H01H89/02	H01H89/02		126
H01H89/04	8	Combination of a thermally actuated switch with a manually operated switch	H01H89/04	H01H89/04		277
H01H89/06	8	Combination of a manual reset circuit with a contactor, i.e. the same circuit controlled by both a protective and a remote control device	H01H89/06	H01H89/06		220
H01H2089/065	9	{Coordination between protection and remote control, e.g. protection job repartition, mutual assistance or monitoring}	H01H89/06	H01H89/06		58
H01H89/08	9	with both devices using the same contact pair	H01H89/08	H01H89/08		161
H01H89/10	10	with each device controlling one of the two co-operating contacts	H01H89/10	H01H89/10		23
H01H2201/00	7	Contacts	CPCONLY	H01H2201/00		10
H01H2201/002	8	bounceless	CPCONLY	H01H2201/002		46
H01H2201/004	8	Wiping action	CPCONLY	H01H2201/004		27
H01H2201/006	8	self-aligning	CPCONLY	H01H2201/006		4
H01H2201/008	8	Both contacts movable	CPCONLY	H01H2201/008		50
H01H2201/01	8	Protective enclosure	CPCONLY	H01H2201/01		7
H01H2201/012	9	Inert gas in contact space	CPCONLY	H01H2201/012		12
H01H2201/014	9	Conductive gas	CPCONLY	H01H2201/014		3
H01H2201/016	8	Roughened contact surface, e.g. anti-adhering	CPCONLY	H01H2201/016		13
H01H2201/018	8	transparent	CPCONLY	H01H2201/018		38
H01H2201/02	8	Piezo element	CPCONLY	H01H2201/02		107
H01H2201/022	8	Material	CPCONLY	H01H2201/022		29
H01H2201/024	9	precious	CPCONLY	H01H2201/024		62
H01H2201/026	9	non precious	CPCONLY	H01H2201/026		133
H01H2201/028	10	Indium tin oxide [ITO]	CPCONLY	H01H2201/028		41
H01H2201/03	9	Composite	CPCONLY	H01H2201/03		108
H01H2201/032	9	Conductive polymer; Rubber	CPCONLY	H01H2201/032		182
H01H2201/034	10	anisotropic; Zebra	CPCONLY	H01H2201/034		17
H01H2201/036	10	Variable resistance	CPCONLY	H01H2201/036		252
H01H2201/038	8	Contact lubricant	CPCONLY	H01H2201/038		9
H01H2203/00	7	Form of contacts	CPCONLY	H01H2203/00		31
H01H2203/002	8	Raised edge	CPCONLY	H01H2203/002		19
H01H2203/004	8	Rivet	CPCONLY	H01H2203/004		14
H01H2203/006	8	Staples	CPCONLY	H01H2203/006		13
H01H2203/008	8	Wires	CPCONLY	H01H2203/008		48
H01H2203/0085	9	Layered switches integrated into garment, clothes or textile	CPCONLY	H01H2203/0085		114
H01H2203/01	9	Woven wire screen	CPCONLY	H01H2203/01		79
H01H2203/012	8	Microprotrusions	CPCONLY	H01H2203/012		23
H01H2203/014	9	Grains; Microspheres	CPCONLY	H01H2203/014		7
H01H2203/016	8	universal; modular	CPCONLY	H01H2203/016		17
H01H2203/018	8	binary coded	CPCONLY	H01H2203/018		15
H01H2203/02	8	Interspersed fingers	CPCONLY	H01H2203/02		159
H01H2203/022	8	Helical networks	CPCONLY	H01H2203/022		28
H01H2203/024	8	Convex contact surface	CPCONLY	H01H2203/024		41
H01H2203/026	8	on different planes	CPCONLY	H01H2203/026		32
H01H2203/028	8	embedded in layer material	CPCONLY	H01H2203/028		37
H01H2203/03	8	printed on casing	CPCONLY	H01H2203/03		23
H01H2203/032	8	Metal foil	CPCONLY	H01H2203/032		40
H01H2203/034	8	Common bus	CPCONLY	H01H2203/034		12
H01H2203/036	8	to solve particular problems	CPCONLY	H01H2203/036		25
H01H2203/038	9	to be bridged by a dome shaped contact	CPCONLY	H01H2203/038		179
H01H2203/04	9	to facilitate connections	CPCONLY	H01H2203/04		37
H01H2203/042	9	to avoid cross-overs	CPCONLY	H01H2203/042		16
H01H2203/044	9	to achieve a predetermined sequence of switching	CPCONLY	H01H2203/044		33
H01H2203/046	9	to save ink	CPCONLY	H01H2203/046		5
H01H2203/048	9	to facilitate application	CPCONLY	H01H2203/048		5
H01H2203/05	9	to avoid damage by deformation of layers	CPCONLY	H01H2203/05		25
H01H2203/052	9	for backlighted keyboards	CPCONLY	H01H2203/052		56
H01H2203/054	9	for redundancy, e.g. several contact pairs in parallel	CPCONLY	H01H2203/054		81
H01H2203/056	8	Cuts or depressions in support, e.g. to isolate contacts	CPCONLY	H01H2203/056		30
H01H2203/058	8	Contact area function of position on layered keyboard	CPCONLY	H01H2203/058		6
H01H2205/00	7	Movable contacts	CPCONLY	H01H2205/00		8
H01H2205/002	8	fixed to operating part	CPCONLY	H01H2205/002		277
H01H2205/004	8	fixed to substrate	CPCONLY	H01H2205/004		64
H01H2205/006	8	mounted on spacer	CPCONLY	H01H2205/006		25
H01H2205/008	9	Hollow rivet	CPCONLY	H01H2205/008		1
H01H2205/01	8	mounted on flap cut out and bend out of layer	CPCONLY	H01H2205/01		17
H01H2205/012	8	mounted on both sides of layer	CPCONLY	H01H2205/012		9
H01H2205/014	8	fixed by mechanical deformation	CPCONLY	H01H2205/014		7
H01H2205/016	8	Separate bridge contact	CPCONLY	H01H2205/016		158
H01H2205/018	9	Support points upwardly concave	CPCONLY	H01H2205/018		26
H01H2205/02	9	avoiding rotation	CPCONLY	H01H2205/02		10
H01H2205/022	9	Conductive rubber	CPCONLY	H01H2205/022		35
H01H2205/024	9	Means to facilitate positioning	CPCONLY	H01H2205/024		59
H01H2205/026	10	Adhesive sheet	CPCONLY	H01H2205/026		145
H01H2205/028	10	Protuberances on substrate	CPCONLY	H01H2205/028		22
H01H2205/03	10	Apertured plate	CPCONLY	H01H2205/03		60
H01H2205/032	8	Several contacts formed in one plate or layer	CPCONLY	H01H2205/032		59
H01H2205/034	9	with snap action	CPCONLY	H01H2205/034		21
H01H2205/036	9	Helicoidal cuts	CPCONLY	H01H2205/036		2
H01H2205/038	9	Cutting of connecting areas	CPCONLY	H01H2205/038		13
H01H2207/00	7	Connections	CPCONLY	H01H2207/00		38
H01H2207/002	8	Conductive rubber; Zebra	CPCONLY	H01H2207/002		61
H01H2207/004	8	Printed circuit tail	CPCONLY	H01H2207/004		159
H01H2207/006	8	Upraised portions	CPCONLY	H01H2207/006		2
H01H2207/008	8	Adhesive means; Conductive adhesive	CPCONLY	H01H2207/008		82
H01H2207/01	8	from bottom to top layer	CPCONLY	H01H2207/01		93
H01H2207/012	8	via underside of substrate	CPCONLY	H01H2207/012		51
H01H2207/014	9	Plated through holes	CPCONLY	H01H2207/014		46
H01H2207/016	8	Jumpers; Cross-overs	CPCONLY	H01H2207/016		41
H01H2207/018	9	Spacer elements	CPCONLY	H01H2207/018		9
H01H2207/02	8	Solder	CPCONLY	H01H2207/02		56
H01H2207/022	8	Plug	CPCONLY	H01H2207/022		92
H01H2207/024	9	in top layer	CPCONLY	H01H2207/024		12
H01H2207/026	8	Pressure contact	CPCONLY	H01H2207/026		63
H01H2207/028	8	on spacer	CPCONLY	H01H2207/028		10
H01H2207/03	8	via return spring	CPCONLY	H01H2207/03		14
H01H2207/032	8	Surface mounted component	CPCONLY	H01H2207/032		63
H01H2207/034	8	sealed	CPCONLY	H01H2207/034		13
H01H2207/036	8	Crimping connector	CPCONLY	H01H2207/036		11
H01H2207/038	8	Conductive paste	CPCONLY	H01H2207/038		10
H01H2207/04	8	Details of printed conductors	CPCONLY	H01H2207/04		46
H01H2207/042	9	Covering maximal area of layer	CPCONLY	H01H2207/042		1
H01H2207/044	9	Resist layer	CPCONLY	H01H2207/044		18
H01H2207/046	9	Non overlapping lower and upper conductors	CPCONLY	H01H2207/046		2
H01H2207/048	8	Inductive or infrared coupling	CPCONLY	H01H2207/048		99
H01H2209/00	7	Layers	CPCONLY	H01H2209/00		7
H01H2209/002	8	Materials	CPCONLY	H01H2209/002		310
H01H2209/0021	9	with metallic appearance, e.g. polymers with dispersed particles to produce a metallic appearance	CPCONLY	H01H2209/0021		86
H01H2209/004	8	Depressions or protrusions on switch sites	CPCONLY	H01H2209/004		76
H01H2209/006	8	Force isolators	CPCONLY	H01H2209/006		131
H01H2209/01	8	Increasing rigidity; Anti-creep	CPCONLY	H01H2209/01		106
H01H2209/012	8	avoiding too large deformation or stress	CPCONLY	H01H2209/012		46
H01H2209/014	8	composed of different layers; Lubricant in between	CPCONLY	H01H2209/014		125
H01H2209/016	8	Protection layer, e.g. for legend, anti-scratch	CPCONLY	H01H2209/016		243
H01H2209/018	8	flat, smooth or ripple-free	CPCONLY	H01H2209/018		26
H01H2209/02	8	UV or light sensitive	CPCONLY	H01H2209/02		70
H01H2209/022	8	Velvet; Mat finish	CPCONLY	H01H2209/022		29
H01H2209/024	8	Properties of the substrate	CPCONLY	H01H2209/024		13
H01H2209/026	9	metallic	CPCONLY	H01H2209/026		48
H01H2209/028	9	Paper	CPCONLY	H01H2209/028		6
H01H2209/03	9	elastomeric	CPCONLY	H01H2209/03		66
H01H2209/032	9	non elastomeric	CPCONLY	H01H2209/032		21
H01H2209/034	9	Conductive rubber	CPCONLY	H01H2209/034		7
H01H2209/036	9	with memory properties	CPCONLY	H01H2209/036		1
H01H2209/038	9	transparent	CPCONLY	H01H2209/038		144
H01H2209/04	10	Glass	CPCONLY	H01H2209/04		36
H01H2209/042	9	Trellis; Lattice	CPCONLY	H01H2209/042		3
H01H2209/044	9	ceramic	CPCONLY	H01H2209/044		3
H01H2209/046	8	Properties of the spacer	CPCONLY	H01H2209/046		15
H01H2209/048	9	metallic	CPCONLY	H01H2209/048		6
H01H2209/05	9	Paper	CPCONLY	H01H2209/05		3
H01H2209/052	9	elastomeric	CPCONLY	H01H2209/052		73
H01H2209/054	9	non elastomeric	CPCONLY	H01H2209/054		3
H01H2209/056	9	Conductive rubber	CPCONLY	H01H2209/056		7
H01H2209/058	9	with memory properties	CPCONLY	H01H2209/058		4
H01H2209/06	9	transparent	CPCONLY	H01H2209/06		108
H01H2209/062	10	Glass	CPCONLY	H01H2209/062		2
H01H2209/064	9	Trellis; Lattice	CPCONLY	H01H2209/064		5
H01H2209/066	9	ceramic	CPCONLY	H01H2209/066		
H01H2209/068	8	Properties of the membrane	CPCONLY	H01H2209/068		21
H01H2209/07	9	metallic	CPCONLY	H01H2209/07		114
H01H2209/072	9	Paper	CPCONLY	H01H2209/072		6
H01H2209/074	9	elastomeric	CPCONLY	H01H2209/074		102
H01H2209/076	9	non elastomeric	CPCONLY	H01H2209/076		7
H01H2209/078	9	Conductive rubber	CPCONLY	H01H2209/078		33
H01H2209/08	9	with memory properties	CPCONLY	H01H2209/08		12
H01H2209/082	9	transparent	CPCONLY	H01H2209/082		252
H01H2209/084	10	Glass	CPCONLY	H01H2209/084		54
H01H2209/086	9	Trellis; Lattice	CPCONLY	H01H2209/086		7
H01H2209/088	9	ceramic	CPCONLY	H01H2209/088		3
H01H2211/00	7	Spacers	CPCONLY	H01H2211/00		24
H01H2211/002	8	Fluid or inflatable keyboards	CPCONLY	H01H2211/002		33
H01H2211/004	8	Adhesive	CPCONLY	H01H2211/004		58
H01H2211/006	8	Individual areas	CPCONLY	H01H2211/006		72
H01H2211/008	9	Spring loaded pins	CPCONLY	H01H2211/008		1
H01H2211/01	9	Ink	CPCONLY	H01H2211/01		46
H01H2211/012	10	Successive layers, one being conductive	CPCONLY	H01H2211/012		9
H01H2211/014	9	universal	CPCONLY	H01H2211/014		21
H01H2211/016	9	Wires	CPCONLY	H01H2211/016		17
H01H2211/018	9	on printed conductors only	CPCONLY	H01H2211/018		15
H01H2211/02	9	Pins forming part of substrate	CPCONLY	H01H2211/02		10
H01H2211/022	8	for larger actuation area	CPCONLY	H01H2211/022		14
H01H2211/024	8	Peripheral edge deformable	CPCONLY	H01H2211/024		10
H01H2211/026	8	without separate element	CPCONLY	H01H2211/026		14
H01H2211/028	9	Contacts in depressions of layers	CPCONLY	H01H2211/028		65
H01H2211/03	9	Ridges on layers	CPCONLY	H01H2211/03		16
H01H2211/032	9	Pressure sensitive layer on contacts	CPCONLY	H01H2211/032		31
H01H2211/034	9	Fixed contacts on different planes	CPCONLY	H01H2211/034		15
H01H2211/036	9	Convexly bowed membrane	CPCONLY	H01H2211/036		6
H01H2213/00	7	Venting	CPCONLY	H01H2213/00		40
H01H2213/002	8	with external pressure	CPCONLY	H01H2213/002		133
H01H2213/004	9	Scavenger; Filter	CPCONLY	H01H2213/004		29
H01H2213/006	9	Labyrinth	CPCONLY	H01H2213/006		15
H01H2213/008	9	Flaps cut out forming valves	CPCONLY	H01H2213/008		10
H01H2213/01	8	with internal pressure of other switch sites	CPCONLY	H01H2213/01		115
H01H2213/012	9	Open-cell foam	CPCONLY	H01H2213/012		4
H01H2213/014	9	Accumulator chamber	CPCONLY	H01H2213/014		39
H01H2213/016	8	in adhesive layer	CPCONLY	H01H2213/016		35
H01H2215/00	7	Tactile feedback	CPCONLY	H01H2215/00		170
H01H2215/002	8	Longer travel	CPCONLY	H01H2215/002		89
H01H2215/004	8	Collapsible dome or bubble	CPCONLY	H01H2215/004		483
H01H2215/006	9	Only mechanical function	CPCONLY	H01H2215/006		411
H01H2215/008	9	Part of substrate or membrane	CPCONLY	H01H2215/008		282
H01H2215/01	9	Part of spacer	CPCONLY	H01H2215/01		12
H01H2215/012	9	Positioning of individual dome	CPCONLY	H01H2215/012		151
H01H2215/014	9	Avoiding permanent dome inversion	CPCONLY	H01H2215/014		24
H01H2215/016	9	Collapsing to second stable position	CPCONLY	H01H2215/016		25
H01H2215/018	9	unstressed in open position of switch	CPCONLY	H01H2215/018		35
H01H2215/02	9	Reversed domes	CPCONLY	H01H2215/02		76
H01H2215/022	9	Asymmetric; Elliptic; Square	CPCONLY	H01H2215/022		60
H01H2215/024	10	Spider	CPCONLY	H01H2215/024		25
H01H2215/026	9	Eccentric actuation	CPCONLY	H01H2215/026		24
H01H2215/028	8	alterable	CPCONLY	H01H2215/028		112
H01H2215/03	8	Sound	CPCONLY	H01H2215/03		284
H01H2215/032	9	Resonance space	CPCONLY	H01H2215/032		13
H01H2215/034	8	Separate snap action	CPCONLY	H01H2215/034		74
H01H2215/036	9	Metallic disc	CPCONLY	H01H2215/036		173
H01H2215/038	9	Resilient conductive tracks	CPCONLY	H01H2215/038		4
H01H2215/04	9	Contact making part moved through contact supporting plane	CPCONLY	H01H2215/04		4
H01H2215/042	9	Permanent magnets	CPCONLY	H01H2215/042		75
H01H2215/044	8	Light	CPCONLY	H01H2215/044		44
H01H2215/046	8	Inflatable bubble or cell	CPCONLY	H01H2215/046		18
H01H2215/048	8	Vent	CPCONLY	H01H2215/048		16
H01H2215/05	8	electromechanical	CPCONLY	H01H2215/05		185
H01H2215/052	9	piezoelectric	CPCONLY	H01H2215/052		117
H01H2215/054	8	common to all switch sites	CPCONLY	H01H2215/054		28
H01H2217/00	7	Facilitation of operation; Human engineering	CPCONLY	H01H2217/00		49
H01H2217/002	8	actuable from both sides	CPCONLY	H01H2217/002		35
H01H2217/004	8	Larger or different actuating area	CPCONLY	H01H2217/004		135
H01H2217/006	8	Different feeling for different switch sites	CPCONLY	H01H2217/006		75
H01H2217/008	8	Pretravel to avoid inadvertent switching	CPCONLY	H01H2217/008		36
H01H2217/01	8	Off centre actuation	CPCONLY	H01H2217/01		144
H01H2217/012	8	Two keys simultaneous considerations	CPCONLY	H01H2217/012		116
H01H2217/014	8	handicapped	CPCONLY	H01H2217/014		80
H01H2217/016	8	Pressure reduction membrane; Spreader layer	CPCONLY	H01H2217/016		51
H01H2217/018	8	Indication of switch sites	CPCONLY	H01H2217/018		193
H01H2217/02	8	After travel	CPCONLY	H01H2217/02		82
H01H2217/022	8	Part of keyboard not operable	CPCONLY	H01H2217/022		98
H01H2217/024	8	Profile on actuator	CPCONLY	H01H2217/024		232
H01H2217/026	8	Pencil operated	CPCONLY	H01H2217/026		37
H01H2217/028	8	on planes with different or alterable inclination, e.g. convex plane	CPCONLY	H01H2217/028		170
H01H2217/03	9	Concave plane	CPCONLY	H01H2217/03		25
H01H2217/032	8	Feedback about selected symbol, e.g. display	CPCONLY	H01H2217/032		156
H01H2217/033	9	by speech	CPCONLY	H01H2217/033		31
H01H2217/034	8	Support for hands or arms	CPCONLY	H01H2217/034		142
H01H2217/036	8	Plural multifunctional miniature keys for one symbol	CPCONLY	H01H2217/036		102
H01H2217/038	8	Prompting	CPCONLY	H01H2217/038		50
H01H2217/04	8	Mimics of controlled apparatus or symbol	CPCONLY	H01H2217/04		65
H01H2217/042	8	Higher keytops	CPCONLY	H01H2217/042		23
H01H2217/044	8	Repetitive strain injury [RSI] considerations	CPCONLY	H01H2217/044		71
H01H2217/046	8	Enhanced legend space by smaller actuators	CPCONLY	H01H2217/046		66
H01H2217/048	8	adapted for operation by left- and right-handed	CPCONLY	H01H2217/048		42
H01H2219/00	7	Legends	CPCONLY	H01H2219/00		30
H01H2219/002	8	replaceable; adaptable	CPCONLY	H01H2219/002		276
H01H2219/0023	9	Images formed with electrophoretic technology, e.g. by charged pigment particles rearranged by applied electric field, e.g. electronic paper or e-paper, active ink	CPCONLY	H01H2219/0023		57
H01H2219/0026	9	having outer surface of housing of electronic apparatus programmable as display and/or input device	CPCONLY	H01H2219/0026		32
H01H2219/004	9	Magnet	CPCONLY	H01H2219/004		30
H01H2219/006	9	Snap mounting	CPCONLY	H01H2219/006		43
H01H2219/008	9	Adhesive	CPCONLY	H01H2219/008		54
H01H2219/01	9	Liquid crystal	CPCONLY	H01H2219/01		68
H01H2219/011	10	with integrated photo- or thermovoltaic cell as power supply	CPCONLY	H01H2219/011		76
H01H2219/012	10	programmable	CPCONLY	H01H2219/012		218
H01H2219/014	9	LED	CPCONLY	H01H2219/014		540
H01H2219/016	10	programmable	CPCONLY	H01H2219/016		152
H01H2219/018	9	Electroluminescent panel	CPCONLY	H01H2219/018		345
H01H2219/02	10	programmable	CPCONLY	H01H2219/02		57
H01H2219/022	9	Plasma display	CPCONLY	H01H2219/022		6
H01H2219/024	10	programmable	CPCONLY	H01H2219/024		12
H01H2219/026	9	with programming switches	CPCONLY	H01H2219/026		62
H01H2219/028	8	Printed information	CPCONLY	H01H2219/028		329
H01H2219/03	9	in transparent keyboard	CPCONLY	H01H2219/03		191
H01H2219/032	9	photographic	CPCONLY	H01H2219/032		15
H01H2219/034	9	Coloured areas	CPCONLY	H01H2219/034		159
H01H2219/036	8	Light emitting elements	CPCONLY	H01H2219/036		500
H01H2219/037	9	using organic materials, e.g. organic LED	CPCONLY	H01H2219/037		174
H01H2219/038	9	ambient light dependent	CPCONLY	H01H2219/038		81
H01H2219/039	9	Selective or different modes of illumination	CPCONLY	H01H2219/039		412
H01H2219/04	9	Attachments; Connections	CPCONLY	H01H2219/04		256
H01H2219/042	9	replaceable	CPCONLY	H01H2219/042		29
H01H2219/044	9	Edge lighting of layer	CPCONLY	H01H2219/044		457
H01H2219/046	9	above switch site	CPCONLY	H01H2219/046		84
H01H2219/048	9	Constituting key	CPCONLY	H01H2219/048		57
H01H2219/05	9	Key offset in relation to switch site	CPCONLY	H01H2219/05		61
H01H2219/052	9	Phosphorescence	CPCONLY	H01H2219/052		105
H01H2219/053	9	protected by inert gas	CPCONLY	H01H2219/053		9
H01H2219/054	8	Optical elements	CPCONLY	H01H2219/054		166
H01H2219/056	9	Diffuser; Uneven surface	CPCONLY	H01H2219/056		488
H01H2219/058	9	Optical grid, collimator or microlouver	CPCONLY	H01H2219/058		59
H01H2219/06	9	Reflector	CPCONLY	H01H2219/06		659
H01H2219/062	9	Light conductor	CPCONLY	H01H2219/062		1546
H01H2219/0621	10	Optical fiber light conductor	CPCONLY	H01H2219/0621		70
H01H2219/0622	10	only an illuminated ring around keys	CPCONLY	H01H2219/0622		256
H01H2219/064	9	Optical isolation of switch sites	CPCONLY	H01H2219/064		329
H01H2219/066	9	Lens	CPCONLY	H01H2219/066		197
H01H2221/00	7	Actuators	CPCONLY	H01H2221/00		25
H01H2221/002	8	integral with membrane	CPCONLY	H01H2221/002		302
H01H2221/004	9	U-shaped openings surrounding keys	CPCONLY	H01H2221/004		91
H01H2221/006	9	Adhesive	CPCONLY	H01H2221/006		97
H01H2221/008	8	other then push button	CPCONLY	H01H2221/008		40
H01H2221/01	9	also rotatable	CPCONLY	H01H2221/01		103
H01H2221/012	9	Joy stick type	CPCONLY	H01H2221/012		346
H01H2221/014	9	Slide selector	CPCONLY	H01H2221/014		112
H01H2221/016	9	Lever; Rocker	CPCONLY	H01H2221/016		458
H01H2221/018	9	Tumbler	CPCONLY	H01H2221/018		104
H01H2221/02	9	pneumatic	CPCONLY	H01H2221/02		38
H01H2221/022	9	electromagnetic	CPCONLY	H01H2221/022		34
H01H2221/024	8	Transmission element	CPCONLY	H01H2221/024		140
H01H2221/026	9	Guiding or lubricating nylon	CPCONLY	H01H2221/026		347
H01H2221/028	10	Telescopic guiding	CPCONLY	H01H2221/028		40
H01H2221/03	9	Stoppers for on or off position	CPCONLY	H01H2221/03		204
H01H2221/032	8	adjustable	CPCONLY	H01H2221/032		82
H01H2221/034	9	Coded keys	CPCONLY	H01H2221/034		26
H01H2221/036	8	Return force	CPCONLY	H01H2221/036		88
H01H2221/038	9	Fluid	CPCONLY	H01H2221/038		39
H01H2221/04	9	magnetic	CPCONLY	H01H2221/04		244
H01H2221/042	9	Foam	CPCONLY	H01H2221/042		69
H01H2221/044	9	Elastic part on actuator or casing	CPCONLY	H01H2221/044		501
H01H2221/046	8	bistable	CPCONLY	H01H2221/046		21
H01H2221/048	9	magnetic	CPCONLY	H01H2221/048		40
H01H2221/05	8	Force concentrator; Actuating dimple	CPCONLY	H01H2221/05		340
H01H2221/052	8	interlocked	CPCONLY	H01H2221/052		76
H01H2221/054	8	connected by flexible webs	CPCONLY	H01H2221/054		92
H01H2221/056	8	Modular conception	CPCONLY	H01H2221/056		100
H01H2221/058	8	to avoid tilting or skewing of contact area or actuator	CPCONLY	H01H2221/058		323
H01H2221/06	8	to avoid sticking in on position	CPCONLY	H01H2221/06		34
H01H2221/062	8	Damping vibrations	CPCONLY	H01H2221/062		291
H01H2221/064	8	Limitation of actuating pressure	CPCONLY	H01H2221/064		241
H01H2221/066	8	replaceable	CPCONLY	H01H2221/066		163
H01H2221/068	8	having a not operable condition	CPCONLY	H01H2221/068		123
H01H2221/07	8	transparent	CPCONLY	H01H2221/07		579
H01H2221/0702	9	Transparent key containing three dimensional (3D) element	CPCONLY	H01H2221/0702		31
H01H2221/072	8	Stroke amplification	CPCONLY	H01H2221/072		31
H01H2221/074	8	One molded piece	CPCONLY	H01H2221/074		61
H01H2221/076	8	Protruding in cavity covered by membrane	CPCONLY	H01H2221/076		19
H01H2221/078	8	Different operating parts on a bigger one	CPCONLY	H01H2221/078		52
H01H2221/08	8	composed of different parts	CPCONLY	H01H2221/08		107
H01H2221/082	9	Superimposed actuators	CPCONLY	H01H2221/082		80
H01H2221/084	8	made at least partly of elastic foam	CPCONLY	H01H2221/084		80
H01H2221/088	8	actuable from different directions	CPCONLY	H01H2221/088		36
H01H2221/09	8	Flexible integral part of housing	CPCONLY	H01H2221/09		108
H01H2223/00	7	Casings	CPCONLY	H01H2223/00		50
H01H2223/002	8	sealed	CPCONLY	H01H2223/002		791
H01H2223/003	9	Membrane embracing all keys	CPCONLY	H01H2223/003		240
H01H2223/004	9	Evacuation of penetrating liquid	CPCONLY	H01H2223/004		150
H01H2223/006	9	Purge gas	CPCONLY	H01H2223/006		14
H01H2223/008	8	metallic	CPCONLY	H01H2223/008		68
H01H2223/01	8	Mounting on appliance	CPCONLY	H01H2223/01		85
H01H2223/012	9	Snap mounting	CPCONLY	H01H2223/012		83
H01H2223/014	9	located in recess	CPCONLY	H01H2223/014		141
H01H2223/016	9	magnetic	CPCONLY	H01H2223/016		22
H01H2223/018	9	rotatably	CPCONLY	H01H2223/018		46
H01H2223/02	9	mounted on raised part	CPCONLY	H01H2223/02		3
H01H2223/022	9	Adhesive	CPCONLY	H01H2223/022		86
H01H2223/024	9	Screw	CPCONLY	H01H2223/024		56
H01H2223/026	9	Hook and loop	CPCONLY	H01H2223/026		52
H01H2223/028	9	detachable	CPCONLY	H01H2223/028		121
H01H2223/03	8	Separate key housing	CPCONLY	H01H2223/03		94
H01H2223/032	9	with formations for assembling similar housings	CPCONLY	H01H2223/032		31
H01H2223/034	8	Bezel	CPCONLY	H01H2223/034		217
H01H2223/0345	9	with keys positioned directly next to each other without an intermediate bezel or frame	CPCONLY	H01H2223/0345		99
H01H2223/036	9	forming chamfered apertures for keys	CPCONLY	H01H2223/036		55
H01H2223/038	8	transparent	CPCONLY	H01H2223/038		62
H01H2223/04	8	portable; hand held	CPCONLY	H01H2223/04		174
H01H2223/042	8	mounted in conventional keyboard	CPCONLY	H01H2223/042		32
H01H2223/044	8	Protecting cover	CPCONLY	H01H2223/044		282
H01H2223/046	8	convertible	CPCONLY	H01H2223/046		56
H01H2223/048	9	assembled by removable part	CPCONLY	H01H2223/048		20
H01H2223/05	9	composed of hingedly connected sections	CPCONLY	H01H2223/05		265
H01H2223/052	9	reductible in size, e.g. for transportation	CPCONLY	H01H2223/052		228
H01H2223/054	8	Mounting of key housings on same printed circuit	CPCONLY	H01H2223/054		138
H01H2223/056	8	Mounting of key housings on same frame	CPCONLY	H01H2223/056		44
H01H2223/058	8	flush mounted	CPCONLY	H01H2223/058		48
H01H2223/06	8	freestanding	CPCONLY	H01H2223/06		5
H01H2223/062	8	Inflatable	CPCONLY	H01H2223/062		13
H01H2225/00	7	Switch site location	CPCONLY	H01H2225/00		9
H01H2225/002	8	superimposed	CPCONLY	H01H2225/002		186
H01H2225/004	8	in different planes to increase density	CPCONLY	H01H2225/004		25
H01H2225/006	8	more then one pole	CPCONLY	H01H2225/006		45
H01H2225/008	8	Two different sites for one circuit, e.g. for safety	CPCONLY	H01H2225/008		71
H01H2225/01	8	Different switch sites under one actuator in same plane	CPCONLY	H01H2225/01		155
H01H2225/012	8	normally closed	CPCONLY	H01H2225/012		33
H01H2225/014	8	normally closed combined with normally open	CPCONLY	H01H2225/014		42
H01H2225/016	8	Make break	CPCONLY	H01H2225/016		10
H01H2225/018	8	Consecutive operations	CPCONLY	H01H2225/018		255
H01H2225/02	8	Push-push	CPCONLY	H01H2225/02		5
H01H2225/022	8	other then row-column disposition	CPCONLY	H01H2225/022		147
H01H2225/024	8	Common site to all actuators, e.g. auxiliary	CPCONLY	H01H2225/024		19
H01H2225/026	8	above actuator	CPCONLY	H01H2225/026		8
H01H2225/028	8	perpendicular to base of keyboard	CPCONLY	H01H2225/028		140
H01H2225/03	8	Different type of switches	CPCONLY	H01H2225/03		103
H01H2227/00	7	Dimensions; Characteristics	CPCONLY	H01H2227/00		19
H01H2227/002	8	Layer thickness	CPCONLY	H01H2227/002		128
H01H2227/004	9	Membrane	CPCONLY	H01H2227/004		55
H01H2227/006	9	Spacer	CPCONLY	H01H2227/006		48
H01H2227/008	9	Substrate	CPCONLY	H01H2227/008		24
H01H2227/01	9	Adhesive	CPCONLY	H01H2227/01		42
H01H2227/012	9	Conductive rubber	CPCONLY	H01H2227/012		24
H01H2227/014	10	Conductive particles	CPCONLY	H01H2227/014		21
H01H2227/016	8	Switch site protrusions; Force concentrators	CPCONLY	H01H2227/016		46
H01H2227/018	8	Printed contacts; Metal foil	CPCONLY	H01H2227/018		85
H01H2227/02	8	Vent opening	CPCONLY	H01H2227/02		33
H01H2227/022	8	Collapsable dome	CPCONLY	H01H2227/022		139
H01H2227/024	8	Spacer elements	CPCONLY	H01H2227/024		56
H01H2227/026	8	Separate dome contact	CPCONLY	H01H2227/026		123
H01H2227/0261	9	with an aperture in contact making centre of dome	CPCONLY	H01H2227/0261		24
H01H2227/028	8	Key stroke	CPCONLY	H01H2227/028		113
H01H2227/03	8	Hardness	CPCONLY	H01H2227/03		35
H01H2227/032	8	Operating force	CPCONLY	H01H2227/032		85
H01H2227/034	9	Regulation of operating force	CPCONLY	H01H2227/034		113
H01H2227/036	8	Minimise height	CPCONLY	H01H2227/036		378
H01H2229/00	7	Manufacturing	CPCONLY	H01H2229/00		88
H01H2229/002	8	Screen printing	CPCONLY	H01H2229/002		144
H01H2229/004	9	Conductive ink	CPCONLY	H01H2229/004		69
H01H2229/006	8	Pad transfer printing	CPCONLY	H01H2229/006		36
H01H2229/008	8	Die stamping	CPCONLY	H01H2229/008		48
H01H2229/01	8	Foil transfer process	CPCONLY	H01H2229/01		17
H01H2229/012	8	Vacuum deposition	CPCONLY	H01H2229/012		61
H01H2229/014	8	Electro deposition	CPCONLY	H01H2229/014		63
H01H2229/016	8	Selective etching	CPCONLY	H01H2229/016		96
H01H2229/018	8	Testing	CPCONLY	H01H2229/018		82
H01H2229/02	8	Laser	CPCONLY	H01H2229/02		130
H01H2229/022	8	Modular assembly	CPCONLY	H01H2229/022		177
H01H2229/024	8	Packing between substrate and membrane	CPCONLY	H01H2229/024		25
H01H2229/026	9	Riveting	CPCONLY	H01H2229/026		43
H01H2229/028	9	Adhesive	CPCONLY	H01H2229/028		315
H01H2229/03	9	Laminating	CPCONLY	H01H2229/03		37
H01H2229/032	9	Screw	CPCONLY	H01H2229/032		44
H01H2229/034	8	Positioning of layers	CPCONLY	H01H2229/034		178
H01H2229/036	8	ultrasonic	CPCONLY	H01H2229/036		64
H01H2229/038	8	Folding of flexible printed circuit	CPCONLY	H01H2229/038		152
H01H2229/04	8	Solder problems	CPCONLY	H01H2229/04		42
H01H2229/042	8	Snap coupling; Snap mounting	CPCONLY	H01H2229/042		178
H01H2229/044	8	Injection moulding	CPCONLY	H01H2229/044		339
H01H2229/046	9	Multi-colour or double shot injection moulding	CPCONLY	H01H2229/046		265
H01H2229/047	9	Preformed layer in mould	CPCONLY	H01H2229/047		160
H01H2229/048	9	Insertion moulding	CPCONLY	H01H2229/048		178
H01H2229/05	8	Forming; Half-punching	CPCONLY	H01H2229/05		119
H01H2229/052	8	Thermoplastic bonding foil	CPCONLY	H01H2229/052		15
H01H2229/054	8	CAD	CPCONLY	H01H2229/054		12
H01H2229/056	8	Laminating	CPCONLY	H01H2229/056		38
H01H2229/058	8	Curing or vulcanising of rubbers	CPCONLY	H01H2229/058		119
H01H2229/06	8	Tempering	CPCONLY	H01H2229/06		3
H01H2229/062	8	Maintenance or repair facilities	CPCONLY	H01H2229/062		130
H01H2229/064	8	Eliminating tolerances	CPCONLY	H01H2229/064		114
H01H2229/066	8	Z-axis assembly	CPCONLY	H01H2229/066		18
H01H2229/068	8	Extrusion	CPCONLY	H01H2229/068		8
H01H2231/00	7	Applications	CPCONLY	H01H2231/00		21
H01H2231/002	8	Calculator, computer	CPCONLY	H01H2231/002		452
H01H2231/004	8	CRT	CPCONLY	H01H2231/004		191
H01H2231/006	8	Bank automat; Cash register; Vending machine	CPCONLY	H01H2231/006		104
H01H2231/008	8	Video game	CPCONLY	H01H2231/008		135
H01H2231/01	8	Toy	CPCONLY	H01H2231/01		21
H01H2231/012	8	Household appliance	CPCONLY	H01H2231/012		743
H01H2231/014	8	Sewing machine	CPCONLY	H01H2231/014		5
H01H2231/016	8	Control panel; Graphic display; Program control	CPCONLY	H01H2231/016		132
H01H2231/018	8	Musical instrument	CPCONLY	H01H2231/018		38
H01H2231/022	8	Telephone handset	CPCONLY	H01H2231/022		577
H01H2231/024	8	Dispensing machine	CPCONLY	H01H2231/024		9
H01H2231/026	8	Car	CPCONLY	H01H2231/026		2035
H01H2231/028	8	Watch	CPCONLY	H01H2231/028		51
H01H2231/03	8	Elevator	CPCONLY	H01H2231/03		36
H01H2231/032	8	Remote control	CPCONLY	H01H2231/032		300
H01H2231/034	8	Coordinate determination	CPCONLY	H01H2231/034		19
H01H2231/036	8	Radio; TV	CPCONLY	H01H2231/036		772
H01H2231/038	8	Level sensing or limit switch	CPCONLY	H01H2231/038		27
H01H2231/04	8	Robot	CPCONLY	H01H2231/04		18
H01H2231/042	8	Briefcase; Note-book	CPCONLY	H01H2231/042		81
H01H2231/044	8	Under water	CPCONLY	H01H2231/044		28
H01H2231/046	8	Camera	CPCONLY	H01H2231/046		202
H01H2231/048	8	Tools; Drilling machines	CPCONLY	H01H2231/048		49
H01H2231/05	8	Card, e.g. credit card	CPCONLY	H01H2231/05		95
H01H2231/052	8	Selectors, e.g. dimmers	CPCONLY	H01H2231/052		64
H01H2233/00	7	Key modules	CPCONLY	H01H2233/00		3
H01H2233/002	8	joined to form button rows	CPCONLY	H01H2233/002		55
H01H2233/004	9	One molded part	CPCONLY	H01H2233/004		117
H01H2233/006	10	Separating individual keys after mounting	CPCONLY	H01H2233/006		31
H01H2233/008	8	Laykey mounted on assembled key modules	CPCONLY	H01H2233/008		5
H01H2233/01	8	mounted on laykey	CPCONLY	H01H2233/01		5
H01H2233/012	9	Locating pins	CPCONLY	H01H2233/012		24
H01H2233/014	9	Snap coupling	CPCONLY	H01H2233/014		17
H01H2233/016	10	with limited freedom	CPCONLY	H01H2233/016		15
H01H2233/018	9	One degree of freedom	CPCONLY	H01H2233/018		3
H01H2233/02	9	captured between assembled parts of support	CPCONLY	H01H2233/02		10
H01H2233/022	10	with limited freedom	CPCONLY	H01H2233/022		34
H01H2233/024	9	Riveting	CPCONLY	H01H2233/024		5
H01H2233/026	9	Inserting	CPCONLY	H01H2233/026		4
H01H2233/028	9	connected by spring	CPCONLY	H01H2233/028		
H01H2233/03	8	mounted on support plate or frame	CPCONLY	H01H2233/03		78
H01H2233/032	9	Locating pins	CPCONLY	H01H2233/032		22
H01H2233/034	9	Snap coupling	CPCONLY	H01H2233/034		49
H01H2233/036	10	with limited freedom	CPCONLY	H01H2233/036		77
H01H2233/038	9	One degree of freedom	CPCONLY	H01H2233/038		3
H01H2233/04	9	captured between assembled parts of support	CPCONLY	H01H2233/04		15
H01H2233/042	10	with limited freedom	CPCONLY	H01H2233/042		9
H01H2233/044	9	Riveting	CPCONLY	H01H2233/044		4
H01H2233/046	9	Inserting	CPCONLY	H01H2233/046		10
H01H2233/048	9	connected by spring	CPCONLY	H01H2233/048		7
H01H2233/05	8	Actuator part on body	CPCONLY	H01H2233/05		6
H01H2233/052	9	Locating pins	CPCONLY	H01H2233/052		3
H01H2233/054	9	Snap coupling	CPCONLY	H01H2233/054		3
H01H2233/056	10	with limited freedom	CPCONLY	H01H2233/056		39
H01H2233/058	9	One degree of freedom	CPCONLY	H01H2233/058		6
H01H2233/06	9	captured between assembled parts of support	CPCONLY	H01H2233/06		1
H01H2233/062	10	with limited freedom	CPCONLY	H01H2233/062		6
H01H2233/064	9	Riveting	CPCONLY	H01H2233/064		
H01H2233/066	9	Inserting	CPCONLY	H01H2233/066		2
H01H2233/068	9	connected by spring	CPCONLY	H01H2233/068		2
H01H2233/07	8	Cap or button on actuator part	CPCONLY	H01H2233/07		123
H01H2233/072	9	Locating pins	CPCONLY	H01H2233/072		9
H01H2233/074	9	Snap coupling	CPCONLY	H01H2233/074		74
H01H2233/076	10	with limited freedom	CPCONLY	H01H2233/076		3
H01H2233/078	9	One degree of freedom	CPCONLY	H01H2233/078		2
H01H2233/08	9	captured between assembled parts of support	CPCONLY	H01H2233/08		2
H01H2233/082	10	with limited freedom	CPCONLY	H01H2233/082		1
H01H2233/084	9	Riveting	CPCONLY	H01H2233/084		3
H01H2233/086	9	Inserting	CPCONLY	H01H2233/086		19
H01H2233/088	9	connected by spring	CPCONLY	H01H2233/088		1
H01H2233/09	8	Actuating striker on actuator part	CPCONLY	H01H2233/09		4
H01H2233/092	9	Locating pins	CPCONLY	H01H2233/092		1
H01H2233/094	9	Snap coupling	CPCONLY	H01H2233/094		7
H01H2233/096	10	with limited freedom	CPCONLY	H01H2233/096		6
H01H2233/098	9	One degree of freedom	CPCONLY	H01H2233/098		7
H01H2233/10	9	captured between assembled parts of support	CPCONLY	H01H2233/10		2
H01H2233/102	10	with limited freedom	CPCONLY	H01H2233/102		4
H01H2233/104	9	Riveting	CPCONLY	H01H2233/104		
H01H2233/106	9	Inserting	CPCONLY	H01H2233/106		2
H01H2233/108	9	connected by spring	CPCONLY	H01H2233/108		2
H01H2235/00	7	Springs	CPCONLY	H01H2235/00		69
H01H2235/002	8	Linear coil spring combined with dome spring	CPCONLY	H01H2235/002		46
H01H2235/004	8	Two parallel coil springs	CPCONLY	H01H2235/004		48
H01H2235/006	8	Elastic arms producing non linear counter force	CPCONLY	H01H2235/006		35
H01H2235/008	8	Rubber spring	CPCONLY	H01H2235/008		38
H01H2235/01	8	Spiral spring	CPCONLY	H01H2235/01		357
H01H2235/012	8	Euler spring	CPCONLY	H01H2235/012		22
H01H2235/014	9	with positive buckling force or action	CPCONLY	H01H2235/014		4
H01H2235/016	8	Preloading	CPCONLY	H01H2235/016		24
H01H2235/018	8	Spring seat	CPCONLY	H01H2235/018		72
H01H2235/02	8	between contact and substrate	CPCONLY	H01H2235/02		12
H01H2235/022	8	Actuating striker	CPCONLY	H01H2235/022		10
H01H2235/024	9	formed by knee or dimple of leaf spring	CPCONLY	H01H2235/024		24
H01H2235/026	9	forming part of return spring	CPCONLY	H01H2235/026		28
H01H2235/028	8	Blade spring	CPCONLY	H01H2235/028		76
H01H2235/03	8	Two serial springs	CPCONLY	H01H2235/03		38
H01H2237/00	7	Mechanism between key and laykey	CPCONLY	H01H2237/00		28
H01H2237/002	8	Bell crank	CPCONLY	H01H2237/002		31
H01H2237/004	8	Cantilever	CPCONLY	H01H2237/004		84
H01H2237/006	8	Guided plunger or ball	CPCONLY	H01H2237/006		70
H01H2237/008	8	Plunger guided by flexible arms	CPCONLY	H01H2237/008		18
H01H2239/00	7	Miscellaneous	CPCONLY	H01H2239/00		5
H01H2239/002	8	Conductive track to monitor integrity	CPCONLY	H01H2239/002		26
H01H2239/004	8	High frequency adaptation or shielding	CPCONLY	H01H2239/004		154
H01H2239/006	8	Containing a capacitive switch or usable as such	CPCONLY	H01H2239/006		582
H01H2239/008	8	Static electricity considerations	CPCONLY	H01H2239/008		222
H01H2239/01	8	combined with other elements on the same substrate	CPCONLY	H01H2239/01		204
H01H2239/012	9	Decoding impedances	CPCONLY	H01H2239/012		118
H01H2239/014	9	on both sides	CPCONLY	H01H2239/014		30
H01H2239/016	8	combined with start switch, discrete keyboard	CPCONLY	H01H2239/016		51
H01H2239/018	8	Ground conductor	CPCONLY	H01H2239/018		43
H01H2239/02	8	Other elements in moving part	CPCONLY	H01H2239/02		27
H01H2239/022	8	with opto-electronic switch	CPCONLY	H01H2239/022		163
H01H2239/024	8	with inductive switch	CPCONLY	H01H2239/024		124
H01H2239/026	8	Internal encoding, e.g. validity bit	CPCONLY	H01H2239/026		93
H01H2239/03	8	Avoiding erroneous switching	CPCONLY	H01H2239/03		324
H01H2239/032	8	Anti-tamper	CPCONLY	H01H2239/032		218
H01H2239/034	8	Environmental protection	CPCONLY	H01H2239/034		103
H01H2239/036	9	Heating, e.g. against condensation	CPCONLY	H01H2239/036		26
H01H2239/038	8	Anti-vandalism	CPCONLY	H01H2239/038		207
H01H2239/04	8	Gadget	CPCONLY	H01H2239/04		5
H01H2239/042	8	Unmixable liquids inside	CPCONLY	H01H2239/042		2
H01H2239/044	8	High voltage application	CPCONLY	H01H2239/044		72
H01H2239/046	8	Getter	CPCONLY	H01H2239/046		4
H01H2239/048	8	comprising microphone or speaker	CPCONLY	H01H2239/048		82
H01H2239/05	8	Mode selector switch, e.g. shift, or indicator	CPCONLY	H01H2239/05		159
H01H2239/052	8	Strain gauge	CPCONLY	H01H2239/052		104
H01H2239/054	8	Acoustic pick-up, e.g. ultrasonic	CPCONLY	H01H2239/054		36
H01H2239/056	8	Keyboard or overlay identification features	CPCONLY	H01H2239/056		56
H01H2239/058	8	Containing a battery	CPCONLY	H01H2239/058		58
H01H2239/06	8	Temperature sensitive	CPCONLY	H01H2239/06		32
H01H2239/062	8	Disposable	CPCONLY	H01H2239/062		14
H01H2239/064	8	Simulating the appearance of touch panel	CPCONLY	H01H2239/064		29
H01H2239/066	8	Duplication of control panel, e.g. duplication of some keys	CPCONLY	H01H2239/066		38
H01H2239/068	8	3D	CPCONLY	H01H2239/068		11
H01H2239/07	8	UV or IR detection, e.g. of human body	CPCONLY	H01H2239/07		31
H01H2239/072	8	High temperature considerations	CPCONLY	H01H2239/072		50
H01H2239/074	8	Actuation by finger touch	CPCONLY	H01H2239/074		256
H01H2239/076	8	Key stroke generating power	CPCONLY	H01H2239/076		160
H01H2239/078	8	Variable resistance by variable contact area or point	CPCONLY	H01H2239/078		148
H01H2300/00	7	Orthogonal indexing scheme relating to electric switches, relays, selectors or emergency protective devices covered by H01H	CPCONLY	H01H2300/00		69
H01H2300/002	8	Application electric motor braking, e.g. pole reversal of rotor, shorting motor coils, also for field discharge	CPCONLY	H01H2300/002		40
H01H2300/004	8	Application hearing aid	CPCONLY	H01H2300/004		146
H01H2300/006	8	Application power roofs	CPCONLY	H01H2300/006		97
H01H2300/008	8	Application power seats	CPCONLY	H01H2300/008		159
H01H2300/01	8	Application power window	CPCONLY	H01H2300/01		472
H01H2300/012	8	Application rear view mirror	CPCONLY	H01H2300/012		203
H01H2300/014	8	Application surgical instrument	CPCONLY	H01H2300/014		212
H01H2300/016	8	Application timepiece	CPCONLY	H01H2300/016		72
H01H2300/018	8	Application transfer; between utility and emergency power supply	CPCONLY	H01H2300/018		561
H01H2300/02	8	Application transmission, e.g. for sensing the position of a gear selector or automatic transmission	CPCONLY	H01H2300/02		118
H01H2300/022	8	Application wake up; switches or contacts specially provided for the wake up or standby shift of a circuit	CPCONLY	H01H2300/022		79
H01H2300/024	8	Avoid unwanted operation	CPCONLY	H01H2300/024		186
H01H2300/026	8	Application dead man switch: power must be interrupted on release of operating member	CPCONLY	H01H2300/026		155
H01H2300/028	8	Application dead man switch, i.e. power being interrupted by panic reaction of operator, e.g. further pressing down push button	CPCONLY	H01H2300/028		54
H01H2300/03	8	Application domotique, e.g. for house automation, bus connected switches, sensors, loads or intelligent wiring	CPCONLY	H01H2300/03		858
H01H2300/032	9	using RFID technology in switching devices	CPCONLY	H01H2300/032		112
H01H2300/034	8	using magnetic shape memory [MSM] also an austenite-martensite transformation, but then magnetically controlled	CPCONLY	H01H2300/034		27
H01H2300/036	8	Application nanoparticles, e.g. nanotubes, integrated in switch components, e.g. contacts, the switch itself being clearly of a different scale, e.g. greater than nanoscale	CPCONLY	H01H2300/036		95
H01H2300/038	8	Preselection, i.e. the output of a switch depends on a particular preselection, e.g. a particular position of another switch	CPCONLY	H01H2300/038		34
H01H2300/04	8	Programmable interface between a set of switches and a set of functions, e.g. for reconfiguration of a control panel	CPCONLY	H01H2300/04		92
H01H2300/042	8	Application rejection, i.e. preventing improper installation of parts	CPCONLY	H01H2300/042		86
H01H2300/044	8	Application rejection 1: coded interacting surfaces, polarising, e.g. to avoid insertion of a circuit breaker or fuse or relay or rating plug of the wrong caliber or in the wrong direction	CPCONLY	H01H2300/044		82
H01H2300/046	8	using snap closing mechanisms	CPCONLY	H01H2300/046		113
H01H2300/048	9	Snap closing by latched movable contact, wherein the movable contact is held in a minimal distance from the fixed contact during first phase of closing sequence in which a closing spring is charged	CPCONLY	H01H2300/048		82
H01H2300/05	9	Snap closing with trip, wherein the contacts are locked open during charging of mechanism and unlocked by separate trip device, e.g. manual, electromagnetic etc.	CPCONLY	H01H2300/05		13
H01H2300/052	8	Controlling, signalling or testing correct functioning of a switch	CPCONLY	H01H2300/052		205
H01H2300/054	8	Application timeslot: duration of actuation or delay between or combination of subsequent actuations determines selected function	CPCONLY	H01H2300/054		144
H01H2300/056	8	Tools for actuating a switch	CPCONLY	H01H2300/056		124
H01H2300/058	9	using apparatus with a spring motor or a snap-acting mechanism for actuating any one of a number of circuit breakers	CPCONLY	H01H2300/058		23
H01H2300/06	8	using tools as locking means	CPCONLY	H01H2300/06		10
H01H2300/062	9	for locking a charged spring	CPCONLY	H01H2300/062		
H01H2300/064	10	by means of removable member	CPCONLY	H01H2300/064		6
H01H2300/066	9	for locking a switch in a test or an "installation" position	CPCONLY	H01H2300/066		30
