E05F1/00	7	Closers or openers for wings, not otherwise provided for in this subclass	E05F1/00	E05F1/00		271
E05F1/002	8	{controlled by automatically acting means (for powered-operated mechanisms E05F15/70)}	E05F1/00	E05F1/00		253
E05F1/004	9	{by thermostats, rain, wind or noise (E05F1/006 takes precedence)}	E05F1/00	E05F1/00		245
E05F1/006	9	{by emergency conditions, e.g. fire (operating or controlling mechanisms for physical fire-barriers A62C2/24)}	E05F1/00	E05F1/00		699
E05F1/008	9	{by time control}	E05F1/00	E05F1/00		141
E05F1/02	8	gravity-actuated {, e.g. by use of counterweights}	E05F1/02	E05F1/02		500
E05F1/025	9	{with rectilinearly-moving counterweights}	E05F1/02	E05F1/02		414
E05F1/04	9	for wings which lift during movement {, operated by their own weight}	E05F1/04	E05F1/04		100
E05F1/043	10	{with cams, helical tracks (E05F1/061 takes precedence)}	E05F1/04	E05F1/04		64
E05F1/046	10	{with rectilinearly-inclined tracks for sliding wings}	E05F1/04	E05F1/04		171
E05F1/06	10	Mechanisms in the shape of hinges or pivots, operated by the weight of the wing	E05F1/06	E05F1/06		147
E05F1/061	11	{with cams or helical tracks}	E05F1/06	E05F1/06		189
E05F1/063	12	{with complementary, substantially identical and slidingly cooperating cam surfaces (E05F1/066 takes precedence)}	E05F1/06	E05F1/06		459
E05F1/065	12	{Cam-and-wheel arrangements}	E05F1/06	E05F1/06		103
E05F1/066	12	{Helical grooves, slots, threads or the like}	E05F1/06	E05F1/06		120
E05F1/068	11	{with inclined pivot-axes}	E05F1/06	E05F1/06		128
E05F1/08	8	spring-actuated {, e.g. for horizontally sliding wings (counterbalancing sliding or lifting wings E05D; springs per seF16F, e.g. gas-springs F16F9/00)}	E05F1/08	E05F1/08		353
E05F1/10	9	for swinging wings {, e.g. counterbalance}	E05F1/10	E05F1/10		910
E05F1/1008	10	{with a coil spring parallel with the pivot axis (E05F1/1207 takes precedence)}	E05F1/10	E05F1/10		302
E05F1/1016	11	{with a canted-coil torsion spring}	E05F1/10	E05F1/10		392
E05F1/1025	11	{with a compression or traction spring}	E05F1/10	E05F1/10		77
E05F1/1033	10	{with a torsion bar (E05F1/123 takes precedence)}	E05F1/10	E05F1/10		155
E05F1/1041	10	{with a coil spring perpendicular to the pivot axis (E05F1/1246 takes precedence)}	E05F1/10	E05F1/10		249
E05F1/105	11	{with a compression spring}	E05F1/10	E05F1/10		552
E05F1/1058	12	{for counterbalancing}	E05F1/10	E05F1/10		552
E05F1/1066	11	{with a traction spring}	E05F1/10	E05F1/10		559
E05F1/1075	12	{for counterbalancing}	E05F1/10	E05F1/10		521
E05F1/1083	10	{with a leaf or similar spring (E05F1/1284 takes precedence)}	E05F1/10	E05F1/10		133
E05F1/1091	10	{with a gas spring (E05F1/1292 takes precedence)}	E05F1/10	E05F1/10		926
E05F1/12	10	Mechanisms in the shape of hinges or pivots, operated by springs	E05F1/12	E05F1/12		763
E05F1/1207	11	{with a coil spring parallel with the pivot axis}	E05F1/12	E05F1/12		490
E05F1/1215	12	{with a canted-coil torsion spring}	E05F1/12	E05F1/12		1230
E05F1/1223	12	{with a compression or traction spring}	E05F1/12	E05F1/12		495
E05F1/123	11	{with a torsion bar}	E05F1/12	E05F1/12		318
E05F1/1238	12	{specially adapted for vehicles}	E05F1/12	E05F1/12		193
E05F1/1246	11	{with a coil spring perpendicular to the pivot axis}	E05F1/12	E05F1/12		188
E05F1/1253	12	{with a compression spring}	E05F1/12	E05F1/12		491
E05F1/1261	13	{for counterbalancing}	E05F1/12	E05F1/12		516
E05F1/1269	12	{with a traction spring}	E05F1/12	E05F1/12		145
E05F1/1276	13	{for counterbalancing}	E05F1/12	E05F1/12		380
E05F1/1284	11	{with a leaf or similar spring}	E05F1/12	E05F1/12		350
E05F1/1292	11	{with a gas spring}	E05F1/12	E05F1/12		209
E05F1/14	10	with double-acting springs, e.g. for closing and opening or checking and closing {no material}	E05F1/14	E05F1/14		364
E05F1/16	9	for sliding wings	E05F1/16	E05F1/16		1482
E05F3/00	7	Closers or openers with braking devices, e.g. checks; Construction of pneumatic or liquid braking devices (construction of non-pneumatic or non-liquid braking devices E05F5/00; friction devices in hinges E05D11/08)	E05F3/00	E05F3/00		516
E05F3/02	8	with pneumatic piston brakes (rotary type E05F3/14)	E05F3/02	E05F3/02		970
E05F3/04	8	with liquid piston brakes (rotary type E05F3/14)	E05F3/04	E05F3/04		787
E05F3/06	9	in which a torsion spring rotates a member around an axis perpendicular to the axis of the piston	E05F3/06	E05F3/06		278
E05F3/08	9	in which a torsion spring rotates a member around an axis arranged in the direction of the axis of the piston	E05F3/08	E05F3/08		177
E05F3/10	9	with a spring, other than a torsion spring, and a piston, the axes of which are the same or lie in the same direction	E05F3/10	E05F3/10		631
E05F3/102	10	{with rack-and-pinion transmission between driving shaft and piston within the closer housing}	E05F3/10	E05F3/10		685
E05F3/104	10	{with cam-and-slide transmission between driving shaft and piston within the closer housing}	E05F3/10	E05F3/10		721
E05F3/106	10	{with crank-arm transmission between driving shaft and piston within the closer housing}	E05F3/10	E05F3/10		151
E05F3/108	10	{with piston rod protruding from the closer housing; Telescoping closers}	E05F3/10	E05F3/10		522
E05F3/12	9	Special devices controlling the circulation of the liquid, e.g. valve arrangement ({E05F3/223 takes precedence}; valves per seF16K)	E05F3/12	E05F3/12		817
E05F3/14	8	with fluid brakes of the rotary type	E05F3/14	E05F3/14		557
E05F3/16	8	with friction brakes	E05F3/16	E05F3/16		441
E05F3/18	8	with counteracting springs (double-acting springs E05F1/14)	E05F3/18	E05F3/18		301
E05F3/20	8	in hinges	E05F3/20	E05F3/20		2162
E05F3/22	8	Additional arrangements for closers, e.g. for holding the wing in opened or other position	E05F3/22	E05F3/22		867
E05F3/221	9	{Mechanical power-locks, e.g. for holding the wing open or for free-moving zones}	E05F3/22	E05F3/22		376
E05F3/222	10	{electrically operated (E05F3/223 takes precedence)}	E05F3/22	E05F3/22		274
E05F3/223	9	{Hydraulic power-locks, e.g. with electrically operated hydraulic valves}	E05F3/22	E05F3/22		171
E05F3/224	9	{for assisting in opening the wing}	E05F3/22	E05F3/22		209
E05F3/225	9	{mounted at the bottom of wings, e.g. details related to seals, covers, connections to the wings, embedding in the floor}	E05F3/22	E05F3/22		299
E05F3/226	10	{with means to adjust the closed position of the wing}	E05F3/22	E05F3/22		114
E05F3/227	9	{mounted at the top of wings, e.g. details related to closer housings, covers, end caps or rails therefor}	E05F3/22	E05F3/22		634
E05F2003/228	9	{Arrangements where the end of the closer arm is sliding in a track}	E05F3/22	E05F3/22		389
E05F5/00	7	Braking devices, e.g. checks; Stops; Buffers (construction of pneumatic or liquid braking devices E05F3/00; braking devices, buffers or end stops on drawers for tables, cabinets or like furniture A47B88/473; combined with devices for holding wings open E05C17/00; devices for limiting opening of wings or for holding wings open by a movable member extending between frame and wing E05C17/04)	E05F5/00	E05F5/00		786
E05F5/003	8	{for sliding wings (Fasteners specially adapted for holding sliding wings open E05D13/04)}	E05F5/00	E05F5/00		2160
E05F5/006	8	{for hinges having a cup-shaped fixing part, e.g. for attachment to cabinets or furniture}	E05F5/00	E05F5/00		542
E05F5/02	8	specially for preventing the slamming of {swinging} wings {during final closing movement, e.g. jamb stops}	E05F5/02	E05F5/02		2230
E05F5/022	9	{specially adapted for vehicles, e.g. for hoods or trunks}	E05F5/02	E05F5/02		730
E05F5/025	10	{specially adapted for vehicle doors}	E05F5/02	E05F5/02		805
E05F5/027	9	{with closing action}	E05F5/02	E05F5/02		515
E05F5/04	9	hand-operated {, e.g. removable}; operated by centrifugal action {or by high closing speed}	E05F5/04	E05F5/04		320
E05F2005/043	10	{operated by centrifugal action at high closing speed}	E05F5/04	E05F5/04		37
E05F2005/046	10	{hand operated}	E05F5/04	E05F5/04		201
E05F5/06	8	Buffers {or stops limiting opening of swinging wings, e.g. floor or wall stops}(E05F5/02 takes precedence)	E05F5/06	E05F5/06		2713
E05F5/08	9	with springs	E05F5/08	E05F5/08		1674
E05F5/10	9	with piston brakes	E05F5/10	E05F5/10		1179
E05F5/12	8	specially for preventing the closing of a wing before another wing has been closed	E05F5/12	E05F5/12		491
E05F7/00	7	Accessories for wings not provided for in other groups of this subclass (specially adapted for furniture A47B95/00; door-lifters B66F, E04F21/00; knobs or handles E05B)	E05F7/00	E05F7/00		286
E05F7/005	8	{Aligning devices for wings}	E05F7/00	E05F7/00		309
E05F7/02	8	for raising wings before being turned {(before sliding E05D15/565)}	E05F7/02	E05F7/02		131
E05F7/04	8	Arrangements affording protection against rattling (with buffering action E05F5/00)	E05F7/04	E05F7/04		669
E05F7/06	8	Devices for taking the weight of the wing, arranged away from the hinge axis	E05F7/06	E05F7/06		426
E05F7/08	8	Means for transmitting movements between vertical and horizontal sliding bars, rods, or cables (means for transmitting movements between vertical and horizontal sliding bars, rods, or cables, for the fastening of wings E05C9/24{; with means for transmitting movements between vertical and horizontal sliding bars, rods or cables E05D15/5208})	E05F7/08	E05F7/08		337
E05F9/00	7	Means for operating wings by hand rods not guided in or on the frame, including those which also operate the fastening (bolts or fastening devices for wings E05C)	E05F9/00	E05F9/00		109
E05F11/00	7	Man-operated mechanisms for operating wings, including those which also operate the fastening (connecting mechanisms for a plurality of wings E05F17/00)	E05F11/00	E05F11/00		2885
E05F11/02	8	for wings in general, e.g. fanlights (E05F11/36 takes precedence; for windows to be lowered vertically E05F11/38; for doors E05F11/54)	E05F11/02	E05F11/02		342
E05F11/04	9	with cords, chains or cables	E05F11/04	E05F11/04		1373
E05F11/06	10	in guide-channels	E05F11/06	E05F11/06		349
E05F11/08	9	with longitudinally-moving bars guided, e.g. by pivoted links, in or on the frame	E05F11/08	E05F11/08		129
E05F11/10	10	Mechanisms by which a handle moves the bar	E05F11/10	E05F11/10		267
E05F11/12	10	Mechanisms by which the bar shifts the wing	E05F11/12	E05F11/12		392
E05F11/14	11	directly, i.e. without links, shifting the wing, e.g. by rack and gear or pin and slot	E05F11/14	E05F11/14		218
E05F11/145	12	{by pin and slot}	E05F11/14	E05F11/14		80
E05F11/16	11	shifting the wing by pivotally-connected members {(moving) in a plane perpendicular to the pivot axis of the wing}	E05F11/16	E05F11/16		498
E05F11/18	12	consisting of a lever, e.g. an angle lever, only {no material}	E05F11/18	E05F11/18		10
E05F11/20	12	consisting of a lever, e.g. an angle lever, and only one additional link {no material}	E05F11/20	E05F11/20		14
E05F11/22	12	consisting of a lever, e.g. an angle lever, and two or more additional links in series {no material}	E05F11/22	E05F11/22		18
E05F11/24	11	shifting the wing by pivotally-connected members {(moving) in a plane parallel to the pivot axis of the wing}	E05F11/24	E05F11/24		179
E05F11/26	12	consisting of a lever, e.g. an angle lever, only {no material}	E05F11/26	E05F11/26		3
E05F11/28	12	consisting of a lever, e.g. an angle lever, and one or more additional links {no material}	E05F11/28	E05F11/28		4
E05F11/30	12	consisting of links in rhomb-form {no material}	E05F11/30	E05F11/30		3
E05F11/32	9	with rotary bars guided in the frame (E05F11/34 takes precedence)	E05F11/32	E05F11/32		142
E05F11/34	9	with screw mechanisms	E05F11/34	E05F11/34		348
E05F11/36	8	specially designed for passing through a wall	E05F11/36	E05F11/36		214
E05F11/38	8	for sliding windows, e.g. vehicle windows, to be opened or closed by vertical movement<br><br><u>WARNING</u><br>Group E05F11/38 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/38	E05F11/38		177
E05F11/382	9	{for vehicle windows (E05F11/40&#160;-&#160;E05F11/52 take precedence)}<br><br><u>WARNING</u><br>Group E05F11/382 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/38	E05F11/38		2452
E05F11/385	10	{Fixing of window glass to the carrier of the operating mechanism}<br><br><u>WARNING</u><br>Group E05F11/385 is impacted by reclassification into groups E05F15/6892 and E05F15/6894.<br>Groups E05F11/385, E05F15/6892 and E05F15/6894 should be considered in order to perform a complete search.	E05F11/38	E05F11/38		740
E05F2011/387	11	{using arrangements in the window glass, e.g. holes}<br><br><u>WARNING</u><br>Group E05F2011/387 is impacted by reclassification into group E05F15/6894.<br>Groups E05F2011/387 and E05F15/6894 should be considered in order to perform a complete search.	E05F11/38	E05F11/38		258
E05F11/40	9	operated by screw mechanism<br><br><u>WARNING</u><br>Group E05F11/40 is impacted by reclassification into group E05F15/6896.<br>Groups E05F11/40 and E05F15/6896 should be considered in order to perform a complete search.	E05F11/40	E05F11/40		58
E05F11/405	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/405 is impacted by reclassification into group E05F15/6896.<br>Groups E05F11/405 and E05F15/6896 should be considered in order to perform a complete search.	E05F11/40	E05F11/40		174
E05F11/42	9	operated by rack bars and toothed wheels {or other push-pull mechanisms}<br><br><u>WARNING</u><br>Group E05F11/42 is impacted by reclassification into groups E05F15/6899 and E05F15/6901.<br>Groups E05F11/42, E05F15/6899 and E05F15/6901 should be considered in order to perform a complete search.	E05F11/42	E05F11/42		178
E05F11/423	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/423 is impacted by reclassification into groups E05F15/6899 and E05F15/6901. <br>Groups E05F11/423, E05F15/6899 and E05F15/6901 should be considered in order to perform a complete search.	E05F11/42	E05F11/42		202
E05F11/426	11	{Flexible rack-and-pinion arrangements}<br><br><u>WARNING</u><br>Group E05F11/426 is impacted by reclassification into group E05F15/6901.<br>Groups E05F11/426 and E05F15/6901 should be considered in order to perform a complete search.	E05F11/42	E05F11/42		185
E05F11/44	9	operated by one or more lifting arms<br><br><u>WARNING</u><br>Group E05F11/44 is impacted by reclassification into groups E05F15/6903 and E05F15/6905.<br>Groups E05F11/44, E05F15/6903 and E05F15/6905 should be considered in order to perform a complete search.	E05F11/44	E05F11/44		37
E05F11/445	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/445 is impacted by reclassification into groups E05F15/6903 and E05F15/6905. <br>Groups E05F11/445, E05F15/6903 and E05F15/6905 should be considered in order to perform a complete search.	E05F11/44	E05F11/44		736
E05F11/46	9	operated by lazy-tongs mechanism<br><br><u>WARNING</u><br>Group E05F11/46 is impacted by reclassification into groups E05F15/6903 and E05F15/6905. <br>Groups E05F11/46, E05F15/6903 and E05F15/6905 should be considered in order to perform a complete search.	E05F11/46	E05F11/46		10
E05F11/465	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/465 is impacted by reclassification into groups E05F15/6903 and E05F15/6905.<br>Groups E05F11/465, E05F15/6903 and E05F15/6905 should be considered in order to perform a complete search.	E05F11/46	E05F11/46		53
E05F11/48	9	operated by cords or chains {or other flexible elongated pulling elements, e.g. tapes}<br><br><u>WARNING</u><br>Group E05F11/48 is impacted by reclassification into groups E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914 and E05F15/6916. <br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/48	E05F11/48		247
E05F11/481	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/481 is impacted by reclassification into groups E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914 and E05F15/6916.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/48	E05F11/48		173
E05F11/483	11	{by cables}<br><br><u>WARNING</u><br>Group E05F11/483 is impacted by reclassification into groups E05F15/6909, E05F15/6911, E05F15/6914 and E05F15/6916.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/48	E05F11/48		717
E05F11/485	12	{with cable tensioners}<br><br><u>WARNING</u><br>Group E05F11/485 is impacted by reclassification into group E05F15/6911.<br>Groups E05F11/485 and E05F15/6911 should be considered in order to perform a complete search.	E05F11/48	E05F11/48		276
E05F11/486	12	{with one cable connection to the window glass}<br><br><u>WARNING</u><br>Group E05F11/486 is impacted by reclassification into group E05F15/6914.<br>Groups E05F11/486 and E05F15/6914 should be considered in order to perform a complete search.	E05F11/48	E05F11/48		424
E05F11/488	12	{with two cable connections to the window glass}<br><br><u>WARNING</u><br>Group E05F11/488 is impacted by reclassification into group E05F15/6916.<br>Groups E05F11/488 and E05F15/6916 should be considered in order to perform a complete search.	E05F11/48	E05F11/48		374
E05F11/50	9	Crank gear with clutches or retaining brakes, for operating window mechanisms<br><br><u>WARNING</u><br>Group E05F11/50 is impacted by reclassification into group E05F15/6918. <br>Groups E05F11/50 and E05F15/6918 should be considered in order to perform a complete search.	E05F11/50	E05F11/50		41
E05F11/505	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/505 is impacted by reclassification into group E05F15/6918.<br>Groups E05F11/505 and E05F15/6918 should be considered in order to perform a complete search.	E05F11/50	E05F11/50		277
E05F11/52	9	combined with means for producing an additional movement, e.g. a horizontal or a rotary movement<br><br><u>WARNING</u><br>Group E05F11/52 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/52	E05F11/52		47
E05F11/525	10	{for vehicle windows}<br><br><u>WARNING</u><br>Group E05F11/525 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F11/52	E05F11/52		139
E05F11/53	8	for sliding windows, e.g. vehicle windows, to be opened or closed by horizontal movement	E05F11/53	E05F11/53		214
E05F11/535	9	{for vehicle windows}	E05F11/53	E05F11/53		91
E05F11/54	8	for doors	E05F11/54	E05F11/54		1306
E05F13/00	7	Mechanisms operated by the movement or weight of a person or vehicle (through power-operated wing-operating mechanisms E05F15/00)	E05F13/00	E05F13/00		116
E05F13/02	8	by devices, e.g. lever arms, affected by the movement of the user	E05F13/02	E05F13/02		450
E05F13/04	8	by platforms lowered by the weight of the user	E05F13/04	E05F13/04		1296
E05F15/00	7	Power-operated mechanisms for wings (motor-operated accessories in locks for completing closing or initiating opening of a wing E05B17/00)	E05F15/00	E05F15/00		1682
E05F15/40	8	Safety devices, e.g. detection of obstructions or end positions	E05F15/40	E05F15/40		2847
E05F15/41	9	Detection by monitoring transmitted force or torque (E05F15/48 takes precedence); Safety couplings with activation dependent upon torque or force, e.g. slip couplings	E05F15/41	E05F15/41		1512
E05F15/42	9	Detection using safety edges	E05F15/42	E05F15/42		868
E05F15/43	10	responsive to disruption of energy beams, e.g. light or sound	E05F15/43	E05F15/43		1128
E05F15/431	11	{specially adapted for vehicle windows or roofs}	E05F15/43	E05F15/43		241
E05F2015/432	11	{with acoustical sensors}	E05F15/43	E05F15/43		128
E05F2015/433	12	{using reflection from the obstruction}	E05F15/43	E05F15/43		165
E05F2015/434	11	{with cameras or optical sensors}	E05F15/43	E05F15/43		463
E05F2015/435	12	{by interruption of the beam}	E05F15/43	E05F15/43		123
E05F2015/436	13	{the beam being parallel to the wing edge}	E05F15/43	E05F15/43		171
E05F2015/437	13	{the beam being perpendicular to the wing edge}	E05F15/43	E05F15/43		40
E05F15/44	10	responsive to changes in electrical conductivity	E05F15/44	E05F15/44		532
E05F15/443	11	{specially adapted for vehicle windows or roofs}	E05F15/44	E05F15/44		237
E05F2015/447	11	{using switches in serial arrangement}	E05F15/44	E05F15/44		63
E05F15/46	10	responsive to changes in electrical capacitance	E05F15/46	E05F15/46		367
E05F15/47	10	responsive to changes in fluid pressure	E05F15/47	E05F15/47		173
E05F15/48	10	by transmission of mechanical forces, e.g. rigid or movable members	E05F15/48	E05F15/48		267
E05F2015/483	10	{for detection during opening}	E05F15/42	E05F15/48		385
E05F2015/487	10	{Fault detection of safety edges}	E05F15/42	E05F15/48		117
E05F15/49	9	specially adapted for mechanisms operated by fluid pressure, e.g. detection by monitoring transmitted fluid pressure (E05F15/47 takes precedence)	E05F15/49	E05F15/49		122
E05F15/50	8	using fluid-pressure actuators	E05F15/50	E05F15/50		1043
E05F15/51	9	for folding wings	E05F15/51	E05F15/51		203
E05F15/53	9	for swinging wings	E05F15/53	E05F15/53		2002
E05F15/54	10	operated by linear actuators acting on a helical track coaxial with the swinging axis	E05F15/54	E05F15/54		128
E05F15/56	9	for horizontally-sliding wings	E05F15/56	E05F15/56		667
E05F15/565	10	{for railway-cars}	E05F15/56	E05F15/56		401
E05F15/57	9	for vertically-sliding wings	E05F15/57	E05F15/57		440
E05F15/59	10	for overhead wings	E05F15/59	E05F15/59		105
E05F15/60	8	using electrical actuators	E05F15/60	E05F15/60		2210
E05F15/603	9	using rotary electromotors	E05F15/603	E05F15/603		2326
E05F15/605	10	for folding wings	E05F15/605	E05F15/605		789
E05F15/608	10	for revolving wings	E05F15/608	E05F15/608		533
E05F15/611	10	for swinging wings	E05F15/611	E05F15/611		2301
E05F15/614	11	operated by meshing gear wheels, one of which being mounted at the wing pivot axis; operated by a motor acting directly on the wing pivot axis	E05F15/614	E05F15/614		1626
E05F15/616	11	operated by push-pull mechanisms	E05F15/616	E05F15/616		884
E05F15/619	12	using flexible or rigid rack-and-pinion arrangements	E05F15/619	E05F15/619		1001
E05F15/622	12	using screw-and-nut mechanisms	E05F15/622	E05F15/622		1939
E05F15/624	12	using friction wheels	E05F15/624	E05F15/624		100
E05F15/627	11	operated by flexible elongated pulling elements, e.g. belts, chains or cables (using flexible elongated push-pull mechanisms E05F15/619)<br><br><u>NOTE</u><br><br>In this group, it is desirable to add the indexing codes of E05Y2201/644.	E05F15/627	E05F15/627		1011
E05F15/63	11	operated by swinging arms	E05F15/63	E05F15/63		2348
E05F2015/631	12	{the end of the arm sliding in a track;  Slider arms therefor}	E05F15/63	E05F15/63		274
E05F15/632	10	for horizontally-sliding wings	E05F15/632	E05F15/632		1714
E05F15/635	11	operated by push-pull mechanisms, e.g. flexible or rigid rack-and-pinion arrangements (E05F15/652 takes precedence)	E05F15/635	E05F15/635		1419
E05F15/638	12	allowing or involving a secondary movement of the wing, e.g. rotational or transversal	E05F15/638	E05F15/638		332
E05F15/641	12	operated by friction wheels	E05F15/641	E05F15/641		222
E05F15/643	11	operated by flexible elongated pulling elements, e.g. belts, chains or cables (by flexible elongated push-pull mechanisms E05F15/635)	E05F15/643	E05F15/643		1984
E05F15/646	12	allowing or involving a secondary movement of the wing, e.g. rotational or transversal	E05F15/646	E05F15/646		715
E05F15/649	11	operated by swinging arms	E05F15/649	E05F15/649		245
E05F15/652	11	operated by screw-and-nut mechanisms	E05F15/652	E05F15/652		828
E05F15/655	11	specially adapted for vehicle wings	E05F15/655	E05F15/655		655
E05F15/657	12	enabling manual drive, e.g. in case of power failure	E05F15/657	E05F15/657		68
E05F15/659	12	Control circuits therefor	E05F15/659	E05F15/659		208
E05F15/662	12	Motor units therefor, e.g. geared motors	E05F15/662	E05F15/662		218
E05F15/665	10	for vertically-sliding wings	E05F15/665	E05F15/665		1066
E05F15/668	11	for overhead wings	E05F15/668	E05F15/668		1137
E05F15/67	12	operated by flexible or rigid rack-and-pinion arrangements	E05F15/67	E05F15/67		392
E05F15/673	12	operated by screw-and-nut mechanisms	E05F15/673	E05F15/673		197
E05F15/676	12	operated by friction wheels	E05F15/676	E05F15/676		78
E05F15/678	12	operated by swinging lever arms	E05F15/678	E05F15/678		69
E05F15/681	12	operated by flexible elongated pulling elements, e.g. belts	E05F15/681	E05F15/681		386
E05F15/684	13	by chains	E05F15/684	E05F15/684		466
E05F15/686	13	by cables or ropes	E05F15/686	E05F15/686		688
E05F15/689	11	specially adapted for vehicle windows<br><br><u>WARNING</u><br>Group E05F15/689 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/689		2258
E05F15/6892	12	{Fixing of window glass to the carrier of the operating mechanism}<br><br><u>WARNING</u><br>Group E05F15/6892 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/385, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/689		196
E05F15/6894	13	{using arrangements in the window glass, e.g. holes}<br><br><u>WARNING</u><br>Group E05F15/6894 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/385, E05F2011/387, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/689		4
E05F15/6896	12	{operated by screw mechanism}<br><br><u>WARNING</u><br>Group E05F15/6896 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/40, E05F11/405, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/689		11
E05F15/6899	12	{operated by rack bars and toothed wheels or other push-pull mechanisms}<br><br><u>WARNING</u><br>Group E05F15/6899 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/42, E05F11/423, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/689		23
E05F15/6901	13	{Flexible rack-and-pinion arrangements}<br><br><u>WARNING</u><br>Group E05F15/6901 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/42, E05F11/423, E05F11/426, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6901		1
E05F15/6903	12	{operated by one or more lifting arms}<br><br><u>WARNING</u><br>Groups E05F15/6903 and E05F15/6905 are incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/44, E05F11/445, E05F11/46, E05F11/465, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6903		64
E05F15/6905	13	{operated by lazy-tongs mechanism}	E05F15/689	E05F15/6905		23
E05F15/6907	12	{operated by cords or chains or other flexible elongated pulling elements, e.g. tapes}<br><br><u>WARNING</u><br>Group E05F15/6907 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/48, E05F11/481, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6907		11
E05F15/6909	13	{by cables}<br><br><u>WARNING</u><br>Group E05F15/6909 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/48, E05F11/481, E05F11/483, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6909		202
E05F15/6911	14	{with cable tensioners}<br><br><u>WARNING</u><br>Group E05F15/6911 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/48, E05F11/481, E05F11/483, E05F11/485, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6911		8
E05F15/6914	14	{with one cable connection to the window glass}<br><br><u>WARNING</u><br>Group E05F15/6914 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/48, E05F11/481, E05F11/483, E05F11/486, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6914		26
E05F15/6916	14	{with two cable connections to the window glass}<br><br><u>WARNING</u><br>Group E05F15/6916 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/48, E05F11/481, E05F11/483, E05F11/488, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6916		50
E05F15/6918	12	{Crank gear with clutches or retaining brakes, for operating window mechanisms}<br><br><u>WARNING</u><br>Group E05F15/6918 is incomplete pending reclassification of documents from groups E05F11/38, E05F11/382, E05F11/50, E05F11/505, E05F11/52, E05F11/525, E05F15/689, E05F15/692, E05F15/695 and E05F15/697.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/689	E05F15/6918		1
E05F15/692	12	enabling manual drive, e.g. in case of power failure<br><br><u>WARNING</u><br>Group E05F15/692 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/692	E05F15/692		192
E05F15/695	12	Control circuits therefor<br><br><u>WARNING</u><br>Group E05F15/695 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/695	E05F15/695		1824
E05F15/697	12	Motor units therefor, e.g. geared motors<br><br><u>WARNING</u><br>Group E05F15/697 is impacted by reclassification into groups E05F15/6892, E05F15/6894, E05F15/6896, E05F15/6899, E05F15/6901, E05F15/6903, E05F15/6905, E05F15/6907, E05F15/6909, E05F15/6911, E05F15/6914, E05F15/6916 and E05F15/6918.<br>All groups listed in this Warning should be considered in order to perform a complete search.	E05F15/697	E05F15/697		1371
E05F15/70	8	with automatic actuation	E05F15/70	E05F15/70		4978
E05F15/71	9	responsive to temperature changes, rain, wind or noise	E05F15/71	E05F15/71		2522
E05F15/72	9	responsive to emergency conditions, e.g. fire	E05F15/72	E05F15/72		2076
E05F15/73	9	responsive to movement or presence of persons or objects	E05F15/73	E05F15/73		4050
E05F15/74	10	using photoelectric cells	E05F15/74	E05F15/74		372
E05F15/75	10	responsive to the weight or other physical contact of a person or object	E05F15/75	E05F15/75		753
E05F15/76	10	responsive to devices carried by persons or objects, e.g. magnets or reflectors (E05F15/77 takes precedence)	E05F15/76	E05F15/76		514
E05F2015/763	10	{using acoustical sensors}	E05F15/73	E05F15/76		333
E05F2015/765	10	{using optical sensors}	E05F15/73	E05F15/76		558
E05F2015/767	10	{using cameras}	E05F15/73	E05F15/76		774
E05F15/77	9	using wireless control	E05F15/77	E05F15/77		2358
E05F15/78	10	using light beams	E05F15/78	E05F15/78		144
E05F15/79	9	using time control	E05F15/79	E05F15/79		845
E05F17/00	7	Special devices for shifting a plurality of wings operated simultaneously (for simultaneously moving a plurality of interconnected ventilating lamellae E06B7/086)	E05F17/00	E05F17/00		1216
E05F17/001	8	{of prison cell doors}	E05F17/00	E05F17/00		174
E05F17/002	8	{for wings which lie one behind the other when closed}	E05F17/00	E05F17/00		362
E05F17/004	8	{for wings which abut when closed}	E05F17/00	E05F17/00		1071
E05F2017/005	8	{for sliding wings}	E05F17/00	E05F17/00		658
E05F2017/007	9	{with means for interlocking the wings}	E05F17/00	E05F17/00		101
E05F2017/008	8	{for swinging wings}	E05F17/00	E05F17/00		318
