B66F1/00	7	Devices, e.g. jacks, for lifting loads in predetermined steps	B66F1/00	B66F1/00		132
B66F1/02	8	with locking elements, e.g. washers, co-operating with posts	B66F1/02	B66F1/02		453
B66F1/025	9	{the devices being operated by fluid pressure (B66F1/08 takes precedence)}	B66F1/02	B66F1/02		106
B66F1/04	9	the posts being toothed	B66F1/04	B66F1/04		34
B66F1/06	10	and the devices being actuated mechanically	B66F1/06	B66F1/06		1127
B66F1/08	10	and the devices being operated by fluid pressure	B66F1/08	B66F1/08		185
B66F3/00	7	Devices, e.g. jacks, adapted for uninterrupted lifting of loads (mobile jacks of the garage type B66F5/00)	B66F3/00	B66F3/00		561
B66F3/005	8	{with rocking arm or sector}	B66F3/00	B66F3/00		324
B66F3/02	8	with racks actuated by pinions	B66F3/02	B66F3/02		692
B66F3/04	9	with several racks	B66F3/04	B66F3/04		79
B66F3/06	9	with racks comprising pivotable toothed sections or segments, e.g. arranged in pairs	B66F3/06	B66F3/06		138
B66F3/08	8	screw operated (B66F3/44 takes precedence; gearings F16H)	B66F3/08	B66F3/08		1490
B66F3/10	9	with telescopic sleeves	B66F3/10	B66F3/10		570
B66F3/12	9	comprising toggle levers (lazy-tongs mechanisms B66F3/22)	B66F3/12	B66F3/12		1116
B66F3/14	9	actuated through pawl-and-ratchet mechanisms	B66F3/14	B66F3/14		214
B66F3/16	9	actuated through bevel-wheel gearings	B66F3/16	B66F3/16		758
B66F3/18	9	actuated through worm gearings	B66F3/18	B66F3/18		388
B66F3/20	9	actuated through multiple or change-speed gearings	B66F3/20	B66F3/20		157
B66F3/22	8	Lazy-tongs mechanisms {(B66F11/042 takes precedence)}	B66F3/22	B66F3/22		385
B66F3/24	8	fluid-pressure operated (water-pressure machines F03B; hydraulic gearings F16H; cylinders, pistons F16J; fluid-pressure servomotors F15B)	B66F3/24	B66F3/24		1566
B66F3/242	9	{suspended jacks}	B66F3/24	B66F3/24		121
B66F3/245	9	{comprising toggle levers (lazy-tongs mechanisms B66F3/22)}	B66F3/24	B66F3/24		66
B66F3/247	9	{pneumatically actuated (B66F3/35 takes precedence)}	B66F3/24	B66F3/24		511
B66F3/25	9	Constructional features	B66F3/25	B66F3/25		1144
B66F3/26	10	Adaptations or arrangements of pistons	B66F3/26	B66F3/26		362
B66F3/28	11	telescopic	B66F3/28	B66F3/28		247
B66F3/30	10	with positive brakes or locks	B66F3/30	B66F3/30		458
B66F3/32	10	with means for avoiding excessive shocks on completion of movements	B66F3/32	B66F3/32		71
B66F3/35	10	Inflatable flexible elements, e.g. bellows (inflatable load-engaging elements B66F3/40; connection of valves to inflatable elastic bodies B60C29/00)	B66F3/35	B66F3/35		662
B66F3/36	10	Load-engaging elements	B66F3/36	B66F3/36		296
B66F3/38	11	adjustable relative to piston	B66F3/38	B66F3/38		124
B66F3/40	11	inflatable (connection of valves to inflatable elastic bodies B60C29/00)	B66F3/40	B66F3/40		16
B66F3/42	10	with self-contained pumps, e.g. actuated by hand	B66F3/42	B66F3/42		1287
B66F3/43	9	Pyrotechnical jacks	B66F3/43	B66F3/43		102
B66F3/44	8	with self-contained electric driving motors	B66F3/44	B66F3/44		956
B66F3/46	8	Combinations of several jacks with means for interrelating lifting or lowering movements	B66F3/46	B66F3/46		1084
B66F5/00	7	Mobile jacks of the garage type mounted on wheels or rollers	B66F5/00	B66F5/00		256
B66F5/02	8	with mechanical lifting gear	B66F5/02	B66F5/02		291
B66F5/025	9	{screw-actuated}	B66F5/02	B66F5/02		213
B66F5/04	8	with fluid-pressure-operated lifting gear	B66F5/04	B66F5/04		925
B66F7/00	7	Lifting frames, e.g. for lifting vehicles; Platform lifts ({B66F11/04 takes precedence } ; for lift-truck platform B66F9/06)	B66F7/00	B66F7/00		1340
B66F7/02	8	with platforms suspended from ropes, cables, or chains {or screws and movable along pillars}	B66F7/02	B66F7/02		2654
B66F7/025	9	{screw operated}	B66F7/02	B66F7/02		1089
B66F7/04	9	hydraulically or pneumatically operated	B66F7/04	B66F7/04		741
B66F7/06	8	with platforms supported by levers for vertical movement	B66F7/06	B66F7/06		504
B66F7/0608	9	{driven by screw or spindle}	B66F7/06	B66F7/06		917
B66F7/0616	9	{Suspended platforms, i.e. the load platform hangs from the base}	B66F7/06	B66F7/06		85
B66F7/0625	9	{with wheels for moving around the floor}	B66F7/06	B66F7/06		1931
B66F7/0633	9	{Mechanical arrangements not covered by the following subgroups}	B66F7/06	B66F7/06		577
B66F7/0641	9	{Single levers, e.g. parallel links}	B66F7/06	B66F7/06		894
B66F7/065	9	{Scissor linkages, i.e. X-configuration}	B66F7/06	B66F7/06		2809
B66F7/0658	10	{Multiple scissor linkages horizontally arranged}	B66F7/06	B66F7/06		291
B66F7/0666	10	{Multiple scissor linkages vertically arranged}	B66F7/06	B66F7/06		1615
B66F7/0675	11	{Auxiliary scissors, e.g. above main scissors}	B66F7/06	B66F7/06		56
B66F7/0683	10	{Scissor linkage plus tilting action}	B66F7/06	B66F7/06		56
B66F7/0691	9	{Asymmetric linkages, i.e. Y-configuration}	B66F7/06	B66F7/06		204
B66F7/08	9	hydraulically or pneumatically operated	B66F7/08	B66F7/08		3074
B66F7/085	10	{pneumatically operated}	B66F7/08	B66F7/08		341
B66F7/10	8	with platforms supported directly by jacks	B66F7/10	B66F7/10		575
B66F7/12	9	by mechanical jacks	B66F7/12	B66F7/12		713
B66F7/14	10	screw operated	B66F7/14	B66F7/14		1530
B66F7/16	9	by one or more hydraulic or pneumatic jacks	B66F7/16	B66F7/16		1330
B66F7/18	10	by a single central jack	B66F7/18	B66F7/18		953
B66F7/20	10	by several jacks with means for maintaining the platforms horizontal during movement	B66F7/20	B66F7/20		959
B66F7/22	8	with tiltable platforms (tilting vehicles for unloading B65G67/34)	B66F7/22	B66F7/22		1186
B66F7/24	8	for raising or lowering vehicles by their own power	B66F7/24	B66F7/24		121
B66F7/243	9	{Ramps}	B66F7/24	B66F7/24		769
B66F7/246	9	{Wheel supporting trolleys}	B66F7/24	B66F7/24		189
B66F7/26	8	for selective lifting of parts of vehicles (mobile garage jacks B66F5/00)	B66F7/26	B66F7/26		222
B66F7/28	8	Constructional details, e.g. end stops, pivoting supporting members, sliding runners adjustable to load dimensions	B66F7/28	B66F7/28		11536
B66F9/00	7	Devices for lifting or lowering bulky or heavy goods for loading or unloading purposes (mobile or transportable lifts in, or associated with, buildings and specially adapted to be shifted from one part of a building or other structure to another part or to another building or structure B66B9/16; cranes B66C)	B66F9/00	B66F9/00		192
B66F9/02	8	Stationary loaders or unloaders, e.g. for sacks	B66F9/02	B66F9/02		934
B66F9/04	9	hydraulically actuated or controlled	B66F9/04	B66F9/04		217
B66F9/06	8	movable, with their loads, on wheels or the like, e.g. fork-lift trucks (vehicle aspects B60&#160;-&#160;B62; vehicles predominantly for transporting loads and modified to facilitate loading or unloading B60P1/00; low-lift hand trucks for transporting goods B62B3/06)	B66F9/06	B66F9/06		3442
B66F9/061	9	{characterised by having a lifting jib}	B66F9/06	B66F9/06		444
B66F9/063	9	{Automatically guided}	B66F9/06	B66F9/06		2283
B66F9/065	9	non-masted (mobile jacks of the garage type mounted on wheels or rollers B66F5/00)	B66F9/065	B66F9/065		1568
B66F9/0655	10	{with a telescopic boom}	B66F9/065	B66F9/065		700
B66F9/07	9	Floor-to-roof stacking devices, e.g. "stacker cranes", "retrievers"	B66F9/07	B66F9/07		1881
B66F9/072	10	{Travelling gear therefor}	B66F9/07	B66F9/07		420
B66F9/075	9	Constructional features or details	B66F9/075	B66F9/075		2595
B66F9/07504	10	{Accessories, e.g. for towing, charging, locking}	B66F9/075	B66F9/075		2912
B66F9/07509	10	{Braking}	B66F9/075	B66F9/075		566
B66F9/07513	10	{Details concerning the chassis}	B66F9/075	B66F9/075		687
B66F9/07518	11	{Fuel or oil tank arrangements}	B66F9/075	B66F9/075		176
B66F9/07522	11	{Variable length or width chassis}	B66F9/075	B66F9/075		88
B66F9/07527	11	{Covers for, e.g. engines or batteries}	B66F9/075	B66F9/075		138
B66F9/07531	11	{Battery compartments}	B66F9/075	B66F9/075		458
B66F9/07536	12	{Battery stoppers, i.e. means to hold battery in position}	B66F9/075	B66F9/075		149
B66F9/0754	11	{Battery removal arrangements}	B66F9/075	B66F9/075		253
B66F9/07545	10	{Overhead guards}	B66F9/075	B66F9/075		609
B66F9/0755	10	{Position control; Position detectors}	B66F9/075	B66F9/075		3209
B66F9/07554	10	{Counterweights}	B66F9/075	B66F9/075		665
B66F9/07559	10	{Stabilizing means}	B66F9/075	B66F9/075		946
B66F9/07563	10	{Fork-lift trucks adapted to be carried by transport vehicles}	B66F9/075	B66F9/075		285
B66F9/07568	10	{Steering arrangements}	B66F9/075	B66F9/075		1340
B66F9/07572	10	{Propulsion arrangements}	B66F9/075	B66F9/075		1680
B66F9/07577	11	{not supported by wheels, e.g. tracks or air cushions}	B66F9/075	B66F9/075		135
B66F9/07581	10	{Remote controls}	B66F9/075	B66F9/075		518
B66F9/07586	10	{Suspension or mounting of wheels on chassis}	B66F9/075	B66F9/075		748
B66F9/0759	10	{Details of operating station, e.g. seats, levers, operator platforms, cabin suspension}	B66F9/075	B66F9/075		1193
B66F9/07595	10	{Cooling arrangements for device or operator}	B66F9/075	B66F9/075		333
B66F9/08	10	Masts; Guides; Chains	B66F9/08	B66F9/08		2107
B66F9/082	11	{inclinable}	B66F9/08	B66F9/08		586
B66F9/085	11	{Multiple forks, i.e. more than one pair mounted on a single mast or with more than one mast}	B66F9/08	B66F9/08		136
B66F9/087	11	{Monomasts}	B66F9/08	B66F9/08		129
B66F9/10	11	movable in a horizontal direction relative to truck	B66F9/10	B66F9/10		758
B66F9/105	12	{Articulated, i.e. front chassis with wheels and mast rotatable relative to rear chassis with wheels}	B66F9/10	B66F9/10		76
B66F9/12	10	Platforms; Forks; Other load supporting or gripping members	B66F9/12	B66F9/12		3463
B66F9/122	11	{longitudinally movable}	B66F9/12	B66F9/12		1144
B66F9/125	11	{rotatable about a longitudinal axis}	B66F9/12	B66F9/12		351
B66F9/127	11	{Working platforms}	B66F9/12	B66F9/12		272
B66F9/14	11	laterally movable, e.g. swingable, for slewing or transverse movements	B66F9/14	B66F9/14		531
B66F9/141	12	{with shuttle-type movement}	B66F9/14	B66F9/14		367
B66F9/142	12	{Movements of forks either individually or relative to each other}	B66F9/14	B66F9/14		250
B66F9/143	13	{Movements of forks relative to each other - symmetric}	B66F9/14	B66F9/14		376
B66F9/144	13	{Movements of forks relative to each other - independent}	B66F9/14	B66F9/14		135
B66F9/145	13	{Rotation of fork around vertical axis}	B66F9/14	B66F9/14		99
B66F9/146	12	{Side shift, i.e. both forks move together sideways relative to fork support}	B66F9/14	B66F9/14		148
B66F9/147	12	{Whole unit including fork support moves relative to mast}	B66F9/14	B66F9/14		200
B66F9/148	13	{Whole unit including fork support moves sideways}	B66F9/14	B66F9/14		236
B66F9/149	13	{Whole unit including fork support rotates}	B66F9/14	B66F9/14		261
B66F9/16	11	inclinable relative to mast	B66F9/16	B66F9/16		598
B66F9/165	12	{Foldable forks, i.e. where only the horizontal section moves}	B66F9/16	B66F9/16		95
B66F9/18	11	Load gripping or retaining means	B66F9/18	B66F9/18		2880
B66F9/181	12	{by suction means}	B66F9/18	B66F9/18		298
B66F9/182	12	{by magnetic means}	B66F9/18	B66F9/18		92
B66F9/183	12	{Coplanar side clamps}	B66F9/18	B66F9/18		632
B66F9/184	12	{Roll clamps}	B66F9/18	B66F9/18		312
B66F9/185	12	{by internally expanding grippers}	B66F9/18	B66F9/18		83
B66F9/186	12	{Container lifting frames}	B66F9/18	B66F9/18		249
B66F9/187	12	{Drum lifting devices}	B66F9/18	B66F9/18		299
B66F9/188	12	{Stacked-bricks lifting devices}	B66F9/18	B66F9/18		152
B66F9/19	11	Additional means for facilitating unloading	B66F9/19	B66F9/19		1009
B66F9/195	12	{for pushing the load}	B66F9/19	B66F9/19		444
B66F9/20	10	Means for actuating or controlling masts, platforms, or forks (power take-off from vehicle transmissions, combined with vehicle propulsion systems B60K)	B66F9/20	B66F9/20		1766
B66F9/205	11	{Arrangements for transmitting pneumatic, hydraulic or electric power to movable parts or devices (for cranes B66C13/12)}	B66F9/20	B66F9/20		632
B66F9/22	11	Hydraulic devices or systems	B66F9/22	B66F9/22		3732
B66F9/24	11	Electrical devices or systems	B66F9/24	B66F9/24		3440
B66F11/00	7	Lifting devices specially adapted for particular uses not otherwise provided for (ground-engaging vehicle fittings for supporting, lifting or manoeuvring the vehicle B60S9/00)	B66F11/00	B66F11/00		3177
B66F11/04	8	for movable platforms or cabins, e.g. on vehicles, permitting workmen to place themselves in any desired position for carrying out required operations ({Working platforms on fork-lift trucks B66F9/127; } vehicle aspects of service vehicles B60P3/14; platforms for cleaning windows A47L3/02; devices for rescuing persons from buildings A62B1/02; liftable or lowerable platforms for use on ladders E06C7/16; maintenance travellers for bridges E01D19/10; scaffolds on an extensible sub-structure E04G1/22)	B66F11/04	B66F11/04		4415
B66F11/042	9	{actuated by lazy-tongs mechanisms or articulated levers}	B66F11/04	B66F11/04		1980
B66F11/044	9	{Working platforms suspended from booms}	B66F11/04	B66F11/04		1623
B66F11/046	10	{of the telescoping type}	B66F11/04	B66F11/04		1558
B66F11/048	9	{Mobile camera platform}	B66F11/04	B66F11/04		289
B66F13/00	7	Common constructional features or accessories	B66F13/00	B66F13/00		3623
B66F13/005	8	{Thrust chain devices}	B66F13/00	B66F13/00		119
B66F15/00	7	Crowbars or levers	B66F15/00	B66F15/00		2147
B66F17/00	7	Safety devices, e.g. for limiting or indicating lifting force	B66F17/00	B66F17/00		2175
B66F17/003	8	{for fork-lift trucks}	B66F17/00	B66F17/00		2825
B66F17/006	8	{for working platforms}	B66F17/00	B66F17/00		3709
B66F19/00	7	Hoisting, lifting, hauling or pushing, not otherwise provided for	B66F19/00	B66F19/00		2309
B66F19/005	8	{Lifting devices for manhole covers}	B66F19/00	B66F19/00		894
B66F2700/00	7	Lifting apparatus	CPCONLY	B66F2700/00		87
B66F2700/02	8	Lifting devices with a toothed post and pawl latch or with a post and locking elements	CPCONLY	B66F2700/02		21
B66F2700/025	9	with a post and locking elements	CPCONLY	B66F2700/025		25
B66F2700/03	8	Lifting jacks with pinion and rack	CPCONLY	B66F2700/03		127
B66F2700/04	8	Jacks with screw and nut	CPCONLY	B66F2700/04		282
B66F2700/05	8	Hydraulic jacks	CPCONLY	B66F2700/05		348
B66F2700/052	9	Support- or transmission members	CPCONLY	B66F2700/052		132
B66F2700/055	9	Jacks with a single cylinder	CPCONLY	B66F2700/055		100
B66F2700/057	10	Pistons, e.g. telescopic; Cylinders or sealing joints; Hydraulic travel-limiting devices or shock damping	CPCONLY	B66F2700/057		129
B66F2700/07	8	Lifting devices actuated by the driving force of water	CPCONLY	B66F2700/07		14
B66F2700/09	8	Other lifting devices	CPCONLY	B66F2700/09		805
B66F2700/12	8	Lifting platforms for vehicles or motorcycles or similar lifting apparatus	CPCONLY	B66F2700/12		474
B66F2700/123	9	Details concerning the support members or devices not related to the lifting itself	CPCONLY	B66F2700/123		182
B66F2700/126	9	Arrangements in which the platform is fixed to the upper end of a single or plural jacks	CPCONLY	B66F2700/126		23
