B26F1/00	7	Perforating; Punching; Cutting-out; Stamping-out; Apparatus therefor (perforating by laser beam B23K26/00; subjecting the grinding tools or the abrading medium to vibration, e.g. grinding with ultrasonic frequency, B24B1/04; perforating by sand-blasting B24C; punching cards or tapes for statistical and record purposes G06K1/00)	B26F1/00	B26F1/00		811
B26F1/0007	8	{Perforation of photographic films}	B26F1/00	B26F1/00		126
B26F1/0015	8	{specially adapted for perforating tubes}	B26F1/00	B26F1/00		289
B26F1/0023	9	{by rotary tools, e.g. saws (B26F1/0076 takes precedence)}	B26F1/00	B26F1/00		86
B26F1/003	10	{of the drill type}	B26F1/00	B26F1/00		116
B26F1/0038	9	{from the inside (B26F1/0053 takes precedence)}	B26F1/00	B26F1/00		69
B26F1/0046	9	{by tools that follow a closed path around the tube (B26F1/0053 takes precedence)}	B26F1/00	B26F1/00		15
B26F1/0053	9	{by machining, e.g. cutting, grinding, projections on the tube wall}	B26F1/00	B26F1/00		103
B26F1/0061	9	{whereby the tube moves axially or radially (B26F1/0038, B26F1/0046, B26F1/0053 take precedence)}	B26F1/00	B26F1/00		44
B26F1/0069	10	{and the tool travels with the tube}	B26F1/00	B26F1/00		46
B26F1/0076	10	{and the tool rotates}	B26F1/00	B26F1/00		31
B26F1/0084	8	{specially adapted for perforating rubber}	B26F1/00	B26F1/00		191
B26F1/0092	8	{Perforating means specially adapted for printing machines (B26F1/02&#160;-&#160;B26F1/46 take precedence)}	B26F1/00	B26F1/00		228
B26F1/02	8	Perforating by punching, e.g. with relatively-reciprocating punch and bed	B26F1/02	B26F1/02		2790
B26F1/04	9	with selectively-operable punches	B26F1/04	B26F1/04		772
B26F1/06	9	with punching tools moving with the work	B26F1/06	B26F1/06		95
B26F1/08	10	wherein the tools are carried by, and in operation move relative to, a rotative drum or similar support	B26F1/08	B26F1/08		228
B26F1/10	10	Roller type punches	B26F1/10	B26F1/10		433
B26F1/12	9	to notch margins of work	B26F1/12	B26F1/12		419
B26F1/14	9	Punching tools; Punching dies	B26F1/14	B26F1/14		2585
B26F1/16	8	Perforating by tool or tools of the drill type	B26F1/16	B26F1/16		3795
B26F1/165	9	{by flow drilling (for metal B21C37/292)}	B26F1/16	B26F1/16		10
B26F1/18	8	Perforating by slitting, i.e. forming cuts closed at their ends without removal of material	B26F1/18	B26F1/18		422
B26F1/20	9	with tools carried by a rotating drum or similar support (B26F1/22 takes precedence)	B26F1/20	B26F1/20		771
B26F1/22	9	to form non-rectilinear cuts, e.g. for tabs	B26F1/22	B26F1/22		187
B26F1/24	8	Perforating by needles or pins	B26F1/24	B26F1/24		1793
B26F1/26	8	Perforating by non-mechanical means, e.g. by fluid jet	B26F1/26	B26F1/26		520
B26F1/28	9	by electrical discharges	B26F1/28	B26F1/28		293
B26F1/31	9	by radiation (by laser beam B23K26/00)	B26F1/31	B26F1/31		86
B26F1/32	8	Hand-held perforating or punching apparatus, e.g. awls	B26F1/32	B26F1/32		788
B26F1/34	9	power actuated (details or components, e.g. casings, bodies, of portable power-driven tools not particularly related to the operation performed B25F5/00)	B26F1/34	B26F1/34		196
B26F1/36	9	Punching or perforating pliers	B26F1/36	B26F1/36		2151
B26F2001/365	10	{hand held pliers with handles}	B26F1/36	B26F1/36		316
B26F1/38	8	Cutting-out; Stamping-out	B26F1/38	B26F1/38		2533
B26F1/3806	9	{wherein relative movements of tool head and work during cutting have a component tangential to the work surface (B26F1/40 takes precedence)}	B26F1/38	B26F1/38		328
B26F1/3813	10	{wherein the tool head is moved in a plane parallel to the work in a coordinate system fixed with respect to the work}	B26F1/38	B26F1/38		663
B26F1/382	11	{wherein the cutting member reciprocates in, or substantially in, a direction parallel to the cutting edge}	B26F1/38	B26F1/38		569
B26F1/3826	11	{using a rotary circular cutting member}	B26F1/38	B26F1/38		179
B26F1/3833	11	{using an endless band-knife or the like}	B26F1/38	B26F1/38		92
B26F1/384	9	{using rotating drums}	B26F1/38	B26F1/38		1158
B26F1/3846	9	{cutting out discs or the like (B26F1/384, B26F1/40 and B26F1/44 take precedence)}	B26F1/38	B26F1/38		590
B26F1/3853	9	{cutting out frames (B26F1/384, B26F1/40 and B26F1/44 take precedence)}	B26F1/38	B26F1/38		171
B26F1/386	9	{Draw punches, i.e. punch and die assembled on opposite sides of a workpiece via a connecting member passing through an aperture in the workpiece}	B26F1/38	B26F1/38		82
B26F1/3866	9	{specially adapted for rubber}	B26F1/38	B26F1/38		122
B26F2001/3873	9	{advancing the material stepwise onto the work surface of the cutting machine}	B26F1/38	B26F1/38		49
B26F2001/388	9	{controlling the blade orientation along the cutting path}	B26F1/38	B26F1/38		50
B26F2001/3886	9	{shearing by reciprocating a straight blade, e.g. nibbling}	B26F1/38	B26F1/38		43
B26F2001/3893	9	{cutting out by using an oscillating needle}	B26F1/38	B26F1/38		50
B26F1/40	9	using a press, e.g. of the ram type (presses in general B30B)	B26F1/40	B26F1/40		4131
B26F2001/402	10	{curvilinear cutting presses, i.e. the stroke comprising an overlay of a linear and a curved movement}	B26F1/40	B26F1/40		42
B26F1/405	10	{Travelling head presses}	B26F1/40	B26F1/40		135
B26F2001/407	10	{stepwise sequential punching processes}	B26F1/40	B26F1/40		53
B26F1/42	10	having a pressure roller	B26F1/42	B26F1/42		355
B26F1/44	9	Cutters therefor; Dies therefor	B26F1/44	B26F1/44		5127
B26F2001/4409	10	{having die balancing or compensating means}	B26F1/44	B26F1/44		96
B26F2001/4418	10	{combining cutting and embossing operations}	B26F1/44	B26F1/44		174
B26F2001/4427	10	{combining cutting and forming operations}	B26F1/44	B26F1/44		250
B26F2001/4436	10	{Materials or surface treatments therefore}	B26F1/44	B26F1/44		132
B26F2001/4445	10	{Matrices, female dies, creasing tools}	B26F1/44	B26F1/44		119
B26F2001/4454	10	{Die heads carrying several moveable tools}	B26F1/44	B26F1/44		35
B26F2001/4463	10	{Methods and devices for rule setting, fixation, preparing cutting dies}	B26F1/44	B26F1/44		724
B26F2001/4472	10	{Cutting edge section features}	B26F1/44	B26F1/44		393
B26F2001/4481	10	{having special lateral or edge outlines or special surface shapes, e.g. apertures}	B26F1/44	B26F1/44		333
B26F2001/449	10	{for shearing, e.g. with adjoining or abutting edges}	B26F1/44	B26F1/44		102
B26F1/46	10	Loose press knives	B26F1/46	B26F1/46		114
B26F3/00	7	Severing by means other than cutting; Apparatus therefor (severing by grinding B24B27/06)	B26F3/00	B26F3/00		464
B26F3/002	8	{Precutting and tensioning or breaking}	B26F3/00	B26F3/00		792
B26F3/004	8	{by means of a fluid jet (methods for use of abrasive blasting for cutting B24C1/045; guns for abrasive fluid jets B24C5/02; perforating by non-mechanical means, e.g. by fluid jet B26F1/26)}	B26F3/00	B26F3/00		1857
B26F2003/006	9	{having a shutter or water jet deflector}	B26F3/00	B26F3/00		106
B26F3/008	9	{Energy dissipating devices therefor, e.g. catchers; Supporting beds therefor (cutting beds in general B26D7/20)}	B26F3/00	B26F3/00		234
B26F3/02	8	Tearing	B26F3/02	B26F3/02		432
B26F3/04	8	Severing by squeezing (B26F3/08 takes precedence)	B26F3/04	B26F3/04		147
B26F3/06	8	Severing by using heat	B26F3/06	B26F3/06		560
B26F3/08	9	with heated members	B26F3/08	B26F3/08		552
B26F3/10	10	with heated rollers or discs	B26F3/10	B26F3/10		52
B26F3/12	10	with heated wires	B26F3/12	B26F3/12		1107
B26F3/16	9	by radiation (by laser beam B23K26/00)	B26F3/16	B26F3/16		131
B26F2210/00	7	Perforating, punching, cutting-out, stamping-out, severing by means other than cutting of specific products	CPCONLY	B26F2210/00		144
B26F2210/02	8	of stacked sheets	CPCONLY	B26F2210/02		143
B26F2210/04	8	Making plastic pilferproof screw caps by cutting a tamper ring	CPCONLY	B26F2210/04		109
B26F2210/06	8	Trimming plastic mouldings	CPCONLY	B26F2210/06		104
B26F2210/08	8	of ceramic green sheets, printed circuit boards and the like	CPCONLY	B26F2210/08		671
B26F2210/11	8	of plastic containers before compressing	CPCONLY	B26F2210/11		29
B26F2210/12	8	of fabrics	CPCONLY	B26F2210/12		266
B26F2210/14	9	the cutting machine comprising a rotary knife	CPCONLY	B26F2210/14		126
B26F2210/16	9	the cutting machine comprising a cutting die	CPCONLY	B26F2210/16		187
