B25C1/00	7	Hand-held nailing tools (hammers per seB25D; nailing machines B27F7/02); Nail feeding devices	B25C1/00	B25C1/00		421
B25C1/001	8	{Nail feeding devices (B25C1/184 takes precedence)}	B25C1/00	B25C1/00		715
B25C1/003	9	{for belts of nails}	B25C1/00	B25C1/00		338
B25C1/005	9	{for rows of contiguous nails}	B25C1/00	B25C1/00		703
B25C1/006	9	{for corrugated nails and marking tags}	B25C1/00	B25C1/00		64
B25C1/008	8	{Safety devices}	B25C1/00	B25C1/00		912
B25C1/02	8	operated by manual power	B25C1/02	B25C1/02		680
B25C1/04	8	operated by fluid pressure {, e.g. by air pressure}	B25C1/04	B25C1/04		850
B25C1/041	9	{with fixed main cylinder}	B25C1/04	B25C1/04		448
B25C1/042	10	{Main valve and main cylinder}	B25C1/04	B25C1/04		148
B25C1/043	10	{Trigger valve and trigger mechanism}	B25C1/04	B25C1/04		245
B25C1/044	9	{with movable main cylinder}	B25C1/04	B25C1/04		52
B25C1/045	10	{main valve and main cylinder}	B25C1/04	B25C1/04		30
B25C1/046	10	{Trigger valve and trigger mechanism}	B25C1/04	B25C1/04		35
B25C1/047	9	{Mechanical details}	B25C1/04	B25C1/04		909
B25C1/048	9	{Hydraulically operated}	B25C1/04	B25C1/04		28
B25C1/06	8	operated by electric power	B25C1/06	B25C1/06		1354
B25C1/08	8	operated by combustion pressure	B25C1/08	B25C1/08		756
B25C1/082	9	{generated by detonation of a pellet}	B25C1/08	B25C1/08		41
B25C1/085	10	{trigger operated}	B25C1/08	B25C1/08		31
B25C1/087	10	{operated by a hammer blow}	B25C1/08	B25C1/08		24
B25C1/10	9	generated by detonation of a cartridge	B25C1/10	B25C1/10		134
B25C1/105	10	{Cartridge ejecting mechanisms and latch mechanisms}	B25C1/10	B25C1/10		99
B25C1/12	10	acting directly on the bolt	B25C1/12	B25C1/12		107
B25C1/123	11	{trigger operated}	B25C1/12	B25C1/12		109
B25C1/126	11	{operated by a hammer blow}	B25C1/12	B25C1/12		44
B25C1/14	10	acting on an intermediate plunger or anvil (pistols for slaughtering or stunning animals A22B3/02)	B25C1/14	B25C1/14		330
B25C1/143	11	{trigger operated}	B25C1/14	B25C1/14		237
B25C1/146	11	{operated by a hammer blow}	B25C1/14	B25C1/14		82
B25C1/16	10	Cartridges specially adapted for impact tools; Cartridge and bolts units (bolts per seF16B19/14)	B25C1/16	B25C1/16		68
B25C1/163	11	{Cartridges}	B25C1/16	B25C1/16		134
B25C1/166	11	{Pellets}	B25C1/16	B25C1/16		36
B25C1/18	10	Details and accessories, e.g. splinter guards, spall minimisers	B25C1/18	B25C1/18		373
B25C1/182	11	{Feeding devices}	B25C1/18	B25C1/18		25
B25C1/184	12	{for nails}	B25C1/18	B25C1/18		160
B25C1/186	12	{for cartridges or pellets}	B25C1/18	B25C1/18		137
B25C1/188	11	{Arrangements at the forward end of the barrel, e.g. splinter guards, spall minimisers, safety arrangements, silencers, bolt retainers}	B25C1/18	B25C1/18		434
B25C3/00	7	Portable devices for holding and guiding nails; Nail dispensers	B25C3/00	B25C3/00		151
B25C3/002	8	{nail dispensers with provision for holding and guiding nails}	B25C3/00	B25C3/00		177
B25C3/004	9	{the nail being hit by a hammer head}	B25C3/00	B25C3/00		40
B25C3/006	8	{only for holding and guiding}	B25C3/00	B25C3/00		362
B25C3/008	9	{the nail being hit by a hammer head}	B25C3/00	B25C3/00		374
B25C5/00	7	Manually operated portable stapling tools; Hand-held power-operated stapling tools ({clip clamping hand tools B25B27/146;} details or components, e.g. casings, bodies, of portable power-driven tools not particularly related to the operation performed B25F5/00; stapling machines B27F7/17); Staple feeding devices therefor (staples F16B15/00)<br><br><u>NOTE</u><br><br>In this group the following term is used with the meaning indicated: <br>"stapling tools" covers tools for driving U-shaped loops, e.g. of metallic material, into a surface to fix an object thereto, or through layers of relatively thin material to hold them together, e.g. by clinching	B25C5/00	B25C5/00		281
B25C5/02	8	with provision for bending the ends of the staples on to the work	B25C5/02	B25C5/02		271
B25C5/0207	9	{Particular clinching mechanisms (B25C5/0271 takes precedence)}	B25C5/02	B25C5/02		214
B25C5/0214	9	{Combined stapling and punching tools}	B25C5/02	B25C5/02		172
B25C5/0221	9	{Stapling tools of the table model type, i.e. tools supported by a table or the work during operation}	B25C5/02	B25C5/02		38
B25C5/0228	10	{power-operated}	B25C5/02	B25C5/02		172
B25C5/0235	10	{manually operated having a plunger cooperating with an anvil (B25C5/025 takes precedence)}	B25C5/02	B25C5/02		64
B25C5/0242	10	{having a pivoting upper leg and a leg provided with an anvil supported by the table or work}	B25C5/02	B25C5/02		193
B25C5/025	11	{the plunger being manually operated}	B25C5/02	B25C5/02		778
B25C5/0257	10	{without an anvil, e.g. using staples of particular shape bent during the stapling operation without the use of external clinching means}	B25C5/02	B25C5/02		104
B25C5/0264	11	{having pivoting clinching means for bending the staple ends}	B25C5/02	B25C5/02		34
B25C5/0271	12	{Clinching means therefor}	B25C5/02	B25C5/02		51
B25C5/0278	10	{having staple forming means}	B25C5/02	B25C5/02		12
B25C5/0285	9	{Hand-held stapling tools, e.g. manually operated, i.e. not resting on a working surface during operation}	B25C5/02	B25C5/02		222
B25C5/0292	10	{with the objects to be stapled together introduced perpendicularly to the longitudinal axis of the tool in an opening formed by an anvil and a plunger}	B25C5/02	B25C5/02		186
B25C5/04	9	with means for forming the staples in the tool	B25C5/04	B25C5/04		68
B25C5/045	10	{starting from performed staples}	B25C5/04	B25C5/04		15
B25C5/06	8	without provision for bending the ends of the staples on to the work	B25C5/06	B25C5/06		424
B25C5/08	9	with means for forming the staples in the tool	B25C5/08	B25C5/08		48
B25C5/085	10	{starting from performed staples}	B25C5/08	B25C5/08		84
B25C5/10	8	Driving means	B25C5/10	B25C5/10		199
B25C5/11	9	operated by manual {or foot} power	B25C5/11	B25C5/11		686
B25C5/13	9	operated by fluid pressure	B25C5/13	B25C5/13		136
B25C5/15	9	operated by electric power	B25C5/15	B25C5/15		337
B25C5/16	8	Staple-feeding devices {, e.g. with feeding means, supports for staples or accessories concerning feeding devices}	B25C5/16	B25C5/16		382
B25C5/1603	9	{for tools with provision for bending the ends of the staples or to the work}	B25C5/16	B25C5/16		104
B25C5/1606	9	{Feeding means}	B25C5/16	B25C5/16		72
B25C5/161	10	{employing a spring-loaded puller}	B25C5/16	B25C5/16		74
B25C5/1613	11	{with means for holding puller out of position during re-loading}	B25C5/16	B25C5/16		37
B25C5/1617	10	{employing a spring-loaded pusher}	B25C5/16	B25C5/16		172
B25C5/162	11	{with means for holding pusher out of position during re-loading}	B25C5/16	B25C5/16		66
B25C5/1624	10	{employing mechanical feeding means (B25C5/161, B25C5/1617 take precedence)}	B25C5/16	B25C5/16		30
B25C5/1627	11	{of incremental type}	B25C5/16	B25C5/16		156
B25C5/1631	11	{for feeding a chosen number of staples to the drive channel}	B25C5/16	B25C5/16		1
B25C5/1634	10	{employing gravity feed}	B25C5/16	B25C5/16		39
B25C5/1637	9	{Supports for the staples being fed}	B25C5/16	B25C5/16		78
B25C5/1641	10	{allowing the feeding of a variety of elements}	B25C5/16	B25C5/16		20
B25C5/1644	11	{of different shapes}	B25C5/16	B25C5/16		35
B25C5/1648	12	{by use or interchangeable supports}	B25C5/16	B25C5/16		12
B25C5/1651	12	{of T-shaped staples or nails}	B25C5/16	B25C5/16		38
B25C5/1655	13	{by use of interchangeable supports}	B25C5/16	B25C5/16		2
B25C5/1658	11	{of different sizes of staples}	B25C5/16	B25C5/16		146
B25C5/1662	12	{by use of interchangeable supports}	B25C5/16	B25C5/16		10
B25C5/1665	9	{with means for preventing jamming or aiding unjamming within the drive channel}	B25C5/16	B25C5/16		160
B25C5/1668	10	{preventing jamming by retaining the next staple}	B25C5/16	B25C5/16		20
B25C5/1672	11	{for multiple-stroke driving}	B25C5/16	B25C5/16		6
B25C5/1675	10	{unjamming by movement of the feeding device}	B25C5/16	B25C5/16		16
B25C5/1679	9	{comprising storing arrangements for a plurality of staple strips}	B25C5/16	B25C5/16		114
B25C5/1682	10	{on a rotating carousel}	B25C5/16	B25C5/16		23
B25C5/1686	9	{using pre-loaded cassettes}	B25C5/16	B25C5/16		57
B25C5/1689	9	{with means for indicating the number of staples remaining}	B25C5/16	B25C5/16		94
B25C5/1693	9	{co-ordinating with the feed of a second item}	B25C5/16	B25C5/16		129
B25C5/1696	9	{Staple support displaceable relative to the tool to allow re-loading}	B25C5/16	B25C5/16		134
B25C7/00	7	Accessories for nailing or stapling tools, e.g. supports (for tools operated by detonation of a cartridge B25C1/18)	B25C7/00	B25C7/00		1415
B25C9/00	7	Nail punches	B25C9/00	B25C9/00		76
B25C11/00	7	Nail, spike, and staple extractors (incorporated in hammers B25D1/00)	B25C11/00	B25C11/00		1344
B25C11/02	8	Pincers (joints therefor B25B7/06)	B25C11/02	B25C11/02		733
B25C13/00	7	Nail straightening devices	B25C13/00	B25C13/00		66
