H02G1/00	7	Methods or apparatus specially adapted for installing, maintaining, repairing or dismantling electric cables or lines	H02G1/00	H02G1/00		3841
H02G1/005	8	{for cutting cables or wires, or splicing}	H02G1/00	H02G1/00		1261
H02G1/02	8	for overhead lines or cables	H02G1/02	H02G1/02		13570
H02G1/04	9	for mounting or stretching	H02G1/04	H02G1/04		4163
H02G1/06	8	for laying cables, e.g. laying apparatus on vehicle	H02G1/06	H02G1/06		4972
H02G1/08	9	through tubing or conduit, e.g. rod or draw wire for pushing or pulling {(inserting electrical cables into tubes using wallbores E21B17/206; for optical cables G02B6/4401)}	H02G1/08	H02G1/08		2565
H02G1/081	10	{using pulling means at cable ends, e.g. pulling eyes or anchors}	H02G1/08	H02G1/08		1059
H02G1/083	10	{using lines, e.g. needles, rods or tapes}	H02G1/08	H02G1/08		582
H02G1/085	10	{using portable tools}	H02G1/08	H02G1/08		488
H02G1/086	10	{using fluid as pulling means, e.g. liquid, pressurised gas or suction means}	H02G1/08	H02G1/08		560
H02G1/088	10	{using pulling devices movable inside conduits}	H02G1/08	H02G1/08		721
H02G1/10	9	in or under water	H02G1/10	H02G1/10		1308
H02G1/12	8	for removing insulation or armouring from cables, e.g. from the end thereof	H02G1/12	H02G1/12		882
H02G1/1202	9	{by cutting and withdrawing insulation}	H02G1/12	H02G1/12		146
H02G1/1204	10	{Hand-held tools}	H02G1/12	H02G1/12		262
H02G1/1207	11	{the cutting element not rotating about the wire or cable (making longitudinal and transverse or helical cut H02G1/1229)}	H02G1/12	H02G1/12		74
H02G1/1209	12	{making a transverse cut}	H02G1/12	H02G1/12		109
H02G1/1212	13	{using wire or cable clamping means}	H02G1/12	H02G1/12		430
H02G1/1214	13	{not using wire or cable clamping means}	H02G1/12	H02G1/12		392
H02G1/1217	12	{making a longitudinal cut}	H02G1/12	H02G1/12		363
H02G1/1219	12	{making a transverse and longitudinal cut}	H02G1/12	H02G1/12		62
H02G1/1221	11	{the cutting element rotating about the wire or cable (making longitudinal and transverse or helical cut H02G1/1229)}	H02G1/12	H02G1/12		170
H02G1/1224	12	{making a transverse cut}	H02G1/12	H02G1/12		540
H02G1/1226	12	{making a helical cut}	H02G1/12	H02G1/12		196
H02G1/1229	11	{the cutting element making a longitudinal, and a transverse or a helical cut}	H02G1/12	H02G1/12		305
H02G1/1231	12	{using a swivelling cutting element}	H02G1/12	H02G1/12		163
H02G1/1234	12	{the tool being of the plier type}	H02G1/12	H02G1/12		86
H02G1/1236	11	{Features relating to cutting elements}	H02G1/12	H02G1/12		204
H02G1/1239	12	{the cutting element being a disc or a circular saw}	H02G1/12	H02G1/12		69
H02G1/1241	12	{the cutting element being a stack of blades}	H02G1/12	H02G1/12		220
H02G1/1243	12	{the cutting element being a wire or filament}	H02G1/12	H02G1/12		15
H02G1/1246	12	{the cutting element being of tubular construction}	H02G1/12	H02G1/12		41
H02G1/1248	10	{Machines}	H02G1/12	H02G1/12		785
H02G1/1251	11	{the cutting element not rotating about the wire or cable (making longitudinal and transverse or helical cut H02G1/1268)}	H02G1/12	H02G1/12		221
H02G1/1253	12	{making a transverse cut}	H02G1/12	H02G1/12		213
H02G1/1256	13	{using wire or cable-clamping means}	H02G1/12	H02G1/12		722
H02G1/1258	13	{not using wire or cable-clamping means}	H02G1/12	H02G1/12		95
H02G1/126	12	{making a longitudinal cut}	H02G1/12	H02G1/12		824
H02G1/1263	12	{making a transverse and longitudinal cut}	H02G1/12	H02G1/12		149
H02G1/1265	11	{the cutting element rotating about the wire or cable (making longitudinal and transverse or helical cut H02G1/1268)}	H02G1/12	H02G1/12		1175
H02G1/1268	11	{the cutting element making a longitudinal in combination with a transverse or a helical cut}	H02G1/12	H02G1/12		339
H02G1/127	11	{Features relating to cutting elements}	H02G1/12	H02G1/12		766
H02G1/1273	9	{by pushing backwards insulation}	H02G1/12	H02G1/12		125
H02G1/1275	9	{by applying heat}	H02G1/12	H02G1/12		435
H02G1/1278	10	{using heated blades}	H02G1/12	H02G1/12		67
H02G1/128	10	{using radiant energy, e.g. a laser beam}	H02G1/12	H02G1/12		215
H02G1/1282	10	{removing metallic shields}	H02G1/12	H02G1/12		36
H02G1/1285	9	{by friction, e.g. abrading, grinding, brushing}	H02G1/12	H02G1/12		255
H02G1/1287	9	{by means of a solvent}	H02G1/12	H02G1/12		73
H02G1/129	9	{by means of a cryogenic fluid}	H02G1/12	H02G1/12		15
H02G1/1292	9	{Devices for dismantling twisted filaments}	H02G1/12	H02G1/12		88
H02G1/1295	9	{Devices for splitting and dismantling flat cables}	H02G1/12	H02G1/12		164
H02G1/1297	9	{Removing armouring from cables}	H02G1/12	H02G1/12		437
H02G1/14	8	for joining or terminating cables	H02G1/14	H02G1/14		3578
H02G1/145	9	{Moulds}	H02G1/14	H02G1/14		409
H02G1/16	8	for repairing insulation or armouring of cables	H02G1/16	H02G1/16		892
H02G3/00	7	Installations of electric cables or lines or protective tubing therefor in or on buildings, equivalent structures or vehicles (installations of bus-bars H02G5/00; overhead installations H02G7/00; installations in or on the ground H02G9/00)	H02G3/00	H02G3/00		1369
H02G3/02	8	Details	H02G3/02	H02G3/02		3157
H02G3/03	9	Cooling	H02G3/03	H02G3/03		1465
H02G3/04	9	Protective tubing or conduits,&#160;e.g. cable ladders or cable troughs	H02G3/04	H02G3/04		2276
H02G3/0406	10	{Details thereof (installation or suspension of conduit channels and other supports H02G3/263)}	H02G3/04	H02G3/04		4760
H02G3/0412	11	{Heat or fire protective means (for fire in electric circuits A62C3/16)}	H02G3/04	H02G3/04		1651
H02G3/0418	11	{Covers or lids; Their fastenings}	H02G3/04	H02G3/04		2781
H02G3/0425	10	{Plinths (borders for use between floor or ceiling and wall E04F19/04)}	H02G3/04	H02G3/04		669
H02G3/0431	10	{Wall trunking}	H02G3/04	H02G3/04		949
H02G3/0437	10	{Channels}	H02G3/04	H02G3/04		2782
H02G3/0443	11	{formed by wire or analogous netting}	H02G3/04	H02G3/04		495
H02G3/045	11	{provided with perforations or slots permitting introduction or exit of wires}	H02G3/04	H02G3/04		1828
H02G3/0456	10	{Ladders or other supports}	H02G3/04	H02G3/04		3548
H02G3/0462	10	{Tubings, i.e. having a closed section}	H02G3/04	H02G3/04		1310
H02G3/0468	11	{Corrugated}	H02G3/04	H02G3/04		1255
H02G3/0475	11	{formed by a succession of articulated units}	H02G3/04	H02G3/04		666
H02G3/0481	11	{with a circular cross-section (H02G3/0468, H02G3/0475 take precedence)}	H02G3/04	H02G3/04		2713
H02G3/0487	11	{with a non-circular cross-section (H02G3/0468, H02G3/0475 take precedence)}	H02G3/04	H02G3/04		1272
H02G3/0493	10	{Service poles}	H02G3/04	H02G3/04		712
H02G3/06	9	Joints for connecting lengths of protective tubing {or channels}, to each other or to casings, e.g. to distribution boxes; Ensuring electrical continuity in the joint	H02G3/06	H02G3/06		2292
H02G3/0608	10	{Joints for connecting non cylindrical conduits, e.g. channels}	H02G3/06	H02G3/06		1638
H02G3/0616	10	{Joints for connecting tubing to casing}	H02G3/06	H02G3/06		1471
H02G3/0625	11	{with means for preventing disengagement of conductors}	H02G3/06	H02G3/06		264
H02G3/0633	12	{with means urging the conductors to follow a non-straight line}	H02G3/06	H02G3/06		177
H02G3/0641	12	{with means distorted around the conductors}	H02G3/06	H02G3/06		90
H02G3/065	12	{with means biting into the conductor-insulation, e.g. teeth-like elements or gripping fingers (H02G3/0675, H02G3/0683 take precedence)}	H02G3/06	H02G3/06		311
H02G3/0658	12	{with means constricting the conductor-insulation (H02G3/065, H02G3/0675, H02G3/0683 take precedence)}	H02G3/06	H02G3/06		336
H02G3/0666	12	{with means clamping the armour of the conductor (H02G3/0675, H02G3/0683 take precedence)}	H02G3/06	H02G3/06		404
H02G3/0675	12	{with bolts operating in a direction parallel to the conductors}	H02G3/06	H02G3/06		658
H02G3/0683	12	{with bolts operating in a direction transverse to the conductors}	H02G3/06	H02G3/06		586
H02G3/0691	11	{Fixing tubing to casing by auxiliary means co-operating with indentations of the tubing, e.g. with tubing-convolutions}	H02G3/06	H02G3/06		792
H02G3/08	9	Distribution boxes; Connection or junction boxes	H02G3/08	H02G3/08		2082
H02G3/081	10	{Bases, casings or covers}	H02G3/08	H02G3/08		3427
H02G3/083	11	{Inlets}	H02G3/08	H02G3/08		2126
H02G3/085	12	{including knock-out or tear-out sections}	H02G3/08	H02G3/08		730
H02G3/086	10	{Assembled boxes}	H02G3/08	H02G3/08		1655
H02G3/088	10	{Dustproof, splashproof, drip-proof, waterproof, or flameproof casings or inlets}	H02G3/08	H02G3/08		3452
H02G3/10	10	for surface mounting on a wall	H02G3/10	H02G3/10		1176
H02G3/105	11	{in association with a plinth, channel, raceway or similar}	H02G3/10	H02G3/10		462
H02G3/12	10	for flush mounting	H02G3/12	H02G3/12		1623
H02G3/121	11	{in plain walls}	H02G3/12	H02G3/12		2026
H02G3/123	11	{in thin walls}	H02G3/12	H02G3/12		1455
H02G3/125	12	{with supporting bar extending between two separate studs of a wall frame}	H02G3/12	H02G3/12		533
H02G3/126	12	{with supporting means for mounting on a single wall stud}	H02G3/12	H02G3/12		562
H02G3/128	11	{in plinths, channels, raceways or similar}	H02G3/12	H02G3/12		529
H02G3/14	10	Fastening of cover or lid to box	H02G3/14	H02G3/14		5012
H02G3/16	10	structurally associated with support for line-connecting terminals within the box	H02G3/16	H02G3/16		3173
H02G3/18	10	providing line outlets	H02G3/18	H02G3/18		2551
H02G3/185	11	{Floor outlets and access cups}	H02G3/18	H02G3/18		1393
H02G3/20	11	Ceiling roses {or other lighting sets}	H02G3/20	H02G3/20		1306
H02G3/22	8	Installations of cables or lines through walls, floors or ceilings, e.g. into buildings	H02G3/22	H02G3/22		5593
H02G3/24	8	{Installation of lines or cables on walls, ceilings or floors by means of insulators (insulators H01B17/00)}	H02G3/30	H02G3/24		345
H02G3/26	8	{Installations of cables, lines, or separate protective tubing therefor directly on or in walls, ceilings, or floors (by means of insulators H02G3/24; supports for pipes, cables or protective tubing F16L3/00; hose-clips F16L33/02)}	H02G3/00	H02G3/26		1297
H02G3/263	9	{Installation, e.g. suspension, of conduit channels or other supports}	H02G3/00	H02G3/26		1214
H02G3/266	9	{Mounting by adhesive material}	H02G3/00	H02G3/26		233
H02G3/28	8	{Installations of cables, lines, or separate protective tubing therefor in conduits or ducts pre-established in walls, ceilings or floors}	H02G3/38	H02G3/28		150
H02G3/281	9	{in ceilings}	H02G3/38	H02G3/28		134
H02G3/283	9	{in floors}	H02G3/38	H02G3/28		381
H02G3/285	10	{in modular floors, e.g. access floors}	H02G3/38	H02G3/28		190
H02G3/286	9	{in walls}	H02G3/38	H02G3/28		248
H02G3/288	10	{in modular walls, e.g. wall panels}	H02G3/38	H02G3/28		260
H02G3/30	8	Installations of cables or lines on walls, floors or ceilings	H02G3/30	H02G3/30		3345
H02G3/305	9	{Mounting by adhesive material}	H02G3/30	H02G3/30		262
H02G3/32	9	using mounting clamps	H02G3/32	H02G3/32		5360
H02G3/34	9	using separate protective tubing	H02G3/34	H02G3/34		808
H02G3/36	8	Installations of cables or lines in walls, floors or ceilings	H02G3/36	H02G3/36		523
H02G3/38	9	the cables or lines being installed in preestablished conduits or ducts	H02G3/38	H02G3/38		427
H02G3/381	10	{in ceilings}	H02G3/38	H02G3/38		219
H02G3/383	10	{in floors}	H02G3/38	H02G3/38		226
H02G3/385	11	{in modular floors, e.g. access floors}	H02G3/38	H02G3/38		112
H02G3/386	10	{in walls}	H02G3/38	H02G3/38		424
H02G3/388	11	{in modular walls, e.g. wall panels}	H02G3/38	H02G3/38		201
H02G3/40	10	using separate protective tubing in the conduits or ducts	H02G3/40	H02G3/40		96
H02G5/00	7	Installations of bus-bars	H02G5/00	H02G5/00		871
H02G5/002	8	{Joints between bus-bars for compensating thermal expansion}	H02G5/00	H02G5/00		365
H02G5/005	8	{Laminated bus-bars}	H02G5/00	H02G5/00		706
H02G5/007	8	{Butt joining of bus-bars by means of a common bolt, e.g. splice joint (electrically conductive connections characterised by contacting members H01R4/58)}	H02G5/00	H02G5/00		644
H02G5/02	8	Open installations	H02G5/02	H02G5/02		363
H02G5/025	9	{Supporting structures}	H02G5/02	H02G5/02		735
H02G5/04	8	Partially-enclosed installations, e.g. in ducts and adapted for sliding or rolling current collection	H02G5/04	H02G5/04		762
H02G5/06	8	Totally-enclosed installations, e.g. in metal casings	H02G5/06	H02G5/06		2437
H02G5/061	9	{Tubular casings (H02G5/063 takes precedence)}	H02G5/06	H02G5/06		506
H02G5/063	9	{filled with oil or gas}	H02G5/06	H02G5/06		411
H02G5/065	10	{Particle traps (gettering in vacuum switches H01H33/6683; in discharge or vacuum tubes H01J7/18, H01J19/70)}	H02G5/06	H02G5/06		285
H02G5/066	9	{Devices for maintaining distance between conductor and enclosure}	H02G5/06	H02G5/06		550
H02G5/068	10	{being part of the junction between two enclosures}	H02G5/06	H02G5/06		446
H02G5/08	9	Connection boxes therefor	H02G5/08	H02G5/08		894
H02G5/10	8	Cooling	H02G5/10	H02G5/10		1375
H02G7/00	7	Overhead installations of electric lines or cables (installations of bus-bars H02G5/00)	H02G7/00	H02G7/00		3065
H02G7/02	8	Devices for adjusting or maintaining mechanical tension, e.g. take-up device	H02G7/02	H02G7/02		2281
H02G7/04	8	Arrangements or devices for relieving mechanical tension	H02G7/04	H02G7/04		477
H02G7/05	8	Suspension arrangements or devices for electric cables or lines	H02G7/05	H02G7/05		3160
H02G7/053	9	{Suspension clamps and clips for electric overhead lines not suspended to a supporting wire}	H02G7/05	H02G7/05		1807
H02G7/056	10	{Dead-end clamps}	H02G7/05	H02G7/05		1066
H02G7/06	9	Suspensions for lines or cables along a separate supporting wire, e.g. S-hook	H02G7/06	H02G7/06		248
H02G7/08	10	Members clamped to the supporting wire or to the line or cable	H02G7/08	H02G7/08		385
H02G7/10	10	Flexible members or lashings wrapped around both the supporting wire and the line or cable	H02G7/10	H02G7/10		329
H02G7/12	8	Devices for maintaining distance between parallel conductors, e.g. spacer	H02G7/12	H02G7/12		909
H02G7/125	9	{Damping spacers}	H02G7/12	H02G7/12		565
H02G7/14	8	Arrangements or devices for damping mechanical oscillations of lines, e.g. for reducing production of sound {(damping spacers H02G7/125)}	H02G7/14	H02G7/14		1799
H02G7/16	8	Devices for removing snow or ice from lines or cables	H02G7/16	H02G7/16		2989
H02G7/18	8	Devices affording mechanical protection in the event of breakage of a line or cable, e.g. net for catching broken lines	H02G7/18	H02G7/18		442
H02G7/20	8	Spatial arrangements or dispositions of lines or cables on poles, posts or towers	H02G7/20	H02G7/20		3121
H02G7/205	9	{Installation of electric cables, extending along a pole}	H02G7/20	H02G7/20		398
H02G7/22	8	Arrangements of earthing wires suspended between mastheads	H02G7/22	H02G7/22		409
H02G9/00	7	Installations of electric cables or lines in or on the ground or water	H02G9/00	H02G9/00		663
H02G9/02	8	laid directly in or on the ground, river-bed or sea-bottom; Coverings therefor, e.g. tile	H02G9/02	H02G9/02		2043
H02G9/025	9	{Coverings therefor, e.g. tile}	H02G9/02	H02G9/02		1100
H02G9/04	8	in surface ducts; Ducts or covers therefor	H02G9/04	H02G9/04		924
H02G9/06	8	in underground tubes or conduits; Tubes or conduits therefor	H02G9/06	H02G9/06		3417
H02G9/065	9	{Longitudinally split tubes or conduits therefor}	H02G9/06	H02G9/06		552
H02G9/08	8	in tunnels	H02G9/08	H02G9/08		586
H02G9/10	8	in cable chambers, e.g. in manhole or in handhole	H02G9/10	H02G9/10		1930
H02G9/12	8	supported on or from floats, e.g. in water	H02G9/12	H02G9/12		306
H02G11/00	7	Arrangements of electric cables or lines between relatively-movable parts	H02G11/00	H02G11/00		2882
H02G11/003	8	{using gravity-loaded or spring-loaded loop}	H02G11/00	H02G11/00		917
H02G11/006	8	{using extensible carrier for the cable, e.g. self-coiling spring (extensible conductors or cables H01B7/06)}	H02G11/00	H02G11/00		1648
H02G11/02	8	using take-up reel or drum	H02G11/02	H02G11/02		6790
H02G13/00	7	Installations of lightning conductors; Fastening thereof to supporting structure	H02G13/00	H02G13/00		1785
H02G13/20	8	{Active discharge triggering}	H02G13/00	H02G13/20		137
H02G13/40	8	{Connection to earth}	H02G13/00	H02G13/40		1374
H02G13/60	8	{Detecting; Measuring; Sensing; Testing; Simulating}	H02G13/00	H02G13/60		301
H02G13/80	8	{Discharge by conduction or dissipation, e.g. rods, arresters, spark gaps}	H02G13/00	H02G13/80		1512
H02G15/00	7	Cable fittings	H02G15/00	H02G15/00		678
H02G15/003	8	{Filling materials, e.g. solid or fluid insulation}	H02G15/00	H02G15/00		676
H02G15/007	8	Devices for relieving mechanical stress	H02G15/007	H02G15/007		1242
H02G15/013	8	Sealing means for cable inlets (inlets for cables filled with, or surrounded by, gas or oil H02G15/32)	H02G15/013	H02G15/013		3469
H02G15/02	8	Cable terminations (for gas- or oil-filled cables H02G15/22)	H02G15/02	H02G15/02		655
H02G15/025	9	{for coaxial cables or hollow conductors (connections between HF conductors H01P1/04; plug and socket connections per seH01R24/38)}	H02G15/02	H02G15/02		102
H02G15/04	9	Cable-end sealings	H02G15/04	H02G15/04		1107
H02G15/043	10	{with end caps, e.g. sleeve closed at one end}	H02G15/04	H02G15/04		432
H02G15/046	11	{with bores or protruding portions allowing passage of cable conductors}	H02G15/04	H02G15/04		378
H02G15/06	9	Cable terminating boxes, frames or other structures	H02G15/06	H02G15/06		1144
H02G15/064	10	with devices for relieving electrical stress	H02G15/064	H02G15/064		401
H02G15/068	11	connected to the cable shield only (H02G15/072 takes precedence)	H02G15/068	H02G15/068		587
H02G15/072	11	of the condenser type	H02G15/072	H02G15/072		135
H02G15/076	10	for multi-conductor cables	H02G15/076	H02G15/076		526
H02G15/08	8	Cable junctions (for gas or oil filled cables H02G15/24)	H02G15/08	H02G15/08		1546
H02G15/085	9	{for coaxial cables or hollow conductors (plug and socket connections between HF conductors H01P1/04; plug and socket connections per seH01R24/38)}	H02G15/08	H02G15/08		391
H02G15/10	9	protected by boxes, e.g. by distribution, connection or junction boxes	H02G15/10	H02G15/10		2234
H02G15/103	10	with devices for relieving electrical stress	H02G15/103	H02G15/103		445
H02G15/105	11	connected to the cable shield only (H02G15/107 takes precedence)	H02G15/105	H02G15/105		351
H02G15/1055	12	{with cross-bonding of cable shields}	H02G15/105	H02G15/105		54
H02G15/107	11	of the condenser type	H02G15/107	H02G15/107		77
H02G15/113	10	Boxes split longitudinally in main cable direction	H02G15/113	H02G15/113		995
H02G15/115	10	Boxes split perpendicularly to main cable direction	H02G15/115	H02G15/115		311
H02G15/117	10	for multiconductor cables	H02G15/117	H02G15/117		644
H02G15/12	10	for incorporating transformers, loading coils or amplifiers	H02G15/12	H02G15/12		285
H02G15/14	11	specially adapted for submarine cables	H02G15/14	H02G15/14		578
H02G15/16	10	structurally associated with support for line-connecting terminals within the box	H02G15/16	H02G15/16		331
H02G15/18	9	protected by sleeves, e.g. for communication cable (two-part covers H02G15/10{; preforms having internal stresses B29C61/00})	H02G15/18	H02G15/18		2136
H02G15/1806	10	{Heat shrinkable sleeves (insulation of electrical connections using a heat shrinking insulating sleeve H01R4/72)}	H02G15/18	H02G15/18		633
H02G15/1813	11	{Wraparound or slotted sleeves}	H02G15/18	H02G15/18		330
H02G15/182	10	{held in expanded condition in radial direction prior to installation}	H02G15/18	H02G15/18		80
H02G15/1826	11	{on a removable hollow core, e.g. a tube}	H02G15/18	H02G15/18		146
H02G15/1833	12	{formed of helically wound strip with adjacent windings, which are removable by applying a pulling force to a strip end}	H02G15/18	H02G15/18		153
H02G15/184	10	with devices for relieving electrical stress	H02G15/184	H02G15/184		466
H02G15/188	11	connected to a cable shield only	H02G15/188	H02G15/188		180
H02G15/192	10	with support means for ends of the sleeves	H02G15/192	H02G15/192		246
H02G15/196	10	having lapped insulation	H02G15/196	H02G15/196		251
H02G15/20	8	Cable fittings for cables filled with or surrounded by gas or oil (H02G15/34 takes precedence)	H02G15/20	H02G15/20		163
H02G15/205	9	{for coaxial cables}	H02G15/20	H02G15/20		20
H02G15/22	9	Cable terminations	H02G15/22	H02G15/22		311
H02G15/23	10	Cable-end sealings	H02G15/23	H02G15/23		96
H02G15/24	9	Cable junctions	H02G15/24	H02G15/24		570
H02G15/25	10	Stop junctions	H02G15/25	H02G15/25		122
H02G15/26	9	Expansion vessels; Locking heads; Auxiliary pipe-lines	H02G15/26	H02G15/26		509
H02G15/28	9	structurally associated with devices for indicating the presence or location of non-electric faults	H02G15/28	H02G15/28		126
H02G15/30	9	with devices for relieving electrical stress	H02G15/30	H02G15/30		76
H02G15/32	9	Cable inlets	H02G15/32	H02G15/32		80
H02G15/34	8	Cable fittings for cryogenic cables {(superconductive cables per seH01B12/00)}	H02G15/34	H02G15/34		434
H02G2200/00	7	Indexing scheme relating to installation of electric cables or lines covered by H02G	CPCONLY	H02G2200/00		234
H02G2200/10	8	Prevention of theft of valuable metals	CPCONLY	H02G2200/10		207
H02G2200/20	8	Identification of installed cables	CPCONLY	H02G2200/20		203
H02G2200/30	8	Tools for installing cables comprising a spirit level	CPCONLY	H02G2200/30		308
