C04B2/00	7	Lime, magnesia or dolomite (hydraulic lime cements C04B7/34)	C04B2/00	C04B2/00		210
C04B2/005	8	{obtained from an industrial by-product}	C04B2/00	C04B2/00		135
C04B2/02	8	Lime {(obtaining Ca(OH)2 otherwise than by simple slaking of quick lime  C01F11/02)}	C04B2/02	C04B2/02		451
C04B2/04	9	Slaking {(simultaneous dehydrating of gypsum and slaking of lime C04B11/022)}	C04B2/04	C04B2/04		393
C04B2/045	10	{After-treatment of slaked lime}	C04B2/04	C04B2/04		133
C04B2/06	10	with addition of substances, e.g. hydrophobic agents {; Slaking in the presence of other compounds}	C04B2/06	C04B2/06		296
C04B2/063	11	{Slaking of impure quick lime, e.g. contained in fly ash}	C04B2/06	C04B2/06		76
C04B2/066	11	{Making use of the hydration reaction, e.g. the reaction heat for dehydrating gypsum; Chemical drying by using unslaked lime}	C04B2/06	C04B2/06		99
C04B2/08	10	Devices therefor	C04B2/08	C04B2/08		503
C04B2/10	8	Preheating, burning calcining or cooling (decarbonation during burning of cement raw materials C04B7/43; {obtaining CaO or MgO otherwise than by thermal decomposition of the corresponding carbonates C01F11/02, C01F5/02})	C04B2/10	C04B2/10		1493
C04B2/102	9	{of magnesia, e.g. dead burning}	C04B2/10	C04B2/10		480
C04B2/104	9	{Ingredients added before or during the burning process}	C04B2/10	C04B2/10		246
C04B2/106	9	{in fluidised bed furnaces}	C04B2/10	C04B2/10		99
C04B2/108	9	{Treatment or selection of the fuel therefor}	C04B2/10	C04B2/10		208
C04B2/12	9	in shaft or vertical furnaces (shaft or vertical furnaces in general F27B1/00)	C04B2/12	C04B2/12		892
C04B5/00	7	Treatment of&#160; {metallurgical} &#160;slag&#160; (manufacture of slag wool&#160;C03B; in, or for, the production of metals&#160;C21B,&#160;C22B); Artificial stone from molten&#160; {metallurgical} &#160;slag&#160; {(other cast stone&#160;C04B32/005; mechanical aspects&#160;B28B1/54)}	C04B5/00	C04B5/00		870
C04B5/06	8	Ingredients, other than water, added to the molten slag {or to the granulating medium or before remelting}; Treatment with gases or gas generating compounds, e.g. to obtain porous slag	C04B5/06	C04B5/06		638
C04B5/065	9	{Porous slag}	C04B5/06	C04B5/06		46
C04B7/00	7	Hydraulic cements (calcium sulfate cements C04B11/00)	C04B7/00	C04B7/00		4522
C04B7/003	8	{Barium or strontium cements}	C04B7/00	C04B7/00		32
C04B7/006	8	{Cement-clinker used in the unground state in mortar - or concrete compositions}	C04B7/00	C04B7/00		43
C04B7/02	8	Portland cement	C04B7/02	C04B7/02		8553
C04B7/04	9	using raw materials containing gypsum {, i.e. processes of the Mueller-Kuehne type}	C04B7/04	C04B7/04		457
C04B7/06	9	using alkaline raw materials (C04B7/60 takes precedence)	C04B7/06	C04B7/06		87
C04B7/12	8	Natural pozzuolanas; Natural pozzuolana cements; {Artificial pozzuolanas or artificial pozzuolana cements other than those obtained from waste or combustion residues, e.g. burned clay; Treating inorganic materials to improve their pozzuolanic characteristics (cements containing slag C04B7/14)}	C04B7/12	C04B7/12		420
C04B7/13	9	Mixtures thereof with inorganic cementitious materials, e.g. Portland cements	C04B7/13	C04B7/13		180
C04B7/14	8	Cements containing slag (slags from waste incineration C04B7/28)	C04B7/14	C04B7/14		619
C04B7/147	9	Metallurgical slag	C04B7/147	C04B7/147		1117
C04B7/153	10	Mixtures thereof with other inorganic cementitious materials or other activators	C04B7/153	C04B7/153		565
C04B7/1535	11	{with alkali metal containing activators, e.g. sodium hydroxide or waterglass}	C04B7/153	C04B7/153		589
C04B7/17	11	with calcium oxide containing activators {(C04B7/1535 takes precedence)}	C04B7/17	C04B7/17		239
C04B7/19	12	Portland cements	C04B7/19	C04B7/19		310
C04B7/21	11	with calcium sulfate containing activators {(C04B7/1535 takes precedence)}	C04B7/21	C04B7/21		775
C04B7/22	8	Iron ore cements {; Iron rich cements, e.g. Ferrari cements, K&#252;hl cements}	C04B7/22	C04B7/22		142
C04B7/24	8	Cements from oil shales, residues or waste other than slag	C04B7/24	C04B7/24		1751
C04B7/243	9	{Mixtures thereof with activators or composition-correcting additives, e.g. mixtures of fly ash and alkali activators}	C04B7/24	C04B7/24		1229
C04B7/246	9	{from waste building materials, e.g. waste asbestos-cement products, demolition waste}	C04B7/24	C04B7/24		351
C04B7/26	9	from raw materials containing flue dust {, i.e. fly ash (C04B7/243 takes precedence)}	C04B7/26	C04B7/26		1167
C04B7/28	9	from combustion residues, {e.g. ashes or slags from waste incineration}({C04B7/243} , C04B7/26 take precedence)	C04B7/28	C04B7/28		574
C04B7/30	9	from oil shale; from oil shale residues {; from lignite processing, e.g. using certain lignite fractions}	C04B7/30	C04B7/30		132
C04B7/32	8	Aluminous cements	C04B7/32	C04B7/32		2956
C04B7/323	9	{Calcium aluminosulfate cements, e.g. cements hydrating into ettringite}	C04B7/32	C04B7/32		1121
C04B7/326	9	{Calcium aluminohalide cements, e.g. based on 11CaO.7Al2O3.CaX2, where X is Cl or F}	C04B7/32	C04B7/32		65
C04B7/34	8	Hydraulic lime cements; Roman cements {; natural cements}	C04B7/34	C04B7/34		401
C04B7/345	8	Hydraulic cements not provided for in one of the groups C04B7/02&#160;-&#160;C04B7/34	C04B7/345	C04B7/345		235
C04B7/3453	9	{Belite cements, e.g. self-disintegrating cements based on dicalciumsilicate}	C04B7/345	C04B7/345		208
C04B7/3456	9	{Alinite cements, e.g. "Nudelman"-type cements, bromo-alinite cements, fluoro-alinite cements}	C04B7/345	C04B7/345		45
C04B7/36	8	Manufacture of hydraulic cements in general	C04B7/36	C04B7/36		1699
C04B7/361	9	{Condition or time responsive control in hydraulic cement manufacturing processes (controlling or regulating in general G05; F27B7/42 takes precedence)}	C04B7/36	C04B7/36		128
C04B7/362	10	{for raw materials handling, e.g. during the grinding or mixing step}	C04B7/36	C04B7/36		58
C04B7/364	9	{Avoiding environmental pollution during cement-manufacturing}	C04B7/36	C04B7/36		411
C04B7/365	10	{by extracting part of the material from the process flow and returning it into the process after a separate treatment, e.g. in a separate retention unit under specific conditions}	C04B7/36	C04B7/36		82
C04B7/367	10	{Avoiding or minimising carbon dioxide emissions}	C04B7/36	C04B7/36		256
C04B7/368	9	{Obtaining spherical cement particles}	C04B7/36	C04B7/36		17
C04B7/38	9	Preparing or treating the raw materials individually or as batches {, e.g. mixing with fuel; (C04B7/362 takes precedence)}	C04B7/38	C04B7/38		1281
C04B7/40	10	Dehydrating; Forming, e.g. granulating (apparatus for granulating B01J2/00)	C04B7/40	C04B7/40		438
C04B7/42	10	Active ingredients added before, or during, the burning process (after the burning process C04B22/00, C04B24/00)	C04B7/42	C04B7/42		323
C04B7/421	11	{Inorganic materials}	C04B7/42	C04B7/42		216
C04B7/422	12	{Elements}	C04B7/42	C04B7/42		41
C04B7/424	12	{Oxides, Hydroxides}	C04B7/42	C04B7/42		179
C04B7/425	12	{Acids or salts thereof}	C04B7/42	C04B7/42		230
C04B7/427	12	{Silicates}	C04B7/42	C04B7/42		88
C04B7/428	11	{Organic materials}	C04B7/42	C04B7/42		170
C04B7/43	9	Heat treatment, e.g. precalcining, burning, melting; Cooling {(aspects only relating to the installation F27B)}	C04B7/43	C04B7/43		809
C04B7/432	10	{Preheating without addition of fuel}	C04B7/43	C04B7/43		243
C04B7/434	10	{Preheating with addition of fuel, e.g. calcining}	C04B7/43	C04B7/43		445
C04B7/436	10	{Special arrangements for treating part or all of the cement kiln dust}	C04B7/43	C04B7/43		128
C04B7/438	10	{Evacuating at least part of the heat treated material before the final burning or melting step, the evacuated material being used as a cement as such}	C04B7/43	C04B7/43		14
C04B7/44	10	Burning; Melting	C04B7/44	C04B7/44		1228
C04B7/4407	11	{Treatment or selection of the fuel therefor, e.g. use of hazardous waste as secondary fuel (fuels in general C10L); Use of particular energy sources, e.g. waste hot gases from other processes}	C04B7/44	C04B7/44		336
C04B7/4415	12	{Waste hot gases}	C04B7/44	C04B7/44		60
C04B7/4423	12	{Waste or refuse used as fuel}	C04B7/44	C04B7/44		267
C04B7/443	13	{Tyres, e.g. shredded}	C04B7/44	C04B7/44		29
C04B7/4438	12	{the fuel being introduced directly into the rotary kiln}	C04B7/44	C04B7/44		86
C04B7/4446	12	{the fuel being treated in a separate gasifying or decomposing chamber, e.g. a separate combustion chamber}	C04B7/44	C04B7/44		117
C04B7/4453	11	{using plasmas or radiations}	C04B7/44	C04B7/44		57
C04B7/4461	11	{Grate sintering}	C04B7/44	C04B7/44		49
C04B7/4469	11	{in shaft or vertical kilns}	C04B7/44	C04B7/44		83
C04B7/4476	11	{Selection of the kiln atmosphere}	C04B7/44	C04B7/44		77
C04B7/4484	11	{Non-electric melting}	C04B7/44	C04B7/44		54
C04B7/4492	11	{Inhibiting the formation of or eliminating incrustations in the cement kiln (removing incrustations from rotary-drum furnaces F27B7/2075)}	C04B7/44	C04B7/44		47
C04B7/45	11	in fluidised beds {, e.g. spouted beds}	C04B7/45	C04B7/45		99
C04B7/46	11	electric	C04B7/46	C04B7/46		80
C04B7/47	10	Cooling {; Waste heat management}	C04B7/47	C04B7/47		609
C04B7/475	11	{using the waste heat, e.g. of the cooled clinker, in an other way than by simple heat exchange in the cement production line, e.g. for generating steam}	C04B7/47	C04B7/47		197
C04B7/48	9	Clinker treatment (C04B7/47 takes precedence)	C04B7/48	C04B7/48		294
C04B7/51	10	Hydrating	C04B7/51	C04B7/51		48
C04B7/52	10	Grinding {; After-treatment of ground cement}	C04B7/52	C04B7/52		866
C04B7/522	11	{After-treatment of ground cement (C04B7/368 takes precedence)}	C04B7/52	C04B7/52		52
C04B7/525	12	{Briquetting}	C04B7/52	C04B7/52		26
C04B7/527	11	{obtaining cements characterised by fineness, e.g. by multi-modal particle size distribution}	C04B7/52	C04B7/52		378
C04B7/60	9	Methods for eliminating alkali metals or compounds thereof {, e.g. from the raw materials or during the burning process; methods for eliminating other harmful components (avoiding environmental pollution C04B7/364)}	C04B7/60	C04B7/60		308
C04B9/00	7	Magnesium cements or similar cements	C04B9/00	C04B9/00		241
C04B9/02	8	Magnesium cements containing chlorides, e.g. Sorel cement	C04B9/02	C04B9/02		165
C04B9/04	8	Magnesium cements containing sulfates, nitrates, phosphates or fluorides	C04B9/04	C04B9/04		160
C04B9/06	8	Cements containing metal compounds other than magnesium compounds, e.g. compounds of zinc or lead	C04B9/06	C04B9/06		71
C04B9/11	8	Mixtures thereof with other inorganic cementitious materials	C04B9/11	C04B9/11		37
C04B9/12	9	with hydraulic cements, e.g. Portland cements	C04B9/12	C04B9/12		33
C04B9/20	8	Manufacture, e.g. preparing the batches (preheating, burning, calcining or cooling lime stone, magnesite or dolomite C04B2/10)	C04B9/20	C04B9/20		166
C04B11/00	7	Calcium sulfate cements	C04B11/00	C04B11/00		595
C04B11/002	8	{Mixtures of different CaSO4-modifications, e.g. plaster of Paris and anhydrite, used as cements}	C04B11/00	C04B11/00		143
C04B11/005	8	{Preparing or treating the raw materials}	C04B11/00	C04B11/00		201
C04B11/007	8	{After-treatment of the dehydration products, e.g. aging, stabilisation}	C04B11/00	C04B11/00		148
C04B11/02	8	{Methods and apparatus for} dehydrating gypsum {(for other purposes than cement manufacture C01F11/466)}	C04B11/02	C04B11/02		508
C04B11/022	9	{Simultaneous dehydrating of gypsum and slaking of lime}	C04B11/02	C04B11/02		12
C04B11/024	9	Ingredients added before, or during, the calcining process, e.g. calcination modifiers	C04B11/024	C04B11/024		355
C04B11/028	9	Devices therefor {characterised by the type of calcining devices used therefor or by the type of hemihydrate obtained}	C04B11/028	C04B11/028		430
C04B11/0281	10	{Kettles; Marmites; Autoclaves}	C04B11/028	C04B11/028		57
C04B11/0282	11	{Autoclaves, e.g. using chariots}	C04B11/028	C04B11/028		14
C04B11/0283	10	{Fluidised beds}	C04B11/028	C04B11/028		58
C04B11/0285	10	{Rotary kilns}	C04B11/028	C04B11/028		60
C04B11/0286	10	{Suspension heaters for flash calcining, e.g. cyclones}	C04B11/028	C04B11/028		12
C04B11/0287	10	{Multi-storey horizontal furnaces}	C04B11/028	C04B11/028		3
C04B11/0288	10	{Grates}	C04B11/028	C04B11/028		3
C04B11/032	10	for the wet process, e.g. dehydrating in solution or under saturated vapour conditions, {i.e. to obtain alpha-hemihydrate (C04B11/0281&#160;-&#160;C04B11/0288 take precedence)}	C04B11/032	C04B11/032		322
C04B11/036	10	for the dry process, e.g. dehydrating in a fluidised bed or in a rotary kiln {, i.e. to obtain beta-hemihydrate (C04B11/0281&#160;-&#160;C04B11/0288 take precedence)}	C04B11/036	C04B11/036		366
C04B11/05	8	obtaining anhydrite, {e.g. Keene&apos;s cement}(C04B11/028 takes precedence)	C04B11/05	C04B11/05		303
C04B11/06	8	starting from anhydrite	C04B11/06	C04B11/06		155
C04B11/26	8	{strating from chemical gypsum}; starting from phosphogypsum or from waste, e.g. purification products of smoke (C04B11/02 takes precedence; chemical purification of smoke, fumes or exhaust gases B01D53/00{purification of gypsum C01F11/46})	C04B11/26	C04B11/26		770
C04B11/262	9	{waste gypsum other than phosphogypsum}	C04B11/26	C04B11/26		249
C04B11/264	10	{Gypsum from the desulfurisation of flue gases}	C04B11/26	C04B11/26		361
C04B11/266	9	{Chemical gypsum}	C04B11/26	C04B11/26		86
C04B11/268	9	{pelletizing of the material before starting the manufacture}	C04B11/26	C04B11/26		33
C04B11/28	8	Mixtures thereof with other inorganic cementitious materials (C04B7/04, C04B7/153 take precedence)	C04B11/28	C04B11/28		162
C04B11/30	9	with hydraulic cements, e.g. Portland cements	C04B11/30	C04B11/30		156
C04B12/00	7	Cements not provided for in groups C04B7/00&#160;-&#160;C04B11/00	C04B12/00	C04B12/00		178
C04B12/005	8	{Geopolymer cements, e.g. reaction products of aluminosilicates with alkali metal hydroxides or silicates}	C04B12/00	C04B12/00		1202
C04B12/007	8	{Non-hydraulic cements containing low lime calcium silicate phases, e.g. wollastonite, pseudowollastonite, rankinite or cements curable in the presence of CO2}	C04B12/00	C04B12/00		18
C04B12/02	8	Phosphate cements (in, or for, the manufacture of ceramics C04B33/00, C04B35/00)	C04B12/02	C04B12/02		175
C04B12/022	9	{Al-phosphates}	C04B12/02	C04B12/02		41
C04B12/025	9	{Phosphates of ammonium or of the alkali or alkaline earth metals}	C04B12/02	C04B12/02		132
C04B12/027	9	{mixtures thereof with other inorganic cementitious materials}	C04B12/02	C04B12/02		54
C04B12/04	8	Alkali metal or ammonium silicate cements {; Alkyl silicate cements; Silica sol cements; Soluble silicate cements (alkali metal silicates per se, their preparation C01B33/32; ammonium silicates per se, their preparation C01C1/00)}	C04B12/04	C04B12/04		5740
C04B14/00	7	Use of inorganic materials as fillers, e.g. pigments, for mortars, concrete or artificial stone; Treatment of inorganic materials specially adapted to enhance their filling properties in mortars, concrete or artificial stone (expanding or defibrillating materials C04B20/00)<br><br><u>NOTE</u><br><br> Fillers with a well-defined shape other than granular are considered to be reinforcing elements and thus are classified in E04C5/00. However, if they are only characterised by their composition, classification is made in C04B only 	C04B14/00	C04B14/00		2234
C04B14/005	8	{Inorganic fillers with a shape other than granular or fibrous (carbon nanotubes C04B14/026)}	C04B14/00	C04B14/00		100
C04B14/02	8	Granular materials {, e.g. microballoons}	C04B14/02	C04B14/02		12626
C04B14/022	9	{Carbon}	C04B14/02	C04B14/02		3977
C04B14/024	10	{Graphite}	C04B14/02	C04B14/02		3048
C04B14/026	10	{of particular shape, e.g. nanotubes}	C04B14/02	C04B14/02		1192
C04B14/028	11	{Carbon aerogels}	C04B14/02	C04B14/02		85
C04B14/04	9	Silica-rich materials; Silicates	C04B14/04	C04B14/04		5700
C04B14/041	10	{Aluminium silicates other than clay}	C04B14/04	C04B14/04		1765
C04B14/042	10	{Magnesium silicates, e.g. talc, sepiolite}	C04B14/04	C04B14/04		3849
C04B14/043	10	{Alkaline-earth metal silicates, e.g. wollastonite}	C04B14/04	C04B14/04		1985
C04B14/044	10	{Polysilicates, e.g. geopolymers}	C04B14/04	C04B14/04		52
C04B14/045	10	{Alkali-metal containing silicates, e.g. petalite (waterglass C04B12/04)}	C04B14/04	C04B14/04		668
C04B14/046	10	{Zircon}	C04B14/04	C04B14/04		244
C04B14/047	10	{Zeolites}	C04B14/04	C04B14/04		2782
C04B14/048	10	{Granite}	C04B14/04	C04B14/04		1269
C04B14/06	10	Quartz; Sand	C04B14/06	C04B14/06		36006
C04B14/062	11	{Microsilica, e.g. collo&#239;dal silica (preparing microsilica slurries or suspensions C04B18/148)}	C04B14/06	C04B14/06		4018
C04B14/064	11	{Silica aerogel}	C04B14/06	C04B14/06		1638
C04B14/066	11	{Precipitated or pyrogenic silica}	C04B14/06	C04B14/06		479
C04B14/068	11	{Specific natural sands, e.g. sea -, beach -, dune - or desert sand}	C04B14/06	C04B14/06		4158
C04B14/08	10	Diatomaceous earth	C04B14/08	C04B14/08		4424
C04B14/10	10	Clay {(sepiolite C04B14/042; grog C04B18/025)}	C04B14/10	C04B14/10		7491
C04B14/102	11	{Attapulgite clay}	C04B14/10	C04B14/10		1109
C04B14/104	11	{Bentonite, e.g. montmorillonite}	C04B14/10	C04B14/10		5140
C04B14/106	11	{Kaolin}	C04B14/10	C04B14/10		5503
C04B14/108	11	{Shale, slate (colliery shale C04B18/125)}	C04B14/10	C04B14/10		656
C04B14/12	11	Expanded clay	C04B14/12	C04B14/12		988
C04B14/14	10	Minerals of vulcanic origin {(granite C04B14/048)}	C04B14/14	C04B14/14		3886
C04B14/16	11	porous, e.g. pumice	C04B14/16	C04B14/16		1274
C04B14/18	11	Perlite	C04B14/18	C04B14/18		2816
C04B14/185	12	{expanded}	C04B14/18	C04B14/18		3180
C04B14/20	10	Mica; Vermiculite {(mechanical splitting B28D)}	C04B14/20	C04B14/20		2470
C04B14/202	11	{Vermiculite}	C04B14/20	C04B14/20		1476
C04B14/204	11	{expanded}	C04B14/20	C04B14/20		1114
C04B14/206	11	{Mica or vermiculite modified by cation-exchange; chemically exfoliated vermiculate}	C04B14/20	C04B14/20		88
C04B14/208	12	{delaminated mica or vermiculite platelets}	C04B14/20	C04B14/20		63
C04B14/22	10	Glass {; Devitrified glass}	C04B14/22	C04B14/22		4460
C04B14/24	11	porous, e.g. foamed glass	C04B14/24	C04B14/24		2730
C04B14/26	9	Carbonates	C04B14/26	C04B14/26		1774
C04B14/28	10	of calcium	C04B14/28	C04B14/28		13521
C04B14/285	11	{Marble}	C04B14/28	C04B14/28		890
C04B14/30	9	Oxides other than silica {(ferrites C04B14/363)}	C04B14/30	C04B14/30		3608
C04B14/301	10	{porous or hollow}	C04B14/30	C04B14/30		204
C04B14/302	11	{Aerogels}	C04B14/30	C04B14/30		253
C04B14/303	10	{Alumina}	C04B14/30	C04B14/30		5406
C04B14/304	10	{Magnesia}	C04B14/30	C04B14/30		1828
C04B14/305	10	{Titanium oxide, e.g. titanates}	C04B14/30	C04B14/30		3554
C04B14/306	10	{Zirconium oxide (zircon C04B14/046)}	C04B14/30	C04B14/30		820
C04B14/307	10	{Chromium oxide}	C04B14/30	C04B14/30		291
C04B14/308	10	{Iron oxide}	C04B14/30	C04B14/30		2412
C04B14/309	10	{Copper oxide or solid solutions thereof}	C04B14/30	C04B14/30		127
C04B14/32	9	Carbides; Nitrides; Borides {; Silicides}	C04B14/32	C04B14/32		363
C04B14/321	10	{Borides}	C04B14/32	C04B14/32		95
C04B14/322	10	{Carbides}	C04B14/32	C04B14/32		282
C04B14/323	11	{Boron carbide}	C04B14/32	C04B14/32		153
C04B14/324	11	{Silicon carbide}	C04B14/32	C04B14/32		1545
C04B14/325	10	{Nitrides}	C04B14/32	C04B14/32		138
C04B14/326	11	{Aluminium nitride}	C04B14/32	C04B14/32		126
C04B14/327	11	{Boron nitride}	C04B14/32	C04B14/32		276
C04B14/328	11	{Silicon nitride}	C04B14/32	C04B14/32		271
C04B14/34	9	Metals {, e.g. ferro-silicon}	C04B14/34	C04B14/34		2240
C04B14/36	9	Inorganic materials not provided for in groups {C04B14/022 and}C04B14/04&#160;-&#160;C04B14/34	C04B14/36	C04B14/36		2018
C04B14/361	10	{Soil, e.g. laterite}	C04B14/36	C04B14/36		1491
C04B14/363	10	{Ferrites}	C04B14/36	C04B14/36		105
C04B14/365	10	{Gypsum (synthetic gypsum C04B18/0445, C04B18/064)}	C04B14/36	C04B14/36		1043
C04B14/366	10	{Phosphates, e.g. apatite}	C04B14/36	C04B14/36		478
C04B14/368	10	{Baryte}	C04B14/36	C04B14/36		739
C04B14/38	8	Fibrous materials; Whiskers	C04B14/38	C04B14/38		2132
C04B14/383	9	{Whiskers}	C04B14/38	C04B14/38		942
C04B14/386	9	{Carbon (carbon nanotubes C04B14/026)}	C04B14/38	C04B14/38		3377
C04B14/40	9	Asbestos	C04B14/40	C04B14/40		2471
C04B14/42	9	Glass	C04B14/42	C04B14/42		7354
C04B14/44	10	Treatment for enhancing alkali resistance {(composition of alkali resistant glass fibres C03C13/00; coating of glass fibres C03C25/10)}	C04B14/44	C04B14/44		284
C04B14/46	9	Rock wool {; Ceramic or silicate fibres (C04B14/40, C04B14/42 take precedence)}	C04B14/46	C04B14/46		3298
C04B14/4606	10	{added as organic or organo-mineral precursors}	C04B14/46	C04B14/46		2
C04B14/4612	10	{Al-borates}	C04B14/46	C04B14/46		13
C04B14/4618	10	{Oxides}	C04B14/46	C04B14/46		139
C04B14/4625	11	{Alumina}	C04B14/46	C04B14/46		378
C04B14/4631	11	{Silica}	C04B14/46	C04B14/46		289
C04B14/4637	10	{Zirconia or zircon}	C04B14/46	C04B14/46		99
C04B14/4643	10	{Silicates other than zircon}	C04B14/46	C04B14/46		1715
C04B14/465	11	{Ca-silicate, e.g. wollastonite}	C04B14/46	C04B14/46		267
C04B14/4656	11	{Al-silicates, e.g. clay}	C04B14/46	C04B14/46		1381
C04B14/4662	11	{Polysilicates, e.g. geopolymers}	C04B14/46	C04B14/46		5
C04B14/4668	11	{of vulcanic origin}	C04B14/46	C04B14/46		261
C04B14/4675	11	{from slags}	C04B14/46	C04B14/46		69
C04B14/4681	10	{Titanates}	C04B14/46	C04B14/46		76
C04B14/4687	10	{Non-oxide ceramics (carbon or graphite fibres C04B14/386)}	C04B14/46	C04B14/46		128
C04B14/4693	11	{Silicon carbide}	C04B14/46	C04B14/46		202
C04B14/48	9	Metal	C04B14/48	C04B14/48		4508
C04B16/00	7	Use of organic materials as fillers, e.g. pigments, for mortars, concrete or artificial stone; Treatment of organic materials specially adapted to enhance their filling properties in mortars, concrete or artificial stone<br><br><u>NOTE</u><br><br> Fillers with a well-defined shape other than granular are considered to be reinforcing elements and thus are classified in E04C5/00. However, if they are only characterised by their composition, classification is made in C04B only 	C04B16/00	C04B16/00		291
C04B16/02	8	Cellulosic materials (cellulosic waste materials, e.g. sawdust, rice husks, C04B18/24)	C04B16/02	C04B16/02		1688
C04B16/04	8	Macromolecular compounds (C04B16/02 takes precedence)	C04B16/04	C04B16/04		1296
C04B16/06	9	fibrous	C04B16/06	C04B16/06		2356
C04B16/0608	10	{Fibrilles, e.g. fibrillated films}	C04B16/06	C04B16/06		106
C04B16/0616	10	{from polymers obtained by reactions only involving carbon-to-carbon unsaturated bonds}	C04B16/06	C04B16/06		271
C04B16/0625	11	{Polyalkenes, e.g. polyethylene}	C04B16/06	C04B16/06		1029
C04B16/0633	12	{Polypropylene}	C04B16/06	C04B16/06		5979
C04B16/0641	11	{Polyvinylalcohols; Polyvinylacetates}	C04B16/06	C04B16/06		2060
C04B16/065	11	{Polyacrylates; Polymethacrylates}	C04B16/06	C04B16/06		174
C04B16/0658	12	{Polyacrylonitrile}	C04B16/06	C04B16/06		524
C04B16/0666	11	{Polystyrene}	C04B16/06	C04B16/06		98
C04B16/0675	10	{from polymers obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds}	C04B16/06	C04B16/06		686
C04B16/0683	11	{Polyesters, e.g. polylactides}	C04B16/06	C04B16/06		1092
C04B16/0691	11	{Polyamides; Polyaramides}	C04B16/06	C04B16/06		1089
C04B16/08	9	porous, e.g. expanded polystyrene beads {or microballoons}	C04B16/08	C04B16/08		2978
C04B16/082	10	{other than polystyrene based, e.g. polyurethane foam}	C04B16/08	C04B16/08		467
C04B16/085	10	{expanded in situ, i.e. during or after mixing the mortar, concrete or artificial stone ingredients}	C04B16/08	C04B16/08		67
C04B16/087	10	{shredded}	C04B16/08	C04B16/08		63
C04B16/10	9	Treatment for enhancing the mixability with the mortar {(coating C04B20/10)}	C04B16/10	C04B16/10		64
C04B16/12	8	characterised by the shape (fibrous macromolecular compounds C04B16/06; porous macromolecular compounds C04B16/08){, e.g. perforated strips}	C04B16/12	C04B16/12		195
C04B18/00	7	Use of agglomerated or waste materials or refuse as fillers for mortars, concrete or artificial stone (use of waste materials for the manufacture of cement C04B7/24); Treatment of agglomerated or waste materials or refuse, specially adapted to enhance their filling properties in mortars, concrete or artificial stone<br><br><u>NOTE</u><br><br> Fillers with a well defined shape other than granular are considered to be reinforcing elements and thus are classified in E04C5/00. However, if they are only characterised by their composition, classification is made in C04B only 	C04B18/00	C04B18/00		99
C04B18/02	8	Agglomerated materials {, e.g. artificial aggregates}	C04B18/02	C04B18/02		954
C04B18/021	9	{agglomerated by a mineral binder, e.g. cement}	C04B18/02	C04B18/02		1697
C04B18/022	9	{agglomerated by an organic binder}	C04B18/02	C04B18/02		603
C04B18/023	9	{Fired or melted materials}	C04B18/02	C04B18/02		2874
C04B18/025	10	{Grog}	C04B18/02	C04B18/02		488
C04B18/026	10	{Melted materials (C04B14/22 takes precedence)}	C04B18/02	C04B18/02		146
C04B18/027	9	{Lightweight materials}	C04B18/02	C04B18/02		3756
C04B18/028	9	{temporarily agglomerated, e.g. agglomerates which fall apart during mixing with the other mortar or concrete ingredients}	C04B18/02	C04B18/02		34
C04B18/04	8	Waste materials; Refuse	C04B18/04	C04B18/04		1995
C04B18/0409	9	{Waste from the purification of bauxite, e.g. red mud}	C04B18/04	C04B18/04		1375
C04B18/0418	9	{Wet materials, e.g. slurries}	C04B18/04	C04B18/04		2045
C04B18/0427	9	{Dry materials}	C04B18/04	C04B18/04		1200
C04B18/0436	9	{Dredged harbour or river sludge (other slurries or sludges C04B18/0418)}	C04B18/04	C04B18/04		458
C04B18/0445	9	{Synthetic gypsum, e.g. phosphogypsum (gypsum from smoke purification C04B18/064)}	C04B18/04	C04B18/04		554
C04B18/0454	9	{Bleaching earth}	C04B18/04	C04B18/04		25
C04B18/0463	9	{Hazardous waste}	C04B18/04	C04B18/04		276
C04B18/0472	10	{Waste material contaminated by heavy metals}	C04B18/04	C04B18/04		294
C04B18/0475	9	{Waste asbestos}	C04B18/04	C04B18/04		94
C04B18/0481	9	{Other specific industrial waste materials not provided for elsewhere in C04B18/00}	C04B18/04	C04B18/04		1735
C04B18/049	10	{Wastes from oil or other wells, e.g. drilling mud}	C04B18/04	C04B18/04		191
C04B18/06	9	Combustion residues, e.g. purification products of smoke, fumes or exhaust gases	C04B18/06	C04B18/06		1903
C04B18/061	10	{Ashes from fluidised bed furnaces}	C04B18/06	C04B18/06		304
C04B18/062	10	{Purification products of smoke, fume or exhaust-gases}	C04B18/06	C04B18/06		405
C04B18/064	11	{Gypsum}	C04B18/06	C04B18/06		520
C04B18/065	10	{Residues from coal gasification}	C04B18/06	C04B18/06		291
C04B18/067	10	{Slags}	C04B18/06	C04B18/06		391
C04B18/068	10	{from burning wood}	C04B18/06	C04B18/06		116
C04B18/08	10	Flue dust {, i.e. fly ash}	C04B18/08	C04B18/08		26815
C04B18/081	11	{from brown coal or lignite}	C04B18/08	C04B18/08		92
C04B18/082	11	{Cenospheres}	C04B18/08	C04B18/08		847
C04B18/084	11	{obtained from mixtures of pulverised coal and additives, added to influence the composition of the resulting flue dust}	C04B18/08	C04B18/08		34
C04B18/085	11	{Pelletizing}	C04B18/08	C04B18/08		172
C04B18/087	11	{from liquid fuels, e.g. oil}	C04B18/08	C04B18/08		28
C04B18/088	11	{in high volume fly ash compositions}	C04B18/08	C04B18/08		53
C04B18/10	10	Burned {or pyrolised} refuse	C04B18/10	C04B18/10		2031
C04B18/101	11	{Burned rice husks or other burned vegetable material}	C04B18/10	C04B18/10		1267
C04B18/103	11	{Burned or pyrolised sludges}	C04B18/10	C04B18/10		313
C04B18/105	11	{Gaseous combustion products or dusts collected from waste incineration, e.g. sludge resulting from the purification of gaseous combustion products of waste incineration}	C04B18/10	C04B18/10		230
C04B18/106	12	{Fly ash from waste incinerators}	C04B18/10	C04B18/10		284
C04B18/108	11	{involving a melting step}	C04B18/10	C04B18/10		102
C04B18/12	9	from quarries, mining or the like	C04B18/12	C04B18/12		8593
C04B18/125	10	{Slate residues, e.g. colliery shale or oil shale or oil shale ash}	C04B18/12	C04B18/12		340
C04B18/14	9	from metallurgical processes (treatment of molten slag C04B5/00)	C04B18/14	C04B18/14		1135
C04B18/141	10	{Slags}	C04B18/14	C04B18/14		14239
C04B18/142	11	{Steelmaking slags, converter slags}	C04B18/14	C04B18/14		4930
C04B18/143	12	{L.D. slags, i.e. Linz-Donawitz slags}	C04B18/14	C04B18/14		53
C04B18/144	11	{Slags from the production of specific metals other than iron or of specific alloys, e.g. ferrochrome slags}	C04B18/14	C04B18/14		1637
C04B18/145	11	{Phosphorus slags}	C04B18/14	C04B18/14		474
C04B18/146	10	{Silica fume}	C04B18/14	C04B18/14		10807
C04B18/147	11	{Conditioning}	C04B18/14	C04B18/14		22
C04B18/148	12	{Preparing silica fume slurries or suspensions}	C04B18/14	C04B18/14		45
C04B18/149	10	{other than silica fume or slag}	C04B18/14	C04B18/14		196
C04B18/16	9	from building or ceramic industry	C04B18/16	C04B18/16		6955
C04B18/162	10	Cement kiln dust; Lime kiln dust	C04B18/162	C04B18/162		404
C04B18/165	10	Ceramic waste	C04B18/165	C04B18/165		1194
C04B18/167	10	Recycled materials, i.e. waste materials reused in the production of the same materials	C04B18/167	C04B18/167		2597
C04B18/18	9	organic (C04B18/10 takes precedence)	C04B18/18	C04B18/18		783
C04B18/20	10	from macromolecular compounds	C04B18/20	C04B18/20		1356
C04B18/22	11	Rubber {, e.g. ground waste tires}	C04B18/22	C04B18/22		2348
C04B18/24	10	Vegetable refuse, e.g. rice husks, maize-ear refuse; Cellulosic materials, e.g. paper {, cork}	C04B18/24	C04B18/24		5365
C04B18/241	11	{Paper, e.g. waste paper; Paper pulp}	C04B18/24	C04B18/24		1548
C04B18/243	12	{Waste from paper processing or recycling paper, e.g. de-inking sludge (burned paper processing waste C04B18/10)}	C04B18/24	C04B18/24		277
C04B18/245	11	{Cork; Bark}	C04B18/24	C04B18/24		294
C04B18/246	11	{expanded}	C04B18/24	C04B18/24		13
C04B18/248	11	{from specific plants, e.g. hemp fibres}	C04B18/24	C04B18/24		2870
C04B18/26	11	Wood, e.g. sawdust, wood shavings	C04B18/26	C04B18/26		4651
C04B18/265	12	{from specific species, e.g. birch}	C04B18/26	C04B18/26		556
C04B18/28	11	Mineralising; Compositions therefor	C04B18/28	C04B18/28		396
C04B18/30	9	Mixed waste; Waste of undefined composition, (C04B18/10 takes precedence)	C04B18/30	C04B18/30		390
C04B18/305	10	{Municipal waste}	C04B18/30	C04B18/30		167
C04B20/00	7	Use of materials as fillers for mortars, concrete or artificial stone according to more than one of groups C04B14/00&#160;-&#160;C04B18/00 and characterised by shape or grain distribution; Treatment of materials according to more than one of the groups C04B14/00&#160;-&#160;C04B18/00 specially adapted to enhance their filling properties in mortars, concrete or artificial stone; Expanding or defibrillating materials<br><br><u>NOTE</u><br><br> Fillers with a well-defined shape other than granular are considered to be reinforcing elements and thus are classified in E04C5/00. However, if they are only characterised by their composition, classification is made in C04B only 	C04B20/00	C04B20/00		171
C04B20/0004	8	{Microcomposites or nanocomposites, e.g. composite particles obtained by polymerising monomers onto inorganic materials}	C04B20/00	C04B20/00		53
C04B20/0008	8	{Materials specified by a shape not covered by C04B20/0016&#160;-&#160;C04B20/0056, e.g. nanotubes}	C04B20/00	C04B20/00		381
C04B20/0012	9	{Irregular shaped fillers}	C04B20/00	C04B20/00		22
C04B20/0016	8	{Granular materials, e.g. microballoons}	C04B20/00	C04B20/00		446
C04B20/002	9	{Hollow or porous granular materials}	C04B20/00	C04B20/00		1280
C04B20/0024	10	{expanded in situ, i.e. the material is expanded or made hollow after primary shaping of the mortar, concrete or artificial stone mixture (C04B16/085 takes precedence)}	C04B20/00	C04B20/00		57
C04B20/0028	10	{crushable}	C04B20/00	C04B20/00		17
C04B20/0032	10	{characterised by the gas filling pores, e.g. inert gas or air at reduced pressure}	C04B20/00	C04B20/00		33
C04B20/0036	10	{Microsized or nanosized}	C04B20/00	C04B20/00		264
C04B20/004	10	{inorganic}	C04B20/00	C04B20/00		181
C04B20/0044	9	{obtained from irregularly shaped particles}	C04B20/00	C04B20/00		11
C04B20/0048	8	{Fibrous materials}	C04B20/00	C04B20/00		3792
C04B20/0052	9	{Mixtures of fibres of different physical characteristics, e.g. different lengths}	C04B20/00	C04B20/00		243
C04B20/0056	9	{Hollow or porous fibres}	C04B20/00	C04B20/00		144
C04B20/006	9	{Microfibres; Nanofibres}	C04B20/00	C04B20/00		202
C04B20/0064	9	{Ground fibres}	C04B20/00	C04B20/00		59
C04B20/0068	9	{Composite fibres, e.g. fibres with a core and sheath of different material}	C04B20/00	C04B20/00		255
C04B20/0072	9	{Continuous fibres}	C04B20/00	C04B20/00		23
C04B20/0076	8	{characterised by the grain distribution}	C04B20/00	C04B20/00		5510
C04B20/008	9	{Micro- or nanosized fillers, e.g. micronised fillers with particle size smaller than that of the hydraulic binder (colloidal silica C04B14/062 ; silica fume C04B18/146)}	C04B20/00	C04B20/00		3989
C04B20/0084	10	{Conditioning, e.g. preparing suspensions thereof (C04B18/148 takes precedence)}	C04B20/00	C04B20/00		21
C04B20/0088	9	{Fillers with mono- or narrow grain size distribution}	C04B20/00	C04B20/00		84
C04B20/0092	10	{Fillers with fine grain sizes only}	C04B20/00	C04B20/00		175
C04B20/0096	9	{Fillers with bimodal grain size distribution}	C04B20/00	C04B20/00		443
C04B20/02	8	Treatment	C04B20/02	C04B20/02		2755
C04B20/023	9	{Chemical treatment}<br><br><u>WARNING</u><br>Group C04B20/023 is impacted by reclassification into group C04B20/0232.<br>Groups C04B20/023 and C04B20/0232 should be considered in order to perform a complete search.	C04B20/02	C04B20/02		4927
C04B20/0232	10	{with carbon dioxide}<br><br><u>WARNING</u><br>Group C04B20/0232 is incomplete pending reclassification of documents from group C04B20/023.<br>Groups C04B20/023 and C04B20/0232 should be considered in order to perform a complete search.	C04B20/02	C04B20/02		249
C04B20/026	9	{Comminuting, e.g. by grinding or breaking; Defibrillating fibres other than asbestos}	C04B20/02	C04B20/02		3562
C04B20/04	9	Heat treatment	C04B20/04	C04B20/04		2584
C04B20/06	10	Expanding clay, perlite, vermiculite or like granular materials	C04B20/06	C04B20/06		843
C04B20/061	11	{in rotary kilns}	C04B20/06	C04B20/06		150
C04B20/063	11	{by grate sintering}	C04B20/06	C04B20/06		29
C04B20/065	11	{in fluidised beds}	C04B20/06	C04B20/06		35
C04B20/066	11	{in shaft or vertical furnaces}	C04B20/06	C04B20/06		91
C04B20/068	11	{Selection of ingredients added before or during the thermal treatment, e.g. expansion promoting agents or particle-coating materials}	C04B20/06	C04B20/06		264
C04B20/08	9	Defibrillating asbestos {(defibrillating other fibres C04B20/026)}	C04B20/08	C04B20/08		124
C04B20/10	8	Coating or impregnating {(roofing granules E04D7/005)}	C04B20/10	C04B20/10		766
C04B20/1003	9	{Non-compositional aspects of the coating or impregnation}	C04B20/10	C04B20/10		91
C04B20/1007	10	{Porous or lightweight coatings}	C04B20/10	C04B20/10		69
C04B20/1011	10	{Temporary coatings}	C04B20/10	C04B20/10		36
C04B20/1014	10	{Coating or impregnating materials characterised by the shape, e.g. fibrous materials}	C04B20/10	C04B20/10		96
C04B20/1018	9	{with organic materials (pigments or dyes C04B20/1096)}	C04B20/10	C04B20/10		713
C04B20/1022	10	{Non-macromolecular compounds}	C04B20/10	C04B20/10		769
C04B20/1025	11	{Fats; Fatty oils; Ester type waxes; Higher fatty acids; Derivatives thereof}	C04B20/10	C04B20/10		329
C04B20/1029	10	{Macromolecular compounds}	C04B20/10	C04B20/10		666
C04B20/1033	11	{obtained by reactions only involving carbon-to-carbon unsaturated bonds}	C04B20/10	C04B20/10		1063
C04B20/1037	11	{obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds}	C04B20/10	C04B20/10		1007
C04B20/104	11	{Natural resins, e.g. tall oil}	C04B20/10	C04B20/10		49
C04B20/1044	11	{Bituminous materials}	C04B20/10	C04B20/10		324
C04B20/1048	11	{Polysaccharides, e.g. cellulose, or derivatives thereof}	C04B20/10	C04B20/10		396
C04B20/1051	9	{Organo-metallic compounds; Organo-silicon compounds, e.g. bentone}	C04B20/10	C04B20/10		1169
C04B20/1055	9	{with inorganic materials}	C04B20/10	C04B20/10		1318
C04B20/1059	10	{Pigments or precursors thereof}	C04B20/10	C04B20/10		98
C04B20/1062	10	{Metals}	C04B20/10	C04B20/10		222
C04B20/1066	10	{Oxides, Hydroxides}	C04B20/10	C04B20/10		1116
C04B20/107	10	{Acids or salts thereof}	C04B20/10	C04B20/10		643
C04B20/1074	10	{Silicates, e.g. glass}	C04B20/10	C04B20/10		511
C04B20/1077	10	{Cements, e.g. waterglass}	C04B20/10	C04B20/10		676
C04B20/1081	11	{Mineral polymers, e.g. geopolymers}	C04B20/10	C04B20/10		47
C04B20/1085	11	{Waterglass}	C04B20/10	C04B20/10		189
C04B20/1088	10	{Water}	C04B20/10	C04B20/10		129
C04B20/1092	9	{with pigments or dyes (C04B20/1059 takes precedence)}	C04B20/10	C04B20/10		142
C04B20/1096	10	{organic}	C04B20/10	C04B20/10		19
C04B20/12	9	Multiple coating or impregnating	C04B20/12	C04B20/12		934
C04B20/123	10	{Multiple coatings, for one of the coatings of which at least one alternative is described}	C04B20/12	C04B20/12		77
C04B20/126	10	{Multiple coatings, comprising a coating layer of the same material as a previous coating layer}	C04B20/12	C04B20/12		38
C04B22/00	7	Use of inorganic materials as active ingredients for mortars, concrete or artificial stone, e.g. accelerators {or shrinkage compensating agents}	C04B22/00	C04B22/00		2771
C04B22/0006	8	{Waste inorganic materials}	C04B22/00	C04B22/00		787
C04B22/0013	8	{Boron compounds}	C04B22/00	C04B22/00		2953
C04B22/002	8	{Water}	C04B22/00	C04B22/00		4584
C04B22/0026	9	{Salt water, e.g. seawater}	C04B22/00	C04B22/00		434
C04B22/0033	10	{other than sea water, e.g. from mining activities}	C04B22/00	C04B22/00		29
C04B22/004	9	{containing dissolved additives or active agents, i.e. aqueous solutions used as gauging water (C04B22/0026 takes precedence)}	C04B22/00	C04B22/00		91
C04B22/0046	9	{Waste slurries or solutions used as gauging water}	C04B22/00	C04B22/00		309
C04B22/0053	9	{added in a particular physical form, e.g. atomised or in the gas phase}	C04B22/00	C04B22/00		57
C04B22/006	9	{released by a chemical reaction, e.g. polymer condensation}	C04B22/00	C04B22/00		25
C04B22/0066	8	{Compounds chosen for their high crystalwater content}	C04B22/00	C04B22/00		53
C04B22/0073	9	{added in the non-hydrated or only partially-hydrated form}	C04B22/00	C04B22/00		3
C04B22/008	8	{Cement and like inorganic materials added as expanding or shrinkage compensating ingredients in mortar or concrete compositions, the expansion being the result of a recrystallisation (mixtures of cements C04B7/00, C04B28/00)}	C04B22/00	C04B22/00		762
C04B22/0086	8	{Seeding materials}	C04B22/00	C04B22/00		79
C04B22/00863	9	{Calcium silicate hydrate}	C04B22/00	C04B22/00		83
C04B22/00867	9	{Ettringite}	C04B22/00	C04B22/00		11
C04B22/0093	8	{Aluminates}	C04B22/00	C04B22/00		1548
C04B22/02	8	Elements	C04B22/02	C04B22/02		1044
C04B22/04	9	Metals, e.g. aluminium used as blowing agent	C04B22/04	C04B22/04		3666
C04B22/06	8	Oxides, Hydroxides (C04B22/0013 takes precedence)	C04B22/06	C04B22/06		5880
C04B22/062	9	{of the alkali or alkaline-earth metals}	C04B22/06	C04B22/06		6460
C04B22/064	10	{of the alkaline-earth metals}	C04B22/06	C04B22/06		10334
C04B22/066	9	{Magnesia; Magnesium hydroxide}	C04B22/06	C04B22/06		2745
C04B22/068	9	{Peroxides, e.g. hydrogen peroxide}	C04B22/06	C04B22/06		1600
C04B22/08	8	Acids or salts thereof {(C04B22/0013 takes precedence)}	C04B22/08	C04B22/08		4462
C04B22/082	9	{Acids}	C04B22/08	C04B22/08		396
C04B22/085	9	{containing nitrogen in the anion, e.g. nitrites}	C04B22/08	C04B22/08		2751
C04B22/087	9	{containing chromium in the anion, e.g. chromates}	C04B22/08	C04B22/08		153
C04B22/10	9	containing carbon in the anion, e.g. carbonates<br><br><u>WARNING</u><br>Group C04B22/10 is impacted by reclassification into group C04B22/103.<br>Groups C04B22/10 and C04B22/103 should be considered in order to perform a complete search.	C04B22/10	C04B22/10		6154
C04B22/103	10	{Acids; Carbonic acids, e.g. from carbon dioxide}<br><br><u>WARNING</u><br>Group C04B22/103 is incomplete pending reclassification of documents from group C04B22/10.<br>Groups C04B22/103 and C04B22/10 should be considered in order to perform a complete search.	C04B22/10	C04B22/10		138
C04B22/106	10	{Bicarbonates}	C04B22/10	C04B22/10		464
C04B22/12	9	containing halogen in the anion	C04B22/12	C04B22/12		2693
C04B22/122	10	{Acids}	C04B22/12	C04B22/12		510
C04B22/124	10	{Chlorides of ammonium or of the alkali or alkaline earth metals, e.g. calcium chloride}	C04B22/12	C04B22/12		4784
C04B22/126	10	{Fluorine compounds, e.g. silico-fluorine compounds}	C04B22/12	C04B22/12		1600
C04B22/128	10	{Bromine compounds}	C04B22/12	C04B22/12		125
C04B22/14	9	containing sulfur in the anion, e.g. sulfides	C04B22/14	C04B22/14		3580
C04B22/141	10	{Acids}	C04B22/14	C04B22/14		506
C04B22/142	10	{Sulfates}	C04B22/14	C04B22/14		3376
C04B22/143	11	{Calcium-sulfate}	C04B22/14	C04B22/14		5567
C04B22/144	12	{Phosphogypsum}	C04B22/14	C04B22/14		591
C04B22/145	12	{Gypsum from the desulfuration of flue gases}	C04B22/14	C04B22/14		808
C04B22/146	12	{other waste Ca-sulfate}	C04B22/14	C04B22/14		237
C04B22/147	11	{Alkali-metal sulfates; Ammonium sulfate}	C04B22/14	C04B22/14		3657
C04B22/148	11	{Aluminium-sulfate}	C04B22/14	C04B22/14		2980
C04B22/149	11	{Iron-sulfates}	C04B22/14	C04B22/14		848
C04B22/16	9	containing phosphorus in the anion, e.g. phosphates	C04B22/16	C04B22/16		5554
C04B22/165	10	{Acids}	C04B22/16	C04B22/16		786
C04B24/00	7	Use of organic materials as active ingredients for mortars, concrete or artificial stone, e.g. plasticisers<br><br><u>NOTE</u><br><br> Groups C04B24/003&#160;-&#160;C04B24/006 take precedence over groups C04B24/008&#160;-&#160;C04B24/226	C04B24/00	C04B24/00		3809
C04B24/001	8	{Waste organic materials}	C04B24/00	C04B24/00		450
C04B24/003	8	{Phosphorus-containing compounds}	C04B24/00	C04B24/00		2020
C04B24/005	8	{Halogen-containing compounds}	C04B24/00	C04B24/00		1184
C04B24/006	8	{Boron-containing compounds}	C04B24/00	C04B24/00		152
C04B24/008	8	{Aldehydes, ketones}	C04B24/00	C04B24/00		1579
C04B24/02	8	Alcohols; Phenols; Ethers	C04B24/02	C04B24/02		4259
C04B24/023	9	{Ethers}	C04B24/02	C04B24/02		1275
C04B24/026	9	{Fatty alcohols}	C04B24/02	C04B24/02		2137
C04B24/04	8	Carboxylic acids; Salts, anhydrides or esters thereof	C04B24/04	C04B24/04		7429
C04B24/045	9	{Esters, e.g. lactones}	C04B24/04	C04B24/04		3283
C04B24/06	9	containing hydroxy groups	C04B24/06	C04B24/06		5495
C04B24/08	8	Fats; Fatty oils; Ester type waxes; Higher fatty acids, i.e. having at least seven carbon atoms in an unbroken chain bound to a carboxyl group; Oxidised oils or fats	C04B24/08	C04B24/08		2986
C04B24/085	9	{Higher fatty acids}	C04B24/08	C04B24/08		3509
C04B24/10	8	Carbohydrates or derivatives thereof	C04B24/10	C04B24/10		3419
C04B24/12	8	Nitrogen containing compounds {organic derivatives of hydrazine (hydrazine C04B22/00)}	C04B24/12	C04B24/12		2169
C04B24/121	9	{Amines, polyamines}	C04B24/12	C04B24/12		3032
C04B24/122	9	{Hydroxy amines}	C04B24/12	C04B24/12		4792
C04B24/123	9	{Amino-carboxylic acids}	C04B24/12	C04B24/12		900
C04B24/124	9	{Amides}	C04B24/12	C04B24/12		1666
C04B24/125	9	{Compounds containing one or more carbon-to-nitrogen double or triple bonds, e.g. imines}	C04B24/12	C04B24/12		665
C04B24/126	9	{Urea}	C04B24/12	C04B24/12		1013
C04B24/127	9	{Nitro-compounds}	C04B24/12	C04B24/12		64
C04B24/128	9	{Heterocyclic nitrogen compounds}	C04B24/12	C04B24/12		1108
C04B24/129	9	{Compounds containing one or more nitrogen-to-nitrogen double bonds, e.g. azo-compounds}	C04B24/12	C04B24/12		445
C04B24/14	9	Peptides; Proteins; Derivatives thereof	C04B24/14	C04B24/14		2963
C04B24/16	8	Sulfur-containing compounds	C04B24/16	C04B24/16		5906
C04B24/161	9	{Macromolecular compounds comprising sulfonate or sulfate groups}	C04B24/16	C04B24/16		364
C04B24/163	10	{obtained by reactions only involving carbon-to-carbon unsaturated bonds}	C04B24/16	C04B24/16		935
C04B24/165	11	{containing polyether side chains}	C04B24/16	C04B24/16		841
C04B24/166	10	{obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds}	C04B24/16	C04B24/16		739
C04B24/168	10	{Polysaccharide derivatives, e.g. starch sulfate}	C04B24/16	C04B24/16		152
C04B24/18	9	Lignin sulfonic acid or derivatives thereof, e.g. sulfite lye	C04B24/18	C04B24/18		4106
C04B24/20	9	Sulfonated aromatic compounds	C04B24/20	C04B24/20		2874
C04B24/22	10	Condensation {or polymerisation} products thereof<br><br><u>NOTE</u><br><br> In this group the following term is used with the meaning indicated: <br>"aldehydes" also covers other organic compounds reacting as aldehydes, e.g. glyoxylic acid 	C04B24/22	C04B24/22		925
C04B24/223	11	{Sulfonated melamine-formaldehyde condensation products}	C04B24/22	C04B24/22		621
C04B24/226	11	{Sulfonated naphtalene-formaldehyde condensation products}	C04B24/22	C04B24/22		1571
C04B24/24	8	Macromolecular compounds (C04B24/14 takes precedence; macromolecular compounds comprising sulfonate or sulfate groups C04B24/16)	C04B24/24	C04B24/24		6817
C04B24/243	9	{Phosphorus-containing polymers}	C04B24/24	C04B24/24		354
C04B24/246	10	{containing polyether side chains}	C04B24/24	C04B24/24		460
C04B24/26	9	obtained by reactions only involving carbon-to-carbon unsaturated bonds {(C04B24/243 takes precedence)}	C04B24/26	C04B24/26		6091
C04B24/2605	10	{containing polyether side chains}	C04B24/26	C04B24/26		414
C04B24/2611	10	{Polyalkenes}	C04B24/26	C04B24/26		1732
C04B24/2617	10	{Coumarone polymers}	C04B24/26	C04B24/26		23
C04B24/2623	10	{Polyvinylalcohols; Polyvinylacetates}	C04B24/26	C04B24/26		5782
C04B24/2629	11	{containing polyether side chains}	C04B24/26	C04B24/26		26
C04B24/2635	10	{Polyvinylacetals}	C04B24/26	C04B24/26		99
C04B24/2641	10	{Polyacrylates; Polymethacrylates}	C04B24/26	C04B24/26		6091
C04B24/2647	11	{containing polyether side chains}	C04B24/26	C04B24/26		1736
C04B24/2652	10	{Nitrogen containing polymers, e.g. polyacrylamides, polyacrylonitriles}	C04B24/26	C04B24/26		3887
C04B24/2658	11	{containing polyether side chains}	C04B24/26	C04B24/26		228
C04B24/2664	10	{of ethylenically unsaturated dicarboxylic acid polymers, e.g. maleic anhydride copolymers}	C04B24/26	C04B24/26		418
C04B24/267	11	{containing polyether side chains}	C04B24/26	C04B24/26		334
C04B24/2676	10	{Polystyrenes}	C04B24/26	C04B24/26		1873
C04B24/2682	10	{Halogen containing polymers, e.g. PVC}	C04B24/26	C04B24/26		1141
C04B24/2688	10	{Copolymers containing at least three different monomers}	C04B24/26	C04B24/26		1148
C04B24/2694	11	{containing polyether side chains}	C04B24/26	C04B24/26		1218
C04B24/28	9	obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds {(C04B24/243 takes precedence)}	C04B24/28	C04B24/28		1616
C04B24/281	10	{Polyepoxides}	C04B24/28	C04B24/28		3386
C04B24/282	10	{Polyurethanes; Polyisocyanates}	C04B24/28	C04B24/28		1953
C04B24/283	10	{Polyesters}	C04B24/28	C04B24/28		1158
C04B24/285	11	{Polylactides}	C04B24/28	C04B24/28		110
C04B24/286	10	{Polycarbonates}	C04B24/28	C04B24/28		169
C04B24/287	10	{Polyamides}	C04B24/28	C04B24/28		754
C04B24/288	10	{Halogen containing polymers}	C04B24/28	C04B24/28		85
C04B24/30	10	Condensation polymers of aldehydes or ketones<br><br><u>NOTE</u><br><br> In this group the following term is used with the meaning indicated: <br> "aldehydes" also covers other organic compounds reacting as aldehydes, e.g. glyoxylic acid 	C04B24/30	C04B24/30		561
C04B24/302	11	{Phenol-formaldehyde condensation polymers}	C04B24/30	C04B24/30		843
C04B24/305	11	{Melamine-formaldehyde condensation polymers}	C04B24/30	C04B24/30		280
C04B24/307	11	{Urea-formaldehyde condensation polymers}	C04B24/30	C04B24/30		394
C04B24/32	10	Polyethers, e.g. alkylphenol polyglycolether	C04B24/32	C04B24/32		6040
C04B24/34	9	Natural resins, e.g. rosin {(C04B24/243 takes precedence)}	C04B24/34	C04B24/34		2030
C04B24/36	9	Bituminous materials, e.g. tar, pitch {(C04B24/243 takes precedence)}	C04B24/36	C04B24/36		3906
C04B24/38	9	Polysaccharides or derivatives thereof {(C04B24/243 takes precedence)}	C04B24/38	C04B24/38		7367
C04B24/383	10	{Cellulose or derivatives thereof}	C04B24/38	C04B24/38		14154
C04B24/386	11	{containing polyether side chains}	C04B24/38	C04B24/38		179
C04B24/40	8	Compounds containing silicon, titanium or zirconium {or other organo-metallic compounds; Organo-clays; Organo-inorganic complexes}	C04B24/40	C04B24/40		1327
C04B24/405	9	{Organo-inorganic complexes}	C04B24/40	C04B24/40		156
C04B24/42	9	Organo-silicon compounds	C04B24/42	C04B24/42		10514
C04B24/425	10	{Organo-modified inorganic compounds, e.g. organo-clays}	C04B24/42	C04B24/42		186
C04B26/00	7	Compositions of mortars, concrete or artificial stone, containing only organic binders {, e.g. polymer or resin concrete (mechanical aspects of moulding polymer or resin concrete B29C67/242)}	C04B26/00	C04B26/00		698
C04B26/003	8	{Oil-based binders, e.g. containing linseed oil}	C04B26/00	C04B26/00		101
C04B26/006	8	{Waste materials as binder}	C04B26/00	C04B26/00		153
C04B26/02	8	Macromolecular compounds	C04B26/02	C04B26/02		2208
C04B26/023	9	{Organic ionomer cements}	C04B26/02	C04B26/02		3
C04B26/026	9	{Proteins or derivatives thereof}	C04B26/02	C04B26/02		123
C04B26/04	9	obtained by reactions only involving carbon-to-carbon unsaturated bonds	C04B26/04	C04B26/04		1546
C04B26/045	10	{Polyalkenes}	C04B26/04	C04B26/04		409
C04B26/06	10	Acrylates	C04B26/06	C04B26/06		1704
C04B26/08	10	containing halogen	C04B26/08	C04B26/08		381
C04B26/10	9	obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds	C04B26/10	C04B26/10		583
C04B26/105	10	{Furfuryl alcohol polymers, e.g. furan-polymers}	C04B26/10	C04B26/10		57
C04B26/12	10	Condensation polymers of aldehydes or ketones<br><br><u>NOTE</u><br><br> In this group the following term is used with the meaning indicated: <br> "aldehydes" also covers other organic compounds reacting as aldehydes, e.g. glyoxylic acid 	C04B26/12	C04B26/12		248
C04B26/122	11	{Phenol-formaldehyde condensation polymers}	C04B26/12	C04B26/12		660
C04B26/125	11	{Melamine-formaldehyde condensation polymers}	C04B26/12	C04B26/12		71
C04B26/127	11	{Urea formaldehyde condensation polymers}	C04B26/12	C04B26/12		117
C04B26/14	10	Polyepoxides	C04B26/14	C04B26/14		1781
C04B26/16	10	Polyurethanes	C04B26/16	C04B26/16		1183
C04B26/18	10	Polyesters; Polycarbonates	C04B26/18	C04B26/18		1341
C04B26/20	10	Polyamides	C04B26/20	C04B26/20		193
C04B26/22	9	Natural resins, e.g. rosin	C04B26/22	C04B26/22		300
C04B26/24	10	Cellulosic waste liquor, e.g. sulfite lye	C04B26/24	C04B26/24		67
C04B26/26	9	Bituminous materials, e.g. tar, pitch {(C08L95/00 takes precedence)}	C04B26/26	C04B26/26		4781
C04B26/28	9	Polysaccharides or derivatives thereof	C04B26/28	C04B26/28		816
C04B26/285	10	{Cellulose or derivatives thereof (C04B26/24 takes precedence)}	C04B26/28	C04B26/28		828
C04B26/30	8	Compounds having one or more carbon-to-metal or carbon-to-silicon linkages {; Other silicon-containing organic compounds; Boron-organic compounds}	C04B26/30	C04B26/30		50
C04B26/32	9	containing silicon	C04B26/32	C04B26/32		850
C04B28/00	7	Compositions of mortars, concrete or artificial stone, containing inorganic binders or the reaction product of an inorganic and an organic binder, e.g. polycarboxylate cements<br><br><u>NOTE</u><br><br> While using Combination Sets in this main group, the presence of an organic binder is indicated with symbols chosen from group C04B24/00, and the presence of a supplementary inorganic binder with symbols chosen from groups C04B7/00&#160;-&#160;C04B12/00	C04B28/00	C04B28/00		14431
C04B28/001	8	{containing unburned clay (polymer binder - clay mixtures used in well cementing C09K8/44)}	C04B28/00	C04B28/00		1310
C04B28/003	8	{containing hybrid binders other than those of the polycarboxylate type}	C04B28/00	C04B28/00		97
C04B28/005	8	{containing gelatineous or gel forming binders, e.g. gelatineous Al(OH)3, sol-gel binders}	C04B28/00	C04B28/00		337
C04B28/006	8	{containing mineral polymers, e.g. geopolymers of the Davidovits type}	C04B28/00	C04B28/00		2838
C04B28/008	9	{Mineral polymers other than those of the Davidovits type, e.g. from a reaction mixture containing waterglass}	C04B28/00	C04B28/00		213
C04B28/02	8	containing hydraulic cements other than calcium sulfates	C04B28/02	C04B28/02		22507
C04B28/021	9	{Ash cements, e.g. fly ash cements (fly ash as filler C04B18/08); Cements based on incineration residues, e.g. alkali-activated slags from waste incineration (alkali-activated combustion residues as such C04B7/243; mixtures of the lime-pozzuolane type C04B28/18); Kiln dust cements}	C04B28/02	C04B28/02		1253
C04B28/023	9	{Barium cements}	C04B28/02	C04B28/02		19
C04B28/025	9	{Belite cements}	C04B28/02	C04B28/02		90
C04B28/026	9	{Oil shale cements}	C04B28/02	C04B28/02		28
C04B28/028	9	{Alinite cements, i.e. "Nudelman"-type cements}	C04B28/02	C04B28/02		11
C04B28/04	9	Portland cements	C04B28/04	C04B28/04		26431
C04B28/06	9	Aluminous cements (monolithic refractories or refractory mortars C04B35/66)	C04B28/06	C04B28/06		5884
C04B28/065	10	{Calcium aluminosulfate cements, e.g. cements hydrating into ettringite}	C04B28/06	C04B28/06		1564
C04B28/08	9	Slag cements	C04B28/08	C04B28/08		2671
C04B28/082	10	{Steelmaking slags; Converter slags}	C04B28/08	C04B28/08		467
C04B28/085	10	{Slags from the production of specific alloys, e.g. ferrochrome slags}	C04B28/08	C04B28/08		66
C04B28/087	10	{Phosphorus slags}	C04B28/08	C04B28/08		43
C04B28/10	9	Lime cements or magnesium oxide cements	C04B28/10	C04B28/10		3012
C04B28/105	10	{Magnesium oxide or magnesium carbonate cements}	C04B28/10	C04B28/10		701
C04B28/12	10	Hydraulic lime	C04B28/12	C04B28/12		874
C04B28/14	8	containing calcium sulfate cements {(gypsum-paper plates E04C)}	C04B28/14	C04B28/14		7635
C04B28/141	9	{containing dihydrated gypsum before the final hardening step, e.g. forming a dihydrated gypsum product followed by a de- and rehydration step}	C04B28/14	C04B28/14		218
C04B28/142	9	{containing synthetic or waste calcium sulfate cements}	C04B28/14	C04B28/14		513
C04B28/143	10	{the synthetic calcium sulfate being phosphogypsum}	C04B28/14	C04B28/14		1278
C04B28/144	10	{the synthetic calcium sulfate being a flue gas desulfurization product}	C04B28/14	C04B28/14		1698
C04B28/145	9	{Calcium sulfate hemi-hydrate with a specific crystal form}	C04B28/14	C04B28/14		547
C04B28/146	10	{alpha-hemihydrate}	C04B28/14	C04B28/14		479
C04B28/147	10	{beta-hemihydrate}	C04B28/14	C04B28/14		364
C04B28/148	9	{containing calcium sulfate formed in situ, e.g. by the reaction of iron sulfate with lime}	C04B28/14	C04B28/14		18
C04B28/16	9	containing anhydrite {, e.g. Keene&apos;s cement}	C04B28/16	C04B28/16		1196
C04B28/165	10	{containing synthetic anhydrite}	C04B28/16	C04B28/16		94
C04B28/18	8	containing mixtures of the silica-lime type	C04B28/18	C04B28/18		2714
C04B28/182	9	{based on calcium silicate forming mixtures not containing lime or lime producing ingredients, e.g. waterglass based mixtures heated with a calcium salt}	C04B28/18	C04B28/18		45
C04B28/184	9	{based on an oxide other than lime}	C04B28/18	C04B28/18		81
C04B28/186	9	{containing formed Ca-silicates before the final hardening step}	C04B28/18	C04B28/18		188
C04B28/188	10	{the Ca-silicates being present in the starting mixture}	C04B28/18	C04B28/18		308
C04B28/24	8	containing alkyl, ammonium or metal silicates; containing silica sols {(reaction mixtures resulting in mineral polymers C04B28/006; polymeric reaction products of alkali metal silicates with isocyanates C08G18/3895)}	C04B28/24	C04B28/24		1561
C04B28/26	9	Silicates of the alkali metals	C04B28/26	C04B28/26		7297
C04B28/28	8	containing organic polyacids, e.g. polycarboxylate cements {, i.e. ionomeric systems}	C04B28/28	C04B28/28		153
C04B28/30	8	containing magnesium cements {or similar cements}(magnesium oxide cements C04B28/10)	C04B28/30	C04B28/30		1324
C04B28/32	9	Magnesium oxychloride cements, e.g. Sorel cement	C04B28/32	C04B28/32		2234
C04B28/34	8	containing cold phosphate binders<br><br><u>NOTE</u><br><br> While using Combination Sets in this main group, the presence of a reactive or reacted oxide is indicated with symbols chosen from C04B14/06 and C04B14/30 (and subgroups), except for boron oxide ( C04B22/0013 ) and oxides of the alkali or alkaline-earth metals, with the exception of magnesium ( C04B22/062 and C04B22/064 ), e.g. a composition containing a mixture of phosphoric acid, AlCr phosphate and magnesium oxide will be classified in C04B28/346 and will be indexed with codes C04B14/303, C04B14/304 and C04B14/307. "Phosphates" includes monobasic and dibasic phosphates 	C04B28/34	C04B28/34		1484
C04B28/342	9	{the phosphate binder being present in the starting composition as a mixture of free acid and one or more reactive oxides}	C04B28/34	C04B28/34		373
C04B28/344	9	{the phosphate binder being present in the starting composition solely as one or more phosphates}	C04B28/34	C04B28/34		869
C04B28/346	9	{the phosphate binder being present in the starting composition as a mixture of free acid and one or more phosphates}	C04B28/34	C04B28/34		130
C04B28/348	10	{the starting mixture also containing one or more reactive oxides}	C04B28/34	C04B28/34		55
C04B28/36	8	containing sulfur, sulfides or selenium	C04B28/36	C04B28/36		552
C04B28/365	9	{containing sulfides or selenium}	C04B28/36	C04B28/36		31
C04B30/00	7	Compositions for artificial stone, not containing binders	C04B30/00	C04B30/00		1343
C04B30/02	8	containing fibrous materials	C04B30/02	C04B30/02		2695
C04B32/00	7	Artificial stone not provided for in other groups of this subclass	C04B32/00	C04B32/00		230
C04B32/005	8	{Artificial stone obtained by melting at least part of the composition, e.g. metal (C04B28/36 and C03C take precedence; cast stone from molten slag C04B5/00; artificial stone obtained by melting the polymeric ingredient of the composition C04B26/00)}	C04B32/00	C04B32/00		378
C04B32/02	8	with reinforcements {(contains no documents; reinforcing elements E04C5/00)}<br><br><u>NOTE</u><br><br>This group is only used for indexing purposes	C04B32/02	C04B32/02		1479
C04B33/00	7	Clay-wares (monolithic refractories or refractory mortars C04B35/66; porous products C04B38/00)<br><br><u>NOTE</u><br><br>In groups C04B33/00 - C04B33/36, the indexing codes of groups C04B2235/00 - C04B2235/9646 are used (with the exception of C04B2235/349, C04B2235/6027, C04B2235/604 and C04B2235/9661) to identify aspects relating to ceramic starting mixtures and sintered ceramic products.	C04B33/00	C04B33/00		3003
C04B33/02	8	Preparing or treating the raw materials individually or as batches	C04B33/02	C04B33/02		760
C04B33/025	9	{Mixtures of materials with different sizes}	C04B33/02	C04B33/02		244
C04B33/04	9	Clay; Kaolin	C04B33/04	C04B33/04		4444
C04B33/06	10	Rendering lime harmless	C04B33/06	C04B33/06		331
C04B33/08	11	Preventing efflorescence	C04B33/08	C04B33/08		23
C04B33/10	9	Eliminating iron or lime	C04B33/10	C04B33/10		276
C04B33/13	9	Compounding ingredients (C04B33/36, C04B35/71 take precedence {; pigments for ceramics C09C1/0009})	C04B33/13	C04B33/13		5366
C04B33/1305	10	{Organic additives}	C04B33/13	C04B33/13		2306
C04B33/131	10	{Inorganic additives}	C04B33/13	C04B33/13		3731
C04B33/1315	10	{Non-ceramic binders}	C04B33/13	C04B33/13		1125
C04B33/132	10	Waste materials; Refuse {; Residues}(C04B33/16 takes precedence)	C04B33/132	C04B33/132		2795
C04B33/1321	11	{Waste slurries, e.g. harbour sludge, industrial muds}	C04B33/132	C04B33/132		1464
C04B33/1322	12	{Red mud}	C04B33/132	C04B33/132		377
C04B33/1324	11	{Recycled material, e.g. tile dust, stone waste, spent refractory material}	C04B33/132	C04B33/132		2038
C04B33/1325	11	{Hazardous waste other than combustion residues (dredging sludge C04B33/1321)}	C04B33/132	C04B33/132		68
C04B33/1327	12	{containing heavy metals}	C04B33/132	C04B33/132		73
C04B33/1328	11	{without additional clay}	C04B33/132	C04B33/132		1000
C04B33/135	11	Combustion residues, e.g. fly ash, incineration waste	C04B33/135	C04B33/135		296
C04B33/1352	12	{Fuel ashes, e.g. fly ash}	C04B33/135	C04B33/135		1474
C04B33/1355	12	{Incineration residues}	C04B33/135	C04B33/135		356
C04B33/1357	13	{Sewage sludge ash or slag}	C04B33/135	C04B33/135		61
C04B33/138	11	from metallurgical processes, e.g. slag, furnace dust, galvanic waste	C04B33/138	C04B33/138		1132
C04B33/14	10	Colouring matters	C04B33/14	C04B33/14		414
C04B33/16	10	Lean materials, e.g. grog, quartz	C04B33/16	C04B33/16		946
C04B33/18	10	for liquefying the batches	C04B33/18	C04B33/18		77
C04B33/20	9	for dry-pressing (C04B33/13 takes precedence)	C04B33/20	C04B33/20		126
C04B33/22	8	Grog products	C04B33/22	C04B33/22		334
C04B33/24	8	Manufacture of porcelain or white ware	C04B33/24	C04B33/24		2637
C04B33/26	9	of porcelain for electrical insulation	C04B33/26	C04B33/26		171
C04B33/28	8	Slip casting (mechanical features B28B1/26)	C04B33/28	C04B33/28		658
C04B33/30	8	Drying methods	C04B33/30	C04B33/30		1349
C04B33/32	8	Burning methods	C04B33/32	C04B33/32		2936
C04B33/323	9	{involving melting, fusion or softening}	C04B33/32	C04B33/32		177
C04B33/326	9	{under pressure}	C04B33/32	C04B33/32		153
C04B33/34	9	combined with glazing	C04B33/34	C04B33/34		1724
C04B33/36	8	Reinforced clay-wares	C04B33/36	C04B33/36		972
C04B35/00	7	Shaped ceramic products characterised by their composition {(porous ceramic products C04B38/00; ceramic articles characterised by particular shape, see the relevant classes, e.g. linings for casting ladles, tundishes, cups or the like B22D41/02; ceramic substrates for microelectronic semi-conductors H10W70/692)}; Ceramics compositions ({shaping of ceramics B28B;} containing free metal bonded to carbides, diamond, oxides, borides, nitrides, silicides, e.g. cermets, or other metal compounds, e.g. oxynitrides or sulfides other than as macroscopic reinforcing agents C22C); Processing powders of inorganic compounds preparatory to the manufacturing of ceramic products {(infiltration of sintered ceramic preforms with molten metal C04B41/51; chemical preparation of powders of inorganic compounds C01)}<br><br><u>NOTE</u><br><br>In this group, in the absence of an indication to the contrary, compositions are classified according to the constituent present in the highest proportion by weight.<br>In this group, magnesium is considered as an alkaline earth metal.<br>In this group, a composite is considered as a sintered material containing more than one phase, where the secondary phases are not resulting from sintering aids<br>In this group, fine ceramics are considered as products having a polycrystalline, fine-grained microstructure, e.g. of dimensions below 100 micrometers.<br>The production of ceramic powder is classified in this group in so far as it relates to the preparation of powder with specific characteristics.<br> In groups C04B35/00&#160;-&#160;C04B35/83, from 01-01-2005 onwards, the indexing codes of groups C04B2235/00&#160;-&#160;C04B2235/9692 are used to identify aspects relating to ceramic starting mixtures and sintered ceramic products 	C04B35/00	C04B35/00		5458
C04B35/01	8	based on oxide ceramics	C04B35/01	C04B35/01		3482
C04B35/013	9	{containing carbon (C04B35/103 takes precedence)}	C04B35/01	C04B35/01		610
C04B35/016	9	{based on manganites}	C04B35/01	C04B35/01		331
C04B35/03	9	based on magnesium oxide, calcium oxide or oxide mixtures derived from dolomite	C04B35/03	C04B35/03		766
C04B35/04	10	based on magnesium oxide	C04B35/04	C04B35/04		1124
C04B35/043	11	Refractories from grain sized mixtures	C04B35/043	C04B35/043		1267
C04B35/0435	12	{containing refractory metal compounds other than chromium oxide or chrome ore}	C04B35/043	C04B35/043		233
C04B35/047	12	containing chromium oxide or chrome ore	C04B35/047	C04B35/047		249
C04B35/0473	13	{obtained from fused grains}	C04B35/047	C04B35/047		59
C04B35/0476	13	{obtained from prereacted sintered grains ("simultaneous sinter")}	C04B35/047	C04B35/047		62
C04B35/05	11	Refractories by fusion casting	C04B35/05	C04B35/05		47
C04B35/051	12	{containing chromium oxide or chrome ore}	C04B35/05	C04B35/05		15
C04B35/053	11	Fine ceramics	C04B35/053	C04B35/053		371
C04B35/057	10	based on calcium oxide	C04B35/057	C04B35/057		482
C04B35/06	10	based on oxide mixtures derived from dolomite	C04B35/06	C04B35/06		238
C04B35/08	9	based on beryllium oxide	C04B35/08	C04B35/08		203
C04B35/10	9	based on aluminium oxide	C04B35/10	C04B35/10		8187
C04B35/101	10	Refractories from grain sized mixtures	C04B35/101	C04B35/101		1235
C04B35/1015	11	{containing refractory metal compounds other than those covered by C04B35/103&#160;-&#160;C04B35/106}	C04B35/101	C04B35/101		176
C04B35/103	11	containing non-oxide refractory materials, e.g. carbon (C04B35/106 takes precedence)	C04B35/103	C04B35/103		747
C04B35/105	11	containing chromium oxide or chrome ore	C04B35/105	C04B35/105		312
C04B35/106	11	containing zirconium oxide or zircon (ZrSiO4)	C04B35/106	C04B35/106		487
C04B35/107	10	Refractories by fusion casting	C04B35/107	C04B35/107		194
C04B35/109	11	containing zirconium oxide or zircon (ZrSiO4)	C04B35/109	C04B35/109		111
C04B35/111	10	Fine ceramics	C04B35/111	C04B35/111		2114
C04B35/1115	11	{Minute sintered entities, e.g. sintered abrasive grains or shaped particles such as platelets (abrasives C09K3/14)}	C04B35/111	C04B35/111		341
C04B35/113	11	based on beta-aluminium oxide	C04B35/113	C04B35/113		237
C04B35/115	11	Translucent or transparent products	C04B35/115	C04B35/115		263
C04B35/117	11	Composites	C04B35/117	C04B35/117		1714
C04B35/119	12	with zirconium oxide	C04B35/119	C04B35/119		766
C04B35/12	9	based on chromium oxide (C04B35/047 and C04B35/105 take precedence)	C04B35/12	C04B35/12		837
C04B35/14	9	based on silica	C04B35/14	C04B35/14		5630
C04B35/16	9	based on silicates other than clay {(zircon C04B35/48)}	C04B35/16	C04B35/16		2053
C04B35/18	10	rich in aluminium oxide	C04B35/18	C04B35/18		2504
C04B35/185	11	Mullite {3Al2O3-2SiO2}	C04B35/185	C04B35/185		2064
C04B35/19	11	Alkali metal aluminosilicates, e.g. spodumene	C04B35/19	C04B35/19		759
C04B35/195	11	Alkaline earth aluminosilicates, e.g. cordierite {or anorthite}	C04B35/195	C04B35/195		2371
C04B35/20	10	rich in magnesium oxide {, e.g. forsterite (C04B35/195 takes precedence)}	C04B35/20	C04B35/20		682
C04B35/22	10	rich in calcium oxide {, e.g. wollastonite (C04B35/195 takes precedence)}	C04B35/22	C04B35/22		458
C04B35/26	9	based on ferrites	C04B35/26	C04B35/26		1261
C04B35/2608	10	{Compositions containing one or more ferrites of the group comprising manganese, zinc, nickel, copper or cobalt and one or more ferrites of the group comprising rare earth metals, alkali metals, alkaline earth metals or lead}	C04B35/26	C04B35/26		251
C04B35/2616	11	{containing lithium}	C04B35/26	C04B35/26		183
C04B35/2625	11	{containing magnesium}	C04B35/26	C04B35/26		329
C04B35/2633	11	{containing barium, strontium or calcium}	C04B35/26	C04B35/26		1080
C04B35/2641	10	{Compositions containing one or more ferrites of the group comprising rare earth metals and one or more ferrites of the group comprising alkali metals, alkaline earth metals or lead}	C04B35/26	C04B35/26		511
C04B35/265	10	{Compositions containing one or more ferrites of the group comprising manganese or zinc and one or more ferrites of the group comprising nickel, copper or cobalt}	C04B35/26	C04B35/26		1086
C04B35/2658	10	{Other ferrites containing manganese or zinc, e.g. Mn-Zn ferrites}	C04B35/26	C04B35/26		749
C04B35/2666	10	{Other ferrites containing nickel, copper or cobalt}	C04B35/26	C04B35/26		330
C04B35/2675	10	{Other ferrites containing rare earth metals, e.g. rare earth ferrite garnets}	C04B35/26	C04B35/26		302
C04B35/2683	10	{Other ferrites containing alkaline earth metals or lead}	C04B35/26	C04B35/26		654
C04B35/2691	10	{Other ferrites containing alkaline metals}	C04B35/26	C04B35/26		81
C04B35/42	9	based on chromites (C04B35/047 and C04B35/105 take precedence)	C04B35/42	C04B35/42		755
C04B35/44	9	based on aluminates	C04B35/44	C04B35/44		2114
C04B35/443	10	Magnesium aluminate spinel	C04B35/443	C04B35/443		943
C04B35/447	9	based on phosphates {, e.g. hydroxyapatite}	C04B35/447	C04B35/447		1419
C04B35/45	9	based on copper oxide or solid solutions thereof with other oxides<br><br><u>NOTE</u><br><br> In groups C04B35/4504&#160;-&#160;C04B35/4525 an invention is classified in the last appropriate place 	C04B35/45	C04B35/45		432
C04B35/4504	10	{containing rare earth oxides}	C04B35/45	C04B35/45		397
C04B35/4508	11	{Type 1-2-3}	C04B35/45	C04B35/45		358
C04B35/4512	10	{containing thallium oxide}	C04B35/45	C04B35/45		151
C04B35/4517	11	{also containing lead oxide}	C04B35/45	C04B35/45		19
C04B35/4521	10	{containing bismuth oxide}	C04B35/45	C04B35/45		255
C04B35/4525	11	{also containing lead oxide}	C04B35/45	C04B35/45		129
C04B35/453	9	based on zinc, tin, or bismuth oxides or solid solutions thereof with other oxides, e.g. zincates, stannates or bismuthates	C04B35/453	C04B35/453		1622
C04B35/457	10	based on tin oxides or stannates	C04B35/457	C04B35/457		642
C04B35/46	9	based on titanium oxides or titanates (containing also zirconium or hafnium oxides, zirconates or hafnates C04B35/49)	C04B35/46	C04B35/46		2177
C04B35/462	10	based on titanates	C04B35/462	C04B35/462		982
C04B35/465	11	based on alkaline earth metal titanates	C04B35/465	C04B35/465		958
C04B35/468	12	based on barium titanates	C04B35/468	C04B35/468		1280
C04B35/4682	13	{based on BaTiO3 perovskite phase}	C04B35/468	C04B35/468		2112
C04B35/4684	14	{containing lead compounds (C04B35/472 takes precedence)}	C04B35/468	C04B35/468		150
C04B35/4686	13	{based on phases other than BaTiO3 perovskite phase}	C04B35/468	C04B35/468		114
C04B35/4688	14	{containing lead compounds (C04B35/472 takes precedence)}	C04B35/468	C04B35/468		16
C04B35/47	12	based on strontium titanates	C04B35/47	C04B35/47		636
C04B35/472	11	based on lead titanates	C04B35/472	C04B35/472		321
C04B35/475	11	based on bismuth titanates	C04B35/475	C04B35/475		730
C04B35/478	11	based on aluminium titanates	C04B35/478	C04B35/478		675
C04B35/48	9	based on zirconium or hafnium oxides, zirconates, {zircon} or hafnates	C04B35/48	C04B35/48		5022
C04B35/481	10	{containing silicon, e.g. zircon}	C04B35/48	C04B35/48		670
C04B35/482	10	Refractories from grain sized mixtures	C04B35/482	C04B35/482		294
C04B35/484	10	Refractories by fusion casting	C04B35/484	C04B35/484		234
C04B35/486	10	Fine ceramics	C04B35/486	C04B35/486		2216
C04B35/488	11	Composites	C04B35/488	C04B35/488		1040
C04B35/4885	12	{with aluminium oxide}	C04B35/488	C04B35/488		550
C04B35/49	10	containing also titanium oxides or titanates	C04B35/49	C04B35/49		988
C04B35/491	11	based on lead zirconates and lead titanates {, e.g. PZT}	C04B35/491	C04B35/491		789
C04B35/493	12	containing also other lead compounds	C04B35/493	C04B35/493		532
C04B35/495	9	based on vanadium, niobium, tantalum, molybdenum or tungsten oxides or solid solutions thereof with other oxides, e.g. vanadates, niobates, tantalates, molybdates or tungstates	C04B35/495	C04B35/495		2584
C04B35/497	10	based on solid solutions with lead oxides	C04B35/497	C04B35/497		177
C04B35/499	11	containing also titanates	C04B35/499	C04B35/499		319
C04B35/50	8	based on rare-earth compounds {(non-oxide rare earth compounds C04B35/5156)}	C04B35/50	C04B35/50		2845
C04B35/505	9	based on yttrium oxide	C04B35/505	C04B35/505		1097
C04B35/51	8	based on compounds of actinides ({non-oxide actinide compounds C04B35/5158;} nuclear fuel materials G21C3/62)	C04B35/51	C04B35/51		562
C04B35/515	8	based on non-oxide ceramics	C04B35/515	C04B35/515		427
C04B35/5152	9	{based on halogenides other than fluorides}	C04B35/515	C04B35/515		94
C04B35/5154	9	{based on phosphides}	C04B35/515	C04B35/515		36
C04B35/5156	9	{based on rare earth compounds}	C04B35/515	C04B35/515		93
C04B35/5158	9	{based on actinide compounds}	C04B35/515	C04B35/515		41
C04B35/52	9	based on carbon, e.g. graphite	C04B35/52	C04B35/52		3686
C04B35/521	10	{obtained by impregnation of carbon products with a carbonisable material}	C04B35/52	C04B35/52		371
C04B35/522	10	{Graphite (C04B35/536 takes precedence)}	C04B35/52	C04B35/52		2650
C04B35/524	10	obtained from polymer precursors, e.g. glass-like carbon material	C04B35/524	C04B35/524		966
C04B35/528	10	obtained from carbonaceous particles with or without other non-organic components	C04B35/528	C04B35/528		605
C04B35/532	11	containing a carbonisable binder	C04B35/532	C04B35/532		1889
C04B35/536	10	based on expanded graphite {or complexed graphite}	C04B35/536	C04B35/536		324
C04B35/547	9	based on sulfides or selenides {or tellurides}	C04B35/547	C04B35/547		612
C04B35/553	9	based on fluorides	C04B35/553	C04B35/553		295
C04B35/56	9	based on carbides {or oxycarbides (containing free metal binder C22C29/00)}	C04B35/56	C04B35/56		1019
C04B35/5603	10	{with a well-defined oxygen content, e.g. oxycarbides}	C04B35/56	C04B35/56		284
C04B35/5607	10	{based on refractory metal carbides}	C04B35/56	C04B35/56		709
C04B35/5611	11	{based on titanium carbides}	C04B35/56	C04B35/56		737
C04B35/5615	12	{based on titanium silicon carbides}	C04B35/56	C04B35/56		124
C04B35/5618	12	{based on titanium aluminium carbides}	C04B35/56	C04B35/56		143
C04B35/5622	11	{based on zirconium or hafnium carbides}	C04B35/56	C04B35/56		659
C04B35/5626	11	{based on tungsten carbides}	C04B35/56	C04B35/56		620
C04B35/563	10	based on boron carbide	C04B35/563	C04B35/563		1191
C04B35/565	10	based on silicon carbide	C04B35/565	C04B35/565		7785
C04B35/571	11	obtained from {Si-containing} polymer precursors {or organosilicon monomers}	C04B35/571	C04B35/571		1524
C04B35/573	11	obtained by reaction sintering {or recrystallisation}	C04B35/573	C04B35/573		2231
C04B35/575	11	obtained by pressure sintering	C04B35/575	C04B35/575		495
C04B35/5755	12	{obtained by gas pressure sintering}	C04B35/575	C04B35/575		67
C04B35/58	9	based on borides, nitrides, {i.e. nitrides, oxynitrides, carbonitrides or oxycarbonitrides} or silicides {(containing free binder metal C22C29/00)}	C04B35/58	C04B35/58		1182
C04B35/58007	10	{based on refractory metal nitrides}	C04B35/58	C04B35/58		261
C04B35/58014	11	{based on titanium nitrides, e.g. TiAlON}	C04B35/58	C04B35/58		445
C04B35/58021	12	{based on titanium carbonitrides}	C04B35/58	C04B35/58		159
C04B35/58028	11	{based on zirconium or hafnium nitrides}	C04B35/58	C04B35/58		152
C04B35/58035	12	{based on zirconium or hafnium carbonitrides}	C04B35/58	C04B35/58		44
C04B35/58042	10	{based on iron group metals nitrides}	C04B35/58	C04B35/58		45
C04B35/5805	10	{based on borides}	C04B35/58	C04B35/58		335
C04B35/58057	11	{based on magnesium boride, e.g. MgB2}	C04B35/58	C04B35/58		63
C04B35/58064	11	{based on refractory borides}	C04B35/58	C04B35/58		347
C04B35/58071	12	{based on titanium borides}	C04B35/58	C04B35/58		641
C04B35/58078	12	{based on zirconium or hafnium borides}	C04B35/58	C04B35/58		661
C04B35/58085	10	{based on silicides}	C04B35/58	C04B35/58		206
C04B35/58092	11	{based on refractory metal silicides}	C04B35/58	C04B35/58		503
C04B35/581	10	based on aluminium nitride	C04B35/581	C04B35/581		2459
C04B35/583	10	based on boron nitride	C04B35/583	C04B35/583		1289
C04B35/5831	11	based on cubic boron nitrides {or Wurtzitic boron nitrides, including crystal structure transformation of powder}	C04B35/5831	C04B35/5831		846
C04B35/584	10	based on silicon nitride	C04B35/584	C04B35/584		3575
C04B35/587	11	Fine ceramics	C04B35/587	C04B35/587		509
C04B35/589	11	obtained from {Si-containing} polymer precursors {or organosilicon monomers}	C04B35/589	C04B35/589		534
C04B35/591	11	obtained by reaction sintering	C04B35/591	C04B35/591		790
C04B35/593	11	obtained by pressure sintering	C04B35/593	C04B35/593		785
C04B35/5935	12	{obtained by gas pressure sintering}	C04B35/593	C04B35/593		392
C04B35/597	10	based on silicon oxynitride, {e.g. SIALONS}	C04B35/597	C04B35/597		888
C04B35/622	8	Forming processes; Processing powders of inorganic compounds preparatory to the manufacturing of ceramic products<br><br><u>NOTE</u><br><br> In groups C04B35/622 and subgroups indexing codes are given for aspects relating to the preparation, properties or mechanical treatment or to heat treatments of green bodies. The codes are chosen from C04B2235/60&#160;-&#160;C04B2235/668	C04B35/622	C04B35/622		23475
C04B35/62204	9	{using waste materials or refuse (clay-wares containing waste materials C04B33/132)}	C04B35/622	C04B35/622		2697
C04B35/62209	10	{using woody material, remaining in the ceramic products (to obtain porous material by burning out C04B38/06)}	C04B35/622	C04B35/622		111
C04B35/62213	10	{using rice material, e.g. bran or hulls or husks}	C04B35/622	C04B35/622		69
C04B35/62218	9	{obtaining ceramic films, e.g. by using temporary supports}	C04B35/622	C04B35/622		1150
C04B35/62222	9	{obtaining ceramic coatings (coating of mortars, concrete, artificial or natural stone or ceramics C04B41/45; laminated ceramic products B32B18/00; coating of glass C03C17/00, applying ceramic coatings on silicon for semi-conductor purposes H10W; coating metallic materials C23)}	C04B35/622	C04B35/622		1557
C04B35/62227	9	{obtaining fibres}	C04B35/622	C04B35/622		266
C04B35/62231	10	{based on oxide ceramics}	C04B35/622	C04B35/622		706
C04B35/62236	11	{Fibres based on aluminium oxide}	C04B35/622	C04B35/622		410
C04B35/6224	11	{Fibres based on silica}	C04B35/622	C04B35/622		223
C04B35/62245	12	{rich in aluminium oxide}	C04B35/622	C04B35/622		219
C04B35/6225	11	{Fibres based on zirconium oxide, e.g. zirconates such as PZT}	C04B35/622	C04B35/622		191
C04B35/62254	11	{Fibres based on copper oxide}	C04B35/622	C04B35/622		40
C04B35/62259	11	{Fibres based on titanium oxide}	C04B35/622	C04B35/622		149
C04B35/62263	11	{Fibres based on magnesium oxide}	C04B35/622	C04B35/622		29
C04B35/62268	11	{Fibres based on metal phosphorus oxides, e.g. phosphates}	C04B35/622	C04B35/622		34
C04B35/62272	10	{based on non-oxide ceramics (carbon nanotubes C01B32/15; carbon fibers D01F9/12)}	C04B35/622	C04B35/622		188
C04B35/62277	11	{Fibres based on carbides}	C04B35/622	C04B35/622		114
C04B35/62281	12	{based on silicon carbide (C04B35/571 takes precedence)}	C04B35/622	C04B35/622		285
C04B35/62286	11	{Fibres based on nitrides}	C04B35/622	C04B35/622		58
C04B35/6229	12	{based on boron nitride}	C04B35/622	C04B35/622		71
C04B35/62295	12	{based on silicon nitride (C04B35/589 takes precedence)}	C04B35/622	C04B35/622		83
C04B35/624	9	Sol-gel processing	C04B35/624	C04B35/624		2011
C04B35/626	9	Preparing or treating the powders individually or as batches {(pigments for ceramics C09C1/0009); preparing or treating macroscopic reinforcing agents for ceramic products, e.g. fibres; mechanical aspects section B}	C04B35/626	C04B35/626		1321
C04B35/62605	10	{Treating the starting powders individually or as mixtures}	C04B35/626	C04B35/626		2973
C04B35/6261	11	{Milling}	C04B35/626	C04B35/626		3393
C04B35/62615	12	{High energy or reactive ball milling}	C04B35/626	C04B35/626		951
C04B35/6262	12	{of calcined, sintered clinker or ceramics}	C04B35/626	C04B35/626		854
C04B35/62625	11	{Wet mixtures}	C04B35/626	C04B35/626		942
C04B35/6263	12	{characterised by their solids loadings, i.e. the percentage of solids}	C04B35/626	C04B35/626		1555
C04B35/62635	12	{Mixing details}	C04B35/626	C04B35/626		586
C04B35/6264	12	{Mixing media, e.g. organic solvents}	C04B35/626	C04B35/626		1566
C04B35/62645	11	{Thermal treatment of powders or mixtures thereof other than sintering}	C04B35/626	C04B35/626		1202
C04B35/6265	12	{involving reduction or oxidation}	C04B35/626	C04B35/626		463
C04B35/62655	12	{Drying, e.g. freeze-drying, spray-drying, microwave or supercritical drying}	C04B35/626	C04B35/626		1926
C04B35/6266	13	{Humidity controlled drying}	C04B35/626	C04B35/626		65
C04B35/62665	12	{Flame, plasma or melting treatment}	C04B35/626	C04B35/626		756
C04B35/6267	12	{Pyrolysis, carbonisation or auto-combustion reactions}	C04B35/626	C04B35/626		550
C04B35/62675	12	{characterised by the treatment temperature}	C04B35/626	C04B35/626		1649
C04B35/6268	12	{characterised by the applied pressure or type of atmosphere, e.g. in vacuum, hydrogen or a specific oxygen pressure}	C04B35/626	C04B35/626		556
C04B35/62685	11	{characterised by the order of addition of constituents or additives}	C04B35/626	C04B35/626		792
C04B35/6269	11	{Curing of mixtures}	C04B35/626	C04B35/626		564
C04B35/62695	11	{Granulation or pelletising (devices for shaping artificial aggregates from ceramic mixtures B28B1/004)}	C04B35/626	C04B35/626		1993
C04B35/628	10	Coating the powders {or the macroscopic reinforcing agents}	C04B35/628	C04B35/628		361
C04B35/62802	11	{Powder coating materials}	C04B35/628	C04B35/628		349
C04B35/62805	12	{Oxide ceramics}	C04B35/628	C04B35/628		288
C04B35/62807	13	{Silica or silicates}	C04B35/628	C04B35/628		368
C04B35/6281	13	{Alkaline earth metal oxides}	C04B35/628	C04B35/628		165
C04B35/62813	13	{Alumina or aluminates}	C04B35/628	C04B35/628		339
C04B35/62815	13	{Rare earth metal oxides}	C04B35/628	C04B35/628		202
C04B35/62818	13	{Refractory metal oxides}	C04B35/628	C04B35/628		98
C04B35/62821	14	{Titanium oxide}	C04B35/628	C04B35/628		188
C04B35/62823	14	{Zirconium or hafnium oxide}	C04B35/628	C04B35/628		184
C04B35/62826	13	{Iron group metal oxides}	C04B35/628	C04B35/628		100
C04B35/62828	12	{Non-oxide ceramics}	C04B35/628	C04B35/628		84
C04B35/62831	13	{Carbides}	C04B35/628	C04B35/628		91
C04B35/62834	14	{Silicon carbide}	C04B35/628	C04B35/628		116
C04B35/62836	13	{Nitrides}	C04B35/628	C04B35/628		144
C04B35/62839	13	{Carbon}	C04B35/628	C04B35/628		287
C04B35/62842	12	{Metals}	C04B35/628	C04B35/628		173
C04B35/62844	11	{Coating fibres}	C04B35/628	C04B35/628		247
C04B35/62847	12	{with oxide ceramics}	C04B35/628	C04B35/628		133
C04B35/62849	13	{Silica or silicates}	C04B35/628	C04B35/628		175
C04B35/62852	13	{Alumina or aluminates}	C04B35/628	C04B35/628		149
C04B35/62855	13	{Refractory metal oxides}	C04B35/628	C04B35/628		122
C04B35/62857	12	{with non-oxide ceramics}	C04B35/628	C04B35/628		102
C04B35/6286	13	{Carbides}	C04B35/628	C04B35/628		191
C04B35/62863	14	{Silicon carbide}	C04B35/628	C04B35/628		466
C04B35/62865	13	{Nitrides}	C04B35/628	C04B35/628		108
C04B35/62868	14	{Boron nitride}	C04B35/628	C04B35/628		531
C04B35/62871	14	{Silicon nitride}	C04B35/628	C04B35/628		188
C04B35/62873	13	{Carbon}	C04B35/628	C04B35/628		656
C04B35/62876	12	{with metals}	C04B35/628	C04B35/628		128
C04B35/62878	12	{with boron or silicon}	C04B35/628	C04B35/628		65
C04B35/62881	12	{with metal salts, e.g. phosphates}	C04B35/628	C04B35/628		53
C04B35/62884	11	{by gas phase techniques}	C04B35/628	C04B35/628		702
C04B35/62886	11	{by wet chemical techniques}	C04B35/628	C04B35/628		753
C04B35/62889	11	{with a discontinuous coating layer}	C04B35/628	C04B35/628		78
C04B35/62892	11	{with a coating layer consisting of particles}	C04B35/628	C04B35/628		260
C04B35/62894	11	{with more than one coating layer}	C04B35/628	C04B35/628		537
C04B35/62897	11	{Coatings characterised by their thickness}	C04B35/628	C04B35/628		601
C04B35/63	10	using additives specially adapted for forming the products {, e.g.. binder binders}	C04B35/63	C04B35/63		776
C04B35/6303	11	{Inorganic additives}	C04B35/63	C04B35/63		3551
C04B35/6306	12	{Binders based on phosphoric acids or phosphates}	C04B35/63	C04B35/63		319
C04B35/6309	13	{Aluminium phosphates}	C04B35/63	C04B35/63		321
C04B35/6313	13	{Alkali metal or alkaline earth metal phosphates}	C04B35/63	C04B35/63		227
C04B35/6316	12	{Binders based on silicon compounds}	C04B35/63	C04B35/63		1524
C04B35/632	11	Organic additives	C04B35/632	C04B35/632		3908
C04B35/6325	12	{based on organo-metallic compounds}	C04B35/632	C04B35/632		380
C04B35/634	12	Polymers (C04B35/636 takes precedence)	C04B35/634	C04B35/634		1909
C04B35/63404	13	{obtained by reactions only involving carbon-to-carbon unsaturated bonds}	C04B35/634	C04B35/634		403
C04B35/63408	14	{Polyalkenes}	C04B35/634	C04B35/634		503
C04B35/63412	14	{Coumarone polymers}	C04B35/634	C04B35/634		10
C04B35/63416	14	{Polyvinylalcohols [PVA]; Polyvinylacetates}	C04B35/634	C04B35/634		1768
C04B35/6342	14	{Polyvinylacetals, e.g. polyvinylbutyral [PVB]}	C04B35/634	C04B35/634		666
C04B35/63424	14	{Polyacrylates; Polymethacrylates}	C04B35/634	C04B35/634		1029
C04B35/63428	14	{of ethylenically unsaturated dicarboxylic acid anhydride polymers, e.g. maleic anhydride copolymers}	C04B35/634	C04B35/634		38
C04B35/63432	14	{Polystyrenes}	C04B35/634	C04B35/634		197
C04B35/63436	14	{Halogen-containing polymers, e.g. PVC}	C04B35/634	C04B35/634		155
C04B35/6344	14	{Copolymers containing at least three different monomers}	C04B35/634	C04B35/634		105
C04B35/63444	14	{Nitrogen-containing polymers, e.g. polyacrylamides, polyacrylonitriles, polyvinylpyrrolidone [PVP], polyethylenimine [PEI]}	C04B35/634	C04B35/634		741
C04B35/63448	13	{obtained otherwise than by reactions only involving carbon-to-carbon unsaturated bonds}	C04B35/634	C04B35/634		342
C04B35/63452	14	{Polyepoxides}	C04B35/634	C04B35/634		430
C04B35/63456	14	{Polyurethanes; Polyisocyanates}	C04B35/634	C04B35/634		237
C04B35/6346	14	{Polyesters}	C04B35/634	C04B35/634		237
C04B35/63464	14	{Polycarbonates}	C04B35/634	C04B35/634		79
C04B35/63468	14	{Polyamides}	C04B35/634	C04B35/634		196
C04B35/63472	14	{Condensation polymers of aldehydes or ketones}<br><br><u>NOTE</u><br><br>In this group the following term is used with the meaning indicated: <br>"aldehydes" also covers other organic compounds reacting as aldehydes, e.g. glyoxylic acid. 	C04B35/634	C04B35/634		155
C04B35/63476	15	{Phenol-formaldehyde condensation polymers}	C04B35/634	C04B35/634		668
C04B35/6348	15	{Melamine-formaldehyde condensation polymers}	C04B35/634	C04B35/634		28
C04B35/63484	15	{Urea-formaldehyde condensation polymers}	C04B35/634	C04B35/634		24
C04B35/63488	14	{Polyethers, e.g. alkylphenol polyglycolether, polyethylene glycol [PEG], polyethylene oxide [PEO]}	C04B35/634	C04B35/634		999
C04B35/63492	13	{Natural resins, e.g. rosin}	C04B35/634	C04B35/634		120
C04B35/63496	13	{Bituminous materials, e.g. tar, pitch}	C04B35/634	C04B35/634		514
C04B35/636	12	Polysaccharides or derivatives thereof	C04B35/636	C04B35/636		826
C04B35/6365	13	{Cellulose or derivatives thereof}	C04B35/636	C04B35/636		1424
C04B35/638	11	Removal thereof	C04B35/638	C04B35/638		2647
C04B35/64	9	Burning or sintering processes (C04B33/32 takes precedence {; powder metallurgy B22F})	C04B35/64	C04B35/64		10814
C04B35/645	10	Pressure sintering	C04B35/645	C04B35/645		4929
C04B35/6455	11	{Hot isostatic pressing}	C04B35/645	C04B35/645		1396
C04B35/65	10	Reaction sintering of free metal- or free silicon-containing compositions {(C04B35/573, C04B35/591 take precedence)}	C04B35/65	C04B35/65		1153
C04B35/651	11	{Thermite type sintering, e.g. combustion sintering}	C04B35/65	C04B35/65		165
C04B35/652	11	{Directional oxidation or solidification, e.g. Lanxide process}	C04B35/65	C04B35/65		287
C04B35/653	9	Processes involving a melting step	C04B35/653	C04B35/653		1156
C04B35/657	10	for manufacturing refractories (C04B35/05, C04B35/107, C04B35/484 take precedence)	C04B35/657	C04B35/657		344
C04B35/66	8	Monolithic refractories or refractory mortars, including those whether or not containing clay {(making or repairing of linings F27D1/16)}	C04B35/66	C04B35/66		8109
C04B35/71	8	Ceramic products containing macroscopic reinforcing agents (C04B35/66 takes precedence {; infiltration of a porous ceramic matrix with a material forming a non-ceramic phase C04B41/00, reaction infiltration with Si in order to form SiC C04B35/573, in order to form Si3N4C04B35/591})<br><br><u>NOTE</u><br><br> In groups C04B35/71&#160;-&#160;C04B35/83 the composition of the ceramic products is also classified in groups C04B35/01&#160;-&#160;C04B35/597	C04B35/71	C04B35/71		357
C04B35/74	9	containing shaped metallic materials	C04B35/74	C04B35/74		120
C04B35/76	10	Fibres, filaments, whiskers, platelets, or the like	C04B35/76	C04B35/76		552
C04B35/78	9	containing non-metallic materials	C04B35/78	C04B35/78		196
C04B35/80	10	Fibres, filaments, whiskers, platelets, or the like	C04B35/80	C04B35/80		6363
C04B35/82	11	Asbestos; Glass; Fused silica	C04B35/82	C04B35/82		658
C04B35/83	11	Carbon fibres in a carbon matrix<br><br><u>NOTE</u><br><br>The products covered by this group are usually referred to as "carbon-carbon composites".	C04B35/83	C04B35/83		3589
C04B37/00	7	Joining burned ceramic articles with other burned ceramic articles or other articles by heating {(soldering and welding materials B23K35/24; laminated products B32B, E04C)}<br><br><u>NOTE</u><br><br>In groups C04B37/00 - C04B37/04 features relating to interlayers, additional compositional information or further processing are indexed with codes chosen from C04B2237/00 - C04B2237/88.	C04B37/00	C04B37/00		398
C04B37/001	8	{directly with other burned ceramic articles}	C04B37/00	C04B37/00		684
C04B37/003	8	{by means of an interlayer consisting of a combination of materials selected from glass, or ceramic material with metals, metal oxides or metal salts}	C04B37/00	C04B37/00		520
C04B37/005	9	{consisting of glass or ceramic material}	C04B37/00	C04B37/00		1272
C04B37/006	9	{consisting of metals or metal salts}	C04B37/00	C04B37/00		810
C04B37/008	8	{by means of an interlayer consisting of an organic adhesive, e.g. phenol resin or pitch}	C04B37/00	C04B37/00		421
C04B37/02	8	with metallic articles	C04B37/02	C04B37/02		429
C04B37/021	9	{in a direct manner, e.g. direct copper bonding [DCB]}	C04B37/02	C04B37/02		871
C04B37/023	9	{characterised by the interlayer used (C04B37/028 takes precedence)}	C04B37/02	C04B37/02		449
C04B37/025	10	{consisting of glass or ceramic material}	C04B37/02	C04B37/02		701
C04B37/026	10	{consisting of metals or metal salts}	C04B37/02	C04B37/02		2126
C04B37/028	9	{by means of an interlayer consisting of an organic adhesive, e.g. phenol resin or pitch}	C04B37/02	C04B37/02		197
C04B37/04	8	with articles made from glass	C04B37/04	C04B37/04		113
C04B37/042	9	{in a direct manner}	C04B37/04	C04B37/04		129
C04B37/045	9	{characterised by the interlayer used (C04B37/047 takes precedence)}	C04B37/04	C04B37/04		156
C04B37/047	9	{by means of an interlayer consisting of an organic adhesive, e.g. phenol resin or pitch}	C04B37/04	C04B37/04		54
C04B38/00	7	Porous mortars, concrete, artificial stone or ceramic ware; Preparation thereof (treating slag with gases or gas generating material C04B5/06{; expanded graphite C04B35/536})<br><br><u>NOTE</u><br><br> Porous mortars, concrete, artificial stone or ceramic ware characterised by the ingredients or compositions are also classified in groups C04B2/00 - C04B35/00.<br>Porous materials based on fibres, i.e. materials where the porosity is due to the spaces between the fibres, are not classified in this maingroup, but in one or more of the other relevant maingroups of this subclass, e.g. in C04B30/02.	C04B38/00	C04B38/00		5758
C04B38/0003	8	{containing continuous channels, e.g. of the "dead-end" type or obtained by pushing bars in the green ceramic product (B28B takes precedence)}	C04B38/00	C04B38/00		561
C04B38/0006	8	{Honeycomb structures (from one or more corrugated sheets by winding or stacking C04B38/0083)}	C04B38/00	C04B38/00		2170
C04B38/0009	9	{characterised by features relating to the cell walls, e.g. wall thickness or distribution of pores in the walls}	C04B38/00	C04B38/00		543
C04B38/0012	9	{characterised by the material used for sealing or plugging (some of) the channels of the honeycombs}	C04B38/00	C04B38/00		191
C04B38/0016	9	{assembled from subunits}	C04B38/00	C04B38/00		136
C04B38/0019	10	{characterised by the material used for joining separate subunits}<br><br><u>NOTE</u><br><br>  When classifying in group C04B38/0019, classification is also made in C04B28/00 or C04B37/00 to give detailed information about the composition of the joining material  	C04B38/00	C04B38/00		162
C04B38/0022	8	{obtained by a chemical conversion or reaction other than those relating to the setting or hardening of cement-like material or to the formation of a sol or a gel, e.g. by carbonising or pyrolysing preformed cellular materials based on polymers, organo-metallic or organo-silicon precursors}	C04B38/00	C04B38/00		823
C04B38/0025	9	{starting from inorganic materials only, e.g. metal foam; Lanxide type products}	C04B38/00	C04B38/00		265
C04B38/0029	9	{Porous deposits from the gas phase, e.g. on a temporary support}	C04B38/00	C04B38/00		14
C04B38/0032	9	{one of the precursor materials being a monolithic element having approximately the same dimensions as the final article, e.g. a paper sheet which after carbonisation will react with silicon to form a porous silicon carbide porous body}	C04B38/00	C04B38/00		184
C04B38/0035	9	{by evaporation induced self-assembly}	C04B38/00	C04B38/00		10
C04B38/0038	8	{by superficial sintering or bonding of particulate matter}	C04B38/00	C04B38/00		768
C04B38/0041	9	{the particulate matter having preselected particle sizes}	C04B38/00	C04B38/00		584
C04B38/0045	8	{by a process involving the formation of a sol or a gel, e.g. sol-gel or precipitation processes}	C04B38/00	C04B38/00		1024
C04B38/0048	9	{Precipitation processes}	C04B38/00	C04B38/00		18
C04B38/0051	8	{characterised by the pore size, pore shape or kind of porosity}	C04B38/00	C04B38/00		1081
C04B38/0054	9	{the pores being microsized or nanosized}	C04B38/00	C04B38/00		2652
C04B38/0058	9	{open porosity}	C04B38/00	C04B38/00		659
C04B38/0061	9	{closed porosity}	C04B38/00	C04B38/00		298
C04B38/0064	9	{Multimodal pore size distribution}	C04B38/00	C04B38/00		255
C04B38/0067	8	{characterised by the density of the end product}<br><br><u>NOTE</u><br><br>This group is mainly used for classification using Combination Sets in C04B38/00.	C04B38/00	C04B38/00		2492
C04B38/007	8	{characterised by the pore distribution, e.g. inhomogeneous distribution of pores}<br><br><u>NOTE</u><br><br>This group is mainly used for classification using Combination Sets in C04B38/00.	C04B38/00	C04B38/00		396
C04B38/0074	9	{expressed as porosity percentage}	C04B38/00	C04B38/00		3894
C04B38/0077	9	{Materials with a non-porous skin}	C04B38/00	C04B38/00		64
C04B38/008	8	{Bodies obtained by assembling separate elements having such a configuration that the final product is porous or by spirally winding one or more corrugated sheets}	C04B38/00	C04B38/00		112
C04B38/0083	9	{from one or more corrugated sheets or sheets bearing protrusions by winding or stacking}	C04B38/00	C04B38/00		83
C04B38/0087	8	{by generating pores in the ceramic material while in the molten state}	C04B38/00	C04B38/00		49
C04B38/009	8	{Porous or hollow ceramic granular materials, e.g. microballoons (C04B18/027, C04B20/002 take precedence)}	C04B38/00	C04B38/00		1811
C04B38/0093	8	{Other features}	C04B38/00	C04B38/00		48
C04B38/0096	9	{Pores with coated inner walls}	C04B38/00	C04B38/00		162
C04B38/02	8	by adding chemical blowing agents	C04B38/02	C04B38/02		7736
C04B38/025	9	{generated by microorganisms}	C04B38/02	C04B38/02		38
C04B38/04	8	by dissolving-out added substances	C04B38/04	C04B38/04		432
C04B38/045	9	{the dissolved-out substance being a monolitic element having approximately the same dimensions as the final article, e.g. a prepreg obtained by bonding together dissolvable particles (C04B38/0022 takes precedence)}	C04B38/04	C04B38/04		64
C04B38/06	8	by burning-out added substances {by burning natural expanding materials or by sublimating or melting out added substances}<br><br><u>NOTE</u><br><br> Documents in which the characteristic feature is the choice of meltable or sublimable material or the physical aspects of the porous body obtained are classified accordingly, and symbols C04B38/0605 or C04B38/061 are allocated in Combination Sets. 	C04B38/06	C04B38/06		923
C04B38/0605	9	{by sublimating}	C04B38/06	C04B38/06		266
C04B38/061	9	{by melting out}	C04B38/06	C04B38/06		144
C04B38/0615	9	{the burned-out substance being a monolitic element having approximately the same dimensions as the final article, e.g. a porous polyurethane sheet or a prepreg obtained by bonding together resin particles (C04B38/0022 takes precedence)}	C04B38/06	C04B38/06		725
C04B38/062	10	{the burned-out substance being formed in situ, e.g. by polymerisation of a prepolymer composition containing ceramic powder}	C04B38/06	C04B38/06		93
C04B38/0625	11	{involving a foaming step of the burnable material}	C04B38/06	C04B38/06		44
C04B38/063	9	{Preparing or treating the raw materials individually or as batches}	C04B38/06	C04B38/06		81
C04B38/0635	10	{Compounding ingredients (C04B38/0615 takes precedence)}	C04B38/06	C04B38/06		120
C04B38/064	11	{Natural expanding materials, e.g. clay}	C04B38/06	C04B38/06		259
C04B38/0645	11	{Burnable, meltable, sublimable materials}	C04B38/06	C04B38/06		1477
C04B38/065	12	{characterised by physical aspects, e.g. shape, size or porosity}<br><br><u>NOTE</u><br><br>Documents having this group as classification symbol or as part of a Combination Set can also get symbol C04B38/0051 in the Combination Set, if the importance of the size of the pores obtained is emphasized.	C04B38/06	C04B38/06		268
C04B38/0655	13	{Porous materials (C04B38/0625 takes precedence)}	C04B38/06	C04B38/06		114
C04B38/066	12	{characterised by distribution, e.g. for obtaining inhomogeneous distribution of pores}<br><br><u>NOTE</u><br><br> Documents having this group as classification symbol or as part of a Combination Set can also get symbol C04B38/007 in the Combination Set, if the importance of the distribution of the pores is emphasized.	C04B38/06	C04B38/06		37
C04B38/0665	12	{Waste material; Refuse other than vegetable refuse}	C04B38/06	C04B38/06		307
C04B38/067	12	{Macromolecular compounds (C04B38/062 takes precedence)}	C04B38/06	C04B38/06		1800
C04B38/0675	12	{Vegetable refuse; Cellulosic materials, e.g. wood chips, cork, peat, paper}	C04B38/06	C04B38/06		1140
C04B38/068	12	{Carbonaceous materials, e.g. coal, carbon, graphite, hydrocarbons}	C04B38/06	C04B38/06		1517
C04B38/0685	12	{Minerals containing carbon, e.g. oil shale}	C04B38/06	C04B38/06		28
C04B38/069	11	{Other materials, e.g. catalysts (C04B33/13, C04B35/00 take precedence)}	C04B38/06	C04B38/06		66
C04B38/0695	9	{Physical aspects of the porous material obtained}	C04B38/06	C04B38/06		61
C04B38/08	8	by adding porous substances	C04B38/08	C04B38/08		3780
C04B38/085	9	{of micro- or nanosize}	C04B38/08	C04B38/08		465
C04B38/10	8	by using foaming agents (C04B38/02 takes precedence){or by using mechanical means, e.g. adding preformed foam}	C04B38/10	C04B38/10		5553
C04B38/103	9	{the foaming being obtained by the introduction of a gas other than untreated air, e.g. nitrogen}	C04B38/10	C04B38/10		170
C04B38/106	9	{by adding preformed foams}	C04B38/10	C04B38/10		981
C04B40/00	7	Processes, in general, for influencing or modifying the properties of mortars, concrete or artificial stone compositions, e.g. their setting or hardening ability (active ingredients C04B22/00&#160;-&#160;C04B24/00; hardening of a well-defined composition C04B26/00&#160;-&#160;C04B28/00; making porous, cellular or lightening C04B38/00; mechanical aspects B28, e.g. conditioning the materials prior to shaping B28B17/02)	C04B40/00	C04B40/00		3078
C04B40/0003	8	{making use of electric or wave energy or particle radiation}	C04B40/00	C04B40/00		25
C04B40/0007	9	{Electric, magnetic or electromagnetic fields}	C04B40/00	C04B40/00		107
C04B40/001	9	{Electromagnetic waves}	C04B40/00	C04B40/00		26
C04B40/0014	10	{Microwaves}	C04B40/00	C04B40/00		75
C04B40/0017	10	{Irradiation, i.e. gamma -, X -, UV rays}	C04B40/00	C04B40/00		25
C04B40/0021	9	{Sonic or ultrasonic waves, e.g. to initiate sonochemical reactions}	C04B40/00	C04B40/00		99
C04B40/0025	8	{obtaining colloidal mortar}	C04B40/00	C04B40/00		72
C04B40/0028	8	{Aspects relating to the mixing step of the mortar preparation}	C04B40/00	C04B40/00		4940
C04B40/0032	9	{Controlling the process of mixing, e.g. adding ingredients in a quantity depending on a measured or desired value (B28C7/00 takes precedence)}	C04B40/00	C04B40/00		843
C04B40/0035	9	{Processes characterised by the absence of a mechanical mixing step, e.g. "no-mix" processes}	C04B40/00	C04B40/00		76
C04B40/0039	9	{Premixtures of ingredients}	C04B40/00	C04B40/00		11970
C04B40/0042	10	{Powdery mixtures}	C04B40/00	C04B40/00		1407
C04B40/0046	10	{characterised by their processing, e.g. sequence of mixing the ingredients when preparing the premixtures}	C04B40/00	C04B40/00		1701
C04B40/005	9	{High shear mixing; Obtaining macro-defect free materials}	C04B40/00	C04B40/00		171
C04B40/0053	10	{Obtaining macro-defect free materials otherwise than by high shear mixing}	C04B40/00	C04B40/00		2
C04B40/0057	9	{Energetic mixing (C04B40/005 takes precedence)}	C04B40/00	C04B40/00		77
C04B40/006	9	{involving the elimination of excess water from the mixture}	C04B40/00	C04B40/00		362
C04B40/0064	10	{Processes of the Magnini or Hatscheck type}	C04B40/00	C04B40/00		147
C04B40/0067	8	{making use of vibrations}	C04B40/00	C04B40/00		710
C04B40/0071	8	{making use of a rise in pressure}	C04B40/00	C04B40/00		1429
C04B40/0075	8	{making use of a decrease in temperature}	C04B40/00	C04B40/00		215
C04B40/0078	9	{by freezing}	C04B40/00	C04B40/00		45
C04B40/0082	8	{making use of a rise in temperature, e.g. caused by an exothermic reaction}	C04B40/00	C04B40/00		1082
C04B40/0085	9	{involving melting of at least part of the composition}	C04B40/00	C04B40/00		121
C04B40/0089	8	{making use of vacuum or reduced pressure}	C04B40/00	C04B40/00		260
C04B40/0091	8	{Processes of mixing characterised by carbon dioxide treatment}<br><br><u>WARNING</u><br>Group C04B40/0091 is incomplete pending reclassification of documents from group C04B40/0231.<br>Groups C04B40/0091 and C04B40/0231 should be considered in order to perform a complete search.	C04B40/00	C04B40/00		87
C04B40/0092	8	{Temporary binders, mortars or concrete, i.e. materials intended to be destroyed or removed after hardening, e.g. by acid dissolution}	C04B40/00	C04B40/00		102
C04B40/0096	8	{Provisions for indicating condition of the compositions or the final products, e.g. degree of homogeneous mixing, degree of wear}	C04B40/00	C04B40/00		132
C04B40/02	8	Selection of the hardening environment<br><br><u>NOTE</u><br><br> In this group the following term is used with the meaning indicated: <br>"hardening" covers also setting, pre-curing and curing 	C04B40/02	C04B40/02		2003
C04B40/0204	9	{making use of electric or wave energy or particle radiation}	C04B40/02	C04B40/02		45
C04B40/0209	10	{Electric, magnetic or electromagnetic fields}	C04B40/02	C04B40/02		103
C04B40/0213	10	{Electromagnetic waves}	C04B40/02	C04B40/02		41
C04B40/0218	11	{Microwaves}	C04B40/02	C04B40/02		140
C04B40/0222	11	{Irradiation, i.e. gamma -, X -, UV rays}	C04B40/02	C04B40/02		52
C04B40/0227	10	{Sonic or ultrasonic waves}	C04B40/02	C04B40/02		31
C04B40/0231	9	{Carbon dioxide hardening}<br><br><u>WARNING</u><br>Group C04B40/0231 is impacted by reclassification into group C04B40/0091.<br>Groups C04B40/0231 and C04B40/0091 should be considered in order to perform a complete search.	C04B40/02	C04B40/02		1104
C04B40/0236	10	{Carbon dioxide post-treatment of already hardened material}	C04B40/02	C04B40/02		160
C04B40/024	9	{Steam hardening, e.g. in an autoclave}	C04B40/02	C04B40/02		2536
C04B40/0245	10	{including a pre-curing step not involving a steam or autoclave treatment}	C04B40/02	C04B40/02		211
C04B40/025	9	{Adiabatic curing or hardening}	C04B40/02	C04B40/02		32
C04B40/0254	9	{Hardening in an enclosed space, e.g. in a flexible container}	C04B40/02	C04B40/02		95
C04B40/0259	9	{Hardening promoted by a rise in pressure (C04B40/024 takes precedence)}	C04B40/02	C04B40/02		1209
C04B40/0263	9	{Hardening promoted by a rise in temperature (C04B40/024 takes precedence)}	C04B40/02	C04B40/02		2331
C04B40/0268	10	{Heating up to sintering temperatures (C04B41/0072 takes precedence)}	C04B40/02	C04B40/02		473
C04B40/0272	9	{Hardening under vacuum or reduced pressure}	C04B40/02	C04B40/02		136
C04B40/0277	9	{Hardening promoted by using additional water, e.g. by spraying water on the green concrete element (steam hardening C04B40/024)}	C04B40/02	C04B40/02		588
C04B40/0281	10	{Hardening in an atmosphere of increased relative humidity}	C04B40/02	C04B40/02		221
C04B40/0286	10	{Hardening under water}	C04B40/02	C04B40/02		121
C04B40/029	10	{using an aqueous solution or dispersion}	C04B40/02	C04B40/02		200
C04B40/0295	9	{Inhomogeneous curing or hardening, e.g. accelerated curing of surface regions of a concrete article; Influencing the setting or hardening process to generate physical or mechanical effects, e.g. to create cracks}	C04B40/02	C04B40/02		59
C04B40/04	8	Preventing evaporation of the mixing water (permanent coverings C04B41/00)	C04B40/04	C04B40/04		481
C04B40/06	8	Inhibiting the setting, e.g. mortars of the deferred action type containing water in breakable containers {; Inhibiting the action of active ingredients}<br><br><u>NOTE</u><br><br> Compositions with prolonged pot-life are not classified here. <br> They are classified as other compositions and the symbol C04B2111/00086 is allocated in Combination Set. 	C04B40/06	C04B40/06		673
C04B40/0608	9	{Dry ready-made mixtures, e.g. mortars at which only water or a water solution has to be added before use}	C04B40/06	C04B40/06		1025
C04B40/0616	10	{preformed, e.g. bandages}	C04B40/06	C04B40/06		112
C04B40/0625	9	{Wet ready-made mixtures, e.g. mortars in water- or airtight packages, or mortars containing an accelerator in a breakable emulsion}	C04B40/06	C04B40/06		108
C04B40/0633	9	{Chemical separation of ingredients, e.g. slowly soluble activator}	C04B40/06	C04B40/06		176
C04B40/0641	9	{Mechanical separation of ingredients, e.g. accelerator in breakable microcapsules}	C04B40/06	C04B40/06		189
C04B40/065	10	{Two or more component mortars}	C04B40/06	C04B40/06		827
C04B40/0658	9	{Retarder inhibited mortars activated by the addition of accelerators or retarder-neutralising agents}	C04B40/06	C04B40/06		182
C04B40/0666	9	{Chemical plugs based on hydraulic hardening materials}	C04B40/06	C04B40/06		155
C04B40/0675	9	{Mortars activated by rain, percolating or sucked-up water; Self-healing mortars or concrete}	C04B40/06	C04B40/06		196
C04B40/0683	9	{inhibiting by freezing or cooling}	C04B40/06	C04B40/06		97
C04B40/0691	9	{Thermally activated mortars, e.g. by melting ingredients}	C04B40/06	C04B40/06		12
C04B41/00	7	After-treatment of mortars, concrete, artificial stone or ceramics; Treatment of natural stone (conditioning of the materials prior to shaping C04B40/00; applying liquids or other fluent materials to surfaces, in general B05; grinding or polishing B24; apparatus or processes for treating or working shaped articles of clay or other ceramic compositions, slag or mixtures containing cementitious material B28B11/00; working stone or stone-like materials B28D; glazes, other than cold glazes, C03C8/00; etching, surface-brightening or pickling compositions C09K13/00)<br><br><u>NOTE</u><br><br>In this group, the following terms or expressions are used with the meanings indicated: <br> "mortars", "concrete" and "artificial stone" cover materials after primary shaping.<br>Treating, e.g. coating or impregnating, a material with the same material or with a substance that ultimately is transformed into the same material is not considered aftertreatment for this group but is classified as preparation of the material, e.g. a carbon body impregnated with a carbonisable substance is classified in C04B35/52. <br>In groups C04B41/45 - C04B41/80, the last place priority rule is applied, i.e. at each hierarchical level, in the absence of an indication to the contrary, classification is made in the last appropriate place.<br>In this group, multiple classification is made according to the following rules: <br>when the substrate to be treated is of the artificial stone type, e.g. concrete, classification is made in the range C04B41/00 - C04B41/5392 as well as in the range C04B41/60 - C04B41/72<br>when the substrate to be treated is of the ceramic type, classification is made in the range C04B41/00 - C04B41/5392 as well as in the range C04B41/80 - C04B41/91<br>when the substrate to be treated is aspecific, classification is made only in the range C04B41/00 - C04B41/5392<br>In groups C04B41/0018 - C04B41/53, in the absence of an indication to the contrary, classification is made in the last appropriate place.<br>In groups C04B41/00 - C04B41/53, it is desirable to add the indexing codes relating to the nature of the substrate being treated. The indexing codes that are chosen from groups C04B26/00 - C04B38/00 should be unlinked.<br>In groups C04B41/00 - C04B41/53, it is desirable to add the indexing codes relating to aspects of the coating composition or to the method of application. The indexing codes that are chosen from groups C04B41/00 - C04B41/5392 should be unlinked.<br>Attention is drawn to internal Note (2) following the title of subclass C04B.	C04B41/00	C04B41/00		593
C04B41/0009	8	{Demolition agents based on cementitous or like materials}<br><br><u>NOTE</u><br><br>Products classified in group C04B41/0009 should also be classified according to their composition, e.g. in C04B28/00.	C04B41/00	C04B41/00		78
C04B41/0018	8	{Coating or impregnating "in situ", e.g. impregnating of artificial stone by subsequent melting of a compound added to the artificial stone composition}	C04B41/00	C04B41/00		167
C04B41/0027	8	{Ion-implantation, ion-irradiation or ion-injection}	C04B41/00	C04B41/00		133
C04B41/0036	8	{Laser treatment (working by laser beam B23K26/00)}	C04B41/00	C04B41/00		435
C04B41/0045	8	{Irradiation; Radiation, e.g. with UV or IR (C04B41/0036 takes precedence)}	C04B41/00	C04B41/00		304
C04B41/0054	8	{Plasma-treatment, e.g. with gas-discharge plasma}	C04B41/00	C04B41/00		175
C04B41/0063	8	{Cooling, e.g. freezing}<br><br><u>NOTE</u><br><br>In this group the term "cooling" is used in the sense of an additional cooling treatment, different from the traditional cooling step in the fabrication of materials involving a heating step, such as sintering of ceramics.	C04B41/00	C04B41/00		49
C04B41/0072	8	{Heat treatment}	C04B41/00	C04B41/00		6093
C04B41/0081	9	{characterised by the subsequent cooling step}	C04B41/00	C04B41/00		138
C04B41/009	8	{characterised by the material treated}	C04B41/00	C04B41/00		22957
C04B41/45	8	Coating or impregnating (paints C09D), {e.g. injection in masonry, partial coating of green or fired ceramics, organic coating compositions for adhering together two concrete elements (ion-implantation C04B41/0027)}<br><br><u>NOTE</u><br><br> In group C04B41/45 and sub-groups, as a general rule, classification is made according to the end products, rather than according to the starting materials, in the coating or impregnating compositions. <br> In groups C04B41/45&#160;-&#160;C04B41/528  the following term is used with the meaning indicated: <br>"coating" covers material applied to the substrates as powdery material or applied from the gas or liquid phase, e.g. as a slurry; it only covers the use of preformed sheet-like elements in so far as the thickness of these sheets is small compared with the thickness of the substrate and so far as the resulting product is not exclusively one of the type classifiable in B32B	C04B41/45	C04B41/45		1247
C04B41/4501	9	{with preformed sheet-like elements}	C04B41/45	C04B41/45		300
C04B41/4503	10	{having an adhesive layer}	C04B41/45	C04B41/45		55
C04B41/4505	9	{characterised by the method of application}	C04B41/45	C04B41/45		2149
C04B41/4507	10	{using keying elements, e.g. particulate material, to facilitate the adherence of coating layers}	C04B41/45	C04B41/45		24
C04B41/4509	11	{The keying element being generated from identations made in the substrate}	C04B41/45	C04B41/45		12
C04B41/4511	10	{using temporarily supports, e.g. decalcomania transfers or mould surfaces}	C04B41/45	C04B41/45		341
C04B41/4513	11	{the temporary support- and coating material being mixed together, e.g. tile glazing paper sheets}	C04B41/45	C04B41/45		13
C04B41/4515	10	{application under vacuum or reduced pressure}	C04B41/45	C04B41/45		511
C04B41/4517	10	{application under inert, e.g. non-oxidising, atmosphere}	C04B41/45	C04B41/45		223
C04B41/4519	10	{application under an other specific atmosphere}	C04B41/45	C04B41/45		348
C04B41/4521	10	{application under increased pressure}	C04B41/45	C04B41/45		337
C04B41/4523	10	{applied from the molten state (vitreous materials C04B41/5022); Thermal spraying, e.g. plasma spraying}<br><br><u>NOTE</u><br><br>Coating or impregnating with a specific material in the molten state is classified according to the specific material and get symbol C04B41/4523 in Combination Sets.	C04B41/45	C04B41/45		1191
C04B41/4525	11	{using a molten bath as vehicle, e.g. molten borax}	C04B41/45	C04B41/45		44
C04B41/4527	11	{Plasma spraying (deposition from the gas phase using plasma C04B41/4533)}	C04B41/45	C04B41/45		560
C04B41/4529	10	{applied from the gas phase}<br><br><u>NOTE</u><br><br>Coating or impregnating with a specific material from the gas phase is classified according to the specific material and symbol C04B41/4529 is allocated in Combination Sets.	C04B41/45	C04B41/45		1184
C04B41/4531	11	{by C.V.D.}	C04B41/45	C04B41/45		918
C04B41/4533	11	{plasma assisted}	C04B41/45	C04B41/45		159
C04B41/4535	10	{applied as a solution, emulsion, dispersion or suspension}<br><br><u>NOTE</u><br><br>Coating or impregnation with a solution or a suspension of a specific material is classified according to the specific material and symbol C04B41/4535 is allocated in Combination Sets.	C04B41/45	C04B41/45		3522
C04B41/4537	11	{by the sol-gel process}	C04B41/45	C04B41/45		401
C04B41/4539	11	{as a emulsion, dispersion or suspension}	C04B41/45	C04B41/45		4806
C04B41/4541	11	{Electroless plating}	C04B41/45	C04B41/45		94
C04B41/4543	11	{by spraying, e.g. by atomising}	C04B41/45	C04B41/45		2139
C04B41/4545	10	{applied as a powdery material}<br><br><u>NOTE</u><br><br>Coating or impregnation with a specific powdery material is classified according to the specific material and symbols C04B41/4545&#160;-&#160;C04B41/4549 are allocated in Combination Sets.	C04B41/45	C04B41/45		790
C04B41/4547	11	{characterised by the grain distribution}	C04B41/45	C04B41/45		66
C04B41/4549	12	{Nanometer-sized particles}	C04B41/45	C04B41/45		166
C04B41/455	10	{the coating or impregnating process including a chemical conversion or reaction}	C04B41/45	C04B41/45		1167
C04B41/4552	11	{the end product being obtained by a multistep reaction or conversion}	C04B41/45	C04B41/45		128
C04B41/4554	11	{the coating or impregnating material being an organic or organo-metallic precursor of an inorganic material}	C04B41/45	C04B41/45		760
C04B41/4556	11	{coating or impregnating with a product reacting with the substrate, e.g. generating a metal coating by surface reduction of a ceramic substrate}	C04B41/45	C04B41/45		933
C04B41/4558	11	{Coating or impregnating involving the chemical conversion of an already applied layer, e.g. obtaining an oxide layer by oxidising an applied metal layer}	C04B41/45	C04B41/45		405
C04B41/456	12	{the conversion only taking place under certain conditions, e.g. avoiding damage of underlaying layers or parts of the substrate}	C04B41/45	C04B41/45		88
C04B41/4562	10	{Photographic methods, e.g. making use of photo-sensitive materials}	C04B41/45	C04B41/45		34
C04B41/4564	10	{Electrolytic or electrophoretic processes, e.g. electrochemical re-alkalisation of reinforced concrete (desalination C04B41/53)}	C04B41/45	C04B41/45		312
C04B41/4566	11	{Electrochemical re-alcalisation (electrochemical desalination C04B41/5369; cathodic protection C23F13/02)}	C04B41/45	C04B41/45		31
C04B41/4568	10	{Electrostatic processes}	C04B41/45	C04B41/45		75
C04B41/457	9	{Non-superficial impregnation or infiltration of the substrate}	C04B41/45	C04B41/45		466
C04B41/4572	9	{Partial coating or impregnation of the surface of the substrate}	C04B41/45	C04B41/45		1257
C04B41/4574	10	{Coating different parts of the substrate with different materials}	C04B41/45	C04B41/45		158
C04B41/4576	10	{Inlaid coatings, i.e. resulting in a plane surface}	C04B41/45	C04B41/45		144
C04B41/4578	9	{Coating or impregnating of green ceramics or unset concrete}	C04B41/45	C04B41/45		1234
C04B41/458	10	{involving a mixing step with the top layer of the substrate}	C04B41/45	C04B41/45		29
C04B41/4582	9	{Porous coatings, e.g. coating containing porous fillers}	C04B41/45	C04B41/45		681
C04B41/4584	9	{Coating or impregnating of particulate or fibrous ceramic material (C04B20/10, C04B35/628 take precedence)}	C04B41/45	C04B41/45		743
C04B41/4586	9	{Non-chemical aspects relating to the substrate being coated or impregnated}	C04B41/45	C04B41/45		20
C04B41/4588	10	{Superficial melting of the substrate before or during the coating or impregnating step}	C04B41/45	C04B41/45		3
C04B41/459	9	{Temporary coatings or impregnations (C04B40/04 takes precedence)}	C04B41/45	C04B41/45		134
C04B41/4592	10	{for masking purposes}	C04B41/45	C04B41/45		53
C04B41/4594	11	{in metallisation processes}	C04B41/45	C04B41/45		9
C04B41/4596	9	{with fibrous materials or whiskers}	C04B41/45	C04B41/45		675
C04B41/4598	9	{with waste materials}	C04B41/45	C04B41/45		172
C04B41/46	9	with organic materials	C04B41/46	C04B41/46		2401
C04B41/463	10	{Organic solvents}	C04B41/46	C04B41/46		882
C04B41/466	10	{Halogenated compounds, e.g. perfluor-compounds}	C04B41/46	C04B41/46		112
C04B41/47	10	Oils, fats or waxes {natural resins}	C04B41/47	C04B41/47		495
C04B41/472	11	{Oils, e.g. linseed oil}	C04B41/47	C04B41/47		220
C04B41/474	11	{Natural resins, e.g. rosin}	C04B41/47	C04B41/47		166
C04B41/476	12	{Cellulosic waste liquor, e.g. sulfite lye}	C04B41/47	C04B41/47		5
C04B41/478	11	{Bitumen, asphalt, e.g. paraffin}	C04B41/47	C04B41/47		511
C04B41/48	10	Macromolecular compounds	C04B41/48	C04B41/48		1858
C04B41/4803	11	{Polysaccharides, e.g. cellulose, or derivatives thereof}	C04B41/48	C04B41/48		663
C04B41/4807	11	{Proteins or derivatives thereof}	C04B41/48	C04B41/48		98
C04B41/4811	11	{Condensation polymers of aldehydes or ketones}<br><br><u>NOTE</u><br><br>In this group the following term is used with the meaning indicated: <br> "aldehydes" also covers other organic compounds reacting as aldehydes, e.g. glyoxylic acid. 	C04B41/48	C04B41/48		111
C04B41/4815	12	{Melamine-formaldehyde condensation products}	C04B41/48	C04B41/48		18
C04B41/4819	12	{Urea-formaldehyde condensation products}	C04B41/48	C04B41/48		25
C04B41/4823	11	{Phenol-formaldehyde condensation products}	C04B41/48	C04B41/48		150
C04B41/4826	11	{Polyesters}	C04B41/48	C04B41/48		270
C04B41/483	11	{Polyacrylates}	C04B41/48	C04B41/48		1306
C04B41/4834	12	{Polyacrylamides}	C04B41/48	C04B41/48		66
C04B41/4838	11	{Halogenated polymers}	C04B41/48	C04B41/48		145
C04B41/4842	12	{Fluorine-containing polymers}	C04B41/48	C04B41/48		274
C04B41/4846	13	{Perfluoro-compounds}	C04B41/48	C04B41/48		99
C04B41/4849	11	{Sulfur-containing polymers}	C04B41/48	C04B41/48		31
C04B41/4853	11	{Epoxides}	C04B41/48	C04B41/48		931
C04B41/4857	11	{Other macromolecular compounds obtained by reactions only involving carbon-to-carbon unsaturated bonds}	C04B41/48	C04B41/48		574
C04B41/4861	12	{Polyalkenes}	C04B41/48	C04B41/48		205
C04B41/4865	12	{Coumarone polymers}	C04B41/48	C04B41/48		2
C04B41/4869	12	{Polyvinylalcohols, polyvinylacetates}	C04B41/48	C04B41/48		510
C04B41/4873	12	{Polyvinylacetals}	C04B41/48	C04B41/48		34
C04B41/4876	12	{Polystyrene}	C04B41/48	C04B41/48		211
C04B41/488	11	{Other macromolecular compounds obtained otherwise than by reactions only involving unsaturated carbon-to-carbon bonds}	C04B41/48	C04B41/48		382
C04B41/4884	12	{Polyurethanes; Polyisocyanates}	C04B41/48	C04B41/48		706
C04B41/4888	12	{Polycarbonates}	C04B41/48	C04B41/48		20
C04B41/4892	12	{Polyamides}	C04B41/48	C04B41/48		115
C04B41/4896	12	{Polyethers}	C04B41/48	C04B41/48		453
C04B41/49	10	Compounds having one or more carbon-to-metal or carbon-to-silicon linkages {; Organo-clay compounds; Organo-silicates, i.e. ortho- or polysilicic acid esters (to obtain SiO2C04B41/5089, C04B41/5035); Organo-phosphorus compounds; Organo-inorganic complexes}<br><br><u>NOTE</u><br><br> As distinct from the general practice in C04B41/00, classification in C04B41/49 and sub-groups is done according to the nature of the starting products, not according to the nature of the end products 	C04B41/49	C04B41/49		262
C04B41/4905	11	{containing silicon}	C04B41/49	C04B41/49		758
C04B41/4911	12	{Organo-clay compounds}	C04B41/49	C04B41/49		8
C04B41/4916	12	{applied to the substrate as a solventless liquid}	C04B41/49	C04B41/49		25
C04B41/4922	12	{applied to the substrate as monomers, i.e. as organosilanes RnSiX4-n, e.g. alkyltrialkoxysilane, dialkyldialkoxysilane}	C04B41/49	C04B41/49		857
C04B41/4927	13	{Alkali metal or ammonium salts}	C04B41/49	C04B41/49		113
C04B41/4933	13	{containing halogens, i.e. organohalogen silanes}	C04B41/49	C04B41/49		177
C04B41/4938	13	{containing silicon bound to hydroxy groups, e.g. trimethyl silanol}	C04B41/49	C04B41/49		53
C04B41/4944	13	{containing atoms other than carbon, hydrogen, oxygen, silicon, alkali metals or halogens, e.g. N-silyldisilazane: Image}	C04B41/49	C04B41/49		150
C04B41/495	12	{applied to the substrate as oligomers or polymers}	C04B41/49	C04B41/49		179
C04B41/4955	13	{Polyorganosilanes, i.e. polymers with a Si-Si-Si- chain}	C04B41/49	C04B41/49		55
C04B41/4961	13	{Polyorganosiloxanes, i.e. polymers with a Si-O-Si-O-chain; "silicones"}	C04B41/49	C04B41/49		997
C04B41/4966	14	{containing silicon bound to hydroxy groups, i.e. OH-blocked polysiloxanes}	C04B41/49	C04B41/49		58
C04B41/4972	14	{Alkali metal or ammonium salts}	C04B41/49	C04B41/49		24
C04B41/4977	13	{characterised by the number of silicon atoms}	C04B41/49	C04B41/49		37
C04B41/4983	13	{Polycarbosilanes, i.e. polymers with a -Si-C-Si-chain; Polysilazanes, i.e. polymers with a -Si-N-Si-chain; Polysilathianes, i.e. polymers with a -Si-S-Si-chain}	C04B41/49	C04B41/49		46
C04B41/4988	12	{Organosilicium-organic copolymers, e.g. olefins with terminal silane groups}	C04B41/49	C04B41/49		81
C04B41/4994	11	{Organo-phosphorus compounds}	C04B41/49	C04B41/49		35
C04B41/50	9	with inorganic materials	C04B41/50	C04B41/50		2155
C04B41/5001	10	{with carbon or carbonisable materials}	C04B41/50	C04B41/50		1492
C04B41/5002	11	{Diamond}	C04B41/50	C04B41/50		136
C04B41/5003	11	{Fullerenes or derivatives thereof}	C04B41/50	C04B41/50		7
C04B41/5005	11	{Carbon fluorides; Halogen containing carbon or graphite intercallation products}	C04B41/50	C04B41/50		7
C04B41/5006	10	{Boron compounds}	C04B41/50	C04B41/50		337
C04B41/5007	10	{with salts or salty compositions, e.g. for salt glazing (C04B41/5006 takes precedence)}	C04B41/50	C04B41/50		708
C04B41/5009	11	{containing nitrogen in the anion, e.g. nitrites}	C04B41/50	C04B41/50		234
C04B41/501	11	{containing carbon in the anion, e.g. carbonates}	C04B41/50	C04B41/50		486
C04B41/5011	11	{containing halogen in the anion}	C04B41/50	C04B41/50		115
C04B41/5012	12	{chlorides}	C04B41/50	C04B41/50		288
C04B41/5014	11	{containing sulfur in the anion, e.g. sulfides}	C04B41/50	C04B41/50		358
C04B41/5015	11	{containing phosphorus in the anion, e.g. phosphates}	C04B41/50	C04B41/50		375
C04B41/5016	10	{Acids}	C04B41/50	C04B41/50		242
C04B41/5018	10	{with fluorine compounds}	C04B41/50	C04B41/50		288
C04B41/5019	11	{applied from the gas phase, e.g. ocratation}	C04B41/50	C04B41/50		36
C04B41/502	10	{Water}	C04B41/50	C04B41/50		554
C04B41/5022	10	{with vitreous materials (composition of vitreous glazes and enamels C03C; ceramic pigments C09C1/0009)}<br><br><u>NOTE</u><br><br>Glazing of concrete, natural or artificial stone or ceramics is only classified in C04B41/5022 when non-compositional aspects are important, e.g. aspects relating to the method of application or the choice of the substrate.	C04B41/50	C04B41/50		7971
C04B41/5023	11	{Glass-ceramics (compositions of glass-ceramics C03C10/00)}	C04B41/50	C04B41/50		167
C04B41/5024	10	{Silicates (C04B41/5022 takes precedence; silico-fluorides C04B41/5018)}	C04B41/50	C04B41/50		1751
C04B41/5025	10	{with ceramic materials (copper oxide or solid solutions thereof C04B41/5074)}<br><br><u>NOTE</u><br><br>In this subgroup, the materials considered as ceramic materials are those covered by groups C04B33/00&#160;-&#160;C04B35/83.	C04B41/50	C04B41/50		1423
C04B41/5027	11	{Oxide ceramics in general; Specific oxide ceramics not covered by C04B41/5029&#160;-&#160;C04B41/5051}	C04B41/50	C04B41/50		1010
C04B41/5028	12	{Manganates}	C04B41/50	C04B41/50		24
C04B41/5029	11	{Magnesia}	C04B41/50	C04B41/50		409
C04B41/5031	11	{Alumina}	C04B41/50	C04B41/50		1854
C04B41/5032	12	{Aluminates (aluminate spinels C04B41/5046)}	C04B41/50	C04B41/50		205
C04B41/5033	11	{Chromium oxide}	C04B41/50	C04B41/50		168
C04B41/5035	11	{Silica}	C04B41/50	C04B41/50		2201
C04B41/5036	11	{Ferrites}	C04B41/50	C04B41/50		169
C04B41/5037	11	{Clay, Kaolin}	C04B41/50	C04B41/50		953
C04B41/5038	12	{Porcelain}	C04B41/50	C04B41/50		22
C04B41/504	12	{Engobes}	C04B41/50	C04B41/50		758
C04B41/5041	11	{Titanium oxide or titanates}	C04B41/50	C04B41/50		1291
C04B41/5042	11	{Zirconium oxides or zirconates; Hafnium oxides or hafnates}	C04B41/50	C04B41/50		1181
C04B41/5044	12	{Hafnates}	C04B41/50	C04B41/50		64
C04B41/5045	11	{Rare-earth oxides}	C04B41/50	C04B41/50		606
C04B41/5046	11	{Spinels, e.g. magnesium aluminate spinels}	C04B41/50	C04B41/50		79
C04B41/5048	11	{Phosphates}	C04B41/50	C04B41/50		215
C04B41/5049	11	{Zinc or bismuth oxides}	C04B41/50	C04B41/50		461
C04B41/505	11	{Tin oxide}	C04B41/50	C04B41/50		102
C04B41/5051	11	{Niobium oxides or niobates}	C04B41/50	C04B41/50		50
C04B41/5053	10	{non-oxide ceramics (carbon or carbonisable materials C04B41/5001)}	C04B41/50	C04B41/50		388
C04B41/5054	11	{Sulfides or selenides}	C04B41/50	C04B41/50		49
C04B41/5055	11	{Fluorides}	C04B41/50	C04B41/50		47
C04B41/5057	11	{Carbides}	C04B41/50	C04B41/50		722
C04B41/5058	12	{Boron carbide}	C04B41/50	C04B41/50		133
C04B41/5059	12	{Silicon carbide}	C04B41/50	C04B41/50		1803
C04B41/5061	12	{Titanium carbide}	C04B41/50	C04B41/50		147
C04B41/5062	11	{Borides, Nitrides or Silicides}	C04B41/50	C04B41/50		362
C04B41/5063	12	{Aluminium nitride}	C04B41/50	C04B41/50		208
C04B41/5064	12	{Boron nitride}	C04B41/50	C04B41/50		336
C04B41/5066	12	{Silicon nitride}	C04B41/50	C04B41/50		487
C04B41/5067	12	{Silicon oxynitrides, e.g. SIALON}	C04B41/50	C04B41/50		58
C04B41/5068	12	{Titanium nitride}	C04B41/50	C04B41/50		250
C04B41/507	12	{Borides}	C04B41/50	C04B41/50		348
C04B41/5071	12	{Silicides}	C04B41/50	C04B41/50		344
C04B41/5072	10	{with oxides or hydroxides not covered by C04B41/5025(C04B40/0236 takes precedence; boron oxide C04B41/5006)}	C04B41/50	C04B41/50		482
C04B41/5074	11	{Copper oxide or solid solutions thereof (CuO-Cu eutectic C04B41/5127)}	C04B41/50	C04B41/50		83
C04B41/5075	12	{Copper oxide}	C04B41/50	C04B41/50		57
C04B41/5076	10	{with masses bonded by inorganic cements (sulfur compositions C04B41/5097)}	C04B41/50	C04B41/50		1051
C04B41/5077	11	{Geopolymer cements}	C04B41/50	C04B41/50		37
C04B41/5079	11	{Portland cements}	C04B41/50	C04B41/50		395
C04B41/508	11	{Aluminous cements}	C04B41/50	C04B41/50		145
C04B41/5081	12	{Calcium alumino sulfate cements}	C04B41/50	C04B41/50		34
C04B41/5083	11	{Slag cements}	C04B41/50	C04B41/50		28
C04B41/5084	11	{Lime, hydraulic lime or magnesium oxide cements}	C04B41/50	C04B41/50		92
C04B41/5085	11	{Calcium sulfate cements}	C04B41/50	C04B41/50		133
C04B41/5087	12	{Anhydrite}	C04B41/50	C04B41/50		20
C04B41/5088	11	{Cementitious compositions of the silica-lime type}	C04B41/50	C04B41/50		14
C04B41/5089	11	{Silica sols, alkyl, ammonium or alkali metal silicate cements}	C04B41/50	C04B41/50		1223
C04B41/509	11	{Magnesium cements, e.g. Sorel cement}	C04B41/50	C04B41/50		58
C04B41/5092	11	{Phosphate cements}	C04B41/50	C04B41/50		382
C04B41/5093	10	{with elements other than metals or carbon (treatment with fluorine gas C04B41/5019)}	C04B41/50	C04B41/50		40
C04B41/5094	11	{Boron}	C04B41/50	C04B41/50		56
C04B41/5096	11	{Silicon (C04B35/573 takes precedence)}	C04B41/50	C04B41/50		891
C04B41/5097	11	{Sulfur}	C04B41/50	C04B41/50		38
C04B41/5098	10	{Cermets}	C04B41/50	C04B41/50		80
C04B41/51	10	Metallising {, e.g. infiltration of sintered ceramic preforms with molten metal (covering materials with metals in general C23C; ceramic compositions containing free metal bonded to carbides, diamond, oxides, borides, nitrides, silicides, e.g. cermets, or other metal compounds, e.g. oxynitrides or sulfides, other than as macroscopic reinforcing agents C22C; infiltration of preforms containing free metal, e.g. cermets C22C)}	C04B41/51	C04B41/51		1374
C04B41/5105	11	{with a composition mainly composed of one or more of the noble metals or copper}	C04B41/51	C04B41/51		193
C04B41/5111	11	{Ag, Au, Pd, Pt or Cu}	C04B41/51	C04B41/51		186
C04B41/5116	11	{Ag or Au}	C04B41/51	C04B41/51		1766
C04B41/5122	11	{Pd or Pt}	C04B41/51	C04B41/51		344
C04B41/5127	11	{Cu, e.g. Cu-CuO eutectic}	C04B41/51	C04B41/51		710
C04B41/5133	11	{with a composition mainly composed of one or more of the refractory metals}	C04B41/51	C04B41/51		917
C04B41/5138	11	{with a composition mainly composed of Mn and Mo, e.g. for the Moly-manganese method}	C04B41/51	C04B41/51		214
C04B41/5144	11	{with a composition mainly composed of one or more of the metals of the iron group}	C04B41/51	C04B41/51		734
C04B41/515	11	{Other specific metals}	C04B41/51	C04B41/51		254
C04B41/5155	12	{Aluminium}	C04B41/51	C04B41/51		612
C04B41/5161	12	{Tin}	C04B41/51	C04B41/51		80
C04B41/5166	12	{Lead}	C04B41/51	C04B41/51		15
C04B41/5172	12	{Cadmium}	C04B41/51	C04B41/51		3
C04B41/5177	11	{characterised by the non-metallic part of the metallising composition}	C04B41/51	C04B41/51		26
C04B41/5183	11	{inorganic}	C04B41/51	C04B41/51		107
C04B41/5188	11	{organic}	C04B41/51	C04B41/51		56
C04B41/5194	11	{Metallisation of multilayered ceramics, e.g. for the fabrication of multilayer ceramic capacitors}	C04B41/51	C04B41/51		82
C04B41/52	9	Multiple coating or impregnating {multiple coating or impregnating with the same composition or with compositions only differing in the concentration of the constituents, is classified as single coating or impregnation}<br><br><u>NOTE</u><br><br> Multiple coating or impregnation with the same composition or with compositions only differing in the concentration of the constituents, is classified as single coating or impregnation and symbol C04B41/52 is allocated in Combination Sets <br> Groups C04B41/522 and C04B41/524 are used for Combination Sets only of documents classified in C04B41/52	C04B41/52	C04B41/52		9578
C04B41/522	10	{Multiple coatings, for one of the coatings of which at least one alternative is described}	C04B41/52	C04B41/52		1383
C04B41/524	10	{Multiple coatings, comprising a coating layer of the same material as a previous coating layer}	C04B41/52	C04B41/52		351
C04B41/526	10	{Multiple coating or impregnation with materials having the same composition but different characteristics}	C04B41/52	C04B41/52		212
C04B41/528	10	{Applying layers containing opposite charged particles or materials in the successive layers}	C04B41/52	C04B41/52		23
C04B41/53	8	involving the removal of at least part of the materials of the treated article, {e.g. etching, drying of hardened concrete (C04B41/0036&#160;-&#160;C04B41/0054 take precedence)}	C04B41/53	C04B41/53		1542
C04B41/5307	9	{Removal of physically bonded water, e.g. drying of hardened concrete (E04B1/7007 takes precedence)}	C04B41/53	C04B41/53		31
C04B41/5315	9	{Cleaning compositions, e.g. for removing hardened cement from ceramic tiles}	C04B41/53	C04B41/53		281
C04B41/5323	9	{to make grain visible, e.g. for obtaining exposed aggregate concrete}	C04B41/53	C04B41/53		239
C04B41/533	10	{Seeding methods, i.e. the exposed aggregates, at least partially, not making part of the starting mixture}	C04B41/53	C04B41/53		7
C04B41/5338	9	{Etching (for obtaining decorative effects B44C1/22; etching of specific electronic compounds, see the relevant places, e.g. etching of semiconductor bodies H10P50/00)}	C04B41/53	C04B41/53		113
C04B41/5346	10	{Dry etching}	C04B41/53	C04B41/53		237
C04B41/5353	10	{Wet etching, e.g. with etchants dissolved in organic solvents}	C04B41/53	C04B41/53		550
C04B41/5361	10	{Etching with molten material}	C04B41/53	C04B41/53		44
C04B41/5369	9	{Desalination, e.g. of reinforced concrete}	C04B41/53	C04B41/53		27
C04B41/5376	10	{Electrochemical desalination (electrochemical re-alkalisation C04B41/4566; drying by electro-osmosis E04B1/7007)}	C04B41/53	C04B41/53		66
C04B41/5384	9	{by electrochemical methods (electrochemical desalination C04B41/5376)}	C04B41/53	C04B41/53		17
C04B41/5392	9	{by burning (C04B38/06 takes precedence)}	C04B41/53	C04B41/53		30
C04B41/60	8	of only artificial stone	C04B41/60	C04B41/60		71
C04B41/61	9	Coating or impregnation	C04B41/61	C04B41/61		481
C04B41/62	10	with organic materials	C04B41/62	C04B41/62		321
C04B41/63	11	Macromolecular compounds	C04B41/63	C04B41/63		1060
C04B41/64	11	Compounds having one or more carbon-to-metal of carbon-to-silicon linkages	C04B41/64	C04B41/64		503
C04B41/65	10	with inorganic materials	C04B41/65	C04B41/65		1035
C04B41/66	11	Fluorides, e.g. ocratation	C04B41/66	C04B41/66		42
C04B41/67	11	Phosphates	C04B41/67	C04B41/67		67
C04B41/68	11	Silicic acid; Silicates	C04B41/68	C04B41/68		441
C04B41/69	11	Metals	C04B41/69	C04B41/69		87
C04B41/70	10	for obtaining at least two superposed coatings having different compositions	C04B41/70	C04B41/70		582
C04B41/71	11	at least one coating being an organic material	C04B41/71	C04B41/71		375
C04B41/72	9	involving the removal of part of the materials of the treated articles, e.g. etching	C04B41/72	C04B41/72		274
C04B41/80	8	of only ceramics	C04B41/80	C04B41/80		758
C04B41/81	9	Coating or impregnation	C04B41/81	C04B41/81		1337
C04B41/82	10	with organic materials	C04B41/82	C04B41/82		342
C04B41/83	11	Macromolecular compounds	C04B41/83	C04B41/83		823
C04B41/84	11	Compounds having one or more carbon-to-metal of carbon-to-silicon linkages	C04B41/84	C04B41/84		333
C04B41/85	10	with inorganic materials	C04B41/85	C04B41/85		2666
C04B41/86	11	Glazes; Cold glazes	C04B41/86	C04B41/86		4734
C04B41/87	11	Ceramics	C04B41/87	C04B41/87		4555
C04B41/88	11	Metals	C04B41/88	C04B41/88		3305
C04B41/89	10	for obtaining at least two superposed coatings having different compositions	C04B41/89	C04B41/89		5715
C04B41/90	11	at least one coating being a metal	C04B41/90	C04B41/90		657
C04B41/91	9	involving the removal of part of the materials of the treated articles, e.g. etching	C04B41/91	C04B41/91		1078
C04B2103/00	7	Function or property of ingredients for mortars, concrete or artificial stone	C04B103/00	C04B103/00		69
C04B2103/0001	8	{Living organisms, e.g. microorganisms, or enzymes}	C04B103/00	C04B103/00		1057
C04B2103/0002	9	{Seeds}	C04B103/00	C04B103/00		79
C04B2103/0003	8	{Unintentionally added compounds, such as impurities in raw materials, e.g. alkali sulfates in construction grade cement}	C04B103/00	C04B103/00		6
C04B2103/0004	8	{Compounds chosen for the nature of their cations}	C04B103/00	C04B103/00		130
C04B2103/0005	9	{Organic ammonium compounds}	C04B103/00	C04B103/00		109
C04B2103/0006	9	{Alkali metal or inorganic ammonium compounds}	C04B103/00	C04B103/00		250
C04B2103/0007	10	{K}	C04B103/00	C04B103/00		99
C04B2103/0008	10	{Li}	C04B103/00	C04B103/00		261
C04B2103/0009	10	{Inorganic ammonium compounds}	C04B103/00	C04B103/00		42
C04B2103/001	9	{Alkaline earth metal or Mg-compounds}	C04B103/00	C04B103/00		295
C04B2103/0011	10	{Ba}	C04B103/00	C04B103/00		61
C04B2103/0012	10	{Mg}	C04B103/00	C04B103/00		117
C04B2103/0013	9	{Iron group metal compounds}	C04B103/00	C04B103/00		67
C04B2103/0014	10	{Fe}	C04B103/00	C04B103/00		158
C04B2103/0015	9	{Noble metal or copper compounds}	C04B103/00	C04B103/00		108
C04B2103/0016	10	{Cu}	C04B103/00	C04B103/00		89
C04B2103/0017	9	{Refractory metal compounds}	C04B103/00	C04B103/00		68
C04B2103/0018	10	{Cr}	C04B103/00	C04B103/00		42
C04B2103/0019	10	{Ti}	C04B103/00	C04B103/00		51
C04B2103/002	9	{Compounds of elements having a valency of 2}	C04B103/00	C04B103/00		77
C04B2103/0021	9	{Compounds of elements having a valency of 3}	C04B103/00	C04B103/00		376
C04B2103/0022	9	{Compounds of elements having a valency of 4}	C04B103/00	C04B103/00		33
C04B2103/0023	9	{Compounds of elements having a valency of 5}	C04B103/00	C04B103/00		4
C04B2103/0024	9	{Compounds of elements having a valency of 6}	C04B103/00	C04B103/00		8
C04B2103/0025	9	{Compounds of the transition metals}	C04B103/00	C04B103/00		103
C04B2103/0026	8	{Compounds of unusual isotopes, e.g. heavy water}	C04B103/00	C04B103/00		2
C04B2103/0027	8	{Standardised cement types}	C04B103/00	C04B103/00		31
C04B2103/0028	9	{according to API}	C04B103/00	C04B103/00		29
C04B2103/0029	10	{Type A}	C04B103/00	C04B103/00		9
C04B2103/003	10	{Type B}	C04B103/00	C04B103/00		
C04B2103/0031	10	{Type C}	C04B103/00	C04B103/00		7
C04B2103/0032	10	{Type D}	C04B103/00	C04B103/00		2
C04B2103/0033	10	{Type E}	C04B103/00	C04B103/00		
C04B2103/0034	10	{Type F}	C04B103/00	C04B103/00		1
C04B2103/0035	10	{Type G}	C04B103/00	C04B103/00		73
C04B2103/0036	10	{Type H}	C04B103/00	C04B103/00		32
C04B2103/0037	10	{Type J}	C04B103/00	C04B103/00		
C04B2103/0038	10	{Type K}	C04B103/00	C04B103/00		1
C04B2103/0039	9	{according to ASTM}	C04B103/00	C04B103/00		10
C04B2103/004	9	{according to DIN}	C04B103/00	C04B103/00		46
C04B2103/0041	8	{Non-polymeric ingredients chosen for their physico-chemical characteristics}	C04B103/00	C04B103/00		18
C04B2103/0042	9	{Amorphous materials}	C04B103/00	C04B103/00		20
C04B2103/0043	9	{Compounds chosen for their specific Moh&apos;s hardness}	C04B103/00	C04B103/00		39
C04B2103/0044	9	{Compounds chosen for their abrasion resistance, e.g. determined according to the L.A. test}	C04B103/00	C04B103/00		17
C04B2103/0045	8	{Polymers chosen for their physico-chemical characteristics}	C04B103/00	C04B103/00		602
C04B2103/0046	9	{added as monomers or as oligomers}	C04B103/00	C04B103/00		199
C04B2103/0047	10	{as a mixture of nonomers and prepolymers or oligomers}	C04B103/00	C04B103/00		41
C04B2103/0048	10	{as oligomers}	C04B103/00	C04B103/00		13
C04B2103/0049	9	{Water-swellable polymers}	C04B103/00	C04B103/00		112
C04B2103/005	10	{Alkali-swellable polymers}	C04B103/00	C04B103/00		18
C04B2103/0051	9	{Water-absorbing polymers, hydrophilic polymers}	C04B103/00	C04B103/00		558
C04B2103/0052	9	{Hydrophobic polymers}	C04B103/00	C04B103/00		110
C04B2103/0053	9	{Water-soluble polymers}	C04B103/00	C04B103/00		366
C04B2103/0054	9	{Water dispersible polymers}	C04B103/00	C04B103/00		150
C04B2103/0055	9	{Water-insoluble polymers}	C04B103/00	C04B103/00		28
C04B2103/0056	9	{Thermohardening polymers}	C04B103/00	C04B103/00		22
C04B2103/0057	9	{added as redispersable powders}	C04B103/00	C04B103/00		2719
C04B2103/0058	9	{Core-shell polymers}	C04B103/00	C04B103/00		65
C04B2103/0059	9	{Graft (co-)polymers}	C04B103/00	C04B103/00		172
C04B2103/006	10	{Comb polymers}	C04B103/00	C04B103/00		123
C04B2103/0061	9	{Block (co-)polymers}	C04B103/00	C04B103/00		83
C04B2103/0062	9	{Cross-linked polymers}	C04B103/00	C04B103/00		195
C04B2103/0063	9	{obtained by an unusual polymerisation process, e.g. by changing the molar ratio of the different monomers during the polymerisation process (C04B2103/0058&#160;-&#160;C04B2103/0061 take precedence)}	C04B103/00	C04B103/00		20
C04B2103/0064	9	{Polymers unstable in the presence of hydraulic binders, e.g. polymers flocculating in concrete mixtures}	C04B103/00	C04B103/00		11
C04B2103/0065	9	{Polymers characterised by their glass transition temperature (Tg)}	C04B103/00	C04B103/00		184
C04B2103/0066	9	{Film forming polymers}	C04B103/00	C04B103/00		63
C04B2103/0067	8	{the ingredients being formed in situ by chemical reactions or conversion of one or more of the compounds of the composition}	C04B103/00	C04B103/00		156
C04B2103/0068	8	{Ingredients with a function or property not provided for elsewhere in C04B2103/00}	C04B103/00	C04B103/00		8957
C04B2103/0069	9	{the ingredients being characterised by their physical state}	C04B103/00	C04B103/00		50
C04B2103/007	10	{Supercritical fluids}	C04B103/00	C04B103/00		12
C04B2103/0071	9	{Phase-change materials, e.g. latent heat storage materials used in concrete compositions}	C04B103/00	C04B103/00		558
C04B2103/0072	9	{Biodegradable materials}	C04B103/00	C04B103/00		67
C04B2103/0073	9	{Self-degrading materials, e.g. materials undergoing a hydrolytic degradation in the course of time}	C04B103/00	C04B103/00		13
C04B2103/0074	9	{Anti-static agents}	C04B103/00	C04B103/00		68
C04B2103/0075	9	{Anti-dusting agents}	C04B103/00	C04B103/00		181
C04B2103/0076	9	{Deodorizing agents}	C04B103/00	C04B103/00		148
C04B2103/0077	9	{Packaging material remaining in the mixture after the mixing step, e.g. soluble bags containing active ingredients}	C04B103/00	C04B103/00		68
C04B2103/0078	9	{Sorbent materials}	C04B103/00	C04B103/00		137
C04B2103/0079	9	{Rheology influencing agents}	C04B103/00	C04B103/00		376
C04B2103/008	9	{Flocking or deflocking agents}	C04B103/00	C04B103/00		180
C04B2103/0081	10	{Deflocking agents}	C04B103/00	C04B103/00		50
C04B2103/0082	9	{Segregation-preventing agents; Sedimentation-preventing agents}	C04B103/00	C04B103/00		290
C04B2103/0083	10	{Bleeding-preventing agents}	C04B103/00	C04B103/00		57
C04B2103/0084	9	{Polyelectrolytes}	C04B103/00	C04B103/00		13
C04B2103/0085	9	{Thixotropic agents}	C04B103/00	C04B103/00		335
C04B2103/0086	9	{Chelating or complexing agents}	C04B103/00	C04B103/00		236
C04B2103/0087	9	{Ion-exchanging agents}	C04B103/00	C04B103/00		49
C04B2103/0088	9	{Compounds chosen for their latent hydraulic characteristics, e.g. pozzuolanes}<br><br><u>NOTE</u><br><br>Code C04B2103/0088 is only used when the chemical nature of the latent hydraulic material is not specified, when no specific group in subclass C04B exists for defining the material or when it is chosen from an important number of alternatives.	C04B103/00	C04B103/00		987
C04B2103/0089	9	{Agents for reducing heat of hydration}	C04B103/00	C04B103/00		59
C04B2103/009	9	{Anhydrous vehicles for hydraulic cement compositions}	C04B103/00	C04B103/00		7
C04B2103/0091	9	{Organic co-binders for mineral binder compositions}	C04B103/00	C04B103/00		163
C04B2103/0092	10	{for improving green strength}	C04B103/00	C04B103/00		71
C04B2103/0093	9	{Organic cosolvents}	C04B103/00	C04B103/00		225
C04B2103/0094	9	{Agents for altering or buffering the pH; Ingredients characterised by their pH}	C04B103/00	C04B103/00		520
C04B2103/0095	9	{Oxidising agents}	C04B103/00	C04B103/00		64
C04B2103/0096	9	{Reducing agents}	C04B103/00	C04B103/00		118
C04B2103/0097	9	{Anion- and far-infrared-emitting materials}	C04B103/00	C04B103/00		1082
C04B2103/0098	9	{Radioactive materials}	C04B103/00	C04B103/00		18
C04B2103/0099	8	{Aspecific ingredients, i.e. high number of alternative specific compounds mentioned for the same function or property}	C04B103/00	C04B103/00		40
C04B2103/10	8	Accelerators; Activators	C04B103/10	C04B103/10		2598
C04B2103/105	9	{for reactions involving organo-silicon compounds}	C04B103/10	C04B103/10		33
C04B2103/12	9	Set accelerators	C04B103/12	C04B103/12		3665
C04B2103/14	9	Hardening accelerators	C04B103/14	C04B103/14		1110
C04B2103/20	8	Retarders	C04B103/20	C04B103/20		1304
C04B2103/22	9	Set retarders	C04B103/22	C04B103/22		4490
C04B2103/24	9	Hardening retarders	C04B103/24	C04B103/24		178
C04B2103/30	8	Water reducers, plasticisers, air-entrainers, flow improvers	C04B103/30	C04B103/30		1868
C04B2103/302	9	{Water reducers}	C04B103/30	C04B103/30		24937
C04B2103/304	9	{Air-entrainers}	C04B103/30	C04B103/30		2784
C04B2103/306	9	{Fluidisers with reduced air-entraning effect}	C04B103/30	C04B103/30		40
C04B2103/308	9	{Slump-loss preventing agents}	C04B103/30	C04B103/30		413
C04B2103/32	9	Superplasticisers	C04B103/32	C04B103/32		1825
C04B2103/34	9	{Flow improvers}	C04B103/30	C04B103/34		717
C04B2103/40	8	Surface-active agents, dispersants	C04B103/40	C04B103/40		2602
C04B2103/402	9	{anionic}	C04B103/40	C04B103/40		366
C04B2103/404	9	{cationic}	C04B103/40	C04B103/40		169
C04B2103/406	9	{non-ionic}	C04B103/40	C04B103/40		441
C04B2103/408	9	{Dispersants}	C04B103/40	C04B103/40		4157
C04B2103/42	8	Pore formers	C04B103/42	C04B103/42		1127
C04B2103/44	8	Thickening, gelling or viscosity increasing agents	C04B103/44	C04B103/44		3936
C04B2103/445	9	{Gelling agents}	C04B103/44	C04B103/44		214
C04B2103/46	8	Water-loss or fluid-loss reducers, hygroscopic or hydrophilic agents, water retention agents	C04B103/46	C04B103/46		1273
C04B2103/465	9	{Water-sorbing agents, hygroscopic or hydrophilic agents}	C04B103/46	C04B103/46		1057
C04B2103/48	8	Foam stabilisers	C04B103/48	C04B103/48		984
C04B2103/50	8	Defoamers, air detrainers	C04B103/50	C04B103/50		6085
C04B2103/52	8	Grinding aids; Additives added during grinding	C04B103/52	C04B103/52		1047
C04B2103/54	8	Pigments; Dyes	C04B103/54	C04B103/54		5709
C04B2103/56	8	Opacifiers	C04B103/56	C04B103/56		131
C04B2103/58	9	{Shrinkage reducing agents}	C04B103/56	C04B103/58		504
C04B2103/60	8	Agents for protection against chemical, physical or biological attack	C04B103/60	C04B103/60		623
C04B2103/601	9	{Agents for increasing frost resistance}	C04B103/60	C04B103/60		879
C04B2103/603	9	{Agents for controlling alkali-aggregate reactions}	C04B103/60	C04B103/60		148
C04B2103/605	9	{UV-stabilising agents}	C04B103/60	C04B103/60		231
C04B2103/606	9	{Agents for neutralising Ca(OH)2 liberated during cement hardening}	C04B103/60	C04B103/60		78
C04B2103/608	9	{Anti-oxidants}	C04B103/60	C04B103/60		571
C04B2103/61	9	Corrosion inhibitors	C04B103/61	C04B103/61		1239
C04B2103/63	9	Flame-proofing agents	C04B103/63	C04B103/63		1065
C04B2103/65	9	Water proofers or repellants	C04B103/65	C04B103/65		3893
C04B2103/67	9	Biocides	C04B103/67	C04B103/67		1803
C04B2103/69	10	Fungicides	C04B103/69	C04B103/69		545
C04B2111/00	7	Mortars, concrete or artificial stone or mixtures to prepare them, characterised by specific function, property or use	C04B111/00	C04B111/00		41
C04B2111/00008	8	{Obtaining or using nanotechnology related materials}	C04B111/00	C04B111/00		1249
C04B2111/00017	8	{Aspects relating to the protection of the environment}	C04B111/00	C04B111/00		8577
C04B2111/00019	9	{Carbon dioxide sequestration}	C04B111/00	C04B111/00		293
C04B2111/00025	8	{Aspects relating to the protection of the health, e.g. materials containing special additives to afford skin protection}	C04B111/00	C04B111/00		1275
C04B2111/00034	8	{Physico-chemical characteristics of the mixtures}	C04B111/00	C04B111/00		8
C04B2111/00043	9	{Anhydrous mixtures}<br><br><u>NOTE</u><br><br>Code C04B2111/00043 is only used in combination with groups C04B26/00&#160;-&#160;C04B26/32.	C04B111/00	C04B111/00		27
C04B2111/00051	9	{Mortar or concrete mixtures with an unusual low cement content, e.g. for foundations}	C04B111/00	C04B111/00		41
C04B2111/0006	10	{for obtaining materials with the consistency of soil}	C04B111/00	C04B111/00		15
C04B2111/00068	9	{Mortar or concrete mixtures with an unusual water/cement ratio}	C04B111/00	C04B111/00		380
C04B2111/00077	9	{Partially hardened mortar or concrete mixtures}	C04B111/00	C04B111/00		8
C04B2111/00086	9	{Mixtures with prolonged pot-life}	C04B111/00	C04B111/00		171
C04B2111/00094	9	{Sag-resistant materials}	C04B111/00	C04B111/00		66
C04B2111/00103	9	{Self-compacting mixtures}	C04B111/00	C04B111/00		200
C04B2111/00112	9	{Mixtures characterised by specific pH values}	C04B111/00	C04B111/00		244
C04B2111/0012	9	{Thixotropic mixtures}	C04B111/00	C04B111/00		76
C04B2111/00129	9	{Extrudable mixtures}	C04B111/00	C04B111/00		712
C04B2111/00137	9	{Injection moldable mixtures}	C04B111/00	C04B111/00		68
C04B2111/00146	9	{Sprayable or pumpable mixtures}	C04B111/00	C04B111/00		1080
C04B2111/00155	10	{Sprayable, i.e. concrete-like, materials able to be shaped by spraying instead of by casting, e.g. gunite}	C04B111/00	C04B111/00		1326
C04B2111/00163	11	{by the dry process}	C04B111/00	C04B111/00		33
C04B2111/00172	11	{by the wet process}	C04B111/00	C04B111/00		103
C04B2111/00181	9	{Mixtures specially adapted for three-dimensional printing (3DP), stereo-lithography or prototyping}	C04B111/00	C04B111/00		994
C04B2111/00189	9	{Compositions or ingredients of the compositions characterised by analysis-spectra, e.g. NMR}	C04B111/00	C04B111/00		59
C04B2111/00198	9	{Characterisation or quantities of the compositions or their ingredients expressed as mathematical formulae or equations}	C04B111/00	C04B111/00		318
C04B2111/00206	9	{Compositions defined by their elemental analysis}	C04B111/00	C04B111/00		38
C04B2111/00215	9	{Mortar or concrete mixtures defined by their oxide composition}	C04B111/00	C04B111/00		396
C04B2111/00224	9	{Green materials, e.g. porous green ceramic preforms}	C04B111/00	C04B111/00		126
C04B2111/00232	9	{Temporary foams}	C04B111/00	C04B111/00		8
C04B2111/00241	8	{Physical properties of the materials not provided for elsewhere in C04B2111/00}	C04B111/00	C04B111/00		163
C04B2111/0025	9	{Compositions or ingredients of the compositions characterised by the crystal structure}	C04B111/00	C04B111/00		99
C04B2111/00258	9	{Electromagnetic wave absorbing or shielding materials}	C04B111/00	C04B111/00		635
C04B2111/00267	9	{Materials permeable to vapours or gases}	C04B111/00	C04B111/00		282
C04B2111/00275	9	{Materials impermeable to vapours or gases}	C04B111/00	C04B111/00		106
C04B2111/00284	9	{Materials permeable to liquids}	C04B111/00	C04B111/00		2625
C04B2111/00293	9	{Materials impermeable to liquids}	C04B111/00	C04B111/00		1322
C04B2111/00301	9	{Non-porous materials, e.g. macro-defect free [MDF] products}	C04B111/00	C04B111/00		58
C04B2111/0031	9	{Heavy materials, e.g. concrete used as ballast material}	C04B111/00	C04B111/00		105
C04B2111/00318	9	{Materials characterised by relatively small dimensions, e.g. small thickness}	C04B111/00	C04B111/00		72
C04B2111/00327	10	{for obtaining microstructures}	C04B111/00	C04B111/00		9
C04B2111/00336	9	{Materials with a smooth surface, e.g. obtained by using glass-surfaced moulds}	C04B111/00	C04B111/00		160
C04B2111/00344	9	{Materials with friction-reduced moving parts, e.g. ceramics lubricated by impregnation with carbon}	C04B111/00	C04B111/00		24
C04B2111/00353	10	{Sliding parts}	C04B111/00	C04B111/00		71
C04B2111/00362	9	{Friction materials, e.g. used as brake linings, anti-skid materials}	C04B111/00	C04B111/00		569
C04B2111/0037	9	{Materials containing oriented fillers or elements}	C04B111/00	C04B111/00		45
C04B2111/00379	10	{the oriented elements being fibres}	C04B111/00	C04B111/00		176
C04B2111/00387	9	{Anisotropic materials}	C04B111/00	C04B111/00		17
C04B2111/00396	10	{only the surface part being anisotropic}	C04B111/00	C04B111/00		4
C04B2111/00405	9	{Materials with a gradually increasing or decreasing concentration of ingredients or property from one layer to another}	C04B111/00	C04B111/00		373
C04B2111/00413	9	{Materials having an inhomogeneous concentration of ingredients or irregular properties in different layers}	C04B111/00	C04B111/00		220
C04B2111/00422	9	{Magnetic properties}	C04B111/00	C04B111/00		140
C04B2111/00431	8	{Refractory materials}	C04B111/00	C04B111/00		332
C04B2111/00439	8	{Physico-chemical properties of the materials not provided for elsewhere in C04B2111/00}	C04B111/00	C04B111/00		104
C04B2111/00448	9	{Low heat cements}	C04B111/00	C04B111/00		104
C04B2111/00456	9	{Odorless cements}	C04B111/00	C04B111/00		28
C04B2111/00465	9	{Heat conducting materials}	C04B111/00	C04B111/00		156
C04B2111/00474	8	{Uses not provided for elsewhere in C04B2111/00}	C04B111/00	C04B111/00		87
C04B2111/00482	9	{Coating or impregnation materials}	C04B111/00	C04B111/00		5810
C04B2111/00491	10	{Primers}	C04B111/00	C04B111/00		205
C04B2111/005	10	{for frescos}	C04B111/00	C04B111/00		8
C04B2111/00508	10	{Cement paints}	C04B111/00	C04B111/00		793
C04B2111/00517	10	{for masonry}	C04B111/00	C04B111/00		375
C04B2111/00525	10	{for metallic surfaces}	C04B111/00	C04B111/00		519
C04B2111/00534	10	{for plastic surfaces, e.g. polyurethane foams}	C04B111/00	C04B111/00		72
C04B2111/00543	10	{for wet surfaces}	C04B111/00	C04B111/00		36
C04B2111/00551	10	{Refractory coatings, e.g. for tamping}	C04B111/00	C04B111/00		347
C04B2111/0056	10	{for ship decks}	C04B111/00	C04B111/00		28
C04B2111/00568	10	{Multiple coating with same or similar material}	C04B111/00	C04B111/00		42
C04B2111/00577	10	{applied by spraying}	C04B111/00	C04B111/00		411
C04B2111/00586	9	{Roofing materials}	C04B111/00	C04B111/00		502
C04B2111/00594	10	{Concrete roof tiles}	C04B111/00	C04B111/00		134
C04B2111/00603	9	{Ceiling materials}	C04B111/00	C04B111/00		113
C04B2111/00612	9	{as one or more layers of a layered structure}	C04B111/00	C04B111/00		3736
C04B2111/0062	10	{Gypsum-paper board like materials}	C04B111/00	C04B111/00		1042
C04B2111/00629	11	{the covering sheets being made of material other than paper}	C04B111/00	C04B111/00		136
C04B2111/00637	9	{as glue or binder for uniting building or structural materials}	C04B111/00	C04B111/00		1185
C04B2111/00646	10	{Masonry mortars}	C04B111/00	C04B111/00		302
C04B2111/00655	9	{Profiles}	C04B111/00	C04B111/00		24
C04B2111/00663	9	{as filling material for cavities or the like}	C04B111/00	C04B111/00		956
C04B2111/00672	10	{Pointing or jointing materials}	C04B111/00	C04B111/00		937
C04B2111/00681	11	{of the drying type}	C04B111/00	C04B111/00		72
C04B2111/00689	11	{of the setting type}	C04B111/00	C04B111/00		56
C04B2111/00698	10	{for cavity walls}	C04B111/00	C04B111/00		58
C04B2111/00706	10	{around pipelines or the like}	C04B111/00	C04B111/00		259
C04B2111/00715	9	{for fixing bolts or the like}	C04B111/00	C04B111/00		255
C04B2111/00724	9	{in mining operations, e.g. for backfilling; in making tunnels or galleries}	C04B111/00	C04B111/00		2736
C04B2111/00732	9	{for soil stabilisation}	C04B111/00	C04B111/00		1595
C04B2111/00741	10	{Preventing erosion}	C04B111/00	C04B111/00		38
C04B2111/0075	9	{for road construction}	C04B111/00	C04B111/00		7558
C04B2111/00758	9	{for agri-, sylvi- or piscicultural or cattle-breeding applications}	C04B111/00	C04B111/00		722
C04B2111/00767	9	{for waste stabilisation purposes}	C04B111/00	C04B111/00		744
C04B2111/00775	10	{the composition being used as waste barriers or the like, e.g. compositions used for waste disposal purposes only, but not containing the waste itself}	C04B111/00	C04B111/00		380
C04B2111/00784	10	{for disposal only}	C04B111/00	C04B111/00		349
C04B2111/00793	9	{as filters or diaphragms}	C04B111/00	C04B111/00		2218
C04B2111/00801	10	{Membranes; Diaphragms}	C04B111/00	C04B111/00		337
C04B2111/0081	9	{as catalysts or catalyst carriers}	C04B111/00	C04B111/00		1549
C04B2111/00818	10	{Enzyme carriers}	C04B111/00	C04B111/00		21
C04B2111/00827	10	{Photocatalysts}	C04B111/00	C04B111/00		306
C04B2111/00836	9	{for medical or dental applications}	C04B111/00	C04B111/00		952
C04B2111/00844	9	{for electronic applications}	C04B111/00	C04B111/00		1195
C04B2111/00853	9	{in electrochemical cells or batteries, e.g. fuel cells}	C04B111/00	C04B111/00		456
C04B2111/00862	9	{for nuclear applications, e.g. ray-absorbing concrete}	C04B111/00	C04B111/00		394
C04B2111/0087	9	{for metallurgical applications}	C04B111/00	C04B111/00		441
C04B2111/00879	10	{Non-ferrous metallurgy}	C04B111/00	C04B111/00		145
C04B2111/00887	10	{Ferrous metallurgy}	C04B111/00	C04B111/00		187
C04B2111/00896	9	{as prepregs}	C04B111/00	C04B111/00		15
C04B2111/00905	9	{as preforms}	C04B111/00	C04B111/00		42
C04B2111/00913	10	{as ceramic preforms for the fabrication of metal matrix comp, e.g. cermets}	C04B111/00	C04B111/00		17
C04B2111/00922	11	{Preforms as such}	C04B111/00	C04B111/00		40
C04B2111/00931	11	{Coated or infiltrated preforms, e.g. with molten metal}	C04B111/00	C04B111/00		65
C04B2111/00939	9	{for the fabrication of moulds or cores}	C04B111/00	C04B111/00		409
C04B2111/00948	9	{for the fabrication of containers}	C04B111/00	C04B111/00		140
C04B2111/00956	9	{for making sculptures or artistic casts}	C04B111/00	C04B111/00		341
C04B2111/00965	9	{for household applications, e.g. use of materials as cooking ware}	C04B111/00	C04B111/00		240
C04B2111/00974	9	{for pyrotechnic applications, e.g. blasting}	C04B111/00	C04B111/00		59
C04B2111/00982	9	{as construction elements for space vehicles or aeroplanes}	C04B111/00	C04B111/00		318
C04B2111/00991	9	{for testing}	C04B111/00	C04B111/00		273
C04B2111/10	8	Compositions or ingredients thereof characterised by the absence or the very low content of a specific material	C04B111/10	C04B111/10		409
C04B2111/1006	9	{Absence of well-defined organic compounds}	C04B111/10	C04B111/10		129
C04B2111/1012	10	{Organic solvents}	C04B111/10	C04B111/10		23
C04B2111/1018	9	{Gypsum free or very low gypsum content cement compositions}	C04B111/10	C04B111/10		77
C04B2111/1025	9	{Alkali-free or very low alkali-content materials}	C04B111/10	C04B111/10		128
C04B2111/1031	9	{Lime-free or very low lime-content materials}	C04B111/10	C04B111/10		60
C04B2111/1037	9	{Cement free compositions, e.g. hydraulically hardening mixtures based on waste materials, not containing cement as such}	C04B111/10	C04B111/10		300
C04B2111/1043	10	{Calciumaluminate-free refractories}	C04B111/10	C04B111/10		9
C04B2111/105	9	{Alumina-free or very low alumina-content materials}	C04B111/10	C04B111/10		14
C04B2111/1056	9	{Silica-free or very low silica-content materials}	C04B111/10	C04B111/10		56
C04B2111/1062	9	{Halogen free or very low halogen-content materials}	C04B111/10	C04B111/10		74
C04B2111/1068	10	{Halogens other than chlorine}	C04B111/10	C04B111/10		8
C04B2111/1075	9	{Chromium-free or very low chromium-content materials}	C04B111/10	C04B111/10		72
C04B2111/1081	10	{Chromium VI, e.g. for avoiding chromium eczema}	C04B111/10	C04B111/10		151
C04B2111/1087	9	{Carbon free or very low carbon content fly ashes; Fly ashes treated to reduce their carbon content or the effect thereof}	C04B111/10	C04B111/10		42
C04B2111/1093	10	{Reducing the effect of the carbon content, without removing the carbon}	C04B111/10	C04B111/10		19
C04B2111/12	9	Absence of mineral fibres, e.g. asbestos	C04B111/12	C04B111/12		136
C04B2111/125	10	{Mineral fibres other than asbestos}	C04B111/12	C04B111/12		9
C04B2111/20	8	Resistance against chemical, physical or biological attack	C04B111/20	C04B111/20		5942
C04B2111/2007	9	{Avoiding unauthorised or unwanted use or treatment}	C04B111/20	C04B111/20		3
C04B2111/2015	9	{Sulfate resistance}	C04B111/20	C04B111/20		466
C04B2111/2023	9	{Resistance against alkali-aggregate reaction}	C04B111/20	C04B111/20		366
C04B2111/203	9	{Oil-proof or grease-repellant materials}	C04B111/20	C04B111/20		120
C04B2111/2038	9	{Resistance against physical degradation}	C04B111/20	C04B111/20		1212
C04B2111/2046	10	{Shock-absorbing materials}	C04B111/20	C04B111/20		228
C04B2111/2053	10	{Earthquake- or hurricane-resistant materials}	C04B111/20	C04B111/20		201
C04B2111/2061	10	{Materials containing photocatalysts, e.g. TiO2, for avoiding staining by air pollutants or the like}	C04B111/20	C04B111/20		367
C04B2111/2069	10	{Self-cleaning materials, e.g. using lotus effect}	C04B111/20	C04B111/20		124
C04B2111/2076	10	{Discolouring resistant materials}	C04B111/20	C04B111/20		68
C04B2111/2084	9	{Thermal shock resistance}	C04B111/20	C04B111/20		162
C04B2111/2092	9	{Resistance against biological degradation}	C04B111/20	C04B111/20		1081
C04B2111/21	9	Efflorescence resistance	C04B111/21	C04B111/21		325
C04B2111/22	9	Carbonation resistance	C04B111/22	C04B111/22		169
C04B2111/23	9	Acid resistance, e.g. against acid air or rain	C04B111/23	C04B111/23		628
C04B2111/24	9	Sea water resistance	C04B111/24	C04B111/24		652
C04B2111/25	9	Graffiti resistance; Graffiti removing	C04B111/25	C04B111/25		47
C04B2111/26	9	Corrosion of reinforcement resistance	C04B111/26	C04B111/26		663
C04B2111/265	10	{Cathodic protection of reinforced concrete structures}	C04B111/26	C04B111/26		56
C04B2111/27	9	Water resistance, i.e. waterproof or water-repellent materials	C04B111/27	C04B111/27		8151
C04B2111/275	10	{Making materials water insoluble}	C04B111/27	C04B111/27		32
C04B2111/28	9	Fire resistance, i.e. materials resistant to accidental fires or high temperatures	C04B111/28	C04B111/28		8016
C04B2111/285	10	{Intumescent materials}	C04B111/28	C04B111/28		304
C04B2111/29	9	{Frost-thaw resistance}	C04B111/20	C04B111/29		1198
C04B2111/30	8	Nailable or sawable materials	C04B111/30	C04B111/30		261
C04B2111/32	8	Expansion-inhibited materials	C04B111/32	C04B111/32		79
C04B2111/325	9	{the expansion being inhibited in one direction only}	C04B111/32	C04B111/32		8
C04B2111/34	8	Non-shrinking or non-cracking materials	C04B111/34	C04B111/34		917
C04B2111/343	9	{Crack resistant materials}	C04B111/34	C04B111/34		3918
C04B2111/346	9	{Materials exhibiting reduced plastic shrinkage cracking}	C04B111/34	C04B111/34		219
C04B2111/40	8	Porous or lightweight materials	C04B111/40	C04B111/40		7773
C04B2111/42	9	Floating materials	C04B111/42	C04B111/42		46
C04B2111/50	8	Flexible or elastic materials<br><br><u>NOTE</u><br><br><br>"flexibility" means ability to bend without breaking; <br>"elasticity" means property to resist and recover from  deformation produced by a force. 	C04B111/50	C04B111/50		250
C04B2111/503	9	{Elastic materials}	C04B111/50	C04B111/50		256
C04B2111/506	9	{Bendable material}	C04B111/50	C04B111/50		32
C04B2111/52	8	Sound-insulating materials	C04B111/52	C04B111/52		3401
C04B2111/54	8	Substitutes for natural stone, artistic materials or the like	C04B111/54	C04B111/54		563
C04B2111/542	9	{Artificial natural stone}	C04B111/54	C04B111/54		976
C04B2111/545	10	{Artificial marble}	C04B111/54	C04B111/54		687
C04B2111/547	9	{Imitating ancient compositions, e.g. mediaeval mortars; Compositions specially designed for restauration of ancient buildings or building elements}	C04B111/54	C04B111/54		110
C04B2111/56	8	Compositions suited for fabrication of pipes, e.g. by centrifugal casting, or for coating concrete pipes	C04B111/56	C04B111/56		398
C04B2111/60	8	Flooring materials	C04B111/60	C04B111/60		1640
C04B2111/62	9	Self-levelling compositions	C04B111/62	C04B111/62		808
C04B2111/70	8	Grouts, e.g. injection mixtures for cables for prestressed concrete	C04B111/70	C04B111/70		2886
C04B2111/72	8	Repairing or restoring existing buildings or building materials	C04B111/72	C04B111/72		3143
C04B2111/723	9	{Repairing reinforced concrete}	C04B111/72	C04B111/72		238
C04B2111/726	9	{by chemical conversion of unwanted deposits, e.g. for the restauration of marble monuments}	C04B111/72	C04B111/72		9
C04B2111/74	8	Underwater applications	C04B111/74	C04B111/74		743
C04B2111/76	8	Use at unusual temperatures, e.g. sub-zero	C04B111/76	C04B111/76		1174
C04B2111/763	9	{High temperatures}	C04B111/76	C04B111/76		234
C04B2111/766	9	{Low temperatures, but above zero}	C04B111/76	C04B111/76		53
C04B2111/80	8	Optical properties, e.g. transparency or reflexibility	C04B111/80	C04B111/80		664
C04B2111/802	9	{White cement}	C04B111/80	C04B111/80		343
C04B2111/805	9	{Transparent material}	C04B111/80	C04B111/80		158
C04B2111/807	9	{Luminescent or fluorescent materials}	C04B111/80	C04B111/80		321
C04B2111/82	9	Coloured materials	C04B111/82	C04B111/82		1426
C04B2111/90	8	Electrical properties	C04B111/90	C04B111/90		263
C04B2111/905	9	{Anti-static materials}	C04B111/90	C04B111/90		131
C04B2111/92	9	Electrically insulating materials	C04B111/92	C04B111/92		303
C04B2111/94	9	Electrically conducting materials	C04B111/94	C04B111/94		866
C04B2201/00	7	Mortars, concrete or artificial stone characterised by specific physical values<br><br><u>NOTE</u><br><br> Indexing codes C04B2201/05&#160;-&#160;C04B2201/30 are only to be used when the specific physical values are claimed or when they deviate considerably from the average usual values. 	CPCONLY	C04B2201/00		112
C04B2201/05	8	Materials having an early high strength, e.g. allowing fast demoulding or formless casting	CPCONLY	C04B2201/05		676
C04B2201/10	8	for the viscosity	CPCONLY	C04B2201/10		1335
C04B2201/20	8	for the density	CPCONLY	C04B2201/20		6539
C04B2201/30	8	for heat transfer properties such as thermal insulation values, e.g. R-values	CPCONLY	C04B2201/30		519
C04B2201/32	9	for the thermal conductivity, e.g. K-factors	CPCONLY	C04B2201/32		5471
C04B2201/40	8	for gas flow through the material	CPCONLY	C04B2201/40		27
C04B2201/50	8	for the mechanical strength	CPCONLY	C04B2201/50		28588
C04B2201/52	9	High compression strength concretes, i.e. with a compression strength higher than about 55 N/mm2, e.g. reactive powder concrete [RPC]	CPCONLY	C04B2201/52		2717
C04B2235/00	7	Aspects relating to ceramic starting mixtures or sintered ceramic products<br><br><u>NOTE</u><br><br>In this group, magnesium is considered as an alkaline earth metal.	CPCONLY	C04B2235/00		11
C04B2235/02	8	Composition of constituents of the starting material or of secondary phases of the final product<br><br><u>NOTE</u><br><br> Indexing codes C04B2235/02&#160;-&#160;C04B2235/5481 are to be used only if the aspect is not trivial or not standard, e.g. if water is used as a mixing medium for a powder, whereas normally an organic mixing medium is used or if not the standard alpha-alumina is used to make an alumina ceramic but gamma-alumina in stead. 	CPCONLY	C04B2235/02		35
C04B2235/30	9	Constituents and secondary phases not being of a fibrous nature<br><br><u>NOTE</u><br><br>Indexing codes C04B2235/30&#160;-&#160;C04B2235/549  are to be given to constituents or additives only if: <br>it is not obvious from the end product as such that the constituent or additive has been used for making the end product. <br> Examples: <br>in case spinel is made from a certain clay in stead of from alumina and silica, the clay is coded, <br>when calcium zirconate and titania are used to make calcium zirconium titanate, a code should be given for the calcium zirconate constituent while normally calcium oxide or calcium carbonate and zirconia are used. The titania constituent of the starting mixture is not coded since it is to be expected that a single metal oxide is used to make a mixed metal oxide. <br>it is not obvious from the "invention information" symbols that this constituent has been used to make the end product, e.g. if the "invention information" symbol given indicates that a zirconia-alumina composite is prepared it is common practice that zirconia and alumina constituents have been used and thus no codes for zirconia or alumina are given. In the same way, if an allocation indicates that an oxide ceramic contains carbon, no code for the addition of carbon is given. However for an alumina composite product comprising titania, the main symbol for composites based on alumina is given together with an indexing code for titania. <br>In groups C04B2235/32&#160;-&#160;C04B2235/349 oxides are considered to comprise also metal salts from which they are formed by heating. 	CPCONLY	C04B2235/30		17
C04B2235/32	10	Metal oxides, mixed metal oxides, or oxide-forming salts thereof, e.g. carbonates, nitrates, (oxy)hydroxides, chlorides<br><br><u>NOTE</u><br><br> In groups C04B2235/32&#160;-&#160;C04B2235/349 metal salts are classified according to the oxides that are formed by heating the metal salts. 	CPCONLY	C04B2235/32		298
C04B2235/3201	11	Alkali metal oxides or oxide-forming salts thereof	CPCONLY	C04B2235/3201		4906
C04B2235/3203	12	Lithium oxide or oxide-forming salts thereof	CPCONLY	C04B2235/3203		2712
C04B2235/3205	11	Alkaline earth oxides or oxide forming salts thereof, e.g. beryllium oxide	CPCONLY	C04B2235/3205		558
C04B2235/3206	12	Magnesium oxides or oxide-forming salts thereof	CPCONLY	C04B2235/3206		10569
C04B2235/3208	12	Calcium oxide or oxide-forming salts thereof, e.g. lime	CPCONLY	C04B2235/3208		9490
C04B2235/321	13	Dolomites, i.e. mixed calcium magnesium carbonates	CPCONLY	C04B2235/321		462
C04B2235/3212	13	Calcium phosphates, e.g. hydroxyapatite	CPCONLY	C04B2235/3212		296
C04B2235/3213	12	Strontium oxides or oxide-forming salts thereof	CPCONLY	C04B2235/3213		3418
C04B2235/3215	12	Barium oxides or oxide-forming salts thereof	CPCONLY	C04B2235/3215		4020
C04B2235/3217	11	Aluminum oxide or oxide forming salts thereof, e.g. bauxite, alpha-alumina	CPCONLY	C04B2235/3217		14403
C04B2235/3218	12	Aluminium (oxy)hydroxides, e.g. boehmite, gibbsite, alumina sol	CPCONLY	C04B2235/3218		1105
C04B2235/322	12	Transition aluminas, e.g. delta or gamma aluminas	CPCONLY	C04B2235/322		258
C04B2235/3222	12	Aluminates other than alumino-silicates, e.g. spinel (MgAl2O4)	CPCONLY	C04B2235/3222		2973
C04B2235/3224	11	Rare earth oxide or oxide forming salts thereof, e.g. scandium oxide	CPCONLY	C04B2235/3224		6015
C04B2235/3225	12	Yttrium oxide or oxide-forming salts thereof	CPCONLY	C04B2235/3225		7720
C04B2235/3227	12	Lanthanum oxide or oxide-forming salts thereof	CPCONLY	C04B2235/3227		4106
C04B2235/3229	12	Cerium oxides or oxide-forming salts thereof	CPCONLY	C04B2235/3229		3501
C04B2235/3231	11	Refractory metal oxides, their mixed metal oxides, or oxide-forming salts thereof	CPCONLY	C04B2235/3231		86
C04B2235/3232	12	Titanium oxides or titanates, e.g. rutile or anatase	CPCONLY	C04B2235/3232		6927
C04B2235/3234	13	Titanates, not containing zirconia	CPCONLY	C04B2235/3234		813
C04B2235/3236	14	Alkaline earth titanates	CPCONLY	C04B2235/3236		1301
C04B2235/3237	13	Substoichiometric titanium oxides, e.g. Ti2O3	CPCONLY	C04B2235/3237		55
C04B2235/3239	12	Vanadium oxides, vanadates or oxide forming salts thereof, e.g. magnesium vanadate	CPCONLY	C04B2235/3239		1716
C04B2235/3241	12	Chromium oxides, chromates, or oxide-forming salts thereof	CPCONLY	C04B2235/3241		2435
C04B2235/3243	13	Chromates or chromites, e.g. aluminum chromate, lanthanum strontium chromite	CPCONLY	C04B2235/3243		158
C04B2235/3244	12	Zirconium oxides, zirconates, hafnium oxides, hafnates, or oxide-forming salts thereof	CPCONLY	C04B2235/3244		6924
C04B2235/3246	13	Stabilised zirconias, e.g. YSZ or cerium stabilised zirconia	CPCONLY	C04B2235/3246		1191
C04B2235/3248	13	Zirconates or hafnates, e.g. zircon	CPCONLY	C04B2235/3248		1088
C04B2235/3249	14	containing also titanium oxide or titanates, e.g. lead zirconate titanate (PZT)	CPCONLY	C04B2235/3249		277
C04B2235/3251	12	Niobium oxides, niobates, tantalum oxides, tantalates, or oxide-forming salts thereof	CPCONLY	C04B2235/3251		3525
C04B2235/3253	13	Substoichiometric niobium or tantalum oxides, e.g. NbO	CPCONLY	C04B2235/3253		50
C04B2235/3255	13	Niobates or tantalates, e.g. silver niobate	CPCONLY	C04B2235/3255		703
C04B2235/3256	12	Molybdenum oxides, molybdates or oxide forming salts thereof, e.g. cadmium molybdate	CPCONLY	C04B2235/3256		1113
C04B2235/3258	12	Tungsten oxides, tungstates, or oxide-forming salts thereof	CPCONLY	C04B2235/3258		1082
C04B2235/326	13	Tungstates, e.g. scheelite	CPCONLY	C04B2235/326		152
C04B2235/3262	11	Manganese oxides, manganates, rhenium oxides or oxide-forming salts thereof, e.g. MnO	CPCONLY	C04B2235/3262		2936
C04B2235/3263	12	Mn3O4	CPCONLY	C04B2235/3263		358
C04B2235/3265	12	Mn2O3	CPCONLY	C04B2235/3265		174
C04B2235/3267	12	MnO2	CPCONLY	C04B2235/3267		1119
C04B2235/3268	12	Manganates, manganites, rhenates or rhenites, e.g. lithium manganite, barium manganate, rhenium oxide	CPCONLY	C04B2235/3268		199
C04B2235/327	11	Iron group oxides, their mixed metal oxides, or oxide-forming salts thereof	CPCONLY	C04B2235/327		168
C04B2235/3272	12	Iron oxides or oxide forming salts thereof, e.g. hematite, magnetite	CPCONLY	C04B2235/3272		4901
C04B2235/3274	13	Ferrites	CPCONLY	C04B2235/3274		436
C04B2235/3275	12	Cobalt oxides, cobaltates or cobaltites or oxide forming salts thereof, e.g. bismuth cobaltate, zinc cobaltite	CPCONLY	C04B2235/3275		2800
C04B2235/3277	13	Co3O4	CPCONLY	C04B2235/3277		451
C04B2235/3279	12	Nickel oxides, nickalates, or oxide-forming salts thereof	CPCONLY	C04B2235/3279		2676
C04B2235/3281	11	Copper oxides, cuprates or oxide-forming salts thereof, e.g. CuO or Cu2O	CPCONLY	C04B2235/3281		2434
C04B2235/3282	12	Cuprates	CPCONLY	C04B2235/3282		60
C04B2235/3284	11	Zinc oxides, zincates, cadmium oxides, cadmiates, mercury oxides, mercurates or oxide forming salts thereof	CPCONLY	C04B2235/3284		4754
C04B2235/3286	11	Gallium oxides, gallates, indium oxides, indates, thallium oxides, thallates or oxide forming salts thereof, e.g. zinc gallate	CPCONLY	C04B2235/3286		1734
C04B2235/3287	11	Germanium oxides, germanates or oxide forming salts thereof, e.g. copper germanate	CPCONLY	C04B2235/3287		603
C04B2235/3289	11	Noble metal oxides	CPCONLY	C04B2235/3289		244
C04B2235/3291	12	Silver oxides	CPCONLY	C04B2235/3291		366
C04B2235/3293	11	Tin oxides, stannates or oxide forming salts thereof, e.g. indium tin oxide [ITO]	CPCONLY	C04B2235/3293		1688
C04B2235/3294	11	Antimony oxides, antimonates, antimonites or oxide forming salts thereof, indium antimonate	CPCONLY	C04B2235/3294		1049
C04B2235/3296	11	Lead oxides, plumbates or oxide forming salts thereof, e.g. silver plumbate	CPCONLY	C04B2235/3296		769
C04B2235/3298	11	Bismuth oxides, bismuthates or oxide forming salts thereof, e.g. zinc bismuthate	CPCONLY	C04B2235/3298		2841
C04B2235/34	10	Non-metal oxides, non-metal mixed oxides, or salts thereof that form the non-metal oxides upon heating, e.g. carbonates, nitrates, (oxy)hydroxides, chlorides	CPCONLY	C04B2235/34		247
C04B2235/3409	11	Boron oxide, borates, boric acids, or oxide forming salts thereof, e.g. borax	CPCONLY	C04B2235/3409		3287
C04B2235/3418	11	Silicon oxide, silicic acids or oxide forming salts thereof, e.g. silica sol, fused silica, silica fume, cristobalite, quartz or flint	CPCONLY	C04B2235/3418		13318
C04B2235/3427	11	Silicates other than clay, e.g. water glass	CPCONLY	C04B2235/3427		3196
C04B2235/3436	12	Alkaline earth metal silicates, e.g. barium silicate	CPCONLY	C04B2235/3436		278
C04B2235/3445	13	Magnesium silicates, e.g. forsterite	CPCONLY	C04B2235/3445		1181
C04B2235/3454	13	Calcium silicates, e.g. wollastonite	CPCONLY	C04B2235/3454		919
C04B2235/3463	12	Alumino-silicates other than clay, e.g. mullite	CPCONLY	C04B2235/3463		4415
C04B2235/3472	13	Alkali metal alumino-silicates other than clay, e.g. spodumene, alkali feldspars such as albite or orthoclase, micas such as muscovite, zeolites such as natrolite	CPCONLY	C04B2235/3472		2627
C04B2235/3481	13	Alkaline earth metal alumino-silicates other than clay, e.g. cordierite, beryl, micas such as margarite, plagioclase feldspars such as anorthite, zeolites such as chabazite	CPCONLY	C04B2235/3481		1360
C04B2235/349	11	Clays, e.g. bentonites, smectites such as montmorillonite, vermiculites or kaolines, e.g. illite, talc or sepiolite	CPCONLY	C04B2235/349		5543
C04B2235/36	10	Glass starting materials for making ceramics, e.g. silica glass	CPCONLY	C04B2235/36		2023
C04B2235/365	11	Borosilicate glass	CPCONLY	C04B2235/365		492
C04B2235/38	10	Non-oxide ceramic constituents or additives	CPCONLY	C04B2235/38		139
C04B2235/3804	11	Borides	CPCONLY	C04B2235/3804		403
C04B2235/3808	12	Magnesium borides	CPCONLY	C04B2235/3808		35
C04B2235/3813	12	Refractory metal borides	CPCONLY	C04B2235/3813		1010
C04B2235/3817	11	Carbides	CPCONLY	C04B2235/3817		535
C04B2235/3821	12	Boron carbides	CPCONLY	C04B2235/3821		1422
C04B2235/3826	12	Silicon carbides	CPCONLY	C04B2235/3826		5393
C04B2235/383	13	Alpha silicon carbide	CPCONLY	C04B2235/383		190
C04B2235/3834	13	Beta silicon carbide	CPCONLY	C04B2235/3834		187
C04B2235/3839	12	Refractory metal carbides	CPCONLY	C04B2235/3839		975
C04B2235/3843	13	Titanium carbides	CPCONLY	C04B2235/3843		1069
C04B2235/3847	13	Tungsten carbides	CPCONLY	C04B2235/3847		543
C04B2235/3852	11	Nitrides, e.g. oxynitrides, carbonitrides, oxycarbonitrides, lithium nitride, magnesium nitride	CPCONLY	C04B2235/3852		584
C04B2235/3856	12	Carbonitrides, e.g. titanium carbonitride, zirconium carbonitride<br><br><u>NOTE</u><br><br> When indexing in group C04B2235/3856 indexing according to the metal is also made in groups C04B2235/3865&#160;-&#160;C04B2235/3886	CPCONLY	C04B2235/3856		370
C04B2235/386	12	Boron nitrides	CPCONLY	C04B2235/386		1584
C04B2235/3865	12	Aluminium nitrides	CPCONLY	C04B2235/3865		1222
C04B2235/3869	13	Aluminium oxynitrides, e.g. AlON, sialon	CPCONLY	C04B2235/3869		272
C04B2235/3873	12	Silicon nitrides, e.g. silicon carbonitride, silicon oxynitride	CPCONLY	C04B2235/3873		1924
C04B2235/3878	13	Alpha silicon nitrides	CPCONLY	C04B2235/3878		201
C04B2235/3882	13	Beta silicon nitrides	CPCONLY	C04B2235/3882		104
C04B2235/3886	12	Refractory metal nitrides, e.g. vanadium nitride, tungsten nitride	CPCONLY	C04B2235/3886		909
C04B2235/3891	11	Silicides, e.g. molybdenum disilicide, iron silicide	CPCONLY	C04B2235/3891		687
C04B2235/3895	11	Non-oxides with a defined oxygen content, e.g. SiOC, TiON	CPCONLY	C04B2235/3895		362
C04B2235/40	10	Metallic constituents or additives not added as binding phase	CPCONLY	C04B2235/40		1260
C04B2235/401	11	Alkaline earth metals	CPCONLY	C04B2235/401		496
C04B2235/402	11	Aluminium	CPCONLY	C04B2235/402		2194
C04B2235/404	11	Refractory metals	CPCONLY	C04B2235/404		1582
C04B2235/405	11	Iron group metals	CPCONLY	C04B2235/405		1248
C04B2235/407	11	Copper	CPCONLY	C04B2235/407		509
C04B2235/408	11	Noble metals	CPCONLY	C04B2235/408		477
C04B2235/42	10	Non metallic elements added as constituents or additives, e.g. sulfur, phosphor, selenium or tellurium	CPCONLY	C04B2235/42		299
C04B2235/421	11	Boron	CPCONLY	C04B2235/421		524
C04B2235/422	11	Carbon	CPCONLY	C04B2235/422		3295
C04B2235/424	12	Carbon black	CPCONLY	C04B2235/424		1202
C04B2235/425	12	Graphite	CPCONLY	C04B2235/425		3471
C04B2235/427	12	Diamond	CPCONLY	C04B2235/427		653
C04B2235/428	11	Silicon	CPCONLY	C04B2235/428		3393
C04B2235/44	10	Metal salt constituents or additives chosen for the nature of the anions, e.g. hydrides or acetylacetonate	CPCONLY	C04B2235/44		437
C04B2235/441	11	Alkoxides, e.g. methoxide, tert-butoxide	CPCONLY	C04B2235/441		672
C04B2235/442	11	Carbonates	CPCONLY	C04B2235/442		2987
C04B2235/443	11	Nitrates or nitrites	CPCONLY	C04B2235/443		1206
C04B2235/444	11	Halide containing anions, e.g. bromide, iodate, chlorite	CPCONLY	C04B2235/444		1318
C04B2235/445	12	Fluoride containing anions, e.g. fluosilicate	CPCONLY	C04B2235/445		1390
C04B2235/446	11	Sulfides, tellurides or selenides	CPCONLY	C04B2235/446		359
C04B2235/447	11	Phosphates or phosphites, e.g. orthophosphate or hypophosphite	CPCONLY	C04B2235/447		2127
C04B2235/448	11	Sulphates or sulphites	CPCONLY	C04B2235/448		1187
C04B2235/449	11	Organic acids, e.g. EDTA, citrate, acetate, oxalate	CPCONLY	C04B2235/449		1188
C04B2235/46	10	Gases other than oxygen used as reactant, e.g. nitrogen used to make a nitride phase	CPCONLY	C04B2235/46		620
C04B2235/465	11	Ammonia	CPCONLY	C04B2235/465		173
C04B2235/48	10	Organic compounds becoming part of a ceramic after heat treatment, e.g. carbonising phenol resins	CPCONLY	C04B2235/48		2835
C04B2235/483	11	Si-containing organic compounds, e.g. silicone resins, (poly)silanes, (poly)siloxanes or (poly)silazanes	CPCONLY	C04B2235/483		1888
C04B2235/486	11	Boron containing organic compounds, e.g. borazine, borane or boranyl	CPCONLY	C04B2235/486		218
C04B2235/50	9	Constituents or additives of the starting mixture chosen for their shape or used because of their shape or their physical appearance	CPCONLY	C04B2235/50		33
C04B2235/52	10	Constituents or additives characterised by their shapes	CPCONLY	C04B2235/52		124
C04B2235/5204	11	Monocrystalline powders	CPCONLY	C04B2235/5204		23
C04B2235/5208	11	Fibers	CPCONLY	C04B2235/5208		247
C04B2235/5212	12	Organic	CPCONLY	C04B2235/5212		813
C04B2235/5216	12	Inorganic	CPCONLY	C04B2235/5216		918
C04B2235/522	13	Oxidic	CPCONLY	C04B2235/522		406
C04B2235/5224	14	Alumina or aluminates	CPCONLY	C04B2235/5224		1269
C04B2235/5228	14	Silica and alumina, including aluminosilicates, e.g. mullite	CPCONLY	C04B2235/5228		1269
C04B2235/5232	14	Silica or silicates other than aluminosilicates, e.g. quartz	CPCONLY	C04B2235/5232		700
C04B2235/5236	14	Zirconia	CPCONLY	C04B2235/5236		423
C04B2235/524	13	Non-oxidic, e.g. borides, carbides, silicides or nitrides	CPCONLY	C04B2235/524		786
C04B2235/5244	14	Silicon carbide	CPCONLY	C04B2235/5244		2029
C04B2235/5248	14	Carbon, e.g. graphite	CPCONLY	C04B2235/5248		3022
C04B2235/5252	12	having a specific pre-form	CPCONLY	C04B2235/5252		606
C04B2235/5256	13	Two-dimensional, e.g. woven structures	CPCONLY	C04B2235/5256		783
C04B2235/526	12	characterised by the length of the fibers	CPCONLY	C04B2235/526		1041
C04B2235/5264	12	characterised by the diameter of the fibers	CPCONLY	C04B2235/5264		1267
C04B2235/5268	12	Orientation of the fibers	CPCONLY	C04B2235/5268		440
C04B2235/5272	12	Fibers of the same material with different length or diameter	CPCONLY	C04B2235/5272		53
C04B2235/5276	11	Whiskers, spindles, needles or pins	CPCONLY	C04B2235/5276		1168
C04B2235/528	11	Spheres	CPCONLY	C04B2235/528		718
C04B2235/5284	11	Hollow fibers, e.g. nanotubes	CPCONLY	C04B2235/5284		190
C04B2235/5288	12	Carbon nanotubes	CPCONLY	C04B2235/5288		673
C04B2235/5292	11	Flakes, platelets or plates	CPCONLY	C04B2235/5292		500
C04B2235/5296	11	with a defined aspect ratio, e.g. indicating sphericity	CPCONLY	C04B2235/5296		500
C04B2235/54	10	Particle size related information	CPCONLY	C04B2235/54		19
C04B2235/5409	11	expressed by specific surface values	CPCONLY	C04B2235/5409		1418
C04B2235/5418	11	expressed by the size of the particles or aggregates thereof	CPCONLY	C04B2235/5418		115
C04B2235/5427	12	millimeter or submillimeter sized, i.e. larger than 0,1 mm	CPCONLY	C04B2235/5427		3393
C04B2235/5436	12	micrometer sized, i.e. from 1 to 100 micron	CPCONLY	C04B2235/5436		9443
C04B2235/5445	12	submicron sized, i.e. from 0,1 to 1 micron	CPCONLY	C04B2235/5445		5645
C04B2235/5454	12	nanometer sized, i.e. below 100 nm	CPCONLY	C04B2235/5454		2987
C04B2235/5463	11	Particle size distributions	CPCONLY	C04B2235/5463		769
C04B2235/5472	12	Bimodal, multi-modal or multi-fraction	CPCONLY	C04B2235/5472		1039
C04B2235/5481	12	Monomodal	CPCONLY	C04B2235/5481		344
C04B2235/549	11	the particle size being expressed by crystallite size or primary particle size	CPCONLY	C04B2235/549		327
C04B2235/60	8	Aspects relating to the preparation, properties or mechanical treatment of green bodies or pre-forms	CPCONLY	C04B2235/60		211
C04B2235/602	9	Making the green bodies or pre-forms by moulding	CPCONLY	C04B2235/602		4284
C04B2235/6021	10	Extrusion moulding	CPCONLY	C04B2235/6021		1217
C04B2235/6022	10	Injection moulding	CPCONLY	C04B2235/6022		1191
C04B2235/6023	10	Gel casting	CPCONLY	C04B2235/6023		424
C04B2235/6025	10	Tape casting, e.g. with a doctor blade	CPCONLY	C04B2235/6025		1435
C04B2235/6026	10	Computer aided shaping, e.g. rapid prototyping	CPCONLY	C04B2235/6026		2017
C04B2235/6027	10	Slip casting	CPCONLY	C04B2235/6027		521
C04B2235/6028	10	Shaping around a core which is removed later	CPCONLY	C04B2235/6028		367
C04B2235/604	9	Pressing at temperatures other than sintering temperatures	CPCONLY	C04B2235/604		2213
C04B2235/605	9	Making or treating the green body or pre-form in a magnetic field	CPCONLY	C04B2235/605		173
C04B2235/606	9	Drying	CPCONLY	C04B2235/606		2192
C04B2235/608	9	Green bodies or pre-forms with well-defined density	CPCONLY	C04B2235/608		1289
C04B2235/61	9	Mechanical properties, e.g. fracture toughness, hardness, Young&apos;s modulus or strength	CPCONLY	C04B2235/61		400
C04B2235/612	9	Machining	CPCONLY	C04B2235/612		920
C04B2235/614	9	Gas infiltration of green bodies or pre-forms	CPCONLY	C04B2235/614		1208
C04B2235/616	9	Liquid infiltration of green bodies or pre-forms	CPCONLY	C04B2235/616		2265
C04B2235/65	8	Aspects relating to heat treatments of ceramic bodies such as green ceramics or pre-sintered ceramics, e.g. burning, sintering or melting processes	CPCONLY	C04B2235/65		119
C04B2235/652	9	Reduction treatment (C04B2235/664 takes precedence)	CPCONLY	C04B2235/652		472
C04B2235/656	9	characterised by specific heating conditions during heat treatment	CPCONLY	C04B2235/656		9929
C04B2235/6562	10	Heating rate	CPCONLY	C04B2235/6562		13169
C04B2235/6565	10	Cooling rate	CPCONLY	C04B2235/6565		3466
C04B2235/6567	10	Treatment time	CPCONLY	C04B2235/6567		19678
C04B2235/658	9	Atmosphere during thermal treatment	CPCONLY	C04B2235/658		3314
C04B2235/6581	10	Total pressure below 1 atmosphere, e.g. vacuum	CPCONLY	C04B2235/6581		2569
C04B2235/6582	10	Hydrogen containing atmosphere	CPCONLY	C04B2235/6582		1182
C04B2235/6583	10	Oxygen containing atmosphere, e.g. with changing oxygen pressures	CPCONLY	C04B2235/6583		1148
C04B2235/6584	11	at an oxygen percentage below that of air	CPCONLY	C04B2235/6584		842
C04B2235/6585	11	at an oxygen percentage above that of air	CPCONLY	C04B2235/6585		416
C04B2235/6586	10	Processes characterised by the flow of gas	CPCONLY	C04B2235/6586		508
C04B2235/6587	10	Influencing the atmosphere by vaporising a solid material, e.g. by using a burying of sacrificial powder	CPCONLY	C04B2235/6587		278
C04B2235/6588	10	Water vapor containing atmospheres	CPCONLY	C04B2235/6588		330
C04B2235/66	9	Specific sintering techniques, e.g. centrifugal sintering	CPCONLY	C04B2235/66		291
C04B2235/661	10	Multi-step sintering	CPCONLY	C04B2235/661		3116
C04B2235/662	11	Annealing after sintering	CPCONLY	C04B2235/662		806
C04B2235/663	12	Oxidative annealing	CPCONLY	C04B2235/663		555
C04B2235/664	12	Reductive annealing	CPCONLY	C04B2235/664		184
C04B2235/665	10	Local sintering, e.g. laser sintering	CPCONLY	C04B2235/665		632
C04B2235/666	10	Applying a current during sintering, e.g. plasma sintering [SPS], electrical resistance heating or pulse electric current sintering [PECS]	CPCONLY	C04B2235/666		1713
C04B2235/667	10	Sintering using wave energy, e.g. microwave sintering	CPCONLY	C04B2235/667		599
C04B2235/668	10	Pressureless sintering	CPCONLY	C04B2235/668		471
C04B2235/70	8	Aspects relating to sintered or melt-casted ceramic products	CPCONLY	C04B2235/70		18
C04B2235/72	9	Products characterised by the absence or the low content of specific components, e.g. alkali metal free alumina ceramics	CPCONLY	C04B2235/72		1970
C04B2235/721	10	Carbon content	CPCONLY	C04B2235/721		331
C04B2235/722	10	Nitrogen content	CPCONLY	C04B2235/722		101
C04B2235/723	10	Oxygen content	CPCONLY	C04B2235/723		242
C04B2235/724	10	Halogenide content	CPCONLY	C04B2235/724		154
C04B2235/725	10	Metal content	CPCONLY	C04B2235/725		266
C04B2235/726	10	Sulfur content	CPCONLY	C04B2235/726		135
C04B2235/727	10	Phosphorus or phosphorus compound content	CPCONLY	C04B2235/727		188
C04B2235/728	10	Silicon content	CPCONLY	C04B2235/728		221
C04B2235/74	9	Physical characteristics	CPCONLY	C04B2235/74		103
C04B2235/75	10	Products with a concentration gradient	CPCONLY	C04B2235/75		470
C04B2235/76	10	Crystal structural characteristics, e.g. symmetry<br><br><u>NOTE</u><br><br> Codes C04B2235/76&#160;-&#160;C04B2235/768 are to be used only if the crystal structure is not identified by the classification. 	CPCONLY	C04B2235/76		747
C04B2235/761	11	Unit-cell parameters, e.g. lattice constants	CPCONLY	C04B2235/761		304
C04B2235/762	11	Cubic symmetry, e.g. beta-SiC	CPCONLY	C04B2235/762		584
C04B2235/763	12	Spinel structure AB2O4	CPCONLY	C04B2235/763		291
C04B2235/764	12	Garnet structure A3B2(CO4)3	CPCONLY	C04B2235/764		550
C04B2235/765	11	Tetragonal symmetry	CPCONLY	C04B2235/765		485
C04B2235/766	11	Trigonal symmetry, e.g. alpha-Si3N4 or alpha-Sialon	CPCONLY	C04B2235/766		105
C04B2235/767	11	Hexagonal symmetry, e.g. beta-Si3N4, beta-Sialon, alpha-SiC or hexa-ferrites	CPCONLY	C04B2235/767		588
C04B2235/768	11	Perovskite structure ABO3	CPCONLY	C04B2235/768		1188
C04B2235/77	10	Density	CPCONLY	C04B2235/77		13635
C04B2235/775	11	Products showing a density-gradient	CPCONLY	C04B2235/775		197
C04B2235/78	10	Grain sizes and shapes, product microstructures, e.g. acicular grains, equiaxed grains, platelet-structures	CPCONLY	C04B2235/78		376
C04B2235/781	11	Nanograined materials, i.e. having grain sizes below 100 nm	CPCONLY	C04B2235/781		560
C04B2235/782	11	Grain size distributions	CPCONLY	C04B2235/782		172
C04B2235/783	12	Bimodal, multi-modal or multi-fractional	CPCONLY	C04B2235/783		115
C04B2235/784	12	Monomodal	CPCONLY	C04B2235/784		86
C04B2235/785	11	Submicron sized grains, i.e. from 0,1 to 1 micron	CPCONLY	C04B2235/785		1339
C04B2235/786	11	Micrometer sized grains, i.e. from 1 to 100 micron	CPCONLY	C04B2235/786		1931
C04B2235/787	11	Oriented grains	CPCONLY	C04B2235/787		344
C04B2235/788	11	Aspect ratio of the grains	CPCONLY	C04B2235/788		182
C04B2235/79	10	Non-stoichiometric products, e.g. perovskites (ABO3) with an A/B-ratio other than 1	CPCONLY	C04B2235/79		708
C04B2235/80	9	Phases present in the sintered or melt-cast ceramic products other than the main phase<br><br><u>NOTE</u><br><br>In this group the term "phases other than the main phase" refers to any phase that is not the main phase, i.e. the phase that is present in the largest amount<br> Codes chosen from groups C04B2235/30&#160;-&#160;C04B2235/5296 are used for identifying the phases other than the main phase 	CPCONLY	C04B2235/80		3132
C04B2235/81	10	Materials characterised by the absence of phases other than the main phase, i.e. single phase materials	CPCONLY	C04B2235/81		316
C04B2235/83	10	Ferrites containing Fe2+	CPCONLY	C04B2235/83		30
C04B2235/85	10	Intergranular or grain boundary phases	CPCONLY	C04B2235/85		795
C04B2235/87	10	Grain boundary phases intentionally being absent	CPCONLY	C04B2235/87		54
C04B2235/94	9	Products characterised by their shape	CPCONLY	C04B2235/94		2307
C04B2235/945	10	Products containing grooves, cuts, recesses or protusions	CPCONLY	C04B2235/945		320
C04B2235/95	9	Products characterised by their size, e.g. microceramics	CPCONLY	C04B2235/95		1969
C04B2235/96	9	Properties of ceramic products, e.g. mechanical properties such as strength, toughness, wear resistance<br><br><u>NOTE</u><br><br>Indexing Codes C04B2235/96 - C04B2235/9692 are to be used only if the property is not identified already by an "invention information" symbol, e.g. by a symbol out of subclass H10N indicating that the ceramic is dielectric, piezoelectric or magnetic.	CPCONLY	C04B2235/96		22162
C04B2235/9607	10	Thermal properties, e.g. thermal expansion coefficient	CPCONLY	C04B2235/9607		8976
C04B2235/9615	11	Linear firing shrinkage	CPCONLY	C04B2235/9615		1103
C04B2235/9623	11	Ceramic setters properties	CPCONLY	C04B2235/9623		268
C04B2235/963	10	Surface properties, e.g. surface roughness	CPCONLY	C04B2235/963		1046
C04B2235/9638	11	Tolerance; Dimensional accuracy	CPCONLY	C04B2235/9638		196
C04B2235/9646	10	Optical properties	CPCONLY	C04B2235/9646		944
C04B2235/9653	11	Translucent or transparent ceramics other than alumina	CPCONLY	C04B2235/9653		1195
C04B2235/9661	11	Colour	CPCONLY	C04B2235/9661		1111
C04B2235/9669	10	Resistance against chemicals, e.g. against molten glass or molten salts	CPCONLY	C04B2235/9669		1482
C04B2235/9676	11	against molten metals such as steel or aluminium	CPCONLY	C04B2235/9676		937
C04B2235/9684	11	Oxidation resistance	CPCONLY	C04B2235/9684		851
C04B2235/9692	11	Acid, alkali or halogen resistance	CPCONLY	C04B2235/9692		619
C04B2237/00	7	Aspects relating to ceramic laminates or to joining of ceramic articles with other articles by heating	CPCONLY	C04B2237/00		7
C04B2237/02	8	Aspects relating to interlayers, e.g. used to join ceramic articles with other articles by heating	CPCONLY	C04B2237/02		114
C04B2237/04	9	Ceramic interlayers	CPCONLY	C04B2237/04		91
C04B2237/06	10	Oxidic interlayers	CPCONLY	C04B2237/06		383
C04B2237/062	11	based on silica or silicates	CPCONLY	C04B2237/062		405
C04B2237/064	11	based on alumina or aluminates	CPCONLY	C04B2237/064		463
C04B2237/066	11	based on rare earth oxides	CPCONLY	C04B2237/066		103
C04B2237/068	11	based on refractory oxides, e.g. zirconia	CPCONLY	C04B2237/068		250
C04B2237/08	10	Non-oxidic interlayers	CPCONLY	C04B2237/08		353
C04B2237/083	11	Carbide interlayers, e.g. silicon carbide interlayers	CPCONLY	C04B2237/083		500
C04B2237/086	11	Carbon interlayers	CPCONLY	C04B2237/086		187
C04B2237/09	10	wherein the active component for bonding is not the largest fraction of the interlayer	CPCONLY	C04B2237/09		222
C04B2237/095	11	The active component for bonding being silicon	CPCONLY	C04B2237/095		16
C04B2237/10	9	Glass interlayers, e.g. frit or flux	CPCONLY	C04B2237/10		647
C04B2237/12	9	Metallic interlayers	CPCONLY	C04B2237/12		660
C04B2237/121	10	based on aluminium	CPCONLY	C04B2237/121		423
C04B2237/122	10	based on refractory metals	CPCONLY	C04B2237/122		892
C04B2237/123	10	based on iron group metals, e.g. steel	CPCONLY	C04B2237/123		754
C04B2237/124	10	based on copper	CPCONLY	C04B2237/124		800
C04B2237/125	10	based on noble metals, e.g. silver	CPCONLY	C04B2237/125		1086
C04B2237/126	10	wherein the active component for bonding is not the largest fraction of the interlayer	CPCONLY	C04B2237/126		556
C04B2237/127	11	The active component for bonding being a refractory metal	CPCONLY	C04B2237/127		510
C04B2237/128	11	The active component for bonding being silicon	CPCONLY	C04B2237/128		129
C04B2237/16	9	Silicon interlayers	CPCONLY	C04B2237/16		202
C04B2237/30	8	Composition of layers of ceramic laminates or of ceramic or metallic articles to be joined by heating, e.g. Si substrates	CPCONLY	C04B2237/30		167
C04B2237/32	9	Ceramic	CPCONLY	C04B2237/32		685
C04B2237/34	10	Oxidic	CPCONLY	C04B2237/34		1123
C04B2237/341	11	Silica or silicates	CPCONLY	C04B2237/341		1140
C04B2237/343	11	Alumina or aluminates	CPCONLY	C04B2237/343		2585
C04B2237/345	11	Refractory metal oxides	CPCONLY	C04B2237/345		162
C04B2237/346	12	Titania or titanates	CPCONLY	C04B2237/346		672
C04B2237/348	12	Zirconia, hafnia, zirconates or hafnates	CPCONLY	C04B2237/348		1116
C04B2237/36	10	Non-oxidic	CPCONLY	C04B2237/36		667
C04B2237/361	11	Boron nitride	CPCONLY	C04B2237/361		273
C04B2237/363	11	Carbon	CPCONLY	C04B2237/363		785
C04B2237/365	11	Silicon carbide	CPCONLY	C04B2237/365		1515
C04B2237/366	11	Aluminium nitride	CPCONLY	C04B2237/366		952
C04B2237/368	11	Silicon nitride	CPCONLY	C04B2237/368		1079
C04B2237/38	10	Fiber or whisker reinforced	CPCONLY	C04B2237/38		918
C04B2237/385	11	Carbon or carbon composite	CPCONLY	C04B2237/385		356
C04B2237/40	9	Metallic	CPCONLY	C04B2237/40		649
C04B2237/401	10	Cermets	CPCONLY	C04B2237/401		257
C04B2237/402	10	Aluminium	CPCONLY	C04B2237/402		524
C04B2237/403	10	Refractory metals	CPCONLY	C04B2237/403		703
C04B2237/404	10	Manganese or rhenium	CPCONLY	C04B2237/404		42
C04B2237/405	10	Iron metal group, e.g. Co or Ni	CPCONLY	C04B2237/405		598
C04B2237/406	11	Iron, e.g. steel	CPCONLY	C04B2237/406		681
C04B2237/407	10	Copper	CPCONLY	C04B2237/407		961
C04B2237/408	10	Noble metals, e.g. palladium, platina or silver	CPCONLY	C04B2237/408		343
C04B2237/50	8	Processing aspects relating to ceramic laminates or to the joining of ceramic articles with other articles by heating	CPCONLY	C04B2237/50		93
C04B2237/52	9	Pre-treatment of the joining surfaces, e.g. cleaning, machining	CPCONLY	C04B2237/52		665
C04B2237/525	10	by heating	CPCONLY	C04B2237/525		184
C04B2237/54	9	Oxidising the surface before joining	CPCONLY	C04B2237/54		166
C04B2237/55	9	Pre-treatments of a coated or not coated substrate other than oxidation treatment in order to form an active joining layer	CPCONLY	C04B2237/55		211
C04B2237/555	10	on a substrate not containing an interlayer coating, leading to the formation of an interlayer coating	CPCONLY	C04B2237/555		61
C04B2237/56	9	Using constraining layers before or during sintering	CPCONLY	C04B2237/56		75
C04B2237/561	10	Constraining layers not covering the whole surface of the layers to be sintered, e.g. constraining layers with holes	CPCONLY	C04B2237/561		23
C04B2237/562	10	made of alumina or aluminates	CPCONLY	C04B2237/562		71
C04B2237/564	10	made of glass	CPCONLY	C04B2237/564		9
C04B2237/565	10	made of refractory metal oxides, e.g. zirconia	CPCONLY	C04B2237/565		41
C04B2237/567	10	made of metal	CPCONLY	C04B2237/567		50
C04B2237/568	10	made of non-oxide ceramics	CPCONLY	C04B2237/568		58
C04B2237/58	9	Forming a gradient in composition or in properties across the laminate or the joined articles	CPCONLY	C04B2237/58		271
C04B2237/582	10	by joining layers or articles of the same composition but having different additives	CPCONLY	C04B2237/582		129
C04B2237/584	11	the different additives being fibers or whiskers	CPCONLY	C04B2237/584		68
C04B2237/586	10	by joining layers or articles of the same composition but having different densities	CPCONLY	C04B2237/586		117
C04B2237/588	10	by joining layers or articles of the same composition but having different particle or grain sizes	CPCONLY	C04B2237/588		77
C04B2237/59	9	Aspects relating to the structure of the interlayer	CPCONLY	C04B2237/59		43
C04B2237/592	10	whereby the interlayer is not continuous, e.g. not the whole surface of the smallest substrate is covered by the interlayer	CPCONLY	C04B2237/592		325
C04B2237/595	10	whereby the interlayer is continuous, but heterogeneous on macro-scale, e.g. one part of the interlayer being a joining material, another part being an electrode material	CPCONLY	C04B2237/595		73
C04B2237/597	10	whereby the interlayer is continuous but porous, e.g. containing hollow or porous particles, macro- or micropores or cracks	CPCONLY	C04B2237/597		97
C04B2237/60	9	Forming at the joining interface or in the joining layer specific reaction phases or zones, e.g. diffusion of reactive species from the interlayer to the substrate or from a substrate to the joining interface, carbide forming at the joining interface	CPCONLY	C04B2237/60		434
C04B2237/61	9	Joining two substrates of which at least one is porous by infiltrating the porous substrate with a liquid, such as a molten metal, causing bonding of the two substrates, e.g. joining two porous carbon substrates by infiltrating with molten silicon	CPCONLY	C04B2237/61		318
C04B2237/62	9	Forming laminates or joined articles comprising holes, channels or other types of openings	CPCONLY	C04B2237/62		874
C04B2237/64	9	Forming laminates or joined articles comprising grooves or cuts	CPCONLY	C04B2237/64		481
C04B2237/66	9	Forming laminates or joined articles showing high dimensional accuracy, e.g. indicated by the warpage	CPCONLY	C04B2237/66		189
C04B2237/68	9	Forming laminates or joining articles wherein at least one substrate contains at least two different parts of macro-size, e.g. one ceramic substrate layer containing an embedded conductor or electrode	CPCONLY	C04B2237/68		491
C04B2237/70	9	Forming laminates or joined articles comprising layers of a specific, unusual thickness	CPCONLY	C04B2237/70		87
C04B2237/702	10	of one or more of the constraining layers	CPCONLY	C04B2237/702		41
C04B2237/704	10	of one or more of the ceramic layers or articles	CPCONLY	C04B2237/704		1477
C04B2237/706	10	of one or more of the metallic layers or articles	CPCONLY	C04B2237/706		500
C04B2237/708	10	of one or more of the interlayers	CPCONLY	C04B2237/708		1133
C04B2237/72	9	Forming laminates or joined articles comprising at least two interlayers directly next to each other	CPCONLY	C04B2237/72		929
C04B2237/74	9	Forming laminates or joined articles comprising at least two different interlayers separated by a substrate	CPCONLY	C04B2237/74		118
C04B2237/76	9	Forming laminates or joined articles comprising at least one member in the form other than a sheet or disc, e.g. two tubes or a tube and a sheet or disc	CPCONLY	C04B2237/76		815
C04B2237/765	10	at least one member being a tube	CPCONLY	C04B2237/765		832
C04B2237/78	9	Side-way connecting, e.g. connecting two plates through their sides	CPCONLY	C04B2237/78		236
C04B2237/80	9	Joining the largest surface of one substrate with a smaller surface of the other substrate, e.g. butt joining or forming a T-joint	CPCONLY	C04B2237/80		284
C04B2237/82	9	Two substrates not completely covering each other, e.g. two plates in a staggered position	CPCONLY	C04B2237/82		154
C04B2237/84	9	Joining of a first substrate with a second substrate at least partially inside the first substrate, where the bonding area is at the inside of the first substrate, e.g. one tube inside another tube	CPCONLY	C04B2237/84		816
C04B2237/86	9	Joining of two substrates at their largest surfaces, one surface being complete joined and covered, the other surface not, e.g. a small plate joined at it&apos;s largest surface on top of a larger plate	CPCONLY	C04B2237/86		343
C04B2237/88	9	Joining of two substrates, where a substantial part of the joining material is present outside of the joint, leading to an outside joining of the joint	CPCONLY	C04B2237/88		213
C04B2290/00	7	Organisational aspects of production methods, equipment or plants	CPCONLY	C04B2290/00		16
C04B2290/10	8	Business methods aspects	CPCONLY	C04B2290/10		7
C04B2290/20	8	Integrated combined plants or devices, e.g. combined foundry and concrete plant	CPCONLY	C04B2290/20		91
