B60B1/00	7	Spoked wheels; Spokes thereof (non-metallic B60B5/00{; spoked wheels comprising rail-engaging elements B60B17/001; making wheel spokes B21F39/00})	B60B1/00	B60B1/00		1725
B60B1/003	8	{specially adapted for bicycles (B60B1/041 takes precedence)}	B60B1/00	B60B1/00		904
B60B1/006	8	{specially adapted for light-weight wheels, e.g. of strollers or wheel-chairs (B60B1/003 takes precedence)}	B60B1/00	B60B1/00		197
B60B1/02	8	Wheels with wire or other tension spokes	B60B1/02	B60B1/02		185
B60B1/0207	9	{characterised by non-standard number of spokes, i.e. less than 12 or more than 32 spokes}	B60B1/02	B60B1/02		160
B60B1/0215	9	{characterised by specific grouping of spokes}	B60B1/02	B60B1/02		107
B60B1/0223	10	{the dominant aspect being the spoke arrangement pattern}	B60B1/02	B60B1/02		325
B60B1/023	11	{multiple exclusively parallel spokes arranged in a group}	B60B1/02	B60B1/02		24
B60B1/0238	10	{the dominant aspect being the number of spokes per group}	B60B1/02	B60B1/02		12
B60B1/0246	9	{characterised by cross-section of the spoke, e.g. polygon or elliptic shape}	B60B1/02	B60B1/02		72
B60B1/0253	9	{the spoke being hollow}	B60B1/02	B60B1/02		27
B60B1/0261	9	{characterised by spoke form}	B60B1/02	B60B1/02		289
B60B1/0269	10	{the spoke being curved or deformed over substantial part of length}	B60B1/02	B60B1/02		84
B60B1/0276	10	{the spoke being crooked in the middle and having double length}	B60B1/02	B60B1/02		113
B60B1/0284	10	{the spoke being threaded at both ends}	B60B1/02	B60B1/02		40
B60B1/0292	10	{the spoke being bent at both ends}	B60B1/02	B60B1/02		8
B60B1/04	9	Attaching spokes to rim or hub	B60B1/04	B60B1/04		81
B60B1/041	10	{of bicycle wheels (bicycle rims characterised by means for attaching spokes B60B21/062)}	B60B1/04	B60B1/04		787
B60B1/042	10	{Attaching spokes to hub}	B60B1/04	B60B1/04		978
B60B1/043	10	{Attaching spokes to rim}	B60B1/04	B60B1/04		234
B60B1/044	11	{by the use of spoke nipples}	B60B1/04	B60B1/04		417
B60B1/045	12	{characterised by their specific shape}	B60B1/04	B60B1/04		108
B60B1/046	12	{characterised by adaptations of the nipple for tightening tools}	B60B1/04	B60B1/04		21
B60B1/047	12	{the nipple comprising sealing means}	B60B1/04	B60B1/04		33
B60B1/048	11	{by the use of screws}	B60B1/04	B60B1/04		181
B60B1/06	8	Wheels with compression spokes (wheels of high resiliency B60B9/00)	B60B1/06	B60B1/06		492
B60B1/08	9	formed by casting	B60B1/08	B60B1/08		406
B60B1/10	9	fabricated by sheet metal (B60B1/12, B60B3/08 take precedence)	B60B1/10	B60B1/10		312
B60B1/12	9	with tubular spokes (B60B1/08 takes precedence)	B60B1/12	B60B1/12		382
B60B1/14	9	Attaching spokes to rim or hub	B60B1/14	B60B1/14		238
B60B3/00	7	Disc wheels, i.e. wheels with load-supporting disc body (non- metallic B60B5/00; wheel cover discs B60B7/00{; disc wheels comprising rail-engaging elements B60B17/0006})	B60B3/00	B60B3/00		398
B60B3/001	8	{Lightweight wheels, e.g. for strollers or toys}	B60B3/00	B60B3/00		328
B60B3/002	8	{characterised by the shape of the disc}	B60B3/00	B60B3/00		305
B60B3/004	9	{in the hub section}	B60B3/00	B60B3/00		100
B60B3/005	9	{in the section adjacent to rim}	B60B3/00	B60B3/00		214
B60B3/007	9	{in the intermediate section}	B60B3/00	B60B3/00		216
B60B3/008	8	{by the form of wheel bolt mounting section}	B60B3/00	B60B3/00		115
B60B3/02	8	with a single disc body integral with rim	B60B3/02	B60B3/02		769
B60B3/04	8	with a single disc body not integral with rim {, i.e. disc body and rim being manufactured independently and then permanently attached to each other in a second step, e.g. by welding}	B60B3/04	B60B3/04		790
B60B3/041	9	{characterised by the attachment of rim to wheel disc}	B60B3/04	B60B3/04		135
B60B3/042	10	{characterised by circumferential position of attachment means}	B60B3/04	B60B3/04		28
B60B3/044	10	{characterised by cross-sectional details of the attachment, e.g. the profile}	B60B3/04	B60B3/04		317
B60B3/045	10	{characterised by the attachment portions}	B60B3/04	B60B3/04		73
B60B3/047	11	{comprising specific torque transmitting means}	B60B3/04	B60B3/04		15
B60B3/048	9	{the rim being rotatably mounted to the wheel disc}	B60B3/04	B60B3/04		108
B60B3/06	8	formed by casting	B60B3/06	B60B3/06		500
B60B3/08	8	with disc body formed by two or more axially spaced discs {(comprising rail-engaging elements formed by two or more axially spaced discs B60B17/0013)}	B60B3/08	B60B3/08		939
B60B3/082	9	{especially for light-weight wheels}	B60B3/08	B60B3/08		163
B60B3/085	9	{Discs having no mutual contact}	B60B3/08	B60B3/08		180
B60B3/087	9	{Discs having several mutual contact regions}	B60B3/08	B60B3/08		107
B60B3/10	8	apertured to simulate spoked wheels	B60B3/10	B60B3/10		675
B60B3/12	8	Means of reinforcing disc bodies	B60B3/12	B60B3/12		258
B60B3/14	8	Attaching disc body to hub (resiliently B60B9/00; attaching rim to wheel body B60B23/00){; Wheel adapters}	B60B3/14	B60B3/14		543
B60B3/142	9	{by central locking nut}	B60B3/14	B60B3/14		125
B60B3/145	9	{using washers or distance bushes}	B60B3/14	B60B3/14		171
B60B3/147	9	{using wheel adapters}	B60B3/14	B60B3/14		173
B60B3/16	9	by bolts or the like	B60B3/16	B60B3/16		1298
B60B3/165	10	{with locking devices for the fixing means, e.g. screw or nut covers}	B60B3/16	B60B3/16		293
B60B3/18	9	by circlips or the like	B60B3/18	B60B3/18		1002
B60B5/00	7	Wheels, spokes, disc bodies, rims, hubs, wholly or predominantly made of non-metallic material (wheel cover discs B60B7/00; wheels of high resiliency B60B9/00{; wheel bodies comprising rail-engaging elements characterised by use of non-metallic material B60B17/0003})	B60B5/00	B60B5/00		98
B60B5/02	8	made of synthetic material	B60B5/02	B60B5/02		1793
B60B5/04	8	made of wood	B60B5/04	B60B5/04		278
B60B7/00	7	Wheel cover discs, rings, or the like, for ornamenting, protecting {, venting,} or obscuring, wholly or in part, the wheel body, rim, hub, or tyre sidewall {, e.g. wheel cover discs, wheel cover discs with cooling fins (wheels with cooling fins not provided on the wheel cover disc B60B19/10; apparatus or tools for removing or attaching cover discs hub caps or the like B60B31/06)}	B60B7/00	B60B7/00		1391
B60B7/0006	8	{for cycle wheels or similar}	B60B7/00	B60B7/00		168
B60B7/0013	8	{Hub caps}	B60B7/00	B60B7/00		864
B60B7/002	9	{being of the ventilated type}	B60B7/00	B60B7/00		143
B60B7/0026	8	{characterised by the surface}	B60B7/00	B60B7/00		33
B60B7/0033	9	{the dominant aspect being the surface appearance}	B60B7/00	B60B7/00		69
B60B7/004	10	{the surface being painted}	B60B7/00	B60B7/00		68
B60B7/0046	10	{the surface being plated or coated}	B60B7/00	B60B7/00		99
B60B7/0053	10	{the surface being decorated}	B60B7/00	B60B7/00		218
B60B7/006	10	{the surface being reflective or including lighting}	B60B7/00	B60B7/00		210
B60B7/0066	9	{the dominant aspect being the surface structure}	B60B7/00	B60B7/00		167
B60B7/0073	10	{being completely closed, i.e. having no cooling openings for the brakes}	B60B7/00	B60B7/00		88
B60B7/008	10	{having decorative holes or openings, i.e. openings going beyond mere cooling openings}	B60B7/00	B60B7/00		103
B60B7/0086	10	{having cooling fins}	B60B7/00	B60B7/00		188
B60B7/0093	8	{being reinforced against thermal deformation}	B60B7/00	B60B7/00		18
B60B7/01	8	Rings specially adapted for covering only the wheel rim or the tyre sidewall, e.g. removable tyre sidewall trim rings	B60B7/01	B60B7/01		511
B60B7/02	8	made essentially in one part ({B60B7/0006,}B60B7/01 take precedence)	B60B7/02	B60B7/02		984
B60B7/04	8	built-up of several main parts (B60B7/01, B60B7/20 take precedence)	B60B7/04	B60B7/04		1029
B60B7/06	8	Fastening arrangements therefor (B60B7/01, B60B7/20 take precedence)	B60B7/06	B60B7/06		511
B60B7/061	9	{characterised by the part of the wheels to which the discs, rings or the like are mounted}	B60B7/06	B60B7/06		193
B60B7/063	10	{to the rim}	B60B7/06	B60B7/06		484
B60B7/065	10	{to the disc}	B60B7/06	B60B7/06		324
B60B7/066	10	{to the hub}	B60B7/06	B60B7/06		498
B60B7/068	10	{to the wheel bolts or wheel nuts}	B60B7/06	B60B7/06		417
B60B7/08	9	having gripping elements consisting of formations integral with the cover	B60B7/08	B60B7/08		877
B60B7/10	9	comprising a plurality of spaced spring clips individually mounted on the cover, e.g. riveted, welded or readily releasable	B60B7/10	B60B7/10		498
B60B7/105	10	{the spring clip mounted on the rim}	B60B7/10	B60B7/10		148
B60B7/12	9	comprising an annular spring or gripping element mounted on the cover (B60B7/08 takes precedence)	B60B7/12	B60B7/12		361
B60B7/14	9	comprising screw-threaded means	B60B7/14	B60B7/14		645
B60B7/16	8	Anti-theft devices	B60B7/16	B60B7/16		323
B60B7/18	8	simulating spoked or wire wheel	B60B7/18	B60B7/18		366
B60B7/20	8	having an element mounted for rotation independently of wheel rotation	B60B7/20	B60B7/20		464
B60B9/00	7	Wheels of high resiliency {, e.g. with conical interacting pressure-surfaces (resilient wheels comprising rail-engaging elements B60B17/0027)}	B60B9/00	B60B9/00		573
B60B9/005	8	{Comprising a resilient hub (hubs per seB60B27/00)}	B60B9/00	B60B9/00		682
B60B9/02	8	using springs {resiliently mounted bicycle rims}(wheels comprising resilient spokes B60B9/26)	B60B9/02	B60B9/02		404
B60B9/04	9	in leaf form	B60B9/04	B60B9/04		511
B60B9/06	9	in helical form	B60B9/06	B60B9/06		1454
B60B9/08	9	in flat coiled form	B60B9/08	B60B9/08		210
B60B9/10	9	of rubber or the like	B60B9/10	B60B9/10		526
B60B9/12	10	in the form of sleeves or rings concentric with the wheel axis	B60B9/12	B60B9/12		351
B60B9/14	10	with means limiting relative lateral movements between hub and remainder of wheel	B60B9/14	B60B9/14		40
B60B9/16	10	modified to ensure electric conductivity	B60B9/16	B60B9/16		26
B60B9/18	8	using fluid (within spokes B60B9/26)	B60B9/18	B60B9/18		294
B60B9/20	9	in rings concentric with wheel axis	B60B9/20	B60B9/20		1037
B60B9/22	10	inflatable	B60B9/22	B60B9/22		449
B60B9/24	9	with pistons and cylinders	B60B9/24	B60B9/24		159
B60B9/26	8	comprising resilient spokes	B60B9/26	B60B9/26		1711
B60B9/28	9	with telescopic action	B60B9/28	B60B9/28		765
B60B11/00	7	Units comprising multiple wheels arranged side by side; Wheels having more than one rim or capable of carrying more than one tyre	B60B11/00	B60B11/00		273
B60B11/02	8	Units of separate wheels mounted for independent or coupled rotation	B60B11/02	B60B11/02		560
B60B11/04	8	Wheels with a rim capable of carrying more than one tyre	B60B11/04	B60B11/04		133
B60B11/06	8	Wheels with more than one rim mounted on a single wheel body	B60B11/06	B60B11/06		992
B60B11/08	8	Arrangements of balancing mechanisms enabling a uniform distribution of load to tyres	B60B11/08	B60B11/08		66
B60B11/10	8	Emergency wheels (collapsible tyres B60C3/08; tyres characterised by means enabling restricted operation in damaged or deflated condition B60C17/00)	B60B11/10	B60B11/10		577
B60B15/00	7	Wheels or wheel attachments designed for increasing traction (vehicle tyres B60C; non-skid devices temporarily attachable to resilient tyres or resiliently-tyred wheels B60C27/00)	B60B15/00	B60B15/00		843
B60B15/02	8	Wheels with spade lugs	B60B15/02	B60B15/02		578
B60B15/021	9	{made of resilient material}	B60B15/02	B60B15/02		82
B60B15/023	9	{being of the broad form type}	B60B15/02	B60B15/02		32
B60B15/025	10	{with non-cylindrical shape}	B60B15/02	B60B15/02		420
B60B15/026	9	{characterised by mud deposit prevention}	B60B15/02	B60B15/02		90
B60B15/028	9	{characterised by active rotation of the lugs}	B60B15/02	B60B15/02		5
B60B15/04	9	with resiliently-mounted spade lugs	B60B15/04	B60B15/04		121
B60B15/06	9	with pivotally-mounted spade lugs	B60B15/06	B60B15/06		110
B60B15/08	9	with spade lugs axially displaced relatively to the tread surface of the tyre	B60B15/08	B60B15/08		30
B60B15/10	9	with radially-adjustable spade lugs; Control mechanisms therefor	B60B15/10	B60B15/10		262
B60B15/12	10	involving cams or eccentric hoops	B60B15/12	B60B15/12		169
B60B15/14	10	involving an axially-displaceable cone	B60B15/14	B60B15/14		26
B60B15/16	10	involving gearing, e.g. gear pinions acting upon threaded shafts on the spade lugs	B60B15/16	B60B15/16		69
B60B15/18	8	Wheels with ground-engaging plate-like shoes	B60B15/18	B60B15/18		371
B60B15/20	9	with resiliently-mounted shoes, e.g. on a spider	B60B15/20	B60B15/20		42
B60B15/22	9	connected by links to the hub	B60B15/22	B60B15/22		77
B60B15/24	8	Tread bands or rings for fairing lugs when travelling on the road	B60B15/24	B60B15/24		51
B60B15/26	8	Auxiliary wheels or rings with traction-increasing surface attachable to the main wheel body	B60B15/26	B60B15/26		519
B60B15/263	9	{Traction increasing surface being located axially beside tyre}	B60B15/26	B60B15/26		310
B60B15/266	9	{Traction increasing surface being located radially outside tyre circumferential surface}	B60B15/26	B60B15/26		154
B60B15/28	8	Wheel-ballasting weights; Their attachment	B60B15/28	B60B15/28		239
B60B17/00	7	Wheels characterised by rail-engaging elements ({wheel-axle combinations B60B37/00;} of model railways A63H19/22)	B60B17/00	B60B17/00		1061
B60B17/0003	8	{Wheel bodies characterised by use of non-metallic material (B60B17/0034 takes precedence)}	B60B17/00	B60B17/00		108
B60B17/0006	8	{Construction of wheel bodies, e.g. disc wheels (B60B17/0003 takes precedence)}	B60B17/00	B60B17/00		577
B60B17/001	9	{Spoked wheels; Spokes thereof}	B60B17/00	B60B17/00		15
B60B17/0013	9	{formed by two or more axially spaced discs}	B60B17/00	B60B17/00		87
B60B17/0017	10	{with insonorisation means}	B60B17/00	B60B17/00		169
B60B17/002	9	{with counter-balance}	B60B17/00	B60B17/00		195
B60B17/0024	9	{with noise reducing means (B60B17/0017 takes precedence)}	B60B17/00	B60B17/00		103
B60B17/0027	8	{Resilient wheels, e.g. resilient hubs (B60B17/02 takes precedence)}	B60B17/00	B60B17/00		97
B60B17/0031	9	{using springs}	B60B17/00	B60B17/00		59
B60B17/0034	10	{of rubber or other non-metallic material}	B60B17/00	B60B17/00		358
B60B17/0037	11	{of circular or elliptical cross section}	B60B17/00	B60B17/00		17
B60B17/0041	11	{of substantially rectangular cross section}	B60B17/00	B60B17/00		232
B60B17/0044	11	{single element arranged in V-form}	B60B17/00	B60B17/00		52
B60B17/0048	11	{pair of elements arranged in V-form}	B60B17/00	B60B17/00		67
B60B17/0051	9	{using fluid}	B60B17/00	B60B17/00		64
B60B17/0055	8	{with non-elastic tyres (e.g. of particular profile or composition)}	B60B17/00	B60B17/00		447
B60B17/0058	9	{characterised by their fixing to wheel bodies}	B60B17/00	B60B17/00		46
B60B17/0062	9	{having teeth or protrusions on the circumference of the wheel}	B60B17/00	B60B17/00		17
B60B17/0065	8	{Flange details}	B60B17/00	B60B17/00		15
B60B17/0068	9	{the flange being provided on a single side}	B60B17/00	B60B17/00		157
B60B17/0072	9	{the flange being provided on both sides}	B60B17/00	B60B17/00		31
B60B17/0075	9	{the flange being movable, for adaptation to variable rail or track widths}	B60B17/00	B60B17/00		12
B60B17/0079	8	{the flange having a guide wheel}	B60B17/00	B60B17/00		15
B60B17/0082	8	{Wheels designed to interact with a particular rail profile}	B60B17/00	B60B17/00		67
B60B17/0086	9	{H-type rail profiles, i.e. the wheels are arranged between upper and lower rail extensions}	B60B17/00	B60B17/00		4
B60B17/0089	9	{Circular rail profiles}	B60B17/00	B60B17/00		18
B60B17/0093	9	{Rectangular rail profiles}	B60B17/00	B60B17/00		5
B60B17/0096	9	{Triangular rail profiles}	B60B17/00	B60B17/00		7
B60B17/02	8	with elastic tyres	B60B17/02	B60B17/02		236
B60B19/00	7	Wheels not otherwise provided for or having characteristics specified in one of the subgroups of this group	B60B19/00	B60B19/00		1785
B60B19/003	8	{Multidirectional wheels}	B60B19/00	B60B19/00		640
B60B19/006	8	{Magnetic wheels}	B60B19/00	B60B19/00		259
B60B19/02	8	convertible, e.g. from road wheel to rail wheel; Wheels specially designed for alternative use on road and rail	B60B19/02	B60B19/02		508
B60B19/04	8	expansible	B60B19/04	B60B19/04		284
B60B19/06	8	with compartments for fluid, packing or loading material; Buoyant wheels	B60B19/06	B60B19/06		232
B60B19/08	8	with lubricating passages, channels, or reservoirs	B60B19/08	B60B19/08		74
B60B19/10	8	with cooling fins	B60B19/10	B60B19/10		434
B60B19/12	8	Roller-type wheels (B60B19/06 takes precedence)	B60B19/12	B60B19/12		753
B60B19/125	9	{with helical projections on radial outer surface translating rotation of wheel into movement along the direction of the wheel axle}	B60B19/12	B60B19/12		262
B60B19/14	8	Ball-type wheels (B60B19/06 takes precedence)	B60B19/14	B60B19/14		367
B60B21/00	7	Rims (non-metallic B60B5/00; of high resiliency B60B9/00; capable of carrying more than one tyre B60B11/04; multiple rims on a single wheel body B60B11/06; of multi-part type B60B25/00; metal tyres B60C)	B60B21/00	B60B21/00		674
B60B21/02	8	characterised by transverse section	B60B21/02	B60B21/02		1043
B60B21/021	9	{with inwardly directed flanges, i.e. the tyre-seat being reversed}	B60B21/02	B60B21/02		166
B60B21/023	9	{the transverse section being non-symmetrical}	B60B21/02	B60B21/02		316
B60B21/025	9	{the transverse section being hollow}	B60B21/02	B60B21/02		698
B60B21/026	9	{the shape of rim well}	B60B21/02	B60B21/02		385
B60B21/028	9	{the shape of hump}	B60B21/02	B60B21/02		166
B60B21/04	9	with substantially radial flanges (with rail-engaging flanges B60B17/00){(B60B21/021 takes precedence)}	B60B21/04	B60B21/04		432
B60B21/06	8	characterised by means for attaching spokes {, i.e. spoke seats}	B60B21/06	B60B21/06		430
B60B21/062	9	{for bicycles}	B60B21/06	B60B21/06		885
B60B21/064	9	{characterised by shape of spoke mounting holes, e.g. elliptical or triangular}	B60B21/06	B60B21/06		156
B60B21/066	9	{the spoke mounting means being located on a flange oriented radially and formed on the radially inner side of the rim well}	B60B21/06	B60B21/06		143
B60B21/068	9	{the spoke seat comprising sealing means, e.g. for tubeless racing bike tyres}	B60B21/06	B60B21/06		63
B60B21/08	8	characterised by having braking surfaces	B60B21/08	B60B21/08		267
B60B21/10	8	characterised by the form of tyre-seat or flange, e.g. corrugated (B60B21/02 takes precedence)	B60B21/10	B60B21/10		642
B60B21/102	9	{the shape of bead seats}	B60B21/10	B60B21/10		244
B60B21/104	9	{the shape of flanges}	B60B21/10	B60B21/10		352
B60B21/106	10	{the shape of flange end-sections}	B60B21/10	B60B21/10		115
B60B21/108	9	{the surface of bead seats}	B60B21/10	B60B21/10		56
B60B21/12	8	Appurtenances, e.g. lining bands	B60B21/12	B60B21/12		1560
B60B21/125	9	{Bead clamping elements}	B60B21/12	B60B21/12		77
B60B23/00	7	Attaching rim to wheel body (attaching spokes to rim B60B1/04, B60B1/14; attaching rims resiliently to wheel body B60B9/00{; devices for fastening or securing constructional elements or machine parts together F16B})<br><br><u>NOTE</u><br><br>Group B60B23/12 takes precedence over groups B60B23/02&#160;-&#160;B60B23/10	B60B23/00	B60B23/00		234
B60B23/02	8	by split or other expansible ring devices	B60B23/02	B60B23/02		212
B60B23/04	8	by bayonet joint, screw-thread, or like attachments	B60B23/04	B60B23/04		788
B60B23/06	8	by screws, bolts, pins, or clips	B60B23/06	B60B23/06		177
B60B23/08	9	arranged radially	B60B23/08	B60B23/08		142
B60B23/10	9	arranged axially	B60B23/10	B60B23/10		1318
B60B23/12	8	by devices arranged to permit variation of axial position of rim relative to wheel body for track width adjustment	B60B23/12	B60B23/12		224
B60B25/00	7	Rims built-up of several main parts {; Locking means for the rim parts}(tools for assembling divided rims B60B31/04)	B60B25/00	B60B25/00		335
B60B25/002	8	{Rims split in circumferential direction}	B60B25/00	B60B25/00		292
B60B25/004	9	{one rim part comprising the wheel disc}	B60B25/00	B60B25/00		203
B60B25/006	9	{Rims split symmetrically}	B60B25/00	B60B25/00		115
B60B25/008	9	{comprising spacer means}	B60B25/00	B60B25/00		52
B60B25/02	8	Segmented rims, e.g. with segments arranged in sections; Connecting equipment, e.g. hinges; Insertable flange rings therefor	B60B25/02	B60B25/02		870
B60B25/04	8	Rims with dismountable flange rings, seat rings, or lock rings	B60B25/04	B60B25/04		411
B60B25/045	9	{on both sides}	B60B25/04	B60B25/04		83
B60B25/06	9	Split flange rings, e.g. transversely split; Connecting equipment for overlapping the slot	B60B25/06	B60B25/06		123
B60B25/08	9	Continuous flange rings; Arrangement of recesses enabling the flange rings to be slipped over the rim body	B60B25/08	B60B25/08		148
B60B25/10	9	Seat rings for the tyre bead part, e.g. split	B60B25/10	B60B25/10		80
B60B25/12	10	with integral flange part	B60B25/12	B60B25/12		189
B60B25/14	9	Locking means for flange rings or seat rings	B60B25/14	B60B25/14		188
B60B25/16	10	Arrangement of bayonet catches	B60B25/16	B60B25/16		305
B60B25/18	10	Arrangement of split rings	B60B25/18	B60B25/18		253
B60B25/20	10	Arrangement of screws, bolts, or shouldered pins	B60B25/20	B60B25/20		737
B60B25/22	8	Other apurtenances, e.g. for sealing the component parts enabling the use of tubeless tyres	B60B25/22	B60B25/22		539
B60B27/00	7	Hubs (non-metallic B60B5/00; of high resiliency B60B9/00)	B60B27/00	B60B27/00		1927
B60B27/0005	8	{with ball bearings}	B60B27/00	B60B27/00		2200
B60B27/001	8	{with roller-bearings}	B60B27/00	B60B27/00		1048
B60B27/0015	8	{for driven wheels}	B60B27/00	B60B27/00		381
B60B27/0021	9	{characterised by torque transmission means from drive axle}	B60B27/00	B60B27/00		168
B60B27/0026	10	{of the radial type, e.g. splined key}	B60B27/00	B60B27/00		445
B60B27/0031	10	{of the axial type, e.g. front teeth}	B60B27/00	B60B27/00		226
B60B27/0036	9	{comprising homokinetic joints}	B60B27/00	B60B27/00		115
B60B27/0042	10	{characterised by the fixation of the homokinetic joint to the hub}	B60B27/00	B60B27/00		265
B60B27/0047	8	{characterised by functional integration of other elements}	B60B27/00	B60B27/00		572
B60B27/0052	9	{the element being a brake disc}	B60B27/00	B60B27/00		631
B60B27/0057	9	{the element being a brake drum}	B60B27/00	B60B27/00		223
B60B27/0063	9	{the element being a brake caliper mount}	B60B27/00	B60B27/00		60
B60B27/0068	9	{the element being a sensor}	B60B27/00	B60B27/00		599
B60B27/0073	8	{characterised by sealing means}	B60B27/00	B60B27/00		975
B60B27/0078	8	{characterised by the fixation of bearings}	B60B27/00	B60B27/00		745
B60B27/0084	9	{caulking to fix inner race}	B60B27/00	B60B27/00		522
B60B27/0089	9	{caulking to fix outer race}	B60B27/00	B60B27/00		59
B60B27/0094	8	{one or more of the bearing races are formed by the hub}	B60B27/00	B60B27/00		568
B60B27/02	8	adapted to be rotatably arranged on axle	B60B27/02	B60B27/02		1302
B60B27/023	9	{specially adapted for bicycles}	B60B27/02	B60B27/02		1777
B60B27/026	10	{comprising quick release devices}	B60B27/02	B60B27/02		253
B60B27/04	9	housing driving means, e.g. sprockets	B60B27/04	B60B27/04		321
B60B27/042	10	{comprising a rotational dampers}	B60B27/04	B60B27/04		23
B60B27/045	10	{comprising a spoke protectors}	B60B27/04	B60B27/04		8
B60B27/047	10	{comprising a freewheel mechanisms}	B60B27/04	B60B27/04		384
B60B27/06	8	adapted to be fixed on axle	B60B27/06	B60B27/06		260
B60B27/065	9	{characterised by the fixation of the hub to the axle}	B60B27/06	B60B27/06		446
B60B29/00	7	Apparatus or tools for mounting or dismounting wheels {(mounting of wheels at assembly lines B62D65/12)}	B60B29/00	B60B29/00		408
B60B29/001	8	{comprising lifting or aligning means (B60B29/002 takes precedence)}	B60B29/00	B60B29/00		594
B60B29/002	8	{provided with a dolly}	B60B29/00	B60B29/00		555
B60B29/003	8	{Wrenches, e.g. of the ratchet type (B60B29/001 takes precedence; wrenches per seB25B13/00)}	B60B29/00	B60B29/00		312
B60B29/004	9	{for dual wheels}	B60B29/00	B60B29/00		13
B60B29/005	9	{hand-driven operating with multiplicated forces (B60B29/004 takes precedence; hand-driven gear-operated wrenches per seB25B17/00, with torque amplification B25B17/02)}	B60B29/00	B60B29/00		117
B60B29/006	9	{with electric or pneumatic drive (power-driven nut setting or loosening tool per seB25B21/00)}	B60B29/00	B60B29/00		154
B60B29/007	9	{Supports for wrenches (B60B29/005, B60B29/006 take precedence)}	B60B29/00	B60B29/00		97
B60B29/008	8	{Wheel pullers; tools for axial movement of wheels (adjustable axle units for varying track B60B35/10)}	B60B29/00	B60B29/00		167
B60B30/00	7	Means for holding wheels or parts thereof (spare wheel stowing, holding or mounting arrangements on vehicles B62D43/00)	B60B30/00	B60B30/00		111
B60B30/02	8	engaging the tyre, e.g. the tyre being mounted on the wheel rim	B60B30/02	B60B30/02		215
B60B30/04	9	the tyre not being mounted on a rim, i.e. holders or supports for tyres alone	B60B30/04	B60B30/04		21
B60B30/06	8	engaging the wheel body, e.g. the rim	B60B30/06	B60B30/06		196
B60B30/08	9	the central part of the wheel body	B60B30/08	B60B30/08		116
B60B30/10	8	characterised by being provided on a dolly	B60B30/10	B60B30/10		131
B60B31/00	7	Apparatus or tools for assembling or disassembling wheels	B60B31/00	B60B31/00		198
B60B31/005	8	{especially for spoked wheels}	B60B31/00	B60B31/00		476
B60B31/02	8	for tightening or straightening wire spokes in situ; for extracting spokes from wheels	B60B31/02	B60B31/02		330
B60B31/04	8	for assembling divided rims	B60B31/04	B60B31/04		25
B60B31/06	8	for removing or attaching cover discs, hub caps, or the like	B60B31/06	B60B31/06		105
B60B33/00	7	Castors in general {; Anti-clogging castors}(castors for large containers B65D90/18)	B60B33/00	B60B33/00		1640
B60B33/0002	8	{assembling to the object, e.g. furniture}	B60B33/00	B60B33/00		3067
B60B33/0005	9	{characterised by mounting method}	B60B33/00	B60B33/00		586
B60B33/0007	10	{by screwing}	B60B33/00	B60B33/00		433
B60B33/001	10	{by snapping, clicking or latching in}	B60B33/00	B60B33/00		222
B60B33/0013	10	{by straps, bands or similar}	B60B33/00	B60B33/00		9
B60B33/0015	9	{characterised by adaptations made to castor}	B60B33/00	B60B33/00		325
B60B33/0018	10	{in the form of a flat mounting plate}	B60B33/00	B60B33/00		325
B60B33/0021	10	{in the form of a mounting pin}	B60B33/00	B60B33/00		581
B60B33/0023	10	{in the form of specific adaptations to the form of the object}	B60B33/00	B60B33/00		220
B60B33/0026	9	{characterised by adaptations made to the object}	B60B33/00	B60B33/00		143
B60B33/0028	8	{Construction of wheels; methods of assembling on axle}	B60B33/00	B60B33/00		1793
B60B33/0036	8	{characterised by type of wheels}	B60B33/00	B60B33/00		82
B60B33/0039	9	{Single wheels}	B60B33/00	B60B33/00		1298
B60B33/0042	9	{Double or twin wheels}	B60B33/00	B60B33/00		1060
B60B33/0044	9	{Roller type wheels, i.e. extra wide wheels}	B60B33/00	B60B33/00		91
B60B33/0047	8	{characterised by details of the rolling axle}	B60B33/00	B60B33/00		42
B60B33/0049	9	{the rolling axle being horizontal}	B60B33/00	B60B33/00		1705
B60B33/0052	9	{the rolling axle being inclined}	B60B33/00	B60B33/00		216
B60B33/0055	9	{the rolling axle intersects swivel axis}	B60B33/00	B60B33/00		91
B60B33/0057	9	{the rolling axle being offset from swivel axis}	B60B33/00	B60B33/00		1243
B60B33/006	8	{characterised by details of the swivel mechanism}	B60B33/00	B60B33/00		191
B60B33/0063	9	{no swivelling action, i.e. no real caster}	B60B33/00	B60B33/00		443
B60B33/0065	9	{characterised by details of the swivel axis}	B60B33/00	B60B33/00		52
B60B33/0068	10	{the swivel axis being vertical}	B60B33/00	B60B33/00		1520
B60B33/0071	10	{the swivel axis being inclined}	B60B33/00	B60B33/00		56
B60B33/0073	10	{the swivel axis being symmetrical to wheel or wheels}	B60B33/00	B60B33/00		1120
B60B33/0076	10	{the swivel axis being offset laterally from wheel center plane}	B60B33/00	B60B33/00		61
B60B33/0078	8	{characterised by details of the wheel braking mechanism}	B60B33/00	B60B33/00		649
B60B33/0081	9	{acting on tyre tread}	B60B33/00	B60B33/00		616
B60B33/0084	9	{acting on axle end}	B60B33/00	B60B33/00		123
B60B33/0086	9	{acting on rim or side portion of tyre}	B60B33/00	B60B33/00		351
B60B33/0089	9	{acting on the floor}	B60B33/00	B60B33/00		425
B60B33/0092	9	{actuated remotely, e.g. by cable or electrically}	B60B33/00	B60B33/00		332
B60B33/0094	9	{actuated automatically}	B60B33/00	B60B33/00		147
B60B33/0097	9	{acting permanently, e.g. for increased security on low friction surfaces}	B60B33/00	B60B33/00		64
B60B33/02	8	with disengageable swivel action {, i.e. comprising a swivel locking mechanism}	B60B33/02	B60B33/02		511
B60B33/021	9	{combined with braking of castor wheel}	B60B33/02	B60B33/02		1287
B60B33/023	9	{by using friction}	B60B33/02	B60B33/02		113
B60B33/025	9	{by using form-fit, e.g. front teeth}	B60B33/02	B60B33/02		611
B60B33/026	9	{being actuated remotely, e.g. by cable or electrically}	B60B33/02	B60B33/02		306
B60B33/028	9	{being actuated automatically}	B60B33/02	B60B33/02		105
B60B33/04	8	adjustable {, e.g. in height; linearly shifting castors}	B60B33/04	B60B33/04		611
B60B33/045	9	{mounted resiliently, by means of dampers}	B60B33/04	B60B33/04		1047
B60B33/06	9	mounted retractably	B60B33/06	B60B33/06		1304
B60B33/063	10	{by linear movement parallel to swivel axis}	B60B33/06	B60B33/06		244
B60B33/066	10	{by use of a hinge and lever mechanism to swing wheel upwards relative to wheel mount}	B60B33/06	B60B33/06		221
B60B33/08	8	Ball castors {(B60B33/0028 takes precedence)}	B60B33/08	B60B33/08		825
B60B35/00	7	Axle units; Parts thereof (steerable vehicle stub axles B62D){; Arrangements for lubrication of axles}	B60B35/00	B60B35/00		574
B60B35/001	8	{Axles of the portal type, i.e. axles designed for higher ground clearance}	B60B35/00	B60B35/00		107
B60B35/002	8	{Axles of the low floor type, e.g. for low-floor city busses}	B60B35/00	B60B35/00		71
B60B35/003	8	{Steerable axles}	B60B35/00	B60B35/00		507
B60B35/004	8	{Mounting arrangements for axles}	B60B35/00	B60B35/00		310
B60B35/005	9	{with adaptations at chassis structure}	B60B35/00	B60B35/00		71
B60B35/006	9	{with mounting plates or consoles fitted to axles}	B60B35/00	B60B35/00		173
B60B35/007	10	{for mounting suspension elements to axles}	B60B35/00	B60B35/00		204
B60B35/008	10	{for mounting air suspension elements to axles}	B60B35/00	B60B35/00		35
B60B35/009	8	{adapted for tiltable wheels}	B60B35/00	B60B35/00		44
B60B35/02	8	Dead axles, i.e. not transmitting torque	B60B35/02	B60B35/02		420
B60B35/025	9	{the wheels being removable}	B60B35/02	B60B35/02		263
B60B35/04	9	straight	B60B35/04	B60B35/04		765
B60B35/06	9	cranked	B60B35/06	B60B35/06		210
B60B35/08	9	of closed hollow section	B60B35/08	B60B35/08		497
B60B35/10	9	adjustable for varying track {(tools for axial movement of wheels on axles B60B29/008)}	B60B35/10	B60B35/10		177
B60B35/1009	10	{operated manually}	B60B35/10	B60B35/10		95
B60B35/1018	11	{comprising a locking pin}	B60B35/10	B60B35/10		105
B60B35/1027	11	{comprising a clamping mechanism}	B60B35/10	B60B35/10		174
B60B35/1036	10	{operated with power assistance}	B60B35/10	B60B35/10		78
B60B35/1045	11	{electrically}	B60B35/10	B60B35/10		84
B60B35/1054	11	{hydraulically}	B60B35/10	B60B35/10		183
B60B35/1063	11	{automatically dependent on operational state of the vehicle}	B60B35/10	B60B35/10		32
B60B35/1072	10	{by transversally movable elements}	B60B35/10	B60B35/10		79
B60B35/1081	11	{the element is a wheel}	B60B35/10	B60B35/10		196
B60B35/109	11	{the element is an axle part}	B60B35/10	B60B35/10		343
B60B35/12	8	Torque-transmitting axles (independent suspension aspects B60G)	B60B35/12	B60B35/12		862
B60B35/121	9	{Power-transmission from drive shaft to hub}	B60B35/12	B60B35/12		328
B60B35/122	10	{using gearings}	B60B35/12	B60B35/12		510
B60B35/124	11	{of the helical or worm type}	B60B35/12	B60B35/12		42
B60B35/125	11	{of the planetary type}	B60B35/12	B60B35/12		439
B60B35/127	10	{using universal joints}	B60B35/12	B60B35/12		66
B60B35/128	11	{of the homokinetic or constant velocity type}	B60B35/12	B60B35/12		132
B60B35/14	9	composite or split, e.g. half- axles; Couplings between axle parts or sections	B60B35/14	B60B35/14		1384
B60B35/16	9	Axle housings	B60B35/16	B60B35/16		935
B60B35/163	10	{characterised by specific shape of the housing, e.g. adaptations to give space for other vehicle elements like chassis or exhaust system}	B60B35/16	B60B35/16		446
B60B35/166	10	{characterised by reinforcements, e.g. reinforcement ribs}	B60B35/16	B60B35/16		111
B60B35/18	9	Arrangement of bearings	B60B35/18	B60B35/18		736
B60B37/00	7	Wheel-axle combinations, e.g. wheel sets (units comprising multiple wheels arranged side-by-side B60B11/00; rail vehicle axle-boxes B61F)	B60B37/00	B60B37/00		459
B60B37/02	8	the wheels being integral with solid axles	B60B37/02	B60B37/02		22
B60B37/04	8	the wheels being rigidly attached to solid axles	B60B37/04	B60B37/04		468
B60B37/06	8	the wheels being integral with, or rigidly attached to, hollow axles	B60B37/06	B60B37/06		154
B60B37/08	9	the hollow axles being rotatable around fixed axles	B60B37/08	B60B37/08		38
B60B37/10	8	the wheels being individually rotatable around the axles	B60B37/10	B60B37/10		1861
B60B37/12	8	Axles with a fixed ground wheel and a loose wheel	B60B37/12	B60B37/12		11
B60B39/00	7	Increasing wheel adhesion (wheels, wheel attachments or tyre attachments, designed for increasing traction B60B15/00, B60C; tyre constructions B60C; road surface conditioning to prevent slipperiness E01C)	B60B39/00	B60B39/00		668
B60B39/003	8	{Vehicle mounted non-skid chains actuated by centrifugal force (non-skid devices temporarily attachable to resilient tyres B60C27/00)}	B60B39/00	B60B39/00		146
B60B39/006	9	{characterised by a control system for the actuation of the rotating chain wheel}	B60B39/00	B60B39/00		93
B60B39/02	8	Vehicle fittings for scattering or dispensing material in front of its wheels	B60B39/02	B60B39/02		111
B60B39/021	9	{Details of the dispensing device}	B60B39/02	B60B39/02		95
B60B39/022	10	{related to reservoirs}	B60B39/02	B60B39/02		53
B60B39/023	10	{related to metering valves}	B60B39/02	B60B39/02		86
B60B39/024	10	{related to preconditioning of the dispensing materials}	B60B39/02	B60B39/02		49
B60B39/025	10	{related to the control system}	B60B39/02	B60B39/02		152
B60B39/026	9	{the material being in gas form}	B60B39/02	B60B39/02		128
B60B39/027	10	{the gas being heated on purpose}	B60B39/02	B60B39/02		30
B60B39/028	10	{the gas being exhaust gas}	B60B39/02	B60B39/02		44
B60B39/04	9	the material being granular, e.g. sand (combined control of sanding apparatus and brakes of rail vehicles B61H)	B60B39/04	B60B39/04		622
B60B39/06	10	the dispensing being effected by mechanical means	B60B39/06	B60B39/06		255
B60B39/08	10	the dispensing being effected by fluid means	B60B39/08	B60B39/08		19
B60B39/083	11	{dispensing being effected by liquid}	B60B39/08	B60B39/08		16
B60B39/086	11	{dispensing being effected by gas}	B60B39/08	B60B39/08		230
B60B39/10	10	the dispensing being controlled electrically or electromagnetically	B60B39/10	B60B39/10		217
B60B39/12	9	the material being sheet-like or web-like	B60B39/12	B60B39/12		427
B60B2200/00	7	Type of product being used or applied	CPCONLY	B60B2200/00		65
B60B2200/20	8	Furniture or medical appliances	CPCONLY	B60B2200/20		572
B60B2200/22	9	Chairs	CPCONLY	B60B2200/22		167
B60B2200/222	10	Office chairs	CPCONLY	B60B2200/222		28
B60B2200/224	10	Arm chairs	CPCONLY	B60B2200/224		11
B60B2200/24	9	Beds	CPCONLY	B60B2200/24		53
B60B2200/242	10	Hospital beds	CPCONLY	B60B2200/242		166
B60B2200/26	9	Medical appliances	CPCONLY	B60B2200/26		191
B60B2200/40	8	Articles of daily use	CPCONLY	B60B2200/40		99
B60B2200/41	9	Waste bins	CPCONLY	B60B2200/41		46
B60B2200/43	9	Carts	CPCONLY	B60B2200/43		423
B60B2200/432	10	Shopping carts	CPCONLY	B60B2200/432		190
B60B2200/434	10	Wheel barrows	CPCONLY	B60B2200/434		132
B60B2200/45	9	Suitcases	CPCONLY	B60B2200/45		190
B60B2200/47	9	Physical activity equipment, e.g. leisure or sports articles	CPCONLY	B60B2200/47		145
B60B2200/49	9	Domestic appliances, e.g. vacuum cleaners	CPCONLY	B60B2200/49		125
B60B2310/00	7	Manufacturing methods	CPCONLY	B60B2310/00		21
B60B2310/20	8	Shaping	CPCONLY	B60B2310/20		90
B60B2310/202	9	by casting	CPCONLY	B60B2310/202		247
B60B2310/204	9	by moulding, e.g. injection moulding, i.e. casting of plastics material	CPCONLY	B60B2310/204		363
B60B2310/206	9	by stamping	CPCONLY	B60B2310/206		261
B60B2310/208	9	by forging	CPCONLY	B60B2310/208		215
B60B2310/2082	10	by swaging	CPCONLY	B60B2310/2082		45
B60B2310/211	9	by folding or bending	CPCONLY	B60B2310/211		89
B60B2310/212	9	by drawing	CPCONLY	B60B2310/212		44
B60B2310/213	9	by punching	CPCONLY	B60B2310/213		58
B60B2310/214	9	by extrusion	CPCONLY	B60B2310/214		56
B60B2310/218	9	by hydroforming	CPCONLY	B60B2310/218		11
B60B2310/221	9	by magnetic pulse forming	CPCONLY	B60B2310/221		2
B60B2310/222	9	by twisting	CPCONLY	B60B2310/222		3
B60B2310/224	9	by rolling	CPCONLY	B60B2310/224		87
B60B2310/226	9	by cutting	CPCONLY	B60B2310/226		106
B60B2310/228	9	by machining	CPCONLY	B60B2310/228		159
B60B2310/231	9	by turning	CPCONLY	B60B2310/231		24
B60B2310/232	9	by milling	CPCONLY	B60B2310/232		39
B60B2310/234	9	by grinding	CPCONLY	B60B2310/234		35
B60B2310/238	9	by thermal spraying of molten material	CPCONLY	B60B2310/238		5
B60B2310/241	9	by weaving or knitting of fibers	CPCONLY	B60B2310/241		19
B60B2310/242	9	by laminating, e.g. fabrication of sandwich sheets	CPCONLY	B60B2310/242		52
B60B2310/30	8	joining	CPCONLY	B60B2310/30		53
B60B2310/302	9	by welding	CPCONLY	B60B2310/302		698
B60B2310/3021	10	by autogen welding	CPCONLY	B60B2310/3021		2
B60B2310/3022	10	by spot welding, plug welding	CPCONLY	B60B2310/3022		35
B60B2310/3023	10	by arc welding, e.g. inert gas arc welding	CPCONLY	B60B2310/3023		35
B60B2310/3025	10	by thermal welding, e.g. friction, induction or ultrasonic welding	CPCONLY	B60B2310/3025		79
B60B2310/3026	10	by laser welding	CPCONLY	B60B2310/3026		35
B60B2310/3027	10	by electron beam welding	CPCONLY	B60B2310/3027		11
B60B2310/3028	10	by magnetic pulse welding	CPCONLY	B60B2310/3028		1
B60B2310/303	9	by soldering	CPCONLY	B60B2310/303		24
B60B2310/305	9	by screwing	CPCONLY	B60B2310/305		1619
B60B2310/306	9	by clamping or wedging, e.g. by clamping inserts as joining means	CPCONLY	B60B2310/306		401
B60B2310/307	9	by removably mountable securing elements, e.g. circlips	CPCONLY	B60B2310/307		147
B60B2310/311	9	by riveting	CPCONLY	B60B2310/311		132
B60B2310/3112	10	by punch-riveting	CPCONLY	B60B2310/3112		
B60B2310/312	9	by hemming or seaming, e.g. by folding of the rim	CPCONLY	B60B2310/312		7
B60B2310/314	9	by deformation	CPCONLY	B60B2310/314		29
B60B2310/3142	9	by caulking	CPCONLY	B60B2310/3142		16
B60B2310/316	9	by press-fitting, shrink-fitting	CPCONLY	B60B2310/316		225
B60B2310/318	9	by adhesive bonding, e.g. glueing	CPCONLY	B60B2310/318		264
B60B2310/321	9	by overmolding	CPCONLY	B60B2310/321		107
B60B2310/323	9	by coextrusion	CPCONLY	B60B2310/323		6
B60B2310/329	9	by splicing, e.g. of ropes	CPCONLY	B60B2310/329		3
B60B2310/50	8	Thermal treatment	CPCONLY	B60B2310/50		51
B60B2310/52	9	Curing	CPCONLY	B60B2310/52		37
B60B2310/54	9	Hardening	CPCONLY	B60B2310/54		56
B60B2310/542	10	Quenching	CPCONLY	B60B2310/542		30
B60B2310/56	9	Co-curing; Vulcanisation	CPCONLY	B60B2310/56		54
B60B2310/60	8	Surface treatment; After treatment	CPCONLY	B60B2310/60		41
B60B2310/612	9	Polishing	CPCONLY	B60B2310/612		30
B60B2310/614	9	Painting	CPCONLY	B60B2310/614		48
B60B2310/616	9	Coating with thin films	CPCONLY	B60B2310/616		79
B60B2310/6162	10	Conductive films	CPCONLY	B60B2310/6162		3
B60B2310/618	9	Coating with foils	CPCONLY	B60B2310/618		21
B60B2310/621	9	Electro-chemical processes	CPCONLY	B60B2310/621		22
B60B2310/622	9	Shot-peening	CPCONLY	B60B2310/622		7
B60B2310/64	9	Effect of treatments	CPCONLY	B60B2310/64		3
B60B2310/642	10	Matted	CPCONLY	B60B2310/642		
B60B2310/644	10	Polished	CPCONLY	B60B2310/644		4
B60B2310/646	10	Engraved	CPCONLY	B60B2310/646		4
B60B2310/648	10	Structured	CPCONLY	B60B2310/648		6
B60B2310/651	10	glossy	CPCONLY	B60B2310/651		4
B60B2310/652	10	Reflecting	CPCONLY	B60B2310/652		9
B60B2310/654	10	Anti-corrosive	CPCONLY	B60B2310/654		20
B60B2310/656	10	Decorative	CPCONLY	B60B2310/656		36
B60B2310/658	10	For advertising	CPCONLY	B60B2310/658		20
B60B2310/661	10	for protection, e.g. against scratches or stone chips	CPCONLY	B60B2310/661		12
B60B2310/80	8	Filament winding	CPCONLY	B60B2310/80		27
B60B2320/00	7	Manufacturing or maintenance operations	CPCONLY	B60B2320/00		13
B60B2320/10	8	Assembling; disassembling	CPCONLY	B60B2320/10		440
B60B2320/12	9	Assembly devices for spoked wheels	CPCONLY	B60B2320/12		29
B60B2320/122	10	for spoke tensioning	CPCONLY	B60B2320/122		12
B60B2320/124	10	for trueing of spoked wheels	CPCONLY	B60B2320/124		3
B60B2320/126	10	for restoring form or removing local distortions of wheel rims in unassembled state	CPCONLY	B60B2320/126		1
B60B2320/14	9	Assembly devices for divided rims	CPCONLY	B60B2320/14		20
B60B2320/16	9	Devices for attaching or removing cover discs, hub caps or other ornamental rings or elements	CPCONLY	B60B2320/16		20
B60B2320/30	8	Balancing	CPCONLY	B60B2320/30		21
B60B2320/50	8	Securing	CPCONLY	B60B2320/50		193
B60B2320/52	9	to prevent loss	CPCONLY	B60B2320/52		20
B60B2320/522	10	by locking washer	CPCONLY	B60B2320/522		17
B60B2320/524	10	by securing plate	CPCONLY	B60B2320/524		4
B60B2340/00	7	Wheel transporting, Mounting of wheels	CPCONLY	B60B2340/00		4
B60B2340/10	8	Operation mode	CPCONLY	B60B2340/10		
B60B2340/12	9	Operated manually	CPCONLY	B60B2340/12		29
B60B2340/14	9	Power driven	CPCONLY	B60B2340/14		26
B60B2340/16	9	Included in assembly line	CPCONLY	B60B2340/16		1
B60B2340/18	9	Automated process	CPCONLY	B60B2340/18		16
B60B2340/30	8	Wheel transporting or handling devices	CPCONLY	B60B2340/30		18
B60B2340/32	9	for gripping the wheel	CPCONLY	B60B2340/32		37
B60B2340/34	9	for positioning the wheel to hub or boltholes	CPCONLY	B60B2340/34		29
B60B2340/36	9	the devices being provided on a dolly	CPCONLY	B60B2340/36		26
B60B2340/50	8	Wheel mounting or removal devices	CPCONLY	B60B2340/50		69
B60B2340/52	9	Auxiliary tools, e.g. For alignment	CPCONLY	B60B2340/52		52
B60B2340/70	8	Lifting jacks	CPCONLY	B60B2340/70		22
B60B2360/00	7	Materials; Physical forms thereof	CPCONLY	B60B2360/00		17
B60B2360/10	8	Metallic materials	CPCONLY	B60B2360/10		903
B60B2360/102	9	Steel	CPCONLY	B60B2360/102		626
B60B2360/104	9	Aluminum	CPCONLY	B60B2360/104		440
B60B2360/106	9	Magnesia	CPCONLY	B60B2360/106		49
B60B2360/108	9	Titanium	CPCONLY	B60B2360/108		31
B60B2360/109	9	Bronze	CPCONLY	B60B2360/109		20
B60B2360/14	8	Physical forms of metallic parts	CPCONLY	B60B2360/14		6
B60B2360/141	9	Sheet-metals	CPCONLY	B60B2360/141		239
B60B2360/143	9	Bars, i.e. being solid	CPCONLY	B60B2360/143		4
B60B2360/1432	10	of circular cross section	CPCONLY	B60B2360/1432		6
B60B2360/1434	10	of polygonal cross section, e.g. triangular or rectangular	CPCONLY	B60B2360/1434		10
B60B2360/1436	10	of elliptical cross section	CPCONLY	B60B2360/1436		
B60B2360/144	9	Tubes, i.e. being hollow	CPCONLY	B60B2360/144		9
B60B2360/1442	10	of circular cross section	CPCONLY	B60B2360/1442		44
B60B2360/1444	10	of rectangular cross section	CPCONLY	B60B2360/1444		25
B60B2360/1446	10	of elliptical cross section	CPCONLY	B60B2360/1446		2
B60B2360/1448	10	of irregular cross-section	CPCONLY	B60B2360/1448		4
B60B2360/145	9	Profiles, i.e. being solid and having irregular cross-section	CPCONLY	B60B2360/145		6
B60B2360/1452	10	L-profiles	CPCONLY	B60B2360/1452		5
B60B2360/1454	10	T or H-Profiles	CPCONLY	B60B2360/1454		12
B60B2360/1456	10	X or Y-Profiles	CPCONLY	B60B2360/1456		5
B60B2360/1458	10	U or V-Profiles	CPCONLY	B60B2360/1458		45
B60B2360/147	9	Castings	CPCONLY	B60B2360/147		103
B60B2360/148	9	Sinterings	CPCONLY	B60B2360/148		2
B60B2360/149	9	Metal foams	CPCONLY	B60B2360/149		8
B60B2360/30	8	Synthetic materials	CPCONLY	B60B2360/30		116
B60B2360/32	9	Plastic compositions	CPCONLY	B60B2360/32		441
B60B2360/322	10	Comprising polypropylene	CPCONLY	B60B2360/322		44
B60B2360/324	10	Comprising polyurethane	CPCONLY	B60B2360/324		114
B60B2360/33	9	Synthetic foams	CPCONLY	B60B2360/33		13
B60B2360/34	9	Reinforced plastics	CPCONLY	B60B2360/34		56
B60B2360/341	10	with fibres	CPCONLY	B60B2360/341		192
B60B2360/3412	11	Glass fibres	CPCONLY	B60B2360/3412		93
B60B2360/3414	11	Aramide fibres	CPCONLY	B60B2360/3414		22
B60B2360/3416	11	Carbone fibres	CPCONLY	B60B2360/3416		237
B60B2360/3418	11	Aramid fibres	CPCONLY	B60B2360/3418		23
B60B2360/342	10	With strands	CPCONLY	B60B2360/342		10
B60B2360/3422	11	consisting of fibres oriented substantially parallel	CPCONLY	B60B2360/3422		4
B60B2360/3424	11	consisting of braided fibres	CPCONLY	B60B2360/3424		3
B60B2360/344	10	With woven material	CPCONLY	B60B2360/344		19
B60B2360/3442	11	characterised by material mixes	CPCONLY	B60B2360/3442		1
B60B2360/3444	11	characterised by weaving patterns	CPCONLY	B60B2360/3444		2
B60B2360/346	10	Material impregnated with resin before being put into form, i.e. prepregs	CPCONLY	B60B2360/346		13
B60B2360/3462	11	comprising strands	CPCONLY	B60B2360/3462		3
B60B2360/3464	11	comprising woven material	CPCONLY	B60B2360/3464		4
B60B2360/348	10	Resins	CPCONLY	B60B2360/348		69
B60B2360/36	9	Composite materials	CPCONLY	B60B2360/36		116
B60B2360/362	10	Compounded sheets	CPCONLY	B60B2360/362		19
B60B2360/364	10	comprising honeycomb structures	CPCONLY	B60B2360/364		4
B60B2360/366	10	comprising foams, e.g. synthetic or metal foams	CPCONLY	B60B2360/366		19
B60B2360/368	10	Coproduced material combinations, e.g. By over-molding, co-extrusion, co-curing or vulcanizing	CPCONLY	B60B2360/368		27
B60B2360/50	8	Rubbers	CPCONLY	B60B2360/50		431
B60B2360/70	8	Ceramics	CPCONLY	B60B2360/70		29
B60B2360/90	8	Wood	CPCONLY	B60B2360/90		36
B60B2360/92	8	Leather	CPCONLY	B60B2360/92		13
B60B2360/94	8	Cardboard or papers	CPCONLY	B60B2360/94		9
B60B2380/00	7	Bearings	CPCONLY	B60B2380/00		99
B60B2380/10	8	Type	CPCONLY	B60B2380/10		10
B60B2380/12	9	Ball bearings	CPCONLY	B60B2380/12		459
B60B2380/14	9	Roller bearings	CPCONLY	B60B2380/14		343
B60B2380/16	9	Needle bearings	CPCONLY	B60B2380/16		25
B60B2380/18	9	Plain or sleeve bearings	CPCONLY	B60B2380/18		44
B60B2380/20	9	Linear bearings	CPCONLY	B60B2380/20		5
B60B2380/22	9	Magnetic bearings	CPCONLY	B60B2380/22		11
B60B2380/30	8	Cage	CPCONLY	B60B2380/30		10
B60B2380/32	9	Without cage	CPCONLY	B60B2380/32		6
B60B2380/40	8	Modularity	CPCONLY	B60B2380/40		1
B60B2380/42	9	Single-piece	CPCONLY	B60B2380/42		2
B60B2380/44	9	Multi-piece	CPCONLY	B60B2380/44		13
B60B2380/50	8	Load bearing capacity	CPCONLY	B60B2380/50		16
B60B2380/60	8	Rolling elements	CPCONLY	B60B2380/60		7
B60B2380/62	9	Specific number	CPCONLY	B60B2380/62		3
B60B2380/64	9	Specific shape	CPCONLY	B60B2380/64		7
B60B2380/70	8	Arrangements	CPCONLY	B60B2380/70		26
B60B2380/71	9	Single track	CPCONLY	B60B2380/71		6
B60B2380/73	9	Double track	CPCONLY	B60B2380/73		97
B60B2380/75	9	Twin or multiple bearings having identical diameters	CPCONLY	B60B2380/75		38
B60B2380/76	9	Twin or multiple bearings having different diameters	CPCONLY	B60B2380/76		18
B60B2380/77	9	Diameters of bearings at opposite ends of hub	CPCONLY	B60B2380/77		
B60B2380/772	10	Identical diameters of bearings at opposite ends of hub	CPCONLY	B60B2380/772		11
B60B2380/774	10	Different diameters of bearings at opposite ends of hub	CPCONLY	B60B2380/774		7
B60B2380/80	8	Shafts specially adapted to receive bearings	CPCONLY	B60B2380/80		12
B60B2380/82	9	Caulked to fix race	CPCONLY	B60B2380/82		13
B60B2380/90	8	Casings or housings specially adapted to receive bearings	CPCONLY	B60B2380/90		26
B60B2380/92	9	Caulked to fix race	CPCONLY	B60B2380/92		4
B60B2900/00	7	Purpose of invention	CPCONLY	B60B2900/00		7
B60B2900/10	8	Reduction of	CPCONLY	B60B2900/10		11
B60B2900/111	9	Weight	CPCONLY	B60B2900/111		787
B60B2900/112	9	Costs	CPCONLY	B60B2900/112		633
B60B2900/113	9	Production or maintenance time	CPCONLY	B60B2900/113		569
B60B2900/114	9	Size	CPCONLY	B60B2900/114		122
B60B2900/115	9	Complexity	CPCONLY	B60B2900/115		289
B60B2900/116	9	Product variety, e.g. by standardisation or use of adapters	CPCONLY	B60B2900/116		143
B60B2900/121	9	Resisting forces	CPCONLY	B60B2900/121		29
B60B2900/1212	10	due to friction	CPCONLY	B60B2900/1212		110
B60B2900/1214	10	due to inertia	CPCONLY	B60B2900/1214		9
B60B2900/1216	10	due to air-drag	CPCONLY	B60B2900/1216		252
B60B2900/131	9	Vibrations	CPCONLY	B60B2900/131		477
B60B2900/133	9	Noise	CPCONLY	B60B2900/133		601
B60B2900/141	9	Corrosions	CPCONLY	B60B2900/141		103
B60B2900/20	8	Avoidance of	CPCONLY	B60B2900/20		31
B60B2900/211	9	Soiling	CPCONLY	B60B2900/211		281
B60B2900/212	9	Damage	CPCONLY	B60B2900/212		549
B60B2900/30	8	Increase in	CPCONLY	B60B2900/30		12
B60B2900/311	9	Rigidity or stiffness	CPCONLY	B60B2900/311		631
B60B2900/313	9	Resiliency	CPCONLY	B60B2900/313		221
B60B2900/321	9	Lifetime	CPCONLY	B60B2900/321		617
B60B2900/323	9	Timespan between services	CPCONLY	B60B2900/323		28
B60B2900/325	9	Reliability	CPCONLY	B60B2900/325		399
B60B2900/331	9	Safety or security	CPCONLY	B60B2900/331		255
B60B2900/3312	10	during regular use	CPCONLY	B60B2900/3312		357
B60B2900/3313	10	during maintenance	CPCONLY	B60B2900/3313		34
B60B2900/3314	10	during production or assembly	CPCONLY	B60B2900/3314		37
B60B2900/3315	10	by avoiding misuse	CPCONLY	B60B2900/3315		20
B60B2900/3316	10	by indicating wear, failure or loss	CPCONLY	B60B2900/3316		79
B60B2900/3318	10	by theft prevention	CPCONLY	B60B2900/3318		106
B60B2900/351	9	versatility, e.g. usable for different purposes or different arrangements	CPCONLY	B60B2900/351		430
B60B2900/50	8	Improvement of	CPCONLY	B60B2900/50		20
B60B2900/511	9	Sealing	CPCONLY	B60B2900/511		171
B60B2900/5112	10	against dust or dirt	CPCONLY	B60B2900/5112		220
B60B2900/5114	10	against humidity or water	CPCONLY	B60B2900/5114		108
B60B2900/5116	10	against air-loss	CPCONLY	B60B2900/5116		51
B60B2900/5118	10	against oil-loss	CPCONLY	B60B2900/5118		76
B60B2900/513	9	Cooling, e.g. of brakes	CPCONLY	B60B2900/513		385
B60B2900/521	9	Tyre mounting or removal (devices therefor B60B2340/50)	CPCONLY	B60B2900/521		127
B60B2900/523	9	Tyre fixation on rim, e.g. fixing axially or circumferentially thereon	CPCONLY	B60B2900/523		87
B60B2900/531	9	User-friendliness	CPCONLY	B60B2900/531		268
B60B2900/541	9	Servicing	CPCONLY	B60B2900/541		393
B60B2900/551	9	Handling of obstacles or difficult terrains	CPCONLY	B60B2900/551		429
B60B2900/561	9	Lubrication	CPCONLY	B60B2900/561		230
B60B2900/571	9	Visibility	CPCONLY	B60B2900/571		57
B60B2900/572	9	Visual appearance	CPCONLY	B60B2900/572		331
B60B2900/70	8	Adaptation for	CPCONLY	B60B2900/70		7
B60B2900/711	9	High loads, e.g. by reinforcements	CPCONLY	B60B2900/711		112
B60B2900/721	9	Use under adverse external conditions	CPCONLY	B60B2900/721		292
B60B2900/731	9	Use in cases of damage, failure or emergency	CPCONLY	B60B2900/731		159
B60B2900/90	8	Providing or changing	CPCONLY	B60B2900/90		8
B60B2900/911	9	Eccentricity	CPCONLY	B60B2900/911		55
B60B2900/921	9	Conductivity	CPCONLY	B60B2900/921		31
B60B2900/931	9	Magnetic effects	CPCONLY	B60B2900/931		90
