E03D1/00	7	Water flushing devices with cisterns {; Setting up a range of flushing devices or water-closets; Combinations of several flushing devices}	E03D1/00	E03D1/00		865
E03D1/003	8	{Cisterns in combination with wash-basins, urinals, or the like (domestic plumbing installations E03C)}	E03D1/00	E03D1/00		765
E03D1/006	8	{Realisations of and provisions for preventing "sweating" of cisterns}	E03D1/00	E03D1/00		74
E03D1/01	8	Shape or selection of material for flushing cisterns	E03D1/01	E03D1/01		400
E03D1/012	9	Details of shape of cisterns, e.g. for connecting to wall, for supporting or connecting flushing-device actuators {(mounting frames with incorporated cisterns E03D11/146)}	E03D1/012	E03D1/012		635
E03D1/0125	10	{of built-in cisterns}	E03D1/012	E03D1/012		186
E03D1/02	8	High-level flushing systems	E03D1/02	E03D1/02		55
E03D1/025	9	{Cisterns with floats actuating the flushing}	E03D1/02	E03D1/02		18
E03D1/04	9	Cisterns with bell siphons	E03D1/04	E03D1/04		55
E03D1/05	10	with movable siphon bells	E03D1/05	E03D1/05		197
E03D1/053	11	{which are pushed upwards by means of own buoyancy, springs, counterweights, or the like}	E03D1/05	E03D1/05		54
E03D1/056	11	{providing an air lock}	E03D1/05	E03D1/05		41
E03D1/06	9	Cisterns with tube siphons	E03D1/06	E03D1/06		76
E03D1/07	10	with movable or deformable siphon tubes	E03D1/07	E03D1/07		94
E03D1/08	10	Siphon action initiated by air or water pressure {(actuating mechanisms therefor E03D5/024)}	E03D1/08	E03D1/08		169
E03D1/082	11	{in tube siphons}	E03D1/08	E03D1/08		87
E03D1/085	12	{by injection of air or water in the short leg of the siphon}	E03D1/08	E03D1/08		221
E03D1/087	12	{by pump, valve, or the like, in the short leg of the siphon or a vacuum pump in the long leg of the siphon}	E03D1/08	E03D1/08		153
E03D1/10	10	Siphon action initiated by raising the water level in the cistern, e.g. by means of displacement members	E03D1/10	E03D1/10		67
E03D1/105	11	{in cisterns with tube siphons}	E03D1/10	E03D1/10		88
E03D1/12	10	Siphon action initiated by outlet of air	E03D1/12	E03D1/12		65
E03D1/125	11	{in cisterns with tube siphons}	E03D1/12	E03D1/12		84
E03D1/14	9	Cisterns discharging variable quantities of water (twin or multiple flushing cisterns E03D1/22; flushing devices operated by pressure of the water supply system and discharging variable quantities of water E03D3/12){also cisterns with bell siphons in combination with flushing valves}	E03D1/14	E03D1/14		720
E03D1/141	10	{in cisterns with tube siphons and with tube siphons in combination with flushing valves}	E03D1/14	E03D1/14		144
E03D1/142	10	{in cisterns with flushing valves}	E03D1/14	E03D1/14		829
E03D1/144	11	{having a single flush outlet and an additional float for delaying the valve closure}	E03D1/14	E03D1/14		345
E03D1/145	11	{having multiple flush outlets}	E03D1/14	E03D1/14		376
E03D2001/147	10	{having provisions for active interruption of flushing}	E03D1/14	E03D1/14		135
E03D2001/148	11	{with means to prevent premature closing of flushing valve}	E03D1/14	E03D1/14		34
E03D1/16	9	Cisterns for periodical discharge	E03D1/16	E03D1/16		65
E03D1/165	10	{with bell or tube siphons}	E03D1/16	E03D1/16		135
E03D1/18	9	Cisterns empty when not in action {, e.g. with pressure tanks, with swivel-mounted cisterns}	E03D1/18	E03D1/18		79
E03D1/183	10	{with bell or tube siphons}	E03D1/18	E03D1/18		46
E03D1/186	10	{with flushing valves}	E03D1/18	E03D1/18		116
E03D1/20	9	Cisterns with tiltably-mounted containers {(for operation, e.g. by the seat E03D5/04)}	E03D1/20	E03D1/20		128
E03D1/22	9	Twin or multiple flushing cisterns	E03D1/22	E03D1/22		303
E03D1/24	8	Low-level flushing systems	E03D1/24	E03D1/24		118
E03D1/26	9	Bowl with flushing cistern mounted on the rearwardly extending end of the bowl (shape or material of the cistern E03D1/01; constructional features of the bowl E03D11/02&#160;-&#160;E03D11/12)	E03D1/26	E03D1/26		320
E03D1/263	10	{provided with a bell or tube siphon}	E03D1/26	E03D1/26		41
E03D1/266	10	{exclusively provided with flushing valves as flushing mechanisms}	E03D1/26	E03D1/26		118
E03D1/28	9	Bowl integral with the flushing cistern	E03D1/28	E03D1/28		142
E03D1/283	10	{provided with a bell or tube siphon}	E03D1/28	E03D1/28		34
E03D1/286	10	{provided with flushing valves}	E03D1/28	E03D1/28		170
E03D1/30	8	Valves for high or low level cisterns; Their arrangement (inlet valves, valves in general F16K){; Flushing mechanisms in the cistern, optionally with provisions for a pre-or a post- flushing and for cutting off the flushing mechanism in case of leakage (flushing valves E03D1/142, E03D1/186, E03D1/266, E03D1/286)}	E03D1/30	E03D1/30		722
E03D1/302	9	{with valves kept in open position by means of air or water pressure or by vacuum}	E03D1/30	E03D1/30		208
E03D1/304	9	{with valves with own buoyancy}	E03D1/30	E03D1/30		330
E03D1/306	10	{with articulated valves}	E03D1/30	E03D1/30		271
E03D1/308	9	{with articulated valves (E03D1/306 takes precedence)}	E03D1/30	E03D1/30		167
E03D1/32	9	Arrangement of inlet valves (devices for reducing noise E03D9/14{; noise-reducing means E03D11/00})	E03D1/32	E03D1/32		1211
E03D1/33	9	Adaptations or arrangements of floats (actuating-floats in general F16K33/00)	E03D1/33	E03D1/33		732
E03D1/34	9	Flushing valves for outlets; Arrangement of outlet valves	E03D1/34	E03D1/34		2124
E03D1/35	10	Flushing valves having buoyancy	E03D1/35	E03D1/35		343
E03D1/36	9	Associated working of inlet and outlet valves	E03D1/36	E03D1/36		391
E03D1/38	8	Adaptations or arrangements of flushing pipes (noise-absorbing means in pipe systems F16L55/00{; noise-reducing means in the flushing mechanism not in combination with flushing valves E03D11/00; provisions in the flushing pipe for evacuating leakage water from the cistern})	E03D1/38	E03D1/38		554
E03D3/00	7	Flushing devices operated by pressure of the water supply system {flushing valves not connected to the water-supply main, also if air is blown in the water seal for a quick flushing}	E03D3/00	E03D3/00		340
E03D3/02	8	Self-closing flushing valves (self-closing valves in general F16K21/04)	E03D3/02	E03D3/02		266
E03D3/04	9	with piston valve and pressure chamber for retarding the valve-closing movement	E03D3/04	E03D3/04		796
E03D3/06	9	with diaphragm valve and pressure chamber for retarding the valve-closing movement	E03D3/06	E03D3/06		315
E03D3/08	9	with other retarding devices	E03D3/08	E03D3/08		55
E03D3/10	8	Flushing devices with pressure-operated reservoir, e.g. air chamber	E03D3/10	E03D3/10		981
E03D3/12	8	Flushing devices discharging variable quantities of water (flushing cisterns discharging variable quantities of water E03D1/14)	E03D3/12	E03D3/12		421
E03D5/00	7	Special constructions of flushing devices (in motor vehicles or trailers B60R15/00; in railway carriages B61D35/00; in ships B63B29/14; in aircraft B64D11/02), {e.g. closed flushing system}	E03D5/00	E03D5/00		797
E03D5/003	8	{Grey water flushing systems}	E03D5/00	E03D5/00		593
E03D5/006	9	{Constructional details of cisterns for using greywater}	E03D5/00	E03D5/00		288
E03D5/01	8	using flushing pumps	E03D5/01	E03D5/01		660
E03D5/012	8	combined with movable closure elements in the bowl outlet (bowls with closure elements between bottom or outlet and outlet pipe E03D11/10)	E03D5/012	E03D5/012		549
E03D5/014	9	with devices for separate removal of liquids and solids	E03D5/014	E03D5/014		113
E03D5/016	8	with recirculation of bowl-cleaning fluid	E03D5/016	E03D5/016		315
E03D5/02	8	operated mechanically or hydraulically (E03D5/01, E03D5/12 take precedence){(or pneumatically) also details such as push buttons, levers and pull-card therefor}	E03D5/02	E03D5/02		321
E03D5/022	9	{Operating automatically (E03D5/10 takes precedence)}	E03D5/02	E03D5/02		260
E03D5/024	9	{Operated hydraulically or pneumatically}	E03D5/02	E03D5/02		400
E03D5/026	9	{Devices preventing overflow or locks inhibiting the use of the flushing system (devices preventing overflow of the bowl contents and seals for the bowl outlet E03D11/00); Devices preventing sucking-up of sealing and flushing water}	E03D5/02	E03D5/02		123
E03D5/028	9	{Pusher plates and actuating mechanisms for built-in cisterns}	E03D5/02	E03D5/02		213
E03D5/04	9	directly by the seat or cover {combined with devices for opening and closing shutters in the bowl outlet and/or with devices for raising and lowering seat or cover; Raising or lowering seat and/or cover by flushing or by the flushing mechanism}	E03D5/04	E03D5/04		674
E03D5/06	9	directly by the door	E03D5/06	E03D5/06		64
E03D5/08	9	directly by the foot {combined with devices for opening or closing shutters in the bowl outlet and/or with devices for raising or lowering seat and cover and/or for swiveling the bowl}	E03D5/08	E03D5/08		472
E03D5/09	9	directly by the hand	E03D5/09	E03D5/09		734
E03D5/092	10	the flushing element, e.g. siphon bell, being actuated through a lever	E03D5/092	E03D5/092		740
E03D5/094	10	the flushing element, e.g. siphon bell, being actuated through a cable, chain or the like	E03D5/094	E03D5/094		201
E03D5/10	8	operated electrically (E03D5/01, E03D5/12 take precedence), {e.g. by a photo-cell; also combined with devices for opening or closing shutters in the bowl outlet and/or with devices for raising/or lowering seat and cover and/or for swiveling the bowl}	E03D5/10	E03D5/10		1481
E03D5/105	9	{touchless, e.g. using sensors}	E03D5/10	E03D5/10		1492
E03D5/12	8	discharging periodically (high-level cisterns for periodical discharge E03D1/16)	E03D5/12	E03D5/12		67
E03D7/00	7	Wheeled lavatories (wheeled closets without flushing A47K11/00; construction of land vehicles B62)	E03D7/00	E03D7/00		487
E03D9/00	7	Sanitary or other accessories for lavatories (hand tools for cleaning the toilet bowl A47K11/10; seats or covers for closets A47K13/00; body supports, other than seats for closets A47K17/02; devices for preventing contamination of drinking-water pipes E03C1/10){; Devices for cleaning or disinfecting the toilet room or the toilet bowl; Devices for eliminating smells (cleaning, disinfecting or deodorising the seat A47K13/30)}	E03D9/00	E03D9/00		3343
E03D9/002	8	{Automatic cleaning devices}	E03D9/00	E03D9/00		911
E03D9/005	8	{Devices adding disinfecting or deodorising agents to the bowl}	E03D9/00	E03D9/00		847
E03D9/007	8	{Devices for eliminating smells by diffusing deodorants in lavatories}	E03D9/00	E03D9/00		489
E03D9/02	8	Devices adding a disinfecting, deodorising, or cleaning agent to the water while flushing (apparatus for disinfection A61L2/00; treatment of water in general C02F)	E03D9/02	E03D9/02		533
E03D9/022	9	{consisting of solid substances introduced in the bowl or the supply line}	E03D9/02	E03D9/02		143
E03D2009/024	9	{using a solid substance}	E03D9/02	E03D9/02		678
E03D2009/026	9	{using a gel-form substance}	E03D9/02	E03D9/02		73
E03D2009/028	9	{using a liquid substance}	E03D9/02	E03D9/02		544
E03D9/03	9	consisting of a separate container with an outlet through which the agent is introduced into the flushing water, e.g. by suction {; Devices for agents in direct contact with flushing water}	E03D9/03	E03D9/03		244
E03D9/031	10	{Devices connected to or dispensing into the flushing pipe}	E03D9/03	E03D9/03		322
E03D9/032	10	{Devices connected to or dispensing into the bowl}	E03D9/03	E03D9/03		769
E03D9/033	10	{Devices placed inside or dispensing into the cistern}	E03D9/03	E03D9/03		342
E03D9/035	11	{Devices connected to the actuation mechanism (E03D9/036 takes precedence)}	E03D9/03	E03D9/03		117
E03D9/036	11	{Scoop-like devices}	E03D9/03	E03D9/03		28
E03D9/037	11	{Active dispensers, i.e. comprising a moving dosing element (E03D9/035 takes precedence)}	E03D9/03	E03D9/03		494
E03D9/038	11	{Passive dispensers, i.e. without moving parts}	E03D9/03	E03D9/03		492
E03D9/04	8	Special arrangement or operation of ventilating devices (ventilating rooms in general F24F)	E03D9/04	E03D9/04		773
E03D9/05	9	ventilating the bowl	E03D9/05	E03D9/05		1280
E03D9/052	10	using incorporated fans	E03D9/052	E03D9/052		1772
E03D9/06	8	Auxiliary chambers with water connection to the flushing pipe and adapted to receive utensils for bowl-cleaning, e.g. brushes	E03D9/06	E03D9/06		119
E03D9/08	8	Devices in the bowl producing upwardly-directed sprays; Modifications of the bowl for use with such devices (showers A47K3/28; bathing devices for special therapeutic or hygienic purposes A61H33/00, for specific parts of the body A61H35/00){; Bidets; Combinations of bowls with urinals or bidets; Hot-air or other devices mounted in or on the bowl, urinal or bidet for cleaning or disinfecting}	E03D9/08	E03D9/08		5066
E03D9/085	9	{Hand-held spray heads for bidet use or for cleaning the bowl}	E03D9/08	E03D9/08		449
E03D9/10	8	Waste-disintegrating apparatus combined with the bowl {(special flushing devices E03D5/00)}	E03D9/10	E03D9/10		433
E03D9/12	8	Means to prevent freezing of lavatories	E03D9/12	E03D9/12		126
E03D9/14	8	Noise-reducing means combined with flushing valves (noise-absorbing means in pipe systems F16L55/00{; if not in combination with flushing valves E03D11/00; noise-reducing means in valves in general F16K47/00})	E03D9/14	E03D9/14		225
E03D9/16	8	Water pressure regulating means in flushing pipes	E03D9/16	E03D9/16		288
E03D11/00	7	Other component parts of water-closets (pipe-joints or couplings in general F16L){, e.g. noise-reducing means in the flushing system (noise-reducing means in combination with flushing valves E03D9/14), flushing pipes mounted in the bowl, seals for the bowl outlet, devices preventing overflow of the bowl contents; devices forming a water seal in the bowl after flushing, devices eliminating obstructions in the bowl outlet or preventing backflow of water and excrements from the waterpipe}	E03D11/00	E03D11/00		1053
E03D11/02	8	Water-closet bowls (auxiliary chambers with connections to flushing water for bowl-cleaning utensils E03D9/06; modified for using upwardly-directed sprays E03D9/08; seats or covers A47K13/00){; Bowls with a double odour seal optionally with provisions for a good siphonic action; siphons as part of the bowl (parts or details of bowls E03D11/13)}	E03D11/02	E03D11/02		2537
E03D11/025	9	{Combined with wash-basins, urinals, flushing devices for chamber-pots, bed-pans, or the like}	E03D11/02	E03D11/02		694
E03D11/04	9	Bowls of flat shape with only slightly inclined bottom {; Squat-type closets}	E03D11/04	E03D11/04		560
E03D11/06	9	Bowls with downwardly-extending flanges {for the sake of flushing}	E03D11/06	E03D11/06		1174
E03D11/08	9	Bowls with means producing a flushing water swirl	E03D11/08	E03D11/08		645
E03D11/10	9	Bowls with closure elements provided between bottom or outlet and the outlet pipe; Bowls with pivotally supported inserts	E03D11/10	E03D11/10		810
E03D11/11	9	Bowls combined with a reservoir, e.g. containing apparatus for disinfecting or for disintegrating	E03D11/11	E03D11/11		436
E03D11/12	8	Swivel-mounted bowls, e.g. for use in restricted spaces {slidably or movably mounted bowls; combinations with flushing and disinfecting devices actuated by the swiveling or sliding movement of the bowl}	E03D11/12	E03D11/12		471
E03D11/125	9	{Height adjustable bowls}	E03D11/12	E03D11/12		258
E03D11/13	8	Parts or details of bowls; Special adaptations of pipe joints or couplings for use with bowls {, e.g. provisions in bowl construction preventing backflow of waste-water from the bowl in the flushing pipe or cistern, provisions for a secondary flushing, for noise-reducing}	E03D11/13	E03D11/13		2446
E03D11/135	9	{Supports for bowls}	E03D11/13	E03D11/13		219
E03D11/14	9	Means for connecting the bowl to the wall, e.g. to a wall outlet	E03D11/14	E03D11/14		595
E03D11/143	10	{Mounting frames for toilets and urinals}	E03D11/14	E03D11/14		391
E03D11/146	11	{with incorporated cistern (wall built-in flushing cisterns, connecting a cistern to the wall E03D1/012)}	E03D11/14	E03D11/14		340
E03D11/16	9	Means for connecting the bowl to the floor, e.g. to a floor outlet	E03D11/16	E03D11/16		1173
E03D11/17	9	Means for connecting the bowl to the flushing pipe	E03D11/17	E03D11/17		409
E03D11/18	8	Siphons (for pipes in general F16L43/00, F16L45/00{; if as part of the bowl E03D11/02; connecting the siphon to the bowl})	E03D11/18	E03D11/18		529
E03D13/00	7	Urinals (without flushing devices A47K11/00){; Means for connecting the urinal to the flushing pipe and the wastepipe; Splashing shields for urinals}	E03D13/00	E03D13/00		1713
E03D13/002	8	{intended for use by women}	E03D13/00	E03D13/00		102
E03D13/005	8	{Accessories specially adapted for urinals}	E03D13/00	E03D13/00		1285
E03D13/007	8	{Waterless or low-flush urinals; Accessories therefor (siphons E03C1/281)}	E03D13/00	E03D13/00		278
E03D2201/00	7	Details and methods of use for water closets and urinals not otherwise provided for	CPCONLY	E03D2201/00		373
E03D2201/20	8	Noise reduction features	CPCONLY	E03D2201/20		287
E03D2201/30	8	Water injection in siphon for enhancing flushing	CPCONLY	E03D2201/30		473
E03D2201/40	8	Devices for distribution of flush water inside the bowl	CPCONLY	E03D2201/40		815
